{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["instructions","summary","results"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":1,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"instructions","index":0,"n_rows":49,"n_cols":12,"rows_kept":49,"cut":false,"hidden":false,"merged":[[0,0,3,11],[18,6,18,11],[31,5,31,11],[32,5,32,11],[14,6,14,11],[14,0,20,2],[21,0,21,3],[6,0,6,4],[7,0,7,4],[11,0,11,4],[16,6,16,11],[17,6,17,11],[19,6,19,11],[20,6,20,11],[21,6,21,11],[6,6,6,11],[36,0,36,3],[34,10,34,11],[41,5,42,5],[41,6,41,7],[41,8,41,9],[41,10,41,11],[35,0,35,3],[34,6,34,7],[34,8,34,9],[34,5,35,5],[7,6,7,11],[8,6,8,11],[9,6,9,11],[10,6,10,11],[11,6,11,11],[12,6,12,11],[13,6,13,11],[15,6,15,11],[8,0,8,4],[9,0,9,4],[10,0,10,4]]}
["How to Use The EEM Selection & Cost Evaluation Tool Small Office\nDeveloped by the National Renewable Energy Laboratory\nRois Langner Rois.Langner@nrel.gov"]
[]
[]
[]
[]
["First, Take These Steps:",null,null,null,null,"Terms:"]
["Step 1: Enable Macros on your spreadsheet.",null,null,null,null,"Energy Efficiency Measure:","(EEM) the energy efficiency improvement."]
["Step 2: In the Summary tab, enter information about your building, under \"Input Building Data.\"",null,null,null,null,"Energy Savings Threshold:","The minimum desired savings the owner or evaluator expects to achieve cost effectively."]
["Step 3: Update additional data (if known) for efficiency measure costs, utility costs, and loan information for your project.",null,null,null,null,"Pre-1980 Construction","Buildings built before 1980."]
["Step 4: Press the \"Run\" button to generate a list of applicable energy efficiency measure (EEM) packages and associated cost analysis.",null,null,null,null,"Post-1980 Construction","Buildings built after 1980."]
["Step 5: Review recommended EEM packages and cost analysis listed under the orange headers. Each header is described in full - below and to the right.",null,null,null,null,"90.1-2004 Construction","Buildings built after 2004, and that comply to  ASHRAE Standard 90.1-2004."]
["Step 6: To restart analysis, press \"Clear\" and start from Step 1.",null,null,null,null,"Energy Savings:","Expected energy savings for each EEM package."]
[null,null,null,null,null,"Energy Cost Savings:","Expected annual energy cost savings for each EEM package, calculated with user input of electric and gas utility rates. "]
["Things to note:",null,null,null,null,"Net Initial Cost:","The net initial cost sums the relevant first cost or incremental costs together for each EEM noted in the EEM package. This cost subtracts the cost of a code-minimum system if the system is due for replacement at the time of a retrofit."]
["1. The predicted energy and energy cost savings represented in the EEM selection and Cost Evaluation Tool may not be accurate for all small office buildings. It is intended to be used by building owners to gain understanding of a wider range of possible EEM options that can be implemented within a building cost effectively.\n\n2. Other EEMs not represented in this tool may also be cost effective and appropriate for a particular building. The EEMs included in this tool represent \"typical\" EEMs that are commonly applied to small office buildings.\n\n3. The full set of EEM combinations, energy savings results, and energy cost savings results (used as input for this tool) is located in the Results tab. It is not intended that the user use this tab; however, these results are provided in the event that the user may want to understand or modify how the cost savings calculations are calculated.",null,null,null,null,"Full Initial Cost:","The full initial cost quantifies total project costs covered by the lease."]
[null,null,null,null,null,"QA Fee:","The QA fee is equal to the minimum of either 1% of the net initial cost, or $500. This is part of the Michigan Saves financing program."]
[null,null,null,null,null,"Rebate:","No rebates are applied to this model at this time."]
[null,null,null,null,null,"Annual Payment:","The annual energy-related lease payment is a factor of the net initial cost, the interest rate, the lease period, fees associated with the loan transaction, and any potential rebates."]
[null,null,null,null,null,"O&M Cost:","Costs associated with operation and maintenance (O&M) of each EEM."]
[null,null,null,null,null,"M&V Cost:","Costs associated with measurement and verification (M&V) of energy cost savings."]
[null,null,null,null,null,"Total 1st Year Cost:","Total first year costs equate to the sum of the annual energy-related lease payment (including annualized fees and rebates), O&M costs, and M&V costs."]
["Tool Assumptions and How To Interpret EEM Recommendations:",null,null,null,null,"Net Cash Flow:","The net cash flow over the lease period is calculated by subtracting the total first year cost from the expected annual energy cost savings. Cost effective is defined as a net positive cash flow, meaning the energy cost savings is greater than the annual costs associated with the lease."]
["Results Column Name","Baseline Option","Low Energy Option 1","Low Energy Option 2"]
["Roof Insulation","Baseline Roof Insulation: Adding insulation to the roof is not recommended as part of this EEM package. Model assumes baseline values:\n- R-30 for roofs with attics (post-1980 and 90.1-2004 construction)\n- R-14 (pre-1980 construction)","Increased Roof Insulation: Increasing roof insulation is recommended. Increase insulation to:\n- R-49 for roofs with attics (post-1980 and 90.1-2004 construction)\n- R-30 continuous insulation for insulation entirely above deck (pre-1980 construction)","N/A"]
["Window Type","Baseline Windows: Replacing windows is not recommended. Model assumes baseline values of:\n- U-0.62 (pre-1980 construction)\n- U-0.59 (post-1980 construction)\n- U-0.57 (90.1-2004 construction)","Replace Windows: Upgrading windows is recommended. Use windows that meet or come close to these specifications:\n- U-0.45, SHGC 0.25, double-glazed, low-e, spectrally selective, aluminum frame with thermal break","N/A"]
["Infiltration","Baseline Infiltration: Weather-stripping and building sealing are not recommended. Model assumes baseline values of (average leakage rates of): \n- 1.5 cfm/ft2 (pre-1980 and post-1980 construction)\n- 0.4 cfm/ft2 (90.1-2004 construction)","Reduce Infiltration: Taking action to reduce building leakage is recommended. It is recommended to reduce infiltration by:\n- 40% (pre-1980 construction)\n- 25% (post-1980 construction)\n- 10% (90.1-2004 construction)","N/A"]
["Lighting Power Density","Baseline Lighting Levels: Lighting upgrades are not recommended. Model assume baseline lighting power density (LPD) values of:\n- 1.8 W/ft2 at 40 fc (pre-1980 construction)\n- 1.8 W/ft2 at 40 fc (post-1980 construction)\n- 1.0 W/ft2 at 40 fc (90.1-2004 construction)","Reduce Lighting Levels to 4 fc: Lighting upgrades are recommended. Retrofit from T12 bulbs to T8 blubs, assuming that 0.5 W/ft2 of the office lighting will remain in place (office ambient LPD moves from 1.3 W/ft2 to 0.9 W/ft2). Recommended LPD targets include:\n- 1.4 W/ft2 at 40 fc (pre-1980 construction)\n- 1.4 W/ft2 at 40 fc (post-1980 construction)\n- 1.0 W/ft2 at 40 fc (90.1-2004 construction)","Reduce Light Levels to 25 fc: Lighting upgrades are recommended. Retrofit to T8 bulbs and change the lighting design (e.g., de-lamp fixtures and/or increase fixture spacing), assuming 0.5 W/ft2 of the office lighting will remain in place (office ambient LPD moves from 0.9 W/ft2 to 0.6 W/ft2). Recommended LPD targets include:\n- 1.1 W/ft2 at 25 fc (pre-1980 construction)\n- 1.1 W/ft2 at 25 fc (post-1980 construction)\n- 0.8 W/ft2 at 25 fc (90.1-2004 construction)"]
["Daylight Sensors","No Daylighting Sensors: Installing daylighting sensors is not recommended.","Install Daylighting Sensors: Daylighting sensors are recommended in areas close to windows."]
["Occupancy Sensors","No Occupancy Sensors: Installing occupancy sensors is not recommended","Install Occupancy Sensors: Occupancy sensors are recommended, particularly in areas such as lavatories and conference rooms  that are not consistently occupied."]
["Plug Loads","No Plug Load Control: Plug load controls are not recommended.","Install Plug Load Controls: Plug load controls, such as advanced power strips, are recommended. Advanced power strips allow occupants to easily turn off office equipment at the end of the day. Based on measured data, advanced power strips can help reduce plug load power to 10% at night."]
["HVAC Efficiency","Baseline HVAC Equipment: HVAC equipment upgrades are not recommended. Assumed efficiencies are noted in the HVAC Heating and Cooling Efficiency tables to the right.","Install High-Efficiency HVAC Equipment: HVAC upgrades are recommended. Low-energy efficiency recommendations are noted in the HVAC Heating and Cooling Efficiency tables to the right.",null,null,"HVAC System Cooling and Heating Efficiency"]
[null,null,null,null,null,"Note 1: High-efficiency values are derived from the U.S. Department of Energy's High Performance Rooftop Unit Challenge, proposed in the Tier 2 Category of the Consortium of Energy Efficiency Commercial Unitary AC and HP Specification."]
[null,null,null,null,null,"Note 2: Baseline efficiency values were developed by the national laboratories to represent typical efficiency values for each building vintage."]
[null,null,null,null,null,"HVAC System Cooling Efficiency:"]
[null,null,null,null,null,"System Type","Pre-1980",null,"Post-1980",null,"90.1-2004"]
[null,null,null,null,null,null,"Baseline (COP)","Low Energy (COP)","Baseline (COP)","Low Energy (COP)","Baseline (COP)","Low Energy (COP)"]
[null,null,null,null,null,"PSZ-AC*",2.81,3.52,2.5499999999999998,3.52,3.05,3.52]
[null,null,null,null,null,"PTAC**",2.92,3.66,2.65,3.66,3.17,3.66]
[null,null,null,null,null,"PTHP***",2.92,3.66,2.65,3.66,3.17,3.66]
[null,null,null,null,null,"HVAC System Heating Efficiency:"]
[]
[null,null,null,null,null,"System Type","Pre-1980",null,"Post-1980",null,"90.1-2004"]
[null,null,null,null,null,null,"Baseline","Low Energy","Baseline","Low Energy","Baseline","Low Energy"]
[null,null,null,null,null,"PSZ-AC*",0.78,0.8,0.8]
[null,null,null,null,null,"PTAC**",0.78,0.9,0.8,0.9,0.8,0.9]
[null,null,null,null,null,"PTHP*** (COP)",1.95,2.64,2,2.64,2,2.64]
[null,null,null,null,null,"*Packaged single zone air-conditioner (rooftop unit with DX cooling and gas forced-air furnace)"]
[null,null,null,null,null,"**Packaged terminal air-conditioner (split system DX air-conditioner with gas forced-air furnace)"]
[null,null,null,null,null,"***Packaged terminal heat pump (split system heat pump with electric supplemental heat)"]

{"sheet":"summary","index":1,"n_rows":66,"n_cols":23,"rows_kept":66,"cut":false,"hidden":false,"merged":[[30,1,30,2],[34,1,34,2],[0,4,0,8],[1,1,1,2],[59,1,59,2],[63,1,63,2],[12,1,12,2],[38,1,38,2],[46,1,46,2],[50,1,50,2],[54,1,54,2],[13,1,13,2],[42,1,42,2],[14,1,14,2],[18,1,18,2],[22,1,22,2],[26,1,26,2]]}
[null,null,null,null,"EEM Selection & Cost Evaluation Tool Small Office\nDeveloped by the National Renewable Energy Laboratory\nRois Langner Rois.Langner@nrel.gov"]
[null,"Input Building Data:",null,null,"Roof Insulation","Window Type","Infiltration","Lighting Power Density","Daylight Sensors","Occupancy Sensors","Plug Loads","HVAC Efficiency","Energy Savings","Energy Cost Savings","Net Initial Cost","Full Initial Cost","QA Fee","Rebate","Annual Payment","O&M Cost","M&V Cost","Total 1st Year Cost","Net Cash Flow"]
[null,"Vintage","Post 1980 Construction"]
[null,"Square Footage","10,000 SF"]
[null,"HVAC System Type","Packaged Air Conditioner"]
[null,"Boundary Conditions","Above Ground, 1 Side Attached"]
[null,"Major Renovation Planned?","Yes"]
[null,"Roof Replacement Planned?","No"]
[null,"HVAC Replacement Planned?","No"]
[null,"Energy Savings Threshold",0.2]
[]
[]
[null,"Additional Data - Update as Necessary"]
[null,"Efficiency Measure Costs"]
[null,"Increase Roof Insulation ($/ft2 of Roof Area)"]
[null,"Incremental Cost:",3]
[null,"Full Cost:",12.15]
[null,"O&M Cost:",0]
[null,"Replace Windows ($/ft2 of Window Area)"]
[null,"Incremental Cost:",7.18]
[null,"Full Cost:",43]
[null,"O&M Cost:",0]
[null,"Reduce Building Leakage ($/ft2 of Exterior Wall Area)"]
[null,"Incremental Cost:",0.43]
[null,"Full Cost:",0.43]
[null,"O&M Cost:",0]
[null,"LPD Reduction: Retrofit from T12s to T8s, 40fc ($/ft2)"]
[null,"Incremental Cost:",0.66]
[null,"Full Cost:",2.06]
[null,"O&M Cost:",-0.12]
[null,"LPD Reduction: Retrofit to T8s and Change Design, 25fc ($/ft2)"]
[null,"Incremental Cost:",0.79]
[null,"Full Cost:",11.15]
[null,"O&M Cost:",-0.19]
[null,"Daylighting Controls Added to Perimeter Zones ($/ft2)"]
[null,"Incremental Cost:",0.55000000000000004]
[null,"Full Cost:",3.41]
[null,"O&M Cost:",0]
[null,"Occupancy Sensors Applied to Entire Office Building ($/ft2)"]
[null,"Incremental Cost:",0.36]
[null,"Full Cost:",0.36]
[null,"O&M Cost:",0]
[null,"Advanced Power Strips ($/ft2)"]
[null,"Incremental Cost:",0.15]
[null,"Full Cost:",0.15]
[null,"O&M Cost:",0]
[null,"Replace HVAC Equipment PSZ-AC: Rooftop Unit with Gas Furnace ($/ft2)"]
[null,"Incremental Cost:",0.41]
[null,"Full Cost:",6.09]
[null,"O&M Cost:",0]
[null,"Replace HVAC Equipment - PTAC: Split System Air-Conditioner with Gas Furnace ($/ft2)"]
[null,"Incremental Cost:",0.66]
[null,"Full Cost:",2.85]
[null,"O&M Cost:",0]
[null,"Replace HVAC Equipment - PTHP: Heat Pump ($/ft2)"]
[null,"Incremental Cost:",1.53]
[null,"Full Cost:",3.3]
[null,"O&M Cost:",0]
[]
[null,"Utility Costs"]
[null,"Electricity ($/kWh):",0.1]
[null,"Gas ($/1000 ft3): ",9.14]
[]
[null,"Loan Information"]
[null,"Interest Rate:",5.8999999999999997E-2]
[null,"Loan Term (yrs): ",5]

{"sheet":"results","index":2,"n_rows":31110,"n_cols":56,"rows_kept":1125,"cut":true,"hidden":false,"merged":[[1,17,1,19],[0,0,0,1],[1,29,1,30]],"bounds":{"rows_first":500,"rows_last":125,"rows_between":500,"halvings":2}}
["Comments:\nFields highlighted in GREEN are inputs that can be selected on the summary tab. Fields highlighted in GRAY are displayed as results in the summary tab. Fields highlighted in BLUE can be updated by the user if necessary - on the summary tab.",null,"Increase Roof Insulation","Replace Windows Option 1",null,"Reduce Building Leakage","LPD Reduction, Retrofit to T8s, 40 fc","LPD Reduction, Retrofit to T8s and change design (e.g., delamp) to 25 fc plus task lights ","Daylighting Controls - reduce total power at perimeter zones by 50%","Occupancy Sensors applied to entire office building. If vacancy, manual-on sensors are used and savings is 20%. If auto-on, use 10% savings.","Add equipment controls to turn equipment off at night","Replace PSZ-AC","Replace PTAC","Replace PTHP"]
[null,"Normalizing Factor:","Roof area","Window Area",null,"Exterior Wall Area","Floor Area","Floor Area","Floor Area","Floor Area","Floor Area","Floor Area","Floor Area","Floor Area","1GJ=277.78kWh",null,null,"Averate State Electricity and Gas Prices for Michigan (179D DOE Calculator)",null,null,null,null,"Enter \"yes\" or \"no\" below:",null,null,null,null,null,null,"Financial Factors:"]
[null,"Incremental Cost:",{"$f":"summary!C16","v":3},{"$f":"summary!C20","v":7.18},null,{"$f":"summary!C24","v":0.43},{"$f":"summary!C28","v":0.66},{"$f":"summary!C32","v":0.79},{"$f":"summary!C36","v":0.55000000000000004},{"$f":"summary!C40","v":0.36},{"$f":"summary!C44","v":0.15},{"$f":"summary!C48","v":0.41},{"$f":"summary!C52","v":0.66},{"$f":"summary!C56","v":1.53},null,null,null,"Electricity: ",{"$f":"summary!C61","v":0.1},"$/kWh",null,null,"Major Renovation Planned?","Roof Replacement Planned?","HVAC Replacement Planned?",null,null,null,null,"Interest Rate:",{"$f":"summary!C65","v":5.8999999999999997E-2}]
[null,"Full Cost:",{"$f":"summary!C17","v":12.15},{"$f":"summary!C21","v":43},null,{"$f":"summary!C25","v":0.43},{"$f":"summary!C29","v":2.06},{"$f":"summary!C33","v":11.15},{"$f":"summary!C37","v":3.41},{"$f":"summary!C41","v":0.36},{"$f":"summary!C45","v":0.15},{"$f":"summary!C49","v":6.09},{"$f":"summary!C53","v":2.85},{"$f":"summary!C57","v":3.3},null,"Gas $/1000 ft3:",{"$f":"summary!C62","v":9.14},"Gas:",{"$f":"(Q4/1000)*(1/1000)*(3412)","v":3.118568E-2},"$/kWh",null,null,{"$f":"summary!C7","v":"Yes"},{"$f":"summary!C8","v":"No"},{"$f":"summary!C9","v":"No"},null,null,null,null,"Loan Term (yrs): ",{"$f":"summary!C66","v":5}]
[null,"O&M Cost Increase",{"$f":"summary!C18","v":0},{"$f":"summary!C22","v":0},null,{"$f":"summary!C26","v":0},{"$f":"summary!C30","v":-0.12},{"$f":"summary!C34","v":-0.19},{"$f":"summary!C38","v":0},{"$f":"summary!C42","v":0},{"$f":"summary!C46","v":0},{"$f":"summary!C50","v":0},{"$f":"summary!C54","v":0},{"$f":"summary!C58","v":0}]
["Vintage","Square Footage","HVAC System Type","Boundaries","Run Code","Roof Insulation","Window Type","Infiltration","Lighting Power Density","Daylight Sensors","Occ Sensors","Plug Loads","HVAC Efficiency","Electric Usage (GJ)","Gas Usage (GJ)","Energy Savings","Elec Savings","Gas Savings","Elec Cost Savings","Gas Cost Savings","Energy Cost Savings","20% savings?","Floor Area ( ft2)","Window Area ( ft2)","Opaque Wall Area ( ft2)",null,"Net Initial Cost","Full Initial Cost","QA Fee","Rebate","Annual Payment","O&M Costs","M&V Costs","Total 1st Yr Costs","Net Cash Flow",null,null,null,"Vintage","Square Footage","HVAC System Type","Boundary Conditions","Roof Insulation","Window Type","Infiltration","Lighting Power Density","Daylight Sensors","Occ Sensors","Plug Loads","HVAC Efficiency",null,"Vintage","Square Footage","HVAC System Type","Boundary Conditions","Yes/No"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alonebaseline",null,null,null,null,null,null,null,null,227.49,96.32,null,null,null,{"$f":"277.8*($N$7-N7)*$S$3","v":0},{"$f":"277.78*($O$7-O7)*$S$4","v":0},{"$f":"SUM(S7:T7)","v":0},{"$f":"IF(P7>0.2,\"yes\",\"no\")","v":"no"},{"$f":"IF(B7=\"5500 ft2\",5500,IF(B7=\"10000 ft2\",10000,25000))","v":5500},{"$f":"IF(B7=\"5500 ft2\",IF(D7=\"stand-alone\",642.39,IF(D7=\"ad-e&flr\",522.37,402.25)),IF(B7=\"10000 ft2\",IF(D7=\"stand-alone\",866.06,IF(D7=\"ad-e&flr\",704.17,542.29)),IF(B7=\"25000 ft2\",IF(D7=\"stand-alone\",1369.38,IF(D7=\"ad-e&flr\",1113.42,857.45)))))","v":642.39},{"$f":"IF(B7=\"5500 ft2\",IF(D7=\"stand-alone\",3030.15,IF(D7=\"ad-e&flr\",2424.14,1818.13)),IF(B7=\"10000 ft2\",IF(D7=\"stand-alone\",4085.12,IF(D7=\"ad-e&flr\",3268.14,2451.05)),IF(B7=\"25000 ft2\",IF(D7=\"stand-alone\",6459.2,IF(D7=\"ad-e&flr\",5167.32,3875.54)))))","v":3030.15},null,{"$f":"SUM(IF(F7=\"eff-roof\",W7*IF(AND(W$4=\"no\",X$4=\"no\"),$C$4,$C$3)),IF(G7=\"eff-win\",X7*IF(W$4=\"no\",$D$4,$D$3),0),IF(H7=\"red-inf\",Y7*IF(W$4=\"no\",$F$4,$F$3),0),IF(I7=\"25 fc\",W7*IF(W$4=\"no\",$H$4,$H$3),0),IF(I7=\"40 fc\",W7*IF(W$4=\"no\",$G$4,$G$3),0),IF(J7=\"yes-day\",W7*IF(W$4=\"no\",$I$4,$I$3),0),IF(K7=\"yes-occ\",W7*IF(W$4=\"no\",$J$4,$J$3),0),IF(L7=\"red-epd\",W7*IF(W$4=\"no\",$K$4,$K$3),0),IF(AND(M7=\"high-eff\",C7=\"psz-ac\"),W7*IF(AND(W$4=\"no\",Y$4=\"no\"),$L$4,$L$3),0),IF(AND(M7=\"high-eff\",C7=\"ptac\"),W7*IF(AND(W$4=\"no\",Y$4=\"no\"),$M$4,$M$3),0),IF(AND(M7=\"high-eff\",C7=\"pthp\"),W7*IF(AND(W$4=\"no\",Y$4=\"no\"),$N$4,$N$3),0))","v":0},{"$f":"SUM(IF(F7=\"eff-roof\",W7*$C$4),IF(G7=\"eff-win\",X7*$D$4,0),IF(H7=\"red-inf\",Y7*$F$4,0),IF(I7=\"25 fc\",W7*$H$4,0),IF(I7=\"40 fc\",W7*$G$4,0),IF(J7=\"yes-day\",W7*$I$4,0),IF(K7=\"yes-occ\",W7*$J$4,0),IF(L7=\"red-epd\",W7*$K$4,0),IF(AND(M7=\"high-eff\",C7=\"psz-ac\"),W7*$L$4,0),IF(AND(M7=\"high-eff\",C7=\"ptac\"),W7*$M$4,0),IF(AND(M7=\"high-eff\",C7=\"pthp\"),W7*$N$4,0))","v":0},{"$f":"MIN(0.01*AA7,500)","v":0},{"$f":"IF(V7=\"yes\",0,0)","v":0},{"$f":"-PMT($AE$3,$AE$4,AA7+AC7-AD7)","v":0},{"$f":"SUM(IF(F7=\"eff-roof\",($C$5*W7),0),IF(G7=\"eff-win\",($D$5*X7),0),IF(H7=\"red-inf\",$F$5*(Y7-X7),0),IF(I7=\"25 fc\",($H$5*W7),0),IF(I7=\"40 fc\",($G$5*W7),0),IF(J7=\"yes-day\",($I$5*W7),0),IF(K7=\"yes-occ\",($J$5*W7),0),IF(L7=\"red-epd\",($K$5*W7),0),IF(M7=\"high-eff\",($L$5*W7),0))","v":0},{"$f":"0.05*U7","v":0},{"$f":"SUM(AE7:AG7)","v":0},{"$f":"U7-AH7","v":0},null,null,null,{"$f":"IF(A7=\"new90.1-2004\",\"New Construction\",IF(A7=\"post1980\",\"Post 1980 Construction\",IF(A7=\"pre1980\",\"Pre 1980 Construction\")))","v":"New Construction"},{"$f":"IF(B7=\"5500 ft2\",\"5,500 SF\",IF(B7=\"10000 ft2\",\"10,000 SF\",IF(B7=\"25000 ft2\",\"25,000 SF\")))","v":"5,500 SF"},{"$f":"IF(C7=\"psz-ac\",\"Packaged Air Conditioner\",IF(C7=\"ptac\",\"Split System Air Conditioner\",IF(C7=\"pthp\",\"Split System Heat Pump\")))","v":"Packaged Air Conditioner"},{"$f":"IF(D7=\"stand-alone\",\"Stand Alone\",IF(D7=\"ad-e&flr\",\"Above Ground, 1 Side Attached\",IF(D7=\"ad-e&w&flr\",\"Above Ground, 2 Sides Attached\")))","v":"Stand Alone"},{"$f":"IF(F7=\"base-roof\",\"Baseline Roof Insulation\",IF(F7=\"eff-roof\",\"Increased Roof Insulation\"))","v":false},{"$f":"IF(G7=\"base-win\",\"Baseline Windows\",IF(G7=\"eff-win\",\"Replace Windows\"))","v":false},{"$f":"IF(H7=\"base-inf\",\"Baseline Infiltration\",IF(H7=\"red-inf\",\"Reduce Infiltration\"))","v":false},{"$f":"IF(I7=\"base-lpd\",\"Baseline Lighting Levels\",IF(I7=\"40 fc\",\"Reduce Lighting Levels to 40 fc\",IF(I7=\"25 fc\",\"Reduce Lighting Levels to 25 fc\")))","v":false},{"$f":"IF(J7=\"no-day\",\"No Daylighting Sensors\",IF(J7=\"yes-day\",\"Install Daylighting Sensors\"))","v":false},{"$f":"IF(K7=\"no-occ\",\"No Occupancy Sensors\",IF(K7=\"yes-occ\",\"Install Occupancy Sensors\"))","v":false},{"$f":"IF(L7=\"base-epd\",\"No Plug Load Control\",IF(L7=\"red-epd\",\"Install Plug Load Controls\"))","v":false},{"$f":"IF(M7=\"base-eff\",\"Baseline HVAC Equipment\",IF(M7=\"high-eff\",\"Install High Efficiency HVAC Equipment\"))","v":false},null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Yes"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","base-lpd","no-day","no-occ","base-epd","high-eff",225.86,96.32,5.0199693750297E-3,7.1651501164886203E-3,0,{"$f":"277.8*($N$7-N8)*$S$3","v":45.281399999999877},{"$f":"277.78*($O$7-O8)*$S$4","v":0},{"$f":"SUM(S8:T8)","v":45.281399999999877},"no",5500,642.39,3030.15,null,2255,33495,{"$f":"MIN(0.01*AA8,500)","v":22.55},{"$f":"IF(V8=\"yes\",0,0)","v":0},{"$f":"-PMT($AE$3,$AE$4,AA8+AC8-AD8)","v":539.21212353955184},0,2.264069999999994,{"$f":"SUM(AE8:AG8)","v":541.47619353955179},{"$f":"U8-AH8","v":-496.19479353955194},null,null,null,{"$f":"IF(A8=\"new90.1-2004\",\"New Construction\",IF(A8=\"post1980\",\"Post 1980 Construction\",IF(A8=\"pre1980\",\"Pre 1980 Construction\")))","v":"New Construction"},"5,500 SF",{"$f":"IF(C8=\"psz-ac\",\"Packaged Air Conditioner\",IF(C8=\"ptac\",\"Split System Air Conditioner\",IF(C8=\"pthp\",\"Split System Heat Pump\")))","v":"Packaged Air Conditioner"},{"$f":"IF(D8=\"stand-alone\",\"Stand Alone\",IF(D8=\"ad-e&flr\",\"Above Ground, 1 Side Attached\",IF(D8=\"ad-e&w&flr\",\"Above Ground, 2 Sides Attached\")))","v":"Stand Alone"},{"$f":"IF(F8=\"base-roof\",\"Baseline Roof Insulation\",IF(F8=\"eff-roof\",\"Increased Roof Insulation\"))","v":"Baseline Roof Insulation"},{"$f":"IF(G8=\"base-win\",\"Baseline Windows\",IF(G8=\"eff-win\",\"Replace Windows\"))","v":"Baseline Windows"},{"$f":"IF(H8=\"base-inf\",\"Baseline Infiltration\",IF(H8=\"red-inf\",\"Reduce Infiltration\"))","v":"Baseline Infiltration"},"Baseline Lighting Levels",{"$f":"IF(J8=\"no-day\",\"No Daylighting Sensors\",IF(J8=\"yes-day\",\"Install Daylighting Sensors\"))","v":"No Daylighting Sensors"},{"$f":"IF(K8=\"no-occ\",\"No Occupancy Sensors\",IF(K8=\"yes-occ\",\"Install Occupancy Sensors\"))","v":"No Occupancy Sensors"},{"$f":"IF(L8=\"base-epd\",\"No Plug Load Control\",IF(L8=\"red-epd\",\"Install Plug Load Controls\"))","v":"No Plug Load Control"},{"$f":"IF(M8=\"base-eff\",\"Baseline HVAC Equipment\",IF(M8=\"high-eff\",\"Install High Efficiency HVAC Equipment\"))","v":"Install High Efficiency HVAC Equipment"},null,"Post 1980 Construction","10,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","No"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","base-lpd","no-day","no-occ","red-epd","base-eff",196.69,107.71,5.9908125088796699E-2,0.135390566618313,-0.118251661129568,855.62400000000036,-98.668815788655991,756.95518421134443,"no",5500,642.39,3030.15,null,825,825,8.25,0,197.27272812422629,0,37.847759210567226,235.12048733479352,521.83469687655088,null,null,null,{"$f":"IF(A9=\"new90.1-2004\",\"New Construction\",IF(A9=\"post1980\",\"Post 1980 Construction\",IF(A9=\"pre1980\",\"Pre 1980 Construction\")))","v":"New Construction"},"5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment",null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","base-lpd","no-day","no-occ","red-epd","high-eff",195.25,107.71,6.4375582111228596E-2,0.14172051518748099,-0.118251661129568,895.62720000000036,-98.668815788655991,796.95838421134431,"no",5500,642.39,3030.15,null,3080,34320,30.8,0,736.48485166377816,0,39.84791921056722,776.33277087434533,20.625613336998981,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","base-lpd","no-day","yes-occ","base-epd","base-eff",212.79,102.2,2.7215179882235999E-2,6.4618224976922101E-2,-6.1046511627907099E-2,408.3660000000005,-50.937018159552082,357.42898184044839,"no",5500,642.39,3030.15,null,1980,1980,19.8,0,473.45454749814303,0,17.87144909202242,491.32599659016546,-133.89701474971707,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","base-lpd","no-day","yes-occ","base-epd","high-eff",211.3,102.2,3.1808925442404497E-2,7.1167963426963798E-2,-6.1046511627907099E-2,449.75819999999999,-50.937018159552082,398.82118184044793,"no",5500,642.39,3030.15,null,4235,35475,42.35,0,1012.666671037695,0,19.9410590920224,1032.6077301297173,-633.78654828926938,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","base-lpd","no-day","yes-occ","red-epd","base-eff",182.02,113.88,8.6207713072442294E-2,0.19987691766671101,-0.18230897009966801,1263.1566000000003,-152.11803382342401,1111.0385661765763,"no",5500,642.39,3030.15,null,2805,2805,28.05,0,670.72727562236935,0,55.55192830882882,726.27920393119814,384.75936224537816,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","base-lpd","no-day","yes-occ","red-epd","high-eff",180.7,113.88,9.0264732347230398E-2,0.20567937052178101,-0.18230897009966801,1299.8262000000007,-152.11803382342401,1147.7081661765767,"no",5500,642.39,3030.15,null,5060,36300,50.6,0,1209.9393991619213,0,57.385408308828836,1267.3248074707501,-119.61664129417341,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","base-lpd","yes-day","no-occ","base-epd","base-eff",204.69,104.71,4.4469351350498197E-2,0.10022418567849101,-8.7105481727574804E-2,633.38400000000047,-72.680541217455996,560.70345878254443,"no",5500,642.39,3030.15,null,3025.0000000000005,18755,30.250000000000004,0,723.33333645549635,0,28.035172939127222,751.36850939462352,-190.66505061207909,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","base-lpd","yes-day","no-occ","base-epd","high-eff",203.28,104.71,4.8826305902410598E-2,0.106422260319135,-8.7105481727574804E-2,672.55380000000025,-72.680541217455996,599.87325878254421,"no",5500,642.39,3030.15,null,5280,52250,52.800000000000004,0,1262.5454599950481,0,29.993662939127212,1292.5391229341753,-692.66586415163113,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","base-lpd","yes-day","no-occ","red-epd","base-eff",173.97,116.47,0.10305144679306,0.23526308848740601,-0.20919850498338899,1486.7856000000004,-174.55457753656003,1312.2310224634402,"no",5500,642.39,3030.15,null,3850.0000000000005,19580,38.500000000000007,0,920.60606457972267,0,65.611551123172021,986.2176157028947,326.01340676054554,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","base-lpd","yes-day","no-occ","red-epd","high-eff",172.73,116.47,0.10688746112681,0.24071387753307799,-0.20919850498338899,1521.2328000000007,-174.55457753656003,1346.6782224634408,"no",5500,642.39,3030.15,null,6105,53075,61.050000000000004,0,1459.8181881192745,0,67.333911123172044,1527.1520992424466,-180.47387677900588,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","base-lpd","yes-day","yes-occ","base-epd","base-eff",194.58,109.16,6.1960313827016299E-2,0.14466569959119099,-0.133305647840532,914.23979999999995,-111.22981516473602,803.00998483526394,"no",5500,642.39,3030.15,null,5005,20735,50.050000000000004,0,1196.7878839536393,0,40.1504992417632,1236.9383831954024,-433.92839836013843,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","base-lpd","yes-day","yes-occ","base-epd","high-eff",193.26,109.16,6.6017333101804396E-2,0.15046815244626099,-0.133305647840532,950.90940000000046,-111.22981516473602,839.67958483526445,"no",5500,642.39,3030.15,null,7260,54230,72.600000000000009,0,1736.0000074931913,0,41.983979241763222,1777.9839867349547,-938.30440189969022,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","base-lpd","yes-day","yes-occ","red-epd","base-eff",163.86,121.08,0.120005682984198,0.27970460240010497,-0.257059800664452,1767.6414000000002,-214.48989279430404,1553.1515072056961,"no",5500,642.39,3030.15,null,5830,21560,58.300000000000004,0,1394.0606120778657,0,77.65757536028481,1471.7181874381506,81.433319767545527,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","base-lpd","yes-day","yes-occ","red-epd","high-eff",162.71,121.08,0.12355754810804,0.284759769660205,-0.257059800664452,1799.5884000000003,-214.48989279430404,1585.0985072056963,"no",5500,642.39,3030.15,null,8085,55055,80.850000000000009,0,1933.2727356174175,0,79.254925360284815,2012.5276609777025,-427.4291537720062,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","40 fc","no-day","no-occ","base-epd","base-eff",227.49,96.32,0,0,0,0,0,0,"no",5500,642.39,3030.15,null,3630,11330,36.300000000000004,0,868.00000374659567,-660,0,208.00000374659567,-208.00000374659567,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","40 fc","no-day","no-occ","base-epd","high-eff",225.86,96.32,5.0199693750297E-3,7.1651501164886203E-3,0,45.281399999999877,0,45.281399999999877,"no",5500,642.39,3030.15,null,5885,44825,58.85,0,1407.2121272861473,-660,2.264069999999994,749.47619728614723,-704.19479728614738,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","40 fc","no-day","no-occ","red-epd","base-eff",196.69,107.71,5.9908125088796699E-2,0.135390566618313,-0.118251661129568,855.62400000000036,-98.668815788655991,756.95518421134443,"no",5500,642.39,3030.15,null,4455,12155,44.550000000000004,0,1065.2727318708219,-660,37.847759210567226,443.1204910813891,313.83469312995533,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","40 fc","no-day","no-occ","red-epd","high-eff",195.25,107.71,6.4375582111228596E-2,0.14172051518748099,-0.118251661129568,895.62720000000036,-98.668815788655991,796.95838421134431,"no",5500,642.39,3030.15,null,6710,45650,67.099999999999994,0,1604.4848554103737,-660,39.84791921056722,984.33277462094088,-187.37439040959657,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","40 fc","no-day","yes-occ","base-epd","base-eff",212.79,102.2,2.7215179882235999E-2,6.4618224976922101E-2,-6.1046511627907099E-2,408.3660000000005,-50.937018159552082,357.42898184044839,"no",5500,642.39,3030.15,null,5610,13310,56.1,0,1341.4545512447387,-660,17.87144909202242,699.32600033676113,-341.89701849631274,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","40 fc","no-day","yes-occ","base-epd","high-eff",211.3,102.2,3.1808925442404497E-2,7.1167963426963798E-2,-6.1046511627907099E-2,449.75819999999999,-50.937018159552082,398.82118184044793,"no",5500,642.39,3030.15,null,7865,46805,78.650000000000006,0,1880.6666747842903,-660,19.9410590920224,1240.6077338763127,-841.78655203586482,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","40 fc","no-day","yes-occ","red-epd","base-eff",182.02,113.88,8.6207713072442294E-2,0.19987691766671101,-0.18230897009966801,1263.1566000000003,-152.11803382342401,1111.0385661765763,"no",5500,642.39,3030.15,null,6435,14135,64.349999999999994,0,1538.7272793689651,-660,55.55192830882882,934.27920767779392,176.75935849878238,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","40 fc","no-day","yes-occ","red-epd","high-eff",180.7,113.88,9.0264732347230398E-2,0.20567937052178101,-0.18230897009966801,1299.8262000000007,-152.11803382342401,1147.7081661765767,"no",5500,642.39,3030.15,null,8690,47630,86.9,0,2077.9394029085165,-660,57.385408308828836,1475.3248112173453,-327.61664504076862,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","40 fc","yes-day","no-occ","base-epd","base-eff",204.69,104.71,4.4469351350498197E-2,0.10022418567849101,-8.7105481727574804E-2,633.38400000000047,-72.680541217455996,560.70345878254443,"no",5500,642.39,3030.15,null,6655,30085,66.55,0,1591.3333402020919,-660,28.035172939127222,959.36851314121918,-398.66505435867475,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","40 fc","yes-day","no-occ","base-epd","high-eff",203.28,104.71,4.8826305902410598E-2,0.106422260319135,-8.7105481727574804E-2,672.55380000000025,-72.680541217455996,599.87325878254421,"no",5500,642.39,3030.15,null,8910,63580,89.100000000000009,0,2130.5454637416437,-660,29.993662939127212,1500.539126680771,-900.66586789822679,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","40 fc","yes-day","no-occ","red-epd","base-eff",173.97,116.47,0.10305144679306,0.23526308848740601,-0.20919850498338899,1486.7856000000004,-174.55457753656003,1312.2310224634402,"no",5500,642.39,3030.15,null,7480,30910,74.8,0,1788.6060683263183,-660,65.611551123172021,1194.2176194494903,118.01340301394998,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","40 fc","yes-day","no-occ","red-epd","high-eff",172.73,116.47,0.10688746112681,0.24071387753307799,-0.20919850498338899,1521.2328000000007,-174.55457753656003,1346.6782224634408,"no",5500,642.39,3030.15,null,9735,64405,97.350000000000009,0,2327.8181918658702,-660,67.333911123172044,1735.1521029890423,-388.47388052560154,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","40 fc","yes-day","yes-occ","base-epd","base-eff",194.58,109.16,6.1960313827016299E-2,0.14466569959119099,-0.133305647840532,914.23979999999995,-111.22981516473602,803.00998483526394,"no",5500,642.39,3030.15,null,8635,32065,86.350000000000009,0,2064.7878877002349,-660,40.1504992417632,1444.938386941998,-641.9284021067341,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","40 fc","yes-day","yes-occ","base-epd","high-eff",193.26,109.16,6.6017333101804396E-2,0.15046815244626099,-0.133305647840532,950.90940000000046,-111.22981516473602,839.67958483526445,"no",5500,642.39,3030.15,null,10890,65560,108.9,0,2604.0000112397865,-660,41.983979241763222,1985.9839904815499,-1146.3044056462854,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","40 fc","yes-day","yes-occ","red-epd","base-eff",163.86,121.08,0.120005682984198,0.27970460240010497,-0.257059800664452,1767.6414000000002,-214.48989279430404,1553.1515072056961,"no",5500,642.39,3030.15,null,9460,32890,94.600000000000009,0,2262.0606158244614,-660,77.65757536028481,1679.7181911847463,-126.56668397905014,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","40 fc","yes-day","yes-occ","red-epd","high-eff",162.71,121.08,0.12355754810804,0.284759769660205,-0.257059800664452,1799.5884000000003,-214.48989279430404,1585.0985072056963,"no",5500,642.39,3030.15,null,11715,66385,117.15,0,2801.272739364013,-660,79.254925360284815,2220.5276647242977,-635.42915751860141,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","25 fc","no-day","no-occ","base-epd","base-eff",212.79,102.2,2.7215179882235999E-2,6.4618224976922101E-2,-6.1046511627907099E-2,408.3660000000005,-50.937018159552082,357.42898184044839,"no",5500,642.39,3030.15,null,4345,61325,43.45,0,1038.9697014542583,-1045,17.87144909202242,11.841150546280677,345.5878312941677,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","25 fc","no-day","no-occ","base-epd","high-eff",211.3,102.2,3.1808925442404497E-2,7.1167963426963798E-2,-6.1046511627907099E-2,449.75819999999999,-50.937018159552082,398.82118184044793,"no",5500,642.39,3030.15,null,6600,94820,66,0,1578.1818249938103,-1045,19.9410590920224,553.12288408583277,-154.30170224538483,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","25 fc","no-day","no-occ","red-epd","base-eff",182.02,113.88,8.6207713072442294E-2,0.19987691766671101,-0.18230897009966801,1263.1566000000003,-152.11803382342401,1111.0385661765763,"no",5500,642.39,3030.15,null,5170,62150,51.7,0,1236.2424295784845,-1045,55.55192830882882,246.79435788731328,864.24420828926304,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","25 fc","no-day","no-occ","red-epd","high-eff",180.7,113.88,9.0264732347230398E-2,0.20567937052178101,-0.18230897009966801,1299.8262000000007,-152.11803382342401,1147.7081661765767,"no",5500,642.39,3030.15,null,7425,95645,74.25,0,1775.4545531180365,-1045,57.385408308828836,787.83996142686533,359.86820474971137,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","25 fc","no-day","yes-occ","base-epd","base-eff",201.25,106.95,4.8179077146510499E-2,0.115345729482615,-0.110361295681063,728.94720000000029,-92.085119563952077,636.86208043604825,"no",5500,642.39,3030.15,null,6325,63305,63.25,0,1512.4242489524013,-1045,31.843104021802414,499.26735297420367,137.59472746184457,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","25 fc","no-day","yes-occ","base-epd","high-eff",199.87,106.95,5.2457101362337603E-2,0.12141193019473399,-0.110361295681063,767.28360000000021,-92.085119563952077,675.19848043604816,"no",5500,642.39,3030.15,null,8580,96800,85.8,0,2051.6363724919529,-1045,33.759924021802412,1040.3962965137553,-365.1978160777071,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","25 fc","no-day","yes-occ","red-epd","base-eff",170.48,118.89,0.106334948774212,0.25060442217240297,-0.23432308970099699,1583.7378000000008,-195.51845235732804,1388.2193476426728,"no",5500,642.39,3030.15,null,7150,64130,71.5,0,1709.6969770766277,-1045,69.410967382133649,734.10794445876138,654.11140318391142,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","25 fc","no-day","yes-occ","red-epd","high-eff",169.27,118.89,0.110092032771876,0.25592333728955102,-0.23432308970099699,1617.3516,-195.51845235732804,1421.833147642672,"no",5500,642.39,3030.15,null,9405,97625,94.05,0,2248.9091006161793,-1045,71.091657382133604,1275.000757998313,146.83238964435895,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","25 fc","yes-day","no-occ","base-epd","base-eff",194.58,109.16,6.1960313827016299E-2,0.14466569959119099,-0.133305647840532,914.23979999999995,-111.22981516473602,803.00998483526394,"no",5500,642.39,3030.15,null,7370,80080,73.7,0,1762.3030379097545,-1045,40.1504992417632,757.45353715151771,45.556447683746228,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","25 fc","yes-day","no-occ","base-epd","high-eff",193.26,109.16,6.6017333101804396E-2,0.15046815244626099,-0.133305647840532,950.90940000000046,-111.22981516473602,839.67958483526445,"no",5500,642.39,3030.15,null,9625,113575,96.25,0,2301.5151614493066,-1045,41.983979241763222,1298.4991406910699,-458.81955585580545,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","25 fc","yes-day","no-occ","red-epd","base-eff",163.86,121.08,0.120005682984198,0.27970460240010497,-0.257059800664452,1767.6414000000002,-214.48989279430404,1553.1515072056961,"no",5500,642.39,3030.15,null,8195,80905,81.95,0,1959.5757660339812,-1045,77.65757536028481,992.23334139426595,560.91816581143019,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","25 fc","yes-day","no-occ","red-epd","high-eff",162.71,121.08,0.12355754810804,0.284759769660205,-0.257059800664452,1799.5884000000003,-214.48989279430404,1585.0985072056963,"no",5500,642.39,3030.15,null,10450,114400,104.5,0,2498.787889573533,-1045,79.254925360284815,1533.0428149338179,52.055692271878343,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","25 fc","yes-day","yes-occ","base-epd","base-eff",186.7,112.73,7.5299540625444097E-2,0.179304584816915,-0.170369601328904,1133.1462000000008,-142.15586190446407,990.9903380955368,"no",5500,642.39,3030.15,null,9350,82060,93.5,0,2235.7575854078977,-1045,49.549516904776844,1240.3071023126745,-249.31676421713769,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","25 fc","yes-day","yes-occ","base-epd","high-eff",185.44,112.73,7.9151341026410096E-2,0.184843289814937,-0.170369601328904,1168.1490000000003,-142.15586190446407,1025.9931380955363,"no",5500,642.39,3030.15,null,11605,115555,116.05,0,2774.9697089474494,-1045,51.299656904776818,1781.2693658522262,-755.27622775668988,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","25 fc","yes-day","yes-occ","red-epd","base-eff",155.97,124.81,0.13285554169889699,0.31438744560200399,-0.29578488372092998,1986.8256000000006,-246.80198084449606,1740.0236191555045,"no",5500,642.39,3030.15,null,10175,82885,101.75,0,2433.0303135321242,-1045,87.001180957775233,1475.0314944898994,264.99212466560516,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","base-inf","25 fc","yes-day","yes-occ","red-epd","high-eff",154.88999999999999,124.81,0.136202187948916,0.31913490702887998,-0.29578488372092998,2016.8280000000007,-246.80198084449606,1770.0260191555046,"no",5500,642.39,3030.15,null,12430,116380,124.3,0,2972.2424370716753,-1045,88.501300957775243,2015.7437380294505,-245.71771887394584,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","base-lpd","no-day","no-occ","base-epd","base-eff",227.4,94.79,4.9883972405955802E-3,3.9562178557300701E-4,1.58845514950165E-2,2.500200000000095,13.254020031311885,15.754220031311981,"no",5500,642.39,3030.15,null,1302.9645,1302.9645,13.029645,0,311.56286250184053,0,0.78771100156559903,312.35057350340611,-296.59635347209411,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","base-lpd","no-day","no-occ","base-epd","high-eff",225.76,94.79,1.0024152682842199E-2,7.6047298782364898E-3,1.58845514950165E-2,48.059400000000508,13.254020031311885,61.31342003131239,"no",5500,642.39,3030.15,null,3557.9645,34797.964500000002,35.579644999999999,0,850.77498604139225,0,3.0656710015656197,853.8406570429579,-792.52723701164552,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","base-lpd","no-day","no-occ","red-epd","base-eff",196.61,106.01,6.5417462547555594E-2,0.135742230427711,-0.10060215946843901,857.84640000000002,-83.942126864976103,773.90427313502391,"no",5500,642.39,3030.15,null,2127.9645,2127.9645,21.279645000000002,0,508.83559062606679,0,38.6952136567512,547.53080428281794,226.37346885220597,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","base-lpd","no-day","no-occ","red-epd","high-eff",195.16,106.01,6.9900705637204602E-2,0.142116136973054,-0.10060215946843901,898.12740000000031,-83.942126864976103,814.1852731350242,"no",5500,642.39,3030.15,null,4382.9645,35622.964500000002,43.829644999999999,0,1048.0477141656186,0,40.709263656751212,1088.7569778223699,-274.57170468734569,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","base-lpd","no-day","yes-occ","base-epd","base-eff",212.71,100.53,3.2614014870475397E-2,6.4969888786320304E-2,-4.3708471760797403E-2,410.58840000000009,-36.470211981584065,374.11818801841605,"no",5500,642.39,3030.15,null,3282.9645,3282.9645,32.829644999999999,0,785.01740999998356,0,18.705909400920802,803.7233194009043,-429.60513138248825,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","base-lpd","no-day","yes-occ","base-epd","high-eff",211.22,100.53,3.7223546497861103E-2,7.1519627236362099E-2,-4.3708471760797403E-2,451.98060000000032,-36.470211981584065,415.51038801841628,"no",5500,642.39,3030.15,null,5537.9645,36777.964500000002,55.379645000000004,0,1324.2295335395354,0,20.775519400920814,1345.0050529404562,-929.49466492203987,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","base-lpd","no-day","yes-occ","red-epd","base-eff",181.94,112.18,9.1669692329549995E-2,0.200228581476109,-0.16465946843853799,1265.3790000000006,-137.39134489974413,1127.9876551002565,"no",5500,642.39,3030.15,null,4107.9645,4107.9645,41.079644999999999,0,982.29013812420976,0,56.399382755012823,1038.6895208792225,89.298134221033933,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","base-lpd","no-day","yes-occ","red-epd","high-eff",180.63,112.18,9.5726711604338002E-2,0.20598707635500499,-0.16465946843853799,1301.7708000000005,-137.39134489974413,1164.3794551002563,"no",5500,642.39,3030.15,null,6362.9645,37602.964500000002,63.629645000000004,0,1521.5022616637616,0,58.218972755012821,1579.7212344187744,-415.34177931851809,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","base-lpd","yes-day","no-occ","base-epd","base-eff",204.6,103.14,4.9631395330481401E-2,0.100619807464064,-7.0805647840531602E-2,635.88420000000042,-59.080010858528063,576.80418914147231,"no",5500,642.39,3030.15,null,4327.9645,20057.964500000002,43.279645000000002,0,1034.8961989573368,0,28.840209457073616,1063.7364084144103,-486.93221927293803,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","base-lpd","yes-day","no-occ","base-epd","high-eff",203.18,103.14,5.3988349882393899E-2,0.10686184008088299,-7.0805647840531602E-2,675.33180000000016,-59.080010858528063,616.25178914147205,"no",5500,642.39,3030.15,null,6582.9645,53552.964500000002,65.829644999999999,0,1574.1083224968886,0,30.812589457073603,1604.9209119539621,-988.66912281249006,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","base-lpd","yes-day","no-occ","red-epd","base-eff",173.88,114.75,0.108623928520688,0.23565871027297899,-0.191341362126246,1489.2858000000006,-159.65463344907204,1329.6311665509286,"no",5500,642.39,3030.15,null,5152.9645,20882.964500000002,51.529645000000002,0,1232.168927081563,0,66.481558327546438,1298.6504854091095,30.980681141819105,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","base-lpd","yes-day","no-occ","red-epd","high-eff",172.64,114.75,0.112459942854437,0.241109499318651,-0.191341362126246,1523.7330000000009,-159.65463344907204,1364.0783665509289,"no",5500,642.39,3030.15,null,7407.9645,54377.964500000002,74.079644999999999,0,1771.381050621115,0,68.203918327546447,1839.5849689486615,-475.50660239773265,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","base-lpd","yes-day","yes-occ","base-epd","base-eff",194.5,107.55,6.7169716008650904E-2,0.14501736340058899,-0.116590531561462,916.46220000000039,-97.282774478192025,819.17942552180841,"no",5500,642.39,3030.15,null,6307.9645,22037.964500000002,63.079644999999999,0,1508.3507464554798,0,40.958971276090423,1549.3097177315701,-730.13029220976171,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","base-lpd","yes-day","yes-occ","base-epd","high-eff",193.18,107.55,7.1258307417873007E-2,0.15081981625565999,-0.116590531561462,953.13180000000011,-97.282774478192025,855.84902552180813,"no",5500,642.39,3030.15,null,8562.9645,55532.964500000002,85.629644999999996,0,2047.5628699950321,0,42.792451276090411,2090.3553212711226,-1234.5062957493146,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","base-lpd","yes-day","yes-occ","red-epd","base-eff",163.78,119.45,0.12530980156913499,0.28005626620950402,-0.24013704318936899,1769.8638000000003,-200.36959694395208,1569.4942030560483,"no",5500,642.39,3030.15,null,7132.9645,22862.964500000002,71.329644999999999,0,1705.6234745797062,0,78.474710152802416,1784.0981847325086,-214.60398167646031,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","base-lpd","yes-day","yes-occ","red-epd","high-eff",162.63,119.45,0.12886166669297699,0.28511143346960299,-0.24013704318936899,1801.8108000000004,-200.36959694395208,1601.4412030560484,"no",5500,642.39,3030.15,null,9387.9645,56357.964500000002,93.879644999999996,0,2244.8355981192581,0,80.072060152802422,2324.9076582720604,-723.46645521601204,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","40 fc","no-day","no-occ","base-epd","base-eff",227.4,94.79,4.9883972405955802E-3,3.9562178557300701E-4,1.58845514950165E-2,2.500200000000095,13.254020031311885,15.754220031311981,{"$f":"IF(P71>0.2,\"yes\",\"no\")","v":"no"},{"$f":"IF(B71=\"5500 ft2\",5500,IF(B71=\"10000 ft2\",10000,25000))","v":5500},{"$f":"IF(B71=\"5500 ft2\",IF(D71=\"stand-alone\",642.39,IF(D71=\"ad-e&flr\",522.37,402.25)),IF(B71=\"10000 ft2\",IF(D71=\"stand-alone\",866.06,IF(D71=\"ad-e&flr\",704.17,542.29)),IF(B71=\"25000 ft2\",IF(D71=\"stand-alone\",1369.38,IF(D71=\"ad-e&flr\",1113.42,857.45)))))","v":642.39},{"$f":"IF(B71=\"5500 ft2\",IF(D71=\"stand-alone\",3030.15,IF(D71=\"ad-e&flr\",2424.14,1818.13)),IF(B71=\"10000 ft2\",IF(D71=\"stand-alone\",4085.12,IF(D71=\"ad-e&flr\",3268.14,2451.05)),IF(B71=\"25000 ft2\",IF(D71=\"stand-alone\",6459.2,IF(D71=\"ad-e&flr\",5167.32,3875.54)))))","v":3030.15},null,{"$f":"SUM(IF(F71=\"eff-roof\",W71*IF(AND(W$4=\"no\",X$4=\"no\"),$C$4,$C$3)),IF(G71=\"eff-win\",X71*IF(W$4=\"no\",$D$4,$D$3),0),IF(H71=\"red-inf\",Y71*IF(W$4=\"no\",$F$4,$F$3),0),IF(I71=\"25 fc\",W71*IF(W$4=\"no\",$H$4,$H$3),0),IF(I71=\"40 fc\",W71*IF(W$4=\"no\",$G$4,$G$3),0),IF(J71=\"yes-day\",W71*IF(W$4=\"no\",$I$4,$I$3),0),IF(K71=\"yes-occ\",W71*IF(W$4=\"no\",$J$4,$J$3),0),IF(L71=\"red-epd\",W71*IF(W$4=\"no\",$K$4,$K$3),0),IF(AND(M71=\"high-eff\",C71=\"psz-ac\"),W71*IF(AND(W$4=\"no\",Y$4=\"no\"),$L$4,$L$3),0),IF(AND(M71=\"high-eff\",C71=\"ptac\"),W71*IF(AND(W$4=\"no\",Y$4=\"no\"),$M$4,$M$3),0),IF(AND(M71=\"high-eff\",C71=\"pthp\"),W71*IF(AND(W$4=\"no\",Y$4=\"no\"),$N$4,$N$3),0))","v":4932.9645},{"$f":"SUM(IF(F71=\"eff-roof\",W71*$C$4),IF(G71=\"eff-win\",X71*$D$4,0),IF(H71=\"red-inf\",Y71*$F$4,0),IF(I71=\"25 fc\",W71*$H$4,0),IF(I71=\"40 fc\",W71*$G$4,0),IF(J71=\"yes-day\",W71*$I$4,0),IF(K71=\"yes-occ\",W71*$J$4,0),IF(L71=\"red-epd\",W71*$K$4,0),IF(AND(M71=\"high-eff\",C71=\"psz-ac\"),W71*$L$4,0),IF(AND(M71=\"high-eff\",C71=\"ptac\"),W71*$M$4,0),IF(AND(M71=\"high-eff\",C71=\"pthp\"),W71*$N$4,0))","v":12632.9645},49.329644999999999,0,{"$f":"-PMT($AE$3,$AE$4,AA71+AC71-AD71)","v":1179.562866248436},{"$f":"SUM(IF(F71=\"eff-roof\",($C$5*W71),0),IF(G71=\"eff-win\",($D$5*X71),0),IF(H71=\"red-inf\",$F$5*(Y71-X71),0),IF(I71=\"25 fc\",($H$5*W71),0),IF(I71=\"40 fc\",($G$5*W71),0),IF(J71=\"yes-day\",($I$5*W71),0),IF(K71=\"yes-occ\",($J$5*W71),0),IF(L71=\"red-epd\",($K$5*W71),0),IF(M71=\"high-eff\",($L$5*W71),0))","v":-660},{"$f":"0.05*U71","v":0.78771100156559903},520.35057725000161,{"$f":"U71-AH71","v":-504.5963572186896},null,null,null,"New Construction",{"$f":"IF(B71=\"5500 ft2\",\"5,500 SF\",IF(B71=\"10000 ft2\",\"10,000 SF\",IF(B71=\"25000 ft2\",\"25,000 SF\")))","v":"5,500 SF"},"Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration",{"$f":"IF(I71=\"base-lpd\",\"Baseline Lighting Levels\",IF(I71=\"40 fc\",\"Reduce Lighting Levels to 40 fc\",IF(I71=\"25 fc\",\"Reduce Lighting Levels to 25 fc\")))","v":"Reduce Lighting Levels to 40 fc"},"No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","40 fc","no-day","no-occ","base-epd","high-eff",225.76,94.79,1.0024152682842199E-2,7.6047298782364898E-3,1.58845514950165E-2,{"$f":"277.8*($N$7-N72)*$S$3","v":48.059400000000508},{"$f":"277.78*($O$7-O72)*$S$4","v":13.254020031311885},{"$f":"SUM(S72:T72)","v":61.31342003131239},"no",5500,642.39,3030.15,null,7187.9645,46127.964500000002,{"$f":"MIN(0.01*AA72,500)","v":71.879644999999996},{"$f":"IF(V72=\"yes\",0,0)","v":0},1718.7749897879878,-660,3.0656710015656197,{"$f":"SUM(AE72:AG72)","v":1061.8406607895533},-1000.527240758241,null,null,null,"New Construction","5,500 SF",{"$f":"IF(C72=\"psz-ac\",\"Packaged Air Conditioner\",IF(C72=\"ptac\",\"Split System Air Conditioner\",IF(C72=\"pthp\",\"Split System Heat Pump\")))","v":"Packaged Air Conditioner"},{"$f":"IF(D72=\"stand-alone\",\"Stand Alone\",IF(D72=\"ad-e&flr\",\"Above Ground, 1 Side Attached\",IF(D72=\"ad-e&w&flr\",\"Above Ground, 2 Sides Attached\")))","v":"Stand Alone"},{"$f":"IF(F72=\"base-roof\",\"Baseline Roof Insulation\",IF(F72=\"eff-roof\",\"Increased Roof Insulation\"))","v":"Baseline Roof Insulation"},{"$f":"IF(G72=\"base-win\",\"Baseline Windows\",IF(G72=\"eff-win\",\"Replace Windows\"))","v":"Baseline Windows"},{"$f":"IF(H72=\"base-inf\",\"Baseline Infiltration\",IF(H72=\"red-inf\",\"Reduce Infiltration\"))","v":"Reduce Infiltration"},"Reduce Lighting Levels to 40 fc",{"$f":"IF(J72=\"no-day\",\"No Daylighting Sensors\",IF(J72=\"yes-day\",\"Install Daylighting Sensors\"))","v":"No Daylighting Sensors"},{"$f":"IF(K72=\"no-occ\",\"No Occupancy Sensors\",IF(K72=\"yes-occ\",\"Install Occupancy Sensors\"))","v":"No Occupancy Sensors"},{"$f":"IF(L72=\"base-epd\",\"No Plug Load Control\",IF(L72=\"red-epd\",\"Install Plug Load Controls\"))","v":"No Plug Load Control"},{"$f":"IF(M72=\"base-eff\",\"Baseline HVAC Equipment\",IF(M72=\"high-eff\",\"Install High Efficiency HVAC Equipment\"))","v":"Install High Efficiency HVAC Equipment"}]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","40 fc","no-day","no-occ","red-epd","base-eff",196.61,106.01,6.5417462547555594E-2,0.135742230427711,-0.10060215946843901,857.84640000000002,-83.942126864976103,773.90427313502391,"no",5500,642.39,3030.15,null,5757.9645,13457.9645,57.579644999999999,0,1376.8355943726624,-660,38.6952136567512,755.53080802941361,18.373465105610308,null,null,null,{"$f":"IF(A73=\"new90.1-2004\",\"New Construction\",IF(A73=\"post1980\",\"Post 1980 Construction\",IF(A73=\"pre1980\",\"Pre 1980 Construction\")))","v":"New Construction"},"5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","40 fc","no-day","no-occ","red-epd","high-eff",195.16,106.01,6.9900705637204602E-2,0.142116136973054,-0.10060215946843901,898.12740000000031,-83.942126864976103,814.1852731350242,"no",5500,642.39,3030.15,null,8012.9645,46952.964500000002,80.129644999999996,0,1916.0477179122142,-660,40.709263656751212,1296.7569815689656,-482.57170843394135,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","40 fc","no-day","yes-occ","base-epd","base-eff",212.71,100.53,3.2614014870475397E-2,6.4969888786320304E-2,-4.3708471760797403E-2,410.58840000000009,-36.470211981584065,374.11818801841605,"no",5500,642.39,3030.15,null,6912.9645,14612.9645,69.129644999999996,0,1653.0174137465792,-660,18.705909400920802,1011.7233231475,-637.60513512908392,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","40 fc","no-day","yes-occ","base-epd","high-eff",211.22,100.53,3.7223546497861103E-2,7.1519627236362099E-2,-4.3708471760797403E-2,451.98060000000032,-36.470211981584065,415.51038801841628,"no",5500,642.39,3030.15,null,9167.9645,48107.964500000002,91.679645000000008,0,2192.2295372861308,-660,20.775519400920814,1553.0050566870516,-1137.4946686686353,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","40 fc","no-day","yes-occ","red-epd","base-eff",181.94,112.18,9.1669692329549995E-2,0.200228581476109,-0.16465946843853799,1265.3790000000006,-137.39134489974413,1127.9876551002565,"no",5500,642.39,3030.15,null,7737.9645,15437.9645,77.379644999999996,0,1850.2901418708054,-660,56.399382755012823,1246.6895246258182,-118.70186952556173,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","40 fc","no-day","yes-occ","red-epd","high-eff",180.63,112.18,9.5726711604338002E-2,0.20598707635500499,-0.16465946843853799,1301.7708000000005,-137.39134489974413,1164.3794551002563,"no",5500,642.39,3030.15,null,9992.9645,48932.964500000002,99.929645000000008,0,2389.5022654103573,-660,58.218972755012821,1787.7212381653701,-623.34178306511376,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","40 fc","yes-day","no-occ","base-epd","base-eff",204.6,103.14,4.9631395330481401E-2,0.100619807464064,-7.0805647840531602E-2,635.88420000000042,-59.080010858528063,576.80418914147231,"no",5500,642.39,3030.15,null,7957.9645,31387.964500000002,79.579644999999999,0,1902.8962027039324,-660,28.840209457073616,1271.736412161006,-694.93222301953369,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","40 fc","yes-day","no-occ","base-epd","high-eff",203.18,103.14,5.3988349882393899E-2,0.10686184008088299,-7.0805647840531602E-2,675.33180000000016,-59.080010858528063,616.25178914147205,"no",5500,642.39,3030.15,null,10212.9645,64882.964500000002,102.129645,0,2442.1083262434845,-660,30.812589457073603,1812.920915700558,-1196.669126559086,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","40 fc","yes-day","no-occ","red-epd","base-eff",173.88,114.75,0.108623928520688,0.23565871027297899,-0.191341362126246,1489.2858000000006,-159.65463344907204,1329.6311665509286,"no",5500,642.39,3030.15,null,8782.9645,32212.964500000002,87.829644999999999,0,2100.1689308281584,-660,66.481558327546438,1506.6504891557049,-177.01932260477633,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","40 fc","yes-day","no-occ","red-epd","high-eff",172.64,114.75,0.112459942854437,0.241109499318651,-0.191341362126246,1523.7330000000009,-159.65463344907204,1364.0783665509289,"no",5500,642.39,3030.15,null,11037.9645,65707.964500000002,110.379645,0,2639.3810543677109,-660,68.203918327546447,2047.5849726952574,-683.50660614432854,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","40 fc","yes-day","yes-occ","base-epd","base-eff",194.5,107.55,6.7169716008650904E-2,0.14501736340058899,-0.116590531561462,916.46220000000039,-97.282774478192025,819.17942552180841,"no",5500,642.39,3030.15,null,9937.9645,33367.964500000002,99.379644999999996,0,2376.3507502020757,-660,40.958971276090423,1757.309721478166,-938.1302959563576,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","40 fc","yes-day","yes-occ","base-epd","high-eff",193.18,107.55,7.1258307417873007E-2,0.15081981625565999,-0.116590531561462,953.13180000000011,-97.282774478192025,855.84902552180813,"no",5500,642.39,3030.15,null,12192.9645,66862.964500000002,121.92964500000001,0,2915.5628737416273,-660,42.792451276090411,2298.3553250177179,-1442.5062994959098,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","40 fc","yes-day","yes-occ","red-epd","base-eff",163.78,119.45,0.12530980156913499,0.28005626620950402,-0.24013704318936899,1769.8638000000003,-200.36959694395208,1569.4942030560483,"no",5500,642.39,3030.15,null,10762.9645,34192.964500000002,107.629645,0,2573.6234783263021,-660,78.474710152802416,1992.0981884791045,-422.6039854230562,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","40 fc","yes-day","yes-occ","red-epd","high-eff",162.63,119.45,0.12886166669297699,0.28511143346960299,-0.24013704318936899,1801.8108000000004,-200.36959694395208,1601.4412030560484,"no",5500,642.39,3030.15,null,13017.9645,67687.964500000002,130.17964499999999,0,3112.8356018658537,-660,80.072060152802422,2532.9076620186561,-931.4664589626077,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","25 fc","no-day","no-occ","base-epd","base-eff",212.71,100.53,3.2614014870475397E-2,6.4969888786320304E-2,-4.3708471760797403E-2,410.58840000000009,-36.470211981584065,374.11818801841605,"no",5500,642.39,3030.15,null,5647.9645,62627.964500000002,56.479645000000005,0,1350.532563956099,-1045,18.705909400920802,324.23847335701981,49.879714661396235,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","25 fc","no-day","no-occ","base-epd","high-eff",211.22,100.53,3.7223546497861103E-2,7.1519627236362099E-2,-4.3708471760797403E-2,451.98060000000032,-36.470211981584065,415.51038801841628,"no",5500,642.39,3030.15,null,7902.9645,96122.964500000002,79.029645000000002,0,1889.7446874956504,-1045,20.775519400920814,865.52020689657115,-450.00981887815487,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","25 fc","no-day","no-occ","red-epd","base-eff",181.94,112.18,9.1669692329549995E-2,0.200228581476109,-0.16465946843853799,1265.3790000000006,-137.39134489974413,1127.9876551002565,"no",5500,642.39,3030.15,null,6472.9645,63452.964500000002,64.729645000000005,0,1547.8052920803252,-1045,56.399382755012823,559.20467483533798,568.78298026491848,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","25 fc","no-day","no-occ","red-epd","high-eff",180.63,112.18,9.5726711604338002E-2,0.20598707635500499,-0.16465946843853799,1301.7708000000005,-137.39134489974413,1164.3794551002563,"no",5500,642.39,3030.15,null,8727.9645,96947.964500000002,87.279645000000002,0,2087.0174156198768,-1045,58.218972755012821,1100.2363883748897,64.14306672536668,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","25 fc","no-day","yes-occ","base-epd","base-eff",201.14,105.36,5.34200514625792E-2,0.115829267220537,-9.3853820598006704E-2,732.00300000000072,-78.311334041216057,653.69166595878471,"no",5500,642.39,3030.15,null,7627.9645,64607.964500000002,76.279645000000002,0,1823.9871114542418,-1045,32.684583297939234,811.671694752181,-157.98002879339629,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","25 fc","no-day","yes-occ","base-epd","high-eff",199.76,105.36,5.7713861745623402E-2,0.121895467932656,-9.3853820598006704E-2,770.33940000000064,-78.311334041216057,692.02806595878462,"no",5500,642.39,3030.15,null,9882.9645,98102.964500000002,98.829644999999999,0,2363.1992349937941,-1045,34.601403297939235,1352.8006382917333,-660.7725723329487,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","25 fc","no-day","yes-occ","red-epd","base-eff",170.37,117.19,0.111907430501839,0.25108795991032601,-0.216673588039867,1586.7936000000002,-180.79176343364801,1406.0018365663523,"no",5500,642.39,3030.15,null,8452.9645,65432.964500000002,84.529645000000002,0,2021.2598395784682,-1045,70.300091828317619,1046.5599314067858,359.44190515956643,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","25 fc","no-day","yes-occ","red-epd","high-eff",169.16,117.19,0.115664514499503,0.256406875027474,-0.216673588039867,1620.4074000000005,-180.79176343364801,1439.6156365663526,"no",5500,642.39,3030.15,null,10707.9645,98927.964500000002,107.079645,0,2560.4719631180201,-1045,71.980781828317632,1587.4527449463378,-147.83710837998524,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","25 fc","yes-day","no-occ","base-epd","base-eff",194.5,107.55,6.7169716008650904E-2,0.14501736340058899,-0.116590531561462,916.46220000000039,-97.282774478192025,819.17942552180841,"no",5500,642.39,3030.15,null,8672.9645,81382.964500000002,86.729645000000005,0,2073.8659004115952,-1045,40.958971276090423,1069.8248716876856,-250.64544616587716,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","25 fc","yes-day","no-occ","base-epd","high-eff",193.18,107.55,7.1258307417873007E-2,0.15081981625565999,-0.116590531561462,953.13180000000011,-97.282774478192025,855.84902552180813,"no",5500,642.39,3030.15,null,10927.9645,114877.9645,109.279645,0,2613.0780239511473,-1045,42.792451276090411,1610.8704752272376,-755.02144970542952,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","25 fc","yes-day","no-occ","red-epd","base-eff",163.78,119.45,0.12530980156913499,0.28005626620950402,-0.24013704318936899,1769.8638000000003,-200.36959694395208,1569.4942030560483,"no",5500,642.39,3030.15,null,9497.9645,82207.964500000002,94.979645000000005,0,2271.1386285358212,-1045,78.474710152802416,1304.6133386886236,264.88086436742469,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","25 fc","yes-day","no-occ","red-epd","high-eff",162.63,119.45,0.12886166669297699,0.28511143346960299,-0.24013704318936899,1801.8108000000004,-200.36959694395208,1601.4412030560484,"no",5500,642.39,3030.15,null,11752.9645,115702.9645,117.529645,0,2810.3507520753733,-1045,80.072060152802422,1845.4228122281756,-243.98160917212726,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","25 fc","yes-day","yes-occ","base-epd","base-eff",186.59,111.01,8.0919380554722406E-2,0.179788122554838,-0.15251245847176101,1136.2020000000002,-127.25591781697609,1008.9460821830241,"no",5500,642.39,3030.15,null,10652.9645,83362.964500000002,106.529645,0,2547.3204479097385,-1045,50.447304109151212,1552.7677520188897,-543.82166983586558,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","25 fc","yes-day","yes-occ","base-epd","high-eff",185.34,111.01,8.4786967022905599E-2,0.18528286957668499,-0.15251245847176101,1170.9270000000004,-127.25591781697609,1043.6710821830243,"no",5500,642.39,3030.15,null,12907.9645,116857.9645,129.079645,0,3086.5325714492897,-1045,52.183554109151217,2093.716125558441,-1050.0450433754168,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","25 fc","yes-day","yes-occ","red-epd","base-eff",155.87,123.15,0.138317520956004,0.31482702536375201,-0.27855066445182702,1989.6036000000004,-232.4218022484321,1757.1817977515682,"no",5500,642.39,3030.15,null,11477.9645,84187.964500000002,114.779645,0,2744.5931760339645,-1045,87.859089887578421,1787.4522659215429,-30.27046816997472,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","base-win","red-inf","25 fc","yes-day","yes-occ","red-epd","high-eff",154.78,123.15,0.14167995327324101,0.31961844476680301,-0.27855066445182702,2019.8838000000005,-232.4218022484321,1787.4619977515683,"no",5500,642.39,3030.15,null,13732.9645,117682.9645,137.329645,0,3283.8052995735165,-1045,89.373099887578419,2328.1783994610951,-540.71640170952674,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","base-lpd","no-day","no-occ","base-epd","base-eff",224.28,94.42,1.5738709015423E-2,1.41105103521034E-2,1.97259136212624E-2,89.173800000000227,16.459240561759923,105.63304056176015,"no",5500,642.39,3030.15,null,4612.3602000000001,27622.77,46.123601999999998,0,1102.9004602976993,0,5.2816520280880077,1108.1821123257873,-1002.5490717640272,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","base-lpd","no-day","no-occ","base-epd","high-eff",222.78,94.42,2.0395598844459999E-2,2.0704206778320002E-2,1.97259136212624E-2,130.84380000000024,16.459240561759923,147.30304056176016,"no",5500,642.39,3030.15,null,6867.3602000000001,61117.770000000004,68.673602000000002,0,1642.1125838372509,0,7.3651520280880085,1649.4777358653389,-1502.1746953035788,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","base-lpd","no-day","no-occ","red-epd","base-eff",193.5,105.74,7.5852052978041706E-2,0.14941316101806701,-9.7799003322259201E-2,944.24220000000025,-81.603182153568014,862.63901784643224,"no",5500,642.39,3030.15,null,5437.3602000000001,28447.77,54.373602000000005,0,1300.1731884219255,0,43.131950892321612,1343.3051393142471,-480.66612146781483,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","base-lpd","no-day","no-occ","red-epd","high-eff",192.18,105.74,7.9956430454480795E-2,0.15521561387313701,-9.7799003322259201E-2,980.91180000000008,-81.603182153568014,899.30861784643207,"no",5500,642.39,3030.15,null,7692.3602000000001,61942.770000000004,76.923602000000002,0,1839.3853119614773,0,44.965430892321606,1884.3507428537989,-985.04212500736685,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","base-lpd","no-day","yes-occ","base-epd","base-eff",209.59,100.32,4.2890744628790702E-2,7.8684777352850704E-2,-4.1528239202657802E-2,497.26200000000017,-34.6510327616,462.61096723840018,"no",5500,642.39,3030.15,null,6592.3602000000001,29602.77,65.923602000000002,0,1576.3550077958423,0,23.13054836192001,1599.4855561577624,-1136.8745889193622,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","base-lpd","no-day","yes-occ","base-epd","high-eff",208.23,100.32,4.7089838508532399E-2,8.4663062112620396E-2,-4.1528239202657802E-2,535.04280000000051,-34.6510327616,500.39176723840052,"no",5500,642.39,3030.15,null,8847.3601999999992,63097.770000000004,88.473602,0,2115.5671313353937,0,25.019588361920029,2140.5867196973136,-1640.1949524589131,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","base-lpd","no-day","yes-occ","red-epd","base-eff",178.82,112.01,0.101835919617346,0.213943470042639,-0.16289451827242499,1352.0526000000007,-135.91867600737609,1216.1339239926247,"no",5500,642.39,3030.15,null,7417.3602000000001,30427.77,74.173602000000002,0,1773.6277359200687,0,60.806696199631233,1834.4344321197,-618.30050812707532,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","base-lpd","no-day","yes-occ","red-epd","high-eff",177.63,112.01,0.10552985934614099,0.21917446920743799,-0.16289451827242499,1385.1108000000004,-135.91867600737609,1249.1921239926244,"no",5500,642.39,3030.15,null,9672.3601999999992,63922.770000000004,96.723602,0,2312.8398594596201,0,62.459606199631224,2375.2994656592514,-1126.107341666627,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","base-lpd","yes-day","no-occ","base-epd","base-eff",201.51,102.94,5.9766050483843002E-2,0.114202822102071,-6.8729235880398698E-2,721.72440000000051,-57.34745922044803,664.37694077955246,"no",5500,642.39,3030.15,null,7637.360200000001,46377.770000000004,76.373602000000005,0,1826.2337967531957,0,33.218847038977621,1859.4526437921734,-1195.075703012621,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","base-lpd","yes-day","no-occ","base-epd","high-eff",200.22,102.94,6.3744139422545698E-2,0.119873401028617,-6.8729235880398698E-2,757.56060000000036,-57.34745922044803,700.2131407795523,"no",5500,642.39,3030.15,null,9892.360200000001,79872.77,98.923602000000017,0,2365.4459202927478,0,35.010657038977619,2400.4565773317254,-1700.2434365521731,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","base-lpd","yes-day","no-occ","red-epd","base-eff",170.8,114.69,0.118332359859188,0.24919776693480999,-0.190718438538206,1574.8482000000001,-159.13486795764803,1415.713332042352,"no",5500,642.39,3030.15,null,8462.360200000001,47202.770000000004,84.623602000000005,0,2023.506524877422,0,70.785666602117601,2094.2921914795397,-678.5788594371877,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","base-lpd","yes-day","no-occ","red-epd","high-eff",169.68,114.69,0.12178950857972699,0.25412106026638498,-0.190718438538206,1605.9618,-159.13486795764803,1446.8269320423519,"no",5500,642.39,3030.15,null,10717.360200000001,80697.77,107.17360200000002,0,2562.7186484169742,0,72.341346602117596,2635.0599950190917,-1188.2330629767398,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","base-lpd","yes-day","yes-occ","base-epd","base-eff",191.4,107.45,7.7067580153756393E-2,0.15864433601476999,-0.115552325581395,1002.5802000000002,-96.416498659152083,906.16370134084809,"no",5500,642.39,3030.15,null,9617.360200000001,48357.770000000004,96.173602000000017,0,2299.688344251339,0,45.308185067042409,2344.9965293183814,-1438.8328279775333,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","base-lpd","yes-day","yes-occ","base-epd","high-eff",190.2,107.45,8.0761519882551799E-2,0.163919293155743,-0.115552325581395,1035.9162000000006,-96.416498659152083,939.49970134084845,"no",5500,642.39,3030.15,null,11872.360200000001,81852.77,118.72360200000001,0,2838.9004677908906,0,46.974985067042425,2885.8754528579329,-1946.3757515170846,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","base-lpd","yes-day","yes-occ","red-epd","base-eff",160.69,119.45,0.13487615830268199,0.29363928084751001,-0.24013704318936899,1855.7040000000006,-200.36959694395208,1655.3344030560486,"no",5500,642.39,3030.15,null,10442.360200000001,49182.770000000004,104.42360200000002,0,2496.9610723755654,0,82.766720152802435,2579.7277925283679,-924.39338947231931,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","base-lpd","yes-day","yes-occ","red-epd","high-eff",159.65,119.45,0.138064943880531,0.298210910369687,-0.24013704318936899,1884.5952000000002,-200.36959694395208,1684.2256030560482,"no",5500,642.39,3030.15,null,12697.360200000001,82677.77,126.97360200000001,0,3036.173195915117,0,84.211280152802416,3120.3844760679194,-1436.1588730118713,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","40 fc","no-day","no-occ","base-epd","base-eff",224.28,94.42,1.5738709015423E-2,1.41105103521034E-2,1.97259136212624E-2,89.173800000000227,16.459240561759923,105.63304056176015,"no",5500,642.39,3030.15,null,8242.3601999999992,38952.770000000004,82.423601999999988,0,1970.9004640442949,-660,5.2816520280880077,1316.182116072383,-1210.5490755106227,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","40 fc","no-day","no-occ","base-epd","high-eff",222.78,94.42,2.0395598844459999E-2,2.0704206778320002E-2,1.97259136212624E-2,130.84380000000024,16.459240561759923,147.30304056176016,"no",5500,642.39,3030.15,null,10497.360199999999,72447.77,104.973602,0,2510.1125875838466,-660,7.3651520280880085,1857.4777396119346,-1710.1746990501745,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","40 fc","no-day","no-occ","red-epd","base-eff",193.5,105.74,7.5852052978041706E-2,0.14941316101806701,-9.7799003322259201E-2,944.24220000000025,-81.603182153568014,862.63901784643224,"no",5500,642.39,3030.15,null,9067.3601999999992,39777.770000000004,90.673601999999988,0,2168.1731921685209,-660,43.131950892321612,1551.3051430608425,-688.66612521441027,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","40 fc","no-day","no-occ","red-epd","high-eff",192.18,105.74,7.9956430454480795E-2,0.15521561387313701,-9.7799003322259201E-2,980.91180000000008,-81.603182153568014,899.30861784643207,"no",5500,642.39,3030.15,null,11322.360199999999,73272.77,113.223602,0,2707.385315708073,-660,44.965430892321606,2092.3507466003948,-1193.0421287539627,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","40 fc","no-day","yes-occ","base-epd","base-eff",209.59,100.32,4.2890744628790702E-2,7.8684777352850704E-2,-4.1528239202657802E-2,497.26200000000017,-34.6510327616,462.61096723840018,"no",5500,642.39,3030.15,null,10222.360199999999,40932.770000000004,102.223602,0,2444.3550115424378,-660,23.13054836192001,1807.4855599043578,-1344.8745926659576,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","40 fc","no-day","yes-occ","base-epd","high-eff",208.23,100.32,4.7089838508532399E-2,8.4663062112620396E-2,-4.1528239202657802E-2,535.04280000000051,-34.6510327616,500.39176723840052,"no",5500,642.39,3030.15,null,12477.360199999999,74427.77,124.773602,0,2983.5671350819894,-660,25.019588361920029,2348.5867234439092,-1848.1949562055088,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","40 fc","no-day","yes-occ","red-epd","base-eff",178.82,112.01,0.101835919617346,0.213943470042639,-0.16289451827242499,1352.0526000000007,-135.91867600737609,1216.1339239926247,"no",5500,642.39,3030.15,null,11047.360199999999,41757.770000000004,110.473602,0,2641.6277396666642,-660,60.806696199631233,2042.4344358662954,-826.30051187367076,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","40 fc","no-day","yes-occ","red-epd","high-eff",177.63,112.01,0.10552985934614099,0.21917446920743799,-0.16289451827242499,1385.1108000000004,-135.91867600737609,1249.1921239926244,"no",5500,642.39,3030.15,null,13302.360199999999,75252.77,133.02360199999998,0,3180.8398632062158,-660,62.459606199631224,2583.299469405847,-1334.1073454132227,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","40 fc","yes-day","no-occ","base-epd","base-eff",201.51,102.94,5.9766050483843002E-2,0.114202822102071,-6.8729235880398698E-2,721.72440000000051,-57.34745922044803,664.37694077955246,"no",5500,642.39,3030.15,null,11267.360199999999,57707.770000000004,112.67360199999999,0,2694.2338004997914,-660,33.218847038977621,2067.4526475387688,-1403.0757067592162,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","40 fc","yes-day","no-occ","base-epd","high-eff",200.22,102.94,6.3744139422545698E-2,0.119873401028617,-6.8729235880398698E-2,757.56060000000036,-57.34745922044803,700.2131407795523,"no",5500,642.39,3030.15,null,13522.360199999999,91202.77,135.223602,0,3233.4459240393426,-660,35.010657038977619,2608.4565810783201,-1908.2434402987678,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","40 fc","yes-day","no-occ","red-epd","base-eff",170.8,114.69,0.118332359859188,0.24919776693480999,-0.190718438538206,1574.8482000000001,-159.13486795764803,1415.713332042352,"no",5500,642.39,3030.15,null,12092.360199999999,58532.770000000004,120.92360199999999,0,2891.5065286240174,-660,70.785666602117601,2302.2921952261349,-886.57886318378291,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","40 fc","yes-day","no-occ","red-epd","high-eff",169.68,114.69,0.12178950857972699,0.25412106026638498,-0.190718438538206,1605.9618,-159.13486795764803,1446.8269320423519,"no",5500,642.39,3030.15,null,14347.360199999999,92027.77,143.473602,0,3430.7186521635695,-660,72.341346602117596,2843.0599987656869,-1396.233066723335,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","40 fc","yes-day","yes-occ","base-epd","base-eff",191.4,107.45,7.7067580153756393E-2,0.15864433601476999,-0.115552325581395,1002.5802000000002,-96.416498659152083,906.16370134084809,"no",5500,642.39,3030.15,null,13247.360199999999,59687.770000000004,132.473602,0,3167.6883479979338,-660,45.308185067042409,2552.9965330649761,-1646.832831724128,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","40 fc","yes-day","yes-occ","base-epd","high-eff",190.2,107.45,8.0761519882551799E-2,0.163919293155743,-0.115552325581395,1035.9162000000006,-96.416498659152083,939.49970134084845,"no",5500,642.39,3030.15,null,15502.360199999999,93182.77,155.02360199999998,0,3706.9004715374858,-660,46.974985067042425,3093.8754566045282,-2154.3757552636798,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","40 fc","yes-day","yes-occ","red-epd","base-eff",160.69,119.45,0.13487615830268199,0.29363928084751001,-0.24013704318936899,1855.7040000000006,-200.36959694395208,1655.3344030560486,"no",5500,642.39,3030.15,null,14072.360199999999,60512.770000000004,140.723602,0,3364.9610761221602,-660,82.766720152802435,2787.7277962749627,-1132.3933932189141,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","40 fc","yes-day","yes-occ","red-epd","high-eff",159.65,119.45,0.138064943880531,0.298210910369687,-0.24013704318936899,1884.5952000000002,-200.36959694395208,1684.2256030560482,"no",5500,642.39,3030.15,null,16327.360199999999,94007.77,163.27360199999998,0,3904.1731996617127,-660,84.211280152802416,3328.3844798145151,-1644.1588767584669,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","25 fc","no-day","no-occ","base-epd","base-eff",209.59,100.32,4.2890744628790702E-2,7.8684777352850704E-2,-4.1528239202657802E-2,497.26200000000017,-34.6510327616,462.61096723840018,{"$f":"IF(P135>0.2,\"yes\",\"no\")","v":"no"},{"$f":"IF(B135=\"5500 ft2\",5500,IF(B135=\"10000 ft2\",10000,25000))","v":5500},{"$f":"IF(B135=\"5500 ft2\",IF(D135=\"stand-alone\",642.39,IF(D135=\"ad-e&flr\",522.37,402.25)),IF(B135=\"10000 ft2\",IF(D135=\"stand-alone\",866.06,IF(D135=\"ad-e&flr\",704.17,542.29)),IF(B135=\"25000 ft2\",IF(D135=\"stand-alone\",1369.38,IF(D135=\"ad-e&flr\",1113.42,857.45)))))","v":642.39},{"$f":"IF(B135=\"5500 ft2\",IF(D135=\"stand-alone\",3030.15,IF(D135=\"ad-e&flr\",2424.14,1818.13)),IF(B135=\"10000 ft2\",IF(D135=\"stand-alone\",4085.12,IF(D135=\"ad-e&flr\",3268.14,2451.05)),IF(B135=\"25000 ft2\",IF(D135=\"stand-alone\",6459.2,IF(D135=\"ad-e&flr\",5167.32,3875.54)))))","v":3030.15},null,{"$f":"SUM(IF(F135=\"eff-roof\",W135*IF(AND(W$4=\"no\",X$4=\"no\"),$C$4,$C$3)),IF(G135=\"eff-win\",X135*IF(W$4=\"no\",$D$4,$D$3),0),IF(H135=\"red-inf\",Y135*IF(W$4=\"no\",$F$4,$F$3),0),IF(I135=\"25 fc\",W135*IF(W$4=\"no\",$H$4,$H$3),0),IF(I135=\"40 fc\",W135*IF(W$4=\"no\",$G$4,$G$3),0),IF(J135=\"yes-day\",W135*IF(W$4=\"no\",$I$4,$I$3),0),IF(K135=\"yes-occ\",W135*IF(W$4=\"no\",$J$4,$J$3),0),IF(L135=\"red-epd\",W135*IF(W$4=\"no\",$K$4,$K$3),0),IF(AND(M135=\"high-eff\",C135=\"psz-ac\"),W135*IF(AND(W$4=\"no\",Y$4=\"no\"),$L$4,$L$3),0),IF(AND(M135=\"high-eff\",C135=\"ptac\"),W135*IF(AND(W$4=\"no\",Y$4=\"no\"),$M$4,$M$3),0),IF(AND(M135=\"high-eff\",C135=\"pthp\"),W135*IF(AND(W$4=\"no\",Y$4=\"no\"),$N$4,$N$3),0))","v":8957.3601999999992},{"$f":"SUM(IF(F135=\"eff-roof\",W135*$C$4),IF(G135=\"eff-win\",X135*$D$4,0),IF(H135=\"red-inf\",Y135*$F$4,0),IF(I135=\"25 fc\",W135*$H$4,0),IF(I135=\"40 fc\",W135*$G$4,0),IF(J135=\"yes-day\",W135*$I$4,0),IF(K135=\"yes-occ\",W135*$J$4,0),IF(L135=\"red-epd\",W135*$K$4,0),IF(AND(M135=\"high-eff\",C135=\"psz-ac\"),W135*$L$4,0),IF(AND(M135=\"high-eff\",C135=\"ptac\"),W135*$M$4,0),IF(AND(M135=\"high-eff\",C135=\"pthp\"),W135*$N$4,0))","v":88947.77},89.573601999999994,0,{"$f":"-PMT($AE$3,$AE$4,AA135+AC135-AD135)","v":2141.8701617519578},{"$f":"SUM(IF(F135=\"eff-roof\",($C$5*W135),0),IF(G135=\"eff-win\",($D$5*X135),0),IF(H135=\"red-inf\",$F$5*(Y135-X135),0),IF(I135=\"25 fc\",($H$5*W135),0),IF(I135=\"40 fc\",($G$5*W135),0),IF(J135=\"yes-day\",($I$5*W135),0),IF(K135=\"yes-occ\",($J$5*W135),0),IF(L135=\"red-epd\",($K$5*W135),0),IF(M135=\"high-eff\",($L$5*W135),0))","v":-1045},{"$f":"0.05*U135","v":23.13054836192001},1120.0007101138779,{"$f":"U135-AH135","v":-657.38974287547762},null,null,null,"New Construction",{"$f":"IF(B135=\"5500 ft2\",\"5,500 SF\",IF(B135=\"10000 ft2\",\"10,000 SF\",IF(B135=\"25000 ft2\",\"25,000 SF\")))","v":"5,500 SF"},"Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration",{"$f":"IF(I135=\"base-lpd\",\"Baseline Lighting Levels\",IF(I135=\"40 fc\",\"Reduce Lighting Levels to 40 fc\",IF(I135=\"25 fc\",\"Reduce Lighting Levels to 25 fc\")))","v":"Reduce Lighting Levels to 25 fc"},"No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","25 fc","no-day","no-occ","base-epd","high-eff",208.23,100.32,4.7089838508532399E-2,8.4663062112620396E-2,-4.1528239202657802E-2,{"$f":"277.8*($N$7-N136)*$S$3","v":535.04280000000051},{"$f":"277.78*($O$7-O136)*$S$4","v":-34.6510327616},{"$f":"SUM(S136:T136)","v":500.39176723840052},"no",5500,642.39,3030.15,null,11212.360199999999,122442.77,{"$f":"MIN(0.01*AA136,500)","v":112.12360199999999},{"$f":"IF(V136=\"yes\",0,0)","v":0},2681.0822852915089,-1045,25.019588361920029,{"$f":"SUM(AE136:AG136)","v":1661.101873653429},-1160.7101064150286,null,null,null,"New Construction","5,500 SF",{"$f":"IF(C136=\"psz-ac\",\"Packaged Air Conditioner\",IF(C136=\"ptac\",\"Split System Air Conditioner\",IF(C136=\"pthp\",\"Split System Heat Pump\")))","v":"Packaged Air Conditioner"},{"$f":"IF(D136=\"stand-alone\",\"Stand Alone\",IF(D136=\"ad-e&flr\",\"Above Ground, 1 Side Attached\",IF(D136=\"ad-e&w&flr\",\"Above Ground, 2 Sides Attached\")))","v":"Stand Alone"},{"$f":"IF(F136=\"base-roof\",\"Baseline Roof Insulation\",IF(F136=\"eff-roof\",\"Increased Roof Insulation\"))","v":"Baseline Roof Insulation"},{"$f":"IF(G136=\"base-win\",\"Baseline Windows\",IF(G136=\"eff-win\",\"Replace Windows\"))","v":"Replace Windows"},{"$f":"IF(H136=\"base-inf\",\"Baseline Infiltration\",IF(H136=\"red-inf\",\"Reduce Infiltration\"))","v":"Baseline Infiltration"},"Reduce Lighting Levels to 25 fc",{"$f":"IF(J136=\"no-day\",\"No Daylighting Sensors\",IF(J136=\"yes-day\",\"Install Daylighting Sensors\"))","v":"No Daylighting Sensors"},{"$f":"IF(K136=\"no-occ\",\"No Occupancy Sensors\",IF(K136=\"yes-occ\",\"Install Occupancy Sensors\"))","v":"No Occupancy Sensors"},{"$f":"IF(L136=\"base-epd\",\"No Plug Load Control\",IF(L136=\"red-epd\",\"Install Plug Load Controls\"))","v":"No Plug Load Control"},{"$f":"IF(M136=\"base-eff\",\"Baseline HVAC Equipment\",IF(M136=\"high-eff\",\"Install High Efficiency HVAC Equipment\"))","v":"Install High Efficiency HVAC Equipment"}]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","25 fc","no-day","no-occ","red-epd","base-eff",178.82,112.01,0.101835919617346,0.213943470042639,-0.16289451827242499,1352.0526000000007,-135.91867600737609,1216.1339239926247,"no",5500,642.39,3030.15,null,9782.3601999999992,89772.77,97.823601999999994,0,2339.1428898761837,-1045,60.806696199631233,1354.949586075815,-138.81566208319032,null,null,null,{"$f":"IF(A137=\"new90.1-2004\",\"New Construction\",IF(A137=\"post1980\",\"Post 1980 Construction\",IF(A137=\"pre1980\",\"Pre 1980 Construction\")))","v":"New Construction"},"5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","25 fc","no-day","no-occ","red-epd","high-eff",177.63,112.01,0.10552985934614099,0.21917446920743799,-0.16289451827242499,1385.1108000000004,-135.91867600737609,1249.1921239926244,"no",5500,642.39,3030.15,null,12037.360199999999,123267.77,120.37360199999999,0,2878.3550134157354,-1045,62.459606199631224,1895.8146196153666,-646.62249562274224,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","25 fc","no-day","yes-occ","base-epd","base-eff",198.06,105.12,6.3665209086460395E-2,0.12936832388236799,-9.1362126245847303E-2,817.5654000000003,-76.2322720755201,741.33312792448021,"no",5500,642.39,3030.15,null,10937.360199999999,90927.77,109.37360199999999,0,2615.3247092501006,-1045,37.066656396224012,1607.3913656463246,-866.05823772184442,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","25 fc","no-day","yes-occ","base-epd","high-eff",196.8,105.12,6.7580153756294795E-2,0.13490702888039,-9.1362126245847303E-2,852.56819999999993,-76.2322720755201,776.33592792447985,"no",5500,642.39,3030.15,null,13192.360199999999,124422.77,131.92360199999999,0,3154.5368327896522,-1045,38.816796396223992,2148.3536291858763,-1372.0177012613965,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","25 fc","no-day","yes-occ","red-epd","base-eff",167.29,117.06,0.12183686678137901,0.26462701657215698,-0.21532392026578101,1672.3560000000007,-179.66560486889608,1492.6903951311047,"no",5500,642.39,3030.15,null,11762.360199999999,91752.77,117.62360199999999,0,2812.5974373743265,-1045,74.634519756555235,1842.2319571308817,-349.54156199977706,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","25 fc","no-day","yes-occ","red-epd","high-eff",166.19,117.06,0.12521508516583299,0.269462393951382,-0.21532392026578101,1702.9140000000004,-179.66560486889608,1523.2483951311044,"no",5500,642.39,3030.15,null,14017.360199999999,125247.77,140.17360199999999,0,3351.8095609138791,-1045,76.162419756555224,2382.9719806704343,-859.72358553932986,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","25 fc","yes-day","no-occ","base-epd","base-eff",191.4,107.45,7.7067580153756393E-2,0.15864433601476999,-0.115552325581395,1002.5802000000002,-96.416498659152083,906.16370134084809,"no",5500,642.39,3030.15,null,11982.360199999999,107702.77,119.82360199999999,0,2865.2034982074538,-1045,45.308185067042409,1865.5116832744961,-959.34798193364804,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","25 fc","yes-day","no-occ","base-epd","high-eff",190.2,107.45,8.0761519882551799E-2,0.163919293155743,-0.115552325581395,1035.9162000000006,-96.416498659152083,939.49970134084845,"no",5500,642.39,3030.15,null,14237.360199999999,141197.77000000002,142.37360200000001,0,3404.4156217470054,-1045,46.974985067042425,2406.3906068140477,-1466.8909054731994,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","25 fc","yes-day","no-occ","red-epd","base-eff",160.69,119.45,0.13487615830268199,0.29363928084751001,-0.24013704318936899,1855.7040000000006,-200.36959694395208,1655.3344030560486,"no",5500,642.39,3030.15,null,12807.360199999999,108527.77,128.07360199999999,0,3062.4762263316802,-1045,82.766720152802435,2100.2429464844827,-444.90854342843409,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","25 fc","yes-day","no-occ","red-epd","high-eff",159.65,119.45,0.138064943880531,0.298210910369687,-0.24013704318936899,1884.5952000000002,-200.36959694395208,1684.2256030560482,"no",5500,642.39,3030.15,null,15062.360199999999,142022.77000000002,150.62360200000001,0,3601.6883498712318,-1045,84.211280152802416,2640.8996300240342,-956.67402696798604,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","25 fc","yes-day","yes-occ","base-epd","base-eff",183.52,110.97,9.0517309422703598E-2,0.19328322124049399,-0.152097176079734,1221.4866,-126.90940748936004,1094.5771925106399,"no",5500,642.39,3030.15,null,13962.360199999999,109682.77,139.62360200000001,0,3338.6580457055966,-1045,54.728859625531996,2348.3869053311287,-1253.8097128204888,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","25 fc","yes-day","yes-occ","base-epd","high-eff",182.39,110.97,9.4006030277676997E-2,0.19825047254824399,-0.152097176079734,1252.8780000000006,-126.90940748936004,1125.9685925106405,"no",5500,642.39,3030.15,null,16217.360199999999,143177.77000000002,162.17360199999999,0,3877.8701692451486,-1045,56.29842962553203,2889.1685988706809,-1763.2000063600403,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","25 fc","yes-day","yes-occ","red-epd","base-eff",152.80000000000001,123.2,0.147631300614078,0.32832212404940903,-0.27906976744186102,2074.8882000000003,-232.85494015795209,1842.0332598420482,"no",5500,642.39,3030.15,null,14787.360199999999,110507.77,147.87360200000001,0,3535.930773829823,-1045,92.101662992102419,2583.0324368219253,-740.99917697987712,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","25 fc","yes-day","yes-occ","red-epd","high-eff",151.83000000000001,123.2,0.150630653385322,0.33258604773836198,-0.27906976744186102,2101.8348000000001,-232.85494015795209,1868.979859842048,"no",5500,642.39,3030.15,null,17042.360199999999,144002.77000000002,170.42360199999999,0,4075.1428973693746,-1045,93.448992992102404,3123.591890361477,-1254.612030519429,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","base-lpd","no-day","no-occ","base-epd","base-eff",224.19,92.83,2.09323251298404E-2,1.45061321376764E-2,3.62333887043189E-2,91.674000000000319,30.233026084495954,121.90702608449627,"no",5500,642.39,3030.15,null,5915.3247000000001,28925.734499999999,59.153247,0,1414.4633227995398,0,6.0953513042248133,1420.5586741037646,-1298.6516480192684,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","base-lpd","no-day","no-occ","base-epd","high-eff",222.68,92.83,2.55892149588774E-2,2.11437865400677E-2,3.62333887043189E-2,133.62180000000009,30.233026084495954,163.85482608449604,"no",5500,642.39,3030.15,null,8170.3247000000001,62420.734499999999,81.703247000000005,0,1953.6754463390916,0,8.1927413042248016,1961.8681876433166,-1798.0133615588206,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","base-lpd","no-day","no-occ","red-epd","base-eff",193.42,104.13,8.1061455159676096E-2,0.149764824827465,-8.1083887043189404E-2,946.4646000000007,-67.656141467024014,878.80845853297672,"no",5500,642.39,3030.15,null,6740.3247000000001,29750.734499999999,67.403247000000007,0,1611.7360509237662,0,43.940422926648836,1655.6764738504151,-776.86801531743833,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","base-lpd","no-day","no-occ","red-epd","high-eff",192.09,104.13,8.5165832636115393E-2,0.15561123565870999,-8.1083887043189404E-2,983.41200000000026,-67.656141467024014,915.75585853297628,"no",5500,642.39,3030.15,null,8995.324700000001,63245.734499999999,89.953247000000019,0,2150.9481744633176,0,45.78779292664882,2196.7359673899664,-1280.9801088569902,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","base-lpd","no-day","yes-occ","base-epd","base-eff",209.51,98.71,4.8147505012076298E-2,7.9036441162249005E-2,-2.4813122923588001E-2,499.48440000000056,-20.703992075056004,478.78040792494454,"no",5500,642.39,3030.15,null,7895.3247000000001,30905.734499999999,78.953247000000005,0,1887.9178702976831,0,23.93902039624723,1911.8568906939304,-1433.0764827689859,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","base-lpd","no-day","yes-occ","base-epd","high-eff",208.14,98.71,5.23623849590353E-2,8.5058683898193405E-2,-2.4813122923588001E-2,537.54300000000069,-20.703992075056004,516.83900792494467,"no",5500,642.39,3030.15,null,10150.324700000001,64400.734499999999,101.50324700000002,0,2427.1299938372349,0,25.841950396247235,2452.9719442334822,-1936.1329363085374,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","base-lpd","no-day","yes-occ","red-epd","base-eff",178.75,110.33,0.107234754605585,0.21425117587586301,-0.14545265780730901,1353.9972000000005,-121.36524224750403,1232.6319577524964,"no",5500,642.39,3030.15,null,8720.324700000001,31730.734499999999,87.203247000000019,0,2085.1905984219093,0,61.631597887624821,2146.8221963095339,-914.19023855703745,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","base-lpd","no-day","yes-occ","red-epd","high-eff",177.55,110.33,0.110944480401598,0.21952613301683599,-0.14545265780730901,1387.3332,-121.36524224750403,1265.967957752496,"no",5500,642.39,3030.15,null,10975.324700000001,65225.734499999999,109.75324700000002,0,2624.4027219614613,0,63.298397887624802,2687.7011198490864,-1421.7331620965904,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","base-lpd","yes-day","no-occ","base-epd","base-eff",201.41,101.36,6.4959666598260302E-2,0.11464240186381799,-5.2325581395348902E-2,724.50240000000042,-43.66030127961605,680.84209872038434,"no",5500,642.39,3030.15,null,8940.324700000001,47680.734499999999,89.403247000000007,0,2137.796659255036,0,34.042104936019221,2171.8387641910554,-1490.9966654706709,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","base-lpd","yes-day","no-occ","base-epd","high-eff",200.12,101.36,6.8953541604180296E-2,0.120312980790364,-5.2325581395348902E-2,760.33860000000016,-43.66030127961605,716.67829872038408,"no",5500,642.39,3030.15,null,11195.324700000001,81175.734499999991,111.95324700000002,0,2677.0087827945881,0,35.833914936019205,2712.8426977306071,-1996.164399010223,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","base-lpd","yes-day","no-occ","red-epd","base-eff",170.71,112.96,0.123920627654033,0.249593388720383,-0.172757475083056,1577.3484000000001,-144.14829628825598,1433.2001037117441,"no",5500,642.39,3030.15,null,9765.324700000001,48505.734499999999,97.653247000000007,0,2335.0693873792629,0,71.66000518558721,2406.7293925648501,-973.52928885310598,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","base-lpd","yes-day","no-occ","red-epd","high-eff",169.59,112.96,0.12739356244178901,0.25451668205195799,-0.172757475083056,1608.4620000000004,-144.14829628825598,1464.3137037117444,"no",5500,642.39,3030.15,null,12020.324700000001,82000.734499999991,120.20324700000002,0,2874.2815109188141,0,73.215685185587219,2947.4971961044012,-1483.1834923926567,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","base-lpd","yes-day","yes-occ","base-epd","base-eff",191.32,105.79,8.2450629074778597E-2,0.15899599982416801,-9.83181063122925E-2,1004.8026000000006,-82.036320063088112,922.7662799369125,"no",5500,642.39,3030.15,null,10920.324700000001,49660.734499999999,109.20324700000002,0,2611.2512067531793,0,46.138313996845625,2657.389520750025,-1734.6232408131125,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","base-lpd","yes-day","yes-occ","base-epd","high-eff",190.12,105.79,8.6176140938008197E-2,0.16427095696514099,-9.83181063122925E-2,1038.1386000000002,-82.036320063088112,956.10227993691205,"no",5500,642.39,3030.15,null,13175.324700000001,83155.734499999991,131.75324700000002,0,3150.4633302927314,0,47.805113996845606,3198.268444289577,-2242.166164352665,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","base-lpd","yes-day","yes-occ","red-epd","base-eff",160.61000000000001,117.68,0.14055914250082899,0.293990944656908,-0.22176079734219301,1857.9264000000001,-185.03651494694412,1672.8898850530559,"no",5500,642.39,3030.15,null,11745.324700000001,50485.734499999999,117.45324700000002,0,2808.5239348774057,0,83.644494252652805,2892.1684291300585,-1219.2785440770026,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","base-lpd","yes-day","yes-occ","red-epd","high-eff",159.58000000000001,117.68,0.14376371414589501,0.29851861620290998,-0.22176079734219301,1886.5398000000002,-185.03651494694412,1701.5032850530561,"no",5500,642.39,3030.15,null,14000.324700000001,83980.734499999991,140.00324700000002,0,3347.7360584169573,0,85.075164252652812,3432.8112226696103,-1731.3079376165542,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","40 fc","no-day","no-occ","base-epd","base-eff",224.19,92.83,2.09323251298404E-2,1.45061321376764E-2,3.62333887043189E-2,91.674000000000319,30.233026084495954,121.90702608449627,"no",5500,642.39,3030.15,null,9545.324700000001,40255.734499999999,95.453247000000019,0,2282.4633265461352,-660,6.0953513042248133,1628.55867785036,-1506.6516517658638,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","40 fc","no-day","no-occ","base-epd","high-eff",222.68,92.83,2.55892149588774E-2,2.11437865400677E-2,3.62333887043189E-2,133.62180000000009,30.233026084495954,163.85482608449604,"no",5500,642.39,3030.15,null,11800.324700000001,73750.734499999991,118.00324700000002,0,2821.6754500856878,-660,8.1927413042248016,2169.8681913899127,-2006.0133653054168,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","40 fc","no-day","no-occ","red-epd","base-eff",193.42,104.13,8.1061455159676096E-2,0.149764824827465,-8.1083887043189404E-2,946.4646000000007,-67.656141467024014,878.80845853297672,"no",5500,642.39,3030.15,null,10370.324700000001,41080.734499999999,103.70324700000002,0,2479.7360546703621,-660,43.940422926648836,1863.6764775970109,-984.86801906403423,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","40 fc","no-day","no-occ","red-epd","high-eff",192.09,104.13,8.5165832636115393E-2,0.15561123565870999,-8.1083887043189404E-2,983.41200000000026,-67.656141467024014,915.75585853297628,"no",5500,642.39,3030.15,null,12625.324700000001,74575.734499999991,126.25324700000002,0,3018.9481782099137,-660,45.78779292664882,2404.7359711365625,-1488.9801126035863,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","40 fc","no-day","yes-occ","base-epd","base-eff",209.51,98.71,4.8147505012076298E-2,7.9036441162249005E-2,-2.4813122923588001E-2,499.48440000000056,-20.703992075056004,478.78040792494454,"no",5500,642.39,3030.15,null,11525.324700000001,42235.734499999999,115.25324700000002,0,2755.917874044279,-660,23.93902039624723,2119.856894440526,-1641.0764865155816,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","40 fc","no-day","yes-occ","base-epd","high-eff",208.14,98.71,5.23623849590353E-2,8.5058683898193405E-2,-2.4813122923588001E-2,537.54300000000069,-20.703992075056004,516.83900792494467,"no",5500,642.39,3030.15,null,13780.324700000001,75730.734499999991,137.80324700000003,0,3295.1299975838306,-660,25.841950396247235,2660.9719479800779,-2144.1329400551331,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","40 fc","no-day","yes-occ","red-epd","base-eff",178.75,110.33,0.107234754605585,0.21425117587586301,-0.14545265780730901,1353.9972000000005,-121.36524224750403,1232.6319577524964,"no",5500,642.39,3030.15,null,12350.324700000001,43060.734499999999,123.50324700000002,0,2953.1906021685049,-660,61.631597887624821,2354.82220005613,-1122.1902423036336,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","40 fc","no-day","yes-occ","red-epd","high-eff",177.55,110.33,0.110944480401598,0.21952613301683599,-0.14545265780730901,1387.3332,-121.36524224750403,1265.967957752496,"no",5500,642.39,3030.15,null,14605.324700000001,76555.734499999991,146.05324700000003,0,3492.4027257080566,-660,63.298397887624802,2895.7011235956816,-1629.7331658431856,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","40 fc","yes-day","no-occ","base-epd","base-eff",201.41,101.36,6.4959666598260302E-2,0.11464240186381799,-5.2325581395348902E-2,724.50240000000042,-43.66030127961605,680.84209872038434,"no",5500,642.39,3030.15,null,12570.324700000001,59010.734499999999,125.70324700000002,0,3005.7966630016317,-660,34.042104936019221,2379.838767937651,-1698.9966692172666,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","40 fc","yes-day","no-occ","base-epd","high-eff",200.12,101.36,6.8953541604180296E-2,0.120312980790364,-5.2325581395348902E-2,760.33860000000016,-43.66030127961605,716.67829872038408,"no",5500,642.39,3030.15,null,14825.324700000001,92505.734499999991,148.25324700000002,0,3545.0087865411842,-660,35.833914936019205,2920.8427014772033,-2204.1644027568191,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","40 fc","yes-day","no-occ","red-epd","base-eff",170.71,112.96,0.123920627654033,0.249593388720383,-0.172757475083056,1577.3484000000001,-144.14829628825598,1433.2001037117441,"no",5500,642.39,3030.15,null,13395.324700000001,59835.734499999999,133.953247,0,3203.0693911258581,-660,71.66000518558721,2614.7293963114453,-1181.5292925997012,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","40 fc","yes-day","no-occ","red-epd","high-eff",169.59,112.96,0.12739356244178901,0.25451668205195799,-0.172757475083056,1608.4620000000004,-144.14829628825598,1464.3137037117444,"no",5500,642.39,3030.15,null,15650.324700000001,93330.734499999991,156.50324700000002,0,3742.2815146654102,-660,73.215685185587219,3155.4971998509973,-1691.1834961392528,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","40 fc","yes-day","yes-occ","base-epd","base-eff",191.32,105.79,8.2450629074778597E-2,0.15899599982416801,-9.83181063122925E-2,1004.8026000000006,-82.036320063088112,922.7662799369125,"no",5500,642.39,3030.15,null,14550.324700000001,60990.734499999999,145.50324700000002,0,3479.2512104997754,-660,46.138313996845625,2865.3895244966211,-1942.6232445597086,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","40 fc","yes-day","yes-occ","base-epd","high-eff",190.12,105.79,8.6176140938008197E-2,0.16427095696514099,-9.83181063122925E-2,1038.1386000000002,-82.036320063088112,956.10227993691205,"no",5500,642.39,3030.15,null,16805.324700000001,94485.734499999991,168.05324700000003,0,4018.463334039327,-660,47.805113996845606,3406.2684480361727,-2450.1661680992606,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","40 fc","yes-day","yes-occ","red-epd","base-eff",160.61000000000001,117.68,0.14055914250082899,0.293990944656908,-0.22176079734219301,1857.9264000000001,-185.03651494694412,1672.8898850530559,"no",5500,642.39,3030.15,null,15375.324700000001,61815.734499999999,153.75324700000002,0,3676.5239386240014,-660,83.644494252652805,3100.1684328766542,-1427.2785478235983,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","40 fc","yes-day","yes-occ","red-epd","high-eff",159.58000000000001,117.68,0.14376371414589501,0.29851861620290998,-0.22176079734219301,1886.5398000000002,-185.03651494694412,1701.5032850530561,"no",5500,642.39,3030.15,null,17630.324700000001,95310.734499999991,176.30324700000003,0,4215.7360621635526,-660,85.075164252652812,3640.8112264162055,-1939.3079413631494,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","25 fc","no-day","no-occ","base-epd","base-eff",209.51,98.71,4.8147505012076298E-2,7.9036441162249005E-2,-2.4813122923588001E-2,499.48440000000056,-20.703992075056004,478.78040792494454,"no",5500,642.39,3030.15,null,10260.324700000001,90250.734499999991,102.60324700000001,0,2453.4330242537981,-1045,23.93902039624723,1432.3720446500454,-953.5916367251009,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","25 fc","no-day","no-occ","base-epd","high-eff",208.14,98.71,5.23623849590353E-2,8.5058683898193405E-2,-2.4813122923588001E-2,537.54300000000069,-20.703992075056004,516.83900792494467,"no",5500,642.39,3030.15,null,12515.324700000001,123745.73449999999,125.15324700000001,0,2992.6451477933501,-1045,25.841950396247235,1973.4870981895974,-1456.6480902646526,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","25 fc","no-day","no-occ","red-epd","base-eff",178.75,110.33,0.107234754605585,0.21425117587586301,-0.14545265780730901,1353.9972000000005,-121.36524224750403,1232.6319577524964,"no",5500,642.39,3030.15,null,11085.324700000001,91075.734499999991,110.85324700000001,0,2650.7057523780245,-1045,61.631597887624821,1667.3373502656493,-434.7053925131529,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","25 fc","no-day","no-occ","red-epd","high-eff",177.55,110.33,0.110944480401598,0.21952613301683599,-0.14545265780730901,1387.3332,-121.36524224750403,1265.967957752496,"no",5500,642.39,3030.15,null,13340.324700000001,124570.73449999999,133.40324700000002,0,3189.9178759175766,-1045,63.298397887624802,2208.2162738052016,-942.2483160527056,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","25 fc","no-day","yes-occ","base-epd","base-eff",197.98,103.47,6.9032471940265502E-2,0.12971998769176701,-7.4231727574750897E-2,819.78780000000063,-61.938721061360042,757.84907893864056,"no",5500,642.39,3030.15,null,12240.324700000001,92230.734499999991,122.40324700000001,0,2926.8875717519413,-1045,37.892453946932029,1919.7800256988733,-1161.9309467602327,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","25 fc","no-day","yes-occ","base-epd","high-eff",196.72,103.47,7.2947416610099999E-2,0.13525869268978899,-7.4231727574750897E-2,854.79060000000027,-61.938721061360042,792.8518789386402,"no",5500,642.39,3030.15,null,14495.324700000001,125725.73449999999,144.953247,0,3466.0996952914934,-1045,39.64259394693201,2460.7422892384252,-1667.8904102997849,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","25 fc","no-day","yes-occ","red-epd","base-eff",167.23,115.31,0.12742513457622301,0.264890764429206,-0.19715531561461799,1674.0228000000006,-164.50577803569607,1509.5170219643046,"no",5500,642.39,3030.15,null,13065.324700000001,93055.734499999991,130.65324700000002,0,3124.1602998761678,-1045,75.47585109821523,2154.6361509743829,-645.11912901007827,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","25 fc","no-day","yes-occ","red-epd","high-eff",166.13,115.31,0.13083492509511099,0.26972614180843102,-0.19715531561461799,1704.5808000000006,-164.50577803569607,1540.0750219643046,"no",5500,642.39,3030.15,null,15320.324700000001,126550.73449999999,153.203247,0,3663.3724234157194,-1045,77.003751098215233,2695.3761745139345,-1155.3011525496299,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","25 fc","yes-day","no-occ","base-epd","base-eff",191.32,105.79,8.2450629074778597E-2,0.15899599982416801,-9.83181063122925E-2,1004.8026000000006,-82.036320063088112,922.7662799369125,"no",5500,642.39,3030.15,null,13285.324700000001,109005.73449999999,132.85324700000001,0,3176.7663607092945,-1045,46.138313996845625,2177.9046747061402,-1255.1383947692277,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","25 fc","yes-day","no-occ","base-epd","high-eff",190.12,105.79,8.6176140938008197E-2,0.16427095696514099,-9.83181063122925E-2,1038.1386000000002,-82.036320063088112,956.10227993691205,"no",5500,642.39,3030.15,null,15540.324700000001,142500.73449999999,155.40324700000002,0,3715.9784842488466,-1045,47.805113996845606,2718.7835982456922,-1762.6813183087802,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","25 fc","yes-day","no-occ","red-epd","base-eff",160.61000000000001,117.68,0.14055914250082899,0.293990944656908,-0.22176079734219301,1857.9264000000001,-185.03651494694412,1672.8898850530559,"no",5500,642.39,3030.15,null,14110.324700000001,109830.73449999999,141.10324700000001,0,3374.0390888335205,-1045,83.644494252652805,2412.6835830861733,-739.79369803311738,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","25 fc","yes-day","no-occ","red-epd","high-eff",159.58000000000001,117.68,0.14376371414589501,0.29851861620290998,-0.22176079734219301,1886.5398000000002,-185.03651494694412,1701.5032850530561,"no",5500,642.39,3030.15,null,16365.324700000001,143325.73449999999,163.65324700000002,0,3913.2512123730726,-1045,85.075164252652812,2953.3263766257255,-1251.8230915726695,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","25 fc","yes-day","yes-occ","base-epd","base-eff",183.44,109.3,9.5931930478159899E-2,0.19363488504989201,-0.134759136212625,1223.7090000000005,-112.44260131139202,1111.2663986886084,"no",5500,642.39,3030.15,null,15265.324700000001,110985.73449999999,152.65324700000002,0,3650.2209082074378,-1045,55.563319934430424,2660.7842281418684,-1549.51782945326,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","25 fc","yes-day","yes-occ","base-epd","high-eff",182.31,109.3,9.9452223467567505E-2,0.19860213635764201,-0.134759136212625,1255.1004000000003,-112.44260131139202,1142.6577986886082,"no",5500,642.39,3030.15,null,17520.324700000001,144480.73449999999,175.203247,0,4189.4330317469894,-1045,57.132889934430409,3201.5659216814197,-2058.9081229928115,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","25 fc","yes-day","yes-occ","red-epd","base-eff",152.72999999999999,121.4,0.153377429081093,0.32862982988263201,-0.26038205980066498,2076.8328000000006,-217.26197541523209,1859.5708245847686,"no",5500,642.39,3030.15,null,16090.324700000001,111810.73449999999,160.90324700000002,0,3847.4936363316638,-1045,92.978541229238431,2895.4721775609023,-1035.9013529761337,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","25 fc","yes-day","yes-occ","red-epd","high-eff",151.76,121.4,0.156392567919554,0.33289375357158602,-0.26038205980066498,2103.7794000000008,-217.26197541523209,1886.5174245847688,"no",5500,642.39,3030.15,null,18345.324700000001,145305.73449999999,183.453247,0,4386.7057598712163,-1045,94.325871229238444,3436.0316311004549,-1549.5142065156861,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","base-lpd","no-day","no-occ","base-epd","base-eff",226.37,89.84,2.3458095884572299E-2,4.92329333157503E-3,6.7275747508305506E-2,31.11360000000013,56.134673073791909,87.248273073792035,{"$f":"IF(P199>0.2,\"yes\",\"no\")","v":"no"},{"$f":"IF(B199=\"5500 ft2\",5500,IF(B199=\"10000 ft2\",10000,25000))","v":5500},{"$f":"IF(B199=\"5500 ft2\",IF(D199=\"stand-alone\",642.39,IF(D199=\"ad-e&flr\",522.37,402.25)),IF(B199=\"10000 ft2\",IF(D199=\"stand-alone\",866.06,IF(D199=\"ad-e&flr\",704.17,542.29)),IF(B199=\"25000 ft2\",IF(D199=\"stand-alone\",1369.38,IF(D199=\"ad-e&flr\",1113.42,857.45)))))","v":642.39},{"$f":"IF(B199=\"5500 ft2\",IF(D199=\"stand-alone\",3030.15,IF(D199=\"ad-e&flr\",2424.14,1818.13)),IF(B199=\"10000 ft2\",IF(D199=\"stand-alone\",4085.12,IF(D199=\"ad-e&flr\",3268.14,2451.05)),IF(B199=\"25000 ft2\",IF(D199=\"stand-alone\",6459.2,IF(D199=\"ad-e&flr\",5167.32,3875.54)))))","v":3030.15},null,{"$f":"SUM(IF(F199=\"eff-roof\",W199*IF(AND(W$4=\"no\",X$4=\"no\"),$C$4,$C$3)),IF(G199=\"eff-win\",X199*IF(W$4=\"no\",$D$4,$D$3),0),IF(H199=\"red-inf\",Y199*IF(W$4=\"no\",$F$4,$F$3),0),IF(I199=\"25 fc\",W199*IF(W$4=\"no\",$H$4,$H$3),0),IF(I199=\"40 fc\",W199*IF(W$4=\"no\",$G$4,$G$3),0),IF(J199=\"yes-day\",W199*IF(W$4=\"no\",$I$4,$I$3),0),IF(K199=\"yes-occ\",W199*IF(W$4=\"no\",$J$4,$J$3),0),IF(L199=\"red-epd\",W199*IF(W$4=\"no\",$K$4,$K$3),0),IF(AND(M199=\"high-eff\",C199=\"psz-ac\"),W199*IF(AND(W$4=\"no\",Y$4=\"no\"),$L$4,$L$3),0),IF(AND(M199=\"high-eff\",C199=\"ptac\"),W199*IF(AND(W$4=\"no\",Y$4=\"no\"),$M$4,$M$3),0),IF(AND(M199=\"high-eff\",C199=\"pthp\"),W199*IF(AND(W$4=\"no\",Y$4=\"no\"),$N$4,$N$3),0))","v":16500},{"$f":"SUM(IF(F199=\"eff-roof\",W199*$C$4),IF(G199=\"eff-win\",X199*$D$4,0),IF(H199=\"red-inf\",Y199*$F$4,0),IF(I199=\"25 fc\",W199*$H$4,0),IF(I199=\"40 fc\",W199*$G$4,0),IF(J199=\"yes-day\",W199*$I$4,0),IF(K199=\"yes-occ\",W199*$J$4,0),IF(L199=\"red-epd\",W199*$K$4,0),IF(AND(M199=\"high-eff\",C199=\"psz-ac\"),W199*$L$4,0),IF(AND(M199=\"high-eff\",C199=\"ptac\"),W199*$M$4,0),IF(AND(M199=\"high-eff\",C199=\"pthp\"),W199*$N$4,0))","v":66825},165,0,{"$f":"-PMT($AE$3,$AE$4,AA199+AC199-AD199)","v":3945.4545624845255},{"$f":"SUM(IF(F199=\"eff-roof\",($C$5*W199),0),IF(G199=\"eff-win\",($D$5*X199),0),IF(H199=\"red-inf\",$F$5*(Y199-X199),0),IF(I199=\"25 fc\",($H$5*W199),0),IF(I199=\"40 fc\",($G$5*W199),0),IF(J199=\"yes-day\",($I$5*W199),0),IF(K199=\"yes-occ\",($J$5*W199),0),IF(L199=\"red-epd\",($K$5*W199),0),IF(M199=\"high-eff\",($L$5*W199),0))","v":0},{"$f":"0.05*U199","v":4.3624136536896021},3949.8169761382151,{"$f":"U199-AH199","v":-3862.5687030644231},null,null,null,"New Construction",{"$f":"IF(B199=\"5500 ft2\",\"5,500 SF\",IF(B199=\"10000 ft2\",\"10,000 SF\",IF(B199=\"25000 ft2\",\"25,000 SF\")))","v":"5,500 SF"},"Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration",{"$f":"IF(I199=\"base-lpd\",\"Baseline Lighting Levels\",IF(I199=\"40 fc\",\"Reduce Lighting Levels to 40 fc\",IF(I199=\"25 fc\",\"Reduce Lighting Levels to 25 fc\")))","v":"Baseline Lighting Levels"},"No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","base-lpd","no-day","no-occ","base-epd","high-eff",224.75,89.84,2.8462279192384799E-2,1.20444854718889E-2,6.7275747508305506E-2,{"$f":"277.8*($N$7-N200)*$S$3","v":76.117200000000253},{"$f":"277.78*($O$7-O200)*$S$4","v":56.134673073791909},{"$f":"SUM(S200:T200)","v":132.25187307379215},"no",5500,642.39,3030.15,null,18755,100320,{"$f":"MIN(0.01*AA200,500)","v":187.55},{"$f":"IF(V200=\"yes\",0,0)","v":0},4484.6666860240766,0,6.6125936536896077,{"$f":"SUM(AE200:AG200)","v":4491.2792796777667},-4359.0274066039747,null,null,null,"New Construction","5,500 SF",{"$f":"IF(C200=\"psz-ac\",\"Packaged Air Conditioner\",IF(C200=\"ptac\",\"Split System Air Conditioner\",IF(C200=\"pthp\",\"Split System Heat Pump\")))","v":"Packaged Air Conditioner"},{"$f":"IF(D200=\"stand-alone\",\"Stand Alone\",IF(D200=\"ad-e&flr\",\"Above Ground, 1 Side Attached\",IF(D200=\"ad-e&w&flr\",\"Above Ground, 2 Sides Attached\")))","v":"Stand Alone"},{"$f":"IF(F200=\"base-roof\",\"Baseline Roof Insulation\",IF(F200=\"eff-roof\",\"Increased Roof Insulation\"))","v":"Increased Roof Insulation"},{"$f":"IF(G200=\"base-win\",\"Baseline Windows\",IF(G200=\"eff-win\",\"Replace Windows\"))","v":"Baseline Windows"},{"$f":"IF(H200=\"base-inf\",\"Baseline Infiltration\",IF(H200=\"red-inf\",\"Reduce Infiltration\"))","v":"Baseline Infiltration"},"Baseline Lighting Levels",{"$f":"IF(J200=\"no-day\",\"No Daylighting Sensors\",IF(J200=\"yes-day\",\"Install Daylighting Sensors\"))","v":"No Daylighting Sensors"},{"$f":"IF(K200=\"no-occ\",\"No Occupancy Sensors\",IF(K200=\"yes-occ\",\"Install Occupancy Sensors\"))","v":"No Occupancy Sensors"},{"$f":"IF(L200=\"base-epd\",\"No Plug Load Control\",IF(L200=\"red-epd\",\"Install Plug Load Controls\"))","v":"No Plug Load Control"},{"$f":"IF(M200=\"base-eff\",\"Baseline HVAC Equipment\",IF(M200=\"high-eff\",\"Install High Efficiency HVAC Equipment\"))","v":"Install High Efficiency HVAC Equipment"}]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","base-lpd","no-day","no-occ","red-epd","base-eff",195.54,100.94,8.4408101409695804E-2,0.140445733878412,-4.7965116279069797E-2,887.57100000000048,-40.021942839648034,847.5490571603525,"no",5500,642.39,3030.15,null,17325,67650,173.25,0,4142.7272906087519,0,42.377452858017627,4185.1047434667698,-3337.5556863064176,null,null,null,{"$f":"IF(A201=\"new90.1-2004\",\"New Construction\",IF(A201=\"post1980\",\"Post 1980 Construction\",IF(A201=\"pre1980\",\"Pre 1980 Construction\")))","v":"New Construction"},"5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","base-lpd","no-day","no-occ","red-epd","high-eff",194.1,100.94,8.88597723649108E-2,0.14677568244757999,-4.7965116279069797E-2,927.57420000000047,-40.021942839648034,887.55225716035238,"no",5500,642.39,3030.15,null,19580,101145,195.8,0,4681.9394141483035,0,44.377612858017621,4726.317027006321,-3838.7647698459687,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","base-lpd","no-day","yes-occ","base-epd","base-eff",211.84,95.42,5.1067927447235102E-2,6.8794232713525902E-2,9.3438538205979204E-3,434.75700000000018,7.7964823713599252,442.55348237136008,"no",5500,642.39,3030.15,null,18480,68805,184.8,0,4418.9091099826683,0,22.127674118568006,4441.0367841012367,-3998.4833017298765,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","base-lpd","no-day","yes-occ","base-epd","high-eff",210.36,95.42,5.5645886940186601E-2,7.5300013187392795E-2,9.3438538205979204E-3,475.87139999999994,7.7964823713599252,483.66788237135984,"no",5500,642.39,3030.15,null,20735,102300,207.35,0,4958.1212335222199,0,24.183394118567993,4982.3046276407877,-4498.6367452694276,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","base-lpd","no-day","yes-occ","red-epd","base-eff",181.03,106.87,0.11088133613272901,0.20422875730801399,-0.10953073089701,1290.6588000000004,-91.392098908720087,1199.2667010912803,"no",5500,642.39,3030.15,null,19305,69630,193.05,0,4616.1818381068952,0,59.96333505456402,4676.1451731614588,-3476.8784720701788,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","base-lpd","no-day","yes-occ","red-epd","high-eff",179.73,106.87,0.1149225693403,0.20994329421073499,-0.10953073089701,1326.7728000000006,-91.392098908720087,1235.3807010912806,"no",5500,642.39,3030.15,null,21560,103125,215.6,0,5155.3939616464468,0,61.769035054564029,5217.1629967010103,-3981.7822956097298,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","base-lpd","yes-day","no-occ","base-epd","base-eff",203.55,97.99,6.8748322730358302E-2,0.105235394962416,-1.73380398671097E-2,665.05319999999995,-14.466806177968014,650.58639382203194,"no",5500,642.39,3030.15,null,19525,85580,195.25,0,4668.7878989400215,0,32.529319691101598,4701.3172186311231,-4050.7308248090912,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","base-lpd","yes-day","no-occ","base-epd","high-eff",202.15,97.99,7.3073705147836607E-2,0.111389511626885,-1.73380398671097E-2,703.94520000000011,-14.466806177968014,689.4783938220321,"no",5500,642.39,3030.15,null,21780,119075,217.8,0,5208.0000224795731,0,34.473919691101607,5242.4739421706745,-4552.9955483486428,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","base-lpd","yes-day","no-occ","red-epd","base-eff",172.79,109.5,0.12818286580264299,0.24045012967602999,-0.136835548172758,1519.5660000000007,-114.17515294947205,1405.3908470505287,"no",5500,642.39,3030.15,null,20350,86405,203.5,0,4866.0606270642484,0,70.269542352526443,4936.3301694167749,-3530.9393223662464,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","base-lpd","yes-day","no-occ","red-epd","high-eff",171.56,109.5,0.13198730800195699,0.24585696074552699,-0.136835548172758,1553.7354000000005,-114.17515294947205,1439.5602470505285,"no",5500,642.39,3030.15,null,22605,119900,226.05,0,5405.2727506038,0,71.97801235252642,5477.2507629563261,-4037.6905159057978,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","base-lpd","yes-day","yes-occ","base-epd","base-eff",193.62,102.23,8.6349787677395998E-2,0.14888566530396899,-6.1357973421927003E-2,940.90860000000021,-51.196900905264087,889.7116990947361,"no",5500,642.39,3030.15,null,21505,87560,215.05,0,5142.2424464381647,0,44.485584954736808,5186.7280313929014,-4297.0163322981653,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","base-lpd","yes-day","yes-occ","base-epd","high-eff",192.3,102.23,9.0391020884966894E-2,0.15468811815903999,-6.1357973421927003E-2,977.57819999999992,-51.196900905264087,926.38129909473582,"no",5500,642.39,3030.15,null,23760,121055,237.6,0,5681.4545699777163,0,46.319064954736795,5727.7736349324532,-4801.3923358377178,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","base-lpd","yes-day","yes-occ","red-epd","base-eff",162.86000000000001,113.97,0.145042385590478,0.28410040001758302,-0.18324335548172799,1795.4214000000002,-152.89768206056004,1642.5237179394401,"no",5500,642.39,3030.15,null,22330,88385,223.3,0,5339.5151745623907,0,82.126185896972004,5421.6413604593627,-3779.1176425199228,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","base-lpd","yes-day","yes-occ","red-epd","high-eff",161.72,113.97,0.148562678579885,0.28911160930150798,-0.18324335548172799,1827.0906000000004,-152.89768206056004,1674.1929179394403,"no",5500,642.39,3030.15,null,24585,121880,245.85,0,5878.7272981019432,0,83.70964589697202,5962.436943998915,-4288.2440260594749,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","40 fc","no-day","no-occ","base-epd","base-eff",226.37,89.84,2.3458095884572299E-2,4.92329333157503E-3,6.7275747508305506E-2,31.11360000000013,56.134673073791909,87.248273073792035,"no",5500,642.39,3030.15,null,20130,78155,201.3,0,4813.4545662311202,-660,4.3624136536896021,4157.8169798848103,-4070.5687068110183,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","40 fc","no-day","no-occ","base-epd","high-eff",224.75,89.84,2.8462279192384799E-2,1.20444854718889E-2,6.7275747508305506E-2,76.117200000000253,56.134673073791909,132.25187307379215,"no",5500,642.39,3030.15,null,22385,111650,223.85,0,5352.6666897706718,-660,6.6125936536896077,4699.2792834243619,-4567.0274103505699,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","40 fc","no-day","no-occ","red-epd","base-eff",195.54,100.94,8.4408101409695804E-2,0.140445733878412,-4.7965116279069797E-2,887.57100000000048,-40.021942839648034,847.5490571603525,"no",5500,642.39,3030.15,null,20955,78980,209.55,0,5010.7272943553471,-660,42.377452858017627,4393.104747213365,-3545.5556900530128,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","40 fc","no-day","no-occ","red-epd","high-eff",194.1,100.94,8.88597723649108E-2,0.14677568244757999,-4.7965116279069797E-2,927.57420000000047,-40.021942839648034,887.55225716035238,"no",5500,642.39,3030.15,null,23210,112475,232.1,0,5549.9394178948987,-660,44.377612858017621,4934.3170307529163,-4046.7647735925639,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","40 fc","no-day","yes-occ","base-epd","base-eff",211.84,95.42,5.1067927447235102E-2,6.8794232713525902E-2,9.3438538205979204E-3,434.75700000000018,7.7964823713599252,442.55348237136008,"no",5500,642.39,3030.15,null,22110,80135,221.1,0,5286.9091137292635,-660,22.127674118568006,4649.0367878478319,-4206.4833054764722,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","40 fc","no-day","yes-occ","base-epd","high-eff",210.36,95.42,5.5645886940186601E-2,7.5300013187392795E-2,9.3438538205979204E-3,475.87139999999994,7.7964823713599252,483.66788237135984,"no",5500,642.39,3030.15,null,24365,113630,243.65,0,5826.121237268816,-660,24.183394118567993,5190.3046313873838,-4706.6367490160237,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","40 fc","no-day","yes-occ","red-epd","base-eff",181.03,106.87,0.11088133613272901,0.20422875730801399,-0.10953073089701,1290.6588000000004,-91.392098908720087,1199.2667010912803,"no",5500,642.39,3030.15,null,22935,80960,229.35,0,5484.1818418534895,-660,59.96333505456402,4884.1451769080531,-3684.8784758167731,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","40 fc","no-day","yes-occ","red-epd","high-eff",179.73,106.87,0.1149225693403,0.20994329421073499,-0.10953073089701,1326.7728000000006,-91.392098908720087,1235.3807010912806,"no",5500,642.39,3030.15,null,25190,114455,251.9,0,6023.3939653930429,-660,61.769035054564029,5425.1630004476065,-4189.7822993563259,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","40 fc","yes-day","no-occ","base-epd","base-eff",203.55,97.99,6.8748322730358302E-2,0.105235394962416,-1.73380398671097E-2,665.05319999999995,-14.466806177968014,650.58639382203194,"no",5500,642.39,3030.15,null,23155,96910,231.55,0,5536.7879026866167,-660,32.529319691101598,4909.3172223777183,-4258.7308285556865,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","40 fc","yes-day","no-occ","base-epd","high-eff",202.15,97.99,7.3073705147836607E-2,0.111389511626885,-1.73380398671097E-2,703.94520000000011,-14.466806177968014,689.4783938220321,"no",5500,642.39,3030.15,null,25410,130405,254.1,0,6076.0000262261683,-660,34.473919691101607,5450.4739459172697,-4760.9955520952371,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","40 fc","yes-day","no-occ","red-epd","base-eff",172.79,109.5,0.12818286580264299,0.24045012967602999,-0.136835548172758,1519.5660000000007,-114.17515294947205,1405.3908470505287,"no",5500,642.39,3030.15,null,23980,97735,239.8,0,5734.0606308108436,-660,70.269542352526443,5144.3301731633701,-3738.9393261128416,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","40 fc","yes-day","no-occ","red-epd","high-eff",171.56,109.5,0.13198730800195699,0.24585696074552699,-0.136835548172758,1553.7354000000005,-114.17515294947205,1439.5602470505285,"no",5500,642.39,3030.15,null,26235,131230,262.35000000000002,0,6273.2727543503952,-660,71.97801235252642,5685.2507667029213,-4245.690519652393,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","40 fc","yes-day","yes-occ","base-epd","base-eff",193.62,102.23,8.6349787677395998E-2,0.14888566530396899,-6.1357973421927003E-2,940.90860000000021,-51.196900905264087,889.7116990947361,"no",5500,642.39,3030.15,null,25135,98890,251.35,0,6010.2424501847599,-660,44.485584954736808,5394.7280351394966,-4505.0163360447605,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","40 fc","yes-day","yes-occ","base-epd","high-eff",192.3,102.23,9.0391020884966894E-2,0.15468811815903999,-6.1357973421927003E-2,977.57819999999992,-51.196900905264087,926.38129909473582,"no",5500,642.39,3030.15,null,27390,132385,273.90000000000003,0,6549.4545737243125,-660,46.319064954736795,5935.7736386790493,-5009.392339584314,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","40 fc","yes-day","yes-occ","red-epd","base-eff",162.86000000000001,113.97,0.145042385590478,0.28410040001758302,-0.18324335548172799,1795.4214000000002,-152.89768206056004,1642.5237179394401,"no",5500,642.39,3030.15,null,25960,99715,259.60000000000002,0,6207.5151783089859,-660,82.126185896972004,5629.6413642059579,-3987.117646266518,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","40 fc","yes-day","yes-occ","red-epd","high-eff",161.72,113.97,0.148562678579885,0.28911160930150798,-0.18324335548172799,1827.0906000000004,-152.89768206056004,1674.1929179394403,"no",5500,642.39,3030.15,null,28215,133210,282.15000000000003,0,6746.7273018485394,-660,83.70964589697202,6170.4369477455111,-4496.244029806071,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","25 fc","no-day","no-occ","base-epd","base-eff",211.84,95.42,5.1067927447235102E-2,6.8794232713525902E-2,9.3438538205979204E-3,434.75700000000018,7.7964823713599252,442.55348237136008,"no",5500,642.39,3030.15,null,20845,128150,208.45000000000002,0,4984.424263938784,-1045,22.127674118568006,3961.5519380573519,-3518.9984556859918,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","25 fc","no-day","no-occ","base-epd","high-eff",210.36,95.42,5.5645886940186601E-2,7.5300013187392795E-2,9.3438538205979204E-3,475.87139999999994,7.7964823713599252,483.66788237135984,"no",5500,642.39,3030.15,null,23100,161645,231,0,5523.6363874783356,-1045,24.183394118567993,4502.8197815969033,-4019.1518992255433,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","25 fc","no-day","no-occ","red-epd","base-eff",181.03,106.87,0.11088133613272901,0.20422875730801399,-0.10953073089701,1290.6588000000004,-91.392098908720087,1199.2667010912803,"no",5500,642.39,3030.15,null,21670,128975,216.70000000000002,0,5181.6969920630108,-1045,59.96333505456402,4196.6603271175745,-2997.3936260262944,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","25 fc","no-day","no-occ","red-epd","high-eff",179.73,106.87,0.1149225693403,0.20994329421073499,-0.10953073089701,1326.7728000000006,-91.392098908720087,1235.3807010912806,"no",5500,642.39,3030.15,null,23925,162470,239.25,0,5720.9091156025625,-1045,61.769035054564029,4737.678150657126,-3502.2974495658455,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","25 fc","no-day","yes-occ","base-epd","base-eff",200.38,100.01,7.2300187854200004E-2,0.11917007340982,-3.8309800664451998E-2,753.11580000000049,-31.9655777225761,721.1502222774244,"no",5500,642.39,3030.15,null,22825,130130,228.25,0,5457.8788114369272,-1045,36.057511113871222,4448.9363225507986,-3727.7861002733744,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","25 fc","no-day","yes-occ","base-epd","high-eff",199,100.01,7.6562426002809894E-2,0.125236274121939,-3.8309800664451998E-2,791.45220000000029,-31.9655777225761,759.4866222774242,"no",5500,642.39,3030.15,null,25080,163625,250.8,0,5997.0909349764788,-1045,37.974331113871209,4990.0652660903497,-4230.5786438129253,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","25 fc","no-day","yes-occ","red-epd","base-eff",169.57,111.75,0.13118221857388701,0.25460459800430801,-0.16019518272425301,1609.0176000000006,-133.66635887787203,1475.3512411221286,"no",5500,642.39,3030.15,null,23650,130955,236.5,0,5655.1515395611532,-1045,73.767562056106428,4683.9191016172599,-3208.5678604951313,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","25 fc","no-day","yes-occ","red-epd","high-eff",168.36,111.75,0.13492351650433301,0.25992351312145601,-0.16019518272425301,1642.6314,-133.66635887787203,1508.965041122128,"no",5500,642.39,3030.15,null,25905,164450,259.05,0,6194.3636631007039,-1045,75.448252056106398,5224.8119151568098,-3715.8468740346816,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","25 fc","yes-day","no-occ","base-epd","base-eff",193.62,102.23,8.6349787677395998E-2,0.14888566530396899,-6.1357973421927003E-2,940.90860000000021,-51.196900905264087,889.7116990947361,"no",5500,642.39,3030.15,null,23870,146905,238.70000000000002,0,5707.7576003942804,-1045,44.485584954736808,4707.243185349017,-3817.5314862542809,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","25 fc","yes-day","no-occ","base-epd","high-eff",192.3,102.23,9.0391020884966894E-2,0.15468811815903999,-6.1357973421927003E-2,977.57819999999992,-51.196900905264087,926.38129909473582,"no",5500,642.39,3030.15,null,26125,180400,261.25,0,6246.969723933832,-1045,46.319064954736795,5248.2887888885689,-4321.9074897938335,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","25 fc","yes-day","no-occ","red-epd","base-eff",162.86000000000001,113.97,0.145042385590478,0.28410040001758302,-0.18324335548172799,1795.4214000000002,-152.89768206056004,1642.5237179394401,"no",5500,642.39,3030.15,null,24695,147730,246.95000000000002,0,5905.0303285185064,-1045,82.126185896972004,4942.1565144154783,-3299.6327964760385,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","25 fc","yes-day","no-occ","red-epd","high-eff",161.72,113.97,0.148562678579885,0.28911160930150798,-0.18324335548172799,1827.0906000000004,-152.89768206056004,1674.1929179394403,"no",5500,642.39,3030.15,null,26950,181225,269.5,0,6444.242452058058,-1045,83.70964589697202,5482.9520979550298,-3808.7591800155897,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","25 fc","yes-day","yes-occ","base-epd","base-eff",185.81,105.58,0.100099452223468,0.18321684469647001,-9.6137873754152905E-2,1157.8704000000002,-80.217140843104048,1077.6532591568962,"no",5500,642.39,3030.15,null,25850,148885,258.5,0,6181.2121478924237,-1045,53.882662957844815,5190.0948108502689,-4112.4415516933732,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","25 fc","yes-day","yes-occ","base-epd","high-eff",184.57,105.58,0.103935466557217,0.18866763374214299,-9.6137873754152905E-2,1192.3176000000005,-80.217140843104048,1112.1004591568965,"no",5500,642.39,3030.15,null,28105,182380,281.05,0,6720.4242714319753,-1045,55.605022957844824,5731.0292943898203,-4618.928835232924,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","25 fc","yes-day","yes-occ","red-epd","base-eff",155.05000000000001,117.58,0.15803431891013001,0.31843157941008399,-0.22072259136212599,2012.3832,-184.17023912790401,1828.2129608720959,"no",5500,642.39,3030.15,null,26675,149710,266.75,0,6378.4848760166497,-1045,91.410648043604795,5424.8955240602545,-3596.6825631881584,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","25 fc","yes-day","yes-occ","red-epd","high-eff",153.97,117.58,0.16136517909293299,0.32317904083695997,-0.22072259136212599,2042.3856000000005,-184.17023912790401,1858.2153608720964,"no",5500,642.39,3030.15,null,28930,183205,289.3,0,6917.6969995562004,-1045,92.910768043604833,5965.6077675998049,-4107.3924067277085,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","base-lpd","no-day","no-occ","base-epd","base-eff",226.27,88.38,2.8288632452997099E-2,5.3628730933227798E-3,8.2433554817275698E-2,33.891599999999976,68.782300031775975,102.67390003177596,"no",5500,642.39,3030.15,null,17802.964500000002,68127.964500000002,178.02964500000002,0,4257.0174249863658,0,5.1336950015887979,4262.1511199879542,-4159.4772199561785,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","base-lpd","no-day","no-occ","base-epd","high-eff",224.64,88.38,3.3308601828026599E-2,1.2528023209811501E-2,8.2433554817275698E-2,79.173000000000641,68.782300031775975,147.95530003177663,"no",5500,642.39,3030.15,null,20057.964500000002,101622.9645,200.57964500000003,0,4796.2295485259192,0,7.3977650015888319,4803.6273135275078,-4655.6720134957313,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","base-lpd","no-day","no-occ","red-epd","base-eff",195.45,99.3,8.9743792129066899E-2,0.14084135566398501,-3.0938538205980099E-2,890.07120000000077,-25.815019407392032,864.25618059260876,"no",5500,642.39,3030.15,null,18627.964500000002,68952.964500000002,186.27964500000002,0,4454.2901531105927,0,43.212809029630442,4497.5029621402227,-3633.2467815476139,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","base-lpd","no-day","no-occ","red-epd","high-eff",194,99.3,9.4195463084281894E-2,0.14721526220932801,-3.0938538205980099E-2,930.35220000000027,-25.815019407392032,904.53718059260825,"no",5500,642.39,3030.15,null,20882.964500000002,102447.9645,208.82964500000003,0,4993.5022766501443,0,45.226859029630418,5038.729135679775,-4134.1919550871671,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","base-lpd","no-day","yes-occ","base-epd","base-eff",211.75,93.86,5.6182613225567203E-2,6.9189854499098896E-2,2.55398671096345E-2,437.2572000000003,21.310385148383943,458.56758514838424,"no",5500,642.39,3030.15,null,19782.964500000002,70107.964500000002,197.82964500000003,0,4730.4719724845099,0,22.928379257419213,4753.4003517419287,-4294.8327665935449,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","base-lpd","no-day","yes-occ","base-epd","high-eff",210.27,93.86,6.0776358785735701E-2,7.5695634972965803E-2,2.55398671096345E-2,478.37159999999994,21.310385148383943,499.68198514838389,"no",5500,642.39,3030.15,null,22037.964500000002,103602.9645,220.37964500000001,0,5269.6840960240615,0,24.984099257419196,5294.6681952814806,-4794.9862101330964,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","base-lpd","no-day","yes-occ","red-epd","base-eff",180.94,105.12,0.11656432033087601,0.20462437909358699,-9.1362126245847303E-2,1293.1590000000006,-76.2322720755201,1216.9267279244805,"no",5500,642.39,3030.15,null,20607.964500000002,70932.964500000002,206.07964500000003,0,4927.7447006087359,0,60.846336396224025,4988.5910370049596,-3771.6643090804791,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","base-lpd","no-day","yes-occ","red-epd","high-eff",179.63,105.12,0.120621339605664,0.21038287397248201,-9.1362126245847303E-2,1329.5508000000004,-76.2322720755201,1253.3185279244803,"no",5500,642.39,3030.15,null,22862.964500000002,104427.9645,228.62964500000001,0,5466.9568241482875,0,62.665926396224023,5529.6227505445113,-4276.3042226200305,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","base-lpd","yes-day","no-occ","base-epd","base-eff",203.45,96.4,7.3973510979209803E-2,0.105674974724164,-8.3056478405328605E-4,667.83120000000065,-0.69302065523210832,667.13817934476856,"no",5500,642.39,3030.15,null,20827.964500000002,86882.964500000002,208.27964500000002,0,4980.3507614418622,0,33.356908967238432,5013.7076704091005,-4346.5694910643324,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","base-lpd","yes-day","no-occ","base-epd","high-eff",202.05,96.4,7.8314679463905204E-2,0.11182909138863199,-8.3056478405328605E-4,706.72320000000002,-0.69302065523210832,706.03017934476793,"no",5500,642.39,3030.15,null,23082.964500000002,120377.9645,230.82964500000003,0,5519.5628849814148,0,35.301508967238398,5554.8643939486528,-4848.8342146038849,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","base-lpd","yes-day","no-occ","red-epd","base-eff",172.69,107.79,0.13378691966470399,0.24088970943777799,-0.119082225913621,1522.3440000000005,-99.361836443888109,1422.9821635561125,"no",5500,642.39,3030.15,null,21652.964500000002,87707.964500000002,216.52964500000002,0,5177.6234895660891,0,71.14910817780563,5248.7725977438949,-3825.7904341877825,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","base-lpd","yes-day","no-occ","red-epd","high-eff",171.46,107.79,0.13759136186401899,0.24629654050727501,-0.119082225913621,1556.5134000000003,-99.361836443888109,1457.1515635561123,"no",5500,642.39,3030.15,null,23907.964500000002,121202.9645,239.07964500000003,0,5716.8356131056407,0,72.857578177805621,5789.6931912834461,-4332.5416277273343,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","base-lpd","yes-day","yes-occ","base-epd","base-eff",193.53,100.59,9.1669692329549995E-2,0.149281287089542,-4.4331395348837302E-2,943.40880000000038,-36.989977473008082,906.41882252699224,"no",5500,642.39,3030.15,null,22807.964500000002,88862.964500000002,228.07964500000003,0,5453.8053089400064,0,45.320941126349616,5499.1262500663561,-4592.7074275393643,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","base-lpd","yes-day","yes-occ","base-epd","high-eff",192.22,100.59,9.5726711604338002E-2,0.15503978196843801,-4.4331395348837302E-2,979.80060000000037,-36.989977473008082,942.81062252699235,"no",5500,642.39,3030.15,null,25062.964500000002,122357.9645,250.62964500000001,0,5993.017432479558,0,47.140531126349622,6040.1579636059078,-5097.3473410789156,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","base-lpd","yes-day","yes-occ","red-epd","base-eff",162.77000000000001,112.23,0.150709583721408,0.28449602180315597,-0.16517857142857201,1797.9216000000001,-137.82448280926408,1660.0971171907361,"no",5500,642.39,3030.15,null,23632.964500000002,89687.964500000002,236.32964500000003,0,5651.0780370642324,0,83.004855859536804,5734.0828929237696,-4073.9857757330337,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","base-lpd","yes-day","yes-occ","red-epd","high-eff",161.62,112.23,0.15424566277803201,0.289551189063256,-0.16517857142857201,1829.8686000000002,-137.82448280926408,1692.0441171907362,"no",5500,642.39,3030.15,null,25887.964500000002,123182.9645,258.87964500000004,0,6190.290160603784,0,84.602205859536809,6274.8923664633212,-4582.8482492725852,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","40 fc","no-day","no-occ","base-epd","base-eff",226.27,88.38,2.8288632452997099E-2,5.3628730933227798E-3,8.2433554817275698E-2,33.891599999999976,68.782300031775975,102.67390003177596,{"$f":"IF(P263>0.2,\"yes\",\"no\")","v":"no"},{"$f":"IF(B263=\"5500 ft2\",5500,IF(B263=\"10000 ft2\",10000,25000))","v":5500},{"$f":"IF(B263=\"5500 ft2\",IF(D263=\"stand-alone\",642.39,IF(D263=\"ad-e&flr\",522.37,402.25)),IF(B263=\"10000 ft2\",IF(D263=\"stand-alone\",866.06,IF(D263=\"ad-e&flr\",704.17,542.29)),IF(B263=\"25000 ft2\",IF(D263=\"stand-alone\",1369.38,IF(D263=\"ad-e&flr\",1113.42,857.45)))))","v":642.39},{"$f":"IF(B263=\"5500 ft2\",IF(D263=\"stand-alone\",3030.15,IF(D263=\"ad-e&flr\",2424.14,1818.13)),IF(B263=\"10000 ft2\",IF(D263=\"stand-alone\",4085.12,IF(D263=\"ad-e&flr\",3268.14,2451.05)),IF(B263=\"25000 ft2\",IF(D263=\"stand-alone\",6459.2,IF(D263=\"ad-e&flr\",5167.32,3875.54)))))","v":3030.15},null,{"$f":"SUM(IF(F263=\"eff-roof\",W263*IF(AND(W$4=\"no\",X$4=\"no\"),$C$4,$C$3)),IF(G263=\"eff-win\",X263*IF(W$4=\"no\",$D$4,$D$3),0),IF(H263=\"red-inf\",Y263*IF(W$4=\"no\",$F$4,$F$3),0),IF(I263=\"25 fc\",W263*IF(W$4=\"no\",$H$4,$H$3),0),IF(I263=\"40 fc\",W263*IF(W$4=\"no\",$G$4,$G$3),0),IF(J263=\"yes-day\",W263*IF(W$4=\"no\",$I$4,$I$3),0),IF(K263=\"yes-occ\",W263*IF(W$4=\"no\",$J$4,$J$3),0),IF(L263=\"red-epd\",W263*IF(W$4=\"no\",$K$4,$K$3),0),IF(AND(M263=\"high-eff\",C263=\"psz-ac\"),W263*IF(AND(W$4=\"no\",Y$4=\"no\"),$L$4,$L$3),0),IF(AND(M263=\"high-eff\",C263=\"ptac\"),W263*IF(AND(W$4=\"no\",Y$4=\"no\"),$M$4,$M$3),0),IF(AND(M263=\"high-eff\",C263=\"pthp\"),W263*IF(AND(W$4=\"no\",Y$4=\"no\"),$N$4,$N$3),0))","v":21432.964500000002},{"$f":"SUM(IF(F263=\"eff-roof\",W263*$C$4),IF(G263=\"eff-win\",X263*$D$4,0),IF(H263=\"red-inf\",Y263*$F$4,0),IF(I263=\"25 fc\",W263*$H$4,0),IF(I263=\"40 fc\",W263*$G$4,0),IF(J263=\"yes-day\",W263*$I$4,0),IF(K263=\"yes-occ\",W263*$J$4,0),IF(L263=\"red-epd\",W263*$K$4,0),IF(AND(M263=\"high-eff\",C263=\"psz-ac\"),W263*$L$4,0),IF(AND(M263=\"high-eff\",C263=\"ptac\"),W263*$M$4,0),IF(AND(M263=\"high-eff\",C263=\"pthp\"),W263*$N$4,0))","v":79457.964500000002},214.32964500000003,0,{"$f":"-PMT($AE$3,$AE$4,AA263+AC263-AD263)","v":5125.0174287329619},{"$f":"SUM(IF(F263=\"eff-roof\",($C$5*W263),0),IF(G263=\"eff-win\",($D$5*X263),0),IF(H263=\"red-inf\",$F$5*(Y263-X263),0),IF(I263=\"25 fc\",($H$5*W263),0),IF(I263=\"40 fc\",($G$5*W263),0),IF(J263=\"yes-day\",($I$5*W263),0),IF(K263=\"yes-occ\",($J$5*W263),0),IF(L263=\"red-epd\",($K$5*W263),0),IF(M263=\"high-eff\",($L$5*W263),0))","v":-660},{"$f":"0.05*U263","v":5.1336950015887979},4470.1511237345503,{"$f":"U263-AH263","v":-4367.4772237027746},null,null,null,"New Construction",{"$f":"IF(B263=\"5500 ft2\",\"5,500 SF\",IF(B263=\"10000 ft2\",\"10,000 SF\",IF(B263=\"25000 ft2\",\"25,000 SF\")))","v":"5,500 SF"},"Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration",{"$f":"IF(I263=\"base-lpd\",\"Baseline Lighting Levels\",IF(I263=\"40 fc\",\"Reduce Lighting Levels to 40 fc\",IF(I263=\"25 fc\",\"Reduce Lighting Levels to 25 fc\")))","v":"Reduce Lighting Levels to 40 fc"},"No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","40 fc","no-day","no-occ","base-epd","high-eff",224.64,88.38,3.3308601828026599E-2,1.2528023209811501E-2,8.2433554817275698E-2,{"$f":"277.8*($N$7-N264)*$S$3","v":79.173000000000641},{"$f":"277.78*($O$7-O264)*$S$4","v":68.782300031775975},{"$f":"SUM(S264:T264)","v":147.95530003177663},"no",5500,642.39,3030.15,null,23687.964500000002,112952.9645,{"$f":"MIN(0.01*AA264,500)","v":236.87964500000001},{"$f":"IF(V264=\"yes\",0,0)","v":0},5664.2295522725144,-660,7.3977650015888319,{"$f":"SUM(AE264:AG264)","v":5011.627317274103},-4863.6720172423265,null,null,null,"New Construction","5,500 SF",{"$f":"IF(C264=\"psz-ac\",\"Packaged Air Conditioner\",IF(C264=\"ptac\",\"Split System Air Conditioner\",IF(C264=\"pthp\",\"Split System Heat Pump\")))","v":"Packaged Air Conditioner"},{"$f":"IF(D264=\"stand-alone\",\"Stand Alone\",IF(D264=\"ad-e&flr\",\"Above Ground, 1 Side Attached\",IF(D264=\"ad-e&w&flr\",\"Above Ground, 2 Sides Attached\")))","v":"Stand Alone"},{"$f":"IF(F264=\"base-roof\",\"Baseline Roof Insulation\",IF(F264=\"eff-roof\",\"Increased Roof Insulation\"))","v":"Increased Roof Insulation"},{"$f":"IF(G264=\"base-win\",\"Baseline Windows\",IF(G264=\"eff-win\",\"Replace Windows\"))","v":"Baseline Windows"},{"$f":"IF(H264=\"base-inf\",\"Baseline Infiltration\",IF(H264=\"red-inf\",\"Reduce Infiltration\"))","v":"Reduce Infiltration"},"Reduce Lighting Levels to 40 fc",{"$f":"IF(J264=\"no-day\",\"No Daylighting Sensors\",IF(J264=\"yes-day\",\"Install Daylighting Sensors\"))","v":"No Daylighting Sensors"},{"$f":"IF(K264=\"no-occ\",\"No Occupancy Sensors\",IF(K264=\"yes-occ\",\"Install Occupancy Sensors\"))","v":"No Occupancy Sensors"},{"$f":"IF(L264=\"base-epd\",\"No Plug Load Control\",IF(L264=\"red-epd\",\"Install Plug Load Controls\"))","v":"No Plug Load Control"},{"$f":"IF(M264=\"base-eff\",\"Baseline HVAC Equipment\",IF(M264=\"high-eff\",\"Install High Efficiency HVAC Equipment\"))","v":"Install High Efficiency HVAC Equipment"}]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","40 fc","no-day","no-occ","red-epd","base-eff",195.45,99.3,8.9743792129066899E-2,0.14084135566398501,-3.0938538205980099E-2,890.07120000000077,-25.815019407392032,864.25618059260876,"no",5500,642.39,3030.15,null,22257.964500000002,80282.964500000002,222.57964500000003,0,5322.2901568571888,-660,43.212809029630442,4705.5029658868189,-3841.24678529421,null,null,null,{"$f":"IF(A265=\"new90.1-2004\",\"New Construction\",IF(A265=\"post1980\",\"Post 1980 Construction\",IF(A265=\"pre1980\",\"Pre 1980 Construction\")))","v":"New Construction"},"5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","40 fc","no-day","no-occ","red-epd","high-eff",194,99.3,9.4195463084281894E-2,0.14721526220932801,-3.0938538205980099E-2,930.35220000000027,-25.815019407392032,904.53718059260825,"no",5500,642.39,3030.15,null,24512.964500000002,113777.9645,245.12964500000001,0,5861.5022803967404,-660,45.226859029630418,5246.7291394263711,-4342.1919588337632,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","40 fc","no-day","yes-occ","base-epd","base-eff",211.75,93.86,5.6182613225567203E-2,6.9189854499098896E-2,2.55398671096345E-2,437.2572000000003,21.310385148383943,458.56758514838424,"no",5500,642.39,3030.15,null,23412.964500000002,81437.964500000002,234.12964500000001,0,5598.4719762311051,-660,22.928379257419213,4961.4003554885239,-4502.8327703401401,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","40 fc","no-day","yes-occ","base-epd","high-eff",210.27,93.86,6.0776358785735701E-2,7.5695634972965803E-2,2.55398671096345E-2,478.37159999999994,21.310385148383943,499.68198514838389,"no",5500,642.39,3030.15,null,25667.964500000002,114932.9645,256.67964500000005,0,6137.6840997706568,-660,24.984099257419196,5502.6681990280758,-5002.9862138796916,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","40 fc","no-day","yes-occ","red-epd","base-eff",180.94,105.12,0.11656432033087601,0.20462437909358699,-9.1362126245847303E-2,1293.1590000000006,-76.2322720755201,1216.9267279244805,"no",5500,642.39,3030.15,null,24237.964500000002,82262.964500000002,242.37964500000001,0,5795.744704355332,-660,60.846336396224025,5196.5910407515557,-3979.6643128270753,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","40 fc","no-day","yes-occ","red-epd","high-eff",179.63,105.12,0.120621339605664,0.21038287397248201,-9.1362126245847303E-2,1329.5508000000004,-76.2322720755201,1253.3185279244803,"no",5500,642.39,3030.15,null,26492.964500000002,115757.9645,264.92964500000005,0,6334.9568278948836,-660,62.665926396224023,5737.6227542911074,-4484.3042263666266,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","40 fc","yes-day","no-occ","base-epd","base-eff",203.45,96.4,7.3973510979209803E-2,0.105674974724164,-8.3056478405328605E-4,667.83120000000065,-0.69302065523210832,667.13817934476856,"no",5500,642.39,3030.15,null,24457.964500000002,98212.964500000002,244.57964500000003,0,5848.3507651884584,-660,33.356908967238432,5221.7076741556966,-4554.5694948109285,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","40 fc","yes-day","no-occ","base-epd","high-eff",202.05,96.4,7.8314679463905204E-2,0.11182909138863199,-8.3056478405328605E-4,706.72320000000002,-0.69302065523210832,706.03017934476793,"no",5500,642.39,3030.15,null,26712.964500000002,131707.9645,267.12964500000004,0,6387.56288872801,-660,35.301508967238398,5762.864397695248,-5056.8342183504801,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","40 fc","yes-day","no-occ","red-epd","base-eff",172.69,107.79,0.13378691966470399,0.24088970943777799,-0.119082225913621,1522.3440000000005,-99.361836443888109,1422.9821635561125,"no",5500,642.39,3030.15,null,25282.964500000002,99037.964500000002,252.82964500000003,0,6045.6234933126852,-660,71.14910817780563,5456.7726014904911,-4033.7904379343786,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","40 fc","yes-day","no-occ","red-epd","high-eff",171.46,107.79,0.13759136186401899,0.24629654050727501,-0.119082225913621,1556.5134000000003,-99.361836443888109,1457.1515635561123,"no",5500,642.39,3030.15,null,27537.964500000002,132532.9645,275.37964500000004,0,6584.8356168522369,-660,72.857578177805621,5997.6931950300423,-4540.5416314739305,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","40 fc","yes-day","yes-occ","base-epd","base-eff",193.53,100.59,9.1669692329549995E-2,0.149281287089542,-4.4331395348837302E-2,943.40880000000038,-36.989977473008082,906.41882252699224,"no",5500,642.39,3030.15,null,26437.964500000002,100192.9645,264.37964500000004,0,6321.8053126866016,-660,45.320941126349616,5707.1262538129513,-4800.7074312859586,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","40 fc","yes-day","yes-occ","base-epd","high-eff",192.22,100.59,9.5726711604338002E-2,0.15503978196843801,-4.4331395348837302E-2,979.80060000000037,-36.989977473008082,942.81062252699235,"no",5500,642.39,3030.15,null,28692.964500000002,133687.9645,286.92964500000005,0,6861.0174362261532,-660,47.140531126349622,6248.157967352503,-5305.3473448255108,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","40 fc","yes-day","yes-occ","red-epd","base-eff",162.77000000000001,112.23,0.150709583721408,0.28449602180315597,-0.16517857142857201,1797.9216000000001,-137.82448280926408,1660.0971171907361,"no",5500,642.39,3030.15,null,27262.964500000002,101017.9645,272.62964500000004,0,6519.0780408108276,-660,83.004855859536804,5942.0828966703648,-4281.9857794796289,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","40 fc","yes-day","yes-occ","red-epd","high-eff",161.62,112.23,0.15424566277803201,0.289551189063256,-0.16517857142857201,1829.8686000000002,-137.82448280926408,1692.0441171907362,"no",5500,642.39,3030.15,null,29517.964500000002,134512.9645,295.17964500000005,0,7058.2901643503801,-660,84.602205859536809,6482.8923702099173,-4790.8482530191814,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","25 fc","no-day","no-occ","base-epd","base-eff",211.75,93.86,5.6182613225567203E-2,6.9189854499098896E-2,2.55398671096345E-2,437.2572000000003,21.310385148383943,458.56758514838424,"no",5500,642.39,3030.15,null,22147.964500000002,129452.9645,221.47964500000003,0,5295.9871264406247,-1045,22.928379257419213,4273.9155056980435,-3815.3479205496592,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","25 fc","no-day","no-occ","base-epd","high-eff",210.27,93.86,6.0776358785735701E-2,7.5695634972965803E-2,2.55398671096345E-2,478.37159999999994,21.310385148383943,499.68198514838389,"no",5500,642.39,3030.15,null,24402.964500000002,162947.9645,244.02964500000002,0,5835.1992499801763,-1045,24.984099257419196,4815.1833492375954,-4315.5013640892112,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","25 fc","no-day","no-occ","red-epd","base-eff",180.94,105.12,0.11656432033087601,0.20462437909358699,-9.1362126245847303E-2,1293.1590000000006,-76.2322720755201,1216.9267279244805,"no",5500,642.39,3030.15,null,22972.964500000002,130277.9645,229.72964500000003,0,5493.2598545648507,-1045,60.846336396224025,4509.1061909610744,-3292.1794630365939,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","25 fc","no-day","no-occ","red-epd","high-eff",179.63,105.12,0.120621339605664,0.21038287397248201,-9.1362126245847303E-2,1329.5508000000004,-76.2322720755201,1253.3185279244803,"no",5500,642.39,3030.15,null,25227.964500000002,163772.9645,252.27964500000002,0,6032.4719781044023,-1045,62.665926396224023,5050.1379045006261,-3796.8193765761457,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","25 fc","no-day","yes-occ","base-epd","base-eff",200.35,98.38,7.7446445766966202E-2,0.119301947338345,-2.13870431893688E-2,753.94920000000047,-17.845281872224017,736.10391812777641,"no",5500,642.39,3030.15,null,24127.964500000002,131432.9645,241.27964500000002,0,5769.441673938768,-1045,36.805195906388825,4761.2468698451567,-4025.1429517173801,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","25 fc","no-day","yes-occ","base-epd","high-eff",198.96,98.38,8.1724469982793202E-2,0.12541210602663899,-2.13870431893688E-2,792.56340000000012,-17.845281872224017,774.71811812777605,"no",5500,642.39,3030.15,null,26382.964500000002,164927.9645,263.82964500000003,0,6308.6537974783196,-1045,38.735905906388808,5302.3897033847088,-4527.6715852569323,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","25 fc","no-day","yes-occ","red-epd","base-eff",169.54,109.96,0.13680205850316501,0.254736471932832,-0.14161129568106301,1609.8510000000006,-118.160021717056,1491.6909782829446,"no",5500,642.39,3030.15,null,24952.964500000002,132257.9645,249.52964500000002,0,5966.714402062993,-1045,74.584548914147234,4996.2989509771405,-3504.6079726941962,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","25 fc","no-day","yes-occ","red-epd","high-eff",168.33,109.96,0.14054335643361199,0.26005538704997999,-0.14161129568106301,1643.4648000000002,-118.160021717056,1525.3047782829442,"no",5500,642.39,3030.15,null,27207.964500000002,165752.9645,272.07964500000003,0,6505.9265256025465,-1045,76.265238914147218,5537.1917645166941,-4011.8869862337497,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","25 fc","yes-day","no-occ","base-epd","base-eff",193.53,100.59,9.1669692329549995E-2,0.149281287089542,-4.4331395348837302E-2,943.40880000000038,-36.989977473008082,906.41882252699224,"no",5500,642.39,3030.15,null,25172.964500000002,148207.9645,251.72964500000003,0,6019.3204628961212,-1045,45.320941126349616,5019.6414040224709,-4113.2225814954782,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","25 fc","yes-day","no-occ","base-epd","high-eff",192.22,100.59,9.5726711604338002E-2,0.15503978196843801,-4.4331395348837302E-2,979.80060000000037,-36.989977473008082,942.81062252699235,"no",5500,642.39,3030.15,null,27427.964500000002,181702.9645,274.27964500000002,0,6558.5325864356719,-1045,47.140531126349622,5560.6731175620216,-4617.8624950350295,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","25 fc","yes-day","no-occ","red-epd","base-eff",162.77000000000001,112.23,0.150709583721408,0.28449602180315597,-0.16517857142857201,1797.9216000000001,-137.82448280926408,1660.0971171907361,"no",5500,642.39,3030.15,null,25997.964500000002,149032.9645,259.979645,0,6216.5931910203471,-1045,83.004855859536804,5254.5980468798844,-3594.5009296891485,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","25 fc","yes-day","no-occ","red-epd","high-eff",161.62,112.23,0.15424566277803201,0.289551189063256,-0.16517857142857201,1829.8686000000002,-137.82448280926408,1692.0441171907362,"no",5500,642.39,3030.15,null,28252.964500000002,182527.9645,282.52964500000002,0,6755.8053145598988,-1045,84.602205859536809,5795.407520419436,-4103.3634032287,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","25 fc","yes-day","yes-occ","base-epd","base-eff",185.78,103.96,0.1052141380018,0.18334871862499499,-7.9318936877076404E-2,1158.7038000000002,-66.183472574655994,1092.5203274253442,"no",5500,642.39,3030.15,null,27152.964500000002,150187.9645,271.52964500000002,0,6492.7750103942644,-1045,54.626016371267212,5502.4010267655312,-4409.8806993401868,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","25 fc","yes-day","yes-occ","base-epd","high-eff",184.53,103.96,0.109065938402766,0.18884346564684201,-7.9318936877076404E-2,1193.4288000000004,-66.183472574655994,1127.2453274253444,"no",5500,642.39,3030.15,null,29407.964500000002,183682.9645,294.07964500000003,0,7031.987133933816,-1045,56.362266371267225,6043.3494003050837,-4916.1040728797398,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","25 fc","yes-day","yes-occ","red-epd","base-eff",155.02000000000001,115.75,0.163796233444362,0.31856345333860803,-0.20172342192691001,2013.2166000000002,-168.31739163947205,1844.8992083605281,"no",5500,642.39,3030.15,null,27977.964500000002,151012.9645,279.77964500000002,0,6690.0477385184895,-1045,92.244960418026409,5737.292698936516,-3892.3934905759879,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","25 fc","yes-day","yes-occ","red-epd","high-eff",153.93,115.75,0.16714287969438199,0.32335487274165903,-0.20172342192691001,2043.4968000000001,-168.31739163947205,1875.179408360528,"no",5500,642.39,3030.15,null,30232.964500000002,184507.9645,302.32964500000003,0,7229.2598620580429,-1045,93.758970418026408,6278.0188324760693,-4402.8394241155411,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","base-lpd","no-day","no-occ","base-epd","base-eff",223.22,87.78,3.9559884445988097E-2,1.87700558266298E-2,8.8662790697674299E-2,118.62060000000029,73.979954946015923,192.60055494601622,"no",5500,642.39,3030.15,null,21112.360199999999,94447.77,211.12360200000001,0,5048.3550227822243,0,9.6300277473008116,5057.9850505295253,-4865.3844955835093,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","base-lpd","no-day","no-occ","base-epd","high-eff",221.72,87.78,4.4169416073373699E-2,2.5363752252846299E-2,8.8662790697674299E-2,160.2906000000003,73.979954946015923,234.2705549460162,"no",5500,642.39,3030.15,null,23367.360199999999,127942.77,233.67360199999999,0,5587.5671463217759,0,11.713527747300811,5599.2806740690767,-5365.0101191230606,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","base-lpd","no-day","no-occ","red-epd","base-eff",192.41,98.93,0.100273098962855,0.15420458042111701,-2.70971760797344E-2,974.5224000000004,-22.609798876944119,951.91260112305633,"no",5500,642.39,3030.15,null,21937.360199999999,95272.77,219.37360200000001,0,5245.6277509064512,0,47.595630056152821,5293.2233809626041,-4341.3107798395476,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","base-lpd","no-day","no-occ","red-epd","high-eff",191.09,98.93,0.104345904304861,0.16000703327618801,-2.70971760797344E-2,1011.1920000000002,-22.609798876944119,988.58220112305617,"no",5500,642.39,3030.15,null,24192.360199999999,128767.77,241.92360199999999,0,5784.8398744460028,0,49.429110056152808,5834.2689845021559,-4845.6867833791002,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","base-lpd","no-day","yes-occ","base-epd","base-eff",208.64,93.47,6.6980283202046006E-2,8.2860785089454603E-2,2.95888704318936E-2,523.65300000000059,24.688860842639947,548.34186084264059,"no",5500,642.39,3030.15,null,23092.360199999999,96427.77,230.92360199999999,0,5521.8095702803676,0,27.417093042132031,5549.2266633224999,-5000.884802479859,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","base-lpd","no-day","yes-occ","base-epd","high-eff",207.28,93.47,7.1179377081787704E-2,8.8839069849224198E-2,2.95888704318936E-2,561.43380000000025,24.688860842639947,586.12266084264024,"no",5500,642.39,3030.15,null,25347.360199999999,129922.77,253.473602,0,6061.0216938199192,0,29.306133042132014,6090.3278268620516,-5504.2051660194111,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","base-lpd","no-day","yes-occ","red-epd","base-eff",177.84,104.95,0.126635831215369,0.21825135170776699,-8.9597176079734303E-2,1379.2770000000003,-74.75960318315208,1304.5173968168483,"no",5500,642.39,3030.15,null,23917.360199999999,97252.77,239.17360199999999,0,5719.0822984045935,0,65.225869840842421,5784.3081682454358,-4479.7907714285875,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","base-lpd","no-day","yes-occ","red-epd","high-eff",176.66,104.95,0.13029819880973101,0.223438392896391,-8.9597176079734303E-2,1412.0574000000006,-74.75960318315208,1337.2977968168484,"no",5500,642.39,3030.15,null,26172.360199999999,130747.77,261.72360199999997,0,6258.2944219441451,0,66.864889840842423,6325.1593117849879,-4987.8615149681391,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","base-lpd","yes-day","no-occ","base-epd","base-eff",200.42,96.08,8.4313385006393501E-2,0.118994241505121,2.4916943521594201E-3,752.00460000000066,2.0790619656959555,754.08366196569659,"no",5500,642.39,3030.15,null,24137.360199999999,113202.77,241.37360200000001,0,5771.6883592377208,0,37.70418309828483,5809.3925423360051,-5055.3088803703085,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","base-lpd","yes-day","no-occ","base-epd","high-eff",199.14,96.08,8.8259901810661998E-2,0.124620862455493,2.4916943521594201E-3,787.56300000000067,2.0790619656959555,789.6420619656966,"no",5500,642.39,3030.15,null,26392.360199999999,146697.77000000002,263.92360200000002,0,6310.9004827772724,0,39.482103098284831,6350.3825858755572,-5560.7405239098607,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","base-lpd","yes-day","no-occ","red-epd","base-eff",169.68,107.61,0.14362163954094101,0.25412106026638498,-0.117213455149502,1605.9618,-97.802539969616035,1508.1592600303841,"no",5500,642.39,3030.15,null,24962.360199999999,114027.77,249.62360200000001,0,5968.9610873619467,0,75.407963001519207,6044.3690503634662,-4536.2097903330823,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","base-lpd","yes-day","no-occ","red-epd","high-eff",168.58,107.61,0.14704721612704599,0.25895643764561099,-0.117213455149502,1636.5198,-97.802539969616035,1538.7172600303841,"no",5500,642.39,3030.15,null,27217.360199999999,147522.77000000002,272.17360200000002,0,6508.1732109014993,0,76.935863001519209,6585.1090739030187,-5046.3918138726349,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","base-lpd","yes-day","yes-occ","base-epd","base-eff",190.44,100.36,0.101930636020648,0.16286430172754901,-4.1943521594684501E-2,1029.2490000000005,-34.997543089216052,994.25145691078444,"no",5500,642.39,3030.15,null,26117.360199999999,115182.77,261.17360200000002,0,6245.142906735864,0,49.712572845539228,6294.8554795814034,-5300.6040226706191,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","base-lpd","yes-day","yes-occ","base-epd","high-eff",189.25,100.36,0.10560878968222601,0.168095300892347,-4.1943521594684501E-2,1062.3072000000004,-34.997543089216052,1027.3096569107843,"no",5500,642.39,3030.15,null,28372.360199999999,148677.77000000002,283.72360199999997,0,6784.3550302754156,0,51.365482845539219,6835.7205131209548,-5808.4108562101701,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","base-lpd","yes-day","yes-occ","red-epd","base-eff",159.69,112.21,0.160291726522172,0.298035078464988,-0.16497093023255799,1883.4840000000004,-137.65122764545598,1745.8327723545444,"no",5500,642.39,3030.15,null,26942.360199999999,116007.77,269.42360200000002,0,6442.41563486009,0,87.29163861772723,6529.7072734778176,-4783.8745011232731,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","base-lpd","yes-day","yes-occ","red-epd","high-eff",158.66999999999999,112.21,0.16346472603280399,0.30251879203481502,-0.16497093023255799,1911.8196000000007,-137.65122764545598,1774.1683723545448,"no",5500,642.39,3030.15,null,29197.360199999999,149502.77000000002,291.97360199999997,0,6981.6277583996416,0,88.708418617727247,7070.3361770173688,-5296.167804662824,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","40 fc","no-day","no-occ","base-epd","base-eff",223.22,87.78,3.9559884445988097E-2,1.87700558266298E-2,8.8662790697674299E-2,118.62060000000029,73.979954946015923,192.60055494601622,"no",5500,642.39,3030.15,null,24742.360199999999,105777.77,247.42360199999999,0,5916.3550265288204,-660,9.6300277473008116,5265.9850542761214,-5073.3844993301054,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","40 fc","no-day","no-occ","base-epd","high-eff",221.72,87.78,4.4169416073373699E-2,2.5363752252846299E-2,8.8662790697674299E-2,160.2906000000003,73.979954946015923,234.2705549460162,"no",5500,642.39,3030.15,null,26997.360199999999,139272.77000000002,269.97360199999997,0,6455.5671500683711,-660,11.713527747300811,5807.2806778156719,-5573.0101228696558,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","40 fc","no-day","no-occ","red-epd","base-eff",192.41,98.93,0.100273098962855,0.15420458042111701,-2.70971760797344E-2,974.5224000000004,-22.609798876944119,951.91260112305633,"no",5500,642.39,3030.15,null,25567.360199999999,106602.77,255.67360199999999,0,6113.6277546530455,-660,47.595630056152821,5501.2233847091984,-4549.310783586142,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","40 fc","no-day","no-occ","red-epd","high-eff",191.09,98.93,0.104345904304861,0.16000703327618801,-2.70971760797344E-2,1011.1920000000002,-22.609798876944119,988.58220112305617,"no",5500,642.39,3030.15,null,27822.360199999999,140097.77000000002,278.22360199999997,0,6652.839878192598,-660,49.429110056152808,6042.2689882487512,-5053.6867871256945,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","40 fc","no-day","yes-occ","base-epd","base-eff",208.64,93.47,6.6980283202046006E-2,8.2860785089454603E-2,2.95888704318936E-2,523.65300000000059,24.688860842639947,548.34186084264059,"no",5500,642.39,3030.15,null,26722.360199999999,107757.77,267.22360199999997,0,6389.8095740269628,-660,27.417093042132031,5757.2266670690951,-5208.8848062264542,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","40 fc","no-day","yes-occ","base-epd","high-eff",207.28,93.47,7.1179377081787704E-2,8.8839069849224198E-2,2.95888704318936E-2,561.43380000000025,24.688860842639947,586.12266084264024,"no",5500,642.39,3030.15,null,28977.360199999999,141252.77000000002,289.77360199999998,0,6929.0216975665153,-660,29.306133042132014,6298.3278306086477,-5712.2051697660072,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","40 fc","no-day","yes-occ","red-epd","base-eff",177.84,104.95,0.126635831215369,0.21825135170776699,-8.9597176079734303E-2,1379.2770000000003,-74.75960318315208,1304.5173968168483,"no",5500,642.39,3030.15,null,27547.360199999999,108582.77,275.47360199999997,0,6587.0823021511887,-660,65.225869840842421,5992.308171992031,-4687.7907751751827,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","40 fc","no-day","yes-occ","red-epd","high-eff",176.66,104.95,0.13029819880973101,0.223438392896391,-8.9597176079734303E-2,1412.0574000000006,-74.75960318315208,1337.2977968168484,"no",5500,642.39,3030.15,null,29802.360199999999,142077.77000000002,298.02360199999998,0,7126.2944256907413,-660,66.864889840842423,6533.1593155315841,-5195.8615187147352,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","40 fc","yes-day","no-occ","base-epd","base-eff",200.42,96.08,8.4313385006393501E-2,0.118994241505121,2.4916943521594201E-3,752.00460000000066,2.0790619656959555,754.08366196569659,"no",5500,642.39,3030.15,null,27767.360199999999,124532.77,277.67360200000002,0,6639.688362984316,-660,37.70418309828483,6017.3925460826013,-5263.3088841169047,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","40 fc","yes-day","no-occ","base-epd","high-eff",199.14,96.08,8.8259901810661998E-2,0.124620862455493,2.4916943521594201E-3,787.56300000000067,2.0790619656959555,789.6420619656966,"no",5500,642.39,3030.15,null,30022.360199999999,158027.77000000002,300.22360199999997,0,7178.9004865238676,-660,39.482103098284831,6558.3825896221524,-5768.7405276564559,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","40 fc","yes-day","no-occ","red-epd","base-eff",169.68,107.61,0.14362163954094101,0.25412106026638498,-0.117213455149502,1605.9618,-97.802539969616035,1508.1592600303841,"no",5500,642.39,3030.15,null,28592.360199999999,125357.77,285.92360200000002,0,6836.961091108542,-660,75.407963001519207,6252.3690541100614,-4744.2097940796775,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","40 fc","yes-day","no-occ","red-epd","high-eff",168.58,107.61,0.14704721612704599,0.25895643764561099,-0.117213455149502,1636.5198,-97.802539969616035,1538.7172600303841,"no",5500,642.39,3030.15,null,30847.360199999999,158852.77000000002,308.47360199999997,0,7376.1732146480945,-660,76.935863001519209,6793.1090776496139,-5254.3918176192301,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","40 fc","yes-day","yes-occ","base-epd","base-eff",190.44,100.36,0.101930636020648,0.16286430172754901,-4.1943521594684501E-2,1029.2490000000005,-34.997543089216052,994.25145691078444,"no",5500,642.39,3030.15,null,29747.360199999999,126512.77,297.47360199999997,0,7113.1429104824583,-660,49.712572845539228,6502.8554833279977,-5508.6040264172134,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","40 fc","yes-day","yes-occ","base-epd","high-eff",189.25,100.36,0.10560878968222601,0.168095300892347,-4.1943521594684501E-2,1062.3072000000004,-34.997543089216052,1027.3096569107843,"no",5500,642.39,3030.15,null,32002.360199999999,160007.77000000002,320.02360199999998,0,7652.3550340220118,-660,51.365482845539219,7043.7205168675509,-6016.4108599567662,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","40 fc","yes-day","yes-occ","red-epd","base-eff",159.69,112.21,0.160291726522172,0.298035078464988,-0.16497093023255799,1883.4840000000004,-137.65122764545598,1745.8327723545444,"no",5500,642.39,3030.15,null,30572.360199999999,127337.77,305.72360199999997,0,7310.4156386066852,-660,87.29163861772723,6737.7072772244128,-4991.8745048698684,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","40 fc","yes-day","yes-occ","red-epd","high-eff",158.66999999999999,112.21,0.16346472603280399,0.30251879203481502,-0.16497093023255799,1911.8196000000007,-137.65122764545598,1774.1683723545448,"no",5500,642.39,3030.15,null,32827.360199999996,160832.77000000002,328.27360199999998,0,7849.6277621462368,-660,88.708418617727247,7278.336180763964,-5504.1678084094192,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","25 fc","no-day","no-occ","base-epd","base-eff",208.64,93.47,6.6980283202046006E-2,8.2860785089454603E-2,2.95888704318936E-2,523.65300000000059,24.688860842639947,548.34186084264059,{"$f":"IF(P327>0.2,\"yes\",\"no\")","v":"no"},{"$f":"IF(B327=\"5500 ft2\",5500,IF(B327=\"10000 ft2\",10000,25000))","v":5500},{"$f":"IF(B327=\"5500 ft2\",IF(D327=\"stand-alone\",642.39,IF(D327=\"ad-e&flr\",522.37,402.25)),IF(B327=\"10000 ft2\",IF(D327=\"stand-alone\",866.06,IF(D327=\"ad-e&flr\",704.17,542.29)),IF(B327=\"25000 ft2\",IF(D327=\"stand-alone\",1369.38,IF(D327=\"ad-e&flr\",1113.42,857.45)))))","v":642.39},{"$f":"IF(B327=\"5500 ft2\",IF(D327=\"stand-alone\",3030.15,IF(D327=\"ad-e&flr\",2424.14,1818.13)),IF(B327=\"10000 ft2\",IF(D327=\"stand-alone\",4085.12,IF(D327=\"ad-e&flr\",3268.14,2451.05)),IF(B327=\"25000 ft2\",IF(D327=\"stand-alone\",6459.2,IF(D327=\"ad-e&flr\",5167.32,3875.54)))))","v":3030.15},null,{"$f":"SUM(IF(F327=\"eff-roof\",W327*IF(AND(W$4=\"no\",X$4=\"no\"),$C$4,$C$3)),IF(G327=\"eff-win\",X327*IF(W$4=\"no\",$D$4,$D$3),0),IF(H327=\"red-inf\",Y327*IF(W$4=\"no\",$F$4,$F$3),0),IF(I327=\"25 fc\",W327*IF(W$4=\"no\",$H$4,$H$3),0),IF(I327=\"40 fc\",W327*IF(W$4=\"no\",$G$4,$G$3),0),IF(J327=\"yes-day\",W327*IF(W$4=\"no\",$I$4,$I$3),0),IF(K327=\"yes-occ\",W327*IF(W$4=\"no\",$J$4,$J$3),0),IF(L327=\"red-epd\",W327*IF(W$4=\"no\",$K$4,$K$3),0),IF(AND(M327=\"high-eff\",C327=\"psz-ac\"),W327*IF(AND(W$4=\"no\",Y$4=\"no\"),$L$4,$L$3),0),IF(AND(M327=\"high-eff\",C327=\"ptac\"),W327*IF(AND(W$4=\"no\",Y$4=\"no\"),$M$4,$M$3),0),IF(AND(M327=\"high-eff\",C327=\"pthp\"),W327*IF(AND(W$4=\"no\",Y$4=\"no\"),$N$4,$N$3),0))","v":25457.360199999999},{"$f":"SUM(IF(F327=\"eff-roof\",W327*$C$4),IF(G327=\"eff-win\",X327*$D$4,0),IF(H327=\"red-inf\",Y327*$F$4,0),IF(I327=\"25 fc\",W327*$H$4,0),IF(I327=\"40 fc\",W327*$G$4,0),IF(J327=\"yes-day\",W327*$I$4,0),IF(K327=\"yes-occ\",W327*$J$4,0),IF(L327=\"red-epd\",W327*$K$4,0),IF(AND(M327=\"high-eff\",C327=\"psz-ac\"),W327*$L$4,0),IF(AND(M327=\"high-eff\",C327=\"ptac\"),W327*$M$4,0),IF(AND(M327=\"high-eff\",C327=\"pthp\"),W327*$N$4,0))","v":155772.77000000002},254.57360199999999,0,{"$f":"-PMT($AE$3,$AE$4,AA327+AC327-AD327)","v":6087.3247242364832},{"$f":"SUM(IF(F327=\"eff-roof\",($C$5*W327),0),IF(G327=\"eff-win\",($D$5*X327),0),IF(H327=\"red-inf\",$F$5*(Y327-X327),0),IF(I327=\"25 fc\",($H$5*W327),0),IF(I327=\"40 fc\",($G$5*W327),0),IF(J327=\"yes-day\",($I$5*W327),0),IF(K327=\"yes-occ\",($J$5*W327),0),IF(L327=\"red-epd\",($K$5*W327),0),IF(M327=\"high-eff\",($L$5*W327),0))","v":-1045},{"$f":"0.05*U327","v":27.417093042132031},5069.7418172786156,{"$f":"U327-AH327","v":-4521.3999564359747},null,null,null,"New Construction",{"$f":"IF(B327=\"5500 ft2\",\"5,500 SF\",IF(B327=\"10000 ft2\",\"10,000 SF\",IF(B327=\"25000 ft2\",\"25,000 SF\")))","v":"5,500 SF"},"Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration",{"$f":"IF(I327=\"base-lpd\",\"Baseline Lighting Levels\",IF(I327=\"40 fc\",\"Reduce Lighting Levels to 40 fc\",IF(I327=\"25 fc\",\"Reduce Lighting Levels to 25 fc\")))","v":"Reduce Lighting Levels to 25 fc"},"No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","25 fc","no-day","no-occ","base-epd","high-eff",207.28,93.47,7.1179377081787704E-2,8.8839069849224198E-2,2.95888704318936E-2,{"$f":"277.8*($N$7-N328)*$S$3","v":561.43380000000025},{"$f":"277.78*($O$7-O328)*$S$4","v":24.688860842639947},{"$f":"SUM(S328:T328)","v":586.12266084264024},"no",5500,642.39,3030.15,null,27712.360199999999,189267.77000000002,{"$f":"MIN(0.01*AA328,500)","v":277.12360200000001},{"$f":"IF(V328=\"yes\",0,0)","v":0},6626.5368477760348,-1045,29.306133042132014,{"$f":"SUM(AE328:AG328)","v":5610.8429808181672},-5024.7203199755268,null,null,null,"New Construction","5,500 SF",{"$f":"IF(C328=\"psz-ac\",\"Packaged Air Conditioner\",IF(C328=\"ptac\",\"Split System Air Conditioner\",IF(C328=\"pthp\",\"Split System Heat Pump\")))","v":"Packaged Air Conditioner"},{"$f":"IF(D328=\"stand-alone\",\"Stand Alone\",IF(D328=\"ad-e&flr\",\"Above Ground, 1 Side Attached\",IF(D328=\"ad-e&w&flr\",\"Above Ground, 2 Sides Attached\")))","v":"Stand Alone"},{"$f":"IF(F328=\"base-roof\",\"Baseline Roof Insulation\",IF(F328=\"eff-roof\",\"Increased Roof Insulation\"))","v":"Increased Roof Insulation"},{"$f":"IF(G328=\"base-win\",\"Baseline Windows\",IF(G328=\"eff-win\",\"Replace Windows\"))","v":"Replace Windows"},{"$f":"IF(H328=\"base-inf\",\"Baseline Infiltration\",IF(H328=\"red-inf\",\"Reduce Infiltration\"))","v":"Baseline Infiltration"},"Reduce Lighting Levels to 25 fc",{"$f":"IF(J328=\"no-day\",\"No Daylighting Sensors\",IF(J328=\"yes-day\",\"Install Daylighting Sensors\"))","v":"No Daylighting Sensors"},{"$f":"IF(K328=\"no-occ\",\"No Occupancy Sensors\",IF(K328=\"yes-occ\",\"Install Occupancy Sensors\"))","v":"No Occupancy Sensors"},{"$f":"IF(L328=\"base-epd\",\"No Plug Load Control\",IF(L328=\"red-epd\",\"Install Plug Load Controls\"))","v":"No Plug Load Control"},{"$f":"IF(M328=\"base-eff\",\"Baseline HVAC Equipment\",IF(M328=\"high-eff\",\"Install High Efficiency HVAC Equipment\"))","v":"Install High Efficiency HVAC Equipment"}]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","25 fc","no-day","no-occ","red-epd","base-eff",177.84,104.95,0.126635831215369,0.21825135170776699,-8.9597176079734303E-2,1379.2770000000003,-74.75960318315208,1304.5173968168483,"no",5500,642.39,3030.15,null,26282.360199999999,156597.77000000002,262.82360199999999,0,6284.5974523607092,-1045,65.225869840842421,5304.8233222015515,-4000.3059253847032,null,null,null,{"$f":"IF(A329=\"new90.1-2004\",\"New Construction\",IF(A329=\"post1980\",\"Post 1980 Construction\",IF(A329=\"pre1980\",\"Pre 1980 Construction\")))","v":"New Construction"},"5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","25 fc","no-day","no-occ","red-epd","high-eff",176.66,104.95,0.13029819880973101,0.223438392896391,-8.9597176079734303E-2,1412.0574000000006,-74.75960318315208,1337.2977968168484,"no",5500,642.39,3030.15,null,28537.360199999999,190092.77000000002,285.37360200000001,0,6823.8095759002608,-1045,66.864889840842423,5845.6744657411036,-4508.3766689242548,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","25 fc","no-day","yes-occ","base-epd","base-eff",197.24,98.07,8.7975752600754603E-2,0.1329728779287,-1.8168604651162799E-2,840.34500000000014,-15.159826833199999,825.18517316680015,"no",5500,642.39,3030.15,null,27437.360199999999,157752.77000000002,274.37360200000001,0,6560.7792717346256,-1045,41.259258658340009,5557.0385303929652,-4731.8533572261649,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","25 fc","no-day","yes-occ","base-epd","high-eff",195.98,98.07,9.1874911203372003E-2,0.138511582926722,-1.8168604651162799E-2,875.34780000000069,-15.159826833199999,860.1879731668007,"no",5500,642.39,3030.15,null,29692.360199999999,191247.77000000002,296.92360200000002,0,7099.9913952741772,-1045,43.009398658340039,6098.0007939325169,-5237.8128207657164,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","25 fc","no-day","yes-occ","red-epd","base-eff",166.45,109.85,0.146715708715488,0.26831948657083798,-0.14046926910299001,1695.6912000000009,-117.20711831611199,1578.4840816838889,"no",5500,642.39,3030.15,null,28262.360199999999,158577.77000000002,282.62360200000001,0,6758.0519998588525,-1045,78.924204084194457,5791.976203943047,-4213.4921222591584,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","25 fc","no-day","yes-occ","red-epd","high-eff",165.36,109.85,0.15007814103272499,0.27311090597388898,-0.14046926910299001,1725.9714000000001,-117.20711831611199,1608.7642816838882,"no",5500,642.39,3030.15,null,30517.360199999999,192072.77000000002,305.17360200000002,0,7297.2641233984032,-1045,80.438214084194414,6332.7023374825976,-4723.9380557987097,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","25 fc","yes-day","no-occ","base-epd","base-eff",190.44,100.36,0.101930636020648,0.16286430172754901,-4.1943521594684501E-2,1029.2490000000005,-34.997543089216052,994.25145691078444,"no",5500,642.39,3030.15,null,28482.360199999999,174527.77000000002,284.82360199999999,0,6810.6580606919797,-1045,49.712572845539228,5815.3706335375191,-4821.1191766267348,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","25 fc","yes-day","no-occ","base-epd","high-eff",189.25,100.36,0.10560878968222601,0.168095300892347,-4.1943521594684501E-2,1062.3072000000004,-34.997543089216052,1027.3096569107843,"no",5500,642.39,3030.15,null,30737.360199999999,208022.77000000002,307.37360200000001,0,7349.8701842315313,-1045,51.365482845539219,6356.2356670770705,-5328.9260101662858,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","25 fc","yes-day","no-occ","red-epd","base-eff",159.69,112.21,0.160291726522172,0.298035078464988,-0.16497093023255799,1883.4840000000004,-137.65122764545598,1745.8327723545444,"no",5500,642.39,3030.15,null,29307.360199999999,175352.77000000002,293.07360199999999,0,7007.9307888162057,-1045,87.29163861772723,6050.2224274339333,-4304.3896550793888,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","25 fc","yes-day","no-occ","red-epd","high-eff",158.66999999999999,112.21,0.16346472603280399,0.30251879203481502,-0.16497093023255799,1911.8196000000007,-137.65122764545598,1774.1683723545448,"no",5500,642.39,3030.15,null,31562.360199999999,208847.77000000002,315.62360200000001,0,7547.1429123557573,-1045,88.708418617727247,6590.8513309734844,-4816.6829586189397,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","25 fc","yes-day","yes-occ","base-epd","base-eff",182.69,103.78,0.11530143495351,0.19693173326300101,-7.7450166112956895E-2,1244.5440000000006,-64.624176100384062,1179.9198238996164,"no",5500,642.39,3030.15,null,30462.360199999999,176507.77000000002,304.62360200000001,0,7284.112608190122,-1045,58.995991194980824,6298.1085993851029,-5118.188775485487,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","25 fc","yes-day","yes-occ","base-epd","high-eff",181.56,103.78,0.118774369741266,0.20189898457075001,-7.7450166112956895E-2,1275.9354000000003,-64.624176100384062,1211.3112238996162,"no",5500,642.39,3030.15,null,32717.360199999999,210002.77000000002,327.17360200000002,0,7823.3247317296727,-1045,60.565561194980809,6838.8902929246533,-5627.5790690250369,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","25 fc","yes-day","yes-occ","red-epd","base-eff",151.94,115.8,0.17314158523687001,0.33210251000044,-0.202242524916944,2098.7790000000005,-168.75052954899201,1930.0284704510084,"no",5500,642.39,3030.15,null,31287.360199999999,177332.77000000002,312.87360200000001,0,7481.3853363143489,-1045,96.501423522550425,6532.8867598368997,-4602.8582893858911,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","25 fc","yes-day","yes-occ","red-epd","high-eff",150.97999999999999,115.8,0.17612515194089701,0.33632247571321799,-0.202242524916944,2125.4478000000008,-168.75052954899201,1956.6972704510088,"no",5500,642.39,3030.15,null,33542.360199999996,210827.77000000002,335.42360199999996,0,8020.5974598538996,-1045,97.834863522550449,7073.4323233764499,-5116.7350529254409,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","base-lpd","no-day","no-occ","base-epd","base-eff",223.13,86.24,4.45640677538005E-2,1.9165677612202801E-2,0.104651162790698,121.1208000000004,87.320602559231986,208.44140255923239,"no",5500,642.39,3030.15,null,22415.324699999997,95750.734500000006,224.15324699999996,0,5359.9178852840641,0,10.42207012796162,5370.339955412026,-5161.8985528527937,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","base-lpd","no-day","no-occ","base-epd","high-eff",221.63,86.24,4.9205171515620399E-2,2.5759374038419301E-2,0.104651162790698,162.79080000000039,87.320602559231986,250.11140255923237,"no",5500,642.39,3030.15,null,24670.324699999997,129245.73450000001,246.70324699999998,0,5899.1300088236167,0,12.505570127961619,5911.6355789515783,-5661.5241763923459,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","base-lpd","no-day","no-occ","red-epd","base-eff",192.33,97.24,0.105719292152746,0.154556244230516,-9.5514950166113097E-3,976.74480000000005,-7.9697375351680142,968.77506246483199,"no",5500,642.39,3030.15,null,23240.324699999997,96575.734500000006,232.40324699999996,0,5557.190613408291,0,48.438753123241604,5605.6293665315325,-4636.8543040667009,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","base-lpd","no-day","no-occ","red-epd","high-eff",191.01,97.24,0.10980788356196799,0.160358697085586,-9.5514950166113097E-3,1013.4144000000006,-7.9697375351680142,1005.4446624648325,"no",5500,642.39,3030.15,null,25495.324699999997,130070.73450000001,254.95324699999998,0,6096.4027369478426,0,50.272233123241627,6146.6749700710843,-5141.2303076062517,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","base-lpd","no-day","yes-occ","base-epd","base-eff",208.56,91.9,7.2094968980377996E-2,8.3212448898852695E-2,4.5888704318936699E-2,525.87540000000024,38.289391201567888,564.16479120156816,"no",5500,642.39,3030.15,null,24395.324699999997,97730.734500000006,243.95324699999998,0,5833.3724327822083,0,28.208239560078411,5861.5806723422866,-5297.4158811407187,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","base-lpd","no-day","yes-occ","base-epd","high-eff",207.2,91.9,7.6294062860119694E-2,8.9190733658622401E-2,4.5888704318936699E-2,563.65620000000069,38.289391201567888,601.94559120156862,"no",5500,642.39,3030.15,null,26650.324699999997,131225.73450000002,266.50324699999999,0,6372.5845563217599,0,30.097279560078434,6402.6818358818382,-5800.7362446802699,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","base-lpd","no-day","yes-occ","red-epd","base-eff",177.77,103.24,0.13217674080856201,0.218559057540991,-7.1843853820598005E-2,1381.2216000000001,-59.946286677568011,1321.2753133224321,"no",5500,642.39,3030.15,null,25220.324699999997,98555.734500000006,252.20324699999998,0,6030.6451609064343,0,66.063765666121611,6096.7089265725563,-4775.4336132501239,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","base-lpd","no-day","yes-occ","red-epd","high-eff",176.58,103.24,0.13583910840292401,0.223790056705789,-7.1843853820598005E-2,1414.2798,-59.946286677568011,1354.3335133224321,"no",5500,642.39,3030.15,null,27475.324699999997,132050.73450000002,274.75324699999999,0,6569.8572844459859,0,67.716675666121603,6637.5739601121077,-5283.2404467896758,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","base-lpd","yes-day","no-occ","base-epd","base-eff",200.33,94.49,8.9491215053593795E-2,0.119389863290694,1.8999169435215901E-2,754.50480000000005,15.852847488431983,770.35764748843201,"no",5500,642.39,3030.15,null,25440.324699999997,114505.73450000001,254.40324699999999,0,6083.2512217395606,0,38.517882374421603,6121.7691041139824,-5351.4114566255503,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","base-lpd","yes-day","no-occ","base-epd","high-eff",199.05,94.49,9.3453517925079402E-2,0.12501648424106601,1.8999169435215901E-2,790.06320000000005,15.852847488431983,805.91604748843201,"no",5500,642.39,3030.15,null,27695.324699999997,148000.73450000002,276.95324699999998,0,6622.4633452791131,0,40.295802374421605,6662.7591476535345,-5856.8431001651024,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","base-lpd","yes-day","no-occ","red-epd","base-eff",169.6,105.9,0.14917833520135099,0.25447272407578397,-9.9460132890365593E-2,1608.1842000000006,-82.989223464032094,1525.1949765359684,"no",5500,642.39,3030.15,null,26265.324699999997,115330.73450000001,262.65324699999996,0,6280.5239498637875,0,76.259748826798429,6356.7836986905859,-4831.5887221546172,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","base-lpd","yes-day","no-occ","red-epd","high-eff",168.49,105.9,0.152603911787456,0.259352059431184,-9.9460132890365593E-2,1639.0200000000002,-82.989223464032094,1556.030776535968,"no",5500,642.39,3030.15,null,28520.324699999997,148825.73450000002,285.20324699999998,0,6819.7360734033391,0,77.801538826798406,6897.5376122301377,-5341.5068356941701,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","base-lpd","yes-day","yes-occ","base-epd","base-eff",190.35,98.77,0.107108466067849,0.16325992351312199,-2.54360465116279E-2,1031.7492000000004,-21.223757566480021,1010.5254424335204,"no",5500,642.39,3030.15,null,27420.324699999997,116485.73450000001,274.20324699999998,0,6556.7057692377048,0,50.526272121676023,6607.2320413593807,-5596.7065989258599,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","base-lpd","yes-day","yes-occ","base-epd","high-eff",189.16,98.77,0.11078661972942699,0.16849092267792001,-2.54360465116279E-2,1064.8074000000004,-21.223757566480021,1043.5836424335203,"no",5500,642.39,3030.15,null,29675.324699999997,149980.73450000002,296.75324699999999,0,7095.9178927772564,0,52.179182121676014,7148.0970748989321,-6104.5134324654118,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","base-lpd","yes-day","yes-occ","red-epd","base-eff",159.61000000000001,110.51,0.165785277913713,0.298386742274386,-0.14732142857142899,1885.7064,-122.92453872177609,1762.7818612782239,"no",5500,642.39,3030.15,null,28245.324699999997,117310.73450000001,282.45324699999998,0,6753.9784973619298,0,88.139093063911204,6842.1175904258407,-5079.3357291476168,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","base-lpd","yes-day","yes-occ","red-epd","high-eff",158.59,110.51,0.16895827742434499,0.30287045584421302,-0.14732142857142899,1914.0420000000004,-122.92453872177609,1791.1174612782243,"no",5500,642.39,3030.15,null,30500.324699999997,150805.73450000002,305.00324699999999,0,7293.1906209014824,0,89.555873063911221,7382.7464939653937,-5591.6290326871695,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","40 fc","no-day","no-occ","base-epd","base-eff",223.13,86.24,4.45640677538005E-2,1.9165677612202801E-2,0.104651162790698,121.1208000000004,87.320602559231986,208.44140255923239,"no",5500,642.39,3030.15,null,26045.324699999997,107080.73450000001,260.45324699999998,0,6227.9178890306603,-660,10.42207012796162,5578.3399591586222,-5369.8985565993898,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","40 fc","no-day","no-occ","base-epd","high-eff",221.63,86.24,4.9205171515620399E-2,2.5759374038419301E-2,0.104651162790698,162.79080000000039,87.320602559231986,250.11140255923237,"no",5500,642.39,3030.15,null,28300.324699999997,140575.73450000002,283.00324699999999,0,6767.1300125702119,-660,12.505570127961619,6119.6355826981735,-5869.5241801389411,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","40 fc","no-day","no-occ","red-epd","base-eff",192.33,97.24,0.105719292152746,0.154556244230516,-9.5514950166113097E-3,976.74480000000005,-7.9697375351680142,968.77506246483199,"no",5500,642.39,3030.15,null,26870.324699999997,107905.73450000001,268.70324699999998,0,6425.1906171548871,-660,48.438753123241604,5813.6293702781286,-4844.8543078132971,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","40 fc","no-day","no-occ","red-epd","high-eff",191.01,97.24,0.10980788356196799,0.160358697085586,-9.5514950166113097E-3,1013.4144000000006,-7.9697375351680142,1005.4446624648325,"no",5500,642.39,3030.15,null,29125.324699999997,141400.73450000002,291.25324699999999,0,6964.4027406944388,-660,50.272233123241627,6354.6749738176804,-5349.2303113528478,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","40 fc","no-day","yes-occ","base-epd","base-eff",208.56,91.9,7.2094968980377996E-2,8.3212448898852695E-2,4.5888704318936699E-2,525.87540000000024,38.289391201567888,564.16479120156816,"no",5500,642.39,3030.15,null,28025.324699999997,109060.73450000001,280.25324699999999,0,6701.3724365288035,-660,28.208239560078411,6069.5806760888818,-5505.415884887314,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","40 fc","no-day","yes-occ","base-epd","high-eff",207.2,91.9,7.6294062860119694E-2,8.9190733658622401E-2,4.5888704318936699E-2,563.65620000000069,38.289391201567888,601.94559120156862,"no",5500,642.39,3030.15,null,30280.324699999997,142555.73450000002,302.803247,0,7240.5845600683551,-660,30.097279560078434,6610.6818396284334,-6008.7362484268651,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","40 fc","no-day","yes-occ","red-epd","base-eff",177.77,103.24,0.13217674080856201,0.218559057540991,-7.1843853820598005E-2,1381.2216000000001,-59.946286677568011,1321.2753133224321,"no",5500,642.39,3030.15,null,28850.324699999997,109885.73450000001,288.50324699999999,0,6898.6451646530295,-660,66.063765666121611,6304.7089303191515,-4983.4336169967191,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","40 fc","no-day","yes-occ","red-epd","high-eff",176.58,103.24,0.13583910840292401,0.223790056705789,-7.1843853820598005E-2,1414.2798,-59.946286677568011,1354.3335133224321,"no",5500,642.39,3030.15,null,31105.324699999997,143380.73450000002,311.053247,0,7437.8572881925811,-660,67.716675666121603,6845.5739638587029,-5491.2404505362711,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","40 fc","yes-day","no-occ","base-epd","base-eff",200.33,94.49,8.9491215053593795E-2,0.119389863290694,1.8999169435215901E-2,754.50480000000005,15.852847488431983,770.35764748843201,"no",5500,642.39,3030.15,null,29070.324699999997,125835.73450000001,290.70324699999998,0,6951.2512254861567,-660,38.517882374421603,6329.7691078605785,-5559.4114603721464,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","40 fc","yes-day","no-occ","base-epd","high-eff",199.05,94.49,9.3453517925079402E-2,0.12501648424106601,1.8999169435215901E-2,790.06320000000005,15.852847488431983,805.91604748843201,"no",5500,642.39,3030.15,null,31325.324699999997,159330.73450000002,313.25324699999999,0,7490.4633490257083,-660,40.295802374421605,6870.7591514001297,-6064.8431039116977,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","40 fc","yes-day","no-occ","red-epd","base-eff",169.6,105.9,0.14917833520135099,0.25447272407578397,-9.9460132890365593E-2,1608.1842000000006,-82.989223464032094,1525.1949765359684,"no",5500,642.39,3030.15,null,29895.324699999997,126660.73450000001,298.95324699999998,0,7148.5239536103836,-660,76.259748826798429,6564.783702437182,-5039.5887259012134,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","40 fc","yes-day","no-occ","red-epd","high-eff",168.49,105.9,0.152603911787456,0.259352059431184,-9.9460132890365593E-2,1639.0200000000002,-82.989223464032094,1556.030776535968,"no",5500,642.39,3030.15,null,32150.324699999997,160155.73450000002,321.50324699999999,0,7687.7360771499352,-660,77.801538826798406,7105.5376159767338,-5549.5068394407663,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","40 fc","yes-day","yes-occ","base-epd","base-eff",190.35,98.77,0.107108466067849,0.16325992351312199,-2.54360465116279E-2,1031.7492000000004,-21.223757566480021,1010.5254424335204,"no",5500,642.39,3030.15,null,31050.324699999997,127815.73450000001,310.50324699999999,0,7424.7057729843,-660,50.526272121676023,6815.2320451059759,-5804.7066026724551,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","40 fc","yes-day","yes-occ","base-epd","high-eff",189.16,98.77,0.11078661972942699,0.16849092267792001,-2.54360465116279E-2,1064.8074000000004,-21.223757566480021,1043.5836424335203,"no",5500,642.39,3030.15,null,33305.324699999997,161310.73450000002,333.053247,0,7963.9178965238516,-660,52.179182121676014,7356.0970786455273,-6312.513436212007,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","40 fc","yes-day","yes-occ","red-epd","base-eff",159.61000000000001,110.51,0.165785277913713,0.298386742274386,-0.14732142857142899,1885.7064,-122.92453872177609,1762.7818612782239,"no",5500,642.39,3030.15,null,31875.324699999997,128640.73450000001,318.75324699999999,0,7621.978501108526,-660,88.139093063911204,7050.1175941724368,-5287.3357328942129,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","40 fc","yes-day","yes-occ","red-epd","high-eff",158.59,110.51,0.16895827742434499,0.30287045584421302,-0.14732142857142899,1914.0420000000004,-122.92453872177609,1791.1174612782243,"no",5500,642.39,3030.15,null,34130.324699999997,162135.73450000002,341.303247,0,8161.1906246480776,-660,89.555873063911221,7590.7464977119889,-5799.6290364337647,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","25 fc","no-day","no-occ","base-epd","base-eff",208.56,91.9,7.2094968980377996E-2,8.3212448898852695E-2,4.5888704318936699E-2,525.87540000000024,38.289391201567888,564.16479120156816,"no",5500,642.39,3030.15,null,26760.324699999997,157075.73450000002,267.60324699999995,0,6398.8875867383231,-1045,28.208239560078411,5382.0958262984013,-4817.9310350968335,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","25 fc","no-day","no-occ","base-epd","high-eff",207.2,91.9,7.6294062860119694E-2,8.9190733658622401E-2,4.5888704318936699E-2,563.65620000000069,38.289391201567888,601.94559120156862,"no",5500,642.39,3030.15,null,29015.324699999997,190570.73450000002,290.15324699999996,0,6938.0997102778747,-1045,30.097279560078434,5923.196989837953,-5321.2513986363847,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","25 fc","no-day","no-occ","red-epd","base-eff",177.77,103.24,0.13217674080856201,0.218559057540991,-7.1843853820598005E-2,1381.2216000000001,-59.946286677568011,1321.2753133224321,"no",5500,642.39,3030.15,null,27585.324699999997,157900.73450000002,275.85324699999995,0,6596.1603148625481,-1045,66.063765666121611,5617.2240805286701,-4295.9487672062378,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","25 fc","no-day","no-occ","red-epd","high-eff",176.58,103.24,0.13583910840292401,0.223790056705789,-7.1843853820598005E-2,1414.2798,-59.946286677568011,1354.3335133224321,"no",5500,642.39,3030.15,null,29840.324699999997,191395.73450000002,298.40324699999996,0,7135.3724384021007,-1045,67.716675666121603,6158.0891140682224,-4803.7556007457906,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","25 fc","no-day","yes-occ","base-epd","base-eff",197.17,96.44,9.3232512984040394E-2,0.133280583761924,-1.2458471760797799E-3,842.28960000000063,-1.0395309828480395,841.25006901715255,"no",5500,642.39,3030.15,null,28740.324699999997,159055.73450000002,287.40324699999996,0,6872.3421342364654,-1045,42.062503450857633,5869.404637687323,-5028.1545686701702,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","25 fc","no-day","yes-occ","base-epd","high-eff",195.91,96.44,9.7115885519440504E-2,0.13881928875994601,-1.2458471760797799E-3,877.2924000000005,-1.0395309828480395,876.25286901715242,"no",5500,642.39,3030.15,null,30995.324699999997,192550.73450000002,309.95324699999998,0,7411.5542577760179,-1045,43.812643450857621,6410.3669012268756,-5534.1140322097235,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","25 fc","no-day","yes-occ","red-epd","base-eff",166.39,108.1,0.15228819044311501,0.26858323442788701,-0.122300664451827,1697.3580000000006,-102.047291482912,1595.3107085170886,"no",5500,642.39,3030.15,null,29565.324699999997,159880.73450000002,295.65324699999996,0,7069.6148623606914,-1045,79.765535425854438,6104.3803977865455,-4509.0696892694568,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","25 fc","no-day","yes-occ","red-epd","high-eff",165.3,108.1,0.15565062276035199,0.27337465383093801,-0.122300664451827,1727.6382000000003,-102.047291482912,1625.5909085170883,"no",5500,642.39,3030.15,null,31820.324699999997,193375.73450000002,318.20324699999998,0,7608.8269859002439,-1045,81.279545425854423,6645.1065313260988,-5019.5156228090109,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","25 fc","yes-day","no-occ","base-epd","base-eff",190.35,98.77,0.107108466067849,0.16325992351312199,-2.54360465116279E-2,1031.7492000000004,-21.223757566480021,1010.5254424335204,"no",5500,642.39,3030.15,null,29785.324699999997,175830.73450000002,297.85324699999995,0,7122.2209231938195,-1045,50.526272121676023,6127.7471953154954,-5117.2217528819747,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","25 fc","yes-day","no-occ","base-epd","high-eff",189.16,98.77,0.11078661972942699,0.16849092267792001,-2.54360465116279E-2,1064.8074000000004,-21.223757566480021,1043.5836424335203,"no",5500,642.39,3030.15,null,32040.324699999997,209325.73450000002,320.40324699999996,0,7661.4330467333712,-1045,52.179182121676014,6668.6122288550469,-5625.0285864215266,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","25 fc","yes-day","no-occ","red-epd","base-eff",159.61000000000001,110.51,0.165785277913713,0.298386742274386,-0.14732142857142899,1885.7064,-122.92453872177609,1762.7818612782239,"no",5500,642.39,3030.15,null,30610.324699999997,176655.73450000002,306.10324699999995,0,7319.4936513180446,-1045,88.139093063911204,6362.6327443819555,-4599.8508831037316,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","25 fc","yes-day","no-occ","red-epd","high-eff",158.59,110.51,0.16895827742434499,0.30287045584421302,-0.14732142857142899,1914.0420000000004,-122.92453872177609,1791.1174612782243,"no",5500,642.39,3030.15,null,32865.324699999997,210150.73450000002,328.65324699999996,0,7858.705774857598,-1045,89.555873063911221,6903.2616479215094,-5112.1441866432851,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","25 fc","yes-day","yes-occ","base-epd","base-eff",182.62,102.16,0.120526623202362,0.19723943909622399,-6.06312292358804E-2,1246.4886000000004,-50.590507831936023,1195.8980921680643,"no",5500,642.39,3030.15,null,31765.324699999997,177810.73450000002,317.65324699999996,0,7595.6754706919619,-1045,59.794904608403215,6610.470375300365,-5414.572283132301,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","25 fc","yes-day","yes-occ","base-epd","high-eff",181.49,102.16,0.124015344057335,0.20220669040397399,-6.06312292358804E-2,1277.8800000000001,-50.590507831936023,1227.289492168064,"no",5500,642.39,3030.15,null,34020.324699999997,211305.73450000002,340.20324699999998,0,8134.8875942315144,-1045,61.364474608403206,7151.2520688399172,-5923.9625766718527,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","25 fc","yes-day","yes-occ","red-epd","base-eff",151.88,114.04,0.17876142516614801,0.33236625785748802,-0.183970099667774,2100.4458000000009,-153.50407513388811,1946.9417248661127,"no",5500,642.39,3030.15,null,32590.324699999997,178635.73450000002,325.90324699999996,0,7792.9481988161888,-1045,97.34708624330564,6845.2952850594947,-4898.3535601933818,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","stand-alone","new90.1-20045500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","25 fc","yes-day","yes-occ","red-epd","high-eff",150.91,114.04,0.18174499187017501,0.33663018154644198,-0.183970099667774,2127.3924000000002,-153.50407513388811,1973.888324866112,"no",5500,642.39,3030.15,null,34845.324699999997,212130.73450000002,348.45324699999998,0,8332.1603223557413,-1045,98.694416243305611,7385.8547385990469,-5411.9664137329346,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flrbaseline",null,null,null,null,null,null,null,null,253.96,80.680000000000007,null,null,null,{"$f":"277.8*($N$391-N391)*$S$3","v":0},{"$f":"277.78*($O$391-O391)*$S$4","v":0},0,{"$f":"IF(P391>0.2,\"yes\",\"no\")","v":"no"},{"$f":"IF(B391=\"5500 ft2\",5500,IF(B391=\"10000 ft2\",10000,25000))","v":5500},{"$f":"IF(B391=\"5500 ft2\",IF(D391=\"stand-alone\",642.39,IF(D391=\"ad-e&flr\",522.37,402.25)),IF(B391=\"10000 ft2\",IF(D391=\"stand-alone\",866.06,IF(D391=\"ad-e&flr\",704.17,542.29)),IF(B391=\"25000 ft2\",IF(D391=\"stand-alone\",1369.38,IF(D391=\"ad-e&flr\",1113.42,857.45)))))","v":522.37},{"$f":"IF(B391=\"5500 ft2\",IF(D391=\"stand-alone\",3030.15,IF(D391=\"ad-e&flr\",2424.14,1818.13)),IF(B391=\"10000 ft2\",IF(D391=\"stand-alone\",4085.12,IF(D391=\"ad-e&flr\",3268.14,2451.05)),IF(B391=\"25000 ft2\",IF(D391=\"stand-alone\",6459.2,IF(D391=\"ad-e&flr\",5167.32,3875.54)))))","v":2424.14},null,{"$f":"SUM(IF(F391=\"eff-roof\",W391*IF(AND(W$4=\"no\",X$4=\"no\"),$C$4,$C$3)),IF(G391=\"eff-win\",X391*IF(W$4=\"no\",$D$4,$D$3),0),IF(H391=\"red-inf\",Y391*IF(W$4=\"no\",$F$4,$F$3),0),IF(I391=\"25 fc\",W391*IF(W$4=\"no\",$H$4,$H$3),0),IF(I391=\"40 fc\",W391*IF(W$4=\"no\",$G$4,$G$3),0),IF(J391=\"yes-day\",W391*IF(W$4=\"no\",$I$4,$I$3),0),IF(K391=\"yes-occ\",W391*IF(W$4=\"no\",$J$4,$J$3),0),IF(L391=\"red-epd\",W391*IF(W$4=\"no\",$K$4,$K$3),0),IF(AND(M391=\"high-eff\",C391=\"psz-ac\"),W391*IF(AND(W$4=\"no\",Y$4=\"no\"),$L$4,$L$3),0),IF(AND(M391=\"high-eff\",C391=\"ptac\"),W391*IF(AND(W$4=\"no\",Y$4=\"no\"),$M$4,$M$3),0),IF(AND(M391=\"high-eff\",C391=\"pthp\"),W391*IF(AND(W$4=\"no\",Y$4=\"no\"),$N$4,$N$3),0))","v":0},{"$f":"SUM(IF(F391=\"eff-roof\",W391*$C$4),IF(G391=\"eff-win\",X391*$D$4,0),IF(H391=\"red-inf\",Y391*$F$4,0),IF(I391=\"25 fc\",W391*$H$4,0),IF(I391=\"40 fc\",W391*$G$4,0),IF(J391=\"yes-day\",W391*$I$4,0),IF(K391=\"yes-occ\",W391*$J$4,0),IF(L391=\"red-epd\",W391*$K$4,0),IF(AND(M391=\"high-eff\",C391=\"psz-ac\"),W391*$L$4,0),IF(AND(M391=\"high-eff\",C391=\"ptac\"),W391*$M$4,0),IF(AND(M391=\"high-eff\",C391=\"pthp\"),W391*$N$4,0))","v":0},0,0,{"$f":"-PMT($AE$3,$AE$4,AA391+AC391-AD391)","v":0},{"$f":"SUM(IF(F391=\"eff-roof\",($C$5*W391),0),IF(G391=\"eff-win\",($D$5*X391),0),IF(H391=\"red-inf\",$F$5*(Y391-X391),0),IF(I391=\"25 fc\",($H$5*W391),0),IF(I391=\"40 fc\",($G$5*W391),0),IF(J391=\"yes-day\",($I$5*W391),0),IF(K391=\"yes-occ\",($J$5*W391),0),IF(L391=\"red-epd\",($K$5*W391),0),IF(M391=\"high-eff\",($L$5*W391),0))","v":0},{"$f":"0.05*U391","v":0},0,{"$f":"U391-AH391","v":0},null,null,null,"New Construction",{"$f":"IF(B391=\"5500 ft2\",\"5,500 SF\",IF(B391=\"10000 ft2\",\"10,000 SF\",IF(B391=\"25000 ft2\",\"25,000 SF\")))","v":"5,500 SF"},"Packaged Air Conditioner","Above Ground, 1 Side Attached",false,false,false,{"$f":"IF(I391=\"base-lpd\",\"Baseline Lighting Levels\",IF(I391=\"40 fc\",\"Reduce Lighting Levels to 40 fc\",IF(I391=\"25 fc\",\"Reduce Lighting Levels to 25 fc\")))","v":false},false,false,false,false]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","base-lpd","no-day","no-occ","base-epd","high-eff",250.75,80.680000000000007,9.5774906058106197E-3,1.2639785793038301E-2,0,{"$f":"277.8*($N$391-N392)*$S$3","v":89.173800000000227},{"$f":"277.78*($O$391-O392)*$S$4","v":0},{"$f":"SUM(S392:T392)","v":89.173800000000227},"no",5500,522.37,2424.14,null,2255,33495,{"$f":"MIN(0.01*AA392,500)","v":22.55},{"$f":"IF(V392=\"yes\",0,0)","v":0},539.21212353955184,0,4.4586900000000114,{"$f":"SUM(AE392:AG392)","v":543.67081353955189},-454.49701353955163,null,null,null,"New Construction","5,500 SF",{"$f":"IF(C392=\"psz-ac\",\"Packaged Air Conditioner\",IF(C392=\"ptac\",\"Split System Air Conditioner\",IF(C392=\"pthp\",\"Split System Heat Pump\")))","v":"Packaged Air Conditioner"},{"$f":"IF(D392=\"stand-alone\",\"Stand Alone\",IF(D392=\"ad-e&flr\",\"Above Ground, 1 Side Attached\",IF(D392=\"ad-e&w&flr\",\"Above Ground, 2 Sides Attached\")))","v":"Above Ground, 1 Side Attached"},{"$f":"IF(F392=\"base-roof\",\"Baseline Roof Insulation\",IF(F392=\"eff-roof\",\"Increased Roof Insulation\"))","v":"Baseline Roof Insulation"},{"$f":"IF(G392=\"base-win\",\"Baseline Windows\",IF(G392=\"eff-win\",\"Replace Windows\"))","v":"Baseline Windows"},{"$f":"IF(H392=\"base-inf\",\"Baseline Infiltration\",IF(H392=\"red-inf\",\"Reduce Infiltration\"))","v":"Baseline Infiltration"},"Baseline Lighting Levels",{"$f":"IF(J392=\"no-day\",\"No Daylighting Sensors\",IF(J392=\"yes-day\",\"Install Daylighting Sensors\"))","v":"No Daylighting Sensors"},{"$f":"IF(K392=\"no-occ\",\"No Occupancy Sensors\",IF(K392=\"yes-occ\",\"Install Occupancy Sensors\"))","v":"No Occupancy Sensors"},{"$f":"IF(L392=\"base-epd\",\"No Plug Load Control\",IF(L392=\"red-epd\",\"Install Plug Load Controls\"))","v":"No Plug Load Control"},{"$f":"IF(M392=\"base-eff\",\"Baseline HVAC Equipment\",IF(M392=\"high-eff\",\"Install High Efficiency HVAC Equipment\"))","v":"Install High Efficiency HVAC Equipment"}]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","base-lpd","no-day","no-occ","red-epd","base-eff",220.7,94.66,5.7602419576573999E-2,0.13096550637895699,-0.17327714427367399,923.9628000000007,-121.1053595017919,802.8574404982088,"no",5500,522.37,2424.14,null,825,825,8.25,0,197.27272812422629,0,40.142872024910446,237.41560014913674,565.44184034907209,null,null,null,{"$f":"IF(A393=\"new90.1-2004\",\"New Construction\",IF(A393=\"post1980\",\"Post 1980 Construction\",IF(A393=\"pre1980\",\"Pre 1980 Construction\")))","v":"New Construction"},"5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","base-lpd","no-day","no-occ","red-epd","high-eff",217.93,94.66,6.5866251183820598E-2,0.14187273586391599,-0.17327714427367399,1000.9134,-121.1053595017919,879.80804049820813,"no",5500,522.37,2424.14,null,3080,34320,30.8,0,736.48485166377816,0,43.990402024910409,780.47525368868855,99.332786809519575,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","base-lpd","no-day","yes-occ","base-epd","base-eff",238.17,87.17,2.77854153300949E-2,6.2175145692235097E-2,-8.0441249380267699E-2,438.64620000000059,-56.221300655695956,382.42489934430466,"no",5500,522.37,2424.14,null,1980,1980,19.8,0,473.45454749814303,0,19.121244967215233,492.57579246535829,-110.15089312105363,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","base-lpd","no-day","yes-occ","base-epd","high-eff",235.2,87.17,3.6644976018085702E-2,7.3869900771775202E-2,-8.0441249380267699E-2,521.15280000000064,-56.221300655695956,464.93149934430471,"no",5500,522.37,2424.14,null,4235,35475,42.35,0,1012.666671037695,0,23.246574967215238,1035.9132460049102,-570.98174666060549,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","base-lpd","no-day","yes-occ","red-epd","base-eff",205.03,101.89,8.2821617328078606E-2,0.19266813671444299,-0.26289043133366402,1359.2754000000004,-183.73710121838394,1175.5382987816165,"no",5500,522.37,2424.14,null,2805,2805,28.05,0,670.72727562236935,0,58.776914939080825,729.50419056145017,446.03410822016633,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","base-lpd","no-day","yes-occ","red-epd","high-eff",202.48,101.89,9.0428619436042995E-2,0.202709088045362,-0.26289043133366402,1430.1144000000006,-183.73710121838394,1246.3772987816167,"no",5500,522.37,2424.14,null,5060,36300,50.6,0,1209.9393991619213,0,62.318864939080839,1272.2582641010022,-25.880965319385496,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","base-lpd","yes-day","no-occ","base-epd","base-eff",230.22,90.26,4.2281489628203897E-2,9.3479288076862496E-2,-0.11874070401586501,659.49720000000025,-82.989223464031966,576.50797653596828,"no",5500,522.37,2424.14,null,3025.0000000000005,18755,30.250000000000004,0,723.33333645549635,0,28.825398826798416,752.15873528229474,-175.65075874632646,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","base-lpd","yes-day","no-occ","base-epd","high-eff",227.37,90.26,5.0820273118870801E-2,0.104701527799653,-0.11874070401586501,738.67020000000014,-82.989223464031966,655.68097653596817,"no",5500,522.37,2424.14,null,5280,52250,52.800000000000004,0,1262.5454599950481,0,32.784048826798411,1295.3295088218465,-639.64853228587833,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","base-lpd","yes-day","no-occ","red-epd","base-eff",197.09,105.11,9.6905263801056907E-2,0.223932902819342,-0.30280118988596899,1579.8486000000003,-211.63118259147191,1368.2174174085283,"no",5500,522.37,2424.14,null,3850.0000000000005,19580,38.500000000000007,0,920.60606457972267,0,68.410870870426422,989.01693545014905,379.20048195837921,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","base-lpd","yes-day","no-occ","red-epd","high-eff",194.67,105.11,0.104160938502429,0.23346196251378201,-0.30280118988596899,1647.0762000000007,-211.63118259147191,1435.4450174085287,"no",5500,522.37,2424.14,null,6105,53075,61.050000000000004,0,1459.8181881192745,0,71.772250870426433,1531.5904389897009,-96.145421581172286,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","base-lpd","yes-day","yes-occ","base-epd","base-eff",219.21,95.19,6.0458864143219299E-2,0.13683257205859201,-0.17984630639563701,965.35500000000013,-125.69662134270391,839.65837865729623,"no",5500,522.37,2424.14,null,5005,20735,50.050000000000004,0,1196.7878839536393,0,41.982918932864813,1238.770802886504,-399.11242422920782,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","base-lpd","yes-day","yes-occ","base-epd","high-eff",216.52,95.19,6.8508844285583403E-2,0.14742479130571701,-0.17984630639563701,1040.0832,-125.69662134270391,914.38657865729613,"no",5500,522.37,2424.14,null,7260,54230,72.600000000000009,0,1736.0000074931913,0,45.719328932864812,1781.7193364260561,-867.33275776875996,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","base-lpd","yes-day","yes-occ","red-epd","base-eff",186.18,110.5,0.113448202120184,0.26689242400377999,-0.36960832920178499,1882.9284,-258.32344923772791,1624.604950762272,"no",5500,522.37,2424.14,null,5830,21560,58.300000000000004,0,1394.0606120778657,0,81.230247538113602,1475.2908596159793,149.31409114629264,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","base-lpd","yes-day","yes-occ","red-epd","high-eff",183.9,110.5,0.12024562368252199,0.27587021578201298,-0.36960832920178499,1946.2668000000003,-258.32344923772791,1687.9433507622725,"no",5500,522.37,2424.14,null,8085,55055,80.850000000000009,0,1933.2727356174175,0,84.397167538113635,2017.6699031555311,-329.72655239325854,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","40 fc","no-day","no-occ","base-epd","base-eff",253.96,80.680000000000007,0,0,0,0,0,0,"no",5500,522.37,2424.14,null,3630,11330,36.300000000000004,0,868.00000374659567,-660,0,208.00000374659567,-208.00000374659567,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","40 fc","no-day","no-occ","base-epd","high-eff",250.75,80.680000000000007,9.5774906058106197E-3,1.2639785793038301E-2,0,89.173800000000227,0,89.173800000000227,"no",5500,522.37,2424.14,null,5885,44825,58.85,0,1407.2121272861473,-660,4.4586900000000114,751.67081728614733,-662.49701728614707,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","40 fc","no-day","no-occ","red-epd","base-eff",220.7,94.66,5.7602419576573999E-2,0.13096550637895699,-0.17327714427367399,923.9628000000007,-121.1053595017919,802.8574404982088,"no",5500,522.37,2424.14,null,4455,12155,44.550000000000004,0,1065.2727318708219,-660,40.142872024910446,445.41560389573232,357.44183660247649,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","40 fc","no-day","no-occ","red-epd","high-eff",217.93,94.66,6.5866251183820598E-2,0.14187273586391599,-0.17327714427367399,1000.9134,-121.1053595017919,879.80804049820813,"no",5500,522.37,2424.14,null,6710,45650,67.099999999999994,0,1604.4848554103737,-660,43.990402024910409,988.47525743528411,-108.66721693707598,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","40 fc","no-day","yes-occ","base-epd","base-eff",238.17,87.17,2.77854153300949E-2,6.2175145692235097E-2,-8.0441249380267699E-2,438.64620000000059,-56.221300655695956,382.42489934430466,"no",5500,522.37,2424.14,null,5610,13310,56.1,0,1341.4545512447387,-660,19.121244967215233,700.57579621195396,-318.15089686764929,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","40 fc","no-day","yes-occ","base-epd","high-eff",235.2,87.17,3.6644976018085702E-2,7.3869900771775202E-2,-8.0441249380267699E-2,521.15280000000064,-56.221300655695956,464.93149934430471,"no",5500,522.37,2424.14,null,7865,46805,78.650000000000006,0,1880.6666747842903,-660,23.246574967215238,1243.9132497515056,-778.98175040720093,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","40 fc","no-day","yes-occ","red-epd","base-eff",205.03,101.89,8.2821617328078606E-2,0.19266813671444299,-0.26289043133366402,1359.2754000000004,-183.73710121838394,1175.5382987816165,"no",5500,522.37,2424.14,null,6435,14135,64.349999999999994,0,1538.7272793689651,-660,58.776914939080825,937.50419430804595,238.03410447357055,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","40 fc","no-day","yes-occ","red-epd","high-eff",202.48,101.89,9.0428619436042995E-2,0.202709088045362,-0.26289043133366402,1430.1144000000006,-183.73710121838394,1246.3772987816167,"no",5500,522.37,2424.14,null,8690,47630,86.9,0,2077.9394029085165,-660,62.318864939080839,1480.2582678475974,-233.88096906598071,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","40 fc","yes-day","no-occ","base-epd","base-eff",230.22,90.26,4.2281489628203897E-2,9.3479288076862496E-2,-0.11874070401586501,659.49720000000025,-82.989223464031966,576.50797653596828,"no",5500,522.37,2424.14,null,6655,30085,66.55,0,1591.3333402020919,-660,28.825398826798416,960.1587390288903,-383.65076249292201,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","40 fc","yes-day","no-occ","base-epd","high-eff",227.37,90.26,5.0820273118870801E-2,0.104701527799653,-0.11874070401586501,738.67020000000014,-82.989223464031966,655.68097653596817,"no",5500,522.37,2424.14,null,8910,63580,89.100000000000009,0,2130.5454637416437,-660,32.784048826798411,1503.3295125684422,-847.648536032474,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","40 fc","yes-day","no-occ","red-epd","base-eff",197.09,105.11,9.6905263801056907E-2,0.223932902819342,-0.30280118988596899,1579.8486000000003,-211.63118259147191,1368.2174174085283,"no",5500,522.37,2424.14,null,7480,30910,74.8,0,1788.6060683263183,-660,68.410870870426422,1197.0169391967447,171.20047821178355,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","40 fc","yes-day","no-occ","red-epd","high-eff",194.67,105.11,0.104160938502429,0.23346196251378201,-0.30280118988596899,1647.0762000000007,-211.63118259147191,1435.4450174085287,"no",5500,522.37,2424.14,null,9735,64405,97.350000000000009,0,2327.8181918658702,-660,71.772250870426433,1739.5904427362966,-304.14542532776795,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","40 fc","yes-day","yes-occ","base-epd","base-eff",219.21,95.19,6.0458864143219299E-2,0.13683257205859201,-0.17984630639563701,965.35500000000013,-125.69662134270391,839.65837865729623,"no",5500,522.37,2424.14,null,8635,32065,86.350000000000009,0,2064.7878877002349,-660,41.982918932864813,1446.7708066330997,-607.11242797580348,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","40 fc","yes-day","yes-occ","base-epd","high-eff",216.52,95.19,6.8508844285583403E-2,0.14742479130571701,-0.17984630639563701,1040.0832,-125.69662134270391,914.38657865729613,"no",5500,522.37,2424.14,null,10890,65560,108.9,0,2604.0000112397865,-660,45.719328932864812,1989.7193401726513,-1075.3327615153553,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","40 fc","yes-day","yes-occ","red-epd","base-eff",186.18,110.5,0.113448202120184,0.26689242400377999,-0.36960832920178499,1882.9284,-258.32344923772791,1624.604950762272,"no",5500,522.37,2424.14,null,9460,32890,94.600000000000009,0,2262.0606158244614,-660,81.230247538113602,1683.290863362575,-58.685912600303027,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","40 fc","yes-day","yes-occ","red-epd","high-eff",183.9,110.5,0.12024562368252199,0.27587021578201298,-0.36960832920178499,1946.2668000000003,-258.32344923772791,1687.9433507622725,"no",5500,522.37,2424.14,null,11715,66385,117.15,0,2801.272739364013,-660,84.397167538113635,2225.6699069021265,-537.72655613985398,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","25 fc","no-day","no-occ","base-epd","base-eff",238.17,87.17,2.77854153300949E-2,6.2175145692235097E-2,-8.0441249380267699E-2,438.64620000000059,-56.221300655695956,382.42489934430466,"no",5500,522.37,2424.14,null,4345,61325,43.45,0,1038.9697014542583,-1045,19.121244967215233,13.09094642147349,369.33395292283114,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","25 fc","no-day","no-occ","base-epd","high-eff",235.2,87.17,3.6644976018085702E-2,7.3869900771775202E-2,-8.0441249380267699E-2,521.15280000000064,-56.221300655695956,464.93149934430471,"no",5500,522.37,2424.14,null,6600,94820,66,0,1578.1818249938103,-1045,23.246574967215238,556.42839996102555,-91.496900616720836,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","25 fc","no-day","no-occ","red-epd","base-eff",205.03,101.89,8.2821617328078606E-2,0.19266813671444299,-0.26289043133366402,1359.2754000000004,-183.73710121838394,1175.5382987816165,"no",5500,522.37,2424.14,null,5170,62150,51.7,0,1236.2424295784845,-1045,58.776914939080825,250.01934451756529,925.51895426405122,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","25 fc","no-day","no-occ","red-epd","high-eff",202.48,101.89,9.0428619436042995E-2,0.202709088045362,-0.26289043133366402,1430.1144000000006,-183.73710121838394,1246.3772987816167,"no",5500,522.37,2424.14,null,7425,95645,74.25,0,1775.4545531180365,-1045,62.318864939080839,792.7734180571174,453.60388072449928,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","25 fc","no-day","yes-occ","base-epd","base-eff",225.5,92.65,4.92622124461553E-2,0.11206489210899399,-0.14836390679226599,790.61880000000031,-103.69321553908797,686.92558446091232,"no",5500,522.37,2424.14,null,6325,63305,63.25,0,1512.4242489524013,-1045,34.34627922304562,501.77052817544688,185.15505628546543,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","25 fc","no-day","yes-occ","base-epd","high-eff",222.71,92.65,5.7571869367305101E-2,0.12305087415341,-0.14836390679226599,868.125,-103.69321553908797,764.43178446091201,"no",5500,522.37,2424.14,null,8580,96800,85.8,0,2051.6363724919529,-1045,38.221589223045605,1044.8579617149985,-280.4261772540865,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","25 fc","no-day","yes-occ","red-epd","base-eff",192.45,107.84,0.10261815293434801,0.24220349661363999,-0.33663857213683701,1708.7478000000008,-235.28051245126395,1473.4672875487367,"no",5500,522.37,2424.14,null,7150,64130,71.5,0,1709.6969770766277,-1045,73.67336437743684,738.3703414540646,735.09694609467215,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","25 fc","no-day","yes-occ","red-epd","high-eff",190.08,107.84,0.109690526380106,0.25153567490943501,-0.33663857213683701,1774.5863999999999,-235.28051245126395,1539.3058875487359,"no",5500,522.37,2424.14,null,9405,97625,94.05,0,2248.9091006161793,-1045,76.965294377436805,1280.8743949936161,258.4314925551198,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","25 fc","yes-day","no-occ","base-epd","base-eff",219.21,95.19,6.0458864143219299E-2,0.13683257205859201,-0.17984630639563701,965.35500000000013,-125.69662134270391,839.65837865729623,"no",5500,522.37,2424.14,null,7370,80080,73.7,0,1762.3030379097545,-1045,41.982918932864813,759.28595684261927,80.372421814676954,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","25 fc","yes-day","no-occ","base-epd","high-eff",216.52,95.19,6.8508844285583403E-2,0.14742479130571701,-0.17984630639563701,1040.0832,-125.69662134270391,914.38657865729613,"no",5500,522.37,2424.14,null,9625,113575,96.25,0,2301.5151614493066,-1045,45.719328932864812,1302.2344903821713,-387.84791172487519,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","25 fc","yes-day","no-occ","red-epd","base-eff",186.18,110.5,0.113448202120184,0.26689242400377999,-0.36960832920178499,1882.9284,-258.32344923772791,1624.604950762272,"no",5500,522.37,2424.14,null,8195,80905,81.95,0,1959.5757660339812,-1045,81.230247538113602,995.8060135720948,628.79893719017718,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","25 fc","yes-day","no-occ","red-epd","high-eff",183.9,110.5,0.12024562368252199,0.27587021578201298,-0.36960832920178499,1946.2668000000003,-258.32344923772791,1687.9433507622725,"no",5500,522.37,2424.14,null,10450,114400,104.5,0,2498.787889573533,-1045,84.397167538113635,1538.1850571116465,149.758293650626,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","25 fc","yes-day","yes-occ","base-epd","base-eff",210.35,99.37,7.4466135093025396E-2,0.17171995589856701,-0.23165592464055501,1211.4858000000004,-161.90695057857599,1049.5788494214244,"no",5500,522.37,2424.14,null,9350,82060,93.5,0,2235.7575854078977,-1045,52.478942471071221,1243.2365278789689,-193.65767845754453,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","25 fc","yes-day","yes-occ","base-epd","high-eff",207.78,99.37,8.2149512724162099E-2,0.18183965978894301,-0.23165592464055501,1282.8804000000002,-161.90695057857599,1120.9734494214242,"no",5500,522.37,2424.14,null,11605,115555,116.05,0,2774.9697089474494,-1045,56.048672471071214,1786.0183814185207,-665.04493199709646,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","25 fc","yes-day","yes-occ","red-epd","base-eff",177.38,115.03,0.126172364280695,0.30154355016537998,-0.425756073376301,2127.3924000000002,-297.56574384023992,1829.8266561597602,"no",5500,522.37,2424.14,null,10175,82885,101.75,0,2433.0303135321242,-1045,91.491332807988016,1479.5216463401123,350.30500981964792,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","25 fc","yes-day","yes-occ","red-epd","high-eff",175.22,115.03,0.13261845843643999,0.310048826586864,-0.425756073376301,2187.3972000000008,-297.56574384023992,1889.8314561597608,"no",5500,522.37,2424.14,null,12430,116380,124.3,0,2972.2424370716753,-1045,94.491572807988049,2021.7340098796633,-131.90255371990247,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","base-lpd","no-day","no-occ","base-epd","base-eff",253.99,79.2,4.3228546115539803E-3,-1.1812883918727799E-4,1.8344075359444802E-2,-0.83340000000003167,12.820882121792033,11.987482121792002,"no",5500,522.37,2424.14,null,1042.3801999999998,1042.3801999999998,10.423801999999998,0,249.252346420214,0,0.59937410608960018,249.85172052630361,-237.86423840451161,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","base-lpd","no-day","no-occ","base-epd","high-eff",250.77,79.2,1.3930895426633699E-2,1.2561033233580101E-2,1.8344075359444802E-2,88.618199999999945,12.820882121792033,101.43908212179198,"no",5500,522.37,2424.14,null,3297.3801999999996,34537.3802,32.973801999999999,0,788.46446995976578,0,5.0719541060895992,793.53642406585539,-692.09734194406337,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","base-lpd","no-day","no-occ","red-epd","base-eff",220.7,93.12,6.2215501176183102E-2,0.13096550637895699,-0.15418939018344099,923.9628000000007,-107.76471188857597,816.19808811142468,"no",5500,522.37,2424.14,null,1867.3801999999998,1867.3801999999998,18.673801999999998,0,446.52507454444032,0,40.809904405571238,487.33497895001153,328.86310916141315,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","base-lpd","no-day","no-occ","red-epd","high-eff",217.92,93.12,7.0525158097332896E-2,0.14191211214364499,-0.15418939018344099,1001.1912000000007,-107.76471188857597,893.42648811142465,"no",5500,522.37,2424.14,null,4122.3801999999996,35362.3802,41.223801999999999,0,985.73719808399221,0,44.671324405571234,1030.4085224895634,-136.98203437813879,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","base-lpd","no-day","yes-occ","base-epd","base-eff",238.2,85.66,3.2199920569455802E-2,6.2057016853047799E-2,-6.1725334655428697E-2,437.81280000000055,-43.140535788191904,394.67226421180862,"no",5500,522.37,2424.14,null,3022.3801999999996,3022.3801999999996,30.223801999999996,0,722.70689391835697,0,19.733613210590434,742.44050712894739,-347.76824291713876,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","base-lpd","no-day","yes-occ","base-epd","high-eff",235.22,85.66,4.1105306571350003E-2,7.3791148212316901E-2,-6.1725334655428697E-2,520.59720000000027,-43.140535788191904,477.45666421180835,"no",5500,522.37,2424.14,null,5277.3801999999996,36517.3802,52.773801999999996,0,1261.9190174579089,0,23.872833210590418,1285.7918506684994,-808.33518645669096,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","base-lpd","no-day","yes-occ","red-epd","base-eff",205.02,100.2,8.7877676962087106E-2,0.19270751299417199,-0.24194348041645999,1359.5532000000001,-169.09703987660797,1190.456160123392,"no",5500,522.37,2424.14,null,3847.3801999999996,3847.3801999999996,38.473801999999999,0,919.97962204258329,0,59.522808006169605,979.5024300487529,210.95373007463911,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","base-lpd","no-day","yes-occ","red-epd","high-eff",202.47,100.2,9.5499954174686097E-2,0.202748464325091,-0.24194348041645999,1430.3922000000002,-169.09703987660797,1261.2951601233922,"no",5500,522.37,2424.14,null,6102.3801999999996,37342.3802,61.023801999999996,0,1459.1917455821351,0,63.064758006169612,1522.2565035883047,-260.96134346491249,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","base-lpd","yes-day","no-occ","base-epd","base-eff",230.25,88.67,4.6970946750985197E-2,9.3361159237675295E-2,-9.9033217649975094E-2,658.66380000000026,-69.21543794129596,589.44836205870433,"no",5500,522.37,2424.14,null,4067.3802000000005,19797.3802,40.673802000000009,0,972.58568287571063,0,29.472418102935219,1002.0581009786458,-412.60973891994149,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","base-lpd","yes-day","no-occ","base-epd","high-eff",227.38,88.67,5.5540280450921103E-2,0.104662151519924,-9.9033217649975094E-2,738.39240000000041,-69.21543794129596,669.17696205870448,"no",5500,522.37,2424.14,null,6322.3802000000005,53292.3802,63.223802000000006,0,1511.7978064152624,0,33.458848102935228,1545.2566545181976,-876.07969245949312,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","base-lpd","yes-day","no-occ","red-epd","base-eff",197.08,103.45,0.101900223016528,0.223972279099071,-0.28222607833416002,1580.1264000000001,-197.25100399540796,1382.8753960045922,"no",5500,522.37,2424.14,null,4892.3802000000005,20622.3802,48.923802000000009,0,1169.8584109999367,0,69.143769800229606,1239.0021808001663,143.87321520442583,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","base-lpd","yes-day","no-occ","red-epd","high-eff",194.64,103.45,0.109186447927168,0.233580091352969,-0.28222607833416002,1647.9096000000006,-197.25100399540796,1450.6585960045927,"no",5500,522.37,2424.14,null,7147.3802000000005,54117.3802,71.473802000000006,0,1709.0705345394888,0,72.532929800229638,1781.6034643397184,-330.94486833512565,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","base-lpd","yes-day","yes-occ","base-epd","base-eff",219.24,93.6,6.5148321266000606E-2,0.13671444321940501,-0.160138820029747,964.52160000000003,-111.92283581996789,852.59876418003216,"no",5500,522.37,2424.14,null,6047.3802000000005,21777.3802,60.473802000000006,0,1446.0402303738535,0,42.629938209001608,1488.6701685828552,-636.07140440282308,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","base-lpd","yes-day","yes-occ","base-epd","high-eff",216.53,93.6,7.3244126722267905E-2,0.14738541502598801,-0.160138820029747,1039.8054000000002,-111.92283581996789,927.88256418003232,"no",5500,522.37,2424.14,null,8302.3801999999996,55272.3802,83.023802000000003,0,1985.2523539134052,0,46.394128209001622,2031.6464821224067,-1103.7639179423745,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","base-lpd","yes-day","yes-occ","red-epd","base-eff",186.16,108.78,0.118595912382,0.26697117656323799,-0.34828953891918701,1883.4840000000004,-243.42350515023992,1640.0604948497605,"no",5500,522.37,2424.14,null,6872.3802000000005,22602.3802,68.723802000000006,0,1643.31295849808,0,82.003024742488037,1725.3159832405681,-85.255488390807614,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","base-lpd","yes-day","yes-occ","red-epd","high-eff",183.88,108.78,0.12543915925824101,0.27594896834147098,-0.34828953891918701,1946.8224000000007,-243.42350515023992,1703.3988948497608,"no",5500,522.37,2424.14,null,9127.3801999999996,56097.3802,91.273802000000003,0,2182.5250820376314,0,85.169944742488042,2267.6950267801194,-564.29613193035857,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","40 fc","no-day","no-occ","base-epd","base-eff",253.99,79.2,4.3228546115539803E-3,-1.1812883918727799E-4,1.8344075359444802E-2,-0.83340000000003167,12.820882121792033,11.987482121792002,{"$f":"IF(P455>0.2,\"yes\",\"no\")","v":"no"},{"$f":"IF(B455=\"5500 ft2\",5500,IF(B455=\"10000 ft2\",10000,25000))","v":5500},{"$f":"IF(B455=\"5500 ft2\",IF(D455=\"stand-alone\",642.39,IF(D455=\"ad-e&flr\",522.37,402.25)),IF(B455=\"10000 ft2\",IF(D455=\"stand-alone\",866.06,IF(D455=\"ad-e&flr\",704.17,542.29)),IF(B455=\"25000 ft2\",IF(D455=\"stand-alone\",1369.38,IF(D455=\"ad-e&flr\",1113.42,857.45)))))","v":522.37},{"$f":"IF(B455=\"5500 ft2\",IF(D455=\"stand-alone\",3030.15,IF(D455=\"ad-e&flr\",2424.14,1818.13)),IF(B455=\"10000 ft2\",IF(D455=\"stand-alone\",4085.12,IF(D455=\"ad-e&flr\",3268.14,2451.05)),IF(B455=\"25000 ft2\",IF(D455=\"stand-alone\",6459.2,IF(D455=\"ad-e&flr\",5167.32,3875.54)))))","v":2424.14},null,{"$f":"SUM(IF(F455=\"eff-roof\",W455*IF(AND(W$4=\"no\",X$4=\"no\"),$C$4,$C$3)),IF(G455=\"eff-win\",X455*IF(W$4=\"no\",$D$4,$D$3),0),IF(H455=\"red-inf\",Y455*IF(W$4=\"no\",$F$4,$F$3),0),IF(I455=\"25 fc\",W455*IF(W$4=\"no\",$H$4,$H$3),0),IF(I455=\"40 fc\",W455*IF(W$4=\"no\",$G$4,$G$3),0),IF(J455=\"yes-day\",W455*IF(W$4=\"no\",$I$4,$I$3),0),IF(K455=\"yes-occ\",W455*IF(W$4=\"no\",$J$4,$J$3),0),IF(L455=\"red-epd\",W455*IF(W$4=\"no\",$K$4,$K$3),0),IF(AND(M455=\"high-eff\",C455=\"psz-ac\"),W455*IF(AND(W$4=\"no\",Y$4=\"no\"),$L$4,$L$3),0),IF(AND(M455=\"high-eff\",C455=\"ptac\"),W455*IF(AND(W$4=\"no\",Y$4=\"no\"),$M$4,$M$3),0),IF(AND(M455=\"high-eff\",C455=\"pthp\"),W455*IF(AND(W$4=\"no\",Y$4=\"no\"),$N$4,$N$3),0))","v":4672.3801999999996},{"$f":"SUM(IF(F455=\"eff-roof\",W455*$C$4),IF(G455=\"eff-win\",X455*$D$4,0),IF(H455=\"red-inf\",Y455*$F$4,0),IF(I455=\"25 fc\",W455*$H$4,0),IF(I455=\"40 fc\",W455*$G$4,0),IF(J455=\"yes-day\",W455*$I$4,0),IF(K455=\"yes-occ\",W455*$J$4,0),IF(L455=\"red-epd\",W455*$K$4,0),IF(AND(M455=\"high-eff\",C455=\"psz-ac\"),W455*$L$4,0),IF(AND(M455=\"high-eff\",C455=\"ptac\"),W455*$M$4,0),IF(AND(M455=\"high-eff\",C455=\"pthp\"),W455*$N$4,0))","v":12372.3802},46.723801999999999,0,{"$f":"-PMT($AE$3,$AE$4,AA455+AC455-AD455)","v":1117.2523501668097},{"$f":"SUM(IF(F455=\"eff-roof\",($C$5*W455),0),IF(G455=\"eff-win\",($D$5*X455),0),IF(H455=\"red-inf\",$F$5*(Y455-X455),0),IF(I455=\"25 fc\",($H$5*W455),0),IF(I455=\"40 fc\",($G$5*W455),0),IF(J455=\"yes-day\",($I$5*W455),0),IF(K455=\"yes-occ\",($J$5*W455),0),IF(L455=\"red-epd\",($K$5*W455),0),IF(M455=\"high-eff\",($L$5*W455),0))","v":-660},{"$f":"0.05*U455","v":0.59937410608960018},457.85172427289933,{"$f":"U455-AH455","v":-445.86424215110731},null,null,null,"New Construction",{"$f":"IF(B455=\"5500 ft2\",\"5,500 SF\",IF(B455=\"10000 ft2\",\"10,000 SF\",IF(B455=\"25000 ft2\",\"25,000 SF\")))","v":"5,500 SF"},"Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration",{"$f":"IF(I455=\"base-lpd\",\"Baseline Lighting Levels\",IF(I455=\"40 fc\",\"Reduce Lighting Levels to 40 fc\",IF(I455=\"25 fc\",\"Reduce Lighting Levels to 25 fc\")))","v":"Reduce Lighting Levels to 40 fc"},"No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","40 fc","no-day","no-occ","base-epd","high-eff",250.77,79.2,1.3930895426633699E-2,1.2561033233580101E-2,1.8344075359444802E-2,{"$f":"277.8*($N$391-N456)*$S$3","v":88.618199999999945},{"$f":"277.78*($O$391-O456)*$S$4","v":12.820882121792033},{"$f":"SUM(S456:T456)","v":101.43908212179198},"no",5500,522.37,2424.14,null,6927.3801999999996,45867.3802,{"$f":"MIN(0.01*AA456,500)","v":69.273802000000003},{"$f":"IF(V456=\"yes\",0,0)","v":0},1656.4644737063613,-660,5.0719541060895992,{"$f":"SUM(AE456:AG456)","v":1001.5364278124509},-900.09734569065893,null,null,null,"New Construction","5,500 SF",{"$f":"IF(C456=\"psz-ac\",\"Packaged Air Conditioner\",IF(C456=\"ptac\",\"Split System Air Conditioner\",IF(C456=\"pthp\",\"Split System Heat Pump\")))","v":"Packaged Air Conditioner"},{"$f":"IF(D456=\"stand-alone\",\"Stand Alone\",IF(D456=\"ad-e&flr\",\"Above Ground, 1 Side Attached\",IF(D456=\"ad-e&w&flr\",\"Above Ground, 2 Sides Attached\")))","v":"Above Ground, 1 Side Attached"},{"$f":"IF(F456=\"base-roof\",\"Baseline Roof Insulation\",IF(F456=\"eff-roof\",\"Increased Roof Insulation\"))","v":"Baseline Roof Insulation"},{"$f":"IF(G456=\"base-win\",\"Baseline Windows\",IF(G456=\"eff-win\",\"Replace Windows\"))","v":"Baseline Windows"},{"$f":"IF(H456=\"base-inf\",\"Baseline Infiltration\",IF(H456=\"red-inf\",\"Reduce Infiltration\"))","v":"Reduce Infiltration"},"Reduce Lighting Levels to 40 fc",{"$f":"IF(J456=\"no-day\",\"No Daylighting Sensors\",IF(J456=\"yes-day\",\"Install Daylighting Sensors\"))","v":"No Daylighting Sensors"},{"$f":"IF(K456=\"no-occ\",\"No Occupancy Sensors\",IF(K456=\"yes-occ\",\"Install Occupancy Sensors\"))","v":"No Occupancy Sensors"},{"$f":"IF(L456=\"base-epd\",\"No Plug Load Control\",IF(L456=\"red-epd\",\"Install Plug Load Controls\"))","v":"No Plug Load Control"},{"$f":"IF(M456=\"base-eff\",\"Baseline HVAC Equipment\",IF(M456=\"high-eff\",\"Install High Efficiency HVAC Equipment\"))","v":"Install High Efficiency HVAC Equipment"}]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","40 fc","no-day","no-occ","red-epd","base-eff",220.7,93.12,6.2215501176183102E-2,0.13096550637895699,-0.15418939018344099,923.9628000000007,-107.76471188857597,816.19808811142468,"no",5500,522.37,2424.14,null,5497.3801999999996,13197.3802,54.973801999999999,0,1314.5250782910359,-660,40.809904405571238,695.3349826966072,120.86310541481748,null,null,null,{"$f":"IF(A457=\"new90.1-2004\",\"New Construction\",IF(A457=\"post1980\",\"Post 1980 Construction\",IF(A457=\"pre1980\",\"Pre 1980 Construction\")))","v":"New Construction"},"5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","40 fc","no-day","no-occ","red-epd","high-eff",217.92,93.12,7.0525158097332896E-2,0.14191211214364499,-0.15418939018344099,1001.1912000000007,-107.76471188857597,893.42648811142465,"no",5500,522.37,2424.14,null,7752.3801999999996,46692.3802,77.523802000000003,0,1853.7372018305875,-660,44.671324405571234,1238.4085262361589,-344.98203812473423,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","40 fc","no-day","yes-occ","base-epd","base-eff",238.2,85.66,3.2199920569455802E-2,6.2057016853047799E-2,-6.1725334655428697E-2,437.81280000000055,-43.140535788191904,394.67226421180862,"no",5500,522.37,2424.14,null,6652.3801999999996,14352.3802,66.523802000000003,0,1590.7068976649525,-660,19.733613210590434,950.44051087554294,-555.76824666373432,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","40 fc","no-day","yes-occ","base-epd","high-eff",235.22,85.66,4.1105306571350003E-2,7.3791148212316901E-2,-6.1725334655428697E-2,520.59720000000027,-43.140535788191904,477.45666421180835,"no",5500,522.37,2424.14,null,8907.3801999999996,47847.3802,89.073802000000001,0,2129.9190212045046,-660,23.872833210590418,1493.791854415095,-1016.3351902032866,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","40 fc","no-day","yes-occ","red-epd","base-eff",205.02,100.2,8.7877676962087106E-2,0.19270751299417199,-0.24194348041645999,1359.5532000000001,-169.09703987660797,1190.456160123392,"no",5500,522.37,2424.14,null,7477.3801999999996,15177.3802,74.773802000000003,0,1787.979625789179,-660,59.522808006169605,1187.5024337953485,2.9537263280435582,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","40 fc","no-day","yes-occ","red-epd","high-eff",202.47,100.2,9.5499954174686097E-2,0.202748464325091,-0.24194348041645999,1430.3922000000002,-169.09703987660797,1261.2951601233922,"no",5500,522.37,2424.14,null,9732.3801999999996,48672.3802,97.323802000000001,0,2327.191749328731,-660,63.064758006169612,1730.2565073349006,-468.96134721150838,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","40 fc","yes-day","no-occ","base-epd","base-eff",230.25,88.67,4.6970946750985197E-2,9.3361159237675295E-2,-9.9033217649975094E-2,658.66380000000026,-69.21543794129596,589.44836205870433,"no",5500,522.37,2424.14,null,7697.3801999999996,31127.3802,76.973801999999992,0,1840.585686622306,-660,29.472418102935219,1210.0581047252413,-620.60974266653693,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","40 fc","yes-day","no-occ","base-epd","high-eff",227.38,88.67,5.5540280450921103E-2,0.104662151519924,-9.9033217649975094E-2,738.39240000000041,-69.21543794129596,669.17696205870448,"no",5500,522.37,2424.14,null,9952.3801999999996,64622.3802,99.523802000000003,0,2379.7978101618578,-660,33.458848102935228,1753.256658264793,-1084.0796962060886,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","40 fc","yes-day","no-occ","red-epd","base-eff",197.08,103.45,0.101900223016528,0.223972279099071,-0.28222607833416002,1580.1264000000001,-197.25100399540796,1382.8753960045922,"no",5500,522.37,2424.14,null,8522.3801999999996,31952.3802,85.223801999999992,0,2037.8584147465322,-660,69.143769800229606,1447.0021845467618,-64.126788542169606,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","40 fc","yes-day","no-occ","red-epd","high-eff",194.64,103.45,0.109186447927168,0.233580091352969,-0.28222607833416002,1647.9096000000006,-197.25100399540796,1450.6585960045927,"no",5500,522.37,2424.14,null,10777.3802,65447.3802,107.773802,0,2577.0705382860838,-660,72.532929800229638,1989.6034680863133,-538.94487208172063,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","40 fc","yes-day","yes-occ","base-epd","base-eff",219.24,93.6,6.5148321266000606E-2,0.13671444321940501,-0.160138820029747,964.52160000000003,-111.92283581996789,852.59876418003216,"no",5500,522.37,2424.14,null,9677.3801999999996,33107.3802,96.773802000000003,0,2314.040234120449,-660,42.629938209001608,1696.6701723294507,-844.07140814941852,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","40 fc","yes-day","yes-occ","base-epd","high-eff",216.53,93.6,7.3244126722267905E-2,0.14738541502598801,-0.160138820029747,1039.8054000000002,-111.92283581996789,927.88256418003232,"no",5500,522.37,2424.14,null,11932.3802,66602.3802,119.323802,0,2853.2523576600006,-660,46.394128209001622,2239.6464858690024,-1311.7639216889702,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","40 fc","yes-day","yes-occ","red-epd","base-eff",186.16,108.78,0.118595912382,0.26697117656323799,-0.34828953891918701,1883.4840000000004,-243.42350515023992,1640.0604948497605,"no",5500,522.37,2424.14,null,10502.3802,33932.3802,105.023802,0,2511.312962244675,-660,82.003024742488037,1933.3159869871629,-293.25549213740237,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","40 fc","yes-day","yes-occ","red-epd","high-eff",183.88,108.78,0.12543915925824101,0.27594896834147098,-0.34828953891918701,1946.8224000000007,-243.42350515023992,1703.3988948497608,"no",5500,522.37,2424.14,null,12757.3802,67427.3802,127.573802,0,3050.5250857842275,-660,85.169944742488042,2475.6950305267155,-772.29613567695469,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","25 fc","no-day","no-occ","base-epd","base-eff",238.2,85.66,3.2199920569455802E-2,6.2057016853047799E-2,-6.1725334655428697E-2,437.81280000000055,-43.140535788191904,394.67226421180862,"no",5500,522.37,2424.14,null,5387.3801999999996,62367.3802,53.873801999999998,0,1288.2220478744723,-1045,19.733613210590434,262.95566108506273,131.71660312674589,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","25 fc","no-day","no-occ","base-epd","high-eff",235.22,85.66,4.1105306571350003E-2,7.3791148212316901E-2,-6.1725334655428697E-2,520.59720000000027,-43.140535788191904,477.45666421180835,"no",5500,522.37,2424.14,null,7642.3801999999996,95862.3802,76.423801999999995,0,1827.4341714140244,-1045,23.872833210590418,806.30700462461482,-328.85034041280647,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","25 fc","no-day","no-occ","red-epd","base-eff",205.02,100.2,8.7877676962087106E-2,0.19270751299417199,-0.24194348041645999,1359.5532000000001,-169.09703987660797,1190.456160123392,"no",5500,522.37,2424.14,null,6212.3801999999996,63192.3802,62.123801999999998,0,1485.4947759986985,-1045,59.522808006169605,500.01758400486813,690.43857611852388,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","25 fc","no-day","no-occ","red-epd","high-eff",202.47,100.2,9.5499954174686097E-2,0.202748464325091,-0.24194348041645999,1430.3922000000002,-169.09703987660797,1261.2951601233922,"no",5500,522.37,2424.14,null,8467.3801999999996,96687.3802,84.673801999999995,0,2024.7068995382501,-1045,63.064758006169612,1042.7716575444197,218.52350257897251,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","25 fc","no-day","yes-occ","base-epd","base-eff",225.53,91.11,5.3768368313322802E-2,0.111946763269806,-0.12927615270203299,789.78540000000021,-90.352567925871924,699.43283207412833,"no",5500,522.37,2424.14,null,7367.3801999999996,64347.3802,73.673801999999995,0,1761.6765953726156,-1045,34.971641603706416,751.64823697632198,-52.215404902193654,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","25 fc","no-day","yes-occ","base-epd","high-eff",222.73,91.11,6.21238505483762E-2,0.122972121593952,-0.12927615270203299,867.56940000000054,-90.352567925871924,777.21683207412866,"no",5500,522.37,2424.14,null,9622.3801999999996,97842.3802,96.223801999999992,0,2300.8887189121674,-1045,38.860841603706433,1294.7495605158738,-517.53272844174512,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","25 fc","no-day","yes-occ","red-epd","base-eff",192.44,106.13,0.107750588091528,0.24224287289336899,-0.31544372830937001,1709.0256000000006,-220.46719594567989,1488.5584040543208,"no",5500,522.37,2424.14,null,8192.3801999999996,65172.3802,81.923801999999995,0,1958.9493234968413,-1045,74.427920202716038,988.37724369955731,500.18116035476351,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","25 fc","no-day","yes-occ","red-epd","high-eff",190.07,106.13,0.114853511746555,0.25157505118916401,-0.31544372830937001,1774.8642000000004,-220.46719594567989,1554.3970040543206,"no",5500,522.37,2424.14,null,10447.3802,98667.3802,104.47380199999999,0,2498.1614470363934,-1045,77.719850202716032,1530.8812972391095,23.515706815211161,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","25 fc","yes-day","no-occ","base-epd","base-eff",219.24,93.6,6.5148321266000606E-2,0.13671444321940501,-0.160138820029747,964.52160000000003,-111.92283581996789,852.59876418003216,"no",5500,522.37,2424.14,null,8412.3801999999996,81122.3802,84.123801999999998,0,2011.5553843299685,-1045,42.629938209001608,1009.1853225389701,-156.58655835893796,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","25 fc","yes-day","no-occ","base-epd","high-eff",216.53,93.6,7.3244126722267905E-2,0.14738541502598801,-0.160138820029747,1039.8054000000002,-111.92283581996789,927.88256418003232,"no",5500,522.37,2424.14,null,10667.3802,114617.3802,106.67380199999999,0,2550.7675078695206,-1045,46.394128209001622,1552.1616360785222,-624.27907189848986,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","25 fc","yes-day","no-occ","red-epd","base-eff",186.16,108.78,0.118595912382,0.26697117656323799,-0.34828953891918701,1883.4840000000004,-243.42350515023992,1640.0604948497605,"no",5500,522.37,2424.14,null,9237.3801999999996,81947.3802,92.373801999999998,0,2208.8281124541945,-1045,82.003024742488037,1245.8311371966824,394.22935765307807,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","25 fc","yes-day","no-occ","red-epd","high-eff",183.88,108.78,0.12543915925824101,0.27594896834147098,-0.34828953891918701,1946.8224000000007,-243.42350515023992,1703.3988948497608,"no",5500,522.37,2424.14,null,11492.3802,115442.3802,114.92380199999999,0,2748.0402359937466,-1045,85.169944742488042,1788.2101807362346,-84.811285886473797,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","25 fc","yes-day","yes-occ","base-epd","base-eff",210.38,97.71,7.9323618366785698E-2,0.17160182705937899,-0.21108081308874499,1210.6524000000004,-147.52677198251189,1063.1256280174885,"no",5500,522.37,2424.14,null,10392.3802,83102.3802,103.92380199999999,0,2485.0099318281118,-1045,53.156281400874427,1493.1662132289862,-430.04058521149773,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","25 fc","yes-day","yes-occ","base-epd","high-eff",207.8,97.71,8.7037546207191493E-2,0.18176090722948501,-0.21108081308874499,1282.3248000000001,-147.52677198251189,1134.7980280174881,"no",5500,522.37,2424.14,null,12647.3802,116597.3802,126.47380199999999,0,3024.2220553676634,-1045,56.739901400874409,2035.9619567685379,-901.16392875104975,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","25 fc","yes-day","yes-occ","red-epd","base-eff",177.37,113.26,0.13150337579812399,0.30158292644510898,-0.40381755081804699,2127.6702,-282.23266184323199,1845.4375381567679,"no",5500,522.37,2424.14,null,11217.3802,83927.3802,112.17380199999999,0,2682.2826599523378,-1045,92.271876907838404,1729.5545368601761,115.88300129659183,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","25 fc","yes-day","yes-occ","red-epd","high-eff",175.2,113.26,0.13798002016313801,0.310127579146322,-0.40381755081804699,2187.9528000000005,-282.23266184323199,1905.7201381567684,"no",5500,522.37,2424.14,null,13472.3802,117422.3802,134.72380200000001,0,3221.4947834918898,-1045,95.286006907838427,2271.7807903997282,-366.0606522429598,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","eff-win","base-inf","base-lpd","no-day","no-occ","base-epd","base-eff",251.45,78.59,1.37323190663856E-2,9.8834462120019704E-3,2.5904809122459099E-2,69.727800000000542,18.10516461793603,87.832964617936568,"no",5500,522.37,2424.14,null,3750.6165999999998,22461.91,37.506166,0,896.84165918789085,0,4.3916482308968288,901.23330741878772,-813.40034280085115,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","eff-win","base-inf","base-lpd","no-day","no-occ","base-epd","high-eff",248.38,78.59,2.28973818470657E-2,2.1971964088832899E-2,2.5904809122459099E-2,155.01240000000035,18.10516461793603,173.11756461793638,"no",5500,522.37,2424.14,null,6005.6165999999994,55956.91,60.056165999999997,0,1436.0537827274427,0,8.6558782308968194,1444.7096609583396,-1271.5920963404033,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","eff-win","base-inf","base-lpd","no-day","no-occ","red-epd","base-eff",218.17,92.64,7.1181987596615107E-2,0.140927705150417,-0.14823996033713399,994.24620000000073,-103.60658795718393,890.63961204281679,"no",5500,522.37,2424.14,null,4575.6165999999994,23286.91,45.756165999999993,0,1094.1143873121168,0,44.531980602140841,1138.6463679142578,-248.00675587144099,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","eff-win","base-inf","base-lpd","no-day","no-occ","red-epd","high-eff",215.54,92.64,7.9048666483365407E-2,0.15128366671916799,-0.14823996033713399,1067.3076000000005,-103.60658795718393,963.70101204281661,"no",5500,522.37,2424.14,null,6830.6165999999994,56781.91,68.30616599999999,0,1633.3265108516687,0,48.185050602140834,1681.5115614538095,-717.81054941099285,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","eff-win","base-inf","base-lpd","no-day","yes-occ","base-epd","base-eff",235.67,85.12,4.1380258454770301E-2,7.2019215624507901E-2,-5.50322260783341E-2,508.09620000000064,-38.462646365375981,469.63355363462466,"no",5500,522.37,2424.14,null,5730.6165999999994,24441.91,57.306165999999997,0,1370.2962066860339,0,23.481677681731234,1393.7778843677652,-924.14433073314058,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","eff-win","base-inf","base-lpd","no-day","yes-occ","base-epd","high-eff",232.83,85.12,4.9842666422265001E-2,8.3202079067569698E-2,-5.50322260783341E-2,586.99139999999989,-38.462646365375981,548.52875363462385,"no",5500,522.37,2424.14,null,7985.6165999999994,57936.91,79.856166000000002,0,1909.5083302255853,0,27.426437681731194,1936.9347679073164,-1388.4060142726926,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","eff-win","base-inf","base-lpd","no-day","yes-occ","red-epd","base-eff",202.52,99.85,9.6416460452754094E-2,0.20255158292644501,-0.23760535448686201,1429.0032000000001,-166.06507450996787,1262.9381254900322,"no",5500,522.37,2424.14,null,6555.6165999999994,25266.91,65.55616599999999,0,1567.5689348102601,0,63.146906274501617,1630.7158410847617,-367.77771559472944,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","eff-win","base-inf","base-lpd","no-day","yes-occ","red-epd","high-eff",200.11,99.85,0.103626309840222,0.212041266341156,-0.23760535448686201,1495.953,-166.06507450996787,1329.8879254900321,"no",5500,522.37,2424.14,null,8810.6165999999994,58761.91,88.106166000000002,0,2106.7810583498117,0,66.494396274501611,2173.2754546243132,-843.38752913428107,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","eff-win","base-inf","base-lpd","yes-day","no-occ","base-epd","base-eff",227.7,88.21,5.5952708276051699E-2,0.103402110568594,-9.33316807139314E-2,729.50280000000066,-65.230569173711885,664.27223082628882,"no",5500,522.37,2424.14,null,6775.6166000000003,41216.910000000003,67.756166000000007,0,1620.1749956433871,0,33.213611541314442,1653.3886071847016,-989.11637635841282,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","eff-win","base-inf","base-lpd","yes-day","no-occ","base-epd","high-eff",224.98,88.21,6.4079063941587897E-2,0.114112458654906,-9.33316807139314E-2,805.06440000000066,-65.230569173711885,739.83383082628882,"no",5500,522.37,2424.14,null,9030.6166000000012,74711.91,90.306166000000019,0,2159.3871191829394,0,36.991691541314445,2196.378810724254,-1456.5449798979653,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","eff-win","base-inf","base-lpd","yes-day","no-occ","red-epd","base-eff",194.56,103.18,0.110240430146946,0.23389510159080201,-0.278879524045612,1650.1320000000005,-194.91205928399998,1455.2199407160006,"no",5500,522.37,2424.14,null,7600.6166000000003,42041.91,76.006166000000007,0,1817.4477237676135,0,72.760997035800031,1890.2087208034136,-434.98878008741303,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","eff-win","base-inf","base-lpd","yes-day","no-occ","red-epd","high-eff",192.27,103.18,0.117098952127822,0.242912269648764,-0.278879524045612,1713.7482,-194.91205928399998,1518.836140716,"no",5500,522.37,2424.14,null,9855.6166000000012,75536.91,98.556166000000019,0,2356.6598473071654,0,75.941807035800011,2432.6016543429655,-913.76551362696546,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","eff-win","base-inf","base-lpd","yes-day","yes-occ","base-epd","base-eff",216.7,93.26,7.3732930070570996E-2,0.146716018270594,-0.15592464055527999,1035.0828000000006,-108.97749803523197,926.10530196476861,"no",5500,522.37,2424.14,null,8755.6166000000012,43196.91,87.556166000000019,0,2093.6295431415306,0,46.305265098238436,2139.9348082397692,-1213.8295062750005,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","eff-win","base-inf","base-lpd","yes-day","yes-occ","base-epd","high-eff",214.14,93.26,8.1385757492438801E-2,0.156796345881241,-0.15592464055527999,1106.1996000000006,-108.97749803523197,997.22210196476863,"no",5500,522.37,2424.14,null,11010.616600000001,76691.91,110.10616600000002,0,2632.8416666810817,0,49.861105098238433,2682.7027717793203,-1685.4806698145517,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","base-roof","eff-win","red-inf","base-lpd","yes-day","no-occ","red-epd","high-eff",192.24,101.56,0.122032810924755,0.24303039848795099,-0.25880019831432799,1714.5816,-180.87839101555195,1533.7032089844481,"no",5500,522.37,2424.14,null,10897.996800000001,76579.290200000003,108.97996800000001,0,2605.9121937273794,0,76.685160449222408,2682.597354176602,-1148.8941451921539,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","eff-roof","base-win","base-inf","40 fc","no-day","yes-occ","red-epd","base-eff",203.69,92.64,0.114486909235328,0.197944558198141,-0.14823996033713399,1396.5006000000003,-103.60658795718393,1292.8940120428165,"no",5500,522.37,2424.14,null,22935,80960,229.35,0,5484.1818418534895,-660,64.64470060214083,4888.8265424556303,-3595.9325304128138,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","eff-roof","base-win","base-inf","25 fc","yes-day","yes-occ","red-epd","high-eff",173.81,105.51,0.165322457458834,0.31560088202866599,-0.30775904809122501,2226.5670000000005,-215.09628586763196,2011.4707141323686,"no",5500,522.37,2424.14,null,28930,183205,289.3,0,6917.6969995562004,-1045,100.57353570661843,5973.2705352628191,-3961.7998211304503,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&flr","new90.1-20045500 ft2psz-acad-e&flr","eff-roof","eff-win","base-inf","25 fc","no-day","no-occ","base-epd","high-eff",231.5,76.23,8.0392875691198504E-2,8.8439124271538896E-2,5.5156172533465601E-2,{"$f":"277.8*($N$391-N712)*$S$3","v":623.93880000000036},{"$f":"277.78*($O$391-O712)*$S$4","v":38.549273947280028},{"$f":"SUM(S712:T712)","v":662.48807394728033},"no",5500,522.37,2424.14,null,26850.616600000001,184106.91,{"$f":"MIN(0.01*AA712,500)","v":268.50616600000001},{"$f":"IF(V712=\"yes\",0,0)","v":0},6420.478046666226,-1045,33.124403697364016,{"$f":"SUM(AE712:AG712)","v":5408.6024503635899},-4746.1143764163098,null,null,null,"New Construction","5,500 SF",{"$f":"IF(C712=\"psz-ac\",\"Packaged Air Conditioner\",IF(C712=\"ptac\",\"Split System Air Conditioner\",IF(C712=\"pthp\",\"Split System Heat Pump\")))","v":"Packaged Air Conditioner"},{"$f":"IF(D712=\"stand-alone\",\"Stand Alone\",IF(D712=\"ad-e&flr\",\"Above Ground, 1 Side Attached\",IF(D712=\"ad-e&w&flr\",\"Above Ground, 2 Sides Attached\")))","v":"Above Ground, 1 Side Attached"},{"$f":"IF(F712=\"base-roof\",\"Baseline Roof Insulation\",IF(F712=\"eff-roof\",\"Increased Roof Insulation\"))","v":"Increased Roof Insulation"},{"$f":"IF(G712=\"base-win\",\"Baseline Windows\",IF(G712=\"eff-win\",\"Replace Windows\"))","v":"Replace Windows"},{"$f":"IF(H712=\"base-inf\",\"Baseline Infiltration\",IF(H712=\"red-inf\",\"Reduce Infiltration\"))","v":"Baseline Infiltration"},"Reduce Lighting Levels to 25 fc",{"$f":"IF(J712=\"no-day\",\"No Daylighting Sensors\",IF(J712=\"yes-day\",\"Install Daylighting Sensors\"))","v":"No Daylighting Sensors"},{"$f":"IF(K712=\"no-occ\",\"No Occupancy Sensors\",IF(K712=\"yes-occ\",\"Install Occupancy Sensors\"))","v":"No Occupancy Sensors"},{"$f":"IF(L712=\"base-epd\",\"No Plug Load Control\",IF(L712=\"red-epd\",\"Install Plug Load Controls\"))","v":"No Plug Load Control"},{"$f":"IF(M712=\"base-eff\",\"Baseline HVAC Equipment\",IF(M712=\"high-eff\",\"Install High Efficiency HVAC Equipment\"))","v":"Install High Efficiency HVAC Equipment"}]
["new90.1-2004","5500 ft2","psz-ac","ad-e&w&flr","new90.1-20045500 ft2psz-acad-e&w&flr","base-roof","base-win","base-inf","40 fc","no-day","yes-occ","red-epd","high-eff",197.85,85.11,0.10048422215722599,0.20742699194808301,-0.31039260969976901,1438.4484000000002,-174.64120511846397,1263.8071948815364,"no",5500,402.25,1818.13,null,8690,47630,86.9,0,2077.9394029085165,-660,63.190359744076822,1481.1297626525934,-217.32256777105704,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&w&flr","new90.1-20045500 ft2psz-acad-e&w&flr","base-roof","base-win","red-inf","base-lpd","no-day","no-occ","base-epd","base-eff",249.67,63.85,3.3635565954956599E-3,-1.6023715098342401E-4,1.6936104695919999E-2,-1.111199999999779,9.5290340094400126,8.4178340094402344,"no",5500,402.25,1818.13,null,781.79590000000007,781.79590000000007,7.817959000000001,0,186.94183033858764,0,0.42089170047201174,187.36272203905963,-178.94488802961939,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&w&flr","new90.1-20045500 ft2psz-acad-e&w&flr","base-roof","eff-win","base-inf","25 fc","no-day","no-occ","red-epd","base-eff",199.84,82.95,0.101020441324624,0.19945519368665601,-0.27713625866050801,1383.1661999999999,-155.92964742719997,1227.2365525727998,"no",5500,402.25,1818.13,null,8058.1549999999997,79446.75,80.581549999999993,0,1926.8536006034842,-1045,61.361827628639993,943.21542823212417,284.02112434067567,null,null,null,{"$f":"IF(A905=\"new90.1-2004\",\"New Construction\",IF(A905=\"post1980\",\"Post 1980 Construction\",IF(A905=\"pre1980\",\"Pre 1980 Construction\")))","v":"New Construction"},"5,500 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&w&flr","new90.1-20045500 ft2psz-acad-e&w&flr","base-roof","eff-win","red-inf","base-lpd","yes-day","no-occ","red-epd","high-eff",189.65,84.92,0.12716518800168999,0.24027560789969199,-0.30746728252501898,1666.2444,-172.99528106228797,1493.249118937712,"no",5500,402.25,1818.13,null,9774.9508999999998,71153.545899999997,97.749509000000003,0,2337.3711894828616,0,74.662455946885601,2412.0336454297471,-918.78452649203518,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&w&flr","new90.1-20045500 ft2psz-acad-e&w&flr","eff-roof","base-win","base-inf","25 fc","yes-day","yes-occ","base-epd","high-eff",201.76,73.48,0.12505280946345601,0.19176381043945001,-0.13133179368745199,1329.8286000000003,-73.893327364111997,1255.9352726358884,"no",5500,402.25,1818.13,null,28105,182380,281.05,0,6720.4242714319753,-1045,62.79676363179442,5738.2210350637697,-4482.2857624278813,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&w&flr","new90.1-20045500 ft2psz-acad-e&w&flr","eff-roof","eff-win","base-inf","25 fc","no-day","no-occ","red-epd","high-eff",196.11,73.78,0.14208183029475799,0.21439730801586299,-0.135950731331794,1486.7855999999997,-76.492154821231978,1410.2934451787678,"no",5500,402.25,1818.13,null,26813.154999999999,179766.75,268.13155,0,6411.5202866275613,-1045,70.51467225893839,5437.0349588864992,-4026.7415137077314,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","psz-ac","ad-e&w&flr","new90.1-20045500 ft2psz-acad-e&w&flr","eff-roof","eff-win","red-inf","base-lpd","yes-day","yes-occ","base-epd","base-eff",212.81,66.290000000000006,0.11278476487602,0.14749829748027099,-2.0631254811393399E-2,1022.8595999999998,-11.608095975136029,1011.2515040248637,"no",5500,402.25,1818.13,null,25174.9509,105638.5459,251.74950900000002,0,6019.7954478017518,0,50.562575201243192,6070.3580230029947,-5059.1065189781311,null,null,null,"New Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","ptac","stand-alone","new90.1-20045500 ft2ptacstand-alone","base-roof","base-win","base-inf","25 fc","yes-day","yes-occ","red-epd","base-eff",133.08000000000001,139.81,0.13445201037613499,0.33748195350226501,-0.222008565684818,1883.2061999999999,-220.03405803616005,1663.1721419638397,"no",5500,642.39,3030.15,null,10175,82885,101.75,0,2433.0303135321242,-1045,83.158607098191993,1471.1889206303163,191.98322133352349,null,null,null,"New Construction","5,500 SF","Split System Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","ptac","stand-alone","new90.1-20045500 ft2ptacstand-alone","base-roof","eff-win","base-inf","25 fc","no-day","yes-occ","base-epd","base-eff",177.55,120.81,5.3680285343709298E-2,0.116094986807388,-5.5939166156804498E-2,647.82959999999991,-55.441652418560047,592.3879475814399,"no",5500,642.39,3030.15,null,10937.360199999999,90927.77,109.37360199999999,0,2615.3247092501006,-1045,29.619397379071998,1599.9441066291727,-1007.5561590477328,null,null,null,"New Construction","5,500 SF","Split System Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","ptac","stand-alone","new90.1-20045500 ft2ptacstand-alone","base-roof","eff-win","red-inf","base-lpd","yes-day","yes-occ","base-epd","high-eff",168.24,110.77,0.115061608300908,0.162443371334694,3.1815400751682599E-2,906.46140000000003,31.532439813056005,937.99383981305607,"no",5500,642.39,3030.15,null,14550.324700000001,65335.734499999999,145.50324700000002,0,3479.2512104997754,0,46.899691990652805,3526.1509024904281,-2588.1570626773719,null,null,null,"New Construction","5,500 SF","Split System Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","ptac","stand-alone","new90.1-20045500 ft2ptacstand-alone","eff-roof","base-win","base-inf","25 fc","yes-day","yes-occ","red-epd","high-eff",132.1,119.78,0.20110246433203599,0.34236073082092899,-4.6936456603443803E-2,1910.4306000000006,-46.519011482448036,1863.9115885175524,"yes",5500,642.39,3030.15,null,30305,165385,303.05,0,7246.4848797632449,-1045,93.195579425877625,6294.6804591891223,-4430.7688706715699,null,null,null,"New Construction","5,500 SF","Split System Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","ptac","stand-alone","new90.1-20045500 ft2ptacstand-alone","eff-roof","base-win","red-inf","40 fc","yes-day","no-occ","base-epd","base-eff",177.75,115.68,6.9293125810635597E-2,0.115099317966844,-1.1100428284241E-2,642.27360000000022,-11.001702901808089,631.27189709819208,"no",5500,642.39,3030.15,null,24457.964500000002,98212.964500000002,244.57964500000003,0,5848.3507651884584,-660,31.563594854909606,5219.9143600433681,-4588.6424629451758,null,null,null,"New Construction","5,500 SF","Split System Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","ptac","stand-alone","new90.1-20045500 ft2ptacstand-alone","eff-roof","eff-win","red-inf","base-lpd","yes-day","no-occ","red-epd","base-eff",145.41,124.13,0.14505512321660199,0.27609896948274998,-8.49576086006468E-2,1540.6788000000004,-84.202009610687995,1456.4767903893123,"no",5500,642.39,3030.15,null,26265.324699999997,115330.73450000001,262.65324699999996,0,6280.5239498637875,0,72.823839519465622,6353.3477893832533,-4896.8709989939407,null,null,null,"New Construction","5,500 SF","Split System Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","ptac","ad-e&flr","new90.1-20045500 ft2ptacad-e&flr","base-roof","base-win","red-inf","base-lpd","no-day","no-occ","base-epd","base-eff",213.54,102.8,3.94328113180205E-3,-3.2791492949825799E-4,1.26776796004611E-2,-1.9445999999998105,11.434840811328062,9.4902408113282508,"no",5500,522.37,2424.14,null,1042.3801999999998,1042.3801999999998,10.423801999999998,0,249.252346420214,0,0.47451204056641255,249.72685846078042,-240.23661764945217,null,null,null,"New Construction","5,500 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","ptac","ad-e&flr","new90.1-20045500 ft2ptacad-e&flr","base-roof","base-win","red-inf","40 fc","yes-day","no-occ","base-epd","high-eff",187.48,102.2,8.7894931676618604E-2,0.12175012882372201,1.8440261237034201E-2,722.00220000000036,16.632495725568013,738.63469572556835,"no",5500,522.37,2424.14,null,11327.3802,46802.3802,113.273802,0,2708.5856903689014,-660,36.931734786278419,2085.5174251551798,-1346.8827294296116,null,null,null,"New Construction","5,500 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","ptac","ad-e&flr","new90.1-20045500 ft2ptacad-e&flr","base-roof","eff-win","red-inf","base-lpd","yes-day","no-occ","red-epd","high-eff",153.83000000000001,114.16,0.15615393281936599,0.27938351993254301,-9.64271993853245E-2,1656.7991999999999,-86.974092231615927,1569.825107768384,"no",5500,522.37,2424.14,null,12272.996800000001,58759.290200000003,122.72996800000001,0,2934.7000739344235,0,78.491255388419205,3013.1913293228426,-1443.3662215544587,null,null,null,"New Construction","5,500 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","ptac","ad-e&flr","new90.1-20045500 ft2ptacad-e&flr","base-roof","eff-win","red-inf","25 fc","no-day","yes-occ","base-epd","base-eff",188.89,111.54,5.40309990182034E-2,0.115144985243828,-7.1263926238955097E-2,682.83240000000046,-64.277665772768003,618.55473422723242,"no",5500,522.37,2424.14,null,11117.996800000001,86809.290200000003,111.17996800000002,0,2658.5182545605066,-1045,30.927736711361622,1644.4459912718683,-1025.8912570446359,null,null,null,"New Construction","5,500 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","ptac","ad-e&flr","new90.1-20045500 ft2ptacad-e&flr","eff-roof","base-win","red-inf","40 fc","no-day","yes-occ","red-epd","base-eff",167.1,114.56,0.113131930920153,0.21722021829765301,-0.10026892047637299,1288.1586000000002,-90.439195507775977,1197.7194044922242,"no",5500,522.37,2424.14,null,23977.3802,82002.3802,239.77380199999999,0,5733.4341882737035,-660,59.885970224611214,5133.3201584983144,-3935.60075400609,null,null,null,"New Construction","5,500 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","ptac","ad-e&flr","new90.1-20045500 ft2ptacad-e&flr","eff-roof","eff-win","red-inf","base-lpd","yes-day","yes-occ","base-epd","base-eff",179.87,106.19,9.925801934622E-2,0.15739916615917901,-1.98809066461774E-2,933.4079999999999,-17.93190945412794,915.47609054587201,"no",5500,522.37,2424.14,null,26297.996800000001,111064.2902,262.97996799999999,0,6288.3364520462701,0,45.773804527293606,6334.1102565735637,-5418.6341660276921,null,null,null,"New Construction","5,500 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","ptac","ad-e&flr","new90.1-20045500 ft2ptacad-e&flr","eff-roof","eff-win","red-inf","25 fc","no-day","yes-occ","base-epd","high-eff",186.58,92.19,0.122257810110895,0.12596617791727199,0.11457933154053,747.00419999999974,103.34670521147206,850.35090521147185,"no",5500,522.37,2424.14,null,31247.996800000001,169309.29019999999,312.47996800000004,0,7471.9728207916269,-1045,42.517545260573598,6469.4903660522004,-5619.1394608407281,null,null,null,"New Construction","5,500 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","ptac","ad-e&w&flr","new90.1-20045500 ft2ptacad-e&w&flr","base-roof","base-win","red-inf","40 fc","no-day","yes-occ","red-epd","high-eff",163.79,96.49,0.12996377554507599,0.226895119418484,-0.105395807079849,1335.3846000000008,-79.697375351679895,1255.6872246483208,"no",5500,402.25,1818.13,null,10846.795900000001,30591.795900000001,108.46795900000001,0,2593.6691134541484,-660,62.784361232416046,1996.4534746865645,-740.7662500382437,null,null,null,"New Construction","5,500 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","ptac","ad-e&w&flr","new90.1-20045500 ft2ptacad-e&w&flr","base-roof","eff-win","red-inf","base-lpd","yes-day","yes-occ","base-epd","high-eff",177.17,89.32,0.109151800970542,0.16374020579628101,-2.3255813953488198E-2,963.68820000000073,-17.585399126511884,946.10280087348883,"no",5500,402.25,1818.13,null,12304.9509,54488.545899999997,123.049509,0,2942.3408890638225,0,47.305140043674442,2989.6460291074968,-2043.543228234008,null,null,null,"New Construction","5,500 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","ptac","ad-e&w&flr","new90.1-20045500 ft2ptacad-e&w&flr","base-roof","eff-win","red-inf","25 fc","no-day","yes-occ","red-epd","base-eff",154.56,110.73,0.113167247624906,0.27046162560181303,-0.26853018673387602,1591.7940000000006,-203.05505198297598,1388.7389480170245,"no",5500,402.25,1818.13,null,10819.9509,82208.545899999997,108.19950900000001,0,2587.2499784402148,-1045,69.436947400851224,1611.6869258410661,-222.94797782404157,null,null,null,"New Construction","5,500 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","ptac","ad-e&w&flr","new90.1-20045500 ft2ptacad-e&w&flr","eff-roof","base-win","red-inf","40 fc","yes-day","no-occ","base-epd","base-eff",187.55,87.2,8.1573371608229098E-2,0.11474558670820401,1.0310459388246499E-3,675.33180000000016,0.77964823713602949,676.11144823713619,"no",5500,402.25,1818.13,null,23936.795900000001,97691.795899999997,239.36795900000001,0,5723.729733025205,-660,33.805572411856808,5097.5353054370617,-4421.4238571999258,null,null,null,"New Construction","5,500 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","ptac","ad-e&w&flr","new90.1-20045500 ft2ptacad-e&w&flr","eff-roof","eff-win","base-inf","base-lpd","no-day","no-occ","base-epd","high-eff",208.75,69.05,7.1355341398400607E-2,1.4679505333711E-2,0.20895864360178701,86.395800000000392,158.00870939289607,244.40450939289644,"no",5500,402.25,1818.13,null,23018.154999999999,99796.75,230.18154999999999,0,5504.0657372561209,0,12.220225469644824,5516.2859627257658,-5271.8814533328696,null,null,null,"New Construction","5,500 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","ptac","ad-e&w&flr","new90.1-20045500 ft2ptacad-e&w&flr","eff-roof","eff-win","red-inf","25 fc","no-day","no-occ","red-epd","high-eff",162.82,86.58,0.16629075251179001,0.23147361465118499,8.1338068507275495E-3,1362.3312000000005,6.1505583151840684,1368.4817583151846,"no",5500,402.25,1818.13,null,28969.9509,162728.5459,289.69950899999998,0,6927.2499971731922,-1045,68.42408791575923,5950.6740850889519,-4582.1923267737675,null,null,null,"New Construction","5,500 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","pthp","stand-alone","new90.1-20045500 ft2pthpstand-alone","base-roof","base-win","red-inf","40 fc","yes-day","no-occ","base-epd","high-eff",270.7,0,8.7451750758202398E-2,8.7415298520041804E-2,0,720.33540000000028,0,720.33540000000028,"no",5500,642.39,3030.15,null,16372.9645,49537.964500000002,163.729645,0,3915.078029571041,-660,36.016770000000015,3291.0947995710412,-2570.7593995710408,null,null,null,"New Construction","5,500 SF","Split System Heat Pump","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","pthp","stand-alone","new90.1-20045500 ft2pthpstand-alone","base-roof","eff-win","base-inf","base-lpd","no-day","no-occ","red-epd","base-eff",268,0,9.65329473393991E-2,9.6517547112564495E-2,0,795.34139999999991,0,795.34139999999991,"no",5500,642.39,3030.15,null,5437.3602000000001,28447.77,54.373602000000005,0,1300.1731884219255,0,39.767069999999997,1339.9402584219256,-544.59885842192568,null,null,null,"New Construction","5,500 SF","Split System Heat Pump","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","pthp","stand-alone","new90.1-20045500 ft2pthpstand-alone","base-roof","eff-win","red-inf","25 fc","no-day","yes-occ","base-epd","base-eff",274.86,0,7.3425006892748806E-2,7.3391093281192005E-2,0,604.7705999999996,0,604.7705999999996,"no",5500,642.39,3030.15,null,12240.324700000001,92230.734499999991,122.40324700000001,0,2926.8875717519413,-1045,30.238529999999983,1912.1261017519414,-1307.3555017519418,null,null,null,"New Construction","5,500 SF","Split System Heat Pump","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","pthp","stand-alone","new90.1-20045500 ft2pthpstand-alone","eff-roof","base-win","red-inf","40 fc","no-day","yes-occ","base-epd","base-eff",281.85000000000002,0,4.9834574028122497E-2,4.9826383036105502E-2,0,410.5883999999993,0,410.5883999999993,"no",5500,642.39,3030.15,null,23412.964500000002,81437.964500000002,234.12964500000001,0,5598.4719762311051,-660,20.529419999999966,4959.001396231105,-4548.4129962311054,null,null,null,"New Construction","5,500 SF","Split System Heat Pump","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","pthp","stand-alone","new90.1-20045500 ft2pthpstand-alone","eff-roof","eff-win","base-inf","base-lpd","no-day","no-occ","red-epd","base-eff",263.83,0,0.11059415494899399,0.110575464383238,0,911.18400000000042,0,911.18400000000042,"no",5500,642.39,3030.15,null,21937.360199999999,95272.77,219.37360200000001,0,5245.6277509064512,0,45.559200000000025,5291.1869509064509,-4380.0029509064507,null,null,null,"New Construction","5,500 SF","Split System Heat Pump","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","pthp","stand-alone","new90.1-20045500 ft2pthpstand-alone","eff-roof","eff-win","red-inf","25 fc","no-day","yes-occ","base-epd","base-eff",270.63,0,8.7675765095119901E-2,8.7651282742810893E-2,0,722.28000000000009,0,722.28000000000009,"no",5500,642.39,3030.15,null,28740.324699999997,159055.73450000002,287.40324699999996,0,6872.3421342364654,-1045,36.114000000000004,5863.456134236465,-5141.1761342364653,null,null,null,"New Construction","5,500 SF","Split System Heat Pump","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","pthp","ad-e&flr","new90.1-20045500 ft2pthpad-e&flr","base-roof","base-win","base-inf","base-lpd","yes-day","yes-occ","base-epd","high-eff",273.83999999999997,0,0.10360752292349901,0.10360404595895099,0,879.23700000000099,0,879.23700000000099,"no",5500,522.37,2424.14,null,13420,38885,134.19999999999999,0,3208.9697108207474,0,43.961850000000055,3252.9315608207476,-2373.6945608207466,null,null,null,"New Construction","5,500 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","pthp","ad-e&flr","new90.1-20045500 ft2pthpad-e&flr","base-roof","base-win","red-inf","25 fc","yes-day","yes-occ","red-epd","high-eff",244.22,0,0.200572250853357,0.200563029886412,0,1702.0806000000005,0,1702.0806000000005,"yes",5500,522.37,2424.14,null,19632.3802,102077.3802,196.323802,0,4694.4644868194455,-1045,85.104030000000023,3734.5685168194454,-2032.487916819445,null,null,null,"New Construction","5,500 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","pthp","ad-e&flr","new90.1-20045500 ft2pthpad-e&flr","base-roof","eff-win","red-inf","25 fc","no-day","yes-occ","base-epd","high-eff",276.75,0,9.4070008700890204E-2,9.40783659039576E-2,0,798.39720000000034,0,798.39720000000034,"no",5500,522.37,2424.14,null,19532.996800000001,104959.2902,195.32996800000001,0,4670.7000814276134,-1045,39.919860000000021,3665.6199414276134,-2867.2227414276131,null,null,null,"New Construction","5,500 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","pthp","ad-e&flr","new90.1-20045500 ft2pthpad-e&flr","eff-roof","base-win","base-inf","base-lpd","yes-day","yes-occ","red-epd","base-eff",252.21,0,0.17441938290609699,0.17440832760483199,0,1480.1184000000003,0,1480.1184000000003,"no",5500,522.37,2424.14,null,22330,88385,223.3,0,5339.5151745623907,0,74.005920000000017,5413.5210945623903,-3933.40269456239,null,null,null,"New Construction","5,500 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","pthp","ad-e&flr","new90.1-20045500 ft2pthpad-e&flr","eff-roof","eff-win","base-inf","base-lpd","no-day","no-occ","base-epd","base-eff",296.58999999999997,0,2.9131249581687901E-2,2.91335231922486E-2,0,247.24200000000098,0,247.24200000000098,"no",5500,522.37,2424.14,null,20250.616600000001,89286.91,202.50616600000001,0,4842.2962216724163,0,12.36210000000005,4854.6583216724166,-4607.4163216724155,null,null,null,"New Construction","5,500 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","pthp","ad-e&flr","new90.1-20045500 ft2pthpad-e&flr","eff-roof","eff-win","base-inf","40 fc","yes-day","no-occ","base-epd","high-eff",271.81,0,0.110233585436048,0.11024910799044201,0,935.63040000000024,0,935.63040000000024,"no",5500,522.37,2424.14,null,35320.616600000001,137521.91,353.206166,0,8445.8113887416166,-660,46.781520000000015,7832.5929087416171,-6896.9625087416171,null,null,null,"New Construction","5,500 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","pthp","ad-e&w&flr","new90.1-20045500 ft2pthpad-e&w&flr","base-roof","base-win","base-inf","base-lpd","yes-day","no-occ","red-epd","high-eff",243.99,0,0.16605810723457801,0.16607423610636399,0,1349.8301999999994,0,1349.8301999999994,"no",5500,402.25,1818.13,null,12265,37730,122.65,0,2932.7878914468306,0,67.491509999999977,3000.2794014468304,-1650.449201446831,null,null,null,"New Construction","5,500 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","pthp","ad-e&w&flr","new90.1-20045500 ft2pthpad-e&w&flr","base-roof","eff-win","base-inf","base-lpd","no-day","no-occ","base-epd","high-eff",284.27999999999997,0,2.8372263666381299E-2,2.8368309522182E-2,0,230.57400000000035,0,230.57400000000035,"no",5500,402.25,1818.13,null,11303.154999999999,35446.75,113.03155,0,2702.792997892107,0,11.528700000000018,2714.3216978921068,-2483.7476978921063,null,null,null,"New Construction","5,500 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","pthp","ad-e&w&flr","new90.1-20045500 ft2pthpad-e&w&flr","base-roof","eff-win","base-inf","40 fc","yes-day","no-occ","red-epd","base-eff",250.06,0,0.14533796886738101,0.14532777360038299,0,1181.2055999999995,0,1181.2055999999995,"no",5500,402.25,1818.13,null,10368.155000000001,48206.75,103.68155000000002,0,2479.2172393513179,-660,59.060279999999977,1878.2775193513178,-697.07191935131823,null,null,null,"New Construction","5,500 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","pthp","ad-e&w&flr","new90.1-20045500 ft2pthpad-e&w&flr","eff-roof","base-win","base-inf","base-lpd","yes-day","yes-occ","base-epd","base-eff",262.36,0,0.10328622093328001,0.103287989609679,0,839.51159999999936,0,839.51159999999936,"no",5500,402.25,1818.13,null,21505,87560,215.05,0,5142.2424464381647,0,41.975579999999972,5184.218026438165,-4344.7064264381661,null,null,null,"New Construction","5,500 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","5500 ft2","pthp","ad-e&w&flr","new90.1-20045500 ft2pthpad-e&w&flr","eff-roof","base-win","base-inf","25 fc","no-day","yes-occ","base-epd","high-eff",262.02,0,0.104456751515575,0.104450064939504,0,848.95680000000016,0,848.95680000000016,"no",5500,402.25,1818.13,null,31240,148280,312.40000000000003,0,7470.0606383040349,-1045,42.447840000000014,6467.5084783040347,-5618.5516783040348,null,null,null,"New Construction","5,500 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","5500 ft2","pthp","ad-e&w&flr","new90.1-20045500 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","40 fc","yes-day","no-occ","red-epd","high-eff",236.35,0,0.192176662764898,0.19218675234124,0,1562.0693999999999,0,1562.0693999999999,"no",5500,402.25,1818.13,null,35283.154999999999,133181.75,352.83154999999999,0,8436.853628702951,-660,78.103470000000002,7854.957098702951,-6292.8876987029507,null,null,null,"New Construction","5,500 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","10000 ft2","psz-ac","stand-alone","new90.1-200410000 ft2psz-acstand-alone","base-roof","base-win","base-inf","base-lpd","yes-day","yes-occ","base-epd","high-eff",322.91000000000003,151.62,7.8829194394849395E-2,0.15924180487931899,-0.15678644998855601,1699.0247999999992,-178.01968081272008,1521.0051191872792,"no",10000,866.06,4085.12,null,13200,98600,132,0,3156.3636499876206,0,76.050255959363966,3232.4139059469844,-1711.4087867597052,null,null,null,"New Construction","10,000 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","10000 ft2","psz-ac","stand-alone","new90.1-200410000 ft2psz-acstand-alone","base-roof","base-win","base-inf","25 fc","no-day","yes-occ","red-epd","base-eff",281.77,167.62,0.127630795866472,0.26635769521181002,-0.27885862516212701,2841.8940000000007,-316.62381185912005,2525.2701881408807,"no",10000,866.06,4085.12,null,13000,116600,130,0,3108.5399583211411,-1900,126.26350940704404,1334.8034677281851,1190.4667204126956,null,null,null,"New Construction","10,000 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","psz-ac","stand-alone","new90.1-200410000 ft2psz-acstand-alone","base-roof","eff-win","base-inf","40 fc","yes-day","no-occ","base-epd","base-eff",338.64,141.97,6.7016537719345598E-2,0.11828572916395499,-8.3161669336995606E-2,1262.0454000000002,-94.424064275360053,1167.6213357246402,"no",10000,866.06,4085.12,null,18318.310799999999,91940.579999999987,183.183108,0,4380.2462377496704,-1200,58.381066786232012,3238.6273045359026,-2071.0059688112624,null,null,null,"New Construction","10,000 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","psz-ac","stand-alone","new90.1-200410000 ft2psz-acstand-alone","eff-roof","base-win","base-inf","base-lpd","yes-day","yes-occ","red-epd","base-eff",267.93,159.46,0.17033670580172799,0.30239279298044602,-0.21660181582360599,3226.3692000000001,-245.93570502545609,2980.4334949745439,"no",10000,866.06,4085.12,null,40600,160700,406,0,9708.2094082952572,0,149.02167474872721,9857.2310830439837,-6876.7975880694394,null,null,null,"New Construction","10,000 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","psz-ac","stand-alone","new90.1-200410000 ft2psz-acstand-alone","eff-roof","base-win","base-inf","25 fc","no-day","yes-occ","red-epd","high-eff",278.35000000000002,156.02000000000001,0.15679272845317299,0.27526232197255701,-0.19035629816128799,2936.9015999999992,-216.13581685048015,2720.7657831495189,"no",10000,866.06,4085.12,null,47100,299000,471,0,11262.479387455827,-1900,136.03828915747596,9498.5176766133027,-6777.7518934637837,null,null,null,"New Construction","10,000 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","10000 ft2","psz-ac","stand-alone","new90.1-200410000 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","40 fc","yes-day","no-occ","base-epd","high-eff",335,131,9.5384948330898597E-2,0.12776316817246899,5.3406576638432299E-4,1363.1646000000001,0.6063930733279409,1363.7709930733281,"no",10000,866.06,4085.12,null,52418.310799999999,274340.57999999996,500,0,12528.46029311936,-1200,68.188549653666414,11396.648842773027,-10032.8778496997,null,null,null,"New Construction","10,000 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","10000 ft2","psz-ac","stand-alone","new90.1-200410000 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","base-lpd","no-day","no-occ","red-epd","base-eff",322.76,133.63,0.114050749337229,0.15963235868461501,-1.9531548027771399E-2,1703.1918000000003,-22.17666096742402,1681.0151390325764,"no",10000,866.06,4085.12,null,39474.912400000001,161997.18159999998,394.74912399999999,0,9439.1801958943615,0,84.050756951628827,9523.23095284599,-7842.2158138134137,null,null,null,"New Construction","10,000 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","psz-ac","ad-e&flr","new90.1-200410000 ft2psz-acad-e&flr","base-roof","base-win","base-inf","25 fc","no-day","yes-occ","base-epd","base-eff",385.24,127.23,5.7784610128960703E-2,0.11818161008995801,-0.188621076233184,1434.2813999999998,-174.90108786417596,1259.3803121358239,"no",10000,704.17,3268.14,null,11500,115100,115,0,2749.862270822548,-1900,62.969015606791203,912.83128642933923,346.54902570648471,null,null,null,"New Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","psz-ac","ad-e&flr","new90.1-200410000 ft2psz-acad-e&flr","base-roof","eff-win","base-inf","40 fc","yes-day","no-occ","red-epd","base-eff",329.38,145.94,0.126091041079512,0.24604573442900601,-0.36341554559043299,2986.0722000000005,-336.98129360655986,2649.0909063934405,"no",10000,704.17,3268.14,null,18655.940600000002,86479.31,186.55940600000002,0,4460.979755012745,-1200,132.45454531967204,3393.434300332417,-744.34339393897653,null,null,null,"New Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","psz-ac","ad-e&flr","new90.1-200410000 ft2psz-acad-e&flr","base-roof","eff-win","red-inf","base-lpd","no-day","no-occ","red-epd","high-eff",367.73,125.98,9.2270902724400194E-2,0.15826218325817701,-0.17694319880418499,1920.7091999999998,-164.07264012617597,1756.6365598738239,"no",10000,704.17,3268.14,null,12061.2408,94084.610199999996,120.612408,0,2884.0653056717883,0,87.831827993691206,2971.8971336654795,-1215.2605737916556,null,null,null,"New Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","10000 ft2","psz-ac","ad-e&flr","new90.1-200410000 ft2psz-acad-e&flr","eff-roof","base-win","base-inf","25 fc","no-day","yes-occ","base-epd","high-eff",377.96,111.29,0.10048680502177799,0.13484560624442099,-3.9704783258594903E-2,1636.5198000000009,-36.816722309199996,1599.7030776908009,"no",10000,704.17,3268.14,null,45600,297500,456,0,10903.801699957234,-1900,79.985153884540054,9083.7868538417733,-7484.083776150972,null,null,null,"New Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","10000 ft2","psz-ac","ad-e&flr","new90.1-200410000 ft2psz-acad-e&flr","eff-roof","base-win","red-inf","base-lpd","yes-day","yes-occ","red-epd","base-eff",310.58999999999997,139.21,0.173029293705697,0.28905624098702098,-0.30054185351270601,3508.0584000000013,-278.680930985168,3229.3774690148334,"no",10000,704.17,3268.14,null,42005.300199999998,162105.3002,420.05300199999999,0,10044.242625613462,0,161.46887345074168,10205.711499064204,-6976.334030049371,null,null,null,"New Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","psz-ac","ad-e&flr","new90.1-200410000 ft2psz-acad-e&flr","eff-roof","eff-win","red-inf","base-lpd","no-day","yes-occ","base-epd","base-eff",402.58,97.35,8.0843795371082106E-2,7.8490168700071E-2,9.0526905829596493E-2,952.57620000000065,83.942126864976103,1036.5183268649766,"no",10000,704.17,3268.14,null,40061.2408,156784.6102,400.61240800000002,0,9579.3821389788609,0,51.825916343248835,9631.2080553221094,-8594.6897284571332,null,null,null,"New Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","psz-ac","ad-e&w&flr","new90.1-200410000 ft2psz-acad-e&w&flr","base-roof","base-win","base-inf","25 fc","no-day","yes-occ","red-epd","base-eff",318.89,130.72,0.13300130779842001,0.26194829541509501,-0.51121387283236996,3144.1404000000002,-383.06716717948797,2761.0732328205122,"no",10000,542.29,2451.0500000000002,null,13000,116600,130,0,3108.5399583211411,-1900,138.05366164102563,1346.5936199621667,1414.4796128583455,null,null,null,"New Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","psz-ac","ad-e&w&flr","new90.1-200410000 ft2psz-acad-e&w&flr","base-roof","base-win","red-inf","base-lpd","yes-day","yes-occ","red-epd","high-eff",303.47000000000003,133.66999999999999,0.157043300668231,0.29763695697456399,-0.54531791907514404,3572.5079999999998,-408.62230384116788,3163.8856961588317,"no",10000,542.29,2451.0500000000002,null,15753.951499999999,101153.9515,157.53951499999999,0,3767.0605953233289,0,158.19428480794159,3925.2548801312705,-761.3691839724388,null,null,null,"New Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","10000 ft2","psz-ac","ad-e&w&flr","new90.1-200410000 ft2psz-acad-e&w&flr","base-roof","eff-win","red-inf","base-lpd","no-day","no-occ","base-epd","high-eff",426.23,81.98,1.99752772353501E-2,1.3516328372717301E-2,5.2254335260115602E-2,162.23519999999931,39.155667020607964,201.39086702060729,"no",10000,542.29,2451.0500000000002,null,9047.5936999999994,85272.421499999997,90.475937000000002,0,2163.4466571618937,0,10.069543351030365,2173.5162005129241,-1972.1253334923167,null,null,null,"New Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","10000 ft2","psz-ac","ad-e&w&flr","new90.1-200410000 ft2psz-acad-e&w&flr","eff-roof","base-win","base-inf","25 fc","no-day","yes-occ","red-epd","high-eff",312.35000000000002,114.32,0.177215643418908,0.27708473164070602,-0.32161849710982598,3325.8215999999993,-240.99793285692792,3084.8236671430714,"no",10000,542.29,2451.0500000000002,null,47100,299000,471,0,11262.479387455827,-1900,154.24118335715357,9516.7205708129804,-6431.8969036699091,null,null,null,"New Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","10000 ft2","psz-ac","ad-e&w&flr","new90.1-200410000 ft2psz-acad-e&w&flr","eff-roof","base-win","red-inf","40 fc","no-day","no-occ","base-epd","base-eff",429.87,70.709999999999994,3.47014457442806E-2,5.0917675376674796E-3,0.18254335260115601,61.115999999999694,136.78495182641603,197.90095182641574,{"$f":"IF(P4487>0.2,\"yes\",\"no\")","v":"no"},{"$f":"IF(B4487=\"5500 ft2\",5500,IF(B4487=\"10000 ft2\",10000,25000))","v":10000},{"$f":"IF(B4487=\"5500 ft2\",IF(D4487=\"stand-alone\",642.39,IF(D4487=\"ad-e&flr\",522.37,402.25)),IF(B4487=\"10000 ft2\",IF(D4487=\"stand-alone\",866.06,IF(D4487=\"ad-e&flr\",704.17,542.29)),IF(B4487=\"25000 ft2\",IF(D4487=\"stand-alone\",1369.38,IF(D4487=\"ad-e&flr\",1113.42,857.45)))))","v":542.29},{"$f":"IF(B4487=\"5500 ft2\",IF(D4487=\"stand-alone\",3030.15,IF(D4487=\"ad-e&flr\",2424.14,1818.13)),IF(B4487=\"10000 ft2\",IF(D4487=\"stand-alone\",4085.12,IF(D4487=\"ad-e&flr\",3268.14,2451.05)),IF(B4487=\"25000 ft2\",IF(D4487=\"stand-alone\",6459.2,IF(D4487=\"ad-e&flr\",5167.32,3875.54)))))","v":2451.0500000000002},null,{"$f":"SUM(IF(F4487=\"eff-roof\",W4487*IF(AND(W$4=\"no\",X$4=\"no\"),$C$4,$C$3)),IF(G4487=\"eff-win\",X4487*IF(W$4=\"no\",$D$4,$D$3),0),IF(H4487=\"red-inf\",Y4487*IF(W$4=\"no\",$F$4,$F$3),0),IF(I4487=\"25 fc\",W4487*IF(W$4=\"no\",$H$4,$H$3),0),IF(I4487=\"40 fc\",W4487*IF(W$4=\"no\",$G$4,$G$3),0),IF(J4487=\"yes-day\",W4487*IF(W$4=\"no\",$I$4,$I$3),0),IF(K4487=\"yes-occ\",W4487*IF(W$4=\"no\",$J$4,$J$3),0),IF(L4487=\"red-epd\",W4487*IF(W$4=\"no\",$K$4,$K$3),0),IF(AND(M4487=\"high-eff\",C4487=\"psz-ac\"),W4487*IF(AND(W$4=\"no\",Y$4=\"no\"),$L$4,$L$3),0),IF(AND(M4487=\"high-eff\",C4487=\"ptac\"),W4487*IF(AND(W$4=\"no\",Y$4=\"no\"),$M$4,$M$3),0),IF(AND(M4487=\"high-eff\",C4487=\"pthp\"),W4487*IF(AND(W$4=\"no\",Y$4=\"no\"),$N$4,$N$3),0))","v":37653.951499999996},{"$f":"SUM(IF(F4487=\"eff-roof\",W4487*$C$4),IF(G4487=\"eff-win\",X4487*$D$4,0),IF(H4487=\"red-inf\",Y4487*$F$4,0),IF(I4487=\"25 fc\",W4487*$H$4,0),IF(I4487=\"40 fc\",W4487*$G$4,0),IF(J4487=\"yes-day\",W4487*$I$4,0),IF(K4487=\"yes-occ\",W4487*$J$4,0),IF(L4487=\"red-epd\",W4487*$K$4,0),IF(AND(M4487=\"high-eff\",C4487=\"psz-ac\"),W4487*$L$4,0),IF(AND(M4487=\"high-eff\",C4487=\"ptac\"),W4487*$M$4,0),IF(AND(M4487=\"high-eff\",C4487=\"pthp\"),W4487*$N$4,0))","v":143153.9515},376.53951499999994,0,{"$f":"-PMT($AE$3,$AE$4,AA4487+AC4487-AD4487)","v":9003.7548328027897},{"$f":"SUM(IF(F4487=\"eff-roof\",($C$5*W4487),0),IF(G4487=\"eff-win\",($D$5*X4487),0),IF(H4487=\"red-inf\",$F$5*(Y4487-X4487),0),IF(I4487=\"25 fc\",($H$5*W4487),0),IF(I4487=\"40 fc\",($G$5*W4487),0),IF(J4487=\"yes-day\",($I$5*W4487),0),IF(K4487=\"yes-occ\",($J$5*W4487),0),IF(L4487=\"red-epd\",($K$5*W4487),0),IF(M4487=\"high-eff\",($L$5*W4487),0))","v":-1200},{"$f":"0.05*U4487","v":9.8950475913207878},7813.6498803941104,{"$f":"U4487-AH4487","v":-7615.7489285676947},null,null,null,"New Construction",{"$f":"IF(B4487=\"5500 ft2\",\"5,500 SF\",IF(B4487=\"10000 ft2\",\"10,000 SF\",IF(B4487=\"25000 ft2\",\"25,000 SF\")))","v":"10,000 SF"},"Packaged Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration",{"$f":"IF(I4487=\"base-lpd\",\"Baseline Lighting Levels\",IF(I4487=\"40 fc\",\"Reduce Lighting Levels to 40 fc\",IF(I4487=\"25 fc\",\"Reduce Lighting Levels to 25 fc\")))","v":"Reduce Lighting Levels to 40 fc"},"No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","psz-ac","ad-e&w&flr","new90.1-200410000 ft2psz-acad-e&w&flr","eff-roof","eff-win","base-inf","40 fc","no-day","no-occ","base-epd","high-eff",423.8,68.88,4.9947150611799003E-2,1.9140417062050101E-2,0.20369942196531801,229.74059999999952,152.63779931484802,382.37839931484757,"no",10000,542.29,2451.0500000000002,null,44593.642200000002,226318.47,445.93642200000005,0,10663.162974290452,-1200,19.118919965742379,9482.2818942561935,-9099.9034949413453,null,null,null,"New Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","10000 ft2","psz-ac","ad-e&w&flr","new90.1-200410000 ft2psz-acad-e&w&flr","eff-roof","eff-win","red-inf","40 fc","yes-day","no-occ","red-epd","base-eff",323.76,105.25,0.17271896666009801,0.25067697363853098,-0.21676300578034699,3008.8518000000004,-162.42671606999997,2846.4250839300003,"no",10000,542.29,2451.0500000000002,null,48547.593700000005,202072.4215,485.47593700000004,0,11608.625761291518,-1200,142.32125419650001,10550.947015488018,-7704.521931558018,null,null,null,"New Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","ptac","stand-alone","new90.1-200410000 ft2ptacstand-alone","base-roof","base-win","red-inf","40 fc","no-day","no-occ","base-epd","base-eff",343.92,161.13,2.8065155183798801E-3,0,8.7357736081206793E-3,0,12.301116630368137,12.301116630368137,{"$f":"IF(P4679>0.2,\"yes\",\"no\")","v":"no"},{"$f":"IF(B4679=\"5500 ft2\",5500,IF(B4679=\"10000 ft2\",10000,25000))","v":10000},{"$f":"IF(B4679=\"5500 ft2\",IF(D4679=\"stand-alone\",642.39,IF(D4679=\"ad-e&flr\",522.37,402.25)),IF(B4679=\"10000 ft2\",IF(D4679=\"stand-alone\",866.06,IF(D4679=\"ad-e&flr\",704.17,542.29)),IF(B4679=\"25000 ft2\",IF(D4679=\"stand-alone\",1369.38,IF(D4679=\"ad-e&flr\",1113.42,857.45)))))","v":866.06},{"$f":"IF(B4679=\"5500 ft2\",IF(D4679=\"stand-alone\",3030.15,IF(D4679=\"ad-e&flr\",2424.14,1818.13)),IF(B4679=\"10000 ft2\",IF(D4679=\"stand-alone\",4085.12,IF(D4679=\"ad-e&flr\",3268.14,2451.05)),IF(B4679=\"25000 ft2\",IF(D4679=\"stand-alone\",6459.2,IF(D4679=\"ad-e&flr\",5167.32,3875.54)))))","v":4085.12},null,{"$f":"SUM(IF(F4679=\"eff-roof\",W4679*IF(AND(W$4=\"no\",X$4=\"no\"),$C$4,$C$3)),IF(G4679=\"eff-win\",X4679*IF(W$4=\"no\",$D$4,$D$3),0),IF(H4679=\"red-inf\",Y4679*IF(W$4=\"no\",$F$4,$F$3),0),IF(I4679=\"25 fc\",W4679*IF(W$4=\"no\",$H$4,$H$3),0),IF(I4679=\"40 fc\",W4679*IF(W$4=\"no\",$G$4,$G$3),0),IF(J4679=\"yes-day\",W4679*IF(W$4=\"no\",$I$4,$I$3),0),IF(K4679=\"yes-occ\",W4679*IF(W$4=\"no\",$J$4,$J$3),0),IF(L4679=\"red-epd\",W4679*IF(W$4=\"no\",$K$4,$K$3),0),IF(AND(M4679=\"high-eff\",C4679=\"psz-ac\"),W4679*IF(AND(W$4=\"no\",Y$4=\"no\"),$L$4,$L$3),0),IF(AND(M4679=\"high-eff\",C4679=\"ptac\"),W4679*IF(AND(W$4=\"no\",Y$4=\"no\"),$M$4,$M$3),0),IF(AND(M4679=\"high-eff\",C4679=\"pthp\"),W4679*IF(AND(W$4=\"no\",Y$4=\"no\"),$N$4,$N$3),0))","v":8356.6016},{"$f":"SUM(IF(F4679=\"eff-roof\",W4679*$C$4),IF(G4679=\"eff-win\",X4679*$D$4,0),IF(H4679=\"red-inf\",Y4679*$F$4,0),IF(I4679=\"25 fc\",W4679*$H$4,0),IF(I4679=\"40 fc\",W4679*$G$4,0),IF(J4679=\"yes-day\",W4679*$I$4,0),IF(K4679=\"yes-occ\",W4679*$J$4,0),IF(L4679=\"red-epd\",W4679*$K$4,0),IF(AND(M4679=\"high-eff\",C4679=\"psz-ac\"),W4679*$L$4,0),IF(AND(M4679=\"high-eff\",C4679=\"ptac\"),W4679*$M$4,0),IF(AND(M4679=\"high-eff\",C4679=\"pthp\"),W4679*$N$4,0))","v":22356.601600000002},83.566016000000005,0,{"$f":"-PMT($AE$3,$AE$4,AA4679+AC4679-AD4679)","v":1998.2176914900297},{"$f":"SUM(IF(F4679=\"eff-roof\",($C$5*W4679),0),IF(G4679=\"eff-win\",($D$5*X4679),0),IF(H4679=\"red-inf\",$F$5*(Y4679-X4679),0),IF(I4679=\"25 fc\",($H$5*W4679),0),IF(I4679=\"40 fc\",($G$5*W4679),0),IF(J4679=\"yes-day\",($I$5*W4679),0),IF(K4679=\"yes-occ\",($J$5*W4679),0),IF(L4679=\"red-epd\",($K$5*W4679),0),IF(M4679=\"high-eff\",($L$5*W4679),0))","v":-1200},{"$f":"0.05*U4679","v":0.61505583151840693},798.83274732154803,{"$f":"U4679-AH4679","v":-786.53163069117988},null,null,null,"New Construction",{"$f":"IF(B4679=\"5500 ft2\",\"5,500 SF\",IF(B4679=\"10000 ft2\",\"10,000 SF\",IF(B4679=\"25000 ft2\",\"25,000 SF\")))","v":"10,000 SF"},"Split System Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration",{"$f":"IF(I4679=\"base-lpd\",\"Baseline Lighting Levels\",IF(I4679=\"40 fc\",\"Reduce Lighting Levels to 40 fc\",IF(I4679=\"25 fc\",\"Reduce Lighting Levels to 25 fc\")))","v":"Reduce Lighting Levels to 40 fc"},"No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","ptac","stand-alone","new90.1-200410000 ft2ptacstand-alone","base-roof","eff-win","red-inf","base-lpd","no-day","no-occ","red-epd","base-eff",286.02,174.71,9.0303764032577505E-2,0.168353105373343,-7.4807751461088895E-2,1608.4620000000011,-105.33913959526396,1503.1228604047371,"no",10000,866.06,4085.12,null,9474.9123999999993,40497.181599999996,94.749123999999995,0,2265.6264459224972,0,75.156143020236854,2340.782588942734,-837.6597285379969,null,null,null,"New Construction","10,000 SF","Split System Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","ptac","stand-alone","new90.1-200410000 ft2ptacstand-alone","base-roof","eff-win","red-inf","40 fc","yes-day","no-occ","red-epd","high-eff",243.45,170.18,0.183303984151442,0.29213189113747401,-4.6939403260535202E-2,2791.0566000000013,-66.096844992751954,2724.9597550072494,"no",10000,866.06,4085.12,null,28174.912400000001,123697.1816,281.74912399999999,0,6737.1416167382931,-1200,136.24798775036248,5673.389604488656,-2948.4298494814066,null,null,null,"New Construction","10,000 SF","Split System Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","10000 ft2","ptac","stand-alone","new90.1-200410000 ft2ptacstand-alone","eff-roof","base-win","red-inf","base-lpd","yes-day","yes-occ","base-epd","high-eff",286.75,152.55000000000001,0.132621615672463,0.16623051872528499,6.1519532451553401E-2,1588.1826000000005,86.627581903999996,1674.8101819040005,"no",10000,866.06,4085.12,null,47456.601600000002,189456.60159999999,474.56601600000005,0,11347.749412286692,0,83.740509095200025,11431.489921381892,-9756.6797394778914,null,null,null,"New Construction","10,000 SF","Split System Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","10000 ft2","ptac","stand-alone","new90.1-200410000 ft2ptacstand-alone","eff-roof","base-win","red-inf","25 fc","no-day","yes-occ","red-epd","base-eff",247.44,182.04,0.15201041895957099,0.28053035589671999,-0.119901568748077,2680.2144000000008,-168.8371571308958,2511.377242869105,"no",10000,866.06,4085.12,null,44756.601600000002,239856.60159999999,447.56601600000005,0,10702.129574789224,-1900,125.56886214345525,8927.6984369326783,-6416.3211940635738,null,null,null,"New Construction","10,000 SF","Split System Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","ptac","stand-alone","new90.1-200410000 ft2ptacstand-alone","eff-roof","eff-win","red-inf","40 fc","yes-day","yes-occ","base-epd","base-eff",286.81,167.02,0.10395113361215,0.16605605954873201,-2.74992310058443E-2,1586.5158000000006,-38.722529111087987,1547.7932708889125,"no",10000,866.06,4085.12,null,53674.912400000001,218797.18159999998,500,0,12825.961914238193,-1200,77.389663544445625,11703.351577782638,-10155.558306893725,null,null,null,"New Construction","10,000 SF","Split System Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","ptac","ad-e&flr","new90.1-200410000 ft2ptacad-e&flr","base-roof","base-win","red-inf","base-lpd","yes-day","yes-occ","red-epd","base-eff",249.43,197.71,0.130505473859161,0.321777197705087,-0.34964844016656399,3287.4851999999992,-443.70647451228797,2843.7787254877112,"no",10000,704.17,3268.14,null,12005.3002,40605.300199999998,120.05300199999999,0,2870.6888756415988,0,142.18893627438555,3012.8778119159842,-169.09908642827304,null,null,null,"New Construction","10,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","ptac","ad-e&flr","new90.1-200410000 ft2ptacad-e&flr","base-roof","base-win","red-inf","25 fc","no-day","yes-occ","red-epd","high-eff",262.18,170.4,0.158832243378979,0.28710879082035001,-0.163219332377637,2933.2901999999995,-207.12654833246395,2726.1636516675353,"no",10000,704.17,3268.14,null,21005.300199999998,146505.3002,210.05300199999999,0,5022.7550006331576,-1900,136.30818258337678,3259.0631832165345,-532.89953154899922,null,null,null,"New Construction","10,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","10000 ft2","ptac","ad-e&flr","new90.1-200410000 ft2ptacad-e&flr","base-roof","eff-win","red-inf","40 fc","yes-day","no-occ","base-epd","high-eff",319.16000000000003,143.91,9.95230696968602E-2,0.132175000679773,1.7612123694450199E-2,1350.3857999999991,22.349916131232106,1372.7357161312311,"no",10000,704.17,3268.14,null,25161.2408,114884.6102,251.61240799999999,0,6016.517109826169,-1200,68.636785806561562,4885.1538956327304,-3512.4181795014993,null,null,null,"New Construction","10,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","10000 ft2","ptac","ad-e&flr","new90.1-200410000 ft2ptacad-e&flr","eff-roof","base-win","red-inf","base-lpd","yes-day","yes-occ","red-epd","high-eff",245.95,162.54,0.20567619322903499,0.33123963346656898,-0.10956379275035801,3384.1596,-139.03726895591984,3245.1223310440801,"yes",10000,704.17,3268.14,null,48605.300199999998,190605.3002,486.05300199999999,0,11622.424450607274,0,162.25611655220402,11784.680567159478,-8539.5582361153974,null,null,null,"New Construction","10,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","10000 ft2","ptac","ad-e&flr","new90.1-200410000 ft2ptacad-e&flr","eff-roof","base-win","red-inf","25 fc","yes-day","no-occ","base-epd","base-eff",308.87,153.97999999999999,9.9974708241500093E-2,0.16015444435380799,-5.1129769950167103E-2,1636.2419999999995,-64.884058846095826,1571.3579411539038,"no",10000,704.17,3268.14,null,44805.300199999998,268505.3002,448.05300199999999,0,10713.77430894417,-1900,78.567897057695191,8892.3422060018656,-7320.9842648479616,null,null,null,"New Construction","10,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","ptac","ad-e&flr","new90.1-200410000 ft2ptacad-e&flr","eff-roof","eff-win","red-inf","40 fc","yes-day","no-occ","red-epd","base-eff",262.08999999999997,171.13,0.15756765545398699,0.28735350898659501,-0.168202607686531,2935.7904000000003,-213.45036181145588,2722.3400381885444,"no",10000,704.17,3268.14,null,50061.2408,209384.6102,500,0,11970.421734127736,-1200,136.11700190942722,10906.538736037164,-8184.1986978486202,null,null,null,"New Construction","10,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","ptac","ad-e&w&flr","new90.1-200410000 ft2ptacad-e&w&flr","base-roof","base-win","base-inf","base-lpd","no-day","no-occ","red-epd","high-eff",302.07,134.19,0.10993385014878999,0.174852491258741,-8.1566857419198904E-2,1778.1977999999999,-87.667112886848031,1690.530687113152,"no",10000,542.29,2451.0500000000002,null,8100,30000,81,0,1936.8595124924034,0,84.526534355657603,2021.3860468480609,-330.85535973490892,null,null,null,"New Construction","10,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","10000 ft2","ptac","ad-e&w&flr","new90.1-200410000 ft2ptacad-e&w&flr","base-roof","base-win","red-inf","25 fc","yes-day","no-occ","base-epd","high-eff",303.92,132.6,0.109422089122235,0.16979895104895101,-6.8751511243652794E-2,1726.8047999999992,-73.893327364111997,1652.9114726358871,"no",10000,542.29,2451.0500000000002,null,21053.951499999999,175153.9515,210.53951499999999,0,5034.3884244850251,-1900,82.645573631794363,3217.0339981168195,-1564.1225254809324,null,null,null,"New Construction","10,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","10000 ft2","ptac","ad-e&w&flr","new90.1-200410000 ft2ptacad-e&w&flr","base-roof","eff-win","red-inf","40 fc","yes-day","no-occ","red-epd","high-eff",258.48,148.59,0.169487670350082,0.29392482517482499,-0.19763036995244601,2989.1279999999992,-212.41083082860806,2776.7171691713911,"no",10000,542.29,2451.0500000000002,null,25147.593699999998,109072.4215,251.47593699999999,0,6013.2538363134599,-1200,138.83585845856956,4952.0896947720294,-2175.3725256006383,null,null,null,"New Construction","10,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","10000 ft2","ptac","ad-e&w&flr","new90.1-200410000 ft2ptacad-e&w&flr","eff-roof","base-win","base-inf","base-lpd","no-day","yes-occ","base-epd","base-eff",342.06,117.44,6.2529615800147903E-2,6.5614073426573397E-2,5.34375755621826E-2,667.27559999999949,57.434086802351956,724.70968680235148,"no",10000,542.29,2451.0500000000002,null,33600,125100,336,0,8034.3801999684874,0,36.235484340117573,8070.6156843086046,-7345.9059975062528,null,null,null,"New Construction","10,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","ptac","ad-e&w&flr","new90.1-200410000 ft2ptacad-e&w&flr","eff-roof","base-win","red-inf","25 fc","no-day","yes-occ","red-epd","base-eff",262.31,151.12,0.15652305767736299,0.28346263111888098,-0.21802208430724601,2882.7305999999999,-234.32760905032006,2648.4029909496799,"no",10000,542.29,2451.0500000000002,null,44053.951499999996,239153.9515,440.53951499999994,0,10534.112966130118,-1900,132.42014954748399,8766.5331156776028,-6118.1301247279225,null,null,null,"New Construction","10,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","ptac","ad-e&w&flr","new90.1-200410000 ft2ptacad-e&w&flr","eff-roof","eff-win","base-inf","base-lpd","yes-day","yes-occ","red-epd","high-eff",242.96,141.26,0.21611478610284501,0.33631993006993,-0.138550818086564,3420.2736,-148.91281329297598,3271.3607867070241,"yes",10000,542.29,2451.0500000000002,null,51093.642200000002,212518.47,500,0,12214.843745165565,0,163.56803933535122,12378.411784500915,-9107.0509977938909,null,null,null,"New Construction","10,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","10000 ft2","pthp","stand-alone","new90.1-200410000 ft2pthpstand-alone","base-roof","base-win","base-inf","base-lpd","no-day","yes-occ","base-epd","high-eff",445.15,0,6.1464331883887599E-2,6.1478779701039502E-2,0,810.06480000000079,0,810.06480000000079,"no",10000,866.06,4085.12,null,18900,36600,189,0,4519.3388624822746,0,40.503240000000041,4559.8421024822746,-3749.7773024822736,null,null,null,"New Construction","10,000 SF","Split System Heat Pump","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","10000 ft2","pthp","stand-alone","new90.1-200410000 ft2pthpstand-alone","base-roof","base-win","red-inf","25 fc","no-day","yes-occ","red-epd","high-eff",382.93,0,0.19265875347671099,0.19265880963926499,0,2538.5364000000004,0,2538.5364000000004,"no",10000,866.06,4085.12,null,30056.601600000002,151356.60159999999,300.56601600000005,0,7187.0882373030117,-1900,126.92682000000002,5414.0150573030114,-2875.478657303011,null,null,null,"New Construction","10,000 SF","Split System Heat Pump","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","10000 ft2","pthp","stand-alone","new90.1-200410000 ft2pthpstand-alone","base-roof","eff-win","base-inf","40 fc","no-day","no-occ","base-epd","base-eff",470.05,0,8.9708935636777492E-3,8.9814678164069697E-3,0,118.34279999999977,0,118.34279999999977,"no",10000,866.06,4085.12,null,12818.310799999999,57840.579999999994,128.183108,0,3065.0947169214946,-1200,5.9171399999999892,1871.0118569214947,-1752.669056921495,null,null,null,"New Construction","10,000 SF","Split System Heat Pump","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","pthp","stand-alone","new90.1-200410000 ft2pthpstand-alone","eff-roof","base-win","base-inf","base-lpd","no-day","yes-occ","red-epd","base-eff",403.17,0,0.149978454185764,0.14998629588244,0,1976.2691999999997,0,1976.2691999999997,"no",10000,866.06,4085.12,null,35100,126600,351,0,8393.0578874670809,0,98.813459999999992,8491.8713474670803,-6515.6021474670806,null,null,null,"New Construction","10,000 SF","Split System Heat Pump","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","pthp","stand-alone","new90.1-200410000 ft2pthpstand-alone","eff-roof","base-win","red-inf","25 fc","yes-day","no-occ","base-epd","base-eff",422.39,0,0.109452736318408,0.109464274419683,0,1442.3376000000007,0,1442.3376000000007,"no",10000,866.06,4085.12,null,45156.601600000002,268856.60159999999,451.56601600000005,0,10797.776958122182,-1900,72.116880000000037,8969.8938381221815,-7527.5562381221807,null,null,null,"New Construction","10,000 SF","Split System Heat Pump","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","pthp","stand-alone","new90.1-200410000 ft2pthpstand-alone","eff-roof","eff-win","base-inf","40 fc","no-day","no-occ","base-epd","high-eff",453.31,0,4.4266854702863699E-2,4.4274841348485201E-2,0,583.38,0,583.38,"no",10000,866.06,4085.12,null,58118.310799999999,212340.58,500,0,13877.940701529908,-1200,29.169,12707.109701529907,-12123.729701529908,null,null,null,"New Construction","10,000 SF","Split System Heat Pump","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","10000 ft2","pthp","ad-e&flr","new90.1-200410000 ft2pthpad-e&flr","base-roof","base-win","base-inf","base-lpd","no-day","no-occ","red-epd","high-eff",435.69,0,0.115518086831881,0.115511886152784,0,1580.6819999999996,0,1580.6819999999996,"no",10000,704.17,3268.14,null,16800,34500,168,0,4017.1900999842437,0,79.034099999999981,4096.2241999842436,-2515.5421999842438,null,null,null,"New Construction","10,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","10000 ft2","pthp","ad-e&flr","new90.1-200410000 ft2pthpad-e&flr","base-roof","base-win","base-inf","40 fc","yes-day","yes-occ","base-epd","base-eff",449.85,0,8.6756440722718903E-2,8.67658701963092E-2,0,1187.3171999999988,0,1187.3171999999988,"no",10000,704.17,3268.14,null,15700,58300,157,0,3754.1597958186094,-1200,59.365859999999941,2613.5256558186093,-1426.2084558186104,null,null,null,"New Construction","10,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","pthp","ad-e&flr","new90.1-200410000 ft2pthpad-e&flr","base-roof","eff-win","base-inf","40 fc","no-day","no-occ","red-epd","base-eff",444.99,0,9.6639130926785097E-2,9.6632087537302805E-2,0,1322.3279999999993,0,1322.3279999999993,"no",10000,704.17,3268.14,null,13155.9406,52379.31,131.559406,0,3145.8282341845697,-1200,66.11639999999997,2011.9446341845696,-689.61663418457033,null,null,null,"New Construction","10,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","pthp","ad-e&flr","new90.1-200410000 ft2pthpad-e&flr","eff-roof","base-win","base-inf","base-lpd","no-day","yes-occ","base-epd","base-eff",464.06,0,5.7938214326128799E-2,5.79183499462027E-2,0,792.56339999999932,0,792.56339999999932,"no",10000,704.17,3268.14,null,33600,125100,336,0,8034.3801999684874,0,39.628169999999969,8074.0083699684874,-7281.4449699684883,null,null,null,"New Construction","10,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","pthp","ad-e&flr","new90.1-200410000 ft2pthpad-e&flr","eff-roof","base-win","base-inf","40 fc","yes-day","yes-occ","base-epd","high-eff",426.7,0,0.13375579947946101,0.13376235814775,0,1830.4241999999999,0,1830.4241999999999,"no",10000,704.17,3268.14,null,61000,212800,500,0,14560.183353903289,-1200,91.521209999999996,13451.704563903289,-11621.28036390329,null,null,null,"New Construction","10,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","10000 ft2","pthp","ad-e&flr","new90.1-200410000 ft2pthpad-e&flr","eff-roof","eff-win","base-inf","base-lpd","yes-day","yes-occ","red-epd","high-eff",379.49,0,0.229602806382256,0.229602712194726,0,3141.9179999999997,0,3141.9179999999997,"yes",10000,704.17,3268.14,null,60955.940600000002,223979.31,500,0,14549.752249147796,0,157.0959,14706.848149147796,-11564.930149147796,null,null,null,"New Construction","10,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","10000 ft2","pthp","ad-e&flr","new90.1-200410000 ft2pthpad-e&flr","eff-roof","eff-win","base-inf","25 fc","yes-day","no-occ","base-epd","base-eff",434.99,0,0.116932594017578,0.11693294626362701,0,1600.1279999999992,0,1600.1279999999992,"no",10000,704.17,3268.14,null,48455.940600000002,297379.31,484.55940600000002,0,11586.709813318132,-1900,80.006399999999971,9766.7162133181318,-8166.5882133181331,null,null,null,"New Construction","10,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","pthp","ad-e&w&flr","new90.1-200410000 ft2pthpad-e&w&flr","base-roof","base-win","base-inf","40 fc","yes-day","yes-occ","red-epd","base-eff",389.61,0,0.18064591758982501,0.18064814620092101,0,2386.3019999999992,0,2386.3019999999992,"no",10000,542.29,2451.0500000000002,null,17200,59800,172,0,4112.837483317202,-1200,119.31509999999997,3032.1525833172018,-645.85058331720256,null,null,null,"New Construction","10,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","pthp","ad-e&w&flr","new90.1-200410000 ft2pthpad-e&w&flr","base-roof","base-win","red-inf","40 fc","yes-day","no-occ","base-epd","base-eff",442.82,0,6.8733759256003002E-2,6.87472398056823E-2,0,908.12819999999999,0,908.12819999999999,"no",10000,542.29,2451.0500000000002,null,13153.951499999999,55753.951499999996,131.53951499999999,0,3145.3526036591011,-1200,45.406410000000001,1990.7590136591011,-1082.630813659101,null,null,null,"New Construction","10,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","pthp","ad-e&w&flr","new90.1-200410000 ft2pthpad-e&w&flr","base-roof","eff-win","base-inf","25 fc","yes-day","no-occ","base-epd","base-eff",430.34,0,9.4992477971201403E-2,9.4992744632079296E-2,0,1254.8226000000004,0,1254.8226000000004,"no",10000,542.29,2451.0500000000002,null,17293.642200000002,168918.47,172.93642200000002,0,4135.2290618160559,-1900,62.741130000000027,2297.9701918160558,-1043.1475918160554,null,null,null,"New Construction","10,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","pthp","ad-e&w&flr","new90.1-200410000 ft2pthpad-e&w&flr","eff-roof","base-win","base-inf","40 fc","yes-day","yes-occ","red-epd","base-eff",377.69,0,0.205712834339527,0.20571596811844101,0,2717.4396000000002,0,2717.4396000000002,"yes",10000,542.29,2451.0500000000002,null,47200,181300,472,0,11286.391233289067,-1200,135.87198000000001,10222.263213289067,-7504.823613289067,null,null,null,"New Construction","10,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","pthp","ad-e&w&flr","new90.1-200410000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","40 fc","no-day","no-occ","base-epd","base-eff",461.78,0,2.8857237754723201E-2,2.8874261319425502E-2,0,381.41940000000056,0,381.41940000000056,"no",10000,542.29,2451.0500000000002,null,40493.642200000002,165418.47,404.93642200000005,0,9682.7772951276311,-1200,19.070970000000028,8501.8482651276317,-8120.4288651276311,null,null,null,"New Construction","10,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","10000 ft2","pthp","ad-e&w&flr","new90.1-200410000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","25 fc","yes-day","no-occ","base-epd","high-eff",408.02,0,0.141922122579763,0.14193182057159701,0,1874.8722000000002,0,1874.8722000000002,"no",10000,542.29,2451.0500000000002,null,62593.642200000002,323418.46999999997,500,0,14937.479656871059,-1900,93.743610000000018,13131.223266871059,-11256.351066871059,null,null,null,"New Construction","10,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","25000 ft2","psz-ac","stand-alone","new90.1-200425000 ft2psz-acstand-alone","base-roof","base-win","base-inf","40 fc","yes-day","no-occ","red-epd","high-eff",637.64,307.10000000000002,0.15709637979982199,0.27712591685655702,-0.286390482972396,6790.8210000000026,-592.27277747764822,6198.5482225223541,"no",25000,1369.38,6459.2,null,44250,292750,442.5,0,10580.9917812085,-3000,309.9274111261177,7890.9191923346179,-1692.3709698122639,null,null,null,"New Construction","25,000 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","25000 ft2","psz-ac","stand-alone","new90.1-200425000 ft2psz-acstand-alone","base-roof","base-win","red-inf","base-lpd","no-day","yes-occ","base-epd","base-eff",818.65,255.83,4.1341152578900399E-2,7.1920098856125894E-2,-7.1629036987391703E-2,1762.3632000000016,-148.13316505584018,1614.2300349441614,"no",25000,1369.38,6459.2,null,11777.456,11777.456,117.77456000000001,0,2816.2071217976213,0,80.711501747208075,2896.9186235448292,-1282.6885886006678,null,null,null,"New Construction","25,000 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","25000 ft2","psz-ac","stand-alone","new90.1-200425000 ft2psz-acstand-alone","base-roof","eff-win","base-inf","25 fc","yes-day","no-occ","red-epd","base-eff",593.73,318.61,0.18600410303168499,0.32690541781450899,-0.33460394588028303,8010.640800000001,-691.98112424915212,7318.6596757508487,"no",25000,1369.38,6459.2,null,47082.148399999998,426633.34,470.821484,0,11258.210740385059,-4750,365.93298378754247,6874.1437241726007,444.51595157824795,null,null,null,"New Construction","25,000 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","25000 ft2","psz-ac","stand-alone","new90.1-200425000 ft2psz-acstand-alone","eff-roof","base-win","base-inf","40 fc","yes-day","yes-occ","base-epd","base-eff",733.79,259.3,0.11395237996560099,0.1681234341167,-8.6164286013488106E-2,4119.7740000000022,-178.19293597652816,3941.581064023474,"no",25000,1369.38,6459.2,null,114250,449500,500,0,27167.171379843941,-3000,197.07905320117371,24364.250433045116,-20422.669369021642,null,null,null,"New Construction","25,000 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","25000 ft2","psz-ac","stand-alone","new90.1-200425000 ft2psz-acstand-alone","eff-roof","base-win","red-inf","base-lpd","no-day","yes-occ","base-epd","high-eff",810.87,234.25,6.7534243736659894E-2,8.0740060538040406E-2,1.8765969924182099E-2,1978.491600000001,38.809156692991913,2017.300756692993,"no",25000,1369.38,6459.2,null,97027.456000000006,467777.45600000001,500,0,23089.717746337163,0,100.86503783464966,23190.582784171813,-21173.282027478821,null,null,null,"New Construction","25,000 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","25000 ft2","psz-ac","stand-alone","new90.1-200425000 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","25 fc","no-day","yes-occ","red-epd","high-eff",617.13,287.39999999999998,0.19296682346602601,0.30037751249872502,-0.203870481296863,7360.5888000000014,-421.61644112676788,6938.9723588732331,"no",25000,1369.38,6459.2,null,127582.14840000001,806383.34000000008,500,0,30323.570163672372,-4750,346.9486179436617,25920.518781616032,-18981.546422742798,null,null,null,"New Construction","25,000 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","25000 ft2","psz-ac","stand-alone","new90.1-200425000 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","40 fc","no-day","no-occ","base-epd","base-eff",874.19,211.32,3.1498021012495603E-2,8.9560022219954596E-3,0.114815900808445,219.46199999999942,237.44620199886396,456.90820199886338,"no",25000,1369.38,6459.2,null,104109.60440000001,416910.79600000003,500,0,24766.423099890868,-3000,22.84541009994317,21789.268509990812,-21332.360307991949,null,null,null,"New Construction","25,000 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","25000 ft2","psz-ac","ad-e&flr","new90.1-200425000 ft2psz-acad-e&flr","base-roof","base-win","red-inf","base-lpd","no-day","yes-occ","red-epd","base-eff",802.25,257.27,0.123320841741136,0.22167568931059201,-0.446962879640045,6347.4522000000006,-688.42939339108761,5659.022806608913,"no",25000,1113.42,5167.32,null,14971.9476,14971.9476,149.71947599999999,0,3580.0690283454087,0,282.95114033044564,3863.0201686758542,1796.0026379330588,null,null,null,"New Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","25000 ft2","psz-ac","ad-e&flr","new90.1-200425000 ft2psz-acad-e&flr","base-roof","eff-win","base-inf","25 fc","yes-day","no-occ","base-epd","base-eff",867.77,226.65,9.4436437013548605E-2,0.158109707588723,-0.27474690663667001,4527.3066000000008,-423.17573760103988,4104.1308623989607,"no",25000,1113.42,5167.32,null,41494.355600000003,411877.06,414.94355600000006,0,9922.0663405682026,-4750,205.20654311994804,5377.2728836881506,-1273.1420212891899,null,null,null,"New Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","25000 ft2","psz-ac","ad-e&flr","new90.1-200425000 ft2psz-acad-e&flr","base-roof","eff-win","red-inf","40 fc","no-day","no-occ","base-epd","high-eff",1014.96,168.57,2.0697607379648399E-2,1.53093893707433E-2,5.1912260967379199E-2,438.36839999999933,79.957258097392156,518.32565809739151,"no",25000,1113.42,5167.32,null,36966.303200000002,253849.00760000001,369.66303200000004,0,8839.3254314318983,-3000,25.916282904869576,5865.2417143367675,-5346.9160562393763,null,null,null,"New Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","25000 ft2","psz-ac","ad-e&flr","new90.1-200425000 ft2psz-acad-e&flr","eff-roof","base-win","red-inf","base-lpd","no-day","yes-occ","red-epd","high-eff",785.8,218.11,0.169328336696454,0.23763509711469399,-0.226715410573678,6804.4332000000031,-349.195782655024,6455.2374173449789,"no",25000,1113.42,5167.32,null,100221.9476,470971.94760000001,500,0,23846.016663711209,0,322.76187086724894,24168.778534578458,-17713.541117233479,null,null,null,"New Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","25000 ft2","psz-ac","ad-e&flr","new90.1-200425000 ft2psz-acad-e&flr","eff-roof","eff-win","base-inf","25 fc","yes-day","no-occ","base-epd","high-eff",849.49,187.85,0.14167387335447301,0.175844538874983,-5.6524184476940298E-2,5035.125,-87.060719813519839,4948.0642801864806,"no",25000,1113.42,5167.32,null,126744.3556,867877.06,500,0,30125.221923337736,-4750,247.40321400932405,25622.625137347059,-20674.560857160577,null,null,null,"New Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","25000 ft2","psz-ac","ad-e&flr","new90.1-200425000 ft2psz-acad-e&flr","eff-roof","eff-win","red-inf","40 fc","no-day","no-occ","red-epd","base-eff",863.7,185.43,0.13191121360622701,0.16205832702718401,-4.2913385826771601E-2,4640.3711999999996,-66.096844992751954,4574.2743550072473,"no",25000,1113.42,5167.32,null,105466.30319999999,409099.00760000001,500,0,25087.622828086322,-3000,228.71371775036238,22316.336545836682,-17742.062190829434,null,null,null,"New Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","25000 ft2","psz-ac","ad-e&w&flr","new90.1-200425000 ft2psz-acad-e&w&flr","base-roof","base-win","red-inf","base-lpd","no-day","yes-occ","base-epd","base-eff",955.29,166.25,4.50302574852669E-2,7.09735769788091E-2,-0.13745210727969401,2027.3844000000006,-174.03481204513602,1853.3495879548645,"no",25000,857.45,3875.54,null,10666.4822,10666.4822,106.664822,0,2550.552779493938,0,92.667479397743236,2643.2202588916812,-789.87067093681662,null,null,null,"New Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","25000 ft2","psz-ac","ad-e&w&flr","new90.1-200425000 ft2psz-acad-e&w&flr","base-roof","base-win","red-inf","40 fc","yes-day","yes-occ","base-epd","high-eff",855.93,195.49,0.104734406518214,0.16760189444406601,-0.33750684181718699,4787.6052000000009,-427.33386153243202,4360.271338467569,"no",25000,857.45,3875.54,null,51166.482199999999,299666.48219999997,500,0,12232.088684279359,-3000,218.01356692337845,9450.1022512027375,-5089.8309127351686,null,null,null,"New Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","25000 ft2","psz-ac","ad-e&w&flr","new90.1-200425000 ft2psz-acad-e&w&flr","base-roof","eff-win","red-inf","40 fc","no-day","no-occ","red-epd","high-eff",855.49,190.48,0.109381798046118,0.16802979762124701,-0.30322933771209598,4799.8283999999994,-383.93344299852788,4415.894957001472,"no",25000,857.45,3875.54,null,38322.9732,246036.8322,383.22973200000001,0,9163.7302702977086,-3000,220.79474785007361,6384.5250181477822,-1968.6300611463103,null,null,null,"New Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","25000 ft2","psz-ac","ad-e&w&flr","new90.1-200425000 ft2psz-acad-e&w&flr","eff-roof","base-win","red-inf","base-lpd","no-day","yes-occ","base-epd","high-eff",936.14,130.44,9.1840367045049998E-2,8.9597090258395198E-2,0.107553366174056,2559.3714,136.17855875308797,2695.549958753088,"no",25000,857.45,3875.54,null,95916.482199999999,466666.48220000003,500,0,22826.693645046387,0,134.7774979376544,22961.471142984043,-20265.921184230956,null,null,null,"New Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","25000 ft2","psz-ac","ad-e&w&flr","new90.1-200425000 ft2psz-acad-e&w&flr","eff-roof","base-win","red-inf","40 fc","yes-day","yes-occ","red-epd","base-eff",703.14,215.16,0.21809120753075201,0.31619127272019998,-0.47208538587848897,9032.1113999999998,-597.73031513759997,8434.3810848623998,"yes",25000,857.45,3875.54,null,119666.4822,454916.48220000003,500,0,28449.528680090338,-3000,421.71905424312001,25871.247734333458,-17436.866649471056,null,null,null,"New Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","25000 ft2","psz-ac","ad-e&w&flr","new90.1-200425000 ft2psz-acad-e&w&flr","eff-roof","eff-win","red-inf","40 fc","no-day","yes-occ","base-epd","base-eff",948.63,125.24,8.5630660918403698E-2,7.7450475069777397E-2,0.14313081554460899,2212.3991999999998,181.224901343168,2393.6241013431677,"no",25000,857.45,3875.54,null,108322.97319999999,402786.8322,500,0,25763.942161120383,-3000,119.68120506715839,22883.623366187541,-20489.999264844373,null,null,null,"New Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","25000 ft2","psz-ac","ad-e&w&flr","new90.1-200425000 ft2psz-acad-e&w&flr","eff-roof","eff-win","red-inf","25 fc","yes-day","no-occ","base-epd","high-eff",848.67,152.03,0.14792548352647999,0.174662296867554,-4.0161466885604798E-2,4989.2880000000014,-50.850390577648035,4938.4376094223535,"no",25000,857.45,3875.54,null,126572.97319999999,858536.83220000006,500,0,30084.646977522581,-4750,246.92188047111767,25581.568857993698,-20643.131248571342,null,null,null,"New Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","25000 ft2","ptac","stand-alone","new90.1-200425000 ft2ptacstand-alone","base-roof","base-win","red-inf","40 fc","yes-day","yes-occ","red-epd","high-eff",525.17999999999995,349.01,0.21756574160690201,0.34778073073197402,-0.118406716657053,7779.5112000000026,-320.08891513527988,7459.4222848647223,"yes",25000,1369.38,6459.2,null,62277.455999999998,223527.45600000001,500,0,14862.622274009695,-3000,372.97111424323612,12235.593388252932,-4776.1711033882093,null,null,null,"New Construction","25,000 SF","Split System Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","25000 ft2","ptac","stand-alone","new90.1-200425000 ft2ptacstand-alone","base-roof","eff-win","red-inf","40 fc","no-day","no-occ","base-epd","high-eff",799.41,271.97000000000003,4.1076811142292897E-2,7.21541938849018E-3,0.12846888418893801,161.40180000000166,347.28997585313573,508.69177585313741,"no",25000,1369.38,6459.2,null,45609.604399999997,184410.796,456.09604399999995,0,10906.098289278441,-3000,25.434588792656871,7931.5328780710979,-7422.8411022179607,null,null,null,"New Construction","25,000 SF","Split System Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","25000 ft2","ptac","stand-alone","new90.1-200425000 ft2ptacstand-alone","base-roof","eff-win","red-inf","25 fc","yes-day","no-occ","red-epd","base-eff",526.34,385.93,0.18349443924747999,0.346340130647525,-0.23671729795552099,7747.2864000000009,-639.91794752484805,7107.3684524751525,"no",25000,1369.38,6459.2,null,49859.604400000004,429410.79599999997,498.59604400000006,0,11922.351737191122,-4750,355.36842262375762,7527.7201598148795,-420.351707339727,null,null,null,"New Construction","25,000 SF","Split System Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","25000 ft2","ptac","stand-alone","new90.1-200425000 ft2ptacstand-alone","eff-roof","base-win","red-inf","25 fc","no-day","no-occ","base-epd","base-eff",749.75,304.32,5.6563766760212103E-2,6.8888005762400395E-2,2.4802922514900998E-2,1540.9566000000009,67.049748393696078,1608.006348393697,"no",25000,1369.38,6459.2,null,97527.456000000006,585277.45600000001,500,0,23208.09322075914,-4750,80.400317419684853,18538.493538178824,-16930.487189785126,null,null,null,"New Construction","25,000 SF","Split System Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","25000 ft2","ptac","stand-alone","new90.1-200425000 ft2ptacstand-alone","eff-roof","eff-win","red-inf","40 fc","no-day","no-occ","red-epd","base-eff",663.38,319.99,0.119842012264837,0.17615061722262201,-2.5411779785938601E-2,3940.3152000000009,-68.695672449872063,3871.6195275501286,"no",25000,1369.38,6459.2,null,107859.60440000001,420660.79600000003,500,0,25654.239158055701,-3000,193.58097637750643,22847.820134433208,-18976.200606883081,null,null,null,"New Construction","25,000 SF","Split System Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","25000 ft2","ptac","stand-alone","new90.1-200425000 ft2ptacstand-alone","eff-roof","eff-win","red-inf","25 fc","yes-day","no-occ","red-epd","high-eff",523.28,323.95,0.24170044693898801,0.350140334318571,-3.8101647119143697E-2,7832.2932000000019,-103.00019488385587,7729.2930051161457,"yes",25000,1369.38,6459.2,null,141359.60440000001,804410.79600000009,500,0,33585.395944328222,-4750,386.46465025580733,29221.860594584028,-21492.567589467882,null,null,null,"New Construction","25,000 SF","Split System Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","25000 ft2","ptac","ad-e&flr","new90.1-200425000 ft2ptacad-e&flr","base-roof","base-win","red-inf","40 fc","yes-day","yes-occ","base-epd","high-eff",711.93,290.10000000000002,0.116664277963187,0.17905697581900601,-8.5906793935991196E-2,4313.6784000000034,-198.81030046968039,4114.868099530323,"no",25000,1113.42,5167.32,null,57971.9476,219221.94760000001,500,0,13843.28907505407,-3000,205.74340497651616,11049.032480030586,-6934.1643805002632,null,null,null,"New Construction","25,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","25000 ft2","ptac","ad-e&flr","new90.1-200425000 ft2ptacad-e&flr","base-roof","eff-win","base-inf","base-lpd","no-day","yes-occ","red-epd","base-eff",655.44,348.47,0.11500583526135801,0.24419690732348601,-0.30439827812090597,5882.9706000000006,-704.45549604332848,5178.5151039566717,"no",25000,1113.42,5167.32,null,20744.355599999999,60627.060000000005,207.443556,0,4960.3583301709941,0,258.92575519783361,5219.2840853688276,-40.768981412155881,null,null,null,"New Construction","25,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","25000 ft2","ptac","ad-e&flr","new90.1-200425000 ft2ptacad-e&flr","base-roof","eff-win","red-inf","40 fc","no-day","no-occ","base-epd","high-eff",855.54,230.89,4.2259576994738098E-2,1.34569481440482E-2,0.135728991203444,324.19260000000207,314.11161198390386,638.30421198390593,"no",25000,1113.42,5167.32,null,43216.303200000002,172849.00760000001,432.16303200000004,0,10333.815796009369,-3000,31.915210599195298,7365.7310066085638,-6727.4267946246582,null,null,null,"New Construction","25,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","25000 ft2","ptac","ad-e&flr","new90.1-200425000 ft2ptacad-e&flr","eff-roof","base-win","red-inf","40 fc","yes-day","yes-occ","base-epd","high-eff",711.51,253.95,0.148911774943183,0.17954128757740301,4.9410443571027501E-2,4325.3460000000014,114.34840811327989,4439.6944081132815,"no",25000,1113.42,5167.32,null,132971.94760000001,522971.94760000001,500,0,31599.610238350768,-3000,221.98472040566409,28821.594958756432,-24381.900550643149,null,null,null,"New Construction","25,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","25000 ft2","ptac","ad-e&flr","new90.1-200425000 ft2ptacad-e&flr","eff-roof","eff-win","base-inf","base-lpd","no-day","yes-occ","red-epd","base-eff",654.46,308.76,0.15087733666386799,0.24532696809307999,-0.15575519371139801,5910.1950000000006,-360.45736830254407,5549.7376316974569,"no",25000,1113.42,5167.32,null,95744.355599999995,364377.06,500,0,22785.942509175104,0,277.48688158487283,23063.429390759975,-17513.691759062516,null,null,null,"New Construction","25,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","25000 ft2","ptac","ad-e&flr","new90.1-200425000 ft2ptacad-e&flr","eff-roof","eff-win","red-inf","25 fc","yes-day","yes-occ","base-epd","base-eff",687.94,291.33,0.13672938719518399,0.20672040220938401,-9.0510948905109495E-2,4980.1206000000002,-209.46549304387204,4770.6551069561283,"no",25000,1113.42,5167.32,null,127716.30319999999,726849.00760000001,500,0,30355.331439864342,-4750,238.53275534780641,25843.864195212147,-21073.209088256019,null,null,null,"New Construction","25,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","25000 ft2","ptac","ad-e&w&flr","new90.1-200425000 ft2ptacad-e&w&flr","base-roof","base-win","base-inf","40 fc","no-day","no-occ","base-epd","high-eff",855.77,207.04,3.16163711008592E-2,1.18585746616784E-2,0.10550419078890499,285.30059999999952,211.54455500956811,496.84515500956763,"no",25000,857.45,3875.54,null,33000,122750,330,0,7890.9091249690509,-3000,24.842257750478382,4915.7513827195289,-4418.9062277099611,null,null,null,"New Construction","25,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","25000 ft2","ptac","ad-e&w&flr","new90.1-200425000 ft2ptacad-e&w&flr","base-roof","eff-win","base-inf","base-lpd","no-day","yes-occ","red-epd","high-eff",646.58000000000004,279.68,0.156029119228002,0.25340630917740498,-0.208329732999222,6096.5987999999988,-417.71819994108796,5678.8806000589111,"no",25000,857.45,3875.54,null,35406.491000000002,120870.35,354.06491,0,8466.3455428798352,0,283.94403000294557,8750.2895728827807,-3071.4089728238696,null,null,null,"New Construction","25,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","25000 ft2","ptac","ad-e&w&flr","new90.1-200425000 ft2ptacad-e&w&flr","base-roof","eff-win","red-inf","25 fc","yes-day","no-occ","base-epd","high-eff",709.4,253.5,0.122656283065984,0.180869243914831,-9.5221636567873497E-2,4351.4592000000002,-190.92719051641592,4160.5320094835843,"no",25000,857.45,3875.54,null,57822.9732,473786.8322,500,0,13808.019244500612,-4750,208.02660047417922,9266.0458449747912,-5105.5138354912069,null,null,null,"New Construction","25,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","25000 ft2","ptac","ad-e&w&flr","new90.1-200425000 ft2ptacad-e&w&flr","eff-roof","base-win","base-inf","40 fc","no-day","no-occ","red-epd","base-eff",713.87,251.92,0.120011004359419,0.17570781950025399,-8.8395403093407002E-2,4227.2825999999995,-177.24003257558383,4050.0425674244157,"no",25000,857.45,3875.54,null,95250,359000,500,0,22668.903351808778,-3000,202.50212837122081,19871.405480179998,-15821.362912755581,null,null,null,"New Construction","25,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","25000 ft2","ptac","ad-e&w&flr","new90.1-200425000 ft2ptacad-e&w&flr","eff-roof","eff-win","base-inf","base-lpd","yes-day","no-occ","base-epd","base-eff",754.56,227.96,0.10477419900960799,0.12872384647360399,1.5121403266223099E-2,3096.914400000001,30.319653666399997,3127.234053666401,"no",25000,857.45,3875.54,null,94906.490999999995,425870.35,500,0,22587.57727012234,0,156.36170268332006,22743.938972805659,-19616.704919139258,null,null,null,"New Construction","25,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","25000 ft2","ptac","ad-e&w&flr","new90.1-200425000 ft2ptacad-e&w&flr","eff-roof","eff-win","red-inf","25 fc","yes-day","no-occ","red-epd","base-eff",565.32000000000005,308.31,0.204003893850256,0.347235693501455,-0.33202281171692699,8354.0015999999978,-665.73296693223995,7688.2686330677579,"yes",25000,857.45,3875.54,null,120072.97319999999,710036.83220000006,500,0,28545.765810036868,-4750,384.41343165338793,24180.179241690257,-16491.9106086225,null,null,null,"New Construction","25,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","25000 ft2","pthp","stand-alone","new90.1-200425000 ft2pthpstand-alone","base-roof","base-win","base-inf","40 fc","no-day","no-occ","red-epd","high-eff",900.51,0,0.135884463660879,0.135894754013415,0,3934.2036000000039,0,3934.2036000000039,"no",25000,1369.38,6459.2,null,58500,137750,500,0,13968.305981793399,-3000,196.71018000000021,11165.016161793399,-7230.8125617933947,null,null,null,"New Construction","25,000 SF","Split System Heat Pump","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","25000 ft2","pthp","stand-alone","new90.1-200425000 ft2pthpstand-alone","base-roof","eff-win","base-inf","base-lpd","no-day","yes-occ","base-epd","high-eff",968.74,0,7.0404956651585707E-2,7.0423075815877201E-2,0,2038.7742000000028,0,2038.7742000000028,"no",25000,1369.38,6459.2,null,57082.148399999998,150383.34,500,0,13632.628270173478,0,101.93871000000014,13734.566980173478,-11695.792780173475,null,null,null,"New Construction","25,000 SF","Split System Heat Pump","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","25000 ft2","pthp","stand-alone","new90.1-200425000 ft2pthpstand-alone","base-roof","eff-win","base-inf","40 fc","yes-day","yes-occ","red-epd","base-eff",807.12,0,0.22550090262764899,0.225509293466266,0,6528.5778000000037,0,6528.5778000000037,"yes",25000,1369.38,6459.2,null,52832.148399999998,208383.34,500,0,12626.436737586664,-3000,326.42889000000019,9952.8656275866651,-3424.2878275866615,null,null,null,"New Construction","25,000 SF","Split System Heat Pump","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","25000 ft2","pthp","stand-alone","new90.1-200425000 ft2pthpstand-alone","eff-roof","base-win","base-inf","40 fc","no-day","yes-occ","base-epd","base-eff",981.51,0,5.8169337404444098E-2,5.8169326283669102E-2,0,1684.0236000000034,0,1684.0236000000034,"no",25000,1369.38,6459.2,null,100500,364250,500,0,23911.845833239549,-3000,84.201180000000178,20996.047013239549,-19312.023413239545,null,null,null,"New Construction","25,000 SF","Split System Heat Pump","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","25000 ft2","pthp","stand-alone","new90.1-200425000 ft2pthpstand-alone","eff-roof","eff-win","base-inf","base-lpd","no-day","yes-occ","red-epd","base-eff",858.12,0,0.176558425639083,0.17657106119198199,0,5111.7978000000039,0,5111.7978000000039,"no",25000,1369.38,6459.2,null,97582.148400000005,375383.34,500,0,23221.041698353696,0,255.5898900000002,23476.631588353695,-18364.833788353691,null,null,null,"New Construction","25,000 SF","Split System Heat Pump","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","25000 ft2","pthp","stand-alone","new90.1-200425000 ft2pthpstand-alone","eff-roof","eff-win","base-inf","40 fc","yes-day","yes-occ","red-epd","high-eff",768.5,0,0.262564354008335,0.26256800974926398,0,7601.4414000000033,0,7601.4414000000033,"yes",25000,1369.38,6459.2,null,166082.14840000001,594633.34000000008,500,0,39438.481694164679,-3000,380.07207000000017,36818.553764164681,-29217.112364164677,null,null,null,"New Construction","25,000 SF","Split System Heat Pump","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","25000 ft2","pthp","ad-e&flr","new90.1-200425000 ft2pthpad-e&flr","base-roof","base-win","base-inf","40 fc","no-day","yes-occ","base-epd","high-eff",1015.35,0,6.4756974157111E-2,6.4762448648748305E-2,0,1953.2118000000019,0,1953.2118000000019,"no",25000,1113.42,5167.32,null,63750,143000,500,0,15211.248463224169,-3000,97.660590000000099,12308.909053224168,-10355.697253224167,null,null,null,"New Construction","25,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","25000 ft2","pthp","ad-e&flr","new90.1-200425000 ft2pthpad-e&flr","base-roof","base-win","base-inf","25 fc","yes-day","no-occ","red-epd","base-eff",870.15,0,0.19850676022591099,0.198505977930476,0,5986.8678000000036,0,5986.8678000000036,"no",25000,1113.42,5167.32,null,37250,367750,372.5,0,8907.1625728817307,-4750,299.34339000000017,4456.5059628817307,1530.3618371182729,null,null,null,"New Construction","25,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","25000 ft2","pthp","ad-e&flr","new90.1-200425000 ft2pthpad-e&flr","base-roof","eff-win","base-inf","25 fc","no-day","no-occ","base-epd","base-eff",1035.3699999999999,0,4.6337497860688102E-2,4.6322052944752702E-2,0,1397.0562000000054,0,1397.0562000000054,{"$f":"IF(P9735>0.2,\"yes\",\"no\")","v":"no"},{"$f":"IF(B9735=\"5500 ft2\",5500,IF(B9735=\"10000 ft2\",10000,25000))","v":25000},{"$f":"IF(B9735=\"5500 ft2\",IF(D9735=\"stand-alone\",642.39,IF(D9735=\"ad-e&flr\",522.37,402.25)),IF(B9735=\"10000 ft2\",IF(D9735=\"stand-alone\",866.06,IF(D9735=\"ad-e&flr\",704.17,542.29)),IF(B9735=\"25000 ft2\",IF(D9735=\"stand-alone\",1369.38,IF(D9735=\"ad-e&flr\",1113.42,857.45)))))","v":1113.42},{"$f":"IF(B9735=\"5500 ft2\",IF(D9735=\"stand-alone\",3030.15,IF(D9735=\"ad-e&flr\",2424.14,1818.13)),IF(B9735=\"10000 ft2\",IF(D9735=\"stand-alone\",4085.12,IF(D9735=\"ad-e&flr\",3268.14,2451.05)),IF(B9735=\"25000 ft2\",IF(D9735=\"stand-alone\",6459.2,IF(D9735=\"ad-e&flr\",5167.32,3875.54)))))","v":5167.32},null,{"$f":"SUM(IF(F9735=\"eff-roof\",W9735*IF(AND(W$4=\"no\",X$4=\"no\"),$C$4,$C$3)),IF(G9735=\"eff-win\",X9735*IF(W$4=\"no\",$D$4,$D$3),0),IF(H9735=\"red-inf\",Y9735*IF(W$4=\"no\",$F$4,$F$3),0),IF(I9735=\"25 fc\",W9735*IF(W$4=\"no\",$H$4,$H$3),0),IF(I9735=\"40 fc\",W9735*IF(W$4=\"no\",$G$4,$G$3),0),IF(J9735=\"yes-day\",W9735*IF(W$4=\"no\",$I$4,$I$3),0),IF(K9735=\"yes-occ\",W9735*IF(W$4=\"no\",$J$4,$J$3),0),IF(L9735=\"red-epd\",W9735*IF(W$4=\"no\",$K$4,$K$3),0),IF(AND(M9735=\"high-eff\",C9735=\"psz-ac\"),W9735*IF(AND(W$4=\"no\",Y$4=\"no\"),$L$4,$L$3),0),IF(AND(M9735=\"high-eff\",C9735=\"ptac\"),W9735*IF(AND(W$4=\"no\",Y$4=\"no\"),$M$4,$M$3),0),IF(AND(M9735=\"high-eff\",C9735=\"pthp\"),W9735*IF(AND(W$4=\"no\",Y$4=\"no\"),$N$4,$N$3),0))","v":27744.355599999999},{"$f":"SUM(IF(F9735=\"eff-roof\",W9735*$C$4),IF(G9735=\"eff-win\",X9735*$D$4,0),IF(H9735=\"red-inf\",Y9735*$F$4,0),IF(I9735=\"25 fc\",W9735*$H$4,0),IF(I9735=\"40 fc\",W9735*$G$4,0),IF(J9735=\"yes-day\",W9735*$I$4,0),IF(K9735=\"yes-occ\",W9735*$J$4,0),IF(L9735=\"red-epd\",W9735*$K$4,0),IF(AND(M9735=\"high-eff\",C9735=\"psz-ac\"),W9735*$L$4,0),IF(AND(M9735=\"high-eff\",C9735=\"ptac\"),W9735*$M$4,0),IF(AND(M9735=\"high-eff\",C9735=\"pthp\"),W9735*$N$4,0))","v":326627.06},277.443556,0,{"$f":"-PMT($AE$3,$AE$4,AA9735+AC9735-AD9735)","v":6634.187538497762},{"$f":"SUM(IF(F9735=\"eff-roof\",($C$5*W9735),0),IF(G9735=\"eff-win\",($D$5*X9735),0),IF(H9735=\"red-inf\",$F$5*(Y9735-X9735),0),IF(I9735=\"25 fc\",($H$5*W9735),0),IF(I9735=\"40 fc\",($G$5*W9735),0),IF(J9735=\"yes-day\",($I$5*W9735),0),IF(K9735=\"yes-occ\",($J$5*W9735),0),IF(L9735=\"red-epd\",($K$5*W9735),0),IF(M9735=\"high-eff\",($L$5*W9735),0))","v":-4750},{"$f":"0.05*U9735","v":69.852810000000275},1954.0403484977624,{"$f":"U9735-AH9735","v":-556.98414849775691},null,null,null,"New Construction",{"$f":"IF(B9735=\"5500 ft2\",\"5,500 SF\",IF(B9735=\"10000 ft2\",\"10,000 SF\",IF(B9735=\"25000 ft2\",\"25,000 SF\")))","v":"25,000 SF"},"Split System Heat Pump","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration",{"$f":"IF(I9735=\"base-lpd\",\"Baseline Lighting Levels\",IF(I9735=\"40 fc\",\"Reduce Lighting Levels to 40 fc\",IF(I9735=\"25 fc\",\"Reduce Lighting Levels to 25 fc\")))","v":"Reduce Lighting Levels to 25 fc"},"No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","25000 ft2","pthp","ad-e&flr","new90.1-200425000 ft2pthpad-e&flr","eff-roof","base-win","base-inf","40 fc","no-day","no-occ","red-epd","base-eff",948.04,0,0.12677562895772701,0.12676160123795699,0,3823.0836000000036,0,3823.0836000000036,"no",25000,1113.42,5167.32,null,95250,359000,500,0,22668.903351808778,-3000,191.1541800000002,19860.057531808779,-16036.973931808776,null,null,null,"New Construction","25,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","25000 ft2","pthp","ad-e&flr","new90.1-200425000 ft2pthpad-e&flr","eff-roof","base-win","base-inf","25 fc","yes-day","no-occ","red-epd","high-eff",815.29,0,0.24903730960123199,0.24903745187259399,0,7510.8786000000036,0,7510.8786000000036,"yes",25000,1113.42,5167.32,null,150500,754000,500,0,35749.393275437345,-4750,375.54393000000022,31374.937205437345,-23864.058605437342,null,null,null,"New Construction","25,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","25000 ft2","pthp","ad-e&flr","new90.1-200425000 ft2pthpad-e&flr","eff-roof","eff-win","base-inf","25 fc","no-day","no-occ","base-epd","high-eff",984.73,0,9.2974499400992602E-2,9.2966490429784707E-2,0,{"$f":"277.8*($N$9607-N9928)*$S$3","v":2803.8354000000018},{"$f":"277.78*($O$9607-O9928)*$S$4","v":0},{"$f":"SUM(S9928:T9928)","v":2803.8354000000018},"no",25000,1113.42,5167.32,null,140994.35560000001,712877.06,{"$f":"MIN(0.01*AA9928,500)","v":500},{"$f":"IF(V9928=\"yes\",0,0)","v":0},33498.922944364109,-4750,140.1917700000001,{"$f":"SUM(AE9928:AG9928)","v":28889.11471436411},-26085.27931436411,null,null,null,"New Construction","25,000 SF",{"$f":"IF(C9928=\"psz-ac\",\"Packaged Air Conditioner\",IF(C9928=\"ptac\",\"Split System Air Conditioner\",IF(C9928=\"pthp\",\"Split System Heat Pump\")))","v":"Split System Heat Pump"},{"$f":"IF(D9928=\"stand-alone\",\"Stand Alone\",IF(D9928=\"ad-e&flr\",\"Above Ground, 1 Side Attached\",IF(D9928=\"ad-e&w&flr\",\"Above Ground, 2 Sides Attached\")))","v":"Above Ground, 1 Side Attached"},{"$f":"IF(F9928=\"base-roof\",\"Baseline Roof Insulation\",IF(F9928=\"eff-roof\",\"Increased Roof Insulation\"))","v":"Increased Roof Insulation"},{"$f":"IF(G9928=\"base-win\",\"Baseline Windows\",IF(G9928=\"eff-win\",\"Replace Windows\"))","v":"Replace Windows"},{"$f":"IF(H9928=\"base-inf\",\"Baseline Infiltration\",IF(H9928=\"red-inf\",\"Reduce Infiltration\"))","v":"Baseline Infiltration"},"Reduce Lighting Levels to 25 fc",{"$f":"IF(J9928=\"no-day\",\"No Daylighting Sensors\",IF(J9928=\"yes-day\",\"Install Daylighting Sensors\"))","v":"No Daylighting Sensors"},{"$f":"IF(K9928=\"no-occ\",\"No Occupancy Sensors\",IF(K9928=\"yes-occ\",\"Install Occupancy Sensors\"))","v":"No Occupancy Sensors"},{"$f":"IF(L9928=\"base-epd\",\"No Plug Load Control\",IF(L9928=\"red-epd\",\"Install Plug Load Controls\"))","v":"No Plug Load Control"},{"$f":"IF(M9928=\"base-eff\",\"Baseline HVAC Equipment\",IF(M9928=\"high-eff\",\"Install High Efficiency HVAC Equipment\"))","v":"Install High Efficiency HVAC Equipment"}]
["new90.1-2004","25000 ft2","pthp","ad-e&w&flr","new90.1-200425000 ft2pthpad-e&w&flr","base-roof","base-win","base-inf","40 fc","no-day","no-occ","red-epd","high-eff",923.13,0,0.12858740216175901,0.12858005928219499,0,3783.913799999998,0,3783.913799999998,"no",25000,857.45,3875.54,null,58500,137750,500,0,13968.305981793399,-3000,189.1956899999999,11157.5016717934,-7373.5878717934011,null,null,null,"New Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","25000 ft2","pthp","ad-e&w&flr","new90.1-200425000 ft2pthpad-e&w&flr","base-roof","base-win","base-inf","25 fc","yes-day","yes-occ","base-epd","base-eff",928.76,0,0.12328166451075399,0.123265429418317,0,3627.5123999999983,0,3627.5123999999983,"no",25000,857.45,3875.54,null,42500,373000,425,0,10162.534479126809,-4750,181.37561999999991,5593.9100991268087,-1966.3976991268105,null,null,null,"New Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["new90.1-2004","25000 ft2","pthp","ad-e&w&flr","new90.1-200425000 ft2pthpad-e&w&flr","base-roof","eff-win","base-inf","25 fc","no-day","no-occ","red-epd","base-eff",901.06,0,0.149415711122317,0.14941378594219001,0,4397.0183999999999,0,4397.0183999999999,"no",25000,857.45,3875.54,null,29656.491000000002,319370.34999999998,296.56491,0,7091.4144074685619,-4750,219.85092,2561.2653274685617,1835.7530725314382,null,null,null,{"$f":"IF(A10121=\"new90.1-2004\",\"New Construction\",IF(A10121=\"post1980\",\"Post 1980 Construction\",IF(A10121=\"pre1980\",\"Pre 1980 Construction\")))","v":"New Construction"},"25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["new90.1-2004","25000 ft2","pthp","ad-e&w&flr","new90.1-200425000 ft2pthpad-e&w&flr","base-roof","eff-win","red-inf","base-lpd","no-day","yes-occ","red-epd","high-eff",874.41,0,0.17458507816096999,0.17457095927653099,0,5137.3553999999995,0,5137.3553999999995,"no",25000,857.45,3875.54,null,58822.9732,133786.8322,500,0,14044.77019334457,0,256.86777000000001,14301.63796334457,-9164.2825633445718,null,null,null,"New Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","25000 ft2","pthp","ad-e&w&flr","new90.1-200425000 ft2pthpad-e&w&flr","eff-roof","base-win","base-inf","25 fc","yes-day","yes-occ","base-epd","high-eff",876.65,0,0.17245839819341799,0.17245643513886,0,5075.1281999999992,0,5075.1281999999992,"no",25000,857.45,3875.54,null,155750,759250,500,0,36992.335756868109,-4750,253.75640999999996,32496.092166868111,-27420.963966868112,null,null,null,"New Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["new90.1-2004","25000 ft2","pthp","ad-e&w&flr","new90.1-200425000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","40 fc","yes-day","yes-occ","red-epd","high-eff",785.37,0,0.258621823682884,0.258623293748938,0,7610.886599999998,0,7610.886599999998,"yes",25000,857.45,3875.54,null,162406.49099999998,572620.35,500,0,38568.266317089357,-3000,380.54432999999995,35948.810647089354,-28337.924047089356,null,null,null,"New Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["new90.1-2004","25000 ft2","pthp","ad-e&w&flr","new90.1-200425000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","base-lpd","yes-day","no-occ","base-epd","base-eff",944.09,0,0.108789546381355,0.108794154851134,0,3201.6449999999968,0,3201.6449999999968,"no",25000,857.45,3875.54,null,96572.973199999993,427536.8322,500,0,22982.118512203902,0,160.08224999999985,23142.200762203902,-19940.555762203905,null,null,null,"New Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","5500 ft2","psz-ac","stand-alone","post19805500 ft2psz-acstand-alone","base-roof","base-win","base-inf","25 fc","yes-day","yes-occ","red-epd","base-eff",187.49,175.7,0.156831100404657,0.37925440339027899,-0.365084298034341,3182.1990000000005,-407.06300736689576,2775.1359926331047,"no",5500,642.39,3030.15,null,10175,82885,101.75,0,2433.0303135321242,-1045,138.75679963165524,1526.7871131637794,1248.3488794693253,null,null,null,"Post 1980 Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","5500 ft2","psz-ac","stand-alone","post19805500 ft2psz-acstand-alone","base-roof","base-win","red-inf","40 fc","no-day","no-occ","red-epd","high-eff",235.08,135.47999999999999,0.139719232457962,0.22169249106078701,-5.2598865667003197E-2,1860.1488000000002,-58.646872949007836,1801.5019270509924,"no",5500,642.39,3030.15,null,8012.9645,46952.964500000002,80.129644999999996,0,1916.0477179122142,-660,90.075096352549622,1346.1228142647637,455.37911278622869,null,null,null,"Post 1980 Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","psz-ac","stand-alone","post19805500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","base-lpd","yes-day","no-occ","base-epd","high-eff",248.16,124.04,0.13593373601205699,0.17838696861342901,3.6283117084919603E-2,1496.7864000000009,40.455080749168012,1537.2414807491689,"no",5500,642.39,3030.15,null,11195.324700000001,81175.734499999991,111.95324700000002,0,2677.0087827945881,0,76.862074037458456,2753.8708568320467,-1216.6293760828778,null,null,null,"Post 1980 Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","psz-ac","stand-alone","post19805500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","25 fc","yes-day","no-occ","red-epd","high-eff",191.67,152.27000000000001,0.20154505215440999,0.36541517679777502,-0.18304716028280599,3066.0786000000012,-204.094582965824,2861.9840170341772,"yes",5500,642.39,3030.15,null,26950,181225,269.5,0,6444.242452058058,-1045,143.09920085170887,5542.3416529097667,-2680.3576358755895,null,null,null,"Post 1980 Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","psz-ac","stand-alone","post19805500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","40 fc","yes-day","no-occ","red-epd","base-eff",204.42,129.41999999999999,0.22497003643095301,0.32320222487087802,-5.51627690156149E-3,2711.883600000001,-6.1505583151838223,2705.7330416848172,"yes",5500,642.39,3030.15,null,25282.964500000002,99037.964500000002,252.82964500000003,0,6045.6234933126852,-660,135.28665208424087,5520.9101453969261,-2815.1771037121089,null,null,null,"Post 1980 Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","5500 ft2","psz-ac","stand-alone","post19805500 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","base-lpd","yes-day","no-occ","base-epd","high-eff",247.95,105.17,0.18019675088110701,0.17908224076281301,0.182891772201072,1502.6202000000012,203.92132780201604,1706.5415278020173,"no",5500,642.39,3030.15,null,27695.324699999997,148000.73450000002,276.95324699999998,0,6622.4633452791131,0,85.327076390100871,6707.7904216692141,-5001.2488938671968,null,null,null,"Post 1980 Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","psz-ac","ad-e&flr","post19805500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","25 fc","yes-day","no-occ","red-epd","high-eff",207.64,161.82,0.15747756148735301,0.36852989477525699,-0.475113947128532,3366.3804000000005,-451.50295688364787,2914.8774431163524,"no",5500,522.37,2424.14,null,10450,114400,104.5,0,2498.787889573533,-1045,145.74387215581763,1599.5317617293506,1315.3456813870018,null,null,null,"Post 1980 Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","psz-ac","ad-e&flr","post19805500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","40 fc","no-day","yes-occ","base-epd","base-eff",274.02999999999997,116.41,0.109651474530831,0.16662611763274701,-6.1166818596171298E-2,1522.0662000000007,-58.127107457583939,1463.9390925424168,"no",5500,522.37,2424.14,null,6652.3801999999996,14352.3802,66.523802000000003,0,1590.7068976649525,-660,73.196954627120846,1003.9038522920733,460.03524025034346,null,null,null,"Post 1980 Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","5500 ft2","psz-ac","ad-e&flr","post19805500 ft2psz-acad-e&flr","base-roof","eff-win","red-inf","base-lpd","yes-day","no-occ","red-epd","base-eff",249.27,122.41,0.15244200955822401,0.24192567362082601,-0.115861440291705,2209.8989999999999,-110.10365659998394,2099.795343400016,"no",5500,522.37,2424.14,null,8642.9968000000008,43084.290200000003,86.429968000000017,0,2066.7000701878278,0,104.9897671700008,2171.6898373578288,-71.894493957812756,null,null,null,"Post 1980 Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","5500 ft2","psz-ac","ad-e&flr","post19805500 ft2psz-acad-e&flr","base-roof","eff-win","red-inf","40 fc","yes-day","yes-occ","red-epd","high-eff",205.85,141.56,0.20776314255740799,0.37397360257891898,-0.29042844120328198,3416.1066000000001,-275.99547594614398,3140.1111240538562,"yes",5500,522.37,2424.14,null,16507.996800000001,89889.290200000003,165.07996800000001,0,3947.3667449721174,-660,157.00555620269282,3444.3723011748102,-304.26117712095402,null,null,null,"Post 1980 Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","psz-ac","ad-e&flr","post19805500 ft2psz-acad-e&flr","eff-roof","base-win","red-inf","40 fc","no-day","yes-occ","base-epd","high-eff",265.74,92.9,0.18216575358433401,0.19183747947205201,0.15314494074749299,1752.3623999999998,145.53433759871996,1897.8967375987197,"no",5500,522.37,2424.14,null,25407.3802,114672.3802,254.073802,0,6075.3735836890291,-660,94.894836879935994,5510.2684205689648,-3612.3716829702453,null,null,null,"Post 1980 Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","psz-ac","ad-e&flr","post19805500 ft2psz-acad-e&flr","eff-roof","eff-win","red-inf","base-lpd","no-day","yes-occ","red-epd","high-eff",256.27,93.51,0.20236624315188301,0.22063743081321099,0.147584320875114,2015.4390000000003,140.25005510257597,2155.6890551025763,"yes",5500,522.37,2424.14,null,26352.996800000001,126629.2902,263.529968,0,6301.4879672545512,0,107.78445275512883,6409.27242000968,-4253.5833649071037,null,null,null,"Post 1980 Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","psz-ac","ad-e&flr","post19805500 ft2psz-acad-e&flr","eff-roof","eff-win","red-inf","25 fc","no-day","no-occ","base-epd","base-eff",269.14,90.55,0.17977619769203901,0.181497475822639,0.17456700091157701,1657.9104000000004,165.89181934616002,1823.8022193461604,"no",5500,522.37,2424.14,null,25637.996800000001,151654.29019999999,256.37996800000002,0,6130.5182695468893,-1045,91.19011096730803,5176.7083805141974,-3352.9061611680372,null,null,null,"Post 1980 Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","5500 ft2","psz-ac","ad-e&w&flr","post19805500 ft2psz-acad-e&w&flr","base-roof","base-win","red-inf","40 fc","no-day","yes-occ","red-epd","base-eff",235.17,108.87,0.15836990909204601,0.27425626465868402,-0.28475336322869998,2468.8086000000012,-209.03235513435206,2259.776244865649,"no",5500,402.25,1818.13,null,7216.7959000000001,14916.795900000001,72.167958999999996,0,1725.6691097075527,-660,112.98881224328245,1178.6579219508351,1081.1183229148139,null,null,null,"Post 1980 Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","5500 ft2","psz-ac","ad-e&w&flr","post19805500 ft2psz-acad-e&w&flr","base-roof","base-win","red-inf","25 fc","yes-day","no-occ","red-epd","high-eff",201.67,121.47,0.20950094409223399,0.37763856314035299,-0.43344347415624301,3399.4386000000013,-318.183108333392,3081.2554916666095,"yes",5500,402.25,1818.13,null,11231.795900000001,115181.7959,112.31795900000002,0,2685.7297199121203,-1045,154.06277458333048,1794.7924944954509,1286.4629971711586,null,null,null,"Post 1980 Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","psz-ac","ad-e&w&flr","post19805500 ft2psz-acad-e&w&flr","base-roof","eff-win","red-inf","25 fc","no-day","no-occ","base-epd","high-eff",259.60000000000002,91.55,0.140963599304748,0.198864337736082,-8.0363464715600699E-2,1790.1432000000002,-58.993383276624016,1731.1498167233763,"no",5500,402.25,1818.13,null,10269.9509,112898.5459,102.69950900000001,0,2455.7348263573977,-1045,86.557490836168824,1497.2923171935665,233.85749952980973,null,null,null,"Post 1980 Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","psz-ac","ad-e&w&flr","post19805500 ft2psz-acad-e&w&flr","eff-roof","base-win","red-inf","40 fc","no-day","yes-occ","red-epd","high-eff",228.67,84.7,0.23339710645108899,0.29431551660288902,4.7203209818258299E-4,2649.3786000000014,0.34651032761593104,2649.7251103276171,"yes",5500,402.25,1818.13,null,25971.795900000001,115236.7959,259.71795900000001,0,6210.3357957316302,-660,132.48625551638085,5682.8220512480111,-3033.096940920394,null,null,null,"Post 1980 Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","psz-ac","ad-e&w&flr","post19805500 ft2psz-acad-e&w&flr","eff-roof","base-win","red-inf","25 fc","yes-day","yes-occ","base-epd","base-eff",227.92,86.81,0.23008340523439699,0.29663004567337398,-2.4427661080953601E-2,2670.213600000001,-17.931909454128064,2652.2816905458731,"yes",5500,402.25,1818.13,null,26631.795900000001,149666.7959,266.31795900000003,0,6368.153978231011,-1045,132.61408452729367,5455.7680627583049,-2803.4863722124319,null,null,null,"Post 1980 Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","5500 ft2","psz-ac","ad-e&w&flr","post19805500 ft2psz-acad-e&w&flr","eff-roof","eff-win","red-inf","25 fc","no-day","no-occ","red-epd","base-eff",233.1,82.24,0.22857035675432399,0.28064436489322298,2.9502006136417298E-2,2526.313200000001,21.656895475999999,2547.970095476001,"yes",5500,402.25,1818.13,null,25339.9509,147053.5459,253.39950899999999,0,6059.249993426597,-1045,127.39850477380006,5141.6484982003967,-2593.6784027243957,null,null,null,"Post 1980 Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","5500 ft2","ptac","stand-alone","post19805500 ft2ptacstand-alone","base-roof","base-win","red-inf","40 fc","no-day","yes-occ","base-epd","base-eff",217.57,137.88,9.4320209426811297E-2,0.16495874112454401,-4.5178896300788397E-2,1193.9844000000007,-51.630038814784065,1142.3543611852167,"no",5500,642.39,3030.15,null,6912.9645,14612.9645,69.129644999999996,0,1653.0174137465792,-660,57.117718059260838,1050.13513180584,92.219229379376657,null,null,null,"Post 1980 Construction","5,500 SF","Split System Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","5500 ft2","ptac","stand-alone","post19805500 ft2ptacstand-alone","base-roof","base-win","red-inf","25 fc","yes-day","yes-occ","base-epd","high-eff",179.98,136.69999999999999,0.19313371797710399,0.30923047399731302,-3.6234081261370503E-2,2238.2346000000011,-41.407984150112007,2196.8266158498891,"no",5500,642.39,3030.15,null,14282.9645,99037.964500000002,142.829645,0,3415.3204516563337,-1045,109.84133079249446,2480.161782448828,-283.33516659893894,null,null,null,"Post 1980 Construction","5,500 SF","Split System Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","ptac","stand-alone","post19805500 ft2ptacstand-alone","base-roof","eff-win","red-inf","25 fc","no-day","no-occ","red-epd","high-eff",181.14,131.01,0.20466000703299,0.30477835348301702,6.8981200727713504E-3,2206.0098000000012,7.8831099532639701,2213.8929099532652,"yes",5500,642.39,3030.15,null,14715.324700000001,106750.73449999999,147.15324700000002,0,3518.7057561246202,-1045,110.69464549766326,2584.4004016222834,-370.50749166901824,null,null,null,"Post 1980 Construction","5,500 SF","Split System Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","ptac","stand-alone","post19805500 ft2ptacstand-alone","eff-roof","base-win","base-inf","base-lpd","yes-day","no-occ","base-epd","base-eff",217.81,132.63999999999999,0.10707075969315299,0.16403761274227599,-5.4578532443905299E-3,1187.3172000000002,-6.237185897087989,1181.0800141029122,"no",5500,642.39,3030.15,null,19525,85580,195.25,0,4668.7878989400215,0,59.054000705145612,4727.8418996451674,-3546.7618855422552,null,null,null,"Post 1980 Construction","5,500 SF","Split System Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","5500 ft2","ptac","stand-alone","post19805500 ft2ptacstand-alone","eff-roof","base-win","red-inf","25 fc","yes-day","yes-occ","red-epd","base-eff",150.46,147.26,0.24141389145752201,0.42252926501631199,-0.116282595512432,3058.3002000000001,-132.88671064073603,2925.4134893592641,"yes",5500,642.39,3030.15,null,27977.964500000002,151012.9645,279.77964500000002,0,6690.0477385184895,-1045,146.2706744679632,5791.318412986453,-2865.904923627189,null,null,null,"Post 1980 Construction","5,500 SF","Split System Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","5500 ft2","ptac","stand-alone","post19805500 ft2ptacstand-alone","eff-roof","eff-win","red-inf","25 fc","no-day","no-occ","base-epd","base-eff",214.33,120.04,0.148031414021698,0.17739397428516601,9.0054578532443794E-2,1283.9916000000003,102.91356730195183,1386.9051673019521,"no",5500,642.39,3030.15,null,26760.324699999997,157075.73450000002,267.60324699999995,0,6398.8875867383231,-1045,69.345258365097607,5423.2328451034209,-4036.3276778014688,null,null,null,"Post 1980 Construction","5,500 SF","Split System Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","5500 ft2","ptac","ad-e&flr","post19805500 ft2ptacad-e&flr","base-roof","base-win","base-inf","base-lpd","yes-day","no-occ","base-epd","high-eff",226.34,127.43,0.113135739822396,0.18013547288731099,-3.7450134332003601E-2,1381.4993999999997,-39.848687675840068,1341.6507123241597,"no",5500,522.37,2424.14,null,6655,34430,66.55,0,1591.3333402020919,0,67.082535616207991,1658.4158758182998,-316.7651634941401,null,null,null,"Post 1980 Construction","5,500 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","ptac","ad-e&flr","post19805500 ft2ptacad-e&flr","base-roof","base-win","red-inf","25 fc","yes-day","yes-occ","red-epd","high-eff",156.97999999999999,148.22999999999999,0.234856930509104,0.43137610026442602,-0.20678987218106301,3308.3202000000006,-220.03405803615993,3088.2861419638407,"yes",5500,522.37,2424.14,null,14847.3802,99602.3802,148.47380200000001,0,3550.2826636989339,-1045,154.41430709819204,2659.6969707971261,428.58917116671455,null,null,null,"Post 1980 Construction","5,500 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","ptac","ad-e&flr","post19805500 ft2ptacad-e&flr","base-roof","eff-win","base-inf","40 fc","no-day","yes-occ","base-epd","base-eff",229.09,140.58000000000001,7.3283870885070199E-2,0.170174231173253,-0.144508670520231,1305.1043999999999,-153.76395787960013,1151.3404421203998,"no",5500,522.37,2424.14,null,9360.6165999999994,35771.910000000003,93.606166000000002,0,2238.2962104326293,-660,57.567022106019991,1635.8632325386493,-484.52279041824954,null,null,null,"Post 1980 Construction","5,500 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","5500 ft2","ptac","ad-e&flr","post19805500 ft2ptacad-e&flr","eff-roof","base-win","base-inf","base-lpd","yes-day","no-occ","red-epd","base-eff",198.2,135.32,0.16391804097950999,0.28206614264498098,-0.10168525604494,2163.2286000000004,-108.19784979809594,2055.0307502019045,"no",5500,522.37,2424.14,null,20350,86405,203.5,0,4866.0606270642484,0,102.75153751009523,4968.812164574344,-2913.7814143724395,null,null,null,"Post 1980 Construction","5,500 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","5500 ft2","ptac","ad-e&flr","post19805500 ft2ptacad-e&flr","eff-roof","eff-win","base-inf","base-lpd","no-day","no-occ","base-epd","base-eff",274.70999999999998,100.14,6.0290367636694403E-2,4.9262868113160198E-3,0.18472685825938301,37.780800000000383,196.55798334017598,234.33878334017635,"no",5500,522.37,2424.14,null,20250.616600000001,89286.91,202.50616600000001,0,4842.2962216724163,0,11.716939167008817,4854.0131608394249,-4619.6743774992483,null,null,null,"Post 1980 Construction","5,500 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","5500 ft2","ptac","ad-e&flr","post19805500 ft2ptacad-e&flr","eff-roof","eff-win","base-inf","40 fc","no-day","yes-occ","base-epd","high-eff",223.27,107.56,0.17065826061328301,0.19125584090991399,0.124318163315151,1466.7839999999997,132.28031756740796,1599.0643175674077,"no",5500,522.37,2424.14,null,29490.616600000001,118271.91,294.90616600000004,0,7051.7507766637509,-660,79.953215878370386,6471.7039925421213,-4872.6396749747137,null,null,null,"Post 1980 Construction","5,500 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","ptac","ad-e&w&flr","post19805500 ft2ptacad-e&w&flr","base-roof","base-win","base-inf","base-lpd","yes-day","no-occ","red-epd","high-eff",192.6,119.92,0.16793913907374899,0.299661830478892,-0.192284748458938,2289.3498,-167.53774340233602,2121.8120565976637,"no",5500,402.25,1818.13,null,7480,35255,74.8,0,1788.6060683263183,0,106.0906028298832,1894.6966711562015,227.11538544146219,null,null,null,"Post 1980 Construction","5,500 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","ptac","ad-e&w&flr","post19805500 ft2ptacad-e&w&flr","base-roof","base-win","red-inf","25 fc","yes-day","yes-occ","base-epd","high-eff",187.73,116.05,0.19121109432627001,0.31737027744445701,-0.15380791409823,2424.6384000000003,-134.01286920548799,2290.6255307945121,"no",5500,402.25,1818.13,null,13761.795900000001,98516.795899999997,137.61795900000001,0,3290.6994194930812,-1045,114.53127653972561,2360.2306960328069,-69.60516523829483,null,null,null,"Post 1980 Construction","5,500 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","ptac","ad-e&w&flr","post19805500 ft2ptacad-e&w&flr","base-roof","eff-win","base-inf","40 fc","no-day","yes-occ","red-epd","base-eff",195.02,132.81,0.12716558472488701,0.290862150467256,-0.32044143965003002,2222.1221999999993,-279.20069647659204,1942.9215035234074,"no",5500,402.25,1818.13,null,9323.1549999999988,31431.75,93.231549999999984,0,2229.3384503939646,-660,97.14607517617037,1666.484525570135,276.43697795327239,null,null,null,"Post 1980 Construction","5,500 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","5500 ft2","ptac","ad-e&w&flr","post19805500 ft2ptacad-e&w&flr","eff-roof","base-win","base-inf","base-lpd","yes-day","yes-occ","base-epd","base-eff",214.97,103.8,0.15128131847194401,0.21831933384240601,-3.2014316961622602E-2,1667.9111999999998,-27.894081373087989,1640.0171186269117,"no",5500,402.25,1818.13,null,21505,87560,215.05,0,5142.2424464381647,0,82.000855931345598,5224.2433023695103,-3584.2261837425986,null,null,null,"Post 1980 Construction","5,500 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","5500 ft2","ptac","ad-e&w&flr","post19805500 ft2ptacad-e&w&flr","eff-roof","base-win","base-inf","25 fc","no-day","no-occ","base-epd","high-eff",221.82,89.14,0.172076375563086,0.19341114868550199,0.11374030622390099,1477.6182000000001,99.101953698175961,1576.7201536981761,"no",5500,402.25,1818.13,null,24475,143825,244.75,0,5852.4242676853792,-1045,78.836007684908807,4886.2602753702877,-3309.5401216721116,null,null,null,"Post 1980 Construction","5,500 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","ptac","ad-e&w&flr","post19805500 ft2ptacad-e&w&flr","eff-roof","eff-win","base-inf","40 fc","no-day","yes-occ","red-epd","high-eff",189.83,99.69,0.22916751724982601,0.30973419148394599,8.8486776695168093E-3,2366.3003999999996,7.7098547894560046,2374.0102547894558,"yes",5500,402.25,1818.13,null,29453.154999999999,113931.75,294.53154999999998,0,7042.7930166250853,-660,118.7005127394728,6501.4935293645585,-4127.4832745751028,null,null,null,"Post 1980 Construction","5,500 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","pthp","stand-alone","post19805500 ft2pthpstand-alone","base-roof","base-win","base-inf","base-lpd","yes-day","no-occ","base-epd","high-eff",325.95,0,0.135762980632395,0.13575500464006399,0,1422.3359999999998,0,1422.3359999999998,"no",5500,642.39,3030.15,null,11440,36905,114.4,0,2735.5151633226046,0,71.116799999999998,2806.6319633226044,-1384.2959633226046,null,null,null,"Post 1980 Construction","5,500 SF","Split System Heat Pump","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","pthp","stand-alone","post19805500 ft2pthpstand-alone","base-roof","base-win","base-inf","25 fc","no-day","no-occ","base-epd","high-eff",323.43,0,0.142431183334915,0.14243669627469199,0,1492.3415999999993,0,1492.3415999999993,"no",5500,642.39,3030.15,null,12760,79475,127.60000000000001,0,3051.1515283213662,-1045,74.617079999999973,2080.7686083213662,-588.42700832136688,null,null,null,"Post 1980 Construction","5,500 SF","Split System Heat Pump","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","pthp","stand-alone","post19805500 ft2pthpstand-alone","base-roof","eff-win","base-inf","40 fc","no-day","yes-occ","red-epd","high-eff",295.85000000000002,0,0.21556456094222301,0.215564099164788,0,2258.5139999999988,0,2258.5139999999988,"yes",5500,642.39,3030.15,null,19462.360199999999,59907.770000000004,194.62360200000001,0,4653.8095665337723,-660,112.92569999999995,4106.7352665337721,-1848.2212665337734,null,null,null,"Post 1980 Construction","5,500 SF","Split System Heat Pump","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","pthp","stand-alone","post19805500 ft2pthpstand-alone","base-roof","eff-win","base-inf","25 fc","yes-day","yes-occ","base-epd","base-eff",314.16000000000003,0,0.16700323922854901,0.16701577621635899,0,1749.8621999999989,0,1749.8621999999989,"no",5500,642.39,3030.15,null,13962.360199999999,109682.77,139.62360200000001,0,3338.6580457055966,-1045,87.493109999999945,2381.1511557055965,-631.28895570559757,null,null,null,"Post 1980 Construction","5,500 SF","Split System Heat Pump","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","5500 ft2","pthp","stand-alone","post19805500 ft2pthpstand-alone","eff-roof","base-win","base-inf","25 fc","no-day","no-occ","red-epd","base-eff",307.14,0,0.18563896832603699,0.185629060055681,0,1944.8778,0,1944.8778,"no",5500,642.39,3030.15,null,21670,128975,216.70000000000002,0,5181.6969920630108,-1045,97.243890000000007,4233.9408820630106,-2289.0630820630104,null,null,null,"Post 1980 Construction","5,500 SF","Split System Heat Pump","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","5500 ft2","pthp","stand-alone","post19805500 ft2pthpstand-alone","eff-roof","eff-win","base-inf","40 fc","yes-day","no-occ","base-epd","base-eff",317.74,0,0.157515958960736,0.15752353175129299,0,1650.4097999999992,0,1650.4097999999992,"no",5500,642.39,3030.15,null,27767.360199999999,124532.77,277.67360200000002,0,6639.688362984316,-660,82.520489999999967,6062.2088529843159,-4411.7990529843164,null,null,null,"Post 1980 Construction","5,500 SF","Split System Heat Pump","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","5500 ft2","pthp","stand-alone","post19805500 ft2pthpstand-alone","eff-roof","eff-win","base-inf","25 fc","yes-day","yes-occ","base-epd","high-eff",284.33999999999997,0,0.24605939037447699,0.24608246055945901,0,2578.2618000000002,0,2578.2618000000002,"yes",5500,642.39,3030.15,null,38877.360199999996,194657.77000000002,388.77360199999998,0,9296.2944350572307,-1045,128.91309000000001,8380.2075250572307,-5801.9457250572304,null,null,null,"Post 1980 Construction","5,500 SF","Split System Heat Pump","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","pthp","ad-e&flr","post19805500 ft2pthpad-e&flr","base-roof","base-win","base-inf","25 fc","no-day","no-occ","red-epd","high-eff",309.64,0,0.20308368305421401,0.20306789519740601,0,2191.842000000001,0,2191.842000000001,"yes",5500,522.37,2424.14,null,13585,80300,135.85,0,3248.4242564455926,-1045,109.59210000000006,2313.0163564455925,-121.17435644559146,null,null,null,"Post 1980 Construction","5,500 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","pthp","ad-e&flr","post19805500 ft2pthpad-e&flr","base-roof","eff-win","base-inf","40 fc","no-day","yes-occ","base-epd","high-eff",332.03,0,0.14546196045413301,0.14544191074278101,0,1569.8478000000014,0,1569.8478000000014,"no",5500,522.37,2424.14,null,17775.616600000001,53921.91,177.75616600000001,0,4250.4780372997375,-660,78.492390000000071,3668.9704272997374,-2099.122627299736,null,null,null,"Post 1980 Construction","5,500 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","pthp","ad-e&flr","post19805500 ft2pthpad-e&flr","base-roof","eff-win","base-inf","25 fc","yes-day","yes-occ","red-epd","base-eff",303.70999999999998,0,0.21834423059213601,0.218330159056983,0,2356.5774000000015,0,2356.5774000000015,"yes",5500,522.37,2424.14,null,13925.616599999999,105346.91,139.25616600000001,0,3329.8719727200146,-1045,117.82887000000008,2402.7008427200149,-46.123442720013372,null,null,null,"Post 1980 Construction","5,500 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","5500 ft2","pthp","ad-e&flr","post19805500 ft2pthpad-e&flr","eff-roof","base-win","base-inf","25 fc","no-day","yes-occ","base-epd","base-eff",328.77,0,0.153828950311131,0.15383229525917499,0,1660.4106000000011,0,1660.4106000000011,"no",5500,522.37,2424.14,null,22825,130130,228.25,0,5457.8788114369272,-1045,83.020530000000065,4495.899341436927,-2835.4887414369259,null,null,null,"Post 1980 Construction","5,500 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","5500 ft2","pthp","ad-e&flr","post19805500 ft2pthpad-e&flr","eff-roof","base-win","red-inf","base-lpd","yes-day","no-occ","base-epd","high-eff",317.5,0,0.18286345756646899,0.182838317805117,0,1973.4912000000008,0,1973.4912000000008,"no",5500,522.37,2424.14,null,28982.3802,104772.3802,289.823802,0,6930.2220722273432,0,98.674560000000042,7028.8966322273436,-5055.4054322273423,null,null,null,"Post 1980 Construction","5,500 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","pthp","ad-e&flr","post19805500 ft2pthpad-e&flr","eff-roof","eff-win","base-inf","25 fc","yes-day","yes-occ","red-epd","high-eff",268.51,0,0.30893399813189898,0.30892572193339202,0,3334.4334000000013,0,3334.4334000000013,"yes",5500,522.37,2424.14,null,38840.616600000001,190321.91,388.40616600000004,0,9287.5083620716487,-1045,166.72167000000007,8409.2300320716495,-5074.7966320716478,null,null,null,"Post 1980 Construction","5,500 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","pthp","ad-e&w&flr","post19805500 ft2pthpad-e&w&flr","base-roof","base-win","base-inf","25 fc","no-day","yes-occ","base-epd","high-eff",308.17,0,0.16938994819795,0.16939787612527599,0,1745.9729999999993,0,1745.9729999999993,"no",5500,402.25,1818.13,null,14740,81455,147.4,0,3524.606075819509,-1045,87.298649999999967,2566.9047258195092,-820.93172581950989,null,null,null,"Post 1980 Construction","5,500 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","pthp","ad-e&w&flr","post19805500 ft2pthpad-e&w&flr","base-roof","base-win","red-inf","base-lpd","yes-day","no-occ","red-epd","base-eff",311.16000000000003,0,0.161330320731842,0.16133901137404999,0,1662.910799999999,0,1662.910799999999,"no",5500,402.25,1818.13,null,4631.795900000001,20361.795900000001,46.317959000000009,0,1107.5478949183105,0,83.145539999999954,1190.6934349183105,472.21736508168851,null,null,null,"Post 1980 Construction","5,500 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","5500 ft2","pthp","ad-e&w&flr","post19805500 ft2pthpad-e&w&flr","base-roof","eff-win","red-inf","base-lpd","no-day","no-occ","base-epd","base-eff",363.94,0,1.9067563099305702E-2,1.90825292437065E-2,0,196.68239999999957,0,196.68239999999957,"no",5500,402.25,1818.13,null,3669.9508999999998,18078.545900000001,36.699508999999999,0,877.55300136358721,0,9.8341199999999791,887.3871213635872,-690.70472136358762,null,null,null,"Post 1980 Construction","5,500 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","5500 ft2","pthp","ad-e&w&flr","post19805500 ft2pthpad-e&w&flr","base-roof","eff-win","red-inf","40 fc","no-day","yes-occ","base-epd","high-eff",313.33999999999997,0,0.15546125867959901,0.15546331734138299,0,1602.3504000000003,0,1602.3504000000003,"no",5500,402.25,1818.13,null,17694.9509,49538.545899999997,176.94950900000001,0,4231.1893794754333,-660,80.117520000000013,3651.3068994754331,-2048.9564994754328,null,null,null,"Post 1980 Construction","5,500 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","pthp","ad-e&w&flr","post19805500 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","base-lpd","yes-day","no-occ","red-epd","high-eff",278.45,0,0.24950402292516299,0.24950137458897101,0,2571.5946000000004,0,2571.5946000000004,"yes",5500,402.25,1818.13,null,29546.795900000001,105336.7959,295.46795900000001,0,7065.1842842699434,0,128.57973000000001,7193.7640142699438,-4622.1694142699434,null,null,null,"Post 1980 Construction","5,500 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","pthp","ad-e&w&flr","post19805500 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","base-lpd","no-day","no-occ","base-epd","high-eff",334.37,0,9.8782100738454795E-2,9.87817368335938E-2,0,1018.1369999999994,0,1018.1369999999994,"no",5500,402.25,1818.13,null,28584.9509,103053.5459,285.84950900000001,0,6835.1893907152207,0,50.90684999999997,6886.096240715221,-5867.9592407152213,null,null,null,"Post 1980 Construction","5,500 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","5500 ft2","pthp","ad-e&w&flr","post19805500 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","40 fc","no-day","yes-occ","red-epd","base-eff",290.60000000000002,0,0.21675575884492501,0.21675381381057601,0,2234.0675999999989,0,2234.0675999999989,"yes",5500,402.25,1818.13,null,26604.9509,99038.545899999997,266.049509,0,6361.7348432170775,-660,111.70337999999995,5813.4382232170774,-3579.3706232170784,null,null,null,"Post 1980 Construction","5,500 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","10000 ft2","psz-ac","stand-alone","post198010000 ft2psz-acstand-alone","base-roof","base-win","red-inf","base-lpd","yes-day","yes-occ","base-epd","base-eff",397.05,183.1,0.14359965989193299,0.21737330731476501,-7.6488917631841902E-2,3063.5783999999994,-112.7024840571039,2950.8759159428955,"no",10000,866.06,4085.12,null,10856.6016,39456.601600000002,108.566016,0,2596.0138373210184,0,147.54379579714478,2743.5576331181633,207.31828282473225,null,null,null,"Post 1980 Construction","10,000 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","10000 ft2","psz-ac","stand-alone","post198010000 ft2psz-acstand-alone","base-roof","eff-win","base-inf","25 fc","yes-day","yes-occ","red-epd","base-eff",296.66000000000003,242.96,0.203420280314874,0.41525239981865802,-0.42842024810394502,5852.4125999999997,-631.255189334448,5221.1574106655517,"yes",10000,866.06,4085.12,null,24718.310799999999,187940.58,247.183108,0,5910.6043710770009,-1900,261.05787053327759,4271.6622416102782,949.49516905527344,null,null,null,"Post 1980 Construction","10,000 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","10000 ft2","psz-ac","stand-alone","post198010000 ft2psz-acstand-alone","base-roof","eff-win","red-inf","40 fc","no-day","yes-occ","red-epd","high-eff",350.28,195.67,0.194081022518445,0.30956182366507001,-0.15039096948674199,4362.8490000000011,-221.59335451043182,4141.2556454895694,"no",10000,866.06,4085.12,null,23774.912400000001,125597.1816,237.74912400000002,0,5685.0204000757531,-1200,207.06278227447848,4692.0831823502313,-550.82753686066189,null,null,null,"Post 1980 Construction","10,000 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","10000 ft2","psz-ac","stand-alone","post198010000 ft2psz-acstand-alone","eff-roof","base-win","red-inf","base-lpd","yes-day","yes-occ","base-epd","high-eff",390.63,151.57,0.199621492635563,0.23002779256105499,0.108883532247634,3241.9259999999999,160.4342816862081,3402.3602816862081,"no",10000,866.06,4085.12,null,44956.601600000002,221856.60159999999,449.56601600000005,0,10749.953266455705,0,170.1180140843104,10920.071280540014,-7517.7109988538068,null,null,null,"Post 1980 Construction","10,000 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","10000 ft2","psz-ac","stand-alone","post198010000 ft2psz-acstand-alone","eff-roof","base-win","red-inf","25 fc","no-day","no-occ","red-epd","base-eff",355.88,169.7,0.224155901149236,0.29852364338793302,2.2929037568347002E-3,4207.2809999999999,3.3784756942561276,4210.6594756942559,"yes",10000,866.06,4085.12,null,41156.601600000002,236256.60159999999,411.56601600000005,0,9841.303124792601,-1900,210.53297378471279,8151.8360985773143,-3941.1766228830584,null,null,null,"Post 1980 Construction","10,000 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","10000 ft2","psz-ac","stand-alone","post198010000 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","40 fc","yes-day","no-occ","base-epd","base-eff",387.93,148.82,0.20767163114731599,0.23534977233753199,0.125051443353519,3316.9319999999993,184.25686670980807,3501.1888667098074,"yes",10000,866.06,4085.12,null,50074.912400000001,215197.18159999998,500,0,11973.658498399953,-1200,175.05944333549039,10948.717941735444,-7447.5290750256363,null,null,null,"Post 1980 Construction","10,000 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","10000 ft2","psz-ac","ad-e&flr","post198010000 ft2psz-acad-e&flr","base-roof","base-win","red-inf","base-lpd","yes-day","yes-occ","red-epd","base-eff",392.48,189.56,0.181514142007969,0.31140235450988601,-0.34287333522244301,4930.6722000000009,-419.27749641536002,4511.3947035846413,"no",10000,704.17,3268.14,null,12005.3002,40605.300199999998,120.05300199999999,0,2870.6888756415988,0,225.56973517923208,3096.2586108208307,1415.1360927638107,null,null,null,"Post 1980 Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","10000 ft2","psz-ac","ad-e&flr","post198010000 ft2psz-acad-e&flr","base-roof","base-win","red-inf","25 fc","no-day","no-occ","red-epd","high-eff",394.18,185.71,0.184545038866026,0.30841974138989797,-0.31559931992065698,4883.4462000000012,-385.92587738232004,4497.5203226176809,"no",10000,704.17,3268.14,null,14905.3002,175305.3002,149.05300199999999,0,3564.1324048055462,-1900,224.87601613088407,1889.0084209364304,2608.5119016812505,null,null,null,"Post 1980 Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","10000 ft2","psz-ac","ad-e&flr","post198010000 ft2psz-acad-e&flr","base-roof","eff-win","red-inf","40 fc","yes-day","no-occ","base-epd","high-eff",432.87,160.44,0.165680318766739,0.24053897573556501,-0.13658260130348501,3808.6380000000008,-167.01797791091201,3641.6200220890887,"no",10000,704.17,3268.14,null,22661.2408,147284.6102,226.61240799999999,0,5418.7209639951798,-1200,182.08100110445446,4400.8019650996339,-759.18194301054518,null,null,null,"Post 1980 Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","10000 ft2","psz-ac","ad-e&flr","post198010000 ft2psz-acad-e&flr","base-roof","eff-win","red-inf","25 fc","yes-day","yes-occ","red-epd","base-eff",332.31,213.64,0.232268600169835,0.41696931417443001,-0.51345990365542604,6602.1948000000011,-627.87671364019184,5974.3180863598091,"yes",10000,704.17,3268.14,null,24961.2408,182384.6102,249.61240799999999,0,5968.6934181596898,-1900,298.71590431799046,4367.4093224776807,1606.9087638821284,null,null,null,"Post 1980 Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","10000 ft2","psz-ac","ad-e&flr","post198010000 ft2psz-acad-e&flr","eff-roof","base-win","red-inf","25 fc","no-day","yes-occ","base-epd","base-eff",433.67,130.19999999999999,0.207067737931935,0.23913539309086401,7.7642391612354797E-2,3786.4140000000007,94.943829766784063,3881.3578297667846,"yes",10000,704.17,3268.14,null,42905.300199999998,238005.3002,429.05300199999999,0,10259.44923811262,-1900,194.06789148833923,8553.5171296009594,-4672.1592998341748,null,null,null,"Post 1980 Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","10000 ft2","psz-ac","ad-e&flr","post198010000 ft2psz-acad-e&flr","eff-roof","eff-win","red-inf","40 fc","yes-day","no-occ","red-epd","base-eff",382.91,144.41999999999999,0.25844927820236502,0.32819271189711702,-2.30943610087843E-2,5196.5268000000005,-28.24059170070392,5168.286208299297,"yes",10000,704.17,3268.14,null,50061.2408,209384.6102,500,0,11970.421734127736,-1200,258.41431041496486,11028.836044542701,-5860.5498362434037,null,null,null,"Post 1980 Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","10000 ft2","psz-ac","ad-e&flr","post198010000 ft2psz-acad-e&flr","eff-roof","eff-win","red-inf","25 fc","yes-day","yes-occ","red-epd","high-eff",321.86,168.9,0.30988307531517401,0.43530361247083199,-0.196514593369226,6892.4958000000015,-240.30491220169606,6652.1908877983051,"yes",10000,704.17,3268.14,null,59061.2408,364784.6102,500,0,14101.180273723341,-1900,332.6095443899153,12533.789818113257,-5881.5989303149518,null,null,null,"Post 1980 Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","10000 ft2","psz-ac","ad-e&w&flr","post198010000 ft2psz-acad-e&w&flr","base-roof","base-win","red-inf","25 fc","no-day","yes-occ","base-epd","high-eff",416.05,142.43,0.17225947702518499,0.26336756373937698,-0.29623225336731002,4132.2749999999987,-281.97277909752006,3850.3022209024784,"no",10000,542.29,2451.0500000000002,null,16653.951499999999,177053.9515,166.53951499999999,0,3982.2672078224846,-1900,192.51511104512394,2274.7823188676084,1575.51990203487,null,null,null,"Post 1980 Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","10000 ft2","psz-ac","ad-e&w&flr","post198010000 ft2psz-acad-e&w&flr","base-roof","eff-win","base-inf","40 fc","yes-day","no-occ","red-epd","base-eff",379.78,173.4,0.18009446043264499,0.32758498583569401,-0.57808518383691299,5139.8555999999999,-550.25840025420803,4589.5971997457918,"no",10000,542.29,2451.0500000000002,null,17493.642200000002,79518.47,174.93642200000002,0,4183.0527534825351,-1200,229.47985998728961,3212.5326134698248,1377.064586275967,null,null,null,"Post 1980 Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","10000 ft2","psz-ac","ad-e&w&flr","post198010000 ft2psz-acad-e&w&flr","base-roof","eff-win","red-inf","25 fc","yes-day","yes-occ","red-epd","high-eff",319.11,182.16,0.257039780785702,0.43500354107648698,-0.65780851838369103,6825.2681999999986,-626.14416200211201,6199.1240379978863,"yes",10000,542.29,2451.0500000000002,null,27547.593699999998,235972.4215,275.47593699999999,0,6587.1381363112096,-1900,309.95620189989432,4997.0943382111036,1202.0296997867827,null,null,null,"Post 1980 Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","10000 ft2","psz-ac","ad-e&w&flr","post198010000 ft2psz-acad-e&w&flr","eff-roof","base-win","red-inf","25 fc","no-day","yes-occ","base-epd","high-eff",416.09,100.71,0.23401677154620401,0.26329674220963201,8.3454677830360396E-2,4131.1638000000003,79.437492605968004,4210.6012926059684,"yes",10000,542.29,2451.0500000000002,null,46653.951499999996,298553.95149999997,466.53951499999994,0,11155.820957794349,-1900,210.53006463029843,9466.3510224246475,-5255.749729818679,null,null,null,"Post 1980 Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","10000 ft2","psz-ac","ad-e&w&flr","post198010000 ft2psz-acad-e&w&flr","eff-roof","eff-win","base-inf","base-lpd","yes-day","no-occ","red-epd","base-eff",421,112.82,0.20879060352780801,0.25460339943342802,-2.67564615944667E-2,3994.7639999999992,-25.468509079775977,3969.2954909202231,"yes",10000,542.29,2451.0500000000002,null,40893.642200000002,180418.47,408.93642200000005,0,9778.4246784605893,0,198.46477454601117,9976.8894530066009,-6007.5939620863774,null,null,null,"Post 1980 Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","10000 ft2","ptac","stand-alone","post198010000 ft2ptacstand-alonebaseline",null,null,null,null,null,null,null,null,448.56,180.1,null,null,null,{"$f":"277.8*($N$14983-N14983)*$S$3","v":0},{"$f":"277.78*($O$14983-O14983)*$S$4","v":0},0,{"$f":"IF(P14983>0.2,\"yes\",\"no\")","v":"no"},{"$f":"IF(B14983=\"5500 ft2\",5500,IF(B14983=\"10000 ft2\",10000,25000))","v":10000},{"$f":"IF(B14983=\"5500 ft2\",IF(D14983=\"stand-alone\",642.39,IF(D14983=\"ad-e&flr\",522.37,402.25)),IF(B14983=\"10000 ft2\",IF(D14983=\"stand-alone\",866.06,IF(D14983=\"ad-e&flr\",704.17,542.29)),IF(B14983=\"25000 ft2\",IF(D14983=\"stand-alone\",1369.38,IF(D14983=\"ad-e&flr\",1113.42,857.45)))))","v":866.06},{"$f":"IF(B14983=\"5500 ft2\",IF(D14983=\"stand-alone\",3030.15,IF(D14983=\"ad-e&flr\",2424.14,1818.13)),IF(B14983=\"10000 ft2\",IF(D14983=\"stand-alone\",4085.12,IF(D14983=\"ad-e&flr\",3268.14,2451.05)),IF(B14983=\"25000 ft2\",IF(D14983=\"stand-alone\",6459.2,IF(D14983=\"ad-e&flr\",5167.32,3875.54)))))","v":4085.12},null,{"$f":"SUM(IF(F14983=\"eff-roof\",W14983*IF(AND(W$4=\"no\",X$4=\"no\"),$C$4,$C$3)),IF(G14983=\"eff-win\",X14983*IF(W$4=\"no\",$D$4,$D$3),0),IF(H14983=\"red-inf\",Y14983*IF(W$4=\"no\",$F$4,$F$3),0),IF(I14983=\"25 fc\",W14983*IF(W$4=\"no\",$H$4,$H$3),0),IF(I14983=\"40 fc\",W14983*IF(W$4=\"no\",$G$4,$G$3),0),IF(J14983=\"yes-day\",W14983*IF(W$4=\"no\",$I$4,$I$3),0),IF(K14983=\"yes-occ\",W14983*IF(W$4=\"no\",$J$4,$J$3),0),IF(L14983=\"red-epd\",W14983*IF(W$4=\"no\",$K$4,$K$3),0),IF(AND(M14983=\"high-eff\",C14983=\"psz-ac\"),W14983*IF(AND(W$4=\"no\",Y$4=\"no\"),$L$4,$L$3),0),IF(AND(M14983=\"high-eff\",C14983=\"ptac\"),W14983*IF(AND(W$4=\"no\",Y$4=\"no\"),$M$4,$M$3),0),IF(AND(M14983=\"high-eff\",C14983=\"pthp\"),W14983*IF(AND(W$4=\"no\",Y$4=\"no\"),$N$4,$N$3),0))","v":0},{"$f":"SUM(IF(F14983=\"eff-roof\",W14983*$C$4),IF(G14983=\"eff-win\",X14983*$D$4,0),IF(H14983=\"red-inf\",Y14983*$F$4,0),IF(I14983=\"25 fc\",W14983*$H$4,0),IF(I14983=\"40 fc\",W14983*$G$4,0),IF(J14983=\"yes-day\",W14983*$I$4,0),IF(K14983=\"yes-occ\",W14983*$J$4,0),IF(L14983=\"red-epd\",W14983*$K$4,0),IF(AND(M14983=\"high-eff\",C14983=\"psz-ac\"),W14983*$L$4,0),IF(AND(M14983=\"high-eff\",C14983=\"ptac\"),W14983*$M$4,0),IF(AND(M14983=\"high-eff\",C14983=\"pthp\"),W14983*$N$4,0))","v":0},0,0,{"$f":"-PMT($AE$3,$AE$4,AA14983+AC14983-AD14983)","v":0},{"$f":"SUM(IF(F14983=\"eff-roof\",($C$5*W14983),0),IF(G14983=\"eff-win\",($D$5*X14983),0),IF(H14983=\"red-inf\",$F$5*(Y14983-X14983),0),IF(I14983=\"25 fc\",($H$5*W14983),0),IF(I14983=\"40 fc\",($G$5*W14983),0),IF(J14983=\"yes-day\",($I$5*W14983),0),IF(K14983=\"yes-occ\",($J$5*W14983),0),IF(L14983=\"red-epd\",($K$5*W14983),0),IF(M14983=\"high-eff\",($L$5*W14983),0))","v":0},{"$f":"0.05*U14983","v":0},0,{"$f":"U14983-AH14983","v":0},null,null,null,"Post 1980 Construction",{"$f":"IF(B14983=\"5500 ft2\",\"5,500 SF\",IF(B14983=\"10000 ft2\",\"10,000 SF\",IF(B14983=\"25000 ft2\",\"25,000 SF\")))","v":"10,000 SF"},"Split System Air Conditioner","Stand Alone",false,false,false,{"$f":"IF(I14983=\"base-lpd\",\"Baseline Lighting Levels\",IF(I14983=\"40 fc\",\"Reduce Lighting Levels to 40 fc\",IF(I14983=\"25 fc\",\"Reduce Lighting Levels to 25 fc\")))","v":false},false,false,false,false]
["post1980","10000 ft2","ptac","stand-alone","post198010000 ft2ptacstand-alone","base-roof","base-win","red-inf","25 fc","no-day","yes-occ","red-epd","base-eff",287,220.33,0.19301304881112499,0.36017478152309601,-0.22337590227651299,4488.1368000000002,-348.50276199979214,4139.6340380002084,"no",10000,866.06,4085.12,null,14756.6016,118356.60159999999,147.56601599999999,0,3528.5758248173606,-1900,206.98170190001042,1835.557526717371,2304.0765112828376,null,null,null,"Post 1980 Construction","10,000 SF","Split System Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","10000 ft2","ptac","stand-alone","post198010000 ft2ptacstand-alone","base-roof","eff-win","base-inf","base-lpd","yes-day","no-occ","red-epd","high-eff",309.82,195.66,0.19593905628869901,0.30930087390761601,-8.6396446418656306E-2,3854.1972000000005,-134.79251744262402,3719.4046825573764,"no",10000,866.06,4085.12,null,19818.310799999999,101340.57999999999,198.183108,0,4738.923925248263,0,185.97023412786882,4924.8941593761319,-1205.4894768187555,null,null,null,"Post 1980 Construction","10,000 SF","Split System Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","10000 ft2","ptac","stand-alone","post198010000 ft2ptacstand-alone","eff-roof","base-win","base-inf","base-lpd","no-day","no-occ","base-epd","high-eff",441.65,140.66,7.3741299561098997E-2,1.5404851079008399E-2,0.218989450305386,{"$f":"277.8*($N$14983-N15176)*$S$3","v":191.95980000000071},{"$f":"277.78*($O$14983-O15176)*$S$4","v":341.65918302937598},{"$f":"SUM(S15176:T15176)","v":533.61898302937675},"no",10000,866.06,4085.12,null,36600,150000,{"$f":"MIN(0.01*AA15176,500)","v":366},{"$f":"IF(V15176=\"yes\",0,0)","v":0},8751.7355749656745,0,26.680949151468837,{"$f":"SUM(AE15176:AG15176)","v":8778.4165241171431},-8244.7975410877661,null,null,null,"Post 1980 Construction","10,000 SF",{"$f":"IF(C15176=\"psz-ac\",\"Packaged Air Conditioner\",IF(C15176=\"ptac\",\"Split System Air Conditioner\",IF(C15176=\"pthp\",\"Split System Heat Pump\")))","v":"Split System Air Conditioner"},{"$f":"IF(D15176=\"stand-alone\",\"Stand Alone\",IF(D15176=\"ad-e&flr\",\"Above Ground, 1 Side Attached\",IF(D15176=\"ad-e&w&flr\",\"Above Ground, 2 Sides Attached\")))","v":"Stand Alone"},{"$f":"IF(F15176=\"base-roof\",\"Baseline Roof Insulation\",IF(F15176=\"eff-roof\",\"Increased Roof Insulation\"))","v":"Increased Roof Insulation"},{"$f":"IF(G15176=\"base-win\",\"Baseline Windows\",IF(G15176=\"eff-win\",\"Replace Windows\"))","v":"Baseline Windows"},{"$f":"IF(H15176=\"base-inf\",\"Baseline Infiltration\",IF(H15176=\"red-inf\",\"Reduce Infiltration\"))","v":"Baseline Infiltration"},"Baseline Lighting Levels",{"$f":"IF(J15176=\"no-day\",\"No Daylighting Sensors\",IF(J15176=\"yes-day\",\"Install Daylighting Sensors\"))","v":"No Daylighting Sensors"},{"$f":"IF(K15176=\"no-occ\",\"No Occupancy Sensors\",IF(K15176=\"yes-occ\",\"Install Occupancy Sensors\"))","v":"No Occupancy Sensors"},{"$f":"IF(L15176=\"base-epd\",\"No Plug Load Control\",IF(L15176=\"red-epd\",\"Install Plug Load Controls\"))","v":"No Plug Load Control"},{"$f":"IF(M15176=\"base-eff\",\"Baseline HVAC Equipment\",IF(M15176=\"high-eff\",\"Install High Efficiency HVAC Equipment\"))","v":"Install High Efficiency HVAC Equipment"}]
["post1980","10000 ft2","ptac","stand-alone","post198010000 ft2ptacstand-alone","eff-roof","base-win","base-inf","40 fc","no-day","yes-occ","red-epd","base-eff",313.35000000000002,198.44,0.18590491953479399,0.30143124665596599,-0.101832315380344,3756.1337999999996,-158.87498521193601,3597.2588147880638,"no",10000,866.06,4085.12,null,41700,147200,417,0,9971.2397124608924,-1200,179.8629407394032,8951.1026532002961,-5353.8438384122328,null,null,null,"Post 1980 Construction","10,000 SF","Split System Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","10000 ft2","ptac","stand-alone","post198010000 ft2ptacstand-alone","eff-roof","eff-win","base-inf","base-lpd","yes-day","yes-occ","base-epd","base-eff",344,185.89,0.15711773485643399,0.233101480292492,-3.2148806218767298E-2,2904.6768000000002,-50.157369922415931,2854.5194300775843,"no",10000,866.06,4085.12,null,45318.310799999999,196440.58,453.183108,0,10836.444612724346,0,142.72597150387921,10979.170584228226,-8124.6511541506425,null,null,null,"Post 1980 Construction","10,000 SF","Split System Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","10000 ft2","ptac","ad-e&flr","post198010000 ft2ptacad-e&flr","base-roof","base-win","base-inf","base-lpd","no-day","no-occ","red-epd","base-eff",418.38,189.92,5.8197405137941999E-2,0.12651885256169401,-0.137926902336728,1683.4680000000008,-199.41669354300782,1484.051306456993,"no",10000,704.17,3268.14,null,1500,1500,15,0,358.67768749859323,0,74.202565322849651,432.88025282144287,1051.1710536355502,null,null,null,{"$f":"IF(A15369=\"new90.1-2004\",\"New Construction\",IF(A15369=\"post1980\",\"Post 1980 Construction\",IF(A15369=\"pre1980\",\"Pre 1980 Construction\")))","v":"Post 1980 Construction"},"10,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","10000 ft2","ptac","ad-e&flr","post198010000 ft2ptacad-e&flr","base-roof","base-win","base-inf","40 fc","no-day","yes-occ","red-epd","high-eff",326.86,202.45,0.18048962918212899,0.31759154870766998,-0.21300179748352299,4225.8936000000003,-307.96105366871984,3917.9325463312807,"no",10000,704.17,3268.14,null,18300,54200,183,0,4375.8677874828372,-1200,195.89662731656404,3371.7644147994015,546.16813153187923,null,null,null,"Post 1980 Construction","10,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","10000 ft2","ptac","ad-e&flr","post198010000 ft2ptacad-e&flr","base-roof","eff-win","base-inf","base-lpd","yes-day","yes-occ","base-epd","high-eff",360.49,186.45,0.15317453467966999,0.24737984884546299,-0.11713600958657901,3291.6522000000004,-169.35692262231984,3122.2952773776806,"no",10000,704.17,3268.14,null,20755.940600000002,96479.31,207.55940600000002,0,4963.128517510776,0,156.11476386888404,5119.2432813796604,-1996.9480040019798,null,null,null,"Post 1980 Construction","10,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","10000 ft2","ptac","ad-e&flr","post198010000 ft2ptacad-e&flr","base-roof","eff-win","base-inf","25 fc","no-day","yes-occ","red-epd","base-eff",304.98,237,0.16086994045050501,0.36327195289991199,-0.42001198322348698,4833.72,-607.25934914703987,4226.4606508529605,"no",10000,704.17,3268.14,null,18055.940600000002,146879.31,180.55940600000002,0,4317.5086800133085,-1900,211.32303254264804,2628.8317125559565,1597.628938297004,null,null,null,"Post 1980 Construction","10,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","10000 ft2","ptac","ad-e&flr","post198010000 ft2ptacad-e&flr","eff-roof","base-win","base-inf","40 fc","yes-day","no-occ","base-epd","base-eff",366.76,175.99,0.15967607376082399,0.234289531922001,-5.4463750748951503E-2,3117.4716000000008,-78.744471950736028,3038.7271280492646,"no",10000,704.17,3268.14,null,42100,176200,421,0,10066.887095793851,-1200,151.93635640246325,9018.8234521963132,-5980.096324147049,null,null,null,"Post 1980 Construction","10,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","10000 ft2","ptac","ad-e&flr","post198010000 ft2ptacad-e&flr","eff-roof","eff-win","base-inf","base-lpd","yes-day","yes-occ","red-epd","base-eff",308.08999999999997,196.64,0.218549523891718,0.35677898868428798,-0.178190533253445,4747.3242000000018,-257.63042858249582,4489.6937714175056,"yes",10000,704.17,3268.14,null,45655.940600000002,190979.31,456.55940600000002,0,10917.178129987424,0,224.48468857087528,11141.662818558299,-6651.9690471407939,null,null,null,"Post 1980 Construction","10,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","10000 ft2","ptac","ad-e&flr","post198010000 ft2ptacad-e&flr","eff-roof","eff-win","base-inf","25 fc","no-day","no-occ","red-epd","high-eff",322.29000000000002,167.54,0.24160697333218301,0.32713265689590398,-3.8346315158776902E-3,4352.8482000000004,-5.5441652418558816,4347.3040347581446,"yes",10000,704.17,3268.14,null,51055.940600000002,293279.31,500,0,12205.91785559263,-1900,217.36520173790723,10523.283057330536,-6175.9790225723918,null,null,null,"Post 1980 Construction","10,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","10000 ft2","ptac","ad-e&w&flr","post198010000 ft2ptacad-e&w&flr","base-roof","base-win","base-inf","40 fc","yes-day","no-occ","base-epd","high-eff",356.74,163.80000000000001,0.15515681544029,0.25382250203936502,-0.186612576064909,3371.1029999999992,-223.15265098470414,3147.9503490152952,"no",10000,542.29,2451.0500000000002,null,18700,83200,187,0,4471.5151708157955,-1200,157.39751745076478,3428.9126882665605,-280.96233925126535,null,null,null,"Post 1980 Construction","10,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","10000 ft2","ptac","ad-e&w&flr","post198010000 ft2ptacad-e&w&flr","base-roof","eff-win","base-inf","base-lpd","yes-day","yes-occ","red-epd","high-eff",300.73,183.22,0.21453558504222001,0.37097617603380101,-0.327296435815706,4927.0607999999993,-391.38341504227202,4535.6773849577276,"yes",10000,542.29,2451.0500000000002,null,21093.642200000002,91018.47,210.93642200000002,0,5043.8792034791586,0,226.7838692478864,5270.6630727270449,-734.98568776931734,null,null,null,"Post 1980 Construction","10,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","10000 ft2","ptac","ad-e&w&flr","post198010000 ft2ptacad-e&w&flr","base-roof","eff-win","base-inf","25 fc","no-day","yes-occ","base-epd","base-eff",364.47,180.7,0.115168878166466,0.237653998201175,-0.30904085772239898,3156.3635999999988,-369.55326440246392,2786.810335597535,"no",10000,542.29,2451.0500000000002,null,15393.6422,138418.47,153.93642199999999,0,3680.9039909845051,-1900,139.34051677987676,1920.2445077643818,866.56582783315321,null,null,null,"Post 1980 Construction","10,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","10000 ft2","ptac","ad-e&w&flr","post198010000 ft2ptacad-e&w&flr","eff-roof","base-win","base-inf","40 fc","yes-day","no-occ","red-epd","base-eff",304.16000000000003,169.69,0.23092581423401701,0.36380179464117601,-0.229281367719502,4831.7753999999986,-274.17629672616005,4557.5991032738384,"yes",10000,542.29,2451.0500000000002,null,43600,177700,436,0,10425.564783292442,-1200,227.87995516369193,9453.4447384561336,-4895.8456351822952,null,null,null,"Post 1980 Construction","10,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","10000 ft2","ptac","ad-e&w&flr","post198010000 ft2ptacad-e&w&flr","eff-roof","base-win","base-inf","25 fc","yes-day","yes-occ","red-epd","high-eff",258.43,169.31,0.30577503015681501,0.45945324102156498,-0.22652854245146301,6102.1548000000003,-270.88444861380805,5831.2703513861925,"yes",10000,542.29,2451.0500000000002,null,55100,300700,500,0,13163.35275572395,-1900,291.56351756930962,11554.91627329326,-5723.6459219070675,null,null,null,"Post 1980 Construction","10,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","10000 ft2","ptac","ad-e&w&flr","post198010000 ft2ptacad-e&w&flr","eff-roof","eff-win","base-inf","25 fc","no-day","yes-occ","base-epd","high-eff",355.13,127.04,0.217430639324487,0.257190068815495,7.9687047232686103E-2,3415.8287999999993,95.290340094399866,3511.119140094399,"yes",10000,542.29,2451.0500000000002,null,51993.642200000002,288418.46999999997,500,0,12427.919599125125,-1900,175.55595700471997,10703.475556129846,-7192.3564160354472,null,null,null,"Post 1980 Construction","10,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","10000 ft2","pthp","stand-alone","post198010000 ft2pthpstand-alone","base-roof","base-win","base-inf","40 fc","yes-day","no-occ","red-epd","high-eff",445.45,0,0.26224766125061499,0.262255713812521,0,4398.9629999999988,0,4398.9629999999988,"yes",10000,866.06,4085.12,null,28900,89200,289,0,6910.5234458062296,-1200,219.94814999999994,5930.4715958062297,-1531.5085958062309,null,null,null,"Post 1980 Construction","10,000 SF","Split System Heat Pump","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","10000 ft2","pthp","stand-alone","post198010000 ft2pthpstand-alone","base-roof","base-win","red-inf","base-lpd","no-day","no-occ","base-epd","base-eff",595.20000000000005,0,1.42325209256524E-2,1.42431268631996E-2,0,238.90799999999751,0,238.90799999999751,"no",10000,866.06,4085.12,null,1756.6016,1756.6016,17.566016000000001,0,420.03586649621923,0,11.945399999999877,431.98126649621912,-193.07326649622161,null,null,null,"Post 1980 Construction","10,000 SF","Split System Heat Pump","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","10000 ft2","pthp","stand-alone","post198010000 ft2pthpstand-alone","base-roof","eff-win","base-inf","25 fc","no-day","yes-occ","red-epd","base-eff",470.9,0,0.22010401280157599,0.22010599536270301,0,3691.9619999999995,0,3691.9619999999995,"yes",10000,866.06,4085.12,null,19218.310799999999,153840.57999999999,192.183108,0,4595.4528502488265,-1900,184.59809999999999,2880.0509502488267,811.91104975117287,null,null,null,"Post 1980 Construction","10,000 SF","Split System Heat Pump","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","10000 ft2","pthp","stand-alone","post198010000 ft2pthpstand-alone","base-roof","eff-win","red-inf","base-lpd","yes-day","yes-occ","red-epd","high-eff",436.31,0,0.27738798621368799,0.27739317654852602,0,4652.8721999999989,0,4652.8721999999989,"yes",10000,866.06,4085.12,null,33874.912400000001,111197.1816,338.74912399999999,0,8100.1168292329485,0,232.64360999999997,8332.7604392329486,-3679.8882392329497,null,null,null,"Post 1980 Construction","10,000 SF","Split System Heat Pump","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","10000 ft2","pthp","stand-alone","post198010000 ft2pthpstand-alone","eff-roof","base-win","red-inf","base-lpd","no-day","no-occ","base-epd","high-eff",554.89,0,8.0994583948793705E-2,8.1003643590592894E-2,0,1358.7197999999992,0,1358.7197999999992,"no",10000,866.06,4085.12,null,47056.601600000002,156256.60159999999,470.56601600000005,0,11252.102028953735,0,67.935989999999961,11320.038018953735,-9961.3182189537365,null,null,null,"Post 1980 Construction","10,000 SF","Split System Heat Pump","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","10000 ft2","pthp","stand-alone","post198010000 ft2pthpstand-alone","eff-roof","eff-win","base-inf","25 fc","no-day","yes-occ","red-epd","high-eff",425.16,0,0.29585179714426402,0.295859556144419,0,4962.6191999999983,0,4962.6191999999983,"yes",10000,866.06,4085.12,null,64518.310799999999,308340.57999999996,500,0,15393.146774131226,-1900,248.13095999999993,13741.277734131227,-8778.6585341312275,null,null,null,"Post 1980 Construction","10,000 SF","Split System Heat Pump","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","10000 ft2","pthp","stand-alone","post198010000 ft2pthpstand-alone","eff-roof","eff-win","red-inf","base-lpd","yes-day","yes-occ","base-epd","base-eff",491.67,0,0.18569977843426899,0.185707187810533,0,3114.9713999999985,0,3114.9713999999985,"no",10000,866.06,4085.12,null,47074.912400000001,198197.18159999998,470.74912399999999,0,11256.480479220567,0,155.74856999999994,11412.229049220567,-8297.2576492205681,null,null,null,"Post 1980 Construction","10,000 SF","Split System Heat Pump","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","10000 ft2","pthp","ad-e&flr","post198010000 ft2pthpad-e&flr","base-roof","base-win","red-inf","base-lpd","no-day","no-occ","red-epd","base-eff",575.94000000000005,0,8.4149566399267295E-2,8.4137711695952896E-2,0,1469.8397999999993,0,1469.8397999999993,"no",10000,704.17,3268.14,null,2905.3001999999997,2905.3001999999997,29.053001999999996,0,694.71090481680017,0,73.491989999999973,768.20289481680015,701.63690518319913,null,null,null,"Post 1980 Construction","10,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","10000 ft2","pthp","ad-e&flr","post198010000 ft2pthpad-e&flr","base-roof","eff-win","base-inf","25 fc","yes-day","no-occ","base-epd","base-eff",528.6,0,0.15942028985507201,0.15941798521110001,0,2784.9450000000002,0,2784.9450000000002,"no",10000,704.17,3268.14,null,18455.940600000002,175879.31,184.55940600000002,0,4413.1560633462659,-1900,139.24725000000001,2652.4033133462658,132.54168665373436,null,null,null,"Post 1980 Construction","10,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","10000 ft2","pthp","ad-e&flr","post198010000 ft2pthpad-e&flr","base-roof","eff-win","red-inf","base-lpd","yes-day","yes-occ","base-epd","high-eff",507.17,0,0.193502637060675,0.193496064244255,0,3380.2704000000008,0,3380.2704000000008,"no",10000,704.17,3268.14,null,30861.2408,102384.6102,308.61240800000002,0,7379.4923223208234,0,169.01352000000006,7548.5058423208238,-4168.2354423208235,null,null,null,"Post 1980 Construction","10,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","10000 ft2","pthp","ad-e&flr","post198010000 ft2pthpad-e&flr","eff-roof","base-win","base-inf","25 fc","no-day","no-occ","red-epd","high-eff",466.66,0,0.25791487538595598,0.257915242108611,0,4505.6382000000003,0,4505.6382000000003,"yes",10000,704.17,3268.14,null,54700,267500,500,0,13068.652376186368,-1900,225.28191000000004,11393.934286186368,-6888.2960861863676,null,null,null,"Post 1980 Construction","10,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","10000 ft2","pthp","ad-e&flr","post198010000 ft2pthpad-e&flr","eff-roof","base-win","red-inf","40 fc","yes-day","no-occ","red-epd","high-eff",440.37,0,0.29972373650076101,0.29972171424027999,0,5235.974400000001,0,5235.974400000001,"yes",10000,704.17,3268.14,null,60305.300199999998,212105.3002,500,0,14395.712517091581,-1200,261.79872000000006,13457.511237091581,-8221.5368370915803,null,null,null,"Post 1980 Construction","10,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","10000 ft2","pthp","ad-e&flr","post198010000 ft2pthpad-e&flr","eff-roof","eff-win","red-inf","base-lpd","yes-day","yes-occ","base-epd","high-eff",483.39,0,0.23132266690304201,0.231311123479367,0,4040.8788000000018,0,4040.8788000000018,"yes",10000,704.17,3268.14,null,60861.2408,223884.6102,500,0,14527.331981642461,0,202.04394000000011,14729.375921642461,-10688.497121642458,null,null,null,"Post 1980 Construction","10,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","10000 ft2","pthp","ad-e&w&flr","post198010000 ft2pthpad-e&w&flr","base-roof","base-win","red-inf","base-lpd","no-day","no-occ","red-epd","high-eff",526.62,0,0.13106461255460999,0.131076131076131,0,2206.8431999999989,0,2206.8431999999989,"no",10000,542.29,2451.0500000000002,null,17853.951499999999,35553.951500000003,178.53951499999999,0,4269.2093578213598,0,110.34215999999995,4379.55151782136,-2172.7083178213611,null,null,null,"Post 1980 Construction","10,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","10000 ft2","pthp","ad-e&w&flr","post198010000 ft2pthpad-e&w&flr","base-roof","base-win","red-inf","40 fc","yes-day","no-occ","base-epd","base-eff",518.67999999999995,0,0.14417107381007099,0.144177144177144,0,2427.4164000000001,0,2427.4164000000001,"no",10000,542.29,2451.0500000000002,null,13153.951499999999,55753.951499999996,131.53951499999999,0,3145.3526036591011,-1200,121.37082000000001,2066.7234236591012,360.69297634089889,null,null,null,"Post 1980 Construction","10,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","10000 ft2","pthp","ad-e&w&flr","post198010000 ft2pthpad-e&w&flr","base-roof","eff-win","red-inf","base-lpd","yes-day","yes-occ","red-epd","base-eff",476.13,0,0.21437878439488001,0.21438471438471399,0,3609.4553999999989,0,3609.4553999999989,"yes",10000,542.29,2451.0500000000002,null,15547.593699999999,63572.421499999997,155.47593699999999,0,3717.7166363224637,0,180.47276999999997,3898.1894063224636,-288.73400632246467,null,null,null,"Post 1980 Construction","10,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","10000 ft2","pthp","ad-e&w&flr","post198010000 ft2pthpad-e&w&flr","base-roof","eff-win","red-inf","25 fc","no-day","yes-occ","red-epd","high-eff",442.25,0,0.27028435655706301,0.27028677028677001,0,4550.6417999999985,0,4550.6417999999985,"yes",10000,542.29,2451.0500000000002,null,33247.593699999998,173972.4215,332.47593699999999,0,7950.113348805864,-1900,227.53208999999993,6277.6454388058637,-1727.0036388058652,null,null,null,"Post 1980 Construction","10,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","10000 ft2","pthp","ad-e&w&flr","post198010000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","40 fc","yes-day","no-occ","base-epd","high-eff",465.1,0,0.23257453820801699,0.232584232584232,0,3915.8687999999984,0,3915.8687999999984,"yes",10000,542.29,2451.0500000000002,null,58453.951499999996,210253.9515,500,0,13957.403955725556,-1200,195.79343999999992,12953.197395725556,-9037.3285957255575,null,null,null,"Post 1980 Construction","10,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","10000 ft2","pthp","ad-e&w&flr","post198010000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","base-lpd","yes-day","yes-occ","red-epd","high-eff",420.82,0,0.30563347896068099,0.30564630564630602,0,5145.9671999999991,0,5145.9671999999991,"yes",10000,542.29,2451.0500000000002,null,60847.593700000005,218072.4215,500,0,14524.101017768493,0,257.29835999999995,14781.399377768494,-9635.4321777684945,null,null,null,"Post 1980 Construction","10,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","10000 ft2","pthp","ad-e&w&flr","post198010000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","25 fc","no-day","yes-occ","base-epd","base-eff",485.42,0,0.19904958994404801,0.19905619905619901,0,3351.379199999998,0,3351.379199999998,"no",10000,542.29,2451.0500000000002,null,46447.593700000005,260972.4215,464.47593700000004,0,11106.476998793487,-1900,167.56895999999992,9374.0459587934874,-6022.6667587934899,null,null,null,"Post 1980 Construction","10,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","25000 ft2","psz-ac","stand-alone","post198025000 ft2psz-acstand-alone","base-roof","base-win","red-inf","40 fc","yes-day","no-occ","red-epd","base-eff",752.83,370.96,0.223853063843439,0.35730810930790402,-0.341578966402662,11627.041199999998,-818.19751108327978,10808.843688916719,"yes",25000,1369.38,6459.2,null,36777.455999999998,143277.45600000001,367.77456000000001,0,8794.1685801075073,-3000,540.44218444583601,6334.610764553343,4474.2329243633758,null,null,null,"Post 1980 Construction","25,000 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","25000 ft2","psz-ac","stand-alone","post198025000 ft2psz-acstand-alone","base-roof","eff-win","red-inf","40 fc","no-day","no-occ","base-epd","base-eff",1030.33,275.95999999999998,9.7802374077638796E-2,0.12040602030101499,1.9890781526889102E-3,3918.0911999999989,4.7645170047200986,3922.8557170047188,"no",25000,1369.38,6459.2,null,29109.6044,113160.796,291.09604400000001,0,6960.6437267939164,-3000,196.14278585023595,4156.786512644152,-233.9307956394332,null,null,null,"Post 1980 Construction","25,000 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","25000 ft2","psz-ac","stand-alone","post198025000 ft2psz-acstand-alone","base-roof","eff-win","red-inf","25 fc","no-day","yes-occ","base-epd","high-eff",850.51,330,0.184664741738851,0.27391857397747899,-0.19344689161332301,8913.4907999999978,-463.37093560449603,8450.1198643955013,"no",25000,1369.38,6459.2,null,51609.604399999997,501660.79599999997,500,0,12336.99828558318,-4750,422.50599321977506,8009.504278802955,440.61558559254627,null,null,null,"Post 1980 Construction","25,000 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","25000 ft2","psz-ac","stand-alone","post198025000 ft2psz-acstand-alone","eff-roof","base-win","red-inf","40 fc","yes-day","no-occ","red-epd","high-eff",740.95,299.38,0.28148861084375998,0.36745007982106398,-8.2709486094535503E-2,11957.067599999997,-198.11727981444801,11758.950320185548,"yes",25000,1369.38,6459.2,null,122027.45600000001,599277.45600000001,500,0,29008.491467436063,-3000,587.94751600927736,26596.43898344534,-14837.488663259792,null,null,null,"Post 1980 Construction","25,000 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","25000 ft2","psz-ac","stand-alone","post198025000 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","base-lpd","no-day","yes-occ","base-epd","base-eff",1048.1400000000001,238.01,0.111709977542509,0.10520160154349199,0.13923547068822101,3423.3293999999946,333.51619033039998,3756.8455903303948,"no",25000,1369.38,6459.2,null,93832.148400000005,371633.34,500,0,22333.225640188859,0,187.84227951651974,22521.06791970538,-18764.222329374985,null,null,null,"Post 1980 Construction","25,000 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","25000 ft2","psz-ac","stand-alone","post198025000 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","25 fc","no-day","yes-occ","red-epd","base-eff",724.71,307.20999999999998,0.28729547641963399,0.38131418766060199,-0.111026725977361,12408.214799999996,-265.94667644527988,12142.268123554717,"yes",25000,1369.38,6459.2,null,120109.60440000001,656910.79600000009,500,0,28554.438281394167,-4750,607.1134061777359,24411.551687571904,-12269.283564017187,null,null,null,"Post 1980 Construction","25,000 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","25000 ft2","psz-ac","ad-e&flr","post198025000 ft2psz-acad-e&flr","base-roof","base-win","red-inf","40 fc","yes-day","yes-occ","base-epd","base-eff",977.77,312.41000000000003,0.17983168463014901,0.27809484432565701,-0.42868248959619498,10463.614800000003,-812.04695276809628,9651.5678472319069,"no",25000,1113.42,5167.32,null,41471.9476,147971.94760000001,414.71947599999999,0,9916.7081741538896,-3000,482.57839236159538,7399.286566515485,2252.2812807164219,null,null,null,"Post 1980 Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","25000 ft2","psz-ac","ad-e&flr","post198025000 ft2psz-acad-e&flr","base-roof","eff-win","base-inf","base-lpd","no-day","no-occ","base-epd","high-eff",1307.99,211.18,3.4268418721393697E-2,3.4287486248827999E-2,3.4252526638313401E-2,1290.1032000000016,64.884058846095826,1354.9872588460973,"no",25000,1113.42,5167.32,null,18244.355599999999,200127.06,182.443556,0,4362.5621843400049,0,67.74936294230487,4430.3115472823101,-3075.3242884362126,null,null,null,"Post 1980 Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","25000 ft2","psz-ac","ad-e&flr","post198025000 ft2psz-acad-e&flr","base-roof","eff-win","red-inf","25 fc","no-day","yes-occ","red-epd","high-eff",829.54,358.2,0.24495792115753701,0.387535716131509,-0.63808478529290702,14581.444200000005,-1208.7146503065119,13372.729549693493,"yes",25000,1113.42,5167.32,null,52966.303200000002,493849.00760000001,500,0,12658.198013778636,-4750,668.63647748467474,8576.8344912633111,4795.895058430182,null,null,null,"Post 1980 Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","25000 ft2","psz-ac","ad-e&flr","post198025000 ft2psz-acad-e&flr","eff-roof","base-win","base-inf","40 fc","no-day","no-occ","base-epd","base-eff",1203.48,172.24,0.12545400856341299,0.111449096667971,0.212329080349385,4193.3910000000014,402.21186278027176,4595.6028627802734,"no",25000,1113.42,5167.32,null,91500,355250,500,0,21781.087293643945,-3000,229.78014313901369,19010.867436782959,-14415.264574002686,null,null,null,"Post 1980 Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","25000 ft2","psz-ac","ad-e&flr","post198025000 ft2psz-acad-e&flr","eff-roof","eff-win","base-inf","base-lpd","no-day","no-occ","red-epd","base-eff",1191.96,174.61,0.131271223977558,0.11995451961341699,0.20149083093245501,4513.4166000000014,381.68112586902373,4895.0977258690255,"no",25000,1113.42,5167.32,null,86744.355599999995,355377.06,500,0,20655.183969579495,0,244.75488629345128,20899.938855872948,-16004.841130003922,null,null,null,"Post 1980 Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","25000 ft2","psz-ac","ad-e&flr","post198025000 ft2psz-acad-e&flr","eff-roof","eff-win","red-inf","25 fc","yes-day","no-occ","base-epd","base-eff",966.05,204.64,0.25580983316108102,0.28674793086390599,6.4160607307815407E-2,10789.196400000004,121.53849741131201,10910.734897411316,"yes",25000,1113.42,5167.32,null,118716.30319999999,717849.00760000001,500,0,28224.572900268737,-4750,545.53674487056583,24020.109645139302,-13109.374747727987,null,null,null,"Post 1980 Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","25000 ft2","psz-ac","ad-e&w&flr","post198025000 ft2psz-acad-e&w&flr","base-roof","base-win","base-inf","base-lpd","yes-day","yes-occ","base-epd","high-eff",1022.35,257.41000000000003,0.16119652915207799,0.24362256222070999,-0.47877290745102602,9147.6762000000035,-721.95426758793622,8425.721932412067,"no",25000,857.45,3875.54,null,33000,246500,330,0,7890.9091249690509,0,421.28609662060336,8312.1952215896545,113.5267108224125,null,null,null,"Post 1980 Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","25000 ft2","psz-ac","ad-e&w&flr","post198025000 ft2psz-acad-e&w&flr","base-roof","eff-win","base-inf","base-lpd","no-day","no-occ","red-epd","high-eff",1150.4000000000001,215.76,0.104566905160603,0.14888579799354901,-0.23950135003159601,5590.4472000000005,-361.15038895777593,5229.2968110422244,"no",25000,857.45,3875.54,null,20156.491000000002,192870.35,201.56491000000003,0,4819.7890533108048,0,261.46484055211124,5081.2538938629159,148.04291717930846,null,null,null,"Post 1980 Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","25000 ft2","psz-ac","ad-e&w&flr","post198025000 ft2psz-acad-e&w&flr","base-roof","eff-win","red-inf","25 fc","yes-day","no-occ","base-epd","high-eff",937.25,261.39,0.21437052823869701,0.30658311384688203,-0.50163727236169398,11511.754200000003,-756.43204518572782,10755.322154814276,"yes",25000,857.45,3875.54,null,51572.9732,554786.83220000006,500,0,12328.325814225887,-4750,537.76610774071378,8116.0919219666011,2639.2302328476744,null,null,null,"Post 1980 Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","25000 ft2","psz-ac","ad-e&w&flr","post198025000 ft2psz-acad-e&w&flr","eff-roof","base-win","base-inf","base-lpd","yes-day","yes-occ","red-epd","base-eff",895.38,214.13,0.272781245242807,0.33756029712053498,-0.23013730108576999,12674.902800000003,-347.03009310742402,12327.87270689258,"yes",25000,857.45,3875.54,null,101500,401750,500,0,24148.596782083507,0,616.39363534462905,24764.990417428136,-12437.117710535556,null,null,null,"Post 1980 Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","25000 ft2","psz-ac","ad-e&w&flr","post198025000 ft2psz-acad-e&w&flr","eff-roof","eff-win","base-inf","base-lpd","no-day","yes-occ","base-epd","base-eff",1221.93,116.72,0.122606180544984,9.5964901896954793E-2,0.32946515769517998,3603.343800000001,496.80918221943995,4100.1529822194407,"no",25000,857.45,3875.54,null,90156.490999999995,349620.35,500,0,21463.010263113549,0,205.00764911097204,21668.017912224521,-17567.864930005082,null,null,null,"Post 1980 Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","25000 ft2","psz-ac","ad-e&w&flr","post198025000 ft2psz-acad-e&w&flr","eff-roof","eff-win","base-inf","40 fc","yes-day","yes-occ","base-epd","high-eff",941.98,180.03,0.26459126198812599,0.30308366132994002,-3.4239099212960401E-2,11380.354800000003,-51.630038814784065,11328.724761185218,"yes",25000,857.45,3875.54,null,130656.49099999999,638620.35,500,0,31051.423691293763,-3000,566.43623805926097,28617.859929353024,-17289.135168167806,null,null,null,"Post 1980 Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","25000 ft2","ptac","stand-alone","post198025000 ft2ptacstand-alone","base-roof","base-win","base-inf","base-lpd","yes-day","yes-occ","red-epd","high-eff",652.83000000000004,391.03,0.244790966527759,0.38173707986476102,-0.19833900278875899,11197.562400000003,-560.65371008268767,10636.908689917314,"yes",25000,1369.38,6459.2,null,43000,169250,430,0,10282.093708293005,0,531.84543449586579,10813.939142788871,-177.03045287155692,null,null,null,"Post 1980 Construction","25,000 SF","Split System Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","25000 ft2","ptac","stand-alone","post198025000 ft2ptacstand-alone","base-roof","eff-win","base-inf","base-lpd","no-day","yes-occ","base-epd","high-eff",939.22,310.61,9.5779002554106707E-2,0.11051131251716501,4.8113756856976497E-2,3241.6482000000019,136.00530358927989,3377.6535035892816,"no",25000,1369.38,6459.2,null,35332.148399999998,139133.34,353.321484,0,8448.568854979414,0,168.88267517946409,8617.4515301588781,-5239.7980265695969,null,null,null,"Post 1980 Construction","25,000 SF","Split System Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","25000 ft2","ptac","stand-alone","post198025000 ft2ptacstand-alone","base-roof","eff-win","base-inf","40 fc","yes-day","no-occ","red-epd","base-eff",651.07000000000005,434.64,0.214511359053636,0.38340388858898999,-0.33198492231313798,11246.455200000002,-938.43659476603182,10308.01860523397,"yes",25000,1369.38,6459.2,null,43832.148399999998,199383.34,438.321484,0,10481.075750804774,-3000,515.40093026169859,7996.4766810664723,2311.5419241674981,null,null,null,"Post 1980 Construction","25,000 SF","Split System Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","25000 ft2","ptac","stand-alone","post198025000 ft2ptacstand-alone","eff-roof","base-win","base-inf","40 fc","no-day","no-occ","base-epd","base-eff",939.28,306.76,9.8517945960478595E-2,0.11045448949247599,5.9912353283687297E-2,3239.9814000000033,169.3569226223201,3409.3383226223232,"no",25000,1369.38,6459.2,null,91500,355250,500,0,21781.087293643945,-3000,170.46691613111616,18951.554209775062,-15542.215887152739,null,null,null,"Post 1980 Construction","25,000 SF","Split System Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","25000 ft2","ptac","stand-alone","post198025000 ft2ptacstand-alone","eff-roof","base-win","base-inf","25 fc","yes-day","no-occ","base-epd","high-eff",731.11,325.94,0.235246672939911,0.30760197365305803,1.1338910851644299E-3,9022.9440000000013,3.205220530448039,9026.1492205304494,"yes",25000,1369.38,6459.2,null,125000,739000,500,0,29712.244079916469,-4750,451.3074610265225,25413.55154094299,-16387.402320412541,null,null,null,"Post 1980 Construction","25,000 SF","Split System Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","25000 ft2","ptac","stand-alone","post198025000 ft2ptacstand-alone","eff-roof","eff-win","base-inf","40 fc","yes-day","no-occ","red-epd","high-eff",641.9,338.97,0.29036160774297598,0.39208834086238398,-3.8797462535625701E-2,11501.197800000004,-109.67051869046421,11391.52728130954,"yes",25000,1369.38,6459.2,null,135332.14840000001,574383.34000000008,500,0,32158.390017213027,-3000,569.57636406547704,29727.966381278504,-18336.439099968964,null,null,null,"Post 1980 Construction","25,000 SF","Split System Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","25000 ft2","ptac","stand-alone","post198025000 ft2ptacstand-alone","eff-roof","eff-win","red-inf","25 fc","yes-day","no-occ","red-epd","base-eff",597.45000000000005,378.02,0.29425998118026597,0.43418473165326599,-0.158468940577978,12736.018800000002,-447.95122602558376,12288.067573974418,"yes",25000,1369.38,6459.2,null,124859.60440000001,733160.79600000009,500,0,29679.005288402954,-4750,614.40337869872099,25543.408667101674,-13255.341093127256,null,null,null,"Post 1980 Construction","25,000 SF","Split System Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","25000 ft2","ptac","ad-e&flr","post198025000 ft2ptacad-e&flr","base-roof","base-win","base-inf","25 fc","yes-day","no-occ","base-epd","high-eff",779.67,376.41,0.190334439456048,0.314834831668029,-0.29845803580668501,9952.462800000003,-749.50183863340828,9202.9609613665943,"no",25000,1113.42,5167.32,null,50000,435250,500,0,11955.922916619775,-4750,460.14804806832973,7666.0709646881041,1536.8899966784902,null,null,null,"Post 1980 Construction","25,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","25000 ft2","ptac","ad-e&flr","post198025000 ft2ptacad-e&flr","base-roof","eff-win","base-inf","40 fc","yes-day","no-occ","red-epd","high-eff",686.3,403.63,0.23664519487279601,0.39688733050363401,-0.39235572113560302,12546.281400000005,-985.30211657609595,11560.979283423909,"yes",25000,1113.42,5167.32,null,58494.355600000003,259627.06,500,0,13966.969664737744,-3000,578.04896417119551,11545.01862890894,15.960654514969065,null,null,null,"Post 1980 Construction","25,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","25000 ft2","ptac","ad-e&flr","post198025000 ft2ptacad-e&flr","eff-roof","base-win","base-inf","40 fc","no-day","no-occ","base-epd","high-eff",987.28,221.16,0.15365345826013399,0.13238951429349799,0.23708993066335499,4185.0570000000034,595.39137042619188,4780.4483704261957,"no",25000,1113.42,5167.32,null,108000,426500,500,0,25687.47794956922,-3000,239.02241852130979,22926.500368090528,-18146.051997664334,null,null,null,"Post 1980 Construction","25,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","25000 ft2","ptac","ad-e&flr","post198025000 ft2ptacad-e&flr","eff-roof","base-win","base-inf","25 fc","no-day","yes-occ","red-epd","base-eff",703.89,368.92,0.248633613117314,0.38142943766312498,-0.27262064921176998,12057.631200000003,-684.6177797873122,11373.013420212692,"yes",25000,1113.42,5167.32,null,107500,595250,500,0,25569.10247514724,-4750,568.6506710106346,21387.753146157873,-10014.739725945181,null,null,null,"Post 1980 Construction","25,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","25000 ft2","ptac","ad-e&flr","post198025000 ft2ptacad-e&flr","eff-roof","eff-win","base-inf","40 fc","yes-day","yes-occ","base-epd","base-eff",801.58,319.55,0.21479927126032899,0.29558057173991398,-0.102314671082135,9343.8030000000017,-256.93740792726419,9086.8655920727379,"yes",25000,1113.42,5167.32,null,122244.3556,497377.06,500,0,29059.842653539934,-3000,454.34327960363692,26514.18593314357,-17427.32034107083,null,null,null,"Post 1980 Construction","25,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","25000 ft2","ptac","ad-e&flr","post198025000 ft2ptacad-e&flr","eff-roof","eff-win","red-inf","base-lpd","no-day","yes-occ","base-epd","high-eff",1001.22,190.36,0.16546294488906199,0.120139200126546,0.343337127876091,3797.8038000000015,862.20432269051162,4660.0081226905131,"no",25000,1113.42,5167.32,null,110716.30319999999,434099.00760000001,500,0,26330.565309517089,0,233.00040613452566,26563.565715651614,-21903.5575929611,null,null,null,"Post 1980 Construction","25,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","25000 ft2","ptac","ad-e&w&flr","post198025000 ft2ptacad-e&w&flr","base-roof","base-win","base-inf","25 fc","no-day","yes-occ","red-epd","high-eff",684.81,368,0.23913992211628801,0.39852972175379398,-0.50118299747083295,12605.175000000001,-1064.3064712725438,11540.868528727457,"yes",25000,857.45,3875.54,null,49000,362750,490,0,11716.804458287379,-4750,577.0434264363729,7543.847884723752,3997.0206440037045,null,null,null,"Post 1980 Construction","25,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","25000 ft2","ptac","ad-e&w&flr","post198025000 ft2ptacad-e&w&flr","base-roof","eff-win","base-inf","40 fc","yes-day","yes-occ","base-epd","high-eff",781.46,326.39999999999998,0.19934201691956499,0.31364179314221502,-0.331484049930652,9920.2379999999976,-703.93573055190393,9216.3022694480933,"no",25000,857.45,3875.54,null,61906.491000000002,253870.35,500,0,14774.795958271796,-3000,460.81511347240468,12235.611071744201,-3019.3088022961074,null,null,null,"Post 1980 Construction","25,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","25000 ft2","ptac","ad-e&w&flr","post198025000 ft2ptacad-e&w&flr","base-roof","eff-win","red-inf","base-lpd","no-day","no-occ","red-epd","base-eff",985.48,277.33,8.7367396266953098E-2,0.13445053400786999,-0.13131271926246199,4252.562399999998,-278.85418614897594,3973.7082138510223,"no",25000,857.45,3875.54,null,11572.9732,42286.832199999997,115.72973200000001,0,2767.3115099061297,0,198.68541069255113,2965.9969205986808,1007.7112932523414,null,null,null,"Post 1980 Construction","25,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","25000 ft2","ptac","ad-e&w&flr","post198025000 ft2ptacad-e&w&flr","eff-roof","base-win","base-inf","25 fc","yes-day","no-occ","base-epd","base-eff",799.14,275.27,0.22352960923862,0.29811340640809397,-0.122909357917924,9429.0875999999989,-261.00890427675193,9168.0786957232467,"yes",25000,857.45,3875.54,null,108500,667750,500,0,25805.853423991197,-4750,458.40393478616238,21514.257358777359,-12346.178663054112,null,null,null,"Post 1980 Construction","25,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","25000 ft2","ptac","ad-e&w&flr","post198025000 ft2ptacad-e&w&flr","eff-roof","base-win","red-inf","40 fc","no-day","no-occ","base-epd","high-eff",988.85,163.21,0.16739962400966801,0.13149065486228201,0.33421718201843797,{"$f":"277.8*($N$19207-N19464)*$S$3","v":4158.9437999999982},{"$f":"277.78*($O$19207-O19464)*$S$4","v":709.73977853947179},{"$f":"SUM(S19464:T19464)","v":4868.6835785394696},"no",25000,857.45,3875.54,null,109666.4822,428166.48220000003,{"$f":"MIN(0.01*AA19464,500)","v":500},{"$f":"IF(V19464=\"yes\",0,0)","v":0},26082.019191650779,-3000,243.43417892697349,{"$f":"SUM(AE19464:AG19464)","v":23325.453370577754},-18456.769792038285,null,null,null,"Post 1980 Construction","25,000 SF",{"$f":"IF(C19464=\"psz-ac\",\"Packaged Air Conditioner\",IF(C19464=\"ptac\",\"Split System Air Conditioner\",IF(C19464=\"pthp\",\"Split System Heat Pump\")))","v":"Split System Air Conditioner"},{"$f":"IF(D19464=\"stand-alone\",\"Stand Alone\",IF(D19464=\"ad-e&flr\",\"Above Ground, 1 Side Attached\",IF(D19464=\"ad-e&w&flr\",\"Above Ground, 2 Sides Attached\")))","v":"Above Ground, 2 Sides Attached"},{"$f":"IF(F19464=\"base-roof\",\"Baseline Roof Insulation\",IF(F19464=\"eff-roof\",\"Increased Roof Insulation\"))","v":"Increased Roof Insulation"},{"$f":"IF(G19464=\"base-win\",\"Baseline Windows\",IF(G19464=\"eff-win\",\"Replace Windows\"))","v":"Baseline Windows"},{"$f":"IF(H19464=\"base-inf\",\"Baseline Infiltration\",IF(H19464=\"red-inf\",\"Reduce Infiltration\"))","v":"Reduce Infiltration"},"Reduce Lighting Levels to 40 fc",{"$f":"IF(J19464=\"no-day\",\"No Daylighting Sensors\",IF(J19464=\"yes-day\",\"Install Daylighting Sensors\"))","v":"No Daylighting Sensors"},{"$f":"IF(K19464=\"no-occ\",\"No Occupancy Sensors\",IF(K19464=\"yes-occ\",\"Install Occupancy Sensors\"))","v":"No Occupancy Sensors"},{"$f":"IF(L19464=\"base-epd\",\"No Plug Load Control\",IF(L19464=\"red-epd\",\"Install Plug Load Controls\"))","v":"No Plug Load Control"},{"$f":"IF(M19464=\"base-eff\",\"Baseline HVAC Equipment\",IF(M19464=\"high-eff\",\"Install High Efficiency HVAC Equipment\"))","v":"Install High Efficiency HVAC Equipment"}]
["post1980","25000 ft2","ptac","ad-e&w&flr","post198025000 ft2ptacad-e&w&flr","eff-roof","eff-win","red-inf","base-lpd","no-day","no-occ","red-epd","high-eff",958.84,170.14,0.18408419497784301,0.157848510399101,0.30594762176715301,4992.6215999999986,649.70686427999988,5642.3284642799981,"no",25000,857.45,3875.54,null,103072.97319999999,417286.8322,500,0,24520.999679689616,0,282.11642321399989,24803.116102903616,-19160.787638623617,null,null,null,"Post 1980 Construction","25,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","25000 ft2","pthp","stand-alone","post198025000 ft2pthpstand-alone","base-roof","base-win","base-inf","25 fc","yes-day","no-occ","base-epd","high-eff",1016.49,0,0.23448541243965601,0.23449584673198401,0,8650.1363999999976,0,8650.1363999999976,"yes",25000,1369.38,6459.2,null,71750,446500,500,0,17105.256053975816,-4750,432.50681999999989,12787.762873975817,-4137.626473975819,null,null,null,"Post 1980 Construction","25,000 SF","Split System Heat Pump","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","25000 ft2","pthp","stand-alone","post198025000 ft2pthpstand-alone","base-roof","base-win","red-inf","40 fc","no-day","no-occ","red-epd","base-eff",1103.4100000000001,0,0.16903379276569,0.16903763169587399,0,6235.4987999999948,0,6235.4987999999948,"no",25000,1369.38,6459.2,null,23027.455999999998,58027.455999999998,230.27455999999998,0,5506.2897780370704,-3000,311.77493999999979,2818.0647180370702,3417.4340819629247,null,null,null,{"$f":"IF(A19657=\"new90.1-2004\",\"New Construction\",IF(A19657=\"post1980\",\"Post 1980 Construction\",IF(A19657=\"pre1980\",\"Pre 1980 Construction\")))","v":"Post 1980 Construction"},"25,000 SF","Split System Heat Pump","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","25000 ft2","pthp","stand-alone","post198025000 ft2pthpstand-alone","base-roof","eff-win","red-inf","base-lpd","no-day","yes-occ","base-epd","base-eff",1223.5,0,7.8587420415588194E-2,7.8599561704082402E-2,0,2899.3985999999973,0,2899.3985999999973,"no",25000,1369.38,6459.2,null,21609.6044,70660.796000000002,216.09604400000001,0,5167.2552893009506,0,144.96992999999986,5312.2252193009508,-2412.8266193009536,null,null,null,"Post 1980 Construction","25,000 SF","Split System Heat Pump","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","25000 ft2","pthp","stand-alone","post198025000 ft2pthpstand-alone","eff-roof","base-win","base-inf","25 fc","yes-day","no-occ","red-epd","base-eff",917.77,0,0.30883999160428199,0.30884047384156599,0,11392.578,0,11392.578,"yes",25000,1369.38,6459.2,null,112250,671500,500,0,26693.669482156027,-4750,569.62890000000004,22513.298382156026,-11120.720382156027,null,null,null,"Post 1980 Construction","25,000 SF","Split System Heat Pump","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","25000 ft2","pthp","stand-alone","post198025000 ft2pthpstand-alone","eff-roof","base-win","red-inf","base-lpd","yes-day","yes-occ","red-epd","high-eff",901.47,0,0.32111872944798198,0.32111577187525903,0,11845.391999999998,0,11845.391999999998,"yes",25000,1369.38,6459.2,null,142527.45600000001,487027.45600000001,500,0,33861.885918737156,0,592.26959999999997,34454.155518737156,-22608.763518737156,null,null,null,"Post 1980 Construction","25,000 SF","Split System Heat Pump","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","25000 ft2","pthp","stand-alone","post198025000 ft2pthpstand-alone","eff-roof","eff-win","red-inf","base-lpd","no-day","yes-occ","base-epd","high-eff",1139.31,0,0.141992583782271,0.14200185259099199,0,5238.1967999999988,0,5238.1967999999988,"no",25000,1369.38,6459.2,null,134859.60440000001,456910.79600000003,500,0,32046.514776842512,0,261.90983999999997,32308.424616842512,-27070.227816842515,null,null,null,"Post 1980 Construction","25,000 SF","Split System Heat Pump","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","25000 ft2","pthp","stand-alone","post198025000 ft2pthpstand-alone","eff-roof","eff-win","red-inf","40 fc","yes-day","yes-occ","red-epd","base-eff",899.91,0,0.32229063177779299,0.32229058567480201,0,11888.728799999999,0,11888.728799999999,"yes",25000,1369.38,6459.2,null,130609.60440000001,514910.79600000003,500,0,31040.323244255702,-3000,594.43643999999995,28634.759684255703,-16746.030884255706,null,null,null,"Post 1980 Construction","25,000 SF","Split System Heat Pump","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","25000 ft2","pthp","ad-e&flr","post198025000 ft2pthpad-e&flr","base-roof","base-win","red-inf","40 fc","no-day","no-occ","base-epd","base-eff",1285.55,0,7.6514949279231206E-2,7.6512506644828504E-2,0,2958.8478,0,2958.8478,{"$f":"IF(P20039>0.2,\"yes\",\"no\")","v":"no"},{"$f":"IF(B20039=\"5500 ft2\",5500,IF(B20039=\"10000 ft2\",10000,25000))","v":25000},{"$f":"IF(B20039=\"5500 ft2\",IF(D20039=\"stand-alone\",642.39,IF(D20039=\"ad-e&flr\",522.37,402.25)),IF(B20039=\"10000 ft2\",IF(D20039=\"stand-alone\",866.06,IF(D20039=\"ad-e&flr\",704.17,542.29)),IF(B20039=\"25000 ft2\",IF(D20039=\"stand-alone\",1369.38,IF(D20039=\"ad-e&flr\",1113.42,857.45)))))","v":1113.42},{"$f":"IF(B20039=\"5500 ft2\",IF(D20039=\"stand-alone\",3030.15,IF(D20039=\"ad-e&flr\",2424.14,1818.13)),IF(B20039=\"10000 ft2\",IF(D20039=\"stand-alone\",4085.12,IF(D20039=\"ad-e&flr\",3268.14,2451.05)),IF(B20039=\"25000 ft2\",IF(D20039=\"stand-alone\",6459.2,IF(D20039=\"ad-e&flr\",5167.32,3875.54)))))","v":5167.32},null,{"$f":"SUM(IF(F20039=\"eff-roof\",W20039*IF(AND(W$4=\"no\",X$4=\"no\"),$C$4,$C$3)),IF(G20039=\"eff-win\",X20039*IF(W$4=\"no\",$D$4,$D$3),0),IF(H20039=\"red-inf\",Y20039*IF(W$4=\"no\",$F$4,$F$3),0),IF(I20039=\"25 fc\",W20039*IF(W$4=\"no\",$H$4,$H$3),0),IF(I20039=\"40 fc\",W20039*IF(W$4=\"no\",$G$4,$G$3),0),IF(J20039=\"yes-day\",W20039*IF(W$4=\"no\",$I$4,$I$3),0),IF(K20039=\"yes-occ\",W20039*IF(W$4=\"no\",$J$4,$J$3),0),IF(L20039=\"red-epd\",W20039*IF(W$4=\"no\",$K$4,$K$3),0),IF(AND(M20039=\"high-eff\",C20039=\"psz-ac\"),W20039*IF(AND(W$4=\"no\",Y$4=\"no\"),$L$4,$L$3),0),IF(AND(M20039=\"high-eff\",C20039=\"ptac\"),W20039*IF(AND(W$4=\"no\",Y$4=\"no\"),$M$4,$M$3),0),IF(AND(M20039=\"high-eff\",C20039=\"pthp\"),W20039*IF(AND(W$4=\"no\",Y$4=\"no\"),$N$4,$N$3),0))","v":18721.9476},{"$f":"SUM(IF(F20039=\"eff-roof\",W20039*$C$4),IF(G20039=\"eff-win\",X20039*$D$4,0),IF(H20039=\"red-inf\",Y20039*$F$4,0),IF(I20039=\"25 fc\",W20039*$H$4,0),IF(I20039=\"40 fc\",W20039*$G$4,0),IF(J20039=\"yes-day\",W20039*$I$4,0),IF(K20039=\"yes-occ\",W20039*$J$4,0),IF(L20039=\"red-epd\",W20039*$K$4,0),IF(AND(M20039=\"high-eff\",C20039=\"psz-ac\"),W20039*$L$4,0),IF(AND(M20039=\"high-eff\",C20039=\"ptac\"),W20039*$M$4,0),IF(AND(M20039=\"high-eff\",C20039=\"pthp\"),W20039*$N$4,0))","v":53721.9476},187.21947599999999,0,{"$f":"-PMT($AE$3,$AE$4,AA20039+AC20039-AD20039)","v":4476.7632470918916},{"$f":"SUM(IF(F20039=\"eff-roof\",($C$5*W20039),0),IF(G20039=\"eff-win\",($D$5*X20039),0),IF(H20039=\"red-inf\",$F$5*(Y20039-X20039),0),IF(I20039=\"25 fc\",($H$5*W20039),0),IF(I20039=\"40 fc\",($G$5*W20039),0),IF(J20039=\"yes-day\",($I$5*W20039),0),IF(K20039=\"yes-occ\",($J$5*W20039),0),IF(L20039=\"red-epd\",($K$5*W20039),0),IF(M20039=\"high-eff\",($L$5*W20039),0))","v":-3000},{"$f":"0.05*U20039","v":147.94239000000002},1624.7056370918915,{"$f":"U20039-AH20039","v":1334.1421629081085},null,null,null,"Post 1980 Construction",{"$f":"IF(B20039=\"5500 ft2\",\"5,500 SF\",IF(B20039=\"10000 ft2\",\"10,000 SF\",IF(B20039=\"25000 ft2\",\"25,000 SF\")))","v":"25,000 SF"},"Split System Heat Pump","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration",{"$f":"IF(I20039=\"base-lpd\",\"Baseline Lighting Levels\",IF(I20039=\"40 fc\",\"Reduce Lighting Levels to 40 fc\",IF(I20039=\"25 fc\",\"Reduce Lighting Levels to 25 fc\")))","v":"Reduce Lighting Levels to 40 fc"},"No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","25000 ft2","pthp","ad-e&flr","post198025000 ft2pthpad-e&flr","base-roof","eff-win","red-inf","base-lpd","no-day","yes-occ","red-epd","base-eff",1178.29,0,0.15356380138814699,0.153563783170266,0,5938.5306,0,5938.5306,"no",25000,1113.42,5167.32,null,22966.303200000002,62849.007600000004,229.66303200000002,0,5491.6670147783616,0,296.92653000000001,5788.5935447783613,149.93705522163873,null,null,null,"Post 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","25000 ft2","pthp","ad-e&flr","post198025000 ft2pthpad-e&flr","base-roof","eff-win","red-inf","40 fc","yes-day","yes-occ","red-epd","high-eff",951.82,0,0.31625400427122302,0.31625073631883699,0,12229.867199999999,0,12229.867199999999,"yes",25000,1113.42,5167.32,null,91466.303199999995,282099.00760000001,500,0,21773.109544270937,-3000,611.49335999999994,19384.602904270938,-7154.7357042709391,null,null,null,"Post 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","25000 ft2","pthp","ad-e&flr","post198025000 ft2pthpad-e&flr","eff-roof","base-win","red-inf","40 fc","no-day","no-occ","base-epd","high-eff",1166.0999999999999,0,0.16232314468766701,0.16232058962975701,0,{"$f":"277.8*($N$19975-N20232)*$S$3","v":6277.1688000000013},{"$f":"277.78*($O$19975-O20232)*$S$4","v":0},{"$f":"SUM(S20232:T20232)","v":6277.1688000000013},"no",25000,1113.42,5167.32,null,131971.94760000001,439971.94760000001,{"$f":"MIN(0.01*AA20232,500)","v":500},{"$f":"IF(V20232=\"yes\",0,0)","v":0},31362.85928950681,-3000,313.85844000000009,{"$f":"SUM(AE20232:AG20232)","v":28676.71772950681},-22399.548929506811,null,null,null,"Post 1980 Construction","25,000 SF",{"$f":"IF(C20232=\"psz-ac\",\"Packaged Air Conditioner\",IF(C20232=\"ptac\",\"Split System Air Conditioner\",IF(C20232=\"pthp\",\"Split System Heat Pump\")))","v":"Split System Heat Pump"},{"$f":"IF(D20232=\"stand-alone\",\"Stand Alone\",IF(D20232=\"ad-e&flr\",\"Above Ground, 1 Side Attached\",IF(D20232=\"ad-e&w&flr\",\"Above Ground, 2 Sides Attached\")))","v":"Above Ground, 1 Side Attached"},{"$f":"IF(F20232=\"base-roof\",\"Baseline Roof Insulation\",IF(F20232=\"eff-roof\",\"Increased Roof Insulation\"))","v":"Increased Roof Insulation"},{"$f":"IF(G20232=\"base-win\",\"Baseline Windows\",IF(G20232=\"eff-win\",\"Replace Windows\"))","v":"Baseline Windows"},{"$f":"IF(H20232=\"base-inf\",\"Baseline Infiltration\",IF(H20232=\"red-inf\",\"Reduce Infiltration\"))","v":"Reduce Infiltration"},"Reduce Lighting Levels to 40 fc",{"$f":"IF(J20232=\"no-day\",\"No Daylighting Sensors\",IF(J20232=\"yes-day\",\"Install Daylighting Sensors\"))","v":"No Daylighting Sensors"},{"$f":"IF(K20232=\"no-occ\",\"No Occupancy Sensors\",IF(K20232=\"yes-occ\",\"Install Occupancy Sensors\"))","v":"No Occupancy Sensors"},{"$f":"IF(L20232=\"base-epd\",\"No Plug Load Control\",IF(L20232=\"red-epd\",\"Install Plug Load Controls\"))","v":"No Plug Load Control"},{"$f":"IF(M20232=\"base-eff\",\"Baseline HVAC Equipment\",IF(M20232=\"high-eff\",\"Install High Efficiency HVAC Equipment\"))","v":"Install High Efficiency HVAC Equipment"}]
["post1980","25000 ft2","pthp","ad-e&flr","post198025000 ft2pthpad-e&flr","eff-roof","base-win","red-inf","25 fc","yes-day","no-occ","red-epd","base-eff",958.12,0,0.31173251468232799,0.311725069321725,0,12054.8532,0,12054.8532,"yes",25000,1113.42,5167.32,null,114471.9476,673721.94760000007,500,0,27219.717684737581,-4750,602.74266,23072.460344737581,-11017.607144737582,null,null,null,"Post 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","25000 ft2","pthp","ad-e&flr","post198025000 ft2pthpad-e&flr","eff-roof","eff-win","red-inf","40 fc","yes-day","yes-occ","base-epd","base-eff",1060.1300000000001,0,0.23843766684463399,0.23844518196054801,0,9221.0153999999948,0,9221.0153999999948,"yes",25000,1113.42,5167.32,null,124466.30319999999,499599.00760000001,500,0,29585.890856121481,-3000,461.05076999999977,27046.941626121479,-17825.926226121483,null,null,null,"Post 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","25000 ft2","pthp","ad-e&w&flr","post198025000 ft2pthpad-e&w&flr","base-roof","base-win","red-inf","40 fc","no-day","no-occ","red-epd","base-eff",1142.1400000000001,0,0.15874020597392799,0.15872513129497701,0,5986.3122000000003,0,5986.3122000000003,"no",25000,857.45,3875.54,null,21916.482199999999,56916.482199999999,219.16482199999999,0,5240.6354357333867,-3000,299.31561000000005,2539.9510457333868,3446.3611542666135,null,null,null,{"$f":"IF(A20425=\"new90.1-2004\",\"New Construction\",IF(A20425=\"post1980\",\"Post 1980 Construction\",IF(A20425=\"pre1980\",\"Pre 1980 Construction\")))","v":"Post 1980 Construction"},"25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["post1980","25000 ft2","pthp","ad-e&w&flr","post198025000 ft2pthpad-e&w&flr","base-roof","base-win","red-inf","25 fc","yes-day","no-occ","red-epd","high-eff",926.11,0,0.31785677626851899,0.31784801455477601,0,11987.625600000005,0,11987.625600000005,"yes",25000,857.45,3875.54,null,77166.482199999999,451916.48220000003,500,0,18387.613354222212,-4750,599.38128000000029,14236.994634222212,-2249.3690342222071,null,null,null,"Post 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","25000 ft2","pthp","ad-e&w&flr","post198025000 ft2pthpad-e&w&flr","base-roof","eff-win","red-inf","40 fc","yes-day","yes-occ","base-epd","high-eff",1035.26,0,0.237451671399733,0.23745055722104,0,8955.438600000005,0,8955.438600000005,"yes",25000,857.45,3875.54,null,85322.973200000008,266786.8322,500,0,20318.670337709402,-3000,447.77193000000028,17766.442267709401,-8811.0036677093958,null,null,null,"Post 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["post1980","25000 ft2","pthp","ad-e&w&flr","post198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","40 fc","no-day","no-occ","red-epd","high-eff",1021,0,0.247955657440038,0.24795415540316601,0,9351.5814000000028,0,9351.5814000000028,"yes",25000,857.45,3875.54,null,135166.4822,443166.48220000003,500,0,32119.168387171652,-3000,467.57907000000017,29586.747457171652,-20235.166057171649,null,null,null,"Post 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["post1980","25000 ft2","pthp","ad-e&w&flr","post198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","25 fc","yes-day","no-occ","base-epd","base-eff",1028.1400000000001,0,0.242703664419886,0.24269499053497601,0,9153.2322000000004,0,9153.2322000000004,"yes",25000,857.45,3875.54,null,110166.4822,669416.48219999997,500,0,26200.39466607276,-4750,457.66161000000005,21908.056276072759,-12754.824076072759,null,null,null,"Post 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["post1980","25000 ft2","pthp","ad-e&w&flr","post198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","40 fc","yes-day","yes-occ","red-epd","base-eff",918.55,0,0.32341670373284997,0.32341654206227,0,12197.642400000004,0,12197.642400000004,"yes",25000,857.45,3875.54,null,125822.97319999999,491786.8322,500,0,29907.083765889613,-3000,609.88212000000021,27516.965885889615,-15319.32348588961,null,null,null,"Post 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","5500 ft2","psz-ac","stand-alone","pre19805500 ft2psz-acstand-alone","base-roof","base-win","base-inf","base-lpd","no-day","yes-occ","red-epd","high-eff",281.18,278.02,5.5920882307254102E-2,0.17256194455888399,-0.10106930693069301,1629.0191999999997,-221.07358901900784,1407.9456109809919,"no",5500,642.39,3030.15,null,5060,36300,50.6,0,1209.9393991619213,0,70.397280549049597,1280.3366797109709,127.608931270021,null,null,null,"Pre 1980 Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","5500 ft2","psz-ac","stand-alone","pre19805500 ft2psz-acstand-alone","base-roof","eff-win","base-inf","base-lpd","no-day","no-occ","red-epd","high-eff",301.02999999999997,263.3,4.7265227221733201E-2,0.114148666941322,-4.2772277227722803E-2,1077.5862000000006,-93.557788456320097,984.02841154368059,"no",5500,642.39,3030.15,null,7692.3602000000001,61942.770000000004,76.923602000000002,0,1839.3853119614773,0,49.201420577184031,1888.5867325386614,-904.55832099498082,null,null,null,"Pre 1980 Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","5500 ft2","psz-ac","stand-alone","pre19805500 ft2psz-acstand-alone","base-roof","eff-win","red-inf","40 fc","yes-day","yes-occ","red-epd","base-eff",214.53,223.02,0.26128341876801497,0.36869519157200897,0.11675247524752499,3480.5562,255.37811145299187,3735.934311452992,"yes",5500,642.39,3030.15,null,15375.324700000001,61815.734499999999,153.75324700000002,0,3676.5239386240014,-660,186.79671557264962,3203.320654196651,532.61365725634096,null,null,null,"Pre 1980 Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","5500 ft2","psz-ac","stand-alone","pre19805500 ft2psz-acstand-alone","eff-roof","base-win","base-inf","base-lpd","no-day","yes-occ","red-epd","high-eff",273.91000000000003,251.62,0.112747890022265,0.19395562356541701,3.48514851485147E-3,1830.9797999999992,7.6232272075519596,1838.6030272075511,"no",5500,642.39,3030.15,null,21560,103125,215.6,0,5155.3939616464468,0,91.930151360377565,5247.3241130068245,-3408.7210857992732,null,null,null,"Pre 1980 Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","5500 ft2","psz-ac","stand-alone","pre19805500 ft2psz-acstand-alone","eff-roof","base-win","red-inf","25 fc","yes-day","no-occ","base-epd","high-eff",238.62,186.73,0.28189129947013197,0.29780472014595999,0.26047524752475298,2811.3359999999998,569.74960618260798,3381.085606182608,"yes",5500,642.39,3030.15,null,27427.964500000002,181702.9645,274.27964500000002,0,6558.5325864356719,-1045,169.05428030913041,5682.5868667448021,-2301.5012605621941,null,null,null,"Pre 1980 Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","5500 ft2","psz-ac","stand-alone","pre19805500 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","40 fc","no-day","no-occ","red-epd","base-eff",271.43,246.51,0.125563092217677,0.20125360484962601,2.3722772277227799E-2,1899.8742,51.88992156049607,1951.7641215604961,"no",5500,642.39,3030.15,null,25567.360199999999,106602.77,255.67360199999999,0,6113.6277546530455,-660,97.588206078024811,5551.2159607310705,-3599.4518391705742,null,null,null,"Pre 1980 Construction","5,500 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","5500 ft2","psz-ac","ad-e&flr","pre19805500 ft2psz-acad-e&flr","base-roof","base-win","base-inf","base-lpd","no-day","yes-occ","base-epd","base-eff",324.91000000000003,234.31,2.4372190911036502E-2,7.3644294919313402E-2,-5.33153517644415E-2,717.55739999999969,-102.74031213814412,614.81708786185561,"no",5500,522.37,2424.14,null,1980,1980,19.8,0,473.45454749814303,0,30.740854393092782,504.1954018912358,110.62168597061981,null,null,null,"Pre 1980 Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","5500 ft2","psz-ac","ad-e&flr","pre19805500 ft2psz-acad-e&flr","base-roof","base-win","red-inf","25 fc","yes-day","no-occ","red-epd","base-eff",229.28,220.21,0.215800456588428,0.34629640189313998,1.0069678579456001E-2,3374.1588000000006,19.404578346495832,3393.5633783464964,"yes",5500,522.37,2424.14,null,9237.3801999999996,81947.3802,92.373801999999998,0,2208.8281124541945,-1045,169.67816891732483,1333.5062813715194,2060.057096974977,null,null,null,"Pre 1980 Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","5500 ft2","psz-ac","ad-e&flr","pre19805500 ft2psz-acad-e&flr","base-roof","eff-win","base-inf","40 fc","no-day","no-occ","red-epd","high-eff",278.97000000000003,251.01,7.5381679389313005E-2,0.20462450818269901,-0.128388401888065,1993.7705999999996,-247.40837391782398,1746.3622260821755,"no",5500,522.37,2424.14,null,10460.616599999999,68111.91,104.606166,0,2501.3265145982641,-660,87.318111304108783,1928.6446259023728,-182.28239982019727,null,null,null,"Pre 1980 Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","5500 ft2","psz-ac","ad-e&flr","pre19805500 ft2psz-acad-e&flr","eff-roof","base-win","base-inf","base-lpd","no-day","yes-occ","base-epd","high-eff",313.91000000000003,201.71,0.100440536491403,0.10500655756400699,9.3234434704427896E-2,1023.1373999999996,179.66560486889583,1202.8030048688954,"no",5500,522.37,2424.14,null,20735,102300,207.35,0,4958.1212335222199,0,60.140150243444772,5018.2613837656645,-3815.4583788967693,null,null,null,"Pre 1980 Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","5500 ft2","psz-ac","ad-e&flr","pre19805500 ft2psz-acad-e&flr","eff-roof","base-win","red-inf","25 fc","yes-day","no-occ","red-epd","high-eff",219.3,186.59,0.29188663765427703,0.37475052745623499,0.16120476511575599,3651.4032000000002,310.64650870774386,3962.0497087077442,"yes",5500,522.37,2424.14,null,27992.3802,182267.38020000001,279.92380200000002,0,6693.494798478273,-1045,198.10248543538722,5846.5972839136602,-1884.547575205916,null,null,null,"Pre 1980 Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","5500 ft2","psz-ac","ad-e&flr","pre19805500 ft2psz-acad-e&flr","eff-roof","eff-win","base-inf","40 fc","no-day","no-occ","base-epd","base-eff",311.91000000000003,199.25,0.108216808161518,0.11070878713577,0.104293099572938,1078.6973999999998,200.97599001727988,1279.6733900172796,"no",5500,522.37,2424.14,null,23880.616600000001,100616.91,238.80616600000002,0,5710.2962254190115,-660,63.983669500863982,5114.2798949198759,-3834.6065049025965,null,null,null,"Pre 1980 Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","5500 ft2","psz-ac","ad-e&w&flr","pre19805500 ft2psz-acad-e&w&flr","base-roof","base-win","base-inf","base-lpd","no-day","yes-occ","red-epd","base-eff",280.29000000000002,202.25,5.7403320985312201E-2,0.17216019847598801,-0.16671473896740699,1619.2961999999991,-250.35371170256002,1368.942488297439,"no",5500,402.25,1818.13,null,2805,2805,28.05,0,670.72727562236935,0,68.447124414871951,739.1744000372413,629.76808826019771,null,null,null,"Pre 1980 Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","5500 ft2","psz-ac","ad-e&w&flr","pre19805500 ft2psz-acad-e&w&flr","base-roof","base-win","base-inf","40 fc","yes-day","yes-occ","red-epd","high-eff",226.26,225.74,0.11706323451588101,0.331738437001595,-0.30222094029420299,3120.2496000000001,-453.84190159505607,2666.4076984049439,"no",5500,402.25,1818.13,null,11715,66385,117.15,0,2801.272739364013,-660,133.32038492024719,2274.5931242842603,391.81457412068357,null,null,null,"Pre 1980 Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","5500 ft2","psz-ac","ad-e&w&flr","pre19805500 ft2psz-acad-e&w&flr","base-roof","eff-win","base-inf","40 fc","no-day","no-occ","base-epd","high-eff",301.58,183.72,5.2021447614102698E-2,0.109279933841337,-5.9821171041246103E-2,1027.8600000000001,-89.832802434448041,938.02719756555211,"no",5500,402.25,1818.13,null,8773.1549999999988,62121.75,87.731549999999984,0,2097.823298311147,-660,46.90135987827761,1484.7246581894246,-546.69746062387253,null,null,null,"Pre 1980 Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","5500 ft2","psz-ac","ad-e&w&flr","pre19805500 ft2psz-acad-e&w&flr","eff-roof","base-win","base-inf","base-lpd","no-day","yes-occ","red-epd","high-eff",272.74,167.98,0.13909995906181699,0.19445921200307201,3.0977790597057998E-2,1829.0351999999996,46.519011482448036,1875.5542114824475,"no",5500,402.25,1818.13,null,21560,103125,215.6,0,5155.3939616464468,0,93.777710574122381,5249.1716722205692,-3373.6174607381217,null,null,null,"Pre 1980 Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","5500 ft2","psz-ac","ad-e&w&flr","pre19805500 ft2psz-acad-e&w&flr","eff-roof","base-win","base-inf","25 fc","no-day","no-occ","base-epd","base-eff",285.39999999999998,161.62,0.126798534213338,0.157067753558982,6.7666570522065095E-2,1477.3404000000003,101.6141535733919,1578.9545535733921,"no",5500,402.25,1818.13,null,20845,128150,208.45000000000002,0,4984.424263938784,-1045,78.947727678669608,4018.3719916174537,-2439.4174380440618,null,null,null,"Pre 1980 Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","5500 ft2","psz-ac","ad-e&w&flr","pre19805500 ft2psz-acad-e&w&flr","eff-roof","eff-win","base-inf","40 fc","no-day","no-occ","red-epd","base-eff",272.33999999999997,166.04,0.14367305368892999,0.195640616693248,4.2169022209403002E-2,1840.1472000000003,63.324762371824015,1903.4719623718242,"no",5500,402.25,1818.13,null,23843.154999999999,96276.75,238.43154999999999,0,5701.3384653803469,-660,95.173598118591215,5136.512063498938,-3233.0401011271138,null,null,null,"Pre 1980 Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","5500 ft2","psz-ac","ad-e&w&flr","pre19805500 ft2psz-acad-e&w&flr","eff-roof","eff-win","base-inf","25 fc","yes-day","no-occ","red-epd","high-eff",220.79,189.36,0.198809797206219,0.34789414613976,-9.23565041822903E-2,3272.2062000000001,-138.69075862830417,3133.5154413716959,"no",5500,402.25,1818.13,null,29838.154999999999,198521.75,298.38155,0,7134.8536230830568,-1045,156.67577206858482,6246.5293951516414,-3113.0139537799455,null,null,null,"Pre 1980 Construction","5,500 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","5500 ft2","ptac","stand-alone","pre19805500 ft2ptacstand-alone","base-roof","base-win","base-inf","40 fc","yes-day","yes-occ","base-epd","high-eff",195.22,200.69,0.152887906992005,0.265289225095028,4.7607240267791102E-3,1958.2121999999997,8.3162478627840688,1966.5284478627839,"no",5500,642.39,3030.15,null,12265,47740,122.65,0,2932.7878914468306,-660,98.326422393139197,2371.1143138399698,-404.5858659771859,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","5500 ft2","ptac","stand-alone","pre19805500 ft2ptacstand-alone","base-roof","eff-win","base-inf","40 fc","no-day","no-occ","red-epd","high-eff",205.3,191.79,0.15037240383668901,0.227353129351549,4.8896603025043499E-2,1678.1897999999992,85.414795757344123,1763.6045957573433,"no",5500,642.39,3030.15,null,12697.360199999999,55452.770000000004,126.973602,0,3036.1731959151166,-660,88.180229787867177,2464.3534257029837,-700.74882994564041,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","5500 ft2","ptac","stand-alone","pre19805500 ft2ptacstand-alone","base-roof","eff-win","base-inf","25 fc","yes-day","yes-occ","base-epd","base-eff",186.74,231.38,0.10536677129701499,0.29720371833954301,-0.147433672204314,2193.786599999999,-257.54380100059188,1936.2427989994071,"no",5500,642.39,3030.15,null,13962.360199999999,109682.77,139.62360200000001,0,3338.6580457055966,-1045,96.812139949970359,2390.4701856555671,-454.22738665615998,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","5500 ft2","ptac","stand-alone","pre19805500 ft2ptacstand-alone","eff-roof","base-win","base-inf","40 fc","yes-day","yes-occ","red-epd","base-eff",163.61000000000001,221.74,0.175494624479127,0.38425350946520598,-9.9628068435407904E-2,2836.3379999999993,-174.03481204513602,2662.3031879548635,"no",5500,642.39,3030.15,null,25960,99715,259.60000000000002,0,6207.5151783089859,-660,133.11515939774318,5680.6303377067288,-3018.3271497518654,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","5500 ft2","ptac","stand-alone","pre19805500 ft2ptacstand-alone","eff-roof","eff-win","base-inf","40 fc","no-day","yes-occ","base-epd","base-eff",218.56,196.98,0.11090087823871,0.17744909864137601,2.3158938755269101E-2,1309.8269999999995,40.45508074916814,1350.2820807491678,"no",5500,642.39,3030.15,null,26722.360199999999,107757.77,267.22360199999997,0,6389.8095740269628,-660,67.514104037458395,5797.3236780644211,-4447.0415973152531,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","5500 ft2","ptac","stand-alone","pre19805500 ft2ptacstand-alone","eff-roof","eff-win","base-inf","25 fc","yes-day","yes-occ","base-epd","high-eff",182.19,185.58,0.213095928165979,0.31432765044597499,7.9692536573270495E-2,2320.1855999999998,139.21052411972792,2459.3961241197276,"yes",5500,642.39,3030.15,null,34092.360199999996,192182.77000000002,340.92360199999996,0,8152.1126119367173,-1045,122.96980620598639,7230.0824181427033,-4770.6862940229757,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","5500 ft2","ptac","ad-e&flr","pre19805500 ft2ptacad-e&flr","base-roof","base-win","base-inf","40 fc","yes-day","yes-occ","red-epd","high-eff",170.58,215.88,0.18465835562074001,0.38331947507320802,-9.3783249734002094E-2,2945.5134000000003,-160.34765410430393,2785.1657458956965,"no",5500,522.37,2424.14,null,13090,48565,130.9,0,3130.0606195710566,-660,139.25828729478482,2609.3189068658412,175.84683902985535,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","5500 ft2","ptac","ad-e&flr","pre19805500 ft2ptacad-e&flr","base-roof","base-win","red-inf","base-lpd","yes-day","no-occ","base-epd","base-eff",234.18,185.63,0.114312828918989,0.15339286359856799,5.9482190809140197E-2,1178.7054000000003,101.70078115529607,1280.4061811552963,"no",5500,522.37,2424.14,null,4067.3802000000005,19797.3802,40.673802000000009,0,972.58568287571063,0,64.02030905776482,1036.6059919334755,243.8001892218208,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","5500 ft2","ptac","ad-e&flr","pre19805500 ft2ptacad-e&flr","base-roof","eff-win","base-inf","25 fc","yes-day","no-occ","red-epd","base-eff",170.91,246.75,0.118831420930032,0.38212645963631098,-0.250189998480012,2936.3460000000009,-427.7669994419519,2508.5790005580488,"no",5500,522.37,2424.14,null,11945.616599999999,103366.91,119.456166,0,2856.4174252218713,-1045,125.42895002790245,1936.8463752497737,571.73262530827515,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","5500 ft2","ptac","ad-e&flr","pre19805500 ft2ptacad-e&flr","eff-roof","base-win","base-inf","25 fc","no-day","no-occ","base-epd","base-eff",228.47,193.41,0.10992364765766501,0.174035645855175,2.0063839489284099E-2,1337.3292000000006,34.304522433984069,1371.6337224339848,"no",5500,522.37,2424.14,null,20845,128150,208.45000000000002,0,4984.424263938784,-1045,68.581686121699235,4008.005950060483,-2636.372227626498,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","5500 ft2","ptac","ad-e&flr","pre19805500 ft2ptacad-e&flr","eff-roof","base-win","red-inf","base-lpd","yes-day","no-occ","base-epd","high-eff",227.83,138.97999999999999,0.22610214821844499,0.17634937276309601,0.29584029994426703,1355.1084000000001,505.81845073745609,1860.9268507374561,"yes",5500,522.37,2424.14,null,24197.3802,102297.3802,241.97380200000001,0,5786.0402491068317,0,93.046342536872814,5879.0865916437042,-4018.1597409062479,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","5500 ft2","ptac","ad-e&flr","pre19805500 ft2ptacad-e&flr","eff-roof","eff-win","base-inf","25 fc","yes-day","no-occ","red-epd","high-eff",165.78,192.97,0.24311966180657399,0.40067242688261501,2.2293154988093498E-2,3078.8574000000008,38.11613603776005,3116.9735360377608,"yes",5500,522.37,2424.14,null,32075.616600000001,185866.91,320.75616600000001,0,7669.8719914529929,-1045,155.84867680188805,6780.7206682548813,-3663.7471322171205,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","5500 ft2","ptac","ad-e&flr","pre19805500 ft2ptacad-e&flr","eff-roof","eff-win","red-inf","40 fc","no-day","yes-occ","base-epd","base-eff",228.5,157.22999999999999,0.186189716159089,0.17392718990636599,0.20337437300501601,1336.4958000000006,347.72311376265606,1684.2189137626567,"no",5500,522.37,2424.14,null,26902.996800000001,103639.2902,269.029968,0,6433.0031193373688,-660,84.210945688132838,5857.2140650255014,-4172.995151262845,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","5500 ft2","ptac","ad-e&w&flr","pre19805500 ft2ptacad-e&w&flr","base-roof","base-win","red-inf","base-lpd","no-day","yes-occ","red-epd","base-eff",219.04,163.33000000000001,0.126254190368285,0.20296921621424899,-3.3171570735304398E-3,1549.5684000000001,-4.6778894228161771,1544.8905105771839,"no",5500,402.25,1818.13,null,3586.7959000000001,3586.7959000000001,35.867958999999999,0,857.66910596095704,0,77.244525528859199,934.91363148981623,609.97687908736771,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","5500 ft2","ptac","ad-e&w&flr","pre19805500 ft2ptacad-e&w&flr","base-roof","eff-win","base-inf","25 fc","yes-day","yes-occ","base-epd","base-eff",192.71,200.97,0.100381951339166,0.29877738155883798,-0.23453529086553199,2281.0157999999997,-330.74410770947202,1950.2716922905277,"no",5500,402.25,1818.13,null,12238.155000000001,99356.75,122.38155,0,2926.3687564328975,-1045,97.513584614526394,1978.8823410474238,-28.610648756896126,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","5500 ft2","ptac","ad-e&w&flr","pre19805500 ft2ptacad-e&w&flr","base-roof","eff-win","red-inf","25 fc","yes-day","yes-occ","base-epd","base-eff",192.67,175.51,0.15866749208648201,0.29892293137326298,-7.8137477732047406E-2,2282.1270000000004,-110.19028418188798,2171.9367158181126,"no",5500,402.25,1818.13,null,13019.9509,100138.5459,130.19950900000001,0,3113.3105867714853,-1045,108.59683579090563,2176.9074225623908,-4.9707067442782318,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","5500 ft2","ptac","ad-e&w&flr","pre19805500 ft2ptacad-e&w&flr","eff-roof","base-win","red-inf","base-lpd","no-day","yes-occ","red-epd","base-eff",216.85,134.78,0.19647717052316799,0.21093806855396299,0.172062165980711,1610.4066000000003,242.64385691310389,1853.0504569131042,"no",5500,402.25,1818.13,null,20086.795900000001,70411.795899999997,200.86795900000001,0,4803.1236684454825,0,92.652522845655213,4895.7761912911374,-3042.7257343780329,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","5500 ft2","ptac","ad-e&w&flr","pre19805500 ft2ptacad-e&w&flr","eff-roof","eff-win","base-inf","25 fc","yes-day","yes-occ","base-epd","base-eff",190.41,172.83,0.16993914475605301,0.30714649588821802,-6.1674550033786003E-2,2344.9098000000004,-86.974092231616169,2257.9357077683844,"no",5500,402.25,1818.13,null,28738.154999999999,166181.75,287.38155,0,6871.8233189174216,-1045,112.89678538841923,5939.7201043058412,-3681.7843965374568,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","5500 ft2","ptac","ad-e&w&flr","pre19805500 ft2ptacad-e&w&flr","eff-roof","eff-win","red-inf","40 fc","no-day","yes-occ","base-epd","high-eff",223.66,112.55,0.23174050669874899,0.186158212648279,0.30861846550770899,1421.2248,435.21697148569592,1856.4417714856959,"yes",5500,402.25,1818.13,null,29409.9509,113888.5459,294.09950900000001,0,7032.4621188394467,-660,92.822088574284805,6465.2842074137316,-4608.8424359280361,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","5500 ft2","pthp","stand-alone","pre19805500 ft2pthpstand-alone","base-roof","base-win","red-inf","base-lpd","no-day","yes-occ","red-epd","high-eff",341.84,0,0.19587566885107899,0.19585979769466,0,2312.9628000000016,0,2312.9628000000016,"no",5500,642.39,3030.15,null,12522.9645,22257.964500000002,125.229645,0,2994.4719649913177,0,115.64814000000008,3110.1201049913179,-797.15730499131632,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Heat Pump","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","5500 ft2","pthp","stand-alone","pre19805500 ft2pthpstand-alone","base-roof","base-win","red-inf","25 fc","no-day","no-occ","base-epd","base-eff",367.45,0,0.135621956351831,0.13561514937661701,0,1601.5170000000012,0,1601.5170000000012,"no",5500,642.39,3030.15,null,5647.9645,62627.964500000002,56.479645000000005,0,1350.532563956099,-1045,80.075850000000059,385.60841395609907,1215.9085860439022,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Heat Pump","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","5500 ft2","pthp","stand-alone","pre19805500 ft2pthpstand-alone","base-roof","eff-win","red-inf","40 fc","no-day","no-occ","red-epd","base-eff",352.61,0,0.17051644321529499,0.17052458245118801,0,2013.7722000000003,0,2013.7722000000003,"no",5500,642.39,3030.15,null,10370.324700000001,41080.734499999999,103.70324700000002,0,2479.7360546703621,-660,100.68861000000003,1920.4246646703621,93.347535329638276,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Heat Pump","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","5500 ft2","pthp","stand-alone","pre19805500 ft2pthpstand-alone","eff-roof","base-win","red-inf","base-lpd","yes-day","no-occ","base-epd","base-eff",353.93,0,0.16741417663680599,0.16741943072218299,0,1977.1026000000006,0,1977.1026000000006,"no",5500,642.39,3030.15,null,20827.964500000002,86882.964500000002,208.27964500000002,0,4980.3507614418622,0,98.855130000000031,5079.2058914418621,-3102.1032914418615,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Heat Pump","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","5500 ft2","pthp","stand-alone","pre19805500 ft2pthpstand-alone","eff-roof","base-win","red-inf","25 fc","no-day","no-occ","base-epd","high-eff",335.99,0,0.209631455540191,0.20962126558456801,0,2475.4758000000006,0,2475.4758000000006,"yes",5500,642.39,3030.15,null,30562.964500000002,147602.9645,305.62964500000004,0,7308.1689533077333,-1045,123.77379000000003,6386.9427433077335,-3911.4669433077329,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Heat Pump","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","5500 ft2","pthp","stand-alone","pre19805500 ft2pthpstand-alone","eff-roof","eff-win","red-inf","40 fc","no-day","no-occ","red-epd","high-eff",321.36,0,0.244032946552035,0.24403669724770599,0,2881.8972000000008,0,2881.8972000000008,"yes",5500,642.39,3030.15,null,35285.324699999997,126055.73450000001,352.85324699999995,0,8437.3724440219939,-660,144.09486000000004,7921.4673040219941,-5039.5701040219938,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Heat Pump","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","5500 ft2","pthp","stand-alone","pre19805500 ft2pthpstand-alone","eff-roof","eff-win","red-inf","25 fc","yes-day","yes-occ","base-epd","base-eff",321.45999999999998,0,0.24381650934888499,0.243801458480358,0,2879.1192000000015,0,2879.1192000000015,"yes",5500,642.39,3030.15,null,31765.324699999997,177810.73450000002,317.65324699999996,0,7595.6754706919619,-1045,143.95596000000009,6694.6314306919621,-3815.5122306919607,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Heat Pump","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","5500 ft2","pthp","ad-e&flr","pre19805500 ft2pthpad-e&flr","base-roof","base-win","red-inf","40 fc","yes-day","yes-occ","red-epd","base-eff",339.27,0,0.21880112519567299,0.21881188118811901,0,2639.9334000000013,0,2639.9334000000013,"yes",5500,522.37,2424.14,null,10502.3802,33932.3802,105.023802,0,2511.312962244675,-660,131.99667000000008,1983.309632244675,656.6237677553263,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","5500 ft2","pthp","ad-e&flr","pre19805500 ft2pthpad-e&flr","base-roof","eff-win","red-inf","40 fc","no-day","yes-occ","base-epd","base-eff",377.3,0,0.13123359580052499,0.13124568270780601,0,1583.46,0,1583.46,"no",5500,522.37,2424.14,null,10402.996800000001,36814.290200000003,104.02996800000001,0,2487.5485568528438,-660,79.173000000000002,1906.7215568528438,-323.2615568528438,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","5500 ft2","pthp","ad-e&flr","pre19805500 ft2pthpad-e&flr","base-roof","eff-win","red-inf","25 fc","yes-day","yes-occ","base-epd","high-eff",333.56,0,0.23194802443416601,0.23195947501726899,0,2798.5572000000006,0,2798.5572000000006,"yes",5500,522.37,2424.14,null,22557.996800000001,123714.2902,225.57996800000001,0,5394.0334178831099,-1045,139.92786000000004,4488.9612778831097,-1690.404077883109,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","5500 ft2","pthp","ad-e&flr","pre19805500 ft2pthpad-e&flr","eff-roof","base-win","red-inf","40 fc","yes-day","yes-occ","red-epd","high-eff",301.87,0,0.30493273542600902,0.30492746949113497,0,3678.9054000000006,0,3678.9054000000006,"yes",5500,522.37,2424.14,null,35417.3802,118907.3802,354.17380200000002,0,8468.9493515963095,-660,183.94527000000005,7992.8946215963097,-4313.9892215963091,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","5500 ft2","pthp","ad-e&flr","pre19805500 ft2pthpad-e&flr","eff-roof","eff-win","red-inf","40 fc","no-day","yes-occ","base-epd","high-eff",341.63,0,0.21336346409613599,0.21337784941284799,0,2574.3726000000006,0,2574.3726000000006,"yes",5500,522.37,2424.14,null,35317.996800000001,121789.2902,353.17996800000003,0,8445.1849462044756,-660,128.71863000000005,7913.9035762044759,-5339.5309762044753,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","5500 ft2","pthp","ad-e&flr","pre19805500 ft2pthpad-e&flr","eff-roof","eff-win","red-inf","25 fc","yes-day","yes-occ","red-epd","base-eff",308.39999999999998,0,0.28987912385391301,0.289891779875662,0,3497.5020000000013,0,3497.5020000000013,"yes",5500,522.37,2424.14,null,31467.996800000001,173214.29019999999,314.67996800000003,0,7524.5788816247541,-1045,174.87510000000009,6654.4539816247543,-3156.951981624753,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","5500 ft2","pthp","ad-e&w&flr","pre19805500 ft2pthpad-e&w&flr","base-roof","base-win","red-inf","25 fc","no-day","no-occ","base-epd","base-eff",358.75,0,0.12277829162812801,0.122774843505477,0,1394.8337999999994,0,1394.8337999999994,"no",5500,402.25,1818.13,null,5126.7959000000001,62106.795899999997,51.267959000000005,0,1225.9115317928458,-1045,69.741689999999977,250.65322179284581,1144.1805782071535,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","5500 ft2","pthp","ad-e&w&flr","pre19805500 ft2pthpad-e&w&flr","base-roof","eff-win","base-inf","base-lpd","yes-day","no-occ","base-epd","high-eff",358.6,0,0.123128265380096,0.12314162754303599,0,1399.0007999999989,0,1399.0007999999989,"no",5500,402.25,1818.13,null,14328.155000000001,54201.75,143.28155000000001,0,3426.1263343476039,0,69.950039999999944,3496.0763743476036,-2097.0755743476047,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","5500 ft2","pthp","ad-e&w&flr","pre19805500 ft2pthpad-e&w&flr","base-roof","eff-win","red-inf","25 fc","yes-day","no-occ","red-epd","high-eff",298.55,0,0.26996725245606601,0.26997750391236303,0,3067.1897999999997,0,3067.1897999999997,"yes",5500,402.25,1818.13,null,20279.9509,117133.5459,202.799509,0,4849.3105942646762,-1045,153.35948999999999,3957.670084264676,-890.48028426467636,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","5500 ft2","pthp","ad-e&w&flr","pre19805500 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","25 fc","no-day","no-occ","base-epd","high-eff",324.58,0,0.20633452491063201,0.20632824726134599,0,2344.0763999999999,0,2344.0763999999999,"yes",5500,402.25,1818.13,null,30041.795900000001,147081.7959,300.417959,0,7183.5479211444799,-1045,117.20382000000001,6255.7517411444796,-3911.6753411444797,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","5500 ft2","pthp","ad-e&w&flr","pre19805500 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","base-lpd","yes-day","no-occ","red-epd","base-eff",332.45,0,0.18708596855235901,0.18708431142410001,0,2125.4477999999999,0,2125.4477999999999,"no",5500,402.25,1818.13,null,23238.154999999999,103701.75,232.38155,0,5556.6717980892472,0,106.27239,5662.9441880892473,-3537.4963880892474,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","5500 ft2","pthp","ad-e&w&flr","pre19805500 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","25 fc","yes-day","yes-occ","base-epd","base-eff",310.5,0,0.240756943229258,0.24075704225352099,0,2735.2187999999996,0,2735.2187999999996,"yes",5500,402.25,1818.13,null,29519.9509,166963.5459,295.19950899999998,0,7058.7651492560099,-1045,136.76093999999998,6150.52608925601,-3415.3072892560103,null,null,null,"Pre 1980 Construction","5,500 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","10000 ft2","psz-ac","stand-alone","pre198010000 ft2psz-acstand-alone","base-roof","base-win","base-inf","40 fc","no-day","yes-occ","base-epd","high-eff",487.97,396.18,6.2762206771582105E-2,0.15109077624299799,-7.4998643295164702E-2,2412.6930000000007,-239.43863638265586,2173.254363617345,"no",10000,866.06,4085.12,null,14300,85100,143,0,3419.3939541532554,-1200,108.66271818086726,2328.0566723341226,-154.80230871677759,null,null,null,"Pre 1980 Construction","10,000 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","10000 ft2","psz-ac","stand-alone","pre198010000 ft2psz-acstand-alone","base-roof","eff-win","base-inf","base-lpd","yes-day","no-occ","red-epd","high-eff",433.14,413.17,0.10287368773512399,0.24647715806687301,-0.12109947359852399,3935.8704000000021,-386.6188980375519,3549.2515019624502,"no",10000,866.06,4085.12,null,17318.310799999999,133740.57999999999,173.183108,0,4141.1277794172747,0,177.46257509812253,4318.5903545153969,-769.33885255294672,null,null,null,"Pre 1980 Construction","10,000 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","10000 ft2","psz-ac","stand-alone","pre198010000 ft2psz-acstand-alone","base-roof","eff-win","red-inf","25 fc","yes-day","yes-occ","base-epd","high-eff",385.85,316.95999999999998,0.25498808374859699,0.32874639017431501,0.13995767080913901,5249.5866000000015,446.82506746083232,5696.411667460834,"yes",10000,866.06,4085.12,null,29074.912400000001,249097.18160000001,290.74912399999999,0,6952.3482292374492,-1900,284.8205833730417,5337.1688126104909,359.24285485034306,null,null,null,"Pre 1980 Construction","10,000 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","10000 ft2","psz-ac","stand-alone","pre198010000 ft2psz-acstand-alone","eff-roof","base-win","base-inf","40 fc","no-day","yes-occ","red-epd","base-eff",424.2,381.71,0.14570325579563101,0.262029852823493,-3.5735605361697398E-2,4184.2236000000021,-114.08852536756763,4070.1350746324342,"no",10000,866.06,4085.12,null,41700,147200,417,0,9971.2397124608924,-1200,203.50675373162173,8974.7464661925133,-4904.611391560079,null,null,null,"Pre 1980 Construction","10,000 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","10000 ft2","psz-ac","stand-alone","pre198010000 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","base-lpd","yes-day","no-occ","base-epd","base-eff",480.65,344.47,0.125327450710051,0.16382519745311599,6.5311770771150995E-2,2616.0426000000025,208.51258964292791,2824.5551896429306,"no",10000,866.06,4085.12,null,41718.310799999999,192840.58,417.183108,0,9975.6181627277238,0,141.22775948214652,10116.84592220987,-7292.2907325669394,null,null,null,"Pre 1980 Construction","10,000 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","10000 ft2","psz-ac","stand-alone","pre198010000 ft2psz-acstand-alone","eff-roof","eff-win","red-inf","25 fc","yes-day","yes-occ","red-epd","base-eff",319.63,300.87,0.34224261881782903,0.44394767057513701,0.183616432408965,7089.1782000000021,586.20884674436809,7675.3870467443703,"yes",10000,866.06,4085.12,null,56474.912400000001,311197.18160000001,500,0,13488.86457100127,-1900,383.76935233721855,11972.633923338488,-4297.2468765941176,null,null,null,"Pre 1980 Construction","10,000 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","10000 ft2","psz-ac","ad-e&flr","pre198010000 ft2psz-acad-e&flr","base-roof","base-win","base-inf","40 fc","no-day","yes-occ","red-epd","high-eff",444.86,409.81,9.0102564609769897E-2,0.25997271850151399,-0.211846112901795,4341.4583999999995,-620.59999676025586,3720.8584032397439,"no",10000,704.17,3268.14,null,15800,86600,158,0,3778.0716416518485,-1200,186.04292016198721,2764.1145618138357,956.74384142590816,null,null,null,"Pre 1980 Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","10000 ft2","psz-ac","ad-e&flr","pre198010000 ft2psz-acad-e&flr","base-roof","eff-win","base-inf","base-lpd","yes-day","no-occ","base-epd","high-eff",505.98,366.34,7.1320482261366697E-2,0.15829923146022601,-8.3301298163645399E-2,2643.5447999999997,-244.02989822356761,2399.514901776432,"no",10000,704.17,3268.14,null,14655.9406,125279.31,146.559406,0,3504.5059216831633,0,119.97574508882161,3624.4816667719847,-1224.9667649955527,null,null,null,"Pre 1980 Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","10000 ft2","psz-ac","ad-e&flr","pre198010000 ft2psz-acad-e&flr","base-roof","eff-win","base-inf","25 fc","no-day","no-occ","red-epd","base-eff",444.03,407.27,9.3702710989347904E-2,0.261353428485877,-0.20433509773191,4364.5158000000001,-598.5965909566396,3765.9192090433608,"no",10000,704.17,3268.14,null,14455.9406,143279.31,144.559406,0,3456.6822300166841,-1900,188.29596045216806,1744.9781904688521,2020.9410185745087,null,null,null,{"$f":"IF(A24713=\"new90.1-2004\",\"New Construction\",IF(A24713=\"post1980\",\"Post 1980 Construction\",IF(A24713=\"pre1980\",\"Pre 1980 Construction\")))","v":"Pre 1980 Construction"},"10,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","10000 ft2","psz-ac","ad-e&flr","pre198010000 ft2psz-acad-e&flr","eff-roof","base-win","base-inf","40 fc","no-day","yes-occ","base-epd","base-eff",500.89,318.52999999999997,0.127646948282513,0.166766477026982,5.8077298400213001E-2,2784.9450000000002,170.13657085945636,2955.0815708594564,"no",10000,704.17,3268.14,null,40200,145700,402,0,9612.5620249622971,-1200,147.75407854297282,8560.316103505269,-5605.2345326458126,null,null,null,"Pre 1980 Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","10000 ft2","psz-ac","ad-e&flr","pre198010000 ft2psz-acad-e&flr","eff-roof","eff-win","base-inf","base-lpd","yes-day","no-occ","red-epd","base-eff",446.24,339.78,0.16319344852483,0.25767708021426,-4.7609190643757796E-3,4303.1219999999994,-13.947040686543625,4289.1749593134555,"no",10000,704.17,3268.14,null,42055.940600000002,187379.31,420.55940600000002,0,10056.351679990799,0,214.45874796567279,10270.810427956472,-5981.6354686430168,null,null,null,"Pre 1980 Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","10000 ft2","psz-ac","ad-e&flr","pre198010000 ft2psz-acad-e&flr","eff-roof","eff-win","red-inf","base-lpd","no-day","no-occ","red-epd","high-eff",499.04,215.01,0.239815245235246,0.16984396313670699,0.364195522961824,2836.3379999999993,1066.9052987296643,3903.2432987296634,"yes",10000,704.17,3268.14,null,42061.2408,215584.6102,420.61240800000002,0,10057.619055643652,0,195.16216493648318,10252.781220580135,-6349.5379218504713,null,null,null,"Pre 1980 Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","10000 ft2","psz-ac","ad-e&w&flr","pre198010000 ft2psz-acad-e&w&flr","base-roof","base-win","base-inf","40 fc","no-day","yes-occ","base-epd","base-eff",494.34,300.66000000000003,6.3312754498883406E-2,0.15354189140596899,-0.13576609247506799,2491.0326000000005,-311.33952936297595,2179.6930706370244,"no",10000,542.29,2451.0500000000002,null,10200,24200,102,0,2439.0082749904341,-1200,108.98465353185122,1347.9929285222852,831.70014211473926,null,null,null,"Pre 1980 Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","10000 ft2","psz-ac","ad-e&w&flr","pre198010000 ft2psz-acad-e&w&flr","base-roof","base-win","base-inf","25 fc","yes-day","yes-occ","base-epd","high-eff",417.7,332.97,0.11553702000963301,0.284772521018476,-0.257819582955576,4620.0918000000011,-591.23324649479991,4028.8585535052011,"no",10000,542.29,2451.0500000000002,null,21100,210100,211,0,5045.3994708135442,-1900,201.44292767526008,3346.8423984888041,682.01615501639708,null,null,null,"Pre 1980 Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","10000 ft2","psz-ac","ad-e&w&flr","pre198010000 ft2psz-acad-e&w&flr","base-roof","eff-win","base-inf","25 fc","no-day","no-occ","red-epd","high-eff",421.32,330.64,0.114015499802969,0.27857399702059898,-0.24901783016016901,4519.5281999999997,-571.04901991116753,3948.4791800888324,"no",10000,542.29,2451.0500000000002,null,17393.642200000002,197218.47,173.93642200000002,0,4159.1409076492964,-1900,197.42395900444163,2456.5648666537381,1491.9143134350943,null,null,null,"Pre 1980 Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","10000 ft2","psz-ac","ad-e&w&flr","pre198010000 ft2psz-acad-e&w&flr","eff-roof","base-win","base-inf","40 fc","no-day","yes-occ","base-epd","high-eff",479.56,241.47,0.150455361443145,0.17884967723155401,8.7828649138712703E-2,2901.6210000000001,201.40912792680024,3103.0301279268006,"no",10000,542.29,2451.0500000000002,null,44300,206600,443,0,10592.947704125119,-1200,155.15150639634004,9548.0992105214591,-6445.0690825946585,null,null,null,"Pre 1980 Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","10000 ft2","psz-ac","ad-e&w&flr","pre198010000 ft2psz-acad-e&w&flr","eff-roof","base-win","base-inf","25 fc","yes-day","yes-occ","red-epd","base-eff",359.32,303.32,0.219263102587679,0.38473656273008999,-0.145814445451798,6241.8882000000012,-334.38246614943967,5907.5057338505612,"yes",10000,542.29,2451.0500000000002,null,48500,272200,485,0,11597.245229121181,-1900,295.37528669252805,9992.6205158137091,-4085.1147819631478,null,null,null,"Pre 1980 Construction","10,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","10000 ft2","psz-ac","ad-e&w&flr","pre198010000 ft2psz-acad-e&w&flr","eff-roof","eff-win","base-inf","25 fc","no-day","no-occ","base-epd","base-eff",483.19,238.29,0.14994089058189899,0.17263403023920801,9.9841341795104399E-2,2800.7795999999998,228.95669897227231,3029.7362989722724,{"$f":"IF(P25287>0.2,\"yes\",\"no\")","v":"no"},{"$f":"IF(B25287=\"5500 ft2\",5500,IF(B25287=\"10000 ft2\",10000,25000))","v":10000},{"$f":"IF(B25287=\"5500 ft2\",IF(D25287=\"stand-alone\",642.39,IF(D25287=\"ad-e&flr\",522.37,402.25)),IF(B25287=\"10000 ft2\",IF(D25287=\"stand-alone\",866.06,IF(D25287=\"ad-e&flr\",704.17,542.29)),IF(B25287=\"25000 ft2\",IF(D25287=\"stand-alone\",1369.38,IF(D25287=\"ad-e&flr\",1113.42,857.45)))))","v":542.29},{"$f":"IF(B25287=\"5500 ft2\",IF(D25287=\"stand-alone\",3030.15,IF(D25287=\"ad-e&flr\",2424.14,1818.13)),IF(B25287=\"10000 ft2\",IF(D25287=\"stand-alone\",4085.12,IF(D25287=\"ad-e&flr\",3268.14,2451.05)),IF(B25287=\"25000 ft2\",IF(D25287=\"stand-alone\",6459.2,IF(D25287=\"ad-e&flr\",5167.32,3875.54)))))","v":2451.0500000000002},null,{"$f":"SUM(IF(F25287=\"eff-roof\",W25287*IF(AND(W$4=\"no\",X$4=\"no\"),$C$4,$C$3)),IF(G25287=\"eff-win\",X25287*IF(W$4=\"no\",$D$4,$D$3),0),IF(H25287=\"red-inf\",Y25287*IF(W$4=\"no\",$F$4,$F$3),0),IF(I25287=\"25 fc\",W25287*IF(W$4=\"no\",$H$4,$H$3),0),IF(I25287=\"40 fc\",W25287*IF(W$4=\"no\",$G$4,$G$3),0),IF(J25287=\"yes-day\",W25287*IF(W$4=\"no\",$I$4,$I$3),0),IF(K25287=\"yes-occ\",W25287*IF(W$4=\"no\",$J$4,$J$3),0),IF(L25287=\"red-epd\",W25287*IF(W$4=\"no\",$K$4,$K$3),0),IF(AND(M25287=\"high-eff\",C25287=\"psz-ac\"),W25287*IF(AND(W$4=\"no\",Y$4=\"no\"),$L$4,$L$3),0),IF(AND(M25287=\"high-eff\",C25287=\"ptac\"),W25287*IF(AND(W$4=\"no\",Y$4=\"no\"),$M$4,$M$3),0),IF(AND(M25287=\"high-eff\",C25287=\"pthp\"),W25287*IF(AND(W$4=\"no\",Y$4=\"no\"),$N$4,$N$3),0))","v":41793.642200000002},{"$f":"SUM(IF(F25287=\"eff-roof\",W25287*$C$4),IF(G25287=\"eff-win\",X25287*$D$4,0),IF(H25287=\"red-inf\",Y25287*$F$4,0),IF(I25287=\"25 fc\",W25287*$H$4,0),IF(I25287=\"40 fc\",W25287*$G$4,0),IF(J25287=\"yes-day\",W25287*$I$4,0),IF(K25287=\"yes-occ\",W25287*$J$4,0),IF(L25287=\"red-epd\",W25287*$K$4,0),IF(AND(M25287=\"high-eff\",C25287=\"psz-ac\"),W25287*$L$4,0),IF(AND(M25287=\"high-eff\",C25287=\"ptac\"),W25287*$M$4,0),IF(AND(M25287=\"high-eff\",C25287=\"pthp\"),W25287*$N$4,0))","v":256318.47},417.93642200000005,0,{"$f":"-PMT($AE$3,$AE$4,AA25287+AC25287-AD25287)","v":9993.6312909597455},{"$f":"SUM(IF(F25287=\"eff-roof\",($C$5*W25287),0),IF(G25287=\"eff-win\",($D$5*X25287),0),IF(H25287=\"red-inf\",$F$5*(Y25287-X25287),0),IF(I25287=\"25 fc\",($H$5*W25287),0),IF(I25287=\"40 fc\",($G$5*W25287),0),IF(J25287=\"yes-day\",($I$5*W25287),0),IF(K25287=\"yes-occ\",($J$5*W25287),0),IF(L25287=\"red-epd\",($K$5*W25287),0),IF(M25287=\"high-eff\",($L$5*W25287),0))","v":-1900},{"$f":"0.05*U25287","v":151.48681494861361},8245.1181059083592,{"$f":"U25287-AH25287","v":-5215.3818069360868},null,null,null,"Pre 1980 Construction",{"$f":"IF(B25287=\"5500 ft2\",\"5,500 SF\",IF(B25287=\"10000 ft2\",\"10,000 SF\",IF(B25287=\"25000 ft2\",\"25,000 SF\")))","v":"10,000 SF"},"Packaged Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration",{"$f":"IF(I25287=\"base-lpd\",\"Baseline Lighting Levels\",IF(I25287=\"40 fc\",\"Reduce Lighting Levels to 40 fc\",IF(I25287=\"25 fc\",\"Reduce Lighting Levels to 25 fc\")))","v":"Reduce Lighting Levels to 25 fc"},"No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","10000 ft2","ptac","stand-alone","pre198010000 ft2ptacstand-alone","base-roof","base-win","base-inf","40 fc","no-day","yes-occ","red-epd","base-eff",324.48,334.96,0.117468606241452,0.29067657667504598,-0.15595127169824299,3693.9065999999993,-391.4700426241759,3302.4365573758232,"no",10000,866.06,4085.12,null,11700,25700,117,0,2797.6859624890271,-1200,165.12182786879117,1762.8077903578182,1539.628767018005,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","10000 ft2","ptac","stand-alone","pre198010000 ft2ptacstand-alone","base-roof","base-win","base-inf","25 fc","yes-day","yes-occ","red-epd","high-eff",257.91000000000003,313.92,0.23471341539226701,0.43620067766969101,-8.3341960865514195E-2,5543.2212,-209.20561029816028,5334.0155897018394,"yes",10000,866.06,4085.12,null,25100,179200,251,0,6001.873304143126,-1900,266.70077948509197,4368.5740836282184,965.44150607362099,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","10000 ft2","ptac","stand-alone","pre198010000 ft2ptacstand-alone","base-roof","eff-win","base-inf","25 fc","no-day","no-occ","base-epd","high-eff",371.81,274.22000000000003,0.13542210617928599,0.18721171712755499,5.3663250163923003E-2,{"$f":"277.8*($N$25351-N25480)*$S$3","v":2379.0791999999997},{"$f":"277.78*($O$25351-O25480)*$S$4","v":134.70588986071959},{"$f":"SUM(S25480:T25480)","v":2513.7850898607194},"no",10000,866.06,4085.12,null,20718.310799999999,177240.58,{"$f":"MIN(0.01*AA25480,500)","v":207.183108},{"$f":"IF(V25480=\"yes\",0,0)","v":0},4954.1305377474191,-1900,125.68925449303597,{"$f":"SUM(AE25480:AG25480)","v":3179.8197922404552},-666.03470237973579,null,null,null,"Pre 1980 Construction","10,000 SF",{"$f":"IF(C25480=\"psz-ac\",\"Packaged Air Conditioner\",IF(C25480=\"ptac\",\"Split System Air Conditioner\",IF(C25480=\"pthp\",\"Split System Heat Pump\")))","v":"Split System Air Conditioner"},{"$f":"IF(D25480=\"stand-alone\",\"Stand Alone\",IF(D25480=\"ad-e&flr\",\"Above Ground, 1 Side Attached\",IF(D25480=\"ad-e&w&flr\",\"Above Ground, 2 Sides Attached\")))","v":"Stand Alone"},{"$f":"IF(F25480=\"base-roof\",\"Baseline Roof Insulation\",IF(F25480=\"eff-roof\",\"Increased Roof Insulation\"))","v":"Baseline Roof Insulation"},{"$f":"IF(G25480=\"base-win\",\"Baseline Windows\",IF(G25480=\"eff-win\",\"Replace Windows\"))","v":"Replace Windows"},{"$f":"IF(H25480=\"base-inf\",\"Baseline Infiltration\",IF(H25480=\"red-inf\",\"Reduce Infiltration\"))","v":"Baseline Infiltration"},"Reduce Lighting Levels to 25 fc",{"$f":"IF(J25480=\"no-day\",\"No Daylighting Sensors\",IF(J25480=\"yes-day\",\"Install Daylighting Sensors\"))","v":"No Daylighting Sensors"},{"$f":"IF(K25480=\"no-occ\",\"No Occupancy Sensors\",IF(K25480=\"yes-occ\",\"Install Occupancy Sensors\"))","v":"No Occupancy Sensors"},{"$f":"IF(L25480=\"base-epd\",\"No Plug Load Control\",IF(L25480=\"red-epd\",\"Install Plug Load Controls\"))","v":"No Plug Load Control"},{"$f":"IF(M25480=\"base-eff\",\"Baseline HVAC Equipment\",IF(M25480=\"high-eff\",\"Install High Efficiency HVAC Equipment\"))","v":"Install High Efficiency HVAC Equipment"}]
["pre1980","10000 ft2","ptac","stand-alone","pre198010000 ft2ptacstand-alone","base-roof","eff-win","red-inf","base-lpd","yes-day","no-occ","red-epd","base-eff",322.08999999999997,282.69,0.19062538853661601,0.29590119138703702,2.44331711357283E-2,3760.3008000000009,61.332327988031857,3821.6331279880328,"no",10000,866.06,4085.12,null,14974.912399999999,74597.181599999996,149.74912399999999,0,3580.7779667506725,0,191.08165639940165,3771.8596231500742,49.773504837958626,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","10000 ft2","ptac","stand-alone","pre198010000 ft2ptacstand-alone","eff-roof","base-win","red-inf","base-lpd","no-day","no-occ","base-epd","base-eff",451.34,211.08,0.11348999129678,1.33566510001093E-2,0.27156020291955701,169.73580000000038,681.67244200257562,851.408242002576,"no",10000,866.06,4085.12,null,31756.601600000002,123256.60159999999,317.56601600000005,0,7593.5896164680844,0,42.570412100128806,7636.1600285682134,-6784.7517865656373,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","10000 ft2","ptac","stand-alone","pre198010000 ft2ptacstand-alone","eff-roof","eff-win","base-inf","25 fc","no-day","no-occ","red-epd","base-eff",314.49,301.52,0.175593683948775,0.31251502896491401,-4.0549401249266703E-2,3971.4287999999997,-101.78740873719998,3869.6413912627995,"no",10000,866.06,4085.12,null,45618.310799999999,271740.57999999996,456.183108,0,10908.180150224065,-1900,193.48206956313999,9201.6622197872057,-5332.0208285244062,null,null,null,{"$f":"IF(A25673=\"new90.1-2004\",\"New Construction\",IF(A25673=\"post1980\",\"Post 1980 Construction\",IF(A25673=\"pre1980\",\"Pre 1980 Construction\")))","v":"Pre 1980 Construction"},"10,000 SF","Split System Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","10000 ft2","ptac","stand-alone","pre198010000 ft2ptacstand-alone","eff-roof","eff-win","red-inf","base-lpd","yes-day","no-occ","red-epd","high-eff",313.43,218.62,0.287964689792366,0.31483222210077599,0.24553956586258099,4000.8755999999994,616.35524524695973,4617.2308452469588,"yes",10000,866.06,4085.12,null,51574.912400000001,224597.18159999998,500,0,12328.784921665887,0,230.86154226234794,12559.646463928235,-7942.4156186812761,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","10000 ft2","ptac","ad-e&flr","pre198010000 ft2ptacad-e&flr","base-roof","base-win","base-inf","25 fc","yes-day","yes-occ","base-epd","high-eff",326.27999999999997,312.7,0.16868314498096301,0.31860329128727799,-7.9057248352255E-2,4238.1168000000007,-198.46379014206369,4039.6530098579369,"no",10000,704.17,3268.14,null,23600,177700,236,0,5643.1956166445334,-1900,201.98265049289685,3945.1782671374303,94.474742720506583,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","10000 ft2","ptac","ad-e&flr","pre198010000 ft2ptacad-e&flr","base-roof","base-win","red-inf","40 fc","no-day","yes-occ","red-epd","base-eff",340.36,303.54000000000002,0.16227714993654399,0.28919889733522702,-4.7448152110148703E-2,3846.9743999999992,-119.11292511799998,3727.8614748819991,"no",10000,704.17,3268.14,null,13105.3002,27105.300200000001,131.05300199999999,0,3133.7191798072345,-1200,186.39307374409998,2120.1122535513346,1607.7492213306646,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","10000 ft2","ptac","ad-e&flr","pre198010000 ft2ptacad-e&flr","base-roof","eff-win","red-inf","base-lpd","yes-day","yes-occ","base-epd","base-eff",371.84,286.73,0.143192119417417,0.22345668699356799,1.05593705786949E-2,2972.4600000000005,26.508040062624019,2998.9680400626244,"no",10000,704.17,3268.14,null,15561.2408,69384.610199999996,155.61240799999999,0,3720.9799098351723,0,149.94840200313124,3870.9283118383037,-871.9602717756793,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","10000 ft2","ptac","ad-e&flr","pre198010000 ft2ptacad-e&flr","eff-roof","base-win","base-inf","25 fc","yes-day","yes-occ","red-epd","base-eff",268.52999999999997,340.85,0.20719163594609299,0.43920725085623602,-0.17619655612685001,5842.4118000000008,-442.32043320182402,5400.0913667981768,"yes",10000,704.17,3268.14,null,48500,272200,485,0,11597.245229121181,-1900,270.00456833990887,9967.2497974610906,-4567.1584306629138,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","10000 ft2","ptac","ad-e&flr","pre198010000 ft2ptacad-e&flr","eff-roof","base-win","red-inf","40 fc","no-day","yes-occ","red-epd","high-eff",329.38,223.81,0.28029250015108498,0.31212931250522102,0.227682114634736,4151.9988000000003,571.56878540259208,4723.5675854025922,"yes",10000,704.17,3268.14,null,49705.300199999998,177105.3002,497.05300199999999,0,11885.454754772909,-1200,236.17837927012962,10921.633134043039,-6198.0655486404467,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","10000 ft2","ptac","ad-e&flr","pre198010000 ft2ptacad-e&flr","eff-roof","eff-win","red-inf","base-lpd","yes-day","no-occ","base-epd","high-eff",387.76,197.71,0.23830301565238399,0.190209673377329,0.317747334276545,2530.2024000000001,797.66677417203198,3327.8691741720322,"yes",10000,704.17,3268.14,null,48561.2408,215784.6102,485.61240800000002,0,11611.889034804224,0,166.39345870860163,11778.282493512826,-8450.4133193407943,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","10000 ft2","ptac","ad-e&w&flr","pre198010000 ft2ptacad-e&w&flr","base-roof","base-win","base-inf","25 fc","yes-day","yes-occ","red-epd","high-eff",265.93,292.62,0.22162812977395699,0.44222581118778398,-0.215098413753011,5857.1352000000006,-448.73087426272008,5408.4043257372805,"yes",10000,542.29,2451.0500000000002,null,25100,179200,251,0,6001.873304143126,-1900,270.42021628686405,4372.2935204299902,1036.1108053072903,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","10000 ft2","ptac","ad-e&w&flr","pre198010000 ft2ptacad-e&w&flr","base-roof","base-win","red-inf","40 fc","yes-day","no-occ","base-epd","base-eff",367.88,251.77,0.13649309960902101,0.228391048094469,-4.5469645378290902E-2,3024.9641999999999,-94.857202184880137,2930.1069978151199,"no",10000,542.29,2451.0500000000002,null,13153.951499999999,55753.951499999996,131.53951499999999,0,3145.3526036591011,-1200,146.50534989075601,2091.857953549857,838.24904426526291,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","10000 ft2","ptac","ad-e&w&flr","pre198010000 ft2ptacad-e&w&flr","base-roof","eff-win","red-inf","base-lpd","yes-day","no-occ","red-epd","base-eff",337.66,261.13,0.165557598197872,0.29177590871908898,-8.4336849098912106E-2,3864.4757999999988,-175.94061884702401,3688.5351811529749,"no",10000,542.29,2451.0500000000002,null,11947.593699999999,59972.421499999997,119.475937,0,2856.8901863258402,0,184.42675905764875,3041.3169453834889,647.218235769486,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","10000 ft2","ptac","ad-e&w&flr","pre198010000 ft2ptacad-e&w&flr","base-roof","eff-win","red-inf","25 fc","no-day","no-occ","red-epd","high-eff",326.86,230.53,0.22325936666580401,0.31442834070935699,4.2729009218503401E-2,4164.4997999999996,89.139781779215923,4253.6395817792154,"yes",10000,542.29,2451.0500000000002,null,20947.593699999998,165872.4215,209.47593699999999,0,5008.956311317399,-1900,212.68197908896079,3321.6382904063598,932.00129137285558,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","10000 ft2","ptac","ad-e&w&flr","pre198010000 ft2ptacad-e&w&flr","eff-roof","base-win","red-inf","40 fc","yes-day","no-occ","base-epd","high-eff",357.89,176.08,0.25589705082726999,0.24934454768546699,0.26883149240096299,3302.4864000000002,560.82696524649577,3863.3133652464958,"yes",10000,542.29,2451.0500000000002,null,49753.951499999996,205753.9515,497.53951499999999,0,11897.088178624774,-1200,193.1656682623248,10890.253846887099,-7026.9404816406031,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","10000 ft2","ptac","ad-e&w&flr","pre198010000 ft2ptacad-e&w&flr","eff-roof","eff-win","red-inf","base-lpd","yes-day","no-occ","red-epd","high-eff",327.62,184.25,0.286709303228813,0.31283428068041202,0.234905738726019,4143.3869999999997,490.0522308309279,4633.439230830928,"yes",10000,542.29,2451.0500000000002,null,48547.593700000005,209972.4215,485.47593700000004,0,11608.625761291518,0,231.67196154154641,11840.297722833064,-7206.8584920021358,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","10000 ft2","ptac","ad-e&w&flr","pre198010000 ft2ptacad-e&w&flr","eff-roof","eff-win","red-inf","25 fc","no-day","yes-occ","base-epd","base-eff",362.37,199.37,0.21720048678180301,0.23994798330431899,0.17212025579270801,3178.0319999999997,359.07132699207989,3537.1033269920795,"yes",10000,542.29,2451.0500000000002,null,46447.593700000005,260972.4215,464.47593700000004,0,11106.476998793487,-1900,176.85516634960399,9383.3321651430906,-5846.2288381510116,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","10000 ft2","pthp","stand-alone","pre198010000 ft2pthpstand-alone","base-roof","base-win","red-inf","40 fc","no-day","yes-occ","red-epd","base-eff",539.26,0,0.20885920676025599,0.20886698061998399,0,3955.0386000000008,0,3955.0386000000008,"yes",10000,866.06,4085.12,null,13456.6016,27456.601600000002,134.56601599999999,0,3217.7218289852467,-1200,197.75193000000004,2215.4737589852466,1739.5648410147542,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Heat Pump","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","10000 ft2","pthp","stand-alone","pre198010000 ft2pthpstand-alone","base-roof","base-win","red-inf","25 fc","yes-day","yes-occ","red-epd","high-eff",462.12,0,0.32202535096088297,0.32203688217948201,0,6097.9877999999999,0,6097.9877999999999,"yes",10000,866.06,4085.12,null,35556.601600000002,185456.60159999999,355.56601600000005,0,8502.239758131187,-1900,304.89938999999998,6907.1391481311866,-809.15134813118675,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Heat Pump","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","10000 ft2","pthp","stand-alone","pre198010000 ft2pthpstand-alone","base-roof","eff-win","red-inf","25 fc","no-day","yes-occ","base-epd","high-eff",532.64,0,0.21857707509881399,0.21857899446914,0,4138.9422000000004,0,4138.9422000000004,"yes",10000,866.06,4085.12,null,34774.912400000001,187097.18160000001,347.74912399999999,0,8315.3234417321037,-1900,206.94711000000004,6622.2705517321037,-2483.3283517321033,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Heat Pump","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","10000 ft2","pthp","stand-alone","pre198010000 ft2pthpstand-alone","eff-roof","base-win","red-inf","40 fc","no-day","yes-occ","red-epd","high-eff",487.99,0,0.284094316478125,0.28408374044569601,0,5379.3191999999999,0,5379.3191999999999,"yes",10000,866.06,4085.12,null,58756.601600000002,181956.60159999999,500,0,14029.056654068278,-1200,268.96596,13098.022614068277,-7718.7034140682772,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Heat Pump","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","10000 ft2","pthp","stand-alone","pre198010000 ft2pthpstand-alone","eff-roof","eff-win","base-inf","base-lpd","no-day","no-occ","base-epd","base-eff",650.62,0,4.5495434101131202E-2,4.5493889646875903E-2,0,861.45779999999979,0,861.45779999999979,"no",10000,866.06,4085.12,null,36218.310799999999,158740.57999999999,362.183108,0,8660.4666418995494,0,43.072889999999994,8703.5395318995488,-7842.0817318995487,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Heat Pump","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","10000 ft2","pthp","stand-alone","pre198010000 ft2pthpstand-alone","eff-roof","eff-win","red-inf","25 fc","no-day","no-occ","red-epd","base-eff",504.65,0,0.25964290581981703,0.25964232794918102,0,4916.5044000000016,0,4916.5044000000016,"yes",10000,866.06,4085.12,null,47374.912400000001,273497.18160000001,473.74912399999999,0,11328.216016720286,-1900,245.82522000000009,9674.0412367202862,-4757.5368367202846,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Heat Pump","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","10000 ft2","pthp","ad-e&flr","pre198010000 ft2pthpad-e&flr","base-roof","base-win","red-inf","base-lpd","yes-day","yes-occ","base-epd","base-eff",597.51,0,0.15222176818739,0.15221555356914801,0,2980.2383999999997,0,2980.2383999999997,"no",10000,704.17,3268.14,null,10505.3002,39105.300199999998,105.05300199999999,0,2512.0111881430062,0,149.01192,2661.0231081430061,319.21529185699364,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","10000 ft2","pthp","ad-e&flr","pre198010000 ft2pthpad-e&flr","base-roof","eff-win","base-inf","base-lpd","no-day","no-occ","base-epd","base-eff",699.9,0,6.9335512700525797E-3,6.9382369216362096E-3,0,135.84419999999963,0,135.84419999999963,"no",10000,704.17,3268.14,null,5055.9405999999999,30279.309999999998,50.559406000000003,0,1208.9687216921666,0,6.7922099999999821,1215.7609316921667,-1079.9167316921671,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","10000 ft2","pthp","ad-e&flr","pre198010000 ft2pthpad-e&flr","base-roof","eff-win","red-inf","25 fc","no-day","no-occ","red-epd","base-eff",564.53,0,0.19900346677563499,0.19900963407539801,0,3896.4227999999998,0,3896.4227999999998,"no",10000,704.17,3268.14,null,15861.2408,144684.6102,158.61240799999999,0,3792.7154473348915,-1900,194.82114000000001,2087.5365873348915,1808.8862126651084,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","10000 ft2","pthp","ad-e&flr","pre198010000 ft2pthpad-e&flr","eff-roof","base-win","base-inf","base-lpd","yes-day","no-occ","red-epd","high-eff",541.04,0,0.232339875828797,0.23233871082166299,0,4548.9750000000004,0,4548.9750000000004,"yes",10000,704.17,3268.14,null,52300,190100,500,0,12500.450098960873,0,227.44875000000002,12727.898848960873,-8178.9238489608724,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","10000 ft2","pthp","ad-e&flr","pre198010000 ft2pthpad-e&flr","eff-roof","eff-win","base-inf","base-lpd","no-day","no-occ","base-epd","high-eff",639.04,0,9.3286582391943304E-2,9.3290199917705999E-2,0,1826.5350000000003,0,1826.5350000000003,"no",10000,704.17,3268.14,null,50355.940600000002,184779.31,500,0,12040.192191401862,0,91.326750000000018,12131.518941401862,-10304.983941401862,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","10000 ft2","pthp","ad-e&flr","pre198010000 ft2pthpad-e&flr","eff-roof","eff-win","red-inf","25 fc","no-day","no-occ","red-epd","high-eff",503.13,0,0.28612103396912802,0.28612778274379602,0,5602.1147999999994,0,5602.1147999999994,"yes",10000,704.17,3268.14,null,61161.2408,299184.6102,500,0,14598.357266295647,-1900,280.10573999999997,12978.463006295646,-7376.3482062956464,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","10000 ft2","pthp","ad-e&w&flr","pre198010000 ft2pthpad-e&w&flr","base-roof","base-win","base-inf","base-lpd","yes-day","yes-occ","base-epd","base-eff",593.32000000000005,0,0.11307391050745801,0.113071035637407,0,2101.2791999999999,0,2101.2791999999999,"no",10000,542.29,2451.0500000000002,null,9100,37700,91,0,2175.9779708247988,0,105.06396000000001,2281.0419308247988,-179.76273082479884,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","10000 ft2","pthp","ad-e&w&flr","pre198010000 ft2pthpad-e&w&flr","base-roof","base-win","red-inf","25 fc","yes-day","yes-occ","red-epd","base-eff",494.83,0,0.26028386523345298,0.26029956948098498,0,4837.3314000000018,0,4837.3314000000018,"yes",10000,542.29,2451.0500000000002,null,19553.951499999999,151753.9515,195.53951499999999,0,4675.7107369864325,-1900,241.86657000000011,3017.5773069864326,1819.7540930135692,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","10000 ft2","pthp","ad-e&w&flr","pre198010000 ft2pthpad-e&w&flr","base-roof","eff-win","base-inf","40 fc","no-day","yes-occ","red-epd","high-eff",535.51,0,0.199483376385301,0.19948875867017499,0,3707.2410000000013,0,3707.2410000000013,"no",10000,542.29,2451.0500000000002,null,30893.642200000002,82018.47,308.93642200000005,0,7387.2400951366344,-1200,185.36205000000007,6372.6021451366341,-2665.3611451366328,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","10000 ft2","pthp","ad-e&w&flr","pre198010000 ft2pthpad-e&w&flr","eff-roof","base-win","base-inf","base-lpd","yes-day","yes-occ","base-epd","high-eff",532.21,0,0.20441352109546401,0.20442178904568301,0,3798.9150000000004,0,3798.9150000000004,"yes",10000,542.29,2451.0500000000002,null,54400,192200,500,0,12997.627091533179,0,189.94575000000003,13187.57284153318,-9388.6578415331787,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","10000 ft2","pthp","ad-e&w&flr","pre198010000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","25 fc","yes-day","yes-occ","red-epd","high-eff",433.87,0,0.35142904757936799,0.35142609423582899,0,6530.8002000000015,0,6530.8002000000015,"yes",10000,542.29,2451.0500000000002,null,64853.951499999996,306253.95149999997,500,0,15472.610028326873,-1900,326.54001000000011,13899.150038326874,-7368.3498383268725,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","10000 ft2","pthp","ad-e&w&flr","pre198010000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","40 fc","yes-day","no-occ","base-epd","base-eff",552.04,0,0.174777101908174,0.17477876106194701,0,3248.0376000000024,0,3248.0376000000024,"no",10000,542.29,2451.0500000000002,null,45993.642200000002,199518.47,459.93642200000005,0,10997.928815955805,-1200,162.40188000000012,9960.3306959558049,-6712.2930959558025,null,null,null,"Pre 1980 Construction","10,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","psz-ac","stand-alone","pre198025000 ft2psz-acstand-alone","base-roof","base-win","base-inf","base-lpd","yes-day","yes-occ","red-epd","base-eff",930.07,880.96,0.119980588222017,0.29731261191154401,-0.19962960945585301,10931.985599999998,-1269.9603507126401,9662.0252492873587,"no",25000,1369.38,6459.2,null,26500,98000,265,0,6336.63914580848,0,483.10126246436795,6819.7404082728481,2842.2848410145107,null,null,null,"Pre 1980 Construction","25,000 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","psz-ac","stand-alone","pre198025000 ft2psz-acstand-alone","base-roof","eff-win","base-inf","base-lpd","no-day","no-occ","base-epd","base-eff",1317.21,723.64,8.3064352301197401E-3,4.8202237853110699E-3,1.4597744975216599E-2,177.23639999999673,92.864767801088234,270.10116780108496,"no",25000,1369.38,6459.2,null,9832.1484,58883.340000000004,98.321483999999998,0,2351.0481675033288,0,13.505058390054248,2364.5532258933831,-2094.4520580922981,null,null,null,"Pre 1980 Construction","25,000 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","psz-ac","stand-alone","pre198025000 ft2psz-acstand-alone","base-roof","eff-win","base-inf","40 fc","yes-day","no-occ","base-epd","high-eff",1039.56,803.44,0.104439879917838,0.214590620962685,-9.4068304373876602E-2,7890.3534,-598.42333579283229,7291.9300642071676,"no",25000,1369.38,6459.2,null,50332.148399999998,347883.33999999997,500,0,12034.559365476776,-3000,364.59650321035838,9399.155868687134,-2107.2258044799664,null,null,null,"Pre 1980 Construction","25,000 SF","Packaged Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","psz-ac","stand-alone","pre198025000 ft2psz-acstand-alone","eff-roof","base-win","base-inf","base-lpd","yes-day","no-occ","red-epd","high-eff",948.68,752.17,0.17352098052050699,0.28325236666943698,-2.4252410261996801E-2,10414.9998,-154.28372337102351,10260.716076628976,"no",25000,1369.38,6459.2,null,102750,545000,500,0,24444.535468138449,0,513.03580383144879,24957.571271969897,-14696.855195340921,null,null,null,"Pre 1980 Construction","25,000 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","psz-ac","stand-alone","pre198025000 ft2psz-acstand-alone","eff-roof","base-win","base-inf","25 fc","no-day","yes-occ","base-epd","base-eff",1018.25,718.84,0.15590366340879799,0.2306907728224,2.11340486954627E-2,8482.3451999999979,134.44600711500783,8616.7912071150058,"no",25000,1369.38,6459.2,null,103750,591500,500,0,24681.286416982406,-4750,430.83956035575034,20362.125977338157,-11745.334770223151,null,null,null,"Pre 1980 Construction","25,000 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","psz-ac","stand-alone","pre198025000 ft2psz-acstand-alone","eff-roof","eff-win","base-inf","40 fc","yes-day","no-occ","red-epd","base-eff",878.9,769.08,0.19920772859625799,0.335972619920066,-4.72792635764476E-2,12353.4882,-300.7709643706882,12052.717235629312,"no",25000,1369.38,6459.2,null,118832.14840000001,503133.34,500,0,28251.999361287755,-3000,602.63586178146568,25854.635223069221,-13801.917987439909,null,null,null,"Pre 1980 Construction","25,000 SF","Packaged Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","psz-ac","ad-e&flr","pre198025000 ft2psz-acad-e&flr","base-roof","base-win","base-inf","base-lpd","yes-day","yes-occ","base-epd","base-eff",1132.3900000000001,793.21,8.0108290431386397E-2,0.195425737509237,-0.15651882308342799,7640.8889999999992,-929.94709173944011,6710.9419082605591,"no",25000,1113.42,5167.32,null,22750,94250,227.5,0,5439.9449270619971,0,335.54709541302799,5775.4920224750249,935.44988578553421,null,null,null,"Pre 1980 Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","psz-ac","ad-e&flr","pre198025000 ft2psz-acad-e&flr","base-roof","base-win","base-inf","25 fc","no-day","yes-occ","base-epd","high-eff",1084,809.53,9.5430942659328902E-2,0.22980730972545901,-0.18031376665791801,8985.1632000000009,-1071.3233054067675,7913.8398945932331,"no",25000,1113.42,5167.32,null,39000,440000,390,0,9325.6198749634241,-4750,395.6919947296617,4971.311869693086,2942.5280249001471,null,null,null,"Pre 1980 Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","psz-ac","ad-e&flr","pre198025000 ft2psz-acad-e&flr","base-roof","eff-win","base-inf","40 fc","no-day","yes-occ","red-epd","high-eff",1005.75,852.54,0.11226255991478799,0.28540470641732502,-0.24302335753652299,11158.948200000003,-1443.9085351758713,9715.0396648241313,"no",25000,1113.42,5167.32,null,47494.355599999995,264377.06,474.94355599999994,0,11356.777090562571,-3000,485.75198324120657,8842.5290738037784,872.51059102035288,null,null,null,"Pre 1980 Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","psz-ac","ad-e&flr","pre198025000 ft2psz-acad-e&flr","base-roof","eff-win","red-inf","base-lpd","no-day","no-occ","base-epd","base-eff",1378.67,473.92,0.114992011361619,2.0441368726197898E-2,0.30901350129764099,799.23059999999953,1835.9849708733759,2635.2155708733753,"no",25000,1113.42,5167.32,null,10216.3032,50099.007600000004,102.163032,0,2442.906671040319,0,131.76077854366878,2574.6674495839879,60.548121289387382,null,null,null,"Pre 1980 Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","psz-ac","ad-e&flr","pre198025000 ft2psz-acad-e&flr","eff-roof","base-win","base-inf","25 fc","no-day","yes-occ","red-epd","base-eff",927.52,738.86,0.20394328066749501,0.34098789291195403,-7.72752456769603E-2,13332.177600000003,-459.12618409119995,12873.051415908803,"yes",25000,1113.42,5167.32,null,107500,595250,500,0,25569.10247514724,-4750,643.65257079544017,21462.755045942678,-8589.703630033875,null,null,null,"Pre 1980 Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","psz-ac","ad-e&flr","pre198025000 ft2psz-acad-e&flr","eff-roof","eff-win","base-inf","40 fc","yes-day","no-occ","base-epd","base-eff",1082.21,643.63,0.17553923309071501,0.23107912237821901,6.1572332546000703E-2,9034.8894000000018,365.82827838059211,9400.7176783805935,"no",25000,1113.42,5167.32,null,113244.3556,488377.06,500,0,26929.084113944329,-3000,470.03588391902969,24399.119997863359,-14998.402319482766,null,null,null,"Pre 1980 Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","psz-ac","ad-e&flr","pre198025000 ft2psz-acad-e&flr","eff-roof","eff-win","red-inf","base-lpd","no-day","no-occ","base-epd","high-eff",1322.33,345,0.20348837209302301,6.0471494344341598E-2,0.49698189134808901,2364.3558000000039,2952.7877567797436,5317.1435567797471,"yes",25000,1113.42,5167.32,null,95466.303199999995,506099.00760000001,500,0,22720.113339646763,0,265.85717783898735,22985.970517485752,-17668.826960706007,null,null,null,"Pre 1980 Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","psz-ac","ad-e&w&flr","pre198025000 ft2psz-acad-e&w&flr","base-roof","base-win","base-inf","25 fc","no-day","yes-occ","red-epd","high-eff",911.23,739.8,0.142136512840317,0.33970754470884901,-0.35857788224923798,13023.541799999999,-1691.4901642575039,11332.051635742495,"no",25000,857.45,3875.54,null,42750,443750,427.5,0,10222.314093709907,-4750,566.60258178712479,6038.916675497032,5293.1349602454629,null,null,null,"Pre 1980 Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","psz-ac","ad-e&w&flr","pre198025000 ft2psz-acad-e&w&flr","base-roof","eff-win","base-inf","40 fc","yes-day","no-occ","base-epd","high-eff",1066.69,642.94000000000005,0.111689032631782,0.227058635981566,-0.180702978660888,8704.8629999999976,-852.4154059353607,7852.4475940646371,"no",25000,857.45,3875.54,null,46656.491000000002,325870.34999999998,466.56491000000005,0,11156.428199119286,-3000,392.6223797032319,8549.0505788225182,-696.60298475788113,null,null,null,"Pre 1980 Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","psz-ac","ad-e&w&flr","pre198025000 ft2psz-acad-e&w&flr","base-roof","eff-win","red-inf","base-lpd","no-day","no-occ","red-epd","base-eff",1207.32,450.36,0.138685074338675,0.12515579258572199,0.17295331839717901,4798.1616000000013,815.85856637187146,5614.0201663718726,"no",25000,857.45,3875.54,null,11572.9732,42286.832199999997,115.72973200000001,0,2767.3115099061297,0,280.70100831859367,3048.0125182247234,2566.0076481471492,null,null,null,"Pre 1980 Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","psz-ac","ad-e&w&flr","pre198025000 ft2psz-acad-e&w&flr","eff-roof","base-win","base-inf","25 fc","no-day","yes-occ","base-epd","base-eff",1056.76,509.23,0.186317339254682,0.23425407959189601,6.4843721306056396E-2,8980.7183999999997,305.88199170302352,9286.600391703023,"no",25000,857.45,3875.54,null,103750,591500,500,0,24681.286416982406,-4750,464.33001958515115,20395.616436567558,-11109.016044864535,null,null,null,"Pre 1980 Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","psz-ac","ad-e&w&flr","pre198025000 ft2psz-acad-e&w&flr","eff-roof","base-win","red-inf","base-lpd","yes-day","yes-occ","base-epd","high-eff",1033.97,352.58,0.27956651863294102,0.25076809367844399,0.35251772137951298,9613.8245999999981,1662.9030622291837,11276.727662229181,"yes",25000,857.45,3875.54,null,109666.4822,551916.48219999997,500,0,26082.019191650779,0,563.8363831114591,26645.855574762238,-15369.127912533057,null,null,null,"Pre 1980 Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","psz-ac","ad-e&w&flr","pre198025000 ft2psz-acad-e&w&flr","eff-roof","eff-win","red-inf","base-lpd","no-day","no-occ","red-epd","high-eff",1160.1199999999999,316.35000000000002,0.23282728325931601,0.15935769977681799,0.41905094207955301,6109.3776000000025,1976.7547914673753,8086.1323914673776,"yes",25000,857.45,3875.54,null,96822.973199999993,498286.8322,500,0,23041.306249414891,0,404.30661957336889,23445.612868988261,-15359.480477520883,null,null,null,"Pre 1980 Construction","25,000 SF","Packaged Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","ptac","stand-alone","pre198025000 ft2ptacstand-alone","base-roof","base-win","base-inf","25 fc","no-day","yes-occ","base-epd","high-eff",808.2,557.54,0.16449275362318799,0.24899643175736,1.6831399512964699E-3,7443.9288000000015,8.1429926989764709,7452.0717926989782,"no",25000,1369.38,6459.2,null,45250,359000,452.5,0,10820.110239540896,-4750,372.60358963494895,6442.7138291758447,1009.3579635231335,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","ptac","stand-alone","pre198025000 ft2ptacstand-alone","base-roof","base-win","red-inf","base-lpd","yes-day","yes-occ","red-epd","base-eff",681.91,583.45000000000005,0.22590224495595301,0.36634887005649702,-4.4710643174330399E-2,10952.265000000005,-216.3090720142882,10735.955927985717,"yes",25000,1369.38,6459.2,null,29277.456000000002,100777.45600000001,292.77456000000001,0,7000.7801426145425,0,536.79779639928586,7537.5779390138287,3198.377988971888,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Air Conditioner","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","ptac","stand-alone","pre198025000 ft2ptacstand-alone","base-roof","eff-win","red-inf","base-lpd","no-day","yes-occ","base-epd","high-eff",958.14,425.61,0.15348110258596201,0.109667707404104,0.237913622690159,3278.5956000000028,1151.020680758448,4429.6162807584506,"no",25000,1369.38,6459.2,null,38109.604399999997,141910.796,381.09604399999995,0,9112.7098517854738,0,221.48081403792253,9334.1906658233966,-4904.574385064946,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","ptac","stand-alone","pre198025000 ft2ptacstand-alone","base-roof","eff-win","red-inf","40 fc","yes-day","no-occ","base-epd","base-eff",809.51,541.09,0.17375674907644201,0.24777914064823101,3.1138089098982899E-2,7407.537000000003,150.64536493105587,7558.1823649310591,"no",25000,1369.38,6459.2,null,42859.604400000004,198410.796,428.59604400000006,0,10248.522528864354,-3000,377.90911824655296,7626.4316471109069,-68.249282179847796,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Air Conditioner","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","ptac","stand-alone","pre198025000 ft2ptacstand-alone","eff-roof","base-win","red-inf","base-lpd","yes-day","yes-occ","red-epd","base-eff",668.03,514.16999999999996,0.27678317703893102,0.379246580434136,7.9340352385045207E-2,11337.851400000005,383.84681541662445,11721.698215416629,"yes",25000,1369.38,6459.2,null,104277.45600000001,404527.45600000001,500,0,24806.162125455841,0,586.08491077083147,25392.247036226672,-13670.548820810043,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Air Conditioner","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","ptac","stand-alone","pre198025000 ft2ptacstand-alone","eff-roof","eff-win","red-inf","base-lpd","no-day","no-occ","base-epd","base-eff",1056.77,392.09,0.113654447286161,1.8017766874814201E-2,0.29793367712362101,538.65420000000279,1441.3963353006563,1980.0505353006592,"no",25000,1369.38,6459.2,null,87609.604400000011,365410.79600000003,500,0,20860.032443965596,0,99.002526765032968,20959.03497073063,-18978.984435429971,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","ptac","stand-alone","pre198025000 ft2ptacstand-alone","eff-roof","eff-win","red-inf","40 fc","yes-day","no-occ","base-epd","high-eff",788.93,410.83,0.26604148905939201,0.26690269104965803,0.26437831256267003,7979.2494000000042,1279.0562468125602,9258.3056468125651,"yes",25000,1369.38,6459.2,null,134359.60440000001,573410.79600000009,500,0,31928.139302420535,-3000,462.91528234062827,29391.054584761165,-20132.7489379486,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Air Conditioner","Stand Alone","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","ptac","ad-e&flr","pre198025000 ft2ptacad-e&flr","base-roof","base-win","red-inf","base-lpd","yes-day","yes-occ","red-epd","high-eff",712.49,557.66,0.25331785909339199,0.37192902037182302,1.5847804602569598E-2,11720.937600000003,77.791568549792146,11798.729168549795,"yes",25000,1113.42,5167.32,null,45221.9476,171471.94760000001,452.21947599999999,0,10813.402392900371,0,589.93645842748981,11403.338851327861,395.39031722193431,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","ptac","ad-e&flr","pre198025000 ft2ptacad-e&flr","base-roof","eff-win","red-inf","base-lpd","no-day","no-occ","base-epd","high-eff",1113.8,403.91,0.10778263244128899,1.8168034484886499E-2,0.28718410278130702,572.54580000000362,1409.6906403237915,1982.2364403237953,"no",25000,1113.42,5167.32,null,26716.303200000002,121349.00760000001,267.16303200000004,0,6388.3612335248445,0,99.111822016189763,6487.4730555410342,-4505.236615217239,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","ptac","ad-e&flr","pre198025000 ft2ptacad-e&flr","base-roof","eff-win","red-inf","40 fc","yes-day","no-occ","red-epd","base-eff",713.68,642.39,0.20279901693063901,0.37088001692509798,-0.13368276154172001,11687.879400000005,-656.20393292279994,11031.675467077206,"yes",25000,1113.42,5167.32,null,44216.303200000002,190599.00760000001,442.16303200000004,0,10572.934254341764,-3000,551.58377335386035,8124.5180276956244,2907.1574393815818,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","ptac","ad-e&flr","pre198025000 ft2ptacad-e&flr","eff-roof","base-win","red-inf","base-lpd","yes-day","yes-occ","base-epd","base-eff",861.59,466.23,0.21941561987984701,0.240495059105614,0.17720245658619199,7578.9396000000024,869.82754989806369,8448.7671498980653,"yes",25000,1113.42,5167.32,null,99971.9476,400221.94760000001,500,0,23786.82892650022,0,422.4383574949033,24209.267283995123,-15760.500134097058,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","ptac","ad-e&flr","pre198025000 ft2ptacad-e&flr","eff-roof","base-win","red-inf","25 fc","no-day","yes-occ","base-epd","high-eff",837.24,409.94,0.26682140906608398,0.26195996156592399,0.27654242552590702,8255.3826000000026,1357.4542084356797,9612.8368084356825,"yes",25000,1113.42,5167.32,null,122471.9476,664971.94760000007,500,0,29113.725275489225,-4750,480.64184042178414,24844.367115911009,-15231.530307475326,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","ptac","ad-e&flr","pre198025000 ft2ptacad-e&flr","eff-roof","eff-win","red-inf","40 fc","yes-day","no-occ","red-epd","high-eff",688.29,459.48,0.32525942108137601,0.39326169550691598,0.18911478187208799,12393.213600000005,928.30116768326366,13321.514767683268,"yes",25000,1113.42,5167.32,null,135716.30319999999,565599.00760000001,500,0,32249.339030615985,-3000,666.0757383841634,29915.414769000148,-16593.900001316881,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Air Conditioner","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","ptac","ad-e&w&flr","pre198025000 ft2ptacad-e&w&flr","base-roof","base-win","red-inf","base-lpd","yes-day","yes-occ","base-epd","high-eff",852.49,442.86,0.19503500036082799,0.24727603440055099,7.0929573919063502E-2,7779.7889999999989,292.88785441742402,8072.6768544174229,"no",25000,857.45,3875.54,null,40916.482199999999,167166.4822,409.16482200000002,0,9783.8861440489,0,403.63384272087114,10187.51998676977,-2114.8431323523473,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","ptac","ad-e&w&flr","pre198025000 ft2ptacad-e&w&flr","base-roof","base-win","red-inf","25 fc","no-day","yes-occ","red-epd","base-eff",711.8,578.47,0.19819585768925499,0.37150122732971902,-0.21356494010531399,11688.157200000001,-881.86878378272002,10806.288416217281,"no",25000,857.45,3875.54,null,34166.482199999999,293166.48220000003,341.66482200000002,0,8169.836550305231,-4750,540.31442081086414,3960.1509711160952,6846.1374451011861,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","ptac","ad-e&w&flr","pre198025000 ft2ptacad-e&w&flr","base-roof","eff-win","red-inf","40 fc","yes-day","yes-occ","base-epd","base-eff",805.11,534.29999999999995,0.16765533665295501,0.289111201370371,-0.120901252438794,9096.0054,-499.23475451275146,8596.7706454872477,"no",25000,857.45,3875.54,null,47072.9732,184286.8322,470.72973200000001,0,11256.01678070617,-3000,429.83853227436242,8685.8553129805314,-89.084667493283632,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","ptac","ad-e&w&flr","pre198025000 ft2ptacad-e&w&flr","eff-roof","base-win","base-inf","base-lpd","no-day","no-occ","base-epd","high-eff",1105.07,318.83999999999997,0.115133145702533,2.42552139438784E-2,0.33110957266033098,{"$f":"277.8*($N$29575-N29768)*$S$3","v":763.11660000000074},{"$f":"277.78*($O$29575-O29768)*$S$4","v":1367.2431251908322},{"$f":"SUM(S29768:T29768)","v":2130.3597251908332},"no",25000,857.45,3875.54,null,91500,375000,{"$f":"MIN(0.01*AA29768,500)","v":500},{"$f":"IF(V29768=\"yes\",0,0)","v":0},21781.087293643945,0,106.51798625954166,{"$f":"SUM(AE29768:AG29768)","v":21887.605279903488},-19757.245554712656,null,null,null,"Pre 1980 Construction","25,000 SF",{"$f":"IF(C29768=\"psz-ac\",\"Packaged Air Conditioner\",IF(C29768=\"ptac\",\"Split System Air Conditioner\",IF(C29768=\"pthp\",\"Split System Heat Pump\")))","v":"Split System Air Conditioner"},{"$f":"IF(D29768=\"stand-alone\",\"Stand Alone\",IF(D29768=\"ad-e&flr\",\"Above Ground, 1 Side Attached\",IF(D29768=\"ad-e&w&flr\",\"Above Ground, 2 Sides Attached\")))","v":"Above Ground, 2 Sides Attached"},{"$f":"IF(F29768=\"base-roof\",\"Baseline Roof Insulation\",IF(F29768=\"eff-roof\",\"Increased Roof Insulation\"))","v":"Increased Roof Insulation"},{"$f":"IF(G29768=\"base-win\",\"Baseline Windows\",IF(G29768=\"eff-win\",\"Replace Windows\"))","v":"Baseline Windows"},{"$f":"IF(H29768=\"base-inf\",\"Baseline Infiltration\",IF(H29768=\"red-inf\",\"Reduce Infiltration\"))","v":"Baseline Infiltration"},"Baseline Lighting Levels",{"$f":"IF(J29768=\"no-day\",\"No Daylighting Sensors\",IF(J29768=\"yes-day\",\"Install Daylighting Sensors\"))","v":"No Daylighting Sensors"},{"$f":"IF(K29768=\"no-occ\",\"No Occupancy Sensors\",IF(K29768=\"yes-occ\",\"Install Occupancy Sensors\"))","v":"No Occupancy Sensors"},{"$f":"IF(L29768=\"base-epd\",\"No Plug Load Control\",IF(L29768=\"red-epd\",\"Install Plug Load Controls\"))","v":"No Plug Load Control"},{"$f":"IF(M29768=\"base-eff\",\"Baseline HVAC Equipment\",IF(M29768=\"high-eff\",\"Install High Efficiency HVAC Equipment\"))","v":"Install High Efficiency HVAC Equipment"}]
["pre1980","25000 ft2","ptac","ad-e&w&flr","pre198025000 ft2ptacad-e&w&flr","eff-roof","base-win","red-inf","25 fc","no-day","yes-occ","red-epd","high-eff",687.66,398.18,0.32523634264270801,0.39281614777403001,0.16466318417353701,12358.7664,679.93989036449602,13038.706290364496,"yes",25000,857.45,3875.54,null,125666.4822,668166.48219999997,500,0,29870.034373154078,-4750,651.93531451822491,25771.969687672303,-12733.263397307806,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","ptac","ad-e&w&flr","pre198025000 ft2ptacad-e&w&flr","eff-roof","eff-win","red-inf","40 fc","yes-day","no-occ","base-epd","high-eff",833.18,338.56,0.27184816338312801,0.26432620481395802,0.28973923259277901,8316.220800000001,1196.413533676144,9512.6343336761456,"yes",25000,857.45,3875.54,null,129572.97319999999,550286.83220000006,500,0,30794.89982405445,-3000,475.63171668380733,28270.531540738259,-18757.897207062113,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Air Conditioner","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","stand-alone","pre198025000 ft2pthpstand-alone","base-roof","base-win","base-inf","base-lpd","no-day","no-occ","red-epd","base-eff",1380.13,0,7.8328576746494599E-2,7.8328057592392197E-2,0,3258.3161999999993,0,3258.3161999999993,"no",25000,1369.38,6459.2,null,3750,3750,37.5,0,896.6942187464831,0,162.91580999999996,1059.6100287464831,2198.706171253516,null,null,null,{"$f":"IF(A29961=\"new90.1-2004\",\"New Construction\",IF(A29961=\"post1980\",\"Post 1980 Construction\",IF(A29961=\"pre1980\",\"Pre 1980 Construction\")))","v":"Pre 1980 Construction"},"25,000 SF","Split System Heat Pump","Stand Alone","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","stand-alone","pre198025000 ft2pthpstand-alone","base-roof","base-win","red-inf","25 fc","yes-day","no-occ","base-epd","base-eff",1175.21,0,0.21517868221863801,0.21517677071229199,0,8950.993800000002,0,8950.993800000002,"yes",25000,1369.38,6459.2,null,36277.455999999998,366777.45600000001,362.77456000000001,0,8674.6093509413095,-4750,447.54969000000011,4372.1590409413093,4578.8347590586927,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Stand Alone","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","stand-alone","pre198025000 ft2pthpstand-alone","base-roof","eff-win","red-inf","40 fc","yes-day","no-occ","red-epd","base-eff",1092.45,0,0.27044298300037201,0.27044516568497801,0,11250.066600000002,0,11250.066600000002,"yes",25000,1369.38,6459.2,null,46609.604400000004,202160.796,466.09604400000006,0,11145.216747610837,-3000,562.50333000000012,8707.7200776108366,2542.3465223891653,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Stand Alone","Baseline Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","stand-alone","pre198025000 ft2pthpstand-alone","eff-roof","base-win","base-inf","base-lpd","no-day","no-occ","red-epd","high-eff",1265.8399999999999,0,0.15464077428961401,0.15465266925779,0,6433.2924000000048,0,6433.2924000000048,"no",25000,1369.38,6459.2,null,117000,390000,500,0,27818.236489164821,0,321.66462000000024,28139.901109164821,-21706.608709164815,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Stand Alone","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","stand-alone","pre198025000 ft2pthpstand-alone","eff-roof","base-win","red-inf","25 fc","no-day","yes-occ","base-epd","high-eff",1107.79,0,0.26019047028167303,0.26020087884494703,0,10823.921400000005,0,10823.921400000005,"yes",25000,1369.38,6459.2,null,144777.45600000001,676777.45600000001,500,0,34394.575553636059,-4750,541.1960700000003,30185.771623636061,-19361.850223636058,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Stand Alone","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","stand-alone","pre198025000 ft2pthpstand-alone","eff-roof","eff-win","base-inf","base-lpd","yes-day","yes-occ","red-epd","base-eff",1116.0899999999999,0,0.25465318277701898,0.25465801178026198,0,10593.347400000006,0,10593.347400000006,"yes",25000,1369.38,6459.2,null,111332.14840000001,460633.34,500,0,26476.367244958088,0,529.66737000000035,27006.034614958087,-16412.687214958081,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Stand Alone","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&flr","pre198025000 ft2pthpad-e&flr","base-roof","base-win","base-inf","base-lpd","no-day","yes-occ","base-epd","base-eff",1486.22,0,5.0170699124239403E-2,5.0162649947913703E-2,0,2180.4522000000006,0,2180.4522000000006,"no",25000,1113.42,5167.32,null,9000,9000,90,0,2152.0661249915593,0,109.02261000000004,2261.0887349915592,-80.636534991558619,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&flr","pre198025000 ft2pthpad-e&flr","base-roof","base-win","red-inf","25 fc","no-day","yes-occ","red-epd","base-eff",1191.96,0,0.23823660382959799,0.23822305730774401,0,10354.995000000001,0,10354.995000000001,"yes",25000,1113.42,5167.32,null,34721.9476,293721.94760000001,347.21947599999999,0,8302.6585804102197,-4750,517.74975000000006,4070.4083304102196,6284.5866695897812,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Baseline Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&flr","pre198025000 ft2pthpad-e&flr","base-roof","eff-win","base-inf","base-lpd","yes-day","yes-occ","red-epd","high-eff",1186.8399999999999,0,0.24150215229330599,0.24149522914789301,0,10497.228600000004,0,10497.228600000004,"yes",25000,1113.42,5167.32,null,72744.35560000001,228377.06,500,0,17340.670685764118,0,524.86143000000027,17865.532115764119,-7368.3035157641152,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&flr","pre198025000 ft2pthpad-e&flr","eff-roof","base-win","base-inf","base-lpd","no-day","yes-occ","base-epd","high-eff",1344.38,0,0.14081935579634899,0.14081203545705001,0,6120.7673999999988,0,6120.7673999999988,"no",25000,1113.42,5167.32,null,122250,395250,500,0,29061.178970595593,0,306.03836999999993,29367.217340595591,-23246.449940595594,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&flr","pre198025000 ft2pthpad-e&flr","eff-roof","base-win","base-inf","40 fc","yes-day","no-occ","red-epd","base-eff",1174.8499999999999,0,0.24916134778091101,0.24915799093761801,0,10830.310800000005,0,10830.310800000005,"yes",25000,1113.42,5167.32,null,109000,444250,500,0,25924.228898413174,-3000,541.51554000000021,23465.744438413174,-12635.433638413169,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&flr","pre198025000 ft2pthpad-e&flr","eff-roof","eff-win","base-inf","40 fc","no-day","no-occ","base-epd","base-eff",1384.29,0,0.115303547573104,0.115305711601511,0,5012.0676000000021,0,5012.0676000000021,"no",25000,1113.42,5167.32,null,99494.355599999995,403127.06,500,0,23673.758567339937,-3000,250.60338000000013,20924.361947339938,-15912.294347339935,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 1 Side Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","base-roof","base-win","base-inf","base-lpd","no-day","no-occ","red-epd","base-eff",1389.4,0,7.3805137097648105E-2,7.38136028210888E-2,0,3076.0794000000005,0,3076.0794000000005,"no",25000,857.45,3875.54,null,3750,3750,37.5,0,896.6942187464831,0,153.80397000000005,1050.4981887464833,2025.5812112535173,null,null,null,{"$f":"IF(A30729=\"new90.1-2004\",\"New Construction\",IF(A30729=\"post1980\",\"Post 1980 Construction\",IF(A30729=\"pre1980\",\"Pre 1980 Construction\")))","v":"Pre 1980 Construction"},"25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","base-roof","base-win","base-inf","40 fc","yes-day","no-occ","red-epd","high-eff",1127.6500000000001,0,0.24829305299664001,0.248298480798331,0,10347.494400000001,0,10347.494400000001,"yes",25000,857.45,3875.54,null,72250,223000,500,0,17223.631528397793,-3000,517.37472000000014,14741.006248397793,-4393.5118483977913,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","base-roof","eff-win","base-inf","40 fc","no-day","no-occ","base-epd","high-eff",1346.18,0,0.10261809286411,0.102624439215268,0,4276.7310000000016,0,4276.7310000000016,"no",25000,857.45,3875.54,null,60906.491000000002,170870.35,500,0,14538.04500942784,-3000,213.8365500000001,11751.88155942784,-7475.1505594278387,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Baseline Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","base-inf","base-lpd","no-day","no-occ","red-epd","high-eff",1250.81,0,0.166204771710353,0.166198929426116,0,6926.1096000000052,0,6926.1096000000052,"no",25000,857.45,3875.54,null,117000,390000,500,0,27818.236489164821,0,346.30548000000027,28164.54196916482,-21238.432369164817,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","base-inf","40 fc","yes-day","yes-occ","base-epd","base-eff",1176.51,0,0.21573332920466301,0.215727970242579,0,8990.1636000000053,0,8990.1636000000053,"yes",25000,857.45,3875.54,null,114250,449500,500,0,27167.171379843941,-3000,449.50818000000027,24616.679559843942,-15626.515959843937,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","40 fc","no-day","no-occ","red-epd","high-eff",1112.6300000000001,0,0.25831023858551799,0.25831094638464702,0,10764.75,0,10764.75,"yes",25000,857.45,3875.54,null,135166.4822,443166.48220000003,500,0,32119.168387171652,-3000,538.23750000000007,29657.405887171652,-18892.655887171652,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","40 fc","no-day","yes-occ","base-epd","base-eff",1207.8699999999999,0,0.194816454814287,0.19482311533000499,0,8118.982800000007,0,8118.982800000007,"no",25000,857.45,3875.54,null,102166.4822,365916.48220000003,500,0,24306.387075321109,-3000,405.9491400000004,21712.336215321109,-13593.353415321102,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","40 fc","no-day","yes-occ","base-epd","high-eff",1162.81,0,0.22485252906841699,0.224860512088952,0,9370.7496000000046,0,9370.7496000000046,"yes",25000,857.45,3875.54,null,140416.4822,448416.48220000003,500,0,33362.110868602424,-3000,468.53748000000024,30830.648348602423,-21459.89874860242,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","40 fc","no-day","yes-occ","red-epd","base-eff",1097.8800000000001,0,0.26814163402436902,0.26814342756961101,0,11174.505000000001,0,11174.505000000001,"yes",25000,857.45,3875.54,null,105916.4822,369666.48220000003,500,0,25194.203133485946,-3000,558.72525000000007,22752.928383485945,-11578.423383485944,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","40 fc","no-day","yes-occ","red-epd","high-eff",1050.6199999999999,0,0.29964854696620202,0.29964736389512903,0,12487.387800000008,0,12487.387800000008,"yes",25000,857.45,3875.54,null,144166.4822,452166.48220000003,500,0,34249.926926767257,-3000,624.36939000000041,31874.296316767257,-19386.908516767249,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","40 fc","yes-day","no-occ","base-epd","base-eff",1157.32,0,0.228521884531422,0.22852019491644099,0,9523.2618000000057,0,9523.2618000000057,"yes",25000,857.45,3875.54,null,106916.4822,442166.48220000003,500,0,25430.954082329903,-3000,476.1630900000003,22907.117172329905,-13383.855372329899,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","40 fc","yes-day","no-occ","base-epd","high-eff",1110.7,0,0.25959528712319402,0.25959750154986599,0,10818.365400000002,0,10818.365400000002,"yes",25000,857.45,3875.54,null,145166.4822,524666.48219999997,500,0,34486.677875611218,-3000,540.91827000000012,32027.59614561122,-21209.230745611218,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","40 fc","yes-day","no-occ","red-epd","base-eff",1048.8599999999999,0,0.30080973540386102,0.30082059554838603,0,12536.280600000007,0,12536.280600000007,"yes",25000,857.45,3875.54,null,110666.4822,445916.48220000003,500,0,26318.770140494737,-3000,626.81403000000046,23945.584170494738,-11409.303570494731,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","40 fc","yes-day","no-occ","red-epd","high-eff",999.69,0,0.33360169688336999,0.33359775486124499,0,13902.223200000002,0,13902.223200000002,"yes",25000,857.45,3875.54,null,148916.4822,528416.48219999997,500,0,35374.493933776044,-3000,695.11116000000015,33069.605093776045,-19167.381893776044,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","40 fc","yes-day","yes-occ","base-epd","base-eff",1118.9000000000001,0,0.254129960209943,0.25413130861992,0,10590.5694,0,10590.5694,"yes",25000,857.45,3875.54,null,115916.4822,451166.48220000003,500,0,27561.712621925504,-3000,529.52847000000008,25091.241091925505,-14500.671691925505,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","40 fc","yes-day","yes-occ","base-epd","high-eff",1071.8800000000001,0,0.28548204802675398,0.28547525881090302,0,11896.785000000002,0,11896.785000000002,"yes",25000,857.45,3875.54,null,154166.4822,533666.48219999997,500,0,36617.436415206823,-3000,594.83925000000011,34212.27566520682,-22315.490665206817,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","40 fc","yes-day","yes-occ","red-epd","base-eff",1011.37,0,0.32581399309479903,0.32581176298054199,0,13577.752800000002,0,13577.752800000002,"yes",25000,857.45,3875.54,null,119666.4822,454916.48220000003,500,0,28449.528680090338,-3000,678.88764000000015,26128.416320090339,-12550.663520090337,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","40 fc","yes-day","yes-occ","red-epd","high-eff",961.76,0,0.35888463979934698,0.358882230206715,0,14955.918600000005,0,14955.918600000005,"yes",25000,857.45,3875.54,null,157916.4822,537416.48219999997,500,0,37505.252473371649,-3000,747.79593000000023,35253.048403371649,-20297.129803371645,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","25 fc","no-day","no-occ","base-epd","base-eff",1203.3599999999999,0,0.1978200622397,0.197829521441475,0,8244.2706000000071,0,8244.2706000000071,"no",25000,857.45,3875.54,null,96416.482199999999,584166.48219999997,500,0,22945.069119468364,-4750,412.21353000000039,18607.282649468365,-10363.012049468358,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","25 fc","no-day","no-occ","base-epd","high-eff",1158.24,0,0.22790258403133701,0.227906914734056,0,9497.7042000000038,0,9497.7042000000038,"yes",25000,857.45,3875.54,null,134666.4822,666666.48219999997,500,0,32000.792912749675,-4750,474.8852100000002,27725.678122749676,-18227.973922749672,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","25 fc","no-day","no-occ","red-epd","base-eff",1093.5,0,0.27105234637476999,0.27106317452487499,0,11296.181400000005,0,11296.181400000005,"yes",25000,857.45,3875.54,null,100166.4822,587916.48219999997,500,0,23832.885177633198,-4750,564.80907000000025,19647.694247633197,-8351.512847633192,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","25 fc","no-day","no-occ","red-epd","high-eff",1046.1600000000001,0,0.30262118936660998,0.30262043956190499,0,12611.286600000001,0,12611.286600000001,"yes",25000,857.45,3875.54,null,138416.4822,670416.48219999997,500,0,32888.608970914516,-4750,630.56433000000015,28769.173300914517,-16157.886700914516,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","25 fc","no-day","yes-occ","base-epd","base-eff",1155.3,0,0.22986886311910701,0.22986674488211001,0,9579.3774000000049,0,9579.3774000000049,"yes",25000,857.45,3875.54,null,105416.4822,593166.48219999997,500,0,25075.827659063965,-4750,478.96887000000027,20804.796529063966,-11225.419129063961,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","25 fc","no-day","yes-occ","base-epd","high-eff",1109.44,0,0.26043134279830898,0.26043742875617398,0,10853.368200000003,0,10853.368200000003,"yes",25000,857.45,3875.54,null,143666.4822,675666.48219999997,500,0,34131.55145234528,-4750,542.66841000000011,29924.219862345279,-19070.851662345274,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","25 fc","no-day","yes-occ","red-epd","base-eff",1046.67,0,0.302280574091564,0.30228046902601802,0,12597.118800000002,0,12597.118800000002,"yes",25000,857.45,3875.54,null,109166.4822,596916.48219999997,500,0,25963.643717228802,-4750,629.85594000000015,21843.499657228804,-9246.3808572288017,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","25 fc","no-day","yes-occ","red-epd","high-eff",998.45,0,0.33442227004598302,0.33442434988967601,0,13936.670400000003,0,13936.670400000003,"yes",25000,857.45,3875.54,null,147416.4822,679416.48219999997,500,0,35019.367510510121,-4750,696.83352000000014,30966.201030510121,-17029.530630510118,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","25 fc","yes-day","no-occ","base-epd","base-eff",1116.1500000000001,0,0.255972379197696,0.25596448307813302,0,10666.964400000003,0,10666.964400000003,"yes",25000,857.45,3875.54,null,110166.4822,669416.48219999997,500,0,26200.39466607276,-4750,533.3482200000002,21983.74288607276,-11316.778486072757,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","25 fc","yes-day","no-occ","base-epd","high-eff",1069.08,0,0.28733994952700898,0.28734176371381198,0,11974.569000000007,0,11974.569000000007,"yes",25000,857.45,3875.54,null,148416.4822,751916.48219999997,500,0,35256.118459354067,-4750,598.72845000000041,31104.846909354066,-19130.277909354059,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","25 fc","yes-day","no-occ","red-epd","base-eff",1008.69,0,0.32759448203254399,0.32759827481618298,0,13652.203200000002,0,13652.203200000002,"yes",25000,857.45,3875.54,null,113916.4822,673166.48219999997,500,0,27088.210724237593,-4750,682.61016000000018,23020.820884237593,-9368.6176842375917,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","25 fc","yes-day","no-occ","red-epd","high-eff",959.03,0,0.36071157627459799,0.360702072487051,0,15031.758000000005,0,15031.758000000005,"yes",25000,857.45,3875.54,null,152166.4822,755666.48219999997,500,0,36143.934517518908,-4750,751.58790000000033,32145.522417518907,-17113.764417518902,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","25 fc","yes-day","yes-occ","base-epd","base-eff",1086.5999999999999,0,0.275666135100404,0.27566277589275601,0,11487.863400000007,0,11487.863400000007,"yes",25000,857.45,3875.54,null,119166.4822,678416.48219999997,500,0,28331.153205668361,-4750,574.3931700000004,24155.54637566836,-12667.682975668353,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","25 fc","yes-day","yes-occ","base-epd","high-eff",1039.01,0,0.307389803217266,0.30738669315326,0,12809.913600000005,0,12809.913600000005,"yes",25000,857.45,3875.54,null,157416.4822,760916.48219999997,500,0,37386.876998949672,-4750,640.49568000000033,33277.372678949672,-20467.459078949665,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","25 fc","yes-day","yes-occ","red-epd","base-eff",979.82,0,0.34683924507268998,0.34684327358295602,0,14454.211800000003,0,14454.211800000003,"yes",25000,857.45,3875.54,null,122916.4822,682166.48219999997,500,0,29218.969263833194,-4750,722.71059000000014,25191.679853833193,-10737.46805383319,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","base-win","red-inf","25 fc","yes-day","yes-occ","red-epd","high-eff",929.6,0,0.38032791961479501,0.38032037223440601,0,15849.323400000003,0,15849.323400000003,"yes",25000,857.45,3875.54,null,161166.4822,764666.48219999997,500,0,38274.693057114513,-4750,792.46617000000015,34317.159227114513,-18467.835827114512,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Baseline Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","base-lpd","no-day","no-occ","base-epd","base-eff",1410.53,0,5.9731533233213202E-2,5.9728156893069401E-2,0,2489.0880000000038,0,2489.0880000000038,"no",25000,857.45,3875.54,null,81156.490999999995,340620.35,500,0,19332.251723517948,0,124.45440000000019,19456.706123517946,-16967.618123517943,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","base-lpd","no-day","no-occ","base-epd","high-eff",1361.78,0,9.2229326975181394E-2,9.2225340470492606E-2,0,3843.3630000000044,0,3843.3630000000044,"no",25000,857.45,3875.54,null,119406.49099999999,423120.35,500,0,28387.975516799259,0,192.16815000000022,28580.14366679926,-24736.780666799255,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","base-lpd","no-day","no-occ","red-epd","base-eff",1296.97,0,0.13542553685612099,0.13542826288388299,0,5643.7848000000031,0,5643.7848000000031,"no",25000,857.45,3875.54,null,84906.490999999995,344370.35,500,0,20220.067781682781,0,282.18924000000015,20502.257021682781,-14858.472221682778,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","base-lpd","no-day","no-occ","red-epd","high-eff",1246.28,0,0.169223861648268,0.16921866771546501,0,7051.953000000005,0,7051.953000000005,"no",25000,857.45,3875.54,null,123156.49099999999,426870.35,500,0,29275.791574964096,0,352.59765000000027,29628.389224964096,-22576.436224964091,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","base-lpd","no-day","yes-occ","base-epd","base-eff",1329.14,0,0.113982257040673,0.11398345476725399,0,4750.1022000000003,0,4750.1022000000003,"no",25000,857.45,3875.54,null,90156.490999999995,349620.35,500,0,21463.010263113549,0,237.50511000000003,21700.515373113547,-16950.413173113546,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","base-lpd","no-day","yes-occ","base-epd","high-eff",1279.3599999999999,0,0.14717676384523701,0.14716724550539001,0,6132.9906000000065,0,6132.9906000000065,"no",25000,857.45,3875.54,null,128406.49099999999,432120.35,500,0,30518.734056394864,0,306.64953000000031,30825.383586394863,-24692.392986394858,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","base-lpd","no-day","yes-occ","red-epd","base-eff",1218.02,0,0.18806607936335901,0.188057035056962,0,7837.0158000000047,0,7837.0158000000047,"no",25000,857.45,3875.54,null,93906.490999999995,353370.35,500,0,22350.826321278382,0,391.85079000000025,22742.677111278383,-14905.661311278378,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","base-lpd","no-day","yes-occ","red-epd","high-eff",1165.92,0,0.22277787239313199,0.22278735842893599,0,9284.3538000000026,0,9284.3538000000026,"yes",25000,857.45,3875.54,null,132156.49099999998,435870.35,500,0,31406.550114559697,0,464.21769000000018,31870.767804559699,-22586.414004559694,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","base-lpd","yes-day","no-occ","base-epd","base-eff",1261.5999999999999,0,0.159005403396863,0.15900621946098001,0,6626.3634000000065,0,6626.3634000000065,"no",25000,857.45,3875.54,null,94906.490999999995,425870.35,500,0,22587.57727012234,0,331.31817000000035,22918.895440122338,-16292.532040122333,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","base-lpd","yes-day","no-occ","base-epd","high-eff",1210.3900000000001,0,0.19314434346405701,0.19314326091738701,0,8048.9772000000012,0,8048.9772000000012,"no",25000,857.45,3875.54,null,133156.49099999998,508370.35,500,0,31643.301063403647,0,402.44886000000008,32045.749923403648,-23996.772723403647,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","base-lpd","yes-day","no-occ","red-epd","base-eff",1152.43,0,0.231773212156869,0.23177991240759099,0,9659.1060000000016,0,9659.1060000000016,"yes",25000,857.45,3875.54,null,98656.490999999995,429620.35,500,0,23475.393328287177,0,482.95530000000008,23958.348628287178,-14299.242628287177,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","base-lpd","yes-day","no-occ","red-epd","high-eff",1098.58,0,0.26767715864930602,0.267676801343884,0,11155.059000000007,0,11155.059000000007,"yes",25000,857.45,3875.54,null,136906.49099999998,512120.35,500,0,32531.117121568484,0,557.7529500000004,33088.870071568483,-21933.811071568474,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","base-lpd","yes-day","yes-occ","base-epd","base-eff",1213.81,0,0.190868414126244,0.19086345850026301,0,7953.9696000000058,0,7953.9696000000058,"no",25000,857.45,3875.54,null,103906.49099999999,434870.35,500,0,24718.335809717941,0,397.6984800000003,25116.03428971794,-17162.064689717932,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","base-lpd","yes-day","yes-occ","base-epd","high-eff",1161.42,0,0.22578147981854499,0.22578709845146799,0,9409.3638000000028,0,9409.3638000000028,"yes",25000,857.45,3875.54,null,142156.49099999998,517370.35,500,0,33774.059602999252,0,470.46819000000016,34244.527792999252,-24835.163992999249,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","base-lpd","yes-day","yes-occ","red-epd","base-eff",1105.8499999999999,0,0.26283113223613902,0.26283055468526101,0,10953.098400000006,0,10953.098400000006,"yes",25000,857.45,3875.54,null,107656.49099999999,438620.35,500,0,25606.151867882778,0,547.65492000000029,26153.806787882779,-15200.708387882773,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","base-lpd","yes-day","yes-occ","red-epd","high-eff",1050.6400000000001,0,0.29963306445370003,0.299634031717251,0,12486.832200000003,0,12486.832200000003,"yes",25000,857.45,3875.54,null,145906.49099999998,521120.35,{"$f":"MIN(0.01*AA31030,500)","v":500},0,34661.875661164093,0,624.34161000000017,{"$f":"SUM(AE31030:AG31030)","v":35286.217271164096},-22799.385071164092,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","40 fc","no-day","no-occ","base-epd","base-eff",1318.72,0,0.120933905154128,0.120929519441648,0,5039.5698000000029,0,5039.5698000000029,"no",25000,857.45,3875.54,null,97656.490999999995,392120.35,500,0,23238.642379443219,-3000,251.97849000000016,20490.620869443221,-15451.051069443218,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","40 fc","no-day","no-occ","base-epd","high-eff",1268.76,0,0.15423678954620801,0.15423329978068601,0,6427.4586000000036,0,6427.4586000000036,"no",25000,857.45,3875.54,null,135906.49099999998,474620.35,500,0,32294.366172724531,-3000,321.37293000000022,29615.739102724532,-23188.280502724527,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","40 fc","no-day","no-occ","red-epd","base-eff",1207.8900000000001,0,0.194816454814287,0.19480978315212699,0,8118.4272000000019,0,8118.4272000000019,"no",25000,857.45,3875.54,null,101406.49099999999,395870.35,500,0,24126.458437608053,-3000,405.92136000000011,21532.379797608053,-13413.952597608051,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","40 fc","no-day","no-occ","red-epd","high-eff",1155.58,0,0.229683072969081,0.229680094391819,0,9571.5990000000056,0,9571.5990000000056,"yes",25000,857.45,3875.54,null,139656.49099999998,478370.35,500,0,33182.182230889361,-3000,478.57995000000028,30660.76218088936,-21089.163180889354,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","40 fc","no-day","yes-occ","base-epd","base-eff",1258.17,0,0.16129681524717801,0.16129268796704299,0,6721.6488000000018,0,6721.6488000000018,"no",25000,857.45,3875.54,null,106656.49099999999,401120.35,500,0,25369.400919038821,-3000,336.08244000000013,22705.483359038823,-15983.83455903882,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","40 fc","no-day","yes-occ","base-epd","high-eff",1207.04,0,0.195373825264364,0.19537640071193799,0,8142.0402000000049,0,8142.0402000000049,"no",25000,857.45,3875.54,null,144906.49099999998,483620.35,500,0,34425.124712320132,-3000,407.10201000000029,31832.226722320131,-23690.186522320124,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","40 fc","no-day","yes-occ","red-epd","base-eff",1148.98,0,0.234080106519686,0.234079713091532,0,9754.9470000000038,0,9754.9470000000038,"yes",25000,857.45,3875.54,null,110406.49099999999,404870.35,500,0,26257.216977203654,-3000,487.74735000000021,23744.964327203656,-13990.017327203652,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","40 fc","no-day","yes-occ","red-epd","high-eff",1095.25,0,0.26989115793710999,0.26989660896055701,0,11247.566400000003,0,11247.566400000003,"yes",25000,857.45,3875.54,null,148656.49099999998,487370.35,500,0,35312.940770484965,-3000,562.37832000000014,32875.319090484969,-21627.752690484966,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","40 fc","yes-day","no-occ","base-epd","base-eff",1207.5999999999999,0,0.19500224496431301,0.19500309973135699,0,8126.4834000000064,0,8126.4834000000064,"no",25000,857.45,3875.54,null,111406.49099999999,477370.35,500,0,26493.967926047611,-3000,406.32417000000032,23900.292096047611,-15773.808696047605,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","40 fc","yes-day","no-occ","base-epd","high-eff",1155.06,0,0.230023688244128,0.230026731016645,0,9586.0446000000065,0,9586.0446000000065,"yes",25000,857.45,3875.54,null,149656.49099999998,559870.35,500,0,35549.691719328926,-3000,479.30223000000035,33028.993949328928,-23442.949349328919,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","40 fc","yes-day","no-occ","red-epd","base-eff",1099.79,0,0.266872067999195,0.26687020458227001,0,11121.445200000006,0,11121.445200000006,"yes",25000,857.45,3875.54,null,115156.49099999999,481120.35,500,0,27381.783984212449,-3000,556.07226000000026,24937.856244212449,-13816.411044212444,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","40 fc","yes-day","no-occ","red-epd","high-eff",1044.3900000000001,0,0.30379786031677197,0.3038003373041,0,12660.457200000003,0,12660.457200000003,"yes",25000,857.45,3875.54,null,153406.49099999998,563620.35,500,0,36437.507777493753,-3000,633.02286000000015,34070.53063749375,-21410.073437493746,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","40 fc","yes-day","yes-occ","base-epd","base-eff",1171.17,0,0.21927882456765099,0.21928766173598299,0,9138.5088000000014,0,9138.5088000000014,"yes",25000,857.45,3875.54,null,120406.49099999999,486370.35,500,0,28624.726465643213,-3000,456.92544000000009,26081.651905643212,-16943.143105643212,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","40 fc","yes-day","yes-occ","base-epd","high-eff",1117.6300000000001,0,0.25498149839756001,0.254977901915167,0,10625.85,0,10625.85,"yes",25000,857.45,3875.54,null,158656.49099999998,568870.35,500,0,37680.450258924531,-3000,531.29250000000002,35211.742758924534,-24585.892758924536,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","40 fc","yes-day","yes-occ","red-epd","base-eff",1064.2,0,0.29059127715245597,0.29059481511602298,0,12110.135400000003,0,12110.135400000003,"yes",25000,857.45,3875.54,null,124156.49099999999,490120.35,500,0,29512.54252380805,-3000,605.50677000000019,27118.04929380805,-15007.913893808047,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","40 fc","yes-day","yes-occ","red-epd","high-eff",1007.7,0,0.32826023007013599,0.32825821762113999,0,13679.705400000004,0,13679.705400000004,"yes",25000,857.45,3875.54,null,162406.49099999998,572620.35,500,0,38568.266317089357,-3000,683.98527000000024,36252.251587089355,-22572.546187089349,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","25 fc","no-day","no-occ","base-epd","base-eff",1253.81,0,0.16420752759757801,0.164199102744429,0,6842.769600000006,0,6842.769600000006,{"$f":"IF(P31047>0.2,\"yes\",\"no\")","v":"no"},{"$f":"IF(B31047=\"5500 ft2\",5500,IF(B31047=\"10000 ft2\",10000,25000))","v":25000},{"$f":"IF(B31047=\"5500 ft2\",IF(D31047=\"stand-alone\",642.39,IF(D31047=\"ad-e&flr\",522.37,402.25)),IF(B31047=\"10000 ft2\",IF(D31047=\"stand-alone\",866.06,IF(D31047=\"ad-e&flr\",704.17,542.29)),IF(B31047=\"25000 ft2\",IF(D31047=\"stand-alone\",1369.38,IF(D31047=\"ad-e&flr\",1113.42,857.45)))))","v":857.45},{"$f":"IF(B31047=\"5500 ft2\",IF(D31047=\"stand-alone\",3030.15,IF(D31047=\"ad-e&flr\",2424.14,1818.13)),IF(B31047=\"10000 ft2\",IF(D31047=\"stand-alone\",4085.12,IF(D31047=\"ad-e&flr\",3268.14,2451.05)),IF(B31047=\"25000 ft2\",IF(D31047=\"stand-alone\",6459.2,IF(D31047=\"ad-e&flr\",5167.32,3875.54)))))","v":3875.54},null,{"$f":"SUM(IF(F31047=\"eff-roof\",W31047*IF(AND(W$4=\"no\",X$4=\"no\"),$C$4,$C$3)),IF(G31047=\"eff-win\",X31047*IF(W$4=\"no\",$D$4,$D$3),0),IF(H31047=\"red-inf\",Y31047*IF(W$4=\"no\",$F$4,$F$3),0),IF(I31047=\"25 fc\",W31047*IF(W$4=\"no\",$H$4,$H$3),0),IF(I31047=\"40 fc\",W31047*IF(W$4=\"no\",$G$4,$G$3),0),IF(J31047=\"yes-day\",W31047*IF(W$4=\"no\",$I$4,$I$3),0),IF(K31047=\"yes-occ\",W31047*IF(W$4=\"no\",$J$4,$J$3),0),IF(L31047=\"red-epd\",W31047*IF(W$4=\"no\",$K$4,$K$3),0),IF(AND(M31047=\"high-eff\",C31047=\"psz-ac\"),W31047*IF(AND(W$4=\"no\",Y$4=\"no\"),$L$4,$L$3),0),IF(AND(M31047=\"high-eff\",C31047=\"ptac\"),W31047*IF(AND(W$4=\"no\",Y$4=\"no\"),$M$4,$M$3),0),IF(AND(M31047=\"high-eff\",C31047=\"pthp\"),W31047*IF(AND(W$4=\"no\",Y$4=\"no\"),$N$4,$N$3),0))","v":100906.49099999999},{"$f":"SUM(IF(F31047=\"eff-roof\",W31047*$C$4),IF(G31047=\"eff-win\",X31047*$D$4,0),IF(H31047=\"red-inf\",Y31047*$F$4,0),IF(I31047=\"25 fc\",W31047*$H$4,0),IF(I31047=\"40 fc\",W31047*$G$4,0),IF(J31047=\"yes-day\",W31047*$I$4,0),IF(K31047=\"yes-occ\",W31047*$J$4,0),IF(L31047=\"red-epd\",W31047*$K$4,0),IF(AND(M31047=\"high-eff\",C31047=\"psz-ac\"),W31047*$L$4,0),IF(AND(M31047=\"high-eff\",C31047=\"ptac\"),W31047*$M$4,0),IF(AND(M31047=\"high-eff\",C31047=\"pthp\"),W31047*$N$4,0))","v":619370.35},500,0,{"$f":"-PMT($AE$3,$AE$4,AA31047+AC31047-AD31047)","v":24008.082963186076},{"$f":"SUM(IF(F31047=\"eff-roof\",($C$5*W31047),0),IF(G31047=\"eff-win\",($D$5*X31047),0),IF(H31047=\"red-inf\",$F$5*(Y31047-X31047),0),IF(I31047=\"25 fc\",($H$5*W31047),0),IF(I31047=\"40 fc\",($G$5*W31047),0),IF(J31047=\"yes-day\",($I$5*W31047),0),IF(K31047=\"yes-occ\",($J$5*W31047),0),IF(L31047=\"red-epd\",($K$5*W31047),0),IF(M31047=\"high-eff\",($L$5*W31047),0))","v":-4750},{"$f":"0.05*U31047","v":342.1384800000003},19600.221443186078,{"$f":"U31047-AH31047","v":-12757.451843186071},null,null,null,"Pre 1980 Construction",{"$f":"IF(B31047=\"5500 ft2\",\"5,500 SF\",IF(B31047=\"10000 ft2\",\"10,000 SF\",IF(B31047=\"25000 ft2\",\"25,000 SF\")))","v":"25,000 SF"},"Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration",{"$f":"IF(I31047=\"base-lpd\",\"Baseline Lighting Levels\",IF(I31047=\"40 fc\",\"Reduce Lighting Levels to 40 fc\",IF(I31047=\"25 fc\",\"Reduce Lighting Levels to 25 fc\")))","v":"Reduce Lighting Levels to 25 fc"},"No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","25 fc","no-day","no-occ","base-epd","high-eff",1202.57,0,0.19834646766477301,0.19835614246765301,0,{"$f":"277.8*($N$30727-N31048)*$S$3","v":8266.2168000000056},{"$f":"277.78*($O$30727-O31048)*$S$4","v":0},{"$f":"SUM(S31048:T31048)","v":8266.2168000000056},"no",25000,857.45,3875.54,null,139156.49099999998,701870.35,500,{"$f":"IF(V31048=\"yes\",0,0)","v":0},33063.806756467391,-4750,413.31084000000033,28727.117596467393,-20460.900796467387,null,null,null,"Pre 1980 Construction","25,000 SF",{"$f":"IF(C31048=\"psz-ac\",\"Packaged Air Conditioner\",IF(C31048=\"ptac\",\"Split System Air Conditioner\",IF(C31048=\"pthp\",\"Split System Heat Pump\")))","v":"Split System Heat Pump"},{"$f":"IF(D31048=\"stand-alone\",\"Stand Alone\",IF(D31048=\"ad-e&flr\",\"Above Ground, 1 Side Attached\",IF(D31048=\"ad-e&w&flr\",\"Above Ground, 2 Sides Attached\")))","v":"Above Ground, 2 Sides Attached"},{"$f":"IF(F31048=\"base-roof\",\"Baseline Roof Insulation\",IF(F31048=\"eff-roof\",\"Increased Roof Insulation\"))","v":"Increased Roof Insulation"},{"$f":"IF(G31048=\"base-win\",\"Baseline Windows\",IF(G31048=\"eff-win\",\"Replace Windows\"))","v":"Replace Windows"},{"$f":"IF(H31048=\"base-inf\",\"Baseline Infiltration\",IF(H31048=\"red-inf\",\"Reduce Infiltration\"))","v":"Baseline Infiltration"},"Reduce Lighting Levels to 25 fc",{"$f":"IF(J31048=\"no-day\",\"No Daylighting Sensors\",IF(J31048=\"yes-day\",\"Install Daylighting Sensors\"))","v":"No Daylighting Sensors"},{"$f":"IF(K31048=\"no-occ\",\"No Occupancy Sensors\",IF(K31048=\"yes-occ\",\"Install Occupancy Sensors\"))","v":"No Occupancy Sensors"},{"$f":"IF(L31048=\"base-epd\",\"No Plug Load Control\",IF(L31048=\"red-epd\",\"Install Plug Load Controls\"))","v":"No Plug Load Control"},{"$f":"IF(M31048=\"base-eff\",\"Baseline HVAC Equipment\",IF(M31048=\"high-eff\",\"Install High Efficiency HVAC Equipment\"))","v":"Install High Efficiency HVAC Equipment"}]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","25 fc","no-day","no-occ","red-epd","base-eff",1144.72,0,0.23691340630757601,0.23691946697952801,0,9873.2898000000041,0,9873.2898000000041,"yes",25000,857.45,3875.54,null,104656.49099999999,623120.35,500,0,24895.89902135091,-4750,493.66449000000023,20639.563511350909,-10766.273711350905,null,null,null,{"$f":"IF(A31049=\"new90.1-2004\",\"New Construction\",IF(A31049=\"post1980\",\"Post 1980 Construction\",IF(A31049=\"pre1980\",\"Pre 1980 Construction\")))","v":"Pre 1980 Construction"},"25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","25 fc","no-day","no-occ","red-epd","high-eff",1090.8800000000001,0,0.27280187028751002,0.27280968982688197,0,11368.965000000002,0,11368.965000000002,"yes",25000,857.45,3875.54,null,142906.49099999998,705620.35,500,0,33951.622814632217,-4750,568.44825000000014,29770.071064632219,-18401.106064632215,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","25 fc","no-day","yes-occ","base-epd","base-eff",1208.27,0,0.19455325210175101,0.194556471772446,0,8107.8708000000042,0,8107.8708000000042,"no",25000,857.45,3875.54,null,109906.49099999999,628370.35,500,0,26138.841502781677,-4750,405.39354000000026,21794.235042781678,-13686.364242781674,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","25 fc","no-day","yes-occ","base-epd","high-eff",1155.32,0,0.22985338060660501,0.22985341270423201,0,9578.8218000000052,0,9578.8218000000052,"yes",25000,857.45,3875.54,null,148156.49099999998,710870.35,500,0,35194.565296062989,-4750,478.94109000000026,30923.506386062989,-21344.684586062984,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","25 fc","no-day","yes-occ","red-epd","base-eff",1100.31,0,0.26653145272414802,0.26652356795744397,0,11106.999600000005,0,11106.999600000005,"yes",25000,857.45,3875.54,null,113656.49099999999,632120.35,500,0,27026.657560946511,-4750,555.3499800000003,22832.00754094651,-11725.007940946505,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","25 fc","no-day","yes-occ","red-epd","high-eff",1044.52,0,0.30372044775426099,0.30371367814789402,0,12656.845800000005,0,12656.845800000005,"yes",25000,857.45,3875.54,null,151906.49099999998,714620.35,500,0,36082.381354227829,-4750,632.84229000000028,31965.22364422783,-19308.377844227827,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","25 fc","yes-day","no-occ","base-epd","base-eff",1168.52,0,0.22105931350539601,0.221054175304807,0,9212.1258000000053,0,9212.1258000000053,"yes",25000,857.45,3875.54,null,114656.49099999999,704620.35,500,0,27263.408509790468,-4750,460.60629000000029,22974.014799790468,-13761.888999790463,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","25 fc","yes-day","no-occ","base-epd","high-eff",1114.9100000000001,0,0.25679295236030902,0.25679107810656399,0,10701.411600000001,0,10701.411600000001,"yes",25000,857.45,3875.54,null,152906.49099999998,787120.35,500,0,36319.132303071783,-4750,535.07058000000006,32104.202883071783,-21402.791283071783,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","25 fc","yes-day","no-occ","red-epd","base-eff",1061.6099999999999,0,0.292325318552695,0.29232133215121398,0,12182.085600000006,0,12182.085600000006,"yes",25000,857.45,3875.54,null,118406.49099999999,708370.35,500,0,28151.224567955305,-4750,609.10428000000036,24010.328847955305,-11828.243247955299,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","25 fc","yes-day","no-occ","red-epd","high-eff",1005.02,0,0.33004071900788101,0.33004472945677998,0,13754.155800000006,0,13754.155800000006,"yes",25000,857.45,3875.54,null,156656.49099999998,790870.35,500,0,37206.948361236617,-4750,687.70779000000039,33144.656151236617,-19390.500351236609,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","25 fc","yes-day","yes-occ","base-epd","base-eff",1141.19,0,0.239266748207899,0.23927259637498099,0,9971.3532000000032,0,9971.3532000000032,"yes",25000,857.45,3875.54,null,123656.49099999999,713620.35,500,0,29394.167049386073,-4750,498.56766000000016,25142.734709386074,-15171.38150938607,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","25 fc","yes-day","yes-occ","base-epd","high-eff",1086.1099999999999,0,0.27599126786294897,0.27598941425076501,0,11501.475600000007,0,11501.475600000007,"yes",25000,857.45,3875.54,null,161906.49099999998,796120.35,500,0,38449.890842667381,-4750,575.0737800000004,34274.964622667379,-22773.489022667374,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","25 fc","yes-day","yes-occ","red-epd","base-eff",1034.8699999999999,0,0.31014569044264501,0.31014645397398899,0,12924.922800000008,0,12924.922800000008,"yes",25000,857.45,3875.54,null,127406.49099999999,717370.35,500,0,30281.983107550906,-4750,646.24614000000042,26178.229247550906,-13253.306447550898,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","base-inf","25 fc","yes-day","yes-occ","red-epd","high-eff",976.68,0,0.34892938426047798,0.34893642550978898,0,14541.441000000006,0,14541.441000000006,"yes",25000,857.45,3875.54,null,165656.49099999998,799870.35,500,0,39337.706900832221,-4750,727.07205000000033,35314.778950832224,-20773.337950832218,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Baseline Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","base-lpd","no-day","no-occ","base-epd","base-eff",1360.77,0,9.2895075012773096E-2,9.2898615453327504E-2,0,3871.4208000000035,0,3871.4208000000035,"no",25000,857.45,3875.54,null,82822.973199999993,342286.8322,500,0,19726.792965599507,0,193.57104000000018,19920.364005599506,-16048.943205599502,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","base-lpd","no-day","no-occ","base-epd","high-eff",1317.36,0,0.121831890879252,0.121836107537347,0,5077.3506000000061,0,5077.3506000000061,"no",25000,857.45,3875.54,null,121072.97319999999,424786.8322,500,0,28782.516758880822,0,253.86753000000033,29036.384288880821,-23959.033688880816,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","base-lpd","no-day","no-occ","red-epd","base-eff",1246.1099999999999,0,0.169332239235783,0.16933199122742701,0,7056.6756000000069,0,7056.6756000000069,"no",25000,857.45,3875.54,null,86572.973199999993,346036.8322,500,0,20614.609023764344,0,352.83378000000039,20967.442803764345,-13910.767203764339,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","base-lpd","no-day","no-occ","red-epd","high-eff",1200.99,0,0.19941476102741901,0.199409384520008,0,8310.1092000000044,0,8310.1092000000044,"no",25000,857.45,3875.54,null,124822.97319999999,428536.8322,500,0,29670.332817045655,0,415.50546000000026,30085.838277045656,-21775.729077045653,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","base-lpd","no-day","yes-occ","base-epd","base-eff",1276.33,0,0.149189490470514,0.14918707045389401,0,6217.1640000000052,0,6217.1640000000052,"no",25000,857.45,3875.54,null,91822.973199999993,351286.8322,500,0,21857.551505195112,0,310.85820000000029,22168.40970519511,-15951.245705195106,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","base-lpd","no-day","yes-occ","base-epd","high-eff",1232.52,0,0.17838950904952899,0.17839120609547199,0,7434.2058000000034,0,7434.2058000000034,"no",25000,857.45,3875.54,null,130072.97319999999,433786.8322,500,0,30913.275298476427,0,371.71029000000021,31284.985588476426,-23850.779788476422,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","base-lpd","no-day","yes-occ","red-epd","base-eff",1164.3900000000001,0,0.22379971821827199,0.22380727003659701,0,9326.8572000000004,0,9326.8572000000004,"yes",25000,857.45,3875.54,null,95572.973199999993,355036.8322,500,0,22745.367563359949,0,466.34286000000003,23211.710423359949,-13884.853223359949,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","base-lpd","no-day","yes-occ","red-epd","high-eff",1118.55,0,0.254362197897475,0.25436462173278301,0,10600.292400000006,0,10600.292400000006,"yes",25000,857.45,3875.54,null,133822.97320000001,437536.8322,500,0,31801.09135664126,0,530.01462000000026,32331.105976641262,-21730.813576641256,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","base-lpd","yes-day","no-occ","base-epd","base-eff",1208.97,0,0.19408877672668701,0.19408984554671899,0,8088.4248000000025,0,8088.4248000000025,"no",25000,857.45,3875.54,null,96572.973199999993,427536.8322,500,0,22982.118512203902,0,404.42124000000013,23386.539752203902,-15298.1149522039,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","base-lpd","yes-day","no-occ","base-epd","high-eff",1163.6099999999999,0,0.224326123643345,0.224327224973836,0,9348.5256000000063,0,9348.5256000000063,"yes",25000,857.45,3875.54,null,134822.97320000001,510036.8322,500,0,32037.842305485217,0,467.42628000000036,32505.268585485217,-23156.742985485209,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","base-lpd","yes-day","no-occ","red-epd","base-eff",1099.26,0,0.26722816578674402,0.267223507296034,0,11136.168600000005,0,11136.168600000005,"yes",25000,857.45,3875.54,null,100322.97319999999,431286.8322,500,0,23869.934570368736,0,556.80843000000027,24426.743000368737,-13290.574400368732,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","base-lpd","yes-day","no-occ","red-epd","high-eff",1051.4000000000001,0,0.29912214154112898,0.29912740895788997,0,12465.719400000002,0,12465.719400000002,"yes",25000,857.45,3875.54,null,138572.97320000001,513786.8322,500,0,32925.658363650058,0,623.28597000000013,33548.944333650055,-21083.224933650054,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","base-lpd","yes-day","yes-occ","base-epd","base-eff",1158.8499999999999,0,0.22750003870628099,0.22750028330878,0,9480.7584000000061,0,9480.7584000000061,"yes",25000,857.45,3875.54,null,105572.97319999999,436536.8322,500,0,25112.877051799507,0,474.03792000000033,25586.914971799506,-16106.1565717995,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","base-lpd","yes-day","yes-occ","base-epd","high-eff",1112.8699999999999,0,0.25815541346049597,0.25815096025011203,0,10758.082800000007,0,10758.082800000007,"yes",25000,857.45,3875.54,null,143822.97320000001,519036.8322,500,0,34168.600845080822,0,537.90414000000044,34706.504985080821,-23948.422185080814,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","base-lpd","yes-day","yes-occ","red-epd","base-eff",1050.46,0,0.299756924553717,0.29975402131815199,0,12491.832600000003,0,12491.832600000003,"yes",25000,857.45,3875.54,null,109322.97319999999,440286.8322,500,0,26000.693109964341,0,624.59163000000024,26625.28473996434,-14133.452139964336,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","base-lpd","yes-day","yes-occ","red-epd","high-eff",1001.88,0,0.33213085819566801,0.332137881383613,0,13841.385000000004,0,13841.385000000004,"yes",25000,857.45,3875.54,null,147572.97320000001,522786.8322,500,0,35056.416903245656,0,692.06925000000024,35748.486153245656,-21907.101153245654,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Baseline Lighting Levels","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","40 fc","no-day","no-occ","base-epd","base-eff",1265.51,0,0.15640434129650599,0.15639977868584701,0,6517.7436000000043,0,6517.7436000000043,"no",25000,857.45,3875.54,null,99322.973199999993,393786.8322,500,0,23633.183621524782,-3000,325.88718000000023,20959.070801524784,-14441.327201524779,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","40 fc","no-day","no-occ","base-epd","high-eff",1221.6199999999999,0,0.185650807413027,0.18565724303893699,0,7737.0078000000067,0,7737.0078000000067,"no",25000,857.45,3875.54,null,137572.97320000001,476286.8322,500,0,32688.907414806101,-3000,386.85039000000035,30075.7578048061,-22338.750004806094,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","40 fc","no-day","no-occ","red-epd","base-eff",1153.9100000000001,0,0.23079781386923501,0.23079333124462501,0,9617.9916000000012,0,9617.9916000000012,"yes",25000,857.45,3875.54,null,103072.97319999999,397536.8322,500,0,24520.999679689616,-3000,480.89958000000007,22001.899259689617,-12383.907659689616,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","40 fc","no-day","no-occ","red-epd","high-eff",1107.95,0,0.26143770611094802,0.26143067600807901,0,10894.760400000003,0,10894.760400000003,"yes",25000,857.45,3875.54,null,141322.97320000001,480036.8322,500,0,33576.723472970931,-3000,544.73802000000012,31121.461492970931,-20226.701092970929,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","40 fc","no-day","yes-occ","base-epd","base-eff",1202.56,0,0.19836195017727501,0.198362808556592,0,8266.4946000000054,0,8266.4946000000054,"no",25000,857.45,3875.54,null,108322.97319999999,402786.8322,500,0,25763.942161120383,-3000,413.32473000000027,23177.266891120384,-14910.772291120378,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","40 fc","no-day","yes-occ","base-epd","high-eff",1158.1099999999999,0,0.22799547910634901,0.22799357389026301,0,9501.3156000000072,0,9501.3156000000072,"yes",25000,857.45,3875.54,null,146572.97320000001,485286.8322,500,0,34819.665954401702,-3000,475.06578000000036,32294.731734401703,-22793.416134401697,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","40 fc","no-day","yes-occ","red-epd","base-eff",1092.73,0,0.27157875179984198,0.27157646337317398,0,11317.572000000004,0,11317.572000000004,"yes",25000,857.45,3875.54,null,112072.97319999999,406536.8322,500,0,26651.758219285221,-3000,565.87860000000023,24217.636819285221,-12900.064819285217,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","40 fc","no-day","yes-occ","red-epd","high-eff",1046.04,0,0.30269860192912101,0.30270043262917201,0,12614.620200000005,0,12614.620200000005,"yes",25000,857.45,3875.54,null,150322.97320000001,489036.8322,500,0,35707.482012566536,-3000,630.73101000000031,33338.213022566539,-20723.592822566534,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","40 fc","yes-day","no-occ","base-epd","base-eff",1152.32,0,0.23185062471937901,0.23185323938592001,0,9662.1618000000053,0,9662.1618000000053,"yes",25000,857.45,3875.54,null,113072.97319999999,479036.8322,500,0,26888.509168129178,-3000,483.10809000000029,24371.617258129179,-14709.455458129174,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","40 fc","yes-day","no-occ","base-epd","high-eff",1106.27,0,0.26255244701110098,0.26255057894982398,0,10941.430800000004,0,10941.430800000004,"yes",25000,857.45,3875.54,null,151322.97320000001,561536.83220000006,500,0,35944.232961410497,-3000,547.07154000000025,33491.304501410494,-22549.873701410492,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","40 fc","yes-day","no-occ","red-epd","base-eff",1044.0999999999999,0,0.30398365046679798,0.30399365388333,0,12668.513400000007,0,12668.513400000007,"yes",25000,857.45,3875.54,null,116822.97319999999,482786.8322,500,0,27776.325226294011,-3000,633.42567000000042,25409.750896294012,-12741.237496294005,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","40 fc","yes-day","no-occ","red-epd","high-eff",995.44,0,0.33643499667125998,0.33643084266030299,0,14020.288200000003,0,14020.288200000003,"yes",25000,857.45,3875.54,null,155072.97320000001,565286.83220000006,500,0,36832.049019575323,-3000,701.01441000000023,34533.063429575326,-20512.775229575323,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","40 fc","yes-day","yes-occ","base-epd","base-eff",1113.96,0,0.25742773537289598,0.25742435655576501,0,10727.802600000003,0,10727.802600000003,"yes",25000,857.45,3875.54,null,122072.97319999999,488036.8322,500,0,29019.267707724779,-3000,536.39013000000011,26555.657837724779,-15827.855237724776,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","40 fc","yes-day","yes-occ","base-epd","high-eff",1067.49,0,0.288408242889656,0.28840167185510601,0,12018.739200000004,0,12018.739200000004,"yes",25000,857.45,3875.54,null,160322.97320000001,570536.83220000006,500,0,38074.991501006094,-3000,600.93696000000023,35675.928461006093,-23657.18926100609,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","40 fc","yes-day","yes-occ","red-epd","base-eff",1006.65,0,0.32895694313273199,0.32895815695973002,0,13708.874400000004,0,13708.874400000004,"yes",25000,857.45,3875.54,null,125822.97319999999,491786.8322,500,0,29907.083765889613,-3000,685.44372000000021,27592.527485889612,-13883.653085889608,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","40 fc","yes-day","yes-occ","red-epd","high-eff",957.54,0,0.36168697456223198,0.36169531973895602,0,15073.150200000004,0,15073.150200000004,"yes",25000,857.45,3875.54,null,164072.97320000001,574286.83220000006,{"$f":"MIN(0.01*AA31094,500)","v":500},0,38962.807559170928,-3000,753.65751000000023,{"$f":"SUM(AE31094:AG31094)","v":36716.465069170925},-21643.314869170921,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 40 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","25 fc","no-day","no-occ","base-epd","base-eff",1198.01,0,0.201396522627692,0.201395879023818,0,8392.8936000000031,0,8392.8936000000031,"yes",25000,857.45,3875.54,null,102572.97319999999,621036.83220000006,500,0,24402.624205267639,-4750,419.64468000000016,20072.26888526764,-11679.375285267637,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","25 fc","no-day","no-occ","base-epd","high-eff",1153.52,0,0.231045534069269,0.231053308713245,0,9628.8258000000042,0,9628.8258000000042,"yes",25000,857.45,3875.54,null,140822.97320000001,703536.83220000006,500,0,33458.347998548954,-4750,481.44129000000021,29189.789288548953,-19560.96348854895,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","25 fc","no-day","no-occ","red-epd","base-eff",1088.32,0,0.27452042917524699,0.274516208595255,0,11440.081800000007,0,11440.081800000007,"yes",25000,857.45,3875.54,null,106322.97319999999,624786.83220000006,500,0,25290.440263432472,-4750,572.00409000000036,21112.444353432475,-9672.3625534324674,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","25 fc","no-day","no-occ","red-epd","high-eff",1041.57,0,0.30568672684203202,0.30568017438488698,0,12738.796800000006,0,12738.796800000006,"yes",25000,857.45,3875.54,null,144572.97320000001,707286.83220000006,500,0,34346.164056713795,-4750,636.93984000000034,30233.103896713794,-17494.30709671379,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","25 fc","no-day","yes-occ","base-epd","base-eff",1149.99,0,0.23341435848209399,0.23340643810869699,0,9726.8892000000033,0,9726.8892000000033,"yes",25000,857.45,3875.54,null,111572.97319999999,630036.83220000006,500,0,26533.38274486324,-4750,486.3444600000002,22269.72720486324,-12542.838004863237,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","25 fc","no-day","yes-occ","base-epd","high-eff",1104.77,0,0.26354332781123702,0.26355049229066801,0,10983.100800000006,0,10983.100800000006,"yes",25000,857.45,3875.54,null,149822.97320000001,712536.83220000006,500,0,35589.106538144559,-4750,549.15504000000033,31388.26157814456,-20405.160778144556,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","25 fc","no-day","yes-occ","red-epd","base-eff",1041.56,0,0.30568672684203202,0.30568684047382599,0,12739.074600000007,0,12739.074600000007,"yes",25000,857.45,3875.54,null,115322.97319999999,633786.83220000006,500,0,27421.198803028077,-4750,636.95373000000041,23308.152533028078,-10569.077933028071,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","25 fc","no-day","yes-occ","red-epd","high-eff",993.96,0,0.33741039495889402,0.337417423823269,0,14061.402600000001,0,14061.402600000001,"yes",25000,857.45,3875.54,null,153572.97320000001,716286.83220000006,500,0,36476.922596309392,-4750,703.07013000000006,32429.992726309392,-18368.590126309391,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","No Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","25 fc","yes-day","no-occ","base-epd","base-eff",1111.1600000000001,0,0.25928563687315198,0.25929086145867403,0,10805.586600000002,0,10805.586600000002,"yes",25000,857.45,3875.54,null,116322.97319999999,706286.83220000006,500,0,27657.949751872035,-4750,540.27933000000019,23448.229081872036,-12642.642481872033,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","25 fc","yes-day","no-occ","base-epd","high-eff",1064.6600000000001,0,0.29028162690241399,0.29028817502483101,0,12097.356600000001,0,12097.356600000001,"yes",25000,857.45,3875.54,null,154572.97320000001,788786.83220000006,500,0,36713.673545153346,-4750,604.86783000000003,32568.541375153345,-20471.184775153342,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","25 fc","yes-day","no-occ","red-epd","base-eff",1003.92,0,0.330783879607983,0.33077799924006601,0,13784.713800000005,0,13784.713800000005,"yes",25000,857.45,3875.54,null,120072.97319999999,710036.83220000006,500,0,28545.765810036868,-4750,689.23569000000032,24485.001500036869,-10700.287700036864,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","25 fc","yes-day","no-occ","red-epd","high-eff",954.78,0,0.36352939354998498,0.36353516028610899,0,15149.823000000004,0,15149.823000000004,"yes",25000,857.45,3875.54,null,158322.97320000001,792536.83220000006,500,0,37601.489603318187,-4750,757.49115000000029,33608.980753318188,-18459.157753318184,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","No Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","25 fc","yes-day","yes-occ","base-epd","base-eff",1081.5899999999999,0,0.27899487528836198,0.27900248645117398,0,11627.041200000007,0,11627.041200000007,"yes",25000,857.45,3875.54,null,125322.97319999999,715286.83220000006,500,0,29788.708291467636,-4750,581.35206000000039,25620.060351467637,-13993.01915146763,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","25 fc","yes-day","yes-occ","base-epd","high-eff",1034.5999999999999,0,0.31031599808016802,0.31032643837534102,0,12932.423400000007,0,12932.423400000007,"yes",25000,857.45,3875.54,null,163572.97320000001,797786.83220000006,500,0,38844.432084748951,-4750,646.62117000000035,34741.053254748949,-21808.629854748942,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","No Plug Load Control","Install High Efficiency HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","25 fc","yes-day","yes-occ","red-epd","base-eff",975.06,0,0.350013160135627,0.35001633191790099,0,14586.444600000006,0,14586.444600000006,"yes",25000,857.45,3875.54,null,129072.97319999999,719036.83220000006,500,0,30676.524349632469,-4750,729.32223000000033,26655.846579632471,-12069.401979632465,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Baseline HVAC Equipment"]
["pre1980","25000 ft2","pthp","ad-e&w&flr","pre198025000 ft2pthpad-e&w&flr","eff-roof","eff-win","red-inf","25 fc","yes-day","yes-occ","red-epd","high-eff",925.39,0,0.38313025437768,0.38312679567770802,0,15966.277200000004,0,15966.277200000004,"yes",25000,857.45,3875.54,null,167322.97320000001,801536.83220000006,500,0,39732.248142913784,-4750,798.3138600000002,35780.562002913786,-19814.284802913782,null,null,null,"Pre 1980 Construction","25,000 SF","Split System Heat Pump","Above Ground, 2 Sides Attached","Increased Roof Insulation","Replace Windows","Reduce Infiltration","Reduce Lighting Levels to 25 fc","Install Daylighting Sensors","Install Occupancy Sensors","Install Plug Load Controls","Install High Efficiency HVAC Equipment"]