{"text_format":"1","workbook":"xlsx","n_sheets":19,"sheets":["Title","Description","ProcessFlow","Input_Sheet_Template","Replacement Costs","Capital Costs","Plant Scaling","Carbon Sequestration","Results","Tornado Charts & Risk Analysis","Cash Flow Analysis","Energy Feed & Utility Prices","Non-Energy Material Prices","AEO Data","HyARC Physical Property Data","Debt Financing Calculations","Depreciation","Constants and Conversions","Lists"],"not_rendered":{"charts":8,"images":2,"macros":1,"external_links":0,"defined_names":390,"comments":6,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Title","index":0,"n_rows":46,"n_cols":4,"rows_kept":46,"cut":false,"hidden":false,"merged":[[25,1,25,3]]}
[]
[null,"Central Hydrogen Production - Project Information"]
[]
[]
[null,"Title:","Current Distributed Ethanol Steam Reformer (SR) 1500kg/day"]
[null,"Authors:","Brian D. James, Strategic Analysis Inc. "]
[null,"Contact:","Michael Penev"]
[null,"Contact phone:","303 275 3880"]
[null,"Contact e-mail:","mike.penev@nrel.gov"]
[null,"Organization:","NREL"]
[null,"Date:","2022-04-28"]
[null,"Web Site:","www.nrel.gov"]
[]
[null,"Plant Design Capacity (kg/day):",1500]
[null,"Start-up Year:",2015]
[null,"Primary Product Feedstock Source:","Ethanol (Neat)"]
[null,"Secondary Feedstock Source:","None"]
[null,"Process Energy Source:","Commercial Electricity"]
[null,"Conversion Technology:","SR of Ethanol/PSA Purification"]
[null,"Primary By-Product:","None"]
[null,"Secondary By-Product:","None"]
[null,"Based on Number of Plants Installed per Year (per manufacturer):","nth plant (~500 units/yr)"]
[null,"H2 Onsite Storage Type","10,000 psia H2 Compressed Gas Storage"]
[null,"Assumed plant location:","distributed installations"]
[]
[null,"Reporting Spreadsheet Change History:"]
[null,"Date spreadsheet created / modified","Name","Comments"]
[null,"2022-04-28","M. Penev","Removed hydrogen fueling tab. Fueling will be added in the future in context of heavy duty vehicle refueling and at larger scale."]
[]
[null,"2020-10-27","M. Penev","Made compatible with Excel for Mac"]
[]
[null,"2015-03-17T08:56:53.800","Michael Penev, NREL","replaced model buttons"]
[null,"2015-03-17T08:56:53.800","Michael Penev, NREL","Implemented closed-form cash flow calculations"]
[null,"2015-03-17T08:56:53.800","Michael Penev, NREL","Implemented new tornado plots generator"]
[null,"2015-03-17T08:56:53.800","Michael Penev, NREL","Implemented waterfall plots generator"]
[null,"2015-03-17T08:56:53.800","Michael Penev, NREL","Added instant results display in the Input_Sheet_Template"]
[null,"2015-03-17T08:56:53.800","Michael Penev, NREL","Fixed depreciation routine"]
[]
[null,"H2A Version 3"]
[null,"2012-02-27","Darlene Steward, NREL","version 3 template, standard calculation of capacity"]
[null,"H2A Version 2"]
[null,"2009-11-23","Darlene M. Steward","Refueling station calculation correction, tornado chart update"]
[null,"2008-09-23","Darlene Steward","H2A Version 2.1 updates"]
[null,"2008-09-08","Darlene Steward/Brian D. James","Addition of ethanol storage tank costs per Excavation Technologies quote."]
[null,"2008-05-27","Darlene Steward","Addition of tornado chart"]
[null,"2008-02-19","Brian D. James","Based on Distributed Production H2A Spreadsheet v26 by Darlene Steward/Todd Ramsden"]

{"sheet":"Description","index":1,"n_rows":21,"n_cols":2,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
[]
[null,"Central Hydrogen Production - Description"]
[]
[]
[]
[null,"Purpose:"]
[null,"The purpose of this analysis is to determine a baseline delivered cost of hydrogen for the distributed production of hydrogen from on-site ethanol reforming."]
[]
[]
[null,"System Description:"]
[]
[]
[]
[null,"Analysis Methodology Summary:"]
[null,"The ethanol reforming process is based on 20-atm conventional tube-in-shell Steam Reactor(SR) with PSA gas cleanup. Precious metal catalyst is assumed.  The catalysted conversion of ethanol to methane is judged to occur rapidly to near full ethanol conversion in a compact adiabatic reformer. Since methane is the primary component of the pre-reformer, the remainder of the system is nearly identical to that of a natural gas reformer system.  Ethanol is the sole feedstock and is also used as a supplemental fuel to the burner.  A  950C burner adiabatic flame temperature and a 850C reformer temperature are assumed.  Flue gas is exhaused at 110C.  The PSA is based on 4 bed Batta cycle achieving 75% hydrogen recovery.  The unit is assumed to be factory built (as opposed to on-site construction) and is skid-mounted for easy and rapid installation.   A single 1500kg/day unit is assumed (as opposed to the previous H2A assumption of parallel 750kg/day units.)  The system is assumed to be air cooled (and thus requires no cooling water flow)."]
[]
[]
[null,"Plant Ownership and Entity Type Assumptions:"]
[null,"The delivered cost of hydrogen was determined using a discounted cash flow analysis on the total capital investment and the periodic expenditures for repair, maintenance, and replacement.\n\nA tornado plot was developed to show the sensitivity of the delivered hydrogen cost to several important variables.\n\nHysys simulation of the reformer system was conducted to confirm mass flows and electrical power requirements.  Capital cost of the steam reformer system was estimated by a combination of scaling, industry quotes, and ground-up component cost estimation.  "]
[]
[null,"References:"]

{"sheet":"ProcessFlow","index":2,"n_rows":4078,"n_cols":3,"rows_kept":4078,"cut":false,"hidden":false,"merged":[[46,2,46,23],[1,7,1,9],[19,17,19,20],[20,17,20,20],[21,17,21,20],[7,2,7,23]]}
[]
[null,"Central Hydrogen Production - Process Flow Diagram"]
[]
[]
[]
[]
[null,null,"Process Flow Diagram"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"Stream Summaries"]
[]
[]
[null,null,"                       DIRECTED TECH                  Case Name: X:\\DOE ETHANOL 2007 DISTRIBUTED REFORMING\\REFORMER SYSTEMS ANALYSIS\\SYSTEM 06 - ETHANOL REFORMER 1500KGPERDAY V7 WITH GENERIC PREREFORMING.HSC "]
[null,null,"                       Calgary, Alberta                                                                                     "]
[null,null,"                       CANADA                         Unit Set: SI                                                          "]
[null,null,"                                                                                                                            "]
[null,null,"                                                      Date/Time: Thu Feb 21 15:40:15 2008                                   "]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"3 (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: 3                                                                   Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall                                                                                    "]
[null,null,"Vapour / Phase Fraction          ---                                                                                        "]
[null,null,"Temperature: (C)                 ---                                                                                        "]
[null,null,"Pressure: (kPa)                  ---                                                                                        "]
[null,null,"Molar Flow (kgmole/h)            ---                                                                                        "]
[null,null,"Mass Flow (kg/h)                 ---                                                                                        "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    ---                                                                                        "]
[null,null,"Molar Enthalpy (kJ/kgmole)       ---                                                                                        "]
[null,null,"Molar Entropy (kJ/kgmole-C)      ---                                                                                        "]
[null,null,"Heat Flow (kJ/h)                 ---                                                                                        "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    ---                                                                                        "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall                                                                                    "]
[null,null,"Molecular Weight                 ---                                                                                        "]
[null,null,"Molar Density (kgmole/m3)        ---                                                                                        "]
[null,null,"Mass Density (kg/m3)             ---                                                                                        "]
[null,null,"Act. Volume Flow (m3/h)          ---                                                                                        "]
[null,null,"Mass Enthalpy (kJ/kg)            ---                                                                                        "]
[null,null,"Mass Entropy (kJ/kg-C)           ---                                                                                        "]
[null,null,"Heat Capacity (kJ/kgmole-C)      ---                                                                                        "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     ---                                                                                        "]
[null,null,"Lower Heating Value (kJ/kgmole)  ---                                                                                        "]
[null,null,"Mass Lower Heating Value (kJ/kg) ---                                                                                        "]
[null,null,"Phase Fraction [Vol. Basis]      ---                                                                                        "]
[null,null,"Phase Fraction [Mass Basis]      ---                                                                                        "]
[null,null,"Partial Pressure of CO2 (kPa)    0.0000                                                                                     "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000                                                                                     "]
[null,null,"Act. Gas Flow (ACT_m3/h)         ---                                                                                        "]
[null,null,"Avg. Liq. Density (kgmole/m3)    ---                                                                                        "]
[null,null,"Specific Heat (kJ/kgmole-C)      ---                                                                                        "]
[null,null,"Std. Gas Flow (STD_m3/h)         ---                                                                                        "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) ---                                                                                       "]
[null,null,"Act. Liq. Flow (m3/s)            ---                                                                                        "]
[null,null,"Z Factor                         ---                                                                                        "]
[null,null,"Watson K                         ---                                                                                        "]
[null,null,"User Property                    ---                                                                                        "]
[null,null,"Cp/(Cp - R)                      ---                                                                                        "]
[null,null,"Cp/Cv                            ---                                                                                        "]
[null,null,"Heat of Vap. (kJ/kgmole)         ---                                                                                        "]
[null,null,"Kinematic Viscosity (cSt)        ---                                                                                        "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) ---                                                                                       "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) ---                                                                                       "]
[null,null,"Liquid Fraction                  ---                                                                                        "]
[null,null,"Molar Volume (m3/kgmole)         ---                                                                                        "]
[null,null,"Mass Heat of Vap. (kJ/kg)        ---                                                                                        "]
[null,null,"Phase Fraction [Molar Basis]     ---                                                                                        "]
[null,null,"Surface Tension (dyne/cm)        ---                                                                                        "]
[null,null,"Thermal Conductivity (W/m-K)     ---                                                                                        "]
[null,null,"Viscosity (cP)                   ---                                                                                        "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    ---                                                                                        "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   ---                                                                                        "]
[null,null,"Cv (kJ/kgmole-C)                 ---                                                                                        "]
[null,null,"Mass Cv (kJ/kg-C)                ---                                                                                        "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   ---                                                                                        "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  ---                                                                                        "]
[null,null,"Cp/Cv (Ent. Method)              ---                                                                                        "]
[null,null,"Reid VP at 37.8 C (kPa)          ---                                                                                        "]
[null,null,"True VP at 37.8 C (kPa)          ---                                                                                        "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) ---                                                                                       "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000                                                                                     "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"( No compositions have been calculated for this stream )                                                                    "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Adiabatic flame (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: Adiabatic flame                                                     Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase      Liquid Phase      Aqueous Phase                        "]
[null,null,"Vapour / Phase Fraction          1.0000            1.0000            0.0000            0.0000                               "]
[null,null,"Temperature: (C)                 949.1             949.1             949.1             949.1                                "]
[null,null,"Pressure: (kPa)                  110.9             110.9             110.9             110.9                                "]
[null,null,"Molar Flow (kgmole/h)            241.2             241.2             0.0000            0.0000                               "]
[null,null,"Mass Flow (kg/h)                 7018              7018              0.0000            0.0000                               "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    8.213             8.213             0.0000            0.0000                               "]
[null,null,"Molar Enthalpy (kJ/kgmole)       -1.426e+004       -1.426e+004       -1.426e+004       -1.426e+004                          "]
[null,null,"Molar Entropy (kJ/kgmole-C)      213.4             213.4             213.4             213.4                                "]
[null,null,"Heat Flow (kJ/h)                 -3.439e+006       -3.439e+006       0.0000            0.0000                               "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    ---               ---               0.0000            0.0000                               "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase      Liquid Phase      Aqueous Phase                        "]
[null,null,"Molecular Weight                 29.10             29.10             29.10             29.10                                "]
[null,null,"Molar Density (kgmole/m3)        1.091e-002        1.091e-002        1.091e-002        1.091e-002                           "]
[null,null,"Mass Density (kg/m3)             0.3174            0.3174            0.3174            0.3174                               "]
[null,null,"Act. Volume Flow (m3/h)          2.211e+004        2.211e+004        0.0000            0.0000                               "]
[null,null,"Mass Enthalpy (kJ/kg)            -490.0            -490.0            -490.0            -490.0                               "]
[null,null,"Mass Entropy (kJ/kg-C)           7.333             7.333             7.333             7.333                                "]
[null,null,"Heat Capacity (kJ/kgmole-C)      36.46             36.46             36.46             36.46                                "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     1.253             1.253             1.253             1.253                                "]
[null,null,"Lower Heating Value (kJ/kgmole)  8.541e-004        8.541e-004        8.541e-004        8.541e-004                           "]
[null,null,"Mass Lower Heating Value (kJ/kg) 2.935e-005        2.935e-005        2.935e-005        2.935e-005                           "]
[null,null,"Phase Fraction [Vol. Basis]      ---               1.000             ---               ---                                  "]
[null,null,"Phase Fraction [Mass Basis]      2.122e-314        1.000             0.0000            0.0000                               "]
[null,null,"Partial Pressure of CO2 (kPa)    8.175             ---               ---               ---                                  "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000            0.0000            0.0000                               "]
[null,null,"Act. Gas Flow (ACT_m3/h)         2.211e+004        2.211e+004        ---               ---                                  "]
[null,null,"Avg. Liq. Density (kgmole/m3)    29.36             29.36             29.36             29.36                                "]
[null,null,"Specific Heat (kJ/kgmole-C)      36.46             36.46             36.46             36.46                                "]
[null,null,"Std. Gas Flow (STD_m3/h)         5702              5702              0.0000            0.0000                               "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 854.4             854.4             854.4             854.4                               "]
[null,null,"Act. Liq. Flow (m3/s)            0.0000            ---               ---               0.0000                               "]
[null,null,"Z Factor                         ---               1.000             1.000             1.000                                "]
[null,null,"Watson K                         6.383             6.383             6.383             6.383                                "]
[null,null,"User Property                    ---               ---               ---               ---                                  "]
[null,null,"Cp/(Cp - R)                      1.295             1.295             1.295             1.295                                "]
[null,null,"Cp/Cv                            1.295             1.295             1.295             1.295                                "]
[null,null,"Heat of Vap. (kJ/kgmole)         1.857e+004        ---               ---               ---                                  "]
[null,null,"Kinematic Viscosity (cSt)        168.2             168.2             1.881             1.881                                "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) ---               ---               ---               ---                                 "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) ---               ---               0.0000            0.0000                              "]
[null,null,"Liquid Fraction                  0.0000            0.0000            1.000             1.000                                "]
[null,null,"Molar Volume (m3/kgmole)         91.68             91.68             91.68             91.68                                "]
[null,null,"Mass Heat of Vap. (kJ/kg)        638.3             ---               ---               ---                                  "]
[null,null,"Phase Fraction [Molar Basis]     1.0000            1.0000            0.0000            0.0000                               "]
[null,null,"Surface Tension (dyne/cm)        ---               ---               0.0000            0.0000                               "]
[null,null,"Thermal Conductivity (W/m-K)     7.944e-002        7.944e-002        5.375e-002        5.375e-002                           "]
[null,null,"Viscosity (cP)                   5.337e-002        5.337e-002        5.970e-004        5.970e-004                           "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    28.15             28.15             28.15             28.15                                "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   0.9673            0.9673            0.9673            0.9673                               "]
[null,null,"Cv (kJ/kgmole-C)                 28.15             28.15             28.15             28.15                                "]
[null,null,"Mass Cv (kJ/kg-C)                0.9673            0.9673            0.9673            0.9673                               "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   28.11             28.11             28.11             22.33                                "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  0.9660            0.9660            0.9660            0.7675                               "]
[null,null,"Cp/Cv (Ent. Method)              1.297             1.297             1.297             1.633                                "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---               ---               ---                                  "]
[null,null,"True VP at 37.8 C (kPa)          1.874e+005        1.874e+005        1.874e+005        1.874e+005                           "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 0.0000            0.0000            0.0000            0.0000                              "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---               ---               ---                                  "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 1.0000    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                34.4900          0.1430           1103.6812        0.1573           0.9701           0.1181           "]
[null,null,"Nitrogen              172.8879         0.7169           4843.1080        0.6901           6.0060           0.7313           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   15.9987          0.0663           288.2173         0.0411           0.2888           0.0352           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   17.7814          0.0737           782.5555         0.1115           0.9482           0.1154           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 241.1580         1.0000           7017.5621        1.0000           8.2131           1.0000           "]
[null,null,"Vapour Phase                                                                                      Phase Fraction 1.000      "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                34.4900          0.1430           1103.6812        0.1573           0.9701           0.1181           "]
[null,null,"Nitrogen              172.8879         0.7169           4843.1080        0.6901           6.0060           0.7313           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   15.9987          0.0663           288.2173         0.0411           0.2888           0.0352           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   17.7814          0.0737           782.5555         0.1115           0.9482           0.1154           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 241.1580         1.0000           7017.5621        1.0000           8.2131           1.0000           "]
[null,null,"Liquid Phase                                                                                      Phase Fraction 0.0000     "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.1430           0.0000           0.1573           0.0000           0.1181           "]
[null,null,"Nitrogen              0.0000           0.7169           0.0000           0.6901           0.0000           0.7313           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   0.0000           0.0663           0.0000           0.0411           0.0000           0.0352           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0737           0.0000           0.1115           0.0000           0.1154           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 0.0000           1.0000           0.0000           1.0000           0.0000           1.0000           "]
[null,null,"Aqueous Phase                                                                                     Phase Fraction 0.0000     "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.1430           0.0000           0.1573           0.0000           0.1181           "]
[null,null,"Nitrogen              0.0000           0.7169           0.0000           0.6901           0.0000           0.7313           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   0.0000           0.0663           0.0000           0.0411           0.0000           0.0352           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0737           0.0000           0.1115           0.0000           0.1154           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 0.0000           1.0000           0.0000           1.0000           0.0000           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"blown air (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: blown air                                                           Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase                                                             "]
[null,null,"Vapour / Phase Fraction          1.0000            1.0000                                                                   "]
[null,null,"Temperature: (C)                 40.48             40.48                                                                    "]
[null,null,"Pressure: (kPa)                  115.1             115.1                                                                    "]
[null,null,"Molar Flow (kgmole/h)            218.6             218.6                                                                    "]
[null,null,"Mass Flow (kg/h)                 6307              6307                                                                     "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    7.293             7.293                                                                    "]
[null,null,"Molar Enthalpy (kJ/kgmole)       442.4             442.4                                                                    "]
[null,null,"Molar Entropy (kJ/kgmole-C)      163.8             163.8                                                                    "]
[null,null,"Heat Flow (kJ/h)                 9.671e+004        9.671e+004                                                               "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    ---               ---                                                                      "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase                                                             "]
[null,null,"Molecular Weight                 28.85             28.85                                                                    "]
[null,null,"Molar Density (kgmole/m3)        4.417e-002        4.417e-002                                                               "]
[null,null,"Mass Density (kg/m3)             1.274             1.274                                                                    "]
[null,null,"Act. Volume Flow (m3/h)          4950              4950                                                                     "]
[null,null,"Mass Enthalpy (kJ/kg)            15.33             15.33                                                                    "]
[null,null,"Mass Entropy (kJ/kg-C)           5.678             5.678                                                                    "]
[null,null,"Heat Capacity (kJ/kgmole-C)      29.19             29.19                                                                    "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     1.012             1.012                                                                    "]
[null,null,"Lower Heating Value (kJ/kgmole)  0.0000            0.0000                                                                   "]
[null,null,"Mass Lower Heating Value (kJ/kg) ---               ---                                                                      "]
[null,null,"Phase Fraction [Vol. Basis]      ---               1.000                                                                    "]
[null,null,"Phase Fraction [Mass Basis]      4.941e-324        1.000                                                                    "]
[null,null,"Partial Pressure of CO2 (kPa)    0.0000            ---                                                                      "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000                                                                   "]
[null,null,"Act. Gas Flow (ACT_m3/h)         4950              4950                                                                     "]
[null,null,"Avg. Liq. Density (kgmole/m3)    29.98             29.98                                                                    "]
[null,null,"Specific Heat (kJ/kgmole-C)      29.19             29.19                                                                    "]
[null,null,"Std. Gas Flow (STD_m3/h)         5169              5169                                                                     "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 864.8             864.8                                                                   "]
[null,null,"Act. Liq. Flow (m3/s)            ---               ---                                                                      "]
[null,null,"Z Factor                         0.9995            0.9995                                                                   "]
[null,null,"Watson K                         6.043             6.043                                                                    "]
[null,null,"User Property                    ---               ---                                                                      "]
[null,null,"Cp/(Cp - R)                      1.398             1.398                                                                    "]
[null,null,"Cp/Cv                            1.401             1.401                                                                    "]
[null,null,"Heat of Vap. (kJ/kgmole)         5862              ---                                                                      "]
[null,null,"Kinematic Viscosity (cSt)        15.35             15.35                                                                    "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) ---               ---                                                                     "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) ---               ---                                                                     "]
[null,null,"Liquid Fraction                  0.0000            0.0000                                                                   "]
[null,null,"Molar Volume (m3/kgmole)         22.64             22.64                                                                    "]
[null,null,"Mass Heat of Vap. (kJ/kg)        203.2             ---                                                                      "]
[null,null,"Phase Fraction [Molar Basis]     1.0000            1.0000                                                                   "]
[null,null,"Surface Tension (dyne/cm)        ---               ---                                                                      "]
[null,null,"Thermal Conductivity (W/m-K)     2.695e-002        2.695e-002                                                               "]
[null,null,"Viscosity (cP)                   1.956e-002        1.956e-002                                                               "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    20.88             20.88                                                                    "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   0.7238            0.7238                                                                   "]
[null,null,"Cv (kJ/kgmole-C)                 20.83             20.83                                                                    "]
[null,null,"Mass Cv (kJ/kg-C)                0.7222            0.7222                                                                   "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   20.80             20.80                                                                    "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  0.7209            0.7209                                                                   "]
[null,null,"Cp/Cv (Ent. Method)              1.404             1.404                                                                    "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---                                                                      "]
[null,null,"True VP at 37.8 C (kPa)          ---               ---                                                                      "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 0.0000            0.0000                                                                  "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---                                                                      "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 1.0000    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                45.7375          0.2092           1463.6010        0.2321           1.2865           0.1764           "]
[null,null,"Nitrogen              172.8879         0.7908           4843.1080        0.7679           6.0060           0.8236           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 218.6254         1.0000           6306.7090        1.0000           7.2925           1.0000           "]
[null,null,"Vapour Phase                                                                                      Phase Fraction 1.000      "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                45.7375          0.2092           1463.6010        0.2321           1.2865           0.1764           "]
[null,null,"Nitrogen              172.8879         0.7908           4843.1080        0.7679           6.0060           0.8236           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 218.6254         1.0000           6306.7090        1.0000           7.2925           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"bs (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: bs                                                                  Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase      Liquid Phase      Aqueous Phase                        "]
[null,null,"Vapour / Phase Fraction          0.0000            0.0000            0.5000            0.5000                               "]
[null,null,"Temperature: (C)                 949.1             949.1             949.1             949.1                                "]
[null,null,"Pressure: (kPa)                  110.9             110.9             110.9             110.9                                "]
[null,null,"Molar Flow (kgmole/h)            0.0000            0.0000            0.0000            0.0000                               "]
[null,null,"Mass Flow (kg/h)                 0.0000            0.0000            0.0000            0.0000                               "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    0.0000            0.0000            0.0000            0.0000                               "]
[null,null,"Molar Enthalpy (kJ/kgmole)       -1.426e+004       -1.426e+004       -1.426e+004       -1.426e+004                          "]
[null,null,"Molar Entropy (kJ/kgmole-C)      213.4             213.4             213.4             213.4                                "]
[null,null,"Heat Flow (kJ/h)                 0.0000            0.0000            0.0000            0.0000                               "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    0.0000            0.0000            0.0000            0.0000                               "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase      Liquid Phase      Aqueous Phase                        "]
[null,null,"Molecular Weight                 29.10             29.10             29.10             29.10                                "]
[null,null,"Molar Density (kgmole/m3)        1.091e-002        1.091e-002        1.091e-002        1.091e-002                           "]
[null,null,"Mass Density (kg/m3)             0.3174            0.3174            0.3174            0.3174                               "]
[null,null,"Act. Volume Flow (m3/h)          0.0000            0.0000            0.0000            0.0000                               "]
[null,null,"Mass Enthalpy (kJ/kg)            -490.0            -490.0            -490.0            -490.0                               "]
[null,null,"Mass Entropy (kJ/kg-C)           7.333             7.333             7.333             7.333                                "]
[null,null,"Heat Capacity (kJ/kgmole-C)      36.46             36.46             36.46             36.46                                "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     1.253             1.253             1.253             1.253                                "]
[null,null,"Lower Heating Value (kJ/kgmole)  8.541e-004        8.541e-004        8.541e-004        8.541e-004                           "]
[null,null,"Mass Lower Heating Value (kJ/kg) 2.935e-005        2.935e-005        2.935e-005        2.935e-005                           "]
[null,null,"Phase Fraction [Vol. Basis]      ---               ---               0.5000            0.5000                               "]
[null,null,"Phase Fraction [Mass Basis]      2.122e-314        0.0000            0.5000            0.5000                               "]
[null,null,"Partial Pressure of CO2 (kPa)    0.0000            ---               ---               ---                                  "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000            0.0000            0.0000                               "]
[null,null,"Act. Gas Flow (ACT_m3/h)         ---               ---               ---               ---                                  "]
[null,null,"Avg. Liq. Density (kgmole/m3)    ---               ---               ---               ---                                  "]
[null,null,"Specific Heat (kJ/kgmole-C)      36.46             36.46             36.46             36.46                                "]
[null,null,"Std. Gas Flow (STD_m3/h)         0.0000            0.0000            0.0000            0.0000                               "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 854.4             854.4             854.4             854.4                               "]
[null,null,"Act. Liq. Flow (m3/s)            0.0000            ---               0.0000            0.0000                               "]
[null,null,"Z Factor                         ---               1.000             1.000             1.000                                "]
[null,null,"Watson K                         6.383             6.383             6.383             6.383                                "]
[null,null,"User Property                    ---               ---               ---               ---                                  "]
[null,null,"Cp/(Cp - R)                      1.295             1.295             1.295             1.295                                "]
[null,null,"Cp/Cv                            1.295             1.295             1.295             1.295                                "]
[null,null,"Heat of Vap. (kJ/kgmole)         1.857e+004        ---               ---               ---                                  "]
[null,null,"Kinematic Viscosity (cSt)        11.38             168.2             1.881             1.881                                "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) ---               ---               ---               ---                                 "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) 0.0000            0.0000            0.0000            0.0000                              "]
[null,null,"Liquid Fraction                  1.000             0.0000            1.000             1.000                                "]
[null,null,"Molar Volume (m3/kgmole)         91.68             91.68             91.68             91.68                                "]
[null,null,"Mass Heat of Vap. (kJ/kg)        638.3             ---               ---               ---                                  "]
[null,null,"Phase Fraction [Molar Basis]     0.0000            0.0000            0.5000            0.5000                               "]
[null,null,"Surface Tension (dyne/cm)        ---               ---               0.0000            0.0000                               "]
[null,null,"Thermal Conductivity (W/m-K)     5.375e-002        7.944e-002        5.375e-002        5.375e-002                           "]
[null,null,"Viscosity (cP)                   3.612e-003        5.337e-002        5.970e-004        5.970e-004                           "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    28.15             28.15             28.15             28.15                                "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   0.9673            0.9673            0.9673            0.9673                               "]
[null,null,"Cv (kJ/kgmole-C)                 28.15             28.15             28.15             28.15                                "]
[null,null,"Mass Cv (kJ/kg-C)                0.9673            0.9673            0.9673            0.9673                               "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   ---               28.11             28.11             22.33                                "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  ---               0.9660            0.9660            0.7675                               "]
[null,null,"Cp/Cv (Ent. Method)              ---               1.297             1.297             1.633                                "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---               ---               ---                                  "]
[null,null,"True VP at 37.8 C (kPa)          1.874e+005        1.874e+005        1.874e+005        1.874e+005                           "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 0.0000            0.0000            0.0000            0.0000                              "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---               ---               ---                                  "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 0.0000    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.1430           0.0000           0.1573           0.0000           0.1181           "]
[null,null,"Nitrogen              0.0000           0.7169           0.0000           0.6901           0.0000           0.7313           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   0.0000           0.0663           0.0000           0.0411           0.0000           0.0352           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0737           0.0000           0.1115           0.0000           0.1154           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 0.0000           1.0000           0.0000           1.0000           0.0000           1.0000           "]
[null,null,"Vapour Phase                                                                                      Phase Fraction 0.0000     "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.1430           0.0000           0.1573           0.0000           0.1181           "]
[null,null,"Nitrogen              0.0000           0.7169           0.0000           0.6901           0.0000           0.7313           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   0.0000           0.0663           0.0000           0.0411           0.0000           0.0352           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0737           0.0000           0.1115           0.0000           0.1154           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 0.0000           1.0000           0.0000           1.0000           0.0000           1.0000           "]
[null,null,"Liquid Phase                                                                                      Phase Fraction 0.5000     "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.1430           0.0000           0.1573           0.0000           0.1181           "]
[null,null,"Nitrogen              0.0000           0.7169           0.0000           0.6901           0.0000           0.7313           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   0.0000           0.0663           0.0000           0.0411           0.0000           0.0352           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0737           0.0000           0.1115           0.0000           0.1154           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 0.0000           1.0000           0.0000           1.0000           0.0000           1.0000           "]
[null,null,"Aqueous Phase                                                                                     Phase Fraction 0.5000     "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.1430           0.0000           0.1573           0.0000           0.1181           "]
[null,null,"Nitrogen              0.0000           0.7169           0.0000           0.6901           0.0000           0.7313           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   0.0000           0.0663           0.0000           0.0411           0.0000           0.0352           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0737           0.0000           0.1115           0.0000           0.1154           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 0.0000           1.0000           0.0000           1.0000           0.0000           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"bs2 (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: bs2                                                                 Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall                                                                                    "]
[null,null,"Vapour / Phase Fraction          ---                                                                                        "]
[null,null,"Temperature: (C)                 ---                                                                                        "]
[null,null,"Pressure: (kPa)                  ---                                                                                        "]
[null,null,"Molar Flow (kgmole/h)            ---                                                                                        "]
[null,null,"Mass Flow (kg/h)                 ---                                                                                        "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    ---                                                                                        "]
[null,null,"Molar Enthalpy (kJ/kgmole)       ---                                                                                        "]
[null,null,"Molar Entropy (kJ/kgmole-C)      ---                                                                                        "]
[null,null,"Heat Flow (kJ/h)                 ---                                                                                        "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    ---                                                                                        "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall                                                                                    "]
[null,null,"Molecular Weight                 ---                                                                                        "]
[null,null,"Molar Density (kgmole/m3)        ---                                                                                        "]
[null,null,"Mass Density (kg/m3)             ---                                                                                        "]
[null,null,"Act. Volume Flow (m3/h)          ---                                                                                        "]
[null,null,"Mass Enthalpy (kJ/kg)            ---                                                                                        "]
[null,null,"Mass Entropy (kJ/kg-C)           ---                                                                                        "]
[null,null,"Heat Capacity (kJ/kgmole-C)      ---                                                                                        "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     ---                                                                                        "]
[null,null,"Lower Heating Value (kJ/kgmole)  ---                                                                                        "]
[null,null,"Mass Lower Heating Value (kJ/kg) ---                                                                                        "]
[null,null,"Phase Fraction [Vol. Basis]      ---                                                                                        "]
[null,null,"Phase Fraction [Mass Basis]      ---                                                                                        "]
[null,null,"Partial Pressure of CO2 (kPa)    0.0000                                                                                     "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000                                                                                     "]
[null,null,"Act. Gas Flow (ACT_m3/h)         ---                                                                                        "]
[null,null,"Avg. Liq. Density (kgmole/m3)    ---                                                                                        "]
[null,null,"Specific Heat (kJ/kgmole-C)      ---                                                                                        "]
[null,null,"Std. Gas Flow (STD_m3/h)         ---                                                                                        "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) ---                                                                                       "]
[null,null,"Act. Liq. Flow (m3/s)            ---                                                                                        "]
[null,null,"Z Factor                         ---                                                                                        "]
[null,null,"Watson K                         ---                                                                                        "]
[null,null,"User Property                    ---                                                                                        "]
[null,null,"Cp/(Cp - R)                      ---                                                                                        "]
[null,null,"Cp/Cv                            ---                                                                                        "]
[null,null,"Heat of Vap. (kJ/kgmole)         ---                                                                                        "]
[null,null,"Kinematic Viscosity (cSt)        ---                                                                                        "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) ---                                                                                       "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) ---                                                                                       "]
[null,null,"Liquid Fraction                  ---                                                                                        "]
[null,null,"Molar Volume (m3/kgmole)         ---                                                                                        "]
[null,null,"Mass Heat of Vap. (kJ/kg)        ---                                                                                        "]
[null,null,"Phase Fraction [Molar Basis]     ---                                                                                        "]
[null,null,"Surface Tension (dyne/cm)        ---                                                                                        "]
[null,null,"Thermal Conductivity (W/m-K)     ---                                                                                        "]
[null,null,"Viscosity (cP)                   ---                                                                                        "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    ---                                                                                        "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   ---                                                                                        "]
[null,null,"Cv (kJ/kgmole-C)                 ---                                                                                        "]
[null,null,"Mass Cv (kJ/kg-C)                ---                                                                                        "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   ---                                                                                        "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  ---                                                                                        "]
[null,null,"Cp/Cv (Ent. Method)              ---                                                                                        "]
[null,null,"Reid VP at 37.8 C (kPa)          ---                                                                                        "]
[null,null,"True VP at 37.8 C (kPa)          ---                                                                                        "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) ---                                                                                       "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000                                                                                     "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"( No compositions have been calculated for this stream )                                                                    "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Burner Gas exiting Reformer (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: Burner Gas exiting Reformer                                         Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase                                                             "]
[null,null,"Vapour / Phase Fraction          1.0000            1.0000                                                                   "]
[null,null,"Temperature: (C)                 561.5             561.5                                                                    "]
[null,null,"Pressure: (kPa)                  108.9             108.9                                                                    "]
[null,null,"Molar Flow (kgmole/h)            241.2             241.2                                                                    "]
[null,null,"Mass Flow (kg/h)                 7018              7018                                                                     "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    8.213             8.213                                                                    "]
[null,null,"Molar Enthalpy (kJ/kgmole)       -2.794e+004       -2.794e+004                                                              "]
[null,null,"Molar Entropy (kJ/kgmole-C)      200.1             200.1                                                                    "]
[null,null,"Heat Flow (kJ/h)                 -6.738e+006       -6.738e+006                                                              "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    ---               ---                                                                      "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase                                                             "]
[null,null,"Molecular Weight                 29.10             29.10                                                                    "]
[null,null,"Molar Density (kgmole/m3)        1.568e-002        1.568e-002                                                               "]
[null,null,"Mass Density (kg/m3)             0.4564            0.4564                                                                   "]
[null,null,"Act. Volume Flow (m3/h)          1.538e+004        1.538e+004                                                               "]
[null,null,"Mass Enthalpy (kJ/kg)            -960.1            -960.1                                                                   "]
[null,null,"Mass Entropy (kJ/kg-C)           6.876             6.876                                                                    "]
[null,null,"Heat Capacity (kJ/kgmole-C)      33.93             33.93                                                                    "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     1.166             1.166                                                                    "]
[null,null,"Lower Heating Value (kJ/kgmole)  8.541e-004        8.541e-004                                                               "]
[null,null,"Mass Lower Heating Value (kJ/kg) 2.935e-005        2.935e-005                                                               "]
[null,null,"Phase Fraction [Vol. Basis]      ---               1.000                                                                    "]
[null,null,"Phase Fraction [Mass Basis]      4.941e-324        1.000                                                                    "]
[null,null,"Partial Pressure of CO2 (kPa)    8.027             ---                                                                      "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000                                                                   "]
[null,null,"Act. Gas Flow (ACT_m3/h)         1.538e+004        1.538e+004                                                               "]
[null,null,"Avg. Liq. Density (kgmole/m3)    29.36             29.36                                                                    "]
[null,null,"Specific Heat (kJ/kgmole-C)      33.93             33.93                                                                    "]
[null,null,"Std. Gas Flow (STD_m3/h)         5702              5702                                                                     "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 854.4             854.4                                                                   "]
[null,null,"Act. Liq. Flow (m3/s)            ---               ---                                                                      "]
[null,null,"Z Factor                         1.000             1.000                                                                    "]
[null,null,"Watson K                         6.383             6.383                                                                    "]
[null,null,"User Property                    ---               ---                                                                      "]
[null,null,"Cp/(Cp - R)                      1.325             1.325                                                                    "]
[null,null,"Cp/Cv                            1.325             1.325                                                                    "]
[null,null,"Heat of Vap. (kJ/kgmole)         1.859e+004        ---                                                                      "]
[null,null,"Kinematic Viscosity (cSt)        83.88             83.88                                                                    "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) ---               ---                                                                     "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) ---               ---                                                                     "]
[null,null,"Liquid Fraction                  0.0000            0.0000                                                                   "]
[null,null,"Molar Volume (m3/kgmole)         63.76             63.76                                                                    "]
[null,null,"Mass Heat of Vap. (kJ/kg)        638.8             ---                                                                      "]
[null,null,"Phase Fraction [Molar Basis]     1.0000            1.0000                                                                   "]
[null,null,"Surface Tension (dyne/cm)        ---               ---                                                                      "]
[null,null,"Thermal Conductivity (W/m-K)     5.848e-002        5.848e-002                                                               "]
[null,null,"Viscosity (cP)                   3.828e-002        3.828e-002                                                               "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    25.61             25.61                                                                    "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   0.8802            0.8802                                                                   "]
[null,null,"Cv (kJ/kgmole-C)                 25.61             25.61                                                                    "]
[null,null,"Mass Cv (kJ/kg-C)                0.8801            0.8801                                                                   "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   31.14             31.14                                                                    "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  1.070             1.070                                                                    "]
[null,null,"Cp/Cv (Ent. Method)              1.090             1.090                                                                    "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---                                                                      "]
[null,null,"True VP at 37.8 C (kPa)          1.874e+005        1.874e+005                                                               "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 0.0000            0.0000                                                                  "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---                                                                      "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 1.0000    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                34.4900          0.1430           1103.6812        0.1573           0.9701           0.1181           "]
[null,null,"Nitrogen              172.8879         0.7169           4843.1080        0.6901           6.0060           0.7313           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   15.9987          0.0663           288.2173         0.0411           0.2888           0.0352           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   17.7814          0.0737           782.5555         0.1115           0.9482           0.1154           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 241.1580         1.0000           7017.5621        1.0000           8.2131           1.0000           "]
[null,null,"Vapour Phase                                                                                      Phase Fraction 1.000      "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                34.4900          0.1430           1103.6812        0.1573           0.9701           0.1181           "]
[null,null,"Nitrogen              172.8879         0.7169           4843.1080        0.6901           6.0060           0.7313           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   15.9987          0.0663           288.2173         0.0411           0.2888           0.0352           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   17.7814          0.0737           782.5555         0.1115           0.9482           0.1154           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 241.1580         1.0000           7017.5621        1.0000           8.2131           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"burner-Liquid (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: burner-Liquid                                                       Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall                                                                                    "]
[null,null,"Vapour / Phase Fraction          ---                                                                                        "]
[null,null,"Temperature: (C)                 ---                                                                                        "]
[null,null,"Pressure: (kPa)                  ---                                                                                        "]
[null,null,"Molar Flow (kgmole/h)            ---                                                                                        "]
[null,null,"Mass Flow (kg/h)                 ---                                                                                        "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    ---                                                                                        "]
[null,null,"Molar Enthalpy (kJ/kgmole)       ---                                                                                        "]
[null,null,"Molar Entropy (kJ/kgmole-C)      ---                                                                                        "]
[null,null,"Heat Flow (kJ/h)                 ---                                                                                        "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    ---                                                                                        "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall                                                                                    "]
[null,null,"Molecular Weight                 ---                                                                                        "]
[null,null,"Molar Density (kgmole/m3)        ---                                                                                        "]
[null,null,"Mass Density (kg/m3)             ---                                                                                        "]
[null,null,"Act. Volume Flow (m3/h)          ---                                                                                        "]
[null,null,"Mass Enthalpy (kJ/kg)            ---                                                                                        "]
[null,null,"Mass Entropy (kJ/kg-C)           ---                                                                                        "]
[null,null,"Heat Capacity (kJ/kgmole-C)      ---                                                                                        "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     ---                                                                                        "]
[null,null,"Lower Heating Value (kJ/kgmole)  ---                                                                                        "]
[null,null,"Mass Lower Heating Value (kJ/kg) ---                                                                                        "]
[null,null,"Phase Fraction [Vol. Basis]      ---                                                                                        "]
[null,null,"Phase Fraction [Mass Basis]      ---                                                                                        "]
[null,null,"Partial Pressure of CO2 (kPa)    0.0000                                                                                     "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000                                                                                     "]
[null,null,"Act. Gas Flow (ACT_m3/h)         ---                                                                                        "]
[null,null,"Avg. Liq. Density (kgmole/m3)    ---                                                                                        "]
[null,null,"Specific Heat (kJ/kgmole-C)      ---                                                                                        "]
[null,null,"Std. Gas Flow (STD_m3/h)         ---                                                                                        "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) ---                                                                                       "]
[null,null,"Act. Liq. Flow (m3/s)            ---                                                                                        "]
[null,null,"Z Factor                         ---                                                                                        "]
[null,null,"Watson K                         ---                                                                                        "]
[null,null,"User Property                    ---                                                                                        "]
[null,null,"Cp/(Cp - R)                      ---                                                                                        "]
[null,null,"Cp/Cv                            ---                                                                                        "]
[null,null,"Heat of Vap. (kJ/kgmole)         ---                                                                                        "]
[null,null,"Kinematic Viscosity (cSt)        ---                                                                                        "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) ---                                                                                       "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) ---                                                                                       "]
[null,null,"Liquid Fraction                  ---                                                                                        "]
[null,null,"Molar Volume (m3/kgmole)         ---                                                                                        "]
[null,null,"Mass Heat of Vap. (kJ/kg)        ---                                                                                        "]
[null,null,"Phase Fraction [Molar Basis]     ---                                                                                        "]
[null,null,"Surface Tension (dyne/cm)        ---                                                                                        "]
[null,null,"Thermal Conductivity (W/m-K)     ---                                                                                        "]
[null,null,"Viscosity (cP)                   ---                                                                                        "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    ---                                                                                        "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   ---                                                                                        "]
[null,null,"Cv (kJ/kgmole-C)                 ---                                                                                        "]
[null,null,"Mass Cv (kJ/kg-C)                ---                                                                                        "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   ---                                                                                        "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  ---                                                                                        "]
[null,null,"Cp/Cv (Ent. Method)              ---                                                                                        "]
[null,null,"Reid VP at 37.8 C (kPa)          ---                                                                                        "]
[null,null,"True VP at 37.8 C (kPa)          ---                                                                                        "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) ---                                                                                       "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000                                                                                     "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"( No compositions have been calculated for this stream )                                                                    "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Co-Fired Ethanol (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: Co-Fired Ethanol                                                    Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Liquid Phase                                                             "]
[null,null,"Vapour / Phase Fraction          0.0000            1.0000                                                                   "]
[null,null,"Temperature: (C)                 25.00             25.00                                                                    "]
[null,null,"Pressure: (kPa)                  115.1             115.1                                                                    "]
[null,null,"Molar Flow (kgmole/h)            1.238             1.238                                                                    "]
[null,null,"Mass Flow (kg/h)                 57.03             57.03                                                                    "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    7.165e-002        7.165e-002                                                               "]
[null,null,"Molar Enthalpy (kJ/kgmole)       -2.789e+005       -2.789e+005                                                              "]
[null,null,"Molar Entropy (kJ/kgmole-C)      -6.461            -6.461                                                                   "]
[null,null,"Heat Flow (kJ/h)                 -3.452e+005       -3.452e+005                                                              "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    7.159e-002        7.159e-002                                                               "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Liquid Phase                                                             "]
[null,null,"Molecular Weight                 46.07             46.07                                                                    "]
[null,null,"Molar Density (kgmole/m3)        17.10             17.10                                                                    "]
[null,null,"Mass Density (kg/m3)             787.6             787.6                                                                    "]
[null,null,"Act. Volume Flow (m3/h)          7.241e-002        7.241e-002                                                               "]
[null,null,"Mass Enthalpy (kJ/kg)            -6053             -6053                                                                    "]
[null,null,"Mass Entropy (kJ/kg-C)           -0.1402           -0.1402                                                                  "]
[null,null,"Heat Capacity (kJ/kgmole-C)      142.5             142.5                                                                    "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     3.093             3.093                                                                    "]
[null,null,"Lower Heating Value (kJ/kgmole)  1.235e+006        1.235e+006                                                               "]
[null,null,"Mass Lower Heating Value (kJ/kg) 2.682e+004        2.682e+004                                                               "]
[null,null,"Phase Fraction [Vol. Basis]      ---               1.000                                                                    "]
[null,null,"Phase Fraction [Mass Basis]      2.122e-314        1.000                                                                    "]
[null,null,"Partial Pressure of CO2 (kPa)    0.0000            ---                                                                      "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000                                                                   "]
[null,null,"Act. Gas Flow (ACT_m3/h)         ---               ---                                                                      "]
[null,null,"Avg. Liq. Density (kgmole/m3)    17.28             17.28                                                                    "]
[null,null,"Specific Heat (kJ/kgmole-C)      142.5             142.5                                                                    "]
[null,null,"Std. Gas Flow (STD_m3/h)         29.27             29.27                                                                    "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 796.0             796.0                                                                   "]
[null,null,"Act. Liq. Flow (m3/s)            2.011e-005        2.011e-005                                                               "]
[null,null,"Z Factor                         2.716e-003        2.716e-003                                                               "]
[null,null,"Watson K                         10.76             10.76                                                                    "]
[null,null,"User Property                    ---               ---                                                                      "]
[null,null,"Cp/(Cp - R)                      1.062             1.062                                                                    "]
[null,null,"Cp/Cv                            1.104             1.104                                                                    "]
[null,null,"Heat of Vap. (kJ/kgmole)         3.920e+004        ---                                                                      "]
[null,null,"Kinematic Viscosity (cSt)        1.222             1.222                                                                    "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) 796.6             796.6                                                                   "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) 7.159e-002        7.159e-002                                                              "]
[null,null,"Liquid Fraction                  1.000             1.000                                                                    "]
[null,null,"Molar Volume (m3/kgmole)         5.849e-002        5.849e-002                                                               "]
[null,null,"Mass Heat of Vap. (kJ/kg)        850.9             ---                                                                      "]
[null,null,"Phase Fraction [Molar Basis]     0.0000            1.0000                                                                   "]
[null,null,"Surface Tension (dyne/cm)        22.10             22.10                                                                    "]
[null,null,"Thermal Conductivity (W/m-K)     0.1574            0.1574                                                                   "]
[null,null,"Viscosity (cP)                   0.9626            0.9626                                                                   "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    134.2             134.2                                                                    "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   2.913             2.913                                                                    "]
[null,null,"Cv (kJ/kgmole-C)                 129.1             129.1                                                                    "]
[null,null,"Mass Cv (kJ/kg-C)                2.803             2.803                                                                    "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   ---               ---                                                                      "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  ---               ---                                                                      "]
[null,null,"Cp/Cv (Ent. Method)              ---               ---                                                                      "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---                                                                      "]
[null,null,"True VP at 37.8 C (kPa)          15.74             15.74                                                                    "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 7.159e-002        7.159e-002                                                              "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---                                                                      "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 0.0000    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               1.2380           1.0000           57.0345          1.0000           0.0717           1.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 1.2380           1.0000           57.0345          1.0000           0.0717           1.0000           "]
[null,null,"Liquid Phase                                                                                      Phase Fraction 1.000      "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               1.2380           1.0000           57.0345          1.0000           0.0717           1.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 1.2380           1.0000           57.0345          1.0000           0.0717           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"cold flue gas (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: cold flue gas                                                       Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase                                                             "]
[null,null,"Vapour / Phase Fraction          1.0000            1.0000                                                                   "]
[null,null,"Temperature: (C)                 109.8             109.8                                                                    "]
[null,null,"Pressure: (kPa)                  107.8             107.8                                                                    "]
[null,null,"Molar Flow (kgmole/h)            241.2             241.2                                                                    "]
[null,null,"Mass Flow (kg/h)                 7018              7018                                                                     "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    8.213             8.213                                                                    "]
[null,null,"Molar Enthalpy (kJ/kgmole)       -4.247e+004       -4.247e+004                                                              "]
[null,null,"Molar Entropy (kJ/kgmole-C)      175.3             175.3                                                                    "]
[null,null,"Heat Flow (kJ/h)                 -1.024e+007       -1.024e+007                                                              "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    ---               ---                                                                      "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase                                                             "]
[null,null,"Molecular Weight                 29.10             29.10                                                                    "]
[null,null,"Molar Density (kgmole/m3)        3.387e-002        3.387e-002                                                               "]
[null,null,"Mass Density (kg/m3)             0.9857            0.9857                                                                   "]
[null,null,"Act. Volume Flow (m3/h)          7120              7120                                                                     "]
[null,null,"Mass Enthalpy (kJ/kg)            -1459             -1459                                                                    "]
[null,null,"Mass Entropy (kJ/kg-C)           6.024             6.024                                                                    "]
[null,null,"Heat Capacity (kJ/kgmole-C)      30.55             30.55                                                                    "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     1.050             1.050                                                                    "]
[null,null,"Lower Heating Value (kJ/kgmole)  8.541e-004        8.541e-004                                                               "]
[null,null,"Mass Lower Heating Value (kJ/kg) 2.935e-005        2.935e-005                                                               "]
[null,null,"Phase Fraction [Vol. Basis]      ---               1.000                                                                    "]
[null,null,"Phase Fraction [Mass Basis]      4.941e-324        1.000                                                                    "]
[null,null,"Partial Pressure of CO2 (kPa)    7.949             ---                                                                      "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000                                                                   "]
[null,null,"Act. Gas Flow (ACT_m3/h)         7120              7120                                                                     "]
[null,null,"Avg. Liq. Density (kgmole/m3)    29.36             29.36                                                                    "]
[null,null,"Specific Heat (kJ/kgmole-C)      30.55             30.55                                                                    "]
[null,null,"Std. Gas Flow (STD_m3/h)         5702              5702                                                                     "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 854.4             854.4                                                                   "]
[null,null,"Act. Liq. Flow (m3/s)            ---               ---                                                                      "]
[null,null,"Z Factor                         0.9995            0.9995                                                                   "]
[null,null,"Watson K                         6.383             6.383                                                                    "]
[null,null,"User Property                    ---               ---                                                                      "]
[null,null,"Cp/(Cp - R)                      1.374             1.374                                                                    "]
[null,null,"Cp/Cv                            1.377             1.377                                                                    "]
[null,null,"Heat of Vap. (kJ/kgmole)         1.859e+004        ---                                                                      "]
[null,null,"Kinematic Viscosity (cSt)        21.84             21.84                                                                    "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) ---               ---                                                                     "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) ---               ---                                                                     "]
[null,null,"Liquid Fraction                  0.0000            0.0000                                                                   "]
[null,null,"Molar Volume (m3/kgmole)         29.52             29.52                                                                    "]
[null,null,"Mass Heat of Vap. (kJ/kg)        638.9             ---                                                                      "]
[null,null,"Phase Fraction [Molar Basis]     1.0000            1.0000                                                                   "]
[null,null,"Surface Tension (dyne/cm)        ---               ---                                                                      "]
[null,null,"Thermal Conductivity (W/m-K)     3.041e-002        3.041e-002                                                               "]
[null,null,"Viscosity (cP)                   2.152e-002        2.152e-002                                                               "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    22.24             22.24                                                                    "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   0.7642            0.7642                                                                   "]
[null,null,"Cv (kJ/kgmole-C)                 22.19             22.19                                                                    "]
[null,null,"Mass Cv (kJ/kg-C)                0.7626            0.7626                                                                   "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   21.53             21.53                                                                    "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  0.7399            0.7399                                                                   "]
[null,null,"Cp/Cv (Ent. Method)              1.419             1.419                                                                    "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---                                                                      "]
[null,null,"True VP at 37.8 C (kPa)          1.874e+005        1.874e+005                                                               "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 0.0000            0.0000                                                                  "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---                                                                      "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 1.0000    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                34.4900          0.1430           1103.6812        0.1573           0.9701           0.1181           "]
[null,null,"Nitrogen              172.8879         0.7169           4843.1080        0.6901           6.0060           0.7313           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   15.9987          0.0663           288.2173         0.0411           0.2888           0.0352           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   17.7814          0.0737           782.5555         0.1115           0.9482           0.1154           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 241.1580         1.0000           7017.5621        1.0000           8.2131           1.0000           "]
[null,null,"Vapour Phase                                                                                      Phase Fraction 1.000      "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                34.4900          0.1430           1103.6812        0.1573           0.9701           0.1181           "]
[null,null,"Nitrogen              172.8879         0.7169           4843.1080        0.6901           6.0060           0.7313           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   15.9987          0.0663           288.2173         0.0411           0.2888           0.0352           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   17.7814          0.0737           782.5555         0.1115           0.9482           0.1154           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 241.1580         1.0000           7017.5621        1.0000           8.2131           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"condensate to drain (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: condensate to drain                                                 Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase      Aqueous Phase                                          "]
[null,null,"Vapour / Phase Fraction          0.0000            0.0000            1.0000                                                 "]
[null,null,"Temperature: (C)                 45.00             45.00             45.00                                                  "]
[null,null,"Pressure: (kPa)                  2135              2135              2135                                                   "]
[null,null,"Molar Flow (kgmole/h)            33.54             0.0000            33.54                                                  "]
[null,null,"Mass Flow (kg/h)                 605.6             0.0000            605.6                                                  "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    0.6073            0.0000            0.6073                                                 "]
[null,null,"Molar Enthalpy (kJ/kgmole)       -2.840e+005       -9.489e+004       -2.840e+005                                            "]
[null,null,"Molar Entropy (kJ/kgmole-C)      58.88             93.15             58.88                                                  "]
[null,null,"Heat Flow (kJ/h)                 -9.525e+006       0.0000            -9.525e+006                                            "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    0.5964            0.0000            0.5964                                                 "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase      Aqueous Phase                                          "]
[null,null,"Molecular Weight                 18.05             12.58             18.05                                                  "]
[null,null,"Molar Density (kgmole/m3)        55.02             0.8090            55.02                                                  "]
[null,null,"Mass Density (kg/m3)             993.3             10.18             993.3                                                  "]
[null,null,"Act. Volume Flow (m3/h)          0.6097            0.0000            0.6097                                                 "]
[null,null,"Mass Enthalpy (kJ/kg)            -1.573e+004       -7541             -1.573e+004                                            "]
[null,null,"Mass Entropy (kJ/kg-C)           3.261             7.403             3.261                                                  "]
[null,null,"Heat Capacity (kJ/kgmole-C)      77.74             31.65             77.74                                                  "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     4.306             2.515             4.306                                                  "]
[null,null,"Lower Heating Value (kJ/kgmole)  ---               ---               ---                                                    "]
[null,null,"Mass Lower Heating Value (kJ/kg) ---               ---               ---                                                    "]
[null,null,"Phase Fraction [Vol. Basis]      ---               ---               1.000                                                  "]
[null,null,"Phase Fraction [Mass Basis]      4.941e-324        0.0000            1.000                                                  "]
[null,null,"Partial Pressure of CO2 (kPa)    0.0000            ---               ---                                                    "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000            0.0000                                                 "]
[null,null,"Act. Gas Flow (ACT_m3/h)         ---               ---               ---                                                    "]
[null,null,"Avg. Liq. Density (kgmole/m3)    55.24             28.63             55.24                                                  "]
[null,null,"Specific Heat (kJ/kgmole-C)      77.74             31.65             77.74                                                  "]
[null,null,"Std. Gas Flow (STD_m3/h)         793.1             0.0000            793.1                                                  "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 997.2             360.2             997.2                                                 "]
[null,null,"Act. Liq. Flow (m3/s)            1.693e-004        ---               1.693e-004                                             "]
[null,null,"Z Factor                         ---               0.9975            1.467e-002                                             "]
[null,null,"Watson K                         8.558             13.36             8.558                                                  "]
[null,null,"User Property                    ---               ---               ---                                                    "]
[null,null,"Cp/(Cp - R)                      1.120             1.356             1.120                                                  "]
[null,null,"Cp/Cv                            1.158             1.385             1.158                                                  "]
[null,null,"Heat of Vap. (kJ/kgmole)         3.762e+004        ---               ---                                                    "]
[null,null,"Kinematic Viscosity (cSt)        0.6363            1.213             0.6363                                                 "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) 1015              ---               1015                                                  "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) 0.5964            0.0000            0.5964                                                "]
[null,null,"Liquid Fraction                  1.000             0.0000            1.000                                                  "]
[null,null,"Molar Volume (m3/kgmole)         1.818e-002        1.236             1.818e-002                                             "]
[null,null,"Mass Heat of Vap. (kJ/kg)        2084              ---               ---                                                    "]
[null,null,"Phase Fraction [Molar Basis]     0.0000            0.0000            1.0000                                                 "]
[null,null,"Surface Tension (dyne/cm)        68.51             ---               68.51                                                  "]
[null,null,"Thermal Conductivity (W/m-K)     0.6357            0.1021            0.6357                                                 "]
[null,null,"Viscosity (cP)                   0.6320            1.234e-002        0.6320                                                 "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    69.43             23.34             69.43                                                  "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   3.846             1.855             3.846                                                  "]
[null,null,"Cv (kJ/kgmole-C)                 67.14             22.85             67.14                                                  "]
[null,null,"Mass Cv (kJ/kg-C)                3.719             1.816             3.719                                                  "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   ---               22.84             ---                                                    "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  ---               1.815             ---                                                    "]
[null,null,"Cp/Cv (Ent. Method)              ---               1.386             ---                                                    "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---               ---                                                    "]
[null,null,"True VP at 37.8 C (kPa)          2441              ---               2441                                                   "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 0.5964            0.0000            0.5964                                                "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---               ---                                                    "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 0.0000    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0010           0.0000           0.0020           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   33.4924          0.9985           603.3686         0.9964           0.6046           0.9956           "]
[null,null,"CO                    0.0000           0.0000           0.0011           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0495           0.0015           2.1794           0.0036           0.0026           0.0043           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0001           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 33.5430          1.0000           605.5513         1.0000           0.6073           1.0000           "]
[null,null,"Vapour Phase                                                                                      Phase Fraction 0.0000     "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0146           0.0000           0.0186           0.0000           0.0224           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.7260           0.0000           0.1163           0.0000           0.5998           "]
[null,null,"H2O                   0.0000           0.0052           0.0000           0.0074           0.0000           0.0027           "]
[null,null,"CO                    0.0000           0.0249           0.0000           0.0554           0.0000           0.0250           "]
[null,null,"CO2                   0.0000           0.2294           0.0000           0.8023           0.0000           0.3502           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 0.0000           1.0000           0.0000           1.0000           0.0000           1.0000           "]
[null,null,"Aqueous Phase                                                                                     Phase Fraction 1.000      "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0010           0.0000           0.0020           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   33.4924          0.9985           603.3686         0.9964           0.6046           0.9956           "]
[null,null,"CO                    0.0000           0.0000           0.0011           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0495           0.0015           2.1794           0.0036           0.0026           0.0043           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0001           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 33.5430          1.0000           605.5513         1.0000           0.6073           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"DI Water (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: DI Water                                                            Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Aqueous Phase                                                            "]
[null,null,"Vapour / Phase Fraction          0.0000            1.0000                                                                   "]
[null,null,"Temperature: (C)                 25.00             25.00                                                                    "]
[null,null,"Pressure: (kPa)                  101.3             101.3                                                                    "]
[null,null,"Molar Flow (kgmole/h)            53.74             53.74                                                                    "]
[null,null,"Mass Flow (kg/h)                 968.2             968.2                                                                    "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    0.9701            0.9701                                                                   "]
[null,null,"Molar Enthalpy (kJ/kgmole)       -2.854e+005       -2.854e+005                                                              "]
[null,null,"Molar Entropy (kJ/kgmole-C)      53.70             53.70                                                                    "]
[null,null,"Heat Flow (kJ/h)                 -1.534e+007       -1.534e+007                                                              "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    0.9540            0.9540                                                                   "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Aqueous Phase                                                            "]
[null,null,"Molecular Weight                 18.02             18.02                                                                    "]
[null,null,"Molar Density (kgmole/m3)        55.92             55.92                                                                    "]
[null,null,"Mass Density (kg/m3)             1007              1007                                                                     "]
[null,null,"Act. Volume Flow (m3/h)          0.9611            0.9611                                                                   "]
[null,null,"Mass Enthalpy (kJ/kg)            -1.584e+004       -1.584e+004                                                              "]
[null,null,"Mass Entropy (kJ/kg-C)           2.981             2.981                                                                    "]
[null,null,"Heat Capacity (kJ/kgmole-C)      77.71             77.71                                                                    "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     4.313             4.313                                                                    "]
[null,null,"Lower Heating Value (kJ/kgmole)  0.0000            0.0000                                                                   "]
[null,null,"Mass Lower Heating Value (kJ/kg) ---               ---                                                                      "]
[null,null,"Phase Fraction [Vol. Basis]      ---               1.000                                                                    "]
[null,null,"Phase Fraction [Mass Basis]      0.0000            1.000                                                                    "]
[null,null,"Partial Pressure of CO2 (kPa)    0.0000            ---                                                                      "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000                                                                   "]
[null,null,"Act. Gas Flow (ACT_m3/h)         ---               ---                                                                      "]
[null,null,"Avg. Liq. Density (kgmole/m3)    55.40             55.40                                                                    "]
[null,null,"Specific Heat (kJ/kgmole-C)      77.71             77.71                                                                    "]
[null,null,"Std. Gas Flow (STD_m3/h)         1271              1271                                                                     "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 998.0             998.0                                                                   "]
[null,null,"Act. Liq. Flow (m3/s)            2.670e-004        2.670e-004                                                               "]
[null,null,"Z Factor                         7.310e-004        7.310e-004                                                               "]
[null,null,"Watson K                         ---               ---                                                                      "]
[null,null,"User Property                    ---               ---                                                                      "]
[null,null,"Cp/(Cp - R)                      1.120             1.120                                                                    "]
[null,null,"Cp/Cv                            1.147             1.147                                                                    "]
[null,null,"Heat of Vap. (kJ/kgmole)         4.101e+004        ---                                                                      "]
[null,null,"Kinematic Viscosity (cSt)        0.8840            0.8840                                                                   "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) 1015              1015                                                                    "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) 0.9540            0.9540                                                                  "]
[null,null,"Liquid Fraction                  1.000             1.000                                                                    "]
[null,null,"Molar Volume (m3/kgmole)         1.788e-002        1.788e-002                                                               "]
[null,null,"Mass Heat of Vap. (kJ/kg)        2276              ---                                                                      "]
[null,null,"Phase Fraction [Molar Basis]     0.0000            1.0000                                                                   "]
[null,null,"Surface Tension (dyne/cm)        72.10             72.10                                                                    "]
[null,null,"Thermal Conductivity (W/m-K)     0.6110            0.6110                                                                   "]
[null,null,"Viscosity (cP)                   0.8904            0.8904                                                                   "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    69.39             69.39                                                                    "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   3.852             3.852                                                                    "]
[null,null,"Cv (kJ/kgmole-C)                 67.75             67.75                                                                    "]
[null,null,"Mass Cv (kJ/kg-C)                3.761             3.761                                                                    "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   ---               ---                                                                      "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  ---               ---                                                                      "]
[null,null,"Cp/Cv (Ent. Method)              ---               ---                                                                      "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---                                                                      "]
[null,null,"True VP at 37.8 C (kPa)          6.467             6.467                                                                    "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 0.9540            0.9540                                                                  "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---                                                                      "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 0.0000    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   53.7425          1.0000           968.1765         1.0000           0.9701           1.0000           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 53.7425          1.0000           968.1765         1.0000           0.9701           1.0000           "]
[null,null,"Aqueous Phase                                                                                     Phase Fraction 1.000      "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   53.7425          1.0000           968.1765         1.0000           0.9701           1.0000           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 53.7425          1.0000           968.1765         1.0000           0.9701           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"dry reformate (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: dry reformate                                                       Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase      Aqueous Phase                                          "]
[null,null,"Vapour / Phase Fraction          1.0000            1.0000            0.0000                                                 "]
[null,null,"Temperature: (C)                 45.00             45.00             45.00                                                  "]
[null,null,"Pressure: (kPa)                  2135              2135              2135                                                   "]
[null,null,"Molar Flow (kgmole/h)            56.93             56.93             0.0000                                                 "]
[null,null,"Mass Flow (kg/h)                 716.3             716.3             0.0000                                                 "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    1.988             1.988             0.0000                                                 "]
[null,null,"Molar Enthalpy (kJ/kgmole)       -9.489e+004       -9.489e+004       -2.840e+005                                            "]
[null,null,"Molar Entropy (kJ/kgmole-C)      93.15             93.15             58.88                                                  "]
[null,null,"Heat Flow (kJ/h)                 -5.402e+006       -5.402e+006       0.0000                                                 "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    ---               ---               0.0000                                                 "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase      Aqueous Phase                                          "]
[null,null,"Molecular Weight                 12.58             12.58             18.05                                                  "]
[null,null,"Molar Density (kgmole/m3)        0.8090            0.8090            55.02                                                  "]
[null,null,"Mass Density (kg/m3)             10.18             10.18             993.3                                                  "]
[null,null,"Act. Volume Flow (m3/h)          70.37             70.37             0.0000                                                 "]
[null,null,"Mass Enthalpy (kJ/kg)            -7541             -7541             -1.573e+004                                            "]
[null,null,"Mass Entropy (kJ/kg-C)           7.403             7.403             3.261                                                  "]
[null,null,"Heat Capacity (kJ/kgmole-C)      31.65             31.65             77.74                                                  "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     2.515             2.515             4.306                                                  "]
[null,null,"Lower Heating Value (kJ/kgmole)  ---               ---               ---                                                    "]
[null,null,"Mass Lower Heating Value (kJ/kg) ---               ---               ---                                                    "]
[null,null,"Phase Fraction [Vol. Basis]      ---               1.000             ---                                                    "]
[null,null,"Phase Fraction [Mass Basis]      4.941e-324        1.000             0.0000                                                 "]
[null,null,"Partial Pressure of CO2 (kPa)    489.7             ---               ---                                                    "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000            0.0000                                                 "]
[null,null,"Act. Gas Flow (ACT_m3/h)         70.37             70.37             ---                                                    "]
[null,null,"Avg. Liq. Density (kgmole/m3)    28.63             28.63             55.24                                                  "]
[null,null,"Specific Heat (kJ/kgmole-C)      31.65             31.65             77.74                                                  "]
[null,null,"Std. Gas Flow (STD_m3/h)         1346              1346              0.0000                                                 "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 360.2             360.2             997.2                                                 "]
[null,null,"Act. Liq. Flow (m3/s)            0.0000            ---               0.0000                                                 "]
[null,null,"Z Factor                         ---               0.9975            1.467e-002                                             "]
[null,null,"Watson K                         13.36             13.36             8.558                                                  "]
[null,null,"User Property                    ---               ---               ---                                                    "]
[null,null,"Cp/(Cp - R)                      1.356             1.356             1.120                                                  "]
[null,null,"Cp/Cv                            1.385             1.385             1.158                                                  "]
[null,null,"Heat of Vap. (kJ/kgmole)         1.247e+004        ---               ---                                                    "]
[null,null,"Kinematic Viscosity (cSt)        1.095             1.213             0.6363                                                 "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) ---               ---               1015                                                  "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) ---               ---               0.0000                                                "]
[null,null,"Liquid Fraction                  0.0000            0.0000            1.000                                                  "]
[null,null,"Molar Volume (m3/kgmole)         1.236             1.236             1.818e-002                                             "]
[null,null,"Mass Heat of Vap. (kJ/kg)        990.7             ---               ---                                                    "]
[null,null,"Phase Fraction [Molar Basis]     1.0000            1.0000            0.0000                                                 "]
[null,null,"Surface Tension (dyne/cm)        ---               ---               68.51                                                  "]
[null,null,"Thermal Conductivity (W/m-K)     0.1021            0.1021            0.6357                                                 "]
[null,null,"Viscosity (cP)                   1.114e-002        1.234e-002        0.6320                                                 "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    23.34             23.34             69.43                                                  "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   1.855             1.855             3.846                                                  "]
[null,null,"Cv (kJ/kgmole-C)                 22.85             22.85             67.14                                                  "]
[null,null,"Mass Cv (kJ/kg-C)                1.816             1.816             3.719                                                  "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   22.84             22.84             ---                                                    "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  1.815             1.815             ---                                                    "]
[null,null,"Cp/Cv (Ent. Method)              1.386             1.386             ---                                                    "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---               ---                                                    "]
[null,null,"True VP at 37.8 C (kPa)          ---               ---               2441                                                   "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 0.0000            0.0000            0.0000                                                "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---               ---                                                    "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 1.0000    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.8295           0.0146           13.3078          0.0186           0.0444           0.0224           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              41.3293          0.7260           83.3198          0.1163           1.1927           0.5998           "]
[null,null,"H2O                   0.2933           0.0052           5.2840           0.0074           0.0053           0.0027           "]
[null,null,"CO                    1.4166           0.0249           39.6808          0.0554           0.0496           0.0250           "]
[null,null,"CO2                   13.0593          0.2294           574.7360         0.8023           0.6964           0.3502           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 56.9280          1.0000           716.3283         1.0000           1.9884           1.0000           "]
[null,null,"Vapour Phase                                                                                      Phase Fraction 1.000      "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.8295           0.0146           13.3078          0.0186           0.0444           0.0224           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              41.3293          0.7260           83.3198          0.1163           1.1927           0.5998           "]
[null,null,"H2O                   0.2933           0.0052           5.2840           0.0074           0.0053           0.0027           "]
[null,null,"CO                    1.4166           0.0249           39.6808          0.0554           0.0496           0.0250           "]
[null,null,"CO2                   13.0593          0.2294           574.7360         0.8023           0.6964           0.3502           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 56.9280          1.0000           716.3283         1.0000           1.9884           1.0000           "]
[null,null,"Aqueous Phase                                                                                     Phase Fraction 0.0000     "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   0.0000           0.9985           0.0000           0.9964           0.0000           0.9956           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0015           0.0000           0.0036           0.0000           0.0043           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 0.0000           1.0000           0.0000           1.0000           0.0000           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"final dry reformate (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: final dry reformate                                                 Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase      Aqueous Phase                                          "]
[null,null,"Vapour / Phase Fraction          0.6292            0.6292            0.3708                                                 "]
[null,null,"Temperature: (C)                 45.00             45.00             45.00                                                  "]
[null,null,"Pressure: (kPa)                  2135              2135              2135                                                   "]
[null,null,"Molar Flow (kgmole/h)            90.47             56.93             33.54                                                  "]
[null,null,"Mass Flow (kg/h)                 1322              716.3             605.6                                                  "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    2.596             1.988             0.6073                                                 "]
[null,null,"Molar Enthalpy (kJ/kgmole)       -1.650e+005       -9.489e+004       -2.840e+005                                            "]
[null,null,"Molar Entropy (kJ/kgmole-C)      80.44             93.15             58.88                                                  "]
[null,null,"Heat Flow (kJ/h)                 -1.493e+007       -5.402e+006       -9.525e+006                                            "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    ---               ---               0.5964                                                 "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase      Aqueous Phase                                          "]
[null,null,"Molecular Weight                 14.61             12.58             18.05                                                  "]
[null,null,"Molar Density (kgmole/m3)        1.275             0.8090            55.02                                                  "]
[null,null,"Mass Density (kg/m3)             18.62             10.18             993.3                                                  "]
[null,null,"Act. Volume Flow (m3/h)          70.98             70.37             0.6097                                                 "]
[null,null,"Mass Enthalpy (kJ/kg)            -1.129e+004       -7541             -1.573e+004                                            "]
[null,null,"Mass Entropy (kJ/kg-C)           5.505             7.403             3.261                                                  "]
[null,null,"Heat Capacity (kJ/kgmole-C)      48.74             31.65             77.74                                                  "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     3.336             2.515             4.306                                                  "]
[null,null,"Lower Heating Value (kJ/kgmole)  ---               ---               ---                                                    "]
[null,null,"Mass Lower Heating Value (kJ/kg) ---               ---               ---                                                    "]
[null,null,"Phase Fraction [Vol. Basis]      0.7661            0.7661            0.2339                                                 "]
[null,null,"Phase Fraction [Mass Basis]      0.5419            0.5419            0.4581                                                 "]
[null,null,"Partial Pressure of CO2 (kPa)    489.7             ---               ---                                                    "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000            0.0000                                                 "]
[null,null,"Act. Gas Flow (ACT_m3/h)         ---               70.37             ---                                                    "]
[null,null,"Avg. Liq. Density (kgmole/m3)    34.85             28.63             55.24                                                  "]
[null,null,"Specific Heat (kJ/kgmole-C)      48.74             31.65             77.74                                                  "]
[null,null,"Std. Gas Flow (STD_m3/h)         2139              1346              793.1                                                  "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 509.3             360.2             997.2                                                 "]
[null,null,"Act. Liq. Flow (m3/s)            1.693e-004        ---               1.693e-004                                             "]
[null,null,"Z Factor                         ---               0.9975            1.467e-002                                             "]
[null,null,"Watson K                         13.34             13.36             8.558                                                  "]
[null,null,"User Property                    ---               ---               ---                                                    "]
[null,null,"Cp/(Cp - R)                      1.206             1.356             1.120                                                  "]
[null,null,"Cp/Cv                            1.129             1.385             1.158                                                  "]
[null,null,"Heat of Vap. (kJ/kgmole)         4.084e+004        ---               ---                                                    "]
[null,null,"Kinematic Viscosity (cSt)        ---               1.213             0.6363                                                 "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) ---               ---               1015                                                  "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) ---               ---               0.5964                                                "]
[null,null,"Liquid Fraction                  0.3708            0.0000            1.000                                                  "]
[null,null,"Molar Volume (m3/kgmole)         0.7845            1.236             1.818e-002                                             "]
[null,null,"Mass Heat of Vap. (kJ/kg)        2795              ---               ---                                                    "]
[null,null,"Phase Fraction [Molar Basis]     0.6292            0.6292            0.3708                                                 "]
[null,null,"Surface Tension (dyne/cm)        68.51             ---               68.51                                                  "]
[null,null,"Thermal Conductivity (W/m-K)     ---               0.1021            0.6357                                                 "]
[null,null,"Viscosity (cP)                   ---               1.234e-002        0.6320                                                 "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    40.43             23.34             69.43                                                  "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   2.767             1.855             3.846                                                  "]
[null,null,"Cv (kJ/kgmole-C)                 43.18             22.85             67.14                                                  "]
[null,null,"Mass Cv (kJ/kg-C)                2.955             1.816             3.719                                                  "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   49.43             22.84             ---                                                    "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  3.383             1.815             ---                                                    "]
[null,null,"Cp/Cv (Ent. Method)              0.9862            1.386             ---                                                    "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---               ---                                                    "]
[null,null,"True VP at 37.8 C (kPa)          ---               ---               2441                                                   "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 0.5964            0.0000            0.5964                                                "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---               ---                                                    "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 0.6292    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.8295           0.0092           13.3078          0.0101           0.0444           0.0171           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              41.3303          0.4568           83.3218          0.0630           1.1927           0.4595           "]
[null,null,"H2O                   33.7857          0.3734           608.6526         0.4604           0.6099           0.2350           "]
[null,null,"CO                    1.4167           0.0157           39.6819          0.0300           0.0496           0.0191           "]
[null,null,"CO2                   13.1088          0.1449           576.9154         0.4364           0.6990           0.2693           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0001           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 90.4710          1.0000           1321.8797        1.0000           2.5957           1.0000           "]
[null,null,"Vapour Phase                                                                                      Phase Fraction 0.6292     "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.8295           0.0146           13.3078          0.0186           0.0444           0.0224           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              41.3293          0.7260           83.3198          0.1163           1.1927           0.5998           "]
[null,null,"H2O                   0.2933           0.0052           5.2840           0.0074           0.0053           0.0027           "]
[null,null,"CO                    1.4166           0.0249           39.6808          0.0554           0.0496           0.0250           "]
[null,null,"CO2                   13.0593          0.2294           574.7360         0.8023           0.6964           0.3502           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 56.9280          1.0000           716.3283         1.0000           1.9884           1.0000           "]
[null,null,"Aqueous Phase                                                                                     Phase Fraction 0.3708     "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0010           0.0000           0.0020           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   33.4924          0.9985           603.3686         0.9964           0.6046           0.9956           "]
[null,null,"CO                    0.0000           0.0000           0.0011           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0495           0.0015           2.1794           0.0036           0.0026           0.0043           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0001           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 33.5430          1.0000           605.5513         1.0000           0.6073           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Flue gas to superheater inlet (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: Flue gas to superheater inlet                                       Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase                                                             "]
[null,null,"Vapour / Phase Fraction          1.0000            1.0000                                                                   "]
[null,null,"Temperature: (C)                 560.6             560.6                                                                    "]
[null,null,"Pressure: (kPa)                  108.9             108.9                                                                    "]
[null,null,"Molar Flow (kgmole/h)            241.2             241.2                                                                    "]
[null,null,"Mass Flow (kg/h)                 7018              7018                                                                     "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    8.213             8.213                                                                    "]
[null,null,"Molar Enthalpy (kJ/kgmole)       -2.797e+004       -2.797e+004                                                              "]
[null,null,"Molar Entropy (kJ/kgmole-C)      200.1             200.1                                                                    "]
[null,null,"Heat Flow (kJ/h)                 -6.745e+006       -6.745e+006                                                              "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    ---               ---                                                                      "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase                                                             "]
[null,null,"Molecular Weight                 29.10             29.10                                                                    "]
[null,null,"Molar Density (kgmole/m3)        1.570e-002        1.570e-002                                                               "]
[null,null,"Mass Density (kg/m3)             0.4568            0.4568                                                                   "]
[null,null,"Act. Volume Flow (m3/h)          1.536e+004        1.536e+004                                                               "]
[null,null,"Mass Enthalpy (kJ/kg)            -961.1            -961.1                                                                   "]
[null,null,"Mass Entropy (kJ/kg-C)           6.875             6.875                                                                    "]
[null,null,"Heat Capacity (kJ/kgmole-C)      33.92             33.92                                                                    "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     1.166             1.166                                                                    "]
[null,null,"Lower Heating Value (kJ/kgmole)  8.541e-004        8.541e-004                                                               "]
[null,null,"Mass Lower Heating Value (kJ/kg) 2.935e-005        2.935e-005                                                               "]
[null,null,"Phase Fraction [Vol. Basis]      ---               1.000                                                                    "]
[null,null,"Phase Fraction [Mass Basis]      4.941e-324        1.000                                                                    "]
[null,null,"Partial Pressure of CO2 (kPa)    8.027             ---                                                                      "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000                                                                   "]
[null,null,"Act. Gas Flow (ACT_m3/h)         1.536e+004        1.536e+004                                                               "]
[null,null,"Avg. Liq. Density (kgmole/m3)    29.36             29.36                                                                    "]
[null,null,"Specific Heat (kJ/kgmole-C)      33.92             33.92                                                                    "]
[null,null,"Std. Gas Flow (STD_m3/h)         5702              5702                                                                     "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 854.4             854.4                                                                   "]
[null,null,"Act. Liq. Flow (m3/s)            ---               ---                                                                      "]
[null,null,"Z Factor                         1.000             1.000                                                                    "]
[null,null,"Watson K                         6.383             6.383                                                                    "]
[null,null,"User Property                    ---               ---                                                                      "]
[null,null,"Cp/(Cp - R)                      1.325             1.325                                                                    "]
[null,null,"Cp/Cv                            1.325             1.325                                                                    "]
[null,null,"Heat of Vap. (kJ/kgmole)         1.859e+004        ---                                                                      "]
[null,null,"Kinematic Viscosity (cSt)        83.72             83.72                                                                    "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) ---               ---                                                                     "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) ---               ---                                                                     "]
[null,null,"Liquid Fraction                  0.0000            0.0000                                                                   "]
[null,null,"Molar Volume (m3/kgmole)         63.70             63.70                                                                    "]
[null,null,"Mass Heat of Vap. (kJ/kg)        638.8             ---                                                                      "]
[null,null,"Phase Fraction [Molar Basis]     1.0000            1.0000                                                                   "]
[null,null,"Surface Tension (dyne/cm)        ---               ---                                                                      "]
[null,null,"Thermal Conductivity (W/m-K)     5.843e-002        5.843e-002                                                               "]
[null,null,"Viscosity (cP)                   3.825e-002        3.825e-002                                                               "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    25.61             25.61                                                                    "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   0.8800            0.8800                                                                   "]
[null,null,"Cv (kJ/kgmole-C)                 25.60             25.60                                                                    "]
[null,null,"Mass Cv (kJ/kg-C)                0.8798            0.8798                                                                   "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   31.07             31.07                                                                    "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  1.068             1.068                                                                    "]
[null,null,"Cp/Cv (Ent. Method)              1.092             1.092                                                                    "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---                                                                      "]
[null,null,"True VP at 37.8 C (kPa)          1.874e+005        1.874e+005                                                               "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 0.0000            0.0000                                                                  "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---                                                                      "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 1.0000    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                34.4900          0.1430           1103.6812        0.1573           0.9701           0.1181           "]
[null,null,"Nitrogen              172.8879         0.7169           4843.1080        0.6901           6.0060           0.7313           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   15.9987          0.0663           288.2173         0.0411           0.2888           0.0352           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   17.7814          0.0737           782.5555         0.1115           0.9482           0.1154           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 241.1580         1.0000           7017.5621        1.0000           8.2131           1.0000           "]
[null,null,"Vapour Phase                                                                                      Phase Fraction 1.000      "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                34.4900          0.1430           1103.6812        0.1573           0.9701           0.1181           "]
[null,null,"Nitrogen              172.8879         0.7169           4843.1080        0.6901           6.0060           0.7313           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   15.9987          0.0663           288.2173         0.0411           0.2888           0.0352           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   17.7814          0.0737           782.5555         0.1115           0.9482           0.1154           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 241.1580         1.0000           7017.5621        1.0000           8.2131           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Fuel ethanol (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: Fuel ethanol                                                        Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Liquid Phase                                                             "]
[null,null,"Vapour / Phase Fraction          0.0000            1.0000                                                                   "]
[null,null,"Temperature: (C)                 25.00             25.00                                                                    "]
[null,null,"Pressure: (kPa)                  101.3             101.3                                                                    "]
[null,null,"Molar Flow (kgmole/h)            7.677             7.677                                                                    "]
[null,null,"Mass Flow (kg/h)                 353.7             353.7                                                                    "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    0.4444            0.4444                                                                   "]
[null,null,"Molar Enthalpy (kJ/kgmole)       -2.789e+005       -2.789e+005                                                              "]
[null,null,"Molar Entropy (kJ/kgmole-C)      -6.460            -6.460                                                                   "]
[null,null,"Heat Flow (kJ/h)                 -2.141e+006       -2.141e+006                                                              "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    0.4440            0.4440                                                                   "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Liquid Phase                                                             "]
[null,null,"Molecular Weight                 46.07             46.07                                                                    "]
[null,null,"Molar Density (kgmole/m3)        17.10             17.10                                                                    "]
[null,null,"Mass Density (kg/m3)             787.6             787.6                                                                    "]
[null,null,"Act. Volume Flow (m3/h)          0.4491            0.4491                                                                   "]
[null,null,"Mass Enthalpy (kJ/kg)            -6053             -6053                                                                    "]
[null,null,"Mass Entropy (kJ/kg-C)           -0.1402           -0.1402                                                                  "]
[null,null,"Heat Capacity (kJ/kgmole-C)      142.5             142.5                                                                    "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     3.093             3.093                                                                    "]
[null,null,"Lower Heating Value (kJ/kgmole)  1.235e+006        1.235e+006                                                               "]
[null,null,"Mass Lower Heating Value (kJ/kg) 2.682e+004        2.682e+004                                                               "]
[null,null,"Phase Fraction [Vol. Basis]      ---               1.000                                                                    "]
[null,null,"Phase Fraction [Mass Basis]      2.122e-314        1.000                                                                    "]
[null,null,"Partial Pressure of CO2 (kPa)    0.0000            ---                                                                      "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000                                                                   "]
[null,null,"Act. Gas Flow (ACT_m3/h)         ---               ---                                                                      "]
[null,null,"Avg. Liq. Density (kgmole/m3)    17.28             17.28                                                                    "]
[null,null,"Specific Heat (kJ/kgmole-C)      142.5             142.5                                                                    "]
[null,null,"Std. Gas Flow (STD_m3/h)         181.5             181.5                                                                    "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 796.0             796.0                                                                   "]
[null,null,"Act. Liq. Flow (m3/s)            1.247e-004        1.247e-004                                                               "]
[null,null,"Z Factor                         2.391e-003        2.391e-003                                                               "]
[null,null,"Watson K                         10.76             10.76                                                                    "]
[null,null,"User Property                    ---               ---                                                                      "]
[null,null,"Cp/(Cp - R)                      1.062             1.062                                                                    "]
[null,null,"Cp/Cv                            1.104             1.104                                                                    "]
[null,null,"Heat of Vap. (kJ/kgmole)         3.949e+004        ---                                                                      "]
[null,null,"Kinematic Viscosity (cSt)        1.222             1.222                                                                    "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) 796.6             796.6                                                                   "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) 0.4440            0.4440                                                                  "]
[null,null,"Liquid Fraction                  1.000             1.000                                                                    "]
[null,null,"Molar Volume (m3/kgmole)         5.849e-002        5.849e-002                                                               "]
[null,null,"Mass Heat of Vap. (kJ/kg)        857.3             ---                                                                      "]
[null,null,"Phase Fraction [Molar Basis]     0.0000            1.0000                                                                   "]
[null,null,"Surface Tension (dyne/cm)        22.10             22.10                                                                    "]
[null,null,"Thermal Conductivity (W/m-K)     0.1574            0.1574                                                                   "]
[null,null,"Viscosity (cP)                   0.9626            0.9626                                                                   "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    134.2             134.2                                                                    "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   2.913             2.913                                                                    "]
[null,null,"Cv (kJ/kgmole-C)                 129.1             129.1                                                                    "]
[null,null,"Mass Cv (kJ/kg-C)                2.803             2.803                                                                    "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   ---               ---                                                                      "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  ---               ---                                                                      "]
[null,null,"Cp/Cv (Ent. Method)              ---               ---                                                                      "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---                                                                      "]
[null,null,"True VP at 37.8 C (kPa)          15.74             15.74                                                                    "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 0.4440            0.4440                                                                  "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---                                                                      "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 0.0000    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               7.6775           1.0000           353.7017         1.0000           0.4444           1.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 7.6775           1.0000           353.7017         1.0000           0.4444           1.0000           "]
[null,null,"Liquid Phase                                                                                      Phase Fraction 1.000      "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               7.6775           1.0000           353.7017         1.0000           0.4444           1.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 7.6775           1.0000           353.7017         1.0000           0.4444           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Hot Reformate #1 (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: Hot Reformate #1                                                    Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase      Liquid Phase      Aqueous Phase                        "]
[null,null,"Vapour / Phase Fraction          1.0000            1.0000            0.0000            0.0000                               "]
[null,null,"Temperature: (C)                 846.0             846.0             846.0             846.0                                "]
[null,null,"Pressure: (kPa)                  2144              2144              2144              2144                                 "]
[null,null,"Molar Flow (kgmole/h)            90.47             90.47             0.0000            0.0000                               "]
[null,null,"Mass Flow (kg/h)                 1322              1322              0.0000            0.0000                               "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    2.425             2.425             0.0000            0.0000                               "]
[null,null,"Molar Enthalpy (kJ/kgmole)       -1.180e+005       -1.180e+005       -1.180e+005       -1.180e+005                          "]
[null,null,"Molar Entropy (kJ/kgmole-C)      168.4             168.4             168.4             168.4                                "]
[null,null,"Heat Flow (kJ/h)                 -1.067e+007       -1.067e+007       0.0000            0.0000                               "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    ---               ---               0.0000            0.0000                               "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase      Liquid Phase      Aqueous Phase                        "]
[null,null,"Molecular Weight                 14.61             14.61             14.61             14.61                                "]
[null,null,"Molar Density (kgmole/m3)        0.2299            0.2299            0.2299            0.2299                               "]
[null,null,"Mass Density (kg/m3)             3.359             3.359             3.359             3.359                                "]
[null,null,"Act. Volume Flow (m3/h)          393.6             393.6             0.0000            0.0000                               "]
[null,null,"Mass Enthalpy (kJ/kg)            -8074             -8074             -8074             -8074                                "]
[null,null,"Mass Entropy (kJ/kg-C)           11.53             11.53             11.53             11.53                                "]
[null,null,"Heat Capacity (kJ/kgmole-C)      38.74             38.74             38.74             38.74                                "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     2.651             2.651             2.651             2.651                                "]
[null,null,"Lower Heating Value (kJ/kgmole)  ---               ---               ---               ---                                  "]
[null,null,"Mass Lower Heating Value (kJ/kg) ---               ---               ---               ---                                  "]
[null,null,"Phase Fraction [Vol. Basis]      ---               1.000             ---               ---                                  "]
[null,null,"Phase Fraction [Mass Basis]      2.122e-314        1.000             0.0000            0.0000                               "]
[null,null,"Partial Pressure of CO2 (kPa)    171.8             ---               ---               ---                                  "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000            0.0000            0.0000                               "]
[null,null,"Act. Gas Flow (ACT_m3/h)         393.6             393.6             ---               ---                                  "]
[null,null,"Avg. Liq. Density (kgmole/m3)    37.30             37.30             37.30             37.30                                "]
[null,null,"Specific Heat (kJ/kgmole-C)      38.74             38.74             38.74             38.74                                "]
[null,null,"Std. Gas Flow (STD_m3/h)         2139              2139              0.0000            0.0000                               "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 545.1             545.1             545.1             545.1                               "]
[null,null,"Act. Liq. Flow (m3/s)            0.0000            ---               ---               0.0000                               "]
[null,null,"Z Factor                         ---               1.002             1.002             1.002                                "]
[null,null,"Watson K                         12.88             12.88             12.88             12.88                                "]
[null,null,"User Property                    ---               ---               ---               ---                                  "]
[null,null,"Cp/(Cp - R)                      1.273             1.273             1.273             1.273                                "]
[null,null,"Cp/Cv                            1.277             1.277             1.277             1.277                                "]
[null,null,"Heat of Vap. (kJ/kgmole)         4.291e+004        ---               ---               ---                                  "]
[null,null,"Kinematic Viscosity (cSt)        8.743             9.390             0.8236            0.8236                               "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) ---               ---               ---               ---                                 "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) ---               ---               0.0000            0.0000                              "]
[null,null,"Liquid Fraction                  0.0000            0.0000            1.000             1.000                                "]
[null,null,"Molar Volume (m3/kgmole)         4.350             4.350             4.350             4.350                                "]
[null,null,"Mass Heat of Vap. (kJ/kg)        2937              ---               ---               ---                                  "]
[null,null,"Phase Fraction [Molar Basis]     1.0000            1.0000            0.0000            0.0000                               "]
[null,null,"Surface Tension (dyne/cm)        ---               ---               0.0000            0.0000                               "]
[null,null,"Thermal Conductivity (W/m-K)     0.1721            0.1721            0.1049            0.1049                               "]
[null,null,"Viscosity (cP)                   2.937e-002        3.154e-002        2.766e-003        2.766e-003                           "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    30.42             30.42             30.42             30.42                                "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   2.082             2.082             2.082             2.082                                "]
[null,null,"Cv (kJ/kgmole-C)                 30.32             30.32             30.32             30.32                                "]
[null,null,"Mass Cv (kJ/kg-C)                2.075             2.075             2.075             2.075                                "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   30.31             30.31             -1.286e+004       -32.70                               "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  2.075             2.075             -879.8            -2.238                               "]
[null,null,"Cp/Cv (Ent. Method)              1.278             1.278             -3.013e-003       -1.185                               "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---               ---               ---                                  "]
[null,null,"True VP at 37.8 C (kPa)          ---               ---               ---               ---                                  "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 0.0000            0.0000            0.0000            0.0000                              "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---               ---               ---                                  "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 1.0000    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.8295           0.0092           13.3078          0.0101           0.0444           0.0183           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              35.4706          0.3921           71.5088          0.0541           1.0236           0.4221           "]
[null,null,"H2O                   39.6453          0.4382           714.2148         0.5403           0.7157           0.2951           "]
[null,null,"CO                    7.2763           0.0804           203.8161         0.1542           0.2550           0.1051           "]
[null,null,"CO2                   7.2492           0.0801           319.0338         0.2413           0.3866           0.1594           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0001           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 90.4710          1.0000           1321.8814        1.0000           2.4252           1.0000           "]
[null,null,"Vapour Phase                                                                                      Phase Fraction 1.000      "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.8295           0.0092           13.3078          0.0101           0.0444           0.0183           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              35.4706          0.3921           71.5088          0.0541           1.0236           0.4221           "]
[null,null,"H2O                   39.6453          0.4382           714.2148         0.5403           0.7157           0.2951           "]
[null,null,"CO                    7.2763           0.0804           203.8161         0.1542           0.2550           0.1051           "]
[null,null,"CO2                   7.2492           0.0801           319.0338         0.2413           0.3866           0.1594           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0001           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 90.4710          1.0000           1321.8814        1.0000           2.4252           1.0000           "]
[null,null,"Liquid Phase                                                                                      Phase Fraction 0.0000     "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0092           0.0000           0.0101           0.0000           0.0183           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.3921           0.0000           0.0541           0.0000           0.4221           "]
[null,null,"H2O                   0.0000           0.4382           0.0000           0.5403           0.0000           0.2951           "]
[null,null,"CO                    0.0000           0.0804           0.0000           0.1542           0.0000           0.1051           "]
[null,null,"CO2                   0.0000           0.0801           0.0000           0.2413           0.0000           0.1594           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 0.0000           1.0000           0.0000           1.0000           0.0000           1.0000           "]
[null,null,"Aqueous Phase                                                                                     Phase Fraction 0.0000     "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0092           0.0000           0.0101           0.0000           0.0183           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.3921           0.0000           0.0541           0.0000           0.4221           "]
[null,null,"H2O                   0.0000           0.4382           0.0000           0.5403           0.0000           0.2951           "]
[null,null,"CO                    0.0000           0.0804           0.0000           0.1542           0.0000           0.1051           "]
[null,null,"CO2                   0.0000           0.0801           0.0000           0.2413           0.0000           0.1594           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 0.0000           1.0000           0.0000           1.0000           0.0000           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Hot Reformate #2 (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: Hot Reformate #2                                                    Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase                                                             "]
[null,null,"Vapour / Phase Fraction          1.0000            1.0000                                                                   "]
[null,null,"Temperature: (C)                 600.0             600.0                                                                    "]
[null,null,"Pressure: (kPa)                  2142              2142                                                                     "]
[null,null,"Molar Flow (kgmole/h)            90.47             90.47                                                                    "]
[null,null,"Mass Flow (kg/h)                 1322              1322                                                                     "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    2.425             2.425                                                                    "]
[null,null,"Molar Enthalpy (kJ/kgmole)       -1.273e+005       -1.273e+005                                                              "]
[null,null,"Molar Entropy (kJ/kgmole-C)      159.1             159.1                                                                    "]
[null,null,"Heat Flow (kJ/h)                 -1.151e+007       -1.151e+007                                                              "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    ---               ---                                                                      "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase                                                             "]
[null,null,"Molecular Weight                 14.61             14.61                                                                    "]
[null,null,"Molar Density (kgmole/m3)        0.2949            0.2949                                                                   "]
[null,null,"Mass Density (kg/m3)             4.309             4.309                                                                    "]
[null,null,"Act. Volume Flow (m3/h)          306.8             306.8                                                                    "]
[null,null,"Mass Enthalpy (kJ/kg)            -8709             -8709                                                                    "]
[null,null,"Mass Entropy (kJ/kg-C)           10.89             10.89                                                                    "]
[null,null,"Heat Capacity (kJ/kgmole-C)      36.76             36.76                                                                    "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     2.516             2.516                                                                    "]
[null,null,"Lower Heating Value (kJ/kgmole)  ---               ---                                                                      "]
[null,null,"Mass Lower Heating Value (kJ/kg) ---               ---                                                                      "]
[null,null,"Phase Fraction [Vol. Basis]      ---               1.000                                                                    "]
[null,null,"Phase Fraction [Mass Basis]      4.941e-324        1.000                                                                    "]
[null,null,"Partial Pressure of CO2 (kPa)    171.6             ---                                                                      "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000                                                                   "]
[null,null,"Act. Gas Flow (ACT_m3/h)         306.8             306.8                                                                    "]
[null,null,"Avg. Liq. Density (kgmole/m3)    37.30             37.30                                                                    "]
[null,null,"Specific Heat (kJ/kgmole-C)      36.76             36.76                                                                    "]
[null,null,"Std. Gas Flow (STD_m3/h)         2139              2139                                                                     "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 545.1             545.1                                                                   "]
[null,null,"Act. Liq. Flow (m3/s)            ---               ---                                                                      "]
[null,null,"Z Factor                         1.000             1.000                                                                    "]
[null,null,"Watson K                         12.88             12.88                                                                    "]
[null,null,"User Property                    ---               ---                                                                      "]
[null,null,"Cp/(Cp - R)                      1.292             1.292                                                                    "]
[null,null,"Cp/Cv                            1.302             1.302                                                                    "]
[null,null,"Heat of Vap. (kJ/kgmole)         4.291e+004        ---                                                                      "]
[null,null,"Kinematic Viscosity (cSt)        5.642             6.090                                                                    "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) ---               ---                                                                     "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) ---               ---                                                                     "]
[null,null,"Liquid Fraction                  0.0000            0.0000                                                                   "]
[null,null,"Molar Volume (m3/kgmole)         3.391             3.391                                                                    "]
[null,null,"Mass Heat of Vap. (kJ/kg)        2937              ---                                                                      "]
[null,null,"Phase Fraction [Molar Basis]     1.0000            1.0000                                                                   "]
[null,null,"Surface Tension (dyne/cm)        ---               ---                                                                      "]
[null,null,"Thermal Conductivity (W/m-K)     0.1415            0.1415                                                                   "]
[null,null,"Viscosity (cP)                   2.431e-002        2.624e-002                                                               "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    28.44             28.44                                                                    "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   1.947             1.947                                                                    "]
[null,null,"Cv (kJ/kgmole-C)                 28.24             28.24                                                                    "]
[null,null,"Mass Cv (kJ/kg-C)                1.933             1.933                                                                    "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   28.23             28.23                                                                    "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  1.932             1.932                                                                    "]
[null,null,"Cp/Cv (Ent. Method)              1.302             1.302                                                                    "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---                                                                      "]
[null,null,"True VP at 37.8 C (kPa)          ---               ---                                                                      "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 0.0000            0.0000                                                                  "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---                                                                      "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 1.0000    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.8295           0.0092           13.3078          0.0101           0.0444           0.0183           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              35.4706          0.3921           71.5088          0.0541           1.0236           0.4221           "]
[null,null,"H2O                   39.6453          0.4382           714.2148         0.5403           0.7157           0.2951           "]
[null,null,"CO                    7.2763           0.0804           203.8161         0.1542           0.2550           0.1051           "]
[null,null,"CO2                   7.2492           0.0801           319.0338         0.2413           0.3866           0.1594           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0001           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 90.4710          1.0000           1321.8814        1.0000           2.4252           1.0000           "]
[null,null,"Vapour Phase                                                                                      Phase Fraction 1.000      "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.8295           0.0092           13.3078          0.0101           0.0444           0.0183           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              35.4706          0.3921           71.5088          0.0541           1.0236           0.4221           "]
[null,null,"H2O                   39.6453          0.4382           714.2148         0.5403           0.7157           0.2951           "]
[null,null,"CO                    7.2763           0.0804           203.8161         0.1542           0.2550           0.1051           "]
[null,null,"CO2                   7.2492           0.0801           319.0338         0.2413           0.3866           0.1594           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0001           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 90.4710          1.0000           1321.8814        1.0000           2.4252           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"HP ethanol (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: HP ethanol                                                          Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Liquid Phase                                                             "]
[null,null,"Vapour / Phase Fraction          0.0000            1.0000                                                                   "]
[null,null,"Temperature: (C)                 27.81             27.81                                                                    "]
[null,null,"Pressure: (kPa)                  2200              2200                                                                     "]
[null,null,"Molar Flow (kgmole/h)            7.677             7.677                                                                    "]
[null,null,"Mass Flow (kg/h)                 353.7             353.7                                                                    "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    0.4444            0.4444                                                                   "]
[null,null,"Molar Enthalpy (kJ/kgmole)       -2.784e+005       -2.784e+005                                                              "]
[null,null,"Molar Entropy (kJ/kgmole-C)      -5.258            -5.258                                                                   "]
[null,null,"Heat Flow (kJ/h)                 -2.137e+006       -2.137e+006                                                              "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    0.4440            0.4440                                                                   "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Liquid Phase                                                             "]
[null,null,"Molecular Weight                 46.07             46.07                                                                    "]
[null,null,"Molar Density (kgmole/m3)        17.10             17.10                                                                    "]
[null,null,"Mass Density (kg/m3)             787.9             787.9                                                                    "]
[null,null,"Act. Volume Flow (m3/h)          0.4489            0.4489                                                                   "]
[null,null,"Mass Enthalpy (kJ/kg)            -6042             -6042                                                                    "]
[null,null,"Mass Entropy (kJ/kg-C)           -0.1141           -0.1141                                                                  "]
[null,null,"Heat Capacity (kJ/kgmole-C)      142.7             142.7                                                                    "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     3.098             3.098                                                                    "]
[null,null,"Lower Heating Value (kJ/kgmole)  1.235e+006        1.235e+006                                                               "]
[null,null,"Mass Lower Heating Value (kJ/kg) 2.682e+004        2.682e+004                                                               "]
[null,null,"Phase Fraction [Vol. Basis]      ---               1.000                                                                    "]
[null,null,"Phase Fraction [Mass Basis]      2.122e-314        1.000                                                                    "]
[null,null,"Partial Pressure of CO2 (kPa)    0.0000            ---                                                                      "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000                                                                   "]
[null,null,"Act. Gas Flow (ACT_m3/h)         ---               ---                                                                      "]
[null,null,"Avg. Liq. Density (kgmole/m3)    17.28             17.28                                                                    "]
[null,null,"Specific Heat (kJ/kgmole-C)      142.7             142.7                                                                    "]
[null,null,"Std. Gas Flow (STD_m3/h)         181.5             181.5                                                                    "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 796.0             796.0                                                                   "]
[null,null,"Act. Liq. Flow (m3/s)            1.247e-004        1.247e-004                                                               "]
[null,null,"Z Factor                         5.141e-002        5.141e-002                                                               "]
[null,null,"Watson K                         10.76             10.76                                                                    "]
[null,null,"User Property                    ---               ---                                                                      "]
[null,null,"Cp/(Cp - R)                      1.062             1.062                                                                    "]
[null,null,"Cp/Cv                            1.101             1.101                                                                    "]
[null,null,"Heat of Vap. (kJ/kgmole)         2.585e+004        ---                                                                      "]
[null,null,"Kinematic Viscosity (cSt)        1.165             1.165                                                                    "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) 796.6             796.6                                                                   "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) 0.4440            0.4440                                                                  "]
[null,null,"Liquid Fraction                  1.000             1.000                                                                    "]
[null,null,"Molar Volume (m3/kgmole)         5.847e-002        5.847e-002                                                               "]
[null,null,"Mass Heat of Vap. (kJ/kg)        561.1             ---                                                                      "]
[null,null,"Phase Fraction [Molar Basis]     0.0000            1.0000                                                                   "]
[null,null,"Surface Tension (dyne/cm)        21.87             21.87                                                                    "]
[null,null,"Thermal Conductivity (W/m-K)     0.1563            0.1563                                                                   "]
[null,null,"Viscosity (cP)                   0.9177            0.9177                                                                   "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    134.4             134.4                                                                    "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   2.918             2.918                                                                    "]
[null,null,"Cv (kJ/kgmole-C)                 129.7             129.7                                                                    "]
[null,null,"Mass Cv (kJ/kg-C)                2.815             2.815                                                                    "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   ---               ---                                                                      "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  ---               ---                                                                      "]
[null,null,"Cp/Cv (Ent. Method)              ---               ---                                                                      "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---                                                                      "]
[null,null,"True VP at 37.8 C (kPa)          15.74             15.74                                                                    "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 0.4440            0.4440                                                                  "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---                                                                      "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 0.0000    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               7.6775           1.0000           353.7017         1.0000           0.4444           1.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 7.6775           1.0000           353.7017         1.0000           0.4444           1.0000           "]
[null,null,"Liquid Phase                                                                                      Phase Fraction 1.000      "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               7.6775           1.0000           353.7017         1.0000           0.4444           1.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 7.6775           1.0000           353.7017         1.0000           0.4444           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"HP H2O (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: HP H2O                                                              Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Aqueous Phase                                                            "]
[null,null,"Vapour / Phase Fraction          0.0000            1.0000                                                                   "]
[null,null,"Temperature: (C)                 26.47             26.47                                                                    "]
[null,null,"Pressure: (kPa)                  2200              2200                                                                     "]
[null,null,"Molar Flow (kgmole/h)            53.74             53.74                                                                    "]
[null,null,"Mass Flow (kg/h)                 968.2             968.2                                                                    "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    0.9701            0.9701                                                                   "]
[null,null,"Molar Enthalpy (kJ/kgmole)       -2.853e+005       -2.853e+005                                                              "]
[null,null,"Molar Entropy (kJ/kgmole-C)      54.06             54.06                                                                    "]
[null,null,"Heat Flow (kJ/h)                 -1.533e+007       -1.533e+007                                                              "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    0.9540            0.9540                                                                   "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Aqueous Phase                                                            "]
[null,null,"Molecular Weight                 18.02             18.02                                                                    "]
[null,null,"Molar Density (kgmole/m3)        55.89             55.89                                                                    "]
[null,null,"Mass Density (kg/m3)             1007              1007                                                                     "]
[null,null,"Act. Volume Flow (m3/h)          0.9616            0.9616                                                                   "]
[null,null,"Mass Enthalpy (kJ/kg)            -1.583e+004       -1.583e+004                                                              "]
[null,null,"Mass Entropy (kJ/kg-C)           3.001             3.001                                                                    "]
[null,null,"Heat Capacity (kJ/kgmole-C)      77.66             77.66                                                                    "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     4.311             4.311                                                                    "]
[null,null,"Lower Heating Value (kJ/kgmole)  0.0000            0.0000                                                                   "]
[null,null,"Mass Lower Heating Value (kJ/kg) ---               ---                                                                      "]
[null,null,"Phase Fraction [Vol. Basis]      ---               1.000                                                                    "]
[null,null,"Phase Fraction [Mass Basis]      0.0000            1.000                                                                    "]
[null,null,"Partial Pressure of CO2 (kPa)    0.0000            ---                                                                      "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000                                                                   "]
[null,null,"Act. Gas Flow (ACT_m3/h)         ---               ---                                                                      "]
[null,null,"Avg. Liq. Density (kgmole/m3)    55.40             55.40                                                                    "]
[null,null,"Specific Heat (kJ/kgmole-C)      77.66             77.66                                                                    "]
[null,null,"Std. Gas Flow (STD_m3/h)         1271              1271                                                                     "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 998.0             998.0                                                                   "]
[null,null,"Act. Liq. Flow (m3/s)            2.671e-004        2.671e-004                                                               "]
[null,null,"Z Factor                         1.580e-002        1.580e-002                                                               "]
[null,null,"Watson K                         ---               ---                                                                      "]
[null,null,"User Property                    ---               ---                                                                      "]
[null,null,"Cp/(Cp - R)                      1.120             1.120                                                                    "]
[null,null,"Cp/Cv                            1.148             1.148                                                                    "]
[null,null,"Heat of Vap. (kJ/kgmole)         3.416e+004        ---                                                                      "]
[null,null,"Kinematic Viscosity (cSt)        0.8554            0.8554                                                                   "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) 1015              1015                                                                    "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) 0.9540            0.9540                                                                  "]
[null,null,"Liquid Fraction                  1.000             1.000                                                                    "]
[null,null,"Molar Volume (m3/kgmole)         1.789e-002        1.789e-002                                                               "]
[null,null,"Mass Heat of Vap. (kJ/kg)        1896              ---                                                                      "]
[null,null,"Phase Fraction [Molar Basis]     0.0000            1.0000                                                                   "]
[null,null,"Surface Tension (dyne/cm)        71.84             71.84                                                                    "]
[null,null,"Thermal Conductivity (W/m-K)     0.6132            0.6132                                                                   "]
[null,null,"Viscosity (cP)                   0.8613            0.8613                                                                   "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    69.35             69.35                                                                    "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   3.850             3.850                                                                    "]
[null,null,"Cv (kJ/kgmole-C)                 67.67             67.67                                                                    "]
[null,null,"Mass Cv (kJ/kg-C)                3.756             3.756                                                                    "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   ---               ---                                                                      "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  ---               ---                                                                      "]
[null,null,"Cp/Cv (Ent. Method)              ---               ---                                                                      "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---                                                                      "]
[null,null,"True VP at 37.8 C (kPa)          6.467             6.467                                                                    "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 0.9540            0.9540                                                                  "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---                                                                      "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 0.0000    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   53.7425          1.0000           968.1765         1.0000           0.9701           1.0000           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 53.7425          1.0000           968.1765         1.0000           0.9701           1.0000           "]
[null,null,"Aqueous Phase                                                                                     Phase Fraction 1.000      "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   53.7425          1.0000           968.1765         1.0000           0.9701           1.0000           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 53.7425          1.0000           968.1765         1.0000           0.9701           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"HP liquid mixture (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: HP liquid mixture                                                   Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Liquid Phase      Aqueous Phase                                          "]
[null,null,"Vapour / Phase Fraction          0.0000            0.1469            0.8531                                                 "]
[null,null,"Temperature: (C)                 24.44             24.44             24.44                                                  "]
[null,null,"Pressure: (kPa)                  2200              2200              2200                                                   "]
[null,null,"Molar Flow (kgmole/h)            61.42             9.023             52.40                                                  "]
[null,null,"Mass Flow (kg/h)                 1322              375.6             946.3                                                  "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    1.414             0.4653            0.9492                                                 "]
[null,null,"Molar Enthalpy (kJ/kgmole)       -2.844e+005       -2.787e+005       -2.854e+005                                            "]
[null,null,"Molar Entropy (kJ/kgmole-C)      46.81             7.633             53.56                                                  "]
[null,null,"Heat Flow (kJ/h)                 -1.747e+007       -2.515e+006       -1.495e+007                                            "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    1.351             0.4567            0.9329                                                 "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Liquid Phase      Aqueous Phase                                          "]
[null,null,"Molecular Weight                 21.52             41.62             18.06                                                  "]
[null,null,"Molar Density (kgmole/m3)        43.91             19.61             55.81                                                  "]
[null,null,"Mass Density (kg/m3)             944.9             816.4             1008                                                   "]
[null,null,"Act. Volume Flow (m3/h)          1.399             0.4600            0.9389                                                 "]
[null,null,"Mass Enthalpy (kJ/kg)            -1.321e+004       -6697             -1.580e+004                                            "]
[null,null,"Mass Entropy (kJ/kg-C)           2.175             0.1834            2.966                                                  "]
[null,null,"Heat Capacity (kJ/kgmole-C)      85.79             132.3             77.78                                                  "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     3.986             3.179             4.306                                                  "]
[null,null,"Lower Heating Value (kJ/kgmole)  1.544e+005        1.040e+006        1984                                                   "]
[null,null,"Mass Lower Heating Value (kJ/kg) 7176              2.498e+004        109.8                                                  "]
[null,null,"Phase Fraction [Vol. Basis]      ---               0.3290            0.6710                                                 "]
[null,null,"Phase Fraction [Mass Basis]      2.122e-314        0.2841            0.7159                                                 "]
[null,null,"Partial Pressure of CO2 (kPa)    0.0000            ---               ---                                                    "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000            0.0000                                                 "]
[null,null,"Act. Gas Flow (ACT_m3/h)         ---               ---               ---                                                    "]
[null,null,"Avg. Liq. Density (kgmole/m3)    43.42             19.39             55.20                                                  "]
[null,null,"Specific Heat (kJ/kgmole-C)      85.79             132.3             77.78                                                  "]
[null,null,"Std. Gas Flow (STD_m3/h)         1452              213.3             1239                                                   "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 934.5             807.2             996.9                                                 "]
[null,null,"Act. Liq. Flow (m3/s)            3.886e-004        1.278e-004        2.608e-004                                             "]
[null,null,"Z Factor                         ---               4.533e-002        1.593e-002                                             "]
[null,null,"Watson K                         10.76             10.76             10.76                                                  "]
[null,null,"User Property                    ---               ---               ---                                                    "]
[null,null,"Cp/(Cp - R)                      1.107             1.067             1.120                                                  "]
[null,null,"Cp/Cv                            1.095             1.106             1.146                                                  "]
[null,null,"Heat of Vap. (kJ/kgmole)         3.679e+004        ---               ---                                                    "]
[null,null,"Kinematic Viscosity (cSt)        1.548             1.224             0.9153                                                 "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) 978.7             822.5             1014                                                  "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) 1.351             0.4567            0.9329                                                "]
[null,null,"Liquid Fraction                  1.000             1.000             1.000                                                  "]
[null,null,"Molar Volume (m3/kgmole)         2.278e-002        5.098e-002        1.792e-002                                             "]
[null,null,"Mass Heat of Vap. (kJ/kg)        1710              ---               ---                                                    "]
[null,null,"Phase Fraction [Molar Basis]     0.0000            0.1469            0.8531                                                 "]
[null,null,"Surface Tension (dyne/cm)        ---               30.08             72.12                                                  "]
[null,null,"Thermal Conductivity (W/m-K)     0.4318            0.2043            0.6096                                                 "]
[null,null,"Viscosity (cP)                   1.463             0.9991            0.9225                                                 "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    77.47             124.0             69.46                                                  "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   3.600             2.979             3.846                                                  "]
[null,null,"Cv (kJ/kgmole-C)                 78.32             119.6             67.84                                                  "]
[null,null,"Mass Cv (kJ/kg-C)                3.639             2.874             3.757                                                  "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   ---               ---               ---                                                    "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  ---               ---               ---                                                    "]
[null,null,"Cp/Cv (Ent. Method)              ---               ---               ---                                                    "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---               ---                                                    "]
[null,null,"True VP at 37.8 C (kPa)          19.69             19.25             15.83                                                  "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 1.390             0.4567            0.9329                                                "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---               ---                                                    "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 0.0000    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   53.7425          0.8750           968.1765         0.7324           0.9701           0.6859           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               7.6775           0.1250           353.7017         0.2676           0.4444           0.3141           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 61.4200          1.0000           1321.8782        1.0000           1.4145           1.0000           "]
[null,null,"Liquid Phase                                                                                      Phase Fraction 0.1469     "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   1.4299           0.1585           25.7590          0.0686           0.0258           0.0555           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               7.5934           0.8415           349.8255         0.9314           0.4395           0.9445           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 9.0232           1.0000           375.5846         1.0000           0.4653           1.0000           "]
[null,null,"Aqueous Phase                                                                                     Phase Fraction 0.8531     "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   52.3126          0.9984           942.4175         0.9959           0.9443           0.9949           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0841           0.0016           3.8761           0.0041           0.0049           0.0051           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 52.3968          1.0000           946.2936         1.0000           0.9492           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"inlet air (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: inlet air                                                           Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase                                                             "]
[null,null,"Vapour / Phase Fraction          1.0000            1.0000                                                                   "]
[null,null,"Temperature: (C)                 25.00             25.00                                                                    "]
[null,null,"Pressure: (kPa)                  101.2             101.2                                                                    "]
[null,null,"Molar Flow (kgmole/h)            218.6             218.6                                                                    "]
[null,null,"Mass Flow (kg/h)                 6307              6307                                                                     "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    7.293             7.293                                                                    "]
[null,null,"Molar Enthalpy (kJ/kgmole)       -8.174            -8.174                                                                   "]
[null,null,"Molar Entropy (kJ/kgmole-C)      163.4             163.4                                                                    "]
[null,null,"Heat Flow (kJ/h)                 -1787             -1787                                                                    "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    ---               ---                                                                      "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase                                                             "]
[null,null,"Molecular Weight                 28.85             28.85                                                                    "]
[null,null,"Molar Density (kgmole/m3)        4.086e-002        4.086e-002                                                               "]
[null,null,"Mass Density (kg/m3)             1.179             1.179                                                                    "]
[null,null,"Act. Volume Flow (m3/h)          5351              5351                                                                     "]
[null,null,"Mass Enthalpy (kJ/kg)            -0.2834           -0.2834                                                                  "]
[null,null,"Mass Entropy (kJ/kg-C)           5.664             5.664                                                                    "]
[null,null,"Heat Capacity (kJ/kgmole-C)      29.16             29.16                                                                    "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     1.011             1.011                                                                    "]
[null,null,"Lower Heating Value (kJ/kgmole)  0.0000            0.0000                                                                   "]
[null,null,"Mass Lower Heating Value (kJ/kg) ---               ---                                                                      "]
[null,null,"Phase Fraction [Vol. Basis]      ---               1.000                                                                    "]
[null,null,"Phase Fraction [Mass Basis]      4.941e-324        1.000                                                                    "]
[null,null,"Partial Pressure of CO2 (kPa)    0.0000            ---                                                                      "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000                                                                   "]
[null,null,"Act. Gas Flow (ACT_m3/h)         5351              5351                                                                     "]
[null,null,"Avg. Liq. Density (kgmole/m3)    29.98             29.98                                                                    "]
[null,null,"Specific Heat (kJ/kgmole-C)      29.16             29.16                                                                    "]
[null,null,"Std. Gas Flow (STD_m3/h)         5169              5169                                                                     "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 864.8             864.8                                                                   "]
[null,null,"Act. Liq. Flow (m3/s)            ---               ---                                                                      "]
[null,null,"Z Factor                         0.9994            0.9994                                                                   "]
[null,null,"Watson K                         6.043             6.043                                                                    "]
[null,null,"User Property                    ---               ---                                                                      "]
[null,null,"Cp/(Cp - R)                      1.399             1.399                                                                    "]
[null,null,"Cp/Cv                            1.402             1.402                                                                    "]
[null,null,"Heat of Vap. (kJ/kgmole)         5899              ---                                                                      "]
[null,null,"Kinematic Viscosity (cSt)        15.97             15.97                                                                    "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) ---               ---                                                                     "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) ---               ---                                                                     "]
[null,null,"Liquid Fraction                  0.0000            0.0000                                                                   "]
[null,null,"Molar Volume (m3/kgmole)         24.47             24.47                                                                    "]
[null,null,"Mass Heat of Vap. (kJ/kg)        204.5             ---                                                                      "]
[null,null,"Phase Fraction [Molar Basis]     1.0000            1.0000                                                                   "]
[null,null,"Surface Tension (dyne/cm)        ---               ---                                                                      "]
[null,null,"Thermal Conductivity (W/m-K)     2.589e-002        2.589e-002                                                               "]
[null,null,"Viscosity (cP)                   1.883e-002        1.883e-002                                                               "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    20.84             20.84                                                                    "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   0.7226            0.7226                                                                   "]
[null,null,"Cv (kJ/kgmole-C)                 20.80             20.80                                                                    "]
[null,null,"Mass Cv (kJ/kg-C)                0.7210            0.7210                                                                   "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   20.76             20.76                                                                    "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  0.7196            0.7196                                                                   "]
[null,null,"Cp/Cv (Ent. Method)              1.405             1.405                                                                    "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---                                                                      "]
[null,null,"True VP at 37.8 C (kPa)          ---               ---                                                                      "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 0.0000            0.0000                                                                  "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---                                                                      "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 1.0000    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                45.7375          0.2092           1463.6010        0.2321           1.2865           0.1764           "]
[null,null,"Nitrogen              172.8879         0.7908           4843.1080        0.7679           6.0060           0.8236           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 218.6254         1.0000           6306.7090        1.0000           7.2925           1.0000           "]
[null,null,"Vapour Phase                                                                                      Phase Fraction 1.000      "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                45.7375          0.2092           1463.6010        0.2321           1.2865           0.1764           "]
[null,null,"Nitrogen              172.8879         0.7908           4843.1080        0.7679           6.0060           0.8236           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 218.6254         1.0000           6306.7090        1.0000           7.2925           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"lowT reformate (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: lowT reformate                                                      Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase      Liquid Phase      Aqueous Phase                        "]
[null,null,"Vapour / Phase Fraction          1.0000            1.0000            0.0000            0.0000                               "]
[null,null,"Temperature: (C)                 400.4             400.4             400.4             400.4                                "]
[null,null,"Pressure: (kPa)                  2142              2142              2142              2142                                 "]
[null,null,"Molar Flow (kgmole/h)            90.47             90.47             0.0000            0.0000                               "]
[null,null,"Mass Flow (kg/h)                 1322              1322              0.0000            0.0000                               "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    2.596             2.596             0.0000            0.0000                               "]
[null,null,"Molar Enthalpy (kJ/kgmole)       -1.370e+005       -1.370e+005       -1.370e+005       -1.370e+005                          "]
[null,null,"Molar Entropy (kJ/kgmole-C)      144.9             144.9             144.9             144.9                                "]
[null,null,"Heat Flow (kJ/h)                 -1.239e+007       -1.239e+007       0.0000            0.0000                               "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    ---               ---               0.0000            0.0000                               "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase      Liquid Phase      Aqueous Phase                        "]
[null,null,"Molecular Weight                 14.61             14.61             14.61             14.61                                "]
[null,null,"Molar Density (kgmole/m3)        0.3836            0.3836            0.3836            0.3836                               "]
[null,null,"Mass Density (kg/m3)             5.604             5.604             5.604             5.604                                "]
[null,null,"Act. Volume Flow (m3/h)          235.9             235.9             0.0000            0.0000                               "]
[null,null,"Mass Enthalpy (kJ/kg)            -9374             -9374             -9374             -9374                                "]
[null,null,"Mass Entropy (kJ/kg-C)           9.918             9.918             9.918             9.918                                "]
[null,null,"Heat Capacity (kJ/kgmole-C)      35.84             35.84             35.84             35.84                                "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     2.453             2.453             2.453             2.453                                "]
[null,null,"Lower Heating Value (kJ/kgmole)  ---               ---               ---               ---                                  "]
[null,null,"Mass Lower Heating Value (kJ/kg) ---               ---               ---               ---                                  "]
[null,null,"Phase Fraction [Vol. Basis]      ---               1.000             ---               ---                                  "]
[null,null,"Phase Fraction [Mass Basis]      2.122e-314        1.000             0.0000            0.0000                               "]
[null,null,"Partial Pressure of CO2 (kPa)    310.3             ---               ---               ---                                  "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000            0.0000            0.0000                               "]
[null,null,"Act. Gas Flow (ACT_m3/h)         235.9             235.9             ---               ---                                  "]
[null,null,"Avg. Liq. Density (kgmole/m3)    34.85             34.85             34.85             34.85                                "]
[null,null,"Specific Heat (kJ/kgmole-C)      35.84             35.84             35.84             35.84                                "]
[null,null,"Std. Gas Flow (STD_m3/h)         2139              2139              0.0000            0.0000                               "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 509.3             509.3             509.3             509.3                               "]
[null,null,"Act. Liq. Flow (m3/s)            0.0000            ---               ---               0.0000                               "]
[null,null,"Z Factor                         ---               0.9970            0.9970            0.9970                               "]
[null,null,"Watson K                         13.34             13.34             13.34             13.34                                "]
[null,null,"User Property                    ---               ---               ---               ---                                  "]
[null,null,"Cp/(Cp - R)                      1.302             1.302             1.302             1.302                                "]
[null,null,"Cp/Cv                            1.319             1.319             1.319             1.319                                "]
[null,null,"Heat of Vap. (kJ/kgmole)         4.085e+004        ---               ---               ---                                  "]
[null,null,"Kinematic Viscosity (cSt)        3.532             3.856             0.4643            0.4643                               "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) ---               ---               ---               ---                                 "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) ---               ---               0.0000            0.0000                              "]
[null,null,"Liquid Fraction                  0.0000            0.0000            1.000             1.000                                "]
[null,null,"Molar Volume (m3/kgmole)         2.607             2.607             2.607             2.607                                "]
[null,null,"Mass Heat of Vap. (kJ/kg)        2796              ---               ---               ---                                  "]
[null,null,"Phase Fraction [Molar Basis]     1.0000            1.0000            0.0000            0.0000                               "]
[null,null,"Surface Tension (dyne/cm)        ---               ---               0.0000            0.0000                               "]
[null,null,"Thermal Conductivity (W/m-K)     0.1248            0.1248            8.988e-002        8.988e-002                           "]
[null,null,"Viscosity (cP)                   1.979e-002        2.161e-002        2.602e-003        2.602e-003                           "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    27.53             27.53             27.53             27.53                                "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   1.884             1.884             1.884             1.884                                "]
[null,null,"Cv (kJ/kgmole-C)                 27.17             27.17             27.17             27.17                                "]
[null,null,"Mass Cv (kJ/kg-C)                1.860             1.860             1.860             1.860                                "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   27.17             27.17             35.63             174.1                                "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  1.860             1.860             2.439             11.92                                "]
[null,null,"Cp/Cv (Ent. Method)              1.319             1.319             1.006             0.2059                               "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---               ---               ---                                  "]
[null,null,"True VP at 37.8 C (kPa)          ---               ---               ---               ---                                  "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 0.0000            0.0000            0.0000            0.0000                              "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---               ---               ---                                  "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 1.0000    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.8295           0.0092           13.3078          0.0101           0.0444           0.0171           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              41.3303          0.4568           83.3218          0.0630           1.1927           0.4595           "]
[null,null,"H2O                   33.7857          0.3734           608.6526         0.4604           0.6099           0.2350           "]
[null,null,"CO                    1.4167           0.0157           39.6819          0.0300           0.0496           0.0191           "]
[null,null,"CO2                   13.1088          0.1449           576.9154         0.4364           0.6990           0.2693           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0001           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 90.4710          1.0000           1321.8797        1.0000           2.5957           1.0000           "]
[null,null,"Vapour Phase                                                                                      Phase Fraction 1.000      "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.8295           0.0092           13.3078          0.0101           0.0444           0.0171           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              41.3303          0.4568           83.3218          0.0630           1.1927           0.4595           "]
[null,null,"H2O                   33.7857          0.3734           608.6526         0.4604           0.6099           0.2350           "]
[null,null,"CO                    1.4167           0.0157           39.6819          0.0300           0.0496           0.0191           "]
[null,null,"CO2                   13.1088          0.1449           576.9154         0.4364           0.6990           0.2693           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0001           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 90.4710          1.0000           1321.8797        1.0000           2.5957           1.0000           "]
[null,null,"Liquid Phase                                                                                      Phase Fraction 0.0000     "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0092           0.0000           0.0101           0.0000           0.0171           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.4568           0.0000           0.0630           0.0000           0.4595           "]
[null,null,"H2O                   0.0000           0.3734           0.0000           0.4604           0.0000           0.2350           "]
[null,null,"CO                    0.0000           0.0157           0.0000           0.0300           0.0000           0.0191           "]
[null,null,"CO2                   0.0000           0.1449           0.0000           0.4364           0.0000           0.2693           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 0.0000           1.0000           0.0000           1.0000           0.0000           1.0000           "]
[null,null,"Aqueous Phase                                                                                     Phase Fraction 0.0000     "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0092           0.0000           0.0101           0.0000           0.0171           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.4568           0.0000           0.0630           0.0000           0.4595           "]
[null,null,"H2O                   0.0000           0.3734           0.0000           0.4604           0.0000           0.2350           "]
[null,null,"CO                    0.0000           0.0157           0.0000           0.0300           0.0000           0.0191           "]
[null,null,"CO2                   0.0000           0.1449           0.0000           0.4364           0.0000           0.2693           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 0.0000           1.0000           0.0000           1.0000           0.0000           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"mid-coil flue gas (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: mid-coil flue gas                                                   Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase                                                             "]
[null,null,"Vapour / Phase Fraction          1.0000            1.0000                                                                   "]
[null,null,"Temperature: (C)                 510.3             510.3                                                                    "]
[null,null,"Pressure: (kPa)                  107.9             107.9                                                                    "]
[null,null,"Molar Flow (kgmole/h)            241.2             241.2                                                                    "]
[null,null,"Mass Flow (kg/h)                 7018              7018                                                                     "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    8.213             8.213                                                                    "]
[null,null,"Molar Enthalpy (kJ/kgmole)       -2.966e+004       -2.966e+004                                                              "]
[null,null,"Molar Entropy (kJ/kgmole-C)      198.0             198.0                                                                    "]
[null,null,"Heat Flow (kJ/h)                 -7.154e+006       -7.154e+006                                                              "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    ---               ---                                                                      "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase                                                             "]
[null,null,"Molecular Weight                 29.10             29.10                                                                    "]
[null,null,"Molar Density (kgmole/m3)        1.655e-002        1.655e-002                                                               "]
[null,null,"Mass Density (kg/m3)             0.4817            0.4817                                                                   "]
[null,null,"Act. Volume Flow (m3/h)          1.457e+004        1.457e+004                                                               "]
[null,null,"Mass Enthalpy (kJ/kg)            -1019             -1019                                                                    "]
[null,null,"Mass Entropy (kJ/kg-C)           6.806             6.806                                                                    "]
[null,null,"Heat Capacity (kJ/kgmole-C)      33.52             33.52                                                                    "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     1.152             1.152                                                                    "]
[null,null,"Lower Heating Value (kJ/kgmole)  8.541e-004        8.541e-004                                                               "]
[null,null,"Mass Lower Heating Value (kJ/kg) 2.935e-005        2.935e-005                                                               "]
[null,null,"Phase Fraction [Vol. Basis]      ---               1.000                                                                    "]
[null,null,"Phase Fraction [Mass Basis]      4.941e-324        1.000                                                                    "]
[null,null,"Partial Pressure of CO2 (kPa)    7.953             ---                                                                      "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000                                                                   "]
[null,null,"Act. Gas Flow (ACT_m3/h)         1.457e+004        1.457e+004                                                               "]
[null,null,"Avg. Liq. Density (kgmole/m3)    29.36             29.36                                                                    "]
[null,null,"Specific Heat (kJ/kgmole-C)      33.52             33.52                                                                    "]
[null,null,"Std. Gas Flow (STD_m3/h)         5702              5702                                                                     "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 854.4             854.4                                                                   "]
[null,null,"Act. Liq. Flow (m3/s)            ---               ---                                                                      "]
[null,null,"Z Factor                         1.000             1.000                                                                    "]
[null,null,"Watson K                         6.383             6.383                                                                    "]
[null,null,"User Property                    ---               ---                                                                      "]
[null,null,"Cp/(Cp - R)                      1.330             1.330                                                                    "]
[null,null,"Cp/Cv                            1.330             1.330                                                                    "]
[null,null,"Heat of Vap. (kJ/kgmole)         1.859e+004        ---                                                                      "]
[null,null,"Kinematic Viscosity (cSt)        75.48             75.48                                                                    "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) ---               ---                                                                     "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) ---               ---                                                                     "]
[null,null,"Liquid Fraction                  0.0000            0.0000                                                                   "]
[null,null,"Molar Volume (m3/kgmole)         60.41             60.41                                                                    "]
[null,null,"Mass Heat of Vap. (kJ/kg)        638.9             ---                                                                      "]
[null,null,"Phase Fraction [Molar Basis]     1.0000            1.0000                                                                   "]
[null,null,"Surface Tension (dyne/cm)        ---               ---                                                                      "]
[null,null,"Thermal Conductivity (W/m-K)     5.544e-002        5.544e-002                                                               "]
[null,null,"Viscosity (cP)                   3.636e-002        3.636e-002                                                               "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    25.21             25.21                                                                    "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   0.8663            0.8663                                                                   "]
[null,null,"Cv (kJ/kgmole-C)                 25.20             25.20                                                                    "]
[null,null,"Mass Cv (kJ/kg-C)                0.8661            0.8661                                                                   "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   28.01             28.01                                                                    "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  0.9626            0.9626                                                                   "]
[null,null,"Cp/Cv (Ent. Method)              1.197             1.197                                                                    "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---                                                                      "]
[null,null,"True VP at 37.8 C (kPa)          1.874e+005        1.874e+005                                                               "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 0.0000            0.0000                                                                  "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---                                                                      "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 1.0000    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                34.4900          0.1430           1103.6812        0.1573           0.9701           0.1181           "]
[null,null,"Nitrogen              172.8879         0.7169           4843.1080        0.6901           6.0060           0.7313           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   15.9987          0.0663           288.2173         0.0411           0.2888           0.0352           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   17.7814          0.0737           782.5555         0.1115           0.9482           0.1154           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 241.1580         1.0000           7017.5621        1.0000           8.2131           1.0000           "]
[null,null,"Vapour Phase                                                                                      Phase Fraction 1.000      "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                34.4900          0.1430           1103.6812        0.1573           0.9701           0.1181           "]
[null,null,"Nitrogen              172.8879         0.7169           4843.1080        0.6901           6.0060           0.7313           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   15.9987          0.0663           288.2173         0.0411           0.2888           0.0352           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   17.7814          0.0737           782.5555         0.1115           0.9482           0.1154           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 241.1580         1.0000           7017.5621        1.0000           8.2131           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"mixed burner fuel (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: mixed burner fuel                                                   Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase      Aqueous Phase                                          "]
[null,null,"Vapour / Phase Fraction          0.9766            0.9766            0.0234                                                 "]
[null,null,"Temperature: (C)                 11.05             11.05             11.05                                                  "]
[null,null,"Pressure: (kPa)                  115.1             115.1             115.1                                                  "]
[null,null,"Molar Flow (kgmole/h)            27.17             26.53             0.6351                                                 "]
[null,null,"Mass Flow (kg/h)                 710.9             683.4             27.51                                                  "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    1.166             1.131             3.426e-002                                             "]
[null,null,"Molar Enthalpy (kJ/kgmole)       -2.122e+005       -2.105e+005       -2.820e+005                                            "]
[null,null,"Molar Entropy (kJ/kgmole-C)      140.7             144.1             -2.022                                                 "]
[null,null,"Heat Flow (kJ/h)                 -5.765e+006       -5.586e+006       -1.791e+005                                            "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    ---               ---               3.375e-002                                             "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase      Aqueous Phase                                          "]
[null,null,"Molecular Weight                 26.16             25.75             43.31                                                  "]
[null,null,"Molar Density (kgmole/m3)        5.002e-002        4.886e-002        18.90                                                  "]
[null,null,"Mass Density (kg/m3)             1.309             1.258             818.6                                                  "]
[null,null,"Act. Volume Flow (m3/h)          543.1             543.1             3.360e-002                                             "]
[null,null,"Mass Enthalpy (kJ/kg)            -8109             -8174             -6510                                                  "]
[null,null,"Mass Entropy (kJ/kg-C)           5.378             5.596             -4.668e-002                                            "]
[null,null,"Heat Capacity (kJ/kgmole-C)      36.56             34.24             133.5                                                  "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     1.397             1.330             3.083                                                  "]
[null,null,"Lower Heating Value (kJ/kgmole)  ---               ---               ---                                                    "]
[null,null,"Mass Lower Heating Value (kJ/kg) ---               ---               ---                                                    "]
[null,null,"Phase Fraction [Vol. Basis]      0.9706            0.9706            2.939e-002                                             "]
[null,null,"Phase Fraction [Mass Basis]      0.9613            0.9613            3.869e-002                                             "]
[null,null,"Partial Pressure of CO2 (kPa)    56.63             ---               ---                                                    "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000            0.0000                                                 "]
[null,null,"Act. Gas Flow (ACT_m3/h)         ---               543.1             ---                                                    "]
[null,null,"Avg. Liq. Density (kgmole/m3)    23.31             23.45             18.54                                                  "]
[null,null,"Specific Heat (kJ/kgmole-C)      36.56             34.24             133.5                                                  "]
[null,null,"Std. Gas Flow (STD_m3/h)         642.4             627.4             15.02                                                  "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 609.9             604.0             802.8                                                 "]
[null,null,"Act. Liq. Flow (m3/s)            9.334e-006        ---               9.334e-006                                             "]
[null,null,"Z Factor                         ---               0.9971            2.578e-003                                             "]
[null,null,"Watson K                         9.988             9.953             10.74                                                  "]
[null,null,"User Property                    ---               ---               ---                                                    "]
[null,null,"Cp/(Cp - R)                      1.294             1.321             1.066                                                  "]
[null,null,"Cp/Cv                            1.290             1.326             1.107                                                  "]
[null,null,"Heat of Vap. (kJ/kgmole)         2.162e+004        ---               ---                                                    "]
[null,null,"Kinematic Viscosity (cSt)        ---               11.47             1.532                                                  "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) ---               ---               815.0                                                 "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) ---               ---               3.375e-002                                            "]
[null,null,"Liquid Fraction                  2.337e-002        0.0000            1.000                                                  "]
[null,null,"Molar Volume (m3/kgmole)         19.99             20.47             5.291e-002                                             "]
[null,null,"Mass Heat of Vap. (kJ/kg)        826.5             ---               ---                                                    "]
[null,null,"Phase Fraction [Molar Basis]     0.9766            0.9766            0.0234                                                 "]
[null,null,"Surface Tension (dyne/cm)        28.03             ---               28.03                                                  "]
[null,null,"Thermal Conductivity (W/m-K)     ---               4.575e-002        0.1881                                                 "]
[null,null,"Viscosity (cP)                   ---               1.443e-002        1.254                                                  "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    28.25             25.93             125.2                                                  "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   1.080             1.007             2.891                                                  "]
[null,null,"Cv (kJ/kgmole-C)                 28.33             25.82             120.5                                                  "]
[null,null,"Mass Cv (kJ/kg-C)                1.083             1.002             2.783                                                  "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   ---               26.55             ---                                                    "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  ---               1.031             ---                                                    "]
[null,null,"Cp/Cv (Ent. Method)              ---               1.290             ---                                                    "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---               72.44                                                  "]
[null,null,"True VP at 37.8 C (kPa)          ---               ---               150.5                                                  "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 3.375e-002        0.0000            3.375e-002                                            "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---               ---                                                    "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 0.9766    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.8295           0.0305           13.3078          0.0187           0.0444           0.0381           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              10.3323          0.3803           20.8300          0.0293           0.2982           0.2558           "]
[null,null,"H2O                   0.2933           0.0108           5.2840           0.0074           0.0053           0.0045           "]
[null,null,"CO                    1.4166           0.0521           39.6808          0.0558           0.0496           0.0426           "]
[null,null,"CO2                   13.0593          0.4807           574.7360         0.8085           0.6964           0.5974           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               1.2380           0.0456           57.0345          0.0802           0.0717           0.0615           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 27.1691          1.0000           710.8730         1.0000           1.1656           1.0000           "]
[null,null,"Vapour Phase                                                                                      Phase Fraction 0.9766     "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.8295           0.0313           13.3074          0.0195           0.0444           0.0393           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              10.3323          0.3894           20.8299          0.0305           0.2982           0.2636           "]
[null,null,"H2O                   0.2314           0.0087           4.1689           0.0061           0.0042           0.0037           "]
[null,null,"CO                    1.4166           0.0534           39.6805          0.0581           0.0496           0.0439           "]
[null,null,"CO2                   13.0527          0.4919           574.4442         0.8406           0.6960           0.6152           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.6715           0.0253           30.9370          0.0453           0.0389           0.0344           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 26.5340          1.0000           683.3680         1.0000           1.1313           1.0000           "]
[null,null,"Aqueous Phase                                                                                     Phase Fraction 2.337e-002 "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0004           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.0001           0.0001           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   0.0619           0.0975           1.1151           0.0405           0.0011           0.0326           "]
[null,null,"CO                    0.0000           0.0000           0.0003           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0066           0.0104           0.2917           0.0106           0.0004           0.0103           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.5665           0.8920           26.0975          0.9488           0.0328           0.9570           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 0.6351           1.0000           27.5050          1.0000           0.0343           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"mixed vapor (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: mixed vapor                                                         Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase      Aqueous Phase                                          "]
[null,null,"Vapour / Phase Fraction          1.0000            1.0000            0.0000                                                 "]
[null,null,"Temperature: (C)                 210.4             210.4             210.4                                                  "]
[null,null,"Pressure: (kPa)                  2199              2199              2199                                                   "]
[null,null,"Molar Flow (kgmole/h)            61.42             61.42             0.0000                                                 "]
[null,null,"Mass Flow (kg/h)                 1322              1322              0.0000                                                 "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    1.414             1.414             0.0000                                                 "]
[null,null,"Molar Enthalpy (kJ/kgmole)       -2.341e+005       -2.341e+005       -2.701e+005                                            "]
[null,null,"Molar Entropy (kJ/kgmole-C)      161.8             161.8             93.02                                                  "]
[null,null,"Heat Flow (kJ/h)                 -1.438e+007       -1.438e+007       0.0000                                                 "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    1.351             1.351             0.0000                                                 "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase      Aqueous Phase                                          "]
[null,null,"Molecular Weight                 21.52             21.52             18.17                                                  "]
[null,null,"Molar Density (kgmole/m3)        0.6133            0.6133            46.26                                                  "]
[null,null,"Mass Density (kg/m3)             13.20             13.20             840.3                                                  "]
[null,null,"Act. Volume Flow (m3/h)          100.2             100.2             0.0000                                                 "]
[null,null,"Mass Enthalpy (kJ/kg)            -1.088e+004       -1.088e+004       -1.487e+004                                            "]
[null,null,"Mass Entropy (kJ/kg-C)           7.519             7.519             5.121                                                  "]
[null,null,"Heat Capacity (kJ/kgmole-C)      47.59             47.59             90.58                                                  "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     2.211             2.211             4.986                                                  "]
[null,null,"Lower Heating Value (kJ/kgmole)  1.544e+005        1.544e+005        6609                                                   "]
[null,null,"Mass Lower Heating Value (kJ/kg) 7176              7176              363.8                                                  "]
[null,null,"Phase Fraction [Vol. Basis]      ---               1.000             ---                                                    "]
[null,null,"Phase Fraction [Mass Basis]      4.941e-324        1.000             0.0000                                                 "]
[null,null,"Partial Pressure of CO2 (kPa)    0.0000            ---               ---                                                    "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000            0.0000                                                 "]
[null,null,"Act. Gas Flow (ACT_m3/h)         100.2             100.2             ---                                                    "]
[null,null,"Avg. Liq. Density (kgmole/m3)    43.42             43.42             54.75                                                  "]
[null,null,"Specific Heat (kJ/kgmole-C)      47.59             47.59             90.58                                                  "]
[null,null,"Std. Gas Flow (STD_m3/h)         1452              1452              0.0000                                                 "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 934.5             934.5             994.6                                                 "]
[null,null,"Act. Liq. Flow (m3/s)            0.0000            ---               0.0000                                                 "]
[null,null,"Z Factor                         ---               0.8918            1.182e-002                                             "]
[null,null,"Watson K                         10.76             10.76             10.76                                                  "]
[null,null,"User Property                    ---               ---               ---                                                    "]
[null,null,"Cp/(Cp - R)                      1.212             1.212             1.101                                                  "]
[null,null,"Cp/Cv                            1.370             1.370             1.212                                                  "]
[null,null,"Heat of Vap. (kJ/kgmole)         3.462e+004        ---               ---                                                    "]
[null,null,"Kinematic Viscosity (cSt)        0.9725            0.9725            0.1095                                                 "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) 978.7             978.7             1013                                                  "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) 1.351             1.351             0.0000                                                "]
[null,null,"Liquid Fraction                  0.0000            0.0000            1.000                                                  "]
[null,null,"Molar Volume (m3/kgmole)         1.631             1.631             2.162e-002                                             "]
[null,null,"Mass Heat of Vap. (kJ/kg)        1609              ---               ---                                                    "]
[null,null,"Phase Fraction [Molar Basis]     1.0000            1.0000            0.0000                                                 "]
[null,null,"Surface Tension (dyne/cm)        ---               ---               35.27                                                  "]
[null,null,"Thermal Conductivity (W/m-K)     3.631e-002        3.631e-002        0.6514                                                 "]
[null,null,"Viscosity (cP)                   1.284e-002        1.284e-002        9.202e-002                                             "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    39.28             39.28             82.26                                                  "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   1.825             1.825             4.529                                                  "]
[null,null,"Cv (kJ/kgmole-C)                 34.73             34.73             74.70                                                  "]
[null,null,"Mass Cv (kJ/kg-C)                1.614             1.614             4.113                                                  "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   ---               34.82             ---                                                    "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  ---               1.618             ---                                                    "]
[null,null,"Cp/Cv (Ent. Method)              ---               1.367             ---                                                    "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---               ---                                                    "]
[null,null,"True VP at 37.8 C (kPa)          19.69             19.69             19.69                                                  "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 1.351             1.351             0.0000                                                "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---               ---                                                    "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 1.0000    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   53.7425          0.8750           968.1765         0.7324           0.9701           0.6859           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               7.6775           0.1250           353.7017         0.2676           0.4444           0.3141           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 61.4200          1.0000           1321.8782        1.0000           1.4145           1.0000           "]
[null,null,"Vapour Phase                                                                                      Phase Fraction 1.000      "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   53.7425          0.8750           968.1765         0.7324           0.9701           0.6859           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               7.6775           0.1250           353.7017         0.2676           0.4444           0.3141           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 61.4200          1.0000           1321.8782        1.0000           1.4145           1.0000           "]
[null,null,"Aqueous Phase                                                                                     Phase Fraction 0.0000     "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   0.0000           0.9947           0.0000           0.9864           0.0000           0.9830           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0053           0.0000           0.0136           0.0000           0.0170           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 0.0000           1.0000           0.0000           1.0000           0.0000           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Pre-Reformer Dummy liquid (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: Pre-Reformer Dummy liquid                                           Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase      Aqueous Phase                                          "]
[null,null,"Vapour / Phase Fraction          0.0000            0.0000            1.0000                                                 "]
[null,null,"Temperature: (C)                 305.4             305.4             305.4                                                  "]
[null,null,"Pressure: (kPa)                  2189              2189              2189                                                   "]
[null,null,"Molar Flow (kgmole/h)            0.0000            0.0000            0.0000                                                 "]
[null,null,"Mass Flow (kg/h)                 0.0000            0.0000            0.0000                                                 "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    0.0000            0.0000            0.0000                                                 "]
[null,null,"Molar Enthalpy (kJ/kgmole)       -2.589e+005       -1.820e+005       -2.589e+005                                            "]
[null,null,"Molar Entropy (kJ/kgmole-C)      112.7             163.5             112.7                                                  "]
[null,null,"Heat Flow (kJ/h)                 0.0000            0.0000            0.0000                                                 "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    0.0000            0.0000            0.0000                                                 "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase      Aqueous Phase                                          "]
[null,null,"Molecular Weight                 18.07             17.22             18.07                                                  "]
[null,null,"Molar Density (kgmole/m3)        28.19             0.4651            28.19                                                  "]
[null,null,"Mass Density (kg/m3)             509.4             8.007             509.4                                                  "]
[null,null,"Act. Volume Flow (m3/h)          0.0000            0.0000            0.0000                                                 "]
[null,null,"Mass Enthalpy (kJ/kg)            -1.433e+004       -1.057e+004       -1.433e+004                                            "]
[null,null,"Mass Entropy (kJ/kg-C)           6.237             9.495             6.237                                                  "]
[null,null,"Heat Capacity (kJ/kgmole-C)      174.1             38.54             174.1                                                  "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     9.634             2.238             9.634                                                  "]
[null,null,"Lower Heating Value (kJ/kgmole)  1866              1.287e+005        1866                                                   "]
[null,null,"Mass Lower Heating Value (kJ/kg) 103.2             7473              103.2                                                  "]
[null,null,"Phase Fraction [Vol. Basis]      ---               ---               1.000                                                  "]
[null,null,"Phase Fraction [Mass Basis]      4.941e-324        0.0000            1.000                                                  "]
[null,null,"Partial Pressure of CO2 (kPa)    0.0000            ---               ---                                                    "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000            0.0000                                                 "]
[null,null,"Act. Gas Flow (ACT_m3/h)         ---               ---               ---                                                    "]
[null,null,"Avg. Liq. Density (kgmole/m3)    ---               ---               ---                                                    "]
[null,null,"Specific Heat (kJ/kgmole-C)      174.1             38.54             174.1                                                  "]
[null,null,"Std. Gas Flow (STD_m3/h)         0.0000            0.0000            0.0000                                                 "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 987.1             630.8             987.1                                                 "]
[null,null,"Act. Liq. Flow (m3/s)            0.0000            ---               0.0000                                                 "]
[null,null,"Z Factor                         ---               0.9783            1.614e-002                                             "]
[null,null,"Watson K                         10.71             13.77             10.71                                                  "]
[null,null,"User Property                    ---               ---               ---                                                    "]
[null,null,"Cp/(Cp - R)                      1.050             1.275             1.050                                                  "]
[null,null,"Cp/Cv                            1.050             1.320             1.050                                                  "]
[null,null,"Heat of Vap. (kJ/kgmole)         7.330e+004        ---               ---                                                    "]
[null,null,"Kinematic Viscosity (cSt)        0.1365            2.350             0.1364                                                 "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) 1008              595.9             1008                                                  "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) 0.0000            0.0000            0.0000                                                "]
[null,null,"Liquid Fraction                  1.000             0.0000            1.000                                                  "]
[null,null,"Molar Volume (m3/kgmole)         3.548e-002        2.150             3.548e-002                                             "]
[null,null,"Mass Heat of Vap. (kJ/kg)        4056              ---               ---                                                    "]
[null,null,"Phase Fraction [Molar Basis]     0.0000            0.0000            1.0000                                                 "]
[null,null,"Surface Tension (dyne/cm)        12.89             ---               12.89                                                  "]
[null,null,"Thermal Conductivity (W/m-K)     0.5018            7.393e-002        0.5005                                                 "]
[null,null,"Viscosity (cP)                   6.954e-002        1.882e-002        6.949e-002                                             "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    165.8             30.22             165.8                                                  "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   9.174             1.755             9.174                                                  "]
[null,null,"Cv (kJ/kgmole-C)                 165.8             29.20             165.8                                                  "]
[null,null,"Mass Cv (kJ/kg-C)                9.174             1.696             9.174                                                  "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   ---               29.23             ---                                                    "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  ---               1.698             ---                                                    "]
[null,null,"Cp/Cv (Ent. Method)              ---               1.319             ---                                                    "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---               ---                                                    "]
[null,null,"True VP at 37.8 C (kPa)          ---               ---               ---                                                    "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 0.0000            0.0000            0.0000                                                "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---               ---                                                    "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 0.0000    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0010           0.0000           0.0009           0.0000           0.0029           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.0044           0.0000           0.0005           0.0000           0.0069           "]
[null,null,"H2O                   0.0000           0.9897           0.0000           0.9866           0.0000           0.9758           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0049           0.0000           0.0120           0.0000           0.0143           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 0.0000           1.0000           0.0000           1.0000           0.0000           1.0000           "]
[null,null,"Vapour Phase                                                                                      Phase Fraction 0.0000     "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.1000           0.0000           0.0932           0.0000           0.1963           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.2000           0.0000           0.0234           0.0000           0.2115           "]
[null,null,"H2O                   0.0000           0.6000           0.0000           0.6278           0.0000           0.3968           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.1000           0.0000           0.2556           0.0000           0.1954           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 0.0000           1.0000           0.0000           1.0000           0.0000           1.0000           "]
[null,null,"Aqueous Phase                                                                                     Phase Fraction 1.000      "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0010           0.0000           0.0009           0.0000           0.0029           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.0044           0.0000           0.0005           0.0000           0.0069           "]
[null,null,"H2O                   0.0000           0.9897           0.0000           0.9866           0.0000           0.9758           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0049           0.0000           0.0120           0.0000           0.0143           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 0.0000           1.0000           0.0000           1.0000           0.0000           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Pre-Reformer Feed (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: Pre-Reformer Feed                                                   Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase                                                             "]
[null,null,"Vapour / Phase Fraction          1.0000            1.0000                                                                   "]
[null,null,"Temperature: (C)                 350.0             350.0                                                                    "]
[null,null,"Pressure: (kPa)                  2189              2189                                                                     "]
[null,null,"Molar Flow (kgmole/h)            61.42             61.42                                                                    "]
[null,null,"Mass Flow (kg/h)                 1322              1322                                                                     "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    1.414             1.414                                                                    "]
[null,null,"Molar Enthalpy (kJ/kgmole)       -2.275e+005       -2.275e+005                                                              "]
[null,null,"Molar Entropy (kJ/kgmole-C)      174.0             174.0                                                                    "]
[null,null,"Heat Flow (kJ/h)                 -1.397e+007       -1.397e+007                                                              "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    1.351             1.351                                                                    "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase                                                             "]
[null,null,"Molecular Weight                 21.52             21.52                                                                    "]
[null,null,"Molar Density (kgmole/m3)        0.4424            0.4424                                                                   "]
[null,null,"Mass Density (kg/m3)             9.522             9.522                                                                    "]
[null,null,"Act. Volume Flow (m3/h)          138.8             138.8                                                                    "]
[null,null,"Mass Enthalpy (kJ/kg)            -1.057e+004       -1.057e+004                                                              "]
[null,null,"Mass Entropy (kJ/kg-C)           8.083             8.083                                                                    "]
[null,null,"Heat Capacity (kJ/kgmole-C)      48.42             48.42                                                                    "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     2.250             2.250                                                                    "]
[null,null,"Lower Heating Value (kJ/kgmole)  1.544e+005        1.544e+005                                                               "]
[null,null,"Mass Lower Heating Value (kJ/kg) 7176              7176                                                                     "]
[null,null,"Phase Fraction [Vol. Basis]      ---               1.000                                                                    "]
[null,null,"Phase Fraction [Mass Basis]      4.941e-324        1.000                                                                    "]
[null,null,"Partial Pressure of CO2 (kPa)    0.0000            ---                                                                      "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000                                                                   "]
[null,null,"Act. Gas Flow (ACT_m3/h)         138.8             138.8                                                                    "]
[null,null,"Avg. Liq. Density (kgmole/m3)    43.42             43.42                                                                    "]
[null,null,"Specific Heat (kJ/kgmole-C)      48.42             48.42                                                                    "]
[null,null,"Std. Gas Flow (STD_m3/h)         1452              1452                                                                     "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 934.5             934.5                                                                   "]
[null,null,"Act. Liq. Flow (m3/s)            ---               ---                                                                      "]
[null,null,"Z Factor                         0.9548            0.9548                                                                   "]
[null,null,"Watson K                         10.76             10.76                                                                    "]
[null,null,"User Property                    ---               ---                                                                      "]
[null,null,"Cp/(Cp - R)                      1.207             1.207                                                                    "]
[null,null,"Cp/Cv                            1.271             1.271                                                                    "]
[null,null,"Heat of Vap. (kJ/kgmole)         3.464e+004        ---                                                                      "]
[null,null,"Kinematic Viscosity (cSt)        1.791             1.791                                                                    "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) 978.7             978.7                                                                   "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) 1.351             1.351                                                                   "]
[null,null,"Liquid Fraction                  0.0000            0.0000                                                                   "]
[null,null,"Molar Volume (m3/kgmole)         2.260             2.260                                                                    "]
[null,null,"Mass Heat of Vap. (kJ/kg)        1610              ---                                                                      "]
[null,null,"Phase Fraction [Molar Basis]     1.0000            1.0000                                                                   "]
[null,null,"Surface Tension (dyne/cm)        ---               ---                                                                      "]
[null,null,"Thermal Conductivity (W/m-K)     5.005e-002        5.005e-002                                                               "]
[null,null,"Viscosity (cP)                   1.705e-002        1.705e-002                                                               "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    40.11             40.11                                                                    "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   1.864             1.864                                                                    "]
[null,null,"Cv (kJ/kgmole-C)                 38.09             38.09                                                                    "]
[null,null,"Mass Cv (kJ/kg-C)                1.770             1.770                                                                    "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   38.08             38.08                                                                    "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  1.770             1.770                                                                    "]
[null,null,"Cp/Cv (Ent. Method)              1.271             1.271                                                                    "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---                                                                      "]
[null,null,"True VP at 37.8 C (kPa)          19.69             19.69                                                                    "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 1.351             1.351                                                                   "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---                                                                      "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 1.0000    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   53.7425          0.8750           968.1765         0.7324           0.9701           0.6859           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               7.6775           0.1250           353.7017         0.2676           0.4444           0.3141           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 61.4200          1.0000           1321.8782        1.0000           1.4145           1.0000           "]
[null,null,"Vapour Phase                                                                                      Phase Fraction 1.000      "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   53.7425          0.8750           968.1765         0.7324           0.9701           0.6859           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               7.6775           0.1250           353.7017         0.2676           0.4444           0.3141           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 61.4200          1.0000           1321.8782        1.0000           1.4145           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Preheated Air into WGS (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: Preheated Air into WGS                                              Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase                                                             "]
[null,null,"Vapour / Phase Fraction          1.0000            1.0000                                                                   "]
[null,null,"Temperature: (C)                 120.3             120.3                                                                    "]
[null,null,"Pressure: (kPa)                  114.9             114.9                                                                    "]
[null,null,"Molar Flow (kgmole/h)            218.6             218.6                                                                    "]
[null,null,"Mass Flow (kg/h)                 6307              6307                                                                     "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    7.293             7.293                                                                    "]
[null,null,"Molar Enthalpy (kJ/kgmole)       2781              2781                                                                     "]
[null,null,"Molar Entropy (kJ/kgmole-C)      170.5             170.5                                                                    "]
[null,null,"Heat Flow (kJ/h)                 6.081e+005        6.081e+005                                                               "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    ---               ---                                                                      "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase                                                             "]
[null,null,"Molecular Weight                 28.85             28.85                                                                    "]
[null,null,"Molar Density (kgmole/m3)        3.511e-002        3.511e-002                                                               "]
[null,null,"Mass Density (kg/m3)             1.013             1.013                                                                    "]
[null,null,"Act. Volume Flow (m3/h)          6227              6227                                                                     "]
[null,null,"Mass Enthalpy (kJ/kg)            96.42             96.42                                                                    "]
[null,null,"Mass Entropy (kJ/kg-C)           5.909             5.909                                                                    "]
[null,null,"Heat Capacity (kJ/kgmole-C)      29.44             29.44                                                                    "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     1.020             1.020                                                                    "]
[null,null,"Lower Heating Value (kJ/kgmole)  0.0000            0.0000                                                                   "]
[null,null,"Mass Lower Heating Value (kJ/kg) ---               ---                                                                      "]
[null,null,"Phase Fraction [Vol. Basis]      ---               1.000                                                                    "]
[null,null,"Phase Fraction [Mass Basis]      4.941e-324        1.000                                                                    "]
[null,null,"Partial Pressure of CO2 (kPa)    0.0000            ---                                                                      "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000                                                                   "]
[null,null,"Act. Gas Flow (ACT_m3/h)         6227              6227                                                                     "]
[null,null,"Avg. Liq. Density (kgmole/m3)    29.98             29.98                                                                    "]
[null,null,"Specific Heat (kJ/kgmole-C)      29.44             29.44                                                                    "]
[null,null,"Std. Gas Flow (STD_m3/h)         5169              5169                                                                     "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 864.8             864.8                                                                   "]
[null,null,"Act. Liq. Flow (m3/s)            ---               ---                                                                      "]
[null,null,"Z Factor                         1.000             1.000                                                                    "]
[null,null,"Watson K                         6.043             6.043                                                                    "]
[null,null,"User Property                    ---               ---                                                                      "]
[null,null,"Cp/(Cp - R)                      1.394             1.394                                                                    "]
[null,null,"Cp/Cv                            1.395             1.395                                                                    "]
[null,null,"Heat of Vap. (kJ/kgmole)         5862              ---                                                                      "]
[null,null,"Kinematic Viscosity (cSt)        22.74             22.74                                                                    "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) ---               ---                                                                     "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) ---               ---                                                                     "]
[null,null,"Liquid Fraction                  0.0000            0.0000                                                                   "]
[null,null,"Molar Volume (m3/kgmole)         28.48             28.48                                                                    "]
[null,null,"Mass Heat of Vap. (kJ/kg)        203.2             ---                                                                      "]
[null,null,"Phase Fraction [Molar Basis]     1.0000            1.0000                                                                   "]
[null,null,"Surface Tension (dyne/cm)        ---               ---                                                                      "]
[null,null,"Thermal Conductivity (W/m-K)     3.216e-002        3.216e-002                                                               "]
[null,null,"Viscosity (cP)                   2.304e-002        2.304e-002                                                               "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    21.12             21.12                                                                    "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   0.7322            0.7322                                                                   "]
[null,null,"Cv (kJ/kgmole-C)                 21.09             21.09                                                                    "]
[null,null,"Mass Cv (kJ/kg-C)                0.7313            0.7313                                                                   "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   21.06             21.06                                                                    "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  0.7299            0.7299                                                                   "]
[null,null,"Cp/Cv (Ent. Method)              1.398             1.398                                                                    "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---                                                                      "]
[null,null,"True VP at 37.8 C (kPa)          ---               ---                                                                      "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 0.0000            0.0000                                                                  "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---                                                                      "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 1.0000    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                45.7375          0.2092           1463.6010        0.2321           1.2865           0.1764           "]
[null,null,"Nitrogen              172.8879         0.7908           4843.1080        0.7679           6.0060           0.8236           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 218.6254         1.0000           6306.7090        1.0000           7.2925           1.0000           "]
[null,null,"Vapour Phase                                                                                      Phase Fraction 1.000      "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                45.7375          0.2092           1463.6010        0.2321           1.2865           0.1764           "]
[null,null,"Nitrogen              172.8879         0.7908           4843.1080        0.7679           6.0060           0.8236           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 218.6254         1.0000           6306.7090        1.0000           7.2925           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"preheated burner air #1 (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: preheated burner air #1                                             Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase                                                             "]
[null,null,"Vapour / Phase Fraction          1.0000            1.0000                                                                   "]
[null,null,"Temperature: (C)                 255.3             255.3                                                                    "]
[null,null,"Pressure: (kPa)                  112.9             112.9                                                                    "]
[null,null,"Molar Flow (kgmole/h)            218.6             218.6                                                                    "]
[null,null,"Mass Flow (kg/h)                 6307              6307                                                                     "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    7.293             7.293                                                                    "]
[null,null,"Molar Enthalpy (kJ/kgmole)       6798              6798                                                                     "]
[null,null,"Molar Entropy (kJ/kgmole-C)      179.4             179.4                                                                    "]
[null,null,"Heat Flow (kJ/h)                 1.486e+006        1.486e+006                                                               "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    ---               ---                                                                      "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase                                                             "]
[null,null,"Molecular Weight                 28.85             28.85                                                                    "]
[null,null,"Molar Density (kgmole/m3)        2.568e-002        2.568e-002                                                               "]
[null,null,"Mass Density (kg/m3)             0.7408            0.7408                                                                   "]
[null,null,"Act. Volume Flow (m3/h)          8514              8514                                                                     "]
[null,null,"Mass Enthalpy (kJ/kg)            235.6             235.6                                                                    "]
[null,null,"Mass Entropy (kJ/kg-C)           6.218             6.218                                                                    "]
[null,null,"Heat Capacity (kJ/kgmole-C)      30.10             30.10                                                                    "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     1.044             1.044                                                                    "]
[null,null,"Lower Heating Value (kJ/kgmole)  0.0000            0.0000                                                                   "]
[null,null,"Mass Lower Heating Value (kJ/kg) ---               ---                                                                      "]
[null,null,"Phase Fraction [Vol. Basis]      ---               1.000                                                                    "]
[null,null,"Phase Fraction [Mass Basis]      4.941e-324        1.000                                                                    "]
[null,null,"Partial Pressure of CO2 (kPa)    0.0000            ---                                                                      "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000                                                                   "]
[null,null,"Act. Gas Flow (ACT_m3/h)         8514              8514                                                                     "]
[null,null,"Avg. Liq. Density (kgmole/m3)    29.98             29.98                                                                    "]
[null,null,"Specific Heat (kJ/kgmole-C)      30.10             30.10                                                                    "]
[null,null,"Std. Gas Flow (STD_m3/h)         5169              5169                                                                     "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 864.8             864.8                                                                   "]
[null,null,"Act. Liq. Flow (m3/s)            ---               ---                                                                      "]
[null,null,"Z Factor                         1.000             1.000                                                                    "]
[null,null,"Watson K                         6.043             6.043                                                                    "]
[null,null,"User Property                    ---               ---                                                                      "]
[null,null,"Cp/(Cp - R)                      1.382             1.382                                                                    "]
[null,null,"Cp/Cv                            1.382             1.382                                                                    "]
[null,null,"Heat of Vap. (kJ/kgmole)         5868              ---                                                                      "]
[null,null,"Kinematic Viscosity (cSt)        38.39             38.39                                                                    "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) ---               ---                                                                     "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) ---               ---                                                                     "]
[null,null,"Liquid Fraction                  0.0000            0.0000                                                                   "]
[null,null,"Molar Volume (m3/kgmole)         38.94             38.94                                                                    "]
[null,null,"Mass Heat of Vap. (kJ/kg)        203.4             ---                                                                      "]
[null,null,"Phase Fraction [Molar Basis]     1.0000            1.0000                                                                   "]
[null,null,"Surface Tension (dyne/cm)        ---               ---                                                                      "]
[null,null,"Thermal Conductivity (W/m-K)     4.042e-002        4.042e-002                                                               "]
[null,null,"Viscosity (cP)                   2.844e-002        2.844e-002                                                               "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    21.79             21.79                                                                    "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   0.7554            0.7554                                                                   "]
[null,null,"Cv (kJ/kgmole-C)                 21.78             21.78                                                                    "]
[null,null,"Mass Cv (kJ/kg-C)                0.7549            0.7549                                                                   "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   21.74             21.74                                                                    "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  0.7537            0.7537                                                                   "]
[null,null,"Cp/Cv (Ent. Method)              1.385             1.385                                                                    "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---                                                                      "]
[null,null,"True VP at 37.8 C (kPa)          ---               ---                                                                      "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 0.0000            0.0000                                                                  "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---                                                                      "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 1.0000    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                45.7375          0.2092           1463.6010        0.2321           1.2865           0.1764           "]
[null,null,"Nitrogen              172.8879         0.7908           4843.1080        0.7679           6.0060           0.8236           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 218.6254         1.0000           6306.7090        1.0000           7.2925           1.0000           "]
[null,null,"Vapour Phase                                                                                      Phase Fraction 1.000      "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                45.7375          0.2092           1463.6010        0.2321           1.2865           0.1764           "]
[null,null,"Nitrogen              172.8879         0.7908           4843.1080        0.7679           6.0060           0.8236           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 218.6254         1.0000           6306.7090        1.0000           7.2925           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Preheated Burner Air #2 (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: Preheated Burner Air #2                                             Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase                                                             "]
[null,null,"Vapour / Phase Fraction          1.0000            1.0000                                                                   "]
[null,null,"Temperature: (C)                 381.3             381.3                                                                    "]
[null,null,"Pressure: (kPa)                  110.9             110.9                                                                    "]
[null,null,"Molar Flow (kgmole/h)            218.6             218.6                                                                    "]
[null,null,"Mass Flow (kg/h)                 6307              6307                                                                     "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    7.293             7.293                                                                    "]
[null,null,"Molar Enthalpy (kJ/kgmole)       1.064e+004        1.064e+004                                                               "]
[null,null,"Molar Entropy (kJ/kgmole-C)      186.0             186.0                                                                    "]
[null,null,"Heat Flow (kJ/h)                 2.326e+006        2.326e+006                                                               "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    ---               ---                                                                      "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase                                                             "]
[null,null,"Molecular Weight                 28.85             28.85                                                                    "]
[null,null,"Molar Density (kgmole/m3)        2.037e-002        2.037e-002                                                               "]
[null,null,"Mass Density (kg/m3)             0.5876            0.5876                                                                   "]
[null,null,"Act. Volume Flow (m3/h)          1.073e+004        1.073e+004                                                               "]
[null,null,"Mass Enthalpy (kJ/kg)            368.8             368.8                                                                    "]
[null,null,"Mass Entropy (kJ/kg-C)           6.449             6.449                                                                    "]
[null,null,"Heat Capacity (kJ/kgmole-C)      30.90             30.90                                                                    "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     1.071             1.071                                                                    "]
[null,null,"Lower Heating Value (kJ/kgmole)  0.0000            0.0000                                                                   "]
[null,null,"Mass Lower Heating Value (kJ/kg) ---               ---                                                                      "]
[null,null,"Phase Fraction [Vol. Basis]      ---               1.000                                                                    "]
[null,null,"Phase Fraction [Mass Basis]      4.941e-324        1.000                                                                    "]
[null,null,"Partial Pressure of CO2 (kPa)    0.0000            ---                                                                      "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000                                                                   "]
[null,null,"Act. Gas Flow (ACT_m3/h)         1.073e+004        1.073e+004                                                               "]
[null,null,"Avg. Liq. Density (kgmole/m3)    29.98             29.98                                                                    "]
[null,null,"Specific Heat (kJ/kgmole-C)      30.90             30.90                                                                    "]
[null,null,"Std. Gas Flow (STD_m3/h)         5169              5169                                                                     "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 864.8             864.8                                                                   "]
[null,null,"Act. Liq. Flow (m3/s)            ---               ---                                                                      "]
[null,null,"Z Factor                         1.000             1.000                                                                    "]
[null,null,"Watson K                         6.043             6.043                                                                    "]
[null,null,"User Property                    ---               ---                                                                      "]
[null,null,"Cp/(Cp - R)                      1.368             1.368                                                                    "]
[null,null,"Cp/Cv                            1.369             1.369                                                                    "]
[null,null,"Heat of Vap. (kJ/kgmole)         5873              ---                                                                      "]
[null,null,"Kinematic Viscosity (cSt)        57.04             57.04                                                                    "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) ---               ---                                                                     "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) ---               ---                                                                     "]
[null,null,"Liquid Fraction                  0.0000            0.0000                                                                   "]
[null,null,"Molar Volume (m3/kgmole)         49.10             49.10                                                                    "]
[null,null,"Mass Heat of Vap. (kJ/kg)        203.6             ---                                                                      "]
[null,null,"Phase Fraction [Molar Basis]     1.0000            1.0000                                                                   "]
[null,null,"Surface Tension (dyne/cm)        ---               ---                                                                      "]
[null,null,"Thermal Conductivity (W/m-K)     4.779e-002        4.779e-002                                                               "]
[null,null,"Viscosity (cP)                   3.351e-002        3.351e-002                                                               "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    22.59             22.59                                                                    "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   0.7830            0.7830                                                                   "]
[null,null,"Cv (kJ/kgmole-C)                 22.58             22.58                                                                    "]
[null,null,"Mass Cv (kJ/kg-C)                0.7827            0.7827                                                                   "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   22.66             22.66                                                                    "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  0.7857            0.7857                                                                   "]
[null,null,"Cp/Cv (Ent. Method)              1.363             1.363                                                                    "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---                                                                      "]
[null,null,"True VP at 37.8 C (kPa)          ---               ---                                                                      "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 0.0000            0.0000                                                                  "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---                                                                      "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 1.0000    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                45.7375          0.2092           1463.6010        0.2321           1.2865           0.1764           "]
[null,null,"Nitrogen              172.8879         0.7908           4843.1080        0.7679           6.0060           0.8236           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 218.6254         1.0000           6306.7090        1.0000           7.2925           1.0000           "]
[null,null,"Vapour Phase                                                                                      Phase Fraction 1.000      "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                45.7375          0.2092           1463.6010        0.2321           1.2865           0.1764           "]
[null,null,"Nitrogen              172.8879         0.7908           4843.1080        0.7679           6.0060           0.8236           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 218.6254         1.0000           6306.7090        1.0000           7.2925           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Product Hydrogen 2 (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: Product Hydrogen 2                                                  Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase                                                             "]
[null,null,"Vapour / Phase Fraction          1.0000            1.0000                                                                   "]
[null,null,"Temperature: (C)                 45.00             45.00                                                                    "]
[null,null,"Pressure: (kPa)                  2135              2135                                                                     "]
[null,null,"Molar Flow (kgmole/h)            31.00             31.00                                                                    "]
[null,null,"Mass Flow (kg/h)                 62.49             62.49                                                                    "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    0.8945            0.8945                                                                   "]
[null,null,"Molar Enthalpy (kJ/kgmole)       569.7             569.7                                                                    "]
[null,null,"Molar Entropy (kJ/kgmole-C)      63.76             63.76                                                                    "]
[null,null,"Heat Flow (kJ/h)                 1.766e+004        1.766e+004                                                               "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    ---               ---                                                                      "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase                                                             "]
[null,null,"Molecular Weight                 2.016             2.016                                                                    "]
[null,null,"Molar Density (kgmole/m3)        0.8009            0.8009                                                                   "]
[null,null,"Mass Density (kg/m3)             1.615             1.615                                                                    "]
[null,null,"Act. Volume Flow (m3/h)          38.70             38.70                                                                    "]
[null,null,"Mass Enthalpy (kJ/kg)            282.6             282.6                                                                    "]
[null,null,"Mass Entropy (kJ/kg-C)           31.63             31.63                                                                    "]
[null,null,"Heat Capacity (kJ/kgmole-C)      28.65             28.65                                                                    "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     14.21             14.21                                                                    "]
[null,null,"Lower Heating Value (kJ/kgmole)  2.419e+005        2.419e+005                                                               "]
[null,null,"Mass Lower Heating Value (kJ/kg) 1.200e+005        1.200e+005                                                               "]
[null,null,"Phase Fraction [Vol. Basis]      ---               1.000                                                                    "]
[null,null,"Phase Fraction [Mass Basis]      4.941e-324        1.000                                                                    "]
[null,null,"Partial Pressure of CO2 (kPa)    0.0000            ---                                                                      "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000                                                                   "]
[null,null,"Act. Gas Flow (ACT_m3/h)         38.70             38.70                                                                    "]
[null,null,"Avg. Liq. Density (kgmole/m3)    34.65             34.65                                                                    "]
[null,null,"Specific Heat (kJ/kgmole-C)      28.65             28.65                                                                    "]
[null,null,"Std. Gas Flow (STD_m3/h)         732.9             732.9                                                                    "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 69.86             69.86                                                                   "]
[null,null,"Act. Liq. Flow (m3/s)            ---               ---                                                                      "]
[null,null,"Z Factor                         1.008             1.008                                                                    "]
[null,null,"Watson K                         47.60             47.60                                                                    "]
[null,null,"User Property                    ---               ---                                                                      "]
[null,null,"Cp/(Cp - R)                      1.409             1.409                                                                    "]
[null,null,"Cp/Cv                            1.416             1.416                                                                    "]
[null,null,"Heat of Vap. (kJ/kgmole)         ---               ---                                                                      "]
[null,null,"Kinematic Viscosity (cSt)        5.606             5.784                                                                    "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) ---               ---                                                                     "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) ---               ---                                                                     "]
[null,null,"Liquid Fraction                  0.0000            0.0000                                                                   "]
[null,null,"Molar Volume (m3/kgmole)         1.249             1.249                                                                    "]
[null,null,"Mass Heat of Vap. (kJ/kg)        ---               ---                                                                      "]
[null,null,"Phase Fraction [Molar Basis]     1.0000            1.0000                                                                   "]
[null,null,"Surface Tension (dyne/cm)        ---               ---                                                                      "]
[null,null,"Thermal Conductivity (W/m-K)     0.1851            0.1852                                                                   "]
[null,null,"Viscosity (cP)                   9.051e-003        9.339e-003                                                               "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    20.34             20.34                                                                    "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   10.09             10.09                                                                    "]
[null,null,"Cv (kJ/kgmole-C)                 20.23             20.23                                                                    "]
[null,null,"Mass Cv (kJ/kg-C)                10.04             10.04                                                                    "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   20.23             20.23                                                                    "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  10.03             10.03                                                                    "]
[null,null,"Cp/Cv (Ent. Method)              1.417             1.417                                                                    "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---                                                                      "]
[null,null,"True VP at 37.8 C (kPa)          ---               ---                                                                      "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 0.0000            0.0000                                                                  "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---                                                                      "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 1.0000    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              30.9970          1.0000           62.4899          1.0000           0.8945           1.0000           "]
[null,null,"H2O                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 30.9970          1.0000           62.4899          1.0000           0.8945           1.0000           "]
[null,null,"Vapour Phase                                                                                      Phase Fraction 1.000      "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              30.9970          1.0000           62.4899          1.0000           0.8945           1.0000           "]
[null,null,"H2O                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 30.9970          1.0000           62.4899          1.0000           0.8945           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"PSA Waste Gas (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: PSA Waste Gas                                                       Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase      Aqueous Phase                                          "]
[null,null,"Vapour / Phase Fraction          0.9964            0.9964            0.0036                                                 "]
[null,null,"Temperature: (C)                 52.16             52.16             52.16                                                  "]
[null,null,"Pressure: (kPa)                  2135              2135              2135                                                   "]
[null,null,"Molar Flow (kgmole/h)            25.93             25.84             9.260e-002                                             "]
[null,null,"Mass Flow (kg/h)                 653.8             652.2             1.675                                                  "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    1.094             1.092             1.681e-003                                             "]
[null,null,"Molar Enthalpy (kJ/kgmole)       -2.090e+005       -2.087e+005       -2.836e+005                                            "]
[null,null,"Molar Entropy (kJ/kgmole-C)      123.3             123.5             60.74                                                  "]
[null,null,"Heat Flow (kJ/h)                 -5.420e+006       -5.393e+006       -2.626e+004                                            "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    ---               ---               1.649e-003                                             "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase      Aqueous Phase                                          "]
[null,null,"Molecular Weight                 25.21             25.24             18.09                                                  "]
[null,null,"Molar Density (kgmole/m3)        0.8131            0.8102            54.63                                                  "]
[null,null,"Mass Density (kg/m3)             20.50             20.45             988.2                                                  "]
[null,null,"Act. Volume Flow (m3/h)          31.89             31.89             1.695e-003                                             "]
[null,null,"Mass Enthalpy (kJ/kg)            -8289             -8270             -1.568e+004                                            "]
[null,null,"Mass Entropy (kJ/kg-C)           4.889             4.893             3.358                                                  "]
[null,null,"Heat Capacity (kJ/kgmole-C)      36.02             35.87             77.83                                                  "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     1.429             1.421             4.303                                                  "]
[null,null,"Lower Heating Value (kJ/kgmole)  ---               ---               ---                                                    "]
[null,null,"Mass Lower Heating Value (kJ/kg) ---               ---               ---                                                    "]
[null,null,"Phase Fraction [Vol. Basis]      0.9985            0.9985            1.537e-003                                             "]
[null,null,"Phase Fraction [Mass Basis]      0.9974            0.9974            2.562e-003                                             "]
[null,null,"Partial Pressure of CO2 (kPa)    1079              ---               ---                                                    "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000            0.0000                                                 "]
[null,null,"Act. Gas Flow (ACT_m3/h)         ---               31.89             ---                                                    "]
[null,null,"Avg. Liq. Density (kgmole/m3)    23.70             23.66             55.09                                                  "]
[null,null,"Specific Heat (kJ/kgmole-C)      36.02             35.87             77.83                                                  "]
[null,null,"Std. Gas Flow (STD_m3/h)         613.1             610.9             2.190                                                  "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 597.7             597.1             996.5                                                 "]
[null,null,"Act. Liq. Flow (m3/s)            4.708e-007        ---               4.708e-007                                             "]
[null,null,"Z Factor                         ---               0.9740            1.445e-002                                             "]
[null,null,"Watson K                         9.906             9.906             8.535                                                  "]
[null,null,"User Property                    ---               ---               ---                                                    "]
[null,null,"Cp/(Cp - R)                      1.300             1.302             1.120                                                  "]
[null,null,"Cp/Cv                            1.366             1.370             1.161                                                  "]
[null,null,"Heat of Vap. (kJ/kgmole)         2.033e+004        ---               ---                                                    "]
[null,null,"Kinematic Viscosity (cSt)        ---               0.8185            0.5656                                                 "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) ---               ---               1016                                                  "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) ---               ---               1.649e-003                                            "]
[null,null,"Liquid Fraction                  3.571e-003        0.0000            1.000                                                  "]
[null,null,"Molar Volume (m3/kgmole)         1.230             1.234             1.830e-002                                             "]
[null,null,"Mass Heat of Vap. (kJ/kg)        806.2             ---               ---                                                    "]
[null,null,"Phase Fraction [Molar Basis]     0.9964            0.9964            0.0036                                                 "]
[null,null,"Surface Tension (dyne/cm)        67.16             ---               67.16                                                  "]
[null,null,"Thermal Conductivity (W/m-K)     ---               5.466e-002        0.6422                                                 "]
[null,null,"Viscosity (cP)                   ---               1.674e-002        0.5590                                                 "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    27.71             27.56             69.52                                                  "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   1.099             1.092             3.843                                                  "]
[null,null,"Cv (kJ/kgmole-C)                 26.37             26.19             67.02                                                  "]
[null,null,"Mass Cv (kJ/kg-C)                1.046             1.038             3.705                                                  "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   31.17             20.37             ---                                                    "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  1.236             0.8070            ---                                                    "]
[null,null,"Cp/Cv (Ent. Method)              1.156             1.761             ---                                                    "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---               ---                                                    "]
[null,null,"True VP at 37.8 C (kPa)          ---               ---               2429                                                   "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 1.649e-003        0.0000            1.649e-003                                            "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---               ---                                                    "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 0.9964    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.8295           0.0320           13.3078          0.0204           0.0444           0.0406           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              10.3323          0.3985           20.8300          0.0319           0.2982           0.2726           "]
[null,null,"H2O                   0.2933           0.0113           5.2840           0.0081           0.0053           0.0048           "]
[null,null,"CO                    1.4166           0.0546           39.6808          0.0607           0.0496           0.0454           "]
[null,null,"CO2                   13.0593          0.5036           574.7360         0.8790           0.6964           0.6366           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 25.9311          1.0000           653.8385         1.0000           1.0939           1.0000           "]
[null,null,"Vapour Phase                                                                                      Phase Fraction 0.9964     "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.8295           0.0321           13.3078          0.0204           0.0444           0.0407           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              10.3323          0.3999           20.8299          0.0319           0.2982           0.2730           "]
[null,null,"H2O                   0.2010           0.0078           3.6205           0.0056           0.0036           0.0033           "]
[null,null,"CO                    1.4166           0.0548           39.6808          0.0608           0.0496           0.0454           "]
[null,null,"CO2                   13.0590          0.5054           574.7243         0.8813           0.6964           0.6375           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 25.8385          1.0000           652.1634         1.0000           1.0922           1.0000           "]
[null,null,"Aqueous Phase                                                                                     Phase Fraction 3.571e-003 "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"H2O                   0.0923           0.9971           1.6634           0.9930           0.0017           0.9916           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0003           0.0029           0.0117           0.0070           0.0000           0.0084           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 0.0926           1.0000           1.6751           1.0000           0.0017           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Reformate into Condensor (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: Reformate into Condensor                                            Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase                                                             "]
[null,null,"Vapour / Phase Fraction          1.0000            1.0000                                                                   "]
[null,null,"Temperature: (C)                 240.5             240.5                                                                    "]
[null,null,"Pressure: (kPa)                  2135              2135                                                                     "]
[null,null,"Molar Flow (kgmole/h)            90.47             90.47                                                                    "]
[null,null,"Mass Flow (kg/h)                 1322              1322                                                                     "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    2.596             2.596                                                                    "]
[null,null,"Molar Enthalpy (kJ/kgmole)       -1.426e+005       -1.426e+005                                                              "]
[null,null,"Molar Entropy (kJ/kgmole-C)      135.4             135.4                                                                    "]
[null,null,"Heat Flow (kJ/h)                 -1.290e+007       -1.290e+007                                                              "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    ---               ---                                                                      "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase                                                             "]
[null,null,"Molecular Weight                 14.61             14.61                                                                    "]
[null,null,"Molar Density (kgmole/m3)        0.5068            0.5068                                                                   "]
[null,null,"Mass Density (kg/m3)             7.404             7.404                                                                    "]
[null,null,"Act. Volume Flow (m3/h)          178.5             178.5                                                                    "]
[null,null,"Mass Enthalpy (kJ/kg)            -9760             -9760                                                                    "]
[null,null,"Mass Entropy (kJ/kg-C)           9.264             9.264                                                                    "]
[null,null,"Heat Capacity (kJ/kgmole-C)      34.87             34.87                                                                    "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     2.386             2.386                                                                    "]
[null,null,"Lower Heating Value (kJ/kgmole)  ---               ---                                                                      "]
[null,null,"Mass Lower Heating Value (kJ/kg) ---               ---                                                                      "]
[null,null,"Phase Fraction [Vol. Basis]      ---               1.000                                                                    "]
[null,null,"Phase Fraction [Mass Basis]      4.941e-324        1.000                                                                    "]
[null,null,"Partial Pressure of CO2 (kPa)    309.3             ---                                                                      "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000                                                                   "]
[null,null,"Act. Gas Flow (ACT_m3/h)         178.5             178.5                                                                    "]
[null,null,"Avg. Liq. Density (kgmole/m3)    34.85             34.85                                                                    "]
[null,null,"Specific Heat (kJ/kgmole-C)      34.87             34.87                                                                    "]
[null,null,"Std. Gas Flow (STD_m3/h)         2139              2139                                                                     "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 509.3             509.3                                                                   "]
[null,null,"Act. Liq. Flow (m3/s)            ---               ---                                                                      "]
[null,null,"Z Factor                         0.9864            0.9864                                                                   "]
[null,null,"Watson K                         13.34             13.34                                                                    "]
[null,null,"User Property                    ---               ---                                                                      "]
[null,null,"Cp/(Cp - R)                      1.313             1.313                                                                    "]
[null,null,"Cp/Cv                            1.350             1.350                                                                    "]
[null,null,"Heat of Vap. (kJ/kgmole)         4.084e+004        ---                                                                      "]
[null,null,"Kinematic Viscosity (cSt)        2.210             2.400                                                                    "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) ---               ---                                                                     "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) ---               ---                                                                     "]
[null,null,"Liquid Fraction                  0.0000            0.0000                                                                   "]
[null,null,"Molar Volume (m3/kgmole)         1.973             1.973                                                                    "]
[null,null,"Mass Heat of Vap. (kJ/kg)        2795              ---                                                                      "]
[null,null,"Phase Fraction [Molar Basis]     1.0000            1.0000                                                                   "]
[null,null,"Surface Tension (dyne/cm)        ---               ---                                                                      "]
[null,null,"Thermal Conductivity (W/m-K)     9.911e-002        9.912e-002                                                               "]
[null,null,"Viscosity (cP)                   1.636e-002        1.777e-002                                                               "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    26.55             26.55                                                                    "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   1.817             1.817                                                                    "]
[null,null,"Cv (kJ/kgmole-C)                 25.82             25.82                                                                    "]
[null,null,"Mass Cv (kJ/kg-C)                1.767             1.767                                                                    "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   27.76             27.76                                                                    "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  1.900             1.900                                                                    "]
[null,null,"Cp/Cv (Ent. Method)              1.256             1.256                                                                    "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---                                                                      "]
[null,null,"True VP at 37.8 C (kPa)          ---               ---                                                                      "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 0.0000            0.0000                                                                  "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---                                                                      "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 1.0000    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.8295           0.0092           13.3078          0.0101           0.0444           0.0171           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              41.3303          0.4568           83.3218          0.0630           1.1927           0.4595           "]
[null,null,"H2O                   33.7857          0.3734           608.6526         0.4604           0.6099           0.2350           "]
[null,null,"CO                    1.4167           0.0157           39.6819          0.0300           0.0496           0.0191           "]
[null,null,"CO2                   13.1088          0.1449           576.9154         0.4364           0.6990           0.2693           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0001           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 90.4710          1.0000           1321.8797        1.0000           2.5957           1.0000           "]
[null,null,"Vapour Phase                                                                                      Phase Fraction 1.000      "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.8295           0.0092           13.3078          0.0101           0.0444           0.0171           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              41.3303          0.4568           83.3218          0.0630           1.1927           0.4595           "]
[null,null,"H2O                   33.7857          0.3734           608.6526         0.4604           0.6099           0.2350           "]
[null,null,"CO                    1.4167           0.0157           39.6819          0.0300           0.0496           0.0191           "]
[null,null,"CO2                   13.1088          0.1449           576.9154         0.4364           0.6990           0.2693           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0001           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 90.4710          1.0000           1321.8797        1.0000           2.5957           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Reformer Feed (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: Reformer Feed                                                       Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase      Aqueous Phase                                          "]
[null,null,"Vapour / Phase Fraction          1.0000            1.0000            0.0000                                                 "]
[null,null,"Temperature: (C)                 305.4             305.4             305.4                                                  "]
[null,null,"Pressure: (kPa)                  2189              2189              2189                                                   "]
[null,null,"Molar Flow (kgmole/h)            76.78             76.78             0.0000                                                 "]
[null,null,"Mass Flow (kg/h)                 1322              1322              0.0000                                                 "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    2.095             2.095             0.0000                                                 "]
[null,null,"Molar Enthalpy (kJ/kgmole)       -1.820e+005       -1.820e+005       -2.589e+005                                            "]
[null,null,"Molar Entropy (kJ/kgmole-C)      163.5             163.5             112.7                                                  "]
[null,null,"Heat Flow (kJ/h)                 -1.397e+007       -1.397e+007       0.0000                                                 "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    2.218             2.218             0.0000                                                 "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase      Aqueous Phase                                          "]
[null,null,"Molecular Weight                 17.22             17.22             18.07                                                  "]
[null,null,"Molar Density (kgmole/m3)        0.4651            0.4651            28.19                                                  "]
[null,null,"Mass Density (kg/m3)             8.007             8.007             509.4                                                  "]
[null,null,"Act. Volume Flow (m3/h)          165.1             165.1             0.0000                                                 "]
[null,null,"Mass Enthalpy (kJ/kg)            -1.057e+004       -1.057e+004       -1.433e+004                                            "]
[null,null,"Mass Entropy (kJ/kg-C)           9.495             9.495             6.237                                                  "]
[null,null,"Heat Capacity (kJ/kgmole-C)      38.54             38.54             174.1                                                  "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     2.238             2.238             9.634                                                  "]
[null,null,"Lower Heating Value (kJ/kgmole)  1.287e+005        1.287e+005        1866                                                   "]
[null,null,"Mass Lower Heating Value (kJ/kg) 7473              7473              103.2                                                  "]
[null,null,"Phase Fraction [Vol. Basis]      ---               1.000             ---                                                    "]
[null,null,"Phase Fraction [Mass Basis]      4.941e-324        1.000             0.0000                                                 "]
[null,null,"Partial Pressure of CO2 (kPa)    218.9             ---               ---                                                    "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000            0.0000                                                 "]
[null,null,"Act. Gas Flow (ACT_m3/h)         165.1             165.1             ---                                                    "]
[null,null,"Avg. Liq. Density (kgmole/m3)    36.64             36.64             54.62                                                  "]
[null,null,"Specific Heat (kJ/kgmole-C)      38.54             38.54             174.1                                                  "]
[null,null,"Std. Gas Flow (STD_m3/h)         1815              1815              0.0000                                                 "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 630.8             630.8             987.1                                                 "]
[null,null,"Act. Liq. Flow (m3/s)            0.0000            ---               0.0000                                                 "]
[null,null,"Z Factor                         ---               0.9783            1.614e-002                                             "]
[null,null,"Watson K                         13.77             13.77             10.71                                                  "]
[null,null,"User Property                    ---               ---               ---                                                    "]
[null,null,"Cp/(Cp - R)                      1.275             1.275             1.050                                                  "]
[null,null,"Cp/Cv                            1.320             1.320             1.050                                                  "]
[null,null,"Heat of Vap. (kJ/kgmole)         5.457e+004        ---               ---                                                    "]
[null,null,"Kinematic Viscosity (cSt)        2.293             2.350             0.1364                                                 "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) 585.2             595.9             1008                                                  "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) 2.218             2.218             0.0000                                                "]
[null,null,"Liquid Fraction                  0.0000            0.0000            1.000                                                  "]
[null,null,"Molar Volume (m3/kgmole)         2.150             2.150             3.548e-002                                             "]
[null,null,"Mass Heat of Vap. (kJ/kg)        3169              ---               ---                                                    "]
[null,null,"Phase Fraction [Molar Basis]     1.0000            1.0000            0.0000                                                 "]
[null,null,"Surface Tension (dyne/cm)        ---               ---               12.89                                                  "]
[null,null,"Thermal Conductivity (W/m-K)     7.393e-002        7.393e-002        0.5005                                                 "]
[null,null,"Viscosity (cP)                   1.836e-002        1.882e-002        6.949e-002                                             "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    30.22             30.22             165.8                                                  "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   1.755             1.755             9.174                                                  "]
[null,null,"Cv (kJ/kgmole-C)                 29.20             29.20             165.8                                                  "]
[null,null,"Mass Cv (kJ/kg-C)                1.696             1.696             9.174                                                  "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   29.23             29.23             ---                                                    "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  1.698             1.698             ---                                                    "]
[null,null,"Cp/Cv (Ent. Method)              1.319             1.319             ---                                                    "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---               ---                                                    "]
[null,null,"True VP at 37.8 C (kPa)          ---               ---               ---                                                    "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 2.221             2.221             0.0000                                                "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---               ---                                                    "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 1.0000    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               7.6775           0.1000           123.1694         0.0932           0.4114           0.1963           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              15.3550          0.2000           30.9557          0.0234           0.4431           0.2115           "]
[null,null,"H2O                   46.0650          0.6000           829.8656         0.6278           0.8315           0.3968           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   7.6775           0.1000           337.8845         0.2556           0.4094           0.1954           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 76.7750          1.0000           1321.8751        1.0000           2.0954           1.0000           "]
[null,null,"Vapour Phase                                                                                      Phase Fraction 1.000      "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               7.6775           0.1000           123.1694         0.0932           0.4114           0.1963           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              15.3550          0.2000           30.9557          0.0234           0.4431           0.2115           "]
[null,null,"H2O                   46.0650          0.6000           829.8656         0.6278           0.8315           0.3968           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   7.6775           0.1000           337.8845         0.2556           0.4094           0.1954           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 76.7750          1.0000           1321.8751        1.0000           2.0954           1.0000           "]
[null,null,"Aqueous Phase                                                                                     Phase Fraction 0.0000     "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0010           0.0000           0.0009           0.0000           0.0029           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.0044           0.0000           0.0005           0.0000           0.0069           "]
[null,null,"H2O                   0.0000           0.9897           0.0000           0.9866           0.0000           0.9758           "]
[null,null,"CO                    0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"CO2                   0.0000           0.0049           0.0000           0.0120           0.0000           0.0143           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 0.0000           1.0000           0.0000           1.0000           0.0000           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"SMR-Liquid (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: SMR-Liquid                                                          Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase      Liquid Phase      Aqueous Phase                        "]
[null,null,"Vapour / Phase Fraction          0.0000            0.0000            0.5000            0.5000                               "]
[null,null,"Temperature: (C)                 846.0             846.0             846.0             846.0                                "]
[null,null,"Pressure: (kPa)                  2144              2144              2144              2144                                 "]
[null,null,"Molar Flow (kgmole/h)            0.0000            0.0000            0.0000            0.0000                               "]
[null,null,"Mass Flow (kg/h)                 0.0000            0.0000            0.0000            0.0000                               "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    0.0000            0.0000            0.0000            0.0000                               "]
[null,null,"Molar Enthalpy (kJ/kgmole)       -1.180e+005       -1.180e+005       -1.180e+005       -1.180e+005                          "]
[null,null,"Molar Entropy (kJ/kgmole-C)      168.4             168.4             168.4             168.4                                "]
[null,null,"Heat Flow (kJ/h)                 0.0000            0.0000            0.0000            0.0000                               "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    0.0000            0.0000            0.0000            0.0000                               "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase      Liquid Phase      Aqueous Phase                        "]
[null,null,"Molecular Weight                 14.61             14.61             14.61             14.61                                "]
[null,null,"Molar Density (kgmole/m3)        0.2299            0.2299            0.2299            0.2299                               "]
[null,null,"Mass Density (kg/m3)             3.359             3.359             3.359             3.359                                "]
[null,null,"Act. Volume Flow (m3/h)          0.0000            0.0000            0.0000            0.0000                               "]
[null,null,"Mass Enthalpy (kJ/kg)            -8074             -8074             -8074             -8074                                "]
[null,null,"Mass Entropy (kJ/kg-C)           11.53             11.53             11.53             11.53                                "]
[null,null,"Heat Capacity (kJ/kgmole-C)      38.74             38.74             38.74             38.74                                "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     2.651             2.651             2.651             2.651                                "]
[null,null,"Lower Heating Value (kJ/kgmole)  ---               ---               ---               ---                                  "]
[null,null,"Mass Lower Heating Value (kJ/kg) ---               ---               ---               ---                                  "]
[null,null,"Phase Fraction [Vol. Basis]      ---               ---               0.5000            0.5000                               "]
[null,null,"Phase Fraction [Mass Basis]      2.122e-314        0.0000            0.5000            0.5000                               "]
[null,null,"Partial Pressure of CO2 (kPa)    0.0000            ---               ---               ---                                  "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000            0.0000            0.0000                               "]
[null,null,"Act. Gas Flow (ACT_m3/h)         ---               ---               ---               ---                                  "]
[null,null,"Avg. Liq. Density (kgmole/m3)    ---               ---               ---               ---                                  "]
[null,null,"Specific Heat (kJ/kgmole-C)      38.74             38.74             38.74             38.74                                "]
[null,null,"Std. Gas Flow (STD_m3/h)         0.0000            0.0000            0.0000            0.0000                               "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 545.1             545.1             545.1             545.1                               "]
[null,null,"Act. Liq. Flow (m3/s)            0.0000            ---               0.0000            0.0000                               "]
[null,null,"Z Factor                         ---               1.002             1.002             1.002                                "]
[null,null,"Watson K                         12.88             12.88             12.88             12.88                                "]
[null,null,"User Property                    ---               ---               ---               ---                                  "]
[null,null,"Cp/(Cp - R)                      1.273             1.273             1.273             1.273                                "]
[null,null,"Cp/Cv                            1.277             1.277             1.277             1.277                                "]
[null,null,"Heat of Vap. (kJ/kgmole)         4.291e+004        ---               ---               ---                                  "]
[null,null,"Kinematic Viscosity (cSt)        5.227             9.390             0.8236            0.8236                               "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) ---               ---               ---               ---                                 "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) 0.0000            0.0000            0.0000            0.0000                              "]
[null,null,"Liquid Fraction                  1.000             0.0000            1.000             1.000                                "]
[null,null,"Molar Volume (m3/kgmole)         4.350             4.350             4.350             4.350                                "]
[null,null,"Mass Heat of Vap. (kJ/kg)        2937              ---               ---               ---                                  "]
[null,null,"Phase Fraction [Molar Basis]     0.0000            0.0000            0.5000            0.5000                               "]
[null,null,"Surface Tension (dyne/cm)        ---               ---               0.0000            0.0000                               "]
[null,null,"Thermal Conductivity (W/m-K)     0.1565            0.1721            0.1049            0.1049                               "]
[null,null,"Viscosity (cP)                   1.756e-002        3.154e-002        2.766e-003        2.766e-003                           "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    30.42             30.42             30.42             30.42                                "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   2.082             2.082             2.082             2.082                                "]
[null,null,"Cv (kJ/kgmole-C)                 30.32             30.32             30.32             30.32                                "]
[null,null,"Mass Cv (kJ/kg-C)                2.075             2.075             2.075             2.075                                "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   ---               30.31             -1.286e+004       -32.70                               "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  ---               2.075             -879.8            -2.238                               "]
[null,null,"Cp/Cv (Ent. Method)              ---               1.278             -3.013e-003       -1.185                               "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---               ---               ---                                  "]
[null,null,"True VP at 37.8 C (kPa)          ---               ---               ---               ---                                  "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 0.0000            0.0000            0.0000            0.0000                              "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---               ---               ---                                  "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 0.0000    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0092           0.0000           0.0101           0.0000           0.0183           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.3921           0.0000           0.0541           0.0000           0.4221           "]
[null,null,"H2O                   0.0000           0.4382           0.0000           0.5403           0.0000           0.2951           "]
[null,null,"CO                    0.0000           0.0804           0.0000           0.1542           0.0000           0.1051           "]
[null,null,"CO2                   0.0000           0.0801           0.0000           0.2413           0.0000           0.1594           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 0.0000           1.0000           0.0000           1.0000           0.0000           1.0000           "]
[null,null,"Vapour Phase                                                                                      Phase Fraction 0.0000     "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0092           0.0000           0.0101           0.0000           0.0183           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.3921           0.0000           0.0541           0.0000           0.4221           "]
[null,null,"H2O                   0.0000           0.4382           0.0000           0.5403           0.0000           0.2951           "]
[null,null,"CO                    0.0000           0.0804           0.0000           0.1542           0.0000           0.1051           "]
[null,null,"CO2                   0.0000           0.0801           0.0000           0.2413           0.0000           0.1594           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 0.0000           1.0000           0.0000           1.0000           0.0000           1.0000           "]
[null,null,"Liquid Phase                                                                                      Phase Fraction 0.5000     "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0092           0.0000           0.0101           0.0000           0.0183           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.3921           0.0000           0.0541           0.0000           0.4221           "]
[null,null,"H2O                   0.0000           0.4382           0.0000           0.5403           0.0000           0.2951           "]
[null,null,"CO                    0.0000           0.0804           0.0000           0.1542           0.0000           0.1051           "]
[null,null,"CO2                   0.0000           0.0801           0.0000           0.2413           0.0000           0.1594           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 0.0000           1.0000           0.0000           1.0000           0.0000           1.0000           "]
[null,null,"Aqueous Phase                                                                                     Phase Fraction 0.5000     "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0092           0.0000           0.0101           0.0000           0.0183           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.3921           0.0000           0.0541           0.0000           0.4221           "]
[null,null,"H2O                   0.0000           0.4382           0.0000           0.5403           0.0000           0.2951           "]
[null,null,"CO                    0.0000           0.0804           0.0000           0.1542           0.0000           0.1051           "]
[null,null,"CO2                   0.0000           0.0801           0.0000           0.2413           0.0000           0.1594           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 0.0000           1.0000           0.0000           1.0000           0.0000           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"WGS-Liquid (Material Stream): Conditions, Properties, Composition"]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Material Stream: WGS-Liquid                                                          Fluid Package: Basis-1                 "]
[null,null,"                                                                                                                            "]
[null,null,"                                                                                     Property Package: Peng Robinson        "]
[null,null,"CONDITIONS                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase      Liquid Phase      Aqueous Phase                        "]
[null,null,"Vapour / Phase Fraction          0.0000            0.0000            0.5000            0.5000                               "]
[null,null,"Temperature: (C)                 400.4             400.4             400.4             400.4                                "]
[null,null,"Pressure: (kPa)                  2142              2142              2142              2142                                 "]
[null,null,"Molar Flow (kgmole/h)            0.0000            0.0000            0.0000            0.0000                               "]
[null,null,"Mass Flow (kg/h)                 0.0000            0.0000            0.0000            0.0000                               "]
[null,null,"Std Ideal Liq Vol Flow (m3/h)    0.0000            0.0000            0.0000            0.0000                               "]
[null,null,"Molar Enthalpy (kJ/kgmole)       -1.370e+005       -1.370e+005       -1.370e+005       -1.370e+005                          "]
[null,null,"Molar Entropy (kJ/kgmole-C)      144.9             144.9             144.9             144.9                                "]
[null,null,"Heat Flow (kJ/h)                 0.0000            0.0000            0.0000            0.0000                               "]
[null,null,"Liq Vol Flow @Std Cond (m3/h)    0.0000            0.0000            0.0000            0.0000                               "]
[null,null,"PROPERTIES                                                                                                                  "]
[null,null,"                                                                                                                            "]
[null,null,"                                 Overall           Vapour Phase      Liquid Phase      Aqueous Phase                        "]
[null,null,"Molecular Weight                 14.61             14.61             14.61             14.61                                "]
[null,null,"Molar Density (kgmole/m3)        0.3836            0.3836            0.3836            0.3836                               "]
[null,null,"Mass Density (kg/m3)             5.604             5.604             5.604             5.604                                "]
[null,null,"Act. Volume Flow (m3/h)          0.0000            0.0000            0.0000            0.0000                               "]
[null,null,"Mass Enthalpy (kJ/kg)            -9374             -9374             -9374             -9374                                "]
[null,null,"Mass Entropy (kJ/kg-C)           9.918             9.918             9.918             9.918                                "]
[null,null,"Heat Capacity (kJ/kgmole-C)      35.84             35.84             35.84             35.84                                "]
[null,null,"Mass Heat Capacity (kJ/kg-C)     2.453             2.453             2.453             2.453                                "]
[null,null,"Lower Heating Value (kJ/kgmole)  ---               ---               ---               ---                                  "]
[null,null,"Mass Lower Heating Value (kJ/kg) ---               ---               ---               ---                                  "]
[null,null,"Phase Fraction [Vol. Basis]      ---               ---               0.5000            0.5000                               "]
[null,null,"Phase Fraction [Mass Basis]      2.122e-314        0.0000            0.5000            0.5000                               "]
[null,null,"Partial Pressure of CO2 (kPa)    0.0000            ---               ---               ---                                  "]
[null,null,"Cost Based on Flow (Cost/s)      0.0000            0.0000            0.0000            0.0000                               "]
[null,null,"Act. Gas Flow (ACT_m3/h)         ---               ---               ---               ---                                  "]
[null,null,"Avg. Liq. Density (kgmole/m3)    ---               ---               ---               ---                                  "]
[null,null,"Specific Heat (kJ/kgmole-C)      35.84             35.84             35.84             35.84                                "]
[null,null,"Std. Gas Flow (STD_m3/h)         0.0000            0.0000            0.0000            0.0000                               "]
[null,null,"Std. Ideal Liq. Mass Density (kg/m3) 509.3             509.3             509.3             509.3                               "]
[null,null,"Act. Liq. Flow (m3/s)            0.0000            ---               0.0000            0.0000                               "]
[null,null,"Z Factor                         ---               0.9970            0.9970            0.9970                               "]
[null,null,"Watson K                         13.34             13.34             13.34             13.34                                "]
[null,null,"User Property                    ---               ---               ---               ---                                  "]
[null,null,"Cp/(Cp - R)                      1.302             1.302             1.302             1.302                                "]
[null,null,"Cp/Cv                            1.319             1.319             1.319             1.319                                "]
[null,null,"Heat of Vap. (kJ/kgmole)         4.085e+004        ---               ---               ---                                  "]
[null,null,"Kinematic Viscosity (cSt)        2.924             3.856             0.4643            0.4643                               "]
[null,null,"Liq. Mass Density (Std. Cond) (kg/m3) ---               ---               ---               ---                                 "]
[null,null,"Liq. Vol. Flow (Std. Cond) (m3/h) 0.0000            0.0000            0.0000            0.0000                              "]
[null,null,"Liquid Fraction                  1.000             0.0000            1.000             1.000                                "]
[null,null,"Molar Volume (m3/kgmole)         2.607             2.607             2.607             2.607                                "]
[null,null,"Mass Heat of Vap. (kJ/kg)        2796              ---               ---               ---                                  "]
[null,null,"Phase Fraction [Molar Basis]     0.0000            0.0000            0.5000            0.5000                               "]
[null,null,"Surface Tension (dyne/cm)        ---               ---               0.0000            0.0000                               "]
[null,null,"Thermal Conductivity (W/m-K)     0.1420            0.1248            8.988e-002        8.988e-002                           "]
[null,null,"Viscosity (cP)                   1.639e-002        2.161e-002        2.602e-003        2.602e-003                           "]
[null,null,"Cv (Semi-Ideal) (kJ/kgmole-C)    27.53             27.53             27.53             27.53                                "]
[null,null,"Mass Cv (Semi-Ideal) (kJ/kg-C)   1.884             1.884             1.884             1.884                                "]
[null,null,"Cv (kJ/kgmole-C)                 27.17             27.17             27.17             27.17                                "]
[null,null,"Mass Cv (kJ/kg-C)                1.860             1.860             1.860             1.860                                "]
[null,null,"Cv (Ent. Method) (kJ/kgmole-C)   ---               27.17             35.63             174.1                                "]
[null,null,"Mass Cv (Ent. Method) (kJ/kg-C)  ---               1.860             2.439             11.92                                "]
[null,null,"Cp/Cv (Ent. Method)              ---               1.319             1.006             0.2059                               "]
[null,null,"Reid VP at 37.8 C (kPa)          ---               ---               ---               ---                                  "]
[null,null,"True VP at 37.8 C (kPa)          ---               ---               ---               ---                                  "]
[null,null,"Liq. Vol. Flow - Sum(Std. Cond) (m3/h) 0.0000            0.0000            0.0000            0.0000                              "]
[null,null,"Partial Pressure of H2S (kPa)    0.0000            ---               ---               ---                                  "]
[null,null,"COMPOSITION                                                                                                                 "]
[null,null,"                                                                                                                            "]
[null,null,"Overall Phase                                                                                     Vapour Fraction 0.0000    "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0092           0.0000           0.0101           0.0000           0.0171           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.4568           0.0000           0.0630           0.0000           0.4595           "]
[null,null,"H2O                   0.0000           0.3734           0.0000           0.4604           0.0000           0.2350           "]
[null,null,"CO                    0.0000           0.0157           0.0000           0.0300           0.0000           0.0191           "]
[null,null,"CO2                   0.0000           0.1449           0.0000           0.4364           0.0000           0.2693           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 0.0000           1.0000           0.0000           1.0000           0.0000           1.0000           "]
[null,null,"Vapour Phase                                                                                      Phase Fraction 0.0000     "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0092           0.0000           0.0101           0.0000           0.0171           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.4568           0.0000           0.0630           0.0000           0.4595           "]
[null,null,"H2O                   0.0000           0.3734           0.0000           0.4604           0.0000           0.2350           "]
[null,null,"CO                    0.0000           0.0157           0.0000           0.0300           0.0000           0.0191           "]
[null,null,"CO2                   0.0000           0.1449           0.0000           0.4364           0.0000           0.2693           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 0.0000           1.0000           0.0000           1.0000           0.0000           1.0000           "]
[null,null,"Liquid Phase                                                                                      Phase Fraction 0.5000     "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0092           0.0000           0.0101           0.0000           0.0171           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.4568           0.0000           0.0630           0.0000           0.4595           "]
[null,null,"H2O                   0.0000           0.3734           0.0000           0.4604           0.0000           0.2350           "]
[null,null,"CO                    0.0000           0.0157           0.0000           0.0300           0.0000           0.0191           "]
[null,null,"CO2                   0.0000           0.1449           0.0000           0.4364           0.0000           0.2693           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 0.0000           1.0000           0.0000           1.0000           0.0000           1.0000           "]
[null,null,"Aqueous Phase                                                                                     Phase Fraction 0.5000     "]
[null,null,"                                                                                                                            "]
[null,null,"COMPONENTS            MOLAR FLOW       MOLE FRACTION    MASS FLOW        MASS FRACTION    LIQUID VOLUME    LIQUID VOLUME    "]
[null,null,"                       (kgmole/h)                        (kg/h)                           FLOW   (m3/h)    FRACTION         "]
[null,null,"Methane               0.0000           0.0092           0.0000           0.0101           0.0000           0.0171           "]
[null,null,"Oxygen                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Nitrogen              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Hydrogen              0.0000           0.4568           0.0000           0.0630           0.0000           0.4595           "]
[null,null,"H2O                   0.0000           0.3734           0.0000           0.4604           0.0000           0.2350           "]
[null,null,"CO                    0.0000           0.0157           0.0000           0.0300           0.0000           0.0191           "]
[null,null,"CO2                   0.0000           0.1449           0.0000           0.4364           0.0000           0.2693           "]
[null,null,"Carbon                0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Ethanol               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Methanol              0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Benzene               0.0000           0.0000           0.0000           0.0000           0.0000           0.0000           "]
[null,null,"Total                 0.0000           1.0000           0.0000           1.0000           0.0000           1.0000           "]
[]
[]
[null,null,"-------------------------------------------------------------------------------"]
[null,null,"Hyprotech Ltd.                     Aspen HYSYS Version 2006 (20.0.0.6728)                                                  "]

{"sheet":"Input_Sheet_Template","index":3,"n_rows":161,"n_cols":8,"rows_kept":161,"cut":false,"hidden":false,"merged":[[155,6,160,6],[130,2,130,3],[143,4,143,6],[99,3,100,3],[87,4,87,6],[140,4,142,6],[151,4,151,6],[144,4,144,6],[145,4,145,6],[91,5,91,6],[92,5,92,6],[102,5,102,6],[147,5,150,6],[1,1,1,6],[2,1,2,3],[3,3,3,4],[53,4,53,6],[49,4,49,6],[46,4,46,6],[31,3,32,3],[44,4,44,6],[35,4,35,6],[42,4,42,6],[41,4,41,6],[40,4,40,6],[48,4,48,6],[45,4,45,6],[23,4,23,6],[24,4,24,6],[25,4,25,6],[27,4,27,6],[34,4,34,6],[28,4,28,6],[43,4,43,6],[36,4,36,6],[29,4,29,6],[30,4,30,6],[33,4,33,6],[32,4,32,6],[39,4,39,6],[37,4,37,6],[38,4,38,6],[47,4,47,6],[86,4,86,6],[58,5,67,5],[55,4,55,6],[88,4,88,6],[52,4,52,6],[51,4,51,6],[50,4,50,6],[54,4,54,6],[84,4,84,6],[85,4,85,6]]}
[]
[null,"H2A Hydrogen Production Cash Flow Analysis Tool v3.2018"]
["title","Distributed Hydrogen Production from Ethanol - Current Timeframe"]
[]
[null,"Table of Contents"]
[null,"View and edit project information"]
[]
[null,"H2A cell color coding"]
[]
[null,"Use H2A default values"]
[]
[]
[]
[null,"Technical Operating Parameters and Specifications"]
[null,"Financial Input Values"]
[null,"Energy Feedstocks, Utilities and Byproducts",null,null,null,null,null,"Cash Flow NPV (Error if not 0)"]
[null,"Capital Cost",null,null,null,null,null,{"$f":"+NPV","v":8.7071894903132806E-9}]
[null,"Fixed Operating Costs"]
[null,"Variable Operating Costs - Other Materials and Byproducts"]
[null,"Variable Operating Costs - Other Variable Operating Costs"]
[]
[]
[]
[null,"Technical Operating Parameters and Specifications",null,null,"Notes"]
["cap_factor","Operating Capacity Factor (%)",{"$f":"0.86*sensitivity_01","v":0.86}]
["design_cap","Plant Design Capacity (kg of H2/day)",{"$f":"1500*sensitivity_02","v":1500}]
[null,"Plant Output (kg/day)",{"$f":"design_cap*cap_factor","v":1290}]
["Soutput_kgyear","Plant Output (kg/year)",{"$f":"output_kgpday*365","v":470850}]
[null,"Financial Input Values",null,null,"Notes "]
["ref_year","Reference year",2016]
["startup_year","Assumed start-up year",2015]
[null,"Basis year",2005,"Costs must be entered in basis year dollars"]
["construct","Length of Construction Period (years)",1]
["percent_cap1","% of Capital Spent in 1st Year of Construction",1]
["percent_cap2","% of Capital Spent in 2nd Year of Construction",0]
["percent_cap3","% of Capital Spent in 3rd Year of Construction",0]
["percent_cap4","% of Capital Spent in 4th Year of Construction"]
["start_time","Start-up Time (years)",0.57999999999999996]
["plant_life","Plant life (years)",20]
["anal_period","Analysis period (years)",20]
["depr_length","Depreciation Schedule Length (years)",7]
["depr_type","Depreciation Type","MACRS"]
["equity"," % Equity Financing",0.4]
["debt_interest","Interest rate on debt, if applicable (%)",3.6999999999999998E-2]
["debt_period","Debt period (years)",0,null,"Enter 0 to enable constant outstanding debt."]
["percnt_fixed","% of Fixed Operating Costs During Start-up (%)",0.75]
["percnt_revs","% of Revenues During Start-up (%)",0.5]
["percnt_var","% of Variable Operating Costs During Start-up (%)",0.5]
["decom_percent","Decommissioning costs (% of depreciable capital investment)",0.1]
["salvage_perct","Salvage value (% of total capital investment)",0.1]
["inflation_rate","Inflation rate (%)",1.9E-2]
["real_irr","After-tax Real IRR (%)",{"$f":"0.08*sensitivity_03","v":0.08}]
["state_tax_rate","State Taxes (%)",0.06]
["fed_tax_rate","Federal Taxes (%)",0.21]
["Stotal_tax_rate","Total Tax Rate (%)",{"$f":"fed_tax_rate+state_tax_rate*(1-fed_tax_rate)","v":0.25739999999999996}]
["WorkingCap","WORKING CAPITAL (% of yearly change in operating costs)",0.15]
[null,"Energy Feedstocks, Utilities, and Byproducts"]
[null,"Select the Price Table to Use"]
[null,"AEO_2017_Reference_Case",null,null,null,"To use a new feedstock, utility or byproduct, select the price table and product from the dropdown lists and enter the usage (or byproduct) amount. Click the \"Add\" button to add the product to the \"In Use\" list. Important; only materials on the \"In Use\" list will be used in H2A calculations. To delete materials from the list, click the \"Delete\" button below"]
[null,"Select the Use"]
[null,"feedstock",{"$f":"IF(OR(TMP_FeedType=\"Feedstock\",TMP_FeedType = \"Utility\"),\" Enter usage in\",\"Enter production in\")","v":" Enter usage in"},{"$f":"VLOOKUP(TMP_FeedName,INDIRECT(TMP_PriceTable),4,FALSE)","v":"kWh"}]
[null,"Select the Feed Type"]
[null,"Commercial Electricity"]
[]
[null,{"$f":"SELECTED_FEED","v":"feedstock"},{"$f":"TMP_FeedName","v":"Commercial Electricity"}]
[null,{"$f":"\"Price Conversion Factor (GJ/\"&TMP_Units&\")\"","v":"Price Conversion Factor (GJ/kWh)"},{"$f":"VLOOKUP(TMP_FeedName,MASTER_PROPERTY_TABLE,9,FALSE)","v":3.5999999999999995E-3}]
[null,{"$f":"\"Price in Startup Year ($\" & ref_year & \")/\" & TMP_Units","v":"Price in Startup Year ($2016)/kWh"},{"$f":"HLOOKUP(startup_year,INDIRECT(TMP_PriceTable),MATCH(TMP_FeedName,INDIRECT(Energy_Feed_List),0),FALSE)*TMP_Conversion","v":0.10775596291985907}]
[null,{"$f":"IF(OR(TMP_FeedType=\"Feedstock\",TMP_FeedType = \"Utility\"),\"Usage (\"&TMP_Units&\"/kg H2)\",\"Production (\"&TMP_Units&\"/kg H2)\")","v":"Usage (kWh/kg H2)"},0.49]
[null,{"$f":"IF(OR(TMP_FeedType = \"Feedstock\",TMP_FeedType = \"Utility\"), \"Cost in Startup Year\",\"Income in Startup Year\")","v":"Cost in Startup Year"},{"$f":"design_cap*365*cap_factor*TMP_Usage*TMP_StartPrice","v":24861.078618999665}]
[null,"Lookup Prices","yes"]
[]
[null,"Energy feedstocks, utilities, and byproducts currently in use "]
["START_TOP"]
[null,"feedstock","Price Conversion Factor (GJ/gallons)","Price in Startup Year ($2016)/gallons","Usage (gallons/kg H2)","Cost in Startup Year","Lookup Prices"]
[null,"Ethanol",8.1000000000000003E-2,2.2678388613174403,2.1909999999999998,{"$f":"output_kgyear*feedstockEthanol_Price*feedstockEthanol_Usage","v":2339575.9339222349},"yes"]
[null,"feedstock","Price Conversion Factor (GJ/kWh)","Price in Startup Year ($2016)/kWh","Usage (kWh/kg H2)","Cost in Startup Year","Lookup Prices"]
[null,"Commercial Electricity",3.5999999999999995E-3,0.10775596291985907,{"$f":"0.49*sensitivity_04","v":0.49},{"$f":"+output_kgyear*feedstockCommercial_Electricity_Price*feedstockCommercial_Electricity_Usage","v":24861.078618999665},"yes"]
["START_TOP"]
["START_UTILITY"]
["START_BYPROD"]
[null,null,null,null,null,"Total"]
["Total_Energy_Feed_Cost","Total Energy Feedstock Cost ($/year)",null,null,null,{"$f":"SUM(Dynamic_Feed_Total)","v":2364437.0125412345}]
["Total_Energy_Utilities_Cost","Total Energy Utilities Cost ($/year)",null,null,null,{"$f":"SUM(Dynamic_Utilities_Total)","v":0}]
["Total_Energy_Byproduct_Credit","Total Energy Byproduct Credit ($/year)",null,null,null,{"$f":"SUM(Dynamic_Byproduct_Total)","v":0}]
[null,null,null,"Notes:"]
[]
[null,"Capital Costs",null,null,"Notes"]
["direct_cap","H2A Total Direct Capital Cost",{"$f":"Det_scaled_cap","v":1560922.5551038363},null,"Click to enter details on the Cost Detail Sheet"]
[null,"H2A Carbon Sequestration Total Direct Capital Cost",{"$f":"Det_CO2_seq","v":0},null,"Click to enter details on the Carbon Sequestration calculation sheet."]
[]
[null,"Indirect Depreciable Capital Costs",{"$f":"\"Enter values in basis year (\" & BasisYear & \") dollars\"","v":"Enter values in basis year (2005) dollars"},"Combined Plant Scaling and Escalation Factor",{"$f":" \"Reference Year (\"& ref_year & \") Dollars\"","v":"Reference Year (2016) Dollars"}]
["Site_prep","Site Preparation ($) (may change to construction costs)",{"$f":"0.1885*direct_cap/(CPIinflator*CEPCIinflator)","v":227460.22276855324},{"$f":"CEPCIinflator*CPIinflator","v":1.2935620041859532},{"$f":"C92*D92","v":294233.90163707314},"Includes buildings and other site improvements"]
["Engin","Engineering & design ($)",{"$f":"50000","v":50000},1.2935620041859532,{"$f":"C93*D93","v":64678.100209297663}]
["Process_cont","Process contingency ($)",0,1.2935620041859532,0]
["Project_cont","Project contingency ($)",{"$f":"0.15*(direct_cap)/(CEPCIinflator*CPIinflator)","v":181002.82978929969},1.2935620041859532,234138.38326557548]
["Other_indirect","Other (Depreciable) capital ($)",0,1.2935620041859532,0]
["Fees","One-time Licensing Fees ($)",null,1.2935620041859532,0]
["Permitting","Up-Front Permitting Costs ($) (legal and contractors fees included here)",30000,1.2935620041859532,38806.860125578598]
["Sdepr_cap","Total Depreciable Capital Costs",null,null,{"$f":"direct_cap+CO2_seq+SUM($E$92:$E$98)","v":2192779.8003413612}]
[null,null,null,"Combined Plant Scaling and Escalation Factor"]
[null,"Non-Depreciable Capital Costs",{"$f":"\"Enter values in basis year (\" & BasisYear & \") dollars\"","v":"Enter values in basis year (2005) dollars"},null,{"$f":" \"Reference Year (\"& ref_year & \") Dollars\"","v":"Reference Year (2016) Dollars"}]
["acre_cost","Cost of land ($/acre)",0,{"$f":"CPIinflator","v":1.0995746738559611},{"$f":"C102*D102","v":0}]
["acres","Land required (acres)",0,{"$f":"Scale_Factor *1","v":1},{"$f":"C103*D103","v":0},"Estimated based on site total cost in NETL report."]
["Sland_cost","Land Cost ($)",null,null,{"$f":"acre_cost*acres","v":0}]
[null,"Other non depreciable capital costs",null,{"$f":"CPIinflator","v":1.0995746738559611},{"$f":"C105*D105","v":0}]
["Snon_dep_cap","Total Non-Depreciable Capital Costs",null,null,{"$f":"land_cost+$E$105","v":0}]
[]
["Stotal_cap","Total Capital Costs",{"$f":"(depr_cap+non_dep_cap)*sensitivity_06","v":2192779.8003413612}]
[]
[null,"Fixed Operating Costs",{"$f":"\"Enter values in basis year (\" & BasisYear & \") dollars\"","v":"Enter values in basis year (2005) dollars"},"Combined Plant Scaling and Escalation Factor",{"$f":" \"Reference Year (\"& ref_year & \") Dollars\"","v":"Reference Year (2016) Dollars"}]
["FTEs","Total plant staff (number of FTEs employed by plant)",0,{"$f":"Scale_Ratio^0.25","v":1},{"$f":"C111*D111","v":0}]
["FTE_cost","Burdened labor cost, including overhead ($/man-hr)",50,{"$f":"VLOOKUP(ref_year,Tbl_labor_indexes,2,FALSE)/VLOOKUP(BasisYear,Tbl_labor_indexes,2,FALSE)","v":1.1548042704626329},{"$f":"C112*D112","v":57.740213523131644},"Using H2A default"]
["Slabor_cost","Labor cost, $/year",null,null,{"$f":"FTEs*2080*FTE_cost","v":0}]
["overhead_rate","G&A rate (% of labor cost)",0.2,null,null,"Using H2A default"]
["Soverhead_GA","G&A ($/year)",null,null,{"$f":"labor_cost*overhead_rate","v":0}]
["licensing","Licensing, Permits and Fees ($/year)",0,{"$f":"Scale_Factor *CEPCIinflator*CPIinflator","v":1.2935620041859532},{"$f":"C116*D116","v":0}]
["tax_ins_rate","Property tax and insurance rate (% of total capital investment per year)",0.02]
["Stax_insurance","Property taxes and insurance ($/year)",null,null,{"$f":"tax_ins_rate*total_cap","v":43855.596006827225}]
["rent","Rent ($/year)",3370,{"$f":"Scale_Factor *CPIinflator","v":1.0995746738559611},{"$f":"C119*D119","v":3705.5666508945887}]
["material","Material costs for maintenance and repairs ($/year)",0,{"$f":"Scale_Factor *CEPCIinflator*CPIinflator","v":1.2935620041859532},{"$f":"C120*D120","v":0}]
["prod_maint","Production Maintenance and Repairs ($/year)",{"$f":"0.05*direct_cap/(CPIinflator*CEPCIinflator)","v":60334.276596433228},{"$f":"Scale_Factor *CEPCIinflator*CPIinflator","v":1.2935620041859532},{"$f":"C121*D121","v":78046.127755191817},"Maintenance labor"]
["other_fees","Other Fees ($/year)",null,{"$f":"Scale_Ratio * CEPCIinflator*CPIinflator","v":1.2935620041859532},{"$f":"C122*D122","v":0},"Administrative & support labor"]
["other_fixed","Other Fixed O&M Costs ($/year)",null,{"$f":"Scale_Factor *CEPCIinflator*CPIinflator","v":1.2935620041859532},{"$f":"C123*D123","v":0}]
["Sfixed","Total Fixed Operating Costs",null,null,{"$f":"(labor_cost+overhead_GA+tax_insurance+licensing+SUM(E119:E123))*sensitivity_07","v":125607.29041291363}]
[]
[null,"Variable Operating Costs"]
[null,"Other Materials and Byproducts"]
[]
[null,"Select the Material"]
[null,"Process Water"]
[null,"Feed or utility",{"$f":"B130","v":"Process Water"}]
[null,{"$f":"\"$(\" & ref_year & \")/ \" & VLOOKUP(TMP_NonE_Feed,Tbl_Other_Inputs_and_Byproducts,2,FALSE)","v":"$(2016)/ gal"},{"$f":"HLOOKUP(startup_year,Tbl_Other_Inputs_and_Byproducts,MATCH(TMP_NonE_Feed,Other_Inputs_List,0),FALSE)","v":2.374951094500801E-3}]
[null,{"$f":"IF(TMP_NonE_Type=\"Feed or utility\",\"Usage per kg H2\",\"Production per kg H2\")","v":"Usage per kg H2"}]
[null,{"$f":"IF(TMP_NonE_Type = \"Feed or utility\", \"Cost in Startup Year\",\"Income in Startup Year\")","v":"Cost in Startup Year"},{"$f":"design_cap*365*cap_factor*TMP_NonE_Usage*TMP_NonE_StartPrice","v":0}]
[null,"Lookup Prices","Yes"]
["START_NONE_TOP"]
[null,"Feed or utility","$(2016)/ gal","Usage per kg H2","Cost in Startup Year","Lookup Prices"]
[null,"Process Water",2.374951094500801E-3,5.77,{"$f":"+D138*output_kgyear*C138","v":6452.2778208197014},"Yes"]
["START_NONE_FEED"]
["START_NONE_BYPROD"]
[null,"Total Non Energy Utility and Material Costs ($/year)",{"$f":"SUM(Dynamic_NonE_Feed_Total)","v":6452.2778208197014}]
["total_non_energy_byproduct_credit","Total Non Energy Byproduct Credits ($/year)",{"$f":"SUM(Dynamic_NonE_Byprod_Total)","v":0}]
[]
["Stotal_feedstock","Total Feedstock Costs ($/year)",{"$f":"Total_Energy_Feed_Cost","v":2364437.0125412345}]
["Stotal_utilities","Total Utility Costs ($/year)",{"$f":"Total_Energy_Utilities_Cost+Total_Non_Energy_Feed_Cost","v":6452.2778208197014}]
["Stotal_byproducts","Total Byproduct Credits ($/year)",{"$f":"Total_Energy_Byproduct_Credit+total_non_energy_byproduct_credit","v":0}]
[null,"Other Variable operating costs (for the first year)",{"$f":"\"Enter values in basis year (\" & BasisYear & \") dollars\"","v":"Enter values in basis year (2005) dollars"},"Combined Plant Scaling and Escalation Factor",{"$f":" \"Reference Year (\"& ref_year & \") Dollars\"","v":"Reference Year (2016) Dollars"}]
["var_misc","Other variable operating costs (e.g. environmental surcharges) ($/year)",1800,{"$f":"Scale_Ratio * VLOOKUP(ref_year,Chemical_price_indexes,2,FALSE)/VLOOKUP(BasisYear,Chemical_price_indexes,2,FALSE)","v":1.4260544580886279},{"$f":"C148*D148","v":2566.8980245595303},"This covers waste disposal costs, non-feedstock fuels, environmental surcharges, etc. and is estimated at $800/month with 50% being attributed to refueling operations (the other 50% goes to convenience store operations) and is further pro-rata for the fraction of hydrogen dispensers out of total dispensers (3 out of 8 for large stations). Thus for a large station, annual “Other Variable Costs” are $800/month * 12 months/year * 50% fueling fraction * (3 H2 dispensers/8 total dispensers) = $1,800/year."]
["total_other_raw","Other Material Costs ($/year)",null,{"$f":"Scale_Ratio * VLOOKUP(ref_year,Chemical_price_indexes,2,FALSE)/VLOOKUP(BasisYear,Chemical_price_indexes,2,FALSE)","v":1.4260544580886279},{"$f":"C149*D149","v":0}]
["waste_treat","Waste treatment costs ($/year)",null,{"$f":"Scale_Ratio * VLOOKUP(ref_year,Chemical_price_indexes,2,FALSE)/VLOOKUP(BasisYear,Chemical_price_indexes,2,FALSE)","v":1.4260544580886279},{"$f":"C150*D150","v":0}]
["solidwaste_treat","Solid waste disposal costs ($/year)",null,{"$f":"Scale_Ratio * VLOOKUP(ref_year,Chemical_price_indexes,2,FALSE)/VLOOKUP(BasisYear,Chemical_price_indexes,2,FALSE)","v":1.4260544580886279},{"$f":"C151*D151","v":0}]
["replace_factor","Total Unplanned Replacement Capital Cost Factor (% of total direct depreciable costs/year)",0,null,"Value added to match other central cases.\nUse this value for all central cases"]
["royalties","Royalties ($/year)",0,{"$f":"Scale_Ratio * CPIinflator","v":1.0995746738559611},0]
["operator_profit","Operator Profit ($/year) ",0,{"$f":"Scale_Ratio * CPIinflator","v":1.0995746738559611},0]
["tax_credit","Subsidies, Tax Incentives ($/year)",0,{"$f":"Scale_Ratio * CPIinflator","v":1.0995746738559611},0]
["CO2_seq","CO2 sequestration O&M costs and credits ($/year)",null,null,{"$f":"Det_CO2_OandMcost","v":0}]
[null,"Process Carbon Tax ($/metric ton carbon produced as CO2)",0,{"$f":"CPIinflator","v":1.0995746738559611},0]
[null,"Process Carbon Tax ($/year)",null,null,{"$f":"ROUND(Proc_CO2_tax*12/44*Proc_CO2_MTpY,-2)","v":0}]
[null,"Upstream Carbon Tax ($/metric ton upstream GHG CO2 eq)",0,{"$f":"CPIinflator","v":1.0995746738559611},0]
[null,"Upstream Carbon Tax ($/year)",null,null,{"$f":"ROUND(Upstream_CO2_tax/1000*Upstream_GHG_total*output_kgyear,2)","v":0}]
["Stotal_var","Total Variable Operating Costs ($/year)",null,null,{"$f":"ROUND(total_feedstock+total_utilities+total_other_raw-total_byproducts+var_misc+waste_treat+solidwaste_treat+royalties+operator_profit-tax_credit+CO2_OandMcost+Proc_CO2_taxpYear + Upstream_CO2_taxpYear,-2)","v":2373500}]

{"sheet":"Replacement Costs","index":4,"n_rows":57,"n_cols":12,"rows_kept":57,"cut":false,"hidden":false,"merged":[]}
[]
["Replacement Costs"]
[]
[]
[null,null,"Color Key"]
[]
[]
[]
[{"$f":"\"NOTE: Enter costs in year \"&TEXT(BasisYear,\"0\")&\" $ - Do not inflate\"","v":"NOTE: Enter costs in year 2005 $ - Do not inflate"}]
["NOTE: All replacement costs are assumed to be equity financed."]
[]
[]
["Unplanned Yearly Replacement Capital (Depreciable)"]
[null,null,"Comments",null,null,"Source","Information"]
["Total Unplanned Replacement Capital Cost Factor (% of total depreciable capital costs/year)",{"$f":"replace_factor","v":0},null,null,null,null,"Enter a fixed percentage.  This input is meant to include, in the Cash Flow Analysis, a factor for unplanned capital expenditures.  "]
["Actual Year","Analysis Year","Operations Year","Specified Yearly Replacement Costs","Carbon Sequestration Related Replacement Costs","Specified Yearly Replacement Costs","Unplanned Replacement Costs","Total Yearly Replacement Costs","Uninstalled costs","Installation factor","Comments:","Data source:"]
[null,null,null,{"$f":"\"Year \"&TEXT(BasisYear,\"0\")&\" $\"","v":"Year 2005 $"},{"$f":"\"Year \"&TEXT(ref_year,\"0\")&\" $\"","v":"Year 2016 $"},{"$f":"\"Year \"&TEXT(ref_year,\"0\")&\" $\"","v":"Year 2016 $"},{"$f":"\"Year \"&TEXT(ref_year,\"0\")&\" $\"","v":"Year 2016 $"},"Inflated to Start-up Year"]
[{"$f":"IF(C18<>\"\",'Cash Flow Analysis'!A65,\"\")","v":2014},{"$f":"construct+1","v":2},1,null,{"$f":"direct_cap*D18","v":0},{"$f":"(D18)*CPIinflator*CEPCIinflator+E18","v":0},{"$f":"IF(C18>anal_period,0,IF(replace_factor<>\"\",replace_factor*depr_cap,0))","v":0},{"$f":"(F18+G18)*((1+inflation_rate)^(startup_year-ref_year))","v":0},null,null,"Initial spares at 0.75% of Production System Direct Capital"]
[{"$f":"IF(C19<>\"\",'Cash Flow Analysis'!A66,\"\")","v":2015},{"$f":"IF(B18<anal_period+construct,B18+1,\"\")","v":3},{"$f":"IF(B19=\"\",\"\",C18+1)","v":2},null,0,0,{"$f":"IF(C19>anal_period,0,IF(replace_factor<>\"\",replace_factor*depr_cap,0))","v":0},{"$f":"(F19+G19)*((1+inflation_rate)^(startup_year-ref_year))","v":0}]
[{"$f":"IF(C20<>\"\",'Cash Flow Analysis'!A67,\"\")","v":2016},4,3,null,0,0,0,0]
[{"$f":"IF(C21<>\"\",'Cash Flow Analysis'!A68,\"\")","v":2017},5,4,null,0,0,0,0]
[{"$f":"IF(C22<>\"\",'Cash Flow Analysis'!A69,\"\")","v":2018},6,5,null,0,0,0,0]
[{"$f":"IF(C23<>\"\",'Cash Flow Analysis'!A70,\"\")","v":2019},7,6,0.15,234138.38326557545,234138.57729987608,0,229772.89234531514,null,null,"x15"]
[{"$f":"IF(C24<>\"\",'Cash Flow Analysis'!A71,\"\")","v":2020},8,7,null,0,0,0,0]
[{"$f":"IF(C25<>\"\",'Cash Flow Analysis'!A72,\"\")","v":2021},9,8,null,0,0,0,0]
[{"$f":"IF(C26<>\"\",'Cash Flow Analysis'!A73,\"\")","v":2022},10,9,null,0,0,0,0]
[{"$f":"IF(C27<>\"\",'Cash Flow Analysis'!A74,\"\")","v":2023},11,10,null,0,0,0,0]
[{"$f":"IF(C28<>\"\",'Cash Flow Analysis'!A75,\"\")","v":2024},12,11,0.5,780461.27755191817,780461.92433292023,0,765909.64115105034,null,null,"x50"]
[{"$f":"IF(C29<>\"\",'Cash Flow Analysis'!A76,\"\")","v":2025},13,12,null,0,0,0,0]
[{"$f":"IF(C30<>\"\",'Cash Flow Analysis'!A77,\"\")","v":2026},14,13,null,0,0,0,0]
[{"$f":"IF(C31<>\"\",'Cash Flow Analysis'!A78,\"\")","v":2027},15,14,null,0,0,0,0]
[{"$f":"IF(C32<>\"\",'Cash Flow Analysis'!A79,\"\")","v":2028},16,15,null,0,0,0,0]
[{"$f":"IF(C33<>\"\",'Cash Flow Analysis'!A80,\"\")","v":2029},17,16,0.15,234138.38326557545,234138.57729987608,0,229772.89234531514,null,null,"x15"]
[{"$f":"IF(C34<>\"\",'Cash Flow Analysis'!A81,\"\")","v":2030},18,17,null,0,0,0,0]
[{"$f":"IF(C35<>\"\",'Cash Flow Analysis'!A82,\"\")","v":2031},19,18,null,0,0,0,0]
[{"$f":"IF(C36<>\"\",'Cash Flow Analysis'!A83,\"\")","v":2032},20,19,null,0,0,0,0]
[{"$f":"IF(C37<>\"\",'Cash Flow Analysis'!A84,\"\")","v":2033},21,20,null,0,0,0,0]
[{"$f":"IF(C38<>\"\",'Cash Flow Analysis'!A85,\"\")","v":""},"","",null,0,0,0,0]
[{"$f":"IF(C39<>\"\",'Cash Flow Analysis'!A86,\"\")","v":""},"","",null,0,0,0,0]
[{"$f":"IF(C40<>\"\",'Cash Flow Analysis'!A87,\"\")","v":""},"","",null,0,0,0,0]
[{"$f":"IF(C41<>\"\",'Cash Flow Analysis'!A88,\"\")","v":""},"","",null,0,0,0,0]
[{"$f":"IF(C42<>\"\",'Cash Flow Analysis'!A89,\"\")","v":""},"","",null,0,0,0,0]
[{"$f":"IF(C43<>\"\",'Cash Flow Analysis'!A90,\"\")","v":""},"","",null,0,0,0,0]
[{"$f":"IF(C44<>\"\",'Cash Flow Analysis'!A91,\"\")","v":""},"","",null,0,0,0,0]
[{"$f":"IF(C45<>\"\",'Cash Flow Analysis'!A92,\"\")","v":""},"","",null,0,0,0,0]
[{"$f":"IF(C46<>\"\",'Cash Flow Analysis'!A93,\"\")","v":""},"","",null,0,0,0,0]
[{"$f":"IF(C47<>\"\",'Cash Flow Analysis'!A94,\"\")","v":""},"","",null,0,0,0,0]
[{"$f":"IF(C48<>\"\",'Cash Flow Analysis'!A95,\"\")","v":""},"","",null,0,0,0,0]
[{"$f":"IF(C49<>\"\",'Cash Flow Analysis'!A96,\"\")","v":""},"","",null,0,0,0,0]
[{"$f":"IF(C50<>\"\",'Cash Flow Analysis'!A97,\"\")","v":""},"","",null,0,0,0,0]
[{"$f":"IF(C51<>\"\",'Cash Flow Analysis'!A98,\"\")","v":""},"","",null,0,0,0,0]
[{"$f":"IF(C52<>\"\",'Cash Flow Analysis'!A99,\"\")","v":""},"","",null,0,0,0,0]
[{"$f":"IF(C53<>\"\",'Cash Flow Analysis'!A100,\"\")","v":""},"","",null,0,0,0,0]
[{"$f":"IF(C54<>\"\",'Cash Flow Analysis'!A101,\"\")","v":""},"","",null,0,0,0,0]
[{"$f":"IF(C55<>\"\",'Cash Flow Analysis'!A102,\"\")","v":""},"","",null,0,0,0,0]
[{"$f":"IF(C56<>\"\",'Cash Flow Analysis'!A103,\"\")","v":""},"","",null,0,0,0,0]
[{"$f":"IF(C57<>\"\",'Cash Flow Analysis'!A104,\"\")","v":""},"","",null,0,0,0,0]

{"sheet":"Capital Costs","index":5,"n_rows":61,"n_cols":8,"rows_kept":61,"cut":false,"hidden":false,"merged":[[15,7,27,7],[10,3,10,7],[11,3,11,7],[7,3,7,7],[1,5,3,7],[6,3,6,7],[8,3,8,7],[9,3,9,7]]}
[]
[null,"Capital Costs"]
[]
[null,null,"Color Key"]
[]
[]
[null,"Design Plant Hydrogen Production (kg/day)",1500,"Capital costs for the design plant (baseline) are entered on this sheet. Use the Plant Scaling sheet to set scaling parameters for scaling up or down in size from the baseline plant. Enter the output kg/day for the plant you wish to analyze on the Input Sheet"]
[null,null,null,"Comments"]
[null,"Basis year for capital costs",{"$f":"BasisYear","v":2005}]
[null,"Enter current year for capital costs",2010]
[null,{"$f":"\"CEPCI Inflator (\"&BasisYear&\" to \"&CurrentYear&\")\"","v":"CEPCI Inflator (2005 to 2010)"},{"$f":"VLOOKUP(CurrentYear,Tbl_PlantCostIndexes,2,FALSE)/VLOOKUP(BasisYear,Tbl_PlantCostIndexes,2,FALSE)","v":1.176420333190944},"The Chemical Engineering Plant Cost Index (CEPCI) is used to adjust the capital cost of the H2 Production facility from the basis year to the current year."]
[null,{"$f":"\"Consumer Price Inflator (\"&CurrentYear&\" to \"&ref_year&\")\"","v":"Consumer Price Inflator (2010 to 2016)"},{"$f":"VLOOKUP(ref_year,DeflatorTable,2,FALSE)/VLOOKUP(CurrentYear,DeflatorTable,2,FALSE)","v":1.0995746738559611},"The Consumer Price Inflator (CPI) is used to deflate all dollars from the current year to the Reference Year."]
[]
[null,{"$f":" \"CAPITAL INVESTMENT (Inputs REQUIRED in Basis Year, (\" & BasisYear & \") $)\"","v":"CAPITAL INVESTMENT (Inputs REQUIRED in Basis Year, (2005) $)"}]
[null,"Major pieces/systems of equipment",{"$f":"\"Baseline Uninstalled Costs $\"&BasisYear&\" Dollars\"","v":"Baseline Uninstalled Costs $2005 Dollars"},{"$f":"\"Baseline Uninstalled Costs $\"&ref_year&\" Dollars\"","v":"Baseline Uninstalled Costs $2016 Dollars"},"Installation Cost Factor","Baseline Installed Costs","Comments","Data Source"]
[null,"Water Feed System",4098.5118954802192,{"$f":"C16*CEPCIinflator*CPIinflator","v":5301.6792616973626},1.1000000000000001,{"$f":"D16*E16","v":5831.8471878670989},null,"Using AACE* cost categories  for a “>150psi, >400F Gas Process”: Installation Costs (% of total direct uninstalled capital) Sales tax: 5%   Typical state sales tax Shipping: 1%   Based on actual low-rider coast-to-coast transport of single large load Insurance: 1%   Shipping insurance estimate Setting: 10% One half of AACE generic recommended value due to Nth  plant considerations. Total Installation: 17% of total direct uninstalled capital\n\n"]
[null,"Primary Feed System: Ethanol",4098.5118954802192,{"$f":"C17*CEPCIinflator*CPIinflator","v":5301.6792616973626},1.1000000000000001,{"$f":"D17*E17","v":5831.8471878670989}]
[null,"Burner Feed System: Ethanol",683.08531591336998,883.61321028289387,1.1000000000000001,971.97453131118334]
[null,"Boiler ",32901.003683499614,42559.488264557185,1.1000000000000001,46815.437091012907]
[null,"Superheater",7470.2955689184882,9663.2905079916454,1.1000000000000001,10629.619558790811]
[null,"Pre-Reformer",19540.817200105743,25277.258660800133,1.1000000000000001,27804.984526880147]
[null,"Burner",2960,3828.9435323904218,1.1000000000000001,4211.8378856294639]
[null,"Reformer",216132.91540971582,279581.32722794509,1.1000000000000001,307539.45995073963]
[null,"Water Gas Shift Reactor",172065.34805740471,222577.19648409006,1.1000000000000001,244834.91613249909]
[null,"Air Preheater",21935.97820129932,28375.54792585213,1.1000000000000001,31213.102718437345]
[null,"Primary Air Feed System",3552,4594.7322388685061,1.1000000000000001,5054.2054627553571]
[null,"Reformate Cooler",33254.964592362085,43017.358647228808,1.1000000000000001,47319.094511951691]
[null,"Condenser",34115.415681392013,44130.405482458351,1.1000000000000001,48543.446030704188]
[null,"Air Feed System for Condenser",666.98964072942601,862.79245643322531,1.1000000000000001,949.07170207654792]
[null,"Pressure Swing Adsorption Unit",60326.41335068248,78035.956159259076,1.1000000000000001,85839.551775184984]
[null,"Water Purification",31644.687190314704,40934.364983741048,1.1000000000000001,45027.801482115159]
[null,"Structural Supports",17908,23165.108370962051,1.1000000000000001,25481.619208058259]
[null,"Controls System",32505.521199999999,42047.907150580992,1.1000000000000001,46252.697865639093]
[null,"System Assembly",186578.47144658293,241350.82146239348,1.1000000000000001,265485.90360863286]
[null,"Miscellaneous",88243.893032988126,114148.947128923,1.1000000000000001,125563.8418418153]
[null,"Ethanol underground storage tank.",{"$f":"150000*113/122","v":138934.42622950819},179720.29484386809,1,179720.29484386809]
[null,null,null,0,null,0]
[null,null,{"$f":"SUM(C16:C37)","v":1109617.2495923773},{"$f":"SUM(D16:D37)","v":1435358.7132620208},null,{"$f":"SUM(F16:F37)","v":1560922.5551038363}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"X = design capacity/115 (kg/day)",{"$f":"design_cap/115","v":13.043478260869565}]
[null,"N (see above) = ",6.6440000000000001]
[null,"PSA uninstalled cost (Q100) =",{"$f":"2*20212*C58^0.4569*0.96^C59+2*1813*C58*0.92^C59+2*14000*C58^0.4*0.96^C59+2*12000*C58^0.4*0.96^C59","v":237584.45007230857}]
[null,"bed volume (L)",{"$f":"C58*623","v":8126.086956521739}]

{"sheet":"Plant Scaling","index":6,"n_rows":35,"n_cols":10,"rows_kept":35,"cut":false,"hidden":false,"merged":[[7,3,7,5],[2,3,2,5],[4,3,4,5],[3,3,3,5],[6,3,6,5],[5,3,5,5]]}
[null,"leave this sheet as is for scaled costs"]
[null,"Plant Scaling Factors"]
[null,"Baseline Design Capacity (kg H2/day)",{"$f":"Baseline_Design_Capacity","v":1500},"Design capacity for original H2A case.  Imported from capital cost sheet"]
[null,"Scale Ratio",{"$f":"design_cap/Baseline_Design_Capacity","v":1},"Ratio of new design capacity (enter on Input Sheet) to the Baseline Design Capacity.  Used for linear scaling"]
[null,"Scale Factor",{"$f":"$G$35/Det_direct_cap","v":1},"Ratio of total scaled installed capital capital cost to total baseline installed capital costs.  Used for exponential scaling."]
[null,"Default Scaling Factor Exponent",0.6,"Scaling factor exponent used for scaling all capital equipment where an individual factor has not been entered below."]
[null,"Lower Limit for Scaling Capacity (kg H2/day)",500,"http://www.chemicals-technology.com/projects/air-products-plant/\n\n"]
[null,"Upper Limit for Scaling Capacity (kg H2/day)",6000,"http://hydrogen.pnl.gov/filedownloads/hydrogen/datasheets/hydrogen_production_capacity_by_state.xls\n"]
[]
[]
[null,{"$f":" \"CAPITAL INVESTMENT (Inputs REQUIRED in Reference Year, (\" & ref_year & \") $)\"","v":"CAPITAL INVESTMENT (Inputs REQUIRED in Reference Year, (2016) $)"}]
[null,"Major pieces/systems of equipment","Baseline Uninstalled Costs","Scaling Factor Exponent","Scaled Uninstalled Costs","Installation Cost Factor","Installed Cost (scaled)","Installed Cost (baseline)","Comments","Data Source"]
[null,{"$f":"'Capital Costs'!B16","v":"Water Feed System"},{"$f":"'Capital Costs'!D16","v":5301.6792616973626},null,{"$f":"IF($D13=\"\",$C13*Scale_Ratio^Scaling_Factor_Exponent,$C13*Scale_Ratio^$D13)","v":5301.6792616973626},{"$f":"'Capital Costs'!E16","v":1.1000000000000001},{"$f":"$E13*$F13","v":5831.8471878670989},{"$f":"C13*F13","v":5831.8471878670989},"Weighted average by sub-component list","https://netl.doe.gov/projects/files/QualityGuidelinesforEnergySystemStudiesCapitalCostScalingMethodologyRevision4Report_110719.pdf"]
[null,{"$f":"'Capital Costs'!B17","v":"Primary Feed System: Ethanol"},{"$f":"'Capital Costs'!D17","v":5301.6792616973626},null,{"$f":"IF($D14=\"\",$C14*Scale_Ratio^Scaling_Factor_Exponent,$C14*Scale_Ratio^$D14)","v":5301.6792616973626},{"$f":"'Capital Costs'!E17","v":1.1000000000000001},{"$f":"$E14*$F14","v":5831.8471878670989},{"$f":"C14*F14","v":5831.8471878670989},null,"https://netl.doe.gov/projects/files/QualityGuidelinesforEnergySystemStudiesCapitalCostScalingMethodologyRevision4Report_110719.pdf"]
[null,{"$f":"'Capital Costs'!B18","v":"Burner Feed System: Ethanol"},{"$f":"'Capital Costs'!D18","v":883.61321028289387},null,883.61321028289387,{"$f":"'Capital Costs'!E18","v":1.1000000000000001},971.97453131118334,971.97453131118334,null,"https://netl.doe.gov/projects/files/QualityGuidelinesforEnergySystemStudiesCapitalCostScalingMethodologyRevision4Report_110719.pdf"]
[null,{"$f":"'Capital Costs'!B19","v":"Boiler "},{"$f":"'Capital Costs'!D19","v":42559.488264557185},null,42559.488264557185,{"$f":"'Capital Costs'!E19","v":1.1000000000000001},46815.437091012907,46815.437091012907,null,"https://netl.doe.gov/projects/files/QualityGuidelinesforEnergySystemStudiesCapitalCostScalingMethodologyRevision4Report_110719.pdf"]
[null,{"$f":"'Capital Costs'!B20","v":"Superheater"},{"$f":"'Capital Costs'!D20","v":9663.2905079916454},null,9663.2905079916454,{"$f":"'Capital Costs'!E20","v":1.1000000000000001},10629.619558790811,10629.619558790811,null,"https://netl.doe.gov/projects/files/QualityGuidelinesforEnergySystemStudiesCapitalCostScalingMethodologyRevision4Report_110719.pdf"]
[null,{"$f":"'Capital Costs'!B21","v":"Pre-Reformer"},{"$f":"'Capital Costs'!D21","v":25277.258660800133},null,25277.258660800133,{"$f":"'Capital Costs'!E21","v":1.1000000000000001},27804.984526880147,27804.984526880147,null,"https://netl.doe.gov/projects/files/QualityGuidelinesforEnergySystemStudiesCapitalCostScalingMethodologyRevision4Report_110719.pdf"]
[null,{"$f":"'Capital Costs'!B22","v":"Burner"},{"$f":"'Capital Costs'!D22","v":3828.9435323904218},null,3828.9435323904218,{"$f":"'Capital Costs'!E22","v":1.1000000000000001},4211.8378856294639,4211.8378856294639,null,"https://netl.doe.gov/projects/files/QualityGuidelinesforEnergySystemStudiesCapitalCostScalingMethodologyRevision4Report_110719.pdf"]
[null,{"$f":"'Capital Costs'!B23","v":"Reformer"},{"$f":"'Capital Costs'!D23","v":279581.32722794509},null,279581.32722794509,{"$f":"'Capital Costs'!E23","v":1.1000000000000001},307539.45995073963,307539.45995073963,null,"https://netl.doe.gov/projects/files/QualityGuidelinesforEnergySystemStudiesCapitalCostScalingMethodologyRevision4Report_110719.pdf"]
[null,{"$f":"'Capital Costs'!B24","v":"Water Gas Shift Reactor"},{"$f":"'Capital Costs'!D24","v":222577.19648409006},null,222577.19648409006,{"$f":"'Capital Costs'!E24","v":1.1000000000000001},244834.91613249909,244834.91613249909,null,"https://netl.doe.gov/projects/files/QualityGuidelinesforEnergySystemStudiesCapitalCostScalingMethodologyRevision4Report_110719.pdf"]
[null,{"$f":"'Capital Costs'!B25","v":"Air Preheater"},{"$f":"'Capital Costs'!D25","v":28375.54792585213},null,28375.54792585213,{"$f":"'Capital Costs'!E25","v":1.1000000000000001},31213.102718437345,31213.102718437345,null,"https://netl.doe.gov/projects/files/QualityGuidelinesforEnergySystemStudiesCapitalCostScalingMethodologyRevision4Report_110719.pdf"]
[null,{"$f":"'Capital Costs'!B26","v":"Primary Air Feed System"},{"$f":"'Capital Costs'!D26","v":4594.7322388685061},null,4594.7322388685061,{"$f":"'Capital Costs'!E26","v":1.1000000000000001},5054.2054627553571,5054.2054627553571]
[null,{"$f":"'Capital Costs'!B27","v":"Reformate Cooler"},{"$f":"'Capital Costs'!D27","v":43017.358647228808},null,43017.358647228808,{"$f":"'Capital Costs'!E27","v":1.1000000000000001},47319.094511951691,{"$f":"C24*F24","v":47319.094511951691}]
[null,{"$f":"'Capital Costs'!B28","v":"Condenser"},{"$f":"'Capital Costs'!D28","v":44130.405482458351},null,44130.405482458351,{"$f":"'Capital Costs'!E28","v":1.1000000000000001},48543.446030704188,48543.446030704188]
[null,{"$f":"'Capital Costs'!B29","v":"Air Feed System for Condenser"},{"$f":"'Capital Costs'!D29","v":862.79245643322531},null,862.79245643322531,{"$f":"'Capital Costs'!E29","v":1.1000000000000001},949.07170207654792,949.07170207654792]
[null,{"$f":"'Capital Costs'!B30","v":"Pressure Swing Adsorption Unit"},{"$f":"'Capital Costs'!D30","v":78035.956159259076},null,78035.956159259076,{"$f":"'Capital Costs'!E30","v":1.1000000000000001},85839.551775184984,85839.551775184984]
[null,{"$f":"'Capital Costs'!B31","v":"Water Purification"},{"$f":"'Capital Costs'!D31","v":40934.364983741048},null,40934.364983741048,{"$f":"'Capital Costs'!E31","v":1.1000000000000001},45027.801482115159,45027.801482115159]
[null,{"$f":"'Capital Costs'!B32","v":"Structural Supports"},{"$f":"'Capital Costs'!D32","v":23165.108370962051},null,23165.108370962051,{"$f":"'Capital Costs'!E32","v":1.1000000000000001},25481.619208058259,25481.619208058259]
[null,{"$f":"'Capital Costs'!B33","v":"Controls System"},{"$f":"'Capital Costs'!D33","v":42047.907150580992},null,42047.907150580992,{"$f":"'Capital Costs'!E33","v":1.1000000000000001},46252.697865639093,46252.697865639093]
[null,{"$f":"'Capital Costs'!B34","v":"System Assembly"},{"$f":"'Capital Costs'!D34","v":241350.82146239348},null,241350.82146239348,{"$f":"'Capital Costs'!E34","v":1.1000000000000001},265485.90360863286,265485.90360863286]
[null,{"$f":"'Capital Costs'!B35","v":"Miscellaneous"},{"$f":"'Capital Costs'!D35","v":114148.947128923},null,114148.947128923,{"$f":"'Capital Costs'!E35","v":1.1000000000000001},125563.8418418153,125563.8418418153]
[null,{"$f":"'Capital Costs'!B36","v":"Ethanol underground storage tank."},{"$f":"'Capital Costs'!D36","v":179720.29484386809},null,179720.29484386809,{"$f":"'Capital Costs'!E36","v":1},179720.29484386809,179720.29484386809]
[null,null,null,null,0,null,0,0]
[null,"TOTALS (including scaling)",{"$f":"SUM(C13:C34)","v":1435358.7132620208},null,{"$f":"SUM(E13:E34)","v":1435358.7132620208},null,{"$f":"SUM(G13:G34)","v":1560922.5551038363},{"$f":"SUM(H13:H34)","v":1560922.5551038363}]

{"sheet":"Carbon Sequestration","index":7,"n_rows":275,"n_cols":28,"rows_kept":275,"cut":false,"hidden":false,"merged":[[68,1,68,2],[38,4,38,5],[41,4,41,5],[42,4,42,5],[44,4,44,5],[40,4,40,5],[43,4,43,5],[36,7,36,8],[37,7,37,8],[42,7,42,9],[43,7,43,9],[44,7,44,9],[40,7,40,8],[26,7,26,8],[29,7,29,9],[33,7,33,9],[35,7,35,8],[30,7,30,8],[34,7,34,8],[27,7,27,8],[29,4,29,5],[39,4,39,5],[37,4,37,5],[36,4,36,5],[35,4,35,5],[32,4,32,5],[3,1,3,9],[4,1,4,9],[20,7,20,8],[21,7,21,8],[25,3,25,5],[19,7,19,10],[22,7,22,8],[20,3,20,5],[24,3,24,5],[23,7,23,8],[24,7,24,8],[25,7,25,8]]}
[]
[null,"Carbon Sequestration"]
[]
[null,"Carbon Sequestration Calculation Information"]
[null,"Costs for carbon (CO₂) transport to the sequestration site and injection are calculated in this section.  Capital and operating costs for carbon capture and compression to 2,200psia are assumed to be included in the capital and operating costs for the production facility and are not included here.  For H2A analysis of hydrogen production processes, it is assumed that only carbon contained in the process feedstock can be captured. CO₂ transport and sequestration is based on NETL's 2018 CO₂ transport model. CO₂ injection into geologic formation is based on NETL's 2017 CO₂ OnShore Saline Storage Cost Model. "]
[]
[null,"Table of Contents"]
[null,"Color Key"]
[]
[]
[null,"Use default values (checkboxes)"]
[]
[]
[]
[null,"Carbon Sequestration Input Values"]
[null,"Summary of Output Values"]
[null,"Carbon Sequestration Calculations"]
[]
[]
[null,"Carbon Sequestration Information",null,null,null,null,null,"Summary of Output Values \n(CO2 Seq. costs are reported on Results Tab as part of total H2 Production cost)"]
[null,"CO₂ Produced from Feedstock (metric tonnes CO₂/year)",{"$f":"Feed_CO2_MTpY","v":5900},"CO2 emissions are based on the carbon content of the feed.  See the Physical Properties Table for specific values",null,null,null,"Capital Costs"]
[null,"CO₂ Produced from Feedstock (kg CO₂/kg H2)",{"$f":"Feed_CO2_kgpkgH2","v":12.580919189999999},null,null,null,null,"CO₂ Pipeline",null,{"$f":"IF(CO2_Capture_Efficiency,SUM(D36,D37,D38),0)","v":0}]
[null,"CO₂ Mass Flowrate (metric tonnes/day)",{"$f":"Feed_CO2_MTpY/365*CO2_Capture_Efficiency","v":0},null,null,null,null,"CO₂ Pumps",null,{"$f":"IF(CO2_Capture_Efficiency,D42,0)","v":0}]
[null,"CO₂ Mass Flowrate (million metric tonnes/year)",{"$f":"CO2_flowrate*365/1000000","v":0},null,null,null,null,"CO₂ Other equipment",null,{"$f":"IF(CO2_Capture_Efficiency,SUM(D39,D41),0)","v":0}]
[null,"Electricity Cost ($/kWh)",{"$f":"HLOOKUP(startup_year,INDIRECT(TMP_PriceTable),MATCH(\"Industrial Electricity\",INDIRECT(Energy_Feed_List),0),FALSE)*VLOOKUP(\"kWh\",CC_feedconversion,2,FALSE)","v":6.9980611257164108E-2},"Price for industrial electricity in the startup year",null,null,null,"CO₂ Surge tanks",null,{"$f":"+D40","v":0}]
[null,"Carbon Sequestration Electricity Usage (kWh/kg H₂)",{"$f":"IF(CO2_Capture_Efficiency,IF(C21=0,0,C58),0)","v":0},null,null,null,null,"CO₂ Injection",null,{"$f":"+D43","v":0}]
[null,null,null,null,null,null,null,"CO₂ Post-Injection",null,{"$f":"+D44","v":0}]
[null,"Carbon Sequestration Input Values",null,null,null,null,null,"CapEx without contingency",null,{"$f":"IF(CO2_Capture_Efficiency,SUM(J22:J27),0)","v":0},{"$f":"\"Total (\"&ref_year&\"$)\"","v":"Total (2016$)"}]
[null,"Process Design Parameters"]
[null,"Carbon Capture Efficiency (%)",{"$f":"+ProcessFlow!C16","v":0},null,"Set to 0 to turn off CCS",null,null,"Electrical Costs (annual cost)"]
[null,"Pipeline Length (miles)",100,null,null,null,null,"CO₂ Booster pumps",null,{"$f":"IF(CO2_Capture_Efficiency,CO2_flowrate_GTpY*1000000*C57*feedstockIndustrial_Electricity_Price,0)","v":0}]
[null,"CO₂ capture credit ($/metric ton CO₂ captured)",0,null,null,null,null,null,null,{"$f":"IF(CO2_Capture_Efficiency,SUM(J31:J31),0)","v":0},{"$f":"\"Total (\"&ref_year&\"$)\"","v":"Total (2016$)"}]
[null,"Approx Capital Charge Rate",{"$f":"+'Cash Flow Analysis'!E22","v":0.10185220882315059}]
[null,null,null,null,null,null,null,"O&M (annual cost)"]
[null,"Major cost depreciable capital components",{"$f":"\"Cost in $\"&2011&\" Dollars\"","v":"Cost in $2011 Dollars"},{"$f":"\"Cost in $\"&ref_year&\" Dollars\"","v":"Cost in $2016 Dollars"},null,null,null,"CO₂ Capture Credit",null,{"$f":"-Feed_CO2_MTpY*CO2_Capture_Efficiency*CO2_credit","v":0}]
[null,"Material costs",{"$f":"IF(CO2_Capture_Efficiency>0,AB73*C54,0)","v":0},{"$f":"+C36*$C$51*$C$52","v":0},null,null,null,"CO₂ Pipeline & pumps",null,{"$f":"IF(CO2_Capture_Efficiency,C64*$C$51*$C$52,0)","v":0}]
[null,"Labor expense",{"$f":"IF(CO2_Capture_Efficiency>0,AB97*C54,0)","v":0},0,null,null,null,"CO₂ Injection",null,{"$f":"IF(CO2_Capture_Efficiency>0,J26*E270,0)","v":0}]
[null,"Right of way",{"$f":"IF(CO2_Capture_Efficiency>0,AB121*C54,0)","v":0},0,null,null,null,"CO₂ Post-Injection",null,{"$f":"IF(CO2_Capture_Efficiency>0,F270*J27,0)","v":0}]
[null,"Miscellaneous",{"$f":"IF(CO2_Capture_Efficiency>0,AB193*C54*C55,0)","v":0},0,null,null,null,null,null,{"$f":"IF(CO2_Capture_Efficiency>0,SUM(J35:J38),0)","v":0},{"$f":"\"Total  (\"&ref_year&\"$)\"","v":"Total  (2016$)"}]
[null,"Surge tank",{"$f":"IF(CO2_Capture_Efficiency>0,1244743.65893146,0)","v":0},0]
[null,"Pipeline controls",{"$f":"IF(CO2_Capture_Efficiency>0,111907.191316147,0)","v":0},0,null,null,null,"Property tax and insurance",null,{"$f":"Det_CO2_seq*tax_ins_rate","v":0},{"$f":"+K39","v":"Total  (2016$)"}]
[null,"Pump",{"$f":"IF(CO2_Capture_Efficiency>0,AB145*C54*C55,0)","v":0},0]
[null,"Injection",{"$f":"IF(CO2_Capture_Efficiency>0,C275,0)","v":0},0,null,null,null,"Carbon Sequestration Energy Charge ($/tonne CO₂)",null,null,{"$f":"IF(CO2_Capture_Efficiency,ROUND(CO2_eCostpY/(Feed_CO2_MTpY*CO2_Capture_Efficiency),1),0)","v":0}]
[null,"Post-Injection (NPV)",{"$f":"IF(CO2_Capture_Efficiency>0,D275,0)","v":0},0,null,null,null,"Carbon Sequestration O&M Charge ($/tonne CO₂)",null,null,{"$f":"IF(CO2_Capture_Efficiency,ROUND((Det_CO2_OandMcost+ CCS_tax_insurance)/(Feed_CO2_MTpY*CO2_Capture_Efficiency),1),0)","v":0}]
[null,"Contingency",{"$f":"+SUM(C36:C42)*C56","v":0},0,"Contingency is 15% of transport costs",null,null,"Approx Carbon Seq. Cap. Charge ($/tonne CO₂)",null,null,{"$f":"IF(CO2_Capture_Efficiency,ROUND((Det_CO2_seq)*CO2_cap_charge_rate/(Feed_CO2_MTpY*CO2_Capture_Efficiency),1),0)","v":0}]
[null,"Total",null,{"$f":"+SUM(D36:D45)","v":0},null,null,null,"Total transportation and storage cost (w/o capture)",null,null,{"$f":"SUM(K43:K45)","v":0}]
[null,"Total without contingency",null,{"$f":"+D46-D45","v":0}]
[null,"Total uninstalled cost",null,{"$f":"IF(CO2_Capture_Efficiency,D46-D45-D37,0)","v":0}]
[]
[null,"CO₂ Transport cost estimate dollar basis",2011]
[null,"CEPCI inflator",{"$f":"VLOOKUP(C50,Tbl_PlantCostIndexes,2,FALSE)/VLOOKUP(BasisYear,Tbl_PlantCostIndexes,2,FALSE)","v":1.2509611277231953}]
[null,"CPI inflator",{"$f":"VLOOKUP(ref_year,DeflatorTable,2,FALSE)/VLOOKUP(C50,DeflatorTable,2,FALSE)","v":1.0771767810026385}]
[]
[null,"Transport distance to sequestration site (km)",{"$f":"+CO2_PipeLength*1.609344","v":160.93440000000001}]
[null,"Transport nameplate capacity (million metric tonnes/year)",{"$f":"+C21*CO2_Capture_Efficiency/1000000","v":0}]
[null,"Contingency factor",0.15]
[null,"Electricity use for booster pump (kWh/ metric tonne CO₂ sequestered)",{"$f":"+AB169*C54","v":{"$error":"#N/A"}}]
[null,"Electricity use for booster pump (kWh/kg H₂)",{"$f":"+C57*CO2_flowrate_GTpY*1000000/output_kgyear","v":{"$error":"#N/A"}}]
[null,"Electricity use (kWh/y)",{"$f":"+C57*CO2_flowrate_GTpY*1000000","v":{"$error":"#N/A"}}]
[]
[null,"% of capital sppent in 1st year",0.12]
[null,"% of capital sppent in 2nd year",0.38]
[null,"% of capital sppent in 3rd year",0.5]
[null,"Pipeline & pumps O&M (2011$/year)",{"$f":"+AB217*C54","v":{"$error":"#N/A"}}]
[null,"Operational life (years)",30]
[]
[]
[]
[null,"Below are lookup tables derived from NETL's CO₂ transport and storage cost models"]
[]
[null,"Materials cost (2011$/km)","Transport distance (km) to injection site →"]
[null,"Capacity (million metric tonnes/year) ↓",50,57,66,75,86,99,113,130,149,170,195,224,256,294,336,386,442,506,580,665,762,873,1000,null,{"$f":"\"Values at \"&ROUND(C54,0)&\" km distance\"","v":"Values at 161 km distance"},{"$f":"\"Value at \"&ROUND($C$55,2)&\" million metric tonnes/y\"","v":"Value at 0 million metric tonnes/y"}]
[null,0.5,55128.085986206912,54955.168059205505,54786.741506931387,54658.737327203089,54538.671391178847,54431.174341019403,54343.069202563333,54261.59615419984,54192.538659199272,54134.171178904682,54081.077439198358,54034.335986206905,53995.048989080475,53959.503610727967,53929.57066053641,53902.429384455972,53879.321228314373,53859.174987160979,53841.423283075725,53825.908127767696,53812.431477503262,53800.684108680609,53790.442308045996,null,{"$f":"FORECAST($C$54,OFFSET(G73:Y73,0,MATCH($C$54,$G$72:$Y$72,1)-1,1,2), OFFSET($G$72:$Y$72,0,MATCH($C$54,$G$72:$Y$72,1)-1,1,2))","v":54159.368142207473},{"$f":"FORECAST($C$55,OFFSET(AA73:AA95,MATCH($C$55,$B$73:$B$95,1)-1,0,2), OFFSET($B$73:$B$95,MATCH($C$55,$B$73:$B$95,1)-1,0,2))","v":{"$error":"#N/A"}}]
[null,0.56999999999999995,55128.085986206912,54955.168059205505,54786.741506931387,54658.737327203089,54538.671391178847,54431.174341019403,54343.069202563333,54261.59615419984,54192.538659199272,54134.171178904682,54081.077439198358,54034.335986206905,53995.048989080475,53959.503610727967,53929.57066053641,53902.429384455972,53879.321228314373,53859.174987160979,53841.423283075725,53825.908127767696,53812.431477503262,53800.684108680609,53790.442308045996,null,54159.368142207473]
[null,0.65,55128.085986206912,54955.168059205505,54786.741506931387,54658.737327203089,54538.671391178847,54431.174341019403,54343.069202563333,54261.59615419984,54192.538659199272,54134.171178904682,54081.077439198358,54034.335986206905,53995.048989080475,53959.503610727967,53929.57066053641,53902.429384455972,53879.321228314373,53859.174987160979,53841.423283075725,53825.908127767696,53812.431477503262,53800.684108680609,53790.442308045996,null,54159.368142207473]
[null,0.74,55128.085986206912,54955.168059205505,54786.741506931387,54658.737327203089,54538.671391178847,54431.174341019403,54343.069202563333,54261.59615419984,54192.538659199272,54134.171178904682,54081.077439198358,54034.335986206905,53995.048989080475,53959.503610727967,53929.57066053641,53902.429384455972,53879.321228314373,53859.174987160979,53841.423283075725,53825.908127767696,53812.431477503262,53800.684108680609,53790.442308045996,null,54159.368142207473]
[null,0.85,55128.085986206912,54955.168059205505,68070.515011299212,67942.510831570893,54538.671391178847,54431.174341019403,54343.069202563333,67545.369658567637,54192.538659199272,54134.171178904682,67364.850943566184,54034.335986206905,53995.048989080475,67243.277115095785,53929.57066053641,53902.429384455972,67163.094732682192,67142.94849152879,67125.19678744355,53825.908127767696,53812.431477503262,67084.457613048435,67074.215812413822,null,54159.368142207473]
[null,0.96,68411.859490574745,68238.941563573317,68070.515011299212,67942.510831570893,54538.671391178847,67714.947845387229,67626.842706931173,67545.369658567637,67476.312163567112,67417.944683272523,67364.850943566184,67318.10949057473,67278.822493448301,67243.277115095785,67213.344164904236,67186.202888823798,67163.094732682192,67142.94849152879,67125.19678744355,67109.681632135529,67096.20498187108,67084.457613048435,67074.215812413822,null,67443.141646575314]
[null,1.1000000000000001,68411.859490574745,68238.941563573317,68070.515011299212,67942.510831570893,67822.444895546665,67714.947845387229,67626.842706931173,67545.369658567637,67476.312163567112,67417.944683272523,67364.850943566184,67318.10949057473,67278.822493448301,67243.277115095785,67213.344164904236,67186.202888823798,67163.094732682192,67142.94849152879,67125.19678744355,67109.681632135529,67096.20498187108,67084.457613048435,67074.215812413822,null,67443.141646575314]
[null,1.25,68411.859490574745,68238.941563573317,68070.515011299212,67942.510831570893,67822.444895546665,67714.947845387229,67626.842706931173,67545.369658567637,67476.312163567112,67417.944683272523,67364.850943566184,67318.10949057473,67278.822493448301,67243.277115095785,67213.344164904236,67186.202888823798,67163.094732682192,67142.94849152879,67125.19678744355,67109.681632135529,67096.20498187108,67084.457613048435,67074.215812413822,null,67443.141646575314]
[null,1.43,68411.859490574745,68238.941563573317,68070.515011299212,67942.510831570893,67822.444895546665,67714.947845387229,67626.842706931173,67545.369658567637,67476.312163567112,67417.944683272523,67364.850943566184,67318.10949057473,67278.822493448301,67243.277115095785,67213.344164904236,67186.202888823798,67163.094732682192,67142.94849152879,67125.19678744355,67109.681632135529,67096.20498187108,67084.457613048435,67074.215812413822,null,67443.141646575314]
[null,1.63,68411.859490574745,68238.941563573317,68070.515011299212,67942.510831570893,67822.444895546665,67714.947845387229,67626.842706931173,67545.369658567637,67476.312163567112,67417.944683272523,67364.850943566184,67318.10949057473,67278.822493448301,67243.277115095785,67213.344164904236,67186.202888823798,67163.094732682192,67142.94849152879,67125.19678744355,67109.681632135529,67096.20498187108,67084.457613048435,67074.215812413822,null,67443.141646575314]
[null,1.86,68411.859490574745,104720.5732012745,68070.515011299212,67942.510831570893,67822.444895546665,67714.947845387229,104108.47434463236,104027.00129626883,67476.312163567112,103899.57632097369,103846.48258126734,103799.7411282759,103760.45413114945,103724.90875279695,103694.97580260543,103667.83452652495,103644.72637038333,103624.58012922997,103606.82842514472,103591.31326983674,103577.83661957226,103566.0892507496,103555.84745011499,null,88175.826628336363]
[null,2.12,104893.4911282759,104720.5732012745,104552.14664900038,67942.510831570893,104304.07653324782,104196.57948308837,104108.47434463236,104027.00129626883,103957.94380126824,103899.57632097369,103846.48258126734,103799.7411282759,103760.45413114945,103724.90875279695,103694.97580260543,103667.83452652495,103644.72637038333,103624.58012922997,103606.82842514472,103591.31326983674,103577.83661957226,103566.0892507496,103555.84745011499,null,103924.77328427647]
[null,2.42,104893.4911282759,104720.5732012745,104552.14664900038,104424.14246927205,104304.07653324782,104196.57948308837,104108.47434463236,104027.00129626883,103957.94380126824,103899.57632097369,103846.48258126734,103799.7411282759,103760.45413114945,103724.90875279695,103694.97580260543,103667.83452652495,103644.72637038333,103624.58012922997,103606.82842514472,103591.31326983674,103577.83661957226,103566.0892507496,103555.84745011499,null,103924.77328427647]
[null,2.76,104893.4911282759,104720.5732012745,104552.14664900038,104424.14246927205,104304.07653324782,104196.57948308837,104108.47434463236,104027.00129626883,103957.94380126824,103899.57632097369,103846.48258126734,103799.7411282759,103760.45413114945,103724.90875279695,103694.97580260543,103667.83452652495,103644.72637038333,103624.58012922997,103606.82842514472,103591.31326983674,103577.83661957226,103566.0892507496,103555.84745011499,null,103924.77328427647]
[null,3.15,104893.4911282759,104720.5732012745,104552.14664900038,104424.14246927205,104304.07653324782,104196.57948308837,104108.47434463236,104027.00129626883,103957.94380126824,103899.57632097369,103846.48258126734,103799.7411282759,103760.45413114945,103724.90875279695,103694.97580260543,103667.83452652495,103644.72637038333,103624.58012922997,103606.82842514472,103591.31326983674,103577.83661957226,103566.0892507496,103555.84745011499,null,103924.77328427647]
[null,3.59,104893.4911282759,104720.5732012745,104552.14664900038,104424.14246927205,104304.07653324782,104196.57948308837,104108.47434463236,104027.00129626883,103957.94380126824,103899.57632097369,103846.48258126734,103799.7411282759,103760.45413114945,103724.90875279695,103694.97580260543,103667.83452652495,103644.72637038333,103624.58012922997,103606.82842514472,103591.31326983674,103577.83661957226,103566.0892507496,103555.84745011499,null,103924.77328427647]
[null,4.09,104893.4911282759,104720.5732012745,104552.14664900038,104424.14246927205,104304.07653324782,104196.57948308837,104108.47434463236,104027.00129626883,103957.94380126824,103899.57632097369,103846.48258126734,103799.7411282759,103760.45413114945,103724.90875279695,103694.97580260543,103667.83452652495,103644.72637038333,103624.58012922997,103606.82842514472,103591.31326983674,103577.83661957226,103566.0892507496,103555.84745011499,null,103924.77328427647]
[null,4.67,104893.4911282759,104720.5732012745,104552.14664900038,172619.50004573187,172485.02619738472,104196.57948308837,104108.47434463236,104027.00129626883,172097.35753756762,172031.98595963765,103846.48258126734,171920.17054381614,103760.45413114945,103724.90875279695,103694.97580260543,103667.83452652495,171746.55401497649,103624.58012922997,103606.82842514472,103591.31326983674,103577.83661957226,103566.0892507496,103555.84745011499,null,172060.2065585368]
[null,5.32,104893.4911282759,172951.50246557462,172762.8647270276,172619.50004573187,172485.02619738472,172364.62950120613,172265.95174613537,172174.70193196827,172097.35753756762,172031.98595963765,171972.52097116658,171920.17054381614,171876.16910703457,171836.35828327975,171802.83337906524,171772.43514985513,171746.55401497649,171723.99022488468,171704.1083163092,171686.73134236431,171671.63749406807,171658.48044098669,171647.00962427593,null,172060.2065585368]
[null,6.07,173145.17054381617,172951.50246557462,172762.8647270276,172619.50004573187,172485.02619738472,172364.62950120613,172265.95174613537,172174.70193196827,172097.35753756762,172031.98595963765,171972.52097116658,171920.17054381614,171876.16910703457,171836.35828327975,171802.83337906524,171772.43514985513,171746.55401497649,171723.99022488468,171704.1083163092,171686.73134236431,171671.63749406807,171658.48044098669,171647.00962427593,null,172060.2065585368]
[null,6.92,173145.17054381617,172951.50246557462,172762.8647270276,172619.50004573187,172485.02619738472,172364.62950120613,255739.1298403581,172174.70193196827,172097.35753756762,172031.98595963765,171972.52097116658,255374.82464505752,171876.16910703457,171836.35828327975,255251.20156076638,171772.43514985513,171746.55401497649,171723.99022488468,171704.1083163092,171686.73134236431,171671.63749406807,171658.48044098669,171647.00962427593,null,172060.2065585368]
[null,7.89,173145.17054381617,172951.50246557462,172762.8647270276,172619.50004573187,255969.94042292444,255843.09390373621,255739.1298403581,255642.99164328922,172097.35753756762,255492.63017244093,255429.97955958743,255374.82464505752,255328.46598844836,171836.35828327975,255251.20156076638,255219.17485499143,255191.90723074434,255168.13466618332,171704.1083163092,255128.87977209929,255112.97732478724,255099.11542957652,255087.03010482763,null,219491.28809631203]
[null,9,173145.17054381617,172951.50246557462,256262.66315951239,256111.61822743306,255969.94042292444,255843.09390373621,255739.1298403581,255642.99164328922,255561.50379918856,255492.63017244093,255429.97955958743,255374.82464505752,255328.46598844836,255286.52244199233,255251.20156076638,255219.17485499143,255191.90723074434,255168.13466618332,255147.18765536268,255128.87977209929,255112.97732478724,255099.11542957652,255087.03010482763,null,255522.36258913821]
[]
[null,"Installation labor cost (2011$/km)",250926.29779080465,250012.30303379725,249122.0484003484,248445.45487892738,247810.82064565635,247242.62195195642,246776.92336297431,246346.28010733871,245981.26191947859,245672.74809506431,245392.10975661658,245145.04779080462,244937.38794885066,244749.50523470176,244591.28821226067,244447.82718154968,244325.68407051548,244219.19679584765,244125.36635996838,244043.35768191179,243972.12395908538,243910.03072387999,243855.89549195414,null,{"$f":"FORECAST($C$54,OFFSET(G97:Y97,0,MATCH($C$54,$G$72:$Y$72,1)-1,1,2), OFFSET($G$72:$Y$72,0,MATCH($C$54,$G$72:$Y$72,1)-1,1,2))","v":245805.93204395051},{"$f":"FORECAST($C$55,OFFSET(AA97:AA119,MATCH($C$55,$B$73:$B$95,1)-1,0,2), OFFSET($B$73:$B$95,MATCH($C$55,$B$73:$B$95,1)-1,0,2))","v":{"$error":"#N/A"}}]
[null,null,250926.29779080465,250012.30303379725,249122.0484003484,248445.45487892738,247810.82064565635,247242.62195195642,246776.92336297431,246346.28010733871,245981.26191947859,245672.74809506431,245392.10975661658,245145.04779080462,244937.38794885066,244749.50523470176,244591.28821226067,244447.82718154968,244325.68407051548,244219.19679584765,244125.36635996838,244043.35768191179,243972.12395908538,243910.03072387999,243855.89549195414,null,{"$f":"FORECAST($C$54,OFFSET(G98:Y98,0,MATCH($C$54,$G$72:$Y$72,1)-1,1,2), OFFSET($G$72:$Y$72,0,MATCH($C$54,$G$72:$Y$72,1)-1,1,2))","v":245805.93204395051}]
[null,null,250926.29779080465,250012.30303379725,249122.0484003484,248445.45487892738,247810.82064565635,247242.62195195642,246776.92336297431,246346.28010733871,245981.26191947859,245672.74809506431,245392.10975661658,245145.04779080462,244937.38794885066,244749.50523470176,244591.28821226067,244447.82718154968,244325.68407051548,244219.19679584765,244125.36635996838,244043.35768191179,243972.12395908538,243910.03072387999,243855.89549195414,null,{"$f":"FORECAST($C$54,OFFSET(G99:Y99,0,MATCH($C$54,$G$72:$Y$72,1)-1,1,2), OFFSET($G$72:$Y$72,0,MATCH($C$54,$G$72:$Y$72,1)-1,1,2))","v":245805.93204395051}]
[null,null,250926.29779080465,250012.30303379725,249122.0484003484,248445.45487892738,247810.82064565635,247242.62195195642,246776.92336297431,246346.28010733871,245981.26191947859,245672.74809506431,245392.10975661658,245145.04779080462,244937.38794885066,244749.50523470176,244591.28821226067,244447.82718154968,244325.68407051548,244219.19679584765,244125.36635996838,244043.35768191179,243972.12395908538,243910.03072387999,243855.89549195414,null,{"$f":"FORECAST($C$54,OFFSET(G100:Y100,0,MATCH($C$54,$G$72:$Y$72,1)-1,1,2), OFFSET($G$72:$Y$72,0,MATCH($C$54,$G$72:$Y$72,1)-1,1,2))","v":245805.93204395051}]
[null,null,250926.29779080465,250012.30303379725,266310.46138793457,265633.86786651344,247810.82064565635,247242.62195195642,246776.92336297431,263534.69309492491,245981.26191947859,245672.74809506431,262580.52274420287,245145.04779080462,244937.38794885066,261937.91822228799,244591.28821226067,244447.82718154968,261514.09705810167,261407.60978343384,261313.77934755458,244043.35768191179,243972.12395908538,261098.44371146613,261044.30847954028,null,{"$f":"FORECAST($C$54,OFFSET(G101:Y101,0,MATCH($C$54,$G$72:$Y$72,1)-1,1,2), OFFSET($G$72:$Y$72,0,MATCH($C$54,$G$72:$Y$72,1)-1,1,2))","v":245805.93204395051}]
[null,null,268114.71077839093,267200.71602138347,266310.46138793457,265633.86786651344,247810.82064565635,264431.0349395427,263965.3363505606,263534.69309492491,263169.67490706476,262861.16108265053,262580.52274420287,262333.46077839087,262125.80093643686,261937.91822228799,261779.70119984687,261636.24016913591,261514.09705810167,261407.60978343384,261313.77934755458,261231.77066949793,261160.53694667161,261098.44371146613,261044.30847954028,null,{"$f":"FORECAST($C$54,OFFSET(C102:Y102,0,MATCH($C$54,$G$72:$Y$72,1)-1,1,2), OFFSET($G$72:$Y$72,0,MATCH($C$54,$G$72:$Y$72,1)-1,1,2))","v":257256.16757274957}]
[null,null,268114.71077839093,267200.71602138347,266310.46138793457,265633.86786651344,264999.23363324249,264431.0349395427,263965.3363505606,263534.69309492491,263169.67490706476,262861.16108265053,262580.52274420287,262333.46077839087,262125.80093643686,261937.91822228799,261779.70119984687,261636.24016913591,261514.09705810167,261407.60978343384,261313.77934755458,261231.77066949793,261160.53694667161,261098.44371146613,261044.30847954028,null,264676.32360990479]
[null,null,268114.71077839093,267200.71602138347,266310.46138793457,265633.86786651344,264999.23363324249,264431.0349395427,263965.3363505606,263534.69309492491,263169.67490706476,262861.16108265053,262580.52274420287,262333.46077839087,262125.80093643686,261937.91822228799,261779.70119984687,261636.24016913591,261514.09705810167,261407.60978343384,261313.77934755458,261231.77066949793,261160.53694667161,261098.44371146613,261044.30847954028,null,264676.32360990479]
[null,null,268114.71077839093,267200.71602138347,266310.46138793457,265633.86786651344,264999.23363324249,264431.0349395427,263965.3363505606,263534.69309492491,263169.67490706476,262861.16108265053,262580.52274420287,262333.46077839087,262125.80093643686,261937.91822228799,261779.70119984687,261636.24016913591,261514.09705810167,261407.60978343384,261313.77934755458,261231.77066949793,261160.53694667161,261098.44371146613,261044.30847954028,null,264676.32360990479]
[null,null,268114.71077839093,267200.71602138347,266310.46138793457,265633.86786651344,264999.23363324249,264431.0349395427,263965.3363505606,263534.69309492491,263169.67490706476,262861.16108265053,262580.52274420287,262333.46077839087,262125.80093643686,261937.91822228799,261779.70119984687,261636.24016913591,261514.09705810167,261407.60978343384,261313.77934755458,261231.77066949793,261160.53694667161,261098.44371146613,261044.30847954028,null,264676.32360990479]
[null,null,268114.71077839093,311866.59200483171,266310.46138793457,265633.86786651344,264999.23363324249,264431.0349395427,308631.21233400883,308200.56907837314,263169.67490706476,307527.03706609888,307246.3987276511,306999.33676183916,306791.6769198851,306603.79420573625,306445.57718329516,306302.11615258415,306179.97304154991,306073.48576688214,305979.65533100296,305897.64665294625,305826.41293011984,305764.31969491445,305710.18446298863,null,264676.32360990479]
[null,null,312780.58676183922,311866.59200483171,310976.33737138286,265633.86786651344,309665.10961669084,309096.91092299088,308631.21233400883,308200.56907837314,307835.550890513,307527.03706609888,307246.3987276511,306999.33676183916,306791.6769198851,306603.79420573625,306445.57718329516,306302.11615258415,306179.97304154991,306073.48576688214,305979.65533100296,305897.64665294625,305826.41293011984,305764.31969491445,305710.18446298863,null,309342.19959335303]
[null,null,312780.58676183922,311866.59200483171,310976.33737138286,310299.74384996179,309665.10961669084,309096.91092299088,308631.21233400883,308200.56907837314,307835.550890513,307527.03706609888,307246.3987276511,306999.33676183916,306791.6769198851,306603.79420573625,306445.57718329516,306302.11615258415,306179.97304154991,306073.48576688214,305979.65533100296,305897.64665294625,305826.41293011984,305764.31969491445,305710.18446298863,null,309342.19959335303]
[null,null,312780.58676183922,311866.59200483171,310976.33737138286,310299.74384996179,309665.10961669084,309096.91092299088,308631.21233400883,308200.56907837314,307835.550890513,307527.03706609888,307246.3987276511,306999.33676183916,306791.6769198851,306603.79420573625,306445.57718329516,306302.11615258415,306179.97304154991,306073.48576688214,305979.65533100296,305897.64665294625,305826.41293011984,305764.31969491445,305710.18446298863,null,309342.19959335303]
[null,null,312780.58676183922,311866.59200483171,310976.33737138286,310299.74384996179,309665.10961669084,309096.91092299088,308631.21233400883,308200.56907837314,307835.550890513,307527.03706609888,307246.3987276511,306999.33676183916,306791.6769198851,306603.79420573625,306445.57718329516,306302.11615258415,306179.97304154991,306073.48576688214,305979.65533100296,305897.64665294625,305826.41293011984,305764.31969491445,305710.18446298863,null,309342.19959335303]
[null,null,312780.58676183922,311866.59200483171,310976.33737138286,310299.74384996179,309665.10961669084,309096.91092299088,308631.21233400883,308200.56907837314,307835.550890513,307527.03706609888,307246.3987276511,306999.33676183916,306791.6769198851,306603.79420573625,306445.57718329516,306302.11615258415,306179.97304154991,306073.48576688214,305979.65533100296,305897.64665294625,305826.41293011984,305764.31969491445,305710.18446298863,null,309342.19959335303]
[null,null,312780.58676183922,311866.59200483171,310976.33737138286,310299.74384996179,309665.10961669084,309096.91092299088,308631.21233400883,308200.56907837314,307835.550890513,307527.03706609888,307246.3987276511,306999.33676183916,306791.6769198851,306603.79420573625,306445.57718329516,306302.11615258415,306179.97304154991,306073.48576688214,305979.65533100296,305897.64665294625,305826.41293011984,305764.31969491445,305710.18446298863,null,309342.19959335303]
[null,null,312780.58676183922,311866.59200483171,310976.33737138286,412926.47555911116,412215.68521784781,309096.91092299088,308631.21233400883,308200.56907837314,410166.57944452879,409821.0439611848,307246.3987276511,409230.01962041401,306791.6769198851,306603.79420573625,306445.57718329516,306302.11615258415,408312.33225368999,306073.48576688214,305979.65533100296,305897.64665294625,305826.41293011984,305764.31969491445,305710.18446298863,null,353612.79474429821]
[null,null,312780.58676183922,414681.3454925656,413684.2603031029,412926.47555911116,412215.68521784781,411579.30268090393,411057.7202612441,410575.39981493214,410166.57944452879,409821.0439611848,409506.72902212327,409230.01962041401,408997.44059742545,408787.01195757859,408609.80889244465,408449.13253804843,408312.33225368999,408193.06650606211,408087.97641787736,407996.12669845379,407916.34492888837,407846.80050545826,407786.16904570139,null,411854.02599170961]
[null,null,415705.01962041395,414681.3454925656,413684.2603031029,412926.47555911116,412215.68521784781,411579.30268090393,411057.7202612441,410575.39981493214,410166.57944452879,409821.0439611848,409506.72902212327,409230.01962041401,408997.44059742545,408787.01195757859,408609.80889244465,408449.13253804843,408312.33225368999,408193.06650606211,408087.97641787736,407996.12669845379,407916.34492888837,407846.80050545826,407786.16904570139,null,411854.02599170961]
[null,null,415705.01962041395,414681.3454925656,413684.2603031029,412926.47555911116,412215.68521784781,411579.30268090393,518160.61391413055,410575.39981493214,410166.57944452879,409821.0439611848,409506.72902212327,516235.00073897012,408997.44059742545,408787.01195757859,515581.56443628826,408449.13253804843,408312.33225368999,408193.06650606211,408087.97641787736,407996.12669845379,407916.34492888837,407846.80050545826,407786.16904570139,null,411854.02599170961]
[null,null,415705.01962041395,414681.3454925656,413684.2603031029,412926.47555911116,519380.61270769528,518710.13824912935,518160.61391413055,517652.45487248036,410166.57944452879,516857.68709799665,516526.53385862825,516235.00073897012,515989.96212546458,408787.01195757859,515581.56443628826,515412.28042004933,515268.15154902905,515142.49656492093,408087.97641787736,514935.00641047669,514850.9506175415,514777.68059999909,514713.80102632655,null,518999.57888015674]
[null,null,415705.01962041395,414681.3454925656,520927.86145823175,520129.48110295495,519380.61270769528,518710.13824912935,518160.61391413055,517652.45487248036,517221.73341080546,516857.68709799665,516526.53385862825,516235.00073897012,515989.96212546458,515768.26052276883,515581.56443628826,515412.28042004933,515268.15154902905,515142.49656492093,515031.77665058343,514935.00641047669,514850.9506175415,514777.68059999909,514713.80102632655,null,518999.57888015674]
[]
[null,"Right of way (2011$/km)",27533.43196302143,27407.38516620978,27284.612312172463,27191.304943104096,27103.784077543856,27025.425175871456,26961.201814664131,26901.812849327904,26851.474077682866,26808.927685549439,26770.225533975077,26736.15381839266,26707.515954002258,26681.605505268082,26659.786180018258,26640.001817745098,26623.157357992524,26608.471956604619,26595.532029110134,26584.222411521478,26574.398741835859,26565.835614595446,26558.369956257051,null,{"$f":"FORECAST($C$54,OFFSET(C121:Y121,0,MATCH($C$54,$G$72:$Y$72,1)-1,1,2), OFFSET($G$72:$Y$72,0,MATCH($C$54,$G$72:$Y$72,1)-1,1,2))","v":27059.252340585805},{"$f":"FORECAST($C$55,OFFSET(AA121:AA143,MATCH($C$55,$B$73:$B$95,1)-1,0,2), OFFSET($B$73:$B$95,MATCH($C$55,$B$73:$B$95,1)-1,0,2))","v":{"$error":"#N/A"}}]
[null,null,27533.43196302143,27407.38516620978,27284.612312172463,27191.304943104096,27103.784077543856,27025.425175871456,26961.201814664131,26901.812849327904,26851.474077682866,26808.927685549439,26770.225533975077,26736.15381839266,26707.515954002258,26681.605505268082,26659.786180018258,26640.001817745098,26623.157357992524,26608.471956604619,26595.532029110134,26584.222411521478,26574.398741835859,26565.835614595446,26558.369956257051,null,27059.252340585805]
[null,null,27533.43196302143,27407.38516620978,27284.612312172463,27191.304943104096,27103.784077543856,27025.425175871456,26961.201814664131,26901.812849327904,26851.474077682866,26808.927685549439,26770.225533975077,26736.15381839266,26707.515954002258,26681.605505268082,26659.786180018258,26640.001817745098,26623.157357992524,26608.471956604619,26595.532029110134,26584.222411521478,26574.398741835859,26565.835614595446,26558.369956257051,null,27059.252340585805]
[null,null,27533.43196302143,27407.38516620978,27284.612312172463,27191.304943104096,27103.784077543856,27025.425175871456,26961.201814664131,26901.812849327904,26851.474077682866,26808.927685549439,26770.225533975077,26736.15381839266,26707.515954002258,26681.605505268082,26659.786180018258,26640.001817745098,26623.157357992524,26608.471956604619,26595.532029110134,26584.222411521478,26574.398741835859,26565.835614595446,26558.369956257051,null,27059.252340585805]
[null,null,27533.43196302143,27407.38516620978,28204.586349537058,28111.278980468691,27103.784077543856,27025.425175871456,26961.201814664131,27821.786886692495,26851.474077682866,26808.927685549439,27690.19957133969,26736.15381839266,26707.515954002258,27601.579542632677,26659.786180018258,26640.001817745098,27543.131395357126,27528.445993969221,27515.506066474736,26584.222411521478,26574.398741835859,27485.809651960055,27478.343993621653,null,27059.252340585805]
[null,null,28453.406000386036,28327.359203574379,28204.586349537058,28111.278980468691,27103.784077543856,27945.399213236051,27881.175852028733,27821.786886692495,27771.448115047464,27728.901722914045,27690.19957133969,27656.127855757259,27627.489991366863,27601.579542632677,27579.76021738286,27559.975855109686,27543.131395357126,27528.445993969221,27515.506066474736,27504.196448886069,27494.372779200447,27485.809651960055,27478.343993621653,null,27582.077966848854]
[null,null,28453.406000386036,28327.359203574379,28204.586349537058,28111.278980468691,28023.758114908454,27945.399213236051,27881.175852028733,27821.786886692495,27771.448115047464,27728.901722914045,27690.19957133969,27656.127855757259,27627.489991366863,27601.579542632677,27579.76021738286,27559.975855109686,27543.131395357126,27528.445993969221,27515.506066474736,27504.196448886069,27494.372779200447,27485.809651960055,27478.343993621653,null,27979.226377950399]
[null,null,28453.406000386036,28327.359203574379,28204.586349537058,28111.278980468691,28023.758114908454,27945.399213236051,27881.175852028733,27821.786886692495,27771.448115047464,27728.901722914045,27690.19957133969,27656.127855757259,27627.489991366863,27601.579542632677,27579.76021738286,27559.975855109686,27543.131395357126,27528.445993969221,27515.506066474736,27504.196448886069,27494.372779200447,27485.809651960055,27478.343993621653,null,27979.226377950399]
[null,null,28453.406000386036,28327.359203574379,28204.586349537058,28111.278980468691,28023.758114908454,27945.399213236051,27881.175852028733,27821.786886692495,27771.448115047464,27728.901722914045,27690.19957133969,27656.127855757259,27627.489991366863,27601.579542632677,27579.76021738286,27559.975855109686,27543.131395357126,27528.445993969221,27515.506066474736,27504.196448886069,27494.372779200447,27485.809651960055,27478.343993621653,null,27979.226377950399]
[null,null,28453.406000386036,28327.359203574379,28204.586349537058,28111.278980468691,28023.758114908454,27945.399213236051,27881.175852028733,27821.786886692495,27771.448115047464,27728.901722914045,27690.19957133969,27656.127855757259,27627.489991366863,27601.579542632677,27579.76021738286,27559.975855109686,27543.131395357126,27528.445993969221,27515.506066474736,27504.196448886069,27494.372779200447,27485.809651960055,27478.343993621653,null,27979.226377950399]
[null,null,28453.406000386036,30167.307278303586,28204.586349537058,28111.278980468691,28023.758114908454,27945.399213236051,29721.123926757933,29661.734961421695,27771.448115047464,29568.849797643248,29530.147646068875,29496.075930486455,29467.438066096056,29441.527617361877,29419.70829211206,29399.923929838897,29383.079470086315,29368.394068698424,29355.454141203936,29344.144523615283,29334.320853929654,29325.757726689251,29318.292068350849,null,27979.226377950399]
[null,null,30293.354075115225,30167.307278303586,30044.534424266254,28111.278980468691,29863.706189637658,29785.347287965262,29721.123926757933,29661.734961421695,29611.396189776657,29568.849797643248,29530.147646068875,29496.075930486455,29467.438066096056,29441.527617361877,29419.70829211206,29399.923929838897,29383.079470086315,29368.394068698424,29355.454141203936,29344.144523615283,29334.320853929654,29325.757726689251,29318.292068350849,null,29819.17445267961]
[null,null,30293.354075115225,30167.307278303586,30044.534424266254,29951.227055197898,29863.706189637658,29785.347287965262,29721.123926757933,29661.734961421695,29611.396189776657,29568.849797643248,29530.147646068875,29496.075930486455,29467.438066096056,29441.527617361877,29419.70829211206,29399.923929838897,29383.079470086315,29368.394068698424,29355.454141203936,29344.144523615283,29334.320853929654,29325.757726689251,29318.292068350849,null,29819.17445267961]
[null,null,30293.354075115225,30167.307278303586,30044.534424266254,29951.227055197898,29863.706189637658,29785.347287965262,29721.123926757933,29661.734961421695,29611.396189776657,29568.849797643248,29530.147646068875,29496.075930486455,29467.438066096056,29441.527617361877,29419.70829211206,29399.923929838897,29383.079470086315,29368.394068698424,29355.454141203936,29344.144523615283,29334.320853929654,29325.757726689251,29318.292068350849,null,29819.17445267961]
[null,null,30293.354075115225,30167.307278303586,30044.534424266254,29951.227055197898,29863.706189637658,29785.347287965262,29721.123926757933,29661.734961421695,29611.396189776657,29568.849797643248,29530.147646068875,29496.075930486455,29467.438066096056,29441.527617361877,29419.70829211206,29399.923929838897,29383.079470086315,29368.394068698424,29355.454141203936,29344.144523615283,29334.320853929654,29325.757726689251,29318.292068350849,null,29819.17445267961]
[null,null,30293.354075115225,30167.307278303586,30044.534424266254,29951.227055197898,29863.706189637658,29785.347287965262,29721.123926757933,29661.734961421695,29611.396189776657,29568.849797643248,29530.147646068875,29496.075930486455,29467.438066096056,29441.527617361877,29419.70829211206,29399.923929838897,29383.079470086315,29368.394068698424,29355.454141203936,29344.144523615283,29334.320853929654,29325.757726689251,29318.292068350849,null,29819.17445267961]
[null,null,30293.354075115225,30167.307278303586,30044.534424266254,29951.227055197898,29863.706189637658,29785.347287965262,29721.123926757933,29661.734961421695,29611.396189776657,29568.849797643248,29530.147646068875,29496.075930486455,29467.438066096056,29441.527617361877,29419.70829211206,29399.923929838897,29383.079470086315,29368.394068698424,29355.454141203936,29344.144523615283,29334.320853929654,29325.757726689251,29318.292068350849,null,29819.17445267961]
[null,null,30293.354075115225,30167.307278303586,30044.534424266254,31791.175129927098,31703.654264366854,29785.347287965262,29721.123926757933,29661.734961421695,31451.344264505864,31408.797872372445,29530.147646068875,31336.024005215655,29467.438066096056,29441.527617361877,29419.70829211206,29399.923929838897,31223.027544815523,29368.394068698424,29355.454141203936,29344.144523615283,29334.320853929654,29325.757726689251,29318.292068350849,null,30613.471274882701]
[null,null,30293.354075115225,32007.255353032782,31884.482498995465,31791.175129927098,31703.654264366854,31625.295362694462,31561.072001487133,31501.683036150906,31451.344264505864,31408.797872372445,31370.095720798083,31336.024005215655,31307.386140825256,31281.475692091073,31259.656366841253,31239.8720045681,31223.027544815523,31208.342143427628,31195.40221593314,31184.092598344487,31174.268928658854,31165.705801418455,31158.240143080046,null,31659.122527408806]
[null,null,32133.302149844425,32007.255353032782,31884.482498995465,31791.175129927098,31703.654264366854,31625.295362694462,31561.072001487133,31501.683036150906,31451.344264505864,31408.797872372445,31370.095720798083,31336.024005215655,31307.386140825256,31281.475692091073,31259.656366841253,31239.8720045681,31223.027544815523,31208.342143427628,31195.40221593314,31184.092598344487,31174.268928658854,31165.705801418455,31158.240143080046,null,31659.122527408806]
[null,null,32133.302149844425,32007.255353032782,31884.482498995465,31791.175129927098,31703.654264366854,31625.295362694462,33401.020076216329,31501.683036150906,31451.344264505864,31408.797872372445,31370.095720798083,33175.972079944855,31307.386140825256,31281.475692091073,33099.60444157046,31239.8720045681,31223.027544815523,31208.342143427628,31195.40221593314,31184.092598344487,31174.268928658854,31165.705801418455,31158.240143080046,null,31659.122527408806]
[null,null,32133.302149844425,32007.255353032782,31884.482498995465,31791.175129927098,33543.602339096047,33465.243437423655,33401.020076216329,33341.631110880109,31451.344264505864,33248.745947101655,33210.043795527286,33175.972079944855,33147.33421555446,31281.475692091073,33099.60444157046,33079.820079297286,33062.975619544726,33048.290218156828,31195.40221593314,33024.040673073687,33014.217003388047,33005.653876147655,32998.188217809249,null,33499.070602138003]
[null,null,32133.302149844425,32007.255353032782,33724.430573724661,33631.123204656295,33543.602339096047,33465.243437423655,33401.020076216329,33341.631110880109,33291.292339235064,33248.745947101655,33210.043795527286,33175.972079944855,33147.33421555446,33121.423766820284,33099.60444157046,33079.820079297286,33062.975619544726,33048.290218156828,33035.350290662347,33024.040673073687,33014.217003388047,33005.653876147655,32998.188217809249,null,33499.070602138003]
[]
[null,"Booster pump (2011$/[Mt/y][km])",0,0,0,0,0,0,0,0,0,3441.942414358618,3000.6677458511026,2612.188439468594,2285.6648845350196,1990.2388110236905,3482.9179192914585,3031.7627483987826,2647.6480110450907,3469.1514453021646,3026.5355712463711,3519.5802131787368,3071.5496611074277,3351.2612281842212,3510.7812626457903,null,{"$f":"FORECAST($C$54,OFFSET(C145:Y145,0,MATCH($C$54,$G$72:$Y$72,1)-1,1,2), OFFSET($G$72:$Y$72,0,MATCH($C$54,$G$72:$Y$72,1)-1,1,2))","v":0},{"$f":"FORECAST($C$55,OFFSET(AA145:AA167,MATCH($C$55,$B$73:$B$95,1)-1,0,2), OFFSET($B$73:$B$95,MATCH($C$55,$B$73:$B$95,1)-1,0,2))","v":{"$error":"#N/A"}}]
[null,null,0,0,0,0,0,0,0,4343.0880513159627,3789.2714541682899,3321.1849804180893,2895.3920342106421,2520.5421726387285,4410.9488021177749,3840.8261678304434,3360.7228968516379,4388.0941451119825,3832.1365158670255,3347.4394071407614,3893.8030804901737,4245.1236591810166,4445.6806824494106,3880.4223138905504,3952.2101266975264,null,0]
[null,null,0,0,0,0,0,5520.7493112972197,4836.7626709595106,4204.2629370648056,3668.1488712645955,3215.0245989319101,2802.8419580432037,4879.9480519502204,4269.9545454564432,5577.0834879431104,4879.9480519502213,4247.8304286406074,4946.1916906644774,5400.7330219211935,4711.6739811933176,4931.3159261812762,5020.838940589204,5008.5148391150033,5465.5418181842479,null,3137.4681228926493]
[null,null,0,0,0,0,6173.4331546020148,5362.7803161189222,4698.3650557148085,4083.9634715059487,3563.1896060119016,6246.0617799502743,5445.284628674598,4740.3147437122616,6221.6631011223435,5417.5025642425844,6320.4196582830155,6877.1405608260784,6005.8286345675706,6295.4377624004737,6407.5978604662296,6386.9503915281002,6967.391749288362,6689.6537963957689,6901.8982668450535,null,5712.7352862404614]
[null,null,0,0,0,0,6003.4706173821378,5215.1360918673117,4569.0130362377331,0,6930.1808469109246,6074.0996834689868,0,6914.7116932347835,8067.1636421072481,1756.1172554247071,7683.0129924830926,8025.3648667595407,1168.0960929748051,1020.3527136262132,1780.3395623960823,8540.2754948022593,8808.2416669727427,1774.2215570270234,1548.8954192845915,null,5555.4563525581307]
[null,null,0,0,0,0,5872.4578282751472,0,0,0,0,0,0,2254.6043447842085,1972.7788016861823,1717.7937865022541,1503.0695631894723,1308.3714332426493,2285.209833627433,1996.1714356982714,1741.487493902285,2278.3370220977267,1988.3124930380422,2314.0040010614557,2525.1568661583133,null,2535.1120803814774]
[null,null,0,0,0,0,0,0,0,0,0,2905.5912142591283,2533.0795201233423,2205.1361893930884,1929.4941657189522,1680.1037633471149,2940.181585857451,2559.3290488292837,2235.0701648147137,2928.5603147671054,2554.916412538199,2971.130865708582,2592.916044220744,2829.0407011686812,2963.7030385443109,null,0]
[null,null,0,0,0,0,0,0,0,3729.4810463258486,3253.909637733962,2851.9560942491785,2486.3206975505659,2164.4309643855372,3787.75418767469,3298.1805171589135,2885.9079525140496,3768.1285183085001,3290.7185702875136,3832.6682689514651,3343.6726622231745,3645.3574137019573,3817.5790237981132,3887.5461078539774,3878.6602881788826,null,0]
[null,null,0,0,0,0,0,4812.2823026187962,4216.0703359226618,3664.7380612250831,3197.4224695252401,2802.446752701534,4886.3174149667775,4253.7138210648282,3721.9995934317249,4861.3872240740893,4253.7138210648282,4936.9528285933757,4311.4565426177451,4707.6674699531704,4928.44084095787,5014.9047153606398,5001.7422357927644,4911.5046181367097,4764.1594795926085,null,2734.842948208272]
[null,null,0,0,0,6256.5913254020525,5456.3296442459759,4739.8419131833734,4152.6048619925132,3609.571918501184,6298.58187121012,5520.5217577076937,4812.7625580015792,6284.5225366761679,5498.9572195916471,6384.276862655156,5586.2422548232616,6078.2946814139113,6369.8327973550304,6491.5226202294025,6472.3358538641924,6350.6754054832863,6158.0623281516264,6450.0941498990223,6569.4208916721545,null,5049.1462548367581]
[null,null,0,0,7013.6917242697764,6172.0487173574029,5382.6006256023866,4675.794482846517,0,0,6213.4718631114793,0,0,0,0,0,0,0,1047.2933343932245,914.82935533953605,798.10974793414698,696.09572000271464,607.48510997612232,530.24473516816181,925.80730760361041,null,4980.9193289306895]
[null,null,0,0,0,6098.5680830478841,0,0,0,0,0,0,0,0,0,0,0,1184.9549384160396,1034.8249009696635,903.9379569735006,788.60794177343325,687.80843041893422,1200.5055281590323,1047.863931795169,914.78521245718264,null,0]
[null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,1539.133287130489,1346.7416262391778,1172.2932290579372,1023.7673900822709,894.27902453826823,1560.3627117805647,1360.9178538838007,1187.6776546361252,1555.0006406060609,1357.5155592490912,null,0]
[null,null,0,0,0,0,0,0,0,0,0,0,0,2001.1184553576591,1750.9786484379517,1524.6616802725023,1334.0789702384395,1161.2708134718023,2028.2829592765413,1771.7412411071764,1545.691496552123,2022.1828601508976,1764.7658818902189,2053.8397892330613,1793.0021360004625,null,0]
[null,null,0,0,0,0,0,0,0,0,0,2614.7129179088756,2279.4933130487634,1984.3803394844147,1736.3327970488629,1511.9088300833637,2645.8404526458862,2303.115005411963,2011.3176291606737,2635.3825852441237,2299.1441174715974,2673.691404779001,2333.339611782199,2545.8258650888256,2667.0071762670532,null,0]
[null,null,0,0,0,0,0,0,0,3394.2241959015446,2961.4036608536967,2595.5832086305927,2262.8161306010297,1969.8622565500034,3447.2589489625061,3001.6948671238147,2626.483008733338,3429.397503631094,2994.9037022660686,3488.1355372901248,3043.0975549462123,3317.6627478736896,3474.4027202141792,3538.0802042043592,3529.9931637376062,null,0]
[null,null,0,0,0,0,0,4428.3128154377418,3879.6722896312958,3372.3305286795112,2942.3018035458822,2578.8409925196261,4496.4407049060146,3914.3122207887182,3425.0231931901285,4473.4996809013919,3914.3122207887182,4543.0359453713618,3967.4476807994247,4332.0451455369212,4535.2031247758941,4614.7680918772257,4602.6558396675746,4519.6182343127466,4384.0296872833642,null,2516.6312602171565]
[null,null,0,0,0,0,0,4402.6761091644585,3857.2118124538179,3352.8071908252418,0,0,4470.4095877669888,0,5107.7922047728289,5930.1351674460057,5188.8682715152554,5645.9188446539047,986.11976200742401,6029.7520625513234,6011.9301352728471,5898.9239297226059,5720.0122678120924,5991.2705815433865,6102.1090873019393,null,2502.0617979624949]
[null,null,0,0,0,0,0,0,0,0,0,0,2223.9908120138257,1936.0634301013215,1694.0555013386563,1475.095946743864,1290.708953400881,2247.0373489258859,1962.3448341298463,1714.1431159790357,2243.1631466001518,1956.4430451550195,2276.5260280456482,1987.0708286034182,2168.3910417134798,null,0]
[null,null,0,0,0,0,0,0,0,0,2897.5638061437712,2539.629453620129,2214.0359339252409,1927.3973531938479,1686.4726840446169,2936.9864429620538,2569.8631375917971,2236.9793114788699,2930.3416772539954,2559.705575783134,2977.4966007960134,2596.9143285138161,2832.9199941956817,2967.2646537142405,3022.159049807954,null,0]
[null,null,0,0,0,0,0,0,0,3308.0435081952069,2886.2124568146101,2529.6803297963347,2205.3623387968046,0,3359.7316880107569,2925.4806535059652,0,3342.3237518034471,3891.8158919943608,3399.5704036788688,3707.290138494629,3880.1111825447538,3950.5506462698663,3940.8536638293413,3870.410904588392,null,0]
[null,null,0,0,0,0,0,0,0,0,2876.2466609874027,0,0,0,0,4373.0689029298264,1275.4784300211995,1110.2610168060182,969.59446264054975,846.95800886783206,4433.3870946943762,1288.9045187582647,1124.8313713572782,1472.7173624987045,1285.6822574613691,null,0]
[null,null,0,0,0,0,0,0,0,0,0,0,0,1907.3850064674864,1668.9618806590506,1453.2457192133229,1271.5900043116576,1106.8762731832046,1933.2771106276784,1688.7519424850473,1473.2904877541964,1927.4627433776704,1682.1033127902242,1957.6368451258509,1709.0169657948679,null,0]
[]
[null,"Electricity use for booster pump (kWh/km-metric tonne CO₂)",0,0,0,0,0,0,0,0,0,1.6250362711955582E-2,1.4166982877089482E-2,1.2332864558180575E-2,1.0791256488408004E-2,9.3964682348042488E-3,1.6443819410907435E-2,1.4313790989805435E-2,1.2500279009196601E-2,1.6378824077267488E-2,1.4289112039823014E-2,1.6616912246811725E-2,1.4501636015918367E-2,1.582223173558104E-2,1.6575369966194697E-2,null,{"$f":"FORECAST($C$54,OFFSET(C169:Y169,0,MATCH($C$54,$G$72:$Y$72,1)-1,1,2), OFFSET($G$72:$Y$72,0,MATCH($C$54,$G$72:$Y$72,1)-1,1,2))","v":0},{"$f":"FORECAST($C$55,OFFSET(AA169:AA191,MATCH($C$55,$B$73:$B$95,1)-1,0,2), OFFSET($B$73:$B$95,MATCH($C$55,$B$73:$B$95,1)-1,0,2))","v":{"$error":"#N/A"}}]
[null,null,0,0,0,0,0,0,0,2.1250474315634219E-2,1.8540682288808379E-2,1.6250362711955579E-2,1.4166982877089481E-2,1.2332864558180574E-2,2.1582512976816005E-2,1.8792936469608494E-2,1.6443819410907431E-2,2.1470686484708151E-2,1.87504185137949E-2,1.6378824077267484E-2,1.905214938643068E-2,2.0771140308514655E-2,2.175245402387755E-2,1.8986678082697241E-2,1.9337931627227141E-2,null,0]
[null,null,0,0,0,0,0,2.7904663242752016E-2,2.4447448327720792E-2,2.1250474315634225E-2,1.8540682288808386E-2,1.6250362711955586E-2,1.4166982877089484E-2,2.4665729116361158E-2,2.1582512976816012E-2,2.8189404704412748E-2,2.4665729116361154E-2,2.1470686484708155E-2,2.500055801839321E-2,2.7298040128779143E-2,2.3815186733038354E-2,2.4925368370217589E-2,2.5377863027857148E-2,2.5315570776929662E-2,2.7625616610324491E-2,null,1.5858353000204772E-2]
[null,null,0,0,0,0,3.2122810012005225E-2,2.7904663242752009E-2,2.4447448327720788E-2,2.1250474315634222E-2,1.8540682288808383E-2,3.2500725423911164E-2,2.8333965754178965E-2,2.4665729116361151E-2,3.2373769465224016E-2,2.8189404704412748E-2,3.288763882181487E-2,3.578447747451359E-2,3.1250697522991505E-2,3.2757648154534975E-2,3.3341261426253703E-2,3.323382449362345E-2,3.6254090039795919E-2,3.4808909818278277E-2,3.5913301593421834E-2,null,2.9725617116625441E-2]
[null,null,0,0,0,0,3.2122810012005225E-2,2.7904663242752009E-2,2.4447448327720788E-2,0,3.7081364577616766E-2,3.2500725423911164E-2,0,3.6998593674541731E-2,4.3165025953632016E-2,9.3964682348042488E-3,4.1109548527268593E-2,4.294137296941631E-2,6.2501395045983007E-3,5.4596080257558284E-3,9.5260746932153417E-3,4.5696508678732241E-2,4.7130317051734698E-2,9.4933390413486224E-3,8.2876849830973483E-3,null,2.9725617116625441E-2]
[null,null,0,0,0,0,3.2122810012005225E-2,0,0,0,0,0,0,1.2332864558180575E-2,1.0791256488408004E-2,9.3964682348042488E-3,8.2219097054537175E-3,7.1568954949027177E-3,1.2500279009196601E-2,1.0919216051511657E-2,9.5260746932153417E-3,1.2462684185108791E-2,1.0876227011938775E-2,1.2657785388464829E-2,1.3812808305162244E-2,null,1.3867264116420669E-2]
[null,null,0,0,0,0,0,0,0,0,0,1.6250362711955586E-2,1.4166982877089484E-2,1.2332864558180579E-2,1.0791256488408006E-2,9.3964682348042505E-3,1.6443819410907438E-2,1.4313790989805437E-2,1.2500279009196605E-2,1.6378824077267488E-2,1.4289112039823014E-2,1.6616912246811725E-2,1.4501636015918371E-2,1.582223173558104E-2,1.6575369966194697E-2,null,0]
[null,null,0,0,0,0,0,0,0,2.1250474315634222E-2,1.8540682288808383E-2,1.6250362711955582E-2,1.4166982877089482E-2,1.2332864558180575E-2,2.1582512976816008E-2,1.8792936469608498E-2,1.6443819410907435E-2,2.1470686484708155E-2,1.8750418513794904E-2,2.1838432103023313E-2,1.9052149386430683E-2,2.0771140308514652E-2,2.1752454023877554E-2,2.215112442981345E-2,2.2100493288259592E-2,null,0]
[null,null,0,0,0,0,0,2.7904663242752009E-2,2.4447448327720788E-2,2.1250474315634222E-2,1.8540682288808383E-2,1.6250362711955582E-2,2.8333965754178965E-2,2.4665729116361151E-2,2.1582512976816008E-2,2.8189404704412748E-2,2.4665729116361154E-2,2.8627581979610871E-2,2.5000558018393203E-2,2.7298040128779143E-2,2.8578224079646029E-2,2.9079596431920519E-2,2.9003272031836735E-2,2.8480017124045871E-2,2.7625616610324491E-2,null,1.5858353000204772E-2]
[null,null,0,0,0,3.6834155480432652E-2,3.2122810012005225E-2,2.7904663242752009E-2,2.4447448327720788E-2,2.1250474315634222E-2,3.7081364577616766E-2,3.2500725423911164E-2,2.8333965754178965E-2,3.6998593674541724E-2,3.2373769465224009E-2,3.7585872939216995E-2,3.288763882181487E-2,3.578447747451359E-2,3.7500837027589801E-2,3.8217256180290801E-2,3.8104298772861367E-2,3.738805255532638E-2,3.6254090039795919E-2,3.7973356165394483E-2,3.8675863254454289E-2,null,2.9725617116625441E-2]
[null,null,0,0,4.1856994864128014E-2,3.6834155480432652E-2,3.2122810012005225E-2,2.7904663242752009E-2,0,0,3.7081364577616766E-2,0,0,0,0,0,0,0,6.2501395045983007E-3,5.4596080257558284E-3,4.7630373466076709E-3,4.1542280617029312E-3,3.6254090039795918E-3,3.1644463471162073E-3,5.525123322064898E-3,null,2.9725617116625441E-2]
[null,null,0,0,0,3.6834155480432659E-2,0,0,0,0,0,0,0,0,0,0,0,7.1568954949027186E-3,6.2501395045983024E-3,5.4596080257558292E-3,4.7630373466076717E-3,4.1542280617029312E-3,7.2508180079591854E-3,6.3288926942324155E-3,5.5251233220648989E-3,null,0]
[null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,9.3964682348042471E-3,8.2219097054537157E-3,7.1568954949027168E-3,6.2501395045982998E-3,5.4596080257558275E-3,9.52607469321534E-3,8.3084561234058607E-3,7.2508180079591828E-3,9.4933390413486207E-3,8.2876849830973466E-3,null,0]
[null,null,0,0,0,0,0,0,0,0,0,0,0,1.2332864558180575E-2,1.0791256488408004E-2,9.3964682348042488E-3,8.2219097054537175E-3,7.1568954949027177E-3,1.2500279009196601E-2,1.0919216051511657E-2,9.5260746932153417E-3,1.2462684185108791E-2,1.0876227011938775E-2,1.2657785388464829E-2,1.1050246644129796E-2,null,0]
[null,null,0,0,0,0,0,0,0,0,0,1.6250362711955586E-2,1.4166982877089484E-2,1.2332864558180579E-2,1.0791256488408006E-2,9.3964682348042505E-3,1.6443819410907438E-2,1.4313790989805437E-2,1.2500279009196605E-2,1.6378824077267491E-2,1.4289112039823016E-2,1.6616912246811725E-2,1.4501636015918371E-2,1.582223173558104E-2,1.65753699661947E-2,null,0]
[null,null,0,0,0,0,0,0,0,2.1250474315634225E-2,1.8540682288808386E-2,1.6250362711955586E-2,1.4166982877089484E-2,1.2332864558180579E-2,2.1582512976816012E-2,1.8792936469608501E-2,1.6443819410907438E-2,2.1470686484708155E-2,1.8750418513794904E-2,2.1838432103023317E-2,1.9052149386430687E-2,2.0771140308514659E-2,2.1752454023877554E-2,2.2151124429813453E-2,2.2100493288259596E-2,null,0]
[null,null,0,0,0,0,0,2.7904663242752016E-2,2.4447448327720792E-2,2.1250474315634225E-2,1.8540682288808386E-2,1.6250362711955586E-2,2.8333965754178968E-2,2.4665729116361158E-2,2.1582512976816012E-2,2.8189404704412748E-2,2.4665729116361154E-2,2.8627581979610874E-2,2.500055801839321E-2,2.7298040128779146E-2,2.8578224079646029E-2,2.9079596431920519E-2,2.9003272031836742E-2,2.8480017124045871E-2,2.7625616610324494E-2,null,1.5858353000204772E-2]
[null,null,0,0,0,0,0,2.7904663242752016E-2,2.4447448327720792E-2,2.1250474315634225E-2,0,0,2.8333965754178968E-2,0,3.2373769465224009E-2,3.7585872939217002E-2,3.2887638821814877E-2,3.578447747451359E-2,6.2501395045983024E-3,3.8217256180290801E-2,3.8104298772861374E-2,3.738805255532638E-2,3.6254090039795919E-2,3.7973356165394483E-2,3.8675863254454289E-2,null,1.5858353000204772E-2]
[null,null,0,0,0,0,0,0,0,0,0,0,1.4166982877089482E-2,1.2332864558180575E-2,1.0791256488408004E-2,9.3964682348042488E-3,8.2219097054537175E-3,1.4313790989805435E-2,1.2500279009196601E-2,1.0919216051511657E-2,1.4289112039823014E-2,1.2462684185108795E-2,1.4501636015918367E-2,1.2657785388464829E-2,1.3812808305162244E-2,null,0]
[null,null,0,0,0,0,0,0,0,0,1.8540682288808386E-2,1.6250362711955586E-2,1.4166982877089484E-2,1.2332864558180579E-2,1.0791256488408006E-2,1.8792936469608501E-2,1.6443819410907438E-2,1.4313790989805437E-2,1.87504185137949E-2,1.6378824077267484E-2,1.9052149386430687E-2,1.6616912246811725E-2,1.812704501989796E-2,1.8986678082697241E-2,1.9337931627227144E-2,null,0]
[null,null,0,0,0,0,0,0,0,2.1250474315634222E-2,1.8540682288808383E-2,1.6250362711955582E-2,1.4166982877089482E-2,0,2.1582512976816008E-2,1.8792936469608498E-2,0,2.1470686484708151E-2,2.5000558018393203E-2,2.1838432103023313E-2,2.3815186733038351E-2,2.4925368370217582E-2,2.5377863027857141E-2,2.5315570776929659E-2,2.4863054949292043E-2,null,0]
[null,null,0,0,0,0,0,0,0,0,1.8540682288808383E-2,0,0,0,0,2.8189404704412748E-2,8.2219097054537175E-3,7.1568954949027177E-3,6.2501395045983007E-3,5.4596080257558284E-3,2.8578224079646029E-2,8.3084561234058624E-3,7.2508180079591837E-3,9.4933390413486224E-3,8.2876849830973483E-3,null,0]
[null,null,0,0,0,0,0,0,0,0,0,0,0,1.2332864558180579E-2,1.0791256488408006E-2,9.3964682348042505E-3,8.2219097054537192E-3,7.1568954949027186E-3,1.2500279009196605E-2,1.0919216051511658E-2,9.5260746932153435E-3,1.2462684185108795E-2,1.0876227011938777E-2,1.2657785388464831E-2,1.1050246644129798E-2,null,0]
[]
[null,"Miscellaneous (2011$/[Mt/y][km])",118103.29291967429,117374.86555526982,116665.35838214855,116126.13293057642,115620.34781708629,115167.5099055593,114796.36161047523,114453.15140133978,114162.24247160676,113916.36588393767,113692.70525168677,113495.80401650876,113330.30513349277,113180.56804885923,113054.47366179942,112940.13937301461,112842.7948491334,112757.92757365482,112683.14743231983,112617.78888977123,112561.01767464413,112511.53116356593,112468.38695074542,null,{"$f":"FORECAST($C$54,OFFSET(C193:Y193,0,MATCH($C$54,$G$72:$Y$72,1)-1,1,2), OFFSET($G$72:$Y$72,0,MATCH($C$54,$G$72:$Y$72,1)-1,1,2))","v":115362.99787559449},{"$f":"FORECAST($C$55,OFFSET(AA193:AA215,MATCH($C$55,$B$73:$B$95,1)-1,0,2), OFFSET($B$73:$B$95,MATCH($C$55,$B$73:$B$95,1)-1,0,2))","v":{"$error":"#N/A"}}]
[null,null,103599.37975410027,102960.40838181564,102338.03366855136,101865.02888647057,101421.35773428623,101024.13149610466,100698.56281620635,100397.50122924543,100142.31795754979,99926.636740296221,99730.443203234026,99557.722821498915,99412.548362712972,99281.200042858982,99170.590931403014,99070.297695626869,98984.907762397721,98910.462783907744,98844.866168701614,98787.534113834423,98737.734802319406,98694.325582075384,98656.479781355636,null,101195.61217157412]
[null,null,90848.686861287919,90288.358119438315,89742.583370883498,89327.794561981864,88938.729090066379,88590.392235045612,88304.893546519408,88040.885693338292,87817.109593543661,87627.97375687513,87455.927116682127,87304.464628083661,87177.157794994433,87061.975422199408,86964.979739845701,86877.030286934314,86802.149883948776,86736.867364349848,86679.344178707557,86629.068376747106,86585.398211264706,86547.331664281475,86514.143808265697,null,88740.767596611156]
[null,null,79799.522243023166,79307.341591398523,78827.944852803077,78463.603331470571,78121.856633166419,77815.88507132385,77565.109196267047,77333.210406310667,77136.650318653221,76970.517489147082,76819.39544032891,76686.354065208623,76574.53049560322,76473.35678976975,76388.157879594204,76310.904981766624,76245.131654819867,76187.788901118111,76137.261778594475,76093.100601196784,76054.741672056844,76021.304840247249,75992.153345098253,null,77947.971537563848]
[null,null,69472.525246867226,69044.038561923429,87835.426289482028,87518.234847380809,68011.969304168408,67745.594062093718,67527.271535573673,86534.128065476893,67154.260277415742,67009.62699055158,86086.8068009751,66762.237656769852,66664.885372642806,85785.549622841238,66502.631565764372,66435.376101773305,85586.859505355475,85536.937578603363,85492.949260171023,66245.758170453671,66212.363338025956,85391.998513845203,85366.619565127257,null,67860.586985643837]
[null,null,78519.874598773546,78140.48534647956,77770.950360478892,77490.103771118418,60218.93115473244,76990.820945588639,76797.514541899043,76618.759224641006,76467.244157071691,76339.183434327409,76222.693521696696,76120.140795041487,76033.94346013735,75955.955395224009,75890.28123529705,75830.732126554954,75780.031853700159,75735.830147721732,75696.882157443106,75662.841249865698,75633.272908653656,75607.498684133781,75585.027739956422,null,69750.475989017883]
[null,null,68526.43601347509,68195.332666018527,67872.829405508834,67627.726927521522,67397.824603207817,67191.989188877356,67023.285418384607,66867.280777868495,66735.049446171659,66623.287360867558,66521.623437117101,66432.122875672561,66356.896110665315,66288.833799468222,66231.518168986498,66179.548037720684,66135.300526865583,66096.724492557129,66062.733519223068,66033.025090791882,66007.219993006816,65984.72612433492,65965.115118507412,null,67280.847357075167]
[null,null,60303.263691858083,60011.892746096295,59728.089876847778,59512.399696218941,59310.085650822883,59128.950486212081,58980.491168178458,58843.207084524285,58726.843512631065,58628.492877563447,58539.028624663064,58460.268130591852,58394.068577385486,58334.173743532047,58283.735988708126,58238.002273194201,58199.06446364172,58165.117553450276,58135.2054969163,58109.062079896852,58086.353593846005,58066.558989414742,58049.301304286528,null,59207.145674226158]
[null,null,52712.643087288532,52457.94820462964,52209.868773468341,52021.328405785796,51844.480464006017,51686.145529905662,51556.373398757401,51436.369829129624,51334.653420132046,51248.682585282731,51170.479567013164,51101.632981286595,51043.76623897333,50991.410614975561,50947.321668451164,50907.344644400524,50873.308097588917,50843.634225043948,50817.487322479283,50794.634685224533,50774.784610005248,50757.481634103795,50742.396245005708,null,51754.497966980904]
[null,null,46244.834119523075,46021.390142711891,45803.749905558121,45638.343325321286,45483.194517502212,45344.287182677981,45230.438012406797,45125.158807150532,45035.922939134252,44960.500672978109,44891.893117072905,44831.493965177804,44780.727436645313,44734.795815592064,44696.116555757762,44661.044688032373,44631.184404633226,44605.151498044695,44582.212804383671,44562.164171700046,44544.749688532211,44529.569777158547,44516.335356047952,null,45404.252817658096]
[null,null,40526.386889689573,57886.952818597456,40139.845347343937,39994.892268964344,39858.928528778815,39737.197907400587,57193.806596878479,57101.545787971096,39466.964726230552,56957.248605873741,56897.124779999845,56844.194340435861,56799.705393388562,56759.453488917177,56725.557148309723,56694.82212444282,56668.654241679062,56645.840457948267,56625.73826941735,56608.168768732226,56592.907689396983,56579.604863838329,56568.006957166166,null,39789.748436979942]
[null,null,50959.408455091274,50787.609548392109,50620.272950957835,35089.858311449847,50373.808195046928,50267.006800818868,50179.471825563189,50098.5260215218,50029.915424886669,49971.925663643946,49919.175514528171,49872.736543967316,49833.703788539024,49798.3884383896,49768.649196158527,49741.683562011152,49718.724947888237,49698.70908103008,49681.072255243518,49665.657504642433,49652.268067112454,49640.596720160043,49630.421198268428,null,50313.112454129056]
[null,null,44642.126415203929,44491.624893632761,44345.032502491988,44233.622285225028,44129.121228718803,44035.55967675041,43958.876144708258,43887.964944473657,43827.859793702381,43777.058845836851,43730.847971404852,43690.165898020954,43655.971913926754,43625.034499746267,43598.981940436395,43575.359153497375,43555.246648563247,43537.712087513959,43522.261645089369,43508.757813984281,43497.028224081987,43486.803738322029,43477.88964476408,null,44075.949753203968]
[null,null,39142.734030722291,39010.772551663504,38882.238643489356,38784.552873277025,38692.92513532591,38610.889281788412,38543.652271809413,38481.476509284876,38428.775616217303,38384.232756132311,38343.714525652082,38308.044012032864,38278.062330327084,38250.936046878975,38228.092860817429,38207.380127341901,38189.745249827203,38174.370743399923,38160.823616346483,38148.98330066738,38138.698660245798,38129.733712586705,38121.91773200329,null,38646.303769113627]
[null,null,34296.490769775723,34180.8673786004,34068.247192390671,33982.655850871291,33902.372499523655,33830.49346594794,33771.581038156815,33717.103227182932,33670.927206590393,33631.899176801642,33596.397489142772,33565.143324828801,33538.873660858015,33515.105869646337,33495.090887573358,33476.942587766236,33461.49107603907,33448.020079931353,33436.15021622739,33425.775844394273,33416.764540405842,33408.9095386474,33402.061250898121,null,33861.523302461464]
[null,null,30093.021148967557,29991.568869802581,29892.751714771759,29817.650676948353,29747.207067827163,29684.137720817827,29632.445757714198,29584.644892932098,29544.128328902436,29509.883678809241,29478.733172924716,29451.309602565656,29428.259618858701,29407.404871695257,29389.8429793471,29373.91898369461,29360.361250563528,29348.541295761501,29338.126234294232,29329.02337321503,29321.116518740502,29314.224247002592,29308.215303712834,null,29711.364457591535]
[null,null,26414.167707773478,26325.11790772403,26238.38108949404,26172.461107639261,26110.629186674698,26055.270028786312,26009.897376575544,25967.940138294925,25932.376699452259,25902.31843690102,25874.976061320227,25850.905005674987,25830.672868386977,25812.367601316862,25796.952639573614,25782.975342656147,25771.075034113219,25760.700061560827,25751.558234991753,25743.568193115396,25736.627946767334,25730.578251036506,25725.303897390972,null,26079.16831363169]
[null,null,23133.607264409751,23055.617182567723,22979.652817137176,29914.396625313802,29860.244043569688,22819.283601228264,22779.546096401282,22742.799821333239,29704.129980884511,29677.80486443171,22661.381604025639,29632.776827233749,22622.580734839987,22606.548927063377,22593.048457356763,22580.807098814483,29562.861498820974,22561.298340853056,22553.291901737957,22546.294199109627,22540.215910552117,22534.917568894925,22530.298274160399,null,25858.832695803998]
[null,null,20307.132692630359,26376.804239203419,26310.121234210812,26259.442150416435,26211.905955539551,26169.346001448666,26134.463642888131,26102.207044285173,26074.86597946065,26051.757277612043,26030.736541498238,26012.230786312331,25996.67638001384,25982.60334574377,25970.752369516347,25960.006665683191,25950.857744265777,25942.881496570426,25935.853287798342,25929.710567634,25924.374927114535,25919.723939231244,25915.669032011276,null,26187.718930963252]
[null,null,23177.728539499905,23117.726285430344,23059.282531466477,23014.865278453941,22973.202583767779,22935.901273098338,22905.328925892067,22877.057903722754,22853.095059428444,22832.841633755532,22814.418187935851,22798.198975812451,22784.56644838116,22772.232256895695,22761.845569328991,22752.427588374725,22744.409093821079,22737.418379201757,22731.258565253243,22725.874830282188,22721.198453418339,22717.122134548637,22713.568245518942,null,22952.004071289048]
[null,null,20330.753213116248,20278.121178115925,20226.856208959758,20187.894832401078,20151.349665241392,20118.630162963425,24810.724406088983,20067.01466410363,20045.995232764548,20028.229583366483,20012.06913305934,24716.753481669439,19985.884153421048,19975.064999907063,24684.865450259811,19957.692985756443,19950.659421892189,19944.527393317148,19939.124203914336,19934.401765868915,19930.299799457996,19926.724184495699,19923.606828078035,null,20132.75501628967]
[null,null,17831.2816520614,17785.120222124489,17740.15779036775,17705.986342232631,21812.700379396869,21784.003426828625,21760.483256037489,21738.733559641074,17581.531940523531,21704.716733443223,21690.54305586078,21678.065157560519,21667.57726890298,17519.321901059175,21650.097454473751,21642.851935539347,21636.683081047508,21631.304926707933,17487.799682013589,21622.424148261569,21618.82647936885,21615.69045205084,21612.956344774509,null,21796.391764600179]
[null,null,15632.09024830716,15591.622061395799,19180.523475108046,19150.566505576262,19122.467332604589,19097.309670853094,19076.690321126196,19057.623087285341,19041.461480077945,19027.801669651893,19015.376078971283,19004.437121461389,18995.242739071611,18986.92401214753,18979.918768421987,18973.566863489494,18968.158834384983,18963.443985747286,18959.289533450898,18955.658503309307,18952.504546913358,18949.755296297899,18947.358395585652,null,19108.170113632827]
[]
[null,"Pipeline & pumps O&M (2011$/[km-y])",6352.628054976064,6219.3430591622637,6089.5200112916782,5990.8544949100333,5898.3077702419805,5815.4491324537776,5747.5377642461572,5684.7384056233941,5631.5089453142473,5655.3581878292925,5605.6080835919429,5561.8102239687069,5524.9973678198658,5491.6904979709134,5498.4717867647114,5468.5282100824907,5443.0341676004709,5443.9355301858068,5421.4002138061878,5419.3020377030607,5399.9536357296583,5396.4930048512879,5391.7890340407967,null,{"$f":"FORECAST($C$54,OFFSET(C217:Y217,0,MATCH($C$54,$G$72:$Y$72,1)-1,1,2), OFFSET($G$72:$Y$72,0,MATCH($C$54,$G$72:$Y$72,1)-1,1,2))","v":5851.218811822002},{"$f":"FORECAST($C$55,OFFSET(AA217:AA239,MATCH($C$55,$B$73:$B$95,1)-1,0,2), OFFSET($B$73:$B$95,MATCH($C$55,$B$73:$B$95,1)-1,0,2))","v":{"$error":"#N/A"}}]
[null,null,6352.628054976064,6219.3430591622637,6089.5200112916782,5990.8544949100333,5898.3077702419805,5815.4491324537776,5747.5377642461572,5783.7608131933985,5717.9043344692845,5662.2423570956526,5611.6096670549232,5567.0348167154971,5579.8537028174505,5539.4565583769736,5505.4379104270993,5507.9415016230687,5477.4539199413384,5450.8741197625732,5449.6482126164356,5445.6992528688133,5439.8841620673566,5417.9414090443079,5411.6837996765844,null,5851.218811822002]
[null,null,6352.628054976064,6219.3430591622637,6089.5200112916782,5990.8544949100333,5898.3077702419805,5958.9886145475048,5873.2935936911044,5794.0492419870798,5726.8808159671271,5670.1099791143497,5618.4686195840441,5636.4451045300402,5590.3028883110328,5596.8898924369596,5555.6920777295873,5518.336546259171,5518.6821913368458,5514.971559849715,5483.373025892286,5477.1246475201997,5469.0644549628287,5459.6891661045938,5463.6774960606717,null,5932.7929830172125]
[null,null,6352.628054976064,6219.3430591622637,6089.5200112916782,5990.8544949100333,6081.0413916181997,5974.1874298108978,5886.6093698953155,5805.6237243799706,5736.9793576521997,5771.4027682286478,5706.7751536836895,5649.8797715932178,5663.445297922387,5612.2437976520205,5615.8978502640593,5611.4563157149669,5567.8537349627695,5560.8974590468179,5550.5343990510601,5537.9641650287185,5544.757438286445,5527.4815326609178,5525.8695974864941,null,6020.3157762947194]
[null,null,6352.628054976064,6219.3430591622637,6089.5200112916782,5990.8544949100333,6102.4257712329736,5992.7637595772658,5902.8842074782406,5684.7384056233941,5867.1350941092187,5793.038728780065,5545.5947286749215,5744.6666527493171,5753.5676339608117,5511.5937084348798,5690.0358701233072,5680.7553605843395,5429.7964745407126,5409.2444935430549,5421.4010475027262,5639.2798002627633,5638.002859184583,5389.7913132265221,5374.2358530435567,null,6040.1043278089801]
[null,null,6352.628054976064,6219.3430591622637,6089.5200112916782,5990.8544949100333,6123.8101508477457,5815.4491324537776,5747.5377642461572,5684.7384056233941,5631.5089453142473,5586.5193395421193,5545.5947286749215,5596.1432620190481,5555.0387761139145,5517.849003152126,5486.5312996053581,5458.134418151034,5477.8332649908634,5451.2054844105778,5427.7426221471078,5436.3985750880393,5414.8738422401702,5418.3255339283633,5418.5394324483605,null,5948.5671157086499]
[null,null,6352.628054976064,6219.3430591622637,6089.5200112916782,5990.8544949100333,5898.3077702419805,5815.4491324537776,5747.5377642461572,5684.7384056233941,5631.5089453142473,5714.3653529695212,5657.0502275603476,5606.5924475126303,5564.1818134207988,5525.810287337712,5558.1814181566106,5520.5034332630039,5488.4242946314171,5503.4091551295169,5473.2858245329408,5479.6401915306642,5452.6109484532226,5453.9455711390247,5451.9763424838302,null,5851.218811822002]
[null,null,6352.628054976064,6219.3430591622637,6089.5200112916782,5990.8544949100333,5898.3077702419805,5815.4491324537776,5747.5377642461572,5871.2124579396868,5794.2044272009452,5729.1171442545783,5669.9107635524497,5617.7880033986121,5668.6717795128998,5616.7947476083855,5573.1088260045844,5596.2993810299404,5554.6171358939455,5566.1859147273362,5528.0531354924178,5531.1783041245844,5529.4015936974147,5523.845085680302,5515.5064231968254,null,5851.218811822002]
[null,null,6352.628054976064,6219.3430591622637,6089.5200112916782,5990.8544949100333,5898.3077702419805,6090.711680163573,5988.696987460934,5894.3614227254693,5814.4015105710905,5746.8192937966478,5825.0920848110209,5752.8788857442432,5692.1824468734594,5729.9570709674772,5672.1258589437903,5690.286656910057,5636.6965216173048,5643.8310805610854,5642.7763184840505,5635.7629831581153,5624.6222983948555,5610.4058444450238,5594.083331020578,null,6007.6518284595168]
[null,null,6352.628054976064,6219.3430591622637,6089.5200112916782,6398.7842493262478,6254.0604630468179,6124.486825193334,6018.2876012480683,5920.0824947096708,6042.1764833171474,5946.4573581446612,5859.3868474566234,5919.3173245706212,5837.8160808465409,5868.1405731955556,5793.0364233933587,5804.1977683427031,5805.3943057671177,5797.7997761187207,5782.865800053205,5762.9744698769964,5740.0283063029956,5750.0139188610192,5749.8996509249055,null,6180.4231476373589]
[null,null,6352.628054976064,6219.3430591622637,6611.338675577349,6450.0549194814239,6298.7732567867988,6163.3282419775587,5747.5377642461572,5684.7384056233941,6093.7912519297406,5586.5193395421193,5545.5947286749215,5509.5664551793352,5479.2840701291652,5451.8857217504392,5428.8134283788822,5407.8929551145156,5467.9998314584254,5442.6158053170248,5420.2488676275598,5400.699955007688,5383.7195346897324,5368.917988584114,5390.4534724735895,null,6221.7992098944469]
[null,null,6352.628054976064,6219.3430591622637,6089.5200112916782,6508.013068352494,5898.3077702419805,5815.4491324537776,5747.5377642461572,5684.7384056233941,5631.5089453142473,5586.5193395421193,5545.5947286749215,5509.5664551793352,5479.2840701291652,5451.8857217504392,5428.8134283788822,5508.3771338921952,5477.8343589817969,5451.2064400311165,5427.7434558436471,5407.2365883390121,5440.3255112953957,5418.326641703834,5399.1471948042499,null,5851.218811822002]
[null,null,6352.628054976064,6219.3430591622637,6089.5200112916782,5990.8544949100333,5898.3077702419805,5815.4491324537776,5747.5377642461572,5684.7384056233941,5631.5089453142473,5586.5193395421193,5545.5947286749215,5509.5664551793352,5479.2840701291652,5600.8738239446711,5559.1780177988348,5521.3709396873237,5489.1818907395336,5461.1187108550685,5511.9126128816179,5480.6472816954383,5453.4898394762868,5479.9918422982701,5452.9809149231933,null,5851.218811822002]
[null,null,6352.628054976064,6219.3430591622637,6089.5200112916782,5990.8544949100333,5898.3077702419805,5815.4491324537776,5747.5377642461572,5684.7384056233941,5631.5089453142473,5586.5193395421193,5545.5947286749215,5730.4899326508212,5672.5921129167155,5620.2083712525236,5576.0957466932059,5536.0972529218025,5614.0036460837,5570.1527342979962,5531.5138436006146,5572.1594212001455,5533.3527958681889,5556.2116930189331,5519.5208446023316,null,5851.218811822002]
[null,null,6352.628054976064,6219.3430591622637,6089.5200112916782,5990.8544949100333,5898.3077702419805,5815.4491324537776,5747.5377642461572,5684.7384056233941,5631.5089453142473,5915.9731671986383,5832.8108861190649,5759.5983779543703,5698.0620025573216,5642.3862343409428,5762.1893254122642,5698.0854457964233,5643.5072286538143,5706.6107070205235,5650.5616611826808,5685.7955504416404,5632.5234335920668,5650.2418392887957,5657.6163129975293,null,5851.218811822002]
[null,null,6352.628054976064,6219.3430591622637,6089.5200112916782,5990.8544949100333,5898.3077702419805,5815.4491324537776,5747.5377642461572,6172.1490001548564,6056.7665110128373,5959.2450883014726,5870.5351250292288,5792.4386752199152,5974.3104552001814,5882.9291046694198,5805.9763884329896,5900.3544366359411,5820.1493790249779,5875.4487644346254,5797.858311271536,5825.3268040341482,5837.4468731302659,5837.5360976113498,5828.4804271006005,null,5851.218811822002]
[null,null,6352.628054976064,6219.3430591622637,6089.5200112916782,5990.8544949100333,5898.3077702419805,6539.9211090593926,6382.2521508298369,6236.4516801153623,6112.8695203743537,6008.4177259183307,6281.2124279975451,6149.9479345003692,6039.6178645350701,6183.750269545907,6069.1949076999172,6151.1336357772707,6039.155647958356,6083.2750870896034,6102.8287335945961,6103.8864932706001,6091.5171378771247,6068.8773234211685,6038.8006656274392,null,6262.9396859935287]
[null,null,6352.628054976064,6219.3430591622637,6089.5200112916782,5990.8544949100333,5898.3077702419805,6637.8690296456989,6468.0649308125303,6311.0427888695494,5631.5089453142473,5586.5193395421193,6380.667239669795,5509.5664551793352,6433.4196539807299,6559.6349710293534,6398.0940214979319,6462.5505952958656,5574.2883789225561,6500.9101865643506,6483.8980516502279,6450.82942351167,6407.0209341348082,6448.6371249199083,6461.447386295883,null,6318.6039556813957]
[null,null,6352.628054976064,6219.3430591622637,6089.5200112916782,5990.8544949100333,5898.3077702419805,5815.4491324537776,5747.5377642461572,5684.7384056233941,5631.5089453142473,5586.5193395421193,6018.8599734714635,5921.5607531048963,5839.7790808140317,5765.7861392175337,5703.4762936625903,5886.0625029659441,5807.6681880824008,5739.3221563601028,5838.2146199777726,5765.2415134484745,5822.9673812756228,5752.3164526144101,5783.0070224645087,null,5851.218811822002]
[null,null,6352.628054976064,6219.3430591622637,6089.5200112916782,5990.8544949100333,5898.3077702419805,5815.4491324537776,5747.5377642461572,5684.7384056233941,6335.0374374459552,6203.1413708810869,6083.1626534319694,5977.5385325348016,5888.7596378151984,6164.9860301016261,6052.7761981861704,5951.0315319415849,6101.5681666168393,5996.0490150799087,6083.8056770545318,5979.4412324026407,6026.355617098222,6049.9196382094215,6055.3536260812525,null,5851.218811822002]
[null,null,6352.628054976064,6219.3430591622637,6089.5200112916782,5990.8544949100333,5898.3077702419805,5815.4491324537776,5747.5377642461572,6600.4048486918273,6430.4125533605311,6286.7348548297459,6156.0390240538773,5509.5664551793352,6409.2578013705424,6261.6587666408905,5428.8134283788822,6333.0481696137094,6467.3358462836086,6315.5535890180745,6387.0474127165735,6422.9252087678742,6432.0350613950086,6420.2960744355651,6392.9031471779481,null,5851.218811822002]
[null,null,6352.628054976064,6219.3430591622637,6089.5200112916782,5990.8544949100333,5898.3077702419805,5815.4491324537776,5747.5377642461572,5684.7384056233941,6539.2523915218717,5586.5193395421193,5545.5947286749215,5509.5664551793352,5479.2840701291652,6832.0262675150925,5831.3544208935728,5758.2913320184953,5696.085219788928,5641.8524488784515,6760.0464694668053,5755.6886995595951,5693.5194233078664,5794.2573798921949,5727.3347292426888,null,5851.218811822002]
[null,null,6352.628054976064,6219.3430591622637,6089.5200112916782,5990.8544949100333,5898.3077702419805,5815.4491324537776,5747.5377642461572,5684.7384056233941,5631.5089453142473,5586.5193395421193,5545.5947286749215,6196.2250575076305,6080.1103471664237,5975.0541806672363,5886.5858299310794,5806.3684134604691,6086.0609672055334,5982.5032005743806,5891.2540779727706,6042.7970210554477,5944.0798351119902,6034.2170445329093,5936.8195164740328,null,5851.218811822002]
[]
[]
[]
[]
[]
[null,"CO₂ Storage","Values from FE/NETL CO₂ OnShore Saline Storage Cost Model (2017)"]
[null,"Capacity (million metric tonnes/year) ↓","NPV Injection CapEx 2008$","NPV Post-Injection CapEx 2008$","Injection FixedOpEx% of CapEx","Post-Injection FixedOpEx% of CapEx"]
[null,0.5,97624774.966992736,78481357.028610617,2.2872737345894539E-2,2.7748085045719149E-2]
[null,0.56999999999999995,101786356.99347538,82133493.314325452,2.3013836908320012E-2,2.7924081599160596E-2]
[null,0.65,104506439.36356887,86187075.937801316,2.3227730383590339E-2,2.6610745803564428E-2]
[null,0.74,111280771.2667349,90621285.77097027,2.3320765185481079E-2,2.8025919602951827E-2]
[null,0.85,115446954.04566029,95892454.843455911,2.347044362126726E-2,2.6485346250437112E-2]
[null,0.96,123968286.57717459,105169256.89884396,2.3516863324812093E-2,2.688606397640542E-2]
[null,1.1000000000000001,132054903.86834562,111547603.89317225,2.3826137412277192E-2,2.7556216019459318E-2]
[null,1.25,138218851.13802677,118218203.26593877,2.4134227659898911E-2,2.6980826820367825E-2]
[null,1.43,148790150.92586643,130180160.96168636,2.4291599894042143E-2,2.6712729064429397E-2]
[null,1.63,156646304.3596887,138679145.23706797,2.457573592851504E-2,2.5910618090346307E-2]
[null,1.86,167246152.86965409,152388054.34049419,2.5063805723438852E-2,2.5468563701597228E-2]
[null,2.12,182282789.12653089,167128279.54632628,2.5213229256799818E-2,2.5637446762237802E-2]
[null,2.42,196977943.92104512,183264677.08103243,2.545787765564848E-2,2.5582561484340596E-2]
[null,2.76,212538114.72414896,200751116.84884009,2.5919318917591937E-2,2.5364827101646871E-2]
[null,3.15,229599236.25573727,219932490.63017336,2.6259854407995158E-2,2.4987917217627179E-2]
[null,3.59,249413492.02992871,240760221.82423592,2.6709664343673226E-2,2.4983725815490316E-2]
[null,4.09,270616575.46090251,263565382.15915081,2.7663901320999398E-2,2.4452053667054705E-2]
[null,4.67,299338716.5723958,293170609.14679205,2.7900487029317689E-2,2.4736415053468845E-2]
[null,5.32,329809742.70631826,325007390.47518396,2.8137614580023135E-2,2.4797174173639924E-2]
[null,6.07,363698274.95211822,360099398.93435419,2.8854296868855989E-2,2.4694653464152099E-2]
[null,6.92,406462974.30423987,402513834.69650584,2.9340485774483328E-2,2.4877747063982492E-2]
[null,7.89,450852304.33460402,448744393.51919061,2.9512122136720723E-2,2.5013237004048072E-2]
[null,9,476324394.82961422,474812241.05296791,3.0054253945978136E-2,2.4788687720501128E-2]
[null,"Values in 2008$",{"$f":"FORECAST($C$55,OFFSET(C247:C269,MATCH($C$55,$B$73:$B$95,1)-1,0,2), OFFSET($B$73:$B$95,MATCH($C$55,$B$73:$B$95,1)-1,0,2))","v":{"$error":"#N/A"}},{"$f":"FORECAST($C$55,OFFSET(D247:D269,MATCH($C$55,$B$73:$B$95,1)-1,0,2), OFFSET($B$73:$B$95,MATCH($C$55,$B$73:$B$95,1)-1,0,2))","v":{"$error":"#N/A"}},{"$f":"FORECAST($C$55,OFFSET(E247:E269,MATCH($C$55,$B$73:$B$95,1)-1,0,2), OFFSET($B$73:$B$95,MATCH($C$55,$B$73:$B$95,1)-1,0,2))","v":{"$error":"#N/A"}},{"$f":"FORECAST($C$55,OFFSET(F247:F269,MATCH($C$55,$B$73:$B$95,1)-1,0,2), OFFSET($B$73:$B$95,MATCH($C$55,$B$73:$B$95,1)-1,0,2))","v":{"$error":"#N/A"}}]
[]
[null,"CEPCI inflator",{"$f":"VLOOKUP(2008,Tbl_PlantCostIndexes,2,FALSE)/VLOOKUP(2011,Tbl_PlantCostIndexes,2,FALSE)","v":0.98241420522451761}]
[null,"CPI inflator",{"$f":"VLOOKUP(2011,DeflatorTable,2,FALSE)/VLOOKUP(2008,DeflatorTable,2,FALSE)","v":1.0395933172707774}]
[]
[null,"Values in 2011$",{"$f":"+C270*$C$272*$C$273","v":{"$error":"#N/A"}},{"$f":"+D270*$C$272*$C$273","v":{"$error":"#N/A"}}]

{"sheet":"Results","index":8,"n_rows":121,"n_cols":9,"rows_kept":121,"cut":false,"hidden":false,"merged":[[16,5,16,7],[22,5,22,7],[29,1,29,2],[51,1,51,2],[92,1,92,2],[107,1,107,2],[85,1,85,2],[58,1,58,2],[76,1,76,2],[77,1,77,2],[78,1,78,2],[79,1,79,2],[89,1,89,2],[87,1,87,2],[82,1,82,2],[83,1,83,2],[84,1,84,2],[88,1,88,2]]}
[]
[null,"Table of Contents"]
[null,"Specific Item Cost Calculation"]
[null,"Energy Data"]
[null,"Production Process Energy Efficiency"]
[null,"Upstream Energy Usage"]
[null,"Emissions Summary"]
[null,"Production Process GHG Emissions Summary"]
[null,"Production Process GHG Emissions"]
[null,"Upstream GHG Emissions"]
[]
[null,"H2a Analysis Results"]
[]
[null,"COST RESULTS"]
[null,"Lang Factor",{"$f":"total_cap/(ProcEqpCap+IF(CO2_Capture_Efficiency>0,CCSEqpCap,0))","v":1.5276876644710033}]
[]
[null,"Specific Item Cost Calculation",null,null,null,{"$f":"IF(CO2_inUse = \"Carbon Sequestration\",\"Approximate Carbon Sequestration Costs*\",\"Carbon Sequestration is not included in this case\")","v":"Approximate Carbon Sequestration Costs*"}]
[null,"Cost Component","Cost Contribution ($/kg)","Percentage of H2 Cost",null,"Cost Component","Cost Contribution ($/ kg H2)","Cost Contribution ($/ tonne CO2 Sequestered)"]
[null,"Capital Costs",{"$f":"'Cash Flow Analysis'!D119","v":0.53432581889775166},{"$f":"'Cash Flow Analysis'!C119","v":7.9158817776594559E-2},null,"Capital Costs",{"$f":"IF(CO2_inUse = \"Carbon Sequestration\",ROUND((Det_CO2_seq)*CO2_cap_charge_rate/output_kgyear,2),\"\")","v":0},{"$f":"IF(CO2_inUse = \"Carbon Sequestration\",CO2_capptonneCO2,\"\")","v":0}]
[null,"Decommissioning Costs",{"$f":"'Cash Flow Analysis'!D120","v":1.046287032349252E-2},{"$f":"'Cash Flow Analysis'!C120","v":1.550043842287121E-3},null,"O&M Cost",{"$f":"IF(CO2_inUse = \"Carbon Sequestration\",ROUND(Det_CO2_OandMcost/output_kgyear,2),\"\")","v":0},{"$f":"IF(CO2_inUse = \"Carbon Sequestration\",CO2_OandMptonneCO2,\"\")","v":0}]
[null,"Fixed O&M",{"$f":"'Cash Flow Analysis'!D121","v":0.27051761030742794},{"$f":"'Cash Flow Analysis'!C121","v":4.0076398074604828E-2},null,"Energy Cost",{"$f":"IF(CO2_inUse = \"Carbon Sequestration\",ROUND(CO2_eCostpY/output_kgyear,2),\"\")","v":0},{"$f":"IF(CO2_inUse = \"Carbon Sequestration\",CO2_energyptonneCO2,\"\")","v":0}]
[null,"Feedstock Costs",{"$f":"'Cash Flow Analysis'!D122","v":5.915586597756497},{"$f":"'Cash Flow Analysis'!C122","v":0.87637696883047222},null,"Total",{"$f":"SUM(G19:G21)","v":0},{"$f":"SUM(H19:H21)","v":0}]
[null,"Other Raw Material Costs",{"$f":"'Cash Flow Analysis'!D123","v":0},{"$f":"'Cash Flow Analysis'!C123","v":0},null,"*Carbon sequestration costs presented in this table do not include carbon capture capital and operating costs."]
[null,"Byproduct Credits",{"$f":"'Cash Flow Analysis'!D124","v":0},{"$f":"'Cash Flow Analysis'!C124","v":0}]
[null,"Other Variable Costs (including utilities)",{"$f":"'Cash Flow Analysis'!D125","v":1.9155093650587731E-2},{"$f":"'Cash Flow Analysis'!C125","v":2.8377714760413533E-3}]
[null,"Total",{"$f":"SUM(C19:C25)","v":6.750047990935756}]
[]
[null,"ENERGY"]
[]
[null,"Energy Data"]
[null,"Feedstock","Energy Input (GJ/kg H2)","Energy Input (kWh/kg H2)","LHV (GJ/usage unit)","Usage (/kg H2)","Unit","Unit System Conversion Factor","Real levelized cost"]
[null,{"$f":"IF('Cash Flow Analysis'!$B$131=0,\"\",'Cash Flow Analysis'!$B$131)","v":"Ethanol"},{"$f":"IF($B$32=\"\",\"\",$E$32*$F$32*$H$32)","v":0.17747099999999999},{"$f":"IF($B32=\"\",\"\",$C32*1000*MJ_to_kWh)","v":49.297500000000007},{"$f":"IF($B$32<>\"\",VLOOKUP($B$32,MASTER_PROPERTY_TABLE,MATCH(\"H2A LHV (GJ/ H2A usage input unit)\",key_MPTable,0),FALSE),\"\")","v":8.1000000000000003E-2},{"$f":"IF('Cash Flow Analysis'!$B$133=\"\",\"\",'Cash Flow Analysis'!$B$133)","v":2.1909999999999998},{"$f":"IF($B$32<>\"\",VLOOKUP($B$32,MASTER_PROPERTY_TABLE,MATCH(\"H2A Usage Input Unit/ kg H2\",key_MPTable,0),FALSE),\"\")","v":"gallons"},{"$f":"IF($B32=\"\",\"\",IF(VLOOKUP($B32,MASTER_PROPERTY_TABLE,MATCH(\"Unit System\",key_MPTable,0),FALSE)=\"English\",mmBTU_to_GJ,1))","v":1},{"$f":"+'Cash Flow Analysis'!$B$233","v":2.7261106049604553}]
[null,{"$f":"IF('Cash Flow Analysis'!$C$131=0,\"\",'Cash Flow Analysis'!$C$131)","v":"Commercial Electricity"},{"$f":"IF($B$33=\"\",\"\",$E$33*$F$33*$H$33)","v":1.7639999999999997E-3},{"$f":"IF($B33=\"\",\"\",$C33*1000*MJ_to_kWh)","v":0.49},{"$f":"IF($B$33<>\"\",VLOOKUP($B$33,MASTER_PROPERTY_TABLE,MATCH(\"H2A LHV (GJ/ H2A usage input unit)\",key_MPTable,0),FALSE),\"\")","v":3.5999999999999995E-3},{"$f":"IF('Cash Flow Analysis'!$C$133=\"\",\"\",'Cash Flow Analysis'!$C$133)","v":0.49},{"$f":"IF($B$33<>\"\",VLOOKUP($B$33,MASTER_PROPERTY_TABLE,MATCH(\"H2A Usage Input Unit/ kg H2\",key_MPTable,0),FALSE),\"\")","v":"kWh"},{"$f":"IF($B$33=\"\",\"\",IF(VLOOKUP($B$33,MASTER_PROPERTY_TABLE,MATCH(\"Unit System\",key_MPTable,0),FALSE)=\"English\",mmBTU_to_GJ,1))","v":1},{"$f":"+'Cash Flow Analysis'!$C$233","v":0.1123967502969597}]
[null,{"$f":"IF('Cash Flow Analysis'!$D$131=0,\"\",'Cash Flow Analysis'!$D$131)","v":""},{"$f":"IF($B$34=\"\",\"\",$E$34*$F$34*$H$34)","v":""},{"$f":"IF($B34=\"\",\"\",$C34*1000*MJ_to_kWh)","v":""},{"$f":"IF($B$34<>\"\",VLOOKUP($B$34,MASTER_PROPERTY_TABLE,MATCH(\"H2A LHV (GJ/ H2A usage input unit)\",key_MPTable,0),FALSE),\"\")","v":""},{"$f":"IF('Cash Flow Analysis'!$D$133=\"\",\"\",'Cash Flow Analysis'!$D$133)","v":""},{"$f":"IF($B$34<>\"\",VLOOKUP($B$34,MASTER_PROPERTY_TABLE,MATCH(\"H2A Usage Input Unit/ kg H2\",key_MPTable,0),FALSE),\"\")","v":""},{"$f":"IF($B$34=\"\",\"\",IF(VLOOKUP($B$34,MASTER_PROPERTY_TABLE,MATCH(\"Unit System\",key_MPTable,0),FALSE)=\"English\",mmBTU_to_GJ,1))","v":""},{"$f":"+'Cash Flow Analysis'!$D$233","v":""}]
[null,{"$f":"IF('Cash Flow Analysis'!$E$131=0,\"\",'Cash Flow Analysis'!$E$131)","v":""},{"$f":"IF($B$35=\"\",\"\",$E$35*$F$35*$H$35)","v":""},{"$f":"IF($B35=\"\",\"\",$C35*1000*MJ_to_kWh)","v":""},{"$f":"IF($B$35<>\"\",VLOOKUP($B$35,MASTER_PROPERTY_TABLE,MATCH(\"H2A LHV (GJ/ H2A usage input unit)\",key_MPTable,0),FALSE),\"\")","v":""},{"$f":"IF('Cash Flow Analysis'!$E$133=\"\",\"\",'Cash Flow Analysis'!$E$133)","v":""},{"$f":"IF($B$35<>\"\",VLOOKUP($B$35,MASTER_PROPERTY_TABLE,MATCH(\"H2A Usage Input Unit/ kg H2\",key_MPTable,0),FALSE),\"\")","v":""},{"$f":"IF($B$35=\"\",\"\",IF(VLOOKUP($B$35,MASTER_PROPERTY_TABLE,MATCH(\"Unit System\",key_MPTable,0),FALSE)=\"English\",mmBTU_to_GJ,1))","v":""},{"$f":"+'Cash Flow Analysis'!$E$233","v":""}]
[null,"Utility"]
[null,{"$f":"IF('Cash Flow Analysis'!$F$131=0,\"\",'Cash Flow Analysis'!$F$131)","v":""},{"$f":"IF($B$37=\"\",\"\",$E$37*$F$37*$H$37)","v":""},{"$f":"IF($B37=\"\",\"\",$C37*1000*MJ_to_kWh)","v":""},{"$f":"IF($B37<>\"\",VLOOKUP($B37,MASTER_PROPERTY_TABLE,MATCH(\"H2A LHV (GJ/ H2A usage input unit)\",key_MPTable,0),FALSE),\"\")","v":""},{"$f":"IF('Cash Flow Analysis'!$F$133=\"\",\"\",'Cash Flow Analysis'!$F$133)","v":""},{"$f":"IF($B$37<>\"\",VLOOKUP($B$37,MASTER_PROPERTY_TABLE,MATCH(\"H2A Usage Input Unit/ kg H2\",key_MPTable,0),FALSE),\"\")","v":""},{"$f":"IF($B$37=\"\",\"\",IF(VLOOKUP($B$37,MASTER_PROPERTY_TABLE,MATCH(\"Unit System\",key_MPTable,0),FALSE)=\"English\",mmBTU_to_GJ,1))","v":""},{"$f":"+'Cash Flow Analysis'!$F$233","v":""}]
[null,{"$f":"IF('Cash Flow Analysis'!$G$131=0,\"\",'Cash Flow Analysis'!$G$131)","v":""},{"$f":"IF($B$38=\"\",\"\",$E$38*$F$38*$H$38)","v":""},{"$f":"IF($B38=\"\",\"\",$C38*1000*MJ_to_kWh)","v":""},{"$f":"IF($B38<>\"\",VLOOKUP($B38,MASTER_PROPERTY_TABLE,MATCH(\"H2A LHV (GJ/ H2A usage input unit)\",key_MPTable,0),FALSE),\"\")","v":""},{"$f":"IF('Cash Flow Analysis'!$G$133=\"\",\"\",'Cash Flow Analysis'!$G$133)","v":""},{"$f":"IF($B$38<>\"\",VLOOKUP($B$38,MASTER_PROPERTY_TABLE,MATCH(\"H2A Usage Input Unit/ kg H2\",key_MPTable,0),FALSE),\"\")","v":""},{"$f":"IF($B$38=\"\",\"\",IF(VLOOKUP($B$38,MASTER_PROPERTY_TABLE,MATCH(\"Unit System\",key_MPTable,0),FALSE)=\"English\",mmBTU_to_GJ,1))","v":""},{"$f":"+'Cash Flow Analysis'!$G$233","v":""}]
[null,{"$f":"IF('Cash Flow Analysis'!$H$131=0,\"\",'Cash Flow Analysis'!$H$131)","v":""},{"$f":"IF($B$39=\"\",\"\",$E$39*$F$39*$H$39)","v":""},{"$f":"IF($B39=\"\",\"\",$C39*1000*MJ_to_kWh)","v":""},{"$f":"IF($B39<>\"\",VLOOKUP($B39,MASTER_PROPERTY_TABLE,MATCH(\"H2A LHV (GJ/ H2A usage input unit)\",key_MPTable,0),FALSE),\"\")","v":""},{"$f":"IF('Cash Flow Analysis'!$H$133=\"\",\"\",'Cash Flow Analysis'!$H$133)","v":""},{"$f":"IF($B$39<>\"\",VLOOKUP($B$39,MASTER_PROPERTY_TABLE,MATCH(\"H2A Usage Input Unit/ kg H2\",key_MPTable,0),FALSE),\"\")","v":""},{"$f":"IF($B$39=\"\",\"\",IF(VLOOKUP($B$39,MASTER_PROPERTY_TABLE,MATCH(\"Unit System\",key_MPTable,0),FALSE)=\"English\",mmBTU_to_GJ,1))","v":""},{"$f":"+'Cash Flow Analysis'!$H$233","v":""}]
[null,{"$f":"IF('Cash Flow Analysis'!$I$131=0,\"\",'Cash Flow Analysis'!$I$131)","v":""},{"$f":"IF($B$40=\"\",\"\",$E$40*$F$40*$H$40)","v":""},{"$f":"IF($B40=\"\",\"\",$C40*1000*MJ_to_kWh)","v":""},{"$f":"IF($B40<>\"\",VLOOKUP($B40,MASTER_PROPERTY_TABLE,MATCH(\"H2A LHV (GJ/ H2A usage input unit)\",key_MPTable,0),FALSE),\"\")","v":""},{"$f":"IF('Cash Flow Analysis'!$I$133=\"\",\"\",'Cash Flow Analysis'!$I$133)","v":""},{"$f":"IF($B$40<>\"\",VLOOKUP($B$40,MASTER_PROPERTY_TABLE,MATCH(\"H2A Usage Input Unit/ kg H2\",key_MPTable,0),FALSE),\"\")","v":""},{"$f":"IF($B$40=\"\",\"\",IF(VLOOKUP($B$40,MASTER_PROPERTY_TABLE,MATCH(\"Unit System\",key_MPTable,0),FALSE)=\"English\",mmBTU_to_GJ,1))","v":""},{"$f":"+'Cash Flow Analysis'!$I$233","v":""}]
[null,"Carbon Sequestration"]
[null,{"$f":"IF('Cash Flow Analysis'!$J$131=0,\"\",'Cash Flow Analysis'!$J$131)","v":""},{"$f":"IF($B$42=\"\",\"\",$E$42*$F$42*$H$42)","v":""},{"$f":"IF($B42=\"\",\"\",$C42*1000*MJ_to_kWh)","v":""},{"$f":"IF($B42<>\"\",VLOOKUP($B42,MASTER_PROPERTY_TABLE,MATCH(\"H2A LHV (GJ/ H2A usage input unit)\",key_MPTable,0),FALSE),\"\")","v":""},{"$f":"CO2_CashFlow_eUse","v":0},{"$f":"IF($B$42<>\"\",VLOOKUP($B$42,MASTER_PROPERTY_TABLE,MATCH(\"H2A Usage Input Unit/ kg H2\",key_MPTable,0),FALSE),\"\")","v":""},{"$f":"IF($B42=\"\",\"\",IF(VLOOKUP($B42,MASTER_PROPERTY_TABLE,MATCH(\"Unit System\",key_MPTable,0),FALSE)=\"English\",mmBTU_to_GJ,1))","v":""}]
[null,null,"Energy Output (GJ/kg H2)","Energy Output (kWh/kg H2)","LHV (GJ/usage unit)","Production (/kg H2)","Unit","Unit System Conversion Factor"]
[null,"Hydrogen (1 kg)",{"$f":"kgH2_to_GJ","v":0.12021163829516093},{"$f":"IF($B44=\"\",\"\",$C44*1000*MJ_to_kWh)","v":33.392121748655818},{"$f":"kgH2_to_GJ","v":0.12021163829516093},1,"kg",1]
[]
[null,"Byproducts"]
[null,{"$f":"IF('Cash Flow Analysis'!$K$131=0,\"\",'Cash Flow Analysis'!$K$131)","v":""},{"$f":"IF($B$47=\"\",\"\",$E$47*$F$47*$H$47)","v":""},{"$f":"IF($B47=\"\",\"\",$C47*1000*MJ_to_kWh)","v":""},{"$f":"IF($B47<>\"\",VLOOKUP($B47,MASTER_PROPERTY_TABLE,MATCH(\"H2A LHV (GJ/ H2A usage input unit)\",key_MPTable,0),FALSE),\"\")","v":""},{"$f":"IF('Cash Flow Analysis'!$K$133=\"\",\"\",'Cash Flow Analysis'!$K$133)","v":""},{"$f":"IF($B$47<>\"\",VLOOKUP($B$47,MASTER_PROPERTY_TABLE,MATCH(\"H2A Usage Input Unit/ kg H2\",key_MPTable,0),FALSE),\"\")","v":""},{"$f":"IF($B$47=\"\",\"\",IF(VLOOKUP($B$47,MASTER_PROPERTY_TABLE,MATCH(\"Unit System\",key_MPTable,0),FALSE)=\"English\",mmBTU_to_GJ,1))","v":""},{"$f":"+'Cash Flow Analysis'!$K$233","v":""}]
[null,{"$f":"IF('Cash Flow Analysis'!$L$131=0,\"\",'Cash Flow Analysis'!$L$131)","v":""},{"$f":"IF($B$48=\"\",\"\",$E$48*$F$48*$H$48)","v":""},{"$f":"IF($B48=\"\",\"\",$C48*1000*MJ_to_kWh)","v":""},{"$f":"IF($B48<>\"\",VLOOKUP($B48,MASTER_PROPERTY_TABLE,MATCH(\"H2A LHV (GJ/ H2A usage input unit)\",key_MPTable,0),FALSE),\"\")","v":""},{"$f":"IF('Cash Flow Analysis'!$L$133=\"\",\"\",'Cash Flow Analysis'!$L$133)","v":""},{"$f":"IF($B$48<>\"\",VLOOKUP($B$48,MASTER_PROPERTY_TABLE,MATCH(\"H2A Usage Input Unit/ kg H2\",key_MPTable,0),FALSE),\"\")","v":""},{"$f":"IF($B$48=\"\",\"\",IF(VLOOKUP($B$48,MASTER_PROPERTY_TABLE,MATCH(\"Unit System\",key_MPTable,0),FALSE)=\"English\",mmBTU_to_GJ,1))","v":""},{"$f":"+'Cash Flow Analysis'!$L$233","v":""}]
[null,{"$f":"IF('Cash Flow Analysis'!$M$131=0,\"\",'Cash Flow Analysis'!$M$131)","v":""},{"$f":"IF($B$49=\"\",\"\",$E$49*$F$49*$H$49)","v":""},{"$f":"IF($B49=\"\",\"\",$C49*1000*MJ_to_kWh)","v":""},{"$f":"IF($B49<>\"\",VLOOKUP($B49,MASTER_PROPERTY_TABLE,MATCH(\"H2A LHV (GJ/ H2A usage input unit)\",key_MPTable,0),FALSE),\"\")","v":""},{"$f":"IF('Cash Flow Analysis'!$M$133=\"\",\"\",'Cash Flow Analysis'!$M$133)","v":""},{"$f":"IF($B$49<>\"\",VLOOKUP($B$49,MASTER_PROPERTY_TABLE,MATCH(\"H2A Usage Input Unit/ kg H2\",key_MPTable,0),FALSE),\"\")","v":""},{"$f":"IF($B$49=\"\",\"\",IF(VLOOKUP($B$49,MASTER_PROPERTY_TABLE,MATCH(\"Unit System\",key_MPTable,0),FALSE)=\"English\",mmBTU_to_GJ,1))","v":""},{"$f":"+'Cash Flow Analysis'!$M$233","v":""}]
[null,{"$f":"IF('Cash Flow Analysis'!$N$131=0,\"\",'Cash Flow Analysis'!$N$131)","v":""},{"$f":"IF($B$50=\"\",\"\",$E$50*$F$50*$H$50)","v":""},{"$f":"IF($B50=\"\",\"\",$C50*1000*MJ_to_kWh)","v":""},{"$f":"IF($B50<>\"\",VLOOKUP($B50,MASTER_PROPERTY_TABLE,MATCH(\"H2A LHV (GJ/ H2A usage input unit)\",key_MPTable,0),FALSE),\"\")","v":""},{"$f":"IF('Cash Flow Analysis'!$N$133=\"\",\"\",'Cash Flow Analysis'!$N$133)","v":""},{"$f":"IF($B$50<>\"\",VLOOKUP($B$50,MASTER_PROPERTY_TABLE,MATCH(\"H2A Usage Input Unit/ kg H2\",key_MPTable,0),FALSE),\"\")","v":""},{"$f":"IF($B$50=\"\",\"\",IF(VLOOKUP($B$50,MASTER_PROPERTY_TABLE,MATCH(\"Unit System\",key_MPTable,0),FALSE)=\"English\",mmBTU_to_GJ,1))","v":""},{"$f":"+'Cash Flow Analysis'!$N$233","v":""}]
[]
[null,"Production Process Energy Efficiency",null,{"$f":"(C56+C57)/(C53+C54+C55)","v":0.67069287971189195}]
[null,"Feedstock energy input (GJ)/kg H2",{"$f":"SUM(C32:C35)","v":0.17923499999999998}]
[null,"Utility energy input (GJ/kg H2)",{"$f":"SUM(C37:C40)","v":0}]
[null,"Carbon sequestration energy input (GJ/kg H2)",{"$f":"IF(C42=\"\",0,C42)","v":0}]
[null,"Hydrogen energy output (GJ/kg)",{"$f":"C44","v":0.12021163829516093}]
[null,"Byproduct energy output (GJ/kg H2)",{"$f":"SUM(C47:C50)","v":0}]
[]
[null,"Upstream Energy Usage (GJ/kg H2)"]
[null,"Feedstock","Total Energy","Fossil Fuels","Petroleum"]
[null,{"$f":"B32","v":"Ethanol"},{"$f":"IF($B61=\"\",\"\",$C32/1000000*VLOOKUP($B61,Tbl_Emissions,3,FALSE))","v":0.32181171372},{"$f":"IF($B61=\"\",\"\",$C32/1000000*VLOOKUP($B61,Tbl_Emissions,4,FALSE))","v":9.7112131199999993E-2},{"$f":"IF($B61=\"\",\"\",$C32/1000000*VLOOKUP($B61,Tbl_Emissions,5,FALSE))","v":8.6571631591199991E-3}]
[null,{"$f":"B33","v":"Commercial Electricity"},{"$f":"IF($B62=\"\",\"\",$C33/1000000*VLOOKUP($B62,Tbl_Emissions,3,FALSE))","v":3.2404679999999994E-3},{"$f":"IF($B62=\"\",\"\",$C33/1000000*VLOOKUP($B62,Tbl_Emissions,4,FALSE))","v":2.5232255999999994E-3},{"$f":"IF($B62=\"\",\"\",$C33/1000000*VLOOKUP($B62,Tbl_Emissions,5,FALSE))","v":4.4823239999999991E-5}]
[null,{"$f":"B34","v":""},{"$f":"IF($B63=\"\",\"\",$C34/1000000*VLOOKUP($B63,Tbl_Emissions,3,FALSE))","v":""},{"$f":"IF($B63=\"\",\"\",$C34/1000000*VLOOKUP($B63,Tbl_Emissions,4,FALSE))","v":""},{"$f":"IF($B63=\"\",\"\",$C34/1000000*VLOOKUP($B63,Tbl_Emissions,5,FALSE))","v":""}]
[null,{"$f":"B35","v":""},{"$f":"IF($B64=\"\",\"\",$C35/1000000*VLOOKUP($B64,Tbl_Emissions,3,FALSE))","v":""},{"$f":"IF($B64=\"\",\"\",$C35/1000000*VLOOKUP($B64,Tbl_Emissions,4,FALSE))","v":""},{"$f":"IF($B64=\"\",\"\",$C35/1000000*VLOOKUP($B64,Tbl_Emissions,5,FALSE))","v":""}]
[null,"Utility"]
[null,{"$f":"B37","v":""},{"$f":"IF($B66=\"\",\"\",$C37/1000000*VLOOKUP($B66,Tbl_Emissions,3,FALSE))","v":""},{"$f":"IF($B66=\"\",\"\",$C37/1000000*VLOOKUP($B66,Tbl_Emissions,4,FALSE))","v":""},{"$f":"IF($B66=\"\",\"\",$C37/1000000*VLOOKUP($B66,Tbl_Emissions,5,FALSE))","v":""}]
[null,{"$f":"B38","v":""},{"$f":"IF($B67=\"\",\"\",$C38/1000000*VLOOKUP($B67,Tbl_Emissions,3,FALSE))","v":""},{"$f":"IF($B67=\"\",\"\",$C38/1000000*VLOOKUP($B67,Tbl_Emissions,4,FALSE))","v":""},{"$f":"IF($B67=\"\",\"\",$C38/1000000*VLOOKUP($B67,Tbl_Emissions,5,FALSE))","v":""}]
[null,{"$f":"B39","v":""},{"$f":"IF($B68=\"\",\"\",$C39/1000000*VLOOKUP($B68,Tbl_Emissions,3,FALSE))","v":""},{"$f":"IF($B68=\"\",\"\",$C39/1000000*VLOOKUP($B68,Tbl_Emissions,4,FALSE))","v":""},{"$f":"IF($B68=\"\",\"\",$C39/1000000*VLOOKUP($B68,Tbl_Emissions,5,FALSE))","v":""}]
[null,{"$f":"B40","v":""},{"$f":"IF($B69=\"\",\"\",$C40/1000000*VLOOKUP($B69,Tbl_Emissions,3,FALSE))","v":""},{"$f":"IF($B69=\"\",\"\",$C40/1000000*VLOOKUP($B69,Tbl_Emissions,4,FALSE))","v":""},{"$f":"IF($B69=\"\",\"\",$C40/1000000*VLOOKUP($B69,Tbl_Emissions,5,FALSE))","v":""}]
[null,"Carbon Sequestration"]
[null,{"$f":"B42","v":""},{"$f":"IF($B71=\"\",\"\",$C42/1000000*VLOOKUP($B71,Tbl_Emissions,3,FALSE))","v":""},{"$f":"IF($B71=\"\",\"\",$C42/1000000*VLOOKUP($B71,Tbl_Emissions,4,FALSE))","v":""},{"$f":"IF($B71=\"\",\"\",$C42/1000000*VLOOKUP($B71,Tbl_Emissions,5,FALSE))","v":""}]
[]
[]
[null,"EMISSIONS"]
[]
[null,"Emissions Summary",null,"CO2","CH4","N2O","Total GHG (CO2 eq)"]
[null,"Total upstream emissions (kg/kg H2) ",null,{"$f":"C121","v":6.1162697987999994},{"$f":"D121","v":1.7159714737199998E-2},{"$f":"E121","v":1.4167664116199997E-2},{"$f":"F121","v":10.767226573857599}]
[null,"Total process emissions (kg/kg H2)",null,{"$f":"D89","v":12.580919189999999},{"$f":"E89","v":0},{"$f":"F89","v":0},{"$f":"G89","v":12.580919189999999}]
[]
[null,"Total well to pump emissions (kg/kg H2)",null,{"$f":"SUM(D77:D79)","v":18.697188988800001},{"$f":"SUM(E77:E79)","v":1.7159714737199998E-2},{"$f":"SUM(F77:F79)","v":1.4167664116199997E-2},{"$f":"SUM(G77:G79)","v":23.348145763857598}]
[]
[null,"Production Process GHG Emissions Summary",null,"CO2","CH4","N2O","Total GHG (CO2 eq)"]
[null,"Total Process Pollutants Produced (kg /kg H2)",null,{"$f":"SUM(C95:C105)","v":12.580919189999999},{"$f":"SUM(D95:D105)","v":0},{"$f":"SUM(E95:E105)","v":0},{"$f":"SUM(F95:F105)","v":12.580919189999999}]
[null,"Total Process Pollutants Produced (metric tons/year)",null,{"$f":"ROUND(D83*output_kgyear/1000,-2)","v":5900},{"$f":"ROUND(E83*output_kgyear/1000,-2)","v":0},{"$f":"ROUND(F83*output_kgyear/1000,-2)","v":0},{"$f":"ROUND(G83*output_kgyear/1000,-2)","v":5900}]
[null,"Total Feedstock Pollutants Produced (kg /kg H2)",null,{"$f":"SUM(C95:C98)","v":12.580919189999999},{"$f":"SUM(D95:D98)","v":0},{"$f":"SUM(E95:E98)","v":0},{"$f":"SUM(F95:F98)","v":12.580919189999999}]
[null,"Total Feedstock Pollutants Produced (metric tons /year)",null,{"$f":"ROUND(D85*output_kgyear/1000,-2)","v":5900},{"$f":"ROUND(E85*output_kgyear/1000,-2)","v":0},{"$f":"ROUND(F85*output_kgyear/1000,-2)","v":0},{"$f":"ROUND(G85*output_kgyear/1000,-2)","v":5900}]
[null,"CO2 Captured (kg/kg H2)*",null,{"$f":"IF(CO2_CashFlow_eUse>0,D85*CO2_Capture_Efficiency,0)","v":0}]
[null,"CO2 Captured (metric tons/year)*",null,{"$f":"ROUND(D87*output_kgyear/1000,-2)","v":0}]
[null,"Total Process Emissions (kg/kg H2)",null,{"$f":"D83-D87","v":12.580919189999999},{"$f":"E83-E87","v":0},{"$f":"F83-F87","v":0},{"$f":"D89*GHG_CO2_factor + E89*GHG_CH4_factor + F89*GHG_N2O_factor","v":12.580919189999999}]
[null,"Total Process Emissions (metric tons/year)",null,{"$f":"ROUND(D89*output_kgyear/1000,-2)","v":5900},{"$f":"ROUND(E89*output_kgyear/1000,-2)","v":0},{"$f":"ROUND(F89*output_kgyear/1000,-2)","v":0},{"$f":"ROUND(G89*output_kgyear/1000,-2)","v":5900}]
[null,"*Carbon sequestration values are only calculated if the detailed Carbon Sequestration sheet is used."]
[]
[null,"Production Process GHG Emissions (/kg H2)"]
[null,"Feedstock","CO2","CH4","N2O","Total GHG (CO2 eq)"]
[null,{"$f":"B32","v":"Ethanol"},{"$f":"IF($B95=\"\",\"\",VLOOKUP($B95,MASTER_PROPERTY_TABLE,MATCH(\"CO2 Emissions Factor (kg CO2 produced/GJ feed)\",key_MPTable,0),FALSE)*$E32*$F32)","v":12.580919189999999},{"$f":"IF($B95=\"\",\"\",VLOOKUP($B95,MASTER_PROPERTY_TABLE,MATCH(\"CH4 Emissions Factor (kg CH4 produced/GJ or mmBtu feed)\",key_MPTable,0),FALSE)*$E32*$F32)","v":0},{"$f":"IF($B95=\"\",\"\",VLOOKUP($B95,MASTER_PROPERTY_TABLE,MATCH(\"N2O Emissions Factor (kg N2O produced/GJ or mmBtu feed)\",key_MPTable,0),FALSE)*$E32*$F32)","v":0},{"$f":"IF($B95=\"\",\"\",$C95*GHG_CO2_factor+$D95*GHG_CH4_factor+$E95*GHG_N2O_factor)","v":12.580919189999999}]
[null,{"$f":"B33","v":"Commercial Electricity"},{"$f":"IF($B96=\"\",\"\",VLOOKUP($B96,MASTER_PROPERTY_TABLE,MATCH(\"CO2 Emissions Factor (kg CO2 produced/GJ feed)\",key_MPTable,0),FALSE)*$E33*$F33)","v":0},{"$f":"IF($B96=\"\",\"\",VLOOKUP($B96,MASTER_PROPERTY_TABLE,MATCH(\"CH4 Emissions Factor (kg CH4 produced/GJ or mmBtu feed)\",key_MPTable,0),FALSE)*$E33*$F33)","v":0},{"$f":"IF($B96=\"\",\"\",VLOOKUP($B96,MASTER_PROPERTY_TABLE,MATCH(\"N2O Emissions Factor (kg N2O produced/GJ or mmBtu feed)\",key_MPTable,0),FALSE)*$E33*$F33)","v":0},{"$f":"IF($B96=\"\",\"\",$C96*GHG_CO2_factor+$D96*GHG_CH4_factor+$E96*GHG_N2O_factor)","v":0}]
[null,{"$f":"B34","v":""},{"$f":"IF($B97=\"\",\"\",VLOOKUP($B97,MASTER_PROPERTY_TABLE,MATCH(\"CO2 Emissions Factor (kg CO2 produced/GJ feed)\",key_MPTable,0),FALSE)*$E34*$F34)","v":""},{"$f":"IF($B97=\"\",\"\",VLOOKUP($B97,MASTER_PROPERTY_TABLE,MATCH(\"CH4 Emissions Factor (kg CH4 produced/GJ or mmBtu feed)\",key_MPTable,0),FALSE)*$E34*$F34)","v":""},{"$f":"IF($B97=\"\",\"\",VLOOKUP($B97,MASTER_PROPERTY_TABLE,MATCH(\"N2O Emissions Factor (kg N2O produced/GJ or mmBtu feed)\",key_MPTable,0),FALSE)*$E34*$F34)","v":""},{"$f":"IF($B97=\"\",\"\",$C97*GHG_CO2_factor+$D97*GHG_CH4_factor+$E97*GHG_N2O_factor)","v":""}]
[null,{"$f":"B35","v":""},{"$f":"IF($B98=\"\",\"\",VLOOKUP($B98,MASTER_PROPERTY_TABLE,MATCH(\"CO2 Emissions Factor (kg CO2 produced/GJ feed)\",key_MPTable,0),FALSE)*$E35*$F35)","v":""},{"$f":"IF($B98=\"\",\"\",VLOOKUP($B98,MASTER_PROPERTY_TABLE,MATCH(\"CH4 Emissions Factor (kg CH4 produced/GJ or mmBtu feed)\",key_MPTable,0),FALSE)*$E35*$F35)","v":""},{"$f":"IF($B98=\"\",\"\",VLOOKUP($B98,MASTER_PROPERTY_TABLE,MATCH(\"N2O Emissions Factor (kg N2O produced/GJ or mmBtu feed)\",key_MPTable,0),FALSE)*$E35*$F35)","v":""},{"$f":"IF($B98=\"\",\"\",$C98*GHG_CO2_factor+$D98*GHG_CH4_factor+$E98*GHG_N2O_factor)","v":""}]
[null,"Utility"]
[null,{"$f":"B37","v":""},{"$f":"IF($B100=\"\",\"\",VLOOKUP($B100,MASTER_PROPERTY_TABLE,MATCH(\"CO2 Emissions Factor (kg CO2 produced/GJ feed)\",key_MPTable,0),FALSE)*$E37*$F37)","v":""},{"$f":"IF($B100=\"\",\"\",VLOOKUP($B100,MASTER_PROPERTY_TABLE,MATCH(\"CH4 Emissions Factor (kg CH4 produced/GJ or mmBtu feed)\",key_MPTable,0),FALSE)*$E37*$F37)","v":""},{"$f":"IF($B100=\"\",\"\",VLOOKUP($B100,MASTER_PROPERTY_TABLE,MATCH(\"N2O Emissions Factor (kg N2O produced/GJ or mmBtu feed)\",key_MPTable,0),FALSE)*$E37*$F37)","v":""},{"$f":"IF($B100=\"\",\"\",$C100*GHG_CO2_factor+$D100*GHG_CH4_factor+$E100*GHG_N2O_factor)","v":""}]
[null,{"$f":"B38","v":""},{"$f":"IF($B101=\"\",\"\",VLOOKUP($B101,MASTER_PROPERTY_TABLE,MATCH(\"CO2 Emissions Factor (kg CO2 produced/GJ feed)\",key_MPTable,0),FALSE)*$E38*$F38)","v":""},{"$f":"IF($B101=\"\",\"\",VLOOKUP($B101,MASTER_PROPERTY_TABLE,MATCH(\"CH4 Emissions Factor (kg CH4 produced/GJ or mmBtu feed)\",key_MPTable,0),FALSE)*$E38*$F38)","v":""},{"$f":"IF($B101=\"\",\"\",VLOOKUP($B101,MASTER_PROPERTY_TABLE,MATCH(\"N2O Emissions Factor (kg N2O produced/GJ or mmBtu feed)\",key_MPTable,0),FALSE)*$E38*$F38)","v":""},{"$f":"IF($B101=\"\",\"\",$C101*GHG_CO2_factor+$D101*GHG_CH4_factor+$E101*GHG_N2O_factor)","v":""}]
[null,{"$f":"B39","v":""},{"$f":"IF($B102=\"\",\"\",VLOOKUP($B102,MASTER_PROPERTY_TABLE,MATCH(\"CO2 Emissions Factor (kg CO2 produced/GJ feed)\",key_MPTable,0),FALSE)*$E39*$F39)","v":""},{"$f":"IF($B102=\"\",\"\",VLOOKUP($B102,MASTER_PROPERTY_TABLE,MATCH(\"CH4 Emissions Factor (kg CH4 produced/GJ or mmBtu feed)\",key_MPTable,0),FALSE)*$E39*$F39)","v":""},{"$f":"IF($B102=\"\",\"\",VLOOKUP($B102,MASTER_PROPERTY_TABLE,MATCH(\"N2O Emissions Factor (kg N2O produced/GJ or mmBtu feed)\",key_MPTable,0),FALSE)*$E39*$F39)","v":""},{"$f":"IF($B102=\"\",\"\",$C102*GHG_CO2_factor+$D102*GHG_CH4_factor+$E102*GHG_N2O_factor)","v":""}]
[null,{"$f":"B40","v":""},{"$f":"IF($B103=\"\",\"\",VLOOKUP($B103,MASTER_PROPERTY_TABLE,MATCH(\"CO2 Emissions Factor (kg CO2 produced/GJ feed)\",key_MPTable,0),FALSE)*$E40*$F40)","v":""},{"$f":"IF($B103=\"\",\"\",VLOOKUP($B103,MASTER_PROPERTY_TABLE,MATCH(\"CH4 Emissions Factor (kg CH4 produced/GJ or mmBtu feed)\",key_MPTable,0),FALSE)*$E40*$F40)","v":""},{"$f":"IF($B103=\"\",\"\",VLOOKUP($B103,MASTER_PROPERTY_TABLE,MATCH(\"N2O Emissions Factor (kg N2O produced/GJ or mmBtu feed)\",key_MPTable,0),FALSE)*$E40*$F40)","v":""},{"$f":"IF($B103=\"\",\"\",$C103*GHG_CO2_factor+$D103*GHG_CH4_factor+$E103*GHG_N2O_factor)","v":""}]
[null,"Carbon Sequestration"]
[null,{"$f":"B42","v":""},{"$f":"IF($B105=\"\",\"\",VLOOKUP($B105,MASTER_PROPERTY_TABLE,MATCH(\"CO2 Emissions Factor (kg CO2 produced/GJ feed)\",key_MPTable,0),FALSE)*$E42*$F42)","v":""},{"$f":"IF($B105=\"\",\"\",VLOOKUP($B105,MASTER_PROPERTY_TABLE,MATCH(\"CH4 Emissions Factor (kg CH4 produced/GJ or mmBtu feed)\",key_MPTable,0),FALSE)*$E42*$F42)","v":""},{"$f":"IF($B105=\"\",\"\",VLOOKUP($B105,MASTER_PROPERTY_TABLE,MATCH(\"N2O Emissions Factor (kg N2O produced/GJ or mmBtu feed)\",key_MPTable,0),FALSE)*$E42*$F42)","v":""},{"$f":"IF($B105=\"\",\"\",$C105*GHG_CO2_factor+$D105*GHG_CH4_factor+$E105*GHG_N2O_factor)","v":""}]
[]
[]
[null,"Upstream GHG Emissions (kg/kg H2) based on GREET.NET 2017"]
[null,"Feedstock","CO2","CH4","N2O","Total GHG (CO2 eq)"]
[null,{"$f":"B32","v":"Ethanol"},{"$f":"IF($B110=\"\",\"\",$C32*VLOOKUP($B110,Tbl_Emissions,6,FALSE))","v":5.8499410787999997},{"$f":"IF($B110=\"\",\"\",$C32*VLOOKUP($B110,Tbl_Emissions,7,FALSE))","v":1.67730681636E-2},{"$f":"IF($B110=\"\",\"\",$C32*VLOOKUP($B110,Tbl_Emissions,8,FALSE))","v":1.4163712050599998E-2},{"$f":"IF($B110=\"\",\"\",$C110*GHG_CO2_factor+$D110*GHG_CH4_factor+$E110*GHG_N2O_factor)","v":10.490053973968799}]
[null,{"$f":"B33","v":"Commercial Electricity"},{"$f":"IF($B111=\"\",\"\",$C33*VLOOKUP($B111,Tbl_Emissions,6,FALSE))","v":0.26632871999999996},{"$f":"IF($B111=\"\",\"\",$C33*VLOOKUP($B111,Tbl_Emissions,7,FALSE))","v":3.8664657359999989E-4},{"$f":"IF($B111=\"\",\"\",$C33*VLOOKUP($B111,Tbl_Emissions,8,FALSE))","v":3.9520655999999995E-6},{"$f":"IF($B111=\"\",\"\",$C111*GHG_CO2_factor+$D111*GHG_CH4_factor+$E111*GHG_N2O_factor)","v":0.27717259988879994}]
[null,{"$f":"B34","v":""},{"$f":"IF($B112=\"\",\"\",$C34*VLOOKUP($B112,Tbl_Emissions,6,FALSE))","v":""},{"$f":"IF($B112=\"\",\"\",$C34*VLOOKUP($B112,Tbl_Emissions,7,FALSE))","v":""},{"$f":"IF($B112=\"\",\"\",$C34*VLOOKUP($B112,Tbl_Emissions,8,FALSE))","v":""},{"$f":"IF($B112=\"\",\"\",$C112*GHG_CO2_factor+$D112*GHG_CH4_factor+$E112*GHG_N2O_factor)","v":""}]
[null,{"$f":"B35","v":""},{"$f":"IF($B113=\"\",\"\",$C35*VLOOKUP($B113,Tbl_Emissions,6,FALSE))","v":""},{"$f":"IF($B113=\"\",\"\",$C35*VLOOKUP($B113,Tbl_Emissions,7,FALSE))","v":""},{"$f":"IF($B113=\"\",\"\",$C35*VLOOKUP($B113,Tbl_Emissions,8,FALSE))","v":""},{"$f":"IF($B113=\"\",\"\",$C113*GHG_CO2_factor+$D113*GHG_CH4_factor+$E113*GHG_N2O_factor)","v":""}]
[null,"Utility"]
[null,{"$f":"B37","v":""},{"$f":"IF($B115=\"\",\"\",$C37*VLOOKUP($B115,Tbl_Emissions,6,FALSE))","v":""},{"$f":"IF($B115=\"\",\"\",$C37*VLOOKUP($B115,Tbl_Emissions,7,FALSE))","v":""},{"$f":"IF($B115=\"\",\"\",$C37*VLOOKUP($B115,Tbl_Emissions,8,FALSE))","v":""},{"$f":"IF($B115=\"\",\"\",$C115*GHG_CO2_factor+$D115*GHG_CH4_factor+$E115*GHG_N2O_factor)","v":""}]
[null,{"$f":"B38","v":""},{"$f":"IF($B116=\"\",\"\",$C38*VLOOKUP($B116,Tbl_Emissions,6,FALSE))","v":""},{"$f":"IF($B116=\"\",\"\",$C38*VLOOKUP($B116,Tbl_Emissions,7,FALSE))","v":""},{"$f":"IF($B116=\"\",\"\",$C38*VLOOKUP($B116,Tbl_Emissions,8,FALSE))","v":""},{"$f":"IF($B116=\"\",\"\",$C116*GHG_CO2_factor+$D116*GHG_CH4_factor+$E116*GHG_N2O_factor)","v":""}]
[null,{"$f":"B39","v":""},{"$f":"IF($B117=\"\",\"\",$C39*VLOOKUP($B117,Tbl_Emissions,6,FALSE))","v":""},{"$f":"IF($B117=\"\",\"\",$C39*VLOOKUP($B117,Tbl_Emissions,7,FALSE))","v":""},{"$f":"IF($B117=\"\",\"\",$C39*VLOOKUP($B117,Tbl_Emissions,8,FALSE))","v":""},{"$f":"IF($B117=\"\",\"\",$C117*GHG_CO2_factor+$D117*GHG_CH4_factor+$E117*GHG_N2O_factor)","v":""}]
[null,{"$f":"B40","v":""},{"$f":"IF($B118=\"\",\"\",$C40*VLOOKUP($B118,Tbl_Emissions,6,FALSE))","v":""},{"$f":"IF($B118=\"\",\"\",$C40*VLOOKUP($B118,Tbl_Emissions,7,FALSE))","v":""},{"$f":"IF($B118=\"\",\"\",$C40*VLOOKUP($B118,Tbl_Emissions,8,FALSE))","v":""},{"$f":"IF($B118=\"\",\"\",$C118*GHG_CO2_factor+$D118*GHG_CH4_factor+$E118*GHG_N2O_factor)","v":""}]
[null,"Carbon Sequestration"]
[null,{"$f":"B42","v":""},{"$f":"IF($B120=\"\",\"\",$C42*VLOOKUP($B120,Tbl_Emissions,6,FALSE))","v":""},{"$f":"IF($B120=\"\",\"\",$C42*VLOOKUP($B120,Tbl_Emissions,7,FALSE))","v":""},{"$f":"IF($B120=\"\",\"\",$C42*VLOOKUP($B120,Tbl_Emissions,8,FALSE))","v":""},{"$f":"IF($B120=\"\",\"\",$C120*GHG_CO2_factor+$D120*GHG_CH4_factor+$E120*GHG_N2O_factor)","v":""}]
[null,"TOTAL",{"$f":"SUM(C110:C120)","v":6.1162697987999994},{"$f":"SUM(D110:D120)","v":1.7159714737199998E-2},{"$f":"SUM(E110:E120)","v":1.4167664116199997E-2},{"$f":"SUM(F110:F120)","v":10.767226573857599}]

{"sheet":"Tornado Charts & Risk Analysis","index":9,"n_rows":2250,"n_cols":25,"rows_kept":2250,"cut":false,"hidden":false,"merged":[[11,15,11,16],[11,17,11,20],[10,1,10,2]]}
[]
[null,"Parameter","Nominal","Enter deviation % for lowering H2 cost","Enter deviation % for increasing H2 cost","Price-decreasing factor","Price-increasing factor","Price-decreasing value","Price-increasing value"]
[null,"Operating Capacity Factor",{"$f":"+cap_factor","v":0.86},0.05,0.05,{"$f":"1+D3","v":1.05},{"$f":"1-E3","v":0.95},{"$f":"+C3*F3","v":0.90300000000000002},{"$f":"+C3*G3","v":0.81699999999999995}]
[null,{"$f":"+Input_Sheet_Template!B26","v":"Plant Design Capacity (kg of H2/day)"},{"$f":"+design_cap","v":1500},0.05,0.05,{"$f":"1+D4","v":1.05},{"$f":"1-E4","v":0.95},1575,1425]
[null,"After-tax Real IRR",{"$f":"+real_irr","v":0.08},0.05,0.05,{"$f":"1-D5","v":0.95},{"$f":"1+E5","v":1.05},7.5999999999999998E-2,8.4000000000000005E-2]
[null,"Feedstock Consumption (% of baseline)",1,0.05,0.05,{"$f":"1-D6","v":0.95},{"$f":"1+E6","v":1.05},0.95,1.05]
[null,"Utilities Consumption (% of baseline)",1,0.05,0.05,{"$f":"1-D7","v":0.95},1.05,0.95,1.05]
[null,"Total Capital Investment",{"$f":"+total_cap","v":2192779.8003413612},0.05,0.05,{"$f":"1-D8","v":0.95},1.05,2083140.8103242931,2302418.7903584293]
[null,"Total Fixed Operating Cost",{"$f":"+fixed","v":125607.29041291363},0.05,0.05,{"$f":"1-D9","v":0.95},1.05,119326.92589226794,131887.65493355933]
[]
[null,"Run Risk Analysis (note: Risk analysis could take ~5 min to run)?",null,"Yes",{"$f":"IF(RunRiskAnalysis=\"Yes\",\"          Please click Update Charts and Risk Analysis button before using results below\",\"\")","v":"          Please click Update Charts and Risk Analysis button before using results below"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Risk variable to plot",null,"Cost of hydrogen ($/kg)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Percentile","Value"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+MIN(OFFSET($B$251:$B$2250,0,$C$194))*$C$198","v":6.6948808964962101}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.05,{"$f":"+PERCENTILE(OFFSET($B$251:$B$2250,0,$C$194),V15)*$C$198","v":6.7155306956101715}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+V15+0.05","v":0.1},6.7208272024941698]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.15000000000000002,6.7249588056455307]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.2,6.7286802320375312]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.25,6.7316109862570332]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.3,6.7342604274279596]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.35,6.736823208068718]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.39999999999999997,6.7394365053985021]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.44999999999999996,6.741998742445853]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.49999999999999994,6.7443232249958589]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.54999999999999993,6.7465262468460976]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.6,6.748895539010924]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.65,6.7512402601775383]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.70000000000000007,6.7536745229719317]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.75000000000000011,6.7560390042321821]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.80000000000000016,6.7595930299057061]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.8500000000000002,6.7635789827792925]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.90000000000000024,6.7683182179649668]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.95000000000000029,6.7758327606418032]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"+MAX(OFFSET($B$251:$B$2250,0,$C$194))*$C$198","v":6.8022060679148275}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"No user interactions below this row"]
[]
[null,"Displayed case"]
[null,1,{"$f":"+OFFSET(C50,$B$48,0)","v":1},1,1,{"$f":"+OFFSET(F50,$B$48,0)","v":1},{"$f":"+OFFSET(G50,$B$48,0)","v":1},{"$f":"+OFFSET(H50,$B$48,0)","v":1},{"$f":"+OFFSET(I50,$B$48,0)","v":1},null,{"$f":"+'Cash Flow Analysis'!F118","v":6.7500479909357587},{"$f":"+'Cash Flow Analysis'!Q118","v":0},{"$f":"+'Cash Flow Analysis'!L118","v":1.0462870323492518E-2},{"$f":"+'Cash Flow Analysis'!H117","v":0.19506796071780513},{"$f":"+'Cash Flow Analysis'!I117","v":0.12245604125561525},{"$f":"+'Cash Flow Analysis'!J117","v":8.3212074775459749E-2},{"$f":"+'Cash Flow Analysis'!K117","v":0},{"$f":"+'Cash Flow Analysis'!M117","v":1.0462870323492518E-2},{"$f":"+'Cash Flow Analysis'!N117","v":0.27051761030742788},{"$f":"+'Cash Flow Analysis'!O117","v":5.9155865977564952},{"$f":"+'Cash Flow Analysis'!P117","v":0},{"$f":"+'Cash Flow Analysis'!R117","v":1.9155093650587738E-2},{"$f":"+'Cash Flow Analysis'!S117","v":0.10267023347944998},{"$f":"+'Cash Flow Analysis'!X117","v":-1.701858677734073E-3},{"$f":"+'Cash Flow Analysis'!Z117","v":4.3084237670649013E-2}]
[]
[null,"Case","Operating capacity factor","Plant design capacity (kg of H2/day)","After-tax real IRR (%)","Feedstock consumption (% of most likely value)","Utilities consumption (% of most likely value)","Total capital investment ($)","Total fixed operating cost ($/year)",null,"Cost of hydrogen ($/kg)","Revenue from byproduct sales ($/kg)","Salvage value ($/kg)","Initial equity depreciable capital ($/kg)","Yearly replacement costs ($/kg)","Cash from working capital reserve ($/kg)","Other non-depreciable capital costs ($/kg)","Decommissioning costs ($/kg)","Fixed operating cost ($/kg)","Feedstock cost ($/kg)","Other raw material cost ($/kg)","Other variable operating costs ($/kg)","Debt interest ($/kg)","Taxes ($/kg)","Principal payment ($/kg)"]
[null,1,1,1,1,1,1,1,1,null,6.744328582053198,0,1.0422448166438392E-2,0.19431433695104025,0.12198294571119789,8.3164470953852682E-2,0,1.0422448166438392E-2,0.26998780784474952,5.9121329147869046,0,1.9155093650587734E-2,0.10227357824296371,-1.6003525108757488E-3,4.2917786422775855E-2]
[null,{"$f":"+B51+1","v":2},{"$f":"+F3","v":1.05},1,1,1,1,1,1,null,6.7104490271023414,0,9.9261411108937068E-3,0.18506127328670499,0.11617423401066466,8.2988743750131641E-2,0,9.9261411108937068E-3,0.25713124556642813,5.9121329147869046,0,1.8895492420334489E-2,9.7403407850441631E-2,-2.1236687667544629E-4,4.0874082307405586E-2]
[null,{"$f":"+B52+1","v":3},{"$f":"+G3","v":0.95},1,1,1,1,1,1,null,6.7817744059462539,0,1.0970998069935152E-2,0.2045414073168845,0.1284031007486294,8.3358695757965437E-2,0,1.0970998069935152E-2,0.28419769246815746,5.9121329147869064,0,1.9442021326130796E-2,0.10765639815048815,-3.1344418960442748E-3,4.5176617287132501E-2]
[null,4,1,{"$f":"+F4","v":1.05},1,1,1,1,1,null,6.7351314435808316,0,1.0207098838426626E-2,0.1902994009957619,0.11962539552399412,8.3158352517765974E-2,0,1.0207098838426626E-2,0.26953113424613762,5.9121329147869046,0,1.9155093650587731E-2,0.10016039466111556,-9.6225902221392496E-4,4.2031016220774882E-2]
[null,5,1,{"$f":"+G4","v":0.95},1,1,1,1,1,null,6.7542753417637762,0,1.0654189505982337E-2,0.1986348827593305,0.12451156328280535,8.3171825395302337E-2,0,1.0654189505982337E-2,0.27053673557643676,5.9121329147869064,0,1.9155093650587738E-2,0.10454761363690285,-2.2873433350939789E-3,4.3872056010597064E-2]
[null,6,1,1,{"$f":"+F5","v":0.95},1,1,1,1,null,6.7398361443768522,0,1.0886462769928731E-2,0.188448293755897,0.12290839424382713,8.0046783020920872E-2,0,1.0886462769928731E-2,0.26990219128405518,5.9148727670211576,0,1.9155093650587731E-2,0.10170587558175297,-2.0317701497742451E-3,4.4828515968428545E-2]
[null,7,1,1,{"$f":"+G5","v":1.05},1,1,1,1,null,6.7488329065114865,0,9.9758378652312855E-3,0.20026037147306291,0.1210349477733048,8.6257605126148634E-2,0,9.9758378652312855E-3,0.27007411349004551,5.9092542574910798,0,1.9155093650587745E-2,0.10284394125693452,-1.1261484457542712E-3,4.1078724696075208E-2]
[null,8,1,1,1,{"$f":"+F6","v":0.95},1,1,1,null,6.7415777638161085,0,1.0422448166438392E-2,0.19431433695104025,0.12198294571119789,8.3128318302260501E-2,0,1.0422448166438392E-2,0.26998780784474952,5.9094307804329169,0,1.9155093650587734E-2,0.10227357824296371,-1.612883742386806E-3,4.2917786422775855E-2]
[null,9,1,1,1,{"$f":"+G6","v":1.05},1,1,1,null,6.7470794002902874,0,1.0422448166438392E-2,0.19431433695104025,0.12198294571119789,8.3200623605444862E-2,0,1.0422448166438392E-2,0.26998780784474952,5.9148350491408914,0,1.9155093650587734E-2,0.10227357824296371,-1.5878212793650056E-3,4.2917786422775855E-2]
[null,10,1,1,1,1,{"$f":"+F7","v":0.95},1,1,null,6.744328582053198,0,1.0422448166438392E-2,0.19431433695104025,0.12198294571119789,8.3164470953852682E-2,0,1.0422448166438392E-2,0.26998780784474952,5.9121329147869046,0,1.9155093650587734E-2,0.10227357824296371,-1.6003525108757488E-3,4.2917786422775855E-2]
[null,11,1,1,1,1,{"$f":"+G6","v":1.05},1,1,null,6.744328582053198,0,1.0422448166438392E-2,0.19431433695104025,0.12198294571119789,8.3164470953852682E-2,0,1.0422448166438392E-2,0.26998780784474952,5.9121329147869046,0,1.9155093650587734E-2,0.10227357824296371,-1.6003525108757488E-3,4.2917786422775855E-2]
[null,12,1,1,1,1,1,{"$f":"+F8","v":0.95},1,null,6.7245082073347655,0,9.9013257581164714E-3,0.18459862010348826,0.12198294571119789,8.3101323062891461E-2,0,9.9013257581164714E-3,0.26527451604907248,5.9121329147869046,0,1.9155093650587734E-2,9.7159899330815536E-2,3.3099753817008036E-4,4.0771897101637068E-2]
[null,13,1,1,1,1,1,{"$f":"+G8","v":1.05},1,null,6.7641489567716313,0,1.0943570574760312E-2,0.20403005379859224,0.12198294571119789,8.322761884481393E-2,0,1.0943570574760312E-2,0.27470109964042666,5.9121329147869046,0,1.9155093650587734E-2,0.1073872571551119,-3.5317025599214246E-3,4.5063675743914657E-2]
[null,14,1,1,1,1,1,1,{"$f":"+F9","v":0.95},null,6.7305856385198117,0,1.0422448166438392E-2,0.19431433695104025,0.12198294571119789,8.2983608391234712E-2,0,1.0422448166438392E-2,0.25648841745251211,5.9121329147869046,0,1.9155093650587734E-2,0.10227357824296371,-1.6630430894075646E-3,4.2917786422775855E-2]
[null,15,1,1,1,1,1,1,{"$f":"+G9","v":1.05},null,6.7580715255865851,0,1.0422448166438392E-2,0.19431433695104025,0.12198294571119789,8.3345333516470665E-2,0,1.0422448166438392E-2,0.28348719823698704,5.9121329147869046,0,1.9155093650587734E-2,0.10227357824296371,-1.537661932343935E-3,4.2917786422775855E-2]
[null,16,{"$f":"(C$72=1)*$F$3\n+(C$72=2)\n+(C$72=3)\n+(C$72=4)\n+(C$72=5)","v":1.05},1,1,{"$f":"(F$72=1)*$F$6\n+(F$72=2)\n+(F$72=3)\n+(F$72=4)\n+(F$72=5)","v":1},{"$f":"(G$72=1)*$F$7\n+(G$72=2)\n+(G$72=3)\n+(G$72=4)\n+(G$72=5)","v":1},{"$f":"(H$72=1)*$F$8\n+(H$72=2)\n+(H$72=3)\n+(H$72=4)\n+(H$72=5)","v":1},{"$f":"(I$72=1)*$F$9\n+(I$72=2)\n+(I$72=3)\n+(I$72=4)\n+(I$72=5)","v":1},null,6.7104490271023414,0,9.9261411108937068E-3,0.18506127328670499,0.11617423401066466,8.2988743750131641E-2,0,9.9261411108937068E-3,0.25713124556642813,5.9121329147869046,0,1.8895492420334489E-2,9.7403407850441631E-2,-2.1236687667544629E-4,4.0874082307405586E-2]
[null,17,{"$f":"(C$72=1)*$F$3\n+(C$72=2)*$F$3\n+(C$72=3)\n+(C$72=4)\n+(C$72=5)","v":1.05},1,1,{"$f":"(F$72=1)*$F$6\n+(F$72=2)*$F$6\n+(F$72=3)\n+(F$72=4)\n+(F$72=5)","v":1},{"$f":"(G$72=1)*$F$7\n+(G$72=2)*$F$7\n+(G$72=3)\n+(G$72=4)\n+(G$72=5)","v":1},{"$f":"(H$72=1)*$F$8\n+(H$72=2)*$F$8\n+(H$72=3)\n+(H$72=4)\n+(H$72=5)","v":0.95},{"$f":"(I$72=1)*$F$9\n+(I$72=2)*$F$9\n+(I$72=3)\n+(I$72=4)\n+(I$72=5)","v":1},null,6.6915724797514544,0,9.4298340553490203E-3,0.17580820962236976,0.11617423401066466,8.2928602901597093E-2,0,9.4298340553490203E-3,0.25264239623721185,5.9121329147869046,0,1.8895492420334489E-2,9.2533237457919568E-2,1.6270141224155809E-3,3.8830378192035303E-2]
[null,18,{"$f":"(C$72=1)*$F$3\n+(C$72=2)*$F$3\n+(C$72=3)*$F$3\n+(C$72=4)\n+(C$72=5)","v":1.05},1,1,{"$f":"(F$72=1)*$F$6\n+(F$72=2)*$F$6\n+(F$72=3)*$F$6\n+(F$72=4)\n+(F$72=5)","v":1},{"$f":"(G$72=1)*$F$7\n+(G$72=2)*$F$7\n+(G$72=3)*$F$7\n+(G$72=4)\n+(G$72=5)","v":1},{"$f":"(H$72=1)*$F$8\n+(H$72=2)*$F$8\n+(H$72=3)*$F$8\n+(H$72=4)\n+(H$72=5)","v":0.95},{"$f":"(I$72=1)*$F$9\n+(I$72=2)*$F$9\n+(I$72=3)*$F$9\n+(I$72=4)\n+(I$72=5)","v":0.95},null,6.6787124539104976,0,9.4298340553490203E-3,0.17580820962236976,0.11617423401066466,8.2759359884387665E-2,0,9.4298340553490203E-3,0.2400102764253513,5.9121329147869046,0,1.8895492420334489E-2,9.2533237457919568E-2,1.5683511105260258E-3,3.8830378192035303E-2]
[null,19,{"$f":"(C$72=1)*$F$3\n+(C$72=2)*$F$3\n+(C$72=3)*$F$3\n+(C$72=4)*$F$3\n+(C$72=5)","v":1.05},1,1,{"$f":"(F$72=1)*$F$6\n+(F$72=2)*$F$6\n+(F$72=3)*$F$6\n+(F$72=4)*$F$6\n+(F$72=5)","v":0.95},{"$f":"(G$72=1)*$F$7\n+(G$72=2)*$F$7\n+(G$72=3)*$F$7\n+(G$72=4)*$F$7\n+(G$72=5)","v":1},{"$f":"(H$72=1)*$F$8\n+(H$72=2)*$F$8\n+(H$72=3)*$F$8\n+(H$72=4)*$F$8\n+(H$72=5)","v":0.95},{"$f":"(I$72=1)*$F$9\n+(I$72=2)*$F$9\n+(I$72=3)*$F$9\n+(I$72=4)*$F$9\n+(I$72=5)","v":0.95},null,6.6759616356734073,0,9.4298340553490203E-3,0.17580820962236976,0.11617423401066466,8.2723207232795498E-2,0,9.4298340553490203E-3,0.2400102764253513,5.9094307804329178,0,1.8895492420334489E-2,9.2533237457919568E-2,1.5558198790151716E-3,3.8830378192035303E-2]
[null,20,{"$f":"(C$72=1)*$F$3\n+(C$72=2)*$F$3\n+(C$72=3)*$F$3\n+(C$72=4)*$F$3\n+(C$72=5)*$F$3","v":1.05},1,1,{"$f":"(F$72=1)*$F$6\n+(F$72=2)*$F$6\n+(F$72=3)*$F$6\n+(F$72=4)*$F$6\n+(F$72=5)*$F$6","v":0.95},{"$f":"(G$72=1)*$F$7\n+(G$72=2)*$F$7\n+(G$72=3)*$F$7\n+(G$72=4)*$F$7\n+(G$72=5)*$F$7","v":0.95},{"$f":"(H$72=1)*$F$8\n+(H$72=2)*$F$8\n+(H$72=3)*$F$8\n+(H$72=4)*$F$8\n+(H$72=5)*$F$8","v":0.95},{"$f":"(I$72=1)*$F$9\n+(I$72=2)*$F$9\n+(I$72=3)*$F$9\n+(I$72=4)*$F$9\n+(I$72=5)*$F$9","v":0.95},null,6.6759616356734073,0,9.4298340553490203E-3,0.17580820962236976,0.11617423401066466,8.2723207232795498E-2,0,9.4298340553490203E-3,0.2400102764253513,5.9094307804329178,0,1.8895492420334489E-2,9.2533237457919568E-2,1.5558198790151716E-3,3.8830378192035303E-2]
[]
[null,"Waterfall Chart Priority",{"$f":"6-RANK($N$101,($N$101,$N$104:$N$107))","v":1},null,null,{"$f":"6-RANK($N$104,($N$101,$N$104:$N$107))","v":4},{"$f":"6-RANK($N$105,($N$101,$N$104:$N$107))","v":5},{"$f":"6-RANK($N$106,($N$101,$N$104:$N$107))","v":2},{"$f":"6-RANK($N$107,($N$101,$N$104:$N$107))","v":3}]
[]
[null,"Visualization data formatting"]
[]
[null,"parameter","level","Chart titles","Revenue from Hydrogen Sales","Revenue from Byproduct Sales","Salvage Value","Initial Equity Depreciable Capital","Yearly Replacement Costs","Cash for Working Capital Reserve","Other Non-Depreciable Capital Costs","Decommissioning Costs","Fixed Operating Cost","Feedstock Cost","Other Raw Material Cost","Other Variable Operating Costs","Debt Interest","Taxes","Principal Payment"]
[null,{"$f":"+$B$3","v":"Operating Capacity Factor"},{"$f":"+H3","v":0.90300000000000002},{"$f":"+B77&\" = \"&C77*100&\"%\"","v":"Operating Capacity Factor = 90.3%"},{"$f":"+K52","v":6.7104490271023414},0,9.9261411108937068E-3,0.18506127328670499,0.11617423401066466,8.2988743750131641E-2,0,9.9261411108937068E-3,0.25713124556642813,5.9121329147869046,0,1.8895492420334489E-2,9.7403407850441631E-2,-2.1236687667544629E-4,4.0874082307405586E-2]
[null,{"$f":"+$B$3","v":"Operating Capacity Factor"},{"$f":"+C3","v":0.86},{"$f":"+B78&\" = \"&C78*100&\"%\"","v":"Operating Capacity Factor = 86%"},{"$f":"+K$51","v":6.744328582053198},0,1.0422448166438392E-2,0.19431433695104025,0.12198294571119789,8.3164470953852682E-2,0,1.0422448166438392E-2,0.26998780784474952,5.9121329147869046,0,1.9155093650587734E-2,0.10227357824296371,-1.6003525108757488E-3,4.2917786422775855E-2]
[null,"Operating Capacity Factor",{"$f":"+I3","v":0.81699999999999995},"Operating Capacity Factor = 81.7%",{"$f":"+K53","v":6.7817744059462539},0,1.0970998069935152E-2,0.2045414073168845,0.1284031007486294,8.3358695757965437E-2,0,1.0970998069935152E-2,0.28419769246815746,5.9121329147869064,0,1.9442021326130796E-2,0.10765639815048815,-3.1344418960442748E-3,4.5176617287132501E-2]
[null,{"$f":"+$B$4","v":"Plant Design Capacity (kg of H2/day)"},{"$f":"ROUND(H4,0)","v":1575},{"$f":"+B80&\" = \"&TEXT(C80,\"0,000\")","v":"Plant Design Capacity (kg of H2/day) = 1,575"},6.7351314435808316,0,1.0207098838426626E-2,0.1902994009957619,0.11962539552399412,8.3158352517765974E-2,0,1.0207098838426626E-2,0.26953113424613762,5.9121329147869046,0,1.9155093650587731E-2,0.10016039466111556,-9.6225902221392496E-4,4.2031016220774882E-2]
[null,{"$f":"+$B$4","v":"Plant Design Capacity (kg of H2/day)"},{"$f":"+ROUND(C4,0)","v":1500},{"$f":"+B81&\" = \"&TEXT(C81,\"0,000\")","v":"Plant Design Capacity (kg of H2/day) = 1,500"},{"$f":"+K$51","v":6.744328582053198},0,1.0422448166438392E-2,0.19431433695104025,0.12198294571119789,8.3164470953852682E-2,0,1.0422448166438392E-2,0.26998780784474952,5.9121329147869046,0,1.9155093650587734E-2,0.10227357824296371,-1.6003525108757488E-3,4.2917786422775855E-2]
[null,"Plant Design Capacity (kg of H2/day)",{"$f":"ROUND(I4,0)","v":1425},"Plant Design Capacity (kg of H2/day) = 1,425",{"$f":"+K55","v":6.7542753417637762},0,1.0654189505982337E-2,0.1986348827593305,0.12451156328280535,8.3171825395302337E-2,0,1.0654189505982337E-2,0.27053673557643676,5.9121329147869064,0,1.9155093650587738E-2,0.10454761363690285,-2.2873433350939789E-3,4.3872056010597064E-2]
[null,{"$f":"+$B$5","v":"After-tax Real IRR"},{"$f":"+ROUND(H5,2)","v":0.08},{"$f":"+B83&\" = \"&C83*100&\"%\"","v":"After-tax Real IRR = 8%"},6.7398361443768522,0,1.0886462769928731E-2,0.188448293755897,0.12290839424382713,8.0046783020920872E-2,0,1.0886462769928731E-2,0.26990219128405518,5.9148727670211576,0,1.9155093650587731E-2,0.10170587558175297,-2.0317701497742451E-3,4.4828515968428545E-2]
[null,{"$f":"+$B$5","v":"After-tax Real IRR"},{"$f":"ROUND(C5,2)","v":0.08},"After-tax Real IRR = 8%",{"$f":"+K$51","v":6.744328582053198},0,1.0422448166438392E-2,0.19431433695104025,0.12198294571119789,8.3164470953852682E-2,0,1.0422448166438392E-2,0.26998780784474952,5.9121329147869046,0,1.9155093650587734E-2,0.10227357824296371,-1.6003525108757488E-3,4.2917786422775855E-2]
[null,"After-tax Real IRR",{"$f":"ROUND(I5,2)","v":0.08},"After-tax Real IRR = 8%",{"$f":"+K57","v":6.7488329065114865},0,9.9758378652312855E-3,0.20026037147306291,0.1210349477733048,8.6257605126148634E-2,0,9.9758378652312855E-3,0.27007411349004551,5.9092542574910798,0,1.9155093650587745E-2,0.10284394125693452,-1.1261484457542712E-3,4.1078724696075208E-2]
[null,{"$f":"+$B$6","v":"Feedstock Consumption (% of baseline)"},{"$f":"+ROUND(H6,3)","v":0.95},{"$f":"+B86&\" = \"&C86*100&\"%\"","v":"Feedstock Consumption (% of baseline) = 95%"},6.7415777638161085,0,1.0422448166438392E-2,0.19431433695104025,0.12198294571119789,8.3128318302260501E-2,0,1.0422448166438392E-2,0.26998780784474952,5.9094307804329169,0,1.9155093650587734E-2,0.10227357824296371,-1.612883742386806E-3,4.2917786422775855E-2]
[null,{"$f":"+$B$6","v":"Feedstock Consumption (% of baseline)"},{"$f":"+ROUND(C6,3)","v":1},{"$f":"+B87&\" = \"&C87*100&\"%\"","v":"Feedstock Consumption (% of baseline) = 100%"},{"$f":"+K$51","v":6.744328582053198},0,1.0422448166438392E-2,0.19431433695104025,0.12198294571119789,8.3164470953852682E-2,0,1.0422448166438392E-2,0.26998780784474952,5.9121329147869046,0,1.9155093650587734E-2,0.10227357824296371,-1.6003525108757488E-3,4.2917786422775855E-2]
[null,"Feedstock Consumption (% of baseline)",{"$f":"+ROUND(I6,3)","v":1.05},{"$f":"+B88&\" = \"&C88*100&\"%\"","v":"Feedstock Consumption (% of baseline) = 105%"},{"$f":"+K59","v":6.7470794002902874},0,1.0422448166438392E-2,0.19431433695104025,0.12198294571119789,8.3200623605444862E-2,0,1.0422448166438392E-2,0.26998780784474952,5.9148350491408914,0,1.9155093650587734E-2,0.10227357824296371,-1.5878212793650056E-3,4.2917786422775855E-2]
[null,{"$f":"+$B$7","v":"Utilities Consumption (% of baseline)"},{"$f":"+ROUND(H7,3)","v":0.95},{"$f":"+B89&\" = \"&C89*100&\"%\"","v":"Utilities Consumption (% of baseline) = 95%"},6.744328582053198,0,1.0422448166438392E-2,0.19431433695104025,0.12198294571119789,8.3164470953852682E-2,0,1.0422448166438392E-2,0.26998780784474952,5.9121329147869046,0,1.9155093650587734E-2,0.10227357824296371,-1.6003525108757488E-3,4.2917786422775855E-2]
[null,{"$f":"+$B$7","v":"Utilities Consumption (% of baseline)"},{"$f":"+ROUND(C7,3)","v":1},"Utilities Consumption (% of baseline) = 100%",{"$f":"+K$51","v":6.744328582053198},{"$f":"+L$51","v":0},1.0422448166438392E-2,0.19431433695104025,0.12198294571119789,8.3164470953852682E-2,0,1.0422448166438392E-2,0.26998780784474952,5.9121329147869046,0,1.9155093650587734E-2,0.10227357824296371,-1.6003525108757488E-3,4.2917786422775855E-2]
[null,"Utilities Consumption (% of baseline)",{"$f":"+ROUND(I7,3)","v":1.05},"Utilities Consumption (% of baseline) = 105%",{"$f":"+K61","v":6.744328582053198},0,1.0422448166438392E-2,0.19431433695104025,0.12198294571119789,8.3164470953852682E-2,0,1.0422448166438392E-2,0.26998780784474952,5.9121329147869046,0,1.9155093650587734E-2,0.10227357824296371,-1.6003525108757488E-3,4.2917786422775855E-2]
[null,{"$f":"+$B$8","v":"Total Capital Investment"},{"$f":"+ROUND(H8,0)","v":2083141},{"$f":"+B92&\" = \"&TEXT(C92/1000,\"$0,000K\")","v":"Total Capital Investment = $2,083K"},6.7245082073347655,0,9.9013257581164714E-3,0.18459862010348826,0.12198294571119789,8.3101323062891461E-2,0,9.9013257581164714E-3,0.26527451604907248,5.9121329147869046,0,1.9155093650587734E-2,9.7159899330815536E-2,3.3099753817008036E-4,4.0771897101637068E-2]
[null,{"$f":"+$B$8","v":"Total Capital Investment"},{"$f":"+ROUND(C8,0)","v":2192780},"Total Capital Investment = $2,193K",{"$f":"+K$51","v":6.744328582053198},0,1.0422448166438392E-2,0.19431433695104025,0.12198294571119789,8.3164470953852682E-2,0,1.0422448166438392E-2,0.26998780784474952,5.9121329147869046,0,1.9155093650587734E-2,0.10227357824296371,-1.6003525108757488E-3,4.2917786422775855E-2]
[null,"Total Capital Investment",{"$f":"+ROUND(I8,0)","v":2302419},"Total Capital Investment = $2,302K",{"$f":"+K63","v":6.7641489567716313},0,1.0943570574760312E-2,0.20403005379859224,0.12198294571119789,8.322761884481393E-2,0,1.0943570574760312E-2,0.27470109964042666,5.9121329147869046,0,1.9155093650587734E-2,0.1073872571551119,-3.5317025599214246E-3,4.5063675743914657E-2]
[null,{"$f":"+$B$9","v":"Total Fixed Operating Cost"},{"$f":"+ROUND(H9,0)","v":119327},"Total Fixed Operating Cost = $0,119K",6.7305856385198117,0,1.0422448166438392E-2,0.19431433695104025,0.12198294571119789,8.2983608391234712E-2,0,1.0422448166438392E-2,0.25648841745251211,5.9121329147869046,0,1.9155093650587734E-2,0.10227357824296371,-1.6630430894075646E-3,4.2917786422775855E-2]
[null,{"$f":"+$B$9","v":"Total Fixed Operating Cost"},{"$f":"+ROUND(C9,0)","v":125607},"Total Fixed Operating Cost = $0,126K",{"$f":"+K$51","v":6.744328582053198},0,1.0422448166438392E-2,0.19431433695104025,0.12198294571119789,8.3164470953852682E-2,0,1.0422448166438392E-2,0.26998780784474952,5.9121329147869046,0,1.9155093650587734E-2,0.10227357824296371,-1.6003525108757488E-3,4.2917786422775855E-2]
[null,"Total Fixed Operating Cost",{"$f":"+ROUND(I9,0)","v":131888},"Total Fixed Operating Cost = $0,132K",{"$f":"+K65","v":6.7580715255865851},0,1.0422448166438392E-2,0.19431433695104025,0.12198294571119789,8.3345333516470665E-2,0,1.0422448166438392E-2,0.28348719823698704,5.9121329147869046,0,1.9155093650587734E-2,0.10227357824296371,-1.537661932343935E-3,4.2917786422775855E-2]
[]
[]
[null,"Standard Toranado","Rank","Titles","Low cost price","Default price","High price","dL0","dL1","dL2",null,"Unsorted titles","Results spread ($/kg)","Importance ranking"]
[null,null,1,{"$f":"OFFSET(L$100,MATCH($C101,$N$101:$N$107,0),0)","v":"Operating Capacity Factor\n(90%, 86%, 82%)"},{"$f":"OFFSET(E$76,MATCH($C101,$N$101:$N$107,0)*3-2,0)","v":6.7104490271023414},{"$f":"+$K$51","v":6.744328582053198},{"$f":"OFFSET(E$76,MATCH($C101,$N$101:$N$107,0)*3,0)","v":6.7817744059462539},{"$f":"+E101","v":6.7104490271023414},{"$f":"+F101-E101","v":3.3879554950856594E-2},{"$f":"+G101-F101","v":3.7445823893055952E-2},null,{"$f":"+B3&\"\n(\"&TEXT(H3,\"0%, \")&TEXT(C3,\"0%, \")&TEXT(I3,\"0%)\")","v":"Operating Capacity Factor\n(90%, 86%, 82%)"},{"$f":"ABS(K52-K53)+0.000000001","v":7.1325379843912545E-2},{"$f":"+RANK(M101,$M$101:$M$107)","v":1}]
[null,null,2,"Total Capital Investment\n($2,083K, $2,193K, $2,302K) ",6.7245082073347655,6.744328582053198,6.7641489567716313,{"$f":"+E102","v":6.7245082073347655},{"$f":"+F102-E102","v":1.9820374718432454E-2},{"$f":"+G102-F102","v":1.9820374718433342E-2},null,{"$f":"+B4&\"\n(\"&TEXT(H4,\"0,000\")&\", \"&TEXT(C4,\"0,000\")&\", \"&TEXT(I4,\"0,000\")&\") \"","v":"Plant Design Capacity (kg of H2/day)\n(1,575, 1,500, 1,425) "},{"$f":"+ABS(K54-K55)+0.000000002","v":1.9143900182944595E-2},4]
[null,null,3,"Total Fixed Operating Cost\n($0,119K, $0,126K, $0,132K) ",6.7305856385198117,6.744328582053198,6.7580715255865851,6.7305856385198117,1.3742943533386232E-2,1.374294353338712E-2,null,{"$f":"+B5&\"\n(\"&TEXT(H5,\"0%, \")&TEXT(C5,\"0%, \")&TEXT(I5,\"0%)\")","v":"After-tax Real IRR\n(8%, 8%, 8%)"},{"$f":"+ABS(K56-K57)+0.000000003","v":8.9967651346342953E-3},5]
[null,null,4,"Plant Design Capacity (kg of H2/day)\n(1,575, 1,500, 1,425) ",6.7351314435808316,6.744328582053198,6.7542753417637762,6.7351314435808316,9.1971384723663618E-3,9.9467597105782346E-3,null,{"$f":"+B6&\"\n(\"&TEXT(H6,\"0%, \")&TEXT(C6,\"0%, \")&TEXT(I6,\"0%)\")","v":"Feedstock Consumption (% of baseline)\n(95%, 100%, 105%)"},{"$f":"+ABS(K58-K59)+0.000000004","v":5.5016404741788944E-3},6]
[null,null,5,"After-tax Real IRR\n(8%, 8%, 8%)",6.7398361443768522,6.744328582053198,6.7488329065114865,{"$f":"+E105","v":6.7398361443768522},{"$f":"+F105-E105","v":4.492437676345773E-3},{"$f":"+G105-F105","v":4.5043244582885222E-3},null,{"$f":"+B7&\"\n(\"&TEXT(H7,\"0%, \")&TEXT(C7,\"0%, \")&TEXT(I7,\"0%)\")","v":"Utilities Consumption (% of baseline)\n(95%, 100%, 105%)"},{"$f":"+ABS(K60-K61)+0.000000004","v":4.0000000000000002E-9},7]
[null,null,6,"Feedstock Consumption (% of baseline)\n(95%, 100%, 105%)",6.7415777638161085,6.744328582053198,6.7470794002902874,6.7415777638161085,2.7508182370894474E-3,2.7508182370894474E-3,null,{"$f":"+B8&\"\n(\"&TEXT(H8/1000,\"$0,000K\")&\", \"&TEXT(C8/1000,\"$0,000K\")&\", \"&TEXT(I8/1000,\"$0,000K\")&\") \"","v":"Total Capital Investment\n($2,083K, $2,193K, $2,302K) "},{"$f":"+ABS(K62-K63)+0.000000006","v":3.9640755436865793E-2},2]
[null,null,7,"Utilities Consumption (% of baseline)\n(95%, 100%, 105%)",6.744328582053198,6.744328582053198,6.744328582053198,6.744328582053198,0,0,null,{"$f":"+B9&\"\n(\"&TEXT(H9/1000,\"$0,000K\")&\", \"&TEXT(C9/1000,\"$0,000K\")&\", \"&TEXT(I9/1000,\"$0,000K\")&\") \"","v":"Total Fixed Operating Cost\n($0,119K, $0,126K, $0,132K) "},{"$f":"+ABS(K64-K65)+0.00000007","v":2.7485957066773353E-2},3]
[]
[]
[null,"Simple bar chart","Rank",{"$f":"+D76","v":"Chart titles"},"Hydrogen Sales","Byproduct Sales","Salvage Value",{"$f":"+H76","v":"Initial Equity Depreciable Capital"},"Yearly Replacement Costs","Cash for Working Capital Reserve","Other Non-Depreciable Capital Costs","Decommissioning Costs","Fixed Operating Cost","Feedstock Cost","Other Raw Material Cost","Other Variable Operating Costs","Debt Interest","Taxes","Principal Payment"]
[null,null,1,"Base case",{"$f":"OFFSET(E$76,MATCH($C111,$N$101:$N$107,0)*3-1,0)","v":6.744328582053198},{"$f":"OFFSET(F$76,MATCH($C111,$N$101:$N$107,0)*3-1,0)","v":0},{"$f":"OFFSET(G$76,MATCH($C111,$N$101:$N$107,0)*3-1,0)","v":1.0422448166438392E-2}]
[null,null,null,null,null,null,null,{"$f":"OFFSET(H$76,MATCH($C111,$N$101:$N$107,0)*3-1,0)","v":0.19431433695104025},0.12198294571119789,8.3164470953852682E-2,0,1.0422448166438392E-2,0.26998780784474952,5.9121329147869046,0,1.9155093650587734E-2,0.10227357824296371,-1.6003525108757488E-3,4.2917786422775855E-2]
[]
[]
[null,null,1,{"$f":"OFFSET(D$76,MATCH($C115,$N$101:$N$107,0)*3-2,0)","v":"Operating Capacity Factor = 90.3%"},6.7104490271023414,0,9.9261411108937068E-3]
[null,null,null,null,null,null,null,{"$f":"OFFSET(H$76,MATCH($C115,$N$101:$N$107,0)*3-2,0)","v":0.18506127328670499},0.11617423401066466,8.2988743750131641E-2,0,9.9261411108937068E-3,0.25713124556642813,5.9121329147869046,0,1.8895492420334489E-2,9.7403407850441631E-2,-2.1236687667544629E-4,4.0874082307405586E-2]
[null,null,1,{"$f":"OFFSET(D$76,MATCH($C117,$N$101:$N$107,0)*3,0)","v":"Operating Capacity Factor = 81.7%"},6.7817744059462539,0,1.0970998069935152E-2]
[null,null,null,null,null,null,null,{"$f":"OFFSET(H$76,MATCH($C117,$N$101:$N$107,0)*3,0)","v":0.2045414073168845},0.1284031007486294,8.3358695757965437E-2,0,1.0970998069935152E-2,0.28419769246815746,5.9121329147869064,0,1.9442021326130796E-2,0.10765639815048815,-3.1344418960442748E-3,4.5176617287132501E-2]
[]
[null,null,2,{"$f":"OFFSET(D$76,MATCH($C120,$N$101:$N$107,0)*3-2,0)","v":"Total Capital Investment = $2,083K"},6.7245082073347655,0,9.9013257581164714E-3]
[null,null,null,null,null,null,null,{"$f":"OFFSET(H$76,MATCH($C120,$N$101:$N$107,0)*3-2,0)","v":0.18459862010348826},0.12198294571119789,8.3101323062891461E-2,0,9.9013257581164714E-3,0.26527451604907248,5.9121329147869046,0,1.9155093650587734E-2,9.7159899330815536E-2,3.3099753817008036E-4,4.0771897101637068E-2]
[null,null,2,{"$f":"OFFSET(D$76,MATCH($C122,$N$101:$N$107,0)*3,0)","v":"Total Capital Investment = $2,302K"},6.7641489567716313,0,1.0943570574760312E-2]
[null,null,null,null,null,null,null,{"$f":"OFFSET(H$76,MATCH($C122,$N$101:$N$107,0)*3,0)","v":0.20403005379859224},0.12198294571119789,8.322761884481393E-2,0,1.0943570574760312E-2,0.27470109964042666,5.9121329147869046,0,1.9155093650587734E-2,0.1073872571551119,-3.5317025599214246E-3,4.5063675743914657E-2]
[]
[null,null,3,{"$f":"OFFSET(D$76,MATCH($C125,$N$101:$N$107,0)*3-2,0)","v":"Total Fixed Operating Cost = $0,119K"},6.7305856385198117,0,1.0422448166438392E-2]
[null,null,null,null,null,null,null,{"$f":"OFFSET(H$76,MATCH($C125,$N$101:$N$107,0)*3-2,0)","v":0.19431433695104025},0.12198294571119789,8.2983608391234712E-2,0,1.0422448166438392E-2,0.25648841745251211,5.9121329147869046,0,1.9155093650587734E-2,0.10227357824296371,-1.6630430894075646E-3,4.2917786422775855E-2]
[null,null,3,{"$f":"OFFSET(D$76,MATCH($C127,$N$101:$N$107,0)*3,0)","v":"Total Fixed Operating Cost = $0,132K"},6.7580715255865851,0,1.0422448166438392E-2]
[null,null,null,null,null,null,null,{"$f":"OFFSET(H$76,MATCH($C127,$N$101:$N$107,0)*3,0)","v":0.19431433695104025},0.12198294571119789,8.3345333516470665E-2,0,1.0422448166438392E-2,0.28348719823698704,5.9121329147869046,0,1.9155093650587734E-2,0.10227357824296371,-1.537661932343935E-3,4.2917786422775855E-2]
[]
[null,null,4,{"$f":"OFFSET(D$76,MATCH($C130,$N$101:$N$107,0)*3-2,0)","v":"Plant Design Capacity (kg of H2/day) = 1,575"},6.7351314435808316,0,1.0207098838426626E-2]
[null,null,null,null,null,null,null,{"$f":"OFFSET(H$76,MATCH($C130,$N$101:$N$107,0)*3-2,0)","v":0.1902994009957619},0.11962539552399412,8.3158352517765974E-2,0,1.0207098838426626E-2,0.26953113424613762,5.9121329147869046,0,1.9155093650587731E-2,0.10016039466111556,-9.6225902221392496E-4,4.2031016220774882E-2]
[null,null,4,{"$f":"OFFSET(D$76,MATCH($C132,$N$101:$N$107,0)*3,0)","v":"Plant Design Capacity (kg of H2/day) = 1,425"},6.7542753417637762,0,1.0654189505982337E-2]
[null,null,null,null,null,null,null,{"$f":"OFFSET(H$76,MATCH($C132,$N$101:$N$107,0)*3,0)","v":0.1986348827593305},0.12451156328280535,8.3171825395302337E-2,0,1.0654189505982337E-2,0.27053673557643676,5.9121329147869064,0,1.9155093650587738E-2,0.10454761363690285,-2.2873433350939789E-3,4.3872056010597064E-2]
[]
[null,null,5,{"$f":"OFFSET(D$76,MATCH($C135,$N$101:$N$107,0)*3-2,0)","v":"After-tax Real IRR = 8%"},6.7398361443768522,0,1.0886462769928731E-2]
[null,null,null,null,null,null,null,{"$f":"OFFSET(H$76,MATCH($C135,$N$101:$N$107,0)*3-2,0)","v":0.188448293755897},0.12290839424382713,8.0046783020920872E-2,0,1.0886462769928731E-2,0.26990219128405518,5.9148727670211576,0,1.9155093650587731E-2,0.10170587558175297,-2.0317701497742451E-3,4.4828515968428545E-2]
[null,null,5,{"$f":"OFFSET(D$76,MATCH($C137,$N$101:$N$107,0)*3,0)","v":"After-tax Real IRR = 8%"},6.7488329065114865,0,9.9758378652312855E-3]
[null,null,null,null,null,null,null,{"$f":"OFFSET(H$76,MATCH($C137,$N$101:$N$107,0)*3,0)","v":0.20026037147306291},0.1210349477733048,8.6257605126148634E-2,0,9.9758378652312855E-3,0.27007411349004551,5.9092542574910798,0,1.9155093650587745E-2,0.10284394125693452,-1.1261484457542712E-3,4.1078724696075208E-2]
[]
[null,null,6,{"$f":"OFFSET(D$76,MATCH($C140,$N$101:$N$107,0)*3-2,0)","v":"Feedstock Consumption (% of baseline) = 95%"},6.7415777638161085,0,1.0422448166438392E-2]
[null,null,null,null,null,null,null,{"$f":"OFFSET(H$76,MATCH($C140,$N$101:$N$107,0)*3-2,0)","v":0.19431433695104025},0.12198294571119789,8.3128318302260501E-2,0,1.0422448166438392E-2,0.26998780784474952,5.9094307804329169,0,1.9155093650587734E-2,0.10227357824296371,-1.612883742386806E-3,4.2917786422775855E-2]
[null,null,6,{"$f":"OFFSET(D$76,MATCH($C142,$N$101:$N$107,0)*3,0)","v":"Feedstock Consumption (% of baseline) = 105%"},6.7470794002902874,0,1.0422448166438392E-2]
[null,null,null,null,null,null,null,{"$f":"OFFSET(H$76,MATCH($C142,$N$101:$N$107,0)*3,0)","v":0.19431433695104025},0.12198294571119789,8.3200623605444862E-2,0,1.0422448166438392E-2,0.26998780784474952,5.9148350491408914,0,1.9155093650587734E-2,0.10227357824296371,-1.5878212793650056E-3,4.2917786422775855E-2]
[]
[null,null,7,{"$f":"OFFSET(D$76,MATCH($C145,$N$101:$N$107,0)*3-2,0)","v":"Utilities Consumption (% of baseline) = 95%"},6.744328582053198,0,1.0422448166438392E-2]
[null,null,null,null,null,null,null,{"$f":"OFFSET(H$76,MATCH($C145,$N$101:$N$107,0)*3-2,0)","v":0.19431433695104025},0.12198294571119789,8.3164470953852682E-2,0,1.0422448166438392E-2,0.26998780784474952,5.9121329147869046,0,1.9155093650587734E-2,0.10227357824296371,-1.6003525108757488E-3,4.2917786422775855E-2]
[null,null,7,{"$f":"OFFSET(D$76,MATCH($C147,$N$101:$N$107,0)*3,0)","v":"Utilities Consumption (% of baseline) = 105%"},6.744328582053198,0,1.0422448166438392E-2]
[null,null,null,null,null,null,null,{"$f":"OFFSET(H$76,MATCH($C147,$N$101:$N$107,0)*3,0)","v":0.19431433695104025},0.12198294571119789,8.3164470953852682E-2,0,1.0422448166438392E-2,0.26998780784474952,5.9121329147869046,0,1.9155093650587734E-2,0.10227357824296371,-1.6003525108757488E-3,4.2917786422775855E-2]
[]
[]
[]
[null,"Parado chart"]
[null,null,null,"Unsorted"]
[null,null,null,"Title","Unsorted values","Unsorted Ranking","Sorted ranking","Sorted titles","Sorted values",null,"Grayed Titles","Revenues\n $/kg H2","Expenses\n $/kg H2","Colored titles"]
[null,"Revenues",1,"Cost of Hydrogen",{"$f":"+K48+C155/10000000000","v":6.7500479910357587},{"$f":"+RANK(E155,$E$155:$E$157)","v":1},1,{"$f":"OFFSET($D$154,MATCH($G155,$F$155:$F$157,0),0)","v":"Cost of Hydrogen"},{"$f":"OFFSET($E$154,MATCH($G155,$F$155:$F$157,0),0)-OFFSET($C$154,MATCH($G155,$F$155:$F$157,0),0)/10000000000","v":6.7500479909357587},null,{"$f":"+H155","v":"Cost of Hydrogen"},{"$f":"+I155","v":6.7500479909357587},null,{"$f":"+IF(L155>0,K155,\"\")","v":"Cost of Hydrogen"}]
[null,null,2,{"$f":"+F110","v":"Byproduct Sales"},{"$f":"+L48+C156/10000000000","v":2.0000000000000001E-10},{"$f":"+RANK(E156,$E$155:$E$157)","v":3},2,{"$f":"OFFSET($D$154,MATCH($G156,$F$155:$F$157,0),0)","v":"Salvage Value"},{"$f":"OFFSET($E$154,MATCH($G156,$F$155:$F$157,0),0)-OFFSET($C$154,MATCH($G156,$F$155:$F$157,0),0)/10000000000","v":1.0462870323492518E-2},null,{"$f":"+H156","v":"Salvage Value"},{"$f":"+I156","v":1.0462870323492518E-2},null,{"$f":"+IF(L156>0,K156,\"\")","v":"Salvage Value"}]
[null,null,3,{"$f":"+G110","v":"Salvage Value"},{"$f":"+M48+C157/10000000000","v":1.0462870623492519E-2},{"$f":"+RANK(E157,$E$155:$E$157)","v":2},3,{"$f":"OFFSET($D$154,MATCH($G157,$F$155:$F$157,0),0)","v":"Byproduct Sales"},{"$f":"OFFSET($E$154,MATCH($G157,$F$155:$F$157,0),0)-OFFSET($C$154,MATCH($G157,$F$155:$F$157,0),0)/10000000000","v":0},null,"Byproduct Sales",0,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+IF(L158>0.01,K158,\"\")","v":""}]
[null,"Expenses",1,{"$f":"+H110","v":"Initial Equity Depreciable Capital"},{"$f":"+N48+C159/10000000000","v":0.19506796081780514},{"$f":"+RANK(E159,$E$159:$E$170)","v":3},1,{"$f":"OFFSET($D$158,MATCH($G159,$F$159:$F$170,0),0)","v":"Feedstock Cost"},{"$f":"OFFSET($E$158,MATCH($G159,$F$159:$F$170,0),0)-OFFSET($C$158,MATCH($G159,$F$159:$F$170,0),0)/10000000000","v":5.9155865977564952},null,"Feedstock Cost",null,{"$f":"+I159","v":5.9155865977564952},{"$f":"+IF(M159>0,K159,\"\")","v":"Feedstock Cost"}]
[null,null,{"$f":"+C159+1","v":2},{"$f":"+I110","v":"Yearly Replacement Costs"},{"$f":"+O48+C160/10000000000","v":0.12245604145561526},4,2,"Fixed Operating Cost",0.27051761030742788,null,"Fixed Operating Cost",null,{"$f":"+I160","v":0.27051761030742788},{"$f":"+IF(M160>0,K160,\"\")","v":"Fixed Operating Cost"}]
[null,null,{"$f":"+C160+1","v":3},{"$f":"+J110","v":"Cash for Working Capital Reserve"},{"$f":"+P48+C161/10000000000","v":8.3212075075459746E-2},6,3,"Initial Equity Depreciable Capital",0.19506796071780513,null,"Initial Equity Depreciable Capital",null,0.19506796071780513,"Initial Equity Depreciable Capital"]
[null,null,4,{"$f":"+K110","v":"Other Non-Depreciable Capital Costs"},{"$f":"+Q48+C162/10000000000","v":4.0000000000000001E-10},11,4,"Yearly Replacement Costs",0.12245604125561525,null,"Yearly Replacement Costs",null,0.12245604125561525,"Yearly Replacement Costs"]
[null,null,5,{"$f":"+L110","v":"Decommissioning Costs"},{"$f":"+R48+C163/10000000000","v":1.0462870823492518E-2},9,5,"Debt Interest",0.10267023347944998,null,"Debt Interest",null,0.10267023347944998,"Debt Interest"]
[null,null,6,{"$f":"+M110","v":"Fixed Operating Cost"},{"$f":"+S48+C164/10000000000","v":0.27051761090742787},2,6,"Cash for Working Capital Reserve",8.3212074775459749E-2,null,"Cash for Working Capital Reserve",null,8.3212074775459749E-2,"Cash for Working Capital Reserve"]
[null,null,7,{"$f":"+N110","v":"Feedstock Cost"},{"$f":"+T48+C165/10000000000","v":5.9155865984564953},1,7,"Principal Payment",4.3084237670649013E-2,null,"Principal Payment",null,4.3084237670649013E-2,"Principal Payment"]
[null,null,8,{"$f":"+O110","v":"Other Raw Material Cost"},{"$f":"+U48+C166/10000000000","v":8.0000000000000003E-10},10,8,"Other Variable Operating Costs",1.9155093650587738E-2,null,"Other Variable Operating Costs",null,1.9155093650587738E-2,"Other Variable Operating Costs"]
[null,null,9,{"$f":"+P110","v":"Other Variable Operating Costs"},{"$f":"+V48+C167/10000000000","v":1.915509455058774E-2},8,9,"Decommissioning Costs",1.0462870323492518E-2,null,"Decommissioning Costs",null,1.0462870323492518E-2,"Decommissioning Costs"]
[null,null,10,{"$f":"+Q110","v":"Debt Interest"},{"$f":"+W48+C168/10000000000","v":0.10267023447944998},5,10,"Other Raw Material Cost",0,null,"Other Raw Material Cost",null,0,""]
[null,null,11,{"$f":"+R110","v":"Taxes"},{"$f":"+X48+C169/10000000000","v":-1.701857577734073E-3},12,11,"Other Non-Depreciable Capital Costs",0,null,"Other Non-Depreciable Capital Costs",null,0,""]
[null,null,12,{"$f":"+S110","v":"Principal Payment"},{"$f":"+Y48+C170/10000000000","v":4.3084238870649015E-2},7,12,"Taxes",-1.701858677734073E-3,null,"Taxes",null,-1.701858677734073E-3,""]
[null,null,null,null,null,null,null,null,null,null,"Total",{"$f":"+SUM(L155:L170)","v":6.7605108612592515},{"$f":"+SUM(M155:M170)","v":6.7605108612592479},{"$f":"+IF(M171<0.01,K171,\"\")","v":""}]
[]
[]
[null,"Waterfall Chart",null,"Values","Base","Decrease","Increase"]
[null,0,"Baseline",{"$f":"+K51","v":6.744328582053198},{"$f":"+D175","v":6.744328582053198}]
[null,1,{"$f":"OFFSET($B$50,0,MATCH($B176,$C$72:$I$72,0))&\nIF(OFFSET($F$2,MATCH($B176,$C$72:$I$72,0),0)<1,\n\"\n= \"&OFFSET($F$2,MATCH($B176,$C$72:$I$72,0),0)*100-100,\n\"\n= +\"&OFFSET($F$2,MATCH($B176,$C$72:$I$72,0),0)*100-100)\n&\"%\"","v":"Operating capacity factor\n= +5%"},{"$f":"+K66","v":6.7104490271023414},{"$f":"+E175+G175-F176","v":6.7104490271023414},{"$f":"+MAX(D175-D176,0)","v":3.3879554950856594E-2},{"$f":"+MAX(D176-D175,0)","v":0}]
[null,2,{"$f":"OFFSET($B$50,0,MATCH($B177,$C$72:$I$72,0))&\nIF(OFFSET($F$2,MATCH($B177,$C$72:$I$72,0),0)<1,\n\"\n= \"&OFFSET($F$2,MATCH($B177,$C$72:$I$72,0),0)*100-100,\n\"\n= +\"&OFFSET($F$2,MATCH($B177,$C$72:$I$72,0),0)*100-100)\n&\"%\"","v":"Total capital investment ($)\n= -5%"},{"$f":"+K67","v":6.6915724797514544},6.6915724797514544,{"$f":"+MAX(D176-D177,0)","v":1.8876547350886952E-2},{"$f":"+MAX(D177-D176,0)","v":0}]
[null,3,{"$f":"OFFSET($B$50,0,MATCH($B178,$C$72:$I$72,0))&\nIF(OFFSET($F$2,MATCH($B178,$C$72:$I$72,0),0)<1,\n\"\n= \"&OFFSET($F$2,MATCH($B178,$C$72:$I$72,0),0)*100-100,\n\"\n= +\"&OFFSET($F$2,MATCH($B178,$C$72:$I$72,0),0)*100-100)\n&\"%\"","v":"Total fixed operating cost ($/year)\n= -5%"},{"$f":"+K68","v":6.6787124539104976},6.6787124539104976,{"$f":"+MAX(D177-D178,0)","v":1.2860025840956801E-2},{"$f":"+MAX(D178-D177,0)","v":0}]
[null,4,{"$f":"OFFSET($B$50,0,MATCH($B179,$C$72:$I$72,0))&\nIF(OFFSET($F$2,MATCH($B179,$C$72:$I$72,0),0)<1,\n\"\n= \"&OFFSET($F$2,MATCH($B179,$C$72:$I$72,0),0)*100-100,\n\"\n= +\"&OFFSET($F$2,MATCH($B179,$C$72:$I$72,0),0)*100-100)\n&\"%\"","v":"Feedstock consumption (% of most likely value)\n= -5%"},{"$f":"+K69","v":6.6759616356734073},6.6759616356734073,{"$f":"+MAX(D178-D179,0)","v":2.7508182370903356E-3},{"$f":"+MAX(D179-D178,0)","v":0}]
[null,5,{"$f":"OFFSET($B$50,0,MATCH($B180,$C$72:$I$72,0))&\nIF(OFFSET($F$2,MATCH($B180,$C$72:$I$72,0),0)<1,\n\"\n= \"&OFFSET($F$2,MATCH($B180,$C$72:$I$72,0),0)*100-100,\n\"\n= +\"&OFFSET($F$2,MATCH($B180,$C$72:$I$72,0),0)*100-100)\n&\"%\"","v":"Utilities consumption (% of most likely value)\n= -5%"},{"$f":"+K70","v":6.6759616356734073},6.6759616356734073,{"$f":"+MAX(D179-D180,0)","v":0},{"$f":"+MAX(D180-D179,0)","v":0}]
[null,6,"Adjusted",{"$f":"+K70","v":6.6759616356734073},6.6759616356734073]
[]
[]
[]
[]
[]
[]
[]
[null,"Min factor",{"$f":"+MIN(F3:G3)","v":0.95},{"$f":"+MIN(F4:G4)","v":0.95},{"$f":"+MIN(F5:G5)","v":0.95},{"$f":"+MIN(F6:G6)","v":0.95},{"$f":"+MIN(F7:G7)","v":0.95},{"$f":"+MIN(F8:G8)","v":0.95},{"$f":"+MIN(F9:G9)","v":0.95}]
[null,"Nominal factor",1,1,1,1,1,1,1]
[null,"Max factor",{"$f":"+MAX(F3:G3)","v":1.05},{"$f":"+MAX(F4:G4)","v":1.05},{"$f":"+MAX(F5:G5)","v":1.05},{"$f":"+MAX(F6:G6)","v":1.05},{"$f":"+MAX(F7:G7)","v":1.05},{"$f":"+MAX(F8:G8)","v":1.05},{"$f":"+MAX(F9:G9)","v":1.05}]
[]
[]
[null,"Variable",{"$f":"+MATCH(R12,C50:Y50,0)","v":9}]
[null,"Min",{"$f":"+MIN(OFFSET($B$251:$B$2250,0,C194))","v":6.6948808964962101}]
[null,"max",{"$f":"+MAX(OFFSET($B$251:$B$2250,0,C194))","v":6.8022060679148275}]
[null,"max-min",{"$f":"+C196-C195","v":0.10732517141861742}]
[null,"gain",{"$f":"+OFFSET(B199,0,C194)","v":1}]
[null,"gain",{"$f":"+C3","v":0.86},{"$f":"+C4","v":1500},{"$f":"+C5","v":0.08},{"$f":"+C6","v":1},{"$f":"+C7","v":1},{"$f":"+C8","v":2192779.8003413612},{"$f":"+C9","v":125607.29041291363},null,1,1,1,1,1,1,1,1,1,1,1,1,1,1]
[null,"Range to plot"]
[null,"Min","Max",null,"Min*gain","Max*gain","Average","Probability","Cumulative probability"]
[null,{"$f":"+C195","v":6.6948808964962101},{"$f":"+B202+($C$197/20)","v":6.7002471550671405},{"$f":"+COUNTIFS(OFFSET(B$251:B$2250,0,$C$194),\">=\"&$B202,\nOFFSET(B$251:B$2250,0,$C$194),\"<=\"&$C202)","v":3},{"$f":"+B202*$C$198","v":6.6948808964962101},{"$f":"+C202*$C$198","v":6.7002471550671405},{"$f":"+AVERAGE(E202:F202)","v":6.6975640257816753},{"$f":"+D202/$D$223","v":1.5E-3},{"$f":"+H202","v":1.5E-3}]
[null,{"$f":"+C202","v":6.7002471550671405},{"$f":"+B203+($C$197/20)","v":6.705613413638071},13,{"$f":"+B203*$C$198","v":6.7002471550671405},{"$f":"+C203*$C$198","v":6.705613413638071},{"$f":"+AVERAGE(E203:F203)","v":6.7029302843526057},{"$f":"+D203/$D$223","v":6.4999999999999997E-3},{"$f":"+I202+H203","v":8.0000000000000002E-3}]
[null,{"$f":"+C203","v":6.705613413638071},6.7109796722090014,34,6.705613413638071,6.7109796722090014,6.7082965429235362,1.7000000000000001E-2,{"$f":"+I203+H204","v":2.5000000000000001E-2}]
[null,6.7109796722090014,6.7163459307799318,61,6.7109796722090014,6.7163459307799318,6.7136628014944666,3.0499999999999999E-2,5.5500000000000001E-2]
[null,6.7163459307799318,6.7217121893508622,109,6.7163459307799318,6.7217121893508622,6.719029060065397,5.45E-2,0.11]
[null,6.7217121893508622,6.7270784479217927,134,6.7217121893508622,6.7270784479217927,6.7243953186363274,6.7000000000000004E-2,0.17699999999999999]
[null,6.7270784479217927,6.7324447064927231,180,6.7270784479217927,6.7324447064927231,6.7297615772072579,0.09,0.26700000000000002]
[null,6.7324447064927231,6.7378109650636535,203,6.7324447064927231,6.7378109650636535,6.7351278357781883,0.10150000000000001,0.36850000000000005]
[null,6.7378109650636535,6.7431772236345839,212,6.7378109650636535,6.7431772236345839,6.7404940943491187,0.106,0.47450000000000003]
[null,6.7431772236345839,6.7485434822055144,229,6.7431772236345839,6.7485434822055144,6.7458603529200492,0.1145,0.58900000000000008]
[null,6.7485434822055144,6.7539097407764448,235,6.7485434822055144,6.7539097407764448,6.7512266114909796,0.11749999999999999,0.70650000000000013]
[null,6.7539097407764448,6.7592759993473752,179,6.7539097407764448,6.7592759993473752,6.75659287006191,8.9499999999999996E-2,0.79600000000000015]
[null,6.7592759993473752,6.7646422579183056,132,6.7592759993473752,6.7646422579183056,6.7619591286328404,6.6000000000000003E-2,0.8620000000000001]
[null,6.7646422579183056,6.7700085164892361,106,6.7646422579183056,6.7700085164892361,6.7673253872037709,5.2999999999999999E-2,0.91500000000000015]
[null,6.7700085164892361,6.7753747750601665,63,6.7700085164892361,6.7753747750601665,6.7726916457747013,3.15E-2,0.94650000000000012]
[null,6.7753747750601665,6.7807410336310969,56,6.7753747750601665,6.7807410336310969,6.7780579043456317,2.8000000000000001E-2,0.97450000000000014]
[null,6.7807410336310969,6.7861072922020274,22,6.7807410336310969,6.7861072922020274,6.7834241629165621,1.0999999999999999E-2,0.98550000000000015]
[null,6.7861072922020274,6.7914735507729578,12,6.7861072922020274,6.7914735507729578,6.7887904214874926,6.0000000000000001E-3,0.99150000000000016]
[null,6.7914735507729578,6.7968398093438882,12,6.7914735507729578,6.7968398093438882,6.794156680058423,6.0000000000000001E-3,0.99750000000000016]
[null,6.7968398093438882,{"$f":"+B221+($C$197/20)+0.000001","v":6.8022070679148188},5,6.7968398093438882,6.8022070679148188,6.7995234386293539,2.5000000000000001E-3,1.0000000000000002]
[null,null,null,null,null,0,0]
[null,"Variable to plot",null,{"$f":"+SUM(D202:D221)","v":2000}]
[null,{"$f":"+TRANSPOSE(Sensitivity_output)","v":"Cost of hydrogen ($/kg)"}]
[null,"Revenue from byproduct sales ($/kg)"]
[null,"Salvage value ($/kg)"]
[null,"Initial equity depreciable capital ($/kg)"]
[null,"Yearly replacement costs ($/kg)"]
[null,"Cash from working capital reserve ($/kg)"]
[null,"Other non-depreciable capital costs ($/kg)"]
[null,"Decommissioning costs ($/kg)"]
[null,"Fixed operating cost ($/kg)"]
[null,"Feedstock cost ($/kg)"]
[null,"Other raw material cost ($/kg)"]
[null,"Other variable operating costs ($/kg)"]
[null,"Debt interest ($/kg)"]
[null,"Taxes ($/kg)"]
[null,"Principal payment ($/kg)"]
[null,{"$f":"+TRANSPOSE(C50:I50)","v":"Operating capacity factor"}]
[null,"Plant design capacity (kg of H2/day)"]
[null,"After-tax real IRR (%)"]
[null,"Feedstock consumption (% of most likely value)"]
[null,"Utilities consumption (% of most likely value)"]
[null,"Total capital investment ($)"]
[null,"Total fixed operating cost ($/year)"]
[]
[]
[null,null,{"$f":"+RAND()","v":0.31981488236913858},{"$f":"+RAND()","v":0.40880350960803991},0.16434606911667282,0.18697075843704847,0.94734197791491537,0.62604012458968539,0.52552158635550639]
[null,null,{"$f":"IFERROR(IF(C$248<=(C$190-C$189)/(C$191-C$189),C$189+SQRT(C$248*(C$191-C$189)*(C$190-C$189)),C$191-SQRT((1-C$248)*(C$191-C$189)*(C$191-C$190))),1)","v":0.98998842847431856},{"$f":"IFERROR(IF(D$248<=(D$190-D$189)/(D$191-D$189),D$189+SQRT(D$248*(D$191-D$189)*(D$190-D$189)),D$191-SQRT((1-D$248)*(D$191-D$189)*(D$191-D$190))),1)","v":0.99521081229131148},0.97866583934901197,0.98057537885595603,1.033773783237445,1.0067588231305904,1.0012927924407233]
[]
[null,1,0.98224588310145378,1.0269308714891683,1.0042726933527857,0.99289844267369454,1.0266140805115191,1.037232385691566,1.0380273719048421,null,6.7776891609079062,0,1.0840851814633677E-2,0.20339820773486916,0.1227939473263867,8.3677665455081457E-2,0,1.0840851814633677E-2,0.28872415386265438,5.9115085244410368,0,1.925363191278107E-2,0.10682796963841808,-3.1356376362951053E-3,4.4640698172970901E-2]
[null,2,0.99899214327333963,1.0107253781616941,0.96047677023867084,1.0088874793118841,1.0052334839531387,0.95732922033758172,0.99395119046916758,null,6.7215911909989003,0,1.0290746845011344E-2,0.18093204141373803,0.12231714431429627,8.0637558297921644E-2,0,1.0290746845011344E-2,0.26447047651542804,5.9147909821625255,0,1.9160593651570086E-2,9.7133244691212511E-2,-2.2631387089748104E-4,4.2375463823100618E-2]
[null,3,0.98650213666886599,0.97477363336145562,0.97124956779601523,1.0075202622514554,0.98918788445137718,1.0009712640726143,0.97350987777223963,null,6.7498393446671816,0,1.0963232293947571E-2,0.19586461626753254,0.12547006898058585,8.1339085450131229E-2,0,1.0963232293947571E-2,0.26673572633013237,5.9141321883951976,0,1.9229685785487793E-2,0.10458086084548193,-2.6575265912421125E-3,4.5144639203872232E-2]
[null,4,1.0171364224020421,0.98461573555736948,0.99503829397741372,0.99074469051094305,1.0033402511309932,0.99484554766041389,1.025626296599655,null,6.7392114629736639,0,1.0306539738260756E-2,0.19074582390771866,0.12076573127710971,8.2873918738019844E-2,0,1.0306539738260756E-2,0.27189930029137388,5.9119108542554901,0,1.9063246223797833E-2,0.10064330662159761,-1.1312144879131365E-3,4.2440496146471482E-2]
[null,5,1.0196604395962314,0.99508030058619246,0.99344428145332209,1.014439900476741,1.0163174900051051,1.000079636199493,0.96383369552268539,null,6.7220296731587164,0,1.0302734116228937E-2,0.19022545186491863,0.11998771024174473,8.2569747515399264E-2,0,1.0302734116228937E-2,0.25524932044244952,5.9132805993884299,0,1.9049978892503198E-2,0.10044841723718526,-1.2063776962364606E-3,4.242482527231993E-2]
[null,6,1.01658206612472,1.0108746946579958,1.0408944864221192,1.0180214080571948,1.0037722090606265,0.96910504620237214,0.97728391380239854,null,6.7171458432549898,0,9.5419605515939601E-3,0.18899243808935753,0.11871735549866727,8.5524242927008109E-2,0,9.5419605515939601E-3,0.25672851193870788,5.9107619311206339,0,1.9066168985181133E-2,9.748907339251571E-2,5.7402615711820955E-4,3.9292095145799621E-2]
[null,7,0.99874715157781058,1.0147421077610492,1.0235627539392922,0.99792613503771843,0.9983706555283115,0.98942609481038679,1.0325206824252666,null,6.7491582081700692,0,1.0051370791189793E-2,0.19404722579287403,0.12098110102653352,8.473228993026799E-2,0,1.0051370791189793E-2,0.27798696014210705,5.9106813283774526,0,1.9161932279178898E-2,0.10095045567782361,-7.7284089697884516E-4,4.1389755840812704E-2]
[null,8,1.0145685872694479,1.0349958404763819,1.0012694501804398,1.0248191869397312,0.98437039393592007,1.0204529327388105,0.96828311777502052,null,6.7284063339915248,0,1.0318233591218366E-2,0.19273348813811234,0.1185652789237558,8.3115149282958517E-2,0,1.0318233591218366E-2,0.25917245305499953,5.9134027963462801,0,1.9076811622404721E-2,0.10137761189352368,-1.5259046220317219E-3,4.2488649351522682E-2]
[null,9,1.0329490510576822,0.99807034037995779,1.0288336505423326,0.98467124444486576,0.99778992813379785,0.99115944286203561,1.0186936229027101,null,6.7252310117536824,0,9.7597242668880022E-3,0.1898910144015846,0.11765612331504877,8.4875488595750448E-2,0,9.7597242668880022E-3,0.265507215389641,5.9096615078563124,0,1.898119746682984E-2,9.8532727338017545E-2,-6.3069974388933053E-5,4.0188807364884102E-2]
[null,10,1.0340693604090927,0.98042558811387148,1.0035585199861896,0.96554741481336326,1.0245246237383323,0.99395536264332018,1.0293677217196608,null,6.7284381543722231,0,1.0071989700450845E-2,0.18877288857607721,0.11883542195414852,8.3336575601449886E-2,0,1.0071989700450845E-2,0.26839650402293369,5.9100707715159899,0,1.8975479581638352E-2,9.9181635250254863E-2,-6.0578296939824779E-4,4.1474660839120672E-2]
[null,11,1.0160536525181996,0.95168519613949165,1.0060727593654197,1.0013225119739033,1.032925719463659,1.0275326350692273,0.98899274928513281,null,6.7511268844799117,0,1.0709382037593125E-2,0.2014678921875509,0.1223430269920457,8.3486138025412909E-2,0,1.0709382037593125E-2,0.26590257661245525,5.9118620722020889,0,1.9068957936590223E-2,0.10571978399230329,-2.8228925004035533E-3,4.4099329031865878E-2]
[null,12,1.0305835549038325,0.9796216223782076,0.96497723587105233,1.0207914799142002,0.98687027838928443,1.0105198636632302,1.0144660469167748,null,6.7330285710594273,0,1.0629780788415094E-2,0.18814665867910843,0.11997839506921119,8.0956270411852244E-2,0,1.0629780788415094E-2,0.26689932684268663,5.9151911274877733,0,1.8993311428024351E-2,0.10077744306109619,-1.6855071765676543E-3,4.3771545256244937E-2]
[null,13,1.0010119551078751,0.97724693811320917,0.96705899065379786,1.0102730676576117,1.0406018385855413,0.96342749128147465,1.013065821606975,null,6.7346268317093854,0,1.0425753164369885E-2,0.18510681982284818,0.1236040627617255,8.111997716345612E-2,0,1.0425753164369885E-2,0.26989917459741741,5.9145093248948672,0,1.9149582427088221E-2,9.9045320166555748E-2,-7.3882594055888157E-4,4.2931395815990044E-2]
[null,14,0.96037077786514513,0.97494577315666153,1.0082705965778955,1.025606396641507,1.0126025625787278,0.97250214369242138,0.95727094869979135,null,6.7573375107298173,0,1.059264322182191E-2,0.19992132062934637,0.1281488642472208,8.3656036937510281E-2,0,1.059264322182191E-2,0.26678022653776134,5.9130498740371236,0,1.9380052277196705E-2,0.10479411201183492,-2.0115953154317885E-3,4.3618619367254627E-2]
[null,15,1.0321268026561661,1.0113817828184757,0.98623983751874356,1.0113899261884389,0.9930651016011155,0.99232577479221529,1.0404550786039843,null,6.7273269820577193,0,1.0092590526639267E-2,0.18436562994005992,0.11790006096278584,8.2332585156685248E-2,0,1.0092590526639267E-2,0.27130439686331487,5.9135166323742201,0,1.8985401993597724E-2,9.7704550729717163E-2,-3.4176733721479323E-4,4.1559491374554232E-2]
[null,16,1.0048496784518159,0.980462155622434,0.98646461453643619,1.0115826165094588,1.037904178282552,0.98231755348768535,1.0322676021193953,null,6.74584509506216,0,1.0397371418094988E-2,0.18999651457660702,0.1226097043323514,8.2408389671939877E-2,0,1.0397371418094988E-2,0.27581224108471958,5.9135145846379116,0,1.9128782618293202E-2,0.100677335298966,-1.1169819952233954E-3,4.2814524836592552E-2]
[null,17,1.0084581829183072,0.99357330416302803,1.0048527837108776,0.99932651775610803,0.99017955557719883,0.98303686303318316,1.0049197799245166,null,6.7346238481980478,0,1.0144708286681242E-2,0.19050061438322449,0.12118168711116242,8.3431299132374417E-2,0,1.0144708286681242E-2,0.26751579326884201,5.9118231442582072,0,1.9109369544919971E-2,0.10002518176425669,-7.3734429873806469E-4,4.1774103033791629E-2]
[null,18,0.9877954976954485,0.99711322185908147,1.0290972978886415,0.98902612880905372,0.98983252128179189,1.0151638718223799,1.0058975011253872,null,6.763500193055517,0,1.0454907279273033E-2,0.20349620726466128,0.12307650429622156,8.5048445352306587E-2,0,1.0454907279273033E-2,0.27647386858777584,5.9098815158017626,0,1.9222450082385528E-2,0.1055786762946362,-2.3289218961544422E-3,4.3051447271922207E-2]
[null,19,1.020459998380832,0.99246161296916291,0.98016253487893223,0.97409803764052583,0.9883419485650059,0.95897794823652383,1.0101227202857914,null,6.7150584149951467,0,9.9978822081548853E-3,0.18099655976053947,0.12026320819389795,8.1824804738853563E-2,0,9.9978822081548853E-3,0.26345509927033212,5.9118365457155351,0,1.9045789752404067E-2,9.6211052554177071E-2,2.5585563292170662E-4,4.1169499376487832E-2]
[null,20,0.99581428139797834,0.9886126274941931,1.0077984836660849,0.98684590101556513,1.0097410691869202,1.0424852348195244,1.018372991867559,null,6.7716781075197048,0,1.0890109994485458E-2,0.20539196844011412,0.12291042669894127,8.3778775423580434E-2,0,1.0890109994485458E-2,0.28035273265821964,5.9109821640768123,0,1.9178008537526402E-2,0.10768686186707907,-3.4463647725407691E-3,4.4843534589971382E-2]
[null,21,1.0407822043875739,0.9820969447715292,1.0109013295838802,0.99713488133758621,1.0150771567728027,1.0471921656228247,1.0064284164244266,null,6.7404646164541271,0,1.0467900528632218E-2,0.19833792478665407,0.11785491474106996,8.3776577675228878E-2,0,1.0467900528632218E-2,0.26560889767523344,5.911362163047964,0,1.894147612511193E-2,0.10382892129816072,-2.351210055369285E-3,4.3104951160071146E-2]
[null,22,1.0379540424530462,1.0001860833474663,0.97759896798217638,0.99136315787746809,1.0377585619292984,1.0336592224447658,1.0062613999395553,null,6.7303182849446932,0,1.0583336028336554E-2,0.190867905894686,0.11791594497697717,8.1693863626084717E-2,0,1.0583336028336554E-2,0.26478033824857566,5.9129109190993558,0,1.8955748371385597E-2,0.10158866923674016,-1.9753985102147651E-3,4.3580294001100611E-2]
[null,23,1.0427493278513258,1.0422471006340872,1.0161397659405482,0.97937785896246987,1.0104337635712803,0.98894668746731818,1.021567525583005,null,6.7094370284280949,0,9.5750928778491635E-3,0.18283368263185956,0.11477534490496775,8.4054308531205907E-2,0,9.5750928778491635E-3,0.2631442224117439,5.910104470691147,0,1.8931594738690095E-2,9.5465214599146753E-2,6.9966175134428136E-4,3.9428528167984325E-2]
[null,24,0.99624756508982937,1.0258096960630911,0.98694004851734285,1.0054404800816152,0.99005314904982233,1.0317624256176672,1.0143083629515004,null,6.7577411311530113,0,1.0799299233749084E-2,0.19748033091764922,0.12144309410743842,8.2458253994125943E-2,0,1.0799299233749084E-2,0.27762374722615746,5.9131562069795081,0,1.917562757390006E-2,0.10461809835984068,-2.6838200465870692E-3,4.4469592040971832E-2]
[null,25,1.0026080903752077,1.0366461834004583,0.98803071998388836,0.96090811688396549,1.03336832362416,0.99626490416672109,0.98481815924058602,null,6.726871462093972,0,1.0305310263674013E-2,0.18875207352483706,0.12014652151516257,8.2319577123648208E-2,0,1.0305310263674013E-2,0.26449963797415021,5.9106885622321066,0,1.9140912303951072E-2,9.9939749970903921E-2,-1.0510059397518439E-3,4.2435433388961587E-2]
[null,26,0.99672707002910355,0.99145575635689098,1.0026431522572374,0.99392915389386749,1.0016262521981683,1.0224049280328495,1.0348699424599104,null,6.7668621738968016,0,1.0705573981789212E-2,0.20037590358468121,0.12275439141097057,8.3493904499213206E-2,0,1.0705573981789212E-2,0.28261561937983398,5.9116561063350694,0,1.9172995030135889E-2,0.10532569128974761,-2.6160857687212188E-3,4.408364813587403E-2]
[null,27,1.000820031395508,1.0254658575506839,0.97295502129032008,1.0226037545076301,0.97947299065589644,0.98585407897254052,1.0113660417056507,null,6.7353964911087481,0,1.0399109040112943E-2,0.18625719640184024,0.12116116534808209,8.15137195431372E-2,0,1.0399109040112943E-2,0.27120721593570568,5.914854499034873,0,1.9150626809196374E-2,9.9365867422941526E-2,-9.3547944180401321E-4,4.2821680054777281E-2]
[null,28,0.9748126635301827,1.0176557501916101,1.0073241046916801,1.0194283473504417,1.0166901151889143,0.97526338041110527,0.99378780442178571,null,6.7493001084083888,0,1.0283388133500212E-2,0.19381276375266523,0.12412172829186746,8.3671786598646519E-2,0,1.0283388133500212E-2,0.27272207310102126,5.9127696561021494,0,1.9295953468436659E-2,0.10163976206773889,-1.0787769330372699E-3,4.2345161958899605E-2]
[null,29,0.99960460712079779,1.0006853478429316,0.98991865845813576,0.99337183373190963,1.0336233723977981,1.0114019860166485,0.99084230693407571,null,6.7451915311064132,0,1.0635562399018396E-2,0.1953470290070948,0.12218623863964727,8.2515709483631475E-2,0,1.0635562399018396E-2,0.26866221435051557,5.9123383912286291,0,1.9157250037243018E-2,0.10333425161330999,-2.1449061532835224E-3,4.3795352899621012E-2]
[null,30,0.99109407836271601,1.0108502916584146,1.0016547655918659,0.98477696006323145,0.97761947663313986,1.0061767713047312,0.97233983611265251,null,6.7427342024696344,0,1.0517057768121904E-2,0.19655946896066465,0.12251775693596607,8.3194561119046384E-2,0,1.0517057768121904E-2,0.26534584020685853,5.9112171695798468,0,1.9204081686683486E-2,0.10337030269310006,-1.9823506351571221E-3,4.3307371922627243E-2]
[null,31,1.0023942682449203,1.0212738055814985,0.99851196002832521,0.99690255817593432,1.0212239844450548,1.0458448574218135,0.99437915883697015,null,6.7547336508109472,0,1.0790677965618958E-2,0.20073651324859007,0.12069878314605555,8.3094876097773565E-2,0,1.0790677965618958E-2,0.27187184385922697,5.9120490821808076,0,1.9142072172877635E-2,0.10573189794122537,-3.0255090289522586E-3,4.4434091193340505E-2]
[null,32,1.0194781796503851,1.0175774706727767,1.0004930286064309,0.97938808570384694,1.0194622363678356,1.0298143891772404,0.98903991642045841,null,6.7349182966075158,0,1.0445362136594591E-2,0.19488383214824118,0.11881226800387092,8.3104803740541466E-2,0,1.0445362136594591E-2,0.26446871336124,5.9109912856047284,0,1.9050934729360598E-2,0.10254821102942535,-1.953894083243072E-3,4.3012142073344438E-2]
[null,33,0.97881452262421953,1.0258821503980493,1.0152258842922954,0.98961069592282236,1.0041135425251453,1.019359770715992,0.98967755667436597,null,6.7604464546940246,0,1.0594114054502259E-2,0.20201822330822525,0.12306625624612073,8.4164957417511801E-2,0,1.0594114054502259E-2,0.27458616586543116,5.9107094830008053,0,1.9273088728435282E-2,0.10552985604470223,-2.5262519116468706E-3,4.3624675994433849E-2]
[null,34,1.0111508590308478,1.021441853192369,0.97630235231550699,0.98959427555462676,1.0088145540680116,0.98872453472205946,0.99152948269506014,null,6.7231723767750102,0,1.0310107356196804E-2,0.1855828510451755,0.12005128054998816,8.1596530022960065E-2,0,1.0310107356196804E-2,0.26347381708086542,5.9128864761288504,0,1.9094973728188785E-2,9.8839949075444591E-2,-8.0868781858685465E-4,4.2455186962119813E-2]
[null,35,0.98175881600148429,0.97267084958946326,1.002054240562529,0.96916564377555303,1.0022761431692351,0.98156398183000138,1.0209429233304028,null,6.7597728036286879,0,1.0525948099053252E-2,0.19684206916476985,0.12559455448323634,8.3395139121224413E-2,0,1.0525948099053252E-2,0.27923760136409753,5.9103510333919216,0,1.9256385442759354E-2,0.10349840186117196,-1.7463619234724167E-3,4.3343980722982609E-2]
[null,36,1.0155051435646758,1.0226391075766981,1.0402905543045724,0.98759074920836687,0.98604682156142565,1.0291062283600541,1.0069169598499761,null,6.7453937508834105,0,1.0098722366287954E-2,0.1998415728055728,0.11830574058482983,8.5651196143166713E-2,0,1.0098722366287954E-2,0.27025306272177246,5.9091537151454574,0,1.907185602075083E-2,0.10311586090306257,-1.5839946400057158E-3,4.1584741198800769E-2]
[null,37,0.95888957442789202,1.019635658787748,0.97379822608871702,1.0351277379821466,0.98732762385084682,0.9919156041850925,1.0086259895796263,null,6.7696594069895806,0,1.0939219814579185E-2,0.19617644853230728,0.12673191955485164,8.1732524327703421E-2,0,1.0939219814579185E-2,0.28295022718689766,5.9154854631348401,0,1.9388820936947614E-2,0.10461336644386293,-2.465123215724205E-3,4.5045760087895223E-2]
[null,38,1.0095966152808631,1.0130828173352229,0.99344880196454466,1.0188701451817801,0.96972802534382485,1.0064103583803272,1.0057226558471186,null,6.7396297823584854,0,1.0391165514391242E-2,0.19185949839898986,0.12031767117037813,8.2762731903521097E-2,0,1.0391165514391242E-2,0.26941185117207384,5.913519794119396,0,1.9103273790056371E-2,0.10131104631292995,-1.4450545386045866E-3,4.2788970029750198E-2]
[null,39,1.0053681387240865,1.0042838524136763,0.98732154955837403,0.98073990495527297,1.0133011889337256,0.97356719289135063,0.98728473835417063,null,6.7237036236286638,0,1.0186433199234981E-2,0.18637862544075107,0.12135952477700147,8.2264663561767426E-2,0,1.0186433199234981E-2,0.26262619733394016,5.9117998848879196,0,1.9125984827034846E-2,9.8718003095421822E-2,-5.1517909209917556E-4,4.1945918796930333E-2]
[null,40,1.0080043525999276,0.98431384934481814,1.0445218902069431,0.98755093248205428,0.9751176668682161,1.0038979541098725,1.0431208664579483,null,6.7583592636285195,0,1.0050953655084436E-2,0.20014308518545099,0.12094035875637935,8.604792835366272E-2,0,1.0050953655084436E-2,0.28002328311084163,5.9089039790484454,0,1.9111803425385598E-2,0.10305836594900628,-1.2575783492276725E-3,4.1388038148578318E-2]
[null,41,0.98930519450713017,0.99221278113085321,0.99002852220101634,1.0070924497709157,1.0239730862680714,1.0065732116231898,0.97957067392057529,null,6.7499657766156629,0,1.0732977458544457E-2,0.19716839745951237,0.12387682443667565,8.2524443654704835E-2,0,1.0732977458544457E-2,0.26800807642976315,5.9130738951253541,0,1.921402802013553E-2,0.10429200127925084,-2.3883805652536705E-3,4.4196490775515102E-2]
[null,42,0.96895941176369471,1.0052935905896605,0.99959810965719353,0.99697455791423473,0.96650922038141629,0.97566709011632191,1.027631463070213,null,6.7637158343835093,0,1.0474572050137191E-2,0.19516988656876136,0.12563283911969783,8.3325369895314305E-2,0,1.0474572050137191E-2,0.28385246464648456,5.911991992226433,0,1.9329736335016071E-2,0.1027443867999394,-1.4632645062789247E-3,4.313242329814207E-2]
[null,43,0.98721352503219384,1.0253778160863229,0.9881094133058993,1.0291073444449346,0.99010929011676752,0.99637248242055954,0.99615334319936177,null,6.7467497680011137,0,1.051547733168786E-2,0.19262396893490993,0.12255322832917716,8.2471742807040158E-2,0,1.051547733168786E-2,0.27182611207804497,5.914370559208125,0,1.9225703579959251E-2,0.1019858214929581,-1.6082323958013583E-3,4.3300863966699035E-2]
[null,44,1.0287942466476501,1.0083914687066939,0.99642690031083336,0.97622865464516695,1.0253317457119415,1.0116155570105518,1.0095914719356784,null,6.7282735436476999,0,1.0243723521852441E-2,0.18997380246123738,0.11823799058500066,8.2869194683572137E-2,0,1.0243723521852441E-2,0.26593185283416287,5.9110486259300421,0,1.9002511674702488E-2,0.10016674225480776,-1.1390069239943605E-3,4.2181830148171763E-2]
[null,45,1.0093048710750503,0.98601729980384178,1.0099285233073181,1.0454390079381077,1.0234249937856923,1.0136858714130514,1.0038294230289313,null,6.750304296982935,0,1.0440037438596996E-2,0.19752533796798188,0.12135521583502701,8.381263598294951E-2,0,1.0440037438596996E-2,0.26997392950932897,5.9140274672732165,0,1.9104834628759164E-2,0.10345329318268891,-1.9386333117726567E-3,4.2990215914751259E-2]
[null,46,1.006135227470536,1.0299009304550109,0.97152445201989512,1.0195992484769743,1.0146743634013295,1.0347950586996852,0.97879194572303452,null,6.7406009137637763,0,1.0851171026257428E-2,0.19394170720058915,0.12033920151456157,8.1346865658644463E-2,0,1.0851171026257428E-2,0.26547765597135992,5.9147702550544734,0,1.9121850639439004E-2,0.10353983166962419,-2.6196447946035557E-3,4.4683190849686319E-2]
[null,47,1.0113572207534012,0.98947532073395728,0.98156675388399917,1.0356682812833145,0.98966874681561201,1.0280354147525201,1.0188639328509781,null,6.7548344588064246,0,1.0815036919727643E-2,0.19619822169787093,0.12146611758233865,8.2105792603771086E-2,0,1.0815036919727643E-2,0.27474226642522587,5.9150875563395644,0,1.9093873621891525E-2,0.10421841527228688,-2.6121817671567872E-3,4.4534397030627858E-2]
[null,48,0.98555636574482575,0.96726074356211622,1.0162146211242917,1.0359677475466746,0.99177094764930029,0.99102149550718488,1.0206994571931849,null,6.7668294184417821,0,1.0481180500923405E-2,0.20015733775994582,0.1251160087962426,8.432106142276187E-2,0,1.0481180500923405E-2,0.2791153122300481,5.9131576839556432,0,1.9234988918274305E-2,0.10450676957036727,-1.9393799337219409E-3,4.3159635722219314E-2]
[null,49,1.0173974344905856,1.0229577028225689,0.98940450388752044,1.0117488973313977,1.0255914389464658,1.0118776374285854,0.99375321508227243,null,6.7305183433434985,0,1.0361059092632857E-2,0.19016011922901427,0.11900629231692318,8.2441184495843436E-2,0,1.0361059092632857E-2,0.26456333304213708,5.9133603001390584,0,1.9061871179091507E-2,0.10061628870889974,-1.3560429111641686E-3,4.2664997143692471E-2]
[null,50,1.0201557134335781,1.0140100051643688,1.0055451989407787,1.0116428868665139,0.9947579778465202,0.99654437050548994,0.96601592123809421,null,6.7183277049757697,0,1.0071825882433922E-2,0.18932604147026263,0.11880785072067018,8.3317083005028506E-2,0,1.0071825882433922E-2,0.25523248396018866,5.9124495830553823,0,1.9047383223015916E-2,9.9374348904017071E-2,-7.0105562848303017E-4,4.147398626568552E-2]
[null,51,0.99243219925996773,1.031430916278073,0.98380062649240019,0.98684664476143424,0.98870403198038737,0.99953794231129811,1.0013427870013258,null,6.7418605092818442,0,1.0506432005006519E-2,0.19123238102193285,0.12170191487675551,8.2175749562458086E-2,0,1.0506432005006519E-2,0.27204084128778472,5.9123249743671149,0,1.9196665072858853E-2,0.10146718115207862,-1.5428149805740725E-3,4.3263616921433413E-2]
[null,52,1.0285402661228522,1.0041773201504547,0.99422756608271523,0.98382326705021561,1.0017122636711036,1.0117461561789303,1.0037443093178511,null,6.7279331032093568,0,1.0285701738759768E-2,0.19013157855192098,0.11850538061769443,8.2719151865545529E-2,0,1.0285701738759768E-2,0.2645073913189645,5.9115820816789109,0,1.9003820183454825E-2,0.10035970092267719,-1.2306909033634971E-3,4.235468897355206E-2]
[null,53,0.98162651885464869,0.99998294249715636,0.96826421323029188,1.0088708016404002,0.98972742866374097,0.9882423048786827,0.97955328367479044,null,6.7448280717320515,0,1.0787211714698404E-2,0.19186753003319568,0.12486814782969063,8.1174145571337092E-2,0,1.0787211714698404E-2,0.26825765027123288,5.9143679466068502,0,1.9257133828366968E-2,0.10260053315286868,-1.9848333505146265E-3,4.4419817789019322E-2]
[null,54,1.0261677866889141,0.99297216887005757,1.0275170632633277,0.97380099749719429,1.04221719898078,1.0121203467365552,0.99684137315266719,null,6.7323673524914263,0,1.0065618959006673E-2,0.1954618591498834,0.1187009206256725,8.4759201351638586E-2,0,1.0065618959006673E-2,0.26350067760768536,5.9091503216906638,0,1.9016074492301065E-2,0.10148896754983623,-1.1590972360573395E-3,4.14484272598033E-2]
[null,55,0.97025508641818947,0.9933539432352414,0.99360677937640896,1.0111687421043252,0.97314154526734331,1.0206092266748759,1.0139736616014263,null,6.7799025924666045,0,1.1056266594143325E-2,0.20418753939122475,0.12618195578179761,8.2967737866098054E-2,0,1.1056266594143325E-2,0.28424805253510782,5.9130947235283102,0,1.9322223039159665E-2,0.10781236375064185,-3.4397413183233656E-3,4.552773789259023E-2]
[null,56,1.0206477224163577,1.0273492325060645,0.98090837999552472,1.0086449759411298,1.0040774882813606,1.0034946689718216,1.0039826301074082,null,6.7261280419933032,0,1.0299779960412826E-2,0.18666840657792189,0.11857741989455937,8.1924277542268234E-2,0,1.0299779960412826E-2,0.26561142316041708,5.9136630323169923,0,1.9044807158497202E-2,9.9188954660236694E-2,-9.6293990208348094E-4,4.2412660584489302E-2]
[null,57,1.0068516042943778,1.0172150589963878,1.0061530525749482,1.0200963915414065,1.0347010799291567,0.98612065382505953,1.0161603196250435,null,6.7368733323119319,0,1.007917961083004E-2,0.18963489382801282,0.1202146004766077,8.3574228597376288E-2,0,1.007917961083004E-2,0.27101523417709439,5.9128720245729909,0,1.9117995449795009E-2,9.9506488891420497E-2,-5.6640129167637209E-4,4.1504267610305873E-2]
[null,58,0.95970475364368002,0.99751525782120676,1.0412571605753949,0.98790454183923604,1.0134674078934995,0.98389152484014697,1.0483844449748325,null,6.7849440943987762,0,1.0317035027139791E-2,0.20445340715507304,0.12641694915667614,8.6034853470557823E-2,0,1.0317035027139791E-2,0.29337956514771862,5.9091141891405554,0,1.9383991762473265E-2,0.10544571713300954,-1.7682924452700826E-3,4.2483713877983588E-2]
[null,59,1.0296387243622607,1.0295823620309452,0.97021890134233491,0.98621662319796422,0.98062883812700108,0.99187121255357447,1.004130887101677,null,6.713148548848114,0,1.0176542234534174E-2,0.18153193563100503,0.11762992885422865,8.1197836372507881E-2,0,1.0176542234534174E-2,0.26223807584341469,5.9130365772742328,0,1.899816556344798E-2,9.6978226934162498E-2,-3.6738718970199467E-4,4.1905189564818521E-2]
[null,60,0.96243893423029014,1.0063625156738609,0.98576776986639547,0.98841663360440102,1.00434222254362,0.98577729789620849,0.99123829353770188,null,6.7605720330342205,0,1.0779311721452267E-2,0.19677245141026292,0.12669789148250454,8.2362016714961753E-2,0,1.0779311721452267E-2,0.27659977301081035,5.9123009796911852,0,1.9367854033890391E-2,0.10430413569384363,-2.2203560262180257E-3,4.438728702297811E-2]
[null,61,0.96421442443147654,0.96356415415428875,1.0056033379247966,0.98483583109858897,0.97602918440571196,1.0326682933148847,1.0142034983423311,null,6.7956211701178351,0,1.1285987171213778E-2,0.21216761217715538,0.12829175372581575,8.3742183587838095E-2,0,1.1285987171213778E-2,0.28769682932901097,5.910997700301917,0,1.9357423716761673E-2,0.11136033254101453,-4.466351601909134E-3,4.6473686340227909E-2]
[null,62,1.0279148814907477,1.0039507181490999,0.96829866609398674,0.97857927923072174,1.0135140759192185,0.99832465143459637,0.99747265274679064,null,6.7189901228385951,0,1.038860169184383E-2,0.18478707745069531,0.11905581844224973,8.1066523275630908E-2,0,1.038860169184383E-2,0.26174817203685663,5.9127282113051907,0,1.9007044924117221E-2,9.8812571522370191E-2,-9.9370878336355788E-4,4.2778412664843349E-2]
[null,63,0.9798029612998137,1.0008889108497194,1.0057763842935128,1.0209282795457435,0.99694389279407292,1.036673682837713,0.96439009210460891,null,6.7652303619284524,0,1.0967701808036308E-2,0.20623694254726535,0.12434259486415915,8.3528282667212905E-2,0,1.0967701808036308E-2,0.26914330271767978,5.9129382774361341,0,1.9267470018412516E-2,0.10823822340073581,-3.6277755904916835E-3,4.5163043867345792E-2]
[null,64,0.97186501426172511,0.98527384095447879,1.0212993539551685,1.0102698111342063,0.98705463206194743,1.0247449518061602,1.0166194910052879,null,6.7853332938796056,0,1.0855505129695159E-2,0.20887108691990858,0.12584610591857762,8.4699679318185644E-2,0,1.0855505129695159E-2,0.28507351541964265,5.9114781863972174,0,1.931291537775796E-2,0.10878346854342132,-3.4327019313134585E-3,4.4701037916201232E-2]
[null,65,1.0118449573027088,1.0005823021906268,1.0227577175482081,0.99573543433375733,0.99965281326398858,0.9957765540379957,1.0047589182552643,null,6.7373154512976265,0,1.0052285203763606E-2,0.19383396211255746,0.12010324968700191,8.4540137515263292E-2,0,1.0052285203763606E-2,0.26773490407076261,5.9106092485381634,0,1.9091275300964463E-2,0.10087945292381664,-8.7030007994018334E-4,4.1393521229032303E-2]
[null,66,0.9815569863853425,0.99323052859340233,0.98165130156838454,0.98819243223569575,0.99321348670264142,1.0320002846207579,1.0197395714270991,null,6.7752005666843029,0,1.116739673359847E-2,0.20261587884085758,0.12496275709300565,8.2197334126994398E-2,0,1.116739673359847E-2,0.28367152760489117,5.9125164194561064,0,1.9257527244253083E-2,0.10762285351530874,-3.6290832235518961E-3,4.5985352026439059E-2]
[null,67,1.0212582458534722,0.96628806417953839,1.0127015924059746,0.97995505135900363,1.0051779762467488,1.0076521200016457,0.9968738129794209,null,6.7382101134653363,0,1.0320622943419086E-2,0.19606919490168448,0.12085651738026677,8.3863597308736354E-2,0,1.0320622943419086E-2,0.264627840829744,5.9103315607907136,0,1.9041614026037462E-2,0.10254996580487651,-1.6286658553259184E-3,4.2498488278596411E-2]
[null,68,0.99389746880182006,0.99228548400601091,0.99132693384175719,1.009104146833868,1.0248568253787604,0.99810106640933083,0.97811799844826086,null,6.7430983121386863,0,1.058113716204348E-2,0.19475356121145893,0.12327639551204836,8.2574038560684321E-2,0,1.058113716204348E-2,0.26558706159455459,5.9131103237883575,0,1.9188566637274113E-2,0.10294801693674248,-1.9108915635275405E-3,4.3571239461089366E-2]
[null,69,1.0026157152747774,0.99440924362635386,0.95955201570487858,0.98475906797536772,1.0247115000168165,1.0119496563643184,0.9831998913847253,null,6.7391475065139739,0,1.0923162633112406E-2,0.19178747199868151,0.12268803827244405,8.0580617212619179E-2,0,1.0923162633112406E-2,0.26585391104393652,5.9135360783065414,0,1.9140870952147476E-2,0.10300905213539772,-2.428172880482408E-3,4.497963947268678E-2]
[null,70,1.0208575847736956,0.989514243896776,1.0389810494029235,0.98071547645260448,1.0000869172038807,0.99159421342870979,1.0018590252732715,null,6.7313737519903638,0,9.8283317589636238E-3,0.19411502227733698,0.11927034432897839,8.5483535775986164E-2,0,9.8283317589636238E-3,0.26435290407837564,5.9088588113833653,0,1.9043709114967292E-2,0.10022514325078666,-4.4703902500403252E-4,4.0471320805573155E-2]
[null,71,0.98576602275554182,0.99017030289246666,1.0237674383963846,1.0029311649277994,1.010943948573837,1.0111552929666368,1.0045000107995921,null,6.7646395241856823,0,1.0515332351458673E-2,0.2030657180005267,0.12377806838669139,8.47271517557803E-2,0,1.0515332351458673E-2,0.27633887761364545,5.9109399423297821,0,1.9233812450276448E-2,0.10563156974589136,-2.3758830608382074E-3,4.3300266963920767E-2]
[null,72,0.99587784753701425,0.98736184893713475,0.98953204509955051,0.99450812911403408,0.97552571700956436,1.0250768439473203,0.97121052301272981,null,6.7504712759266674,0,1.0885682168246353E-2,0.19982649201515548,0.12331008022558725,8.245374474126016E-2,0,1.0885682168246353E-2,0.26572687745538065,5.912421313845563,0,1.9177659101681864E-2,0.10572417137072472,-2.9943644183301949E-3,4.482530158964243E-2]
[null,73,1.0317234908130455,1.0209730081989241,0.97061326519482582,1.0057360466581839,1.0163746572966335,0.97513418703072274,1.0012130050342789,null,6.7072818789587583,0,1.0017106481196457E-2,0.17879253419397803,0.11778020497449222,8.1200259190828919E-2,0,1.0017106481196457E-2,0.2595045845946658,5.9140704473062087,0,1.8987466758651241E-2,9.5495847631746886E-2,2.0187279710130008E-4,4.1248661511079976E-2]
[null,74,1.0417515786649993,1.0103959962827223,0.97191491135136587,1.0265136592640614,0.99358165415454824,1.012593802409913,1.0200294891597872,null,6.7229851377702099,0,1.0336084401497851E-2,0.18484274158329142,0.11711034811624775,8.1372232503504685E-2,0,1.0336084401497851E-2,0.26536809969672454,5.9151227634174077,0,1.8936602035526173E-2,9.8662802239859695E-2,-9.9260763327708675E-4,4.2562155810927815E-2]
[null,75,1.0191278713786476,0.96528220989639191,1.0252449229722036,1.0300277099680277,0.99293838974784898,1.0023728067901652,0.9916093813099115,null,6.740257447255229,0,1.0180214501336774E-2,0.1970241334845256,0.12092358471907569,8.4658378598276948E-2,0,1.0180214501336774E-2,0.26332146910984666,5.9123186960256033,0,1.9052772832257626E-2,0.10241440607315475,-1.3763048933857149E-3,4.1920311305872496E-2]
[null,76,0.98410884764845774,1.0163376415630598,0.98266985620942382,0.95337594558741223,0.99778262941905926,0.978120936762787,0.99503994319421563,null,6.7384535069662039,0,1.0444175340916762E-2,0.18978063315041582,0.12347829206627438,8.2064674930072357E-2,0,1.0444175340916762E-2,0.27072547970168093,5.9105781081804585,0,1.9243125189903398E-2,0.10075384330275283,-1.1779046153466404E-3,4.30072550599849E-2]
[null,77,1.0091108073763455,0.99533280826160997,1.014198084126023,0.96643205160365353,0.98026706029887078,0.96320336158297126,0.97894925396991694,null,6.7180298329117694,0,9.8452889045535768E-3,0.18745360716227,0.12084297662704795,8.3865782135620071E-2,0,9.8452889045535768E-3,0.25861545923731177,5.909515716401172,0,1.9105873374171665E-2,9.7971318655912687E-2,1.1795200541067696E-4,4.0541147312853174E-2]
[null,78,1.0295323692411837,0.99576389562692824,1.0056208952144585,0.98575507210966529,1.0137477765648886,1.0144902493623218,0.98782681829353658,null,6.7267491314500711,0,1.0238449649350813E-2,0.1924797415778558,0.11858257630002171,8.3372034680664356E-2,0,1.0238449649350813E-2,0.26041413081959969,5.9110463821937573,0,1.8998712528494357E-2,0.10102588862844684,-1.3304485586959091E-3,4.2160113279924361E-2]
[null,79,0.9920535015299301,1.0095017503071664,0.98050447792733064,0.99692350526736373,1.0023971053662302,0.95690667511118199,0.99599623403465476,null,6.7281057238187616,0,1.0184362275248292E-2,0.18446605961074108,0.1228609309648568,8.1909459536137555E-2,0,1.0184362275248292E-2,0.2668720107653697,5.9130516433126781,0,1.9198761997398631E-2,9.8038525144237304E-2,-2.2905861322936245E-4,4.1937391100563881E-2]
[null,80,0.99025311275952665,0.99962253188436268,1.0132597594750672,1.0009567846513929,1.0237901806689544,0.99830526756554916,1.0183328077252738,null,6.7570657671261012,0,1.0387784834512231E-2,0.19750822157614953,0.12295044755018403,8.4090016833937103E-2,0,1.0387784834512231E-2,0.27750663551932986,5.9114345531080765,0,1.9208753044948051E-2,0.10327413856096974,-1.6820480592435951E-3,4.2775048991747007E-2]
[null,81,1.0127125959318923,1.0208506942997631,1.0013942820372848,1.0034238354933178,1.0171595281964763,1.032088262004955,0.98073904066730266,null,6.7390088330541564,0,1.0515603109707054E-2,0.19645646307291662,0.11943591612454878,8.3174626800383775E-2,0,1.0515603109707054E-2,0.26417506902225707,5.9122395322420349,0,1.9086659312262447E-2,0.10332949009117741,-2.1903055096166688E-3,4.3301381898194422E-2]
[null,82,0.97957326024183178,1.0147095986951689,0.98070387196909303,1.0041522058561443,0.98113090609418152,1.021100968149087,0.98626898034874522,null,6.7593786446702442,0,1.0979913251459176E-2,0.19893445791376138,0.12416664832868729,8.2017371026603947E-2,0,1.0979913251459176E-2,0.27364560296771862,5.9134314320896069,0,1.9268774726538564E-2,0.10571751951443119,-3.0164903149149116E-3,4.5213328417805274E-2]
[null,83,0.98318125538162993,1.0063518946499319,1.0092938414618426,0.97412674158882329,1.0098348660611387,1.0052487638429672,0.97573918624212641,null,6.7500124659853897,0,1.0541545953935059E-2,0.1992585659957794,0.12357871936134111,8.3701889007041008E-2,0,1.0541545953935059E-2,0.26838739836168946,5.9102101585289288,0,1.9248351635498678E-2,0.10439383738621461,-2.1746642041742537E-3,4.3408209913071219E-2]
[null,84,0.98631997208320132,0.97614149545275897,1.0040037839279863,0.98445633327240112,1.0099322179851722,0.97892412226653658,1.0080369222613916,null,6.7520791562190521,0,1.041539026404263E-2,0.19533780273424481,0.12479831546944413,8.3458551330185149E-2,0,1.041539026404263E-2,0.27414288960557137,5.911067491700007,0,1.9230706429128146E-2,0.10260819610780589,-1.4535203943095798E-3,4.2888723236969913E-2]
[null,85,0.97500205717935606,1.0186308664522217,1.0309262076885282,1.0307364702306694,0.99236318777090726,1.0472536646025514,0.9848522679715066,null,6.7783209091313195,0,1.0810131776520673E-2,0.21097997222883413,0.1235957080408986,8.5201331558208887E-2,0,1.0810131776520673E-2,0.27705205703208524,5.9120287685668487,0,1.9294867130968955E-2,0.10936326325893091,-3.7092572094369483E-3,4.45141985239845E-2]
[null,86,1.0005041281487039,0.99473458979130414,0.98451500144893378,1.01329856910901,0.98839010279332129,0.9951902569566814,0.9989489597195913,null,6.742125113072726,0,1.0531952924589466E-2,0.19190012417882266,0.12246877423096442,8.2200148201463472E-2,0,1.0531952924589466E-2,0.26914105613113709,5.9137153507403264,0,1.9152346717354322E-2,0.1017851305033249,-1.6065251563956175E-3,4.3368707525721618E-2]
[null,87,0.96431554880177617,1.024956124317729,0.96861992837103772,0.97185143010653008,1.0071789209045365,0.98321992488688248,0.9905914723184327,null,6.7519340218942396,0,1.0806940798843517E-2,0.19232000331125373,0.1258549935529395,8.1265391825706232E-2,0,1.0806940798843517E-2,0.27543663137914398,5.9123469582000849,0,1.9356830806348722E-2,0.10282408935051894,-1.9719351776364856E-3,4.4501058645882823E-2]
[null,88,1.0083358667709055,0.97165372394198868,0.97619561294326807,0.98620832931455515,0.9804817255472128,1.0316532750694256,1.0031964790365513,null,6.7544599535656467,0,1.1022230385904013E-2,0.19836970257811573,0.12281895913186956,8.1698185111207133E-2,0,1.1022230385904013E-2,0.27187343538227354,5.9127092772621337,0,1.9110025307642074E-2,0.10565577974451172,-3.1629937973877975E-3,4.5387582845279967E-2]
[null,89,1.0260362719754492,0.96865383786996784,0.96601650161140873,0.98979494302892612,1.04136709128244,0.9820300047686884,1.0135293375961458,null,6.7252839086543554,0,1.0416657241083843E-2,0.1846592008434722,0.12103518677802286,8.0978338220775409E-2,0,1.0416657241083843E-2,0.2652716026977569,5.913458673742924,0,1.9016755448680461E-2,9.8857685559701161E-2,-8.874750598923363E-4,4.2893940422912114E-2]
[null,90,0.97265255401441009,1.004967471835013,1.0140980338377144,0.99896323235104967,1.0238500933626786,1.0056823614619952,0.99408750728627815,null,6.7652396214688046,0,1.062180977551053E-2,0.20220856711251814,0.12489233888868079,8.4127712635415214E-2,0,1.062180977551053E-2,0.27645848162258158,5.9112790950337297,0,1.9308373506225478E-2,0.10568811650583927,-2.4617858800798486E-3,4.3738722043891343E-2]
[null,91,0.99772496557053547,1.0041059403479584,1.012637489941409,0.99952176276471005,1.0094808304499563,0.99284659506728146,1.0256095751530623,null,6.7504723848603705,0,1.0239556523327004E-2,0.19451065518623506,0.12182318401281773,8.404054770098747E-2,0,1.0239556523327004E-2,0.27682189349161362,5.9113924334379888,0,1.9167524567824352E-2,0.10173802571889735,-1.1865504459414612E-3,4.2164671189942098E-2]
[null,92,1.0229024829359694,0.99070938013568066,0.95596194389418654,0.98849891127922151,0.97314975493696987,1.0085988846764722,1.0128006726843808,null,6.7323766472500282,0,1.0721548333726032E-2,0.18724586793366416,0.12049889638323395,8.0387317808826644E-2,0,1.0721548333726032E-2,0.26814601734575999,5.9139315138123525,0,1.9033033366494694E-2,0.10075235664793662,-1.767783722067606E-3,4.4149427673821219E-2]
[null,93,1.0303661124187169,0.98402923772589179,1.000024056834784,1.033676710460504,0.99620457969164378,1.002110987745205,1.0017425582092345,null,6.7294988115581083,0,1.0206587739379519E-2,0.19029665415202038,0.11915238709487966,8.3092429124428061E-2,0,1.0206587739379519E-2,0.26284246309654991,5.9139515420236952,0,1.899442776592327E-2,0.10015775228354531,-1.0177555888111606E-3,4.202891160587114E-2]
[null,94,1.0159118556259288,0.96527951934062739,1.0032214468628504,1.0076219659142274,0.98302446303556401,1.0235302863751687,0.97881515979740263,null,6.7441485728847308,0,1.0630893733425247E-2,0.19914862270234801,0.12172133666679963,8.3270402975771707E-2,0,1.0630893733425247E-2,0.26266114406754854,5.9123634740874325,0,1.9069706830129048E-2,0.10465055871847352,-2.5128013294682967E-3,4.3776128165699903E-2]
[null,95,1.0369249490889243,0.97533363282436669,0.99441914156081601,0.99314303138315274,0.99620984932659362,1.0227570236988479,0.99431345888995415,null,6.7300226577712472,0,1.0441420844013576E-2,0.19306486206812612,0.11892199828751798,8.2693199852047622E-2,0,1.0441420844013576E-2,0.26121058900650385,5.9120750880571959,0,1.8960960983032706E-2,0.10189829742637707,-1.7982504415734444E-3,4.2995912532019745E-2]
[null,96,0.99338542742287195,1.0425284913760122,0.98676008332058374,1.0394106898741304,0.97346699189111308,0.96654158232276433,1.022696318165863,null,6.7352480364995193,0,1.0077448596047039E-2,0.18423110646887755,0.12101125398445857,8.2427964468998041E-2,0,1.0077448596047039E-2,0.27433589890093169,5.9150024167679547,0,1.9191393936212629E-2,9.7607898103092103E-2,-5.7035730546221226E-5,4.1497139599538616E-2]
[null,97,0.98474442941524487,1.0229862479042109,1.0244564616441985,0.99809799507038621,1.0038411610722542,1.0198934747235282,0.99268995886412037,null,6.7589905290306378,0,1.0463686874767694E-2,0.20227437545758167,0.12228786923241318,8.4732489331753494E-2,0,1.0463686874767694E-2,0.2738586995816551,5.9106392057602681,0,1.9239549739140348E-2,0.1051842793336062,-2.3135394892462424E-3,4.3087600083459486E-2]
[null,98,0.99679723034798129,0.98359341516162946,1.0345221785142553,0.99049886990114544,0.98770707377099487,0.99393566532384514,0.97063008629378567,null,6.7418730794729624,0,1.0154948172632981E-2,0.19924893289182952,0.12252867618836225,8.5193039410583607E-2,0,1.0154948172632981E-2,0.26256238010580735,5.909646752121434,0,1.9172610053370495E-2,0.10310053802994869,-1.3961183898842688E-3,4.1816269061509141E-2]
[null,99,1.0142943516490415,1.0299043220960047,1.0333729806481236,0.95715871258656893,0.99964201666122954,0.99147749850464506,1.042713636350197,null,6.7376114880192803,0,9.7707177998608875E-3,0.19138470390021098,0.11824052470721565,8.5287674092421217E-2,0,9.7707177998608875E-3,0.27650460306592894,5.9079126275407106,0,1.9078264417907557E-2,9.9086982886348679E-2,-1.179693683563146E-4,4.0234076776890518E-2]
[null,100,1.0151889494715938,0.98123387615033208,0.9955167285042632,1.0064519291674632,1.0228675034976598,1.0228673685918073,0.98027512288703123,null,6.7408306909000366,0,1.0628399681377866E-2,0.19684208940482109,0.12115515905041421,8.2796030927759265E-2,0,1.0628399681377866E-2,0.26298123926693873,5.9127330176545518,0,1.9073528076618679E-2,0.10383515945223788,-2.3513910365998013E-3,4.3765858103293517E-2]
[null,101,1.0109661028024062,1.0201014438226335,1.0061268132551757,1.0414615684304678,0.9831616055050787,1.0134160095569411,0.95782091579694206,null,6.7294026358955712,0,1.030374287414149E-2,0.19385241075355117,0.11959020599471198,8.3396610251018577E-2,0,1.030374287414149E-2,0.25680921097300302,5.9140280281880804,0,1.9095959037483876E-2,0.10172085478866955,-1.5196232488039951E-3,4.2428979157851605E-2]
[null,102,0.98238465993234125,1.0072107786418301,0.99563173860104748,0.97598734753578908,1.0397200540831779,0.99932236825748255,0.99555738324810361,null,6.7524581283059044,0,1.0609973913126803E-2,0.19653433171538734,0.12389689760993662,8.2923584553548105E-2,0,1.0609973913126803E-2,0.27346372853660433,5.9110800800116241,0,1.9252847867370169E-2,0.10366688365229861,-2.050209710166521E-3,4.3689984069300115E-2]
[null,103,1.0380817722833351,0.99604857560284998,0.96651346019919626,0.98990487361275237,1.0093742093068743,0.9975951598266849,1.039271831584399,null,6.7249395830321355,0,1.0330230236538829E-2,0.18326229567097088,0.1182947803789903,8.1071028557798325E-2,0,1.0330230236538829E-2,0.27005242718872857,5.9134376339777868,0,1.8955102109287577E-2,9.8085302187756115E-2,-7.5703644081173856E-4,4.2538049401629086E-2]
[null,104,1.0340818638656954,0.98164030490213761,1.0193127612919382,0.99880446448995708,1.0131469239163462,1.0406380684083134,1.0464079858101554,null,6.7542489533178518,0,1.0395084498099639E-2,0.19942521145230724,0.11848595608382122,8.4458299903203415E-2,0,1.0395084498099639E-2,0.27733989869093123,5.9109726458037546,0,1.8975415835843515E-2,0.1039655789412689,-2.1791611003901625E-3,4.2805107707108277E-2]
[null,105,1.009120289373552,1.0380458782603847,0.97191400859089083,1.0223203782837376,0.98775486524078604,0.99663880372581193,1.0014833291560499,null,6.7287578187032473,0,1.0381561009756551E-2,0.18565576214478444,0.11959873378947115,8.1395904530396551E-2,0,1.0381561009756551E-2,0.26723491143362288,5.9148960954628045,0,1.9105822611547068E-2,9.9096810053317191E-2,-9.7564171189706969E-4,4.2749420389202632E-2]
[null,106,0.98808406838537632,0.98908481242411916,0.99567300989111962,1.0265593964194928,1.0231394662155353,0.96325609272648238,0.99608716587745572,null,6.7402324173649575,0,1.0247095820380253E-2,0.18982415268587666,0.12407951799639833,8.2899509790207729E-2,0,1.0247095820380253E-2,0.26877137743707868,5.9138110082196356,0,1.922083825949366E-2,0.10012537820699381,-6.9508190399292333E-4,4.219571667326253E-2]
[null,107,0.96304310078798572,1.0247159032741247,0.96686476890820616,1.0068412182069282,1.0091739032746234,1.0233909563710708,0.9940153712655212,null,6.7719048218802911,0,1.1281691009445627E-2,0.20024602930036656,0.12606638402021927,8.1248263887545344E-2,0,1.1281691009445627E-2,0.28061995035883192,5.9143343177972554,0,1.9364300472559277E-2,0.10715635050157289,-3.5867699688182687E-3,4.6455995510754938E-2]
[null,108,0.98393801010029702,0.98546064577866976,1.0028682665503308,1.0011142213842812,1.00225990493513,1.0072150116162371,0.97135275146269284,null,6.7540221370267872,0,1.0709297959468357E-2,0.20051245180473753,0.12464766007923411,8.3309262406223383E-2,0,1.0709297959468357E-2,0.26736259220721759,5.9120317045266306,0,1.924408702029699E-2,0.10538569711185075,-2.5703009425197482E-3,4.4098982813113433E-2]
[null,109,0.98069879993729081,1.030319220499307,1.0214020129388421,1.0198753471032458,0.96684060155812868,0.99040106232499747,0.98345781075576,null,6.7471250362020676,0,1.0199133231617783E-2,0.1962716173597471,0.12250031218285605,8.4501756157959171E-2,0,1.0199133231617783E-2,0.26960041766305481,5.91199122866362,0,1.9262387470995408E-2,0.10221629304323827,-1.2171916091625547E-3,4.1998215269761226E-2]
[null,110,0.98684771370215629,0.99629878679772621,1.0281064585463917,1.0230402000999732,1.0137717509144937,1.0002627290303592,1.0065626100674585,null,6.7602912631259615,0,1.0323907605345989E-2,0.20065227373646144,0.12325407946186073,8.499892369344228E-2,0,1.0323907605345989E-2,0.2754942900573541,5.9117761468188395,0,1.9227750599354269E-2,0.10415382082578657,-1.778035998904317E-3,4.2512013931763369E-2]
[null,111,1.0254336282978684,0.99773613205028333,1.0237454312999108,0.97088709429521169,1.0275777045065264,0.98241989897390225,0.96632924765364747,null,6.7117934347504091,0,9.7895042710910082E-3,0.1890428138658472,0.11862853238795601,8.4379939781026592E-2,0,9.7895042710910082E-3,0.25292269137839252,5.9092101098618848,0,1.9019878048828417E-2,9.8338141551100267E-2,-6.0108246178776069E-5,4.0311436121548923E-2]
[null,112,1.0425039666626026,1.0443738698907801,1.0236598259010266,0.98126439220215544,0.96806169530330322,0.98829630103715227,1.0071547072264759,null,6.705954620036918,0,9.4999595790165852E-3,0.18342826085065425,0.11457468324422629,8.446985695338112E-2,0,9.4999595790165852E-3,0.25943038634171373,5.9097756380109647,0,1.8932825217880315E-2,9.5421526032841986E-2,8.023007686364295E-4,3.9119142616620424E-2]
[null,113,0.97746317985294373,0.96878622521892754,0.97581082954462051,1.0076781842284557,1.0480141551551163,0.9771140314511122,1.0362942362288343,null,6.7659455694796033,0,1.0786530671792279E-2,0.1940169309104382,0.12685539017355291,8.1854158521055251E-2,0,1.0786530671792279E-2,0.28422636675554236,5.9138911151620528,0,1.9280788728921118E-2,0.10335734808106253,-1.9535422285794917E-3,4.4417013375553004E-2]
[null,114,0.98511049364512504,0.98303096439440019,1.0154823049671331,1.0051422292178926,1.00353472231444,0.99781605480518998,0.96095771435406474,null,6.7483345995432096,0,1.0491587818153521E-2,0.20013908813495049,0.12437963956599217,8.4039598983296701E-2,0,1.0491587818153521E-2,0.26336294150493855,5.9115340173488704,0,1.9237492546998851E-2,0.10453500750941065,-2.09567725338664E-3,4.3202491202139509E-2]
[null,115,1.0060733275909677,0.96929261181925741,1.013480229197973,0.97114336989326555,0.98829228686327397,0.99604934580436233,1.0037397630783294,null,6.7450826568467379,0,1.0334942088524354E-2,0.19656762493416943,0.12251360566056109,8.3970120260228612E-2,0,1.0334942088524354E-2,0.26933270755983868,5.9098111461088756,0,1.9122184012002497E-2,0.10277112242963508,-1.5633060880005658E-3,4.255745196942709E-2]
[null,116,1.0184052547923648,1.0040169933511482,0.96277246633248947,0.99712113971297434,1.014777033350478,0.97358084509868803,1.0068080007007953,null,6.7188880903037447,0,1.0274724042172402E-2,0.18126752913561753,0.12026416147145197,8.0769687364330073E-2,0,1.0274724042172402E-2,0.26435348127384528,5.9140306360828028,0,1.9056568469124353E-2,9.720071309372047E-2,-3.6417136010717747E-4,4.2309484772962432E-2]
[null,117,0.98404962168537291,1.0111497404721859,0.99248317828210519,1.0239997638403981,0.96424623063233694,0.97620415511331182,0.99845701512724161,null,6.7443988611677028,0,1.0358142496118916E-2,0.19097623099506619,0.12355383509994997,8.2736769147638667E-2,0,1.0358142496118916E-2,0.27155154251112884,5.9138509506351342,0,1.9243458599455036E-2,0.10089315068416806,-1.0600636232198368E-3,4.2652987118382897E-2]
[null,118,0.9876834605955076,1.0490620588340662,1.0180320238120499,1.0261688661816288,0.9912251765335115,1.0052951519943711,0.98650978702856673,null,6.745445006206233,0,1.0230486728493703E-2,0.19589594498990662,0.12082336835485746,8.4299104930373098E-2,0,1.0230486728493703E-2,0.26973809572424706,5.9125243656103859,0,1.9223076123817313E-2,0.10219016462738008,-1.3764375439147406E-3,4.2127323389181869E-2]
[null,119,0.99621660002386392,0.99793305379840591,0.9834360223938976,0.99387074435534406,0.99680491315810682,0.99550243061616484,1.0164336862268353,null,6.748336340703057,0,1.0576004409697784E-2,0.19239462305779445,0.12285817422685484,8.2197284107242002E-2,0,1.0576004409697784E-2,0.27502616540091179,5.9127248284393943,0,1.9175797663203816E-2,0.10210247306891396,-1.6931089617841573E-3,4.3550103700525637E-2]
[null,120,1.0308059147435227,1.0079252206337375,1.0067167668529542,1.0071687259633777,1.0086278722939999,0.9869576267452892,1.0050700838682356,null,6.7189300839943957,0,9.8872154296380833E-3,0.18617852529243517,0.1178424622825717,8.3476546977326718E-2,0,9.8872154296380833E-3,0.26198736990269672,5.912141561970599,0,1.8992170331760861E-2,9.7665565663769549E-2,-6.7911707276032779E-5,4.07137932805079E-2]
[null,121,0.98437212552340381,0.96321191854783961,0.9735059095770201,0.99274502182159785,0.97657196826518788,0.99461151336897025,1.0309783215040043,null,6.7665911876966511,0,1.0951609665135125E-2,0.19631343907027557,0.12630011784178818,8.1677621398211331E-2,0,1.0951609665135125E-2,0.28259525061869334,5.9132100290648051,0,1.9241643566050279E-2,0.10470178169044927,-2.5454748408016863E-3,4.50967792871734E-2]
[null,122,0.99683810261356975,1.0045231527906722,1.0402630236569661,1.0345969105292154,1.0228413150927398,0.97918127177030367,0.99241130763565188,null,6.7408464983310763,0,9.8641668489771375E-3,0.19519206353831461,0.12138644190685952,8.5639081759756416E-2,0,9.8641668489771375E-3,0.26686275067737425,5.9116940494731498,0,1.9172385808095858E-2,0.10071812435443984,-4.3728251475916638E-4,4.0618883327840555E-2]
[null,123,1.017529852921401,1.0039231027620625,0.98813451113657147,0.95071351146350158,1.0018032094115321,0.99101501003334924,0.9823634947958727,null,6.7193389804470707,0,1.0239369383688949E-2,0.18757316568656207,0.11991138611862467,8.2255039695108043E-2,0,1.0239369383688949E-2,0.2597833002339035,5.9101317541043512,0,1.9061173851771737E-2,9.9310402010410401E-2,-8.5114183588280668E-4,4.2163900582222191E-2]
[null,124,0.99870900195120027,0.95650229489771554,1.0025736091425306,1.0092650203175795,0.98617236065155045,0.99310117749855653,1.042083485702415,null,6.7633933110291622,0,1.0539675748910611E-2,0.19725047217762168,0.1242836246410082,8.3485820795278526E-2,0,1.0539675748910611E-2,0.28151882336289963,5.9124887819743384,0,1.9162140786742922E-2,0.1036864151338981,-1.8832765842861736E-3,4.3400508741664616E-2]
[null,125,1.0074967237911796,0.96022658440360098,0.99924033201857687,1.0256005843004854,1.0197297412319382,1.0295124697358042,1.0108724063744223,null,6.7629782643553131,0,1.0844295851403051E-2,0.20195177512447585,0.12307126476314306,8.3191144335772557E-2,0,1.0844295851403051E-2,0.27416130733842264,5.9135591326399632,0,1.9114528423788343E-2,0.10633351135215681,-3.0592797257849892E-3,4.4654880103371486E-2]
[null,126,0.95454262879144591,1.0087015406674309,0.99776125144474648,0.99667468825013716,1.013170568382832,1.0045816755686161,0.99444002723676328,null,6.776380877641877,0,1.0949582404840248E-2,0.20346613195046689,0.12739370555560672,8.3182205997313366E-2,0,1.0949582404840248E-2,0.28162755755664753,5.91207887668316,0,1.9414711787914887E-2,0.10720963583893459,-3.080379118286152E-3,4.5088431390117971E-2]
[null,127,1.0400394325236562,0.98702852725844636,0.97871501993106391,1.0005372319146613,0.97747127970869296,1.0247055884732816,1.0032137409368609,null,6.7277962050111224,0,1.0519960688394787E-2,0.19003940884053813,0.11828451065118445,8.1743347589941534E-2,0,1.0519960688394787E-2,0.26277983103229158,5.9133455277974489,0,1.8945216988269488E-2,0.10109115506534859,-1.7521185855164324E-3,4.3319325631610422E-2]
[null,128,0.99639272644862953,0.99644356520834376,0.958604166704636,1.0127726293708132,1.0039142457769128,0.97645274918201563,1.0018798326295044,null,6.735762909380413,0,1.060528735898268E-2,0.18594417410502398,0.12337090069309557,8.0584989391438433E-2,0,1.060528735898268E-2,0.26920457368449319,5.9151020788484763,0,1.9174830351956263E-2,9.9918433835380696E-2,-1.207757202961239E-3,4.3670685673510151E-2]
[null,129,0.99567129823585654,1.0020075869709446,0.9955048808066026,0.95121555576382932,1.0237045586354889,1.0280213098582804,0.99232349320701319,null,6.7529449255729528,0,1.0794133410540946E-2,0.19990803241526917,0.12249946690570908,8.2873077735207384E-2,0,1.0794133410540946E-2,0.2716825925316409,5.9097483459223135,0,1.9178794707766556E-2,0.10545308092049928,-2.8467856659420343E-3,4.4448320100482976E-2]
[null,130,1.0110715939600057,0.97341434064331234,1.0094082587543225,1.0003261673135602,1.0043198131299884,0.97291314910528692,1.0039146286698262,null,6.7328269942372474,0,1.0062492357983826E-2,0.1902356132595816,0.12177791976260366,8.3691151650750875E-2,0,1.0062492357983826E-2,0.26580538623682742,5.9116193482475579,0,1.9095396406563575E-2,9.9660967793482644E-2,-4.9434159342375038E-4,4.1435552473305444E-2]
[null,131,0.97894265351632004,1.0237003072793569,0.99955151946176668,0.99837151080651898,0.98264955766672835,0.97191106216522227,0.98666698345010828,null,6.7399956153095282,0,1.0248348660917748E-2,0.19094154680689152,0.12345328307237494,8.3127088154973369E-2,0,1.0248348660917748E-2,0.269246347316417,5.9120701049697102,0,1.9272359737320523E-2,0.10052076424701763,-8.3675464278003318E-4,4.2200875647598626E-2]
[null,132,0.98325599472103697,1.0055950185649913,1.036622780163009,0.97741093061069884,0.99308074962797566,1.0045336682754866,0.98247472826790982,null,6.7543807669438793,0,1.0287462392748718E-2,0.20247645433372227,0.12308118683900546,8.5419122435320627E-2,0,1.0287462392748718E-2,0.27020709091380773,5.9088177145008132,0,1.9247930157311896E-2,0.10466293746787513,-1.8936087372752981E-3,4.2361939033293827E-2]
[null,133,1.0262371378646411,0.99396009888318992,1.0126878356625235,0.96756789211725092,0.99821269480717068,0.99667962454277659,1.0042086324879029,null,6.7264443289188316,0,1.0036626385242635E-2,0.19067000100587247,0.11891972858087065,8.3844409717352866E-2,0,1.0036626385242635E-2,0.26396653052916519,5.9096630422984155,0,1.9015715476333291E-2,9.9726706131319898E-2,-6.9084582203217761E-4,4.1329041001528746E-2]
[null,134,0.98219459504998474,1.0122928553663217,1.0126155021583927,1.017332685396912,1.0070980730797554,1.0447244795898167,0.97922266911588529,null,6.7690541273545977,0,1.0907177248548243E-2,0.20718603827238108,0.12334855568218145,8.400509545354333E-2,0,1.0907177248548243E-2,0.27325421016891832,5.9123560425481028,0,1.9253921730199453E-2,0.10836901178497844,-3.6325627900520726E-3,4.4913814504343938E-2]
[null,135,1.0202845415532835,0.97622632475442661,0.97497080951254267,1.0171489493401662,1.02426938912813,0.98407491467998531,1.0083083511524171,null,6.7294370658027995,0,1.0380947801904284E-2,0.18648907706914783,0.12117531642639182,8.1559492299132869E-2,0,1.0380947801904284E-2,0.26552319303709954,5.9144492018512311,0,1.9046708463626931E-2,9.9388958265767283E-2,-9.4177691801380881E-4,4.2746895308413919E-2]
[null,136,0.99756143385870399,0.99925777263278748,1.0095502947830053,0.99787743340148971,0.99936217768323909,0.97758155439617467,1.0110152333421176,null,6.7410383004200449,0,1.0132021281277555E-2,0.19159036918194522,0.12213759173828649,8.377614291343484E-2,0,1.0132021281277555E-2,0.27151063775209827,5.9114789751679444,0,1.9168420298677557E-2,0.10036364718417951,-7.0934402026311344E-4,4.172186020374203E-2]
[null,137,1.0175426798211997,1.0179164672773771,0.99173131539784631,0.98390698876081295,1.0023311198152585,0.98515550220553139,1.0210243729013817,null,6.7270433720647391,0,1.008684542818122E-2,0.18576708721985727,0.11918232067920503,8.2629190079025347E-2,0,1.008684542818122E-2,0.26932982633098734,5.9117258847127054,0,1.906110631381009E-2,9.8177920126582524E-2,-3.6579747912687523E-4,4.1535834081693417E-2]
[null,138,1.0109786108861354,0.99279293595036733,0.99942923853724808,0.9747306138022086,0.98333123939339995,0.99043034213860026,1.0012995380000389,null,6.7331200836255301,0,1.0247405156145164E-2,0.19088938257760688,0.12101849631355824,8.3064315089095939E-2,0,1.0247405156145164E-2,0.26657816444726995,5.9107993443003952,0,1.9095892320215083E-2,0.10049940679920102,-1.0219086847010103E-3,4.2196990462882715E-2]
[null,139,1.0119916366913584,1.0178865850754899,1.0081085189082857,1.0252587405082725,1.0205955433076781,0.98595036960260662,0.96963743041289452,null,6.7210027684373754,0,1.0006301815587235E-2,0.18880963294922101,0.1195363699439584,8.3513719196295313E-2,0,1.0006301815587235E-2,0.25727609738233564,5.9130402738995178,0,1.9090494385115425E-2,9.8977563555751158E-2,-4.4555269607878461E-4,4.1204169821259989E-2]
[null,140,0.98838941190212259,0.97889721136032715,0.99212821703331378,1.0356513394136109,1.0064556393684772,0.97274745047816402,0.97079316808130389,null,6.7390153020323389,0,1.0423077597201208E-2,0.19207237024451115,0.12462353650584261,8.2606689890407606E-2,0,1.0423077597201208E-2,0.26283735159783028,5.9145005155566492,0,1.9219133776144939E-2,0.10149018941822315,-1.254863263898495E-3,4.2920378306622625E-2]
[null,141,0.97794533982507437,0.99828787634112026,1.0035232337001123,0.99832287911179984,0.99454648466458362,1.0117442409527826,0.97558071450512007,null,6.7588138786697796,0,1.075741072206113E-2,0.20160876146431225,0.12475182078475347,8.3389977081928315E-2,0,1.075741072206113E-2,0.27046342591757333,5.9118439358328896,0,1.9278038921966906E-2,0.10592748092850385,-2.7466648678671685E-3,4.4297102605717974E-2]
[null,142,1.0190016539883358,1.0061996050493049,1.0196035720208299,0.99613237659403286,1.0314453454685684,1.0067725905099516,1.0101715661843786,null,6.7368167685814528,0,1.0095585379952069E-2,0.19376279096393881,0.11905141441133234,8.4351860635717257E-2,0,1.0095585379952069E-2,0.26825217851997851,5.9108116283436685,0,1.9053435417363929E-2,0.10099913852698826,-1.0375018849717273E-3,4.1571823647432338E-2]
[null,143,1.0293518250989548,0.99924503861661051,0.97147007867145851,0.98310388691823647,0.97499935279135264,1.0085046300142899,0.99782121627640918,null,6.7234146544107967,0,1.0472037541566587E-2,0.18715039083878893,0.11905635703401247,8.127642308388032E-2,0,1.0472037541566587E-2,0.26245481513674007,5.9128000234967795,0,1.8999641292976349E-2,9.9916875265002966E-2,-1.361858380354025E-3,4.3121986642974043E-2]
[null,144,0.98893454783640489,1.0011437235702196,1.0187878672883197,0.99586224915438459,0.97807245952377708,0.99794915831575681,0.96349172307604636,null,6.7425778204851294,0,1.034100841294076E-2,0.19823379181767339,0.1229340154436056,8.423031800524021E-2,0,1.034100841294076E-2,0.26287379919606252,5.910843737918352,0,1.9216093344679219E-2,0.10337119520916969,-1.7075624632624212E-3,4.2582432013608347E-2]
[null,145,1.009378540270067,1.0195308428581165,0.98085968452475614,1.0214130750169885,0.9770719366782028,0.99892378418218764,1.0079762730280721,null,6.73530511540815,0,1.0401722706449045E-2,0.18850235073925642,0.12026911178346798,8.1979719980648166E-2,0,1.0401722706449045E-2,0.26929112216608864,5.9143559493476099,0,1.910444041159556E-2,0.10016588874846802,-1.1959104365208703E-3,4.2832442667534096E-2]
[null,146,0.9951572227743295,0.97748480030674978,0.96456466827850507,1.0006208044540394,1.0061055181749661,1.0009462430354634,1.0393660345231321,null,6.760265624501189,0,1.0918026873304183E-2,0.19313021339627554,0.1243657521600789,8.1119013908341739E-2,0,1.0918026873304183E-2,0.28225764261383585,5.9141228135034982,0,1.9181623136415672E-2,0.10346830176264898,-2.3382273078362153E-3,4.4958491327927688E-2]
[null,147,1.0127991471296389,0.99599358869525378,0.98393493607835136,0.96977338743293662,0.99372622825666845,1.0237181442909189,0.96829866504941731,null,6.7335970479106129,0,1.0701954866603889E-2,0.19482999141243126,0.12093151975549259,8.2014778233623631E-2,0,1.0701954866603889E-2,0.26027833567702413,5.9113946287850512,0,1.9086199278628879E-2,0.10336911883811739,-2.3762693334832539E-3,4.4068745263719365E-2]
[null,148,1.0163460599267891,0.98699347706344731,0.95650147189164836,0.99980629488562089,1.0028222555669544,0.97672554450983418,1.0044057488451665,null,6.7235959752577239,0,1.0461640725420249E-2,0.18285329775608708,0.12144887848609598,8.0384669147992013E-2,0,1.0461640725420249E-2,0.26469421382648822,5.9145140312193334,0,1.9067414260549094E-2,9.8361988209799509E-2,-8.0769205326836069E-4,4.3079174404647723E-2]
[null,149,1.0010882604920026,1.0169936611877848,1.0191343099828811,1.0114436336984336,1.0005586600699274,0.98833984957952659,0.98263773461484316,null,6.7333473234162522,0,1.0046235476581582E-2,0.19268181945546523,0.12067439414306384,8.4274991521734691E-2,0,1.0046235476581582E-2,0.26381101432793702,5.911665711923086,0,1.9149167310975216E-2,0.10045890545397272,-7.3729024928919338E-4,4.1368609529308008E-2]
[null,150,0.99402409043563056,1.0253173097104493,0.9729737294353582,0.96602608454780314,0.96754167572966954,0.99602734199668475,0.98438660416485435,null,6.7336762507596513,0,1.0578733591184088E-2,0.18947969226116526,0.12199624432367501,8.1416372918764718E-2,0,1.0578733591184088E-2,0.266717865893285,5.9117945535883516,0,1.9187867929686304E-2,0.10108407873778628,-1.5617668771738694E-3,4.3561341984110026E-2]
[null,151,0.99044557227365237,0.99652462191843938,0.99263802947472934,1.0087598376675344,0.98592381595605061,1.0276873568911826,0.96321954372552621,null,6.7524551484543283,0,1.0900330919044148E-2,0.20101885994299168,0.1234705297490357,8.2649406324667524E-2,0,1.0900330919044148E-2,0.26512984454452887,5.9130186063482686,0,1.9207683279430305E-2,0.10619050131534648,-3.1159055879936984E-3,4.4885622538047301E-2]
[null,152,1.0311845439032885,1.0382035569413948,0.97760353780872378,1.0045559027433275,1.0011877698293787,1.0242809090925731,0.99125901899902136,null,6.7210403646575463,0,1.0388904083402416E-2,0.18736264335755648,0.11693197230777803,8.1658403746264735E-2,0,1.0388904083402416E-2,0.26131965526111578,5.9136238929469265,0,1.8990228432028237E-2,9.972277905425446E-2,-1.3488683078366434E-3,4.277965785945792E-2]
[null,153,0.99125833071674352,1.0015757832868377,1.0011114640570833,0.97824624038910724,0.98584739461512738,1.0027729656367217,0.98798568661444308,null,6.7469771540996337,0,1.052618339367103E-2,0.19657175679565653,0.12296019969750989,8.3209727497699351E-2,0,1.052618339367103E-2,0.26934302939749094,5.910894805986163,0,1.9203170230255879E-2,0.10340464616158378,-1.9551312910707896E-3,4.3344949624337714E-2]
[null,154,0.99785565424444944,1.0140359107805583,0.95843064304944769,0.9945167160387588,0.98393889701041581,0.95618007753426915,0.99586350192261319,null,6.7208821579779618,0,1.029400608926233E-2,0.1804398955284382,0.12233383061628417,8.0508565739768514E-2,0,1.029400608926233E-2,0.26514422876793442,5.9141241767790111,0,1.9166808942945989E-2,9.6969169449933321E-2,-1.9340265715655602E-4,4.238888481080233E-2]
[null,155,1.0191082555363229,0.9947655022080174,1.0338543905097646,0.9898046682608852,1.0096101986830379,1.0010740407463619,0.98098875275251773,null,6.7297114040869923,0,9.9614972326320852E-3,0.195260475501985,0.11931847980126084,8.5115779726675111E-2,0,9.9614972326320852E-3,0.26009379426800977,5.9096480337452117,0,1.9052875795925309E-2,0.10106977648090849,-8.6748375655440382E-4,4.1019672523569146E-2]
[null,156,1.03042770302085,0.98310155810440947,1.0229109970005092,1.0156841629062492,1.0143280210622825,0.97369104662979655,0.96173792768740163,null,6.709021673675835,0,9.7239288341192786E-3,0.18754491626935624,0.11876886523840881,8.4319297996054823E-2,0,9.7239288341192786E-3,0.24985774550384779,5.9116781346129699,0,1.899411151529426E-2,9.7599004587508031E-2,2.1818980829910509E-4,4.0041408144092017E-2]
[null,157,1.0308086906095433,1.036325359197348,1.0063587014222826,0.99289605895891075,0.97878641045579806,0.97582169203950986,1.0079795306107338,null,6.7096169554051777,0,9.6630920861066685E-3,0.1818617809326728,0.11654603307593951,8.3437322502947178E-2,0,9.6630920861066685E-3,0.26149144376284644,5.9113905612841933,0,1.8992156089807196E-2,9.5418008274341368E-2,6.8875623811432362E-4,3.9790893244313549E-2]
[null,158,0.98462223832717843,0.9592140177119729,1.028178933806569,0.96670897495458952,1.0070608763764715,1.0002151296221817,0.96140500183539979,null,6.7536772356802635,0,1.051570925690829E-2,0.2044019712526722,0.125419920880805,8.4806350448902779E-2,0,1.051570925690829E-2,0.26411899620534735,5.9087290236987977,0,1.9240236763917531E-2,0.10609642435782744,-2.4375069214850327E-3,4.3301818993475613E-2]
[null,159,1.0221517385841119,0.99940997101177265,1.0007120628388759,0.99461636368097139,0.95455188254337386,1.0433462808997609,1.0020364232726677,null,6.7461599596277928,0,1.0634632248817999E-2,0.19847952231323929,0.11935448858213514,8.3185779498140294E-2,0,1.0634632248817999E-2,0.26868830396894527,5.911801940336467,0,1.9036947796304236E-2,0.10442891186317303,-2.6074574372646356E-3,4.379152270665633E-2]
[null,160,0.97779482286690655,0.97827788641832603,0.98583764268845586,0.96339794306727278,0.99677636138944348,1.0204816818315785,1.0230147372342269,null,6.7763669102048967,0,1.1116880302202222E-2,0.20295567426082328,0.12612672244466253,8.2454971787859085E-2,0,1.1116880302202222E-2,0.28472413379237566,5.9109447278813212,0,1.9278897044209375E-2,0.1075779519991137,-3.4735033590110199E-3,4.5777334353538916E-2]
[null,161,0.99397353540016486,0.99211003356862804,0.9696161176186282,0.97808333668146541,0.98649374171203497,1.0183204354507811,0.95607319856351036,null,6.7412807478875996,0,1.1001732075818348E-2,0.19607632875692119,0.12368237928163114,8.1145878850831826E-2,0,1.1001732075818348E-2,0.26138654348495138,5.9126296731413008,0,1.9188146874781355E-2,0.10477990203257295,-2.9112789883050339E-3,4.5303174452910391E-2]
[null,162,0.97523114520664,0.99949878802228542,1.0181794612937112,1.0275014089132146,0.98841856782055304,1.0267276402505756,1.0301715180672901,null,6.7851686176029551,0,1.0802067298825567E-2,0.20688583796003104,0.12475523603640488,8.4556820847649941E-2,0,1.0802067298825567E-2,0.28789846453957157,5.9125879225325368,0,1.9293553675543255E-2,0.10791525703664326,-3.2054654656810989E-3,4.4480990440259563E-2]
[null,163,0.99013814445903281,1.011786276067641,0.96211725593988628,1.0123986395658073,1.0157209611261431,1.014087252189519,0.98576052486393773,null,6.7480288759379761,0,1.0977726320133234E-2,0.19348152865929091,0.12332883754459398,8.0814091106328229E-2,0,1.0977726320133234E-2,0.26992971109664088,5.9148922094256049,0,1.9209392282301077E-2,0.10378448909184339,-2.6157062924972462E-3,4.5204323023864318E-2]
[null,164,1.0066563858570474,1.0122833879167232,0.98143803203913138,1.0408104484596095,0.96674039622811248,1.0038397334360647,0.98299225907073828,null,6.7347569328366257,0,1.0507935482002281E-2,0.19059062084791933,0.12092834280795987,8.195780968366663E-2,0,1.0507935482002281E-2,0.26384409859488556,5.9153726398093589,0,1.9119045476038824E-2,0.10124623848878242,-1.5716708440772266E-3,4.3269807972093031E-2]
[null,165,0.98143407004749039,1.0003982938852383,1.0020597910794447,1.0225818354343124,1.0413205131782388,1.0046914453093196,1.0085271933336151,null,6.7634277076126832,0,1.0648433024279907E-2,0.19913425407903679,0.12423137602442148,8.3416173400748056E-2,0,1.0648433024279907E-2,0.27789492181317293,5.9132373813459003,0,1.925822284334228E-2,0.10470333082275737,-2.2963045602588999E-3,4.3848351843562013E-2]
[null,166,0.97578182417348747,1.0334304947289601,1.0078413206284402,1.0114029077521303,1.0288505879644907,1.0133001697795776,0.96385179360284368,null,6.7520615965331627,0,1.0599023831807561E-2,0.19991464256105515,0.12322800659084054,8.3629078520877462E-2,0,1.0599023831807561E-2,0.26761049985123403,5.9123067005483865,0,1.9290398930671148E-2,0.10481288110355877,-2.3755051569317458E-3,4.3644893583469305E-2]
[null,167,0.99203173561768909,1.01146577490884,0.97237456705638303,0.99050552206958076,1.003085935572775,1.0021431915940731,0.96816338685914038,null,6.7368706892939541,0,1.0732936212767073E-2,0.19207076063276399,0.12291925592796232,8.1354736155421284E-2,0,1.0732936212767073E-2,0.26353214794717483,5.9131508070603189,0,1.9198882568229769E-2,0.10249720551017752,-2.0494274408421665E-3,4.4196320932745316E-2]
[null,168,1.0013880885145519,1.0051378812856639,1.0420998040018072,1.022645404227368,0.97878019336117872,1.042699433798016,1.0018993469697848,null,6.7649301927130949,0,1.0436741973260317E-2,0.20708320667424007,0.12077037131286535,8.5844061080193657E-2,0,1.0436741973260317E-2,0.27416672920241314,5.9109411605069768,0,1.914753680095627E-2,0.10675808989000579,-2.7576085296211845E-3,4.2976645775065783E-2]
[null,169,1.0081024257494047,0.99645138884072404,1.0043968970414383,0.97044218767238133,0.98872666402379483,1.0281491949937724,1.0204439715739979,null,6.7547778332158561,0,1.0605081823405686E-2,0.19901124852394159,0.12109278069539409,8.3496512744672485E-2,0,1.0605081823405686E-2,0.27602710355024995,5.9102880032817833,0,1.91112772759655E-2,0.10451743315733521,-2.4363653280718642E-3,4.3669839314588066E-2]
[null,170,1.0034061902699183,0.99704277282716203,0.95307286855533768,1.0124919468995091,0.97223582641910589,0.9606403313377847,1.0106707666867925,null,6.7264050980596348,0,1.0407878514393063E-2,0.18098885668749082,0.12258028690301534,8.0224872838644837E-2,0,1.0407878514393063E-2,0.26815074590607829,5.9153840682057766,0,1.9136587411483795E-2,9.7528070877123979E-2,-4.4618195892964443E-4,4.285779118895458E-2]
[null,171,0.97287803858170374,0.95631040286288471,0.98022205944847551,1.0007714513370773,1.0150359112252942,0.97650479736858697,1.037718460720257,null,6.7721149457507339,0,1.0849205687539828E-2,0.19642583219643842,0.12803019075490324,8.2149058378214693E-2,0,1.0849205687539828E-2,0.28604357341792752,5.9132752231452042,0,1.930707445363684E-2,0.10440956936368166,-2.2006738939387323E-3,4.4675097934664489E-2]
[null,172,1.0281900511952502,0.99488822273008948,0.99867241291393749,1.0393637286890538,0.99437922710000826,0.98946811580113925,0.99970980733648029,null,6.7236789235512857,0,1.0063642040021402E-2,0.1872561419033035,0.11890621103810332,8.2996071318451034E-2,0,1.0063642040021402E-2,0.26158990111876246,5.914334841811085,0,1.9005625552529097E-2,9.8623655527387194E-2,-4.7381137763705258E-4,4.1440286659300413E-2]
[null,173,0.96592156354088643,1.0088839731094099,0.99065817851613669,1.0256775184409253,1.014206749690586,1.0112607774250226,0.9902448382475787,null,6.770047317536922,0,1.0959440934390772E-2,0.20151663387475888,0.12602078335961212,8.2708494308232128E-2,0,1.0959440934390772E-2,0.27776440031986566,5.9140433794338652,0,1.9347431094579245E-2,0.10655853725008521,-3.0413691641282743E-3,4.5129027060054172E-2]
[null,174,0.99344815300407052,1.0271187752939757,1.0125890559108297,0.99698734075530149,1.0310455152971463,0.99699813649647473,0.99098689672422435,null,6.7411991484471558,0,1.0227387407259538E-2,0.1942655637684878,0.12124459263459963,8.3927563849546263E-2,0,1.0227387407259538E-2,0.26880378692790813,5.9112582494646055,0,1.9191047432618579E-2,0.10161226321464197,-1.2184797812522209E-3,4.2114560935998184E-2]
[null,175,1.0209544228535223,1.0117593529784807,1.0253146315487249,1.0137378422170698,1.0108330545634634,0.97976591143235903,0.98681038355017958,null,6.7191544164214525,0,9.7340680435123086E-3,0.18840899875533773,0.11845664601696218,8.4592295991646138E-2,0,9.7340680435123086E-3,0.25905464372741843,5.9114346833272648,0,1.9043202590188428E-2,9.7932848249171367E-2,1.4793815979810299E-4,4.0083159603660518E-2]
[null,176,0.97139365132741418,1.0027012192645759,1.0310614424840059,1.0026206356972946,0.98819248820189409,0.99947323051094517,1.0348518323707343,null,6.777399074493375,0,1.0424130481851162E-2,0.20348710462262473,0.12483678672895009,8.5333832771269283E-2,0,1.0424130481851162E-2,0.28760080246969011,5.9105022240932037,0,1.9315637328492636E-2,0.10547227671737555,-2.0743041364335402E-3,4.2924713898204667E-2]
[null,177,1.0428248100862152,0.99477569762785745,0.98990736573477456,1.0345677907777506,0.97148678112159803,0.99148317887737858,0.97631718747311902,null,6.7076308327893033,0,1.0019477309524393E-2,0.18402810136810599,0.1174002141948962,8.2320685166616878E-2,0,1.0019477309524393E-2,0.25204886967493378,5.9145657159554617,0,1.8931216313953107E-2,9.7347337805895107E-2,-2.6973185070087411E-4,4.1258424160142713E-2]
[null,178,1.0413304778422834,1.0254878602095885,1.0313918686552594,1.013627634743834,0.99732306683331995,0.97846431160742187,0.9999486328076167,null,6.7068012153048029,0,9.4257697104468859E-3,0.1840882137344117,0.11540461784680568,8.4939603256046853E-2,0,9.4257697104468859E-3,0.25714786594435307,5.9110776393355318,0,1.8938718248555985E-2,9.5401905049649571E-2,9.8900994629256785E-4,3.8813641943154731E-2]
[null,179,0.99455916179560555,0.95195171832432746,0.96764524663192886,1.0284953221089372,0.98564545261382019,0.97557182437308987,1.0278025905545292,null,6.7541658462876457,0,1.0740380526952285E-2,0.19085905123605851,0.12570682478245807,8.1263576196418816E-2,0,1.0740380526952285E-2,0.27706795761475689,5.915462731925949,0,1.918491733052578E-2,0.10209304463617669,-1.6992327282195829E-3,4.4226975293521494E-2]
[null,180,0.99990103601949543,1.0349270677197542,0.98486938246756728,1.0198385704446189,1.0076024759181907,0.9884768855661783,1.0162996504090398,null,6.7376121732206506,0,1.0288045053466333E-2,0.18755449250089493,0.12060985801280463,8.2277609363273788E-2,0,1.0288045053466333E-2,0.27296815115027534,5.914049257420035,0,1.9155633218578424E-2,9.946256133373238E-2,-8.297281053642777E-4,4.236433832641924E-2]
[null,181,0.99825749737427549,0.96709886415486013,1.0191495226041916,0.99565437861692585,1.015104946389024,0.97295037702625686,0.98404548571532913,null,6.7382450324392247,0,1.0133799022340356E-2,0.19436561909195679,0.12347608408027273,8.4266743455089374E-2,0,1.0133799022340356E-2,0.26397138512280971,5.9108118052368059,0,1.9164609704669471E-2,0.10133603179286541,-8.7642667026019991E-4,4.1729180625012519E-2]
[null,182,0.98501258493123167,0.9846275375984832,1.0022730082340041,1.0130743675222578,1.006442769804992,0.98179048408599223,0.99405105065992683,null,6.7500693748138243,0,1.0436788868861468E-2,0.19523798991782496,0.12456521761366121,8.3328191305163252E-2,0,1.0436788868861468E-2,0.27088506351054148,5.9127115783053847,0,1.9238042620421707E-2,0.10264384369115223,-1.5173910331314666E-3,4.2976838882804208E-2]
[null,183,0.98735084793123185,1.0222721414207045,0.95901572732329909,1.0213453998687698,0.97632725222159056,0.99563199825991477,1.0177780776970724,null,6.749896785341261,0,1.0789842251201623E-2,0.18929573923232129,0.12322519542604526,8.0726281884809598E-2,0,1.0789842251201623E-2,0.27759473544325142,5.9155434956656077,0,1.9224935535422746E-2,0.10169827956506351,-1.842527281385451E-3,4.443064987012154E-2]
[null,184,1.0247449809437323,0.97786382985372566,1.0076929545338664,0.97877746885904482,1.0377703688605326,0.99275141783392484,0.96541655189427966,null,6.7187697120341303,0,1.0126056432610279E-2,0.19095176445943893,0.11996580231961997,8.3408293473160394E-2,0,1.0126056432610279E-2,0.25393660369326038,5.9105521521675506,0,1.9023450773661337E-2,0.1001211038334445,-8.8675670463682973E-4,4.1697298018633658E-2]
[null,185,0.99238469145917696,1.0114440619333827,0.96272621395050961,1.0254384578703957,1.0302114995951226,1.0268793259176954,1.0006864079573778,null,6.7564463833779955,0,1.1086770256046232E-2,0.19558027632415889,0.12305506414787216,8.092207623023881E-2,0,1.1086770256046232E-2,0.27461083486614718,5.9155643896673462,0,1.9196928045195363E-2,0.10487805402191086,-3.014586467735524E-3,4.5653346542856986E-2]
[null,186,0.99328467348311178,1.0042052484621591,0.99164912077202882,0.97077291730378545,0.96111272200581932,1.0235229735406639,0.98072079516238364,null,6.7499490350836524,0,1.0798907444689846E-2,0.19885673669607129,0.12275863669350953,8.2608036138839588E-2,0,1.0798907444689846E-2,0.26870269107320022,5.9110205703620933,0,1.91919506046004E-2,0.1051001056556895,-2.7576708637125523E-3,4.4467978723361758E-2]
[null,187,1.0231710883508329,0.97102359276115302,1.034029431506285,0.97678566416685852,0.98567530347119037,1.0056118660332223,1.0137655822959408,null,6.7414453435543003,0,1.0069099022184403E-2,0.19742069414164071,0.11999529634803145,8.5230748018785649E-2,0,1.0069099022184403E-2,0.26839820137930137,5.908934667450187,0,1.9031634235711737E-2,0.1021791776621619,-1.2078332220633848E-3,4.1462757540541045E-2]
[null,188,0.98624105823974995,1.0383773091663406,1.0100731686048645,1.0267304276161924,1.020691340522808,1.004880164118497,0.99564198511171698,null,6.7501285317687101,0,1.0358026084914164E-2,0.19601565297027826,0.12164653786891882,8.3846137938621126E-2,0,1.0358026084914164E-2,0.27267438585514792,5.913008351785308,0,1.9231148689809761E-2,0.10265525575807452,-1.6014468552075388E-3,4.2652507757762151E-2]
[null,189,0.97973261259154687,1.0089787227222971,1.024565684919168,1.0108184813503984,1.0074642419018245,0.98591361916860953,1.0018887567651622,null,6.7549640768355275,0,1.0226013138638787E-2,0.19771181691883355,0.12359106199020926,8.4760390054237911E-2,0,1.0226013138638787E-2,0.27469337967742363,5.9113201026580739,0,1.9267869535957174E-2,0.10280619149607199,-1.2956374377101313E-3,4.2108901942428625E-2]
[null,190,1.0121275567565606,1.0099520047802282,1.0122218599453328,1.0008505594278272,0.99257369596648637,0.97086748209548535,1.0370609804998323,null,6.7336448911720534,0,9.8494698141067347E-3,0.1869855010999581,0.1198188103342054,8.3973255061602178E-2,0,9.8494698141067347E-3,0.27375802238482971,5.9114878750211481,0,1.9089770953569962E-2,9.7822111468826925E-2,1.5118129368835078E-4,4.0558363554218914E-2]
[null,191,0.99403978827343753,0.99438772377690854,1.0177173929952055,1.0330385963953923,1.0236498315860911,1.0021880645132999,1.0118265642126494,null,6.7572526053076221,0,1.0371320423811508E-2,0.1985002401322645,0.12265474739218529,8.4357222057549003E-2,0,1.0371320423811508E-2,0.27511813148275771,5.9129135199323501,0,1.9187781320252267E-2,0.1035647727575664,-1.7510612463394173E-3,4.2707251479037291E-2]
[null,192,1.0273250269783514,0.98599869970472676,0.99633153627364179,0.95812097392136386,0.97463838108227907,0.97710754709714587,0.969036477203438,null,6.7083074940209126,0,1.0005050528497433E-2,0.1855213004287263,0.11947723955464087,8.2674216381449769E-2,0,1.0005050528497433E-2,0.25275107303829486,5.9100753195893674,0,1.901009005473055E-2,9.7823728738257149E-2,-2.2449100830035037E-4,4.1199017243744987E-2]
[null,193,1.0117362075506084,1.0212630709973025,0.98297828613951155,0.9753794959912393,1.021423594762062,1.0133714346687321,1.0010371153940287,null,6.7347192548886312,0,1.0500515909670041E-2,0.19089171095922564,0.11986882751226928,8.2063348032502856E-2,0,1.0500515909670041E-2,0.26813708637659461,5.9117505348439794,0,1.9091854426950137E-2,0.10132807880139198,-1.6514415581507789E-3,4.3239255493863496E-2]
[null,194,0.98100316767654261,0.96894674037115491,0.98495198124842165,1.015321725649668,1.0095433980966888,0.98589645354161437,0.97919680789340613,null,6.7521999236524497,0,1.0757377839695432E-2,0.19613461181691508,0.12621410940347427,8.2221050383094671E-2,0,1.0757377839695432E-2,0.26844843158232756,5.9138005228344568,0,1.9260662750969999E-2,0.10400841599431541,-2.1848483150957235E-3,4.429696720198887E-2]
[null,195,0.98373766456064027,1.0265846855774499,0.99937871311094184,1.0157406546396197,1.0069538570875181,0.97337328259209599,0.99470570383606494,null,6.739767479900002,0,1.0202988676254512E-2,0.19004776256478689,0.12271660771960766,8.3141735736445246E-2,0,1.0202988676254512E-2,0.27023103290279171,5.9130184956462903,0,1.9245215408875221E-2,0.10005882217004483,-7.0628355337508083E-4,4.2014091304531709E-2]
[null,196,1.0025862492211643,0.9819556497988623,1.0068677943667885,0.9881782661550923,0.98502272971623062,1.0048036321208935,0.99035265258160465,null,6.7452174357022336,0,1.0464320533149284E-2,0.19708961683933826,0.12242818980991568,8.3546195772384202E-2,0,1.0464320533149284E-2,0.26734035189007999,5.9111068326263343,0,1.9141030757662925E-2,0.10338157513599962,-1.906566505367408E-3,4.3090209375887874E-2]
[null,197,1.0081134594377099,1.034537024012198,1.0256506503982181,0.99490154506205186,1.0189798029502888,0.99265468939984691,1.0342704656014023,null,6.7406711183960102,0,9.8901209487368084E-3,0.19152463950885862,0.11889567763350699,8.4831590596638209E-2,0,9.8901209487368084E-3,0.27600517157991528,5.9103977719225735,0,1.9111218088099874E-2,9.953588301202089E-2,-3.5659163660317411E-4,4.072575769099334E-2]
[null,198,1.0230902810733482,1.0010396006285325,1.0043031373603908,0.97698439481659816,0.97019708874139865,1.0173728250290672,1.007253121546418,null,6.7358860603878092,0,1.0320713290847031E-2,0.19364799677524841,0.11910148266334659,8.3378642292206095E-2,0,1.0320713290847031E-2,0.26741717040025559,5.9106468271315435,0,1.9032055073080988E-2,0.10170546890423715,-1.5424431653316263E-3,4.2498860313223447E-2]
[null,199,0.9794046166312157,0.95426807011701498,1.0323767496418639,1.000594695864975,1.0399111066265128,0.98992958444828894,0.98728670198737278,null,6.7638336327418109,0,1.044774121100003E-2,0.20434487216291358,0.12626606928013193,8.5195529075879045E-2,0,1.044774121100003E-2,0.27174257171563554,5.9103165766892038,0,1.9269733016336034E-2,0.10584860313444466,-2.1722610110253677E-3,4.3021938678286589E-2]
[null,200,1.0381866153621877,1.0245943917931342,1.0254631257705686,0.98240962852510871,0.95536062494094287,1.0241786763926688,0.98849744305351228,null,6.7210754730920215,0,9.9512785954766064E-3,0.19265554373845953,0.11590185694841318,8.4576857483822043E-2,0,9.9512785954766064E-3,0.25903148368926709,5.9097337486247694,0,1.8954571763875452E-2,0.10013284527730627,-8.8902842850419148E-4,4.0977593994612496E-2]
[null,201,0.99994909910173846,0.99085278239869279,0.98972247289851634,1.0102498328240859,1.0392258081604033,0.99036113812939541,1.0084005918078114,null,6.7442358579012138,0,1.0456637207798053E-2,0.19200479302137635,0.12263121205466207,8.2552338561186794E-2,0,1.0456637207798053E-2,0.27142597006696989,5.9132615854507753,0,1.9155371157365084E-2,0.10157622038422066,-1.4302036050172586E-3,4.3058570809672438E-2]
[null,202,1.0075936456572785,1.0061084159799429,0.96480582296037576,1.017825964595628,1.0359779399884101,0.9785714113439663,1.0389515435324388,null,6.7378382888391766,0,1.0410474631058599E-2,0.18421804000140587,0.12141642506117251,8.1066193824120683E-2,0,1.0410474631058599E-2,0.2761887460156226,5.9150400720099778,0,1.9114007926171052E-2,9.8681669459669788E-2,-7.5534699426031053E-4,4.2868481535291721E-2]
[null,203,0.98717551479523791,0.97541953392377045,0.95944265222524616,1.0327119369191253,1.0327264887656922,0.99584348981842719,0.96109873005634006,null,6.7440269292982338,0,1.1009071393694612E-2,0.19326443739112598,0.12557377423187413,8.0566959111251238E-2,0,1.1009071393694612E-2,0.26265339640573082,5.9161351479936402,0,1.922591620829819E-2,0.10380806241964471,-2.5341609209119523E-3,4.5333396457574962E-2]
[null,204,0.96303615433994783,1.0138790777636526,1.0135842665901755,1.0126343883784918,1.0049516418382458,0.99293811415942557,1.0425723732969721,null,6.7800795450767684,0,1.055670935409244E-2,0.20081649288257231,0.1257047971498042,8.4309483057776052E-2,0,1.055670935409244E-2,0.2914480235532329,5.912047028419968,0,1.9364341304546433E-2,0.10498715618718091,-2.0684275742480851E-3,4.3470650095934704E-2]
[null,205,0.98453110470532001,0.99105890410386266,0.99555498311489821,0.9841109198018777,0.98504194739468121,0.98419906617246355,0.9888001839246191,null,6.7464841688452912,0,1.0499779017001942E-2,0.19447100943899023,0.1244302665160557,8.2874792245424281E-2,0,1.0499779017001942E-2,0.26974055118064338,5.9115234238332537,0,1.9240749277747986E-2,0.10258245074632073,-1.6152954941646804E-3,4.3236221101018289E-2]
[null,206,0.95969524580700527,0.97253613916280179,1.0073753081036652,0.99106975162715594,1.0041028447370557,0.98517220675776429,1.027471774776946,null,6.7816262326463095,0,1.0758017652172165E-2,0.20277355977414102,0.12838381232621232,8.3859532471720302E-2,0,1.0758017652172165E-2,0.28786385689880223,5.9112343609652269,0,1.9384048040228266E-2,0.10633630857334964,-2.5088482392564017E-3,4.4299601835885695E-2]
[null,207,0.99089355227572129,0.99785929778120419,1.0170482819376279,1.0138910628278734,1.0190535455356358,0.98155891586622557,1.0298136859272278,null,6.754401883867966,0,1.0180847155649351E-2,0.19466189638820147,0.12288555558012403,8.4352427502147984E-2,0,1.0180847155649351E-2,0.27883670527783055,5.9119172794531094,0,1.9205194840132892E-2,0.10159568582268889,-9.7577745999435645E-4,4.1922916463723404E-2]
[null,208,1.0464221222974648,1.0362494298346487,1.042272410770428,0.98145990391701465,1.0250119015385593,0.98126971436060439,1.0125409931254337,null,6.7051730832107106,0,9.2759400797627137E-3,0.1840977914491804,0.114169110532174,8.56152985496519E-2,0,9.2759400797627137E-3,0.25930500094773823,5.9087067658179278,0,1.8913244748644094E-2,9.4900368526061471E-2,1.2688324466598525E-3,3.8196670192677411E-2]
[null,209,0.99378894011758701,1.0411038887360684,1.0334607060755945,1.0126927617350037,0.99329141669045895,1.0096723082895729,0.96454831355287396,null,6.7387919886038965,0,1.0107674424296284E-2,0.19801053725574996,0.12015762699833904,8.5144759068425932E-2,0,1.0107674424296284E-2,0.26259940971798357,5.9109071642122437,0,1.9189165648325655E-2,0.10251301758333435,-1.3512960607769079E-3,4.1621604180272144E-2]
[null,210,1.040002052666964,1.0348395247548934,0.99108291107950075,0.97408958546632785,1.0085967571138814,1.0235455977234087,1.013038559652863,null,6.7208307548276114,0,1.0187270832259513E-2,0.18743634608085233,0.11585344386951038,8.2519816447259906E-2,0,1.0187270832259513E-2,0.26478483956905718,5.9112313716338054,0,1.8945405387736956E-2,9.9092140234503717E-2,-9.8197641574661147E-4,4.1949368020632254E-2]
[null,211,0.99247839572630947,1.0293133918227881,0.98546681260960511,1.0258023998530661,0.97529462455471994,0.99074951290402691,0.96369955491655279,null,6.7306716675449714,0,1.0407595674009633E-2,0.1899021294239773,0.1217654647837203,8.2161414971181429E-2,0,1.0407595674009633E-2,0.26102854213865978,5.9143385419722208,0,1.9196409383361427E-2,0.10067748590157446,-1.2549475323267746E-3,4.2856626502599332E-2]
[null,212,0.97375666519345483,0.97880644678062234,1.0217114883503999,1.0056373375186336,0.99325613543587921,0.99671264414770255,0.97905911977374416,null,6.7627820955380606,0,1.0564011969579566E-2,0.2033864048709049,0.12592485832556,8.4535531869117872E-2,0,1.0564011969579566E-2,0.2714029251374574,5.9112042668067382,0,1.9302018284996104E-2,0.10590546735704283,-2.3800980804523897E-3,4.3500720966693572E-2]
[null,213,1.0164862556598544,0.96877395347300488,1.0144182595084132,0.99116352444600664,1.0370107953162135,0.95806288752687385,0.98503090504371471,null,6.7189969665359097,0,9.8331486109360135E-3,0.18728347140817445,0.12126690422485541,8.3889874196287365E-2,0,9.8331486109360135E-3,0.25809421934189508,5.9108394253651575,0,1.906667445477226E-2,9.7871758244459775E-2,1.9348355567800902E-4,4.0491155744627763E-2]
[null,214,0.99152600437807659,0.99725188303075529,0.98354979893331163,1.0116729896852166,1.0108828217753789,1.0051558815316748,0.99453616075799389,null,6.7506326507926229,0,1.0731151361115148E-2,0.19524994541688181,0.12347096109073309,8.2168061004634807E-2,0,1.0731151361115148E-2,0.27129487968201838,5.9136808719723737,0,1.92016855233746E-2,0.10361187814491661,-2.234603273647225E-3,4.4188971231334424E-2]
[null,215,1.0143760683082996,1.0159158738342684,1.0115712272400963,0.97510480104072716,0.98885021391210337,1.0027967353354932,0.97647347678683638,null,6.725648635747719,0,1.0131051998100698E-2,0.19214601213141461,0.11928399828891713,8.3728330545138119E-2,0,1.0131051998100698E-2,0.26002190269056635,5.9101337535410785,0,1.9077831432118272E-2,0.1005541796285101,-1.0152413781697477E-3,4.1717868868145699E-2]
[null,216,0.99063250567060945,0.99291681325162784,0.99949066545304588,0.98872403967716804,0.97380004880848947,1.0176354917124624,1.0151504414919836,null,6.7630723005768845,0,1.0743977516384725E-2,0.20015778218775995,0.12349670601520593,8.3238737746462718E-2,0,1.0743977516384725E-2,0.27845141947778768,5.911552143753994,0,1.9206644628176259E-2,0.10537581668506467,-2.6487369733299623E-3,4.424178705576403E-2]
[null,217,1.0141177053821044,1.0051895137942242,1.0163069874710713,1.012431711064528,1.0093506082784702,0.96221061327285673,0.96281722219488342,null,6.7108518160538635,0,9.7273979736174701E-3,0.18578787057375001,0.11973413891129035,8.3952345032341003E-2,0,9.7273979736174701E-3,0.25293300585110673,5.9118807844748433,0,1.9079200638378192E-2,9.6999718586925118E-2,4.2905854216231289E-4,4.0055693443061764E-2]
[null,218,1.0272794242845182,1.0205487300816516,0.98972272074366252,0.97903584519246578,0.96364094029487091,0.98613954041426954,1.0253441545812714,null,6.721069171153121,0,1.0007698111700028E-2,0.18376143997844066,0.1179669786503818,8.2482102343230959E-2,0,1.0007698111700028E-2,0.2679711540006024,5.9115744090026432,0,1.9010325624784354E-2,9.7215230538980499E-2,-1.2238850606065841E-4,4.1209919520121027E-2]
[null,219,0.99090125816669516,1.0272503175318104,1.0044700055273581,1.0159071802525466,0.9597404295871842,0.97900789953592349,0.98528227593542228,null,6.7346337159369467,0,1.013983023184656E-2,0.19030110363782171,0.12170251898125933,8.3404012944815004E-2,0,1.013983023184656E-2,0.2662613023110933,5.912740755008449,0,1.9205152055134622E-2,9.993938626873379E-2,-6.7453134260438564E-4,4.1754016072243806E-2]
[null,220,1.0196534347626174,1.0129060872451652,0.98508728085495512,1.0211609945168514,0.96215745405323083,1.0053103831397894,0.98639800811073097,null,6.7264441034975526,0,1.0353461699594132E-2,0.18880806740385092,0.1192913820346294,8.2139039138930073E-2,0,1.0353461699594132E-2,0.26151705764659422,5.9141086747982881,0,1.9050015622061749E-2,0.10011644675987574,-1.2202923381284508E-3,4.2633712431444558E-2]
[null,221,0.97997798652361712,0.96294499050319005,0.99300258303270184,0.97075638369641781,0.97671197135016419,1.0310027504785448,1.0167350708714982,null,6.7815327081535894,0,1.1212326734106305E-2,0.20688430562044846,0.12650509726436487,8.2891586849045018E-2,0,1.1212326734106305E-2,0.28359555186434737,5.9109442250179152,0,1.9266476281059011E-2,0.10926914670793351,-3.9940472228166199E-3,4.6170365771288371E-2]
[null,222,0.95962636483574881,0.99672708228734597,0.95473144576905433,1.0060691494508376,1.0457234572753877,1.0002114548238958,0.96937611436656468,null,6.76237574656784,0,1.131620239639167E-2,0.19727003081018815,0.12815716010977812,8.03862297586867E-2,0,1.131620239639167E-2,0.27270597908510774,5.9149477892246818,0,1.9384455786302712E-2,0.1062121922753729,-3.2861977416790773E-3,4.6598107259400876E-2]
[null,223,1.0221322745464807,0.98631639533194293,0.97020994593293186,0.98407806444128765,1.0107070595587548,0.98927429964239622,0.98868388281276909,null,6.7207952314931951,0,1.0414212039179202E-2,0.18576908430585903,0.12054636874364506,8.1170313676719535E-2,0,1.0414212039179202E-2,0.26025552943806768,5.9129214373392962,0,1.9037049359534014E-2,9.9242248805716304E-2,-1.0306716923393579E-3,4.2883871516698514E-2]
[null,224,1.0318357622107033,0.96419963576148282,0.98442663608267034,1.0322827536670212,1.0204383292323354,0.99476390346842303,0.96465602836998321,null,6.7181477006022794,0,1.034591016184761E-2,0.18848557975689167,0.12024184368288672,8.1982709267500203E-2,0,1.034591016184761E-2,0.25227390791605803,5.9147464511069474,0,1.8986891820305104E-2,9.9978448340978424E-2,-1.1507478324161307E-3,4.2602616543127983E-2]
[null,225,0.99310698382594675,0.99823362593422182,0.989207701625337,0.98925523286797346,1.026384645170469,0.9889079082983051,0.959271154144958,null,6.7323913354527427,0,1.0484565894023095E-2,0.19237074243037547,0.12311976153163286,8.2350968999255911E-2,0,1.0484565894023095E-2,0.25977768900450743,5.9121554189400651,0,1.9192932620275556E-2,0.10179595179947348,-1.5457060412788516E-3,4.3173576168426347E-2]
[null,226,0.99990614165171809,0.99441936023499222,0.9778205107463579,0.9613496006537624,0.98611383849847001,0.96907311417725794,1.0122090290657983,null,6.7324238332913238,0,1.0323156320768795E-2,0.18623684389182144,0.12268214201029989,8.1762578350187534E-2,0,1.0323156320768795E-2,0.27037045547349275,5.9112761617956675,0,1.9155605379214107E-2,9.9112799898383189E-2,-6.8167378334450855E-4,4.2508920275598161E-2]
[null,227,1.037678002060898,0.9959839078422752,0.97538388564193157,0.96742753734169651,1.0094948405495785,1.0280375918342188,0.98762595902408357,null,6.7226577414707807,0,1.056795948055164E-2,0.18996508847257362,0.11818572122748247,8.1469335312256141E-2,0,1.056795948055164E-2,0.25948282577447701,5.9117384256371128,0,1.8957145569342474E-2,0.10122051211139013,-1.878288748097486E-3,4.351697611424582E-2]
[null,228,0.99624973853615417,1.004907353084507,0.99467842885186641,0.97639426489239245,0.97796775680153003,1.0193958153597784,1.0138348376436717,null,6.7558260777754242,0,1.069183335143209E-2,0.19777104679937113,0.12230238516789514,8.2904792243058009E-2,0,1.069183335143209E-2,0.27655127151028414,5.9111553717296648,0,1.9175615635683083E-2,0.10436871865705533,-2.4301906333921057E-3,4.4027066665804436E-2]
[null,229,1.0092593041289499,1.0008526105796423,1.0048738012063914,1.0277069960097935,1.0023177248618491,0.98162469937940877,0.97768836321414432,null,6.7263404764659045,0,1.00903073480113E-2,0.18948495373853472,0.12073206644782447,8.335025328576226E-2,0,1.00903073480113E-2,0.25986468604989182,5.9133555964087607,0,1.9105078494522337E-2,9.9490857602730021E-2,-5.9310521347751281E-4,4.1550089651354927E-2]
[null,230,1.0025587336358368,1.0360434309393132,1.0080700970759437,0.99658237799582894,1.0110942019149745,1.034703155321878,0.99498561635015559,null,6.7485058093627819,0,1.0520355805339145E-2,0.19849806256602251,0.11981144510533427,8.3673798618601997E-2,0,1.0520355805339145E-2,0.27082491460478425,5.911492901444559,0,1.9141179993535214E-2,0.10405839975501631,-2.3158453779358783E-3,4.3320952652859082E-2]
[null,231,1.0090881140156045,0.95837915504488447,1.0081824636055534,1.0167815500220097,1.0228898963785347,1.0046571264104263,1.0077567646408261,null,6.7517204367140247,0,1.0492212738989886E-2,0.19799999749845734,0.12280265680618264,8.3691165422100519E-2,0,1.0492212738989886E-2,0.27054149263065336,5.9125780124636336,0,1.9105994868753286E-2,0.10379152665444499,-1.9954741451173558E-3,4.3205064514911913E-2]
[null,232,0.99837767279712963,1.0169368978682998,1.0081876075192193,0.98085864575653336,1.0348892867130595,0.98634798793374578,0.99493567702600416,null,6.7351883350389778,0,1.0150192040667062E-2,0.1915471364210827,0.12121014674227737,8.3626936919315775E-2,0,1.0150192040667062E-2,0.26763389026091494,5.9106366022208894,0,1.9163952343178227E-2,0.10040868357308762,-8.3569759840739194E-4,4.1796684156633415E-2]
[null,233,0.98896262260293444,0.96846739747823385,0.99649418190274708,0.96896851947183937,1.0347083403466011,1.0222664966875825,0.98850733964405191,null,6.7623085001681345,0,1.0955884355494308E-2,0.20320135840253173,0.12500255284387973,8.2956330410004595E-2,0,1.0955884355494308E-2,0.27231883490535602,5.9106524803463261,0,1.9215936851732802E-2,0.1071375986626313,-3.2909739555344289E-3,4.5114381701205998E-2]
[null,234,0.99912462524989376,0.9604119242171133,1.0219768639862166,0.98963803590852595,1.0148113156851328,0.97092888980454484,1.0105717234200944,null,6.745299034425094,0,1.0109027474071249E-2,0.19470310550110362,0.12365737332424999,8.4529098266465874E-2,0,1.0109027474071249E-2,0.27073001879248332,5.9103246868637331,0,1.9159870047328092E-2,0.10137073858572823,-8.0303275441091435E-4,4.1627175798411575E-2]
[null,235,1.0068151320223002,0.9880167268668183,0.98675186338724308,0.97987062312019502,1.005703895760736,1.0122277178675914,0.99898569885140243,null,6.7440605026023164,0,1.0655253526579539E-2,0.19479188603454944,0.12198988487052949,8.2314897965093933E-2,0,1.0655253526579539E-2,0.26913687166600825,5.9117844915862605,0,1.9118191593176997E-2,0.1032035521406358,-2.1557107119672667E-3,4.3876437458027738E-2]
[null,236,0.98582410156671219,1.010035648047849,0.99506020241126958,0.96803222554359103,0.99448722920728727,0.99672116119165655,1.0227538051882554,null,6.7554446909661134,0,1.053805451337482E-2,0.19503686086172337,0.12333719165839495,8.296492905447439E-2,0,1.053805451337482E-2,0.27967134712413022,5.9106820904990247,0,1.9233486635720609E-2,0.10290626647743721,-1.7813141270895331E-3,4.3393832782297408E-2]
[null,237,1.0012512004895702,0.95679028565607582,1.0152558724049443,1.0176774720953576,1.0038794659396177,0.98903464694410459,0.98285523580763257,null,6.7452044472395762,0,1.0353065596593616E-2,0.19743045272190315,0.12371051801568306,8.4048669724027011E-2,0,1.0353065596593616E-2,0.26447882602736389,5.9122242108217398,0,1.9148281097543327E-2,0.10313177963062271,-1.6003721490975751E-3,4.2632081349792142E-2]
[null,238,1.0140242239262927,0.98604931597647816,1.0302905142226453,0.98662088791770186,1.0146878963199146,1.0008322178049174,1.0251639791600333,null,6.7462815049364613,0,1.007827257374496E-2,0.19651163238391681,0.12040682543994907,8.5074077390455194E-2,0,1.007827257374496E-2,0.27323127772382699,5.9096825961772428,0,1.9079696219566972E-2,0.10189524068805143,-1.1003736795878233E-3,4.1500532593036099E-2]
[null,239,0.99134449279627468,1.0129352381889245,0.97908081548461656,0.96977808781421793,0.97843001702749433,0.98667017924534783,1.044784501547025,null,6.7515920196374806,0,1.0506409947613206E-2,0.1898976618095336,0.12280843961161952,8.2014929925370822E-2,0,1.0506409947613206E-2,0.28305400886829085,5.9116625427007214,0,1.9202692227099225E-2,0.10099724453276254,-1.309026130933596E-3,4.3263526093013802E-2]
[null,240,0.9677689977615721,0.9982287655707861,1.0186357666372972,1.0403220950566101,0.98437479993146459,1.0065547621874529,1.0186344571896031,null,6.780315773218252,0,1.0673035454673189E-2,0.20455260888623836,0.12577221764600138,8.4554153600141568E-2,0,1.0673035454673189E-2,0.28488167171439704,5.9132544642867382,0,1.9336656983271073E-2,0.10667420833818611,-2.6598685095751274E-3,4.394966027285218E-2]
[null,241,1.0087489636739757,1.0003593579159002,0.98697055230761277,0.96996176156009595,1.0194505805222511,1.0076301434777055,1.0186389748940001,null,6.7433542235554471,0,1.0528357329301611E-2,0.19253448724474737,0.12114884732492166,8.2376953778979273E-2,0,1.0528357329301611E-2,0.2733347454521603,5.9112367531997618,0,1.9107811246228585E-2,0.10199641178211148,-1.7356879777863095E-3,4.3353901504318337E-2]
[null,242,1.0099696551023416,0.99941936978256218,0.98741904183807894,0.99733496099624697,0.98553465336221568,0.96756509644568567,1.0331315463708137,null,6.7323550717870333,0,1.0097628655716066E-2,0.18478050233997051,0.12103966012146448,8.2420408770226425E-2,0,1.0097628655716066E-2,0.27303520411630289,5.9126914965022701,0,1.9101279331463838E-2,9.7866772063736368E-2,-1.6048895174578337E-4,4.1580237493338952E-2]
[null,243,1.01301067153692,0.97323573527569884,1.004734422781602,0.99232370798080383,1.0371891459985167,1.0150711838880138,1.0090613844073026,null,6.7487981930243395,0,1.0522152505692783E-2,0.19755375234876452,0.12164143658053661,8.3460767137366568E-2,0,1.0522152505692783E-2,0.27065547633118703,5.911451405162472,0,1.9085075322964506E-2,0.10373462241001971,-2.1126934140906495E-3,4.3328351145114623E-2]
[null,244,1.004848719243981,1.022151311931603,1.0426611095708744,1.0272059537822555,0.95686193983720624,1.0083935882520212,1.0194613689223053,null,6.7507010900010602,0,9.9816665675180483E-3,0.19821796200673053,0.11953851912493869,8.5887397893994522E-2,0,9.9816665675180483E-3,0.27456807545245115,5.9111545998516579,0,1.9128787797186669E-2,0.10215977590312904,-1.0567542836562326E-3,4.1102726254621774E-2]
[null,245,1.0031195410730842,1.0123349618651525,1.0155042838077923,0.97575300919496721,0.98898427612302886,1.0384832190387596,1.0110701655401324,null,6.7580889218650331,0,1.0588868807317813E-2,0.20200140450950049,0.1207194494939838,8.4184946626733856E-2,0,1.0588868807317813E-2,0.27567054872058033,5.9099448801598342,0,1.9138139967589816E-2,0.10550657293763273,-2.6800975509723266E-3,4.360307700014749E-2]
[null,246,0.9963259700882624,0.96586964923412422,1.0051152792136675,0.99586787775818464,0.98649217277107448,1.0013586155018395,0.97285495516786746,null,6.7469646417184563,0,1.0584750847889526E-2,0.19884115819994089,0.1240476193178614,8.3400257153553384E-2,0,1.0584750847889526E-2,0.26411836149971973,5.9116214207318292,0,1.9175196947086963E-2,0.1043909263481648,-2.216418455894471E-3,4.3586119976191259E-2]
[null,247,1.0173839558981952,1.0123761587910931,0.98771775934905481,0.98049151551312053,1.0311056540842909,0.98072615853047251,1.0340320379715804,null,6.7293826639905134,0,1.010186809696881E-2,0.18493998301388256,0.1195346194082634,8.2418304722639057E-2,0,1.010186809696881E-2,0.27242451808058193,5.9117644740661959,0,1.9061942168745315E-2,9.7936634783514956E-2,-2.9550701114044802E-4,4.1597694757825342E-2]
[null,248,0.99013985977652197,0.9778931776880514,0.9979171071132612,0.96378396491321128,1.0085472818803556,0.99931032672313014,0.99231810682161625,null,6.7511612770286709,0,1.0639563473690388E-2,0.19775099429833501,0.12434401440313472,8.3019819039560364E-2,0,1.0639563473690388E-2,0.27074338868006725,5.9102925751271389,0,1.9209382743841992E-2,0.10419016416107971,-2.2008900374432395E-3,4.3811828612955524E-2]
[null,249,0.98809192651665811,0.97520219905391192,0.99776166400425992,1.0192833311641651,1.0195745024743506,1.0026542218931942,1.0057070080604842,null,6.7613171918149364,0,1.0711389727129202E-2,0.19904013571345425,0.12474212341239908,8.3111580239073446E-2,0,1.0711389727129202E-2,0.27531894191751416,5.9133007286905244,0,1.9220794380761227E-2,0.104877484456199,-2.4021933350169482E-3,4.4107596340020039E-2]
[null,250,1.024484529276503,0.99945147734935891,1.0223149756962517,1.0052317284338557,0.99486096435255567,0.98301936908559895,1.0054595959569557,null,6.7245442136439895,0,9.8096220228974743E-3,0.18903096874319261,0.11868333064362338,8.4460397657833045E-2,0,9.8096220228974743E-3,0.2634456224095072,5.9111477032157156,0,1.9024803257170417E-2,9.8401206456480414E-2,-4.4096182200049684E-5,4.0394277442661622E-2]
[null,251,0.99298709824297959,1.0028925148560459,1.0180450210281911,1.0009583261772272,0.97539436170023808,1.010478748044831,0.97333483966226253,null,6.7472649361894304,0,1.0427095879336845E-2,0.19966450609076442,0.12236098465384769,8.4225027428006222E-2,0,1.0427095879336845E-2,0.26561383923556825,5.9111615652200582,0,1.9193595375803275E-2,0.1041553872526793,-2.0468939445319754E-3,4.2936924877229624E-2]
[null,252,1.0235375119811887,0.99887031705940255,1.0132092865730051,1.0020922598500928,0.97029831350302598,1.0194821389340116,1.0049733622828476,null,6.738376053875081,0,1.0266936255715254E-2,0.19519588429727669,0.1189889778200388,8.3942155246833822E-2,0,1.0266936255715254E-2,0.26692863941984701,5.9114987779444021,0,1.9029726766703444E-2,0.10206759612871555,-1.5531198032441062E-3,4.2277416054506231E-2]
[null,253,1.0184902410324213,1.0089298834181626,0.96972735092874118,1.0037930562422936,1.0289015567446294,0.99019763500060143,1.0000883494513053,null,6.7235232838741359,0,1.036447334373122E-2,0.18474941413796497,0.11989416361516977,8.1204360547025095E-2,0,1.036447334373122E-2,0.26406869456726767,5.9140137037878882,0,1.9056121788460306E-2,9.8721467028767329E-2,-8.6369802041315411E-4,4.2679056422001489E-2]
[null,254,0.96917269207358947,0.987560268529448,0.98682108011244207,0.99352274163821908,1.0313902385037588,1.0067213037941776,0.97747787278492215,null,6.7642156854083071,0,1.1010401672367142E-2,0.20130511747764349,0.12675003360462189,8.2383663676828964E-2,0,1.1010401672367142E-2,0.27304948891112529,5.912518605229649,0,1.9328498194173628E-2,0.1066506700780801,-3.1092660721873723E-3,4.5338874308367645E-2]
[null,255,0.98251790329733368,1.0170206298709827,1.0084596765068221,0.95436685393966403,0.97801588722468291,1.0092126386835842,1.0023219625454083,null,6.7563249766603208,0,1.0550245030925188E-2,0.19917686484872196,0.12315748567815253,8.374061553271861E-2,0,1.0550245030925188E-2,0.27615578493388493,5.9091896951756731,0,1.9252095292715522E-2,0.10439411560120462,-2.1857115664925507E-3,4.3444031163738586E-2]
[null,256,1.0074413883402613,0.9753006161598371,0.97051688518113666,0.96779374714237965,1.0040419680049044,0.98652653393266321,1.0137393934730203,null,6.7378279119838629,0,1.0584746569034777E-2,0.18889715089934397,0.12284923591019381,8.1314338805898403E-2,0,1.0584746569034777E-2,0.27059351552706873,5.9120242409014709,0,1.9114825635598551E-2,0.10089776699040967,-1.4492650427525378E-3,4.3586102356629026E-2]
[null,257,1.0409410165199431,0.97213897859799958,1.010976032127445,1.0444169364436025,0.99997632494423327,1.0285474714438934,1.0199556660378872,null,6.741342950877228,0,1.0324292585371623E-2,0.1956385819132915,0.11831691013102445,8.3841478117844079E-2,0,1.0324292585371623E-2,0.26752016593738931,5.9139127254210218,0,1.8940676983512306E-2,0.10241204607667434,-1.7532329145166288E-3,4.2513599210985034E-2]
[null,258,0.98764983127520489,0.98953403334357382,0.9943251370292997,1.0155021501760282,0.97772880152448749,1.0017390775756736,1.0108373722803279,null,6.759322489755446,0,1.0671639246146713E-2,0.19729417652398007,0.12413714713218757,8.2912187134475235E-2,0,1.0671639246146713E-2,0.27659430611130181,5.9132887966085095,0,1.9223264065605872E-2,0.10413537303735595,-2.206671792626529E-3,4.3943910934656001E-2]
[null,259,1.0182560288374467,0.97768672668349077,0.96386060474662372,1.0240224843319494,1.0036023410148673,0.98919193072421907,1.0017602919662065,null,6.7301844296097286,0,1.0550578711146822E-2,0.18643529972917117,0.12154735788942198,8.0861940287202394E-2,0,1.0550578711146822E-2,0.26477013362962948,5.9154263838231627,0,1.9057352968831938E-2,9.9916989435693743E-2,-1.276433352889431E-3,4.3445405199498403E-2]
[null,260,0.97321453744749786,1.0061814886765537,1.0263023091340868,0.9986536803268472,1.0037128237278183,1.0293494705404069,1.0034548284411082,null,6.7780111195644617,0,1.0744467847211638E-2,0.20826986377017392,0.12452329238889905,8.4948402336945394E-2,0,1.0744467847211638E-2,0.28120624029528296,5.9105629108316178,0,1.930513694941181E-2,0.10820376761559145,-3.2523007742949546E-3,4.4243806150833613E-2]
[null,261,0.9688157115746262,0.98295942060327124,1.0386109324089003,0.99500862168007653,1.0033787066100714,0.99543558215478145,1.019352688133166,null,6.7775357189845007,0,1.0429438856735019E-2,0.20587462923031694,0.12601909033823458,8.5744424010258474E-2,0,1.0429438856735019E-2,0.28387049434310546,5.9096523630097986,0,1.9330570854770832E-2,0.10631607717117449,-2.2185028142816441E-3,4.2946572841120884E-2]
[null,262,1.0067101073800533,1.0096896772440733,0.95988236569647567,0.9914271367080506,1.0191770695383275,0.95662221790258861,1.0391162539368897,null,6.7273370870236722,0,1.0214070261550247E-2,0.17942537345783,0.12143998984159289,8.0715440923482928E-2,0,1.0214070261550247E-2,0.27430725923951454,5.9138788555499016,0,1.9118756482139041E-2,9.6353297120554057E-2,3.8391108328414902E-5,4.2059723300330899E-2]
[null,263,1.001771231884987,1.0135400096998715,0.99402021168766863,1.0283949397887486,0.99937145732848609,0.97178551883959763,0.99342009016896016,null,6.7286674094326822,0,1.0105048352385135E-2,0.18673479681942728,0.12122505703222719,8.2746470184366427E-2,0,1.0105048352385135E-2,0.26497355228285457,5.9140026654606253,0,1.9145454630023765E-2,9.8576907316451967E-2,-3.4828477686387117E-4,4.1610790483565412E-2]
[null,264,1.0381050253117994,0.99394772607550408,0.96939456844469329,0.98683934102971027,0.99901634835314468,0.98995320180178759,0.99978956798419294,null,6.7120465587445892,0,1.0234443633123473E-2,0.18234147917802351,0.118340764436367,8.1105513676179616E-2,0,1.0234443633123473E-2,0.25911694262360607,5.9131151693880897,0,1.8954984475330772E-2,9.7451085052595851E-2,-5.2299730375308321E-4,4.2143617218144497E-2]
[null,265,0.96866221235913896,1.0057686649113851,1.021237547448665,0.98107426422022259,0.97827466922183559,0.98807028264788599,0.97585446108216067,null,6.7554112707721252,0,1.0409955719814727E-2,0.20027994722593892,0.12522789688073244,8.4480916162126274E-2,0,1.0409955719814727E-2,0.27084144777218844,5.9099044565885324,0,1.9331462554571872E-2,0.10431223702006753,-1.8334381831912434E-3,4.2866344751152224E-2]
[null,266,0.98711304451822202,1.0021215814329623,1.0007235862899939,0.98317496932404946,0.99430657274971268,1.0252692122246923,1.0013377367148213,null,6.7628625573489547,0,1.0808664280937462E-2,0.20173101387606537,0.12345701502002179,8.3282420853551628E-2,0,1.0808664280937462E-2,0.27627241026397159,5.9111829757102834,0,1.9226265701076998E-2,0.10613905906163158,-2.9367587760275862E-3,4.4508155638377324E-2]
[null,267,0.95344843600861617,0.96296727391013348,1.0233471012402786,0.97777121347308138,0.95510505160946169,0.99061772688285532,1.0128304818326965,null,6.7874027943681297,0,1.0782870063388498E-2,0.20810283932487625,0.12941605271289081,8.4821155126014458E-2,0,1.0782870063388498E-2,0.28631245194385635,5.9096049019568548,0,1.9421266103491729E-2,0.10827418435049598,-2.9519967920607435E-3,4.4401939641710256E-2]
[null,268,1.011910502232535,1.0070542251276451,0.97166293853394003,0.99323290660818642,1.0053942352141989,0.99924961737118423,1.0137419807496915,null,6.7351736298240148,0,1.0517879175139817E-2,0.1880234742743376,0.12072837314033875,8.1399484013087525E-2,0,1.0517879175139817E-2,0.2702873114947002,5.9133371407281459,0,1.9090926314109618E-2,0.10037327514938221,-1.377109620611573E-3,4.3310754330522006E-2]
[null,269,1.0265606332497599,1.0007155439683284,1.0098113146760084,0.95172781010403462,1.0069993117241216,1.0019064605506445,1.0140381300700767,null,6.7284965099275738,0,1.008219317318663E-2,0.19072183422918401,0.11861336630323692,8.3694151657116619E-2,0,1.008219317318663E-2,0.2668814491345543,5.9089705040874332,0,1.9014041451879876E-2,9.9895770197209091E-2,-8.1128405673603688E-4,4.1516676923696205E-2]
[null,270,1.019351609489094,1.0068958225750053,1.0338287452014878,0.99184173460375258,0.96556673392234671,1.0100182469634245,0.98962036764135952,null,6.7331844547142774,0,9.9962981078238825E-3,0.19593519980993854,0.11871353399934718,8.5155868483597644E-2,0,9.9962981078238825E-3,0.26301789276849274,5.909759552234795,0,1.9051598710016028E-2,0.10142029797696434,-1.0324656021538483E-3,4.1162976333284106E-2]
[null,271,1.0147513089787474,0.99770650448951637,1.0199540332146257,1.0152658722759824,0.98417137513849295,0.98411393920274692,1.0233930254727241,null,6.7371042829456558,0,9.9426966999767302E-3,0.19092738463304154,0.11994956897726096,8.4422986362749794E-2,0,9.9426966999767302E-3,0.27083301447228142,5.9118252507303559,0,1.9075844068525864E-2,9.9503997936023603E-2,-3.7601951104961588E-4,4.094225527646448E-2]
[null,272,0.97689169026580969,0.98733718214287647,0.99159196235257074,0.98434500453735374,1.0130271663025003,0.98079554874663233,0.9868963313307213,null,6.7505410955566054,0,1.0598912910535099E-2,0.19515739588907349,0.12566836657174052,8.2646451605029314E-2,0,1.0598912910535099E-2,0.27103052969602442,5.911757324363462,0,1.9284051507034605E-2,0.10314786170743666,-1.795322612607231E-3,4.364443682941254E-2]
[null,273,0.98762427228201544,1.0284342872494956,1.0175750454526697,1.0227980086130009,1.0395021595770408,1.0070128133993439,0.98965979773832824,null,6.7506064391851588,0,1.0340136222375611E-2,0.19786171902527955,0.12180290720399348,8.4284910472170516E-2,0,1.0340136222375611E-2,0.27095843867762814,5.9123683873641451,0,1.9223406913892131E-2,0.10323887890272362,-1.7110498627766833E-3,4.2578840488105209E-2]
[null,274,0.96406593482584146,0.9661499883795398,1.0341857856473289,1.017193133517488,1.0110507878540689,1.017494948139821,1.029131354912356,null,6.7976088281394675,0,1.0834567459373258E-2,0.21247800759171692,0.12760543797936882,8.5577840117811707E-2,0,1.0834567459373258E-2,0.29044451030076451,5.9111081409339246,0,1.9358294563507489E-2,0.1099639817477428,-3.5422054119526648E-3,4.4614820316582038E-2]
[null,275,1.0282677076635194,0.99069286550360813,1.0138424773787704,1.0121771947127913,1.0354800181883028,1.0183351995474754,1.0018934849499204,null,6.7360318436524658,0,1.0238549022503681E-2,0.194838685754224,0.1188200483602687,8.3960519748008819E-2,0,1.0238549022503681E-2,0.26486936983566695,5.9120076160095012,0,1.9005225124857368E-2,0.10184896128531752,-1.479104946260989E-3,4.2160522480880112E-2]
[null,276,0.98867588784699267,0.98323731843149431,0.99902295934449636,0.99833404520628677,0.99000526288085244,1.0338125042763284,1.0050894776055803,null,6.7706660832850973,0,1.098686503806026E-2,0.20454093685753874,0.12423586890379908,8.320947378970249E-2,0,1.098686503806026E-2,0.27790806860676948,5.9120977632830787,0,1.92175355722875E-2,0.1077084117873484,-3.4939301530908661E-3,4.5241954637656651E-2]
[null,277,1.0018340816201377,0.98523382368457091,1.0252972446300728,0.97789797594009431,0.95469207011719059,0.96537781969747871,1.0137774646305995,null,6.736826675484938,0,9.8861845071565417E-3,0.19134838874989407,0.122007445684302,8.4716754403701244E-2,0,9.8861845071565417E-3,0.2700800447024776,5.9094995760711129,0,1.9145113228751561E-2,9.9461559646005018E-2,-1.417551265354033E-4,4.0709548125226272E-2]
[null,278,1.002895058398827,0.96462487324059332,0.98972740829530592,1.0171495658732701,1.0214749147987296,1.0026972844158268,1.0080140073536126,null,6.7525021156090057,0,1.0677836964893037E-2,0.19606789807332953,0.1235900114200761,8.2564848876253649E-2,0,1.0677836964893037E-2,0.27198754088414473,5.9136342517162594,0,1.9139356435582386E-2,0.10372546794709343,-2.1766917810301287E-3,4.3969432037300547E-2]
[null,279,1.0022750895615453,1.0174134539304476,1.0061742132095328,1.0239687895859462,0.96908969701874925,0.97990962965618367,0.98070010040328259,null,6.7281580084504933,0,1.0060403470966194E-2,0.18928756102115937,0.12075370137727555,8.3459784615145138E-2,0,1.0060403470966194E-2,0.26218174695595703,5.913080082112157,0,1.9142718867296633E-2,9.932319292329371E-2,-4.9773023016377567E-4,4.1426950808374885E-2]
[null,280,0.96587621097686915,0.99140519927293846,0.99705406450628864,0.97011371073350816,0.97977753774180298,1.0045623647071777,1.014969286840474,null,6.7754058216488771,0,1.0908086631225257E-2,0.20248276375136903,0.12678665187316421,8.3153205523447876E-2,0,1.0908086631225257E-2,0.2842507409101841,5.9106830226635463,0,1.9347696105978252E-2,0.10672900077107079,-2.9448191302280683E-3,4.4917559180343805E-2]
[null,281,1.0226874270302391,0.99433476969818968,0.95688867255776866,1.014313977997324,1.0047427111786045,0.98963427162219764,0.962062958167336,null,6.7124306002589593,0,1.0497249475915691E-2,0.18358129998715558,0.12033161531384849,8.0267622794268759E-2,0,1.0497249475915691E-2,0.25304625725751712,5.9152777862963148,0,1.9034154094604221E-2,9.8734273992087104E-2,-1.0682143779012605E-3,4.3225804901066631E-2]
[null,282,1.0172145952012455,1.003218288712119,1.0170851186683625,1.0320126414678379,0.9994410014417483,0.99291710301662661,1.0039228770667503,null,6.733255020816423,0,1.0008860938315892E-2,0.19138388158039649,0.11944894507954704,8.4189119285745309E-2,0,1.0008860938315892E-2,0.2657992408699717,5.9128942483940241,0,1.9062834325577673E-2,9.9883047623317719E-2,-6.2100417530874515E-4,4.1214707833149726E-2]
[null,283,1.0082858038157667,1.0178497333454715,0.99498383935854851,0.96146643238378948,1.0089871848911043,0.99927790064646516,0.96699355172053558,null,6.723308760315426,0,1.0296389597408457E-2,0.19054259455580266,0.12021983440821638,8.2673795839372732E-2,0,1.0296389597408457E-2,0.25869213314659967,5.9103314975122609,0,1.9110293751613171E-2,0.10053880110850877,-1.1988896800475064E-3,4.2398699673099442E-2]
[null,284,0.99301075094808611,0.99700832200348288,1.0224444952209564,1.0114028727365059,0.98512546169926718,0.99888133786034838,1.0137644847546854,null,6.7559349393011923,0,1.0293465096619421E-2,0.19839260377929124,0.1225624938608884,8.4640743383665978E-2,0,1.0293465096619421E-2,0.27559290475170101,5.9114736508549344,0,1.9193464605448504E-2,0.10326787947091425,-1.5754585050444445E-3,4.238665709939192E-2]
[null,285,0.98446439162005606,1.0201999613234478,0.97519249608920722,1.0096958761620256,1.0198644026972696,0.9871027305165988,1.0142852868640295,null,6.7488275604243819,0,1.0587958694036113E-2,0.19027052978774839,0.12338631029725934,8.1717231739601159E-2,0,1.0587958694036113E-2,0.27667984838524434,5.9140341062160502,0,1.9241124516439678E-2,0.10139299750499205,-1.4939173385989011E-3,4.3599329315647577E-2]
[null,286,1.0029109129533893,0.99339003101076429,1.0249257687678934,1.0285100314062068,0.98627322571762555,0.98415477013008246,1.0282712359003945,null,6.7487407985855334,0,1.0035415359228283E-2,0.19413010387764851,0.12148223144452433,8.4803481406309916E-2,0,1.0035415359228283E-2,0.27539158559494464,5.9122550943952339,0,1.9139270502134476E-2,0.10092590368564734,-7.1092653286861205E-4,4.1324054211956236E-2]
[null,287,1.0335606761130445,1.0305876896416539,0.98556551207247167,1.0074944865970403,0.9949113154457927,1.0212368984414004,0.98061152723205147,null,6.7176900026564166,0,1.0295106646435662E-2,0.18787709823531995,0.11686588706311384,8.2107891887104795E-2,0,1.0295106646435662E-2,0.25773308101248044,5.9133434372842189,0,1.8978074291030926E-2,9.9598995121763095E-2,-1.2078789479647771E-3,4.2393416709350241E-2]
[null,288,1.035637205836051,0.9998497934378654,0.99755563467472841,0.97826674435545269,1.001618580054721,1.0410786641434717,1.0208062460925296,null,6.7397819831522341,0,1.0500278549136708E-2,0.19505768967513198,0.11783668684017676,8.2993791845219086E-2,0,1.0500278549136708E-2,0.26993580451317833,5.9110955516025863,0,1.8967498312239931E-2,0.10278959594762165,-2.132913669351639E-3,4.3238278085435837E-2]
[null,289,0.99496437929831749,0.98960392802764274,0.99836755428211954,0.99417018626540132,0.99082383563107967,0.99408932106858128,1.0114434550369953,null,6.750265328818073,0,1.047493230709118E-2,0.19482108079097799,0.12314474339020645,8.3112893316056272E-2,0,1.047493230709118E-2,0.27399551559853785,5.9119095162550472,0,1.918268490961705E-2,0.10262348674072704,-1.6584989552575619E-3,4.3133906772155249E-2]
[null,290,1.0318726259185802,1.0400302314200285,1.0028029352245607,1.0302321936210819,0.98917293548371299,1.001842939520639,0.96980122731102725,null,6.7097279908333585,0,9.9262236817508325E-3,0.18583280308267497,0.11632349989321199,8.3137563254852734E-2,0,9.9262236817508325E-3,0.25356206366304535,5.9136089300711614,0,1.8986703069683922E-2,9.767350615249519E-2,-2.7150067326346813E-4,4.0874422319498158E-2]
[null,291,0.978851672082103,0.9992406669967544,0.96964171321113035,0.98999104520701775,1.0011257179347086,0.96182641200378671,1.0242693744567373,null,6.7478710569977949,0,1.0519356352256093E-2,0.18748640218534493,0.12523334652218884,8.1383653513702303E-2,0,1.0519356352256093E-2,0.27870251235003513,5.9132721137544397,0,1.9272877349731602E-2,0.10018829984503987,-9.8498560565070154E-4,4.3316837082959088E-2]
[null,292,0.98755564504598981,0.99539812746240663,0.99503032320218143,1.0211835405162653,1.0290944546097762,0.97565648363008184,1.0021798213385054,null,6.7457215849769936,0,1.0362107205977479E-2,0.19177196015528,0.12384254109967181,8.2894714595680374E-2,0,1.0362107205977479E-2,0.27169111122515216,5.9135564267398815,0,1.9223790505606984E-2,0.10118512872067983,-1.1134011528559822E-3,4.2669313087888398E-2]
[null,293,0.9617557362599638,1.0216388630137685,1.0174086082466733,0.9900830962886018,0.99337481543116557,1.0329968158130993,0.96642767873328828,null,6.7732712299978131,0,1.0924775416459023E-2,0.20899749870981604,0.12541443010075556,8.4296898355061198E-2,0,1.0924775416459023E-2,0.2742176552991295,5.9106103898004978,0,1.9371877817707616E-2,0.10905817675712624,-3.6819774697215966E-3,4.4986280627443413E-2]
[null,294,1.0021339348739715,0.97960358764014788,0.97399554470503347,0.98625873021741373,0.99300084001273692,1.0006549377150753,0.9996166957764524,null,6.7438172069189672,0,1.0740258501737196E-2,0.19266483449233499,0.12321788902660107,8.1530838835508893E-2,0,1.0740258501737196E-2,0.26953866563040918,5.912832552919606,0,1.9143485008184767E-2,0.10273058195001955,-2.0681137591020277E-3,4.4226472815405406E-2]
[null,295,1.00936751754986,1.0000751055094912,1.0399355249481284,1.024804933718976,1.0118810346960685,1.0244255066843746,1.0170757069928307,null,6.7570092284452175,0,1.0214173263317295E-2,0.20202023777656872,0.1200988424191317,8.5715220340989731E-2,0,1.0214173263317295E-2,0.27443885040968291,5.9111843328911942,0,1.9104499392500682E-2,0.10425810849905175,-1.8710107271794878E-3,4.2060147443273965E-2]
[null,296,0.98609421490573823,1.0409100143013168,1.0201299645330251,1.0169200466615163,1.0458037762824415,0.99709391094151778,1.0183156981362549,null,6.7533600732311951,0,1.0178629801760736E-2,0.19550883037037714,0.12135672629168291,8.4537080080119245E-2,0,1.0178629801760736E-2,0.27817519385566397,5.9119045342357612,0,1.9231971839440629E-2,0.10188284130630598,-1.1508905432461812E-3,4.1913785795084361E-2]
[null,297,0.96263211855131725,0.98358603201628236,0.96634795992761624,0.983933545044547,0.99145116077040552,1.0231626688636932,0.99995776205095743,null,6.7807713259967128,0,1.1488865404385219E-2,0.2037668420603613,0.12821382982765936,8.1229027082420968E-2,0,1.1488865404385219E-2,0.28285616853082468,5.9131237426096321,0,1.9366717285401944E-2,0.10906879522973646,-4.16289942277166E-3,4.7309102793448549E-2]
[null,298,1.0019392087878576,0.97780648519807323,1.0040269651706422,1.0060288963038637,0.97157767961916575,1.0060323462178065,1.0379152426439988,null,6.760800548727425,0,1.0529041181050015E-2,0.197476074380217,0.12276867597220385,8.3560228225240021E-2,0,1.0529041181050015E-2,0.28052379101197095,5.9122319490245392,0,1.9144542271187417E-2,0.10373020782966308,-1.9916374716908943E-3,4.3356717484097189E-2]
[null,299,1.0014562342804996,1.0244612526849208,0.99346306688883435,1.029842142513169,1.0042946804959096,0.9996536385557242,0.9866111634674577,null,6.7359658586851854,0,1.0355547990704712E-2,0.19120590937553542,0.12075472785756684,8.2722775301553086E-2,0,1.0355547990704712E-2,0.26571211837985942,5.914112015056169,0,1.9147166350168512E-2,0.10096520266160335,-1.2963597041635395E-3,4.2642303406891943E-2]
[null,300,1.0184897799124162,0.99100727413436174,0.98250404165763328,1.0062384032799421,1.0231134515822398,0.98366560595057995,0.9725993880826207,null,6.7181858272628441,0,1.0260595004345193E-2,0.18639894933837534,0.1205237087487246,8.1900297271199421E-2,0,1.0260595004345193E-2,0.25640565562836676,5.9134448814621488,0,1.9056124211867843E-2,9.8966727433930146E-2,-7.6182074183411689E-4,4.2251303910064986E-2]
[null,301,0.97187925341190018,0.996040525934209,0.98762327777390091,0.95342589441681325,1.0115653458611003,1.0066426004317268,0.99718729257298411,null,6.7639054424061245,0,1.0931081811087222E-2,0.20009278068596245,0.12595009339588292,8.2466130771010754E-2,0,1.0931081811087222E-2,0.27768104153712181,5.9103067313526587,0,1.9312833192891898E-2,0.10596593256587876,-2.8823503333090762E-3,4.501224923802593E-2]
[null,302,1.0182080423872588,1.0125067642863046,1.0227335456276208,1.0332339277814759,0.96200525877024201,1.0209969567985968,0.99218971566779168,null,6.739164746030097,0,1.0190859152015423E-2,0.19649899995270864,0.11878888170999997,8.4527480468636326E-2,0,1.0190859152015423E-2,0.26492646832514416,5.9126364287424451,0,1.9057605288527416E-2,0.10226766849182878,-1.5029310318783223E-3,4.1964144082689975E-2]
[null,303,1.0143384653530128,1.005293032924498,1.0171291547907886,0.98558134786402918,1.0187883247551066,1.0251005874063952,1.0208770590397052,null,6.7495356938335211,0,1.0353015380486457E-2,0.19797751076562994,0.11968787147903437,8.4270451482781242E-2,0,1.0353015380486457E-2,0.27408132197145091,5.9103831383650034,0,1.9078030667345647E-2,0.10332201187476497,-1.8965173412925597E-3,4.2631874568801006E-2]
[null,304,0.98712631928763095,0.97062620452841863,0.9968343876374397,1.0003476440977912,0.96250288894011893,1.0275034221406993,0.98551445109434277,null,6.7662605626442325,0,1.1018691921218052E-2,0.20446931882968161,0.12511707306493361,8.3002299551669129E-2,0,1.1018691921218052E-2,0.27247302847112559,5.9123293303837805,0,1.9226191431080345E-2,0.10778789084455047,-3.5175820101189586E-3,4.5373012077526413E-2]
[null,305,0.96359329074563027,0.96488516408360836,0.98111129995871682,0.99590779826363007,1.0076388393218549,0.98647214618250856,1.0304090126311944,null,6.7793933266365931,0,1.1014717081520855E-2,0.19968569886439183,0.12878572520896772,8.2223579815769957E-2,0,1.1014717081520855E-2,0.28769058574660816,5.9129632843835926,0,1.9361068265247455E-2,0.10609510519108428,-2.7683652342136394E-3,4.5356644395148457E-2]
[null,306,0.98316680308224147,0.99043170766921707,1.0039020331052368,0.96697697527366167,1.0297982074899639,0.9761912503593938,1.0042419043902275,null,6.7484537709667194,0,1.0355844167034757E-2,0.19419176544744107,0.12447480159274213,8.3432229741295175E-2,0,1.0355844167034757E-2,0.27357969771055762,5.9101286578646199,0,1.9248433143866147E-2,0.10201134534546619,-1.2566828875777006E-3,4.264352300830164E-2]
[null,307,0.99491213120654998,1.0000791596846872,0.97161198686820271,1.010119226812646,0.96839299039641547,1.0322158235532126,0.99054712947745571,null,6.7560733620266866,0,1.1083936672992416E-2,0.19812764630281052,0.12313384923023113,8.1428992520395774E-2,0,1.1083936672992416E-2,0.27177689229492508,5.9142529166557809,0,1.9182972652251367E-2,0.10576993073882054,-3.2415167207261622E-3,4.5641678352200343E-2]
[null,308,1.0129765175609882,1.0229923796619449,1.0040758073705778,0.99823611495838627,1.0094258470007682,1.0188501402116261,0.99780528407932989,null,6.7379287750330361,0,1.0344448342720058E-2,0.19402800211671076,0.11925552140723072,8.3381346375710028E-2,0,1.0344448342720058E-2,0.2674671955650208,5.9118080772285051,0,1.9085256771685283E-2,0.10191653676042003,-1.6097582244046843E-3,4.259659703215482E-2]
[null,309,0.98765628405788952,0.99290825648609438,1.0203170921954663,0.98624421135069162,0.99759545939711192,0.97863637568589723,0.98396080291382992,null,6.7426252050862994,0,1.0176368605319248E-2,0.19551951237589807,0.12347113033314451,8.4374993995771683E-2,0,1.0176368605319248E-2,0.26707141137425561,5.9102365339498029,0,1.9223228002406324E-2,0.10187901731216399,-1.0550968477623759E-3,4.1904474590616289E-2]
[null,310,0.96420206314713341,1.0204440299400772,1.0090535299581276,1.022302045756065,1.0129565878975939,0.9853384592330926,1.0023849249676453,null,6.7635034172138253,0,1.0475808316926251E-2,0.1979455424000908,0.12531689299672077,8.386758962144239E-2,0,1.0475808316926251E-2,0.27906622314544227,5.9128269305741465,0,1.9357496201730579E-2,0.10371826074253696,-1.7330324930166965E-3,4.3137514024732142E-2]
[null,311,0.97461275709664008,1.0193778840928447,0.97541947233996862,1.0215285114360615,0.99774337107581523,0.97905621931155962,1.022665351416062,null,6.7559926415603684,0,1.0609365204119333E-2,0.19071945294309872,0.12466944671966516,8.1797390541465814E-2,0,1.0609365204119333E-2,0.28100436600604878,5.9146613790099609,0,1.9297100563889155E-2,0.10162065158500178,-1.4646233227233387E-3,4.3687477513953528E-2]
[null,312,0.98892439119819675,0.99579453015855568,0.98944610851148618,0.96431094021020369,1.0048563422546946,0.96989023779310035,0.97466584210548768,null,6.7311572337428842,0,1.0335105547937672E-2,0.18969548576816614,0.12375703596382213,8.2395220067271499E-2,0,1.0335105547937672E-2,0.26331673517310589,5.9107938823712649,0,1.9216149961487929E-2,0.10036836202617962,-9.437626546137521E-4,4.255812506619646E-2]
[null,313,0.97371063904962762,1.0192898880887582,0.99156234534217202,1.0079578022889875,1.0178208466769494,0.9987664841549182,1.017784144687143,null,6.7639923134579245,0,1.0681953086484243E-2,0.19667777639440184,0.12448342804208271,8.2806221848167855E-2,0,1.0681953086484243E-2,0.28187788972292005,5.9130352442696434,0,1.9302282921818188E-2,0.10395297300952296,-2.1298842440101843E-3,4.3986381493370801E-2]
[null,314,1.0273317745926491,1.0005768475412371,0.97398422238721671,1.0208557324155392,1.0087431512860536,1.000933097664821,1.0005522209029543,null,6.7246530093768397,0,1.0385149011795143E-2,0.18629154864292033,0.11918168395437789,8.1466860082579196E-2,0,1.0385149011795143E-2,0.26298655203445137,5.9147036601864666,0,1.9010055200323246E-2,9.9332854479060165E-2,-1.0844003462974359E-3,4.2764195142956991E-2]
[null,315,1.002591552751122,0.97149530776616477,1.041655425152781,0.98501230071945423,0.98833684618736584,1.0059357683417025,1.0335617225851021,null,6.7626345265826924,0,1.0208437571941429E-2,0.20242035549948584,0.12228781613400729,8.5859375884584574E-2,0,1.0208437571941429E-2,0.279296111377973,5.9089347042082494,0,1.9141001993927716E-2,0.10437688162755673,-1.7182490301985136E-3,4.2036528887103165E-2]
[null,316,0.98517294784341702,0.97725713462984731,0.97441098369469203,1.0208588083208356,1.0056070006427371,0.95557885487498628,0.98437181163121223,null,6.7360788808373346,0,1.0439976404420797E-2,0.18739372381285979,0.12545165719102494,8.1532555496977452E-2,0,1.0439976404420797E-2,0.26573680145314033,5.9146804513675226,0,1.9237141722223666E-2,9.9899147498293941E-2,-8.4256229158745453E-4,4.2989964586877358E-2]
[null,317,1.0211869448068938,1.0128810130494978,1.01538015349276,0.97941925758427062,0.97026214675747979,0.9958926182441209,0.98256982718287333,null,6.7211316952506479,0,9.9737147823351704E-3,0.1902313070970538,0.11856032131785799,8.3956910143238431E-2,0,9.9737147823351704E-3,0.25931172758507726,5.9101500452957634,0,1.9041986744679766E-2,9.9365065728932403E-2,-5.556508805606515E-4,4.1069982218603682E-2]
[null,318,1.0194772014309021,0.9996531470119151,1.0087134585336186,0.98969416985007308,0.96249719171836601,1.0234933039274805,1.006532156614711,null,6.7419348253912545,0,1.0385668202575409E-2,0.19614352182139033,0.11950853388826771,8.3679680115536739E-2,0,1.0385668202575409E-2,0.26876474948884649,5.9110842418611327,0,1.9050939860418253E-2,0.10279134551375964,-1.8545202362749932E-3,4.2766333078177621E-2]
[null,319,1.0378297083702877,1.0303414394081494,1.0193024328365334,1.0090119963609119,1.0060720132550289,0.97163643931709986,0.98509231184871648,null,6.7004644891189917,0,9.472395074312686E-3,0.18172103628412403,0.11579368448198764,8.4141113648018642E-2,0,9.472395074312686E-3,0.25352130405174261,5.9115247114202374,0,1.8956377605141437E-2,9.4736411479757768E-2,1.0642132554352748E-3,3.9005636892548705E-2]
[null,320,1.0236457670278221,1.0033577281086326,1.0141565677103506,1.0025767508858394,1.0092115186713486,0.96213719081703675,1.0128231332540323,null,6.7173775086359813,0,9.6618131278941588E-3,0.1839489388952322,0.11874583279286487,8.3956051760041991E-2,0,9.6618131278941588E-3,0.26359769487080426,5.9114710003390627,0,1.9029163491369606E-2,9.6141599085886861E-2,7.0160067867439829E-4,3.9785626722040508E-2]
[null,321,0.95896647260800905,1.0320943446879638,1.0077583165523727,1.0312339509886128,1.0276524748689686,0.99941544514263314,1.026250039530916,null,6.7782400007753809,0,1.0643758130176352E-2,0.20073373211336762,0.12545530741397792,8.3922036826799273E-2,0,1.0643758130176352E-2,0.28856278951487369,5.9133829932819895,0,1.9388365036432997E-2,0.10524664471371076,-2.2809695875214558E-3,4.3829101461743701E-2]
[null,322,1.0242856328174739,0.97267503110098463,1.0027274584727139,1.0198061208530986,0.97625417341283438,0.96492629452371581,1.0007622884856813,null,6.7204617184916531,0,9.9120664509810309E-3,0.18554701560643119,0.12036738017770496,8.3223089283151225E-2,0,9.9120664509810309E-3,0.26080404850988342,5.9130497566923168,0,1.9025836557592497E-2,9.7526948119616971E-2,1.0151818187168392E-4,4.0816125363081247E-2]
[null,323,0.98097491332572984,0.98083606216939168,1.0116573998299048,0.99910590383407027,1.0018660508808488,0.99129902439331308,1.0170350646504629,null,6.7641483288670674,0,1.0512155770830218E-2,0.1993994767900121,0.12508983676330088,8.401395282315241E-2,0,1.0512155770830218E-2,0.27928177246197311,5.9114257020702565,0,1.926082281106237E-2,0.10434563060063796,-1.9560518236301713E-3,4.3287186370303071E-2]
[null,324,0.9991504020829336,1.0222577326184707,0.98894552952093862,1.0153560751968536,1.0045022871376856,0.96222472040208429,1.0135833733051587,null,6.7294745839810295,0,1.0039534464037691E-2,0.18413371889560534,0.12122132176946547,8.2489754125857406E-2,0,1.0039534464037691E-2,0.27007340852147677,5.913580797803947,0,1.9159729278962263E-2,9.7449947735673059E-2,2.4889897649795974E-5,4.1341015952388052E-2]
[null,325,0.96362493821806949,1.0089806488234272,0.97554872187392105,1.0250522851444928,1.0153599035121481,1.0248221693032213,0.99988889131302672,null,6.7786345211116972,0,1.1280061044796175E-2,0.20281513144863855,0.12660666097091647,8.1827565063309959E-2,0,1.1280061044796175E-2,0.28243122771034213,5.9148447982866523,0,1.9360882457733347E-2,0.10805856061760959,-3.7595890499601916E-3,4.644928360645139E-2]
[null,326,1.0133305127591246,1.0219113297664109,1.0278954789663524,1.0129115069159678,0.96722833970383437,1.0034260981321961,0.98700034225233468,null,6.7318927507174626,0,9.9787174177585498E-3,0.19388277960723738,0.11882428111613412,8.4807216120211429E-2,0,9.9787174177585498E-3,0.26312579242568651,5.9112411923406931,0,1.9083376706470659E-2,0.10065036314940458,-8.1283292921937949E-4,4.1090582180841252E-2]
[null,327,0.99077099328799645,1.0405481731252382,1.0174391315217406,1.0338334011978518,0.99858701755791757,0.97401837240693345,0.99332105543912408,null,6.7347079640352217,0,9.9209451083424258E-3,0.18980219505978044,0.12085121856584506,8.4243100672842783E-2,0,9.9209451083424258E-3,0.26792066062779452,5.9129723775521654,0,1.9205875407185696E-2,9.9040275180337228E-2,-1.8042512448322804E-4,4.0852686093753393E-2]
[null,328,0.9903439653884466,1.0263511709222144,1.005838092832275,1.0003404831842626,0.98961947607408485,1.019341734738799,0.99196645432700881,null,6.7522487929013835,0,1.0554848870087145E-2,0.19849178294585834,0.12178798218513678,8.3554732488733574E-2,0,1.0554848870087145E-2,0.27199454089875719,5.9118222714641107,0,1.920824799856664E-2,0.10417018807634286,-2.2439421100789877E-3,4.346298895395468E-2]
[null,329,1.0108032470921615,1.0029238955199951,1.003304273484549,0.99501444374263748,1.0223922823818563,1.0296215355957468,1.0144258469958312,null,6.7517660640654151,0,1.0572649892575016E-2,0.1980818388240099,0.12047712976922863,8.3415442388274336E-2,0,1.0572649892575016E-2,0.27373076176385691,5.9116774950214337,0,1.9096827849481177E-2,0.10408569883446671,-2.3354207814395454E-3,4.3536290396095849E-2]
[null,330,1.0125723263022375,0.96850466232545129,1.0034434883695504,1.0265590909509195,1.0176220653309687,1.0373844931888925,1.0083518658962893,null,6.7605088409257439,0,1.0792778644161461E-2,0.20224771622028143,0.12195578101479673,8.3433773260462377E-2,0,1.0792778644161461E-2,0.27275905090595831,5.9133743103319336,0,1.9087405035069654E-2,0.10626739741862276,-3.0593346750535616E-3,4.4442741413671695E-2]
[null,331,1.0018898393490654,0.98101617386068407,1.0400605539335674,1.0447636524116408,0.99675794321632394,0.97751520941476222,0.98555514914381981,null,6.739770258333138,0,9.8993931486991947E-3,0.19583054639967351,0.12192765087714151,8.5590746082716357E-2,0,9.8993931486991947E-3,0.26374484057917569,5.912254970966945,0,1.9144810387283381E-2,0.10105757419885771,-5.4482011870382889E-4,4.0763938960048367E-2]
[null,332,1.0128468803650581,1.0002242927718175,0.99947839596906307,1.0097524331699319,0.97981581796571504,1.007071792219099,0.98227144783606024,null,6.7336964588035064,0,1.0366748123697402E-2,0.19312657641372,0.12043456738790087,8.3037671990149178E-2,0,1.0366748123697402E-2,0.2624809136241914,5.9126892730998444,0,1.9085945602389021E-2,0.10167476140103272,-1.5216742767286881E-3,4.268842356100646E-2]
[null,333,0.98667550379418401,1.0189739297251337,1.0055322908417035,0.99299423951467258,1.0167555754472519,1.0038257500896894,1.0236342310685531,null,6.7585446605579076,0,1.0467888630999234E-2,0.1967673048638747,0.12259980787925225,8.3642328138527275E-2,0,1.0467888630999234E-2,0.28029169362164935,5.9114425778132631,0,1.9228714782843374E-2,0.10328081505368684,-1.8134837629297941E-3,4.3104902167736228E-2]
[null,334,0.99229186424529903,1.0314900415676469,1.0122322070913596,1.0119782090097522,0.96713357408939771,0.98941545881065429,0.96949376687147748,null,6.7330971005487417,0,1.0146149915889267E-2,0.19262072152998441,0.12118654395053531,8.3831953636467102E-2,0,1.0146149915889267E-2,0.26255258540728105,5.9120885382485016,0,1.919744194904369E-2,0.1007696812718301,-9.3040485117225195E-4,4.1780039406269835E-2]
[null,335,0.98665076790171036,0.97545705801572269,1.0141211729521231,0.99329976999388192,0.99750876481269601,0.99148766115082487,1.0335522504651637,null,6.7655909103149829,0,1.0455784766244678E-2,0.19905474704376722,0.1245965625340453,8.420258668480636E-2,0,1.0455784766244678E-2,0.2822670692485546,5.9109717762234961,0,1.9228853303908087E-2,0.10403852432827619,-1.8242696589554509E-3,4.3055060607084583E-2]
[null,336,0.98772431670287653,0.98100544011102109,1.0236963020544179,1.0237156054523444,1.0094474000383353,1.0132132643293759,0.98423648339033687,null,6.7613314091883385,0,1.0558491323064344E-2,0.20387772835142232,0.12399438295228382,8.4658573265176867E-2,0,1.0558491323064344E-2,0.27052293946583827,5.9120668599412491,0,1.9222847811416911E-2,0.10605767534074925,-2.5475858667805152E-3,4.3477987926982348E-2]
[null,337,1.0332004868345239,1.0011266595321786,0.99966466383594332,0.99406497810505912,1.0082410629683214,0.99239609763820757,1.0002624236924316,null,6.7180560847554061,0,1.0008936990871773E-2,0.18651222309601537,0.11801610418645518,8.301228348630281E-2,0,1.0008936990871773E-2,0.260675637560142,5.911831011111798,0,1.8979913098431059E-2,9.8183438266035497E-2,-3.6954705381553001E-4,4.1215021004037997E-2]
[null,338,1.0228525325586411,1.0315334542667445,1.014536317729358,0.96552035145287718,1.0378606140623778,1.0001305163096255,1.0067027086354956,null,6.72391020914728,0,9.9293869333815423E-3,0.189149483566146,0.11752180932165479,8.3977861881518318E-2,0,9.9293869333815423E-3,0.26546831385113628,5.909447189548243,0,1.9033293632566083E-2,9.884114923155099E-2,-4.1633991221426116E-4,4.0887448026675606E-2]
[null,339,0.96101218525406529,1.0131830199860798,0.97468429476804574,0.97866506763678851,0.99343445951431597,1.0019899639801253,0.99727631061728861,null,6.7671231371542637,0,1.1047389933501409E-2,0.19837703182193217,0.12675655263200286,8.1711412468756461E-2,0,1.1047389933501409E-2,0.28019071300023179,5.9123842958677697,0,1.9376263560181912E-2,0.10573981908401738,-2.9041366646879048E-3,4.5491185384053522E-2]
[null,340,1.031456117750871,0.98640073131964179,1.0061001103986613,0.96429994347306325,1.0255834759917695,0.97549311898091251,0.9837343778846912,null,6.7099676027735997,0,9.8622460343107676E-3,0.1855388471040629,0.11880076531802775,8.3318816839462684E-2,0,9.8622460343107676E-3,0.25542325835526042,5.9098599199256885,0,1.8988836471772033E-2,9.7359737313501976E-2,6.6447690886712324E-5,4.0610973754936712E-2]
[null,341,0.96492857870016213,0.97617524162612246,1.0142323389465073,0.98836415579238013,0.99594169496142737,0.98938915527943072,0.9910342620354502,null,6.7687174234749028,0,1.0664131319682579E-2,0.20305460255159186,0.12736174863712008,8.4129943743724164E-2,0,1.0664131319682579E-2,0.27653525117751682,5.9106987684542931,0,1.9353239161727088E-2,0.10612327500089576,-2.4523998818041515E-3,4.3912994629837776E-2]
[null,342,1.0270921893794289,0.98457544498414407,0.98256828743277624,1.0095806714615727,0.99318272375943595,1.0031881902514994,0.99637840313997172,null,6.7277139547258402,0,1.040500196617726E-2,0.18904033140515644,0.11982477873733903,8.1984442035542268E-2,0,1.040500196617726E-2,0.26233270639979206,5.9136220082960289,0,1.9011293044290202E-2,0.10036591848341106,-1.3134697511324399E-3,4.2845946075408411E-2]
[null,343,1.0026471353998492,0.98763637998214793,0.96565646483640455,0.99059998768139423,0.97709785867185217,1.0143382459992361,0.99203071844755353,null,6.7446871274189117,0,1.0922548972715426E-2,0.19352378221071093,0.12290748774069184,8.1000719457549705E-2,0,1.0922548972715426E-2,0.26854020310803289,5.9135217448163315,0,1.9140700559313748E-2,0.10362214472027834,-2.5467677223957601E-3,4.4977112528399497E-2]
[null,344,0.98515405935990397,1.0284446598068395,1.0089513170457034,0.99774720365541936,0.99717945732376345,0.95998924870202829,0.99638342946433189,null,6.7334060638797482,0,9.9567999181281331E-3,0.18811015579946683,0.1222710622791499,8.3706484594828753E-2,0,9.9567999181281331E-3,0.26903819216023994,5.9115059060713664,0,1.9237247820054097E-2,9.856976185265659E-2,-3.3076516543736041E-5,4.1000329818532688E-2]
[null,345,0.9571303078362251,1.0326254167238234,1.0176611163424794,1.001642697043224,0.99148749603575348,0.99191178556169768,1.0264247245258202,null,6.7758051915625606,0,1.0490510381114114E-2,0.20076474027642616,0.12547754932871572,8.4514345273193348E-2,0,1.0490510381114114E-2,0.28843053280249725,5.9112204941106823,0,1.9399270978835245E-2,0.10474915109637441,-1.948946812356312E-3,4.3198054508187873E-2]
[null,346,0.98541753361245954,0.98628909190863767,0.97544820830301571,0.97456133442675708,0.98927971462969067,1.0344325289312626,0.99653519589007944,null,6.7667950519475459,0,1.1244041530765334E-2,0.20213734470872,0.12494024386190422,8.17049580100596E-2,0,1.1244041530765334E-2,0.27643496599892042,5.9121205808977253,0,1.9235768235511666E-2,0.10770287065844446,-3.7826420826442323E-3,4.6300961658906882E-2]
[null,347,1.008284769541715,1.0328720622805274,1.0128663699609126,1.0272120115233363,1.0144518491579655,1.0450725363802122,1.0075223069744526,null,6.7546459495446953,0,1.05350246529751E-2,0.20019117449699217,0.11918878191964731,8.4031729851049106E-2,0,1.05350246529751E-2,0.27368374238589616,5.9128755601360226,0,1.9110299297804039E-2,0.10469735904663856,-2.5140539458218605E-3,4.3381356356466387E-2]
[null,348,1.0072520935910998,0.97605493614353322,0.97861745572474124,0.99879431276356034,1.0079562539505336,1.020357657116957,1.0034842190594564,null,6.7508643210886792,0,1.086918879439638E-2,0.19631966944868837,0.12268405005388699,8.1848246015402665E-2,0,1.086918879439638E-2,0.27112237240707476,5.9132566705519753,0,1.9115842602083655E-2,0.10443703405112992,-2.67694885340606E-3,4.4757384811839343E-2]
[null,349,0.99786850529916871,1.0254907115209253,1.0202768388222911,1.0156629432991324,1.0136301806536074,1.0243490423163217,0.96689024108804922,null,6.7441526630074069,0,1.0398320306001565E-2,0.19977199515647567,0.12064007794566409,8.4346166195430769E-2,0,1.0398320306001565E-2,0.26360452515827654,5.9118281986679362,0,1.9166738583278949E-2,0.10409691504752297,-2.1203859352746661E-3,4.2818432188096077E-2]
[null,350,0.98233576283053603,1.0297079270533334,0.99384442038568144,0.98803076549466395,1.0164493206169349,0.99030487121774502,0.9746830593153325,null,6.7393479065366533,0,1.0432072939269723E-2,0.1927277794267962,0.12284667714660544,8.2730946669386643E-2,0,1.0432072939269723E-2,0.26669915330599325,5.9118308885069304,0,1.9253124095327694E-2,0.10174949504648384,-1.4475771850242893E-3,4.2957419524149568E-2]
[null,351,1.0042117539044941,1.0032492762202498,1.0380856843246198,1.0061089075977332,0.98347019631874733,0.99939796541802539,1.0310957535453951,null,6.7527550929842111,0,1.0018452466097592E-2,0.19760846410610827,0.12059763466406466,8.5625405032377172E-2,0,1.0018452466097592E-2,0.27719174620829751,5.9102825134619019,0,1.9132229044284851E-2,0.10207354181453335,-1.0106453846803411E-3,4.1254204037326478E-2]
[null,352,1.0237864291351071,1.0024783466335074,1.0015302694725865,1.0150008836073248,1.0079913031725045,0.99556884010101299,1.0063917481210829,null,6.7282959931398425,0,1.0110919274288508E-2,0.18893406228251169,0.11900291570795292,8.3201304641837698E-2,0,1.0110919274288508E-2,0.26496870138276651,5.9128575180263336,0,1.9028431772765766E-2,9.936625334235144E-2,-6.9815991165866095E-4,4.1634965894978351E-2]
[null,353,1.022749385221591,0.98430338218846058,0.9929120523923034,1.0317876546991256,1.0281441840804404,1.0245333304197035,0.97408674847822196,null,6.7351247831098942,0,1.0576901991444626E-2,0.19513357601570303,0.12015729042139382,8.2605672531284799E-2,0,1.0576901991444626E-2,0.25950165927100033,5.9142479394739969,0,1.9033831161454327E-2,0.1030674642948801,-2.1764498422158895E-3,4.3553799782395514E-2]
[null,354,1.0133524938360612,0.98966346885535261,0.99256458181571439,1.0059896463985645,0.97908793516194215,1.0141933577436528,1.0246506729617475,null,6.7488745083734631,0,1.0545880481652628E-2,0.194461076630492,0.12101479292600277,8.2765369004135683E-2,0,1.0545880481652628E-2,0.27445053134054548,5.9128729781454794,0,1.9083260008488472E-2,0.10273003614045481,-1.9295945488275834E-3,4.3426058726694985E-2]
[null,355,0.97558140195369092,0.9896006183047531,1.014503545815753,0.98813331530307857,1.0076244935266678,0.98204277574809695,1.0020911903267395,null,6.7581071715365901,0,1.040578472382939E-2,0.19821499196147754,0.12527936417371463,8.4134608163213928E-2,0,1.040578472382939E-2,0.2757122056643066,5.9106708417097877,0,1.929154670279323E-2,0.10358005857014761,-1.6256147409457499E-3,4.2849169332094213E-2]
[null,356,1.0209327990111758,0.98844648164370585,1.0212460532553382,0.9777738186958993,1.0140971472810583,1.0296926674255624,0.95762218313201319,null,6.7326878349557102,0,1.0369853269830831E-2,0.19951091547960362,0.11964476301161729,8.4273458706861842E-2,0,1.0369853269830831E-2,0.25602922414916035,5.9097256636712308,0,1.9043315688311104E-2,0.10391126539811486,-2.1519811492807617E-3,4.2701210000088537E-2]
[null,357,1.0076392559560756,1.0059088695950733,1.003911969998319,0.97733116398192077,1.0414822958191332,0.99554781527638214,1.0278456664284259,null,6.7427556705431932,0,1.0236383486101067E-2,0.19195447556079503,0.12070055342130967,8.3456583866945488E-2,0,1.0236383486101067E-2,0.27492207401953928,5.9106876310703829,0,1.911376302071539E-2,0.10083557236053857,-1.0665879644559729E-3,4.2151605187425265E-2]
[null,358,0.97912391652229303,1.0050360866104155,1.0021241357309199,0.99727340668381537,0.9860213451708052,0.98072395736605145,1.0359851762710612,null,6.7608045217227408,0,1.0397730624233929E-2,0.19446445139493618,0.12429308914041222,8.3479914394454971E-2,0,1.0397730624233929E-2,0.28369950000630317,5.9118660670123289,0,1.9271328780898468E-2,0.10224471824344385,-1.3305512335773182E-3,4.2816003983536383E-2]
[null,359,0.9629036116027716,1.0287561042307722,1.0079656710002856,0.99657110688184347,0.97909118327849431,1.0365086470678961,1.0097184430903048,null,6.784376862763609,0,1.1006917102693718E-2,0.20764639321507106,0.12510035262610369,8.3880365626476758E-2,0,1.1006917102693718E-2,0.28640769409696165,5.9114982071495241,0,1.9365120518226846E-2,0.10885984511823231,-3.7056410576734372E-3,4.5324525470682782E-2]
[null,360,1.0063620432064251,0.97191303663702644,0.98175647693525014,1.0076550000298043,0.97732890084544732,0.9861241691968563,0.97994231821829025,null,6.7330908990867089,0,1.0504218784597803E-2,0.19061323534001315,0.12294305468534084,8.1927895178217552E-2,0,1.0504218784597803E-2,0.26186851149424839,5.9135627311702779,0,1.9120629434311202E-2,0.10124211818842553,-1.4417796778543588E-3,4.3254503273728859E-2]
[null,361,0.98413894084240416,1.0134204613187616,1.0021213917095717,1.0361336939601113,0.99166511299086024,1.0168259016003307,0.98377435728177487,null,6.757581732191329,0,1.0687492579763966E-2,0.19988293685169253,0.12324950985244572,8.3341607777938156E-2,0,1.0687492579763966E-2,0.27133692859630876,5.9139662653413678,0,1.9242955797171488E-2,0.10509377030259549,-2.541434468903044E-3,4.4009192140703653E-2]
[null,362,1.0144468370491317,0.97351803058429587,0.98851163589406144,0.98524163507386975,1.0130329168468701,1.0121798468788921,0.9919087830754959,null,6.7400493146711922,0,1.0625488638499537E-2,0.19475528903879846,0.12175755070766396,8.2377719370406416E-2,0,1.0625488638499537E-2,0.26537785013596377,5.9119771538110673,0,1.9077456511588139E-2,0.10309356628174474,-2.1211421329096324E-3,4.3753870946866877E-2]
[null,363,0.99269939908414551,1.0293375476751474,0.99857106369152826,1.0007192567859002,1.0185126537007874,1.0108828614448051,1.0070569140929324,null,6.7502009818733493,0,1.0495885933532177E-2,0.1952696636274612,0.12149363254366866,8.3139005607264366E-2,0,1.0495885933532177E-2,0.27463578244814735,5.9122520348548759,0,1.9195186497025379E-2,0.10284937918327666,-1.853892964602756E-3,4.3220190076232796E-2]
[null,364,0.99760255001300802,0.98539629029986875,1.0185504035870583,1.0151320080382147,0.97358542211334143,0.98473968923986432,1.0213649715436595,null,6.7511169966067435,0,1.0186526501471265E-2,0.19520383391728133,0.12264569297248117,8.439552378600837E-2,0,1.0186526501471265E-2,0.27512297805277514,5.9118984113420447,0,1.916819506085158E-2,0.10180310426488394,-1.0670457885172786E-3,4.1946302998932199E-2]
[null,365,1.0023844897613674,1.027478183227247,1.0006363830437137,0.99878863114329008,0.97754082046840951,0.9949945638134855,0.97532044820797126,null,6.7287911546873591,0,1.0220563568885002E-2,0.19073016458282194,0.12036861482622226,8.3095737923650242E-2,0,1.0220563568885002E-2,0.26199101379167933,5.9120316742496701,0,1.9142125227672266E-2,0.10035540056645155,-1.010038064975654E-3,4.2086461584169794E-2]
[null,366,1.0272004236323073,0.98024214958905598,1.0253914546931655,1.0040526427804379,1.0108502617896538,0.98482107922470508,1.0196369250807618,null,6.7309950964049969,0,9.8568686160368981E-3,0.19080755520417797,0.11923477550781439,8.469541552832513E-2,0,9.8568686160368981E-3,0.26681413678463162,5.9109070534141761,0,1.9010733768335026E-2,9.9175845584498976E-2,-2.3924989059264073E-4,4.0588830503629679E-2]
[null,367,0.96535458017634812,1.0030964112644352,1.0202990575607715,0.98152635857948944,1.036522200562785,1.0177439917412778,0.98494069463619172,null,6.7730990484373841,0,1.078044632927754E-2,0.2071201880315546,0.12580913849637185,8.4509584745339178E-2,0,1.078044632927754E-2,0.27717436927172201,5.9099826838267333,0,1.9350745973231269E-2,0.10792472014975088,-3.1643411933743822E-3,4.4391959136049937E-2]
[null,368,1.0021624584344648,1.0197465769700951,0.98580103126574226,1.0080541247486043,0.97461820134590615,1.01452092230387,1.0057721077654507,null,6.7455300460181853,0,1.0593495476714563E-2,0.19338998214014361,0.12103392511145954,8.2315612538810243E-2,0,1.0593495476714563E-2,0.27210667751603568,5.9133606389478981,0,1.9143330174347023E-2,0.10250947045809884,-1.9517196698190561E-3,4.3622128801206861E-2]
[null,369,0.99161246188703034,0.99081223469672375,1.0135775579669672,0.9979211090707526,1.0050607577985349,1.0264814099648991,1.0362167504382098,null,6.7740434176886053,0,1.070387932276772E-2,0.20361403273710288,0.1232113862430997,8.4207125600439706E-2,0,1.070387932276772E-2,0.28487360159391301,5.9112524361335623,0,1.9201206140324261E-2,0.1064500668147732,-2.8431074062737266E-3,4.4076669831661579E-2]
[null,370,1.0250514702323625,0.99470693620744077,1.0298026769572577,0.98921673309015401,0.9743309848022047,0.98156463851628328,0.98572793291672578,null,6.7189840167660133,0,9.7455276777494541E-3,0.18988661185150663,0.11870481083968522,8.4837155217782276E-2,0,9.7455276777494541E-3,0.25805597290829796,5.9098510335265022,0,1.9021860104470774E-2,9.8483600504578772E-2,1.2623475479977557E-5,4.013034833771021E-2]
[null,371,0.95529641750818572,1.0221766285673322,0.97062488364213606,0.97512370215183675,0.98648343187657295,1.0373740290619242,1.0304482162759432,null,6.7933185550506954,0,1.1503104559679419E-2,0.20531924035660551,0.12714287870845928,8.1646001742272309E-2,0,1.1503104559679419E-2,0.29470718072371382,5.9124146678836951,0,1.9410205258646854E-2,0.10966352974081851,-4.3528864639889473E-3,4.7367737100474913E-2]
[null,372,1.0387602056510263,1.0480465827807608,0.99402109678624651,0.98766419376809123,1.0107677353212656,1.0095971324533339,1.0378746436421726,null,6.7216882258902473,0,9.9804116926656972E-3,0.184431833423714,0.11535321618402476,8.2784237824275728E-2,0,9.9804116926656972E-3,0.27019326712001823,5.9118012084491136,0,1.8951672170481122E-2,9.736113487166087E-2,-2.8590305637972647E-4,4.1097558903339187E-2]
[null,373,1.0047855229483897,1.0246270888398175,0.99722560936318261,0.99123718125231286,0.98372007401079997,0.99207297396094762,1.0100054149492623,null,6.7352487759086257,0,1.020866495898992E-2,0.18954783470193465,0.1202774871431506,8.2991096258957717E-2,0,1.020866495898992E-2,0.27040543108599829,5.9118150328933998,0,1.9129129024361435E-2,9.9902456702136044E-2,-8.5715712781245983E-4,4.2037465226495464E-2]
[null,374,0.96815532259766779,1.0321133460476406,0.96199442222734721,1.0021277857153013,0.98926396201864431,0.98365947261826558,0.98847651808115289,null,6.7483985019778343,0,1.0798960934775701E-2,0.19029607329282597,0.12513187147302718,8.085024585778261E-2,0,1.0798960934775701E-2,0.2737277078854769,5.9143434520595459,0,1.9334409161221002E-2,0.10208211892249945,-1.8355756605562064E-3,4.4468198986014409E-2]
[null,375,0.96953572916000952,0.99132113735538863,1.0267700329886609,0.99202816675310201,1.0137169327255726,1.023284213751591,0.99890830415087872,null,6.7797352095868,0,1.0785816988524068E-2,0.20921600847913208,0.12573275244283533,8.496416189714695E-2,0,1.0785816988524068E-2,0.28057596194345413,5.910178032893846,0,1.9326391933848837E-2,0.10867035066561564,-3.3425252239649064E-3,4.441407455488542E-2]
[null,376,1.0217073940566863,1.0056827408909754,0.99847807960831936,1.0046818061471194,0.99351369572311288,0.99805865840258656,0.99830155179662672,null,6.7270695917680152,0,1.0170039690025221E-2,0.18918142449104797,0.11914879922169895,8.2985873723464415E-2,0,1.0170039690025221E-2,0.26356684162648181,5.9124714049160891,0,1.9039267347533383E-2,9.9647281494968903E-2,-8.4971429720821778E-4,4.1878413243940413E-2]
[null,377,0.96182083556094944,1.0018591989389449,0.97446940512917202,0.99534479163022294,0.99175432458841073,0.98684821251515298,1.0178765468528468,null,6.7692775491425126,0,1.0925788644463301E-2,0.19613088088753949,0.12722478456911385,8.176436236722423E-2,0,1.0925788644463301E-2,0.2843461738005798,5.9132978454966389,0,1.9371494160465848E-2,0.10455383967557005,-2.4022847346394467E-3,4.4990452920017167E-2]
[null,378,0.97509590788296818,1.0274290431177104,0.98281218576519558,0.97506152377942024,1.0160398070901793,1.0018182193831813,0.97965519358945485,null,6.749299661882656,0,1.0744719054905962E-2,0.19528302471524084,0.12407705922602603,8.2095018776318987E-2,0,1.0744719054905962E-2,0.27112846417197128,5.9117425187244148,0,1.9294328971844601E-2,0.10366766288938342,-2.2332561719479362E-3,4.4244840579405524E-2]
[null,379,1.0154826297745392,0.98097318733036565,1.0072824680228409,0.96753429745162101,1.0211819014075401,1.0276399807586074,1.0027627576200828,null,6.7476318402829936,0,1.0566933393465011E-2,0.19914451169659017,0.12091405267815628,8.3583807255237605E-2,0,1.0566933393465011E-2,0.26940737524640052,5.909967842905993,0,1.907197504077331E-2,0.10443800345429716,-2.4084788647133776E-3,4.3512750870259791E-2]
[null,380,1.0267057222077076,0.9974425637943648,1.0136979416529701,0.99448682003517974,0.97156211200534925,1.0014556967937562,1.0141078283473806,null,6.731550324494922,0,1.0056137460530376E-2,0.19132647900542107,0.11868070580500467,8.3965698999600394E-2,0,1.0056137460530376E-2,0.26685939592466029,5.9110600220817346,0,1.9013290987965645E-2,0.10002014764712205,-7.8480009330534879E-4,4.1409384136721718E-2]
[null,381,1.0002950679132971,1.0106513060035729,1.0119391484212801,0.98387100322878485,1.0052573109603411,1.0200268869757465,0.98027575189724581,null,6.7447462254410322,0,1.0470088006603259E-2,0.19868435802262246,0.12120788930873194,8.3843971430410516E-2,0,1.0470088006603259E-2,0.2663439307991145,5.9105865048067461,0,1.9153485525234604E-2,0.1039569320319995,-2.1448052888287149E-3,4.3113958804999339E-2]
[null,382,1.0142160641000133,1.0012928700745962,1.022556645564118,0.99731759649792262,0.97730171610765304,0.99770976524278443,0.98828768397206435,null,6.7319021059339974,0,1.0046968430836078E-2,0.19367383670982188,0.11979219673657986,8.4462821820867492E-2,0,1.0046968430836078E-2,0.262900574404067,5.91070627293412,0,1.9078679299575723E-2,0.10080609003167593,-8.8999370718002542E-4,4.1371627704467034E-2]
[null,383,1.0032665154717593,0.9656500840420581,1.0003899900686217,0.98747183680107564,0.97000916952777838,0.99395222946159278,0.98293623340810843,null,6.7409861183531508,0,1.0477971975073164E-2,0.19546241003452378,0.12329028918793859,8.3103282495382472E-2,0,1.0477971975073164E-2,0.2643093414215556,5.9114339419464104,0,1.9137343810577453E-2,0.102857922123002,-1.7548362501058699E-3,4.3146423583864342E-2]
[null,384,1.0306402012455245,0.98409544462233922,0.97891521774595247,1.0021014918805224,0.98212160106042201,0.98069858021150413,0.99435929626834818,null,6.7154769007824298,0,1.0171181571225823E-2,0.18379342486991287,0.11950179332190855,8.1705599658077555E-2,0,1.0171181571225823E-2,0.25883956804676506,5.9134190788473937,0,1.8993020686125867E-2,9.7758809347741851E-2,-4.1750930297807128E-4,4.1883115307477216E-2]
[null,385,0.98537663720423307,0.98079803245791874,0.97286349870088396,1.024189751587794,1.0180334401604862,0.97227135238218054,0.98834500023629324,null,6.7431099471830906,0,1.0618001228015624E-2,0.19015191205118948,0.12527367774181136,8.1472249131312902E-2,0,1.0618001228015624E-2,0.268310974155689,5.9149452540045342,0,1.923599784438193E-2,0.10144831153531969,-1.4514684043564997E-3,4.3723039123203501E-2]
[null,386,0.96230644025082623,1.0054804763466063,0.99851145789796347,0.98473279867534214,1.0090012870591487,0.99091869266574228,0.98230380697627828,null,6.761367178844611,0,1.0721177659715279E-2,0.19944346657800674,0.1265131097760199,8.3126513179357195E-2,0,1.0721177659715279E-2,0.27466848773645514,5.9113914083447865,0,1.9368633927944853E-2,0.10505085085869344,-2.3431928608732321E-3,4.4147901304222435E-2]
[null,387,1.0201697175008515,0.99998642381874747,0.96096176560577984,1.0279614391722511,1.0181283763944222,0.96745195388627137,0.96759438022111621,null,6.7071665458261309,0,1.022605243014834E-2,0.17992419157134393,0.12028211754360425,8.0531936645895807E-2,0,1.022605243014834E-2,0.25310107634217899,5.9157962406842772,0,1.9047309866054241E-2,9.6568541772473163E-2,-1.9393233756966719E-4,4.2109063737871336E-2]
[null,388,1.0364733695928974,1.0123081823792788,0.99682131545167807,1.0064725240314099,1.0370640539956657,1.0062323171384784,1.0031617307302578,null,6.7203321458426313,0,1.0093471997703893E-2,0.18729676641081688,0.11717304782706341,8.2859130122865776E-2,0,1.0093471997703893E-2,0.26175432380774888,5.9126610843714387,0,1.8963251612184151E-2,9.8735862983200487E-2,-6.7444240819180548E-4,4.1563121115502373E-2]
[null,389,1.022792380888268,1.0011810716490133,1.0192648103146709,0.97322406557366703,0.96226445004627548,1.0054946425871925,0.98967891163101196,null,6.7278416308464779,0,1.006992055673755E-2,0.19317337786833955,0.1188539032700467,8.4225698218660883E-2,0,1.006992055673755E-2,0.26176848246534851,5.909593379027374,0,1.9033607086138566E-2,0.10070871400516122,-9.8167156819833705E-4,4.146614047360319E-2]
[null,390,1.0013367887437128,1.0247365649378171,1.0104754502795208,1.0124256804207103,0.97492041960977105,1.0185677235389914,1.0257602649174313,null,6.7547660612822868,0,1.0395842528939455E-2,0.19684848493552082,0.12044057800975178,8.3933127153529782E-2,0,1.0395842528939455E-2,0.27812355176664749,5.9122125669952217,0,1.9147815707608391E-2,0.1030709097690581,-1.8192021982308005E-3,4.2808229143182171E-2]
[null,391,1.0403731782426913,0.98018013118258973,1.0062935148360281,1.0427299303386053,0.98142886794105677,1.027650629782574,1.0324508377819541,null,6.742625282020982,0,1.0326730604110651E-2,0.19433286246662784,0.11807742968705297,8.3593546101496136E-2,0,1.0326730604110651E-2,0.2707558870700022,5.9140871352425268,0,1.8943535465347387E-2,0.10196454333460389,-1.653295884879089E-3,4.2523638538201194E-2]
[null,392,0.97986207844419881,0.97887317590529921,0.95878877644850369,1.0137506240774299,0.99071826330283985,1.0405057589152582,0.98054586956348422,null,6.7709883254335885,0,1.1577703670235305E-2,0.20304939845999428,0.12634465073229001,8.0662992307894768E-2,0,1.1577703670235305E-2,0.27418060604798095,5.9151450187209145,0,1.9267134330432707E-2,0.10909987520464853,-4.4362733301617939E-3,4.7674922959597368E-2]
[null,393,0.95792894757336489,0.96283533714039438,1.0097407600602382,0.9846474708859051,1.0033193101024291,0.98346550459175863,0.99196839198414788,null,6.7740217459875112,0,1.0783211825195609E-2,0.20396148966977287,0.12909015869340329,8.3873960801550962E-2,0,1.0783211825195609E-2,0.27837108866356586,5.9107532972422909,0,1.9394522302273294E-2,0.10683412983380114,-2.660248175147528E-3,4.4403346956000608E-2]
[null,394,0.98795860209466191,0.99079041584072891,1.0115064094952604,0.99547134097173706,1.034020439956888,1.0311910273061826,1.0285923329445148,null,6.7762325503133347,0,1.0812432253860324E-2,0.20504942807693902,0.12370782651969349,8.4069001619050648E-2,0,1.0812432253860324E-2,0.28428393652366241,5.9112378984756804,0,1.9221538940678743E-2,0.10731025541582012,-3.1710067383944247E-3,4.4523671480199485E-2]
[null,395,1.0190183006418805,0.98862286256300491,1.035319725625234,0.99443108151376758,1.0167383336982663,0.97536459723691427,0.97480454266074656,null,6.7196007181542612,0,9.7198219208742866E-3,0.19093626301205019,0.11959752324194339,8.5156116361958592E-2,0,9.7198219208742866E-3,0.25621001363557805,5.909812796096193,0,1.9053348020447624E-2,9.8760609679096653E-2,4.9551500634463099E-5,4.0024496606352447E-2]
[null,396,0.98149386600628918,1.0286777038077348,1.0011057402334234,1.0022321087611072,1.0204048738083886,0.99578120497014899,0.98551522398492608,null,6.7467741660740934,0,1.0436861377383026E-2,0.19490205558787907,0.12286437963619895,8.3242010399702041E-2,0,1.0436861377383026E-2,0.27042792149610373,5.9121913659873364,0,1.9257884428692626E-2,0.10252660751940848,-1.615196441218772E-3,4.2977137459989954E-2]
[null,397,0.99560723602839929,0.97928876385182106,0.97002595455966067,0.98826938281664667,0.99394310443486167,1.018146828086085,1.0109491556529691,null,6.7584352761433832,0,1.103925428639136E-2,0.19686482235028849,0.12411590098892376,8.1370703927430399E-2,0,1.103925428639136E-2,0.27606697281760972,5.9131580849278764,0,1.9179147016904704E-2,0.10517958369798235,-2.9576238209775094E-3,4.545768423734553E-2]
[null,398,0.99448875185445984,0.99004408256020382,0.99929883760144234,0.97381176120041457,0.99982764815345593,0.96951206223993802,0.96071708943643175,null,6.7257473681651936,0,1.0210586098545749E-2,0.19016677164154286,0.12316411764590592,8.2943602971826208E-2,0,1.0210586098545749E-2,0.25812794403766293,5.9107570075094653,0,1.9185305417909443E-2,0.10012545247798114,-7.682096743439888E-4,4.2045376137236273E-2]
[null,399,1.0274684518634869,1.0178366791995466,1.0294678294916837,1.0366808514567258,1.0021322618243651,0.97522646509570465,0.99840510655857362,null,6.7166759788308177,0,9.5680115346779577E-3,0.18633554489387166,0.11734783162860363,8.4877750281161901E-2,0,9.5680115346779577E-3,0.25997969280439598,5.9124342898712152,0,1.9009349300419507E-2,9.6657739202380327E-2,6.3441239153420002E-4,3.9399368457237398E-2]
[null,400,1.0167613519563425,0.97018724216937968,1.0092148591214469,0.98852515163654064,0.96252949527271103,0.99947342868737499,0.98508338770714088,null,6.7342878877902015,0,1.0295737275021954E-2,0.19458948272785209,0.12126103826186652,8.3616785882527148E-2,0,1.0295737275021954E-2,0.26184825875066187,5.9109926513297797,0,1.9065223378488736E-2,0.10195163527667167,-1.4332013432707769E-3,4.2396013525620876E-2]
[null,401,1.0153151212418043,0.99522070007887142,1.0137387724733791,0.96680727215721596,1.0053631081661885,0.99005001163514783,0.97670109866510013,null,6.7237065396771607,0,1.0062388660036262E-2,0.1914569824840418,0.12011849992556567,8.384086243194995E-2,0,1.0062388660036262E-2,0.25888472469230261,5.9095621444946831,0,1.907286074684577E-2,0.10008635300002762,-7.5101356187391656E-4,4.1435125463614927E-2]
[null,402,0.99722643218738904,0.9978556858562625,1.0096866620449676,0.99046547775327454,1.0001785351712158,0.97339448138115903,0.99340495280695218,null,6.7346614087063976,0,1.0096881406996093E-2,0.19096444384229114,0.12224468571718985,8.3711472714630447E-2,0,1.0096881406996093E-2,0.26649042447058369,5.9110707384361021,0,1.9170256158775635E-2,0.10002901127206862,-5.9678436136361888E-4,4.1577160456115425E-2]
[null,403,0.98454976958660867,0.9811902397323532,1.0003666747592392,1.0158545565807555,0.99683049508414612,1.0154538125896542,1.0143585732824001,null,6.7704119815958927,0,1.0833945105863071E-2,0.20209596699425714,0.12483480630380969,8.333237547642075E-2,0,1.0833945105863071E-2,0.27987673055796825,5.9129691220278042,0,1.9240644303165324E-2,0.10634992115969599,-2.8998428028334535E-3,4.4612257575601888E-2]
[null,404,1.0295781257864396,0.99432016477145801,0.97841351473730021,1.0173160894051481,1.0026657005803878,1.0138035183156735,1.0159061254273025,null,6.7335689754920365,0,1.0483439797426754E-2,0.18929496509984667,0.11914054925167439,8.1802194103263615E-2,0,1.0483439797426754E-2,0.26770958458761135,5.9142691964169254,0,1.8998477197052974E-2,0.10071036110726422,-1.5252913746873981E-3,4.3168939103080325E-2]
[null,405,1.038288695379564,1.0211541896033645,1.027513491648989,0.98144703560100177,0.9961328266914693,1.0126744193040464,0.9828295412165694,null,6.7158918797175051,0,9.8350207433372701E-3,0.19098291878615464,0.11600931874418094,8.4668574272435473E-2,0,9.8350207433372701E-3,0.25653976480231516,5.9095635606783903,0,1.8954055498231124E-2,9.9163557166902949E-2,-4.88735083733642E-4,4.0498864852628991E-2]
[null,406,1.0222043559954574,1.0098657572098604,1.0181761743996924,0.97522920343992325,1.0038343703136072,1.0197944949259321,0.99132363418721581,null,6.7326079460570289,0,1.0190987417552795E-2,0.19518122414637123,0.11853218420929829,8.4184396738265665E-2,0,1.0190987417552795E-2,0.26356997304990504,5.9097639917743212,0,1.9036673258333057E-2,0.10181009154022612,-1.4352609170391159E-3,4.1964672257342454E-2]
[null,407,1.0197903386782632,1.0134624095435096,0.9998517394500045,0.99572962044916091,1.0041771881107533,1.0183341903561203,0.95339777508763179,null,6.7222284206273057,0,1.0349480311642741E-2,0.19291155977867427,0.11898029839980061,8.2935162167282375E-2,0,1.0349480311642741E-2,0.25389388006886565,5.9119104629986587,0,1.9049297863418441E-2,0.10154273038022432,-1.6122888141469982E-3,4.2617317784521359E-2]
[null,408,0.9787575378885377,1.0237488214380708,0.98215529175610983,0.99366770312588559,1.0307114084737996,1.0429540191964475,0.98496967738749197,null,6.7661350175031272,0,1.1167581153557933E-2,0.20277077065935323,0.12380278438088006,8.2124569605145525E-2,0,1.1167581153557933E-2,0.2754751704895827,5.9127845920236224,0,1.9273413000140252E-2,0.10767797179210588,-3.760365882709605E-3,4.5986111435006617E-2]
[null,409,0.99907554068344295,0.99021292687180729,1.0357443772104966,1.02266423867283,0.98728117975127427,0.98946832360016057,1.0277165066034557,null,6.7547301365853407,0,1.0046530086618356E-2,0.19747799201431734,0.12189831464378001,8.5488935457768866E-2,0,1.0046530086618356E-2,0.27686792214481937,5.9113130397184799,0,1.9160138120288578E-2,0.10212304950296486,-9.6907769807751619E-4,4.1369822681000826E-2]
[null,410,1.0366205061565694,1.0215793826967958,0.97328097101838285,0.98723545691627956,0.97369203939231097,0.9982640493914805,1.0268617492387704,null,6.7187080944434214,0,1.0179994350525337E-2,0.18242090280385559,0.11714881443661346,8.145174363296255E-2,0,1.0179994350525337E-2,0.26703450101559473,5.912924455972921,0,1.8962505045326788E-2,9.7303326566066758E-2,-4.5755979393891403E-4,4.1919404764016392E-2]
[null,411,1.0228621379706417,0.98752156110412725,1.0226603899687112,1.0093394934268229,1.0252577884817209,1.0064665532791222,0.97657469730491508,null,6.7295242301261906,0,1.0108361408664087E-2,0.19488720042291247,0.11943750111318162,8.4417682662529969E-2,0,1.0108361408664087E-2,0.25851461245227741,5.9113497765055598,0,1.9033243581663865E-2,0.10143246049238984,-1.1726801639510309E-3,4.1624433059620082E-2]
[null,412,1.0055978999301176,0.98860934604531336,0.99066267112730799,0.99141316458463769,1.0080023330388992,0.96251850302027087,1.006226324474458,null,6.7280995821978111,0,1.0107100095566509E-2,0.18584546120072729,0.122035445130565,8.2534076500197812E-2,0,1.0107100095566509E-2,0.26670436635665956,5.9121911173061132,0,1.9124745878496448E-2,9.8271670012487558E-2,-2.2653938423206863E-4,4.1619239196789622E-2]
[null,413,1.0224569331235693,0.97438730738390211,0.98812586837105643,1.0213574501887859,0.96213093145004636,0.98797942743570677,0.99352526091207771,null,6.7272679911680475,0,1.028971562158814E-2,0.1884930337389063,0.12076766507001797,8.2327266956017595E-2,0,1.028971562158814E-2,0.26147621256045961,5.9139507409491188,0,1.9035355798721017E-2,9.9797855561321272E-2,-9.5135689511550265E-4,4.237121742859478E-2]
[null,414,1.0029045059357693,0.98402888936653055,0.99719853301757566,0.99253829556205231,1.0214334952885837,1.0084780287516062,0.95938017281074039,null,6.7368877306391113,0,1.0578766680386554E-2,0.19641176167998212,0.12246814467212484,8.2840591925542925E-2,0,1.0578766680386554E-2,0.25919347339628562,5.9118868690031645,0,1.9139305228554952E-2,0.10352152905477399,-2.1354225608745947E-3,4.356147823955614E-2]
[null,415,0.99634871172570316,1.0084095473607648,1.0027664386518114,1.0097103344099498,0.97970879893530216,0.99535946495814953,0.98550028852621607,null,6.7402832788341138,0,1.034977981629329E-2,0.19375189276615987,0.12196865651546061,8.3297199665833141E-2,0,1.034977981629329E-2,0.26653970949270145,5.9125019799008554,0,1.9175072054989806E-2,0.10183761425692445,-1.4073969101710349E-3,4.2618551091362492E-2]
[null,416,1.026109756325589,1.0089814007510574,0.96756618093816094,1.0125799022507267,0.9631093054978026,0.98173851839979176,0.99471664874502175,null,6.7140125092344478,0,1.0218610201947285E-2,0.18156575163535216,0.11904016486230314,8.1021187486919471E-2,0,1.0218610201947285E-2,0.25992604563637323,5.9146064782141758,0,1.9016374940175933E-2,9.7125799662596907E-2,-3.6771117025614442E-4,4.2078417966806628E-2]
[null,417,0.99180035204304096,0.98298809541027032,1.012708158393721,0.97153784272597599,1.0105015661595147,0.99975346925355368,0.97777864384613655,null,6.7468611618744507,0,1.0466621878779232E-2,0.19884478679879339,0.12359596445566373,8.3883198411198262E-2,0,1.0466621878779232E-2,0.26634254099562982,5.9098763901406146,0,1.9200164629389661E-2,0.10400134476344688,-1.9829142278570476E-3,4.3099685907567749E-2]
[null,418,1.0148438542082689,0.99273447485296917,0.98497691313753266,1.0453548956608036,1.0360260018102734,1.0185356017594598,1.0238922094780281,null,6.7502087067175607,0,1.0631589602607476E-2,0.19384833721951517,0.12082704629072638,8.2317955932014866E-2,0,1.0631589602607476E-2,0.27421154938768094,5.9154226023026082,0,1.9075354152967537E-2,0.1027947445325704,-2.0678767316525994E-3,4.3778993631132225E-2]
[null,419,1.0298124632193382,0.98404224394458129,0.98423586118657158,0.96310905429625238,1.0089601424809931,0.99831833293136651,0.96692675981967913,null,6.7138326870317364,0,1.0314529161902876E-2,0.18786070501889765,0.11950386284508796,8.1937540965205904E-2,0,1.0314529161902876E-2,0.25348011584148022,5.9110177434641775,0,1.8997272299122511E-2,9.9656498075913175E-2,-1.0944466491191478E-3,4.2473395170965336E-2]
[null,420,1.0213826828010026,1.0008421078440417,1.0145462680464661,1.0189471090383106,1.0177844553312754,1.0058365472154043,0.98764473266412423,null,6.7305456385179987,0,1.0130458400482215E-2,0.19298262864470397,0.11912130416246923,8.3965469608488844E-2,0,1.0130458400482215E-2,0.26161761007372925,5.912333284059434,0,1.9040963669779084E-2,0.10084368582689873,-1.0747320663125784E-3,4.1715424538809227E-2]
[null,421,1.0218586826388016,1.0025544809363132,0.97241052824874608,1.0160345746389912,1.0288546726165579,1.0302564311541378,1.0105281063814351,null,6.7415972974243958,0,1.0752288341029492E-2,0.19242734820593058,0.1197538757116634,8.1454373279193151E-2,0,1.0752288341029492E-2,0.26973910727233685,5.9145291052491045,0,1.9038477369858978E-2,0.1026856412043026,-2.3066404203740229E-3,4.4276009552379529E-2]
[null,422,1.0023538605242175,0.97943815134887713,1.0097689260565277,1.0008137248893183,0.98464378347566095,1.0168729520716282,1.019521691674115,null,6.75970603406435,0,1.0577266205906129E-2,0.20007442723534999,0.12252747161630452,8.3858541127251301E-2,0,1.0577266205906129E-2,0.27647892517196937,5.9116252322679914,0,1.9142291418410121E-2,0.10479664355833442,-2.3527978839860695E-3,4.3555299552720243E-2]
[null,423,0.99990265435397863,1.004062874283371,0.99181311852172194,0.986940651557209,1.0112243810645016,0.96092283288975022,1.0256214258570773,null,6.7336740008878406,0,1.0070498252091499E-2,0.18548851674193956,0.12195000344750882,8.2687975026325425E-2,0,1.0070498252091499E-2,0.27310476875544148,5.9118852945905234,0,1.9155624394292123E-2,9.8026699661938263E-2,-9.3401050374422023E-5,4.1468519320244798E-2]
[null,424,0.96270477944151778,1.0471223568124084,0.98549362861775858,1.0297536074459743,1.0130846267067639,0.96154431836730214,1.0188923256643834,null,6.7530120459721577,0,1.0336826476818014E-2,0.18861834094851646,0.12467241292738032,8.2439414647061671E-2,0,1.0336826476818014E-2,0.28149978499487127,5.9145506390659248,0,1.9366289847254022E-2,9.9995539897765551E-2,-6.9558790162992871E-4,4.2565211545011764E-2]
[null,425,0.96337110966957218,1.0098294185101973,1.0021435370871703,0.98049170781579931,1.0010604589757346,1.008496271336804,0.98024382835104784,null,6.7664004485923215,0,1.0844710010791634E-2,0.20282995070591339,0.12608492964455506,8.3359261933030282E-2,0,1.0844710010791634E-2,0.27543340487318951,5.9109580770984484,0,1.9362373070574583E-2,0.10664206936796083,-2.926203639373192E-3,4.4656585538016061E-2]
[null,426,0.9875302688424803,1.0128239311621321,0.98359638740712707,0.98649642889758971,0.99711532559412863,1.0035187344396448,1.0204462769830873,null,6.755722742169139,0,1.0685449643346336E-2,0.19443185250810152,0.12320371589366919,8.2257461053092853E-2,0,1.0685449643346336E-2,0.27916914602984855,5.9123173328423944,0,1.922393235931661E-2,0.10317534337232033,-2.0568215817712743E-3,4.4000779692164996E-2]
[null,427,0.97920843948788838,1.0347003542438251,1.0056598862568387,0.98700535785487087,0.9935070431866786,0.99484955890927063,1.030750227333036,null,6.7591879191245683,0,1.0383955216601504E-2,0.19522647414377758,0.12277779558540411,8.3687791248002866E-2,0,1.0383955216601504E-2,0.28336240546534858,5.9111117419545174,0,1.9270848176257134E-2,0.10246557292295587,-1.4739896785283429E-3,4.2759279306837213E-2]
[null,428,1.011292808023488,1.009747560983514,0.98986648552815637,0.98712563048178681,1.0052628521966724,1.0217844545430264,1.0250114564820252,null,6.7482784447507784,0,1.0580115421015673E-2,0.19431358435126989,0.12034026787239298,8.2599492269930255E-2,0,1.0580115421015673E-2,0.27560815928098842,5.9120036778005192,0,1.9094216955444956E-2,0.10279025665049976,-2.0382425436709026E-3,4.3567032113399969E-2]
[null,429,0.99730179347945824,0.98555662175333769,1.0045786802305767,0.98133416925014372,1.0118752996167975,1.0153317203223424,0.97085650514429578,null,6.7464979531392091,0,1.0634586569193931E-2,0.19961865813087001,0.12294021443248791,8.3360124619930018E-2,0,1.0634586569193931E-2,0.26439656733322781,5.9108663358278974,0,1.9169843059916571E-2,0.10482698785243971,-2.4721127236597483E-3,4.3791334606095078E-2]
[null,430,1.0243780891614054,0.97027404090942071,1.004570042778788,1.0113219592947593,0.99050366048210181,0.99758856409563568,1.0106728298119192,null,6.7360247322275599,0,1.0241020663488736E-2,0.19222869071176438,0.12044138314212678,8.3407229293695304E-2,0,1.0241020663488736E-2,0.26646629302760844,5.912487326810747,0,1.9025356181488977E-2,0.1009466805022077,-1.1489277005963163E-3,4.2170700258520877E-2]
[null,431,1.0106553955450308,0.99448048013027579,0.97473743448187111,0.99114678514893173,0.97950011138493343,0.97405868276533636,1.0327123065063122,null,6.7337948405486125,0,1.0293247385154329E-2,0.18484953798808942,0.12143094831169329,8.1630535918233119E-2,0,1.0293247385154329E-2,0.27338857373896058,5.9130562018232391,0,1.9097616858899005E-2,9.8526706119374127E-2,-5.7104081220829431E-4,4.2385760602329868E-2]
[null,432,0.97571615397931022,1.0056041279160279,0.99702984246676329,1.0319666938847838,1.0080016662026088,1.0308336700127876,0.95974241452437892,null,6.7634603645049491,0,1.1013416422247003E-2,0.20443062393965081,0.12479660638579203,8.2983141557790033E-2,0,1.1013416422247003E-2,0.26836021098824875,5.9140272380372334,0,1.9290774956885033E-2,0.10775701892968813,-3.5365388021105586E-3,4.5351288511767458E-2]
[null,433,1.0185203398683524,0.9662345673485685,1.0189762556269077,1.0091183198908695,1.0168464903847199,0.96675055267541421,1.0050681351697528,null,6.7282761353734148,0,9.8741859494619593E-3,0.18933771777562119,0.12106615302100752,8.4260329967057984E-2,0,9.8741859494619593E-3,0.26367002613261276,5.9115491337452921,0,1.9055963609337655E-2,9.872307337488534E-2,-4.6402452701976743E-5,4.0660140200303639E-2]
[null,434,1.0047442915781521,1.0025943313400727,0.98394921166616967,1.0017228674052356,1.0208510455130941,1.0068541225511216,1.0133929472293848,null,6.745497955311448,0,1.0579932470879121E-2,0.19261264177803622,0.12157908353763225,8.2206225525971524E-2,0,1.0579932470879121E-2,0.27290883131956578,5.9131209151325965,0,1.9129351675485684E-2,0.10219195117925127,-1.8173235943940776E-3,4.3566278757301555E-2]
[null,435,1.0038289222589192,0.96202756038634496,1.0101933820401121,0.99867008277706193,0.98621220392655606,0.99501843423958503,1.0343199806528123,null,6.757311288712895,0,1.0410657854108231E-2,0.19704672183020255,0.1232202660899948,8.3905566845478854E-2,0,1.0410657854108231E-2,0.27813481368478432,5.9114853138062369,0,1.9134299418577375E-2,0.10318910096120237,-1.6740299387760374E-3,4.2869236015197619E-2]
[null,436,1.0193111593167339,0.99121140309853428,0.99063234588801485,0.98477424116417689,0.99522262740407297,0.97356363969373383,1.0345766626737771,null,6.7297755832721045,0,1.0074459456176377E-2,0.18523694973993901,0.12026768403711662,8.2591139598964441E-2,0,1.0074459456176377E-2,0.2715668336485621,5.9118339670010123,0,1.9051810944341663E-2,9.7951381154922898E-2,-2.0901370634932649E-4,4.1484830853598297E-2]
[null,437,0.99210893805907374,0.98761196071650026,0.98639945368774229,1.0352470476242117,0.98757460341542092,1.0011186671357906,0.97510384044929355,null,6.746648565114719,0,1.0699691425531861E-2,0.19550207092291266,0.12382509979058018,8.2286329852735013E-2,0,1.0699691425531861E-2,0.26556603494376579,5.9147973633329158,0,1.9198454934308662E-2,0.10359804806316708,-2.1842615419326917E-3,4.4059424816262245E-2]
[null,438,0.99684232206303769,0.96885266322921593,0.99555515511709836,1.0081737005987064,1.0012035937078714,1.0035260465742064,0.98323364107093414,null,6.7495349488801821,0,1.0676954570635245E-2,0.19775260593498248,0.12401256502581733,8.2854002785022821E-2,0,1.0676954570635245E-2,0.26695247130853528,5.9128239231368509,0,1.9172362659175917E-2,0.10431346698299385,-2.3122474480093873E-3,4.3965798494807293E-2]
[null,439,0.99976613714118034,0.98421990575463747,1.0107325548235866,1.0007710320375138,1.0018515187500672,1.0274086283031987,1.0054431351048279,null,6.7610393509667439,0,1.0683167188140778E-2,0.20236607118198691,0.1225872651424756,8.3889325140630688E-2,0,1.0683167188140778E-2,0.27431932790811997,5.9115682226906818,0,1.9156368881619961E-2,0.10594647681606105,-2.7850877427201435E-3,4.3991380947890374E-2]
[null,440,1.012493476592748,0.99551924844386031,0.96180036885890496,1.0077058918805679,1.0195614805824005,0.98891774850138292,0.99575650813689676,null,6.7279528826701913,0,1.0544720737373231E-2,0.18576236521256173,0.1213960272374931,8.0718464457114614E-2,0,1.0544720737373231E-2,0.26447572537425584,5.9146555817404431,0,1.9087824318645776E-2,9.9659818723354096E-2,-1.2242074998542098E-3,4.3421283106179223E-2]
[null,441,1.0116175224332544,0.98852736401465569,0.97996947758793673,0.97836167927897533,0.99686726296298878,0.96964176295202498,1.041909548751011,null,6.7347198566875912,0,1.02165097716891E-2,0.18490151203410818,0.12151087636836351,8.1971365396801263E-2,0,1.02165097716891E-2,0.27519607402195173,5.9120776680339828,0,1.9092486603917394E-2,9.8296281393035631E-2,-3.9617593343785438E-4,4.2069768768866089E-2]
[null,442,0.96995312927231458,1.0179885698420841,0.96021959535558732,1.0087127371161624,1.0056642970224041,1.0354932910714401,0.95949335468748065,null,6.7623993971672052,0,1.1431681114109951E-2,0.20091517337325693,0.1256236722665228,8.0696914887763704E-2,0,1.1431681114109951E-2,0.27012030594984771,5.9147954145865116,0,1.9323972219856739E-2,0.1078751778935793,-4.0248620746502917E-3,4.7073628064519243E-2]
[null,443,0.97500846317684497,0.97550425412967068,0.98726724590284287,0.98634137582447601,1.0266191851827156,0.99945442612500424,0.99492846321673822,null,6.7638801086853748,0,1.0918603643837753E-2,0.19975887893567174,0.12660332868321236,8.2440883031213066E-2,0,1.0918603643837753E-2,0.27569021268177918,5.9121056770322404,0,1.9294830394375056E-2,0.10580790679221379,-2.782475231653616E-3,4.4960866366323599E-2]
[null,444,0.98486739847557703,1.0327091127616095,0.99767034038691238,1.0174541573367173,1.0298627360831498,0.99504189111821095,0.96920281984151935,null,6.739283953869907,0,1.0407194861537584E-2,0.19336138883387863,0.12231661632299269,8.2965913814365688E-2,0,1.0407194861537584E-2,0.26493255025893397,5.9132069938216123,0,1.9238858512287696E-2,0.10188988573670164,-1.4832294590456493E-3,4.2854976028181405E-2]
[null,445,1.0074183392763656,1.0176018973800016,1.0021576283817999,1.0259608381501666,1.0248581221312654,0.96296519546172377,0.97457872200455087,null,6.7161027569724352,0,9.8697724802389569E-3,0.18459942670463825,0.12020265135281072,8.3151409289887429E-2,0,9.8697724802389569E-3,0.25767313375884787,5.913414473760481,0,1.9114949443878895E-2,9.7056313200348868E-2,2.4843314192750149E-4,4.0641966319611554E-2]
[null,446,0.96643770661987038,1.0224769196310948,1.0267464643873379,0.99511629501143783,0.99533512709588778,0.97913082281917019,1.0393520488363106,null,6.7694376297611187,0,1.0217430065654287E-2,0.19818391572309638,0.12458458462688148,8.5067778626289267E-2,0,1.0217430065654287E-2,0.28807878203870585,5.9103462122641357,0,1.9344416836583396E-2,0.10294128600615095,-1.1829047363300055E-3,4.20735583756085E-2]
[null,447,0.9791576868919124,1.0072281867505484,1.0338028135488253,0.95652582400985886,0.98634464778190711,0.98063212922906839,1.0125397250891599,null,6.7543924301810447,0,1.0102665455610803E-2,0.19801249412887034,0.12357085259320007,8.5327293295214476E-2,0,1.0102665455610803E-2,0.2772962421263066,5.9078535088096658,0,1.9271136749803457E-2,0.10249685235126564,-1.0369280120730746E-3,4.1600978138788519E-2]
[null,448,1.01790859938265,1.0003061521145535,0.9733269976591471,1.0123475239647219,0.97290487718228602,1.0302624901432005,1.0013808310034851,null,6.742166113910514,0,1.0795840460636284E-2,0.19346980499360844,0.12030995607252083,8.1491097647519328E-2,0,1.0795840460636284E-2,0.26836154446401145,5.9142796371824264,0,1.9059180340563624E-2,0.10319442725906486,-2.4548834781403352E-3,4.4455349428931985E-2]
[null,449,0.98543431496541223,1.0250793077196774,1.0195659695628474,0.98522681211497509,1.0078115767594391,0.97856122618943397,0.99289889107671581,null,6.740497885870024,0,1.0066852564089882E-2,0.19320057969370927,0.12219543258161036,8.4365195316544725E-2,0,1.0066852564089882E-2,0.26981026633834565,5.910224598328587,0,1.9235674023767108E-2,0.10070795076295798,-6.9531820146585105E-4,4.1453507025962434E-2]
[null,450,1.0127855549507954,0.99857598040445927,1.0028501355040753,0.98178558986256848,0.99449321693409398,1.0166871521907241,1.0321478231026981,null,6.7501833683627899,0,1.0442950045814442E-2,0.19552031266535855,0.12045888715378783,8.3418365938725481E-2,0,1.0442950045814442E-2,0.27677306038848498,5.9109882023262657,0,1.9086271518056412E-2,0.10276284383562011,-1.826784976357498E-3,4.3002209512847937E-2]
[null,451,0.96914710458647213,0.96344150867450551,1.0000555356891248,0.99721243699824014,1.000047830159257,1.030697581281649,1.0127204520270567,null,6.7906631656393612,0,1.1262193871636994E-2,0.20998768793642636,0.12775431439521465,8.3377517210382293E-2,0,1.1262193871636994E-2,0.28560827851082965,5.9119791463679388,0,1.932864670660446E-2,0.11051989395831895,-4.2680292139730767E-3,4.6375709767620149E-2]
[null,452,1.017242417923679,1.0454325589622337,0.98982782876566178,0.99362424480365741,0.9860985583302242,0.99701132404945902,1.0053963077363544,null,6.7230964219764422,0,1.0112172851392553E-2,0.1857087434695017,0.11798660441565097,8.247545138702618E-2,0,1.0112172851392553E-2,0.26613971768143824,5.9123570872247093,0,1.9062687740885358E-2,9.8240261846828783E-2,-5.1425969196261794E-4,4.1640127902364391E-2]
[null,453,1.010963607224328,0.98910893093914765,0.98295495482344097,1.006803081122958,1.0199819363813303,0.99644989581898635,1.0102847362786957,null,6.7389373356345077,0,1.0475812938911299E-2,0.19043603815602342,0.12150579080868071,8.2103101865487985E-2,0,1.0475812938911299E-2,0.26955243911473237,5.9134504976701612,0,1.9095972348925312E-2,0.10108738057931069,-1.431417966059174E-3,4.3137533057243889E-2]
[null,454,1.0359870425571183,0.99229452471443824,1.0124955234806619,1.0108442370318034,0.97903695112320521,0.98187274578407824,0.97456615305865923,null,6.7090541550658607,0,9.8031555663088549E-3,0.18618165537753001,0.11788311087943751,8.3707819709559483E-2,0,9.8031555663088549E-3,0.25246185265615551,5.9120122864826579,0,1.8965720730964308E-2,9.7388406451707751E-2,8.5653052430793893E-5,4.0367649725416052E-2]
[null,455,0.99844153144895798,1.0430840705619497,0.97771034152576419,1.0198819562232053,0.98116372484876357,1.010089825467535,1.0341467821281882,null,6.7499045110271565,0,1.0558759463610625E-2,0.19045614784669787,0.12053836240348373,8.1926357769762578E-2,0,1.0558759463610625E-2,0.28015788248812279,5.9144465778686808,0,1.9163603099712968E-2,0.10136385446446507,-1.6273669957953371E-3,4.3479092082024683E-2]
[null,456,1.0282049340307389,0.9938285704390647,0.97737594517553428,0.98200123197192701,1.0182543611207464,1.0202228518763887,1.0000305871772561,null,6.7307689388775582,0,1.0575706158002258E-2,0.19066719012331032,0.11934201756942556,8.1669914103473892E-2,0,1.0575706158002258E-2,0.26447148152961275,5.9124170450964586,0,1.9005548806018045E-2,0.1014931838104404,-1.8463177143149333E-3,4.3548875553130272E-2]
[null,457,1.0050026257205691,0.98921305457695996,1.0363378122244535,1.00867866032141,0.98216874180511038,0.98547645475503254,0.98956908090293538,null,6.7379658579404778,0,9.9461169312873472E-3,0.19567573469999816,0.12121708704609206,8.5346703550703826E-2,0,9.9461169312873472E-3,0.26465721098543304,5.9105231183154183,0,1.9127956961663025E-2,0.10116165368356307,-6.9994648261903752E-4,4.0956339180223116E-2]
[null,458,0.98186637053928016,0.97823729406989446,1.0053912026572698,0.98705820242121434,0.96719821380925153,0.97545989692316137,1.0158361565971874,null,6.755948066699716,0,1.0403403491740133E-2,0.19551430885212906,0.12523010581401173,8.3587443750846299E-2,0,1.0403403491740133E-2,0.27715674376085825,5.91112977673078,0,1.925577717109762E-2,0.10263030730893062,-1.3957605311347198E-3,4.2839363842194174E-2]
[null,459,0.98228355631801267,0.98649392555525939,0.99223869150136568,0.97302426814174803,0.9805339707522458,1.0022254453513442,0.95953092557938202,null,6.7471874686315312,0,1.0768908299788398E-2,0.19847770245884189,0.12500892385283763,8.2585304649772012E-2,0,1.0768908299788398E-2,0.26406254966148113,5.9111094000295159,0,1.9253419049058942E-2,0.10486896634136572,-2.523244995653171E-3,4.4344447584306321E-2]
[null,460,1.0010971549718388,1.0049743064130741,1.0027522455170186,0.99554111746889951,0.98146327724224725,1.0038825242826994,1.0086399302889042,null,6.7465146072791518,0,1.0404211628306499E-2,0.1947667828595,0.12155620194185129,8.3363646016164444E-2,0,1.0404211628306499E-2,0.27234505971973511,5.9117370706483889,0,1.9149118927395164E-2,0.10237176975420219,-1.6177341928185745E-3,4.284269160473151E-2]
[null,461,0.98749527641386992,1.0276069667207062,1.0180329797474648,1.0169719322138182,1.0090813872286071,0.9822128551978464,0.99391878187331129,null,6.741902748285451,0,1.0086234973925575E-2,0.19313404909437507,0.12184937035788222,8.4293858861999638E-2,0,1.0086234973925575E-2,0.2698425948042189,5.9120274255603897,0,1.9224127979960141E-2,0.10074935942158209,-7.5135813468334871E-4,4.1533320339725469E-2]
[null,462,0.99863197459454434,1.0321314841938896,1.0081617869245627,0.96857216876241703,0.96947889942196996,1.0095631310713815,0.98714904424518068,null,6.7385094020333627,0,1.0320969385759819E-2,0.19476247802992519,0.12046300424946002,8.3614260294764514E-2,0,1.0320969385759819E-2,0.26747660915496096,5.9099741561139814,0,1.9162561829890512E-2,0.10209546501886724,-1.5390475249828404E-3,4.2499914866491115E-2]
[null,463,0.97689855640162904,1.034877930575276,0.98523757618806984,1.0139818663959759,1.0488614910886227,1.0175616380545924,1.0251265386216275,null,6.7680469804734473,0,1.083687284348233E-2,0.19766771843479278,0.12344521886229684,8.2452919886032858E-2,0,1.083687284348233E-2,0.28465818219884548,5.9137122797152308,0,1.9284012283877466E-2,0.10480645137836915,-2.6041157639964661E-3,4.4624313478000117E-2]
[null,464,0.99088533209847673,1.033926165384379,0.97711928297449391,0.98470374377604941,0.99977597227264647,0.99576671019420659,0.99679863037878669,null,6.739058404281832,0,1.0533470078155626E-2,0.18983340674931296,0.12189764254486855,8.1742370263005945E-2,0,1.0533470078155626E-2,0.27084285424139198,5.9125772429203494,0,1.9205240481308342E-2,0.10106235802253788,-1.4776658350054003E-3,4.3374954894063809E-2]
[null,465,0.98921608471633926,1.0381439625292228,0.96603576329433516,0.97772069281105811,0.99430674907006111,0.98639740437607326,1.0078149457608929,null,6.7374862020622537,0,1.0534975117410869E-2,0.18676200002957161,0.12210862071206913,8.1079143045360597E-2,0,1.0534975117410869E-2,0.27335671679609119,5.9128047508800172,0,1.9214524418116299E-2,9.9982453646040415E-2,-1.2031598428459702E-3,4.3381152377829899E-2]
[null,466,1.001525008343676,0.98464132511982827,0.98093912338937639,0.98152933214182503,1.0280643605571058,1.0289105992327754,0.99869801900135147,null,6.7545915593753474,0,1.0959466568174545E-2,0.19863331837865714,0.12291080657432767,8.1993702550876985E-2,0,1.0959466568174545E-2,0.27208611332342936,5.9121954915098369,0,1.9146792534972836E-2,0.10554505929518854,-3.048857407359341E-3,4.5129132615413105E-2]
[null,467,1.0003269654390683,0.97416264709965406,0.95854134002484614,0.9776479751892535,0.98897589841087363,1.0032748643081297,0.98946678711819303,null,6.7425554405280685,0,1.0960046757566675E-2,0.19214628632838618,0.12400348376663745,8.0534873168414595E-2,0,1.0960046757566675E-2,0.26756333233840901,5.9132059812017799,0,1.9153311739976021E-2,0.10325445996951901,-2.4378097171153454E-3,4.5131521732060038E-2]
[null,468,1.0041552844521144,1.0005252264936304,1.015199945464381,1.0066184367327906,1.0286631761280094,0.98469848955855022,1.0330179666292809,null,6.7459469717851004,0,1.0083309030001261E-2,0.19227034713376628,0.12116802811144059,8.4196916899661786E-2,0,1.0083309030001261E-2,0.27628596817717316,5.9116298854386669,0,1.9132534334889262E-2,0.10043906676323536,-6.9704689717945128E-4,4.1521271823443749E-2]
[null,469,0.9999233307884795,0.99691530981283816,1.0073111519844478,0.98420161155041341,0.98425185998066633,0.95971317888200747,0.98598977771367424,null,6.7249503898682148,0,9.9527794061280515E-3,0.18757812732499121,0.1220057214928076,8.3506024313447641E-2,0,9.9527794061280515E-3,0.26251876975639843,5.910866862308632,0,1.9155511654490087E-2,9.8370809736855483E-2,-3.5210785158442348E-5,4.0983774065740823E-2]
[null,470,0.98623415290951244,0.98382208271129556,1.0038444126164583,1.0006928594471609,1.018369404716456,1.0013546410347161,1.0258323053230551,null,6.7655804354565872,0,1.0620713432625675E-2,0.19914157240742639,0.12442156326111943,8.3554485848995219E-2,0,1.0620713432625675E-2,0.28114222980122822,5.9119538929301871,0,1.9231187393054617E-2,0.10461452929764578,-2.2132329821044731E-3,4.373420749903327E-2]
[null,471,0.99860272816144202,1.0041428394211032,0.99549399222878743,0.96371825170283798,0.99743057129700363,0.98374947321736961,0.99093743521152045,null,6.7332189198605494,0,1.0289674096305009E-2,0.19056233900471548,0.12203611353079041,8.2809988174765578E-2,0,1.0289674096305009E-2,0.26634947442360085,5.9104246822032316,0,1.9162721712317591E-2,0.10052369772996445,-1.0211433537030562E-3,4.2371046434870073E-2]
[null,472,0.97749221164915023,1.0253809019422151,1.0081032437634156,0.9955021898115447,1.0251799348577098,0.98762642962070712,1.0035832031102478,null,6.7523637966475532,0,1.0344593310938387E-2,0.1951913551348049,0.12339276599369914,8.3743671356283939E-2,0,1.0344593310938387E-2,0.27577476688395569,5.9114326550855409,0,1.9280623080906518E-2,0.10232324963000551,-1.3724845031200131E-3,4.2597193985474534E-2]
[null,473,1.023449057626169,0.99459869670322332,0.99976543134134155,1.0031844632981264,0.99132978000527461,0.98914250742910714,1.0229848778140314,null,6.7311305356219249,0,1.0098547704255346E-2,0.18821017557126515,0.1194508877626537,8.3135886470801001E-2,0,1.0098547704255346E-2,0.26889413515675814,5.9123181934633804,0,1.9030187103050142E-2,9.9072312707803339E-2,-5.6526458542769428E-4,4.1584021971639157E-2]
[null,474,0.96268578311080422,0.98106855378158719,0.98803777640840096,1.0272830269964122,0.95804516415044128,0.97667835682119808,1.0337528820454787,null,6.7760117655373806,0,1.0772801536751402E-2,0.19731670873008222,0.12791747313746005,8.2678957573114775E-2,0,1.0772801536751402E-2,0.28772744497449931,5.9142759296122298,0,1.9366401589675064E-2,0.10447415343057662,-2.1057827514123222E-3,4.4360479241149622E-2]
[null,475,1.0031422771250635,1.0071815588875772,0.98491654624913438,1.0030271962204822,1.0288687351640895,1.0196468925728304,1.0065341107836683,null,6.7490744601128956,0,1.070147892531848E-2,0.19510517710593112,0.12153321091394509,8.226415889893815E-2,0,1.070147892531848E-2,0.27265595326574332,5.9131378965456056,0,1.9138016791654226E-2,0.10346434806696531,-2.2910868981144525E-3,4.4066785422220436E-2]
[null,476,1.0293914115407299,0.99675927343383575,1.0089383114955648,1.0090820575571617,0.95940390225269478,0.98860501815781099,0.96693919574060017,null,6.7127085122981827,0,9.9454204486090457E-3,0.18789154983582637,0.11849074563260976,8.3489570441907218E-2,0,9.9454204486090457E-3,0.25264255084828768,5.9121191227213066,0,1.8999437622476814E-2,9.8455845885261559E-2,-3.3378187801248293E-4,4.0953471188523161E-2]
[null,477,1.006088248822776,0.98047856125727684,1.0266787064127576,1.0372717393102089,1.0008022270586094,0.9622757731616991,1.0075917983737179,null,6.7352251514855661,0,9.8212251861286883E-3,0.19047978434101981,0.12170064181450267,8.4804175582471344E-2,0,9.8212251861286883E-3,0.26704798747594094,5.9126273533247353,0,1.9122103647361943E-2,9.8942876230493207E-2,5.8171865476907741E-5,4.0442057203561706E-2]
[null,478,0.98016217012823315,0.98020459297961215,0.99064968308753432,0.97788184993626959,0.99105343764118703,0.95736953143226666,0.99748144227527891,null,6.7425196568749648,0,1.0351840220460432E-2,0.19034198324756432,0.12563089836107394,8.2580263459230571E-2,0,1.0351840220460432E-2,0.27082667752354322,5.911460463361788,0,1.9265430928582662E-2,0.10065000007334034,-8.6309554913861623E-4,4.2627035468984512E-2]
[null,479,1.0212504508011786,0.98232144392596776,1.0407029301808879,0.99939639036063255,0.9974465658020043,0.97668677402441739,0.99272588095739367,null,6.7253365748835732,0,9.6924996105738487E-3,0.19191977567185481,0.11954047858792313,8.5550869450173372E-2,0,9.6924996105738487E-3,0.26053957261669242,5.909767227756805,0,1.9041654771310885E-2,9.9008361985994123E-2,5.6645847090831267E-5,3.9911988195725182E-2]
[null,480,0.99180128469599727,1.0105913036127423,1.0146175537275481,0.99582161404539116,1.0027512885645118,0.95664890341484432,1.0104608791983187,null,6.7348321263819031,0,9.8807106504762553E-3,0.18824485594442589,0.122198103624703,8.4080085737230068E-2,0,9.8807106504762553E-3,0.2708419529320496,5.9110797442193084,0,1.9200159460500882E-2,9.8364485882132452E-2,1.3573082382247042E-4,4.0687007757727024E-2]
[null,481,0.99346640735619196,0.99551458480343846,1.0295285733707946,1.0107086306299817,0.99587593238710825,1.0213444118340063,1.0380798561630902,null,6.7723430577655543,0,1.0461753447016791E-2,0.20375932610611114,0.12244426346152658,8.5198169776921531E-2,0,1.0461753447016791E-2,0.28431945103033968,5.9110278212969325,0,1.9190946601619272E-2,0.10569281771686494,-2.3693767968783292E-3,4.3079638572118571E-2]
[null,482,0.99698985047454769,1.0266427689833442,1.0119285725445681,1.0245259678636625,0.99772773868274378,1.0053294172366176,0.9920838352821244,null,6.7438055477435732,0,1.0284194277478446E-2,0.19515371318275856,0.12084864409369679,8.3908058710971692E-2,0,1.0284194277478446E-2,0.2689212846282707,5.9127837949913502,0,1.9171553405833285E-2,0.10211013860546345,-1.4401213910818801E-3,4.2348481516313694E-2]
[null,483,1.0241075419277144,1.0117727487719197,1.0073523290315023,1.0317786190197755,0.9923525082874799,1.0030801911412377,1.0017736799525652,null,6.7294640398299626,0,1.0092359588132021E-2,0.19022036565002484,0.11842098978183339,8.3565184079998439E-2,0,1.0092359588132021E-2,0.26428205589870141,5.9134354221780105,0,1.9026762110179618E-2,9.9754433798726797E-2,-7.9971407839857201E-4,4.1558540410886927E-2]
[null,484,0.99246017144810816,0.99080348937701124,0.9758884043837448,1.0025611528625598,0.960704352452312,1.0013052822703585,1.004113642788979,null,6.7511334300074548,0,1.0781459867559341E-2,0.1939480508144551,0.12381900671380887,8.1711019986445241E-2,0,1.0781459867559341E-2,0.27333582200476425,5.9136102157775952,0,1.9196510248764558E-2,0.10331663407747285,-2.1999623221485875E-3,4.439613270629128E-2]
[null,485,0.98180676954980761,0.97638095262219393,0.9766222798048545,1.0361423928459439,1.0051359197702556,0.98932546921009945,1.0308759549194266,null,6.7663206993507723,0,1.0829014958349559E-2,0.19501580456667431,0.12588484690714835,8.1903756524085228E-2,0,1.0829014958349559E-2,0.28263125442417802,5.9153854395808203,0,1.9256114226353021E-2,0.10384720424092363,-2.1956772250904975E-3,4.459195610567479E-2]
[null,486,1.0071144137582466,0.99676913008520418,1.0078520089121548,1.0113276218983556,0.99526043644366602,0.97616615259045025,1.0033255261906215,null,6.7327356995152394,0,1.0047001659663267E-2,0.18950561518784007,0.12113155828249909,8.3616103838269701E-2,0,1.0047001659663267E-2,0.26677647017716627,5.9123020269796784,0,1.9116582512907872E-2,9.9355025536564265E-2,-4.3944753454699481E-4,4.1371764534862895E-2]
[null,487,0.99358707159656423,1.0016572202300302,0.98516159678477422,0.99220417106751646,0.96713751107393997,1.0199459127071355,0.96826286706095044,null,6.745925139703596,0,1.0830733031126064E-2,0.19753346603319574,0.12296763997930864,8.2169575329630873E-2,0,1.0830733031126064E-2,0.26489632779144856,5.9125392856773304,0,1.9190280185480982E-2,0.10473924482515813,-2.709710941524131E-3,4.4599030823562875E-2]
[null,488,0.98493522995476912,1.0004765155395949,0.98077057497099807,1.0221207275856687,0.9998788296502048,0.97896006649625533,1.003353328272675,null,6.7470808570932448,0,1.0532370091896502E-2,0.19084474021764539,0.12418918107249939,8.2025123869616523E-2,0,1.0532370091896502E-2,0.27297826934804065,5.9143991185236553,0,1.9238477295607206E-2,0.10141510490990242,-1.3795834901659902E-3,4.3370425346439E-2]
[null,489,0.98563904947958969,1.0040006200871701,0.97278265588755219,1.0255711089114519,0.96847836498016471,1.0244784218315843,0.97763376772627353,null,6.7563492493380402,0,1.1074457861486121E-2,0.19830254200897637,0.12407598286764189,8.1490247325945064E-2,0,1.1074457861486121E-2,0.26999368319514505,5.9150243605316062,0,1.9234524887527995E-2,0.10580106496422453,-3.1758027366107031E-3,4.5602646293582974E-2]
[null,490,1.045120140979382,1.0081013237897039,0.98688608742313122,1.0053515619230053,1.0089388444024365,0.99550026183075169,1.0041849578617061,null,6.7106974341652172,0,1.0007276288679728E-2,0.18298243784306156,0.11657421481709331,8.2203181269580469E-2,0,1.0007276288679728E-2,0.25890842613065779,5.9131543940663702,0,1.8919734942424406E-2,9.6940238899466888E-2,-1.9337633144741147E-4,4.1208182528005136E-2]
[null,491,0.99534508469819161,1.0082160453151197,1.0173243007605972,0.98803030212106735,0.9909911462278107,1.0117656214949506,0.99949285794101161,null,6.7515354124890896,0,1.0398612632790551E-2,0.19890687634140838,0.12182651689785105,8.425980212079949E-2,0,1.0398612632790551E-2,0.27217143181969172,5.9105042998423789,0,1.9180589186669317E-2,0.10379704671708354,-1.9307863745753162E-3,4.2819635937780889E-2]
[null,492,1.0138555121954667,1.0383733549159271,1.0323246287382772,0.9841178256057197,0.98186581972404219,0.97220527098432219,0.97450984719694489,null,6.7119550479311991,0,9.5602048662478557E-3,0.18697135776679005,0.11792422038043122,8.497161727088616E-2,0,9.5602048662478557E-3,0.25674083506910178,5.9094295984517942,0,1.9080590856710516E-2,9.6851770247684099E-2,6.178359016213317E-4,3.9367221986177411E-2]
[null,493,1.0069581739542375,1.0138955418499853,1.0118464665945297,1.0322066040200237,1.0081721934541694,1.0317887715123106,0.97533042500516665,null,6.745294410098424,0,1.0507164365070074E-2,0.19936058178385696,0.12025331712417051,8.3845124043684383E-2,0,1.0507164365070074E-2,0.26428170402318663,5.9132034694469864,0,1.9117422412718351E-2,0.10431552841212383,-2.3493697981278859E-3,4.3266632649819885E-2]
[null,494,1.0069569533736584,1.0046628143873586,1.0046995746487815,0.97765095414039549,1.020863365271659,1.0169111576861527,0.99479934241699486,null,6.7429442829210613,0,1.0461481354336655E-2,0.19640451305817902,0.12082757751792943,8.3416214528236082E-2,0,1.0461481354336655E-2,0.26826215451638002,5.9106604764373767,0,1.91174289752311E-2,0.10313294326573272,-1.9555435209012368E-3,4.3078518142892451E-2]
[null,495,1.0047423123215635,1.0106433147237879,1.0128194127352792,0.97119314123553813,1.003863179755309,0.98195668637754319,1.000292422123997,null,6.7314989540624497,0,1.0027012184490178E-2,0.19052445607787438,0.12065532914579535,8.389809799115025E-2,0,1.0027012184490178E-2,0.26702419130549093,5.9098514370654645,0,1.9129362364013712E-2,9.964410364702235E-2,-5.1747496845709401E-4,4.1289451434094078E-2]
[null,496,0.97636878779857661,0.98155682679587963,0.99517601309537085,0.9908320328716852,0.97330470710970896,1.0121171886546234,1.0029095749453334,null,6.7700405320429677,0,1.0936548636056625E-2,0.20244687884918439,0.12596224857861602,8.2976272222341829E-2,0,1.0936548636056625E-2,0.27869724176929966,5.9119078736678388,0,1.9287040235287208E-2,0.10680981937949419,-3.081603309294874E-3,4.503476065019138E-2]
[null,497,1.0198718166601421,0.96617405899387654,0.99351584813711713,1.0129350504115522,1.039520744589483,0.99311935173539401,0.98977367597981625,null,6.7316451707491947,0,1.0358334447162235E-2,0.19127232185938495,0.12138446232611218,8.2659357006575465E-2,0,1.0358334447162235E-2,0.26172014885227551,5.9131952679614086,0,1.9048870782841554E-2,0.10099761686639026,-1.286652444407752E-3,4.2653777538613255E-2]
[null,498,0.98595441906655457,0.98623826538557968,0.98521950839170969,1.0384715155389976,0.97670799140884568,1.0061650109380635,0.99502132465013737,null,6.7590238529969779,0,1.0838356451978129E-2,0.19768948244352597,0.12468982603716358,8.2316533070952658E-2,0,1.0838356451978129E-2,0.273177527109565,5.9150370772194742,0,1.9232755711234829E-2,0.10481893722823206,-2.5687085368849951E-3,4.4630422713713355E-2]
[null,499,0.99648849065459955,1.0292414956679545,0.98720604819041857,0.97323508803680836,1.0421003542176239,0.9682721563639558,0.96423060638976421,null,6.7165547523225992,0,1.0115489154284079E-2,0.18504888304942965,0.12124672402360571,8.2192698984887444E-2,0,1.0115489154284079E-2,0.2580998907412545,5.9114006293097354,0,1.9174304544890945E-2,9.8019338494711006E-2,-2.8150067330446634E-4,4.1653783847391788E-2]
[null,500,0.9920210745096143,1.0083408683815887,0.9885831768263601,1.0208356649807739,0.97044270158135459,1.0126790768824181,0.96095217275334832,null,6.7427469291507709,0,1.070790474850682E-2,0.19628671972381551,0.12277055051884923,8.2372229184903695E-2,0,1.070790474850682E-2,0.26258705272689326,5.9138971251033254,0,1.9198941626663218E-2,0.10390051903513038,-2.3594545871686613E-3,4.4093245818356129E-2]
[null,501,1.0155864192019664,0.99728643354263413,1.021005029742738,1.0179201311842301,0.98896595246385333,0.98033112028371205,1.0103653529510277,null,6.731847172930431,0,9.8890155642836503E-3,0.19019201451742282,0.11985152321643996,8.4435257707930589E-2,0,9.8890155642836503E-3,0.26681600199688588,5.9119083798508925,0,1.9071426397860664E-2,9.9069458503263097E-2,-2.1809517483136661E-4,4.0721205914566329E-2]
[null,502,0.99476768647432068,1.0033163668654197,1.0359714769724981,0.99072800013239304,1.0063175579215209,1.0151181915151681,1.0061584074951133,null,6.7579445307366628,0,1.0291419497038597E-2,0.20235951197310009,0.12177976747330732,8.5447672018547138E-2,0,1.0291419497038597E-2,0.27454842780328859,5.9095748845476308,0,1.9183768300943708E-2,0.10463583045845477,-1.9635655230337721E-3,4.2378233684421236E-2]
[null,503,1.013629884023614,1.0087454849731838,0.98871911691964232,0.990353472774685,1.0377411426666401,0.96304401957014008,1.0094369077901906,null,6.7197484600788719,0,9.963092909201738E-3,0.18267038143411432,0.12013152711657382,8.2393431230479236E-2,0,9.963092909201738E-3,0.26530977908310704,5.9122419346160644,0,1.9081787773317642E-2,9.6686419752523803E-2,2.0695583702756991E-4,4.1026243235663146E-2]
[null,504,1.0100858441809804,1.0420284257479022,0.98942482842919888,1.0181866658786443,1.0029362727954056,0.97337374567910695,1.0197253611189685,null,6.7246563036650162,0,9.9597545968149546E-3,0.18280034674982271,0.11898498814667946,8.2515363255455984E-2,0,9.9597545968149546E-3,0.2696633628930139,5.9137071423444567,0,1.9100658427062135E-2,9.672115311151061E-2,1.5079207756146174E-4,4.1012496659451829E-2]
[null,505,0.99057832657915978,1.0016588039852916,1.0221013851826075,0.96237342751386812,1.0060096082890573,0.99202455308378035,0.99521858564100751,null,6.7461818226320851,0,1.0230575629347344E-2,0.19708045586991063,0.12264151834277974,8.4514536023776093E-2,0,1.0230575629347344E-2,0.27051924353513096,5.9088446004150725,0,1.9206945621153607E-2,0.1026022001551891,-1.3553667980003286E-3,4.212768946707339E-2]
[null,506,1.031469198886533,1.0113683945810681,0.9796897338927284,0.96723181404524272,1.0133886013140281,0.96845609018817802,0.98863214420377665,null,6.7019411541045786,0,9.9126082599285542E-3,0.17932696367594811,0.11809333249390941,8.1688758256675056E-2,0,9.9126082599285542E-3,0.25579906424902793,5.9114913872598338,0,1.8988769442504942E-2,9.5346127133767514E-2,3.8839515701987495E-4,4.081835643588877E-2]
[null,507,1.0179431437609481,0.97014517467483363,0.98766800783649278,0.98035058902402139,0.9993312965208585,0.99853620837819312,0.98739748992770937,null,6.731361415800821,0,1.0469519446803001E-2,0.19165662165210273,0.12152354810278966,8.2277190185020346E-2,0,1.0469519446803001E-2,0.26203635128001118,5.911759617574492,0,1.905899859194566E-2,0.10149601171345009,-1.558540875937675E-3,4.3111617576941749E-2]
[null,508,1.0183364988053267,1.040527044915339,1.0339648329134072,0.98424705915711852,1.012764288156335,0.99930460301734236,1.0019270920880614,null,6.7265113345757612,0,9.7607350256448278E-3,0.19135645976093707,0.11727788450943527,8.5189526435501442E-2,0,9.7607350256448278E-3,0.26526079692688354,5.9093414349759259,0,1.9056929899476313E-2,9.9043640940565239E-2,-2.0830836249783043E-4,4.0192969489536358E-2]
[null,509,0.97982099236465459,0.96462080904607672,0.99662823363390241,1.0012355411303921,1.0356619503176707,1.0061789353083725,0.98703869464298144,null,6.7647241909031797,0,1.0901395253247311E-2,0.20223090455642243,0.126367225082857,8.2997019048518084E-2,0,1.0901395253247311E-2,0.27294746940443243,5.9123888656221126,0,1.9267367627378577E-2,0.10661882006405755,-2.9834857794548198E-3,4.4890005276851504E-2]
[null,510,0.9943123679865834,0.99946900436789321,1.0055509013589286,0.99436343552935236,1.0108261266172935,1.0049215007389514,1.0016158518289529,null,6.7511041120698829,0,1.0485068640493037E-2,0.19709567329210012,0.12260199844335232,8.3538450270735684E-2,0,1.0485068640493037E-2,0.27245337679026449,5.9115155148391745,0,1.9186277856501739E-2,0.10345221772042293,-1.9150435315770631E-3,4.3175646388904011E-2]
[null,511,0.98211826873927588,1.0120583540636634,0.98643159351049314,1.0172541652194174,0.99072074602614202,0.97702449222289334,1.0092660771965318,null,6.7480439724282357,0,1.0438212125101239E-2,0.19073347752358991,0.12386666451492057,8.2402499836672125E-2,0,1.0438212125101239E-2,0.27509148806032047,5.9138229874749673,0,1.9254353089317347E-2,0.10106951157978475,-1.1797092500048837E-3,4.2982699598669412E-2]
[null,512,0.96165924893092525,1.0161183604358537,0.98463799811818331,0.97866186354850893,0.97415029772600292,0.98545070258320533,1.0104950347764878,null,6.7639850302226323,0,1.0750612131213436E-2,0.19591999739314195,0.12633395189558969,8.2357229565500373E-2,0,1.0750612131213436E-2,0.28207507894415856,5.9118362259842829,0,1.9372446553194391E-2,0.10391091092925397,-2.0899182612088654E-3,4.4269107218711225E-2]
[null,513,1.014593498128576,0.96915005599629511,0.97555456688533759,0.95463816479176866,1.0210775250920265,0.97738957528768899,1.0107470898577497,null,6.7293388283433782,0,1.0395361599268847E-2,0.18690988556800198,0.12219934013226172,8.1572558950561633E-2,0,1.0395361599268847E-2,0.26709638503935318,5.9110376320941853,0,1.9076679693104105E-2,9.9584058830490388E-2,-9.4396072497800003E-4,4.2806248760400907E-2]
[null,514,0.98585961798390764,0.99432960679191529,0.99229942102426849,0.99521170547258786,1.0138079281079588,0.99509256645549182,1.0136449552334958,null,6.7564958220893896,0,1.0616865093061307E-2,0.1956930669806668,0.12416076991126405,8.2779288345388224E-2,0,1.0616865093061307E-2,0.27716569633082888,5.9123052297038248,0,1.923328741216793E-2,0.10339452994931805,-1.9544072657525511E-3,4.3718360721686118E-2]
[null,515,0.98258695249004557,1.0318244431257522,0.98811605123413093,0.99554859707775278,0.97074291412732927,1.0042459318054799,0.98191591920655896,null,6.7462064525169758,0,1.0619897816241562E-2,0.19453867258472185,0.12282185748559436,8.2422576501634329E-2,0,1.0619897816241562E-2,0.26987737264923228,5.9125562437035022,0,1.9251705374808498E-2,0.10299923068491808,-1.992055403375677E-3,4.3730848935937788E-2]
[null,516,1.0205715960578914,0.96186910383056357,1.0064581586211472,0.99231994263601253,0.95932923334477826,0.99341367727401786,1.0155422185351113,null,6.7390835356671541,0,1.0257522174202168E-2,0.19307753530586,0.1212767371089911,8.3537431017213171E-2,0,1.0257522174202168E-2,0.26844766100604672,5.9113538054446213,0,1.9045205579063765E-2,0.10129762384864106,-1.1911141857613365E-3,4.2238650542479363E-2]
[null,517,0.97584593525894103,0.97171297214079089,0.99364426963173336,0.96364059817384917,1.0026373688606423,1.0336914348996891,0.97481581653128224,null,6.7716707187104612,0,1.1239071139212299E-2,0.20757511455431871,0.12656856224374541,8.2788154838488393E-2,0,1.1239071139212299E-2,0.27320160229516183,5.9105238221855965,0,1.9290031880704342E-2,0.10959897976027999,-4.1560435190305962E-3,4.6280494471188198E-2]
[null,518,0.9795985910424978,0.99472379291122548,1.0231067236099038,0.99970893889567247,0.97658218138245245,0.99922413545755417,0.96813150704180739,null,6.7530179777148502,0,1.0442183996640592E-2,0.20145617419760931,0.12434178061895439,8.455495265111275E-2,0,1.0442183996640592E-2,0.26684695110353102,5.9108038551241293,0,1.926863081689913E-2,0.10482837499763503,-2.0817968537208496E-3,4.2999055058701698E-2]
[null,519,0.99796416182256498,1.0071077727930688,1.0344663487969759,0.98519761504257253,0.97301221460144516,1.0149647404451685,1.0369657557569147,null,6.7629189043582354,0,1.0253876281619763E-2,0.20117339113501523,0.12123535399442578,8.5452636229563367E-2,0,1.0253876281619763E-2,0.28198967656159452,5.9093636567851986,0,1.9166214919696611E-2,0.10409918694427064,-1.7848496173034788E-3,4.2223637405769718E-2]
[null,520,0.98349943537332674,1.0214479573363848,1.0097290808621742,0.9803197846213908,0.99025492290694439,0.98294999205051259,1.0061282210380205,null,6.7468426550485852,0,1.0235007064497984E-2,0.19358900001369703,0.12279689881029927,8.3814172644734397E-2,0,1.0235007064497984E-2,0.27437631936008922,5.9105201159519547,0,1.9246557764526918E-2,0.10140165126531846,-1.04799809029487E-3,4.2145937328257679E-2]
[null,521,1.0141338022860593,0.99701818116295005,1.0209784687283321,0.98972616438525107,0.98870281086608403,1.0080640029281995,0.99529162401384452,null,6.7381701960161413,0,1.0184744784500809E-2,0.19587197660166752,0.12003660756467271,8.4398965132766277E-2,0,1.0184744784500809E-2,0.26578355677790005,5.9103867310756772,0,1.9079115311713437E-2,0.10202943849016195,-1.3551611439978767E-3,4.1938966205581636E-2]
[null,522,0.99414496218627513,1.002763111188834,0.99872107126280896,1.0189142702378469,1.0173185375138549,0.98477162378991123,0.98009284618746573,null,6.7373764190092116,0,1.0323512323746953E-2,0.19210544777826491,0.12259008681788143,8.302876014940426E-2,0,1.0323512323746953E-2,0.26472872438651879,5.9132269430521323,0,1.9187201116426394E-2,0.10117523107660847,-1.1763616005244777E-3,4.2510386232496047E-2]
[null,523,1.0062024299704595,1.0018296933595658,0.99101666531973143,1.0212436207847273,0.96944795848884213,1.006519682395254,0.9643182268508671,null,6.7327560477459212,0,1.0499608249162722E-2,0.1931640942173207,0.12130922484297461,8.2479000487640106E-2,0,1.0499608249162722E-2,0.25930551080538777,5.9137837538312832,0,1.9121488755129767E-2,0.10212360605936262,-1.7661491626295403E-3,4.3235517909451904E-2]
[null,524,1.0139169000883517,1.0063760520066252,0.99846057532059551,1.0236617535686574,1.003215127266722,1.0003129155957224,0.98863444536985545,null,6.7315734711811626,0,1.0268455068502463E-2,0.19100717748028748,0.12003151624915975,8.2994404504175667E-2,0,1.0268455068502463E-2,0.26322014019101853,5.9134981396003754,0,1.9080265297235909E-2,0.10060983311895287,-1.151675515271467E-3,4.228367025522535E-2]
[null,525,0.99033036084505532,0.99837305085650774,1.0288507511026577,0.99460577957555241,1.0055139375496245,0.97934826243928397,0.99105050667556616,null,6.7431238946781686,0,1.0056968017409114E-2,0.19567931277863612,0.12270422039475166,8.4925227119737767E-2,0,1.0056968017409114E-2,0.2683003535510835,5.9101971643330717,0,1.9208323619817724E-2,0.10153537071848184,-8.3888205952959403E-4,4.1412804222114755E-2]
[null,526,1.0130905712933793,0.9776952522197343,1.0213695372806502,0.99618182492379426,1.0066208649682682,1.0095821220581271,0.96145378624690259,null,6.7344210931328883,0,1.0293053804640668E-2,0.19806950554569527,0.12109719713952943,8.4313118351445143E-2,0,1.0293053804640668E-2,0.25734805842159586,5.9107130633737839,0,1.908465088990648E-2,0.10315426445011298,-1.7437285114153781E-3,4.2384963472230669E-2]
[null,527,1.0358304755708512,1.0261072968063363,1.0077621970482107,0.99704144656000426,0.95432555260857099,1.0104855742908434,0.99664395331705069,null,6.7185916738309714,0,9.9878808543085364E-3,0.18836543396055097,0.11641640078852658,8.3513375534987444E-2,0,9.9878808543085364E-3,0.26048769450852238,5.9115351455894105,0,1.8966516126638987E-2,9.8761636176039058E-2,-5.8284443522854071E-4,4.1128315581523189E-2]
[null,528,0.98707645469009886,0.99321507974322709,0.99420245161855569,0.97420992995016298,1.0058769464817774,1.0052119672054289,0.99688679379074918,null,6.7542462440123643,0,1.0698970034212062E-2,0.19776349693667669,0.1240272426538068,8.2829967632216589E-2,0,1.0698970034212062E-2,0.27322817233063196,5.9110639063623509,0,1.9226470425062075E-2,0.10438946384460664,-2.3389304281977723E-3,4.4056454255210181E-2]
[null,529,1.0126122070347479,1.0307830262473598,1.0105653976386006,1.0235493163382643,1.013016654113664,1.0026869226736574,1.0210479819167673,null,6.7387766151202264,0,1.0093568823745451E-2,0.19115028935903336,0.11881787813797409,8.3866186973308235E-2,0,1.0093568823745451E-2,0.27221378317513634,5.9128085093827405,0,1.9087192994015199E-2,0.10008285265503966,-8.135973849285092E-4,4.1563519827907104E-2]
[null,530,0.96468408136168138,1.0116807153432941,1.007263164991228,0.99058898160584208,1.029937574455337,1.028870926451811,1.0183332535977463,null,6.7853286129480583,0,1.099079677332915E-2,0.20712672424595291,0.12572189483001436,8.3850330930742095E-2,0,1.099079677332915E-2,0.28775384811738502,5.9112147288364625,0,1.9354671085487347E-2,0.10862517936734112,-3.5769092889981033E-3,4.5258144823671138E-2]
[null,531,1.0481597854964595,0.9887652293024054,1.0146581598779014,1.0031886499183646,1.0019542362343143,0.98415305009721643,0.98641946648439871,null,6.7055756688958761,0,9.7082623096479814E-3,0.18497052773314837,0.11664116760880862,8.3839629760337819E-2,0,9.7082623096479814E-3,0.25280358781474993,5.9114754716048017,0,1.8904607861618534E-2,9.6651597971542103E-2,3.1218235600720759E-4,3.9976896184856614E-2]
[null,532,1.0195425941188914,1.0033582581919991,1.0067247708852602,1.0162258892260823,1.0270186806127894,1.0077814489035684,0.97827727507034634,null,6.7287047625525354,0,1.0227156911506973E-2,0.19258198351004024,0.11936079803325915,8.345417632611446E-2,0,1.0227156911506973E-2,0.25974212539650499,5.9126305304653455,0,1.9050596877620875E-2,0.10102429249612777,-1.2533523479937669E-3,4.2113611795515836E-2]
[null,533,0.99079256050620168,0.95263269932117622,1.0227527318017617,1.0180314966400923,0.97267094996179349,0.9971562493898759,1.0211986779640496,null,6.7682370377431909,0,1.0498867165078489E-2,0.20244372031069663,0.12508846818516756,8.4705377559290057E-2,0,1.0498867165078489E-2,0.27856507563607491,5.911814040976644,0,1.920575563274457E-2,0.10536059641051683,-2.1784632250412658E-3,4.3232466257101095E-2]
[null,534,1.0066115733961665,1.0167987041997693,0.96612013799747309,0.9597183725888353,1.0206373044334329,0.99294628758952985,1.0319440153036012,null,6.7372246553433728,0,1.0513935613443364E-2,0.18641237447436981,0.12099825655337004,8.1103404861743597E-2,0,1.0513935613443364E-2,0.27587899982979441,5.9118267535173477,0,1.9119286567407655E-2,9.9791042642144931E-2,-1.1999785481937183E-3,4.3294515445383819E-2]
[null,535,1.0061047144613944,0.99154237436090065,0.9711727178273224,1.0120039339122249,0.99027337400012594,1.0428271987940045,1.0130709333807393,null,6.7601684883135826,0,1.1118301851922341E-2,0.19861236346155783,0.12219037842249353,8.1457112675969848E-2,0,1.1118301851922341E-2,0.27597313412689922,5.9143788045290346,0,1.9122014967428189E-2,0.10605210116256329,-3.4006090746231147E-3,4.5783188042259955E-2]
[null,536,1.0038397037702997,0.99919571743218361,0.98653595936281335,0.9790089903082182,0.95549299692807865,0.99956721549926864,1.0281615401865074,null,6.746935139196566,0,1.0504402283565329E-2,0.19197265460536236,0.12180607796148075,8.2398338730953966E-2,0,1.0504402283565329E-2,0.27647206675531971,5.9117498858564757,0,1.9134241089969226E-2,0.10172084879184821,-1.574233484664839E-3,4.3255258889815532E-2]
[null,537,0.98181397077363242,0.97717455419750054,0.99041934817403054,1.019618567155097,1.0240926849592173,1.0293376434987647,1.0276276231048207,null,6.781991644475549,0,1.1128284409360992E-2,0.20454880434405245,0.12557937097484637,8.2794156135291952E-2,0,1.1128284409360992E-2,0.28574140993610037,5.9137291892301249,0,1.9256073499850004E-2,0.10817477662887842,-3.6564307105610826E-3,4.5824294436963328E-2]
[null,538,1.0233141802718719,1.0078083762692471,1.0006872281986359,0.99231832885175975,0.98274091113720752,1.0039745520334704,1.005600412540427,null,6.7293483236181562,0,1.0185353322331151E-2,0.19008740891945758,0.11882096556471046,8.3141185862036143E-2,0,1.0185353322331151E-2,0.26560666767493385,5.9116791462522773,0,1.9030889188312403E-2,0.10001468063081018,-9.7409253043955E-4,4.1941472056051296E-2]
[null,539,0.99255473963626217,1.0087347380935936,0.98296057898588862,1.0377194267251912,1.0109642861592751,1.0395810202313773,0.98274395952041393,null,6.7593896446198922,0,1.1038615849975836E-2,0.20066870408788451,0.12279042823710609,8.2144470147679616E-2,0,1.1038615849975836E-2,0.27088512257915998,5.9151214410582842,0,1.9195986885115521E-2,0.10651879130522346,-3.3903549503859752E-3,4.5455055269823852E-2]
[null,540,1.0334702915529037,1.0051028049636446,0.97238401037217481,0.98456077994384794,1.0317096040475968,0.98857319268040078,1.0228108930014759,null,6.7187644757535638,0,1.0190491207485752E-2,0.18236601780974901,0.11828867220750092,8.1381155167289276E-2,0,1.0190491207485752E-2,0.26604260643497435,5.9128288802492026,0,1.8978535594069958E-2,9.7317876421042393E-2,-4.0189708287151137E-4,4.196262895260848E-2]
[null,541,1.0221464484300138,1.0183351814862018,0.97737662326411356,0.99305381285527605,0.99197039399880116,0.9831118179084215,1.0093414389026785,null,6.7191838916053337,0,1.0145029125392842E-2,0.18290278820124695,0.11888530526415328,8.1682979072509057E-2,0,1.0145029125392842E-2,0.26483233615977519,5.9130145335855158,0,1.9036975399913329E-2,9.7360117285185482E-2,-3.0656755346358724E-4,4.1775424190498824E-2]
[null,542,1.0020414497297503,1.0160195882994647,1.0236662946584327,0.99957020833742771,0.96341345701563241,0.99884289602770948,1.0040250055815803,null,6.7426016236787136,0,1.0107312822565419E-2,0.19515709869026007,0.1205207509632213,8.4634816361869022E-2,0,1.0107312822565419E-2,0.27029849325296407,5.91076419179024,0,1.9143987103956133E-2,0.1015226816010356,-1.0605112535399977E-3,4.1620115168707138E-2]
[null,543,1.0088896552357134,0.98606950361068879,0.98754041634246459,1.006348320132666,1.0301289751188822,0.97931182468169087,0.96457778249120429,null,6.7222181289487724,0,1.0289186307991267E-2,0.18831978254993983,0.12182051064237516,8.2213329128746293E-2,0,1.0289186307991267E-2,0.25637024702756583,5.9131719627165777,0,1.9107057600363037E-2,9.9735266354175942E-2,-8.8906488038920247E-4,4.2369037809417184E-2]
[null,544,1.0321658584367701,0.97204499380914833,1.0106064039331537,0.97610379559174409,0.99974511354593465,1.0332473219615645,1.0270060985738088,null,6.7473118449092215,0,1.0463459138377987E-2,0.19816723809028805,0.11933424124071139,8.3831325294365655E-2,0,1.0463459138377987E-2,0.27210624029455321,5.910242526797961,0,1.8985202132247202E-2,0.10375469689419618,-2.1962881406456317E-3,4.3086662305542235E-2]
[null,545,0.97478640037976594,0.99734109991791275,1.0086661649653728,0.99502903823618694,0.98733434025668998,1.0077407012185629,1.0089599264492253,null,6.7694663428535469,0,1.0705698335919538E-2,0.20217344794059647,0.12510434594604719,8.383885179276962E-2,0,1.0705698335919538E-2,0.2802521790410557,5.9113751931599738,0,1.9296104143796802E-2,0.10595387976830117,-2.6118191430480079E-3,4.4084160204048511E-2]
[null,546,1.013792866673747,0.99311628766908344,1.0359732852141645,1.0070776578247669,1.0395714923956161,0.98157845326480764,1.0003382660636058,null,6.7323711415078673,0,9.8074554507400144E-3,0.19284387365053532,0.11998378956113216,8.5324566632223972E-2,0,9.8074554507400144E-3,0.26481578142574796,5.9104578574078692,0,1.9080923126436763E-2,9.9715406579511945E-2,-2.3641275974293938E-4,4.0385355884152672E-2]
[null,547,0.96876389365851867,0.96955935799442439,1.0167221840376892,0.98846483140795405,1.0205819549236843,0.9845746384056312,0.98200282935101413,null,6.7628389458506435,0,1.0578018507268912E-2,0.20215840665317689,0.12715394911491704,8.4229861752634624E-2,0,1.0578018507268912E-2,0.27253956130289103,5.9105621753335127,0,1.9330871841167135E-2,0.10552514886362993,-2.2194264071112978E-3,4.3558397395827543E-2]
[null,548,1.0110671963611373,0.97620125707593663,0.96683225554164109,1.0254650277152251,1.0025716224017633,0.98611066561494642,1.0250262444822633,null,6.7408523837723076,0,1.0572028799563583E-2,0.18764071508020161,0.12243138977570997,8.1150703331772475E-2,0,1.0572028799563583E-2,0.27256910446099503,5.9153430961230153,0,1.9095419858554875E-2,0.1004125944813366,-1.3243721849084721E-3,4.3533732845625221E-2]
[null,549,0.97662193167229905,1.0164062031385916,1.0246488669183811,1.0389958511012278,1.026765895684977,0.99166382481284576,1.0008354471054424,null,6.7594403308770019,0,1.0285318246841112E-2,0.19888289669489434,0.12361990314548436,8.4801109987605428E-2,0,1.0285318246841112E-2,0.27576200289086944,5.9128375022562354,0,1.9285592953482641E-2,0.10341090019021744,-1.5126870638757319E-3,4.2353109822090063E-2]
[null,550,1.0342448644422735,1.0195699864083536,0.97376699512064357,1.0136384839373824,1.0190095336460803,1.0126658366975432,0.98634450159909248,null,6.7168204681158592,0,1.0354921152354778E-2,0.18568942955682829,0.11750178781192624,8.1387381949089024E-2,0,1.0354921152354778E-2,0.25838943826963368,5.9143253524663981,0,1.8974584958556528E-2,9.9022594356312388E-2,-1.1098234510249561E-3,4.2639722198139968E-2]
[null,551,1.0099854465860747,0.98823864265516637,1.0179167298654959,1.0016498623027545,0.980178092435948,0.97396403894762373,1.0211298278532142,null,6.7366334000691701,0,9.9447726877864573E-3,0.1903925406538744,0.12101442343624089,8.4284397388972629E-2,0,9.9447726877864573E-3,0.27062547069698217,5.9112062644659131,0,1.9101194934749963E-2,9.9324929869924986E-2,-2.6662520224530383E-4,4.0950803824752871E-2]
[null,552,1.0241841345353662,1.0002201307029912,1.0101676528754466,1.0042548081475631,1.0323659452767731,0.99382986507241655,0.99652094151871262,null,6.7252959650676631,0,1.0023126606983125E-2,0.18970453583998637,0.11890559516492473,8.3690697429659427E-2,0,1.0023126606983125E-2,0.26214441624799739,5.9117885392554976,0,1.9026364012828183E-2,9.9345421317654947E-2,-5.8305551841339497E-4,4.1273451317527035E-2]
[null,553,1.002782665706506,0.99730709854571264,1.0215421954953805,0.9990458982406959,0.99181745189911574,1.0160557022696397,1.0053886333408482,null,6.7526201350856558,0,1.0375277916718934E-2,0.19970274068554369,0.12137065772333956,8.4529855875239979E-2,0,1.0375277916718934E-2,0.27227319752441498,5.9108578858588743,0,1.9139965694376038E-2,0.10399601054854826,-1.9737265551018962E-3,4.2723547730422598E-2]
[null,554,1.0138423641874905,0.98677283569946028,0.97733856027554034,0.97265870186528725,1.0465637654237012,1.0031458114981224,1.0050912160778436,null,6.7362183471366777,0,1.0578585846243183E-2,0.19070852698138679,0.12137878926567783,8.1709041172373986E-2,0,1.0578585846243183E-2,0.26804890873572185,5.9119140210970409,0,1.9080660589895021E-2,0.10151708997881455,-1.6994242809737063E-3,4.3560733596741008E-2]
[null,555,1.0181582295283009,1.0027437317763663,1.0325612753616473,1.0034424459716145,1.0326039624097014,1.033374114824904,1.0059575316383433,null,6.7488959427133191,0,1.0268981797299287E-2,0.2009033415239439,0.11907295542207416,8.5180649392350871E-2,0,1.0268981797299287E-2,0.26988630553563547,5.9104596980323727,0,1.9057867236903506E-2,0.10405651389745223,-2.0072275580722437E-3,4.2285839230656444E-2]
[null,556,0.99994425854653601,1.0123994007181902,0.99410243029714562,1.0263566552411936,0.99900580472723677,0.9890559344035631,1.0299309712075937,null,6.7468231154722709,0,1.0307652548863738E-2,0.19050200507273748,0.12149972765456385,8.2909209654504962E-2,0,1.0307652548863738E-2,0.27689195189455373,5.9138879053164839,0,1.9155397549075266E-2,0.10056149240497818,-1.0296525770866207E-3,4.2445078502461667E-2]
[null,557,0.99009838176728582,1.0044155553138803,0.98957041296957737,0.99623306000517531,1.0107594936762339,1.041420763203518,0.97022137684476406,null,6.7575793972279268,0,1.1042126407946728E-2,0.20270984141729279,0.12318247337898443,8.249233587448028E-2,0,1.1042126407946728E-2,0.26832578186236944,5.9125124154243878,0,1.9209613402122488E-2,0.10724764110933849,-3.5702163637415093E-3,4.5469511122691944E-2]
[null,558,1.046906288977165,0.98134058862189721,1.0014403758185553,0.97194159520879664,0.9998687147012747,0.99154361299524729,0.99308338948556363,null,6.7094500308010074,0,9.9387607510095094E-3,0.1856923552069828,0.11737274600470482,8.3036399165812708E-2,0,9.9387607510095094E-3,0.25553078745609437,5.9105355919867408,0,1.8910835363557425E-2,9.7665697028124665E-2,-2.204291501993614E-4,4.0926047739190251E-2]
[null,559,0.99784519781287329,0.99506160829428936,1.006364674063577,0.99380898064971313,1.0306920049394148,1.0042409348100843,1.0097000375825598,null,6.7514154997025662,0,1.0453217206750529E-2,0.19673387089708511,0.12236873381079919,8.3604555730240462E-2,0,1.0453217206750529E-2,0.27366234035030346,5.9114395553275756,0,1.916686619336198E-2,0.10322069039344729,-1.8256008543423255E-3,4.3044487854096238E-2]
[null,560,1.0008832363247258,0.98236074549134411,0.98624116460433031,0.96768351308900269,0.97490013521781049,1.0417488969478335,0.98434675074127143,null,6.7563489584849643,0,1.1063102079100379E-2,0.20209477365468678,0.12300456788532604,8.2280751164753654E-2,0,1.1063102079100379E-2,0.26958298785580104,5.9111540312903541,0,1.9150282825716458E-2,0.10710003802752285,-3.5743594221743797E-3,4.5555885202972421E-2]
[null,561,0.98888612137567555,0.98899684623112616,0.99771515721359283,1.0040212335230638,1.0186904300809381,0.98933785360438176,1.0188809091581472,null,6.7554208182878801,0,1.0497680359535204E-2,0.19505552462601355,0.12394448374969828,8.3123417949608744E-2,0,1.0497680359535204E-2,0.27724833923510089,5.9124785026443494,0,1.9216363301894652E-2,0.10278030414113309,-1.6536965630346034E-3,4.3227579203117358E-2]
[null,562,0.98793201249893803,0.96253989830311526,1.0296622849509627,1.0098397078962218,0.97044969461150454,1.0405488005082368,0.97702331188219194,null,6.7738916562906342,0,1.0872785766489788E-2,0.21180669691233597,0.12479783357865273,8.5027861375169031E-2,0,1.0872785766489788E-2,0.27129787614514594,5.910973150929788,0,1.9221687456243121E-2,0.10985989380831981,-3.8655404177063979E-3,4.4772196502682833E-2]
[null,563,0.99499744208687613,1.0207944663182813,1.0387300062125959,1.0061507312079212,0.98752712550291155,1.0365470037613929,0.97112020172977753,null,6.7542579197029671,0,1.0403644943410079E-2,0.20540159087440293,0.12086103717253292,8.5521428140536787E-2,0,1.0403644943410079E-2,0.26671221090152952,5.9102472008088567,0,1.9182502840610023E-2,0.10606562038822021,-2.574029520915917E-3,4.2840358097194199E-2]
[null,564,0.99024929977701204,0.99320656014709352,1.0054956332396157,1.0094501401368754,1.023252987491825,0.98311030872971505,1.0108381879995747,null,6.7498748294354245,0,1.0327852493855089E-2,0.19412447504905647,0.12341599498193417,8.3567772577797392E-2,0,1.0327852493855089E-2,0.27405120111887465,5.9123338926598752,0,1.9208774243202206E-2,0.10189547601419925,-1.2510154900022543E-3,4.2528258280479868E-2]
[null,565,0.99067867249061425,1.0150248470647847,0.99979713006505155,1.0113972648932621,0.98285441330188461,1.0149929605990768,0.95807499713918409,null,6.7430414190473718,0,1.0612156393752041E-2,0.19779176930862391,0.12240218336276694,8.3058067879140343E-2,0,1.0612156393752041E-2,0.26231866884156063,5.9127602556064005,0,1.9206388173504896E-2,0.10411434688457315,-2.3092321452441522E-3,4.3698971136047787E-2]
[null,566,0.98218621841122977,0.95467764418008527,0.97412238779062865,0.99935444125299822,0.97179651536636724,1.0385365530446125,0.98891942356459017,null,6.7765913298386407,0,1.1498380038054335E-2,0.20630328620596095,0.12702079483174544,8.1634627445531543E-2,0,1.1498380038054335E-2,0.27602095640794078,5.913533628383699,0,1.9253969067605032E-2,0.10999572097702283,-4.5199358422218037E-3,4.7348282361356325E-2]
[null,567,1.0016377867895443,0.97720355078648258,1.0013428460601832,0.99871036256136436,1.0228414073016152,0.99169838440260438,0.97814682849064793,null,6.7383412119682848,0,1.0409277929801879E-2,0.19445523913005613,0.12288667057066467,8.3154656991926992E-2,0,1.0409277929801879E-2,0.26311876370198073,5.9119877036433692,0,1.9146179649047076E-2,0.10227952484611341,-1.5510802973964543E-3,4.2863553732521445E-2]
[null,568,1.0212400840315703,0.98098536269424141,0.95590484278977161,0.98694478019623166,1.0111968789282255,0.99009793805943458,1.0157097202818828,null,6.7288704180423924,0,1.0587194937027533E-2,0.18488376873266563,0.12117322101055884,8.0377139315865487E-2,0,1.0587194937027533E-2,0.26771082131646878,5.9138505323273547,0,1.9041708960090945E-2,9.9484242115788088E-2,-1.247200036633106E-3,4.3596184300229927E-2]
[null,569,1.0317133941712822,1.011364129266473,0.98291833716016974,0.98322078001699686,0.99928056229528806,0.99992211084659843,1.0183376689260091,null,6.7228044377800877,0,1.0203514502235354E-2,0.18547594796745992,0.11800773428750964,8.204008959900401E-2,0,1.0203514502235354E-2,0.26634142095304564,5.9121777245350735,0,1.8987518469373108E-2,9.8456265303007426E-2,-6.98519896709148E-4,4.2016256562327298E-2]
[null,570,1.019461890028079,1.0199859176733577,0.9989216334265768,1.0333425706675206,0.96236158851599629,0.99215502738626649,0.99740366886716592,null,6.7250748192586238,0,1.0067177487147361E-2,0.18739110776259651,0.11873051947918252,8.3029853360690825E-2,0,1.0067177487147361E-2,0.26323815307071174,5.9139954389115399,0,1.9051020174650064E-2,9.868251822328615E-2,-4.9863672531266171E-4,4.1454845001278967E-2]
[null,571,0.99739893902743371,1.0333075066641364,1.0009820911279648,1.0066424389964792,1.00771296498895,0.99296458783724384,0.99677403125994501,null,6.7367729999308095,0,1.0222826342688196E-2,0.19087011631778794,0.1206904290018794,8.3215226137018261E-2,0,1.0222826342688196E-2,0.26885332750657936,5.9124366647802074,0,1.9169310641044025E-2,0.10041180265688861,-9.696563945267516E-4,4.2095779283932641E-2]
[null,572,0.95957139378423373,0.97502906205245721,0.98766650600472894,1.0205645087844961,1.0053184548001652,0.95898609869898888,0.97949865420509163,null,6.7564778844354274,0,1.0643561293005505E-2,0.19484222435592322,0.12865730067043873,8.2440496144741068E-2,0,1.0643561293005505E-2,0.27185093846326946,5.9139333943066861,0,1.9384781233564314E-2,0.10318309557730054,-1.6426372378071641E-3,4.3828290921309854E-2]
[null,573,0.99578805558009331,1.0129028583122468,1.0114481489861358,1.001919179918112,0.96693781283271818,1.0000984894374532,0.99165835798555146,null,6.7437583952935869,0,1.0306600612992841E-2,0.19543986644603398,0.12165739742789217,8.3859863425360032E-2,0,1.0306600612992841E-2,0.26877131906248264,5.9115896048918906,0,1.9178152719119258E-2,0.10228414768423864,-1.4627031812163623E-3,4.2440746817782919E-2]
[null,574,0.98373532015728016,1.0191024607750154,0.99582038574061982,0.99326947833536994,0.98077117626475474,1.0028578436635738,1.0170213763939833,null,6.7575846642798441,0,1.0577854581755631E-2,0.19599415342207904,0.1231436978583855,8.3024290878133192E-2,0,1.0577854581755631E-2,0.27920118348828288,5.912003561511086,0,1.9245228615772852E-2,0.10337225110128966,-1.9574249749277121E-3,4.3557722379741495E-2]
[null,575,0.99017759240817105,1.0156657379433447,0.98615820399129617,1.0220598414839324,0.95795589855291874,0.96161263397391039,0.95587299611857623,null,6.7210637580674266,0,1.0176854754562823E-2,0.18588241559686933,0.12268885658689814,8.2148391810083876E-2,0,1.0176854754562823E-2,0.25699431238969073,5.9140979156050459,0,1.9209172930308046E-2,9.8512387559378148E-2,-3.7617087751485738E-4,4.1906476466669978E-2]
[null,576,0.96461300042762532,1.0083329170710591,1.0025344157132914,1.0074909430850176,1.0027710878985725,0.9933744569476245,0.99937498678475145,null,6.7665423193661303,0,1.0671478272630763E-2,0.1997055680030087,0.12598974602843768,8.3450769530687863E-2,0,1.0671478272630763E-2,0.27899204499015678,5.9123951184314656,0,1.9355087514466438E-2,0.10497899871117228,-2.2682619176401055E-3,4.3943248074369542E-2]
[null,577,1.0109742393950756,0.99844751120042974,1.00514591060813,0.99060606870239032,1.0092964133536901,1.0097920281082917,1.0000103224958603,null,6.7406907586566511,0,1.0370454376914529E-2,0.19482430263401304,0.12063825587661811,8.3449447030667548E-2,0,1.0370454376914529E-2,0.26799766933906227,5.9113353515251488,0,1.9095915637263709E-2,0.10228053824223728,-1.6344068804244509E-3,4.270368525206613E-2]
[null,578,1.0233519402239455,0.98572370723892577,0.98404490344176954,1.0021305271163636,0.99774447240277997,0.99347349451255229,0.98579540817007938,null,6.7231471608595745,0,1.0323437452922435E-2,0.18796970682743608,0.12017969493012362,8.2034990423022272E-2,0,1.0323437452922435E-2,0.25959805659648294,5.9131376592237261,0,1.9030692615493394E-2,9.9723839902095601E-2,-1.0375575865760316E-3,4.251007792776719E-2]
[null,579,1.009931442770982,0.96768677175212081,0.97750011220872612,1.0038651026293357,1.029110417782692,0.99909196628827412,0.991718106344888,null,6.7391760272932126,0,1.0664064197250843E-2,0.19229560764932976,0.12280150126661069,8.1705791722627139E-2,0,1.0664064197250843E-2,0.26533271245708046,5.9135922299713153,0,1.9101483566081667E-2,0.10235362896718801,-1.9196465386324634E-3,4.3912718231611234E-2]
[null,580,0.97858961541085054,1.0012929596616553,0.98752588607625336,1.0050340500263701,1.0102236298658047,0.99835733254648817,0.99680555682861094,null,6.7572201481280363,0,1.0743457477563698E-2,0.19662993005384968,0.12482540567767919,8.2458568570575597E-2,0,1.0743457477563698E-2,0.27482088579024216,5.9131017285507674,0,1.9274368782810841E-2,0.10413712474483673,-2.2675096711845142E-3,4.4239645628462498E-2]
[null,581,0.98396757960373549,0.99500691768000182,1.0118996514380076,0.99528182042203117,0.99155481973355464,1.0299421018894777,1.028427333144045,null,6.7778646924191364,0,1.0819707137754138E-2,0.20530686006669668,0.12399123384702071,8.410621464777851E-2,0,1.0819707137754138E-2,0.28521771868554435,5.911205305165681,0,1.9243920517495423E-2,0.10742409788260324,-3.1842865508736793E-3,4.4553628157193138E-2]
[null,582,1.0175815520069145,1.0283141198116756,1.0125996551617154,1.0026045582211467,1.019201914253745,0.95792471405121682,1.0175115083835631,null,6.7165082830464939,0,9.5886520563928691E-3,0.18213587167788745,0.11831385221851838,8.3889968216055308E-2,0,9.5886520563928691E-3,0.26580264544799692,5.9115611554690508,0,1.9060901649016106E-2,9.5267225203617328E-2,9.923007125665895E-4,3.9484362451783495E-2]
[null,583,0.95734074381826562,0.96296076458593893,1.0051318365414077,0.96244936643861723,1.0117471312618365,1.0068473641867,1.0269420414404145,null,6.7927148423194028,0,1.1090346117828725E-2,0.20834418980096883,0.1292546586813727,8.3738292388519223E-2,0,1.1090346117828725E-2,0.2907557074524002,5.9098146061344998,0,1.9398018967009809E-2,0.1093790878191455,-3.6377902297148349E-3,4.5668071305197608E-2]
[null,584,1.0397810022149152,0.97018656372541145,0.98886183158617036,0.9747430585594743,0.99657101144099602,0.99323565490831822,1.0065125004220976,null,6.7194599547113372,0,1.0184426836782041E-2,0.18676799080004303,0.11894758250709744,8.2332198043404553E-2,0,1.0184426836782041E-2,0.26101077155774727,5.9113902267191332,0,1.8946519788430486E-2,9.8848223188196568E-2,-7.2121484618136757E-4,4.1937656953468343E-2]
[null,585,1.0039598037001431,1.0339853073640366,0.9996503229652185,0.97849399817528637,0.9840108564746527,1.012064567626493,0.99965843739915361,null,6.7386076389906577,0,1.03605178718627E-2,0.19305967930342327,0.11989480468322097,8.3122114182190426E-2,0,1.03605178718627E-2,0.26962852660757336,5.9109903144576155,0,1.913359142701767E-2,0.1016308626411026,-1.5150228043762622E-3,4.266276849289468E-2]
[null,586,0.98021997012862905,0.99066664022734441,1.0013051021818331,0.99251001796719274,1.0005016675563796,1.0163243716299861,0.99667525094812948,null,6.7659180967137038,0,1.0837471719340932E-2,0.20244298830810792,0.12488706173366831,8.3324724021731508E-2,0,1.0837471719340932E-2,0.276190083237563,5.9116547512001469,0,1.9265102959881826E-2,0.1064829143523478,-2.956308641932648E-3,4.4626779542189916E-2]
[null,587,1.0026072353855049,0.99172546827762875,1.0306253045816918,0.98747331553332385,1.0116720734540956,0.99438607212864849,1.0302987170809388,null,6.7521923347079893,0,1.009954357506607E-2,0.197023862845046,0.12149228599500556,8.5148442781486283E-2,0,1.009954357506607E-2,0.27703954566954825,5.9097092693420201,0,1.9140916940820731E-2,0.1021440677568167,-1.0941794131408607E-3,4.158812279037933E-2]
[null,588,0.98847124218443883,0.99924424862578576,1.0080943702187646,1.0099132054983706,1.0063385436405634,1.0215342745417255,1.0053570212854515,null,6.7642064849029957,0,1.0698602505440417E-2,0.20186847588042708,0.12328918846974336,8.3765067791322173E-2,0,1.0698602505440417E-2,0.27668720248735923,5.9122118679768834,0,1.9218677163465186E-2,0.10582399596259326,-2.7129316659418997E-3,4.4054940837146235E-2]
[null,589,0.99815862538154609,1.0054631575449648,0.99507774316393149,0.9893346494669486,0.99302032416302244,0.97366653705011175,1.0105280753799022,null,6.736017981081468,0,1.0186711147368337E-2,0.18853914741780187,0.12203403566386076,8.2861547527975005E-2,0,1.0186711147368337E-2,0.27076302278800357,5.911832440039487,0,1.9165150654742381E-2,9.9477043999391265E-2,-6.0147034766394364E-4,4.1947063337870599E-2]
[null,590,1.0063848115038094,1.0310277413379072,1.045597548872842,0.98382429641786284,1.0232460627873954,0.96746324418733487,0.98671268965664904,null,6.7208697059617313,0,9.5020635790217609E-3,0.1895138817829996,0.11888883783027093,8.5855382955682166E-2,0,9.5020635790217609E-3,0.26153072353954193,5.9086396327417745,0,1.9120506877268115E-2,9.7533972894664478E-2,6.5896082538040854E-4,3.9127806514143694E-2]
[null,591,0.98664095925583795,1.0260164444102371,0.9819409874571754,0.97483994489364834,0.97033378569114892,0.97053050013432474,1.0007379879117306,null,6.7345441302496116,0,1.0301229768018314E-2,0.18698089834266651,0.12270892804885328,8.2035093499542105E-2,0,1.0301229768018314E-2,0.2707755901616607,5.9117786255750868,0,1.9228908234274672E-2,9.9303674658156954E-2,-6.8621890478452242E-4,4.2418630634152597E-2]
[null,592,1.0058866674182989,0.99354449404569078,1.0053664810995031,0.99317197749737796,1.0026353110608337,0.99812962826256624,1.0157907414336811,null,6.7450773389463619,0,1.0322287409749244E-2,0.1939827679574842,0.12148327483242637,8.3526497811197142E-2,0,1.0322287409749244E-2,0.27254294998399353,5.9114615499315137,0,1.9123189551228402E-2,0.10182761097080337,-1.3758443469626506E-3,4.2505342254680029E-2]
[null,593,1.0418434839376691,1.0198071997275695,1.0021281989678212,1.021979504657762,0.97326565020254774,0.96951167021410378,0.97503535908075412,null,6.6955492345552647,0,9.599878241831037E-3,0.17954362919235806,0.11613077366349883,8.3039081872181356E-2,0,9.599878241831037E-3,0.24983209845465212,5.9132009771186587,0,1.8936140399364105E-2,9.4399519478131133E-2,9.3642449118341755E-4,3.9530589885231344E-2]
[null,594,1.0091806873545972,1.0035473070307408,0.99974826642652703,0.99982043581332447,1.0057235042434409,0.96853060992821893,1.0066943591196909,null,6.7266150548596659,0,9.9896673055215844E-3,0.18617619887713494,0.12070682838931873,8.3099081355861429E-2,0,9.9896673055215844E-3,0.26633232256378531,5.9121373561262809,0,1.9105499288551833E-2,9.80024793615831E-2,-8.0382972495837376E-5,4.1135671869642065E-2]
[null,595,1.0159841506204179,0.99384646248743924,1.0032646946486055,0.97808342982997976,0.98460465345174009,1.0262405262981165,1.0269556417081007,null,6.7510170315116067,0,1.0525470033502821E-2,0.1971863500824404,0.12030022203584023,8.3423824415721187E-2,0,1.0525470033502821E-2,0.27547899137144466,5.9107647761767472,0,1.906932498143606E-2,0.10361718198308655,-2.165651669247223E-3,4.3342012134138443E-2]
[null,596,1.0031081373420307,0.97166858780681897,0.99083340770408623,0.99434296012972956,0.95568963490521652,1.034350416662515,1.0017037622692926,null,6.7606952685617125,0,1.0967678228130944E-2,0.20172049256148525,0.12318388394050196,8.263293817289552E-2,0,1.0967678228130944E-2,0.27316587975510487,5.9123399682697375,0,1.9138201751097771E-2,0.1066570168526035,-3.3060595112065611E-3,4.5162946769492569E-2]
[null,597,1.0331381463059826,1.041207344592225,1.0043068592902593,1.0143590641581028,0.99487650741730294,1.0277067692582995,1.0028869561367308,null,6.7265183412490055,0,1.0151738902248809E-2,0.19047857285586217,0.11610156839324824,8.3362180279240028E-2,0,1.0151738902248809E-2,0.26421019312166893,5.9126663069937822,0,1.8980231484107688E-2,0.10004067764634636,-1.1244433825503891E-3,4.1803053857295956E-2]
[null,598,1.0219892852283241,0.9614396437593784,0.97429921239576001,0.97306107832209465,1.0044031383464593,1.0104656002841235,1.0321998390610612,null,6.7454829491179575,0,1.071770864184678E-2,0.19234700153393874,0.12172635173547593,8.1598576132219575E-2,0,1.071770864184678E-2,0.27407238483791346,5.9121024022277258,0,1.9037795595526302E-2,0.10254548010075765,-2.0806595517027051E-3,4.4133616506102133E-2]
[null,599,1.0111166205052626,1.001501559578388,1.0287898340524706,1.0083978975636561,1.0227368054043227,0.99077759519823816,1.0319336719236036,null,6.7442777908631317,0,9.9523611509462918E-3,0.19362652989495469,0.12003253271829255,8.501763537368498E-2,0,9.9523611509462918E-3,0.2746948497747369,5.9109457085050341,0,1.9095156295866351E-2,0.10047321326462461,-5.8988672941500341E-4,4.0982051765348977E-2]
[null,600,0.99269766179049179,1.0033660152909309,1.0200789011885665,0.98296622122285238,0.98519825074359091,0.9742773423850023,0.98065471149723737,null,6.7341869542571757,0,1.0036548405880179E-2,0.19276520145866438,0.12233486363813177,8.4320070566650362E-2,0,1.0036548405880179E-2,0.26432130096530654,5.9100730876186054,0,1.9195196107935492E-2,0.10045561818374255,-6.0710417825150342E-4,4.1328719896393959E-2]
[null,601,0.99599506286407635,0.9672589174469175,0.97557145751292651,1.0031253911709841,1.0426043623232801,1.029472510726037,0.96789645922608136,null,6.7544692735980005,0,1.1162948774447999E-2,0.20071622938616551,0.12457817209420709,8.1587134504007841E-2,0,1.1162948774447999E-2,0.26540679423436714,5.9136581031710067,0,1.9177014862422098E-2,0.1069390598722192,-3.5602706487647862E-3,4.5967036122364642E-2]
[null,602,1.0118204019978607,1.0269385474773631,0.99026867669456931,1.0120001037981239,0.95981162617769744,0.99688337899732615,0.9898434566281149,null,6.7268748851951177,0,1.0239020616824489E-2,0.18816122632368931,0.11946072224300555,8.2482270934258375E-2,0,1.0239020616824489E-2,0.26357206224808893,5.9133257926285019,0,1.9091406054658502E-2,9.9515750555235344E-2,-8.9681021467107698E-4,4.2162464422352545E-2]
[null,603,0.97183139298835486,0.98551993157968443,1.0034933290483279,1.0105286774728099,0.9793108614020638,0.99531496130622465,1.0236249649715579,null,6.7734832503750555,0,1.0708477793485433E-2,0.2006828019017525,0.12618528323492226,8.3580244993530436E-2,0,1.0708477793485433E-2,0.28407178373532221,5.9125052198909414,0,1.9313109441019629E-2,0.10544253523925295,-2.3933335772654872E-3,4.4095605515579867E-2]
[null,604,1.0069182563112749,0.97705476934943225,0.98550275308975699,1.0172557162645182,0.9850574347886526,1.0095708522461555,0.98065053313551764,null,6.7420106876973689,0,1.0688771835883189E-2,0.19504300450057993,0.12254627051783704,8.2196409545015642E-2,0,1.0688771835883189E-2,0.2640410229915342,5.9138745584690886,0,1.9117637040177209E-2,0.10340108779933672,-2.2237630559069038E-3,4.4014459889703497E-2]
[null,605,0.98328735358471042,0.97921473412033921,1.0362825871204138,1.0091549466384298,1.0005962152119103,1.0048712056843583,0.9683339512075464,null,6.7574776510671066,0,1.0411572230685532E-2,0.20481619436020138,0.12439963804105671,8.5372219489117829E-2,0,1.0411572230685532E-2,0.26661290649261032,5.9105520574864805,0,1.9247753334089179E-2,0.10589000657641659,-2.2861259680600704E-3,4.2873001255189988E-2]
[null,606,0.98241713384861173,0.97695312007608814,1.0285411790022441,0.99284552982881669,0.97902648729447084,1.0046737749835777,1.0187701736926928,null,6.7710405826691513,0,1.050009496471385E-2,0.20420779523008456,0.12477637025548645,8.5075673481310773E-2,0,1.050009496471385E-2,0.28074056473605596,5.9101199637787563,0,1.9252664431946512E-2,0.10597678810211812,-2.346759464071715E-3,4.3237522117459314E-2]
[null,607,1.0197314877601515,1.010042776357609,1.0032126547249345,1.0049967292407649,0.97306564374955118,0.99593936500424818,1.0417515463319089,null,6.7389149112089273,0,1.0107397025770213E-2,0.18933948877748907,0.11908657896920495,8.343787828481404E-2,0,1.0107397025770213E-2,0.27533335489820376,5.9122221021986654,0,1.9049606382876897E-2,9.9496393322270463E-2,-6.7095352711295947E-4,4.1620461902516878E-2]
[null,608,0.95721963782427411,0.98337804558853659,1.0243136095153398,1.0036263846162372,1.0203507789797253,1.0195273274786931,1.0113240512631509,null,6.7934230174832653,0,1.0945599747454897E-2,0.21154557811468161,0.12780996369321959,8.4915095182320849E-2,0,1.0945599747454897E-2,0.28743284556667636,5.9109460799745861,0,1.9398739433087106E-2,0.11001310552072797,-3.7104215179310481E-3,4.5072031515891675E-2]
[null,609,1.0008853864022922,1.0050153774686945,0.99729605204800154,1.0377113433230107,0.99882952134020853,0.99839430211427216,1.0060640062073927,null,6.7456069791040525,0,1.0398786399559183E-2,0.1930980403064374,0.12168188536846482,8.3039622923825385E-2,0,1.0398786399559183E-2,0.2711782452763809,5.9143227815010402,0,1.9150271125001315E-2,0.10177005196576185,-1.4542708412650458E-3,4.2820351478404788E-2]
[null,610,1.0154636990038506,0.97278643737790382,1.0073862299395462,0.96431433793369126,0.96487143541865494,1.0160754076013669,0.9993315581800426,null,6.7436040711243619,0,1.0484866779100295E-2,0.19762824447633734,0.1213203830574838,8.3562231138356063E-2,0,1.0484866779100295E-2,0.26750213978493559,5.9097879773457249,0,1.9072075123109433E-2,0.10363749773624227,-2.0812926974500138E-3,4.3174815159618692E-2]
[null,611,0.9948551284578705,1.0085289316430481,1.0337131307229164,1.0192433778178493,0.98943544169886155,0.96909366371265793,0.98749524248844367,null,6.734707461498699,0,9.8216070411496787E-3,0.1924782309944171,0.12156001688732122,8.5199222050336268E-2,0,9.8216070411496787E-3,0.26508271710548476,5.9112463341158401,0,1.9183286614383333E-2,9.9636538556098844E-2,-1.2251443975823428E-4,4.0443629614570473E-2]
[null,612,0.97111184354423075,1.0021372667356174,0.99490066142197175,1.0028626111536785,1.0192709064669219,1.0183200243477248,1.0186402295158652,null,6.7775347991400752,0,1.0967855660858505E-2,0.20294357062275448,0.12560260419542046,8.3052057193951132E-2,0,1.0967855660858505E-2,0.28497982841115765,5.9125734874385367,0,1.9317265928802573E-2,0.10708654381385717,-3.1842358702879898E-3,4.5163677405882827E-2]
[null,613,0.99384193461137771,0.99834292298469385,1.0055806766612803,0.99738472024960712,1.0008597256063512,1.0324612732781093,0.96158479186242629,null,6.7516413182874722,0,1.0782434722549934E-2,0.20269442311616359,0.12271479172046904,8.3431658138346299E-2,0,1.0782434722549934E-2,0.26421307627350482,5.9116770963652563,0,1.9188873135231151E-2,0.10638933806634843,-3.0680855134743532E-3,4.4400146985624826E-2]
[null,614,1.0043531547190025,1.0106601802235968,0.98932337275511373,0.96725330749345118,1.0195268472883268,1.0130155417893507,1.0327024522243389,null,6.7505651903045143,0,1.0562714121910632E-2,0.19383784610950217,0.12113802882864702,8.2593522854470344E-2,0,1.0562714121910632E-2,0.27873790436703255,5.91095974406206,0,1.9131464740159417E-2,0.10256637426709866,-1.8950715854600172E-3,4.3495376661001194E-2]
[null,615,0.99163723346863097,0.99176012577374695,0.99199671112167043,0.98115435794989037,0.98053625726209637,0.9728020205482637,0.98040645471051957,null,6.7338901003655041,0,1.0332745115824176E-2,0.19037064471667517,0.12357090757919,8.2580660639187828E-2,0,1.0332745115824176E-2,0.2644555830081104,5.9115623150567869,0,1.920106880414027E-2,0.10059759637489207,-9.9708104037313987E-4,4.254840522689432E-2]
[null,616,1.0123748162741788,1.0066863255804446,1.0043104590855589,0.98307339207458555,1.018616444605126,0.98824874947158248,0.98094961612716391,null,6.7240862344432983,0,1.0106935980175541E-2,0.18963894005220011,0.12009146377035151,8.3291023277645163E-2,0,1.0106935980175541E-2,0.26047989068376032,5.91097545736966,0,1.908845541836076E-2,9.9599518880974736E-2,-6.97078408480112E-4,4.1618563398821078E-2]
[null,617,1.0089639874585659,1.007181771287929,1.0222453501734918,0.98735591824932201,1.0156183599039181,1.0286412199934012,0.96996106343032185,null,6.7409454847317285,0,1.0389085291472333E-2,0.20017658444673669,0.1201394713075514,8.4425843716227716E-2,0,1.0389085291472333E-2,0.26210761330603927,5.9101859846833049,0,1.9106659508017716E-2,0.10420669426891351,-2.1837705471010748E-3,4.2780404042036001E-2]
[null,618,1.0410051948290975,1.0072259950973019,1.0004015939153326,0.97441486744713091,0.98382394064807477,0.9864664291344738,1.002166039081841,null,6.7090430044312175,0,9.8425507953742129E-3,0.18361203636566706,0.11683384011635545,8.3015702311904763E-2,0,9.8425507953742129E-3,0.2586223273950376,5.9107276604659544,0,1.8940354107862163E-2,9.6621359138963706E-2,1.3985226285026536E-4,4.052987226661782E-2]
[null,619,1.0259615081801168,1.0216436155946085,0.99025254720754241,0.99185711863977211,0.96924001037447494,0.97664021086200159,1.0242257173989884,null,6.7185623038851494,0,9.9148890263101915E-3,0.18220034286093936,0.11805831589474249,8.2513117328442992E-2,0,9.9148890263101915E-3,0.26712834850424227,5.9122379412304413,0,1.90171426382056E-2,9.6363900518506601E-2,2.154466837405913E-4,4.082774822588707E-2]
[null,620,1.001171242277076,0.96983215470708928,0.97861098379165479,1.005224442654437,0.99640588335905023,1.0191899371817228,0.98110762347517211,null,6.7501845057537997,0,1.0952747171571766E-2,0.19782700399599301,0.12374550074022034,8.1793901699267924E-2,0,1.0952747171571766E-2,0.26664993562167888,5.9136046460244804,0,1.914871594576812E-2,0.10523923863628691,-2.925900246107691E-3,4.5101463336210873E-2]
[null,621,0.98813160606189376,1.044196024636026,0.96064187809151858,1.0195348901453403,1.0186913738562133,0.983689831668913,1.0181094631569534,null,6.7407849001736526,0,1.054082526034939E-2,0.18537439392349059,0.12205745928975013,8.0807720169562031E-2,0,1.054082526034939E-2,0.27613423618709693,5.9153578428255553,0,1.9220572826256031E-2,9.9509826053006969E-2,-1.0823933262331185E-3,4.3405242225164113E-2]
[null,622,0.97802828603790071,1.004544389509435,1.0270734655388145,0.99166270219633668,0.99110449995308914,1.0133410563777756,1.004136601557756,null,6.7680374190859025,0,1.0525538101245372E-2,0.20425891119818165,0.12397620233272247,8.4953435064327468E-2,0,1.0525538101245372E-2,0.27848555639821498,5.9101407901919494,0,1.9277566144678095E-2,0.10607973804011191,-2.4770727092691498E-3,4.3342292424986648E-2]
[null,623,1.0237189235553121,1.0313211388881705,1.020502319700437,0.97282291488708028,0.99909326844872826,1.0194308667420746,0.99890589425966159,null,6.72959830486292,0,1.0060657605600317E-2,0.19334931607569197,0.11732324857326527,8.4345137596756881E-2,0,1.0060657605600317E-2,0.2649534416624989,5.9095008299317033,0,1.9028782908972249E-2,0.10073900635284884,-1.0694555283828132E-3,4.1427997289563902E-2]
[null,624,0.99667413477708344,0.99947840720865633,0.97581549793980094,0.96012839740045119,0.9522744152725573,0.97024194720376966,1.0151273726440375,null,6.7347723254713259,0,1.0364700070229915E-2,0.18643077106889339,0.12286767681765615,8.1659683765388152E-2,0,1.0364700070229915E-2,0.2720923317581822,5.9113201539087035,0,1.9173285527091178E-2,9.9315791098068235E-2,-7.6735851402525324E-4,4.2679990041367306E-2]
[null,625,0.96917663181740932,0.98488670973218351,0.98465633700288779,1.0072568946863814,0.99680788853544289,0.98245527059237558,1.0028694735932853,null,6.7625603833289674,0,1.0777783365320048E-2,0.19642051058800566,0.12692885555256889,8.2321422108488362E-2,0,1.0777783365320048E-2,0.27778505530550401,5.9133809398956867,0,1.9328475328188249E-2,0.10417541543659181,-2.1612844105273784E-3,4.4380993524462869E-2]
[null,626,0.99851012445265985,1.0008569346498188,0.96705776586627545,1.0103554130279278,0.99355073610322053,0.99810546118275756,1.0265366784947336,null,6.7493802765770265,0,1.0717896943219132E-2,0.19029341845903544,0.12273616196431283,8.1217018043906741E-2,0,1.0717896943219132E-2,0.27731555250576956,5.9145138439704512,0,1.9163228013801856E-2,0.10182058227143767,-1.813920549322887E-3,4.4134391897637078E-2]
[null,627,1.0014631597588466,1.0403299788474363,1.0066006697012091,1.0118763602567513,0.99620190113486806,1.0180826575268087,1.0277883756182413,null,6.7517782849221302,0,1.0357704214014826E-2,0.19500441030388571,0.11977174682805149,8.3696282977762812E-2,0,1.0357704214014826E-2,0.27843186894784278,5.9124025167340939,0,1.9147128705033021E-2,0.102301332349192,-1.6281842744228041E-3,4.265118235068955E-2]
[null,628,0.99098997906406339,1.0092578382106965,1.0196092054831207,0.98071711748246015,1.0048024904089632,1.0006517016900114,0.97296816671612574,null,6.7424969423720125,0,1.0304387768552073E-2,0.19777194658766309,0.12226794388841555,8.4299849353316345E-2,0,1.0304387768552073E-2,0.26508167585369785,5.9099784818136403,0,1.9204659502865578E-2,0.10308863064878195,-1.6278799946220811E-3,4.2431634718247457E-2]
[null,629,1.0060275061479762,0.9817767158891394,1.028474931160404,0.99782555159895969,1.0301223492249789,0.98027428006099826,0.98588096888189103,null,6.7343110138871083,0,9.9841283820501954E-3,0.19415416536183602,0.12160944812354617,8.4830355280082051E-2,0,9.9841283820501954E-3,0.26297708909922174,5.9103928031681114,0,1.912243081777449E-2,0.10076257841764247,-6.5071994978878496E-4,4.1112863568678507E-2]
[null,630,1.0125755625477662,0.98596210543379126,0.99015257597393769,0.98602181310566717,0.99773839004363518,0.98302598094968086,0.99035650005382858,null,6.7272457150299285,0,1.0267665752375803E-2,0.18865515923647455,0.12133400294357656,8.244361234283451E-2,0,1.0267665752375803E-2,0.26261354646281637,5.9119280994746832,0,1.9087387827719012E-2,9.9782760849869104E-2,-8.7927409995941595E-4,4.2280419991908784E-2]
[null,631,1.0054055619533604,0.97944956532940941,1.011219856832329,1.0116470525154644,0.99130987432682649,0.98047312814779741,0.9678734528593308,null,6.7296103933803915,0,1.0154743565808595E-2,0.19249520285993516,0.12212758966263072,8.3711232468779817E-2,0,1.0154743565808595E-2,0.25834538593452144,5.9121282053767121,0,1.9125782989980189E-2,0.10075441743015728,-8.9284986935552943E-4,4.1815426527024961E-2]
[null,632,0.99699496446633695,1.0117474896371279,1.0032876368273467,1.0030309360574772,0.97232292392935393,0.9975920733676481,0.99358524564473083,null,6.741984142694001,0,1.0346900374329506E-2,0.19384757571818831,0.1217188172689737,8.3354061036998134E-2,0,1.0346900374329506E-2,0.26873030804118747,5.9121116431970551,0,1.9171525357803153E-2,0.10186156888035532,-1.4180508684393117E-3,4.2606694061877184E-2]
[null,633,0.98907798578547057,0.97856109672475444,0.97964744564637773,1.0159350648542536,1.0017151391574781,1.0232518340688839,0.96919430565644371,null,6.7561534016966682,0,1.107815878038999E-2,0.20040012492266518,0.12479077183210753,8.1870397087958041E-2,0,1.107815878038999E-2,0.26691222529200548,5.9141266194897728,0,1.9215293893360651E-2,0.10655274610254738,-3.3326629426394111E-3,4.5617886018890101E-2]
[null,634,0.99150470338171925,0.98752651432092597,0.9724398886320571,1.0019251938929097,1.0117738186743201,0.9778649627472582,1.0402423748167089,null,6.7526742947626186,0,1.0585938334090784E-2,0.18945853800920082,0.1241673477406541,8.159794818271103E-2,0,1.0585938334090784E-2,0.28114298074536986,5.9137646574465963,0,1.9201803644362796E-2,0.10109989432218346,-1.3498851614632396E-3,4.3591009833003388E-2]
[null,635,0.97974785473614268,1.0121507145464128,0.97946905041151766,1.0195140539232102,0.96683072526891178,1.0097594038031952,0.97046960683837291,null,6.7515009453331816,0,1.0879467163430636E-2,0.19675377548609269,0.12429324564342192,8.187931356523484E-2,0,1.0879467163430636E-2,0.26818474934202108,5.9143299251001213,0,1.9267782969382724E-2,0.10462332878432826,-2.630884863466383E-3,4.4799709306040922E-2]
[null,636,1.0038465126264651,1.0442003304839156,1.0126291928888569,1.0055936801963727,0.9952709100355086,1.0142109469527276,0.99159897189689161,null,6.7381083506245592,0,1.0223443991544024E-2,0.19420219656777113,0.11919891567864102,8.391943335952394E-2,0,1.0223443991544024E-2,0.26761129924723209,5.9117209827107837,0,1.9134204254303979E-2,0.10157710406642073,-1.3541079121013242E-3,4.2098322651983523E-2]
[null,637,0.97801631678899303,1.0126341571248789,1.0234074910340267,0.99047215264688582,0.97892035984090842,0.98951853776150833,1.0110213477149463,null,6.7583274063603236,0,1.0275926625801257E-2,0.19833685206723839,0.12365131589157567,8.4718903915394952E-2,0,1.0275926625801257E-2,0.2779969240844879,5.9102875704890456,0,1.9277634362119059E-2,0.10318995656666541,-1.4461878144981688E-3,4.231443679829415E-2]
[null,638,0.9632663543369292,1.0117352229829191,0.99808572384029881,1.0150293820994771,0.95881207371439925,0.98019029238350452,0.98310709774124416,null,6.7569100098350479,0,1.0570369690416635E-2,0.19651402303071744,0.12608215204107001,8.3106649121798382E-2,0,1.0570369690416635E-2,0.27353183215629762,5.9130526469542897,0,1.9362988477206126E-2,0.10352975713523198,-1.7969400110298046E-3,4.3526900929468502E-2]
[null,639,0.99097254406576418,0.99400696026491553,0.97357882797332829,0.98315056577985394,0.96828474666791586,1.0454820003054108,1.0153429492817239,null,6.7711189512535555,0,1.1281120735645352E-2,0.20224198996063666,0.12388810797786874,8.1654558135152808E-2,0,1.1281120735645352E-2,0.28104657474347655,5.9126873117497833,0,1.9204756289873743E-2,0.10785976563273658,-3.9177604607256453E-3,4.6453647224750365E-2]
[null,640,1.0170497753097256,0.98825979234227523,0.97421849658737891,0.98952652962618315,0.98853880452710952,1.0225101601140987,1.0007493168781132,null,6.7407330676846424,0,1.0771092122104649E-2,0.19328189835542972,0.12098022575468301,8.1523605255809442E-2,0,1.0771092122104649E-2,0.26783345510705187,5.9129970218701766,0,1.9063702847677836E-2,0.10304807373678625,-2.3483554188703055E-3,4.4353440175898755E-2]
[null,641,1.0098187960825289,0.9812209654106181,0.98910384964382714,0.97253500694596484,0.96967259504608605,1.0185529271916309,1.0302083344624444,null,6.754135590743501,0,1.069963447251287E-2,0.19628659298220183,0.12191955998708003,8.256570484879909E-2,0,1.069963447251287E-2,0.2774172708861849,5.9112574295923741,0,1.9102085722231776E-2,0.10387346571968964,-2.3457092889290058E-3,4.4059190293867297E-2]
[null,642,0.96729973856972418,1.0103172747846378,1.0151316553900627,1.0291950854730723,0.99326075165575178,0.98052016599015945,0.97513824078815936,null,6.7543683325051607,0,1.0380321366749129E-2,0.19791383012270991,0.12529696498874995,8.4130286408942254E-2,0,1.0380321366749129E-2,0.27025651888119612,5.9128535917678349,0,1.9339389771972547E-2,0.10339062011427284,-1.5571853104677635E-3,4.2744315759946291E-2]
[null,643,1.0085383575910847,1.0264041506432953,1.0284831257937601,0.98078961626122629,0.96573935968177427,1.0015996943848195,1.0006685604660195,null,6.7356817438554044,0,9.9839707912039305E-3,0.19415345289110764,0.11916862205255631,8.4884487097309946E-2,0,9.9839707912039305E-3,0.26782784770683349,5.9094720760952271,0,1.9108939797851856E-2,0.10076180332550998,-8.0769974861870267E-4,4.1112214637623719E-2]
[null,644,0.97209560183996424,1.0202355995228034,1.0336553153372565,1.0058387417282915,1.0016457720604013,1.0198931730692877,0.98033098993378709,null,6.7667304961847519,0,1.0526857593319826E-2,0.20628170218818759,0.12383423006294006,8.5310157865557693E-2,0,1.0526857593319826E-2,0.27401211392691827,5.9105256533922628,0,1.9311584779279519E-2,0.1067849426852715,-2.677614574158159E-3,4.3347725858488423E-2]
[null,645,0.99014498286559827,1.0217303380754275,1.0150607986218854,0.97333769146316185,1.0006748914286026,1.0058458791901232,1.0085088724933964,null,6.7518669298048586,0,1.035348644650263E-2,0.19738149108586828,0.12185860344347961,8.4152516539671582E-2,0,1.035348644650263E-2,0.27536487355898875,5.909839669945824,0,1.9209354255799234E-2,0.10311613130273856,-1.6895246623268695E-3,4.2633814334808964E-2]
[null,646,1.0020625542116595,0.99603223834317944,0.97790298392705088,1.0273411661778953,0.99010992567445066,0.99939108208699601,1.0030837125132817,null,6.7437466298386806,0,1.0615075912286089E-2,0.19152671242118829,0.12233727368319755,8.1812345839123585E-2,0,1.0615075912286089E-2,0.27020747292279751,5.9148392443780793,0,1.9143872520948905E-2,0.10192378566019206,-1.7550707805668231E-3,4.3710993193716068E-2]
[null,647,1.0331621336739953,1.0034840912270901,1.003882994195852,0.9947270983782931,0.99653129798620665,0.96291076558473432,0.9550661067536288,null,6.6948808964962101,0,9.6664480247071541E-3,0.18125916602312547,0.11783303292828347,8.308135975375687E-2,0,9.6664480247071541E-3,0.24632651279037773,5.9116293304403413,0,1.8980108971224249E-2,9.5218589196986933E-2,7.4808398997784588E-4,3.9804712402135574E-2]
[null,648,1.0132774517361913,0.99321474963180478,0.99327810493558411,1.0190085007429761,0.97998379090786036,0.9979113047402286,1.0307324126850659,null,6.7442511765028872,0,1.0354978052296793E-2,0.19114297649655654,0.12083729226078779,8.2819730662518867E-2,0,1.0354978052296793E-2,0.27449602839400822,5.9135368048196142,0,1.9083658429377398E-2,0.10094126833222308,-1.2465393941691557E-3,4.2639956501973407E-2]
[null,649,1.0011633353833169,0.96238608012107929,1.0104714130974821,0.96833339450761857,1.0401888209390795,0.98569357540449298,1.0000910629734174,null,6.7443656725267251,0,1.0336386257836437E-2,0.19572149239428424,0.12352461579319379,8.3774184168506405E-2,0,1.0336386257836437E-2,0.26875023664268205,5.9098303253890148,0,1.9148758950737397E-2,0.10248101509985584,-1.4283547131580809E-3,4.2563398801601718E-2]
[null,650,1.0234320871697666,0.96840056449036227,0.96864904727509749,1.0184686132537928,1.0340925642212444,1.0287615560551102,0.99768070890463112,null,6.7429062590225248,0,1.091630279162178E-2,0.19427460631611476,0.12130781968593515,8.1174370846335775E-2,0,1.091630279162178E-2,0.26614791047175113,5.9148659467515312,0,1.9030275430217673E-2,0.10386759840810496,-2.7136607538996967E-3,4.4951391866434647E-2]
[null,651,1.0050874201746682,0.97234887449560969,1.0256613930431073,1.0223402297965047,0.99545589994711725,0.99941879290616842,1.0007604600751212,null,6.749626938794159,0,1.0256120249800283E-2,0.19861546149145101,0.12224764345265099,8.4758445544097172E-2,0,1.0256120249800283E-2,0.26910435129127036,5.9118794123574387,0,1.9127499323265917E-2,0.10322045778052526,-1.5592101138698123E-3,4.2232877667325641E-2]
[null,652,1.0085271739456136,0.99837698472799297,0.99580381468281887,1.0069191097291661,1.0031633250191681,0.97790908277642441,1.0129128714100712,null,6.7334364314039172,0,1.0150194964096793E-2,0.18806554773859596,0.12110812316625851,8.289608351021456E-2,0,1.0150194964096793E-2,0.26907812900765526,5.9127422006463064,0,1.910899973960041E-2,9.9191322557849876E-2,-5.5067115736335431E-4,4.1796696194796701E-2]
[null,653,0.96781196911062584,0.99936498626180081,1.03698742816338,0.98343261295860385,1.0103819503071398,1.0119088643353338,0.96589985488228847,null,6.765802778759725,0,1.0553045191046296E-2,0.20781554990066073,0.12534932317134015,8.5453352913599123E-2,0,1.0553045191046296E-2,0.27064534856682304,5.9091217298578602,0,1.9336406866775565E-2,0.1074036293435086,-2.7781235855511219E-3,4.3455561724707381E-2]
[null,654,1.0223066836540766,0.99817591209681478,0.9977824683891412,1.0077072705690882,0.97347728434524183,1.0392006545226236,0.9934292464346276,null,6.7427883066658652,0,1.0623528352334155E-2,0.1974135721469735,0.11944911233003652,8.2976991273368439E-2,0,1.0623528352334155E-2,0.26596913014650236,5.9126739383310634,0,1.9036139431806567E-2,0.1040193459316071,-2.495721762849735E-3,4.3745798837355764E-2]
[null,655,0.97731962351151569,1.012576702031404,0.96434431445982494,1.0024204721186951,0.99239069233142951,0.98926750094464599,1.0132242934940854,null,6.7546909875133663,0,1.0824885361710383E-2,0.19141995836528333,0.12486567603982719,8.1061066225187384E-2,0,1.0824885361710383E-2,0.27867266893454923,5.9142320717329619,0,1.9281607969388683E-2,0.10256343103833598,-1.980443953925493E-3,4.4574951161755465E-2]
[null,656,0.95364183175935191,1.0060483470836052,0.98487868470166562,0.97422056664549395,0.99296446281507278,1.0093666838764188,1.0396385847590781,null,6.7902120376840678,0,1.1149205104727045E-2,0.20325653166042845,0.12789992218323562,8.2543536274691243E-2,0,1.1149205104727045E-2,0.29520098172727749,5.9115828314094125,0,1.9420106550863393E-2,0.10778905374336294,-3.391368001941356E-3,4.5910442136735778E-2]
[null,657,0.99212527302364628,1.0184908684022678,0.99671077997461033,1.0305113604501894,1.016006376356791,1.0103285127475869,0.98001666090992279,null,6.7463869862005597,0,1.0561035487848522E-2,0.1959408842149864,0.1221149857705857,8.2949067729991888E-2,0,1.0561035487848522E-2,0.26746457569311338,5.9139664681577235,0,1.9198364461439618E-2,0.1032983971574411,-2.0342213294463518E-3,4.3488464344719133E-2]
[null,658,0.99742397824652318,0.99792267375581811,1.0031608391469578,1.0116056983226831,1.01827373874944,1.0281969378148346,1.002546215274756,null,6.7594202948966071,0,1.0723923238717344E-2,0.20087331241328227,0.12234027769530312,8.3424153738100429E-2,0,1.0723923238717344E-2,0.27407485913723745,5.912582172156303,0,1.916917342714201E-2,0.10556003862546307,-2.7628994060826281E-3,4.4159207109858101E-2]
[null,659,0.97319480768017574,1.0048696630553096,1.0177882631746269,0.99648115210874677,0.98183793375136819,0.97856918368254997,1.0001728061928965,null,6.7557169264338759,0,1.0296813229641049E-2,0.19709488681758916,0.12475615216659455,8.4340008890222654E-2,0,1.0296813229641049E-2,0.2753818621771546,5.9109343585879079,0,1.9305250513137973E-2,0.10282795587630571,-1.3239927102719239E-3,4.2400444115229537E-2]
[null,660,0.96148250413655867,1.0161907217166124,0.96295692273920619,0.99610292741453133,1.0077110210220619,1.0019811884435383,1.014138597277896,null,6.7708730023029338,0,1.1141052933645642E-2,0.19660524178773098,0.12676804495489527,8.1050020600680228E-2,0,1.1141052933645642E-2,0.28473654626788558,5.9139655955357258,0,1.9373488654820758E-2,0.10541541810823996,-2.918226554301647E-3,4.5876872947254933E-2]
[null,661,1.0081487456341509,0.96072043177631739,1.0259350697200444,1.0202492791023356,1.0183029846900289,1.000978371578412,0.9705906275082592,null,6.7420799654050896,0,1.0291443369625626E-2,0.1993801808872018,0.12245913897621682,8.4655653199595324E-2,0,1.0291443369625626E-2,0.26046996423451102,5.9117506834901858,0,1.9111028811528066E-2,0.10360394756804463,-1.7289637496834165E-3,4.2378331987485481E-2]
[null,662,1.0134908458774337,0.99702272315012541,0.99263136043132061,1.0050302521729415,0.98145269581321259,0.96668707383387187,0.97155873878186172,null,6.71438974418498,0,1.0018089961984653E-2,0.18474715404856676,0.1206390002735807,8.2520605756948653E-2,0,1.0018089961984653E-2,0.25581988537116968,5.9128173980969514,0,1.9082525610901069E-2,9.7595111643067139E-2,-8.4647926119714234E-5,4.1252711309912704E-2]
[null,663,1.0227596502917378,0.995604135639923,0.99330440643121864,0.96984783754692039,0.97549653975783412,1.0030281707521214,1.0348485970832584,null,6.737618212630256,0,1.0300733138816985E-2,0.19014908008351658,0.11960149740724708,8.2772077895064022E-2,0,1.0300733138816985E-2,0.27350164610923955,5.9108782797939048,0,1.9033777662517758E-2,0.10041508333921639,-1.1498152639499665E-3,4.2416585603498216E-2]
[null,664,1.0439608351471341,1.0141088242857104,1.0311321448183695,0.99391319119439669,0.96511989621572425,0.99630727145309395,1.0062995606221641,null,6.7144367689448741,0,9.6214926217180474E-3,0.18783862039560326,0.11563348554304577,8.4945652527037105E-2,0,9.6214926217180474E-3,0.25983334108860445,5.9100277871305282,0,1.8925527543736137E-2,9.7357914261555711E-2,2.5484640037087131E-4,3.9619594054389862E-2]
[null,665,1.028642810119051,0.99176824139169262,1.0229077169270488,0.98244170838692069,0.99518552056461551,0.97160011755256881,0.99613261889370897,null,6.7150584344020166,0,9.6834226602060414E-3,0.18676276975862882,0.11855804613189315,8.4419002231370818E-2,0,9.6834226602060414E-3,0.25897199341278454,5.9098824617095849,0,1.9003291798569678E-2,9.7192129766113661E-2,3.9412866331941799E-4,3.9874610929747492E-2]
[null,666,0.97707785478152676,0.99986805781383625,1.0060884320629795,1.0148387936526444,0.98206135623590207,0.9829379655513435,0.97905893993701643,null,6.7496318066680825,0,1.0429911063850541E-2,0.19621495978650993,0.12473429591146508,8.354062509828325E-2,0,1.0429911063850541E-2,0.26893526131152873,5.9125915718982291,0,1.9282988227731612E-2,0.10296252112134313,-1.5789339929808213E-3,4.2948517305972884E-2]
[null,667,1.0199460369369031,1.0243417079497916,1.0268413271958174,1.0317418886553815,1.0056022031498375,1.0162496538887877,0.98142292203916526,null,6.7313006162020539,0,1.0039759038537151E-2,0.19476500863283761,0.11796088073809849,8.4727423966709403E-2,0,1.0039759038537151E-2,0.26106976508634228,5.912319248031098,0,1.9048481804137509E-2,0.10116071286282548,-1.0928456301992201E-3,4.1341940710204063E-2]
[null,668,0.98882097779091038,0.99502730846258114,0.97447531225188022,0.96825083998108996,0.99740767652435269,1.0101600917865372,1.0242638817696246,null,6.7601012362830124,0,1.0910378461326241E-2,0.1958559670327473,0.12408992537986156,8.1695125407465138E-2,0,1.0910378461326241E-2,0.28066584322897864,5.9118326984287739,0,1.9216726491776855E-2,0.10440697854226541,-2.5890247576233296E-3,4.4926996528769109E-2]
[null,669,1.0313623750980034,1.007581773912738,1.0025890930079882,0.96609061960624143,0.99387763604569312,0.96217380683922538,1.00712182664858,null,6.7070322082741454,0,9.6699623417145913E-3,0.18097790003136155,0.11786987701517311,8.3165695276305865E-2,0,9.6699623417145913E-3,0.26010270704646382,5.9101547444745837,0,1.8989316869827279E-2,9.5131866196810369E-2,8.2091762956759467E-4,3.9819183734047074E-2]
[null,670,1.0225075151986269,0.97591202296569912,0.97264559085846636,0.97661139936237384,1.0247741300639348,1.0354205303279362,1.0379663621479656,null,6.7536733603826464,0,1.092244797672149E-2,0.19554081687634528,0.12096993099792444,8.1545538665155459E-2,0,1.092244797672149E-2,0.27770226265301834,5.9123847930698927,0,1.9035092037375301E-2,0.10433477346054823,-2.8165440224828153E-3,4.4976696644873089E-2]
[null,671,0.96749099504439573,1.0156945910385162,0.95544535364214123,0.97942990588163359,1.0114310882367268,1.026826481968103,0.98195591144246497,null,6.7656179997305026,0,1.1423151059305463E-2,0.19934584446415649,0.12614705139513882,8.0458724815973798E-2,0,1.1423151059305463E-2,0.27634088727539663,5.9134687919173849,0,1.9338275646290263E-2,0.10729107942165172,-3.811158022622203E-3,4.70385028171275E-2]
[null,672,1.0108757615390629,1.0193981637516571,0.96016106699295078,0.97854916387126456,1.0028059205426649,1.0289538534134102,1.0357736432143367,null,6.7493336349550885,0,1.0893728994746161E-2,0.19144385625871599,0.12047248718282294,8.0786443280286668E-2,0,1.0893728994746161E-2,0.2791486753805133,5.9131674197100619,0,1.9096440960671771E-2,0.10279288447167061,-2.4330092785445376E-3,4.4858436988886911E-2]
[null,673,0.98834199219979235,1.0268666382069194,1.014761132278537,0.97025917702471942,0.96113659158224496,1.0027853584604742,1.013883385508888,null,6.7522955036173915,0,1.0321353476124345E-2,0.19668166013414826,0.12184194361676931,8.4153910054334535E-2,0,1.0321353476124345E-2,0.27699477451011445,5.9096904187885011,0,1.9219398412515843E-2,0.10276572534207665,-1.5538237233241035E-3,4.2501496482246694E-2]
[null,674,1.0113343387274696,0.98941715561579313,1.0197928430385736,0.98503207472366794,1.0405559300336129,1.0193563128888516,0.96776699073034034,null,6.7381451592093304,0,1.0372018987735153E-2,0.19912407801579324,0.12076019240186588,8.4247124867931317E-2,0,1.0372018987735153E-2,0.26024721097246323,5.9102010838032086,0,1.9093995582949046E-2,0.10378403944782603,-2.02269392364988E-3,4.2710128040935116E-2]
[null,675,1.035894184971843,0.96116611287337761,1.0071311838932993,0.98832812362114897,0.99678665810633238,0.99657661742936599,1.0043462283981701,null,6.7268758026400173,0,1.0135187442726777E-2,0.19096504211150236,0.11950539176254951,8.3486508054455857E-2,0,1.0135187442726777E-2,0.26186392999531771,5.9111000286036059,0,1.8966192439470789E-2,0.10015592022975144,-9.0210844967779792E-4,4.1734897893034195E-2]
[null,676,0.99039868731773917,0.99275867507662829,1.004550151641485,1.0014698351653555,1.0009296757184578,1.0259631088397021,1.0171402495617095,null,6.7683605255901673,0,1.0787401201451571E-2,0.20247854113560573,0.12343762961381843,8.3581670544138967E-2,0,1.0787401201451571E-2,0.2798826056678177,5.9119560529918633,0,1.9207943846111873E-2,0.10633031970557966,-2.9348359765156364E-3,4.4420598061741486E-2]
[null,677,0.99196438682092614,1.0040049271555451,1.0030732771747088,0.98241918465026945,1.0030932095480807,0.97005502588916248,0.96340048443572945,null,6.7266456487629958,0,1.0147532480552925E-2,0.19005209892955344,0.12271664024059285,8.3201477794033585E-2,0,1.0147532480552925E-2,0.25944304334273111,5.9110098682181427,0,1.9199255675950412E-2,9.9877768670188202E-2,-6.4023666966737112E-4,4.1785732561467441E-2]
[null,678,0.99983093479829466,0.99490072235808824,0.98216014708973021,0.99603046639313431,0.99062616125469405,0.99327666912081092,0.9735870986748616,null,6.733697291437962,0,1.0539646358926423E-2,0.19137068074699287,0.1225869149682,8.1950913706165307E-2,0,1.0539646358926423E-2,0.26230300909089205,5.9129120502458763,0,1.915601548665961E-2,0.10162390094006608,-1.6065814658324466E-3,4.3400387718940961E-2]
[null,679,0.99699320765570931,0.98928784538548042,1.018707420401552,0.95508893841206932,1.0025970784992666,0.99792097418044046,1.0141300098859516,null,6.750829636609387,0,1.031033946258716E-2,0.19762235646074483,0.12252433454622236,8.4353799071458721E-2,0,1.031033946258716E-2,0.2745722181223153,5.9086454941996447,0,1.9171534993116159E-2,0.10305644139113766,-1.5726849101770058E-3,4.2456142734921896E-2]
[null,680,1.0070219740630053,1.0237423498502156,1.0123239102860451,1.0154542524916343,1.0228312382200559,0.9941676512063099,0.96977090953164991,null,6.7263817880696335,0,1.0077409109151222E-2,0.19134167361453944,0.11977287308201906,8.3794794310525569E-2,0,1.0077409109151222E-2,0.25927769834459025,5.9122711394819705,0,1.911707941037967E-2,0.10009601039507948,-7.8645756899810315E-4,4.149697699953004E-2]
[null,681,0.99344843272618732,0.99093238217514523,1.0029428159649385,0.97033805185285149,0.99840550400562722,0.99303847369319675,1.0359396281882478,null,6.7565453256662771,0,1.0432023417312591E-2,0.1953425503769721,0.12317984718823713,8.3473321981842957E-2,0,1.0432023417312591E-2,0.28095010029017536,5.9103643534053907,0,1.9191045887498249E-2,0.10266469437448671,-1.5778034398747627E-3,4.2957215601544696E-2]
[null,682,1.0107708566467719,0.98060769579884355,0.98707230578631344,1.0221179509567546,1.0202549146857962,0.99641282274139897,1.0038658618289769,null,6.7401624894719117,0,1.0478557521769153E-2,0.19165270321113023,0.12187292792721517,8.2349486082535048E-2,0,1.0478557521769153E-2,0.26798250415580704,5.9140503495346382,0,1.9097000681268395E-2,0.10152412303087682,-1.5154399124946256E-3,4.3148834760934993E-2]
[null,683,1.0003494645343463,0.96703030834337211,0.98207167662112771,0.9888892417153734,0.99715073027883772,0.98009058227780399,1.003500729077877,null,6.7412873674320455,0,1.0522513779179102E-2,0.19103452747215582,0.12392549061160386,8.2032084104221983E-2,0,1.0522513779179102E-2,0.26924949924110475,5.9125308928191886,0,1.9153189166253491E-2,0.10144988293557135,-1.4180377230825513E-3,4.3329838805027013E-2]
[null,684,0.99242899754958069,1.0025641790490265,1.0018202084021908,0.99314897732705365,0.99753464326187669,0.98660307754015786,0.98887863952609767,null,6.7406382999331704,0,1.0333460736212888E-2,0.19317545170924538,0.12275333150961713,8.3242939044602046E-2,0,1.0333460736212888E-2,0.26774261531100441,5.9116602912687819,0,1.919668279465734E-2,0.10158231268641366,-1.2666764154252367E-3,4.2551352024279371E-2]
[null,685,1.008248488849651,0.95993559744442369,1.0001604852224295,0.98356659017093262,0.98182297272165853,0.9766722799126254,1.01680541204209,null,6.7406762216899843,0,1.0273112788166658E-2,0.19157569632261828,0.12297702975877393,8.3168254619268439E-2,0,1.0273112788166658E-2,0.27045805296823461,5.9112357915355513,0,1.911049385657624E-2,0.10082411194565621,-9.7605923245557555E-4,4.2302849915759298E-2]
[null,686,0.99305017382285865,0.9787838441123351,0.99498791358228611,0.96946852029602471,1.0207346188871707,0.98049856149321479,1.0122662058001377,null,6.7468496706416463,0,1.0431268451428152E-2,0.19303979689851955,0.12399011811942305,8.2879059539084518E-2,0,1.0431268451428152E-2,0.27353740782883335,5.9107637584953849,0,1.9193246659304716E-2,0.1018562303146965,-1.3640540000160375E-3,4.295410678641149E-2]
[null,687,1.0364190374124964,0.99384619132433949,1.0336884559036723,0.98260279378476045,1.0340719610812528,0.98749678184215872,0.98973533072634412,null,6.7149305958563641,0,9.6675015550568028E-3,0.18945125159226733,0.11737201780583827,8.5053910830759527E-2,0,9.6675015550568028E-3,0.25681288220438131,5.9092686638617611,0,1.896352734575503E-2,9.8070805162404392E-2,1.2848640060031131E-4,3.9809050652594005E-2]
[null,688,0.99785937175900619,1.015656091417539,1.0213714935712741,0.9682166066829383,0.99119617742572053,1.0430241178331785,1.0077635122266151,null,6.7622817659578205,0,1.0621564107569247E-2,0.20439162939238087,0.1210864690641594,8.4556193142953345E-2,0,1.0621564107569247E-2,0.27662026265252532,5.9092021459333228,0,1.9166788589326283E-2,0.10644671336677478,-2.9261466106591401E-3,4.3737710427036405E-2]
[null,689,0.98529716899509878,1.0095487292820398,1.0139755051036974,1.0223711204577342,1.002175352770623,0.9812868382792177,0.98782816144970143,null,6.7447137947227338,0,1.0212331379933215E-2,0.19437803078696325,0.12306779776292068,8.4033223463610154E-2,0,1.0212331379933215E-2,0.26884977054752013,5.9125508216450324,0,1.9236444065346737E-2,0.10160148630423334,-1.0563427482330066E-3,4.2052562895341351E-2]
[null,690,1.0068577818842526,1.0024925248619021,0.99165629097712216,0.99236366472053072,1.0226556194208456,0.98338292197375132,1.0096220576428747,null,6.7339302725841694,0,1.024295490181984E-2,0.18862114030076391,0.1211863547065293,8.2628577893697513E-2,0,1.024295490181984E-2,0.26912080038420871,5.9121871472561995,0,1.9117962228885642E-2,9.9690014378426103E-2,-8.0038967222715142E-4,4.2178665107686766E-2]
[null,691,1.0304258769365755,0.96476176619863641,1.0222473957070122,0.99932116004049287,1.0050209645373751,0.97419636882151683,0.99379045639969832,null,6.7202157870052313,0,9.8135620620997035E-3,0.18908799216128441,0.11967945574916439,8.4382806593896631E-2,0,9.8135620620997035E-3,0.25840619323053704,5.9108322737746075,0,1.8994120891185781E-2,9.8434164052926695E-2,-1.1721271164907042E-5,4.0410501822795562E-2]
[null,692,0.99143518968350375,0.98817300238048522,1.0008441145298026,1.0068751450632354,1.0083663674507146,1.0310399508132004,1.0008840228117462,null,6.7659551381111243,0,1.0886148736939603E-2,0.20321345068924715,0.12360762550099019,8.329843731588181E-2,0,1.0886148736939603E-2,0.275653533941009,5.9124570026490861,0,1.9202189155853089E-2,0.10691263283529198,-3.2169568127086733E-3,4.4827222836475111E-2]
[null,693,1.0104165246827777,1.0104762144096928,0.99946203805596523,0.98896800733864643,0.98640534082933595,1.0299746472193778,1.020522611274721,null,6.751718356225199,0,1.0581852622961331E-2,0.19712907249917247,0.12023312125555999,8.3195153907205263E-2,0,1.0581852622961331E-2,0.27542449599143509,5.9115669362672296,0,1.9098892080554337E-2,0.10378278664313194,-2.2862880208932386E-3,4.3574185601801763E-2]
[null,694,1.0150568309194967,1.0014244064059854,0.98708446442791919,0.99944115950029888,0.98202461598700563,0.9790416676263155,0.99273568020451153,null,6.722216473320354,0,1.0160434885058564E-2,0.1858375942752396,0.12034266906295883,8.2255450758567092E-2,0,1.0160434885058564E-2,0.26208428592359601,5.9128239089614629,0,1.9074227037075661E-2,9.8443089712156984E-2,-4.8361477737873587E-4,4.1838862366679282E-2]
[null,695,0.97161185838267183,1.0477932394005429,0.99544236692303345,0.97831886448567562,1.0070260606407968,1.005386562314581,1.0012975919545195,null,6.7569665168833613,0,1.0613580425760039E-2,0.196545970042936,0.12331039718124431,8.2978753707835348E-2,0,1.0613580425760039E-2,0.27828994981884936,5.9112166822339001,0,1.9314376933230373E-2,0.10368279111152397,-2.0772391925512686E-3,4.3704835046388481E-2]
[null,696,1.0185783154301884,0.99419307532937196,0.99174216373545887,0.97433735487870765,1.0094932960871825,1.002974802689556,0.97922238891915114,null,6.7258462459381567,0,1.0362875266948391E-2,0.19085373376887202,0.12018932423150741,8.2496953920793689E-2,0,1.0362875266948391E-2,0.2598690785867851,5.9112080437514454,0,1.9055658955344751E-2,0.10086566795707803,-1.3646910599296822E-3,4.2672475826256863E-2]
[null,697,1.0357068113710961,1.0237345343035262,0.97230723904815441,1.0256964329000391,0.98374227177516216,1.0382480279389594,1.0260140403730462,null,6.7359041825515256,0,1.0596509197408474E-2,0.1896103848260913,0.11717058577116432,8.146675944446051E-2,0,1.0596509197408474E-2,0.27072417579837149,5.9150571340906462,0,1.8967144538705554E-2,0.10118766518879418,-1.9142058733080418E-3,4.3634538766602088E-2]
[null,698,0.96225274630012447,0.99673850254679641,0.99672133269368202,1.0017196918000726,0.98622707847053381,1.0107065740343395,1.0094575823153906,null,6.7798042390364834,0,1.0994033269889326E-2,0.20397756343588588,0.12699773656304633,8.3156517678815489E-2,0,1.0994033269889326E-2,0.28432126696069548,5.9124098167840184,0,1.9368950045670845E-2,0.10753470296971254,-3.2337875417969E-3,4.5271472140431042E-2]
[null,699,0.96064206954861864,1.0310419984315651,0.97786748591917572,0.96742404232365331,0.99257514341284847,0.97331393105643726,0.97473194693408693,null,6.7456502042402553,0,1.0625868619491665E-2,0.19171134527694406,0.12586157804900241,8.1782270263360962E-2,0,1.0625868619491665E-2,0.27109248046487083,5.9116019760714531,0,1.9378449172144502E-2,0.10202385572267147,-1.5571864211517384E-3,4.3755435640958358E-2]
[null,700,1.004917201687302,1.0085996768579928,0.99873435779169828,1.0239427175751774,1.0057979728011179,1.030617410340664,1.003799729257681,null,6.7535071288098445,0,1.0661651818151067E-2,0.19840163425357044,0.12099452282911499,8.313608970092988E-2,0,1.0661651818151067E-2,0.27247315786055459,5.9134979533354652,0,1.912841807601208E-2,0.10449052278649017,-2.5179545161614901E-3,4.3902784483865843E-2]
[null,701,1.0040567435082157,1.0310287887216421,0.98494467495268223,1.0101172044614852,1.0066885921639326,1.0242645868502733,0.9785264580806361,null,6.7384147050418051,0,1.0632854651542602E-2,0.19386213370557207,0.12029073390192747,8.2169664865316933E-2,0,1.0632854651542602E-2,0.26501165309974389,5.913519593916023,0,1.9133067158699071E-2,0.1028037166737486,-2.1600611567053046E-3,4.3784202877476745E-2]
[null,702,0.99519710543485151,1.0037744531412367,1.0132469788007761,1.0086263260481421,1.0183896601744433,1.0313694453887219,1.0146887479991289,null,6.7653181818858554,0,1.0659696715274072E-2,0.20267438629767867,0.12213722383274843,8.4104798362054978E-2,0,1.0659696715274072E-2,0.27827107466071704,5.9118496765431345,0,1.9181403598589677E-2,0.10597611899443536,-2.7712341217210148E-3,4.3894733718213716E-2]
[null,703,1.0008436475474347,1.0283662917055787,0.99874672592060632,0.99923973488064632,0.98745399358041774,0.98818783915886921,1.0365726232665748,null,6.743646872790932,0,1.0179303814654343E-2,0.18942913873929862,0.12054725421653938,8.319603238066281E-2,0,1.0179303814654343E-2,0.27820516863242672,5.9121622167992109,0,1.9150498276698149E-2,9.9764440800175547E-2,-7.2443831429147836E-4,4.1916561260210428E-2]
[null,704,1.0378605741353233,0.99991570356229853,1.0320126194694064,0.99179895555327313,1.0090314394139983,1.0212945641348843,1.0129349561255461,null,6.7323811661224333,0,9.9731257641018697E-3,0.1949570341149445,0.11695461682922056,8.5076807000862259E-2,0,9.9731257641018697E-3,0.26551797825659401,5.909862579894547,0,1.8956221384659265E-2,0.10100382205580341,-1.0154501605580614E-3,4.1067556746360291E-2]
[null,705,0.98848710677371299,0.98981209936718351,1.0054241715546617,1.0041970243870662,0.98670400339386377,1.0250663041132191,1.0198391016595947,null,6.7710001616486952,0,1.0804319833854152E-2,0.20305876469436301,0.1238067996035105,8.3654703349835213E-2,0,1.0804319833854152E-2,0.28111653309702728,5.9120540628504257,0,1.9218588647863438E-2,0.10658883780786441,-2.9883943807629521E-3,4.4490265978571003E-2]
[null,706,0.97945950206787646,0.99379857208726718,0.9861714038625311,1.0065317853488742,1.0005492818305206,1.0042653258715855,0.96830235974650991,null,6.7523776079635871,0,1.0845046355381655E-2,0.19809095491407952,0.12511570708567865,8.2276180968501159E-2,0,1.0845046355381655E-2,0.2673494536376258,5.9132578217574823,0,1.9269421102575939E-2,0.10498187366544001,-2.6217757129697108E-3,4.4657970545170657E-2]
[null,707,0.98009261683584903,0.97422733062636535,0.98664165935396164,0.98149615199286733,0.99906467141900313,0.98014062001235225,0.9952222888194131,null,6.7522293665567927,0,1.066386523387957E-2,0.19491746200042195,0.12602459967952664,8.235556598752973E-2,0,1.066386523387957E-2,0.27248481068295866,5.9118784679040681,0,1.9265825639082489E-2,0.10327576714672852,-1.8850314193887686E-3,4.391189893586251E-2]
[null,708,0.98719950018211888,0.97425111625491456,0.98748604854037414,1.0030349059143997,1.0455238242499978,1.0017887706954833,1.0140261486258881,null,6.7622988590176654,0,1.0812849763399005E-2,0.19788827790510066,0.12510002745889054,8.2492952965056446E-2,0,1.0812849763399005E-2,0.27775524454831574,5.9129958792619917,0,1.9225782032722519E-2,0.10480564215227714,-2.4903380168543468E-3,4.4525390710165848E-2]
[null,709,0.99776774118629574,0.99870145230419438,1.0033998076887658,0.97615985312614828,0.9812235377938644,1.0351607819893871,1.0372568570311149,null,6.7695410102610847,0,1.0786976536480549E-2,0.20212591243188868,0.12225547423978168,8.3548479478718463E-2,0,1.0786976536480549E-2,0.28414049585207068,5.9106532108099028,0,1.9167290316522683E-2,0.10620569853411602,-2.9744007688962066E-3,4.4418849366978361E-2]
[null,710,1.0447116884874696,1.0228011160040436,0.99165220811690136,0.97856596029461607,0.96853763259722647,1.0160728217041997,0.96880859336702208,null,6.7056654352257752,0,1.0112807987827556E-2,0.18622339429311999,0.1158621667206661,8.2381837752476261E-2,0,1.0112807987827556E-2,0.25154714997651273,5.9114416110856434,0,1.8921774354187508E-2,9.8422958301086313E-2,-7.7820053906840737E-4,4.164274328115368E-2]
[null,711,1.0054002410831651,0.96773271884442258,1.0062321196880113,1.022247940328578,0.9787669720778106,0.99873128732635963,1.0053457748615937,null,6.7495431930632881,0,1.0442854489149495E-2,0.1965002663715156,0.12281215618344453,8.3569901359242069E-2,0,1.0442854489149495E-2,0.27020540908214602,5.9129838165668147,0,1.9125811686447555E-2,0.10310489454603966,-1.7608787598752439E-3,4.3001816027510138E-2]
[null,712,0.98018545301768767,1.0139909473470372,1.0048247137587096,1.0226062735704313,0.98081396387612774,0.96654797355364075,0.9748430134605145,null,6.7372642704674943,0,1.0173495248692755E-2,0.19103324381150719,0.12366729021465346,8.3418363030114143E-2,0,1.0173495248692755E-2,0.26527106286929991,5.9130827337588689,0,1.9265298812183751E-2,0.10030624231635241,-6.7260696495001515E-4,4.1892642619466812E-2]
[null,713,0.9794599709688957,0.98565327714744089,0.96762021028317857,0.99964480591433935,1.0028935189939836,0.97290111218371544,1.015235490036843,null,6.7523602334218733,0,1.0715269954716708E-2,0.19040575112466701,0.12588115418589613,8.1245540004778183E-2,0,1.0715269954716708E-2,0.27728087434528809,5.9139041322614352,0,1.9269418437963551E-2,0.10185185165253088,-1.6020630172581959E-3,4.4123574426570611E-2]
[null,714,1.024376761329594,0.97254668155506629,1.0057237299394897,1.001126237972735,1.0186705591011351,0.9936621335025152,0.98268854058540689,null,6.7260799692432043,0,1.0180227379044672E-2,0.19141432766523309,0.12030748743790526,8.3366952475216985E-2,0,1.0180227379044672E-2,0.25870707063440357,5.9118711957163779,0,1.9025363079900708E-2,0.10046157115782141,-9.9436325763250198E-4,4.1920364333981476E-2]
[null,715,1.0099324451466607,1.0131450064410557,1.0031164092278455,1.014947217314955,1.0089787061627415,0.98094098228911364,0.99377732838623756,null,6.7268434991498971,0,1.0039431866885251E-2,0.18803950604446945,0.12009640895647779,8.3284785583599322E-2,0,1.0039431866885251E-2,0.2637898498101508,5.9127652530212709,0,1.9101478208456292E-2,9.8817979911982004E-2,-3.9235586208658354E-4,4.1340593475575914E-2]
[null,716,1.0065169765928703,1.0255356435859166,1.0348234328669483,1.0269773204292254,1.0011857175127754,0.98990756594549212,0.99732809712237103,null,6.7348627798144323,0,9.8360055398796099E-3,0.19307693137418983,0.11932978408408085,8.5290822353752335E-2,0,9.8360055398796099E-3,0.26640796623798596,5.9115995609234044,0,1.9119795569394776E-2,9.989212517897883E-2,-3.5712597685511207E-4,4.0502920069503082E-2]
[null,717,1.0154307171245556,0.98561073331952376,0.99928362297589346,1.0230451535270637,0.96114909878991184,0.99126136704285983,0.98903889860631233,null,6.7310683537933835,0,1.0244156582028163E-2,0.19078770349590543,0.12084103526542062,8.3032674692932379E-2,0,1.0244156582028163E-2,0.26230614118198736,5.9134185966283166,0,1.9072249499120741E-2,0.10045314099362218,-1.0268013768172438E-3,4.2183613412893547E-2]
[null,718,1.0116097304027771,0.98427426831587383,1.0088233032098652,0.99333937829343422,0.99310955391760447,1.0142339055374474,0.97810067642962883,null,6.7392368601786252,0,1.0439872521763233E-2,0.19719929087476765,0.1211851361479325,8.3605507194337403E-2,0,1.0439872521763233E-2,0.26252220016539679,5.9112749856487712,0,1.9092528113402108E-2,0.10333901643872616,-1.9713412212935626E-3,4.298953681658392E-2]
[null,719,1.0212329568212304,1.010932312452393,1.0098070168693511,1.0074429891050276,0.99502858384961212,1.0283990840798594,0.99815589584359077,null,6.7392752966316616,0,1.0357664991156937E-2,0.19593160564021553,0.11874877249175045,8.3728380164684063E-2,0,1.0357664991156937E-2,0.26640305460749875,5.9119812785877839,0,1.9041746215809379E-2,0.10262474844706326,-1.835310361088796E-3,4.2651020837942186E-2]
[null,720,0.98891708809489876,1.0194345709487176,1.0130131734868977,0.98942356235646911,0.99676385867774897,0.96240509287887932,0.97674901277603654,null,6.7278347753576639,0,9.9459927026119312E-3,0.18903919984804091,0.12215850375486915,8.3870545110290753E-2,0,9.9459927026119312E-3,0.26303058259502032,5.9108254323698342,0,1.9216190672370227E-2,9.8857852796889467E-2,-1.1935941830407934E-4,4.0955827628649626E-2]
[null,721,0.9996869242512656,1.0041236867382628,1.0099507708510922,1.018640867619546,1.0350103693926236,0.98727076023718663,0.98711583827062122,null,6.7371102746182956,0,1.0185898925907431E-2,0.19272338870990183,0.12163378914626065,8.3733270971705451E-2,0,1.0185898925907431E-2,0.2653863257978315,5.9125781883535025,0,1.9156800956944147E-2,0.10093717617803123,-9.8238425034560687E-4,4.19437187544646E-2]
[null,722,0.96909095713057902,1.0001937099159095,0.97339160768736099,1.0322327641273428,1.0163906139183585,0.99015197743467043,1.0004335000693749,null,6.7624236926737042,0,1.0898108850212859E-2,0.19532126551563647,0.12637498053222745,8.1635516075390296E-2,0,1.0898108850212859E-2,0.27771256757212631,5.9153512078373822,0,1.932897261975159E-2,0.10417859416577185,-2.3558840986957433E-3,4.487647245411356E-2]
[null,723,0.99543285267182524,1.0052665506485454,0.97306583884213771,1.0118740145998999,1.0213419852178711,1.0109929304221501,1.0034658008218489,null,6.750118644696733,0,1.0812652315251262E-2,0.19369598142333977,0.1227880744556475,8.1538381198392546E-2,0,1.0812652315251262E-2,0.27310944646527247,5.9142683243759606,0,1.9180106265251941E-2,0.10332861549418015,-2.3148626351497479E-3,4.452457765383791E-2]
[null,724,0.99526788837733426,1.0018859182359998,0.98097510727507531,0.9802410952178171,1.008129513526707,1.0110820150573945,1.008209155431508,null,6.7512159317957376,0,1.0756622226266728E-2,0.19496730249111296,0.12282687825317286,8.2027398399731402E-2,0,1.0756622226266728E-2,0.27450352186594013,5.9121238672732463,0,1.9181014010602359E-2,0.10359523295237692,-2.3031391708324645E-3,4.4293855720383649E-2]
[null,725,0.98094247850914695,0.99029883474247393,0.96820142966660605,0.95424193843953009,1.0043061953914199,1.0094911082445812,1.0282357176153383,null,6.7663948675237311,0,1.1073509260056916E-2,0.1969414201477446,0.12544375511268915,8.1337442716691438E-2,0,1.1073509260056916E-2,0.2839924714316896,5.9114175810282372,0,1.926100656474207E-2,0.10531710597068857,-2.9146555704988048E-3,4.5598740121742268E-2]
[null,726,0.98798242020233806,0.98536899130473066,1.017041661779031,1.0451275223711864,1.0051378846263248,1.0004410245071247,0.95040129542230134,null,6.7462488320089227,0,1.0463648842943003E-2,0.20006721878117831,0.12387031408604549,8.4118551096728694E-2,0,1.0463648842943003E-2,0.25993116737793093,5.9136053052519362,0,1.9221405911983538E-2,0.10441711009644924,-2.0696840685054873E-3,4.3087443475174819E-2]
[null,727,0.98630569692094017,0.97958989097757454,0.98821469921521266,1.0401891244608628,0.95476760005527173,1.0026946165610346,1.0015987453278841,null,6.7608964585286611,0,1.0800218585391609E-2,0.19787078701259264,0.12492610470005122,8.2523524931177317E-2,0,1.0800218585391609E-2,0.27462914149438422,5.9149637101360328,0,1.9230786426869529E-2,0.10475827386363135,-2.479247803481507E-3,4.4473377767397272E-2]
[null,728,0.97983461674644923,1.0185941395303395,0.98255779125571263,0.99637968782367969,1.0180198540527508,1.01241939029558,0.99906866127117189,null,6.7583195268306202,0,1.0848322231665999E-2,0.19709160135461254,0.12390907066477266,8.216185355511986E-2,0,1.0848322231665999E-2,0.27625790587144222,5.9129089739529643,0,1.9267290262592718E-2,0.10464107474307345,-2.5897035945847188E-3,4.4671460020625359E-2]
[null,729,1.0028550449474989,0.96786568777744186,1.0229667789313051,1.0015409219120366,1.0432457869918086,1.007642933153436,1.0235170846858643,null,6.7603053371671376,0,1.0408629419515496E-2,0.20076726387146154,0.12279806228992296,8.4679984604491484E-2,0,1.0408629419515496E-2,0.27668497283989874,5.9109108669850112,0,1.9139573325018058E-2,0.1044770913101155,-2.0133613413768456E-3,4.2860883282592639E-2]
[null,730,0.99065762136016122,1.028458995180938,1.0255245550884737,1.0070777736060159,1.0163811134676604,0.99335043816461521,1.0082548864282879,null,6.7479927295444559,0,1.0097979910612429E-2,0.19551342199166091,0.12127856983864382,8.4805619634993556E-2,0,1.0097979910612429E-2,0.2739227402190913,5.9110628064304205,0,1.9206505108651642E-2,0.10161516137698084,-9.9377895446429066E-4,4.1581683898481145E-2]
[null,731,0.97009095624841468,0.98170808358262451,1.0148479012200105,0.97022307957723208,0.99268249888103155,0.9647051035846963,0.973067166784366,null,6.7475334411502956,0,1.0312157530298858E-2,0.19653165819651208,0.12638584825694385,8.4034301770257461E-2,0,1.0312157530298858E-2,0.26766760502568748,5.9096835232856559,0,1.9323173679141305E-2,0.10268295139757411,-1.2392496756318335E-3,4.2463629214154676E-2]
[null,732,1.0177162887998423,1.019229116821454,0.97351363106452782,0.98868460016479442,1.0282567302168188,1.0070069682194194,1.0066662040456311,null,6.7299209752539904,0,1.0468097531169772E-2,0.18764837718110886,0.11943065912955124,8.1474340535126588E-2,0,1.0468097531169772E-2,0.26747557672552247,5.912990078201684,0,1.9060192371331365E-2,0.10007997085357043,-1.3439821253689946E-3,4.3105762381455671E-2]
[null,733,0.97861229212456402,0.95853907948083616,0.97582367396136327,0.99498519552611886,1.0003059584391321,1.0264263296270839,1.0018529103242013,null,6.7771116292688074,0,1.136920280499047E-2,0.20450133151763764,0.12724627480296136,8.1782546249665439E-2,0,1.136920280499047E-2,0.27941232909863939,5.913204184025405,0,1.927423969213073E-2,0.10894193118194011,-4.0675608078619297E-3,4.6816353508289672E-2]
[null,734,1.0150896658378863,0.96681654131820693,0.98375672355748867,0.9603721940347133,0.99968683330790753,1.0063516486431812,1.0118287605102296,null,6.7422496617026733,0,1.0632942832913021E-2,0.19352246002284904,0.12210549073738791,8.2126139192161787E-2,0,1.0632942832913021E-2,0.27005010169086291,5.9108962822502704,0,1.9074053310116676E-2,0.1026845422128978,-1.993973706536934E-3,4.3784565992664462E-2]
[null,735,0.98305666773928846,1.0034247596083239,0.97028752447636324,0.9989649851960013,0.97777802718651385,0.98285111694941274,1.0118022793705215,null,6.7495804683321516,0,1.067817673582732E-2,0.19049963738249673,0.12447730461552374,8.1396390158081061E-2,0,1.067817673582732E-2,0.27613395004349583,5.9137221169086986,0,1.9249054366098986E-2,0.10176545352356813,-1.6342698193502242E-3,4.3970831153530961E-2]
[null,736,1.006686314011878,1.0111587004689868,1.0088771719191401,1.0337867928411573,0.97439513742070383,0.97077172643072118,1.0150051086644667,null,6.7327335667343755,0,9.9256612211061652E-3,0.18750128031065916,0.12047121550722154,8.3730848599182006E-2,0,9.9256612211061652E-3,0.26935893700825364,5.9134575121072164,0,1.9118884474300289E-2,9.8254315764665603E-2,-3.1533243800517715E-5,4.0872106206677687E-2]
[null,737,1.0195223430727007,1.0472959958518406,1.0158423476260627,0.9869525790474164,0.97085277250552249,1.0142986803763281,1.0165139395755616,null,6.7327589038524831,0,1.002616207697824E-2,0.19136248418680438,0.11716889138185482,8.4137421621150718E-2,0,1.002616207697824E-2,0.27010315728183282,5.9105306986496764,0,1.9050703089081907E-2,9.9933127100193933E-2,-8.1353030078179294E-4,4.1285950842673405E-2]
[null,738,1.0210843814878592,0.98046940958833617,0.99009020813354742,1.0248612382143416,0.96916139855663497,1.0018586532986242,1.0062382684938795,null,6.7362424141419792,0,1.0402613486274951E-2,0.19111697802770447,0.12059323359299209,8.2517626111772907E-2,0,1.0402613486274951E-2,0.26641934765350089,5.9140308861483595,0,1.9042522974819068E-2,0.10108800028508028,-1.4022913925549765E-3,4.2836110740304266E-2]
[null,739,0.97960681518515014,0.97179301621128211,1.0392129394352188,0.97552223956232031,1.0229867954295999,0.99934376680759951,1.0227548079914419,null,6.7731633495039016,0,1.0400394021841718E-2,0.20548394656818517,0.12518990175449918,8.5743194467649206E-2,0,1.0400394021841718E-2,0.2821955666042647,5.9085648028714122,0,1.926858409540463E-2,0.10608310301335672,-2.192721251687655E-3,4.2826971380818153E-2]
[null,740,1.0090559009107791,1.0050950352564567,0.97268766590562861,0.99285175687125793,0.97137133552052357,0.98635332053258629,0.97822412802151637,null,6.7229326579250595,0,1.0410897085733827E-2,0.18639433960895549,0.12114552236915252,8.1333585017938359E-2,0,1.0410897085733827E-2,0.26039973172852227,5.9132605470829303,0,1.9106167339049667E-2,9.945238327194357E-2,-1.0298396218877542E-3,4.2870221128450181E-2]
[null,741,1.0327138052495639,0.96792611254433691,0.98346781370791903,0.9605908205959337,1.0287314824814968,0.99103959322012625,0.98089231497998353,null,6.7156948085511221,0,1.0289989420341292E-2,0.18720037529744565,0.11997187243586005,8.1920202189335253E-2,0,1.0289989420341292E-2,0.25592290031347331,5.9109240630197659,0,1.8982399700953733E-2,9.9344343152888245E-2,-9.4369244172409837E-4,4.2372344883125905E-2]
[null,742,1.0148982442047589,0.96264645344807687,1.0032224537681442,0.9798773070436132,0.98131774915018621,1.0005343119033712,0.97106748926301911,null,6.7326772729298758,0,1.0414610306476467E-2,0.19509727438546445,0.12197608337484571,8.3198105905844741E-2,0,1.0414610306476467E-2,0.25876533608573848,5.9108640978945592,0,1.9075066265112083E-2,0.10252156552962931,-1.7057680218608999E-3,4.2885511510539709E-2]
[null,743,1.023306836137778,0.9867167989187281,0.96968933652399159,1.0057312568207328,1.032806721034861,0.97056095452751312,1.0043418658640244,null,6.7180074091344064,0,1.0208338251556797E-2,0.18195599512922483,0.12039790118139715,8.1180246117893706E-2,0,1.0208338251556797E-2,0.26232801496780805,5.9141205717846059,0,1.9030927422491566E-2,9.7230652736317674E-2,-2.7302010877107804E-4,4.203611990343762E-2]
[null,744,1.0056331853224521,1.0149768309619787,0.9951325994657565,0.96298309179321551,0.99568562022256057,1.0102486643598596,0.96538030959547882,null,6.7295797040148111,0,1.0448166165217272E-2,0.19339396857379487,0.12067055326220304,8.2701150748827182E-2,0,1.0448166165217272E-2,0.25995437417726142,5.9104051537523681,0,1.9124555658119661E-2,0.10203575981404281,-1.729500535919829E-3,4.3023688564114156E-2]
[null,745,1.0006777651930328,1.0034882464801043,0.98444396497226139,1.0322487368886091,1.0027933018865913,1.0032073420479231,1.0085785777097218,null,6.7471825398013285,0,1.0575848151637373E-2,0.19267962645281211,0.12202046297898797,8.2251901319507187E-2,0,1.0575848151637373E-2,0.27236184303506522,5.9147436529898485,0,1.9151401230944613E-2,0.10220221229033492,-1.7780207538179147E-3,4.3549460257645764E-2]
[null,746,0.99840299890148931,1.0045780537064786,0.99784921263092374,1.0035371595370242,1.0108423192801983,0.99381785885748963,1.0077960557601697,null,6.744286956495249,0,1.037377854657825E-2,0.1927916181821378,0.12199531744505512,8.3059044471108331E-2,0,1.037377854657825E-2,0.27189118340297813,5.9124448233216382,0,1.9163813829170189E-2,0.10158061820698412,-1.3568359548867274E-3,4.2717373591061196E-2]
[null,747,1.0154700631489422,0.97223636026659765,0.99752395075113764,0.99888569518582981,1.0334953541938687,1.0104382693804461,1.0226699664624259,null,6.7488354718341412,0,1.0519424112739881E-2,0.19540417190551002,0.12153134950393739,8.3051692046532136E-2,0,1.0519424112739881E-2,0.27319533461829121,5.9122116745163922,0,1.9072041477020692E-2,0.10297380371014472,-1.9217120522559369E-3,4.3317116108570419E-2]
[null,748,0.97891563231115564,1.0251319878181093,0.99902011115065248,1.0176480619180832,1.0137200206211601,1.00140260440743,0.99520987701336761,null,6.7549399022899177,0,1.0558201159215429E-2,0.19655973164750898,0.12339776359541607,8.3176604927910708E-2,0,1.0558201159215429E-2,0.27436886268862859,5.9131417207532362,0,1.9272513456564753E-2,0.10350576662612798,-1.9598544893781522E-3,4.3476793083899741E-2]
[null,749,1.0071627383976027,1.0319112406813129,0.96849318090771508,0.98836211537758845,0.9853027982625866,1.0398299191349158,0.97088204838776837,null,6.7372605455634282,0,1.0912523170273133E-2,0.19416239690562567,0.12017757278333706,8.1109756854751691E-2,0,1.0912523170273133E-2,0.26348997439870359,5.9132465834281325,0,1.9116322786445046E-2,0.10381574621810813,-2.793635870145608E-3,4.4935828058468442E-2]
[null,750,0.97710682303557683,1.0146424644075063,1.0070743812229139,0.99361957898117659,1.0275222223039697,1.0067482187171655,1.0093749641955077,null,6.7638269475822224,0,1.0606214095375625E-2,0.19982321852211421,0.12398204936569178,8.3727601787624936E-2,0,1.0606214095375625E-2,0.27942218670920421,5.9113891751145786,0,1.9282822811872286E-2,0.10480473843695694,-2.2793469748421166E-3,4.3674501809023387E-2]
[null,751,1.023461572997578,1.0249268375264273,1.012776402344904,0.99778665213186268,0.99342753663784278,1.0427137475947623,1.0180697322603476,null,6.745786181352881,0,1.0390464454739895E-2,0.19741788829745791,0.117786242109507,8.3985056928067903E-2,0,1.0390464454739895E-2,0.27231375720288498,5.9112907779867649,0,1.9030121965411342E-2,0.10325155590861462,-2.0753022367226521E-3,4.2786083190889911E-2]
[null,752,0.99657032955212377,1.025746826934822,0.99798229868682797,1.0120135047338201,0.97883536291991147,0.97709230988710249,0.99832587766550462,null,6.7329496077635973,0,1.0125963568000069E-2,0.18822321059987823,0.12120195219236618,8.3022501597091403E-2,0,1.0125963568000069E-2,0.26807390397500319,5.912895458090679,0,1.9173855276803004E-2,9.9166994464296665E-2,-5.0518405122469267E-4,4.1696915618698108E-2]
[null,753,0.98683081861386113,1.0235917332000339,1.0170541313423509,0.99090804229449059,0.98672311479245889,0.97443760599209472,0.99813018414151533,null,6.7396595892081299,0,1.0038514596042292E-2,0.19194210176947504,0.12214107873029308,8.4222685896941096E-2,0,1.0038514596042292E-2,0.27046684268743332,5.9106752158077995,0,1.9227845178124644E-2,0.10017591307517866,-5.2891025463103756E-4,4.1336816317512751E-2]
[null,754,1.0057219971550262,1.0197634034773879,0.98088456476638763,0.97817652492601737,1.0272991730742991,1.0057807288782419,1.0245876422264639,null,6.7426564847305119,0,1.0509947143044644E-2,0.19047064874795966,0.12069491147817402,8.2031040414598771E-2,0,1.0509947143044644E-2,0.27537500085684591,5.9120172489548324,0,1.9124076940594096E-2,0.10121053740653597,-1.5450717032276459E-3,4.327809163420316E-2]
[null,755,1.0142768015175856,0.95875090946388464,0.9832450123380726,0.99086039485723421,0.99532334364554176,0.96348810626402426,0.97271464285983389,null,6.7185434737848597,0,1.0229451932720627E-2,0.1860375560560372,0.12262307517920025,8.1929791060534565E-2,0,1.0229451932720627E-2,0.25596358052242568,5.9125726538568628,0,1.9078357418542868E-2,9.873825238013928E-2,-5.2285497325968617E-4,4.2123062284375117E-2]
[null,756,1.0303154310818252,0.98914677771867254,1.030828759698621,0.99755371210346866,0.99110452922472081,0.9810996553802408,0.9708086858033097,null,6.7129198986288063,0,9.7057144222719386E-3,0.18939791620503985,0.11834442073556616,8.483500673394731E-2,0,9.7057144222719386E-3,0.25286199747533333,5.9102420002824436,0,1.8994688028863775E-2,9.8180712833403364E-2,9.6751896053868565E-5,3.9966404438149118E-2]
[null,757,1.0117289738301136,0.9979359465203772,0.96310019887092724,0.99303905845476159,1.0198471356623102,0.97141541720717262,1.0289488745461248,null,6.7294475734956922,0,1.0343458566020045E-2,0.18256901435187917,0.12134634118604706,8.0884667898270382E-2,0,1.0343458566020045E-2,0.27179763616708552,5.9137921645765186,0,1.9091892953159901E-2,9.7882429623050091E-2,-5.0909456820026318E-4,4.259252130787787E-2]
[null,758,1.0117266999368537,1.0053260722683015,1.0341661045080444,1.0302225883233438,1.013276352154405,1.0315612856678686,1.0153089742971524,null,6.7564161024267149,0,1.0290287652377203E-2,0.20179820162517434,0.11967655634697698,8.5355644305700529E-2,0,1.0290287652377203E-2,0.27392943543297371,5.9118130514108147,0,1.9091905063845137E-2,0.10443785643546996,-2.0601211438109656E-3,4.2373572949566458E-2]
[null,759,1.0175418000378638,1.0444842002312766,1.0190121603545954,1.027727207099733,0.99964977859582871,1.0236301410174444,0.95557291732003835,null,6.7241668522105025,0,1.0121638359515338E-2,0.19409293225410656,0.1174654176797169,8.4161754373871772E-2,0,1.0121638359515338E-2,0.2552441757739673,5.9125524500816251,0,1.9061110946112233E-2,0.10120071153164199,-1.2908056105542212E-3,4.1679105180016413E-2]
[null,760,0.99757668890109408,1.0257532885778751,1.0186471972331941,1.0119776724975011,1.005651726096898,0.97175544818982185,1.0353121685992825,null,6.7420343371309004,0,9.8803247456338145E-3,0.18936322191319552,0.12069359391458218,8.4428044389971063E-2,0,9.8803247456338145E-3,0.27724515662939297,5.9117224524407659,0,1.91683367280782E-2,9.875238498972555E-2,-2.4272545083893672E-5,4.0685418670274365E-2]
[null,761,1.0001460060358145,0.98400101103555437,1.0029913159744273,0.99946906194660057,0.99629941656729992,0.96764083067140494,0.9944831746757854,null,6.7331401407257827,0,1.0127133106070416E-2,0.1896470172035391,0.12269807100383437,8.3290481374101638E-2,0,1.0127133106070416E-2,0.26557407738865857,5.9119358644840521,0,1.9154297796510268E-2,9.9668938622330505E-2,-5.3033871554504497E-4,4.1701731568301793E-2]
[null,762,0.97744556500390289,1.0101484408339798,1.0042689936007085,0.98216780332327569,1.0167026294535895,0.97681122894553851,1.0159363050733652,null,6.7532577341646167,0,1.0332132013128666E-2,0.1938524439217148,0.12421305776950446,8.3529386833072025E-2,0,1.0332132013128666E-2,0.27826137846892379,5.9109288598250531,0,1.928088923954745E-2,0.10181456960138578,-1.1687320737087776E-3,4.2545880579122425E-2]
[null,763,0.99415792703077588,0.97814995969377194,0.98526567652819674,0.98963480847348018,1.0287664434353803,1.0351159613627612,1.0156763754209615,null,6.7693586769714233,0,1.1096859164452836E-2,0.20241838043145574,0.12406805979331677,8.2367007329174111E-2,0,1.1096859164452836E-2,0.27945215968515275,5.9123946352823848,0,1.9187129602889572E-2,0.10732381828908569,-3.5474043139609715E-3,4.5694890871916624E-2]
[null,764,1.0071761535018369,0.98058426163649448,0.98362272741844414,0.95899983486097229,0.96940473171043651,1.0158173187351773,0.99871365395422551,null,6.7451763195899428,0,1.0753161081916467E-2,0.19567157078576713,0.12237329965205694,8.210853880311425E-2,0,1.0753161081916467E-2,0.26938197000552377,5.9108295009778642,0,1.9116250689807917E-2,0.10383183299463966,-2.4162476628409486E-3,4.4279603344010002E-2]
[null,765,0.97052196841885352,1.0133041336305209,0.98848829025748519,1.0204150674986947,0.96499664010615538,1.0203167309019983,1.0065269848091172,null,6.7735076857334038,0,1.1005408359436305E-2,0.20171188040922228,0.12524576124736644,8.2623128851434108E-2,0,1.1005408359436305E-2,0.28182357013622966,5.913879664384007,0,1.9320677948286742E-2,0.10677727653455089,-3.1925865121910065E-3,4.5318312734495041E-2]
[null,766,0.9749565941358227,0.99531877920704448,0.99122111256703305,1.0106397700922336,1.0232684987905492,1.0151013259200694,0.98044870822565477,null,6.7639056599111376,0,1.0957102882435912E-2,0.20164185024150866,0.1255200279682003,8.2668314483519231E-2,0,1.0957102882435912E-2,0.2729754186322752,5.9131992210517792,0,1.9295127862607724E-2,0.10659483384151004,-3.108533548523727E-3,4.5119399378261794E-2]
[null,767,1.0208582004523412,0.99687033682523785,1.0190370163479279,0.96590376786962828,0.99269624448014293,1.0232860983833854,0.99007293659046747,null,6.7365847890558515,0,1.0288562410241387E-2,0.19730112936512628,0.11928902164225613,8.423726670934463E-2,0,1.0288562410241387E-2,0.2640403479373844,5.9092109269666491,0,1.9043705894272654E-2,0.10287221629325287,-1.7762944619656492E-3,4.236646870953284E-2]
[null,768,1.0112516675457617,0.99532842175448588,1.0025811154095914,1.0235456017288089,1.0429041784078403,0.99946587729242342,0.99063650049008078,null,6.7360695868176057,0,1.0298410276231648E-2,0.19273732166627952,0.12080390087199784,8.3267062605485234E-2,0,1.0298410276231648E-2,0.26448502368163662,5.9132600884458233,0,1.9094436265832317E-2,0.10131366128271044,-1.2989284709903201E-3,4.2407020468825912E-2]
[null,769,1.0075564202022549,0.99248288838138765,1.0261877395885552,1.0152289260169847,0.98582812569559086,1.0154992136322814,1.0295392456186858,null,6.7578723566157155,0,1.0299933433900326E-2,0.19961922695344672,0.12094248815174306,8.4900283368005189E-2,0,1.0299933433900326E-2,0.27750047499583963,5.9114649154032399,0,1.9114207825465537E-2,0.10371528544821522,-1.7978180912371919E-3,4.2413292560993583E-2]
[null,770,1.0287731734607906,0.99479819008244896,1.0348413134962451,0.96794992156311832,0.97106818701172515,1.0084260475115763,1.0303726349477436,null,6.7381357221935385,0,9.931646188901553E-3,0.19495947088981683,0.11817767046387832,8.5314048150356994E-2,0,9.931646188901553E-3,0.27131787307088368,5.908410275635589,0,1.9002620219272189E-2,0.1008652107526803,-8.0819822771304448E-4,4.0896751238774537E-2]
[null,771,0.99666684575871289,1.0240001227004791,1.003345338037279,1.0283232212350615,1.004604406268663,1.0313184223075589,0.96692824362253016,null,6.7471748081428577,0,1.0644699742240211E-2,0.19944384494230311,0.12117294614444117,8.3319845767511919E-2,0,1.0644699742240211E-2,0.2645497361857968,5.9134751803193213,0,1.9173325530028915E-2,0.10479925527850766,-2.592304877675792E-3,4.3832978852621961E-2]
[null,772,1.0067163683277482,0.99873618879179671,0.98912716723828376,0.98057084962743224,1.0190130299266604,1.037838213100329,1.0182274061146628,null,6.757697179187911,0,1.0853006239754605E-2,0.19910710733695219,0.12143239789519653,8.2563320303850898E-2,0,1.0853006239754605E-2,0.27667818664829691,5.911690487254031,0,1.9118722803498134E-2,0.1053648362060529,-2.9486271921854053E-3,4.4690747932211852E-2]
[null,773,1.016453589703963,1.0023837762841958,1.0108407834041846,0.98102564997719344,1.0211235024821501,0.998453810937871,0.99924105824006337,null,6.7314749255374418,0,1.0130993734037738E-2,0.19193726432004601,0.11969394943711911,8.3758170742005117E-2,0,1.0130993734037738E-2,0.26526769303807135,5.9104951651294337,0,1.9066846813130089E-2,0.10048121520947183,-9.4300809894408953E-4,4.171762894710504E-2]
[null,774,0.9619443694050076,0.98615030521768932,1.0087526249962686,0.9812299338707462,1.0080681617751392,0.98402694193924678,0.98708989270664893,null,6.7647346785044808,0,1.0643869254483324E-2,0.20103155857470204,0.12734630398291313,8.3773149886626846E-2,0,1.0643869254483324E-2,0.27565234927825372,5.9106246554282169,0,1.9370766266935926E-2,0.1053509373680855,-2.2446013331177887E-3,4.3829559051860423E-2]
[null,775,0.96524044791158015,1.0174985755245609,0.97220231715491712,0.97567803302125955,0.98172523814323598,1.0340046276310157,1.0207498793332497,null,6.7824012324818046,0,1.1354313348280146E-2,0.20313863504150195,0.12603414390104517,8.1664923627223218E-2,0,1.1354313348280146E-2,0.28864873544760256,5.9123585474688616,0,1.9351413720472194E-2,0.10841287798737301,-3.9630860880556932E-3,4.6755041375781042E-2]
[null,776,1.0155714596435992,1.0121477897860727,0.97904208352963706,0.99318447169619706,0.98343482897879286,0.97706965726444583,0.99890255254154148,null,6.719760719289285,0,1.0159708166767397E-2,0.18362066220145512,0.11991678412299564,8.1766844795934102E-2,0,1.0159708166767397E-2,0.26328925367843464,5.9129300378163654,0,1.9071505468898929E-2,9.7660711258254249E-2,-3.3094992316517671E-4,4.1835869870107276E-2]
[null,777,1.0240038186515481,1.0331203600564614,0.98929934561924637,0.97474317810548894,1.0114641798718165,0.99248866816703674,0.98400589021822926,null,6.7121610585097651,0,1.0055268263459266E-2,0.18451906267847057,0.11777379124039822,8.2326452311144854E-2,0,1.0055268263459266E-2,0.25845360949988322,5.9113659208056797,0,1.902730131668863E-2,9.7636650650832532E-2,-3.4753493122624969E-4,4.1405804937894204E-2]
[null,778,1.0126383260806398,0.99624939614508312,0.98747326353621834,0.9737769924053894,1.0249184842982666,0.98640065186745252,0.98584103992337835,null,6.7244550133128147,0,1.0280564620089031E-2,0.18814324665146626,0.120873180318169,8.2255086578858716E-2,0,1.0280564620089031E-2,0.26160907707592762,5.9114150984763771,0,1.9087054131243193E-2,9.9645112055471941E-2,-9.0637720794221009E-4,4.2333535233239003E-2]
[null,779,0.96962316660165049,1.0175762822067591,0.99218190582153687,0.98303167161109251,0.97904405813012541,1.0004118072715182,1.0065607306022175,null,6.7635766178333778,0,1.0746582484070141E-2,0.19804955211581005,0.12508051079547894,8.2803827743174144E-2,0,1.0746582484070141E-2,0.28012214709992844,5.9116534594153043,0,1.9325884876966955E-2,0.10464570660126846,-2.3569846635838948E-3,4.42525138490256E-2]
[null,780,1.0037604551340711,0.98287702716636627,0.99447280486804734,0.98980562331586064,0.99944341501974365,1.0024364099391896,0.97777540307075417,null,6.7387826530505137,0,1.0536747383842776E-2,0.19484297310186771,0.12247218819365741,8.2725478700729202E-2,0,1.0536747383842776E-2,0.26338687767461139,5.9118917108072404,0,1.9134669858978298E-2,0.10283402522414659,-1.8937207662701996E-3,4.338845025554483E-2]
[null,781,1.0409993406179026,1.0393190314871918,0.98246033195767879,1.0080656843161844,0.96998836406336209,1.0135357774934401,0.96770727224304076,null,6.704734182854402,0,1.0135324386008943E-2,0.18411128445520464,0.11569451414805727,8.1836171497671736E-2,0,1.0135324386008943E-2,0.25177738470256356,5.9135460740726122,0,1.8940383558253844E-2,9.7754251035183676E-2,-6.6134241623662469E-4,4.1735461801095157E-2]
[null,782,0.96979915762400737,1.0285813723900314,1.0062637087217803,0.96746761927505054,0.99838683204834278,0.96198457245160007,0.99893600421828888,null,6.7440884161825316,0,1.0158735379375531E-2,0.19116301851371736,0.12425192261858034,8.3588300185223244E-2,0,1.0158735379375531E-2,0.27418372088167969,5.910021847487946,0,1.9324864567845195E-2,0.10030283830142298,-5.7996047866452005E-4,4.1831864104777301E-2]
[null,783,1.0019633600974927,0.97262564951422315,1.0234121270262475,0.97420062652121298,1.0135530409263811,1.0232331991650296,0.97943723843651842,null,6.7526224116538343,0,1.0552729730451561E-2,0.20368085738770475,0.12265787570200909,8.4547364251901722E-2,0,1.0552729730451561E-2,0.26640593166197957,5.9094082722288679,0,1.9144411119611272E-2,0.10597007403085734,-2.6466374432276927E-3,4.3454262714128146E-2]
[null,784,1.016380409353189,1.016158211842592,1.0135364047458948,1.0308236686311423,0.99234277742587451,1.0319572051178525,1.0160066409836812,null,6.7495422172868755,0,1.0386162549126391E-2,0.19755824763647692,0.11900119153943087,8.4062637432798126E-2,0,1.0386162549126391E-2,0.27274586478163926,5.913032541778823,0,1.9067232981490649E-2,0.10328618230901965,-1.9800498820893653E-3,4.276836870928416E-2]
[null,785,1.000408156866623,0.97412691714850297,0.97807312059173523,0.98915268993267624,1.0083563471233428,0.99460822403784066,1.0455212814318986,null,6.7568393675360019,0,1.0681491099930359E-2,0.19277369741027098,0.12363127870942688,8.1949564001498151E-2,0,1.0681491099930359E-2,0.28187024685916873,5.9127653618250973,0,1.9152869439895637E-2,0.10257864110291946,-1.8667709272450134E-3,4.3984479114972455E-2]
[null,786,1.0078658320528417,1.0014371007539677,1.0154311007783625,0.96716160141441954,0.96391991487970685,1.0031758587599171,0.96675777039181432,null,6.7302514830128759,0,1.0228636413959302E-2,0.19510820391423633,0.12067362830650716,8.3951546440995353E-2,0,1.0228636413959302E-2,0.25927448411410647,5.9094848645573377,0,1.9112546744172433E-2,0.10190989251058892,-1.3833876983461841E-3,4.21197041232729E-2]
[null,787,1.0195341913438061,1.0257741797459308,1.0004952029060732,0.98027593593921813,1.0223751243873,1.0207522693984912,1.0307567103052253,null,6.7412449077516534,0,1.03173709033893E-2,0.19249646203037463,0.1184250474028337,8.3242277812900695E-2,0,1.03173709033893E-2,0.27466810727322849,5.9110391448253043,0,1.9050640947474794E-2,0.10129186337001438,-1.4537328670811793E-3,4.2485096956595296E-2]
[null,788,1.0226972998522454,0.97138939679286607,0.99038981404134108,0.99854504481521167,0.98393614122472883,0.99799830989408178,1.0017307248042804,null,6.7327515602410832,0,1.0384822824249133E-2,0.19087489201922081,0.1208464446056549,8.2492316921352352E-2,0,1.0384822824249133E-2,0.26454512037028477,5.9125917904419731,0,1.9034102633710737E-2,0.10094487191903641,-1.3408306308503812E-3,4.2762851960701752E-2]
[null,789,0.99203944817625955,1.0135566752921457,0.96108566199819379,0.96946130510183848,0.98209491330325838,1.0015640936723249,1.0105438895423102,null,6.7458051924960856,0,1.0822992074463932E-2,0.19046221513786971,0.12302543662475721,8.0784903839369884E-2,0,1.0822992074463932E-2,0.27497041966997138,5.9126260848206034,0,1.9198839844416497E-2,0.10221809727770048,-2.0479596604729327E-3,4.4567154941867131E-2]
[null,790,0.99463001604313728,1.0002331357164183,1.0002877693834615,0.97331503373940564,1.0246600930220369,0.99888557656105748,0.99038610428379015,null,6.7435830653816211,0,1.046336526238595E-2,0.19516037140211703,0.122624672165435,8.3146568798382198E-2,0,1.046336526238595E-2,0.26872939357349374,5.9106746193207966,0,1.9184526849669072E-2,0.1027041937903992,-1.7275562595895277E-3,4.3086275740916329E-2]
[null,791,0.97297477944460486,0.99997027059021593,1.014226190872169,1.0228009033489569,0.99427771628354222,0.97927149184864215,1.0105836480985602,null,6.7611573972564702,0,1.0360373999734093E-2,0.19726899648556676,0.12509768937143223,8.4179612382760075E-2,0,1.0360373999734093E-2,0.27841979282056595,5.9125597544560264,0,1.9306517298659117E-2,0.10309983251272395,-1.4369741243374676E-3,4.2662176053077351E-2]
[null,792,1.0141939466967529,0.96706039396855192,0.995703817038044,0.98659146872185732,0.97811895492076295,0.96591627863847918,1.0121064441671688,null,6.7293615204772674,0,1.010769586875411E-2,0.18725036212160848,0.12197839376463582,8.2840679076211107E-2,0,1.010769586875411E-2,0.26652178580308139,5.9116491623088034,0,1.9078796521454611E-2,9.8766282942038292E-2,-3.4563454529620586E-4,4.1621692484732499E-2]
[null,793,1.0265868344097733,1.0063136641721011,1.009393703794107,0.97838568687400485,1.0076346269646361,0.99098437374084769,1.0062005101833154,null,6.7225480011492449,0,9.9518679558650916E-3,0.1881401587474805,0.11835360410331065,8.3645444188667512E-2,0,9.9518679558650916E-3,0.26375010588659398,5.910434627514638,0,1.901390591225971E-2,9.8563907130908415E-2,-3.3377321040765277E-4,4.0980020875790051E-2]
[null,794,0.99880773474237883,0.96917786578039888,0.98338567790830433,0.98928919749260424,0.99279180846004966,0.9956845714345558,0.97317287215139536,null,6.7400153834867496,0,1.0684007699448501E-2,0.19434486407911203,0.12398194131093694,8.2030892434326805E-2,0,1.0684007699448501E-2,0.26294714038199285,5.912479946516493,0,1.9161601193385915E-2,0.10314004855716104,-2.0658930105075914E-3,4.3994842023850129E-2]
[null,795,0.98077596537204548,0.98935116489197372,0.99121487269323283,1.0259483061148753,1.0097920024845171,0.99375053260249901,1.0469613683277794,null,6.7715918743797019,0,1.0690561641806517E-2,0.19673491362684092,0.12507588961078331,8.2874120809938681E-2,0,1.0690561641806517E-2,0.28767551333512592,5.9140269983816465,0,1.9261950106635839E-2,0.1040011814262287,-2.0805229094266846E-3,4.4021829991922203E-2]
[null,796,1.0300799892803199,0.99720506791390451,0.98568375274149478,1.0044425713589684,0.98152386966396221,0.99436282576175905,0.97460928482555498,null,6.7141291972592754,0,1.0199795099659351E-2,0.18617038572809644,0.11881332965293821,8.2076388518475291E-2,0,1.0199795099659351E-2,0.25494873791566797,5.9131719151115698,0,1.8995897424670099E-2,9.8688388735667806E-2,-7.3678655235466788E-4,4.200094072454829E-2]
[null,797,1.0220245448026866,1.0214421310788948,0.97757905646052523,0.99023529421159573,0.99453344896197959,0.96576655743681816,1.0344274292598032,null,6.7185803185675272,0,9.9524838355692299E-3,0.17948533571802655,0.11875104924919228,8.1758750328924643E-2,0,9.9524838355692299E-3,0.26978028752161226,5.9128510385368394,0,1.9037611562639816E-2,9.5531295770560659E-2,4.0239292093864241E-4,4.098255695878919E-2]
[null,798,0.98197316987236527,1.0198590436307859,1.0252665436132329,0.99822710572444795,1.0403177181653729,1.0178886927519601,0.99562750204990269,null,6.7617435105499997,0,1.0478883652991114E-2,0.20281095049851874,0.12276773776698664,8.4802432229252558E-2,0,1.0478883652991114E-2,0.27528743054366106,5.9105995460205163,0,1.9255173302321477E-2,0.10542131025301443,-2.3512477755333037E-3,4.3150177711257842E-2]
[null,799,0.98448510571836334,0.98706482112783411,1.0336198619283818,1.0219360318425084,1.0052464399976335,1.0199592172031784,1.0075366977048639,null,6.7726166665039917,0,1.0543572309099206E-2,0.2065984150325787,0.123903872122028,8.5379774439945294E-2,0,1.0543572309099206E-2,0.27844130268528505,5.9113971908837595,0,1.9241008001151996E-2,0.10695075144583011,-2.7122021895433276E-3,4.3416554082959392E-2]
[null,800,0.99757001064075623,1.0007150658549782,1.004378092612328,0.99211849874424507,0.97959653691045678,1.0018466092458693,0.99941103120952601,null,6.746457469826769,0,1.042397234942786E-2,0.19560716400164868,0.12216282180381466,8.3439701506616046E-2,0,1.042397234942786E-2,0.27066079870359966,5.9114604290849089,0,1.9168373312796017E-2,0.10273062164752328,-1.6965029711788937E-3,4.2924062737032025E-2]
[null,801,1.0008693047434927,1.0166126009173042,1.0383728979754867,1.0010595319987929,1.0085322457494306,0.96689434846095612,0.96482510319952419,null,6.7214041721305549,0,9.6676130385097529E-3,0.19076927564774573,0.120356192822671,8.5363834278607678E-2,0,9.6676130385097529E-3,0.257185102719168,5.909993051620682,0,1.915035864255428E-2,9.8526960272021999E-2,2.4988640549543215E-4,3.9809509721609945E-2]
[null,802,1.0266921893013758,0.99829199948832614,0.97054370727961581,0.99476227752262147,1.0378129429775329,0.99693057623502079,1.0330761968331528,null,6.7309240668066677,0,1.0391293919530163E-2,0.18545214786648462,0.11942701919053787,8.1343555959472569E-2,0,1.0391293919530163E-2,0.27134171737702245,5.9134809125533714,0,1.9013360977140976E-2,9.9056313137276059E-2,-9.8045903389554017E-4,4.2789498779257015E-2]
[null,803,0.98113956921486967,0.99199113070848466,0.98957599412042829,0.99686437797058525,0.98573708978129593,0.98070348214868908,0.97277417205804217,null,6.7430658938070911,0,1.0549336044162914E-2,0.1936648660628934,0.12492759193994005,8.2462080580828101E-2,0,1.0549336044162914E-2,0.26593914653248552,5.9125462287853923,0,1.925989016981865E-2,0.10246193322300841,-1.6361316053197712E-3,4.3440288118045157E-2]
[null,804,0.99826117759828092,1.0033806544615906,1.0214638161671896,1.0486558531369674,0.99169334193278125,1.0205244578885198,0.98521853167982054,null,6.7536042883140297,0,1.0441639740990563E-2,0.2009567703416997,0.12162613761884415,8.4508645678268351E-2,0,1.0441639740990563E-2,0.26837058607236236,5.9135425296527924,0,1.9164589571435863E-2,0.10465308957548716,-2.2148741076702103E-3,4.2996813910808777E-2]
[null,805,0.99797621848947371,0.99826729470079401,1.0082741597554663,0.98662944022284571,1.0219593372461526,1.0098097069328109,1.0060609798371904,null,6.7516952242996036,0,1.0477826199814213E-2,0.19775535324489654,0.12215934884001613,8.3710758246010125E-2,0,1.0477826199814213E-2,0.27313986749513142,5.9109435284069551,0,1.9166148923612701E-2,0.10365857941037225,-1.984183574689144E-3,4.3145823307295002E-2]
[null,806,1.0128489408439485,0.98043508114866851,1.0229502320934074,1.0137818502447875,1.0010216880545104,0.99670636156056747,1.0204898145553267,null,6.7461237220842634,0,1.01379774545332E-2,0.19554199724116123,0.12096079062821345,8.4622739016970178E-2,0,1.01379774545332E-2,0.27195347945737447,5.9115731106864571,0,1.9085934652600355E-2,0.10175874804346603,-1.1194643070335773E-3,4.1746386665049449E-2]
[null,807,0.97946302024288112,0.99705537536807798,0.97769669972717521,1.0062320511323177,1.0221679646162289,0.9610906773945096,0.99358778748440824,null,6.7406535418214135,0,1.0441090378293697E-2,0.18832985109699649,0.12511252853597513,8.1785344513645247E-2,0,1.0441090378293697E-2,0.2701476245213244,5.9137093889869528,0,1.9269401109990914E-2,0.10023289009783762,-9.2803877431982425E-4,4.2994551733005988E-2]
[null,808,1.0044485178622971,0.98710871393545885,1.0168903459524334,0.99424553424315865,1.0009336302802339,1.0242287670911145,1.0337040344675212,null,6.7638161089604871,0,1.053026687045254E-2,0.20129589658183386,0.12175660753006291,8.4348200674708051E-2,0,1.053026687045254E-2,0.28038121520970233,5.9108648915856472,0,1.9130949401802756E-2,0.10506621025114057,-2.3896269293028211E-3,4.3361764654892214E-2]
[null,809,1.0151960469542687,0.99254157761675033,1.035835576167365,0.99539251137599516,0.98322775477602964,1.0052153485412132,1.0311618855066016,null,6.7485539644810437,0,1.0033441085101007E-2,0.19724728791465543,0.11984828980381951,8.544571048112945E-2,0,1.0033441085101007E-2,0.27487460572306716,5.9098347291458451,0,1.9073490533220251E-2,0.10199919115443506,-1.0852647776306453E-3,4.1315924502507803E-2]
[null,810,1.0107382770344431,1.0158812575512737,0.9932244933462463,1.0153426958613165,0.99761526003948042,0.97702565200243119,0.9596130521731473,null,6.714220211749593,0,1.0066453618733097E-2,0.18580232657274093,0.12005335246959858,8.2542496137634716E-2,0,1.0066453618733097E-2,0.2541313897341006,5.9133416672779981,0,1.9097174533603718E-2,9.8123528230111057E-2,-3.2358744618734382E-4,4.1451864239992801E-2]
[null,811,0.98843057429326098,0.98650452860931925,0.97831072828653065,1.0084931448355321,0.97645357166311841,1.0129345433431272,0.98982437736027085,null,6.7561394584272803,0,1.0948430822012606E-2,0.19766095842552536,0.12449455708357668,8.1844975583394819E-2,0,1.0948430822012606E-2,0.27169787377880444,5.9137978703476906,0,1.9218904080700885E-2,0.10516672598266423,-2.8260962320818335E-3,4.5083689377007845E-2]
[null,812,1.0179163398757765,1.0244196042615912,0.99696377386446677,1.0205608188546429,1.023050935918109,1.014955276043767,0.96367779722052771,null,6.724081820940321,0,1.0312654379585104E-2,0.19140436546638406,0.11874032880714967,8.2811804474683323E-2,0,1.0312654379585104E-2,0.25669650959109208,5.9134145080458635,0,1.9059139614371914E-2,0.10089408831317685,-1.404598523483943E-3,4.2465675151079581E-2]
[null,813,1.0047186723348855,0.97927935882470185,1.0032538647749805,1.0015027585666314,1.0092053812248938,0.99839135876288931,0.99049976388732131,null,6.7421295217094634,0,1.0420481691705662E-2,0.19521634522762124,0.12236992500361858,8.331676649229415E-2,0,1.0420481691705662E-2,0.26623401888113835,5.9120309648164833,0,1.9129490029676142E-2,0.10258253784427351,-1.6602154154921269E-3,4.2909688829845943E-2]
[null,814,0.97429959814729672,1.0251888192898235,0.96633220548292775,1.0037256384322335,0.99795860659551627,1.0111163349571244,1.0157572504818297,null,6.7642950844146599,0,1.1020530697683682E-2,0.19545587106349366,0.12459686459037486,8.1233138567454302E-2,0,1.1020530697683682E-2,0.28224567170722248,5.914194788415033,0,1.9298898466872872E-2,0.10462107215577053,-2.7318043832857343E-3,4.5380583831721874E-2]
[null,815,1.0130795834615267,0.9915775496264192,1.0033154629445491,0.99856618812488473,0.97345305138773586,1.0049059549549579,1.0180799530891842,null,6.7438032392608527,0,1.034587267314647E-2,0.19383631046166791,0.12075453487393366,8.3393672158735083E-2,0,1.034587267314647E-2,0.2718786415306827,5.9118687999089108,0,1.9084709254062412E-2,0.10185424362207023,-1.4701347205435056E-3,4.2602462171329437E-2]
[null,816,1.0010293592779211,0.97931879817107659,1.0019558720925013,0.9887217511376144,0.9928555632873356,1.0012459762926536,1.0103786824980325,null,6.7505184838100156,0,1.0500512699950771E-2,0.19633780032130149,0.12284347633514477,8.3316039383936613E-2,0,1.0500512699950771E-2,0.27284949957954036,5.9114134018465236,0,1.9149487739451031E-2,0.1032382995287293,-1.8687632014259378E-3,4.3239242276810863E-2]
[null,817,1.0419934743927106,1.0185478854930703,0.98786302273146509,0.98107690590456398,0.97331717590109745,1.0190095852512253,1.0254737432967078,null,6.7241233348793585,0,1.022038241021089E-2,0.18714999192234066,0.116425511337141,8.2357524362596093E-2,0,1.022038241021089E-2,0.26725990923267429,5.9117880537968155,0,1.8935387178771773E-2,9.9099779571639873E-2,-9.7853812761673417E-4,4.2085715604994862E-2]
[null,818,1.0128072666749142,1.0058209336985398,0.97796368624266061,0.99061998862411316,1.0416067404812639,0.99893043384205704,0.9929297550539895,null,6.7294299278518297,0,1.0453189336178476E-2,0.18862279947259186,0.12056574048560205,8.1714019263729329E-2,0,1.0453189336178476E-2,0.26449681254589774,5.9128507009820197,0,1.9086156125964721E-2,0.10037537177992034,-1.3260458919417697E-3,4.3044373088041279E-2]
[null,819,1.0178851886491842,1.0220251909861444,0.98346352086790279,1.0158291489809967,1.0144564342290807,0.97598647348299439,1.0067569468134867,null,6.7197460101905433,0,1.0044582084062335E-2,0.18273464488911254,0.11910037769950318,8.2074945649397227E-2,0,1.0044582084062335E-2,0.26458073783890523,5.91391031114751,0,1.9059303518658584E-2,9.6974657259236416E-2,-5.0768964988344487E-5,4.1361801153206659E-2]
[null,820,1.0296657210911886,1.0001259553090327,1.0154295774440474,1.0057748650830605,1.0342629100308869,0.97560659304791097,1.0217280702158287,null,6.7218169123637015,0,9.7424040587894365E-3,0.18583304713658688,0.11818069313981666,8.4064550214383915E-2,0,9.7424040587894365E-3,0.26564974880604919,5.9115712068691701,0,1.8998026742161684E-2,9.7065319223702859E-2,3.3683440101179755E-4,4.011748583081632E-2]
[null,821,1.0091884888515463,1.011207485030531,0.98440552463865783,0.98085765485300591,1.0114330246337284,0.99231716095466949,0.97903552363885904,null,6.7246201706501711,0,1.0339189390505384E-2,0.18835724028168085,0.120621846827451,8.2062926616774473E-2,0,1.0339189390505384E-2,0.26108923447578453,5.9119677816627476,0,1.9105457528333078E-2,9.9911427428534927E-2,-1.0706857741310462E-3,4.2574941602993403E-2]
[null,822,1.0157089027595374,0.98328938915579212,1.0082369292481745,1.0050951424273484,0.98235721660262632,1.0264963998385708,0.99805595762755162,null,6.7474290569613515,0,1.0533367734741821E-2,0.19879266926812089,0.12075533820426318,8.3650645176923347E-2,0,1.0533367734741821E-2,0.26795108833236747,5.9119434434315989,0,1.9070779079852249E-2,0.10420423563737101,-2.3136756312509593E-3,4.3374533462102217E-2]
[null,823,1.0008829623911613,1.0405658248631648,1.0085009300919905,1.0049640402096505,1.0075051813705083,1.0234183840287991,1.0239712471266109,null,6.7529826297836282,0,1.0399722144622918E-2,0.19634715269310132,0.1197951677326945,8.3804369926028494E-2,0,1.0399722144622918E-2,0.27806564039597503,5.9119213990778992,0,1.9150284316465614E-2,0.10290888390810005,-1.8344729766568786E-3,4.2824204710020838E-2]
[null,824,1.0014828707162098,0.98915163239783988,1.0377024571969184,1.0137263387523248,0.99854364850269894,1.0114319755299239,0.95655708490749813,null,6.7421166899271245,0,1.0231973915040722E-2,0.2017058281978904,0.1216200387630033,8.5358007823779503E-2,0,1.0231973915040722E-2,0.25907866542729635,5.9107162710947723,0,1.9147021564141414E-2,0.10420953937600547,-1.8521296784422331E-3,4.2133447358673158E-2]
[null,825,0.99971703076844609,1.0052552222451749,1.0039603138414439,1.0070983224352263,0.99350708193158876,0.95229727411999476,0.96807041628653379,null,6.7167567988227859,0,9.8715987039660492E-3,0.18512722130474227,0.12168777094761653,8.3241618040917731E-2,0,9.8715987039660492E-3,0.25705259665680835,5.9122935009307245,0,1.9156636729604951E-2,9.7246817514811151E-2,3.0115031369403134E-4,4.0649486383864029E-2]
[null,826,0.98945989175548565,1.0136278451166021,1.0083860623209304,1.0236786484565072,1.0204915774381069,1.0314515269962046,1.0196252921205575,null,6.7694206098141461,0,1.0723094913380438E-2,0.20241801518531397,0.12245838356100397,8.3853075840457661E-2,0,1.0723094913380438E-2,0.28113431180207171,5.9129391622839025,0,1.921316647081181E-2,0.10609675775787704,-2.8480593008548367E-3,4.4155796213557134E-2]
[null,827,0.98912438312887596,1.0118162853556136,1.0366685075198689,0.9949670668160705,0.99134875994207716,1.01300887039719,1.0013805076477689,null,6.7585403604529635,0,1.0285097136511026E-2,0.20244357847384944,0.1220486070806794,8.5493852161091871E-2,0,1.0285097136511026E-2,0.27451554986512899,5.9097632855619295,0,1.9215035347426808E-2,0.10464360231229343,-1.9353496785478228E-3,4.2352199329106936E-2]
[null,828,0.97600907878934406,1.0371069251408638,1.0315024002410573,0.99767943524300695,0.99000577598106476,0.98963591029193543,1.0024470694889476,null,6.7540008749013962,0,1.0121539881904271E-2,0.19770911864700216,0.12257253901057016,8.5198179452775566E-2,0,1.0121539881904271E-2,0.27601237699085446,5.9102097800912112,0,1.9289098065841059E-2,0.10245525243541616,-1.1241694590201851E-3,4.1678699666742376E-2]
[null,829,1.0274755229829031,1.0070222785881162,0.97415070931690773,1.0092170834068062,0.97156463238359658,0.96880717187104604,0.98687371173467942,null,6.7068277328970591,0,1.0021368604024875E-2,0.17981038912477981,0.11885634665539785,8.1382375404739568E-2,0,1.0021368604024875E-2,0.25639439779773687,5.9140653002630721,0,1.900931278517342E-2,9.586901211802655E-2,1.7438657387263201E-4,4.1266212174257813E-2]
[null,830,1.0015083473882291,1.0254345522232353,1.0073383245745116,0.97456861635137271,0.98822996137077723,1.0009255854098671,1.0057590272367194,null,6.7396962445859376,0,1.023910413294373E-2,0.19298219887719542,0.12044551305425925,8.3614701109359743E-2,0,1.023910413294373E-2,0.27098904482811348,5.9103447920785497,0,1.9146883089375993E-2,0.10120348263926258,-1.1931794170488143E-3,4.2162808326866266E-2]
[null,831,0.96383371249602623,0.9732161787933159,1.003129187905762,0.98626373651629817,1.0098956148863152,0.99017451094804465,1.0095794339592195,null,6.7746208823858298,0,1.0803009228831631E-2,0.2023452118248813,0.1278804933830279,8.3514437999912233E-2,0,1.0803009228831631E-2,0.28212118515309076,5.9112144769124093,0,1.9359657015375648E-2,0.10633519925300131,-2.6346482962390249E-3,4.4484869140367263E-2]
[null,832,1.0045176224389731,1.0024160396415669,0.99029033508209241,0.97801059321285888,1.008369908450665,1.0032359587973041,0.97286342192680542,null,6.732432267999334,0,1.0486925023167859E-2,0.19272312336691441,0.12149772802234067,8.2435314740942886E-2,0,1.0486925023167859E-2,0.26173562612768442,5.9114874196717277,0,1.913057602476179E-2,0.10192737117681187,-1.6881817741858502E-3,4.3183290642335136E-2]
[null,833,1.0381547743437605,0.98366788377813208,0.96971670691583778,1.0205808628306676,0.98540557829841435,0.99034429643749788,1.0398240235040441,null,6.7265127281882693,0,1.0280822405010165E-2,0.18325541829468159,0.11882245143165705,8.1286911929706537E-2,0,1.0280822405010165E-2,0.26962066980422522,5.9149219787287048,0,1.895473281933821E-2,9.7923669442413874E-2,-6.0770100812066819E-4,4.233459674566023E-2]
[null,834,1.0126529285495094,0.99980642346831594,1.0106513873903311,1.013139947745874,0.97134058352392716,1.0221574161152778,1.0107700147412852,null,6.7487869320313152,0,1.0423644796181757E-2,0.1974263412089903,0.12027049356991738,8.3855521602115415E-2,0,1.0423644796181757E-2,0.27159114396267053,5.9122411691385697,0,1.9086976499855995E-2,0.10336448526726531,-1.9719131491368648E-3,4.2922713931066885E-2]
[null,835,1.0142892352589437,0.98963942991127907,0.98942397690809591,0.98413041713421756,1.0182063975618534,0.99521506859821762,1.0195300868464154,null,6.7378662043824828,0,1.0367465438050743E-2,0.19028319080639353,0.12096221698661723,8.2508551777050201E-2,0,1.0367465438050743E-2,0.27101544121496968,5.9118663898645583,0,1.9078291530051875E-2,0.1006804296413477,-1.2196847723469548E-3,4.269137733383635E-2]
[null,836,0.97298140919990062,1.0174890348995274,0.99415534380443349,0.99906786416902327,0.99533862015601071,0.95764692040677146,0.97167411237372214,null,6.7351246583453372,0,1.0234419875801436E-2,0.18916338189600601,0.1246154504998311,8.274276282977687E-2,0,1.0234419875801436E-2,0.26548827379742523,5.9124100514942333,0,1.930647912028631E-2,9.9852234645923063E-2,-5.9749532786814797E-4,4.2143519389720989E-2]
[null,837,0.99167170363129264,0.98404914933022181,1.0124208283286316,0.99720103951252481,0.95109488534361331,1.0202408590740915,0.99583053309538661,null,6.7613949074357667,0,1.068024007826982E-2,0.20281683144698334,0.12356416449677426,8.3977372177514678E-2,0,1.068024007826982E-2,0.27323609084074268,5.911279366257725,0,1.9200877709446725E-2,0.10609389519751097,-2.7530183213887159E-3,4.3979327630447901E-2]
[null,838,1.015288648920909,0.99518146400275365,0.98884214490622291,0.98365622476184755,0.99831778225865875,0.96088700101260116,1.000327849556176,null,6.7174501735671974,0,9.9811743811822305E-3,0.18303528529893334,0.12058421398512648,8.2357482300066162E-2,0,9.9811743811822305E-3,0.26239850269710063,5.911873097125464,0,1.9073000746729386E-2,9.6873614998667257E-2,1.5427689621089078E-4,4.110069951889677E-2]
[null,839,0.99879196347944732,0.96664631073359275,0.96290098865535956,0.99504021095551587,0.99384547545372981,1.0139000854607909,0.98278900113343159,null,6.7488952698759936,0,1.1087923019533461E-2,0.19565140454515598,0.12449813455230786,8.0815411770301229E-2,0,1.1087923019533461E-2,0.26725656891291372,5.913911156428167,0,1.9161687379158125E-2,0.10490695014284225,-2.964137272574152E-3,4.5658093417713146E-2]
[null,840,1.0332216807213643,0.96222539882036351,0.99760930268094095,1.0024239856362642,1.0002062136059324,0.9953076264721763,0.98655492350550933,null,6.7231689346605359,0,1.0228418723451158E-2,0.19002261510080215,0.11993730004600699,8.2851720507478369E-2,0,1.0228418723451158E-2,0.25774727183680807,5.9123981153797409,0,1.8979804865719384E-2,0.10013358996352878,-1.0202907520588025E-3,4.2118807712507846E-2]
[null,841,0.97785740771552665,0.99866162717767881,0.99753148158117166,0.98343822924685453,1.035385232201893,0.9734523849586979,1.0284217432628064,null,6.7567157552924941,0,1.0403858827567914E-2,0.19325963879628594,0.12485927415932219,8.3152487524473115E-2,0,1.0403858827567914E-2,0.28132494766038052,5.9113763971144335,0,1.9278540205480591E-2,0.10184329951363777,-1.2200685156033991E-3,4.28412388340862E-2]
[null,842,0.96025826130486225,0.97325295728591144,1.0078057509560991,1.0333031127527421,1.0058584048292378,1.0254832271260734,1.0063268944182211,null,6.7942619307677328,0,1.1183901109847559E-2,0.2109352597925957,0.12826220722961662,8.3889107048623138E-2,0,1.1183901109847559E-2,0.28579638249144568,5.9134921150345345,0,1.9380717420922681E-2,0.11059280767077602,-4.1399800309492949E-3,4.6053314110163376E-2]
[null,843,0.98588236895222736,0.99139701087051446,0.9876310052667181,0.99770625650129019,0.95356558096122679,0.97774674120307525,0.98809531754024738,null,6.7426899369418889,0,1.0487402440399024E-2,0.19197345681776279,0.12439329056812078,8.2376089822086912E-2,0,1.0487402440399024E-2,0.26855015953930889,5.9126998019042825,0,1.9233159801862278E-2,0.10166567651566247,-1.3869545887173432E-3,4.3185256561515992E-2]
[null,844,0.96113869289575249,1.0239855241370128,0.98183295447149932,1.0199076301702181,1.0064056627401858,1.0433094456284318,0.96874538577771585,null,6.7763978595418886,0,1.137824381848729E-2,0.20649702630142253,0.12606675333236544,8.2130617171956452E-2,0,1.137824381848729E-2,0.27593447091237738,5.9142208663838405,0,1.9375516891655516E-2,0.10967442184869926,-4.3553960930574022E-3,4.6853582792629168E-2]
[null,845,0.98768749529455968,1.0151087719700058,0.99230753840239061,0.95945304650961349,0.96118357418776246,0.96909666103074688,1.0057353216718068,null,6.7366549436871477,0,1.0229297488765084E-2,0.18855157978675444,0.12290979436059855,8.2682622943597919E-2,0,1.0229297488765084E-2,0.2718107728114933,5.9103720473606707,0,1.9223053576241763E-2,9.9620918739631859E-2,-6.382722034950504E-4,4.2122426311656191E-2]
[null,846,0.99740031514791372,0.98004048518239495,0.99805047805099711,1.0287619738424694,0.99013242940373458,1.0107375469463691,0.98733668691571119,null,6.7522715762657537,0,1.0671609994911319E-2,0.19838582355029877,0.12332808839851662,8.3044148454604408E-2,0,1.0671609994911319E-2,0.26847618862491274,5.9137967934945763,0,1.9169303099780884E-2,0.10451771134926019,-2.3902711894724666E-3,4.394379048327518E-2]
[null,847,0.96636341022980532,0.98615679811470247,0.96778930072852354,1.0131946011929829,0.98900721816086579,0.99816322159800297,1.0342624937457685,null,6.778590764346486,0,1.1138410501157778E-2,0.19797448329731349,0.12755784137490644,8.1418056384103613E-2,0,1.1138410501157778E-2,0.28886442423757358,5.9146275780000721,0,1.9344850526584908E-2,0.10589150725564207,-2.9539686103189403E-3,4.5865991880605347E-2]
[null,848,0.99475704393186259,1.0302613987573255,1.0262134839988617,1.0206534640217719,0.99116521149447678,1.0107434622190981,1.0106323616303943,null,6.7530788865965921,0,1.0218615530087528E-2,0.19805077338095828,0.12068123239825786,8.4873581198840933E-2,0,1.0218615530087528E-2,0.27506727157526772,5.9117564663561604,0,1.9183826932677901E-2,0.10289906928517416,-1.5117744378823957E-3,4.2078439907139782E-2]
[null,849,0.99125098822632163,1.0261143030703233,0.99942762133161056,1.0389386378070908,0.97227826720490274,0.9750794444138895,0.99693741792654378,null,6.7370681506092938,0,1.0144958287679594E-2,0.18898054232977587,0.12180787368515089,8.3143799130052404E-2,0,1.0144958287679594E-2,0.26894834006291346,5.9142694407081757,0,1.9203210968184805E-2,9.9494520867463451E-2,-5.5470963583175088E-4,4.1775132493404317E-2]
[null,850,0.97699654446792072,0.98245064536290394,1.0049949889358971,1.0091925858676449,0.99962539873477996,1.0091376543777824,0.97505620194085174,null,6.7622205348066098,0,1.080005901077854E-2,0.20284971747449287,0.12564581136927094,8.3489851913828933E-2,0,1.080005901077854E-2,0.27050749748485375,5.9123482603498605,0,1.9283452582039815E-2,0.10650175534638727,-2.8785323816709675E-3,4.4472720667543868E-2]
[null,851,1.0103536744973425,0.98935746339650787,0.98925333691207118,1.0340867424510451,0.98327237264871026,1.0098189403742477,1.0204900254581464,null,6.7494374036314779,0,1.0563437013590974E-2,0.19383098369737381,0.12145039702714433,8.257007894308542E-2,0,1.0563437013590974E-2,0.27372663860481394,5.9145761101816561,0,1.9099227708982421E-2,0.10256632619153164,-1.880712123386223E-3,4.3498353400270896E-2]
[null,852,1.0170176742197272,1.0064420490426871,0.97350460443398956,1.0260205110608165,1.0057389180338179,0.98087675816418307,1.0078342157391602,null,6.725008171801254,0,1.0258850958227424E-2,0.18389501382731294,0.12011793806608775,8.1476460970185127E-2,0,1.0258850958227424E-2,0.26566050172150835,5.9150091541615923,0,1.906387203784194E-2,9.807860480104863E-2,-5.3749602290445832E-4,4.2244122238580657E-2]
[null,853,0.99568681854979824,0.95846417944450413,0.99542343110846687,1.0238448513763014,1.0071570381089672,1.0171458399288769,1.0224772528483101,null,6.7697434636746463,0,1.0885885956409377E-2,0.20158296146106108,0.12469553605387033,8.3023328670589716E-2,0,1.0885885956409377E-2,0.27939528557159055,5.9136782663455385,0,1.9178709360857544E-2,0.1063409288005306,-2.9776933424197492E-3,4.482614075302481E-2]
[null,854,1.0146866620048212,1.0135709716131629,0.97016156253552488,1.0206622157367899,1.0203311712140588,1.033065648859548,1.0072895585232613,null,6.7447595699577345,0,1.0828309383225704E-2,0.19314189206027857,0.12011500906805034,8.1333236762817548E-2,0,1.0828309383225704E-2,0.27091311564862763,5.9149021182285999,0,1.9076186349429477E-2,0.10318348724103232,-2.4945260740011307E-3,4.4589050672902433E-2]
[null,855,1.0092140859353607,1.024466425900465,1.0140699030455962,0.97016299030805431,1.0068206057432298,0.97315366987382745,0.96782649624998429,null,6.7137524834992384,0,9.8249778044955764E-3,0.18703140215859951,0.11944660934254769,8.3829390176576077E-2,0,9.8249778044955764E-3,0.25631219530804272,5.9097246016732932,0,1.9105320515596762E-2,9.7756843245274075E-2,8.8611261250436631E-5,4.0457509818055369E-2]
[null,856,1.0296791005193444,1.003796990177807,0.97181458386522235,1.022309202157258,1.00972280788168,0.98782546507506763,0.9997637919759037,null,6.7171513115628096,0,1.0231039469753156E-2,0.18293694787227013,0.11879616113555239,8.1305852402346709E-2,0,1.0231039469753156E-2,0.26094796119405106,5.9149009240548214,0,1.8997957945804899E-2,9.7650475717236646E-2,-5.1456823858151476E-4,4.212959947930401E-2]
[null,857,0.99540362520010861,1.0189437048654633,1.0111433956298297,0.98607398693058224,1.0177719619538375,1.0201942295853765,1.0078100638974137,null,6.7544299972919122,0,1.0493819026572324E-2,0.19890026697073679,0.1214209803344664,8.3914947248890093E-2,0,1.0493819026572324E-2,0.2750988990576545,5.9107507569502822,0,1.9180267072678558E-2,0.1041108441150404,-2.1586433791103126E-3,4.3211678921267857E-2]
[null,858,0.98755456540163788,1.0087874850979277,0.98958136948602582,0.98098005657792087,1.0114083044152846,1.0028274911558566,1.0168288756119686,null,6.7554304432563796,0,1.064040351153576E-2,0.19533824073918385,0.12328519893140706,8.2612939404137942E-2,0,1.064040351153576E-2,0.27815696802434742,5.9116873566025454,0,1.9223796540701568E-2,0.10334698557541828,-2.0363303006506197E-3,4.3815287739281603E-2]
[null,859,0.9733889867409371,1.0187570435877771,1.0056711557621385,1.0105180712569775,0.99008562118463472,1.0287787500854648,1.0121897907516273,null,6.7763602882340619,0,1.0874205061698495E-2,0.20444696630651352,0.12428118608675423,8.3706116538526082E-2,0,1.0874205061698495E-2,0.2833701815368479,5.912381681351861,0,1.9304133026791116E-2,0.10730439430288806,-3.2124118238527296E-3,4.4778040907727162E-2]
[null,860,1.0011604206893017,0.98304219590667585,1.0128398717537292,1.0156751194673341,0.98208707691716279,0.97839761099810807,0.96159860609936609,null,6.7296974364328692,0,1.014587018604567E-2,0.19278872888497095,0.12243524583039195,8.3803767468369775E-2,0,1.014587018604567E-2,0.25753798871343936,5.9122537107335198,0,1.9148774803698771E-2,0.10082729698429099,-8.7696451438020796E-4,4.177888752856395E-2]
[null,861,0.97964416930522258,0.97453743832365169,1.0180552516970993,1.0152097259064023,0.97970648690130546,1.0086682532054836,1.0103347830469318,null,6.7731523020458626,0,1.0680541215428758E-2,0.20452073041614693,0.12545843672360979,8.4427139119317873E-2,0,1.0680541215428758E-2,0.27960584791130233,5.9119309441935357,0,1.9268371895885442E-2,0.10668810825307155,-2.7278441266809384E-3,4.3980567659667992E-2]
[null,862,0.97451361698570915,0.99226066609003316,0.97015337776757304,1.0356235211655624,1.0013385693651058,0.99331750304776489,0.98754640412106987,null,6.7574676028164795,0,1.0940072507779315E-2,0.19513301207543851,0.12613430353411484,8.1373345690006649E-2,0,1.0940072507779315E-2,0.27298590494039227,5.9157114972852654,0,1.9297669620453879E-2,0.10424764557818915,-2.4650472340986798E-3,4.5049271326719625E-2]
[null,863,0.99831403840976018,0.97769201074741985,1.0028593427699586,1.0217699871132218,1.0004632852891637,0.98956206645445177,0.99422823728874909,null,6.7455619518604113,0,1.0405406565317982E-2,0.19482005385521683,0.12324240812830303,8.333290859899796E-2,0,1.0405406565317982E-2,0.2681300014038247,5.9131484500100751,0,1.9164300404584035E-2,0.10239432956572082,-1.5181122489633376E-3,4.2847612142653937E-2]
[null,864,0.98408048353816502,0.96607634444291768,1.0004569834246777,1.0210562567215222,1.0389467880038363,0.97918214886262966,0.99059648295445268,null,6.7526849888895955,0,1.0520909551022747E-2,0.19628287286112225,0.12567052604039219,8.321123109803244E-2,0,1.0520909551022747E-2,0.27013534679801332,5.913245155265793,0,1.9243284859214369E-2,0.10328623726090461,-1.7128981729011455E-3,4.3323232879021095E-2]
[null,865,1.0081706434357636,0.9665223753974318,0.99840686806218781,1.023748343880748,1.0364863680712442,0.98709325321247543,1.0004048407509114,null,6.7412049830464458,0,1.0368986633044468E-2,0.19286185309867851,0.12268361030510558,8.3042581785514963E-2,0,1.0368986633044468E-2,0.26703408713693161,5.9135058340208451,0,1.9110911357505103E-2,0.10158946383003724,-1.3209998322307186E-3,4.2697641344057902E-2]
[null,866,1.0260175263652191,0.97987604679634077,1.0064113513426374,1.0030860237957631,1.0382222617872323,0.99175496080103198,1.0077407317666753,null,6.7296873172365892,0,1.0105763471410054E-2,0.19020779438756755,0.11974220924753035,8.3490498246192799E-2,0,1.0105763471410054E-2,0.26462450128779108,5.911938221283525,0,1.9016852523843844E-2,9.9794335491875649E-2,-7.4083044816170322E-4,4.1613735216423579E-2]
[null,867,1.0075034652665071,1.0287367087021211,1.0021759611842409,0.97037279770449869,1.0175997249609841,0.9683739013456546,0.97653123243682005,null,6.7136361860076361,0,9.8780984798450423E-3,0.18476016931266276,0.11967008305506974,8.3124347339995672E-2,0,9.8780984798450423E-3,0.25857227414617456,5.9104094172890989,0,1.9114492216933641E-2,9.7139942731770679E-2,1.6920861190718127E-4,4.0676251304016739E-2]
[null,868,1.001829818014238,1.0347410732733175,1.0038666707078403,0.97775061927250817,1.0034326960058504,1.0015837378472572,1.0188878450942571,null,6.7414934301804799,0,1.0234042441264177E-2,0.19189770088453947,0.12003673927354019,8.3447608252466374E-2,0,1.0234042441264177E-2,0.27440939954731763,5.9107128528580519,0,1.9145136387406919E-2,0.10080801233270667,-1.1059845370292416E-3,4.2141965181477392E-2]
[null,869,0.98035474890586427,0.98012749897820783,1.0121858707848912,0.98448813758732279,1.0007554926178039,1.0225266908942914,0.95430313929166677,null,6.7590703807355466,0,1.0848512188502728E-2,0.20594067211083986,0.12519491405866934,8.3844643218232623E-2,0,1.0848512188502728E-2,0.26511961962297076,5.9106058231015428,0,1.9264338348515313E-2,0.10774049082641103,-3.3123627807012525E-3,4.4672242229067946E-2]
[null,870,1.0296275353799991,1.0027260867140737,0.97570619264347169,1.0095118037828004,1.0143572150589284,1.0129909175483247,0.99183539611383076,null,6.7245218900244934,0,1.0461482025295536E-2,0.18814107293033336,0.11878300444857624,8.154225112994333E-2,0,1.0461482025295536E-2,0.2611897801600348,5.9139959864476204,0,1.8998223101030408E-2,0.10023240179882895,-1.4393508976552171E-3,4.3078520905781709E-2]
[null,871,1.0163576626955573,1.0294151367086359,1.0260158097426864,0.96861298571727006,1.0251422035320992,1.0034822132696035,0.99739559211804263,null,6.7286815801555822,0,9.9348004706254437E-3,0.19249377723186517,0.11815887591121252,8.4684406317530103E-2,0,9.9348004706254437E-3,0.26503905420314172,5.9089566114962713,0,1.9067353025579777E-2,0.10002159635865228,-6.4983439814086225E-4,4.0909740009472312E-2]
[null,872,0.98411161637100841,1.0173104455701514,1.0026071974645856,0.96947791419426643,1.0069186984186602,1.021616655816405,0.9809959779743922,null,6.7543587248521408,0,1.0715998783629676E-2,0.2005603429578724,0.12305499975195731,8.3318784960942763E-2,0,1.0715998783629676E-2,0.27098660498354238,5.9103367758755363,0,1.9243109604502234E-2,0.10542452055907946,-2.692989455601427E-3,4.4126575614307502E-2]
[null,873,0.99986329919703654,1.0302850171357389,1.0221823248741715,0.9775714242095529,0.9931476964369762,0.98537592199096502,0.99880180051422729,null,6.7334392557962728,0,9.9462314625024858E-3,0.19162582642578224,0.12013932911655578,8.4496964920284245E-2,0,9.9462314625024858E-3,0.26809303376181548,5.9096610081553003,0,1.9155838994105934E-2,9.975848752658209E-2,-4.4804390354090683E-4,4.0956810799381245E-2]
[null,874,0.98046166186652439,0.99013663122652884,0.96901195633753123,0.98803790392361801,1.0131420717990272,0.97155942474255319,1.0193315720528153,null,6.7508368870096795,0,1.0655874853474787E-2,0.18974205995661841,0.12549818302641352,8.1332862514916934E-2,0,1.0655874853474787E-2,0.27794202385733335,5.9132008126143463,0,1.926373197178927E-2,0.10142578694063026,-1.4475698439639555E-3,4.3878995971590291E-2]
[null,875,1.0004254497978766,1.0045032717234414,0.992807761384772,0.9951388578124587,1.0173858379708349,0.97087319877155276,1.0155765980038893,null,6.734987310658342,0,1.0158728515965033E-2,0.18738971101949181,0.12184636932130749,8.2730798553623017E-2,0,1.0158728515965033E-2,0.27123700695414105,5.9122729367116973,0,1.9152775243843664E-2,9.8982379350322919E-2,-4.5650233855874312E-4,4.1831835842474498E-2]
[null,876,0.96763911129013769,0.96295182757510633,1.0087393460272243,1.0045781680849777,1.042255038282822,1.044939487096294,1.007860160961719,null,6.7977404508062573,0,1.1351618718536665E-2,0.21439466089511541,0.12780834304883149,8.3930092655580893E-2,0,1.1351618718536665E-2,0.28612401566521695,5.9118870347484993,0,1.9337413127845437E-2,0.11235463265400286,-4.8396873589605371E-3,4.6743945370123614E-2]
[null,877,0.98616338489485522,0.99017013763870831,1.0078523132410888,0.98771272157324452,0.99853129410172115,0.97805660961505114,0.9955448172483421,null,6.7461665190006546,0,1.03096147691799E-2,0.19445908697011605,0.1240341072772133,8.3651676959431071E-2,0,1.03096147691799E-2,0.27057385841997506,5.9110259556521196,0,1.9231584067425301E-2,0.10195204306656336,-1.2149519886488448E-3,4.2453158576461418E-2]
[null,878,0.99180816164256647,1.0011932049099643,0.97612119616359339,0.99815449685370905,0.99031232978694905,0.99367916261480449,0.99494982798376197,null,6.7438055051747838,0,1.0656481763707589E-2,0.1917660573876164,0.12338014698141296,8.1681104430024187E-2,0,1.0656481763707589E-2,0.27019263431731966,5.9133592071221637,0,1.9200121347833325E-2,0.1021423544821225,-1.7976160136180688E-3,4.388149511990299E-2]
[null,879,0.98029151181796415,0.98791633708131421,1.0247909038488567,1.0030712730186448,1.0083010735018219,1.0102250851083512,1.0101784262745432,null,6.7704970286854671,0,1.0565174707099279E-2,0.20433727859809755,0.12456294500427498,8.4832675288527989E-2,0,1.0565174707099279E-2,0.27938922560801732,5.9108886211523988,0,1.9264697071664966E-2,0.10623953457786525,-2.5234575282158602E-3,4.3505508912840184E-2]
[null,880,1.0126838785984145,0.9933607242193313,1.0111082304968941,1.0448992094345517,0.99932566993196292,1.0182670305443673,0.98392216062575499,null,6.7429321912522671,0,1.0408304138342797E-2,0.19726914551203631,0.12056984628077257,8.3805540606796444E-2,0,1.0408304138342797E-2,0.26408164961296854,5.913931268914677,0,1.90868119669148E-2,0.10325885743452023,-1.9304729090461822E-3,4.2859543832621368E-2]
[null,881,1.0091390962812032,0.98142670566377865,1.0277999876568751,0.97390067411662762,1.0057486249207435,0.99110840584862159,1.0403752631669128,null,6.7499551698774942,0,1.007084117837922E-2,0.19564508750731349,0.12126456467224676,8.4972493827250473E-2,0,1.007084117837922E-2,0.27772134212466126,5.9091393814750015,0,1.910572193009679E-2,0.10156999230315682,-9.3334539189101316E-4,4.1469931429659046E-2]
[null,882,1.025260389728663,1.0166952554569264,0.98121881775893238,0.98310531862402273,0.98667398840541631,1.0139266814746462,0.99112762423167622,null,6.7240867596736447,0,1.0403539509662557E-2,0.18863575315193104,0.11853160106286813,8.1878319030111876E-2,0,1.0403539509662557E-2,0.26207158576891454,5.9122652687892749,0,1.9020776364330888E-2,0.10021876031757246,-1.3752287511462032E-3,4.2839923939788416E-2]
[null,883,0.98972667066247755,0.98105191318912499,0.98684496671052879,1.0001396838697434,1.0108973130205303,1.0461768352040406,1.0109158309353345,null,6.7759184508363717,0,1.123586594946689E-2,0.20543459745397749,0.12444603026008283,8.2486207897168665E-2,0,1.123586594946689E-2,0.28042783099907159,5.912874952437833,0,1.9211681342211389E-2,0.10883715444805042,-4.0673000723434041E-3,4.6267296070319118E-2]
[null,884,1.0047024122191623,1.028908468413434,0.99720736109666419,0.99145251749730023,0.97729161337929626,1.0343818793245951,1.0173884214406497,null,6.7531043859500164,0,1.0626107584064758E-2,0.19729330229152398,0.12008731134116001,8.3069683114118581E-2,0,1.0626107584064758E-2,0.27635620420171331,5.9118276933389682,0,1.9129577844483835E-2,0.10398570076828417,-2.4015066047751608E-3,4.3756419654536249E-2]
[null,885,0.98635387594142077,0.98135324895343545,1.0346948439600083,1.0182689548482831,0.96429391344434889,0.98011079659929212,1.0256204440062704,null,6.7610040522615478,0,1.0128085292147248E-2,0.19877256943596541,0.1239356182811598,8.5451534086971329E-2,0,1.0128085292147248E-2,0.27903335119404882,5.9111366701172265,0,1.9230516441823473E-2,0.10284534997864446,-1.1072097753725329E-3,4.1705652501083358E-2]
[null,886,0.98577440045180487,0.97799793786800182,1.0012368766373234,1.0280632976474886,1.0263463337464738,0.99951210689362435,0.9852557536278993,null,6.7562814612840096,0,1.0657397062714883E-2,0.19905909106610264,0.12482565583482287,8.3263195833678361E-2,0,1.0657397062714883E-2,0.27003071150379343,5.9135799469421686,0,1.923376545012349E-2,0.10470656534561638,-2.3027348505967188E-3,4.3885264158297868E-2]
[null,887,1.0013039399202024,1.0257065072876657,1.0148049680722186,1.008629821305522,1.0106443207847793,0.99972727515714321,1.0112838306105194,null,6.7433760142471266,0,1.0161198696750692E-2,0.19364234383628179,0.12031826556429569,8.4121877899274958E-2,0,1.0161198696750692E-2,0.27243086433318553,5.9117610878245017,0,1.9147994315137949E-2,0.10117550002049236,-1.0639271533164579E-3,4.1842007607274044E-2]
[null,888,1.0360732301557876,1.0097165646986588,0.98247477169467312,0.99078455621159822,1.0137787391203601,1.0045692027186988,1.0134408717600059,null,6.721043684327527,0,1.0218877878044746E-2,0.18563303555475161,0.11759573787653951,8.1991759311760379E-2,0,1.0218877878044746E-2,0.26438674193557987,5.9126110982748594,0,1.8965282981074423E-2,9.8561515899077343E-2,-7.8100771544393599E-4,4.2079520209331422E-2]
[null,889,0.99318910992480036,1.0144744242906465,1.0031137515214392,0.99605998152961428,0.95388506319246169,0.97040156436817249,1.005418189278811,null,6.7362521760146743,0,1.0093349975702279E-2,0.18904865313045061,0.12205702402958228,8.3360488951757253E-2,0,1.0093349975702279E-2,0.27036753870743568,5.9117447362230724,0,1.9192478700347591E-2,9.9348434947405431E-2,-4.2979732600266691E-4,4.1562618650618846E-2]
[null,890,0.97610218853571751,1.0080735681488846,0.9669215975135691,0.99430301705202695,1.0072667122005494,0.9831740645062359,0.99470634326903984,null,6.7485970157284232,0,1.076802361121236E-2,0.19114474593170261,0.12519602088136331,8.1147475242726474E-2,0,1.076802361121236E-2,0.27338430138269881,5.9136532748888486,0,1.9288565256241733E-2,0.10228311403280174,-1.8412864821832273E-3,4.4340804594218894E-2]
[null,891,1.0027426384856113,1.0179598675063322,0.97961208457743487,1.0127383028448502,0.97280373324046954,0.98662479659266666,0.97981244585909788,null,6.7271587902096899,0,1.0359730858280899E-2,0.1873941760631391,0.12116264906721202,8.1805240112041197E-2,0,1.0359730858280899E-2,0.26238724391914497,5.9139557494774566,0,1.9140182707090145E-2,9.9639247542350443E-2,-9.852263897984952E-4,4.2659527711048008E-2]
[null,892,1.0038807344182212,1.0376680785791268,0.98357079113707291,0.99949956997534717,0.97166070724859821,0.97327560037618033,1.0269156278543516,null,6.7300624918245209,0,1.0089683277645039E-2,0.18358435036857698,0.12002839163051225,8.2185750633471694E-2,0,1.0089683277645039E-2,0.27325784812135478,5.9130216554618977,0,1.9134019123217064E-2,9.7420358585260977E-2,-1.174019404394571E-4,4.1547519840667055E-2]
[null,893,1.00212751323001,1.0206613629051544,0.96450456417489383,0.96994173456637633,0.99934125494475401,0.98632438848403314,0.96542788601423624,null,6.7193699274309457,0,1.0488274214138404E-2,0.18551170716634521,0.12138492634837447,8.0784982283193696E-2,0,1.0488274214138404E-2,0.25861915060835283,5.9124671566000107,0,1.9143519867873871E-2,9.9389744819558021E-2,-1.120106633371172E-3,4.3188846370604807E-2]
[null,894,1.0193744382373899,0.95833842037935413,1.0101477113325394,0.98574576136414183,0.99820315467344567,0.99206384983921325,1.0289293765974872,null,6.7436527632664971,0,1.0238722836853653E-2,0.19377933664185665,0.12152863525729249,8.3812367725619258E-2,0,1.0238722836853653E-2,0.27222166554176758,5.9107895532032897,0,1.9051478939370974E-2,0.1014803342654301,-1.1718465255706955E-3,4.2161238217435497E-2]
[null,895,0.99247325992012936,1.0268168554184354,1.0138901564876017,1.0273175459301107,1.012772356058202,1.0096500697961472,0.99734176143424069,null,6.750499373849137,0,1.0356856001947192E-2,0.19710396495217161,0.1213535008218609,8.4073431863311149E-2,0,1.0356856001947192E-2,0.27198333035164024,5.9128229449620306,0,1.9196437807989478E-2,0.1030306756344123,-1.7126021086556113E-3,4.2647689564371156E-2]
[null,896,0.97339001836131267,1.0107029905934442,0.98932404989922229,0.97872488927641421,1.0237664257069337,0.98079422034970953,0.98731008957171262,null,6.7482204795113452,0,1.0551853242728596E-2,0.19363873100208154,0.12498924908191747,8.2513159420148266E-2,0,1.0551853242728596E-2,0.27189578632226086,5.9115797664840128,0,1.9304127091081619E-2,0.1024609809020238,-1.6119742858732794E-3,4.345065349369398E-2]
[null,897,1.0042042735516798,1.0166748965723349,1.0275226390690158,0.96004892921114293,0.97576038769291029,1.0351274746903889,1.0129333465485419,null,6.7559036837964612,0,1.041379516754916E-2,0.20222467714683792,0.1201578105133068,8.491559270423206E-2,0,1.041379516754916E-2,0.27553632038532827,5.9084071242590142,0,1.9132269483317463E-2,0.10500011403115105,-2.352379640260617E-3,4.2882154913526378E-2]
[null,898,1.0003261885535664,0.98306427036748933,1.0129301024490851,1.000717437437513,1.0025101096533604,1.0054072836596735,1.0364931000986242,null,6.760803956061598,0,1.0433728185958417E-2,0.19828499747416622,0.12253453894766074,8.4108944646636541E-2,0,1.0433728185958417E-2,0.28048561988832638,5.9114403862953058,0,1.9153315972500161E-2,0.10369718846424737,-1.8652711626359223E-3,4.2964235535390687E-2]
[null,899,0.96702551240446144,1.0237988399849545,1.0036735409980897,0.97688247842861353,0.95385305831870448,1.0081777259751428,1.0330796852566775,null,6.7757785352842115,0,1.0722641610910934E-2,0.20100188189773641,0.12489065738850277,8.3633755124756418E-2,0,1.0722641610910934E-2,0.28900816779398081,5.9106768293978336,0,1.934098798964734E-2,0.10560074810443904,-2.5284220073580684E-3,4.4153929594672549E-2]
[null,900,1.0104129465743903,0.97019953635861989,1.0075882431694401,0.9711905813797741,1.0197263560582761,0.98082432030335853,0.96040271852344705,null,6.7235217998283927,0,1.0181525876395746E-2,0.19196801254106566,0.12205295821715141,8.3414290396469581E-2,0,1.0181525876395746E-2,0.25519613169534427,5.9101481127497282,0,1.9098911187012617E-2,0.10065916796123345,-9.4149623456385152E-4,4.1925711314949272E-2]
[null,901,0.99500168830939606,1.0133540324907082,0.96311677214384184,0.99254912129322703,0.98561474889628009,0.96891788188605221,0.98808917750889302,null,6.7261627553928856,0,1.0421506676434836E-2,0.18395114497123424,0.12263164659986092,8.0798369078606574E-2,0,1.0421506676434836E-2,0.26502738534322051,5.9137647745510451,0,1.9182479458537224E-2,9.8622620125924029E-2,-7.2957427005962438E-4,4.2913909534520185E-2]
[null,902,0.99864638131420091,1.0022781135537311,0.98020189219090681,0.98295334875420703,1.0334459152623652,0.97771096735317298,0.99573666001374528,null,6.732170179129068,0,1.0371658351115517E-2,0.1877741767453171,0.12240654258963715,8.1882568176629006E-2,0,1.0371658351115517E-2,0.2670519592154118,5.9123130935052526,0,1.916248307565023E-2,9.9811815333432669E-2,-9.4110251578674597E-4,4.2708643003526385E-2]
[null,903,1.0006116835401107,0.9850313764212123,1.0172192584238806,1.0037634453023845,1.0209033760646979,0.99302646571438125,0.99460514184266413,null,6.744280214255447,0,1.0254923225566741E-2,0.19612787031650097,0.12232027252098386,8.420634459144663E-2,0,1.0254923225566741E-2,0.26789196381322333,5.9113603321762032,0,1.915176101931311E-2,0.10235215923378443,-1.3584379506036215E-3,4.2227948534594301E-2]
[null,904,1.0306815068629458,0.97117829553453794,0.98474243440585885,1.0058333362998162,1.0310287125344879,0.99966754741156694,0.96885405910071032,null,6.7191438802254293,0,1.0373554556499878E-2,0.18907775575944519,0.12002398810888343,8.2006653411199795E-2,0,1.0373554556499878E-2,0.25402357615624077,5.9132992226864385,0,1.8992808701874905E-2,0.10027672873841272,-1.2733045768558492E-3,4.2716451239787206E-2]
[null,905,0.99787906164853679,1.0013301226844211,1.0208607896584045,0.99224992872109619,1.0118874221588967,1.0259476773586842,1.0137387731115408,null,6.7612039911231996,0,1.0515903091399551E-2,0.20220557859104146,0.1217837476046579,8.4544461112780592E-2,0,1.0515903091399551E-2,0.27678561058030243,5.9105298253898884,0,1.9166680788504874E-2,0.10533470646653993,-2.4492365799271814E-3,4.3302617169409377E-2]
[null,906,0.99355709435002615,0.99551028257698837,1.0217769226432243,0.98782994889800557,1.0060628808548193,0.99676411813177201,0.99121983904434074,null,6.747385080810326,0,1.0278620494088411E-2,0.19791098445806038,0.1225815432776198,8.4494030900920142E-2,0,1.0278620494088411E-2,0.26913037420138242,5.9102384826437975,0,1.9190445731606186E-2,0.10305103834716262,-1.5373484186360547E-3,4.2325529668409988E-2]
[null,907,0.97750940753727866,0.99531431217529087,0.98801275156533874,0.99535885370788579,0.96147078784762929,1.0267038766753396,0.99242968422691846,null,6.7689419739622636,0,1.1084408907864612E-2,0.20301663595367464,0.12525376252845177,8.2506930374904752E-2,0,1.1084408907864612E-2,0.2766965453864127,5.9125517237834879,0,1.9280524970200597E-2,0.10749346168645377,-3.5012336526753299E-3,4.5643622931349381E-2]
[null,908,1.0330994471312922,0.99805217109112032,0.99951488890128548,0.98798103628379763,1.0014983047767434,0.98640484579197585,0.96193185122910019,null,6.7058897383163556,0,9.9639042057689045E-3,0.18563186112072214,0.11817566393027126,8.2858472557504878E-2,0,9.9639042057689045E-3,0.25021220866362087,5.911510629105698,0,1.8980429147943019E-2,9.7727269879024053E-2,-2.3638009894813911E-4,4.1029584010521328E-2]
[null,909,1.0154427271657074,0.97622054246052914,1.0225953718987082,0.98773349807660693,1.0059393675447548,1.0132905159469059,1.0182034663269628,null,6.7496426129732576,0,1.0302539256865419E-2,0.19861181096757766,0.12086658127596975,8.4585886541302738E-2,0,1.0302539256865419E-2,0.27227972511149617,5.9101862828812655,0,1.9072186000424818E-2,0.10337430656852319,-1.7581892494521205E-3,4.2424022876144628E-2]
[null,910,1.0145994354048726,0.98553680580818104,0.99950710239619978,0.97396689857426821,0.99774269035405783,0.99119253859902146,1.0331832338724547,null,6.740874564550694,0,1.0250166352228439E-2,0.19096284623173657,0.12093952097076847,8.3170853732771374E-2,0,1.0250166352228439E-2,0.27423281447159009,5.9107536988391498,0,1.9076648249913414E-2,0.10053419537059556,-1.0043738927102109E-3,4.2208360576879059E-2]
[null,911,1.0266337917898705,1.0088075949573623,0.97231260474309866,0.98353177387558244,1.0244988748973962,0.96967105822972588,1.013117240293778,null,6.7127674267958044,0,1.0046989831925073E-2,0.1797789014629137,0.11890254057866496,8.1342962198982183E-2,0,1.0046989831925073E-2,0.26349043973884773,5.9127771469726751,0,1.9013663017215535E-2,9.5940727497708503E-2,1.4932949845177459E-4,4.1371715830342277E-2]
[null,912,0.98057304354664465,0.97641806905027628,1.0087716299926293,1.0293671912764708,1.022546396099892,1.0435045404309027,0.96306639922645731,null,6.772805009529355,0,1.1119772148341252E-2,0.21002588177414303,0.125423235840079,8.3724853077874625E-2,0,1.1119772148341252E-2,0.26949396265321213,5.9132246841207738,0,1.9263100390523855E-2,0.11006339293081703,-4.2033437192785109E-3,4.5789242461210029E-2]
[null,913,0.97932013182149014,1.0063897158480153,1.0186766200374644,1.0142473380453165,1.0082941315858205,1.0120645682117622,1.0131293394852736,null,6.7691885603758681,0,1.0567586619864899E-2,0.20254388497837358,0.12388380569721473,8.4476459449407376E-2,0,1.0567586619864899E-2,0.28044997304697472,5.9118433909028445,0,1.9270213211566474E-2,0.10562453180862608,-2.4191394594449815E-3,4.3515440740304542E-2]
[null,914,1.0111336937423583,1.0474557780871474,0.9883362195537212,1.009918745727135,1.0387179272970164,1.0075864345039798,1.0150584204168351,null,6.7343698131395708,0,1.0286053194257442E-2,0.18848472308945677,0.11863464512168193,8.2463148419344837E-2,0,1.0286053194257442E-2,0.27128230163948558,5.913320760775048,0,1.9095065255901659E-2,9.978298059542183E-2,-1.0499479615072298E-3,4.2356136204734732E-2]
[null,915,1.0385933218296923,1.0315620877077931,0.98732824727662771,0.99437396439031411,1.0077654325666696,0.98867733767749288,1.013569823768729,null,6.7101327093194714,0,9.8993352158323299E-3,0.18112746423134976,0.11622443756753663,8.2266130148483357E-2,0,9.8993352158323299E-3,0.26214284337494115,5.9125364826164892,0,1.8952515465329559E-2,9.5936332545213776E-2,1.8280296731495359E-4,4.0763700402814289E-2]
[null,916,0.96813827719215195,0.99855153589315304,0.97539368866445741,0.99217578982870824,1.0023497699109334,1.0097264328398754,0.9965702883258718,null,6.7683224620095341,0,1.111292549464233E-2,0.1997640692996126,0.12654422184520384,8.1746880473495362E-2,0,1.111292549464233E-2,0.27883246867391448,5.9130758732003184,0,1.9334508301685698E-2,0.10644125255407287,-3.1778614987095014E-3,4.5761049159936812E-2]
[null,917,1.0019494350274349,1.0277839380728473,0.97622552183011246,1.0062319671725795,1.032269411685514,0.97094887077038672,1.0018091542562977,null,6.7251654195384329,0,1.0191382962128697E-2,0.18342488544832153,0.1208555845302519,8.1649808162343532E-2,0,1.0191382962128697E-2,0.26693919680997535,5.9137901762867982,0,1.9144486737715394E-2,9.7694397732355359E-2,-2.9941720883380242E-4,4.1966301039501705E-2]
[null,918,0.99777180002403354,0.97519233405388162,0.99111761172860635,1.0275178740612358,1.0405199634866553,0.97405164655061705,0.99207782611013851,null,6.7389045855027492,0,1.036486740307528E-2,0.19071376896196077,0.12365814341291516,8.2582559406001219E-2,0,1.036486740307528E-2,0.26623207484196237,5.91411725432949,0,1.9167268090229072E-2,0.10082307443031926,-1.0702370583673564E-3,4.2680679088240386E-2]
[null,919,1.0031589837403763,1.0367798515443973,0.97103949248165367,0.96879043565237632,1.0193537226409042,0.96441219090996733,0.99997836004804863,null,6.7172128657656041,0,1.0118547267552605E-2,0.18071744703879664,0.12038407321136974,8.1280500379082798E-2,0,1.0118547267552605E-2,0.26544709639157982,5.9120496292754945,0,1.913792628464521E-2,9.6503298268746762E-2,2.6518302383105757E-5,4.1666376613507729E-2]
[null,920,0.99104370345000581,0.98706788707204951,1.00792107237788,0.9598979684717045,0.98630621185980605,0.99659741227358634,1.0032972730761316,null,6.7513351318637858,0,1.0466756532036004E-2,0.19744318154920737,0.12357701571604499,8.3670031799616518E-2,0,1.0466756532036004E-2,0.27314748746463341,5.9095190665354709,0,1.9204361283781668E-2,0.10351303655977483,-1.8392894304614892E-3,4.3100240385711752E-2]
[null,921,0.99019843353695736,0.97215738182253797,0.96057802525150471,0.99126684038535395,0.99463182557471397,0.99583558425531815,0.99826819317498283,null,6.7506319916111526,0,1.0980302662512889E-2,0.19308486744932768,0.12533698168702823,8.0730201524595202E-2,0,1.0980302662512889E-2,0.27201521939852574,5.9138326517068629,0,1.920905704938412E-2,0.10365218392250684,-2.4441030702911691E-3,4.5214931943211877E-2]
[null,922,1.0119643135565954,1.0241303276952829,0.99019798643675105,1.0198197730893235,1.0363416372421779,1.0018822870535993,0.99747925682243987,null,6.7317106702804193,0,1.0301599685033214E-2,0.18929139500592357,0.1195759251621424,8.2516461413688361E-2,0,1.0301599685033214E-2,0.26605200568422571,5.9137523892720942,0,1.9090639835356107E-2,0.10011700924014763,-1.1053092197385117E-3,4.2420153886577147E-2]
[null,923,1.0068690484745033,0.99124627035026891,1.0012178607431206,1.0228044341931422,0.97787983893069608,0.97854087807161383,1.0033160244479993,null,6.7349281212109604,0,1.0156625201169476E-2,0.18970031971960094,0.12155482921740471,8.3217388834830847E-2,0,1.0156625201169476E-2,0.26710255527826854,5.9132968197446694,0,1.9117901642168783E-2,9.9784723756746824E-2,-6.6959174925502595E-4,4.1823174766522468E-2]
[null,924,1.0275438371081671,1.0098510373009568,0.99888811242098163,0.99253932530831235,1.004029056158281,0.96165768670910012,1.0195506404048615,null,6.7133620571435948,0,9.7227374947569719E-3,0.18097069086468162,0.11826874423066112,8.301085422236712E-2,0,9.7227374947569719E-3,0.26421840037883537,5.9117921658305574,0,1.900896003705229E-2,9.5303033065974069E-2,7.5270609281881612E-4,4.0036502420648552E-2]
[null,925,1.0123718903516143,0.96903590096048464,1.0414410340586508,0.95710579977452914,1.0316377886777663,0.95807838820018842,0.97012973263004887,null,6.7182178769859915,0,9.6411265495509497E-3,0.1911107749696295,0.12123336664634506,8.5492591957635505E-2,0,9.6411265495509497E-3,0.25526607773965837,5.907440081322596,0,1.9088470981867472E-2,9.855547858063915E-2,3.3059171312668138E-4,3.9700443074496862E-2]
[null,926,1.0372899016392856,0.98398788625351574,1.0338123787770845,0.99645980564812986,0.99717498165715246,0.98853212923588474,0.96313858307155398,null,6.7103384711496394,0,9.7098505280614356E-3,0.19031600193837342,0.11773975609228014,8.4976553148951792E-2,0,9.7098505280614356E-3,0.24988406137619651,5.9100099421368189,0,1.8959111224795357E-2,9.8512469336706932E-2,-4.2860290075215834E-5,3.9983436185590873E-2]
[null,927,1.0320073482726559,0.99679382615884538,0.98644583780694539,1.0276064348601326,0.95866880499718177,1.0148179516706077,1.0441411056151622,null,6.7406844040537361,0,1.038510574554353E-2,0.18976709343667769,0.11859724212973281,8.2400541385927839E-2,0,1.038510574554353E-2,0.27458635277095716,5.9143817822650231,0,1.8986013375088436E-2,0.10055671013950047,-1.3553484294070446E-3,4.2764016980233958E-2]
[null,928,0.98240483660151368,1.0098078188054407,0.9892314445699204,1.0029071978332027,1.024807114074717,1.0279772823003437,1.0216553448385739,null,6.7716920123523732,0,1.0963030234170073E-2,0.20115668399331321,0.12388796535682189,8.2676754367220787E-2,0,1.0963030234170073E-2,0.28338630176521029,5.9128920139334822,0,1.9252733893984405E-2,0.10644390789283202,-3.1481560081704331E-3,4.5143807157673799E-2]
[null,929,1.0080302047257095,0.97746884024153569,1.0268376739074672,1.0092913988357606,1.0086463023710075,0.98157541520334135,1.010177114131378,null,6.7413444613827114,0,1.0010693790755049E-2,0.19420011213030425,0.12161263190787111,8.4821096967445872E-2,0,1.0010693790755049E-2,0.2690869212637616,5.9111066882192871,0,1.9111664722227903E-2,0.10086748730739054,-6.8439632883810354E-4,4.1222255193258603E-2]
[null,930,0.96616344521143305,1.0239490459768006,0.98561754040295468,0.99368301819353033,0.97843790943741826,0.99776873508767139,0.96117251393924386,null,6.7510016259222247,0,1.0789487390957853E-2,0.19691432752731011,0.1253407645058692,8.2243939236574581E-2,0,1.0789487390957853E-2,0.26813322069520201,5.9125939756373551,0,1.9346018112880062E-2,0.10438717426310234,-2.3869826748703182E-3,4.442918861880045E-2]
[null,931,1.014145318208693,0.98668380212534634,1.0277991769281682,0.99408817372196412,0.97019424154035028,0.98389547933792498,0.97950375439985182,null,6.7272069834112198,0,9.9254532639342172E-3,0.19282042189282556,0.1204083920903882,8.4737294614113876E-2,0,9.9254532639342172E-3,0.25946873176795587,5.9102299361260648,0,1.9079054269632412E-2,0.10010359479795977,-5.1169202377416699E-4,4.0871249876058599E-2]
[null,932,1.0271396554902614,1.0357297865032709,1.0004819823526554,1.0252004132467083,0.98918461284886205,1.0175079057065439,1.0069876651495486,null,6.7290260044037939,0,1.0166446411795671E-2,0.18967687174089587,0.11709513847366086,8.3156669031921523E-2,0,1.0166446411795671E-2,0.26595708052510769,5.9134677088843928,0,1.901104775941655E-2,9.9808846852604577E-2,-1.0109756279785081E-3,4.1863616763770817E-2]
[null,933,1.0041833737174901,1.0071629915658793,0.99914222626185478,1.0241958980537502,1.0116784759437878,0.98762332290829524,0.99945436842177016,null,6.7362446263657603,0,1.0226946121273525E-2,0.19042727841621374,0.12114441523670484,8.3094905227482863E-2,0,1.0226946121273525E-2,0.26748680083379039,5.9134887298148024,0,1.9132382471699537E-2,0.10027041398259751,-9.130434163896285E-4,4.2112743798853769E-2]
[null,934,0.96743159634458165,0.970577687615373,0.97741725476083652,0.99284485814066148,1.0155899097708652,1.0440527658538024,1.0318094976094947,null,6.7991260533371207,0,1.1619492751067889E-2,0.20949824215116725,0.12804497820600166,8.2056700227519819E-2,0,1.1619492751067889E-2,0.2927298524698147,5.9130010051888986,0,1.9338621614170715E-2,0.11151474630774193,-4.9050957844842423E-3,4.7847002956286834E-2]
[null,935,0.99245128379778791,1.0104736307724023,1.0207782924981488,0.98936430592145075,1.0003600802064694,1.0108992087103867,0.99611369929449844,null,6.75230081114056,0,1.0378600848326461E-2,0.19954110396056554,0.12200694124991336,8.4471747176156728E-2,0,1.0378600848326461E-2,0.27194357474714503,5.9103786602781563,0,1.9196559440338136E-2,0.10395092774459715,-1.9259344276393075E-3,4.2737230971322607E-2]
[null,936,0.99220301579555681,0.98935618944471648,0.96771075272455009,1.0338713802940993,0.99571624180180895,1.0283037463699156,1.003028703336033,null,6.7630594880497936,0,1.1161174761018007E-2,0.19835595722669558,0.12407650361056118,8.125370835367729E-2,0,1.1161174761018007E-2,0.27569644570860646,5.9157498533850355,0,1.9197933915986887E-2,0.10609974168940894,-3.3303868910061207E-3,4.5959731050822565E-2]
[null,937,1.0013271559670505,0.95538056200384103,0.97705731144268804,1.0193216740236719,1.0321962182618996,1.0068802878376406,0.96675221640337428,null,6.7447901969377639,0,1.0903424435536687E-2,0.19648262589224791,0.12450077450081155,8.1642440558021098E-2,0,1.0903424435536687E-2,0.26173399362385807,5.9144521729752322,0,1.9147868082286346E-2,0.10460547869040543,-2.6735184734401523E-3,4.4898361088338161E-2]
[null,938,0.98730414895556495,1.0113180471626342,1.0102385169917307,0.98263406228589711,0.99851294896665432,0.98928577355903025,1.0120261865226901,null,6.750322471948528,0,1.0300563554760601E-2,0.19497594968843251,0.1228026519631861,8.3863988429753386E-2,0,1.0300563554760601E-2,0.27562223069931602,5.9106162625149734,0,1.9225196697990526E-2,0.10210240326092114,-1.3020985925930447E-3,4.2415887286538841E-2]
[null,939,0.97783040237934671,1.0215385656329148,0.99857172528129445,1.0056088603403108,1.0200361340446329,1.0223637783287816,1.0019583258737776,null,6.7660334818010819,0,1.0811628391961942E-2,0.20114405989101594,0.12371686799185361,8.3196420912630201E-2,0,1.0811628391961942E-2,0.27857539329998693,5.91251625101944,0,1.927869417564123E-2,0.10594341435664288,-2.8579811661111599E-3,4.452036131998402E-2]
[null,940,0.9737903399913288,1.0195958054610312,1.0144597115030622,1.0164931977218714,1.0048587521593106,1.0153326152378013,1.0338620619384546,null,6.7777289959358207,0,1.064177252746828E-2,0.20269706533533008,0.12402045006510086,8.4319055170658672E-2,0,1.064177252746828E-2,0.28799042200246394,5.9122056336323565,0,1.9301824680636213E-2,0.10592452196306824,-2.5509020170134651E-3,4.3820925103215967E-2]
[null,941,0.99841565848233316,1.0004772054154918,1.0448648512524072,0.98819572662954858,0.99908744198700872,1.0119691286093073,1.0042055233621112,null,6.7547196612007081,0,1.0154876171527931E-2,0.20231490731991958,0.121302376419983,8.5969716070972285E-2,0,1.0154876171527931E-2,0.27276145592052625,5.9089186909588669,0,1.9163744593785888E-2,0.10415926638665755,-1.6864690437808406E-3,4.181597257377425E-2]
[null,942,0.97526307287504344,0.97963610249826694,1.0299744597186635,1.0078321983746525,0.96361701185013182,0.9928937879613563,1.0301492985982217,null,6.7751843139097678,0,1.0427712412931714E-2,0.20323023163182635,0.12552570962764245,8.5230916779218055E-2,0,1.0427712412931714E-2,0.2847464663041902,5.9108466523347127,0,1.9293370670144354E-2,0.105395309366141,-2.0238064569456254E-3,4.2939463652834416E-2]
[null,943,0.98018606510204576,0.98487665687623127,0.97529394745432796,1.0178839123552847,1.0127528249656865,0.97811289107541644,1.026608658438434,null,6.7589522209341268,0,1.0696608653928161E-2,0.19225196602705616,0.12568203243884721,8.1782788885566893E-2,0,1.0696608653928161E-2,0.28071857221911511,5.914471221486135,0,1.9265295339057714E-2,0.10244366813613306,-1.7100541092973881E-3,4.4046730511511104E-2]
[null,944,1.0062745415839098,0.9563839784159428,0.99538842736894806,1.0067488558354483,1.0009327224904692,1.0178070281837723,1.0206722285089755,null,6.7612584139782266,0,1.0788731213542926E-2,0.19977350313559444,0.1234914658697904,8.2963507336354284E-2,0,1.0788731213542926E-2,0.27605811425575205,5.9127562442537194,0,1.9121100489089504E-2,0.10538822192412524,-2.7198181010008281E-3,4.4426074814800341E-2]
[null,945,1.0076974395488454,0.97322565973725839,0.97851467209171317,1.0325155341743342,0.96866397528053816,0.99467298211772659,0.99742305411021592,null,6.7411202509139416,0,1.0605043724035729E-2,0.19151946025394725,0.12277421808351482,8.1811134648196962E-2,0,1.0605043724035729E-2,0.26697441853093906,5.9150853307141498,0,1.9113450634873557E-2,0.10188869236925802,-1.7161367491067955E-3,4.3669682428164019E-2]
[null,946,0.99280101012605204,0.96475340189119729,1.0019768156107807,0.98846701574760598,0.99905028180679079,0.98767671156233794,0.98836924910087542,null,6.7478028999681134,0,1.0511182825349453E-2,0.19654340678215496,0.12460584536747385,8.3252508598084696E-2,0,1.0511182825349453E-2,0.26798642117442101,5.9113984565967526,0,1.9194624431463976E-2,0.10334533740937291,-1.8068803456032707E-3,4.3283179953991092E-2]
[null,947,0.97568088292945954,0.99514045799880513,0.9903985724341452,0.99376722433924558,0.99437740656332019,0.97325810872134377,0.97896332811739062,null,6.7450561133437699,0,1.0505989003426306E-2,0.19310445533496012,0.12545159734658212,8.2544043041346687E-2,0,1.0505989003426306E-2,0.26839435400112177,5.9123330573580901,0,1.9290976939102956E-2,0.1021235385268813,-1.4477019240983291E-3,4.3261792719777419E-2]
[null,948,1.0010090100116742,0.98224928962149305,0.9690583814976873,1.0326979442883291,1.0208378286551809,1.026190812562271,0.98571493589917714,null,6.7524845269315428,0,1.1061434236938696E-2,0.19697716391463169,0.12331513869065636,8.1241507649215713E-2,0,1.1061434236938696E-2,0.26844067622793349,5.9156130200057042,0,1.9149598450252148E-2,0.10529082149860061,-3.0924168312685468E-3,4.5549017325815427E-2]
[null,949,0.98304600927398389,0.98929787878616871,1.021924720931926,1.0114722393842377,0.97409939673277712,1.0068353779028296,1.0224793790416444,null,6.7704203346258751,0,1.0520308366333072E-2,0.20260888063314317,0.12419998475956159,8.4691781095915949E-2,0,1.0520308366333072E-2,0.2816442673215625,5.9115072502140045,0,1.9249114492930573E-2,0.10548952955016191,-2.2912307488893932E-3,4.33207573074759E-2]
[null,950,1.0432573770731546,1.0061332899302824,0.96709988867633156,1.0003154886101653,1.0026035264194226,1.0166264988891873,1.0060398322788349,null,6.718724538149317,0,1.0424655648906135E-2,0.18509857582571362,0.11722422988659845,8.1006173486591046E-2,0,1.0424655648906135E-2,0.26175036227413678,5.9139686858493619,0,1.8929048726676698E-2,9.9038870155323658E-2,-1.2182844977442016E-3,4.2926876442660807E-2]
[null,951,0.97867588404338668,1.0126565988309464,0.99013759935931422,0.98122985610938507,1.0245449340943387,0.97474133016044717,0.98568322654392593,null,6.7413132218551235,0,1.0414079208319228E-2,0.19134106973336029,0.12420276910392447,8.2531888992376568E-2,0,1.0414079208319228E-2,0.2693941536250215,5.9116699220229982,0,1.9273877717263712E-2,0.10120413807429983,-1.1879219569818616E-3,4.2883324542860146E-2]
[null,952,1.0013934313927106,1.0304858283673106,1.0087229074938326,0.98580358346057484,1.0269188149592343,1.0243743183594376,0.99739196964399957,null,6.7464722075741772,0,1.0445514209441705E-2,0.19727653207535589,0.12019709833228774,8.3707477179878934E-2,0,1.0445514209441705E-2,0.27089586513410413,5.9108734776342029,0,1.9147507754433336E-2,0.10338462958668015,-2.0231484050315641E-3,4.3012768282260909E-2]
[null,953,0.96935880262953567,1.0049998395259172,0.98922666778788859,0.95793495790480998,1.0253414251059814,0.96855852112193497,0.97944443742978593,null,6.7439660775651298,0,1.0489825028763226E-2,0.192472649345204,0.12579531476978353,8.2463852044850031E-2,0,1.0489825028763226E-2,0.26973997619201384,5.9104614436441842,0,1.9327418225096968E-2,0.10184891383848582,-1.338722843686576E-3,4.3195232349195097E-2]
[null,954,0.99046757891915815,1.0050984810379375,0.9646298955624969,0.99115864634342588,1.0185694493580533,1.0091400665564478,1.0319849058487891,null,6.7590347933120203,0,1.0927677603761005E-2,0.19331965553187466,0.12356871640756791,8.1114514293390894E-2,0,1.0927677603761005E-2,0.28208456729460712,5.9136076293217119,0,1.9207560984343518E-2,0.10356639030100026,-2.4324721406575817E-3,4.4998231318182896E-2]
[null,955,0.96527227094931045,1.0144512714588321,1.0094021508370463,1.0157723995156254,0.99553053347107723,1.0382398578146781,1.0353164000601753,null,6.7946513198349123,0,1.1050465102180562E-2,0.20891176080585397,0.12546646162551223,8.4076300773489696E-2,0,1.1050465102180562E-2,0.29328831953160356,5.9124543264081248,0,1.935122751933387E-2,0.1094453915484524,-3.8463167587724435E-3,4.5503848381314625E-2]
[null,956,1.0139050636397107,1.0168752465996924,1.0187600783007171,0.99899343593970191,0.99402450818521415,0.98734472539560281,0.98148542191448607,null,6.7231127206825176,0,9.9129941444000957E-3,0.19002108425990527,0.11916142781070418,8.4191102398570083E-2,0,9.9129941444000957E-3,0.26008095251445495,5.9110144959174269,0,1.9080328066610988E-2,9.9089945431305643E-2,-3.4656115591951049E-4,4.0819945439457689E-2]
[null,957,1.0118348392951062,1.0377099527914275,0.99756113142429248,0.9682752774772766,0.98811514773995879,0.99642705868068759,1.0309374949116044,null,6.7341324699160925,0,1.0123949184079304E-2,0.18806836533414484,0.11882879035070594,8.304806401355827E-2,0,1.0123949184079304E-2,0.27438403177891485,5.9105552569557789,0,1.909132917722468E-2,9.9106159261845031E-2,-6.3814770033747642E-4,4.1688620744259351E-2]
[null,958,0.98697665596843553,1.0146644434848437,0.96462681861180899,1.040837566279863,1.0033686957683932,0.98237971133001745,0.98366730223935039,null,6.7384593016512442,0,1.0632343270014248E-2,0.18809408721395632,0.1235368682298229,8.0955936307048962E-2,0,1.0632343270014248E-2,0.26723494627820393,5.9162940884314068,0,1.9227028886700311E-2,0.10076707305197849,-1.4328238472356954E-3,4.3782097099365522E-2]
[null,959,0.97856321983718764,1.0079298303658031,0.96974608584429922,1.0033087767686626,0.9903586307059471,1.0047023393253667,1.0160262115751926,null,6.7621929742120326,0,1.0949847707482013E-2,0.19518929301312685,0.12483520399571731,8.1425067946326882E-2,0,1.0949847707482013E-2,0.2806474439572062,5.913986498263978,0,1.9274519051208309E-2,0.10429906868116662,-2.5536445558727414E-3,4.5089523859174661E-2]
[null,960,0.99434442812480017,0.99230374849005265,1.0202894158677029,0.98290193930495373,0.99223535652596917,1.0297601286979818,0.98947792583946648,null,6.759771433962352,0,1.0638989361030618E-2,0.20439951942707724,0.12267104845577517,8.4431659113687219E-2,0,1.0638989361030618E-2,0.27158022596341874,5.9100575525721535,0,1.9186101077065185E-2,0.10650755921756989,-2.8716963836081196E-3,4.3809464519210833E-2]
[null,961,0.99969402268913765,0.98566389429344392,1.0140991707996712,1.0066978855225992,0.99152903623831468,0.97015802322685885,0.98681963071741963,null,6.7334329905018713,0,1.0052609034239492E-2,0.19137295167617879,0.12246038635807815,8.3961140608798168E-2,0,1.0052609034239492E-2,0.26388589663587714,5.9116969384975473,0,1.9156762234949595E-2,0.10002462183786565,-5.2056205271571474E-4,4.1394854705292333E-2]
[null,962,1.0255296372097944,1.0199688264251245,0.96611416055768662,0.97875334403254932,1.010547434049472,0.97402812292593166,1.0133883429975046,null,6.7124709642718488,0,1.0109935058340146E-2,0.17924784193242371,0.1186185033180812,8.0961977704436083E-2,0,1.0109935058340146E-2,0.26414525858194932,5.9128563330334156,0,1.9019380332581749E-2,9.595598430193944E-2,3.4771998131413014E-5,4.1630913068886902E-2]
[null,963,1.0004400312987021,1.0190047121064767,1.0310483403751369,0.97717108592811874,0.98923800861132838,0.95357526959755079,0.97348561916051835,null,6.7164347297606559,0,9.5903366102572454E-3,0.18720717665950229,0.12043308440405708,8.4911038529613611E-2,0,9.5903366102572454E-3,0.25836190970439937,5.9091282947602393,0,1.9152695819712011E-2,9.7034620639933761E-2,7.1461009844227144E-4,3.9491299144757588E-2]
[null,964,1.0053771444156974,1.0200628817373287,0.95823931966589104,1.0241127782911055,1.0033949580932979,0.9977755161969154,0.97085269576422795,null,6.7255650837256242,0,1.0636210442684391E-2,0.1863852708937361,0.12113461613671275,8.0453456095964479E-2,0,1.0636210442684391E-2,0.26025978533057459,5.9157349933345245,0,1.9125936254699369E-2,0.10017392086889668,-1.5009166175756819E-3,4.3798021428090105E-2]
[null,965,1.038273076663712,1.0215921336754574,1.019499279016195,0.98846893248171019,1.0188250444461759,0.99786109606492712,0.95550190383019695,null,6.702676464666439,0,9.7577697598206017E-3,0.18725026322135768,0.11613618019042538,8.4064736455004341E-2,0,9.7577697598206017E-3,0.24812018207613454,5.9104035762502374,0,1.8954134482689955E-2,9.7609489287000931E-2,-4.2856349083762721E-5,4.018075905266983E-2]
[null,966,1.0148133846631473,1.0155385703625905,0.9885123060207357,0.97620846079921397,0.99701592913471038,1.0487992469205978,1.0288017226203308,null,6.7555465909728722,0,1.0808466842812984E-2,0.19810930558060033,0.11967349820114512,8.2541136825374339E-2,0,1.0808466842812984E-2,0.27816859840505198,5.9114888506432379,0,1.9075515442654532E-2,0.10486897735885609,-2.8866341073727148E-3,4.4507342623323405E-2]
[null,967,0.97261380984786205,1.0323322954333962,0.99357358205093438,0.99680456645411297,1.0263054154437052,1.0229921962598056,1.0208762833756191,null,6.7725760646370858,0,1.0874850167726987E-2,0.20082725226986409,0.1239534876757023,8.2969140988354423E-2,0,1.0874850167726987E-2,0.28529732061341945,5.9123202199585849,0,1.9308596778193639E-2,0.10603986289036184,-2.9205138769293373E-3,4.47806973395279E-2]
[null,968,0.98104936926716113,0.98014310981443542,1.0348382406580785,1.0135185200098218,0.97476136334299512,1.0372376805699126,0.97702920973805807,null,6.7746989651920639,0,1.0780711920884659E-2,0.21162577768496868,0.12466444379598665,8.5369839285532906E-2,0,1.0780711920884659E-2,0.27267345458580122,5.9108717500968089,0,1.9260401040139274E-2,0.1094879396442424,-3.6476937364325851E-3,4.4393052795014494E-2]
[null,969,1.009225838550371,0.98024106619704066,0.99359689383928129,1.0141077906031279,1.0061939387448058,1.0069640347115671,1.0410133534974708,null,6.7557858374098254,0,1.0547205346495624E-2,0.19478332346532334,0.12195621363194553,8.2901369854103846E-2,0,1.0547205346495624E-2,0.27937475180106369,5.9132541258627773,0,1.9105257610057956E-2,0.10284738213869271,-1.8681012384392007E-3,4.3431514284301302E-2]
[null,970,0.97487468717792636,1.0069709553710304,0.99228349197138477,0.99744817127438778,1.0105720882490024,1.0022364419620584,1.0001466685880158,null,6.7614065600257218,0,1.075537102553405E-2,0.19824136664441575,0.12492722877578159,8.2780101160114056E-2,0,1.075537102553405E-2,0.27711814102126503,5.912426997412747,0,1.9295597662336954E-2,0.10474175656595855,-2.4133327153707911E-3,4.4288703498471922E-2]
[null,971,1.0123275066801785,0.98519943716424152,0.96759115522967054,1.0237311635978215,1.0002003406888256,1.0275661147016941,0.9865439726401386,null,6.7440051728991781,0,1.0952330655292053E-2,0.19460982087675943,0.12181710517814484,8.1107714706771958E-2,0,1.0952330655292053E-2,0.26575358206435645,5.9152080743770146,0,1.9088707077606897E-2,0.10410221498295363,-2.7817945607360567E-3,4.5099748196308159E-2]
[null,972,0.9956361204915295,1.025107527246873,1.0295573014669361,0.98221304998795567,1.0172807648463191,0.97481813055794875,1.0016154143945393,null,6.7348553817698331,0,9.8389918674015447E-3,0.1916381897267008,0.12075366171565409,8.4969663853528263E-2,0,9.8389918674015447E-3,0.26905569403273177,5.9094869006292576,0,1.9178988161625429E-2,9.940401319163196E-2,-1.4694677599426921E-4,4.0515217234691925E-2]
[null,973,1.0262590527096365,1.0027598317455086,1.0190758971045826,1.034238551982462,0.99386429325296222,1.0165534295874343,1.0467932650476435,null,6.7481964311117553,0,1.0141115326673918E-2,0.19448476079024768,0.11838126286819937,8.4465332103762156E-2,0,1.0141115326673918E-2,0.2769853659823745,5.9129005840948219,0,1.901560203803156E-2,0.10140182732160663,-1.1976119512915875E-3,4.1759307864004495E-2]
[null,974,0.98264828125418846,0.96582489536087035,1.0333023227833336,1.0226746103412718,0.98141578735999202,1.0032325973713898,1.0005732327947447,null,6.7695332422520806,0,1.0490318289685012E-2,0.20545847994170996,0.12522656770482407,8.532258564868353E-2,0,1.0490318289685012E-2,0.27565732436423174,5.9114555199387038,0,1.9251359099789051E-2,0.10637718279782155,-2.4130407535591972E-3,4.3197263509873844E-2]
[null,975,0.99529826503144492,0.99169090171335195,1.0059041173024843,1.0219156290629352,0.96949253829006377,0.99100036678410564,0.99025875986317369,null,6.7447515156037188,0,1.0361007366023566E-2,0.19486550065923652,0.12285722310562963,8.3518592442125519E-2,0,1.0361007366023566E-2,0.26786779574608927,5.9129844093242863,0,1.9180846835061112E-2,0.10226373882015742,-1.4513754715921058E-3,4.2664784142722401E-2]
[null,976,1.0124036928683382,1.0195569821206634,0.97336271806829755,1.0359359496837321,1.0073792292686103,1.0026597038054368,0.99918458141576483,null,6.7323987941788097,0,1.0477535797583499E-2,0.18777549572863686,0.12004466361334089,8.1485678094055672E-2,0,1.0477535797583499E-2,0.26647642745087319,5.9155530039407349,0,1.9088301823403847E-2,0.10015535612421383,-1.3247600790479656E-3,4.3144627482598584E-2]
[null,977,0.99691721831823665,0.97638978626338779,1.0115662136887567,1.0072656153640156,0.99462954404516024,1.0021270921346297,1.0031379975546402,null,6.7543141498664507,0,1.047826074964203E-2,0.19872971495804009,0.12331509400706774,8.391658700522199E-2,0,1.047826074964203E-2,0.27214482766336101,5.9118717772452314,0,1.917195179282075E-2,0.10399983197740377,-1.9832474888406494E-3,4.3147612706138976E-2]
[null,978,0.99875579622199495,0.97849643580485268,1.0213651135798123,0.98212102911871679,1.0250298780238116,1.0138826971354125,1.0002100517874697,null,6.7559976011196348,0,1.0481620890625237E-2,0.20169678718758138,0.12279510482716458,8.4502567822150279E-2,0,1.0481620890625237E-2,0.27196510070032087,5.9099536905148806,0,1.9161885033913108E-2,0.10504357538279165,-2.2825595177969945E-3,4.3161449168625014E-2]
[null,979,1.0126132997254487,1.0175049797255538,0.99997051750622468,1.0038079726066558,0.95099389594358885,1.0212598546816412,1.0005685578518473,null,6.7408302531896487,0,1.0433898188633191E-2,0.19451931283767093,0.11963075276394095,8.3145546037227944E-2,0,1.0433898188633191E-2,0.26857424584887979,5.9123403648284816,0,1.9087187184545364E-2,0.10238296241051836,-1.815054297763672E-3,4.2964935576146057E-2]
[null,980,0.97678953485820896,1.0229581235227259,1.0275258763595492,1.0035014094731443,1.0376851551500967,0.97771784056147559,0.9723652260326946,null,6.7428011474004048,0,1.0085637314985253E-2,0.19585314276616145,0.12322605646023621,8.4826646484578674E-2,0,1.0085637314985253E-2,0.26652168470306831,5.9107542057097371,0,1.9284635140234336E-2,0.10169169223490393,-8.877753851097987E-4,4.1530859286588548E-2]
[null,981,0.98174864401450679,1.0078858669550221,1.0003267192041478,0.95804030531118201,1.0323412798509912,1.0306605853233475,1.003105615025345,null,6.7669685322753743,0,1.0901850584652156E-2,0.20335063594063141,0.12385469171732308,8.3272860348655955E-2,0,1.0901850584652156E-2,0.2787254128755482,5.9098469474932953,0,1.9256442977043872E-2,0.10701229471503192,-3.2426340426861002E-3,4.4891880250530689E-2]
[null,982,1.0325639353337366,1.0068673908292378,1.0217813976591998,1.0269660466765682,0.99665956017846336,1.0144292217812465,0.9826027109483223,null,6.7249126649389277,0,1.0016784821996019E-2,0.19287071334871589,0.1174167474590707,8.4371196728905015E-2,0,1.0016784821996019E-2,0.2581861400909834,5.9123525178445702,0,1.8983165903462176E-2,0.10042637881249583,-9.4153222502284326E-4,4.1247336975745771E-2]
[null,983,1.0228150015288302,0.95709665958603019,0.99409829837452801,1.0093630942747891,0.98265719277477337,1.0133862265511708,1.0241191616021816,null,6.7485441614173469,0,1.057668810530232E-2,0.1954730179700512,0.1214822214356939,8.2830841688696408E-2,0,1.057668810530232E-2,0.27207473859922238,5.9129696726686189,0,1.9033489204445E-2,0.10318578452327,-2.0585237099837563E-3,4.3552919037331814E-2]
[null,984,0.98946387390936352,1.005464175206668,0.99910129373872225,1.0438015836771872,0.99222721629781696,1.0116661821344994,0.96023835530760304,null,6.7467564601576155,0,1.0639823504288635E-2,0.19810310325465855,0.12303041102555216,8.3047859697882989E-2,0,1.0639823504288635E-2,0.26302394918970817,5.9145505880642366,0,1.9213144296714862E-2,0.10431427834918422,-2.339773093000578E-3,4.3812899372675372E-2]
[null,985,0.97532386560521667,1.0164089611005147,0.99702634646351884,1.0069352996210155,1.0419511195617399,0.97199401748721037,0.99010435684016607,null,6.7452078744896458,0,1.0341554925804807E-2,0.19195856153182944,0.12431429602950748,8.3003538316501466E-2,0,1.0341554925804807E-2,0.2712509894810311,5.9126746064888138,0,1.9293022246950845E-2,0.10118307085076456,-1.0548929120581055E-3,4.2584682456306824E-2]
[null,986,0.9877722803053921,0.97515081410223703,1.030477845132568,0.99550731078521237,1.0205724051880163,0.98356010554593043,0.98851889927736969,null,6.7506925826551534,0,1.0214447411346911E-2,0.19922200106936086,0.12415396855712217,8.5035327140156769E-2,0,1.0214447411346911E-2,0.26893708463970439,5.9101517724996535,0,1.9222579804960824E-2,0.10329112985400077,-1.3825572458697414E-3,4.2061276336063408E-2]
[null,987,1.0106420378195227,0.97754050792682823,0.98091663750003344,0.97935260443058114,0.97863639650142931,0.96026083545862273,1.0086911724182117,null,6.724960290782704,0,1.0167665377692576E-2,0.18427628101199403,0.12215557996115994,8.1908325887152925E-2,0,1.0167665377692576E-2,0.26589286015235414,5.912079059049276,0,1.9097688153738884E-2,9.7917459480655292E-2,-2.3559916198720156E-4,4.1868636248366425E-2]
[null,988,0.95216492145063913,0.97555140702821219,1.0356357242601688,0.9685487227234888,0.96436349642831742,0.99928618660072088,1.0217001811368125,null,6.7926706276759035,0,1.0715396506498021E-2,0.21059164479200801,0.12867158120930966,8.5626052434065264E-2,0,1.0715396506498021E-2,0.28997234685721984,5.9083964571268606,0,1.9428973673028455E-2,0.10891038783518729,-3.0509117960594288E-3,4.4124095544280692E-2]
[null,989,0.98210251286325867,1.0122269562392006,0.9777698089609268,0.98504291359740848,0.98696682632736354,1.0134651958757808,0.99424282801141606,null,6.7558625852455911,0,1.0909006667089152E-2,0.19679118065666718,0.12402343728186503,8.1831223127040928E-2,0,1.0909006667089152E-2,0.27444366367721834,5.912559848812152,0,1.9254442142200342E-2,0.10473234036051843,-2.6948985363392428E-3,4.4921347724271053E-2]
[null,990,1.0457372997830812,1.0099151645381925,0.97698000294911114,1.0242494862121958,1.0002427940841154,1.0297844861680716,0.95328788791876351,null,6.7095472806066097,0,1.0427518689228081E-2,0.1878851203792497,0.11659693160764843,8.1464437185861022E-2,0,1.0427518689228081E-2,0.24854271301990388,5.9147228291578786,0,1.8916656477899259E-2,0.10003212544295066,-1.5521985978841093E-3,4.2938665933104379E-2]
[null,991,1.0245892316983041,1.0135919828049125,1.0378524882089617,0.9825571751182598,0.99950129901534368,0.97294038037506603,1.009989806333349,null,6.7192875891366848,0,9.5193107447415458E-3,0.18769849366626445,0.11771952620004723,8.5404336570655742E-2,0,9.5193107447415458E-3,0.26357367864833575,5.9090240669088967,0,1.9024259471728672E-2,9.6965658756680437E-2,6.787416413724254E-4,3.9198827272696711E-2]
[null,992,0.9991164280938003,0.97895545525698013,0.97128489194696865,1.0125239060787332,1.0103035906532498,1.0085219442605777,0.97564250876570091,null,6.7438116948670315,0,1.0886139963474078E-2,0.1944975161786465,0.1236733399844869,8.1315945529057215E-2,0,1.0886139963474078E-2,0.26460172498472673,5.9144007935527325,0,1.9159914813863362E-2,0.10384906170853636,-2.5137885939298258E-3,4.4827186708905689E-2]
[null,993,1.0052678244826321,1.0224647677935079,0.97986494213014397,1.0179704018284164,1.0308379163163719,0.95814325803139988,0.99997597923856352,null,6.7193076499715971,0,1.0014242760850896E-2,0.18121271401588041,0.12064038907915513,8.1851473041531619E-2,0,1.0014242760850896E-2,0.26443031610143919,5.9142246695762264,0,1.9126525932268264E-2,9.6340306423218891E-2,2.4438658145566045E-4,4.1236869220420178E-2]
[null,994,1.0146001133600675,1.0080033231958154,0.99466599152004498,1.0020907557007741,1.0044837171472358,1.0027853035969998,0.98451555141725267,null,6.729119909171053,0,1.0313908139594746E-2,0.19077689889725633,0.11994294033392673,8.2729046524225483E-2,0,1.0313908139594746E-2,0.26215062546988765,5.9125448915636012,0,1.9076644659557437E-2,0.10067835542684542,-1.2503316158876978E-3,4.2470837911638304E-2]
[null,995,1.0156273481443092,0.96971948187427892,1.0261697132235013,0.96811946393042703,1.0197554354506029,0.99386905610150211,0.98743874612834392,null,6.7339796933982612,0,1.010055144669457E-2,0.19574986029380756,0.12110048359639373,8.4655909487303768E-2,0,1.010055144669457E-2,0.26228039237563289,5.9089210849331977,0,1.9071210073568382E-2,0.10170579643287218,-1.0973168208676051E-3,4.1592273026351038E-2]
[null,996,1.0158499750781336,1.0105198942531284,1.0316942774024069,0.9691309496685796,1.0038091650257281,0.99936591311434475,0.98357944488187288,null,6.7276871492303512,0,9.9282681801912704E-3,0.19398885267117044,0.1189914841571026,8.4984167883938241E-2,0,9.9282681801912704E-3,0.26130633794952923,5.9086565985999506,0,1.907003371482463E-2,0.10051790943275987,-7.1107637909356952E-4,4.0882841200168732E-2]
[null,997,0.96960818690356076,0.98941667764291674,1.0051656799883941,1.0031501719913987,0.97352492770329335,1.0142752479315023,1.0264841079200944,null,6.7828008506081074,0,1.0903062878520622E-2,0.20483613685627647,0.12624260542256549,8.3723565378949039E-2,0,1.0903062878520622E-2,0.28737986184128339,5.9120120966234548,0,1.932597173897084E-2,0.10753558350911152,-3.1518430234039781E-3,4.4896872260900757E-2]
[null,998,0.99696926297267419,1.0145155875459653,0.97654878688014191,1.0054919291226152,1.0238305529628862,0.98602478315377862,0.97212112246475091,null,6.7287990436924341,0,1.0456381874728559E-2,0.18828465358319005,0.12208625182379081,8.1602212960702761E-2,0,1.0456381874728559E-2,0.26180508540596187,5.9137324256348105,0,1.9171666322275661E-2,0.10026651663187812,-1.2072880637130372E-3,4.3057519393539856E-2]
[null,999,1.0013089617855755,0.97983268980689509,0.98971659733210537,0.97265292084741739,1.0044624835658904,1.0304660614429941,0.99700360702197577,null,6.7561865161321064,0,1.0917564031443198E-2,0.2004665859582877,0.12301387136827888,8.2531230896467939E-2,0,1.0917564031443198E-2,0.27190239085102325,5.9112297428887626,0,1.914796700920127E-2,0.10605307015023387,-3.1149284176728753E-3,4.4956585427526924E-2]
[null,1000,0.96436894016988062,0.98243452065668768,1.0092701416559915,1.0319145828035741,1.0095084093936304,0.99881304578265173,1.0012652075420707,null,6.776631095569094,0,1.0789209010867093E-2,0.20393279084304783,0.12720792348585441,8.39060953223522E-2,0,1.0789209010867093E-2,0.28040547608580574,5.9133340542636113,0,1.9356517813289838E-2,0.10684396994280335,-2.7837744868075883E-3,4.4428042299136529E-2]
[null,1001,0.99001342970648776,1.0310147914515468,1.0355038842336912,1.0160884389722362,1.0026359764888704,0.96879218298212333,0.98104918519990814,null,6.7321132987856993,0,9.758554434794826E-3,0.19174929536756979,0.12104777637034564,8.5298838751395059E-2,0,9.758554434794826E-3,0.26443514210338193,5.9109718555020851,0,1.9210085878960302E-2,9.9172205258923604E-2,4.4109348490171705E-5,4.0183990204546743E-2]
[null,1002,0.98610122606946982,1.0057940129135625,0.99353184669794758,1.0179558064832677,0.99087435001086821,0.9902711655254115,1.032734605225559,null,6.758833501950237,0,1.0499796554515977E-2,0.19388909481921471,0.12353916160639736,8.2933124212693984E-2,0,1.0499796554515977E-2,0.28172591919650519,5.9134657374051676,0,1.923193253186662E-2,0.10237853716156918,-1.5662983005576751E-3,4.3236293317379521E-2]
[null,1003,0.9887802137044569,0.97733691745800499,0.98678832250379678,0.96417610156345956,1.0187330614057579,1.0049362385246026,0.99617731058096004,null,6.7546126840146803,0,1.0821394168851181E-2,0.1978398491712699,0.12475540663288653,8.2354451313040353E-2,0,1.0821394168851181E-2,0.27269640444481075,5.9109341182721309,0,1.9216953784910576E-2,0.10481649879313114,-2.5615734484718904E-3,4.4560575050970427E-2]
[null,1004,0.95462193804912199,0.9887333881536694,1.0057918095671752,1.0205578869817522,0.97091866137123362,0.96907388313029519,1.0102528311642593,null,6.7720988803688753,0,1.0578042710727603E-2,0.19891432665636444,0.12824749889406323,8.3714091703022173E-2,0,1.0578042710727603E-2,0.28275354213108861,5.912917390149917,0,1.9414237302150611E-2,0.10439433650484493,-1.8150400339405851E-3,4.3558497061362354E-2]
[null,1005,0.96190113458852544,1.0233178861092276,0.99789935297904575,0.99410373262081719,1.0168904467980218,1.0303233416736681,1.0364679005707906,null,6.7903301883872311,0,1.1074493730251354E-2,0.20582935960284338,0.12569109364413866,8.3350143734059065E-2,0,1.1074493730251354E-2,0.29372221418310418,5.9119321865312697,0,1.9371020996449894E-2,0.10844741436240406,-3.6160386618152196E-3,4.5602793994773808E-2]
[null,1006,1.0184553481901335,1.015524716984872,1.0408213655005163,1.0217081772188161,1.0095621477867771,0.95252283766519852,1.0163393437362642,null,6.7191924028293073,0,9.3436634210150599E-3,0.18504488835338873,0.11828301823094607,8.5635321658583091E-2,0,9.3436634210150599E-3,0.26490840053606346,5.9109653200530392,0,1.9056305173339384E-2,9.5456194766058891E-2,1.367411200240243E-3,3.8475542857649196E-2]
[null,1007,0.97947956916388879,1.0164281674667239,1.0219370743329683,0.99553111764055158,0.97000836536709389,1.0039067224621159,0.97511302213756257,null,6.7524039077430054,0,1.0406509957652268E-2,0.20042091787032842,0.12331028982620754,8.4509262677320798E-2,0,1.0406509957652268E-2,0.26902706847571101,5.9106453384358826,0,1.9269307070060589E-2,0.10434971911722901,-1.9801514456258573E-3,4.2852155715890024E-2]
[null,1008,1.0021903822948206,0.95933200652942363,1.0407235076075703,0.99318274345791413,0.96885777090011105,0.99418496595486516,0.99206913280551146,null,6.7495818049932375,0,1.015621645634473E-2,0.20110787778134112,0.12297292248427061,8.564106397261867E-2,0,1.015621645634473E-2,0.26721268785244745,5.9094304388241126,0,1.9143178604386298E-2,0.1037473150675237,-1.4951712215491568E-3,4.1821491628088049E-2]
[null,1009,0.96513335846005766,0.96362126935426462,0.99722779637113401,0.99916325339018042,0.97696275735677252,0.9732419861167122,1.006048763092021,null,6.7676905801699396,0,1.070416620611579E-2,0.19874862286085423,0.12833172699105916,8.3117019104533382E-2,0,1.070416620611579E-2,0.27916316051381113,5.9122432753877652,0,1.9352040406332659E-2,0.10475167986425081,-2.0947961248875321E-3,4.4077851166225611E-2]
[null,1010,0.99714706133992126,1.0028413395211078,0.98304738069781084,1.0271243328504243,1.0290887052605828,1.0147032990319826,0.99027093689976575,null,6.7489114272517616,0,1.0750965146338795E-2,0.19546472758711583,0.12251011292444848,8.2122913223314137E-2,0,1.0750965146338795E-2,0.26944366492423366,5.9145439010174981,0,1.9170691303841584E-2,0.10375191703413164,-2.3670616349911679E-3,4.4270560872163106E-2]
[null,1011,1.0036639482953453,0.99120567191587328,0.99850811264001171,1.0205896845858646,0.99559143103053216,0.95517085951505865,1.0043091472129431,null,6.7278103602382329,0,9.9694644107119531E-3,0.18545860818018731,0.12199576942607682,8.3033122364158482E-2,0,9.9694644107119531E-3,0.26600376275437854,5.9133294442859698,0,1.9135192093677082E-2,9.7684909464126016E-2,1.1707172485951843E-4,4.1052479944797216E-2]
[null,1012,1.0360490336346289,1.0069903070063086,1.0030249838545038,0.99011353713542716,0.97881414673076639,1.0132925537816235,0.97094175384949444,null,6.7153419581932932,0,1.0136332620483244E-2,0.1898287590521556,0.11735637232607225,8.3129606549722165E-2,0,1.0136332620483244E-2,0.25413221329417601,5.911428393282768,0,1.8965405868715732E-2,9.9762786942347609E-2,-1.0011926538659786E-3,4.1739613531201286E-2]
[null,1013,1.0353349546124426,0.99149017607979706,0.99369348624320641,0.98988102486739205,0.97736991710621857,1.0180776395091391,1.0116601331202071,null,6.7305712628846077,0,1.0343119134008835E-2,0.19104165593869898,0.11833760806103805,8.2703916728284324E-2,0,1.0343119134008835E-2,0.26555917825232167,5.911939320025061,0,1.8969035070611477E-2,0.10086689596212373,-1.4374707408094922E-3,4.2591123587272336E-2]
[null,1014,0.97175710768179879,1.0036654597321351,1.0000426240259015,0.98022777809079153,0.99777979720625343,1.0268384092169065,0.96127218579626927,null,6.7630798721676832,0,1.0995561558944274E-2,0.20501231021789576,0.12534382827264123,8.3148909211551478E-2,0,1.0995561558944274E-2,0.26953748336253447,5.9110619760128458,0,1.9313538266231764E-2,0.107901964618471,-3.5179031572218208E-3,4.5277765362733993E-2]
[null,1015,1.0127824564965577,1.0067598482747067,1.0024959766455315,0.99143057864002815,0.99886738148707077,0.97922975837751358,0.98629877303544056,null,6.7220298114236483,0,1.0026239348360284E-2,0.18761991291730876,0.12007315819655422,8.3191167842222982E-2,0,1.0026239348360284E-2,0.26096561329822493,5.9115293733451386,0,1.908628798592751E-2,9.8627827020330364E-2,-3.4979821453125736E-4,4.128626903247086E-2]
[null,1016,0.9938806852563784,0.98913459353141842,0.98352700397600157,0.97611110394064904,0.99749804072573989,0.99789117561619334,1.0043740773972882,null,6.7483758498112634,0,1.0665844940644898E-2,0.19405515409159019,0.12358221728293818,8.2159926851923387E-2,0,1.0665844940644898E-2,0.27272006614600974,5.9117597701282847,0,1.9188659263488405E-2,0.10297902052488092,-1.9890154938047053E-3,4.3920051015947467E-2]
[null,1017,0.99868222484154634,0.97500433846574375,0.98929516941143747,0.96863491396273915,1.0035166074800415,1.0199422112370482,1.0009430327444138,null,6.755696980483104,0,1.0861449850823397E-2,0.19931165274775944,0.12358932200918593,8.2513562206754501E-2,0,1.0861449850823397E-2,0.27274769587926678,5.9110359898834348,0,1.9162287147097688E-2,0.1054642402016885,-2.8532868117695552E-3,4.4725517219686414E-2]
[null,1018,0.98331874211824644,1.0212944154798673,1.024407460591481,1.0071927596165404,1.0045661465604698,0.98785291734835534,1.0096879289312195,null,6.7527532609382632,0,1.0157286451267435E-2,0.19633709645001743,0.12254721583849072,8.4764049402658595E-2,0,1.0157286451267435E-2,0.27589521492452085,5.9111333415110279,0,1.9247576354861091E-2,0.10209930711103817,-1.0964383310810319E-3,4.1825897676727751E-2]
[null,1019,0.97747007917321305,0.997481849276322,0.99182481668774414,1.0288518924682957,1.0237104249279201,0.96729864145245248,0.97362760415010452,null,6.7414741713418174,0,1.0399106687963722E-2,0.19154447739813993,0.12507705696353444,8.2624078825693462E-2,0,1.0399106687963722E-2,0.26586404548275933,5.9141499322344098,0,1.9280749362270345E-2,0.10122655481259621,-1.1143941066291154E-3,4.282167036904546E-2]
[null,1020,1.0083956157318352,0.97851057645690054,1.0174324417602778,1.0308987373905127,0.97273053480607086,1.024360062375707,0.96736729621611961,null,6.7465343876936839,0,1.052480788291933E-2,0.20135298044058653,0.12169493401115969,8.415167011977967E-2,0,1.052480788291933E-2,0.26147013661045859,5.9128142067326594,0,1.9109704960957364E-2,0.10506791225236659,-2.4664429501814176E-3,4.333928551589402E-2]
[null,1021,1.0312399189009693,0.98208878809209965,0.99910417626277714,0.98638182923678475,0.99247362043050358,1.0386202500058614,1.0265720659110429,null,6.74745565704709,0,1.0586923376524296E-2,0.19711899646742079,0.11916229351340965,8.3131784437742079E-2,0,1.0586923376524296E-2,0.27260089946092725,5.9114472642502145,0,1.898994454624036E-2,0.10379593292907677,-2.3865246203628606E-3,4.3595066062413569E-2]
[null,1022,1.0017476228347966,1.019819362018449,0.99509803915157258,1.009582875448886,1.0062180278576676,1.024678688880637,1.000774195952971,null,6.7493420301265594,0,1.0617177110099216E-2,0.19651227007037572,0.12090883249731509,8.2891383644534689E-2,0,1.0617177110099216E-2,0.27183050137409814,5.9129256586910799,0,1.914558288602048E-2,0.10368277658493667,-2.274621174109434E-3,4.3719645552311254E-2]
[null,1023,1.0143261260835417,1.0021214911255945,1.00072658752023,1.0149164351761457,0.96164302406229962,0.99258202445917376,0.99584818690646937,null,6.7307472870968308,0,1.0183303203042842E-2,0.19006022944234841,0.12014476903392939,8.3143950221617219E-2,0,1.0183303203042842E-2,0.2643640050319383,5.9128981813330563,0,1.9078096048861133E-2,9.9998425980957956E-2,-8.7340002560675107E-4,4.193303002972968E-2]
[null,1024,1.0236051260128061,0.98606674419306162,0.99294689910580192,1.0414700594402106,0.99032342766710491,1.0011893154269829,0.99988317387696568,null,6.7326384627021705,0,1.0319033588383833E-2,0.19038598778854623,0.11997027452207282,8.2674272839872567E-2,0,1.0319033588383833E-2,0.26396897114284762,5.9147693155394521,0,1.9029374941735004E-2,0.1005580937421351,-1.2097714119450481E-3,4.2491943597455901E-2]
[null,1025,1.0291085288217867,1.0087016967695681,1.0011801880724152,0.97402915865147788,1.0253934495806005,0.9921370648235962,1.0262445909108213,null,6.7252443040411887,0,1.0000485473939004E-2,0.18677359723978243,0.11810113414324418,8.3195805155187597E-2,0,1.0000485473939004E-2,0.26841657692282661,5.9106630424788582,0,1.9000893385689884E-2,9.8247068628246267E-2,-3.3403307427062071E-4,4.1180219161622796E-2]
[null,1026,1.0054993925194555,0.99775485720757873,1.0057461560976775,1.0162783149492089,1.0305670134662668,0.98173653550296625,1.0333193019728828,null,6.7441121274788696,0,1.0134919833715889E-2,0.19056875851432983,0.12131756838540429,8.3609615948284199E-2,0,1.0134919833715889E-2,0.27572009097027161,5.9126887127091274,0,1.9125276993749676E-2,0.1000166727347051,-6.6836470376223465E-4,4.1733795926759985E-2]
[null,1027,1.0036213513404251,1.0245981729454083,1.0168930148786048,1.0130902228943068,1.03780576672948,0.99941382663014744,0.96095864627414451,null,6.7284769056580975,0,1.0120737869658829E-2,0.19346813084810127,0.12005346649774948,8.4062076111630468E-2,0,1.0120737869658829E-2,0.25826106213486738,5.9118828847586489,0,1.9135422633724791E-2,0.10098038211443308,-1.0419165641285632E-3,4.1675397123068517E-2]
[null,1028,1.0012890209956891,0.96813441203983719,1.0158733003063949,0.96120983055129006,1.0102524220434947,1.015303109919945,0.99927329490236971,null,6.7549195899346932,0,1.0568331355298789E-2,0.20171973658936726,0.12311219085249228,8.4137634733003286E-2,0,1.0568331355298789E-2,0.27126911741394838,5.9091380741884922,0,1.9148075437049952E-2,0.10534027233625483,-2.4640190441761541E-3,4.3518507428263339E-2]
[null,1029,0.99442630260811715,0.96848328678221152,0.96261685225451177,1.0089644444097894,0.96783425263185996,0.98858920318531618,1.0315057120242901,null,6.755714036288798,0,1.0852432463074681E-2,0.19141525260409289,0.12495509555244527,8.0963309398110098E-2,0,1.0852432463074681E-2,0.27920427866833347,5.9146794796084334,0,1.9185649673311728E-2,0.10265026064312721,-2.0276750810315877E-3,4.4688385221972375E-2]
[null,1030,1.0464297254150199,0.99976943224876536,1.0255294534335582,0.99658147248801188,0.96620044724553789,0.99964242225247801,1.0344427760994919,null,6.7237514082391963,0,9.7375200948178215E-3,0.18853569544641069,0.116121358705859,8.4698383676827582E-2,0,9.7375200948178215E-3,0.26690750462727814,5.9104955046201555,0,1.8913206895603902E-2,9.7988357018252079E-2,-5.9772876849285888E-6,4.0097374536494396E-2]
[null,1031,1.0019700376687835,0.97467498305374789,0.99749966070571372,1.0195921309859013,0.97432285186508927,1.004183653359028,1.0002422523824936,null,6.7504491157674416,0,1.0584015334628721E-2,0.1965969138678331,0.12304589896959435,8.302578660349115E-2,0,1.0584015334628721E-2,0.27018114937796989,5.9133321119774536,0,1.9144374858759697E-2,0.10360360417947556,-2.0638153306343087E-3,4.3583091263499747E-2]
[null,1032,0.99600494194968825,0.97952984129000276,0.95552451937788641,0.9887162150423755,0.99397075552001246,1.0185054321299756,1.0349369219300395,null,6.7635923841394767,0,1.1177700206901323E-2,0.19508542674962415,0.12432418085052814,8.0547962290477629E-2,0,1.1177700206901323E-2,0.28251123213973151,5.9139667549443082,0,1.9176960571888377E-2,0.10499385149726846,-3.0417647999009005E-3,4.6027779895550347E-2]
[null,1033,1.0335544346155654,1.0039840120380272,0.99825975326701177,1.026959254194306,1.0064858722876577,0.98523092539471491,1.0015872430646244,null,6.7165936829757449,0,9.933333708196903E-3,0.1847184948862223,0.11786668875695797,8.2943206596468019E-2,0,9.933333708196903E-3,0.26024914191979731,5.913687622154999,0,1.8978106143676451E-2,9.7307085784271663E-2,-6.0363409516592096E-5,4.0903700142865561E-2]
[null,1034,1.0289790928607228,1.0314788900304779,0.99493115420459721,0.99813221597548329,1.0155620505634486,1.0045529236485404,1.0199413311269117,null,6.7250975226451803,0,1.008548068911456E-2,0.18662499080196304,0.11717799358311996,8.2816150709793465E-2,0,1.008548068911456E-2,0.26773280139636413,5.9123161185086532,0,1.9001559752358205E-2,9.8474279908066883E-2,-5.7658634427558636E-4,4.1530214329131399E-2]
[null,1035,0.97529568232042996,0.98336738716926408,1.0180734138753171,0.98416161490504717,1.0212313564456277,0.96978535035750224,0.96535299823745813,null,6.744363672178519,0,1.0274637094062481E-2,0.1967533955105551,0.12556360940509703,8.4202009767213384E-2,0,1.0274637094062481E-2,0.26459632005348349,5.9102524611313338,0,1.9293183769253527E-2,0.10263536400165918,-1.2417981962024698E-3,4.2309126736121971E-2]
[null,1036,1.0171624425431867,1.020988701465011,0.97589631868455617,1.0320272073009165,1.006666653710073,1.0045889323714037,1.0034763506177822,null,6.7307825809397581,0,1.0419287472921319E-2,0.18743512077792626,0.11937027571081919,8.1641268234393757E-2,0,1.0419287472921319E-2,0.26653778027805058,5.9152028159517389,0,1.9063109114733578E-2,9.9846782872325027E-2,-1.2193432496810171E-3,4.290477124945502E-2]
[null,1037,0.98844281432018555,0.95549298850900999,0.97850234373400802,0.98716356186687015,1.0245521552592682,1.0115436167184246,0.96518016824845065,null,6.753848470165182,0,1.108218320407422E-2,0.20013259487299986,0.12609010815123978,8.17554854635172E-2,0,1.108218320407422E-2,0.26515328720863562,5.9126342301612311,0,1.9218835782274915E-2,0.10647155289577939,-3.2420822497993811E-3,4.5634457879301059E-2]
[null,1038,0.99431026473637296,1.0073244941839941,1.0001315716098034,0.97088003771176523,1.0017002279947123,0.95524357877598787,1.0215145869459299,null,6.7334747564130737,0,9.9805555400904727E-3,0.18611203999154879,0.12232089668043236,8.3192088674743273E-2,0,9.9805555400904727E-3,0.2729796751022921,5.9105518023341901,0,1.9186289454211004E-2,9.7950058124133321E-2,8.3754810085567892E-5,4.1098151241430535E-2]
[null,1039,1.0440531910931756,0.9880754086178718,0.99095195923990043,1.000901340056956,0.99292287520347344,1.0291149785694464,1.0297335213718708,null,6.7347719005924498,0,1.0408161134462406E-2,0.19146335026286906,0.11756075950273019,8.2588226584758909E-2,0,1.0408161134462406E-2,0.26911050010473381,5.9126878497577975,0,1.8925065605330468E-2,0.10122770747499542,-1.6505136688614659E-3,4.2858954968095643E-2]
[null,1040,0.99777148652433822,0.99834668220762657,1.0178037285113641,0.97404281766124456,1.0004194692529904,0.96235085844607116,1.0286996369218055,null,6.7391970716829155,0,9.9041888109132788E-3,0.18958386403183988,0.12200031897084768,8.4313986380397096E-2,0,9.9041888109132788E-3,0.27474335495198843,5.9097211876647204,0,1.9167269806954556E-2,9.8908565694078299E-2,-2.5162461363367978E-5,4.0783686643449925E-2]
[null,1041,0.96262003393063578,1.0071402733203707,1.0013950178196231,0.98193443559425586,0.95839391540587349,0.97783040327117232,1.0142221950922874,null,6.7646056397965761,0,1.0542067501453201E-2,0.1969510954839408,0.12633250885396533,8.3404540929780044E-2,0,1.0542067501453201E-2,0.28219377864722001,5.9110781715735854,0,1.9366788381181447E-2,0.10358961226662848,-1.7212138926469966E-3,4.3410357552918923E-2]
[null,1042,1.0155383399404165,0.96770573729960596,1.0084850729965931,0.9967304798311194,1.0137790581326318,1.017899898746244,0.98407296263885691,null,6.7430143929807427,0,1.0516423733337195E-2,0.1985458218016575,0.12154521007825202,8.3601653571461584E-2,0,1.0516423733337195E-2,0.26362748426591232,5.9114773937765115,0,1.9071680536453525E-2,0.10406206046668116,-2.2216725964306835E-3,4.3304761080237793E-2]
[null,1043,0.98358575603420484,1.0350346966050765,0.9652769971992633,1.0199433795551143,1.0094758290864518,1.0265858620706771,1.0009679195891401,null,6.7583058916021717,0,1.1048410266819138E-2,0.19564347138473129,0.12296905710707688,8.1107828112604058E-2,0,1.1048410266819138E-2,0.27687646051935577,5.9151290034374346,0,1.9246071296331546E-2,0.10477715522268666,-2.9385424130936072E-3,4.5495386935043361E-2]
[null,1044,1.0144562324384894,0.97260796614090395,0.9548071817278907,0.98423794628519778,1.0111503403440405,1.006225734292058,0.97729800740367045,null,6.7308202336494505,0,1.0881878460605517E-2,0.18972002325025022,0.12242277109340258,8.0218652240061999E-2,0,1.0881878460605517E-2,0.26087365785951361,5.9137630598077688,0,1.9077406740376158E-2,0.1021432776670443,-2.2082536075842428E-3,4.4809638598612186E-2]
[null,1045,1.0163823568191201,1.0003434102409972,0.9989364640504077,0.98468818282381165,1.0008864407037186,1.0246291934932965,1.0140431301554478,null,6.7452920100863007,0,1.05152341926703E-2,0.19573556577911255,0.12001990681780664,8.3108811868741833E-2,0,1.05152341926703E-2,0.27167716495004801,5.9113651477449833,0,1.9067222704108457E-2,0.10307605541340144,-2.057727955401897E-3,4.329986276350186E-2]
[null,1046,1.0132034487238892,1.0034398590273477,1.0000502993544618,0.97704835754246666,0.99408819728553255,0.98286304138369418,0.9875027327514545,null,6.7230873196702259,0,1.0095045466233589E-2,0.18822432260225344,0.1202271525479417,8.303677863918496E-2,0,1.0095045466233589E-2,0.26153394717151834,5.9108897204813973,0,1.9084051391237828E-2,9.9065742737298873E-2,-5.4399627944824052E-4,4.1569600378840707E-2]
[null,1047,0.99985883438428946,0.95446463279939309,1.0193572823808033,0.99679087580108117,0.9805881577310458,1.0033964126686032,1.007579774003813,null,6.7585162132563319,0,1.0491290588536036E-2,0.20128414050037516,0.12392448606647428,8.4402156281271512E-2,0,1.0491290588536036E-2,0.27293512111238499,5.9108613098280802,0,1.9155863341359269E-2,0.10493238537656656,-2.1805165136612082E-3,4.3201267263479622E-2]
[null,1048,1.0155998687739116,1.0088785890165421,0.98337738837223576,0.97928547992354331,0.983854752328161,1.0238287197545874,1.0171833939817876,null,6.7430489328875662,0,1.062016004423276E-2,0.19318108335714423,0.11998972672068535,8.2148860195664059E-2,0,1.062016004423276E-2,0.27253362172577883,5.9119396342468242,0,1.9071355310075647E-2,0.10252284771535783,-2.070125128101394E-3,4.3731928744130698E-2]
[null,1049,1.0379058379661832,1.0363340362996076,1.0085520200128903,1.0045369366543935,1.0132363355644307,0.98642405573134906,0.98610830811608785,null,6.7040565731990727,0,9.6826688777903909E-3,0.18282298792212084,0.11570953122185455,8.3493677962994464E-2,0,9.6826688777903909E-3,0.25500702004049441,5.911895424815528,0,1.895599230824364E-2,9.5818216244367788E-2,4.8221569553812122E-4,3.9871506987928101E-2]
[null,1050,0.99293335480917289,1.0125551957357231,0.99937833672247167,1.0286680618146304,0.98200032419508676,0.99059054433281313,1.0342047902586435,null,6.7542171042113273,0,1.0348068395984067E-2,0.19275000798882444,0.12225116295717883,8.3283358062597804E-2,0,1.0348068395984067E-2,0.28016193192108613,5.9137171554911028,0,1.9193892534022115E-2,0.1014815545229671,-1.2334630336084634E-3,4.261150376715056E-2]
[null,1051,0.98022322680643015,1.0048729103661214,1.0389913731769189,0.97381326231316834,1.0160426997332082,0.97988036802990797,1.042422366029361,null,6.7634919420012496,0,1.0048234591536056E-2,0.19846125220744115,0.12345147961474105,8.5768603479868533E-2,0,1.0048234591536056E-2,0.28512647135046215,5.9084854244365577,0,1.9265084481995126E-2,0.10246866433580613,-9.1187943448327996E-4,4.1376841528861362E-2]
[null,1052,1.0303501038654346,1.0072979039058525,0.99375953851290788,0.96998762813143369,1.0167694159731191,0.97561759192319908,0.98881412739716534,null,6.7075285470087653,0,9.8918807225569175E-3,0.18272498528962897,0.11815895615997629,8.2577582818194092E-2,0,9.8918807225569175E-3,0.25682563703729983,5.910860432606909,0,1.8994509971587099E-2,9.6472655898068763E-2,1.8078310074388489E-4,4.0733004126356484E-2]
[null,1053,0.96975339085732282,1.0038870626855765,0.99153375618358353,0.96878335518163616,0.99066183414411479,0.98494689744595298,0.98923352205898585,null,6.7540925422084532,0,1.0646580326918984E-2,0.19601818006933547,0.12575555888239484,8.2670556023817052E-2,0,1.0646580326918984E-2,0.27391198399373823,5.9109194611722131,0,1.9325129865348702E-2,0.10360582305567619,-1.9548736196678684E-3,4.3840722765597563E-2]
[null,1054,0.97833729398400027,1.0040352559385375,1.0013165559637327,0.99904401054531633,1.0181931386553593,0.97586472911917177,0.98700383598552932,null,6.7459791009012298,0,1.0366262146666328E-2,0.19364412176496618,0.12445806589575613,8.3247961944684465E-2,0,1.0366262146666328E-2,0.27004996252584862,5.9120072138991517,0,1.9275805565083789E-2,0.10185422264271901,-1.244675731065878E-3,4.2686422394093211E-2]
[null,1055,1.0165018673639186,1.0187623153494554,1.0034041735396579,0.97775937372671495,0.98419699121048654,0.99412745987638329,0.98871334848893755,null,6.7230619653101362,0,1.0082201478650573E-2,0.18892108867078905,0.11905137623236636,8.324984380190914E-2,0,1.0082201478650573E-2,0.2619020517203674,5.9107394024494528,0,1.9066592085228654E-2,9.926709794280697E-2,-6.5219871690295832E-4,4.1516711124118401E-2]
[null,1056,1.0022854003255373,0.98200636647073392,1.0384716005153307,1.004255706798163,1.03684333706899,0.98741149259026784,1.0330077916320279,null,6.7538671425753298,0,1.0005282896108631E-2,0.19746124435833279,0.12186083364702723,8.5649382136202962E-2,0,1.0005282896108631E-2,0.27729099261167511,5.9101599215291474,0,1.9142662912342203E-2,0.10197825254086446,-8.7612125246986554E-4,4.1199974092207998E-2]
[null,1057,1.0137766875418046,0.99937096011405024,1.0160836425180637,0.96983393313765853,1.0100835526149234,1.0223592716028191,1.0152707524260389,null,6.7474993060765316,0,1.0366706828363253E-2,0.19793288812886994,0.12005703250884944,8.4173176818114342E-2,0,1.0366706828363253E-2,0.2725313562692912,5.9095920255183829,0,1.9081008946677122E-2,0.10335201149936356,-1.9084471271864098E-3,4.2688253514170757E-2]
[null,1058,0.99051957444987204,0.99596138790757016,0.97720682902557277,1.0306226651541031,1.0032710569165073,1.031927456591246,1.0016940352330408,null,6.7647573693573326,0,1.1095458875261945E-2,0.19998750686316327,0.12377949485684205,8.1849495159313196E-2,0,1.1095458875261945E-2,0.27608373600555869,5.9150549158390504,0,1.9207272056943406E-2,0.10646346390868168,-3.3576400624954778E-3,4.5689124730270723E-2]
[null,1059,1.0133882799340688,0.97504074498118964,0.98327663910457841,1.0284057484750015,1.014425843485792,0.98960548445769581,1.0067428920300217,null,6.7375190276300545,0,1.0439957542973582E-2,0.18987481601117109,0.12190567879535932,8.2110766129664045E-2,0,1.0439957542973582E-2,0.26746475462837843,5.9146004964680658,0,1.9083070030200298E-2,0.1007732600366497,-1.2837013882289379E-3,4.2989886918794927E-2]
[null,1060,1.0035420815374287,1.0016657500072033,1.0030649202528403,0.96624344565792109,0.98661464392552156,1.0193897030692489,1.0159480760516615,null,6.7519740704504283,0,1.0551199444866325E-2,0.19760989026352621,0.12141426517090091,8.3399489024487808E-2,0,1.0551199444866325E-2,0.27516305930972995,5.9101362011890766,0,1.9135851703911556E-2,0.10385003285804879,-2.1826803397257061E-3,4.3447961270468835E-2]
[null,1061,1.0096561453589488,0.99519916688321475,1.0182949968702111,1.011322998165576,0.98671373299592335,1.0073458552957499,1.0221579376860672,null,6.7496479464760588,0,1.0254686373451016E-2,0.19643573755640786,0.12070741874756927,8.4362320828385989E-2,0,1.0254686373451016E-2,0.27411440514826851,5.9117072385016103,0,1.9102955413475616E-2,0.10245846713931157,-1.4675700787109168E-3,4.2226973219739866E-2]
[null,1062,0.99770287657392931,0.99932291498380721,1.0209987963028413,1.0339159949386509,0.97738574130585099,1.0237308065026585,1.0125125312187582,null,6.7628037869109674,0,1.0502787763308858E-2,0.20199462036567495,0.12190043776437803,8.45771475853829E-2,0,1.0502787763308858E-2,0.27631020195940215,5.9127729101112259,0,1.9167645541246291E-2,0.10521766190997926,-2.385448909098923E-3,4.3248610582773274E-2]
[null,1063,0.9651606380053892,0.99133772900362327,0.99551523961887511,0.97157709872624876,1.0292214731603544,1.0213388807174322,1.0432383518989194,null,6.7909563339853873,0,1.1113724887896463E-2,0.20583004653269776,0.12691403387521044,8.319000304580218E-2,0,1.1113724887896463E-2,0.29409796872219729,5.910848237477671,0,1.9351880753642744E-2,0.10857643097978444,-3.6166083206873481E-3,4.5764340919070605E-2]
[null,1064,1.0077049653361356,1.0427227477940202,0.97541313692505727,0.99753668670044737,1.0018193094175072,1.0061265029008217,0.9624190669833812,null,6.7208442929692573,0,1.0443074035114012E-2,0.18772835141536279,0.11948838194961355,8.1474801790646784E-2,0,1.0443074035114012E-2,0.25797844796298469,5.9133646375103917,0,1.9113410231797873E-2,0.10002722704697083,-1.3336850172229299E-3,4.3002720078714293E-2]
[null,1065,0.99082359102215645,1.0110819509483839,1.0262928530168338,0.98001401056768411,0.99452112120568559,1.0194980224370929,0.98647444168092857,null,6.7541010295046,0,1.0430877153969245E-2,0.20218842108542023,0.12207295863934894,8.478726321549282E-2,0,1.0430877153969245E-2,0.27056119972169301,5.9095565363595259,0,1.9205583312634878E-2,0.10504472504206229,-2.2681533647022681E-3,4.2952495493124056E-2]
[null,1066,0.99838842469943023,1.0297001344353953,0.99966713513056549,0.97108924017570741,0.98676258476154999,0.98679649619096621,0.99889220965142145,null,6.7328201051298597,0,1.0176134887896565E-2,0.18962857805975533,0.12076399487816523,8.3104595501895639E-2,0,1.0176134887896565E-2,0.26861203645113196,5.9105891951233529,0,1.9163893537812789E-2,9.9823821862023931E-2,-7.6952246815119372E-4,4.1903512183869833E-2]
[null,1067,1.0018818232575033,0.99416238991363304,1.0160645323046207,0.96599972575050641,0.99216078452678702,0.99922869538590997,1.0118766748397501,null,6.746639034239811,0,1.0275604444180037E-2,0.19618791057033311,0.12173696065479699,8.4172275177181205E-2,0,1.0275604444180037E-2,0.27269519588988211,5.9093859577370162,0,1.9144853923655898E-2,0.10244182541578996,-1.4390552405676832E-3,4.2313110111724166E-2]
[null,1068,0.9990815378365645,1.0274779369605864,0.95924837590785694,1.0185314317707255,0.97426219502640432,1.0287520526548672,0.98698182024219883,null,6.7447984685018501,0,1.099172068006448E-2,0.19290414852450272,0.12152694435323164,8.062691182814001E-2,0,1.099172068006448E-2,0.2690366795775192,5.9153787782257492,0,1.9160105365717408E-2,0.10362470578554769,-2.7217544657223958E-3,4.5261949307157968E-2]
[null,1069,1.0318117848939945,0.99437274730451786,0.96519790864793298,1.034071590442674,0.99948397018357427,0.98114508012055368,1.0019198412693999,null,6.715546294459009,0,1.0240719972973895E-2,0.18131972060591581,0.11911735343834831,8.0894976139516628E-2,0,1.0240719972973895E-2,0.2604338050624746,5.9158972441881073,0,1.8987014596893368E-2,9.7109917758860964E-2,-3.8319939960937773E-4,4.2169462068501681E-2]
[null,1070,0.99429436340425892,1.0437942342537148,0.98448921342060902,0.9784959397575379,0.98541501569042567,0.99471877128416097,0.99912950238583687,null,6.7354043886026078,0,1.0376908766493961E-2,0.18906787102228526,0.12088374395750338,8.2190475269910468E-2,0,1.0376908766493961E-2,0.27037635767894314,5.9118354875596335,0,1.918637713867449E-2,0.10028417668610441,-1.1503639899652766E-3,4.2730263279515721E-2]
[null,1071,0.97447508978179675,0.98472061389007493,0.97576429556405619,1.0308977908254107,1.008183442942161,0.99645664463012129,0.96819281378492605,null,6.7550615203326307,0,1.0957332534065143E-2,0.19707552661606353,0.1264176211418637,8.1654928974483121E-2,0,1.0957332534065143E-2,0.26802818772355008,5.9151490005189711,0,1.9297890794864523E-2,0.10498918384940974,-2.6711643293679775E-3,4.5120345042794496E-2]
[null,1072,0.98101247631488897,0.97804740215602726,0.98776873122498021,1.0049058888092766,0.99409812516005724,1.002669667188085,1.00761053419151,null,6.7648199146190251,0,1.086978853702711E-2,0.19901373035507014,0.12568790645236305,8.2512722882580269E-2,0,1.086978853702711E-2,0.27778230648548174,5.9130813194338643,0,1.9260610019818117E-2,0.1053868332984314,-2.6653687538266634E-3,4.475985444524249E-2]
[null,1073,0.99340827014145183,0.98715598614672495,0.96357530209495734,1.029522744091113,0.9693572934953455,0.96267386948199896,1.0249553481938014,null,6.7418076963484026,0,1.0483776626312981E-2,0.18517636910979018,0.1241134665172173,8.0982805128061039E-2,0,1.0483776626312981E-2,0.27498338853879245,5.9157392633917034,0,1.9191267745243858E-2,9.9256558763371167E-2,-8.0574895025400071E-4,4.3170326104480496E-2]
[null,1074,1.04244635052688,0.96541008874106526,0.99771622810434324,1.0433659403337336,0.9973150858749571,0.98259023069999274,1.0193220776115381,null,6.722413946388726,0,9.9932636388208561E-3,0.18568334222828839,0.11871700587077862,8.2953874669805278E-2,0,9.9932636388208561E-3,0.26272666287876428,5.9146048132008762,0,1.8933114245095674E-2,9.7841782565878083E-2,-1.9713020080264223E-4,4.1150480930044989E-2]
[null,1075,1.0079217193458618,0.95843368107481763,0.95443946567795646,1.0079296801817546,1.0041555040069303,1.0124187313653066,0.96222754191838444,null,6.7377767685782475,0,1.1092985312569623E-2,0.19329487977201146,0.12394894630929718,8.0191564596219816E-2,0,1.1092985312569623E-2,0.25923994480212709,5.9150640743315188,0,1.9112246821298178E-2,0.10408730562898161,-2.8411327225853411E-3,4.5678939039381472E-2]
[null,1076,0.98719150380797815,1.0013552742717002,1.0418712023987455,1.0250446064070498,0.98319418424756488,0.95371234969575025,0.9993140432018609,null,6.7395626042019732,0,9.7009129566196471E-3,0.19241809759874873,0.1226964644569546,8.5760678767359488E-2,0,9.7009129566196471E-3,0.26894707975175897,5.9110841118959048,0,1.9225826764155528E-2,9.9208823149960296E-2,2.7488895990211302E-4,3.9946632857222004E-2]
[null,1077,1.010723225873192,1.01065725714594,0.96794994773034293,1.0078986142001882,1.0085214603265196,1.0296534265180868,1.0304783646357927,null,6.7522380207326957,0,1.0869134765014107E-2,0.19323446045720696,0.12076517644604565,8.1278315688942296E-2,0,1.0869134765014107E-2,0.27793865095563158,5.914332482177012,0,1.9097254853861E-2,0.10334783508459586,-2.5133172590572029E-3,4.4757162328460019E-2]
[null,1078,1.0076418034047687,0.9613121617553031,0.97746194158418409,0.96802916230082625,1.022464565220097,1.0293648612441386,1.0107641586458804,null,6.7573713670634756,0,1.1043784070972085E-2,0.19913147937883166,0.12340707299235275,8.1792586254090693E-2,0,1.1043784070972085E-2,0.27402639975734772,5.9116569636587997,0,1.9113749342789966E-2,0.10599420213566907,-3.2274235403850255E-3,4.5476337083977379E-2]
[null,1079,0.97782496664213214,1.0267940759025789,1.0284512963515728,0.96297390456345555,0.98247860271381826,0.96151306929958469,1.012901022286625,null,6.7439440182053723,0,9.884100172346328E-3,0.19220227286436009,0.12289363659194065,8.4980007949497643E-2,0,9.884100172346328E-3,0.27574239703186554,5.9085115377843787,0,1.9278725168371459E-2,9.9750738048730178E-2,-1.1626243924838171E-4,4.0700965205475594E-2]
[null,1080,1.0036191067179829,1.0208118216496178,1.0057255718100486,1.0075779289270319,0.96319907932745952,0.96977603879985208,0.9776680260352536,null,6.7208963491970151,0,9.9327454046017442E-3,0.18676154259607805,0.12043957828162574,8.3391567339931444E-2,0,9.9327454046017442E-3,0.26006970344981151,5.9122197267356578,0,1.9135434782444963E-2,9.8019521879188401E-2,-4.2003481099055651E-5,4.0901277613374816E-2]
[null,1081,1.0032489976424315,1.0377909178523805,1.0195280700453089,1.0266655473357522,0.98248498395622719,1.0034109323958955,1.0304950515248281,null,6.7479211967942208,0,1.0086210496006488E-2,0.19356123984501211,0.11943607356015017,8.4493970926279846E-2,0,1.0086210496006488E-2,0.27731714442766614,5.9124655381325173,0,1.9137438692020125E-2,0.10089783287490359,-9.2126120834082543E-4,4.1533219544011568E-2]
[null,1082,0.99122584748619469,0.99098807575795789,1.007206183560257,0.98217207815840679,1.0125205707619178,0.98936898064703183,1.0344066984542166,null,6.7572856813201607,0,1.037778506638142E-2,0.19555773064423365,0.12337218384498291,8.3745065079074824E-2,0,1.037778506638142E-2,0.28080805455582514,5.9107631333325079,0,1.9203350459718167E-2,0.10256085021792266,-1.4585585405854878E-3,4.2733871726476719E-2]
[null,1083,1.0086220167655318,1.0029287278951793,1.0209222292779596,0.99750668395801112,0.97256263701912538,1.0295173907705029,0.98683997695219872,null,6.7474353803003586,0,1.0432405140940583E-2,0.2006182655585666,0.12040860661653369,8.441656706481597E-2,0,1.0432405140940583E-2,0.26688326155816533,5.9108102973775072,0,1.9108491446223543E-2,0.10450466771299249,-2.2735645059469107E-3,4.295878747150049E-2]
[null,1084,0.97991269612415333,1.0345975528369569,0.96841570044778635,0.96116804245111509,0.99339989917593419,0.98872816855833501,0.96098190546225937,null,6.7320046942853384,0,1.0653647289788478E-2,0.18953450819521439,0.12339260036828846,8.1086170340257321E-2,0,1.0653647289788478E-2,0.26337339470362409,5.9117804214760969,0,1.9266846937594416E-2,0.10134523318539519,-1.6443041819581255E-3,4.3869823260821644E-2]
[null,1085,1.0008334374601162,0.9948129830309731,0.97662421636820829,1.0306193030374953,0.99981884465451398,0.99971962804939629,0.98725920882077278,null,6.740703227544687,0,1.0649045875800667E-2,0.19177535775662158,0.12257126888775638,8.1683795433891704E-2,0,1.0649045875800667E-2,0.26631198918784282,5.9150867398121809,0,1.915055384504202E-2,0.10212154574794566,-1.8488985836325222E-3,4.3850875457040993E-2]
[null,1086,0.99943267567022875,0.98837376688001322,1.044379938789235,1.0273465371568868,0.99009987422983059,1.0120461178214777,1.0081348902810587,null,6.7595879287254919,0,1.0202695273487727E-2,0.20312211202888539,0.12177967304260551,8.5981793530834849E-2,0,1.0202695273487727E-2,0.2736873426850685,5.9110614578873539,0,1.9158188246200299E-2,0.10459957787023154,-1.8150996898527035E-3,4.2012883124161855E-2]
[null,1087,0.98283140176753891,0.97767565902532716,1.0434835617429468,1.039113670041959,1.0408624774618265,1.00100396932435,0.97842763767134611,null,6.7616896960278217,0,1.0317923964517335E-2,0.20514444123963305,0.12439454645395019,8.5874167224435E-2,0,1.0317923964517335E-2,0.26917979080520454,5.9117495028629321,0,1.9250325420260485E-2,0.10568719705489894,-2.0776493973708146E-3,4.2487374363879338E-2]
[null,1088,1.0100444839316722,1.015473500908322,1.0135005650396869,0.97715781235547505,0.95700492607334331,0.96379180324161196,0.97957072285879143,null,6.714661634361736,0,9.7640808513990759E-3,0.18571559786964056,0.11978063205982684,8.3827916964097512E-2,0,9.7640808513990759E-3,0.25842978993383908,5.9101349558145655,0,1.9100879436287778E-2,9.7096400040530842E-2,3.687152384903113E-4,4.0206747004457567E-2]
[null,1089,0.97180891209544418,0.99892967170422764,0.96602152103737859,1.01245680667243,0.99987593375972716,1.0019318095559882,0.97291641626351877,null,6.7558671765869516,0,1.1073709673748537E-2,0.1963084294516981,0.12622536145332003,8.1065825616967471E-2,0,1.1073709673748537E-2,0.27043026901911238,5.914683770823812,0,1.9313239209074958E-2,0.10509385857359657,-2.8531429502843975E-3,4.5599565389652048E-2]
[null,1090,1.0210194023141888,1.0121670976160302,1.0123530929852151,0.99043172717254002,0.99858259637180358,1.0208166605832425,0.98845126255671267,null,6.7329190279565365,0,1.0255212942636214E-2,0.19472607949110804,0.11866887944840945,8.3829989032687333E-2,0,1.0255212942636214E-2,0.26317113900422345,5.9109174588369724,0,1.9042862760127427E-2,0.1018650158187428,-1.5315379736567662E-3,4.2229141537918666E-2]
[null,1091,1.0004718865870292,0.99398893954258538,0.96151121044660992,1.0121483240284495,0.97702392114649728,0.9773854789008023,0.97836733726046332,null,6.7275406071717807,0,1.0556588566072287E-2,0.1858915595358987,0.12293566086021514,8.0671243158326564E-2,0,1.0556588566072287E-2,0.26192807750444913,5.9149114392450421,0,1.9152522314857395E-2,9.9743679310397307E-2,-1.1637274697762932E-3,4.347015271236717E-2]
[null,1092,1.0351811881433199,0.99491030416809234,0.99634636024659118,1.0115250978387411,0.99033620655412369,0.99651506659464895,1.0247491861087923,null,6.7266331173903735,0,1.0087240417442774E-2,0.18704943716650482,0.11814426741668885,8.2903292802132253E-2,0,1.0087240417442774E-2,0.26698580332392657,5.9129607594755473,0,1.8969817221305543E-2,9.8628774421327919E-2,-5.4649501423404713E-4,4.1537460577167007E-2]
[null,1093,0.99676804117147322,0.98803505002385472,0.99704193847765721,1.019107025702374,1.0100413300125346,1.0375232292796739,1.0312860975865592,null,6.7734703065677166,0,1.0932893738812359E-2,0.20293960234674707,0.12302496289205199,8.3170577021683179E-2,0,1.0932893738812359E-2,0.28313739683527334,5.9133315563166029,0,1.917277021075069E-2,0.10697044612525358,-3.2967156145344758E-3,4.5019710433886952E-2]
[null,1094,1.0204208020044354,1.0215835063779861,0.98225794554222745,1.0160217992915539,0.97414673845915201,0.99503891694550217,0.96347902008209541,null,6.7137217340627133,0,1.0227853340365101E-2,0.18573633048443075,0.11884674042082609,8.186348937711152E-2,0,1.0227853340365101E-2,0.25425957216386291,5.9139873410401398,0,1.9045994961530616E-2,9.8627056860490378E-2,-7.612708112722424E-4,4.2116479565593896E-2]
[null,1095,0.98537073682006837,1.0145819184605782,0.99703492031992891,1.0181769702106152,1.0224392501340125,0.99791195993749737,1.0260360855500488,null,6.7592451911632736,0,1.0517073184823519E-2,0.19521898822041914,0.12313520618563516,8.3138707753123278E-2,0,1.0517073184823519E-2,0.28077299576554687,5.913281684633283,0,1.9236030973082976E-2,0.10290123216167558,-1.747089935354309E-3,4.330743540586042E-2]
[null,1096,1.0305383433896083,0.9952102404250045,0.95505505389082745,0.95822414363386987,0.9568486332402385,0.96632348610496266,0.98637571321978024,null,6.7014219183916532,0,1.0184286646302058E-2,0.17762329723041898,0.11940554531414144,8.0143334478182782E-2,0,1.0184286646302058E-2,0.25534646672593819,5.9123429002973396,0,1.8993543502688323E-2,9.5618536355658854E-2,1.121481325824822E-5,4.1937079674024734E-2]
[null,1097,0.96921074178675704,1.0296471072887683,0.99601499854105224,1.0091936576108007,1.040798445422366,1.0203886249929628,1.0114354562046768,null,6.7728495016569887,0,1.0874191857555381E-2,0.20154302229121918,0.12447182657390896,8.3105479206768654E-2,0,1.0874191857555381E-2,0.28343038055057507,5.9128533094622329,0,1.9328277364189749E-2,0.10628857367172963,-2.9493539990569392E-3,4.4777986535416064E-2]
[null,1098,1.0370221964331165,1.0013022072028068,1.0240836565020115,0.99000477956166166,1.0287075608868663,0.97979980562848923,1.0063821831219231,null,6.7141749032076978,0,9.6366941684195781E-3,0.18618503821776342,0.11712941254363234,8.451320817814198E-2,0,9.6366941684195781E-3,0.26019116647510798,5.9102234424594959,0,1.8960467958631277E-2,9.6835446757968513E-2,4.5452929902032815E-4,3.9682191317932318E-2]
[null,1099,0.9819961384490038,0.97530303843733879,0.96783716401343312,1.0300897322908,0.98444747433999635,0.99697110577383041,1.0398543682633179,null,6.7708973746873244,0,1.0999603007162502E-2,0.19552121099471467,0.12608322016259757,8.1391815827098535E-2,0,1.0999603007162502E-2,0.28580519427612133,5.9155384989976403,0,1.9255043449699912E-2,0.1045767956062756,-2.5688119539771094E-3,4.5294407327145694E-2]
[null,1100,1.01437031293767,1.0045018056206692,0.99514589654525187,0.9700908746566419,1.0149366661281902,0.98687170466908347,0.99544002538070187,null,6.7249817541551362,0,1.0163412241558575E-2,0.18812692398436248,0.12012838831319377,8.2756273480482659E-2,0,1.0163412241558575E-2,0.26368513948751127,5.9107885637133091,0,1.9077861925375136E-2,9.9256180304871336E-2,-6.8869964476229019E-4,4.1851122590796631E-2]
[null,1101,0.97621901685276524,0.97797850439094325,0.98132768567798168,1.0324097972618609,1.0196933804294961,1.0305691461246991,0.98790334312825512,null,6.7751530609178809,0,1.1290683633592568E-2,0.2047544131105421,0.12643243232488738,8.2112533958016085E-2,0,1.1290683633592568E-2,0.27636285068124777,5.914924602052408,0,1.9287896863674794E-2,0.10877638590642742,-3.9910795156937913E-3,4.6493025536364613E-2]
[null,1102,1.0344040608577789,1.0363808497720819,1.0037961856622362,0.99155385186310874,1.0286285588647843,1.0074106253247734,0.99638440220801616,null,6.7158309210677691,0,9.9632906872793529E-3,0.18680135496714012,0.11618433154748667,8.3262774372345957E-2,0,9.9632906872793529E-3,0.2604052005962737,5.9114627466569969,0,1.8973773725319262E-2,9.8134221387033899E-2,-4.2053983541055149E-4,4.1027057650583593E-2]
[null,1103,0.96632453092429782,0.98505867367043809,1.0135145411235675,1.0131505856009488,1.0066246138393158,0.9984351246336084,1.0025309371920457,null,6.7741619463419633,0,1.0711164839156679E-2,0.20373361908263118,0.12673184613039409,8.4152122775298863E-2,0,1.0711164839156679E-2,0.28013335348118984,5.9120788906587327,0,1.9345077503169789E-2,0.10651590204424517,-2.6355356250753297E-3,4.4106670291377742E-2]
[null,1104,1.0032210836998958,0.9839925050129843,0.99388535864709593,1.0207898359843808,0.99254861014070772,0.96936140655169611,1.0009084481962514,null,6.7337954664987816,0,1.0194841859731837E-2,0.1883564721930043,0.12249346328729403,8.2754448359805055E-2,0,1.0194841859731837E-2,0.26661819577520618,5.9135991619590813,0,1.9137589888554234E-2,9.9439662325302755E-2,-5.8407145363966264E-4,4.1980544164170623E-2]
[null,1105,0.97982094836023059,0.99463998069203674,1.0133848055411629,1.0124209390251058,1.0138686672296773,1.0200939656374752,1.0287654358468881,null,6.7782386333254099,0,1.0749328827274755E-2,0.20442026960141624,0.12450570382329437,8.4215778901964231E-2,0,1.0749328827274755E-2,0.28554900226463814,5.9120468559408215,0,1.9267367877257111E-2,0.10688174485644361,-2.9119127419425092E-3,4.4263822801511324E-2]
[null,1106,0.96741770057446319,1.0080132102594745,0.98719000577100624,0.9990376400424299,0.98739600241515924,0.96729951472006126,1.0106969568037167,null,6.7551692959920002,0,1.0502405575859923E-2,0.19212241335187957,0.12593596152051609,8.2486364797117157E-2,0,1.0502405575859923E-2,0.27875147367175068,5.9127962416252506,0,1.9338702556251589E-2,0.1017669622219497,-1.2758605556006516E-3,4.3247036802885393E-2]
[null,1107,1.0167623733958846,1.0197480242251999,1.030149086560987,0.98049236326841427,1.0291106366961376,1.004278495937549,1.0180551935611919,null,6.7370873660725348,0,9.9428612243622639E-3,0.19383078291683378,0.11848186545627948,8.5024451330085279E-2,0,9.9428612243622639E-3,0.27059274478481193,5.9093597334800432,0,1.9065217992068752E-2,0.10051213913840178,-7.2250178458478143E-4,4.0942932758599858E-2]
[null,1108,1.0028746183232453,0.9752188602670474,0.97018148816374095,1.0063911488372252,0.96216669973540292,1.0194792047656187,0.96130459121958367,null,6.7418188401995724,0,1.0991719884251346E-2,0.19606240537320077,0.12341902846064229,8.1192463317802319E-2,0,1.0991719884251346E-2,0.26077519775945129,5.9141294191330829,0,1.9139467227073419E-2,0.104742683412042,-2.9037705138691698E-3,4.526194603014113E-2]
[null,1109,0.98649011647126195,0.98270235124797822,0.99210927950587435,1.0392848794059182,1.0169654912980215,0.98362004598223818,1.0240015352724459,null,6.7589411214015174,0,1.0542498843264209E-2,0.19426756439647636,0.12467021600752314,8.2820998782223515E-2,0,1.0542498843264209E-2,0.2788108705858493,5.9146979629324301,0,1.9229753121420404E-2,0.10265108882658287,-1.6194669927087951E-3,4.3412133741720677E-2]
[null,1110,0.97848349855439731,1.0185704784127081,1.0121864708910633,0.99629868162103774,0.98949102744492134,1.0383652992413122,1.0173315918879886,null,6.7776917751603154,0,1.0857215495131398E-2,0.20610607275283951,0.12351877743379368,8.4112417652475693E-2,0,1.0857215495131398E-2,0.28427286033333116,5.9112439394876128,0,1.9274972948848577E-2,0.10782699030668681,-3.3723366519132353E-3,4.4708080896633952E-2]
[null,1111,1.0132519953225092,0.98338107462326652,1.0235427550604352,0.97882739566072074,0.99164692093083906,1.0280099306863646,0.99766656320781377,null,6.7495924561324312,0,1.043337381267498E-2,0.20141604638873142,0.12075649920330328,8.4588788662610104E-2,0,1.043337381267498E-2,0.26866270280355825,5.9096507148847994,0,1.9083793598475111E-2,0.10478501611378102,-2.3138818121139753E-3,4.296277628928561E-2]
[null,1112,1.0017958561155991,0.99789955507723105,0.98129859272034903,0.97551423961409722,1.0154336444826648,0.97119465225368939,0.98900559401233146,null,6.726074339882115,0,1.0279588054953324E-2,0.18641034022436798,0.12221525864447172,8.1902962827377926E-2,0,1.0279588054953324E-2,0.26384713418708922,5.9118505060675632,0,1.9145320865507267E-2,9.9032484912666446E-2,-6.5918175876421715E-4,4.2329513911832276E-2]
[null,1113,1.0390951530442871,1.0039274960881721,0.98706109760537697,1.0066765150425827,1.0108880410008807,0.9774772369143746,0.97049578064424347,null,6.6997805128511274,0,9.8991371585704559E-3,0.18105210183833303,0.11744176059079064,8.2098900276651093E-2,0,9.8991371585704559E-3,0.25012697088325414,5.9132163036129199,0,1.8949980436703959E-2,9.5909206667587621E-2,2.2240370662613023E-4,4.0762884838262771E-2]
[null,1114,1.0395115414295601,0.99888452588082011,0.99163774640990565,1.0144086114662529,1.0071429027813152,1.0026433433313822,1.0371445398712198,null,6.7283885498224736,0,1.0131309501620712E-2,0.18656009289429676,0.11754931752844057,8.2647629237534326E-2,0,1.0131309501620712E-2,0.26961857975992798,5.9133797067978149,0,1.8947878885319781E-2,9.8601621146246571E-2,-6.3520564891384628E-4,4.1718929221807186E-2]
[null,1115,1.0183534269335781,0.97415621508415973,1.0138778456471913,1.0297957199555146,0.95962274119925217,0.99853015667196376,1.0272117503291616,null,6.7461077273868755,0,1.0210249665098779E-2,0.19431032213029639,0.12078671998692053,8.4079486942102738E-2,0,1.0210249665098779E-2,0.27249279049046204,5.9129575443519391,0,1.9056840908669825E-2,0.10157099318733072,-1.1909613750306178E-3,4.2043990764184573E-2]
[null,1116,0.99216900827736021,1.0115577776683433,1.0371109762919466,0.97404315499263217,1.0289360459263801,0.96868011664383891,0.98379447164296008,null,6.7326740522427579,0,9.8021143113952384E-3,0.19306310160183818,0.12167805583678264,8.5370849142764368E-2,0,9.8021143113952384E-3,0.26474626323552974,5.9086074025066351,0,1.9198122243937382E-2,9.9773210679009572E-2,-1.2631502675659894E-4,4.0363362023018254E-2]
[null,1117,0.97942383065620919,1.0094386356309288,1.0183953274211617,0.98447743287972711,1.0269225870487935,0.98079139101639801,0.98542109485840768,null,6.7464347487335132,0,1.0229223389181598E-2,0.19597706408552046,0.12372630607642461,8.4292038294939572E-2,0,1.0229223389181598E-2,0.26976474223778152,5.910251112741248,0,1.9269623819116864E-2,0.10221417350846035,-1.1824332127441882E-3,4.2122121182760625E-2]
[null,1118,0.99052539552346353,1.027133860979188,1.0179470381464801,1.0410807917960132,1.0141691137539746,0.97353902284272642,1.0238836261237261,null,6.745937997291219,0,9.9692958908572538E-3,0.19087059580000096,0.12150062109709212,8.4393603799507888E-2,0,9.9692958908572538E-3,0.27629578210077854,5.913334879981675,0,1.9207239712442516E-2,9.9572836206952939E-2,-2.8934741725974999E-4,4.1051786010030983E-2]
[null,1119,0.97867672433417341,1.0157943105752627,0.97263456992860342,1.0122360904397791,0.97263730278192595,1.0246863115669147,0.99222271772094917,null,6.7626483909922914,0,1.1101297010077173E-2,0.19873943790577459,0.12437908356585363,8.1549106929524842E-2,0,1.1101297010077173E-2,0.27586456655889013,5.9143114863245048,0,1.9273872934515747E-2,0.10604204959390105,-3.2243779509662403E-3,4.571316513029057E-2]
[null,1120,0.97260719779519755,0.99287926210730337,1.0100608614280191,1.0457332012957148,0.97296644199980376,1.0213930692473978,1.0018985644233684,null,6.7785199992302436,0,1.0882674288235016E-2,0.20594036205925473,0.12558266306218677,8.3963138791851175E-2,0,1.0882674288235016E-2,0.2802949565865484,5.9140358480725181,0,1.930863488341017E-2,0.10785357650850298,-3.2720964091692115E-3,4.4812915675138419E-2]
[null,1121,1.0062548631194397,0.98173708979315444,1.008974790328558,1.0210785140571257,1.0199640899055362,0.99455313204913143,0.95714773834371403,null,6.7315336521157674,0,1.0301796451961312E-2,0.19463481218425999,0.12195302315851173,8.3554422591102934E-2,0,1.0301796451961312E-2,0.25651413906936021,5.9127652829410779,0,1.912120643709133E-2,0.10198749859966402,-1.4176970030660707E-3,4.2420964137763868E-2]
[null,1122,0.99607692413105686,0.9962804773380286,1.0154497779511418,1.0043551076373114,1.0320334666620716,1.0289259709684684,1.0086624735937477,null,6.7634628000274555,0,1.0638683641060255E-2,0.20293534178149064,0.12235388952223482,8.4210588355077623E-2,0,1.0638683641060255E-2,0.27622990076657411,5.9114933455141969,0,1.9176565026184259E-2,0.10599722527030082,-2.7422618273960872E-3,4.3808205618788995E-2]
[null,1123,0.97175542304032159,1.0201696665862219,0.99627868024458921,1.0210841861464492,0.97563298763345219,0.98147592151986029,0.98935051530353535,null,6.7514453831420846,0,1.0471063940492235E-2,0.19414727009469337,0.12460089458826387,8.2989709905320119E-2,0,1.0471063940492235E-2,0.27290912372498249,5.9134811791228143,0,1.931354799188615E-2,0.10237481705956672,-1.4891368724908208E-3,4.3117977527044382E-2]
[null,1124,1.0069215239249263,0.9975240932709919,0.96925974270282622,0.96356397951454498,0.99090062375545329,0.9871026575428421,1.0061764378032831,null,6.7317771806508988,0,1.0506070856336404E-2,0.18714344345657102,0.12183299408195745,8.1206163093161379E-2,0,1.0506070856336404E-2,0.26854428572132166,5.9118640356258947,0,1.9117619470373728E-2,0.10002424193423011,-1.217732508103283E-3,4.3262129775491938E-2]
[null,1125,0.9991244402315631,0.97208490315489582,0.98848027432014995,0.96777927043683498,0.99433172423991423,0.97760933103657499,1.0396213764591615,null,6.7494443504058159,0,1.042683452147143E-2,0.19110525766137593,0.12369826570712915,8.2545177700074315E-2,0,1.042683452147143E-2,0.27899369509433264,5.9110350103018439,0,1.9159871057747205E-2,0.10116300795595427,-1.1917837247003935E-3,4.2935848652059828E-2]
[null,1126,1.0019932968716774,0.97249957252888475,1.0094368426105664,0.99733525583706473,0.96835952818205417,0.99420641082457151,0.97283685902111905,null,6.7392135807255817,0,1.0379808957007327E-2,0.19624292007888122,0.12292693524122648,8.3638597008849722E-2,0,1.0379808957007327E-2,0.26189188274108605,5.9114561141739852,0,1.9144248559351068E-2,0.10280663244348701,-1.6359552691204934E-3,4.2742205747835084E-2]
[null,1127,0.97951357426301944,1.016175708277512,0.97743138953445818,1.0182356031052648,1.0060391049359998,1.0049305987243695,1.0228806480955166,null,6.7634430778416377,0,1.0830861887680909E-2,0.19528340607524444,0.12416409212057722,8.1936301958068641E-2,0,1.0830861887680909E-2,0.28221868099730707,5.9143729045397135,0,1.9269113844646888E-2,0.10394753185661333,-2.3485149824550183E-3,4.4599561431920128E-2]
[null,1128,1.0186058882499935,1.000454386085186,0.98668264722586574,0.99971816332228158,1.0047755697649035,0.97492291912687412,0.99799691030426219,null,6.7197828524318215,0,1.0090160278054464E-2,0.18444231407650036,0.11997720800201088,8.2231743422523026E-2,0,1.0090160278054464E-2,0.26218297098012627,5.9128611700140157,0,1.9055514075952646E-2,9.772357705090963E-2,-2.4112923366333765E-4,4.1549484043450144E-2]
[null,1129,0.99755532218021303,0.9884074845827171,0.99175151031822539,0.96547645861943243,0.9963930607417073,0.98520814274287272,1.0419983647065534,null,6.7512854414580259,0,1.0419770423364881E-2,0.19190423435263171,0.12300891672537845,8.2769502402775988E-2,0,1.0419770423364881E-2,0.2806616039676153,5.9107285937184582,0,1.9168453780562533E-2,0.101420382228972,-1.2830056717902663E-3,4.2906759953419651E-2]
[null,1130,1.0028998453938773,1.0117209507222718,0.99571597451045479,1.0264183066629247,1.0322826408221761,0.97325798172648392,1.0323747496911491,null,6.7394053521465285,0,1.0101780939438153E-2,0.18714415666443732,0.12114421571156291,8.2987038915212821E-2,0,1.0101780939438153E-2,0.27521492364350408,5.9138009775550984,0,1.9139330489250823E-2,9.8709667223568748E-2,-3.3229391473137517E-4,4.159733585862755E-2]
[null,1131,0.99671126736024873,1.0140700746628375,0.99330119489227486,1.0221420431201313,1.001509920142025,1.041386243640871,0.95666448751064437,null,6.748850282807477,0,1.0888157270645816E-2,0.20099183286826847,0.12182839835562835,8.2667630438351639E-2,0,1.0888157270645816E-2,0.26271927478494123,5.9137048784537267,0,1.9173081748456638E-2,0.10614115996657338,-3.2114674292414748E-3,4.4835493620771619E-2]
[null,1132,1.017633927826187,0.99620247808654061,1.0219266239916094,0.97661606045712313,1.0185473432029299,1.0437253845847703,0.98145865213722072,null,6.7454261458010283,0,1.0503733369226326E-2,0.20229023490335465,0.11964525041030369,8.4429480559643166E-2,0,1.0503733369226326E-2,0.26444584295943058,5.9096240719487731,0,1.9060625911367656E-2,0.10532352608243327,-2.6453913939086461E-3,4.3252504419629842E-2]
[null,1133,0.96718744702128934,1.0167361236821086,1.0275886666105911,0.99153370741194469,1.0408815016365911,0.9894883067678738,1.0298932015758764,null,6.7714321911988433,0,1.0334773336890512E-2,0.20070975056667256,0.12475227578997305,8.5093259907847579E-2,0,1.0334773336890512E-2,0.28632170131601598,5.9101040964533347,0,1.9340044108839025E-2,0.10421014721127589,-1.6558412353577521E-3,4.2556757080235597E-2]
[null,1134,0.96456509107284005,1.0236419915530421,1.0175385400258041,0.97855521548204794,1.0298914062406046,0.97074184679173448,1.008970630361161,null,6.7568802110845017,0,1.0226736998948651E-2,0.19568122026051696,0.12494869197567002,8.4366023606549795E-2,0,1.0226736998948651E-2,0.2793550989242175,5.9099801384960733,0,1.9355368226940669E-2,0.1021029916487054,-1.0212047245172951E-3,4.2111882670342327E-2]
[null,1135,1.0160599242333495,1.0153637433419569,0.98582043066842928,0.99345974318927011,1.0264186841593534,1.0264280722282784,1.0128536579521319,null,6.7423343474083239,0,1.059056045834829E-2,0.19334196418111016,0.11958394749953467,8.2296418323707085E-2,0,1.059056045834829E-2,0.27142955391761553,5.9125706669271727,0,1.906892481765218E-2,0.10248302465746914,-2.0501958339256719E-3,4.361004291798834E-2]
[null,1136,0.99116299259240315,0.98881044938526164,0.97115043857040051,0.98971145006413053,0.97466765388287124,0.99477600539854505,0.95663633480739507,null,6.7355745814265564,0,1.0778823420992139E-2,0.1925417040518082,0.12416976747002344,8.1233895941672671E-2,0,1.0778823420992139E-2,0.26016799467434482,5.9131747228918314,0,1.9203699236399745E-2,0.10281173102318768,-2.1142101513084905E-3,4.4385276288597557E-2]
[null,1137,1.037043299921637,0.99675746113355601,1.0049185616605998,0.97210640190932174,1.0013274890327246,1.0387837482628735,0.97304190042265581,null,6.7260270159918871,0,1.0409638618559956E-2,0.19549460476761144,0.11768951242313258,8.3269508785667759E-2,0,1.0409638618559956E-2,0.25679925134047549,5.9103484961302755,0,1.8960360980415245E-2,0.1026440042173099,-2.0437616376310537E-3,4.2865038984626985E-2]
[null,1138,0.96038166542953596,0.97196181908100787,0.9742749098558372,0.98132444177254052,0.95612477911553773,0.98087577561446748,0.98973837251602326,null,6.7650843480559706,0,1.1019927941844483E-2,0.19776369258866902,0.12897270504602448,8.1640874638067282E-2,0,1.1019927941844483E-2,0.27661943561935343,5.9125504893134222,0,1.9379987923428769E-2,0.10543455314978677,-2.6554920132489594E-3,4.5378101790462588E-2]
[null,1139,1.0264580096655289,0.9822792127220964,1.0030656516159966,0.97944140855944806,1.0015337319416298,0.98283838308228222,1.0221659359617781,null,6.7276980789732157,0,1.0029387957300892E-2,0.18783726067541079,0.11963526609657396,8.3303533126839746E-2,0,1.0029387957300892E-2,0.26742321885504039,5.9108493787430652,0,1.9014572394301071E-2,9.8714181717681246E-2,-3.7856707935117934E-4,4.1299234443656789E-2]
[null,1140,0.97775972021071211,1.0225758693331519,0.99355443017866707,0.97883850345282841,1.0112002960247315,0.98628039944459556,1.0138090998834259,null,6.7527830406673894,0,1.0472044632143379E-2,0.19338310122052291,0.12377071640699126,8.2862370007139835E-2,0,1.0472044632143379E-2,0.27837764295885681,5.9113502558610627,0,1.9279097208289877E-2,0.10211021097321946,-1.4723698094022181E-3,4.3122015840707205E-2]
[null,1141,1.0087507309364192,1.0048724877809032,0.97189062156958295,1.0093281494517252,1.0171367765637602,1.0126743562551983,1.0217043795986369,null,6.7461219152064986,0,1.0700386608586363E-2,0.19135074741016034,0.12120748325663522,8.1481380803817352E-2,0,1.0700386608586363E-2,0.27456437480189039,5.9141949249293058,0,1.9107801778187699E-2,0.10213780191012001,-1.9848871399641174E-3,4.4062287456342719E-2]
[null,1142,1.0100097459222701,1.0474602239575836,0.98981767191634806,0.98717115101055619,0.98475384110272546,0.97948588398915615,1.0082444761139129,null,6.7213610785248763,0,9.997363796782217E-3,0.18359752533465143,0.11873962282370211,8.2484415504517114E-2,0,9.997363796782217E-3,0.26717141233155156,5.9120088533866211,0,1.9101065073442666E-2,9.7123915583716636E-2,-3.3096164056481829E-5,4.1167364650728969E-2]
[null,1143,0.96791216103570643,0.97391813866504651,0.98728114793828137,1.0020090110009019,0.98007760883239059,0.96301234593862062,1.0000469474616227,null,6.7568323494646538,0,1.0604888924215412E-2,0.19402338097638841,0.12761429602547369,8.2451901707236458E-2,0,1.0604888924215412E-2,0.27556870542230749,5.9129517976829149,0,1.9335823781832392E-2,0.10276922579127264,-1.5518269128363047E-3,4.3669044990057311E-2]
[null,1144,1.0081098495004686,1.0394504332357939,1.0126870634562302,1.0071373898005096,0.98610460237438058,1.0174617703720641,0.98735921313436514,null,6.7361710909728219,0,1.0232253352366327E-2,0.19438618637931573,0.11891041290727589,8.3897681427725856E-2,0,1.0232253352366327E-2,0.26567785270716715,5.9118010991053183,0,1.9111237452695017E-2,0.10167043257329142,-1.4184096118121583E-3,4.213459803184199E-2]
[null,1145,1.0247875599434053,0.97259997594411784,1.0421366414864914,1.010166215697383,1.0117580480841095,0.99324722134552912,0.98334676844764779,null,6.7295284821719221,0,9.8523894545011446E-3,0.19549926682867641,0.11957572341511861,8.5622859953340888E-2,0,9.8523894545011446E-3,0.25879827208853351,5.9102650436072999,0,1.9023229733163297E-2,0.1007843818850639,-6.1068145295984592E-4,4.0570386113686484E-2]
[null,1146,1.042895298016802,1.0264584261629643,1.0029909314948964,0.96701682407559597,0.97825415262745408,0.98708682494510447,1.0251677102314927,null,6.7104999381528909,0,9.7295821261727741E-3,0.18220212559226742,0.11569700572055273,8.3242430793659422E-2,0,9.7295821261727741E-3,0.26397218093236507,5.9101821630707683,0,1.8930862977262458E-2,9.5756296110575276E-2,4.5218556091703056E-4,4.0064687394519828E-2]
[null,1147,0.96375349130561216,0.96279486368860967,1.0144730662929253,0.99467390722888127,0.95294617194726239,0.97196966086136116,0.99411458596666502,null,6.766331967155212,0,1.0549190970007429E-2,0.20093760759252616,0.12821818478946345,8.414449166495537E-2,0,1.0549190970007429E-2,0.2761599579569069,5.9110259690091187,0,1.9360127826879753E-2,0.10500438010452603,-1.9584425176632286E-3,4.3439690728495108E-2]
[null,1148,0.96220465490155793,0.9598391328914575,0.96118519932694479,0.98478476464529607,1.0057163481453761,1.028053723756216,1.0244617223043793,null,6.7947823561968734,0,1.1723117135090782E-2,0.20633306149360739,0.12963126962865459,8.100878639299311E-2,0,1.1723117135090782E-2,0.29071152254319488,5.91344934306154,0,1.9369233208886269E-2,0.11073017114149558,-4.7247409987376116E-3,4.8273709725240331E-2]
[null,1149,1.0031052282283608,0.99941883987931857,1.0098556466348718,0.99104028101247588,1.0068983349568634,1.0090910592910936,1.0025001900372996,null,6.7469168293279553,0,1.0397302043192041E-2,0.19669556306587549,0.12144901952524555,8.377880720254266E-2,0,1.0397302043192041E-2,0.27070445604616111,5.9110922106488797,0,1.9138217512414082E-2,0.10302241469653695,-1.7780985327934924E-3,4.2814239163090469E-2]
[null,1150,0.96118814261994678,0.98149522672359302,0.97153072851792843,0.99554638758141734,1.0031567601237072,0.9761285595295589,0.97491613582300762,null,6.7569132019516243,0,1.0937749414707191E-2,0.1954909341929546,0.12841553889835858,8.1414967855703138E-2,0,1.0937749414707191E-2,0.27168836163899418,5.9134694430306389,0,1.937522508482812E-2,0.10436658972954341,-2.3475637223401239E-3,4.5039705242943755E-2]
[null,1151,0.96374179651670344,0.99939555139824277,1.015614197035547,0.96322571037395011,1.0210255018566214,1.0013907784842848,1.0253973575983615,null,6.778460609915733,0,1.0685535701168414E-2,0.20387865406188951,0.12629802804348667,8.4345083074618341E-2,0,1.0685535701168414E-2,0.28743491320392739,5.9092617691222209,0,1.9360196469170657E-2,0.1064812961107707,-2.6004642333090316E-3,4.4001134062958559E-2]
[null,1152,1.0352800305851446,1.0036509334763257,1.0156178450861928,1.0241167644905318,1.0043521892622922,1.0059466343571652,1.0104271326041476,null,6.7271614052024349,0,9.9742168628225158E-3,0.19030780896410468,0.11737107112143744,8.4067455664038407E-2,0,9.9742168628225158E-3,0.26404360467921645,5.9125514646832498,0,1.8969314421271304E-2,9.9393365978471884E-2,-6.1473000603895142E-4,4.1072049696683578E-2]
[null,1153,0.9822753281756561,1.0248128403053836,0.9989400510926193,0.96748106297715175,1.0268440137667649,0.96130808966189207,1.007983325505315,null,6.7372993822618348,0,1.0102853999527242E-2,0.18806032436773332,0.1229925329070502,8.311820731012963E-2,0,1.0102853999527242E-2,0.27310480834252832,5.9104350118075937,0,1.9253465538864277E-2,9.9034029870875284E-2,-3.0075241201300097E-4,4.1601754529076863E-2]
[null,1154,0.99258988009700355,0.99313318197599787,1.0121476763976041,1.0038142144386792,1.0176349218014831,1.0131068285027653,1.008669123008392,null,6.7599559319610929,0,1.0556631574726525E-2,0.20038848292950018,0.12300214863673443,8.3998680485915467E-2,0,1.0556631574726525E-2,0.27571275608950896,5.9116522272511851,0,1.9195792434562868E-2,0.10483777094937864,-2.3022566300411724E-3,4.3470329814350069E-2]
[null,1155,0.96123679810192852,1.0192181046193014,1.0141535587349892,1.0066693651530505,0.99781198377142832,0.97762924026947207,1.0408876145087176,null,6.7733464548344591,0,1.0384846737765813E-2,0.19771372164961962,0.12566471534063844,8.4319970362816202E-2,0,1.0384846737765813E-2,0.28991982762188911,5.91169229817279,0,1.9374937994192213E-2,0.10333596766888221,-1.4379344086807068E-3,4.2762950432306997E-2]
[null,1156,1.0124480323433023,1.0058888225140985,1.0404935566543103,1.006380694693245,0.98600428489279679,0.97331230607815655,0.98020370399298384,null,6.7225979151687172,0,9.6463030991686145E-3,0.19094598551644804,0.11944563607197362,8.5522148826916708E-2,0,9.6463030991686145E-3,0.25897028860497978,5.9101566699338832,0,1.9088065998250303E-2,9.8516074086081082E-2,2.3128694575103153E-4,3.9721759184430917E-2]
[null,1157,1.0165279331695471,0.96522028654745706,0.98338441527948517,1.0258272776687025,0.97158041424194441,1.0186162764243585,0.97484107028618316,null,6.7399046938558218,0,1.0758412442327123E-2,0.19569793908468847,0.12202025117418296,8.2029266539552934E-2,0,1.0758412442327123E-2,0.26095291215529065,5.9144551529222156,0,1.90664545640153E-2,0.10385819958998578,-2.4767096855847588E-3,4.4301227511473765E-2]
[null,1158,1.0215596399167071,1.0458166611137203,1.0029096806648445,1.0035474319087798,0.98812639700631166,0.96727198192178399,1.0002023013589709,null,6.7090750258748706,0,9.6566042161241403E-3,0.1808137350722101,0.1172354224199775,8.3225046612251483E-2,0,9.6566042161241403E-3,0.26097197909911285,5.9121608615796326,0,1.9040039095398326E-2,9.5030457672541715E-2,8.3330697321705785E-4,3.9764177350523323E-2]
[null,1159,0.99154416180933735,1.0098952056726176,0.9990952982625978,1.007311329962435,1.0064344443835702,1.0152721388348369,0.96205809877147408,null,6.7443332633333117,0,1.0635357458792636E-2,0.19801819089739783,0.12255664700687571,8.3024047699715955E-2,0,1.0635357458792636E-2,0.26325410047217046,5.9125788653080633,0,1.9201584838489407E-2,0.10426987700664064,-2.3645588882882959E-3,4.379450899224932E-2]
[null,1160,1.0161466125423753,1.019857870836653,0.9923193232067844,1.010116706835481,1.0050288587213829,1.0222141380499357,1.0050882864789317,null,6.7391893667303178,0,1.0466745109519926E-2,0.19293170458400608,0.11924441898033343,8.2678960015373032E-2,0,1.0466745109519926E-2,0.26890079547057238,5.9131097242104058,0,1.9068467086071968E-2,0.10193455203687603,-1.7794490031495453E-3,4.3100193349823658E-2]
[null,1161,0.99319477691592228,1.0169946654997886,0.99012663118496103,1.0049454866539431,1.0065289888388025,1.0029167597204838,0.9894627328986999,null,6.7435969581568553,0,1.0539263965493803E-2,0.19363797887313425,0.1221782424650754,8.2542757220760724E-2,0,1.0539263965493803E-2,0.2690640686662773,5.9129523892631806,0,1.9192447381036731E-2,0.1024195796393654,-1.7893184428307181E-3,4.339881309084892E-2]
[null,1162,0.99805544127862755,0.96006684543267373,1.0483923550520278,0.97927253572011086,0.98145422960572981,1.0104961031164155,0.95781378760015645,null,6.749481966255324,0,1.0292691087757044E-2,0.20613131419114394,0.12329518104304861,8.601109960741779E-2,0,1.0292691087757044E-2,0.26056167791497153,5.9082296165115178,0,1.9165715311595E-2,0.10594184128543455,-2.2379494784687788E-3,4.2383469868665105E-2]
[null,1163,1.0036836314484083,0.98297162908240188,0.99405823373588043,0.9597007081081157,0.99847923001765782,1.0174490814401209,0.99684635747556238,null,6.7483160245295686,0,1.0698796543724978E-2,0.1977180235195542,0.1224846192420241,8.2765733801815705E-2,0,1.0698796543724978E-2,0.269958792797731,5.910287769866355,0,1.9135085572601084E-2,0.10437295393654998,-2.4626940593236346E-3,4.4055739852264526E-2]
[null,1164,1.0328811224681356,1.0342524881028832,1.0194123125115706,1.0077881885775632,0.99591489624151652,0.98876850716084175,0.96702120137672409,null,6.7046239730066324,0,9.6689809401674168E-3,0.18552254822507008,0.1161702829823443,8.4120204107332716E-2,0,9.6689809401674168E-3,0.25152512161937723,5.9114523004437789,0,1.898154456266056E-2,9.6713012971025775E-2,3.2381559788048349E-4,3.9815142497158763E-2]
[null,1165,0.99279996615508348,0.9710931112720671,1.016588592161757,0.98630516099322041,0.99783648233493694,0.99272996889146126,0.99713224185035776,null,6.7522010665460064,0,1.0401582335363193E-2,0.19874721311647964,0.12399965056553319,8.4194615358554326E-2,0,1.0401582335363193E-2,0.27080411158164996,5.9104531209225737,0,1.9194630205646383E-2,0.10375136842900136,-1.7755082778232493E-3,4.2831864644387672E-2]
[null,1166,0.96586805105880058,1.0220179861035488,0.99143575157084762,1.0079108836749902,1.0220163075607112,1.0196291403637869,1.0159621366759652,null,6.7773745388762627,0,1.0982272749950752E-2,0.20216936502764904,0.12536252315279911,8.284952423580598E-2,0,1.0982272749950752E-2,0.28568058108495226,5.9130397637609482,0,1.9347743789966114E-2,0.10686226410172957,-3.1602706902063328E-3,4.5223044412618499E-2]
[null,1167,1.0385827137703363,1.0116372829043594,1.0083054561989642,0.99065167734761062,0.9970837919455976,1.0239265011261478,0.98742069366809093,null,6.7217317215237733,0,1.0150637223461073E-2,0.19158896389367377,0.11675957788221711,8.3518430903523441E-2,0,1.0150637223461073E-2,0.25872686519896509,5.9111590994901881,0,1.8952569078978545E-2,0.10042475143716317,-1.1970537010784182E-3,4.179851734013957E-2]
[null,1168,1.0194901866752994,0.96929804326258939,0.99464658746218859,1.0145421069146554,1.008541357171604,1.0345261287215244,0.99291620319200413,null,6.748601586887605,0,1.0768681865599228E-2,0.19918314410098534,0.12125221969842975,8.2794107233679443E-2,0,1.0768681865599228E-2,0.26647043313193691,5.9132189378930722,0,1.9050871749677886E-2,0.10511558351784679,-2.8272256066459449E-3,4.4343515168619098E-2]
[null,1169,0.98938296904734224,1.002276989333365,0.98888924306671144,0.98534787439176885,0.96546531948138725,0.98571149047139428,0.96042952351675437,null,6.7330698296901197,0,1.0474776682037747E-2,0.1921004038998326,0.12338951103045197,8.2341456492194168E-2,0,1.0474776682037747E-2,0.26074014965768177,5.9119619175155877,0,1.9213594839759807E-2,0.10166904852731949,-1.4795182085919904E-3,4.3133265935885449E-2]
[null,1170,1.0005560468457579,1.0153935753843308,0.98781078403856415,1.0128405126065112,0.99041342997348758,1.0040434968690219,0.97262327664566639,null,6.734706005670561,0,1.050174257645348E-2,0.19228720849487171,0.12139869192301037,8.2318753378586587E-2,0,1.050174257645348E-2,0.26265261444416033,5.9135078758193105,0,1.9152063975878826E-2,0.10182269643653766,-1.6782054911350711E-3,4.3244306689339165E-2]
[null,1171,0.98896403289878454,0.98871399533310156,0.9997035101056152,1.0217299686613672,1.0192020721145674,1.0013343317049157,1.0171321024145472,null,6.760940142628292,0,1.0607000648875696E-2,0.19766825711863922,0.12391107605345179,8.3268913985875825E-2,0,1.0607000648875696E-2,0.27792581019471496,5.9133239263033461,0,1.9215928990767239E-2,0.10405417045388007,-2.1056811687213692E-3,4.3677740696335364E-2]
[null,1172,1.0032302903763386,1.0332463954519144,1.0195150326490914,1.0404839568890827,1.0140965801906412,1.0117662805815251,0.99594231568203007,null,6.7433137733393309,0,1.0189614293779667E-2,0.19554185764983434,0.11964839686842652,8.4387979984490352E-2,0,1.0189614293779667E-2,0.26883489661293847,5.9132128388358884,0,1.9137540019442283E-2,0.10193092595007144,-1.3396805598184735E-3,4.1959017978051634E-2]
[null,1173,0.97768090689760156,1.0078666328826504,0.97690768138980288,0.9741171824260364,0.99334140337849675,1.0428388611030346,1.0125453440551375,null,6.7763232520428245,0,1.1305304031194554E-2,0.20367937115508455,0.12481594563823534,8.1891380460591065E-2,0,1.1305304031194554E-2,0.2836618743940772,5.9120165240246569,0,1.9279546673777091E-2,0.10844509189083773,-4.0197119257954295E-3,4.6553229731355818E-2]
[null,1174,0.98091258815049753,1.0071634506277367,1.0008744865417127,0.97670810442771983,1.0000125245322393,1.0173054990631656,1.0132106751603078,null,6.7662796901846258,0,1.0767911135474402E-2,0.20101533480688588,0.12398537638016374,8.3344075171768006E-2,0,1.0767911135474402E-2,0.28048593076861483,5.9108250087745278,0,1.926117591400768E-2,0.10575458741232199,-2.7321404828213095E-3,4.4340341439149916E-2]
[null,1175,1.0074084634678744,0.98821400538177218,0.99971808293678932,1.0074770590576354,0.97568631261493077,1.0111220486581198,1.0241743617498502,null,6.7527621473471688,0,1.0516726404429211E-2,0.1959901700507255,0.12166675622427933,8.3228008798496469E-2,0,1.0516726404429211E-2,0.27567449153146117,5.9125528383092893,0,1.9115002493618062E-2,0.10317006506918867,-1.941192555816376E-3,4.3306007425921257E-2]
[null,1176,1.0201466423917458,1.0236203375886253,1.0066359748708988,1.026552180964486,1.0028591182759592,1.0225142045873452,0.99366113529413813,null,6.7349308417173956,0,1.0282938632591235E-2,0.19360692051105541,0.11834155675699927,8.3524452948020689E-2,0,1.0282938632591235E-2,0.26481558856828158,5.9131935567890244,0,1.9047430740576816E-2,0.10156641869082833,-1.5083942815552272E-3,4.23433109941646E-2]
[null,1177,0.98723603336838672,0.99297469187809728,0.98718195763350869,0.98545934734846963,0.97480447893438404,0.97138536533055531,0.98252084108561322,null,6.7366150591521237,0,1.0401871145013652E-2,0.19028104782087765,0.12415223628161258,8.2306183250161785E-2,0,1.0401871145013652E-2,0.26605488736359922,5.9120627315620444,0,1.9225577676593761E-2,0.10079199856266716,-1.0926572765539014E-3,4.2833053911122076E-2]
[null,1178,0.9946465209115064,1.0011288365823927,0.97148786266373999,0.97207971721542397,1.034042106306847,0.97853040262647784,1.0074290151782959,null,6.7373633763927598,0,1.0506682665621209E-2,0.18777450673413756,0.12311736363096146,8.1388724559427028E-2,0,1.0506682665621209E-2,0.27134804633637249,5.9122030070768838,0,1.9184435898606571E-2,0.10024918587571342,-1.1665428165716393E-3,4.3264649097228776E-2]
[null,1179,1.0141777865738457,1.0262066306923203,1.01231261347142,0.97282782858379624,1.0067820532104204,1.0135504454408042,1.0189388384095679,null,6.7395402735822465,0,1.0191003834516071E-2,0.19349528274344976,0.11881367276362764,8.3938499531544392E-2,0,1.0191003834516071E-2,0.27229465435688055,5.9099685843312448,0,1.9078882173076739E-2,0.10122318669174354,-1.2372288687941494E-3,4.1964739859475131E-2]
[null,1180,0.98054994501644177,0.99812735754606574,1.0245952185265799,1.0021860511179046,0.99266075437633372,1.0106492900754249,0.96280060674205792,null,6.7550327617137729,0,1.0522179147291951E-2,0.20344683587656695,0.12402274232024778,8.4639173433200418E-2,0,1.0522179147291951E-2,0.26614736265254135,5.9108520641197293,0,1.9263231357173349E-2,0.10578675055371231,-2.4538594498806567E-3,4.3328460850477965E-2]
[null,1181,1.0040685537040432,0.99165145004507371,1.0330457875427552,0.9820860927026559,0.99467513903821025,1.0237588047685562,0.96656910914692673,null,6.7452726214198844,0,1.0361062039108682E-2,0.20285000812737569,0.12127308207883807,8.5090307273417196E-2,0,1.0361062039108682E-2,0.26220520187987917,5.9092780409294834,0,1.91330032939049E-2,0.10503983472145988,-2.2618661612310237E-3,4.266500927675547E-2]
[null,1182,1.0198414430671849,1.0003494884400643,1.0012840324620775,0.95821561583907378,0.9958274764315892,1.0028846583702131,1.0063580910302854,null,6.7310728663385877,0,1.0236132538746133E-2,0.19120405914028155,0.11956940175023903,8.3168230615422972E-2,0,1.0236132538746133E-2,0.26668531192631917,5.9098026127272174,0,1.904902998317122E-2,0.10057240587694177,-1.1287575118936106E-3,4.2150571830884602E-2]
[null,1183,1.0114740036931644,1.0145693648085528,0.98805710705619865,0.98835244642635312,1.0076150453399386,1.0217406462589036,0.99584110656367553,null,6.7391447808574574,0,1.0572893252911102E-2,0.19366070097311558,0.12012280420739015,8.2382212331976068E-2,0,1.0572893252911102E-2,0.26766012766600483,5.9121705439930201,0,1.9093251255489292E-2,0.10253740156906327,-2.0195536492460947E-3,4.3537292510643338E-2]
[null,1184,0.96008430678253998,0.98348151440789777,0.98146161934053777,1.0150473871590651,1.0157798164238039,0.97165960160395792,1.0187559257347427,null,6.7699157697907086,0,1.0796920432700516E-2,0.19583901899918402,0.12826636817155995,8.2207712427838392E-2,0,1.0796920432700516E-2,0.28377933284824108,5.9139786231260834,0,1.9381746063132789E-2,0.10403308357378434,-2.0299119807757004E-3,4.4459796561664641E-2]
[null,1185,1.0285799156622564,0.98526816792721561,0.99562663118982997,0.97383651097881285,0.97934429373961529,1.0063525329478442,0.96417746108744617,null,6.7183659312976527,0,1.0301539933365703E-2,0.19081959662319845,0.11937975240963619,8.2655582977999756E-2,0,1.0301539933365703E-2,0.25378294876095225,5.9109641206564518,0,1.9003615866292047E-2,0.10065276135362018,-1.3123551903482782E-3,4.2419907839845755E-2]
[null,1186,0.9675836304559523,0.99999279885861803,0.96865441444135947,0.98852385358911588,0.98574683190074819,0.95974209956852319,1.0159029639439823,null,6.7527053956328604,0,1.0624505378490471E-2,0.18908307048149633,0.12667246457794024,8.1331306190908989E-2,0,1.0624505378490471E-2,0.2794304567341826,5.913246553002975,0,1.9337736175875458E-2,0.1010917061072583,-1.2377196949386153E-3,4.3749822057163282E-2]
[null,1187,0.97717007957976287,1.0044583464322918,1.0133987481442392,1.0156011886109788,1.0295699048547011,1.018327608804567,0.978561073233565,null,6.7635361212807288,0,1.071451984897095E-2,0.20376251098825932,0.12435362772364082,8.4036859061749319E-2,0,1.071451984897095E-2,0.27207787766093661,5.9122178947178847,0,1.9282461635529234E-2,0.10653710013276983,-2.8526962646625623E-3,4.4120485624623437E-2]
[null,1188,0.97407170777738383,1.0033359786455909,0.97054865876761631,1.0187880227280171,0.97723316643876357,1.0346770061618793,1.0169943809974329,null,6.7798141590142791,0,1.1342779756758929E-2,0.20243468709209084,0.12562500099884269,8.1546201564708445E-2,0,1.1342779756758929E-2,0.28520488671941546,5.9147796659251108,0,1.9300207554028184E-2,0.10812699705817051,-3.911035996884118E-3,4.6707548098799449E-2]
[null,1189,0.99165591735425695,1.000549500741273,0.96723691093691455,0.96087625261653253,1.0028215172547583,1.029515112770123,0.97382086653717159,null,6.7494899993653616,0,1.1131322430756842E-2,0.19768626532253186,0.12359635763096803,8.1069513500089257E-2,0,1.1131322430756842E-2,0.26780249477093143,5.911828725274165,0,1.9200965223305146E-2,0.10576674616697158,-3.2978729919258148E-3,4.5836804468323784E-2]
[null,1190,1.042052273919345,0.95914924050636918,1.0045823852238971,0.98876128943126795,0.98376741913705645,1.0272772939920976,1.0050258153566041,null,6.7350582986072203,0,1.0418221959070518E-2,0.19555841548445818,0.1189457628433679,8.3348546469572432E-2,0,1.0418221959070518E-2,0.26335218198152471,5.9112674791434916,0,1.893509195905041E-2,0.10269461876358531,-1.9441816909080375E-3,4.2900383653071826E-2]
[null,1191,0.97130551843249668,1.0039333359321541,1.0259845929987947,1.0106440532170862,0.96265700573371915,0.9952193857954531,1.0297980270134137,null,6.7740125131901339,0,1.0421506607157028E-2,0.20191473222313738,0.12488591277297292,8.5000130158761983E-2,0,1.0421506607157028E-2,0.28577556072390081,5.9112289494452011,0,1.9316146557295095E-2,0.10491842350814377,-1.9412514485263931E-3,4.2913909249246505E-2]
[null,1192,1.0034831871568277,0.99815418772307896,0.99522017916361749,0.98175033563790381,0.99576346457797338,0.96851124253702725,1.016562727627472,null,6.732827171828359,0,1.0109295865565821E-2,0.18714581964638002,0.12173862057183335,8.2861142790155246E-2,0,1.0109295865565821E-2,0.27050803302696491,5.9114145672059717,0,1.9136170530264E-2,9.8734897792380719E-2,-3.4036072240542921E-4,4.1628280986814301E-2]
[null,1193,0.9681481900770299,0.99860303367192282,0.97568592154090161,1.0071345405140932,0.97552408529519341,0.97809599937493341,1.0276722240382028,null,6.7650258500071603,0,1.0761716532580711E-2,0.193534718737049,0.12653472390085471,8.1848499789590898E-2,0,1.0761716532580711E-2,0.28436516568496067,5.9138685749752513,0,1.9334450645371655E-2,0.10310692199860345,-1.8820388915538613E-3,4.4314833167031914E-2]
[null,1194,0.98945895535356543,1.0027342808881592,1.0333527264619398,0.97071534710403207,0.96572357756797123,0.98405691786097094,0.95437934885602549,null,6.7337633719109435,0,1.0055598815281602E-2,0.19695893770269476,0.12251192514127866,8.5057844042028125E-2,0,1.0055598815281602E-2,0.25899680812111558,5.9086460535954153,0,1.921317168506791E-2,0.10197398301244007,-1.002517480560455E-3,4.1407166091462541E-2]
[null,1195,1.0042269377183728,0.99578128611313654,0.96684394362113524,1.0474315801319762,1.0098315325709224,1.0075144955786031,0.97635197101668014,null,6.7382408740674746,0,1.0782803238945997E-2,0.19138502835565221,0.12228982571301497,8.1044636245506646E-2,0,1.0782803238945997E-2,0.26316947873843194,5.9165302179384387,0,1.9132146961941709E-2,0.1024156945906524,-2.1278189467134573E-3,4.4401664470550342E-2]
[null,1196,1.0125130162294451,0.99942901706219611,1.0004306105988208,1.0077537562616417,0.98760102219870993,0.99006846013648819,1.0006615304775206,null,6.7323981663100723,0,1.0190071396046678E-2,0.19010317840229235,0.12049498916743812,8.3141238694360201E-2,0,1.0190071396046678E-2,0.2659085058674861,5.912527740560102,0,1.9087720410480444E-2,0.1000357230867555,-8.6183012267471181E-4,4.1960900243826017E-2]
[null,1197,0.9895621216060646,1.0187031302831759,1.0049652705597896,0.99916815402874404,0.96267302859673631,1.0429969776215051,1.0090093281770403,null,6.7683177464044588,0,1.0851249341572698E-2,0.20380221879577712,0.12226585849303068,8.3596923593983768E-2,0,1.0851249341572698E-2,0.27921821530723206,5.9118082342896106,0,1.9212597273933717E-2,0.10700342114536593,-3.2732358326918978E-3,4.4683513338214999E-2]
[null,1198,0.97853927875814439,0.98806485567882418,0.98722291724944577,1.0221739848816918,0.97113234603759435,0.98926657598744905,1.0195439066437699,null,6.7634438128480134,0,1.0709836672488206E-2,0.19592654985528266,0.12550344978273353,8.2525294636770261E-2,0,1.0709836672488206E-2,0.28034617861857625,5.9140450191493708,0,1.9274655353328118E-2,0.10378030259130101,-2.0588382767979907E-3,4.4101201137441828E-2]
[null,1199,1.0210080911997443,1.0178737276455248,1.0249140939324941,1.0154360737376196,0.98664430765624744,1.0235902727126986,0.96706927710258328,null,6.7296339628761661,0,1.0146297671366209E-2,0.19627167839179097,0.1181726778076668,8.4550215389946545E-2,0,1.0146297671366209E-2,0.25769195447990928,5.9115494930495265,0,1.9042921911967461E-2,0.1020398681374122,-1.465494129080854E-3,4.1780647837024384E-2]
[null,1200,0.96651254790291052,1.0407696995725519,1.0148421230161255,1.0177099246476433,0.97118159073321397,0.97591265611269284,1.0449307455187724,null,6.766411977541396,0,1.0211983052240133E-2,0.19462084393510326,0.1239238433924274,8.435928231000496E-2,0,1.0211983052240133E-2,0.28909803160144698,5.9122495670462962,0,1.93439800332918E-2,0.10168488803947705,-9.1958736055381405E-4,4.2051128543901244E-2]
[null,1201,0.96330472689388824,1.0052921377913497,0.98427067786832578,0.98837504399357445,0.97748053725592443,1.00873358210038,1.0035076187435545,null,6.7728721869618731,0,1.1039849245918793E-2,0.20108149706817907,0.12666676361658288,8.2340521311654299E-2,0,1.1039849245918793E-2,0.28202840402248464,5.912381601211627,0,1.9362763034235793E-2,0.10666801815305657,-3.1175156307294942E-3,4.5460134174780648E-2]
[null,1202,0.99261292252304645,0.98326316689576698,1.0290727260025538,0.98136897894696329,1.0160142630887674,0.98333538433244483,0.9719469337179576,null,6.7400355103519951,0,1.0138764532933669E-2,0.19733557938553259,0.12316684711730941,8.4856901762729822E-2,0,1.0138764532933669E-2,0.26303534403486256,5.9094693127931128,0,1.9195664936239022E-2,0.10238363055545696,-1.157397947053268E-3,4.1749627713807844E-2]
[null,1203,0.98895872626741321,0.96912813418421995,1.0187985808374567,1.0465435023435683,0.98878289770266869,1.0053846088821501,1.0095863133522678,null,6.7675381379919317,0,1.0563826698508931E-2,0.20250835610021592,0.12453941583459328,8.4453445547072598E-2,0,1.0563826698508931E-2,0.27651146658361458,5.9135812620788624,0,1.9215958569958613E-2,0.10559965628838411,-2.3713810641760764E-3,4.349995805340174E-2]
[null,1204,1.0020808237626426,0.98709925389471187,0.98650741339318737,0.99888390562953078,0.98285310284497029,0.9943670600822514,1.0101735851709317,null,6.744609954940751,0,1.052312611875174E-2,0.19230670006315437,0.1226163443288265,8.2348161744856652E-2,0,1.052312611875174E-2,0.27173993378543188,5.9128257918594525,0,1.9143773333589163E-2,0.10189930256174334,-1.6024130466972127E-3,4.3332360310394752E-2]
[null,1205,1.0311877503434166,1.0022439853166389,0.99385271450333146,0.99254802012744814,0.98644563082075165,0.99343590091053302,1.0255531822070607,null,6.7257212353904468,0,1.0085241991169697E-2,0.18632252666751209,0.11829906641809661,8.2746755468161293E-2,0,1.0085241991169697E-2,0.26786502491119912,5.9120745736693179,0,1.8990211993041881E-2,9.8367473400343547E-2,-4.7362855071344606E-4,4.1529231413481103E-2]
[null,1206,0.98431878336206802,0.97981285522334272,1.0183011103103627,0.98702879164742574,0.96439291918272929,0.99129781237476289,0.95689817225545859,null,6.745048674311291,0,1.0420368284483792E-2,0.19961129662876106,0.12458851870221498,8.4180826482763524E-2,0,1.0420368284483792E-2,0.26189662262772501,5.9103943442779787,0,1.9241943690633263E-2,0.10411448598103462,-1.8885859189136274E-3,4.2909221839092009E-2]
[null,1207,1.0129118826078369,1.0411650146931715,1.0001314501380179,1.0070178476084424,0.98850477915865309,1.0289058147272938,0.98153089300560015,null,6.7341963532493958,0,1.0404604953672059E-2,0.19401945081955774,0.11849795219527121,8.3094514264408406E-2,0,1.0404604953672059E-2,0.26384849517134346,5.9125047894447507,0,1.9085600189195754E-2,0.10211170449937966,-1.8104645830887805E-3,4.2844311248577592E-2]
[null,1208,1.0375317308834946,0.9888773888671043,1.024959120471723,0.99124048752602378,1.0131737868410797,1.007086395045933,0.97316685139443393,null,6.7179714981550287,0,9.9456730594985453E-3,0.19240357273943146,0.11764200323934422,8.4483828098160435E-2,0,9.9456730594985453E-3,0.25401531200476329,5.9102398210999079,0,1.8957886232599249E-2,0.1000266609133063,-7.5209756769050015E-4,4.0954511395203071E-2]
[null,1209,0.99541294076048614,1.0267869472451905,0.9889954104445341,0.97909067073700462,0.98873545460568946,0.9936367671357359,0.96615728988621064,null,6.7286200757548622,0,1.0386083520103489E-2,0.19050381618104456,0.12146057164449883,8.2349374190987645E-2,0,1.0386083520103489E-2,0.26121102090512438,5.9116178026077737,0,1.9180215818116669E-2,0.10081871521248041,-1.2894840869999405E-3,4.2768043281834485E-2]
[null,1210,1.0221226796946259,0.9928810516426223,0.99301748934592959,0.97573398840055559,0.98670516325525859,1.0481126492403867,0.9711889626641641,null,6.7391259614412053,0,1.0785788000905612E-2,0.19901842118165836,0.11981247113283505,8.2590756505918794E-2,0,1.0785788000905612E-2,0.26091355212370326,5.911212426369624,0,1.9037099426835912E-2,0.1051138777644739,-2.9865982528732718E-3,4.4413955189032205E-2]
[null,1211,1.0173466268069309,0.97356100696819303,1.0029864875292995,1.0276009582763841,0.99982471410188523,1.0172078430334901,1.0443318443497331,null,6.7579048870754592,0,1.0513905270219845E-2,0.19688854613566167,0.12113941303864928,8.3491282934271951E-2,0,1.0513905270219845E-2,0.27912418182627319,5.9134563880200179,0,1.9062138785093063E-2,0.10347497002159324,-2.0264241834911487E-3,4.3294390497390249E-2]
[null,1212,1.0353277862140811,1.0098933910310359,0.97740368840859781,1.0260033986593642,0.99890187092961924,1.014299037555211,1.0358930752709217,null,6.7326911041645641,0,1.0370245693992801E-2,0.18697068390494329,0.11776269631032595,8.1792914902815983E-2,0,1.0370245693992801E-2,0.27134191065935209,5.914794369941017,0,1.8969071528324864E-2,9.9524129410299006E-2,-1.1674984254571846E-3,4.2702825932938622E-2]
[null,1213,0.96472982634339743,1.0042638912731026,1.0047351729571043,1.0201240364154565,1.0126265391525389,1.0178943790406261,0.97232503875816045,null,6.7704546298552968,0,1.0931466790125053E-2,0.20523886924473103,0.1261356582385236,8.3526563498424286E-2,0,1.0931466790125053E-2,0.27377598202900072,5.9129536546454258,0,1.9354403120111743E-2,0.10777000403773469,-3.3143394718353203E-3,4.5013834513180022E-2]
[null,1214,0.99230670489989214,0.97867690144991681,0.99562138204898942,0.97395783743174025,0.97914997904687173,0.99758796528798743,0.9890767259181481,null,6.7481929441106203,0,1.0615654252042644E-2,0.19663653372716219,0.12407639994751118,8.2862387026055723E-2,0,1.0615654252042644E-2,0.26909403114723973,5.9109709715225192,0,1.9197359782741601E-2,0.10372132706022284,-2.0794407967246738E-3,4.3713374693892935E-2]
[null,1215,1.027740357230291,0.97641543251352358,1.0056894576509281,0.98233955127353689,1.0317079839455263,0.98829755592435242,0.99056505250374793,null,6.722046377186822,0,1.007526683353358E-2,0.18943118648391635,0.11972410146344671,8.3360207897655872E-2,0,1.007526683353358E-2,0.25939472531797508,5.9108579410703106,0,1.9007945543486875E-2,9.9422430994879393E-2,-6.403170747019863E-4,4.148815548984746E-2]
[null,1216,0.99562374277477173,1.0321004759871315,1.0036924511063412,0.99213244563336334,1.0028793148479269,1.0191141098385659,1.0113114633771794,null,6.7519953556744179,0,1.0491131181301506E-2,0.19666759816575841,0.12091172982141846,8.3465636850242705E-2,0,1.0491131181301506E-2,0.27574629086771707,5.911499864200505,0,1.9179056233967411E-2,0.10332266817321029,-1.9980994912614006E-3,4.3200610852861254E-2]
[null,1217,0.97835316473869882,0.96091602655539909,1.0099295399769674,1.0252279858056905,0.98661289957258069,0.96057555473760059,1.0021409878582845,null,6.7545674854702691,0,1.0319489294993394E-2,0.19524486291524265,0.12649248910203825,8.3842858584753405E-2,0,1.0319489294993394E-2,0.27312797624107055,5.9129353231794752,0,1.9275715171135382E-2,0.10225884990793835,-1.1044097475466947E-3,4.2493820116161304E-2]
[null,1218,1.0041685732339209,0.99318485313726113,0.95803224740458914,1.0290797803356178,1.0112545685742087,0.96365586780353341,1.0050313855305952,null,6.7275958993584677,0,1.0405010714162133E-2,0.18227770627741055,0.12258655555875032,8.0528656256071321E-2,0,1.0405010714162133E-2,0.26677884226330179,5.9160147568388899,0,1.9132462488704934E-2,9.7976533977564673E-2,-5.4559640027796754E-4,4.2845982098053029E-2]
[null,1219,0.99838303144921359,0.98041124245449141,1.0424642239861943,0.96769444173887842,1.0154728594203246,0.99327543884053815,0.99919725796499115,null,6.7484281925217644,0,1.007572692971037E-2,0.20002766215851572,0.12233975941248747,8.5766040571466307E-2,0,1.007572692971037E-2,0.26984483373469287,5.9079521191276481,0,1.9163923034950927E-2,0.10310238646768177,-1.2585820696859561E-3,4.1490050084009404E-2]
[null,1220,1.0249270896912301,1.0332650792075007,1.0463006662109808,1.0044459187001897,0.99330115878344327,1.0166848356012923,0.99526576425846869,null,6.7304232016426573,0,9.78971610663288E-3,0.19545376641171158,0.11662384649930128,8.5939383141892908E-2,0,9.78971610663288E-3,0.26345416016467743,5.9097119942126888,0,1.9022505520635041E-2,0.10055648820158559,-6.5125093243994928E-4,4.0312308422605032E-2]
[null,1221,1.0043920463947251,1.0088077499823596,0.99020149944350122,0.98762993866403315,1.0424197787655758,1.0332312407541695,1.0101454551634343,null,6.7538447268945081,0,1.077329342156608E-2,0.19795977557526065,0.12120601688213632,8.2607372631310655E-2,0,1.077329342156608E-2,0.2745687024184213,5.9120122982858341,0,1.9131254559386912E-2,0.10470156851602253,-2.7047667091377723E-3,4.4362504735264228E-2]
[null,1222,0.98752953526625875,0.99724837330317895,0.99149505553378692,0.99142663216657334,1.0165839146304325,1.0140861130787715,1.0405748726717527,null,6.7696020686001326,0,1.0795237760680599E-2,0.19874376546197989,0.12382079350167112,8.2842713862208983E-2,0,1.0795237760680599E-2,0.28590476690220301,5.9121454853306847,0,1.9223936460137283E-2,0.10504846300156827,-2.5807235381137498E-3,4.4452867617791068E-2]
[null,1223,1.0326210175725217,0.98241328076691969,0.97312029307438497,0.97083438041400116,1.0015790328499581,0.99035778799236329,1.0277353649159178,null,6.7248235180761755,0,1.0311106239115615E-2,0.18472630342671548,0.11945887921366734,8.144218389527294E-2,0,1.0311106239115615E-2,0.26793408494158039,5.9120465064334393,0,1.8982874047125876E-2,9.8540977142673403E-2,-7.6759120848922196E-4,4.2459300184184944E-2]
[null,1224,0.99332285748561022,0.9986457043130097,0.96270878039683883,0.98388148843144574,1.0052068796631957,1.0294817288808482,1.0047072496679261,null,6.7581193652814164,0,1.1165259456713733E-2,0.19695979300446595,0.12356697885598096,8.0907747631133578E-2,0,1.1165259456713733E-2,0.27584314153434764,5.9133181511119108,0,1.9191739623609743E-2,0.10561873515413454,-3.2634727348217966E-3,4.5976551100648827E-2]
[null,1225,1.0053724857880428,1.013171025180875,1.0169686003332239,1.0103703316773602,0.99993280873338974,0.97111292331588883,1.0045339688630515,null,6.729997018737329,0,9.8636012564419888E-3,0.18857379323620355,0.12038180005189106,8.4182633957203434E-2,0,9.8636012564419888E-3,0.26695733582388503,5.9117316145747756,0,1.9125961380970277E-2,9.842212120595327E-2,5.2041879862221551E-6,4.061655431845252E-2]
[null,1226,0.95940072230731899,1.006196526179298,0.964492723110151,1.0136846492191158,1.000149213856421,1.0271702432993413,1.0191551302390052,null,6.7873327103868171,0,1.1479100332820225E-2,0.20303340676767384,0.1275169813723242,8.12193109669333E-2,0,1.1479100332820225E-2,0.28938662438586182,5.9148331174352533,0,1.9385791904214602E-2,0.1087778189337788,-4.0892333460822152E-3,4.7268891966861862E-2]
[null,1227,1.0029802326807322,1.0229144388135705,0.99481623545282094,1.0342358705136778,0.98735531411708222,0.98248727916928591,0.98949955671719136,null,6.729640985159965,0,1.0156822295635715E-2,0.18791311183565984,0.12061915795922558,8.2793978910343194E-2,0,1.0156822295635715E-2,0.26452036227721532,5.9142738427123858,0,1.9138894813414124E-2,9.915963903578498E-2,-6.0198875051733396E-4,4.1823986366452931E-2]
[null,1228,1.014672114695985,1.0069184331973946,0.99659659740003681,1.0061486560020141,1.0357501587853113,0.99459733986817778,1.0146271734046555,null,6.7346310945786589,0,1.0216448151575182E-2,0.18951562133891187,0.11995061922766311,8.2948555387460918E-2,0,1.0216448151575182E-2,0.2693938736039343,5.9126561698826068,0,1.9076263377855392E-2,9.991672581099946E-2,-8.9624907898040956E-4,4.2069515028204947E-2]
[null,1229,1.029646006152442,1.0238987351804576,1.0256456379447123,1.0269671616413123,1.0404173857453092,0.98121615046060318,1.0207810957536358,null,6.7215300020104358,0,9.614177188019532E-3,0.18617954037345,0.11689165155793332,8.4713193140365434E-2,0,9.614177188019532E-3,0.26574202406033498,5.9121302709013959,0,1.8998128118658388E-2,9.675825861505484E-2,5.2746484272088402E-4,3.9589470400518037E-2]
[null,1230,1.0180377180526567,1.0247787834882229,1.0139667085540693,1.0409397803568967,1.019334923060393,1.0012391916910055,1.0068468592876081,null,6.7329699611659333,0,1.0020513639120649E-2,0.1907245544065311,0.11839878579521478,8.4017756390896883E-2,0,1.0020513639120649E-2,0.26692363186204587,5.9135546016076983,0,1.9058501070566104E-2,9.9692245558320111E-2,-6.6280710630721234E-4,4.1262691580960298E-2]
[null,1231,1.0419092823546348,0.99623086542149297,0.99897358929294833,1.0300659643889654,1.0183957337161365,0.97986524123902918,1.010009920307199,null,6.7129195580205563,0,9.8264820089951129E-3,0.18292486679378964,0.11727182138046,8.2984666242969407E-2,0,9.8264820089951129E-3,0.25991403383159156,5.9138154410915797,0,1.8935809946820509E-2,9.6328052802919298E-2,2.8116206598033535E-4,4.0463703864446039E-2]
[null,1232,0.96752342321343465,1.0053557677759273,0.99535733533608317,1.0047792061305885,1.0061835213980339,0.99682402026787142,0.99758357674346787,null,6.7650098422942779,0,1.0757074210941867E-2,0.19917813666807907,0.12589805129639361,8.2989045056347938E-2,0,1.0757074210941867E-2,0.27800517045714679,5.9126515307928882,0,1.9338086786262233E-2,0.10507576873795936,-2.4216644136320336E-3,4.4295716912825606E-2]
[null,1233,0.98598832019146221,0.98531972187502714,1.0015626996492055,1.030462997742992,1.0150709306744283,0.99753707455297336,1.0198167912252309,null,6.7636624333027653,0,1.0597071738148372E-2,0.19802788859907233,0.12442056474252851,8.3407713260767749E-2,0,1.0597071738148372E-2,0.27916814805676959,5.9136912857888042,0,1.9232565598354415E-2,0.10414730087059847,-2.069888823371831E-3,4.3636855209240467E-2]
[null,1234,0.99042155592296754,1.0180622740240444,0.97530720852184027,1.0100944145169015,0.99486933891452578,0.98818380982292786,0.99283044930012543,null,6.7394535302204872,0,1.0544209976776773E-2,0.18951660872703771,0.12274498504196137,8.1627459327262411E-2,0,1.0544209976776773E-2,0.26931881807065439,5.9140493638656508,0,1.9207816749030254E-2,0.10098542975316191,-1.4161311992346008E-3,4.3419179884954993E-2]
[null,1235,0.97504485415484055,0.96709423365279379,0.99972840710634203,1.0048194020662369,1.0158043827035097,1.0381157216413748,1.0315106746113547,null,6.7941318818602401,0,1.1259571498975978E-2,0.20983707301016263,0.12679587653256535,8.3419000812228944E-2,0,1.1259571498975978E-2,0.28984882127104306,5.912408630647044,0,1.9294621711511164E-2,0.11045856767922201,-4.2956211073053073E-3,4.6364911303767013E-2]
[null,1236,0.98980163152824441,1.0453223377450394,0.96021804334753247,0.99776356767549768,0.98631473344039011,1.0028782571980441,0.99463115075361086,null,6.7391615202495094,0,1.0727318123155633E-2,0.18853535090896706,0.12180671513977527,8.0700201619192002E-2,0,1.0727318123155633E-2,0.27108466017226068,5.9142034013532943,0,1.9211264187458707E-2,0.10122829505821296,-1.7815548293562519E-3,4.4173186639708061E-2]
[null,1237,0.97130169533252242,0.96431106342780781,0.99196490311195562,0.96953510076884919,0.97552584507265028,1.0010495726524906,0.99034428791811369,null,6.7678497503141717,0,1.0987097055992117E-2,0.202416889898478,0.12758300579783816,8.2722378078167597E-2,0,1.0987097055992117E-2,0.27575837977920392,5.9109360720718804,0,1.9316168649125106E-2,0.10696489128125448,-3.0909452879784396E-3,4.5242910046202379E-2]
[null,1238,0.99296869871730409,1.0087645685231605,0.98661210698940172,0.97127238203469801,0.98631411818198544,1.0222622396637757,1.0133904426779403,null,6.7574678398560657,0,1.0815559223541918E-2,0.19768150863780098,0.12266962245675352,8.2412791339432467E-2,0,1.0815559223541918E-2,0.27756246270224905,5.9113274688942381,0,1.9193697106847894E-2,0.10474182520790909,-2.6580842739377304E-3,4.4536547784768447E-2]
[null,1239,1.0068287064247068,1.0131775911535883,1.0114384094743776,0.98222469075891206,1.0164572844558606,1.0127392266957169,1.0081890906824906,null,6.744313186658407,0,1.0321312048956095E-2,0.19571601181318679,0.12031046003566638,8.3880141558389895E-2,0,1.0321312048956095E-2,0.27143923828141614,5.9105260078889792,0,1.9118118590054405E-2,0.10242916247712645,-1.6072798789515648E-3,4.2501325892541623E-2]
[null,1240,1.0190734464903124,0.99919194259917699,0.97281194740484223,1.0186523304803969,0.98372926885272627,0.9651045675704063,1.0065697246150436,null,6.7180204125389373,0,1.0110866514766481E-2,0.18105606085215023,0.12023536988019866,8.1398106812949123E-2,0,1.0110866514766481E-2,0.26338741862924836,5.9146486874653332,0,1.9053058518563377E-2,9.6598067198061785E-2,8.8945417759033502E-6,4.1634748640657485E-2]
[null,1241,0.97936074324745814,0.98335678472369958,0.99053368421422328,0.96101174271403444,1.0279340221287794,0.98026187764204209,0.96397861148851116,null,6.7415232465149231,0,1.0594528279903533E-2,0.19477085419756673,0.12557455511072774,8.2470935276005755E-2,0,1.0594528279903533E-2,0.2640558555369944,5.9105550766915078,0,1.9269982373777542E-2,0.10299787721958042,-1.7982715921467541E-3,4.3626381700906915E-2]
[null,1242,0.96395616696536435,1.0096097486395721,0.97424293822285701,0.95811881610739846,1.0071734242199628,0.97700934314785792,1.0152155251142245,null,6.7592951514392263,0,1.075946123276433E-2,0.19308019246794508,0.12655658304625084,8.1691851780213209E-2,0,1.075946123276433E-2,0.28192584543411209,5.911297632106125,0,1.9358938491369351E-2,0.10293927164979196,-1.8607097803996202E-3,4.4305546243816461E-2]
[null,1243,0.98983998317824973,1.0049450352612497,1.0225219213010595,0.99043812835177203,1.0344103243606066,0.99721753999437379,0.980283735761866,null,6.7456061796903048,0,1.0273590578137396E-2,0.1980322256234055,0.12256427378160625,8.4514804401687696E-2,0,1.0273590578137396E-2,0.26711183892599749,5.9103366148312659,0,1.9211050786219784E-2,0.1030763670350904,-1.545813064787123E-3,4.230481736981536E-2]
[null,1244,0.99275181043632432,1.0181400904320754,1.0183293812907936,1.0035847740150723,0.95716127154688213,0.99928722543869497,1.0232033562741922,null,6.7540640308119286,0,1.0245086418056593E-2,0.19626182740929171,0.12164812761598578,8.4413516515301226E-2,0,1.0245086418056593E-2,0.27805213662957984,5.911287197752821,0,1.9194896567156821E-2,0.10236602270540328,-1.347136695764084E-3,4.2187442312153975E-2]
[null,1245,1.0447525342649822,0.99398013210985792,0.98076392504321863,0.99952863737159647,1.004585911815687,1.0119514876146751,1.0038124636646331,null,6.7187910111631082,0,1.0292704424063531E-2,0.18650019942607204,0.11738432840545007,8.1839942636969878E-2,0,1.0292704424063531E-2,0.26051991039724004,5.9131781751998114,0,1.8921570338613594E-2,9.9106741043749877E-2,-1.0433810700016049E-3,4.2383524785201451E-2]
[null,1246,0.97354822289522835,1.0113892782389391,1.0192780151900367,1.0256137499535101,0.99189324513806343,1.0259970848646776,1.0320579957083447,null,6.7843233648697234,0,1.0748078065151748E-2,0.20618664202061471,0.12435987727463252,8.4634904638202668E-2,0,1.0748078065151748E-2,0.28871643125451762,5.9124230398823103,0,1.9303216966991721E-2,0.10749232986962974,-3.051749422894733E-3,4.4258672385716145E-2]
[null,1247,1.033465451109937,1.0013386266034816,0.96259930165079333,0.98702486901319708,1.0089729064426627,1.0148552003344955,1.0262482273162001,null,6.7297128941205075,0,1.0567911285036365E-2,0.18639200690308022,0.11864138587995776,8.0816658249969378E-2,0,1.0567911285036365E-2,0.2694148433228335,5.9134940503796827,0,1.8978560300909147E-2,9.995732925521332E-2,-1.4987178248301203E-3,4.3516777653692398E-2]
[null,1248,0.99509220680705723,0.97204384247396947,1.0300234563405357,0.99092361670628171,0.99292088211103557,0.99605811379897824,0.99736317052782986,null,6.7532370779500912,0,1.0286303460371493E-2,0.20048877113241129,0.12340688299230559,8.5025743883767296E-2,0,1.0286303460371493E-2,0.27057413891553772,5.909930465449559,0,1.9181981060600622E-2,0.10397108725926431,-1.6991594994083055E-3,4.2357166756046678E-2]
[null,1249,0.99230192274326079,1.0344733433282465,0.98382779352101801,1.0101560117689443,0.9967314472873261,0.97272215526445494,0.99388759817181915,null,6.7301119570308758,0,1.0212787215161933E-2,0.18589510834256079,0.12157407306021331,8.2134392219302702E-2,0,1.0212787215161933E-2,0.2675288869028678,5.9135834965030565,0,1.9197386259211413E-2,9.8633904753621243E-2,-4.8973095363426993E-4,4.2054439943677559E-2]
[null,1250,0.99747114240625945,1.0120407328945416,0.99483043869112142,1.0326031977765779,1.0022575352106426,0.98369154003732373,1.0288488021038831,null,6.7466348552061302,0,1.0272192721531785E-2,0.19005160040482783,0.12180466184197337,8.2957596149491095E-2,0,1.0272192721531785E-2,0.27677257740861372,5.9141848069213827,0,1.9168914988174128E-2,0.1002873865322035,-8.9175028566192572E-4,4.2299061245122657E-2]
[null,1251,0.99383922064475005,0.97374468604372799,1.0069128760075536,1.034154903721882,0.97976808139974181,1.0008497021623028,0.99595269152641164,null,6.7556254129881994,0,1.0552381906296907E-2,0.19876147107500225,0.12392037825169658,8.3631413784756303E-2,0,1.0552381906296907E-2,0.27093151333487236,5.9135887115133876,0,1.9188888114723471E-2,0.10425620348389632,-2.1059970063060664E-3,4.3452830436169682E-2]
[null,1252,1.0356495252399456,1.0362109630433645,0.98107036098245959,0.98085778875006446,1.0099535720529551,1.0329246456153987,1.0061481302388586,null,6.7246579667021829,0,1.0408483796472046E-2,0.18868384139698935,0.11645612798915805,8.1904201953803574E-2,0,1.0408483796472046E-2,0.26490525509108853,5.9121519544371992,0,1.8967435694804004E-2,0.10025175706021028,-1.5228905538920677E-3,4.2860283632819643E-2]
[null,1253,1.0127435471170363,0.98727884455232784,0.97483002296397103,0.9969930412998258,1.0190911248660564,0.97712526759923779,0.96166399155354598,null,6.7161048203257012,0,1.0335667694099729E-2,0.18563684527010149,0.12153167892507011,8.1390691151246461E-2,0,1.0335667694099729E-2,0.25439475634482062,5.9133672034484039,0,1.908649479266895E-2,9.8941752167416727E-2,-8.0504165805981795E-4,4.2560439884033512E-2]
[null,1254,1.003528138196095,1.0173412323246536,1.0047439823994226,0.98899470171861514,0.990086341718731,1.0255584995807097,0.97685339517117864,null,6.7420255868319749,0,1.0529392611552042E-2,0.19769248436662928,0.12063294143467108,8.3383365405745966E-2,0,1.0529392611552042E-2,0.26498365376954197,5.9112709705356092,0,1.913592718319302E-2,0.10380697810872379,-2.2388985844917493E-3,4.3358164612352257E-2]
[null,1255,0.98501027617764736,1.0117846832053035,0.95899861836151445,0.9831932899117185,1.0306053553715364,1.0059383259442969,1.0012435023294413,null,6.7509592338681115,0,1.0975941214312517E-2,0.1925557422632859,0.12402885699218667,8.0662547504817717E-2,0,1.0975941214312517E-2,0.27481455889251144,5.9134812305563464,0,1.9238055592844132E-2,0.10345059530499856,-2.4693255147082861E-3,4.5196972275831589E-2]
[null,1256,1.0017927008316165,1.0148492168611321,0.98219183746362093,1.016765043475617,1.0237298607136145,1.0091349451138074,0.98134883935165351,null,6.7380357080575042,0,1.0596186221009716E-2,0.19240633243544045,0.12137857036618618,8.2005094606334067E-2,0,1.0596186221009716E-2,0.26514460372785709,5.9140311698437511,0,1.9145338005372384E-2,0.10217224502494772,-1.8808547596671781E-3,4.3633208807279673E-2]
[null,1257,0.9794706447048489,1.0129436593790373,0.95873201923724616,0.98161011583709723,1.0131447267020786,1.0149109631687692,1.0126993958868085,null,6.7615098706727359,0,1.1133597763132504E-2,0.195244215135537,0.12467819868019213,8.0717510093168951E-2,0,1.1133597763132504E-2,0.28038822533937718,5.9134099776360367,0,1.926935778327463E-2,0.10490910246944411,-2.9528903463503925E-3,4.5846173882052706E-2]
[null,1258,1.0301300957316109,0.96770029841975524,0.99750029585927802,0.97402229999266898,0.96828800629985201,1.0368679594803933,1.0114924955453315,null,6.7455075111636562,0,1.0662537415962433E-2,0.19805563923973643,0.12002655464380742,8.2973771828254009E-2,0,1.0662537415962433E-2,0.2688966072052178,5.910869262715245,0,1.8995639996149675E-2,0.10437229746094767,-2.5886931437280642E-3,4.3906431218022512E-2]
[null,1259,0.97478705313608627,0.98462733543049508,0.96863521057030577,0.99630874195496977,0.99918646830582492,0.9672795742326239,0.98947711846524411,null,6.7464459676159123,0,1.0699746228739735E-2,0.1904166929505457,0.12651797521019911,8.1224945878596133E-2,0,1.0699746228739735E-2,0.2710114613590936,5.9136685243059697,0,1.9296100398744281E-2,0.10180569984532703,-1.555082818687903E-3,4.4059650486117659E-2]
[null,1260,0.96914047887394916,0.99227886541962596,1.0014061495057862,1.016040730719465,1.0071001453882995,1.0133689547682605,0.96990326182380104,null,6.7664370949819137,0,1.0920917528115781E-2,0.20403228667173168,0.12623071198942487,8.3286608017224123E-2,0,1.0920917528115781E-2,0.27154661913746037,5.9129207000783248,0,1.9328685164205866E-2,0.10731348630401469,-3.1923969104011552E-3,4.4970394529924476E-2]
[null,1261,1.0038810385798784,0.98260024216205366,1.0395917519539142,0.97610319004611434,1.004767553452143,0.96696256911245881,1.0108758289109565,null,6.7368957906885045,0,9.7703634886790718E-3,0.193144277280273,0.12161627767671887,8.5582534535141086E-2,0,9.7703634886790718E-3,0.26895844603004948,5.9085740795961152,0,1.913401747783736E-2,9.9694169769693183E-2,-4.0629463831536676E-5,4.0232617786508836E-2]
[null,1262,0.98472076743959447,0.99864483990206243,0.98978265016479305,1.0282089715912621,0.97026442285105596,1.0319991965576447,1.0060285323187119,null,6.7708182935504642,0,1.1027127830053478E-2,0.20249820887994674,0.1241369455220744,8.2669572231303487E-2,0,1.1027127830053478E-2,0.27890915916059655,5.9142289546998876,0,1.9239682766329369E-2,0.1071243330548949,-3.3963124131482819E-3,4.5407749648574906E-2]
[null,1263,1.0024212631567988,0.95644015708306385,0.97009055026632629,1.0116653984550876,1.0004540481482391,0.96451232755665162,1.02404242484271,null,6.7414266089251011,0,1.0491738343695519E-2,0.18711882695432006,0.12444061945865838,8.1347472478174934E-2,0,1.0491738343695519E-2,0.27275875779006736,5.9144195482004909,0,1.9141925712850533E-2,9.9969313687645348E-2,-9.7296639663913085E-4,4.3203111039528917E-2]
[null,1264,1.010350738246351,1.0337303172459857,0.98430769104945215,1.0047859856691075,1.0077627262082369,1.0029922283944119,0.99674384277556949,null,6.729967803211621,0,1.034133134590132E-2,0.18836892639291114,0.11942789150545066,8.2142667981092168E-2,0,1.034133134590132E-2,0.26628640148894017,5.9132666661020785,0,1.9099243389977871E-2,9.9922512160161778E-2,-1.1302676030515656E-3,4.2583761794060017E-2]
[null,1265,0.98498678347593094,1.0258019534942036,0.96137556799815216,1.0121106156021209,1.0009710320376821,0.98050500304139687,0.9554109406807797,null,6.7274065273997365,0,1.0613904854512265E-2,0.18686318343404304,0.12330718902641441,8.0636388363020201E-2,0,1.0613904854512265E-2,0.25981512499249421,5.9149167307441397,0,1.9238187597072E-2,0.10027188459096291,-1.3483323346592229E-3,4.3706170986243964E-2]
[null,1266,0.95944625585241661,1.0023654218583362,1.0306015417206214,0.97337017396321535,0.95974460058471978,1.0245955481353739,0.98358629118931251,null,6.7807743803442024,0,1.0825129601887973E-2,0.21117131892090077,0.12641734217194905,8.5169314205507995E-2,0,1.0825129601887973E-2,0.27918561509152989,5.9089488410303526,0,1.9385522231621093E-2,0.10947988020988875,-3.5594104168833233E-3,4.4575956899333635E-2]
[null,1267,1.0003101655152595,1.0037900263810786,1.0020738899599169,1.0002388085299683,1.0097041936347269,0.97861623419974375,1.0170184263760738,null,6.739762588174389,0,1.0161479994586501E-2,0.1900318097228752,0.12172192933155845,8.3325950994494358E-2,0,1.0161479994586501E-2,0.27241661929266037,5.9120291495494017,0,1.9153403268549748E-2,9.9916633289518053E-2,-6.7607321636710621E-4,4.184316594169276E-2]
[null,1268,1.003519622006994,0.96489676227495413,0.98289743940131102,1.0123290482549561,0.98905643733608173,1.0109471154973761,1.0048678739102697,null,6.7535526831519235,0,1.0821969814966075E-2,0.19671191621186243,0.12362768595144955,8.2132998579452721E-2,0,1.0821969814966075E-2,0.27174565087324642,5.9137523946829944,0,1.9135973284784127E-2,0.10442174977165466,-2.5386316627386829E-3,4.4562945459210364E-2]
[null,1269,1.0128414647444532,0.99599527520760267,0.99732014245542455,1.0120261044008212,0.98655952017257686,0.98702245905105745,0.97088971305380167,null,6.7235387538699527,0,1.0198078420333653E-2,0.18937779643159233,0.12067946459492288,8.2841039139941258E-2,0,1.0198078420333653E-2,0.25766458021248428,5.9129332721971704,0,1.9085974382270787E-2,9.9808145732012618E-2,-8.4539056508356914E-4,4.19938717446426E-2]
[null,1270,0.97681132978497109,0.99506118334127991,0.99088920363007948,0.9707130126758402,0.98553263429073212,0.98606255433172729,0.97027922878144413,null,6.7457618684516234,0,1.0627701779882707E-2,0.1954837232239898,0.12530101916872097,8.253812966933341E-2,0,1.0627701779882707E-2,0.26690862467617565,5.9110596509217075,0,1.9284510611444195E-2,0.10335653356588498,-1.9333076547981476E-3,4.376298426915827E-2]
[null,1271,1.0166434297690485,1.0206731865346397,1.0024742964881119,0.9815581998284898,0.98434570814885147,1.0302787944765273,0.98518567144225844,null,6.7357250270818154,0,1.0447494643684168E-2,0.1954965388235454,0.11896263177129937,8.3225633050360445E-2,0,1.0447494643684168E-2,0.26418654418099796,5.9109970856102967,0,1.9065845297566001E-2,0.10276950836139204,-1.9996833716079535E-3,4.3020923357967214E-2]
[null,1272,1.018640358556623,1.0143651753217684,1.0051609293040389,0.98398094510056333,1.03395836121089,1.0109856229871543,0.97130207214752196,null,6.7247022422622065,0,1.0234883381505515E-2,0.19228167781869104,0.11897497297391757,8.3314552698315905E-2,0,1.0234883381505515E-2,0.25829730584132005,5.9109764930814555,0,1.9055332965245465E-2,0.10094493784895442,-1.2884589893999987E-3,4.2145428023709443E-2]
[null,1273,0.98039147106452307,1.040357483623306,1.0010777874975243,0.9983961872025241,1.0144828228341169,0.99330010245081712,0.97763960645807668,null,6.74203047781217,0,1.0372600716186398E-2,0.19369400604917092,0.12244882267439328,8.3208225356718485E-2,0,1.0372600716186398E-2,0.26823848551481921,5.9119856386906831,0,1.9264130057056218E-2,0.10189253695281873,-1.413890978644665E-3,4.2712523495153538E-2]
[null,1274,0.96961431725041125,1.0205565705203374,0.99565488154467219,1.0207744318753664,0.97819403227815283,0.98148368863807944,1.0318249499298888,null,6.7648404945821339,0,1.0498283031158769E-2,0.19447209028851076,0.12486903470979176,8.3115671272634833E-2,0,1.0498283031158769E-2,0.2852501866579365,5.9134993665092468,0,1.9325936190919813E-2,0.10257792242262592,-1.4997743671234234E-3,4.3230060897591661E-2]
[null,1275,1.0042628867230461,1.0069567429129898,0.99681640423708062,0.98565736178765107,1.0179486520913898,0.98422134639575731,0.99910706376251002,null,6.7324688816153841,0,1.0212528869688009E-2,0.18950463371536572,0.12118798450173111,8.2916878099762323E-2,0,1.0212528869688009E-2,0.26705252897542198,5.911536395497297,0,1.913195263472461E-2,9.9900012181068754E-2,-8.1488011298835145E-4,4.2053376122999718E-2]
[null,1276,1.0006862500401008,0.99063493327884988,1.0130517167679427,1.0193122213600971,1.0071316459395065,1.0380755230104057,0.97578783136955105,null,6.7563218288114708,0,1.0732383817319524E-2,0.20399743401284068,0.12211284639489038,8.3946218764780811E-2,0,1.0732383817319524E-2,0.26689940804514967,5.9124381688615451,0,1.9151355037762816E-2,0.10667821458369924,-3.0958631558088028E-3,4.4194046266615009E-2]
[null,1277,0.9911237981402875,0.98705036705855154,0.96321017012181798,0.98035685349226154,1.0177368916282721,1.0092805863361758,0.99528617372472361,null,6.751196831337043,0,1.1020676189781142E-2,0.19455414278404159,0.12441167838742097,8.0887686868446884E-2,0,1.1020676189781142E-2,0.27207484317993896,5.913100431036094,0,1.9203916745612493E-2,0.10430234526148592,-2.7193958682821366E-3,4.5381182942282577E-2]
[null,1278,1.0164057582462276,1.0265510138254326,1.0065989487261369,0.99450576299067783,1.0179525240264335,1.0120320604857194,1.0413141201804978,null,6.7440894825897404,0,1.0202823983313965E-2,0.19208799199294962,0.11864203674574134,8.3670005358415872E-2,0,1.0202823983313965E-2,0.27750558560965755,5.9114639583885236,0,1.9067099210594154E-2,0.10077143500906768,-1.1320428535296916E-3,4.2013413128316787E-2]
[null,1279,0.99848560219942561,1.0108564734884302,0.99770320627625886,1.0181974640168221,0.9850293299425118,1.0111298277067451,1.0190525651323923,null,6.753801058383198,0,1.0526838027489717E-2,0.19559383442349643,0.12168432385822804,8.3122218552875674E-2,0,1.0526838027489717E-2,0.27650212595437401,5.9132453222643715,0,1.9163362102487667E-2,0.10306456716915591,-1.9223412316785385E-3,4.3347645289882615E-2]
[null,1280,0.99915188264212906,1.0173646815835817,1.0204994462137795,1.0121314074538317,0.96787005426925843,0.96366054081776442,1.0053471448486841,null,6.7312424073091695,0,9.8011074744364969E-3,0.18836038818714906,0.12086495709183766,8.4418486659686418E-2,0,9.8011074744364969E-3,0.26810601867319289,5.9116246430256796,0,1.9159721193787005E-2,9.8139810269620653E-2,2.0916616058219649E-4,4.0359216047632457E-2]
[null,1281,1.000155580680117,1.023807479836202,0.99254251561462814,1.0142063860642319,0.96809084031161463,0.99655820174833321,1.0339926656245106,null,6.7478399728887721,0,1.0348043130405006E-2,0.19080680776458889,0.12095967034157369,8.2825342174046343E-2,0,1.0348043130405006E-2,0.27854086456528859,5.9133183164034557,0,1.9154245614870492E-2,0.10080066439657069,-1.1773380996110028E-3,4.2611399727993084E-2]
[null,1282,0.95878841518028057,1.0151494952769333,0.96920274959037078,1.0159658648790773,1.0040775328850722,0.97365264218943004,0.98617455792778896,null,6.7552794478933214,0,1.0802373383214627E-2,0.19240516323329829,0.12705707229500451,8.1327081637860565E-2,0,1.0802373383214627E-2,0.27495584158415393,5.9147004632447171,0,1.9389420783624021E-2,0.10283946833794018,-1.8773140645736922E-3,4.4482250841292731E-2]
[null,1283,1.0148869722117075,0.98389572005789339,0.97444102579736436,1.0023085488729815,0.98597788576312184,0.99105162335935904,0.99575236385053223,null,6.7301575559786082,0,1.0479786012893622E-2,0.18811667977269811,0.12144877572251996,8.1498741255805932E-2,0,1.0479786012893622E-2,0.26418408597149368,5.9136758926432886,0,1.9075125925568908E-2,0.10028304164889754,-1.2786804303870647E-3,4.3153893468722275E-2]
[null,1284,1.0252696425043166,0.96680631736760181,0.97749587956822825,1.0007202579966787,0.99294145868968542,1.0170794486406936,0.98364947875035702,null,6.7334363902172543,0,1.0697864651860211E-2,0.19290388961443616,0.12100850060828512,8.1643808079353106E-2,0,1.0697864651860211E-2,0.26089656751335527,5.9134224459508893,0,1.9020728377088267E-2,0.10267761844890687,-2.1890708624981319E-3,4.4051902487435964E-2]
[null,1285,0.99903584632389952,0.9989324072324447,0.96385446133648411,0.99621361804129283,1.0355133188569001,1.0208842771569013,0.96795687002371034,null,6.7411184129429671,0,1.099638041101153E-2,0.19431112028931741,0.1228251445440635,8.0826090467955469E-2,0,1.099638041101153E-2,0.26344696617253099,5.9139229871009933,0,1.9160354928357878E-2,0.1041382307897433,-2.7936185997919707E-3,4.5281137249796738E-2]
[null,1286,1.0273327169062991,0.97803812100301069,1.0150324624848606,0.99561664277284323,1.0012948700939899,0.96351171049214412,0.98082124406523685,null,6.7113236191504297,0,9.7395837055805189E-3,0.18567010774063561,0.11951928577953834,8.3884229928524484E-2,0,9.7395837055805189E-3,0.25469206815457462,5.9110450135516883,0,1.9010050332893595E-2,9.6999221579026199E-2,3.9776996524289057E-4,4.0105872118306157E-2]
[null,1287,0.9655057029060673,0.98029379652135884,1.0001689755582457,0.95753759853076026,1.0317523521957206,1.0117251935231888,0.96379189440838609,null,6.7658860152743943,0,1.1013288371165362E-2,0.20538126763413009,0.1273475229113919,8.3158093503875902E-2,0,1.1013288371165362E-2,0.27082582350594031,5.9098286415401446,0,1.9349862050859638E-2,0.10808937150448446,-3.4453285966362271E-3,4.5350761220205489E-2]
[null,1288,0.98870893283666028,1.0201818888483358,0.96810909086984198,1.0040501051477271,1.0047993357123228,1.0043002756722283,1.0047379167904942,null,6.7489784996198834,0,1.0792629742643767E-2,0.19191968367365148,0.12298881627189082,8.1242415818578301E-2,0,1.0792629742643767E-2,0.27451984225753723,5.9141157334374936,0,1.9217351279108768E-2,0.10263643233241636,-2.1039037145196846E-3,4.4442128263725296E-2]
[null,1289,0.97508393459823506,0.97319255672161009,1.029012164801256,1.0357511470256138,0.97842944619466532,1.0333217656159825,1.0281865731134749,null,6.7943623465742995,0,1.0894229520027011E-2,0.21202056991970575,0.12589957426594039,8.5241862539465987E-2,0,1.0894229520027011E-2,0.28839287217277598,5.9124104245323075,0,1.9294397623342355E-2,0.1100059146391615,-3.7637671813073531E-3,4.4860498062903278E-2]
[null,1290,0.98011314158115914,0.95715922814576171,1.0283750458972623,1.0437929268820465,0.99249522714871163,1.0000245635735023,0.99326863457375536,null,6.770564784051464,0,1.0569980119714661E-2,0.2055164525465786,0.12610118397183129,8.5012767929275715E-2,0,1.0569980119714661E-2,0.27413408367384068,5.9128816603257119,0,1.9265709156634895E-2,0.10666463458652099,-2.5370048855926286E-3,4.3525296746658781E-2]
[null,1291,0.99082632935148907,0.9895178769717079,1.0015494373407674,1.031594016356522,1.0157788916930599,1.0025133882028117,0.9735601394397293,null,6.7484997385748269,0,1.0578766267156859E-2,0.19768192993784162,0.1236029104673957,8.322567790930871E-2,0,1.0578766267156859E-2,0.26562456651426214,5.9137531543984965,0,1.920556810653486E-2,0.10396603779985228,-2.1215830968114276E-3,4.3561476537949811E-2]
[null,1292,0.96646674638501839,0.97302220388642224,0.98889418456223044,0.98786533026190393,0.98797087265923567,0.97934547409808548,1.0485498564474054,null,6.7779293550963837,0,1.0789949967020403E-2,0.1978819211400219,0.12782077325547822,8.2748217047924191E-2,0,1.0789949967020403E-2,0.29106824972335726,5.9120977169669633,0,1.9344247341010586E-2,0.1047286556252173,-2.1915194282795827E-3,4.4431093424690565E-2]
[null,1293,0.96077675709280719,1.0082827923249367,0.98349209266842452,1.0288933349133822,0.9737792859026595,1.0196106265998277,0.96853589796594097,null,6.7707816065352313,0,1.1181618368027377E-2,0.20342863856225382,0.12686425115699992,8.2213746718907979E-2,0,1.1181618368027377E-2,0.2739140941395532,5.914614940029467,0,1.9377653618654452E-2,0.10795512089188757,-3.6307527681578413E-3,4.6043914185660756E-2]
[null,1294,0.96051066322030598,0.99973835990780457,0.96984889063061785,1.0009911600685126,1.0207607117512181,1.0296285963917453,1.0034568685198615,null,6.7840518570261947,0,1.1471409810966324E-2,0.20451774704024356,0.12759528478066226,8.148723489059552E-2,0,1.1471409810966324E-2,0.28492578354804371,5.9138555841648603,0,1.9379225559634922E-2,0.10927806352836975,-4.2242902529427981E-3,4.7237223766729355E-2]
[null,1295,0.95788912599261022,0.99856206851861917,0.99067642143966128,0.99387602166181555,1.009964430381044,0.97949358731675618,0.97371018891522476,null,6.7587258990706687,0,1.0751255895094219E-2,0.19769397971497896,0.1276009914499093,8.2617117058016082E-2,0,1.0751255895094219E-2,0.27247939613561589,5.9123234708818657,0,1.9394758892061922E-2,0.10453623261385768,-2.191805799426798E-3,4.4271758123786586E-2]
[null,1296,1.0231624497957306,0.98011841158234314,0.9987729103057561,0.98718119158292328,0.98600176539184792,1.0186088048302675,0.97756338574231771,null,6.7323793943352408,0,1.0476954215357227E-2,0.19497575137455189,0.12020566776290058,8.2941548090630202E-2,0,1.0476954215357227E-2,0.25984100838788482,5.9115090583249863,0,1.9031679221392366E-2,0.10268427475399611,-1.9518262116106466E-3,4.3142232630508578E-2]
[null,1297,0.98105005885048002,1.0026049924094493,1.0247091318180839,0.99637863202636134,1.0146345844733498,0.95624710252613587,0.96510960190185058,null,6.7322450985186286,0,9.930656826834746E-3,0.19204207089043304,0.12373558073646411,8.4579342721378001E-2,0,9.930656826834746E-3,0.2615637800454973,5.9105317812693583,0,1.9260397134152608E-2,9.9850994459496356E-2,-2.1152596003817516E-4,4.089267722188332E-2]
[null,1298,1.0208997343774124,0.99919511374060155,1.0328254962775225,1.0028611488924253,1.0102397523137085,1.0324602562768117,1.028316460186198,null,6.7533885207402191,0,1.0245523957702186E-2,0.20052269747591941,0.1189167933989092,8.5267899631669378E-2,0,1.0245523957702186E-2,0.27509819784863787,5.9104129748466887,0,1.9043488633908312E-2,0.10384591499758121,-1.9086901156279859E-3,4.2189244022535391E-2]
[null,1299,0.99212375671694208,0.98825693531604886,0.97795452488486956,0.95809939955959145,1.0071853458716353,0.99891936391914049,0.99000554091963078,null,6.7447541385455763,0,1.07519135703235E-2,0.19401049782249358,0.12394979235948671,8.1756278115782288E-2,0,1.07519135703235E-2,0.26939131380671766,5.911093089321791,0,1.9198372859533668E-2,0.1032429022768243,-2.1625743303753907E-3,4.4274466313318953E-2]
[null,1300,0.96113497477442555,1.0253287605022663,1.0178334559155708,1.0111187763309131,0.96550092912299834,1.0048908472514892,1.0028524076437779,null,6.7732311718060751,0,1.061405409481919E-2,0.20318088969546913,0.12530631496024569,8.4443833820904785E-2,0,1.061405409481919E-2,0.28196191085366507,5.9117226080284562,0,1.9375538833804325E-2,0.10600077141467196,-2.4674813324070178E-3,4.3706785531264114E-2]
[null,1301,0.99510832802197102,1.047854160679327,0.99173913668904323,0.98337693285590544,1.0309328886911906,0.98998432376238099,1.0104423402271558,null,6.7362806667521795,0,1.0237001629105512E-2,0.18853466495855933,0.12046422891965487,8.2676420131612319E-2,0,1.0237001629105512E-2,0.27274856311184315,5.9116967994705938,0,1.9181892306153536E-2,9.9640196833741465E-2,-8.1624957027235322E-4,4.2154150590292212E-2]
[null,1302,1.0072129724963936,0.96955261805591819,0.97179749015643391,1.0254657657556623,0.99882105268732291,1.029052101013229,0.99169918777851296,null,6.7532424856534172,0,1.1059205832618246E-2,0.19774002694085124,0.12314418923283657,8.1411926491747305E-2,0,1.1059205832618246E-2,0.26883091214544541,5.9150725236612054,0,1.9116052823786912E-2,0.105553163251175,-3.1661500470970654E-3,4.5539841153465016E-2]
[null,1303,1.0387697732281986,1.0317917781275341,0.99315612360913563,1.0274389801314556,0.98116393488233733,1.0228545299810419,0.99565130008236191,null,6.7204191038118211,0,1.018688798070075E-2,0.18800619944652291,0.11609101109551161,8.263015948038592E-2,0,1.018688798070075E-2,0.26051923699958202,5.9139992712266887,0,1.8951623831954659E-2,9.9290789874452362E-2,-1.0169796493391741E-3,4.1947791506058298E-2]
[null,1304,0.99801600814378777,0.99252545806456494,1.0026330625431308,1.0059896854886798,0.98142077480068712,1.0241479360510404,0.99328530748850219,null,6.7555118159904515,0,1.0705122550208947E-2,0.20036445972349606,0.12254317571875778,8.3346803203135408E-2,0,1.0705122550208947E-2,0.27106090957082041,5.9123084311566512,0,1.9165931133325619E-2,0.10532020311118968,-2.6798868479052697E-3,4.4081789220978322E-2]
[null,1305,1.0013237185613102,1.0391067191927819,0.99294037605904528,0.99077039143655288,1.0192427772459927,0.97932843795704039,0.99663285832575188,null,6.7260543935301591,0,1.0089513225263512E-2,0.18614954127887898,0.12009653760523507,8.2671915693323231E-2,0,1.0089513225263512E-2,0.266440463848019,5.9120294269106326,0,1.9147886772158968E-2,9.8320806355172805E-2,-3.4900452849452633E-4,4.1546819595228102E-2]
[null,1306,0.98376291387092252,0.98137126236208005,1.0159332269774903,1.0353069809156223,1.0161511115879891,0.9879789736018898,1.0063226327945551,null,6.7600089639973158,0,1.0405815190558792E-2,0.19863537322702887,0.12462551177821997,8.4250656980878066E-2,0,1.0405815190558792E-2,0.27523602192845975,5.913138056049946,0,1.924507317409228E-2,0.10372651662965521,-1.6975405596277554E-3,4.2849294788663013E-2]
[null,1307,1.0203114224962413,0.97060408053364156,0.97868479937666197,1.0103016728791483,1.0064442770616007,0.96127974339472966,1.0019670284165236,null,6.7198116833500841,0,1.0132514571796326E-2,0.18303212261386811,0.12138414506273694,8.1736476098940539E-2,0,1.0132514571796326E-2,0.26177272034437443,5.9138750654059242,0,1.9046567691560747E-2,9.7365114605877309E-2,-1.2441995949287585E-4,4.1723891486295878E-2]
[null,1308,1.0131756551903992,0.96779393123229696,1.013021212705626,0.98854477254706807,0.97904303855254127,0.97609193853491338,0.99786513826085121,null,6.7317652325000861,0,1.0067586856051724E-2,0.1913525643466491,0.12173876615010348,8.388194475235887E-2,0,1.0067586856051724E-2,0.26401574705892938,5.91077749247372,0,1.9084198991931815E-2,0.10006722694842481,-6.0923893160060624E-4,4.1456530709562192E-2]
[null,1309,0.99245064926527105,0.97915511888197593,1.0179461669126715,0.98607925336019486,1.025924607661953,0.98153805472003119,0.96697397717371603,null,6.7381255112017051,0,1.0239360881748575E-2,0.19604096560980458,0.12360768726698448,8.4153371479750938E-2,0,1.0239360881748575E-2,0.26158726108535912,5.9103633420870834,0,1.9196562952397158E-2,0.10227014413174677,-1.2576889841698041E-3,4.2163865572745027E-2]
[null,1310,1.0027890944247997,0.99345792051048143,0.95990446097925874,0.98660545508900743,0.99918062106981642,1.0108609479824797,1.0283990563376508,null,6.7513449621719843,0,1.0910653914754776E-2,0.19166819655252446,0.12270732596409552,8.0760815463626359E-2,0,1.0910653914754776E-2,0.27793309313874764,5.9136169209455751,0,1.9139930841869601E-2,0.10292667270767333,-2.3361242390838336E-3,4.4928130796958919E-2]
[null,1311,0.97035388444615189,0.99704755563191239,1.0165220696393769,1.0256842170355056,0.96993568852350753,0.99441169383158101,1.0021581910689985,null,6.7679005089182871,0,1.0541004975663277E-2,0.20139139335827869,0.12553780916514218,8.4323431389181386E-2,0,1.0541004975663277E-2,0.27835219504925685,5.9125845136404855,0,1.9321650957216586E-2,0.10513515125487867,-2.1516181569973931E-3,4.3405982260838569E-2]
[null,1312,0.99625249128295279,1.0102775725986761,0.97735121216597465,0.99723435304035668,0.98577018258736049,0.96943103549806553,0.98659496426150806,null,6.7271474310799757,0,1.0299058784326812E-2,0.1856727577169503,0.12236397249763643,8.168038689793973E-2,0,1.0299058784326812E-2,0.26439133184930408,5.9132419382320505,0,1.917560051558298E-2,9.8835845538972636E-2,-6.2409307819304908E-4,4.2409690909731658E-2]
[null,1313,0.99376456340035302,0.95170776637966659,0.99126308617125758,0.99098739020901894,1.0209489940381853,0.98131486057089379,1.0149371611064595,null,6.7536604164316882,0,1.0593113448081785E-2,0.19495554005824853,0.12537052979953175,8.2674719923132134E-2,0,1.0593113448081785E-2,0.27442704265529894,5.9121346677205278,0,1.9189300210685625E-2,0.10305806373895052,-1.7700033499782246E-3,4.3620555675295637E-2]
[null,1314,0.9952262448362863,1.0318448831020266,0.98147683403109376,1.0373095343793346,1.0040452927950865,1.0108038780795807,1.0356606300686526,null,6.7562723331958363,0,1.0614689021352661E-2,0.19253797588718036,0.12138361013080398,8.2193848310817108E-2,0,1.0614689021352661E-2,0.28165657630050045,5.9151812435548363,0,1.9181243209159989E-2,0.10227873350913635,-1.8502977523187874E-3,4.3709400045716232E-2]
[null,1315,0.97980854519205829,1.0076272580490622,1.0110196655737531,0.97769836410465971,0.99295727397135902,0.98524422559723868,0.99989581093323665,null,6.7512965127101348,0,1.0346084521516105E-2,0.19606418811287052,0.12390823159672493,8.3888180980747282E-2,0,1.0346084521516105E-2,0.27405043209331903,5.9103052226409147,0,1.9267438309372126E-2,0.10263262649807972,-1.4231420471012405E-3,4.2603334525207974E-2]
[null,1316,1.036566466734719,0.98612272224811648,1.0069345173625108,0.99399516358565498,1.0160730220657384,1.0198596553163184,0.99639277325605535,null,6.7287839875214379,0,1.0253716636735875E-2,0.19314209157887827,0.11821318205400483,8.3473270213439726E-2,0,1.0253716636735875E-2,0.26148289991591822,5.9114173842650848,0,1.8962779215233427E-2,0.10130758885730066,-1.4381885949785165E-3,4.2222980016553592E-2]
[null,1317,1.0060433378760885,0.99595760458227578,1.0159915025029045,0.97687818274545768,0.98672326748531081,1.0058386245359918,1.0174898634112048,null,6.7480898469266162,0,1.029349110077513E-2,0.19650817657817518,0.12114730990426012,8.4188846422644348E-2,0,1.029349110077513E-2,0.27368641264497334,5.9099778769302667,0,1.9122345541578444E-2,0.10261275339476442,-1.5406386699268215E-3,4.2386764179876558E-2]
[null,1318,1.0072980405691661,0.98855494512776643,1.0298060301097895,0.98935650523495144,1.0150917137979829,0.99211488837812234,1.0139068175088657,null,6.7441091312004584,0,1.0050535999882385E-2,0.19583051334884041,0.12109703528534158,8.501849565516395E-2,0,1.0050535999882385E-2,0.27117665532199647,5.9098583897226078,0,1.9115595721562084E-2,0.10156620378270977,-9.4007595655935491E-4,4.1386318318796113E-2]
[null,1319,1.0245276800833576,1.0326048284809,1.0370468469876852,0.9838361363229543,0.97229527943162786,1.0235912760994512,1.0114342257331277,null,6.7358809752971096,0,9.943169624161332E-3,0.19582278217937543,0.11686950737267089,8.5422967922736709E-2,0,9.943169624161332E-3,0.26846286011906034,5.9091400654111395,0,1.9024579134462642E-2,0.10120256256217132,-1.0085520985899368E-3,4.0944202694079293E-2]
[null,1320,1.0213070171316283,0.98169140733635396,1.0005765747750257,0.99368034307718089,1.007274365315574,1.0070583359471519,1.0073383690061395,null,6.7374082111674847,0,1.0353513441285694E-2,0.19319407922724274,0.12031349266091643,8.3156060782527158E-2,0,1.0353513441285694E-2,0.26714454409173388,5.9117589742957994,0,1.9041359109338244E-2,0.10165484309349182,-1.4890675880856632E-3,4.2633925494520712E-2]
[null,1321,1.0362763823973531,1.0281401208322216,0.97348118807764827,0.96757627430665216,1.0075036405686559,0.99059347246736729,0.98534823662996218,null,6.702850010803278,0,1.0075725435035186E-2,0.18060611977706506,0.11688449003528373,8.1300039262290305E-2,0,1.0075725435035186E-2,0.2555885493024756,5.9118506218538753,0,1.8964251451683432E-2,9.6325637767339614E-2,-1.5974257593765891E-4,4.1490043929203024E-2]
[null,1322,0.96111704419558941,0.97205481664835658,0.96314538060455546,0.98591013301701935,1.0023835295125214,1.0111245974980858,0.96230709755554589,null,6.7683664599117401,0,1.1461119159127403E-2,0.20231005547685907,0.12908519085240461,8.0883808471209365E-2,0,1.1461119159127403E-2,0.27161621860897867,5.9134042271425464,0,1.9375644651838868E-2,0.10846390745611249,-3.9674414423393374E-3,4.7194848694124408E-2]
[null,1323,1.0339636037219906,1.0241529098675823,0.97530335546930436,1.0156415333245143,1.0495826000707755,1.0104947596222587,0.97875416300383711,null,6.7135876927787077,0,1.0301915964322901E-2,0.18516067265425221,0.11729585298291834,8.1456153636109307E-2,0,1.0301915964322901E-2,0.2562393485560055,5.9143494738997138,0,1.8976018817735998E-2,9.8664525345116133E-2,-9.7580938154570986E-4,4.2421456268396475E-2]
[null,1324,0.99887525158985258,0.98996777539055747,0.99558272676574611,1.0076685656811992,0.99489009170470166,1.0282973927314831,0.98484254895345658,null,6.7541429146159722,0,1.0817542184804933E-2,0.20036467821641132,0.12269694180843799,8.2881602666591239E-2,0,1.0817542184804933E-2,0.26892956703608112,5.9127950794681867,0,1.9161232262472669E-2,0.10568987162612302,-2.9207717346242052E-3,4.4544713266295576E-2]
[null,1325,1.0078688906304072,0.98468191246493508,0.9558347375991324,0.98684894796543954,1.006421577665874,0.97206225045016548,0.98880580588383227,null,6.7230358486850061,0,1.0515913987999861E-2,0.18361985810781836,0.12259750596424096,8.0304340905492655E-2,0,1.0515913987999861E-2,0.26236147627120254,5.9138491146271734,0,1.9112530329252173E-2,9.8807646238981847E-2,-9.1928579883001032E-4,4.3302662039669933E-2]
[null,1326,1.0039079415426031,0.98953617843102826,1.0306058759943602,1.0187674545006005,1.011236431605077,1.0213913400804431,0.98977249422096036,null,6.7530686512592428,0,1.0370375109982516E-2,0.20230148739938231,0.12144255225407291,8.5051048768013435E-2,0,1.0370375109982516E-2,0.26834101995534809,5.9114007960819084,0,1.9133871948681637E-2,0.10488117248900215,-2.1866564821159083E-3,4.270335884494908E-2]
[null,1327,1.0102674118253643,1.0338970445737525,1.0249052949505411,0.98741678188088244,1.0100145570001198,0.99644025539767189,0.97554414007687118,null,6.7243368161233272,0,9.9157655289491102E-3,0.19180973033652671,0.11868536062790651,8.4562987070363235E-2,0,9.9157655289491102E-3,0.26012222202774737,5.9100363575550059,0,1.90996884312232E-2,9.9720573105656435E-2,-5.3146053884245556E-4,4.0831357507742479E-2]
[null,1328,1.0020458905906433,1.0015851707013981,1.04363356588559,0.96654225913050451,0.95600972987213662,1.0229971447515698,1.0016687423506057,null,6.7542879909620925,0,1.0234556673094558E-2,0.20353198477424667,0.12083290975205171,8.5868356794186126E-2,0,1.0234556673094558E-2,0.27211178471715841,5.9078214529256234,0,1.9143962992695798E-2,0.10484881126093117,-2.015354951428878E-3,4.2144082696625056E-2]
[null,1329,0.99184494440803594,1.0282468478051172,0.99315193988037753,1.0056147797585513,1.0074130990502166,1.0057080961469118,0.97359477000382644,null,6.7394750201957221,0,1.0505487096553546E-2,0.19388496840707478,0.12175092306397207,8.2680785554302694E-2,0,1.0505487096553546E-2,0.26526679419462029,5.9128199384028317,0,1.9199917503352475E-2,0.10239572857721804,-1.7837614642614314E-3,4.325972595661149E-2]
[null,1330,1.0032553823603032,1.031622666540688,1.0296919023190394,0.96457856076468462,0.98041168641248777,1.0027348439977202,1.0070794565896506,null,6.7398473843888578,0,1.0015526196626542E-2,0.19511544188614122,0.11953077195051241,8.4991338021045831E-2,0,1.0015526196626542E-2,0.27102378643772035,5.9085265503093405,0,1.9137404110226137E-2,0.10120100330425284,-9.2106581089014441E-4,4.1242154180501235E-2]
[null,1331,0.9908814400357896,0.98231443572269994,1.0028696645666746,0.98236283160991456,1.0001804161560894,0.98041164796884606,0.9839209027295962,null,6.741292364516239,0,1.0365445741019672E-2,0.19407483582831028,0.123932606946108,8.3282720657444631E-2,0,1.0365445741019672E-2,0.26643012143397682,5.9110182962888169,0,1.9205262091607275E-2,0.10200213252506604,-1.3366718360503119E-3,4.2683060580955071E-2]
[null,1332,0.98106275456656777,1.0010259432972872,0.98252826295705153,0.964269376756001,0.96160195648504343,1.0222558788763632,0.99470507329788682,null,6.7617676888460503,0,1.1022091530058391E-2,0.20023985933140712,0.12461874633218176,8.2131312674455614E-2,0,1.1022091530058391E-2,0.27582733048413854,5.9111747959362901,0,1.9260325223159538E-2,0.10631413728586793,-3.1858294830772104E-3,4.5387011061623107E-2]
[null,1333,0.98163098673116989,1.0233245475747137,1.0110659277662084,0.97383460910061115,0.99866904976147475,0.98573697364341561,1.0122722306524961,null,6.7504470708809334,0,1.0263482036041794E-2,0.19451214386174318,0.12291492406008685,8.3925663616413446E-2,0,1.0263482036041794E-2,0.27683135681102478,5.9100938241956502,0,1.9257108550951793E-2,0.1018178577542295,-1.1690001618874237E-3,4.2263192192719096E-2]
[null,1334,1.0104908290692016,0.96642100005394405,0.99496001187203009,0.98616520387768447,1.0348555182157428,0.98740069833491961,0.99608267932910366,null,6.7361768256966554,0,1.0380062792298056E-2,0.19208424805110011,0.12247174929884436,8.2778068032463167E-2,0,1.0380062792298056E-2,0.26529414670248547,5.9116677237398436,0,1.909849533901252E-2,0.10135344832237884,-1.31430478585907E-3,4.2743250996381314E-2]
[null,1335,0.98740839414195636,1.0039363087891116,0.96031589020470676,0.98633201237661661,0.98078605668841157,0.9907437306808875,1.0212611853411109,null,6.7505065852105721,0,1.0807525754203094E-2,0.18997263786668245,0.12408916342666476,8.0791352290551358E-2,0,1.0807525754203094E-2,0.27823268854723288,5.9135799391530277,0,1.9224613744007153E-2,0.10199496472975798,-1.8822419352917787E-3,4.450346738793539E-2]
[null,1336,0.99979158501259469,0.99595770860375787,0.97726132808721311,1.0322741296353892,0.96021289402324284,1.0046350347348287,0.99664164821445933,null,6.7458890292611597,0,1.0701337658946037E-2,0.19289936130405083,0.12263074027170043,8.176769928000055E-2,0,1.0701337658946037E-2,0.26957515895416401,5.9151412027649801,0,1.9156230087968112E-2,0.10268728019578875,-2.0348473099380234E-3,4.40662037124432E-2]
[null,1337,0.97265442128433433,1.0047040963578999,1.0033413647041838,0.98260226345357027,1.0363524778145494,1.0067020005144411,0.98918904177439804,null,6.7624253483600416,0,1.0734240268162974E-2,0.20112033260761245,0.1251129077530185,8.3431015143249812E-2,0,1.0734240268162974E-2,0.27517705972241913,5.9110046517504342,0,1.9308362746112105E-2,0.10568038647463732,-2.6110586381919852E-3,4.4201690800752411E-2]
[null,1338,1.0267782865339266,0.96345726844282753,0.96395302736792254,0.98091741904751828,0.99669253279134895,0.97006055835707949,0.9951846655344071,null,6.7155730721825293,0,1.0324529309564167E-2,0.18246591488175648,0.12124580503454241,8.0764481578433134E-2,0,1.0324529309564167E-2,0.25922086944116207,5.9130905262979443,0,1.9012915732912139E-2,9.7785106525283744E-2,-5.2712130858275068E-4,4.2514573999074594E-2]
[null,1339,0.99559874928887282,0.99055489277807629,0.9786266658030488,0.99069270884119809,0.97906022644387758,1.0132808709135341,0.96910691044342245,null,6.7435747896340725,0,1.0851257852554429E-2,0.19599847868428549,0.12338990147538806,8.1751132157529452E-2,0,1.0851257852554429E-2,0.26408505669769733,5.9128181829571487,0,1.9179193693001039E-2,0.1042656876926885,-2.5963921085913875E-3,4.4683548384922861E-2]
[null,1340,0.98890120741377385,0.98193839056606536,1.0043204804081756,0.99602259309803221,0.99498567827542539,1.0024204493041811,1.0090962038266225,null,6.7595408359323805,0,1.0607642236054197E-2,0.19903676941012466,0.12417205573796279,8.351048812098355E-2,0,1.0607642236054197E-2,0.27593438115225144,5.9116746536794205,0,1.9216279200721841E-2,0.10453479638209623,-2.2189703893182779E-3,4.3680382638138171E-2]
[null,1341,0.98212739066502386,1.0200668242570363,1.0102251650894172,1.0206477715324007,0.98314503558780886,0.99178571954618711,1.0137222495332903,null,6.7560275516340136,0,1.0342938637918325E-2,0.19577418394154661,0.12302558329250278,8.3919287469047046E-2,0,1.0342938637918325E-2,0.27769906338153788,5.9126710509185871,0,1.9254301533110099E-2,0.10252108890173858,-1.4273881405541034E-3,4.2590380336498736E-2]
[null,1342,0.98968095806148726,0.98990402625332308,1.0152329792439212,0.99372721755415361,0.96216892512282148,1.0062830168386681,1.0271880214982281,null,6.7648604724291355,0,1.0502644026385998E-2,0.20027609216408443,0.1234654552733168,8.4254112072436535E-2,0,1.0502644026385998E-2,0.28097138659181337,5.9109314926686887,0,1.921193576235062E-2,0.1046194388785246,-2.1174596817895045E-3,4.3248018699709165E-2]
[null,1343,1.0223002729285227,1.0000729265492228,1.0285576982653484,1.0261528541769167,0.97875683786186962,0.96190229971032537,1.0017489808949087,null,6.7183713338553268,0,9.5643961917498618E-3,0.18601469454093011,0.11879153487496004,8.4829345087205521E-2,0,9.5643961917498618E-3,0.26108810585077302,5.9119182153039871,0,1.9036172872367151E-2,9.6534414822550207E-2,7.7436938398212378E-4,3.9384481118566558E-2]
[null,1344,1.001311040622789,1.0084721714212785,1.0131876108507474,1.0041625544842907,0.99101447585785896,1.0223083491696712,1.0127949763450135,null,6.7555641020851223,0,1.0481098902016081E-2,0.19926117057595719,0.12116607077806332,8.4055066658309835E-2,0,1.0481098902016081E-2,0.2751423073687439,5.9116118729155138,0,1.9147955705792991E-2,0.10419444301939623,-2.1740846491044986E-3,4.3159299712443006E-2]
[null,1345,1.011632714929898,0.99755227148318115,1.0224291286569778,1.0131574870544189,1.0124914470154698,0.98788143555318586,0.98190635276426319,null,6.7296652595407194,0,9.9905174068667547E-3,0.19254932099365918,0.12028042736058889,8.4440954038744506E-2,0,9.9905174068667547E-3,0.26100560810417106,5.9115693240779459,0,1.9092405672717108E-2,0.10022707528981009,-6.3902843258600199E-4,4.1139172435669072E-2]
[null,1346,1.0015181105975688,1.00090040749646,1.0089670338704013,1.003563153726754,1.0050467932967473,0.99667190549523543,1.0015873303101941,null,6.7431963193718865,0,1.0287080243602999E-2,0.19435454274716052,0.12158612156162514,8.3719389605530756E-2,0,1.0287080243602999E-2,0.26969925380040344,5.9118192800046563,0,1.9146830024731141E-2,0.10184102992842707,-1.3304937117796128E-3,4.2360365411131778E-2]
[null,1347,0.98298885435261618,0.98960459671912826,0.97745744305376858,0.95490705323930769,1.0132709009251586,0.99246872765887439,1.0058800856095693,null,6.7527412978736434,0,1.0780128677329921E-2,0.19437618730354481,0.12504289420142611,8.1805675711119824E-2,0,1.0780128677329921E-2,0.2756144214989007,5.9109478028251985,0,1.9249436939109268E-2,0.10346327665918401,-2.1490483667117506E-3,4.4390651101869558E-2]
[null,1348,0.99830955385311726,1.0139732731548365,0.99694731622851407,1.025367152227884,0.98666553354241249,0.98127673903485935,1.0313711964599976,null,6.7451989788266813,0,1.0211120342356312E-2,0.18951525716573395,0.121570094150938,8.3086654708958985E-2,0,1.0211120342356312E-2,0.2769703224591834,5.9136751901930742,0,1.916432493546523E-2,9.9899109016815077E-2,-7.2954986164295405E-4,4.2047576058156309E-2]
[null,1349,1.0258098244037401,1.0109874150032347,0.99396897580649757,0.99899354642538529,0.97869890752735633,0.97521272159298977,1.0180776045833102,null,6.7190886683487872,0,9.9141916970372918E-3,0.18319397647690697,0.11850469687855698,8.2727810557342255E-2,0,9.9141916970372918E-3,0.26552740427149052,5.9124164468374962,0,1.9017928357199908E-2,9.6710182539853917E-2,1.6534568187798887E-4,4.0824876748061241E-2]
[null,1350,0.99542648091331676,0.99580198468496983,0.95551140425723269,1.013941455902742,1.0105227679835258,0.97479268541385289,0.97681668888859152,null,6.7288455292175904,0,1.0629000802702912E-2,0.18550530944700341,0.12357955576721558,8.0306691065889571E-2,0,1.0629000802702912E-2,0.26257175058466831,5.9153316640967084,0,1.918014132139954E-2,9.98385498410327E-2,-1.2364663202431823E-3,4.3768333413914444E-2]
[null,1351,1.0104641347043071,0.97757360367694324,0.99865703786129256,1.0077333914358286,0.96876373880787892,0.99856282749768299,0.98466899427568932,null,6.7368424740714588,0,1.0412491400167419E-2,0.19374283616455446,0.12184507864408037,8.2994903589103622E-2,0,1.0412491400167419E-2,0.26318798600826782,5.9126262804745036,0,1.9098637864440569E-2,0.10204083306540764,-1.5708679704137135E-3,4.2876786231510339E-2]
[null,1352,0.9841626086291817,0.98801109131993892,1.002656814300245,0.98465751276038005,0.98184312953713826,0.98690304377163551,0.99800602623833778,null,6.7516667531427732,0,1.0481257247611925E-2,0.19618134397664896,0.12449448851933197,8.3355269757375117E-2,0,1.0481257247611925E-2,0.27265608827419319,5.9111542932768453,0,1.9242822579937573E-2,0.10312016193733912,-1.6976669303183697E-3,4.3159951751422239E-2]
[null,1353,1.0203835980576317,1.000969099186833,0.97645293798667843,1.0363413153097176,1.030206794543441,0.97743766483744554,0.9932406743548674,null,6.719320944019703,0,1.0186782941366285E-2,0.18340398330333543,0.11992965481769775,8.1601813942501739E-2,0,1.0186782941366285E-2,0.2606880704503558,5.9154054938725977,0,1.9046189754053849E-2,9.7672125816714292E-2,-3.73746910327749E-4,4.1947358972775274E-2]
[null,1354,1.0201521528636495,1.0081478558040424,0.98711752800313746,0.98570249953248201,1.0166422855594304,0.98637468806888329,1.0017017587502623,null,6.7220247330604552,0,1.0155970580348955E-2,0.18576504854088965,0.11942092597393281,8.2269376773612249E-2,0,1.0155970580348955E-2,0.26374751949909297,5.9120794487918129,0,1.9047401874532216E-2,9.8403035938329289E-2,-5.2850348625314326E-4,4.1820479154501725E-2]
[null,1355,0.99118996791135106,0.99500935225014031,1.0183813459203528,1.0166174480995898,0.9534059138618306,1.0209918788062231,1.0238247280531576,null,6.7693031098302701,0,1.0587302591824105E-2,0.20283314588514437,0.12296396732241821,8.4466592969998852E-2,0,1.0587302591824105E-2,0.28101048103396387,5.9119883406541787,0,1.9203549547135663E-2,0.10579077376323261,-2.550368949322133E-3,4.3596627603520371E-2]
[null,1356,0.98057782026862894,1.0304940329881391,1.0316653597199115,1.0115020327817019,1.0146101575742625,1.0278729370290995,0.9947996248802462,null,6.7658381704801522,0,1.0490803121934442E-2,0.20497148591986167,0.12231088490330755,8.522204748009081E-2,0,1.0490803121934442E-2,0.27629811194677695,5.9109469762054641,0,1.9263073307697175E-2,0.1062102129437545,-2.5838821895782277E-3,4.3199259962780068E-2]
[null,1357,1.010002574556754,0.98923472902575238,0.99588991651500336,0.99959008226175228,1.0411825006123896,0.95363604942574554,0.97724724617610093,null,6.7145860564181454,0,9.9220783333180997E-3,0.18386240021719014,0.12137542190347557,8.2735835334561483E-2,0,9.9220783333180997E-3,0.25708302748707673,5.9123412750146676,0,1.910110339823887E-2,9.6970304769640817E-2,2.5933578079837579E-4,4.0857352512496677E-2]
[null,1358,1.0115314737110555,1.003154550991723,1.0000091047988551,1.0168189027650181,1.0222282271649199,0.99583820545651291,1.0029779334013975,null,6.7357285157027844,0,1.0246837217924042E-2,0.19104285341162097,0.12044033897530643,8.3140155444787825E-2,0,1.0246837217924042E-2,0.2672851956679933,5.9130413416687073,0,1.909294503570394E-2,0.10055124173671531,-1.0602080324248367E-3,4.2194651794377362E-2]
[null,1359,1.011620514323321,1.0223749543489236,0.99413206768558315,1.0150884602555919,1.0124044471354874,0.98400246570539374,0.97522059916303172,null,6.7194197714779857,0,1.0093907134930458E-2,0.18655984060615191,0.11962671222216599,8.2658335446258641E-2,0,1.0093907134930458E-2,0.25861622446427701,5.9132772285748434,0,1.9092470665775026E-2,9.8479064231175001E-2,-4.5501766581582288E-4,4.1564912933149831E-2]
[null,1360,0.99103395124404114,0.97948347326722796,0.986465095733709,0.95638813360759967,0.9739106880812638,0.96592256134389032,1.0022349151783387,null,6.7380508018506688,0,1.0370800011043653E-2,0.18951109682683845,0.12436863491596337,8.2292233194388234E-2,0,1.0370800011043653E-2,0.26995411044708961,5.9105310593975764,0,1.9204415414970612E-2,0.10042009294616822,-9.3594980421362424E-4,4.2705108511889286E-2]
[null,1361,0.95858712008601277,0.98304032530594199,1.0262453080521032,1.0053504138041098,0.99099591544080756,1.0040982133362375,1.0014069668454157,null,6.783359174694275,0,1.0747958293588865E-2,0.20831996392339178,0.12760669481025316,8.4971179914258593E-2,0,1.0747958293588865E-2,0.28268495846616859,5.91092795614545,0,1.9390614785102619E-2,0.10823282764896168,-3.0332001870492344E-3,4.4258179187738729E-2]
[null,1362,0.97990608919405875,1.0312852597692361,1.0217309109071178,1.0194547914115992,1.0067268532656142,0.99893384782836603,1.0238691364777419,null,6.7622604351882423,0,1.0288235190910355E-2,0.19808263069667009,0.12254718434818776,8.4687000958923536E-2,0,1.0288235190910355E-2,0.28172713962039397,5.911949627861147,0,1.9266884448185834E-2,0.10314274953069434,-1.5079035545318249E-3,4.2365121278570506E-2]
[null,1363,1.0022023544691965,1.041475092186501,0.98492815364808428,0.99397071939937931,0.99013997864323744,1.0122611291658836,0.97899931241692484,null,6.7324133372624919,0,1.0482543314505096E-2,0.1911169188230197,0.12002863421577688,8.2149726464498654E-2,0,1.0482543314505096E-2,0.26444540488535584,5.9126477005782769,0,1.9143113622333712E-2,0.101348785363852,-1.6321942366038825E-3,4.3165247545976934E-2]
[null,1364,1.0141227308670089,0.96555021513541206,1.0227168934996032,1.0267759921882353,0.97599226446444864,1.0044334835767339,1.0092345688725637,null,6.748889974851398,0,1.027299011997504E-2,0.19807776164850682,0.12155481431002448,8.4584506796371625E-2,0,1.027299011997504E-2,0.2695134005484035,5.9122885069762088,0,1.9079173998935689E-2,0.10309017779655817,-1.600712013593749E-3,4.2302344789980337E-2]
[null,1365,0.98625244391429789,1.007751366421749,0.99066055868236125,1.00194903504556,1.0201046241308296,1.0157099438848072,1.0140361536707425,null,6.7622268298934731,0,1.0785907403960448E-2,0.19832648726686955,0.12347837837910722,8.2706707325052933E-2,0,1.0785907403960448E-2,0.27901600224522582,5.912760705971281,0,1.9231084876152521E-2,0.10487151803838597,-2.5785010781653656E-3,4.4414446869559081E-2]
[null,1366,1.0070071307968744,1.0115500751155162,0.9614657447280589,1.0057811571485296,0.99197883161208644,0.9756777425602402,1.0373507506343147,null,6.7347282024159716,0,1.0391931218215158E-2,0.18297973849780119,0.12128604778407892,8.0841150104466311E-2,0,1.0391931218215158E-2,0.27558891722762113,5.9145695867911057,0,1.9117159206912569E-2,9.8183538039552723E-2,-6.3005829737275757E-4,4.2792123061806873E-2]
[null,1367,1.025302423878049,1.0081411392503072,1.0369229405429079,1.0001020414014039,0.97713360022564699,1.0036060012150561,1.0186481901608229,null,6.7349311027779333,0,9.8432165326191486E-3,0.19381880148246294,0.11790888034174088,8.5428628719030203E-2,0,9.8432165326191486E-3,0.26855568060723584,5.910025819987661,0,1.9020558371535129E-2,0.10017296321026672,-5.3284359609801477E-4,4.0532613654095655E-2]
[null,1368,0.99602074363917614,1.0241506060538179,1.0237123267332653,1.0037954563900591,1.0069185748759397,1.0351586215761437,0.99513780341453462,null,6.757515072600019,0,1.0501796708563429E-2,0.20278779727221047,0.12086242826737127,8.4675831692577225E-2,0,1.0501796708563429E-2,0.27283634199039497,5.9109898029575545,0,1.9176873735912814E-2,0.10548985917700067,-2.5483920887363781E-3,4.3244529595732779E-2]
[null,1369,0.99098599640070428,1.0326172480920701,0.97093712659962039,1.0004108963369727,1.0028956549003345,1.0381357003669369,0.98619362057180326,null,6.7531728906936035,0,1.1045819644798973E-2,0.19724856929908938,0.1220609810025321,8.1381320853196673E-2,0,1.1045819644798973E-2,0.27185459360863534,5.9137648568253169,0,1.920468161154789E-2,0.10533635303215726,-3.1631847535564181E-3,4.5484719214677845E-2]
[null,1370,1.0195112648451414,0.97174093049047139,0.96328204193874123,1.0466301999703707,0.98835234794309679,1.0052621585704591,1.0033591087092482,null,6.738378746270171,0,1.0742229859868703E-2,0.18965882274454832,0.12170484656992059,8.0863344741441232E-2,0,1.0742229859868703E-2,0.26643574926446184,5.9166802224260486,0,1.9050761193284589E-2,0.10167423299072666,-1.9238241775593398E-3,4.4234590517302302E-2]
[null,1371,0.99002352174472785,0.96591646600469039,0.97995332682511216,0.99762462157148313,0.96207149622099719,1.0049344314760646,0.9798847719928766,null,6.7526915334973063,0,1.0927326010055808E-2,0.19776134232703915,0.12531605153311703,8.1890888504335901E-2,0,1.0927326010055808E-2,0.26801559218136584,5.91311990973698,0,1.9210029745950472E-2,0.10513360082981185,-2.7526648791806789E-3,4.4996783517886246E-2]
[null,1372,1.0077809465810919,0.982513797696564,1.0167188732140655,1.0026302566754348,0.97399008293328271,1.0077727770358218,1.0068851433903101,null,6.7488219919112531,0,1.0349042144251521E-2,0.19778142945522215,0.12158392853094532,8.4212043849613422E-2,0,1.0349042144251521E-2,0.27069489236616967,5.9113276997357147,0,1.9113002351334042E-2,0.10324056869583423,-1.7470865627789332E-3,4.261551348919522E-2]
[null,1373,0.99420455057571844,0.96869031812075579,1.0000819858646102,0.96905057466625666,1.006201022302569,1.043564552558655,1.0121493490472244,null,6.7739745407961571,0,1.1089270918846896E-2,0.20677157902339158,0.1242635977480581,8.3274217380364321E-2,0,1.1089270918846896E-2,0.27943726259933011,5.9104557191094811,0,1.9186872444791007E-2,0.10882577465517498,-3.9041259916073796E-3,4.5663643827168719E-2]
[null,1374,0.9889957226172208,0.98111449999483047,1.0091069584151124,0.98119209137317598,0.99486254244372752,1.0023298148463484,0.97368792987943387,null,6.7493635924998063,0,1.0565184812197755E-2,0.19965014688271449,0.12411020223938919,8.3665976778974846E-2,0,1.0565184812197755E-2,0.26623505946427045,5.9106025277755316,0,1.9215752358716611E-2,0.10460866319704933,-2.2302867206769298E-3,4.3505550523837082E-2]
[null,1375,1.0144447781493666,0.97936730782982506,1.0057645500690136,1.0446935963205135,0.99332469055303041,1.0022593832853044,0.99206625587321262,null,6.7398628005379537,0,1.0337451224665466E-2,0.1943822880970294,0.12114546747107348,8.3479251082257955E-2,0,1.0337451224665466E-2,0.26446158101469941,5.91422317090126,0,1.9077467418543652E-2,0.10201720714537162,-1.4914167377320837E-3,4.2567784145446604E-2]
[null,1376,1.0021388999202807,0.98640432426779301,0.99165995282415831,1.007149501123775,0.96169114058344918,0.98595144358352349,0.9988802730164611,null,6.7391858299439891,0,1.0389795781088814E-2,0.1913262124640461,0.12254741743334233,8.2623610132086162E-2,0,1.0389795781088814E-2,0.26790700924980371,5.9129861151642622,0,1.9143458055895731E-2,0.10111951415424962,-1.250836421511071E-3,4.2783329711814228E-2]
[null,1377,0.99000734603360185,1.0108835923552246,0.99065620632003681,0.98782608291984941,0.98827900539750224,1.0039426771259152,0.96020174923498791,null,6.738423273820505,0,1.0606452768628679E-2,0.19502549654112222,0.12285753001216068,8.2470970254439738E-2,0,1.0606452768628679E-2,0.26209907995926529,5.9119975929640214,0,1.9210119717560745E-2,0.10312623663334429,-2.039236884411033E-3,4.3675484622997189E-2]
[null,1378,0.99614344464807569,0.95679158731960157,0.96591630339406476,0.99988979127136801,1.0059464914051877,1.0108197938479104,0.97479677918471908,null,6.7499171893990537,0,1.1103283126661499E-2,0.19680193379184294,0.12528512812150813,8.0985833505734808E-2,0,1.1103283126661499E-2,0.2656201977979506,5.9140099609446954,0,1.9176199543423561E-2,0.10536363919282157,-3.0470471037901386E-3,4.5721343604869256E-2]
[null,1379,0.98564583237374659,1.0226739407971033,0.96951379456307007,0.98762162433277023,1.0202563276073402,0.99789245788517555,1.0002417280507512,null,6.7461700711637551,0,1.0732735721532518E-2,0.19125313141662784,0.1232246265841816,8.1305555732204701E-2,0,1.0732735721532518E-2,0.27351230693645512,5.9131509715926773,0,1.9234486824591512E-2,0.10220772503709474,-1.9142283056007136E-3,4.4195495345527525E-2]
[null,1380,1.0045434657079877,1.0124448910444945,1.0378064246418137,1.0019097613611443,1.0143635967880911,1.020969175830998,1.0163978618764908,null,6.7550649183589719,0,1.0193915728889601E-2,0.2009864446915606,0.12012389773293003,8.5576270043594735E-2,0,1.0193915728889601E-2,0.27510653367341059,5.9100719927540339,0,1.9130436404902411E-2,0.1038325968436187,-1.7399843072911669E-3,4.1976730522207427E-2]
[null,1381,1.0032822419009717,0.98950489520205032,0.97182801079312731,1.0097100160863792,0.99382767513115167,0.99459695728641784,1.0181720031056956,null,6.7448520419455127,0,1.0637222234010571E-2,0.19020352375682112,0.12262287086270915,8.1464635441735891E-2,0,1.0637222234010571E-2,0.27353521292481314,5.9142189917781547,0,1.9137258634679133E-2,0.10152863872951426,-1.6612779875922806E-3,4.3802187804679156E-2]
[null,1382,0.98361789608440975,1.0002566045891474,1.0152682937175985,0.99269113127838771,0.99830811428105359,0.96245469965468533,0.96938846836395365,null,6.7334980171190502,0,1.006186611056554E-2,0.19188087603284101,0.12370992365582106,8.4007263574040952E-2,0,1.006186611056554E-2,0.26261742876200683,5.9108734990743814,0,1.9245890189872564E-2,0.10023223182264396,-5.0206969046401762E-4,4.1432973697904829E-2]
[null,1383,0.99672278850773233,1.0109155685963784,1.0254191516870939,0.99524136021159482,1.0120112596201325,1.0118212235098802,0.95530794680169984,null,6.738944007604923,0,1.0299666761903812E-2,0.19938733085045493,0.12137500236826192,8.4596691752263961E-2,0,1.0299666761903812E-2,0.25977210450662652,5.9104294637808001,0,1.9173018525031286E-2,0.10363393588983007,-1.83573452152123E-3,4.2412194453177773E-2]
[null,1384,1.023406461407302,0.99684312924111595,1.0128500948510928,1.004598510981783,0.96695264835599404,1.0033178520106332,1.0033973552426569,null,6.7322422674716105,0,1.0117420171058877E-2,0.1922510392982929,0.11910758537223809,8.3896594436128041E-2,0,1.0117420171058877E-2,0.2650690837254564,5.9116546407726833,0,1.9030408811734997E-2,0.10054558088697105,-9.7440126265965722E-4,4.1661735430762251E-2]
[null,1385,0.99048747128031656,1.0042502915961022,0.98844777950482432,1.007345828923065,0.98498720924856653,1.0148688802691801,0.99842795711288546,null,6.7551915823015065,0,1.0767671175806581E-2,0.1973426763832907,0.1231632795412289,8.2499187916516642E-2,0,1.0767671175806581E-2,0.27349987436105455,5.9131754895764574,0,1.9207450443410549E-2,0.10446652638573817,-2.502255634140681E-3,4.4339353327949055E-2]
[null,1386,1.0096368535882854,0.96228009290202987,0.99126599826973016,1.0038620724588463,1.0339688443334076,1.0066585090512863,1.0090613136669073,null,6.7494485018110559,0,1.0645257105622374E-2,0.19591603711204958,0.12285544850238515,8.26355429705002E-2,0,1.0645257105622374E-2,0.27086114276407436,5.9128303842665009,0,1.9103058584904093E-2,0.10356565465631329,-2.1540410214900153E-3,4.3835273975822743E-2]
[null,1387,1.0440868767748011,1.0068023724771256,0.96694473950720128,0.98781912061689792,0.9938513769666204,0.98885303048466222,0.98891818717915125,null,6.7024063849569391,0,1.0130290195939216E-2,0.17983042817408673,0.11710268777002913,8.0894399727681601E-2,0,1.0130290195939216E-2,0.25461234601024441,5.9133014260539065,0,1.8924897139387036E-2,9.6227609221838067E-2,-2.021410426789905E-4,4.1714731902440447E-2]
[null,1388,0.9710997884406688,1.0014517717588856,1.0040987272573705,0.97802276002578037,0.99448194073863028,0.97329149675573834,0.96817444130089991,null,6.7445557349614313,0,1.0402162251360918E-2,0.19511714935390076,0.12546119767732813,8.3360357207567889E-2,0,1.0402162251360918E-2,0.26665845125397475,5.9107144708507855,0,1.9317335617745381E-2,0.10248746537813332,-1.3949450132476598E-3,4.2834252635245096E-2]
[null,1389,1.0012446281022951,0.99278044132220244,0.96451806972772292,0.96636239166537519,0.98915752916703559,0.97267723322483168,0.97346225591343727,null,6.7217964642738428,0,1.0475660119313066E-2,0.18529231203959712,0.1228451616765532,8.0801328821058324E-2,0,1.0475660119313066E-2,0.25999692060793816,5.9122728784108673,0,1.9148316838480693E-2,9.9271526117706427E-2,-9.6888401170158072E-4,4.3136903773339244E-2]
[null,1390,0.96784642009368671,1.0071585857074719,1.0333390111618928,0.98936378826222626,1.0043684321376154,0.9973376277218039,1.0132111023632038,null,6.7716996704464139,0,1.0399385915330883E-2,0.20368856443854819,0.12502758269432543,8.5393494489218361E-2,0,1.0399385915330883E-2,0.28236674167655262,5.9096541308762509,0,1.9336206359459717E-2,0.10545890437823592,-2.0487746438211329E-3,4.2822820177642815E-2]
[null,1391,0.99301042004033691,0.99589744822743098,0.98284647734941377,0.96783348821247561,1.0148752013539684,1.0330840096759846,1.0074679092114047,null,6.7620837238108633,0,1.1026001009442626E-2,0.2004054592655147,0.12336661573138713,8.2169627075926524E-2,0,1.1026001009442626E-2,0.27710005230088031,5.9113498963700231,0,1.9193466434918205E-2,0.10638512650427104,-3.2896294739227869E-3,4.5403109601866012E-2]
[null,1392,1.0256059748042776,0.99716525158464531,0.99725252085537885,0.97349545963648576,0.99825200077550691,1.0243887676690193,0.97855948084160227,null,6.7290316262978038,0,1.0447786493441408E-2,0.19399542324913993,0.11912279244163332,8.2836991509433827E-2,0,1.0447786493441408E-2,0.25982186110318339,5.9108546727705118,0,1.9018984660185125E-2,0.10224521998043055,-1.8864445600392935E-3,4.3022125143320211E-2]
[null,1393,0.97879417872026742,0.99505292336860529,0.99190548872828155,1.0006403670836184,0.98242256410610418,1.0251441034293975,1.0057930668804131,null,6.7718370462337187,0,1.1016799982389297E-2,0.20294623618074331,0.1250281840136209,8.2795785091549223E-2,0,1.1016799982389297E-2,0.27991282606700446,5.9126206107760595,0,1.9273204491110776E-2,0.1072477932523894,-3.3528150489388177E-3,4.536522141018217E-2]
[null,1394,0.96215860187080726,0.9991782946936868,0.97300299406141766,1.0008791551776823,1.0051228476117939,0.99793818948207713,1.0293470233714324,null,6.7775531200830521,0,1.1071507115490337E-2,0.19831455992267094,0.12734471036578912,8.1732350045508731E-2,0,1.1071507115490337E-2,0.28859259864705966,5.9136773154103901,0,1.9369504396679421E-2,0.105795770340522,-2.8641846923507922E-3,4.5590495646785544E-2]
[null,1395,0.99782442424752738,1.0150729108026753,1.0054671349228308,1.0177814853811473,0.99110979503120333,1.0049235464562511,1.0020241758291604,null,6.746999036487483,0,1.0379866897881194E-2,0.19509391502059201,0.12141733674117587,8.3536486216930758E-2,0,1.0379866897881194E-2,0.27144933614000177,5.9127857124573575,0,1.9166979935078939E-2,0.10240577887329676,-1.5989532349928906E-3,4.2742444338040593E-2]
[null,1396,0.97678293510279401,1.0067991912687013,0.99008579928169116,1.0385756719033985,1.0077467041899024,1.0085019838478659,0.99246062897194098,null,6.7624399829434862,0,1.0822993219438005E-2,0.19883890137358326,0.12473354711811618,8.2645145115863308E-2,0,1.0822993219438005E-2,0.27504750592783045,5.9147724129391941,0,1.9284672850085661E-2,0.10517260850393689,-2.6219705417917984E-3,4.4567159656666591E-2]
[null,1397,1.0277837741874269,0.98981481808074534,1.0312477477130348,1.0082309558645046,0.9746815569007633,1.0022112481502616,1.0409918124189386,null,6.7420664464620126,0,9.9324635109042814E-3,0.19394278346833663,0.11859611188922961,8.5156441744940845E-2,0,9.9324635109042814E-3,0.27382930365373809,5.910794481517935,0,1.900772146495211E-2,0.10051604161244079,-6.7655571486116052E-4,4.0900116825303874E-2]
[null,1398,1.0020313073122211,1.0267619247710109,1.0207211490645589,0.97877046540004331,0.9950865724858895,1.0152311993149221,0.99819199859988872,null,6.7440500680956932,0,1.0253521490526253E-2,0.19711963998935189,0.12007107451256184,8.4435300758002763E-2,0,1.0253521490526253E-2,0.27014917251534881,5.9098096044495723,0,1.914404217211399E-2,0.10269235592172271,-1.5932986621797578E-3,4.2222176439197109E-2]
[null,1399,0.97822938083894884,1.0284665954029732,1.0080212974505156,0.97942525396302049,1.040978924735251,0.98964046799564409,1.0075193380191274,null,6.7522664897758737,0,1.0345309851458337E-2,0.19518119281356092,0.12315323114917193,8.3740837196426665E-2,0,1.0345309851458337E-2,0.27681355550424203,5.9105685661627581,0,1.9276420276217676E-2,0.1023220727915857,-1.3895306898870823E-3,4.2600144571796228E-2]
[null,1400,1.0146715187787296,0.99114226329966459,0.97898041459498475,1.0316555933512326,1.0116167014277762,1.0093124866122716,0.98742500592238436,null,6.7358081083825629,0,1.0599626333103206E-2,0.19155395884154561,0.12103534953177196,8.1795182093582497E-2,0,1.0599626333103206E-2,0.26364795534562951,5.9150132074245585,0,1.9076266533301793E-2,0.10188327136738226,-1.8444573317739335E-3,4.3647374576563536E-2]
[null,1401,0.98455532764738274,1.0078870786608745,1.0352401662204163,0.99594495291216034,0.9994861571703112,0.98067143233941634,1.0110872363172509,null,6.752213060918435,0,1.0032217527849512E-2,0.19704979867182648,0.12283354145463582,8.5418594347048848E-2,0,1.0032217527849512E-2,0.27538067784151316,5.9098991892488479,0,1.9240613044420846E-2,0.10192676809813038,-8.4700789952515162E-4,4.1310886111531234E-2]
[null,1402,0.98367647548156878,0.99411369144977546,1.0164627353434752,0.95442738553872197,0.98834958735926137,0.98847499689980134,0.98704864342790699,null,6.7480019965231133,0,1.0349757082485747E-2,0.1977201430109666,0.12398476873515578,8.4152034291781572E-2,0,1.0349757082485747E-2,0.2699085611719339,5.9087379951464785,0,1.9245560130376791E-2,0.10322161856178851,-1.5871420029590548E-3,4.2618457477589487E-2]
[null,1403,0.98458620432992761,1.0205977855401986,0.9628086355215415,1.0070493269351617,1.0206208105447638,1.0080218357238939,1.0067212854022818,null,6.7536168339930311,0,1.0926368741834882E-2,0.19277425656670674,0.12358203161486146,8.094018859275813E-2,0,1.0926368741834882E-2,0.27655571742548807,5.9145655423248469,0,1.9240439399213653E-2,0.10336905652065573,-2.4032401092440457E-3,4.4992841657739861E-2]
[null,1404,0.99836758729881547,0.99268115469157114,1.0331114946783411,1.0179364930938837,1.0146572182649254,0.96450445999516543,0.98879710759917505,null,6.7335998072089991,0,9.8121827750995965E-3,0.19212264509169658,0.12191370846752832,8.514880030798401E-2,0,9.8121827750995965E-3,0.26420467332636327,5.9112106694640394,0,1.916400750493244E-2,9.9481786471813688E-2,-5.1305589787472967E-5,4.0404822164433071E-2]
[null,1405,1.0174856408087236,1.0350935111274446,0.98457927370138765,0.97656818066290718,1.0065486464893667,0.98412125608771528,1.0006452567420445,null,6.7171366953671114,0,1.0067547432947447E-2,0.18345579343027105,0.11852303563544554,8.2104894895590613E-2,0,1.0067547432947447E-2,0.26371896517643834,5.9117262988282997,0,1.9061406656534257E-2,9.7303074446878385E-2,-2.1314207458343168E-4,4.1456368372235826E-2]
[null,1406,0.99720923875902301,0.96993414492642838,0.99384909477699623,1.0375985990503427,1.0295887829555004,0.99067877374197932,0.99179432815988178,null,6.7477240486196095,0,1.0547047159306553E-2,0.19485322556532106,0.12394399805928752,8.2782387212543274E-2,0,1.0547047159306553E-2,0.26794224371797548,5.9145096675175752,0,1.9170350414655073E-2,0.10287137239279763,-1.7800591581595836E-3,4.3430862897612978E-2]
[null,1407,1.0177734997228298,0.99279521166246243,0.97673892621202729,1.0121043272806984,1.0240615711572343,1.0149715942331201,0.99105639874822304,null,6.7352572105473421,0,1.0639749235864315E-2,0.19164055852544906,0.12062699789068092,8.1650257226388315E-2,0,1.0639749235864315E-2,0.2643110883840295,5.9140794711344666,0,1.9059891259977837E-2,0.10204389518180923,-1.9675426039820042E-3,4.3812593548523314E-2]
[null,1408,0.99712695850657229,0.99549665943579868,0.9845423690821381,1.0070138483460163,0.99224923752170058,1.0033940499326526,0.98791414520630272,null,6.7442487542489999,0,1.0650988058099036E-2,0.19407691172003652,0.12284541590583925,8.2180238737916231E-2,0,1.0650988058099036E-2,0.26782959392416744,5.9133741095145451,0,1.9170801527200524E-2,0.10293830542471336,-2.025495523467237E-3,4.3858873018050124E-2]
[null,1409,1.0350447547922081,0.9999290581429624,0.98058169029613351,0.99973144340072373,0.99979729454885491,1.0370699106887327,0.99820873959064382,null,6.7321977682478336,0,1.062162669832164E-2,0.19240812848531236,0.11820608582284188,8.1871613243554409E-2,0,1.062162669832164E-2,0.26371754865500063,5.9131991834380875,0,1.8970511399691796E-2,0.10225555899046741,-2.1688299517421245E-3,4.3737968164614012E-2]
[null,1410,1.0000226195636006,1.0408479440634262,1.0337852300643235,1.015616583523592,1.0210587841549139,0.98903037069531186,1.0181423898909581,null,6.7412727903861818,0,9.8375479935714702E-3,0.19281117510211074,0.11941428464044378,8.5316487734488897E-2,0,9.8375479935714702E-3,0.27351763936660994,5.9110462500790728,0,1.9154970339979652E-2,9.9805362514691895E-2,-3.0265101047850112E-4,4.0509271619259664E-2]
[null,1411,0.98426879384587596,0.99547879689470442,0.99230356219254823,1.0091650295534238,1.0133842202443544,1.027066729108741,1.0172314763293355,null,6.7721470852394692,0,1.0970245995535454E-2,0.20220792521132841,0.12430392044475823,8.2850158480909861E-2,0,1.0970245995535454E-2,0.28170497165708297,5.9130591658895293,0,1.9242224981405844E-2,0.10683643814130506,-3.2312399454679356E-3,4.5173520378618784E-2]
[null,1412,1.0366086360953282,0.99363388194007896,0.97949220190812991,1.0069392675949012,1.0009679166307934,1.0309029694653156,0.99479665376640436,null,6.7293728229951597,0,1.0581139872136209E-2,0.19136513790640158,0.11834584762586636,8.178526254011656E-2,0,1.0581139872136209E-2,0.26192872515688337,5.9136488536832115,0,1.8962565265830282E-2,0.10175675436749898,-1.9915741714184093E-3,4.3571250620768831E-2]
[null,1413,1.0218542127394739,0.99701763729596138,1.0093960074150954,1.0096427752952795,0.98300543452207367,0.99787812079442939,1.0246819443493729,null,6.7368452392189004,0,1.0107585123031317E-2,0.19108464495355357,0.11934391955278868,8.3760838053942424E-2,0,1.0107585123031317E-2,0.27058040491171176,5.9121234628259467,0,1.9038500706804032E-2,0.10010636676441025,-8.1413500381309113E-4,4.1621236453558037E-2]
[null,1414,0.99541234250055122,1.0026619431926356,0.97523873753967505,0.9882377206919577,0.99878693229861593,1.014698253710155,0.97847700792439252,null,6.7440674007723711,0,1.0844023946953494E-2,0.19488551607364282,0.12287774825280222,8.1572714437374488E-2,0,1.0844023946953494E-2,0.26668678124768214,5.9128714588000166,0,1.9180219109736406E-2,0.1038498618876994,-2.5106594858291861E-3,4.4653760449245405E-2]
[null,1415,1.0019313062699979,0.9932546568767846,1.0238252499193043,0.99306425685699962,0.95605802581358101,1.0288539111398036,0.97822347908201457,null,6.7514793723616204,0,1.0512210562817861E-2,0.20302278880635927,0.12162851332219693,8.4586286379705208E-2,0,1.0512210562817861E-2,0.26636984345887976,5.9104035838463416,0,1.91445851864929E-2,0.105606235866047,-2.569876498361749E-3,4.3287411993955562E-2]
[null,1416,0.98601046792526215,1.0186732171123303,0.9938221158339372,1.007650627356014,0.99085902172658336,1.0243685063485473,0.98590002821409339,null,6.7564654292916426,0,1.0800582259407008E-2,0.19952922436192988,0.12291786133073106,8.2814694663873936E-2,0,1.0800582259407008E-2,0.27204500665876397,5.9128925480019072,0,1.9232441403946914E-2,0.10534144763169923,-2.7826700734734353E-3,4.447487531226111E-2]
[null,1417,0.97385372828477124,0.99395298834678047,0.98249501959003593,0.97527445901392651,1.0021547134530362,1.0151208479303648,0.97563343919136536,null,6.7608919154956189,0,1.106004538461077E-2,0.20091946400063426,0.1258984622061845,8.2086300297415843E-2,0,1.106004538461077E-2,0.27194395273771593,5.9117715401444162,0,1.9301460282700991E-2,0.10667673629736585,-3.2492987499502628E-3,4.554329827913553E-2]
[null,1418,1.0089437749606196,1.025830910156438,0.99038684593187409,0.98144090080013691,1.0020801488046878,0.95879841456117409,1.0170674534105009,null,6.7199478738214893,0,9.8794688722665547E-3,0.18158559738954028,0.11985088296076829,8.2527090182631005E-2,0,9.8794688722665547E-3,0.26802401998849879,5.9116674608653952,0,1.9106767751909691E-2,9.6032337218657851E-2,4.7182312799988853E-4,4.0681894336087765E-2]
[null,1419,0.98157736481620417,0.98762146843134568,0.96545630738026011,0.95429458655818311,0.96472820627966516,0.99103215175286974,0.96687314859865336,null,6.7415803485400216,0,1.0902622748256867E-2,0.19311331408894894,0.12555025699493358,8.0920241665881229E-2,0,1.0902622748256867E-2,0.26517287066283085,5.911569486107016,0,1.9257411936973039E-2,0.10341278489112234,-2.3110776904946822E-3,4.4895059882814878E-2]
[null,1420,0.99450452979999682,0.957006816911669,1.0175658818581945,1.0114092339436875,0.99937130901177629,0.98586067669872868,1.0164984112494859,null,6.7578307550693451,0,1.0367861429094273E-2,0.19838955967563271,0.12449384591638631,8.4331401933569958E-2,0,1.0367861429094273E-2,0.27507748551335909,5.9117536023349988,0,1.9185218447832837E-2,0.1035147595594048,-1.6081262663132517E-3,4.2693007954469828E-2]
[null,1421,0.9910985565780267,1.0011203984472428,0.99136548236009614,1.0326869328838773,0.99713632036197242,0.98536003609778633,0.99446627782998698,null,6.7441501979123011,0,1.0435513290747553E-2,0.1920842238959474,0.12318625146505728,8.2645599062969297E-2,0,1.0435513290747553E-2,0.26949510448769853,5.9143828272418277,0,1.9204056832512237E-2,0.10153503688446884,-1.3544882373553114E-3,4.2971586279175543E-2]
[null,1422,1.0111807868154525,1.0046298365943924,0.99110768793014381,0.95955044000379996,1.0374928097309468,0.99477172210511611,0.99098361210909447,null,6.728084597602054,0,1.0312813854404364E-2,0.1897531910228559,0.12057561132110096,8.2503161824944271E-2,0,1.0312813854404364E-2,0.26405308432259567,5.9104441467660918,0,1.9094814156498188E-2,0.10031574982121326,-1.1214934732480934E-3,4.2466331839999823E-2]
[null,1423,1.012066075044167,1.0177688474184841,0.98384811470422773,1.0198455593160205,1.0119679315966856,1.0325437034649865,0.9892014035128458,null,6.7418447851837753,0,1.0703270987691303E-2,0.19482886023725621,0.11997828628791253,8.2129772805737591E-2,0,1.0703270987691303E-2,0.26666848316793934,5.9141061559983212,0,1.9090098164558023E-2,0.1033730053048922,-2.4040415989377891E-3,4.4074164816096516E-2]
[null,1424,0.98564434771271747,0.98319442315224581,1.0162883433130958,0.99175286542924801,1.0247592583880143,1.0157215910560817,1.0155199457220105,null,6.7697743269757691,0,1.0665785695188152E-2,0.20370493234001602,0.12428845894614622,8.4304149192762384E-2,0,1.0665785695188152E-2,0.27991723566483306,5.910764596642994,0,1.9234495155880982E-2,0.10635518236718772,-2.7145303877516703E-3,4.3919807053701874E-2]
[null,1425,0.9790063776712572,1.0311208263507945,0.98631237066198785,1.0237302412859342,0.96344012161367054,1.0283938631499927,1.01249130633986,null,6.7685741623995401,0,1.0935415270683757E-2,0.19978335557046928,0.12333859332155601,8.2486576066042844E-2,0,1.0935415270683757E-2,0.28162541469169367,5.9141796594355363,0,1.9271997254562731E-2,0.10587133792578238,-3.0128655194219837E-3,4.5030093653317414E-2]
[null,1426,0.97858839553701693,1.0186360076716516,0.97447458586891045,1.0015482259301451,0.95620732530598707,1.0086637232240738,0.9789908854157171,null,6.7516277874353499,0,1.0898156014116551E-2,0.19563634673936622,0.12421686562020481,8.1588324475146148E-2,0,1.0898156014116551E-2,0.27068518420208315,5.9136329479380594,0,1.9274375727299821E-2,0.1042899412837365,-2.5728652172223236E-3,4.4876666666674107E-2]
[null,1427,1.013806266613722,0.97476343518927,0.99975071377321134,1.0134772032282799,1.0393567914368893,0.96120785332332914,0.97264011391092553,null,6.7175545997441883,0,9.992717342507661E-3,0.18623371727935953,0.12156291045855636,8.2966772957722215E-2,0,9.992717342507661E-3,0.25573137390315615,5.9128752699433598,0,1.9080852050156461E-2,9.8032637676413334E-2,-7.7165903599984317E-5,4.1148231379064377E-2]
[null,1428,1.0004212481118326,0.99764405597542194,1.0139276760789315,0.98144444395375097,0.98409291012883204,0.99104841099698049,0.9814710027675676,null,6.7360761149057664,0,1.0210159814495917E-2,0.19432294238079431,0.12178467613293108,8.3934810675962118E-2,0,1.0210159814495917E-2,0.26409162978694611,5.9103422469793241,0,1.9152798130481697E-2,0.10157509059388248,-1.1717005499527491E-3,4.2043620775394794E-2]
[null,1429,1.0022584725058605,1.0354895455976467,0.99007406781460972,0.96930045783485486,1.0323876762814743,1.0367538128256266,1.0153556911283952,null,6.7521212696556345,0,1.071387190181681E-2,0.19683071246630227,0.12020463879835326,8.2613706515264007E-2,0,1.071387190181681E-2,0.27661914236375562,5.9110286582226239,0,1.9142809047963703E-2,0.10411101862487128,-2.5472338770748579E-3,4.4117817493572985E-2]
[null,1430,1.01592882724444,1.0261375299863866,1.0085160369157762,0.98403659825551248,0.97609770109538307,1.017586537370617,1.0041814535375353,null,6.7361634651671745,0,1.0248215868340287E-2,0.19349103603616233,0.11868173783223386,8.3656699660444117E-2,0,1.0248215868340287E-2,0.26825458435516902,5.9107897201047086,0,1.9069617184320251E-2,0.10141118636031818,-1.3914451975795322E-3,4.2200328831400839E-2]
[null,1431,1.0404228540834761,0.99046765659223945,0.99818652952745557,0.96699367425257399,0.98987455227176824,1.0272412266819204,0.98490371577678004,null,6.7228662764807527,0,1.0349091497946593E-2,0.19242897379384083,0.11772644681862073,8.2866286211520451E-2,0,1.0349091497946593E-2,0.25811052302476106,5.9104509375744643,0,1.8943285274028263E-2,0.10137254588284923,-1.6484388182601811E-3,4.2615716718926888E-2]
[null,1432,1.0118457821864923,0.97244211459421692,0.96594282500899531,0.97668358896735985,0.9892471614206263,0.96762885220062977,0.99175205972567648,null,6.7220097388707831,0,1.0391105926194188E-2,0.18418608913520357,0.12254251189118438,8.0920519428430912E-2,0,1.0391105926194188E-2,0.26182715753222002,5.9127537166016157,0,1.9091270908679479E-2,9.8608062783805614E-2,-7.0831406651578684E-4,4.2788724656161022E-2]
[null,1433,1.0273047316626518,1.014389364746787,0.99629742427045598,1.0165493074935226,0.97759600158108417,1.0015209047116456,0.99214593383101191,null,6.7218380997118405,0,1.0131600102831269E-2,0.18785838294191595,0.11813121917482573,8.2821019276584751E-2,0,1.0131600102831269E-2,0.26074365132524358,5.913235037843747,0,1.9010194891757305E-2,9.9057732193285203E-2,-7.3926380138662274E-4,4.1720125865867194E-2]
[null,1434,1.0307149429139115,0.98499380563452255,0.96254181836972075,0.99451720020089451,1.0156873291876061,1.0023890493391936,1.0401614467557796,null,6.7339676500464352,0,1.0540535507881001E-2,0.18589328997038265,0.11974470988687294,8.0862348612254595E-2,0,1.0540535507881001E-2,0.27278194316381638,5.9139023063396259,0,1.899263711741047E-2,9.9692769833617981E-2,-1.3064039536238128E-3,4.3404049076073301E-2]
[null,1435,1.0161972111768767,0.98369985197190246,1.0356600965606231,1.0007876042254151,0.96136753424473409,0.96857600316646941,1.0188869032520491,null,6.7319521773960886,0,9.6968010200571813E-3,0.19057986468478733,0.12016283718863571,8.5343403559308764E-2,0,9.6968010200571813E-3,0.26794096890354147,5.9101363360492645,0,1.9068199951273516E-2,9.855984265054224E-2,2.3102377437405532E-4,3.9929700634355199E-2]
[null,1436,0.96509256226143159,0.98362052732103222,1.025458050690591,1.0074588426293742,0.95645046300666525,0.97566847656300437,1.0276855398766918,null,6.7738349637112263,0,1.0377777471171972E-2,0.20091100237945184,0.12673219596863522,8.4958659292638489E-2,0,1.0377777471171972E-2,0.28526494057495955,5.9110872234378347,0,1.9352279181656797E-2,0.1044238857959324,-1.6290633706384546E-3,4.2733840450756108E-2]
[null,1437,1.0421238625882072,0.99534519112430819,1.0066063882795204,1.0033912816081214,0.98206576025866565,1.010209799704499,1.0088222418791726,null,6.7234232551292532,0,1.0065206301634051E-2,0.18949915920154192,0.11715170231472152,8.3471078728991371E-2,0,1.0065206301634051E-2,0.26235028531949561,5.9119436846978166,0,1.893473257277983E-2,9.9412939053651769E-2,-7.8705476993745302E-4,4.1446728010193119E-2]
[null,1438,0.97193938188520168,1.0217063283114773,0.99217159053844439,1.0413868726860842,0.98123538207842331,0.99705541411105914,1.0198927536098801,null,6.7666611324278092,0,1.0666591773697567E-2,0.19657239171773946,0.12458062080418522,8.2880442586432526E-2,0,1.0666591773697567E-2,0.28278662952159522,5.9148080977132258,0,1.9312486172714919E-2,0.10386573626802506,-2.0683986976429637E-3,4.3923126341527022E-2]
[null,1439,1.0066731469562427,0.99155294008121841,0.99591704091186339,1.0066125304290037,1.0120664085988977,0.99146481470108316,0.98632657359074061,null,6.7341305018590383,0,1.0339164472850432E-2,0.19159897218681282,0.12166238424967661,8.2832759256609129E-2,0,1.0339164472850432E-2,0.26381699908622452,5.9127192933493582,0,1.9118955306717599E-2,0.1010492629582156,-1.2429635311016628E-3,4.2574838996525491E-2]
[null,1440,0.98501215510092144,0.99891315915557122,0.97404610616923737,1.0068767709615727,0.95829075033738709,1.0277578334092323,0.99998428521171068,null,6.7644997301155367,0,1.1128938731872455E-2,0.19965218379301142,0.12438375819869985,8.1644103469962134E-2,0,1.1128938731872455E-2,0.27671465275579016,5.9139444991755852,0,1.9238045035547227E-2,0.10645359629164935,-3.3580974253136467E-3,4.5826988820600482E-2]
[null,1441,0.99768440811921388,0.99997940952738562,1.0306367974368489,1.020173867179724,1.0042517606753159,1.0100863934857622,1.0059001507592447,null,6.7555210523518747,0,1.0272981459115213E-2,0.2004107273922266,0.12168743399608846,8.5121389963988839E-2,0,1.0272981459115213E-2,0.27322338025510806,5.9114749753135722,0,1.9167746690385304E-2,0.10389935124288592,-1.7662616284848845E-3,4.2302309126101167E-2]
[null,1442,1.0418766633972012,0.96362669570712012,0.97868925138931639,0.99496422044564559,1.0121769135002265,1.0054676200686141,1.0015256178432601,null,6.722951910862677,0,1.0411038173697783E-2,0.18806457076219379,0.1192151436711254,8.1705941462488704E-2,0,1.0411038173697783E-2,0.26037378456603089,5.9130456629029791,0,1.8935973760399669E-2,0.10004193462921811,-1.3019029953349967E-3,4.2870802103573025E-2]
[null,1443,0.9905106335449928,1.032905473973962,1.0110955276845857,0.97888269505047343,0.98743876236189732,0.99955048921608003,1.018075618255571,null,6.7496213497326032,0,1.0272700260381927E-2,0.19469537696146175,0.1213592457538747,8.3934937195935741E-2,0,1.0272700260381927E-2,0.27715924243395146,5.9103649074573061,0,1.9207321737369349E-2,0.10191228018092398,-1.313113187986959E-3,4.2301151199769002E-2]
[null,1444,1.0321676635743924,1.0039855015953161,0.96332634399971406,0.98388870253932081,1.0012646799053979,1.0061631769213424,1.0005830074090147,null,6.7198169968375323,0,1.047209332301516E-2,0.18490161088787091,0.11865225091457485,8.0765812935812822E-2,0,1.047209332301516E-2,0.26218887854866973,5.9132851256439745,0,1.8985192895126478E-2,9.9121724563479077E-2,-1.205815893032402E-3,4.312221634105054E-2]
[null,1445,0.98535775512727186,1.0342822751177732,0.98889847903418693,1.0309993079392252,0.99204394292477749,0.98253079778790053,1.0077843539677398,null,6.7443740898261968,0,1.0343439721366204E-2,0.18969436950673652,0.12234538360901458,8.2552867512726086E-2,0,1.0343439721366204E-2,0.27412363873837331,5.9144289647519148,0,1.9236103862381223E-2,0.10039519335712073,-9.9487522102209526E-4,4.2592443708947575E-2]
[null,1446,0.98453444027944625,1.0151605527899044,1.0027487792099261,0.99828007721365197,1.0037839615788373,0.99087187269145593,0.98465716458600017,null,6.7448292629513631,0,1.0397171140874396E-2,0.19463398567758597,0.12310360062846168,8.3322050786785132E-2,0,1.0397171140874396E-2,0.2690235115210427,5.9118852802705684,0,1.9240730517598999E-2,0.10230214586767845,-1.495742449007227E-3,4.281370013064615E-2]
[null,1447,1.0351857246254488,0.99519389355071131,1.0101233416806406,0.98824694724059392,0.98329598644813643,1.0183759939228865,0.98878951033684814,null,6.7253477038036582,0,1.0183876276482665E-2,0.1927343506169755,0.11788001771513917,8.3641290555708792E-2,0,1.0183876276482665E-2,0.25960828547035925,5.9109260852947925,0,1.8969794142644943E-2,0.10093430188561886,-1.2818117217319213E-3,4.1935389844151599E-2]
[null,1448,0.99258704067463199,1.0243014443996417,0.98734036514724632,0.97254199919349982,1.0163015504169366,0.98249696758847027,0.9911350146283513,null,6.7330637302886762,0,1.032446469770322E-2,0.18890942402478864,0.12195528143209255,8.2328323294027075E-2,0,1.032446469770322E-2,0.26770830606174972,5.9113557152505356,0,1.919580814606095E-2,0.10005753554229993,-9.6097140180729298E-4,4.2514307938931704E-2]
[null,1449,1.0046258417005713,1.0104047310381041,0.97981422974408727,1.0117716098250547,0.99771825181478702,1.0086086960252045,0.99542969413655102,null,6.7400488502909113,0,1.0602609396735968E-2,0.19184506622771383,0.1212927104557706,8.1893433338289273E-2,0,1.0602609396735968E-2,0.26818124606745475,5.9138923565274446,0,1.9129991411447392E-2,0.10199550242515942,-1.8411144640074464E-3,4.3659658301637712E-2]
[null,1450,0.98524723069947917,0.99953350843866917,0.98226417680940847,0.99471917968999779,0.99285856156762808,0.98748097412639457,1.0224820717270118,null,6.7543911078981154,0,1.0611144555566944E-2,0.19269862448867317,0.12416853439097679,8.217741384988396E-2,0,1.0611144555566944E-2,0.27893971664320893,5.9128354221030834,0,1.9236724510086945E-2,0.10232375595057962,-1.6838886048842884E-3,4.3694804566502043E-2]
[null,1451,1.0009171373518726,1.0048048372950444,1.033248927538106,0.9716227131641666,1.0156046670875558,0.98943262706124679,1.0149950484581072,null,6.7440894585506221,0,9.9868717277000803E-3,0.19558277649220404,0.12101152967369423,8.5240646416590168E-2,0,9.9868717277000803E-3,0.27278666212413422,5.9087010851665918,0,1.9150098342289552E-2,0.10126663573352943,-7.7413557618125149E-4,4.1124160177767405E-2]
[null,1452,1.0112620369780736,0.99554457276585206,1.0298043192139608,0.98966772451247442,1.0292949561485145,1.0013626140399996,1.0097231565833833,null,6.742530751234697,0,1.0074014377241185E-2,0.19628748333888801,0.12028291714442894,8.4999492825266018E-2,0,1.0074014377241185E-2,0.26980167198616517,5.9098752998767221,0,1.9094380987100989E-2,0.10180329370778614,-1.0967867294280815E-3,4.1482998097764283E-2]
[null,1453,0.97809115038334704,1.0139231172962411,1.0282019658781461,0.98579199518480709,0.98071779302289386,1.0087677811827751,1.0158425919285909,null,6.7673811470832836,0,1.0425442669676481E-2,0.20265429016444059,0.1234864921916172,8.5055696599074346E-2,0,1.0425442669676481E-2,0.28117138319752316,5.9097585327200379,0,1.9277207883545925E-2,0.10518808754146637,-2.1406604685363585E-3,4.2930117254108606E-2]
[null,1454,1.0105478147034201,1.0335862100270634,1.0118437977672692,0.97397084071155104,1.0280056010374377,0.97280490823731747,1.0429086894514634,null,6.7313361530275309,0,9.7904188023705922E-3,0.1857604782943833,0.11890781738633892,8.3956838983118801E-2,0,9.7904188023705922E-3,0.27571972062697642,5.9100569937131668,0,1.9098191108910197E-2,9.7199395375952471E-2,3.2151554009721259E-4,4.031520199857775E-2]
[null,1455,0.99574737130206437,1.0140589846356374,1.0020126155029203,1.0318544100163942,0.9921279938285924,1.0170583514583758,1.0046497488228725,null,6.7546749988324883,0,1.0563467882347258E-2,0.19753153382287106,0.12178401726079323,8.3365004226414047E-2,0,1.0563467882347258E-2,0.27387947232733439,5.9137411377019093,0,1.9178376403970625E-2,0.10386306361671808,-2.1660870398405481E-3,4.3498480512314849E-2]
[null,1456,0.96484806140025081,0.98764929351634811,0.97379368803365463,0.99544224589271002,1.0036879562643772,1.0237272383942169,1.0119786503376262,null,6.7832333867643655,0,1.1374579541719892E-2,0.20398251655720712,0.12756539814686399,8.1738697435405072E-2,0,1.1374579541719892E-2,0.28561961319413737,5.9133401082645127,0,1.9353710639415805E-2,0.1087762905475643,-3.9814419738660985E-3,4.6838493953117954E-2]
[null,1457,0.98070495682943637,0.98566161775592231,1.0024062566325564,0.97795006676518503,0.99371111809085955,0.97679865371427765,1.0347673984929484,null,6.7603897950657341,0,1.0423428921740932E-2,0.19502655800727861,0.12505727165269676,8.3470051372559029E-2,0,1.0423428921740932E-2,0.28270902537092601,5.910805931769465,0,1.9262352571948031E-2,0.10252590764251794,-1.3891283202029381E-3,4.2921824998543794E-2]
[null,1458,1.034633268554624,1.0029108452078788,1.0006617585932067,1.0442413853058834,1.0379112466191056,0.99717339389818638,0.95814780830802748,null,6.7102802265354216,0,1.0026798133964707E-2,0.18712126170431398,0.11775072394843422,8.2963924589643759E-2,0,1.0026798133964707E-2,0.24975667279237043,5.9144866104981491,0,1.8972606167000753E-2,9.845528431852904E-2,-5.1542749514840985E-4,4.1288570012129745E-2]
[null,1459,1.0328650578456735,0.99831824508551115,1.0209186964802011,1.0159700904146569,0.99886056486510477,0.9911212761588527,0.99700669460726854,null,6.7205008995067388,0,9.8269970533274992E-3,0.18897509975786084,0.11779939347865707,8.4332554576812283E-2,0,9.8269970533274992E-3,0.25985702443774567,5.9118079822672245,0,1.8981626655001284E-2,9.8439762231119388E-2,-1.5836862301525618E-4,4.0465824725332326E-2]
[null,1460,0.96376812533079792,1.0245157599481252,0.99259635977978478,1.0172773573828611,0.99898375280700524,1.0125603010925863,0.99360313361732089,null,6.769851657582457,0,1.0907432245294302E-2,0.20113739534757774,0.12549079906577398,8.284374064084471E-2,0,1.0907432245294302E-2,0.27929875658702819,5.9134812950243099,0,1.936004193515653E-2,0.10625532452224669,-2.9305600760406955E-3,4.491486453555648E-2]
[null,1461,1.0030060273404626,1.0169539279413609,1.0063387875433565,1.0104476451404354,1.0132259641222008,1.009717881220384,0.9867913767549632,null,6.7403368402293431,0,1.0359393152627305E-2,0.19496058995257751,0.1206844460584036,8.351644591669552E-2,0,1.0359393152627305E-2,0.26636686921580954,5.9123401270356242,0,1.9138755028621123E-2,0.10229161175941291,-1.6201418370752007E-3,4.2658137099275864E-2]
[null,1462,0.97943532335419381,1.010748904112065,0.96050024078549723,0.97550419277469635,1.0056634817167975,0.99890237091977563,0.98951860586370333,null,6.7488709112600755,0,1.095170507379049E-2,0.19255973243250429,0.12475790505937639,8.0721213541196171E-2,0,1.095170507379049E-2,0.27248835469067256,5.9129844589933978,0,1.9269558505820131E-2,0.10337433820364821,-2.3818223295742126E-3,4.509717216303407E-2]
[null,1463,0.98900601908371955,1.0173877745130615,1.0191809618787682,1.0214482159597498,1.0097452791994002,0.96164717011890988,1.0074414647996621,null,6.7385572440880113,0,9.8922817472084333E-3,0.18974215798516331,0.12212880375700547,8.4386905757096939E-2,0,9.8922817472084333E-3,0.2712262619519204,5.9122035509372362,0,1.9215694970741191E-2,9.8923974154140545E-2,-4.7608997873197683E-6,4.0734655474491704E-2]
[null,1464,0.984565510285207,0.97883766393193494,1.01679421431887,1.0176216459899352,0.98234818259195622,0.99306985469872,0.97347635288579626,null,6.7519475240720697,0,1.0454614688863832E-2,0.19982130983854246,0.12463608890988383,8.4173059736835254E-2,0,1.0454614688863832E-2,0.26654139070780386,5.9121333555756719,0,1.9240555777795234E-2,0.10430149636785944,-1.9499752790180117E-3,4.3050242436696272E-2]
[null,1465,0.96261312949229938,1.0144170840277962,0.97875668730173038,0.98716892990070582,1.0163314887665782,1.0145074159868133,0.9633363640435938,null,6.7618708933678739,0,1.1121446588048351E-2,0.20091746285874629,0.1264062111822031,8.1855266827646725E-2,0,1.1121446588048351E-2,0.27137356947500585,5.912620533008373,0,1.9366829001911022E-2,0.10687548729588142,-3.3406037877763309E-3,4.5796137505884703E-2]
[null,1466,0.96881026536249992,1.00002048525955,0.98963196292147737,0.98981843722503671,0.99074741379608777,0.99564545949961913,1.0074154179490287,null,6.7660368973010749,0,1.0808443791174628E-2,0.19843803572144067,0.12610905575475337,8.2652346573920538E-2,0,1.0808443791174628E-2,0.28030073851026532,5.9121622717642106,0,1.9330602487793207E-2,0.10498433516829535,-2.4477363803851581E-3,4.4507247700779684E-2]
[null,1467,1.0054059071181933,0.98622814092989675,0.9977970065820666,0.98811441620818985,1.0033693613472576,0.99485212271432266,1.0256882955592757,null,6.7472699984722508,0,1.0394480347277364E-2,0.19316140852431757,0.1220432055737176,8.3086767638837752E-2,0,1.0394480347277364E-2,0.27507674552604766,5.9116142355321575,0,1.9125781128450946E-2,0.10177809941674444,-1.4188647895887888E-3,4.2802619921556984E-2]
[null,1468,0.98959185228720448,0.97982967961782519,0.9637036451404235,1.0142911574248115,0.96859809193083457,0.99007651631049898,0.9778617546377496,null,6.7431393678243872,0,1.0857180556489746E-2,0.1918084184425716,0.12496151499767798,8.0863353852105316E-2,0,1.0857180556489746E-2,0.26600080111802765,5.9149086783632301,0,1.921243176108018E-2,0.10280475866417654,-2.1285264000105737E-3,4.470793702552648E-2]
[null,1469,0.98995556031878795,1.0415286081527939,0.99197146424422777,1.0038246715006935,1.0368145027046849,0.99475040396462167,1.0355113141082866,null,6.7510369637753245,0,1.0364531003088508E-2,0.19094912195583325,0.12138057862414507,8.2822295900563392E-2,0,1.0364531003088508E-2,0.28148607368417505,5.9127890428313421,0,1.9210407776859999E-2,0.10090455054342408,-1.1844013939937891E-3,4.2679293852971811E-2]
[null,1470,0.98728019549409773,0.98621159416000581,0.96751739954230109,1.0027295075081168,1.0066262844974458,1.0333792630454068,0.98593366237296898,null,6.7628214880901787,0,1.128947893086946E-2,0.20057857187047884,0.12485769864505462,8.1183019398414713E-2,0,1.128947893086946E-2,0.27286562843892198,5.9140765147830292,0,1.9225330666564597E-2,0.10729904889546311,-3.7523893927269751E-3,4.6488064784979966E-2]
[null,1471,0.96942456719679748,0.9972052080480166,0.986772025708885,0.9928824858595523,0.9898482622643846,1.035110464214323,0.98380780331235951,null,6.775401665372323,0,1.1271401428748487E-2,0.20606203170762522,0.12622637261563757,8.2437327027719984E-2,0,1.1271401428748487E-2,0.277361632682399,5.9124867172719719,0,1.9327036703235923E-2,0.10917353882878698,-4.0866163139762126E-3,4.6413624848921205E-2]
[null,1472,0.98652986974917511,1.0345123806861474,0.99955434312582736,0.98694459245689115,1.0053793880730693,0.99853205003835188,0.97509885890345893,null,6.7392669423302607,0,1.0401191031310273E-2,0.19379003174895454,0.12199002552236625,8.308035337887372E-2,0,1.0401191031310273E-2,0.26640335609865223,5.9114524006238769,0,1.9229530433834002E-2,0.10202019989064075,-1.529208690886141E-3,4.2830253323947284E-2]
[null,1473,1.0112124339682418,0.98350422995694986,1.0031125573724693,1.0108347468746124,1.0019670340349318,1.0319654891644832,1.0293093007729408,null,6.7611633249438263,0,1.0683326256794837E-2,0.20009856712333446,0.12137754788524439,8.3473482739558139E-2,0,1.0683326256794837E-2,0.2780874585607388,5.9125432322071889,0,1.9094645427598429E-2,0.10515542387832262,-2.6590688424558734E-3,4.3992035964294636E-2]
[null,1474,0.98835531512699115,0.98631577610395971,1.0219317739776039,1.0107305900172994,0.99214844299068217,1.0275060608521376,0.99205464539410537,null,6.7668884031248382,0,1.0692377436850951E-2,0.20592487863206213,0.12368192833736488,8.4584370311900095E-2,0,1.0692377436850951E-2,0.27379564804775114,5.9114667784028043,0,1.9219324058343139E-2,0.10721565160252863,-3.0294833806347146E-3,4.4029307112715715E-2]
[null,1475,1.0165520822286278,0.99805475105080443,1.0048598977652188,0.99574399994478746,1.0371513850027272,0.95929937367956764,0.96934810980968877,null,6.7092374746138717,0,9.8019441528587291E-3,0.18406601780833659,0.12000048369831746,8.3244336106464631E-2,0,9.8019441528587291E-3,0.25381574321090289,5.9116291485468908,0,1.9066327161704973E-2,9.6646260318839661E-2,4.0649642196094904E-4,4.0362661340451987E-2]
[null,1476,1.0025852053845143,1.0010013392994241,0.98761159767829876,1.0068022044603648,0.96819640474340762,1.015483172579092,1.011353419822153,null,6.7507988446595091,0,1.0666742408243576E-2,0.19525068244554533,0.12185047480314247,8.2449707492812441E-2,0,1.0666742408243576E-2,0.27378900972970271,5.9131925452223397,0,1.9141036418954815E-2,0.10340223772381291,-2.2005958045792518E-3,4.3923746627775546E-2]
[null,1477,0.9875843208041174,1.0218800641212253,1.0029644502822654,1.0413061763879736,1.012639692741734,1.0132573962538063,0.97164468285166006,null,6.7490030272226482,0,1.0567347565919885E-2,0.19788287365614557,0.12239593338475943,8.3334462600879372E-2,0,1.0567347565919885E-2,0.26664643721250508,5.9141982627069849,0,1.9223630216065171E-2,0.10399867665113227,-2.191705564529967E-3,4.3514456358709007E-2]
[null,1478,0.98857582033241809,1.002376128316127,1.0120155842714029,1.0045463631704865,0.9938985512743399,1.0351252410935201,1.0200829351215337,null,6.7731885481435734,0,1.0788217694921819E-2,0.20474447060764822,0.1230473163512852,8.4076363826780881E-2,0,1.0788217694921819E-2,0.28200297693822202,5.9116992992214943,0,1.9218093727812118E-2,0.10712369714730227,-3.1476299134944753E-3,4.4423960236521544E-2]
[null,1479,0.99909816043005439,1.0298863961578693,0.99426001483995607,0.97209615303259855,1.0266314244532992,1.0267368020276342,1.000548654280081,null,6.7479526101565233,0,1.0629745207879545E-2,0.1965006848819433,0.12076955915312899,8.282247290609128E-2,0,1.0629745207879545E-2,0.27257861214135576,5.9109464465124493,0,1.9160014580375757E-2,0.10371991632014413,-2.3164950808979741E-3,4.3771398741932636E-2]
[null,1480,1.0080074501535246,0.98203413134059936,1.0095974702007111,0.99473796857684527,1.0064649640576437,0.99115319387847389,0.99119984099731917,null,6.736798523804179,0,1.0241822009461794E-2,0.19368016041512981,0.12171454493471992,8.3686247419377191E-2,0,1.0241822009461794E-2,0.26485855564277122,5.9113066596684556,0,1.9111786805856252E-2,0.10145600601402049,-1.1894371547588249E-3,4.2174000058603653E-2]
[null,1481,1.0234552287405776,0.98719546921689205,0.99530930033269116,0.99522510890887506,1.0057782330792073,0.99820388448249375,0.99111943950391668,null,6.7266763214293519,0,1.0263537653262414E-2,0.19002627886582898,0.11988959526234526,8.2753539783155472E-2,0,1.0263537653262414E-2,0.26141202581859302,5.9121378505963147,0,1.903015498460155E-2,0.10025013243800088,-1.0866775340239259E-3,4.2263421214534115E-2]
[null,1482,0.97443726411971665,0.9990576495170761,0.98885103846752032,1.0237714565325247,1.0053587793951353,1.0182555136048388,0.98700392663469927,null,6.767188335109366,0,1.1002089656414065E-2,0.20175954222244344,0.12544409000377083,8.2559900034173572E-2,0,1.1002089656414065E-2,0.2752034755654833,5.9140409211669036,0,1.9298107958925236E-2,0.10678317823525989,-3.2055269837542762E-3,4.5304646906156577E-2]
[null,1483,1.0261627328900758,0.97521476039901767,1.0034676057464222,0.98500632638611485,0.99647419366238144,0.99592218450844361,1.0289002918025381,null,6.736524830987034,0,1.0193747290380143E-2,0.19102918921013989,0.12000826945657102,8.3374985062163245E-2,0,1.0193747290380143E-2,0.27058484640158659,5.9111274500110671,0,1.9016100656616543E-2,0.10037162518707353,-9.6367192059539607E-4,4.197603692240643E-2]
[null,1484,1.0171999465441952,0.98189616791998047,1.0060099243889191,1.0007876898989829,1.0279966677183452,1.0410044587776957,0.97393243847488786,null,6.7453019888661823,0,1.0693867758086423E-2,0.20115731522066499,0.1206882069448087,8.3434943615455101E-2,0,1.0693867758086423E-2,0.26242306815881233,5.9118367241249912,0,1.9062911505607291E-2,0.10556009542199801,-2.8967201164500369E-3,4.4035443990296089E-2]
[null,1485,1.0244026935681572,1.0086197331284334,0.98887029592914633,1.035902829099171,1.0013665653036632,1.0140221247487602,1.0160962168554524,null,6.7365092855897402,0,1.0379347799680702E-2,0.19034495454293371,0.11887138838717577,8.2483782344900655E-2,0,1.0379347799680702E-2,0.26900157211701137,5.9146955781500976,0,1.902522835880081E-2,0.10074093004366307,-1.3944551388918756E-3,4.2740306784046993E-2]
[null,1486,0.98859223262438767,1.0439720910385797,1.0350790160434999,1.0249717700083558,0.96861661391831322,0.97848099988394865,0.98917706060897803,null,6.7373237831807131,0,9.8213902468735678E-3,0.19286286250785176,0.12062576573188777,8.532572051618792E-2,0,9.8213902468735678E-3,0.26780852686289186,5.9114763754748596,0,1.921800217575698E-2,9.9768887359075034E-2,-2.0509434212540541E-4,4.0442736894329388E-2]
[null,1487,0.987674808976298,1.000704126186621,1.0051236720001588,0.99783865837330288,1.019008734186762,0.98171507914790035,0.97647451234094362,null,6.7395676449037225,0,1.0310172068058813E-2,0.19368543156946053,0.1233730977681279,8.3417725962671121E-2,0,1.0310172068058813E-2,0.2652242428102542,5.9117274443522527,0,1.9223124473283001E-2,0.1016837645954108,-1.2226400617868084E-3,4.245545343404928E-2]
[null,1488,1.0009644670529148,1.0087834167857681,1.0146182467264204,1.0164101648225059,1.0442014188715079,1.0323143647482045,1.0444910702162176,null,6.769331482697452,0,1.0572708624330593E-2,0.20142883679654291,0.12116619629183754,8.4283991221205362E-2,0,1.0572708624330593E-2,0.28483112248454634,5.9121921081314746,0,1.9149840803282914E-2,0.10525353851182688,-2.5106837862785255E-3,4.3536532243011468E-2]
[null,1489,0.99096196722936425,0.98816996778284472,0.98508125585188699,1.0266881437492794,0.96781017263943359,0.96627734013459077,0.96898697006064038,null,6.7312123010085161,0,1.0348658828747945E-2,0.18871879480409107,0.12396528565151529,8.2137420246506276E-2,0,1.0348658828747945E-2,0.26097000252334451,5.9144077811882543,0,1.9204815006787317E-2,0.10006941076570065,-8.7514424186705363E-4,4.2613935064179091E-2]
[null,1490,0.98551364649250572,1.0467868760073393,0.99378967491302328,1.0204079878357133,1.0103969306621379,0.96958936015153707,0.98818649071947495,null,6.731363189035906,0,1.0110017793661896E-2,0.18676280297031239,0.12164847701923845,8.2760752426567483E-2,0,1.0110017793661896E-2,0.26745970897320215,5.9135838700961418,0,1.923522869419882E-2,9.8603008497084602E-2,-3.2191339905480684E-4,4.1631253758215525E-2]
[null,1491,1.0090882360318361,1.0269722991412766,0.98367165424178071,1.0467061500823474,0.98478965485565717,0.97642524668488029,0.98299695243339835,null,6.7203250104365466,0,1.0113942653993331E-2,0.18405328973012763,0.11990304084682703,8.2057748335711417E-2,0,1.0113942653993331E-2,0.26058923984426308,5.9155679106421371,0,1.9105994215494273E-2,9.7664279454869884E-2,-2.6390826735039327E-4,4.1647415634461289E-2]
[null,1492,0.9936226711515157,1.0038462707188762,0.99774386641611912,0.98192044903886966,1.0033819583588102,0.98237913241168351,1.009059372947525,null,6.7424339440932046,0,1.0307875795256768E-2,0.19153694757825634,0.12261995585305277,8.3044794000056946E-2,0,1.0307875795256768E-2,0.272455459999625,5.911282464258365,0,1.9190083603736075E-2,0.10092482548326959,-1.0665844745327262E-3,4.244599779137178E-2]
[null,1493,0.99187720381636246,0.98693055519628359,1.0073153136731221,0.97117937122497733,1.0089254848167575,0.98412548940563394,1.0031190047059315,null,6.746249420746218,0,1.0333171703377291E-2,0.19474850816030553,0.12349158981405983,8.362075081889532E-2,0,1.0333171703377291E-2,0.27167406933617666,5.9101629514073712,0,1.9199738739071836E-2,0.10213093199405762,-1.3292813622316343E-3,4.2550161838508301E-2]
[null,1494,0.98974225391230775,1.0287853825845859,0.95988929630810482,1.0123665467264455,0.96816115286167004,1.0004345682314562,1.0255905865257342,null,6.7506100427809876,0,1.0778147067883737E-2,0.1893361734136737,0.12259953915223633,8.0798628682946183E-2,0,1.0778147067883737E-2,0.27945428026427915,5.9150108257814846,0,1.921159461673597E-2,0.10167514432533843,-1.8586346425901231E-3,4.4382491186883512E-2]
[null,1495,0.97278108770381788,0.99248332884497426,1.0009415614400243,1.0156718532936198,1.0225816009330255,0.9787967428167158,0.99280220126264285,null,6.7559811889128172,0,1.0512199786903362E-2,0.19626121631029697,0.12575691476711792,8.3284437028223232E-2,0,1.0512199786903362E-2,0.27357753009879748,5.9129269114526011,0,1.9307632929320407E-2,0.10324999753310636,-1.6708188273045514E-3,4.3287367620657699E-2]
[null,1496,0.97310423762853204,0.970987143640763,1.0028880136742451,0.96252582782338147,0.97082446060001226,1.03224902908461,1.0168192958430766,null,6.7861517361508188,0,1.1168086229300741E-2,0.20910855773849332,0.12678314187556367,8.352901977236582E-2,0,1.1168086229300741E-2,0.28565882972323525,5.9099452664592471,0,1.9305771889706488E-2,0.10990257745442604,-4.0696200092353047E-3,4.5988191247015364E-2]
[null,1497,1.0179249834917363,1.0196975284706,0.97269634556909479,0.97541918329330768,0.97002244832319717,1.0219359310711942,1.0065378726377008,null,6.7345994394335396,0,1.0626583253302069E-2,0.19025838725267494,0.11939896224674418,8.1430857299226264E-2,0,1.0626583253302069E-2,0.26876055695190482,5.9123175608674892,0,1.9059094137179607E-2,0.10151363829072001,-1.8979959881954697E-3,4.3758378375789518E-2]
[null,1498,1.0279529560874707,1.031858732810693,0.96118528961266347,1.0190075989920651,0.98157914551042336,1.0085394340449674,0.9734559412284981,null,6.7129788440419507,0,1.0436464155728589E-2,0.18368731323467172,0.11787867624050766,8.0577768342729117E-2,0,1.0436464155728589E-2,0.25607854736856428,5.9152999739490095,0,1.9006848483649384E-2,9.8577157519801159E-2,-1.1029428689061647E-3,4.2975501771919805E-2]
[null,1499,1.0166387209428727,0.98105266372338384,0.99040847861027614,1.0134702967554527,1.0164954277926292,1.0119507541737855,1.0295531698331051,null,6.7489014258142994,0,1.054773114110834E-2,0.19387454048820846,0.12108588361222439,8.2640342081872653E-2,0,1.054773114110834E-2,0.27474985946720659,5.9133974748904254,0,1.9065870134809502E-2,0.102530292640701,-1.8765169140808587E-3,4.3433679412928514E-2]
[null,1500,0.9941003527185418,0.99566949712527775,0.98868516283690577,0.98481745751836314,1.0051737691932241,1.0135233823102285,1.0302314370968293,null,6.7613161566786362,0,1.0751539853389103E-2,0.19711640054613636,0.123133149614314,8.259915151707202E-2,0,1.0751539853389103E-2,0.28114927910978582,5.9119445863366158,0,1.9187447194624729E-2,0.10433438503750182,-2.4211700909190629E-3,4.4272927413502243E-2]
[null,1501,0.97888619976599989,1.0094849079556329,1.0169321631694364,0.98557205551543658,1.032793868895423,1.0030768323501522,0.99189371922728875,null,6.7575530120191711,0,1.0480604178501723E-2,0.20035894440326965,0.12382012919497654,8.4257106908989632E-2,0,1.0480604178501723E-2,0.27380315182265896,5.9103938899986108,0,1.9272680903186585E-2,0.10457501204429495,-2.0851657858874852E-3,4.3157262529068388E-2]
[null,1502,1.0277192693908126,0.99281441004474558,0.990960435915619,1.0063701367917322,1.0090746135896786,0.97095776175018822,0.98944710209015463,null,6.712023848539169,0,9.9555441280259668E-3,0.18313953455984416,0.11920068549130795,8.2437231477730813E-2,0,9.9555441280259668E-3,0.25734496062718648,5.9129829684626536,0,1.9008054386415261E-2,9.6826452021241349E-2,8.8802814374507304E-5,4.0995158698414282E-2]
[null,1503,1.0208422932731998,1.0402479948903072,1.0462984355755292,0.98176572228738823,0.9814283129302499,1.0201333153534786,1.0196608754343051,null,6.7386376005430764,0,9.8338744797679348E-3,0.19633475113301016,0.11677551100367432,8.603061820987222E-2,0,9.8338744797679348E-3,0.27124574763050341,5.9084873205943529,0,1.9043789108030888E-2,0.10100984447601287,-7.8412635566193253E-4,4.0494144743277782E-2]
[null,1504,0.99490701090274847,1.0162368775233406,1.0122707339362571,1.0321083095977799,0.97927229468775379,1.0152397923121714,1.0002804839831028,null,6.7538829616352727,0,1.0449663626385258E-2,0.19839412473626369,0.12158970029005579,8.3986628997557489E-2,0,1.0449663626385258E-2,0.27274315263341248,5.913174020150274,0,1.9183000852604919E-2,0.10378806572123658,-2.005586588801673E-3,4.3029854842665763E-2]
[null,1505,1.0241771541643654,1.0214794893400547,0.99791231995565566,0.95869223776611967,0.98066554186738453,1.0292932559550403,0.9633214516360642,null,6.7224306364958508,0,1.0398581609677614E-2,0.19327064233630456,0.11813303458476655,8.2820479445903677E-2,0,1.0398581609677614E-2,0.25632129761399353,5.9100176637417334,0,1.9026400291503327E-2,0.10182981855343738,-1.8082082619192115E-3,4.2819508190123728E-2]
[null,1506,0.99518288488571371,0.97584245893400301,1.0192688841200415,1.0286098001620219,1.0177531813496761,0.97579336431972785,0.97812268512731393,null,6.7400495080012224,0,1.0154480178112548E-2,0.19479667662177119,0.12341016503263365,8.4290400948482905E-2,0,1.0154480178112548E-2,0.26337395700388389,5.9125854282516528,0,1.9181481874910707E-2,0.10155479824568751,-9.5774192117718284E-4,4.1814341943373905E-2]
[null,1507,0.97497618248228635,1.0282928846337598,0.99645987485559651,1.0160213739091417,0.98139355848302179,0.99535854548617997,1.0175734498426363,null,6.7608002390670761,0,1.0546563841705716E-2,0.19559965051905107,0.12379248882167246,8.310579326321986E-2,0,1.0546563841705716E-2,0.28104553747520838,5.9131974060714372,0,1.9295015519992294E-2,0.10313136973321597,-1.7958950184806608E-3,4.3428872681760038E-2]
[null,1508,1.0135538382694229,0.98511461857591043,1.0287502405810214,0.99533749918418168,1.0218782180131165,1.0011573403233316,1.014425261662929,null,6.7443481204588247,0,1.0103954756352229E-2,0.19656432872886007,0.12053746010737028,8.4948390357556525E-2,0,1.0103954756352229E-2,0.27053274238844854,5.9102424979423569,0,1.9082191302347923E-2,0.10199962547100612,-1.1654030888754679E-3,4.1606287249754743E-2]
[null,1509,0.97452519876707,1.0134648325970208,0.99860340119179092,1.035622102010713,1.0225326742660628,1.032828054648383,1.0014332380097466,null,6.7758282506315624,0,1.0996315185586617E-2,0.20458965191572792,0.1245304918442646,8.3245636392491523E-2,0,1.0996315185586617E-2,0.28046679043424344,5.9141365052976562,0,1.9297603135952253E-2,0.10775652588607497,-3.4758229379625097E-3,4.528086866310662E-2]
[null,1510,1.0164153893136465,1.0396690815154128,0.99164743307523873,0.98725696455565382,1.0247161591381759,0.98757228679074827,1.0036830725904984,null,6.7203991437609218,0,1.0032371958105905E-2,0.18474088864573796,0.11831113122272459,8.2570008805276054E-2,0,1.0032371958105905E-2,0.2650893289396391,5.9119116245482166,0,1.9067048387381418E-2,9.7639655401796976E-2,-2.4206421769670865E-4,4.1311522027839491E-2]
[null,1511,0.98633475652328284,1.0021198018697679,0.98703188731947744,1.0278803697319503,1.0318859923883081,1.0138450646896304,0.97881011494641557,null,6.7537460943718797,0,1.0825289906272651E-2,0.19798256797949362,0.12381365674743815,8.2368742174505696E-2,0,1.0825289906272651E-2,0.26917890158158314,5.9143640732691694,0,1.9230623579844387E-2,0.1048793566087458,-2.6484445731575481E-3,4.4576617004256622E-2]
[null,1512,1.0230328161522539,0.99108230127473795,1.0378563680215644,1.0446300303835896,0.99159181513464678,1.0011577901155149,0.96285978871270872,null,6.7262641458465966,0,9.9050746340102244E-3,0.19530597274460881,0.11896243527361333,8.5323821096321847E-2,0,9.9050746340102244E-3,0.25435760162085896,5.9123764219496344,0,1.9032354385909944E-2,0.10089551602456118,-7.7731155420451598E-4,4.0787334305292501E-2]
[null,1513,0.98054282622641808,0.96562081015307033,1.0083080935629138,1.0011630038793362,1.0050416739361026,0.98034086605382975,1.0125869296355094,null,6.7615920629988988,0,1.0501196773987377E-2,0.19820640038862633,0.12599524535634907,8.3780315661229787E-2,0,1.0501196773987377E-2,0.27726166826661192,5.9117269357309832,0,1.9263271721335091E-2,0.10389326245454505,-1.7770957527148965E-3,4.3242059171932953E-2]
[null,1514,0.96100721616244278,1.0154162834344758,0.99418530314907305,1.0078807629323461,1.0043774493199673,0.96233948677101422,1.0021971718451643,null,6.755268417126608,0,1.0421536274786461E-2,0.19263041850954377,0.12627054066086066,8.2914989578484311E-2,0,1.0421536274786461E-2,0.27771501087499939,5.9128846941572668,0,1.9376292892575392E-2,0.10168083636428747,-1.1183973266737041E-3,4.2914031415263891E-2]
[null,1515,1.0097909459292504,1.0118729683083467,0.98985311501722639,0.98783545682873319,0.96641021153761875,0.95796075836980987,1.0035833587509155,null,6.7182042920011398,0,9.9251796207880036E-3,0.18228147051276519,0.12041817293787369,8.2448627063833171E-2,0,9.9251796207880036E-3,0.26427680338794934,5.9120427886105746,0,1.9102234616749824E-2,9.6426012277737172E-2,3.3805953136180919E-4,4.0870123062289168E-2]
[null,1516,1.0140511027455108,0.99504146164201068,1.0172344617707265,1.0078500013294989,1.0308683074729816,0.97120782721091559,1.0409046313584882,null,6.7370414967460439,0,9.8537652996832439E-3,0.18845986792448205,0.12021168789002494,8.429799603514411E-2,0,9.8537652996832439E-3,0.27442711629878985,5.9115802515449856,0,1.9079553715238586E-2,9.834976415169068E-2,5.9207586427561321E-5,4.0576051599255071E-2]
[null,1517,0.99476222892818389,1.0075552055788053,1.0055239270786704,1.0064512445327556,1.0458589296851679,1.0027100540529261,0.98866708509552759,null,6.7454282833576107,0,1.0421484826400738E-2,0.19589261561977508,0.12215270819799273,8.3492626040716361E-2,0,1.0421484826400738E-2,0.26852193256729573,5.9121702394878914,0,1.9183798367417779E-2,0.10282212721668199,-1.7215837001342716E-3,4.2913819559968938E-2]
[null,1518,0.96022588352757432,0.97398165586707308,1.0070740541465271,0.9984235970797386,0.9672706878144588,0.9672440349145216,0.99307135977074967,null,6.7640021994126984,0,1.0552464889802512E-2,0.19881047633435991,0.1282426198996291,8.3690183120379638E-2,0,1.0552464889802512E-2,0.27628837676241458,5.9116487866040526,0,1.9380908851633398E-2,0.10427358492007664,-1.7859092273243638E-3,4.3453172147475246E-2]
[null,1519,1.0174652601340801,1.0163339625959265,1.022909123377941,1.0051136470679083,1.0008710464192911,1.0014164192439434,0.98721562884522318,null,6.7284893830131844,0,9.9850397190010872E-3,0.19258041485485033,0.11869309142710653,8.4477469482307402E-2,0,9.9850397190010872E-3,0.26197394964862869,5.9111071899666889,0,1.9061513980501536E-2,0.10021958735710636,-7.4044999603497608E-4,4.1116616292030346E-2]
[null,1520,0.98113804425090745,0.97884937643326586,1.0019802378823448,1.0009740864829322,0.99927161927754748,0.99323386888891407,0.97589862169008645,null,6.7529298505786155,0,1.0629625182429088E-2,0.19875910937744573,0.12535753926800036,8.3264554441117924E-2,0,1.0629625182429088E-2,0.26812812453356483,5.9120741584409657,0,1.9259898806058905E-2,0.10451020807476276,-2.1946468617961698E-3,4.3770904498491386E-2]
[null,1521,0.99444271292985398,1.0016173711547738,0.97810705889813054,1.019990398993516,0.95764225292740368,0.97317844540288212,1.0107128800814216,null,6.7394109681655241,0,1.0389095815413599E-2,0.18750615026600009,0.12299545270706128,8.1841141557575645E-2,0,1.0389095815413599E-2,0.27178292166336976,5.9144306283215196,0,1.9185559206191857E-2,9.9773979792703443E-2,-8.8531272665069607E-4,4.2780447377752946E-2]
[null,1522,0.98304055735530749,0.97658553187631247,0.95910390698264902,0.9703052398331381,0.95263125891098754,1.0234797382085483,0.96826361159349661,null,6.7564021160584122,0,1.1359711285217611E-2,0.19931957128674532,0.12604811649366837,8.0575707086417217E-2,0,1.1359711285217611E-2,0.26830307112356805,5.9127785993055175,0,1.9249145248950199E-2,0.10707876943937668,-3.7281330451257077E-3,4.6777269119292586E-2]
[null,1523,0.9906636168320897,0.99028720636788681,1.0001448789254213,1.0036328534295811,0.96191292560936659,0.98235062777293258,0.97470882561735162,null,6.7390667167564837,0,1.0376980188815318E-2,0.19350816880270047,0.12361147017145352,8.3097800704524161E-2,0,1.0376980188815318E-2,0.26409344500930293,5.9123211008102476,0,1.9206471804404851E-2,0.10184193953698797,-1.3442374670671294E-3,4.2730557383922368E-2]
[null,1524,0.98803092232830259,0.97959006392509329,1.0032267394281562,0.99685640016446264,0.99113372358817708,0.97699569965733135,1.0407855200798652,null,6.759027851707609,0,1.0368234442418063E-2,0.19422974652481784,0.12442147215016429,8.3529099868839732E-2,0,1.0368234442418063E-2,0.28232813264290019,5.9117814052891866,0,1.9221135038144908E-2,0.10206547181334512,-1.2431555767346712E-3,4.2694543956943297E-2]
[null,1525,1.0311101292947527,1.0055002549495979,0.97354752817292134,0.99174035531885418,1.0160023771991415,0.99432863332954691,1.0057628268065024,null,6.7184384456330903,0,1.0261138301338632E-2,0.18394773557237099,0.1185198616538488,8.141544252306189E-2,0,1.0261138301338632E-2,0.26273323604339843,5.9131534343689696,0,1.8990609974416924E-2,9.8104609318834551E-2,-6.8002493219465252E-4,4.2253541110380717E-2]
[null,1526,1.0050800303630345,1.0092639470046438,0.97746348797746896,1.0287232362832825,0.96758971426616358,0.99138843130816956,0.99532214668916896,null,6.7339077866161317,0,1.0443291671649571E-2,0.1883043781920094,0.12133590745982642,8.1736075276609518E-2,0,1.0443291671649571E-2,0.26643742915357638,5.9149381232835916,0,1.9127539203245544E-2,0.10023104793409522,-1.2063301540527164E-3,4.3003616267229879E-2]
[null,1527,0.97426745788171942,0.99201459248728308,0.98560752937436868,1.0012939353581525,0.97909890337034822,0.9930199948710523,1.0219312198669019,null,6.7667755151223385,0,1.0794365731780742E-2,0.19700043516020241,0.12588370808972824,8.2439359124827929E-2,0,1.0794365731780742E-2,0.28256300724844241,5.9130059384870286,0,1.9299083055432945E-2,0.10443334346652769,-2.298636267856204E-3,4.4449276757996821E-2]
[null,1528,0.99810295905075364,1.0079275787101956,1.0241909837876944,1.003816747718818,0.96840920282909115,1.0125682562843248,0.98814770150252684,null,6.7482775039132115,0,1.0317164836803353E-2,0.19936366193844809,0.12137402133237242,8.4645167500808124E-2,0,1.0317164836803353E-2,0.2684278785641861,5.9109634195334495,0,1.9165455264443066E-2,0.10368421947619366,-1.8305681077560546E-3,4.2484248411072852E-2]
[null,1529,1.036207215914247,0.99807454832721088,0.99668523707514278,0.98414343225899215,1.0023380913438764,1.0277990484672808,1.0166103356072664,null,6.7337463686328176,0,1.0376412019567937E-2,0.19250824348195805,0.11787134308486957,8.2910961974960409E-2,0,1.0376412019567937E-2,0.26746816125289608,5.9114619205935464,0,1.8964602607221569E-2,0.10149002681958737,-1.6571089463132036E-3,4.2728217764092004E-2]
[null,1530,0.99683128623917328,1.0370498029809709,0.98219860882935661,0.97661988126922461,1.0025335623232692,1.0260349295388753,0.99255907012125411,null,6.7449042398265178,0,1.0727403764022302E-2,0.19479094692407301,0.12093124739938871,8.2052784046387842E-2,0,1.0727403764022302E-2,0.27086093790017707,5.9118606306011436,0,1.9172423204787854E-2,0.10343818048081913,-2.3764500238177069E-3,4.4173539293553513E-2]
[null,1531,1.0320450314653395,0.97737292939582177,1.0109086875743483,0.99845954854725028,0.9949054261028244,1.028116414970548,0.99269993254131139,null,6.7363478431980992,0,1.0385598439913518E-2,0.19678066987301759,0.1190819771898534,8.3736802039197783E-2,0,1.0385598439913518E-2,0.2625148355226925,5.9114333213331456,0,1.8985820492824473E-2,0.10301333130212349,-1.9649603627158443E-3,4.2766045807953249E-2]
[null,1532,1.0000998189021055,0.99601188609999824,1.0281554038284646,0.98511763455432266,0.97730422185477539,1.0005439616693099,0.9840961108451779,null,6.7425834861089537,0,1.0190792165804707E-2,0.19807941589852446,0.12163394760890919,8.4840387014674612E-2,0,1.0190792165804707E-2,0.2658053048597197,5.9097247930713293,0,1.9154549529595739E-2,0.10281584082671107,-1.4346209459123146E-3,4.1963868245397357E-2]
[null,1533,0.96111044364259068,1.0375818946361146,0.95274818324308641,1.0071784981484262,1.0290862291179286,0.98706852323776695,1.0107611006468649,null,6.759782914253047,0,1.097907854509278E-2,0.19082966190688727,0.12595681562419178,8.0385679422853906E-2,0,1.097907854509278E-2,0.28221950506950455,5.9151140885722606,0,1.9375683606262951E-2,0.10284781493842547,-2.1562261329002002E-3,4.520989124556065E-2]
[null,1534,0.99860463598931404,0.98806477656518299,1.0465734091639469,1.0056660006042475,1.0265172784971792,0.98481913027052548,0.9985508370296815,null,6.7456443340458465,0,9.9186601442146551E-3,0.19810791931769245,0.12185365841472011,8.6032296365125716E-2,0,9.9186601442146551E-3,0.26873701650647991,5.9097618602191586,0,1.9162711282447412E-2,0.10190844361626704,-7.6284869423457575E-4,4.0843277018183681E-2]
[null,1535,1.0001886524085859,0.97808895930789475,1.0178043847848599,1.0205556807167888,0.98271758514395724,0.99548024101978605,1.0277408527424183,null,6.7570039013738405,0,1.0310555496813222E-2,0.19736263985899496,0.12270755457281594,8.4381949016990004E-2,0,1.0310555496813222E-2,0.27724932543079872,5.9122341228302462,0,1.9154065382228483E-2,0.10296682902554125,-1.509617069187104E-3,4.2457032325412175E-2]
[null,1536,0.99705056204267095,1.0000535145728171,0.97622178556841943,0.99716971039395896,1.0093655150946033,0.99615019233176894,0.99014286406223451,null,6.7398888664193048,0,1.0631065210882199E-2,0.19133724177345982,0.12278548527589982,8.1653709112731523E-2,0,1.0631065210882199E-2,0.26771591474705309,5.9133004476813555,0,1.9171220447743231E-2,0.10190880903079907,-1.7607959290848599E-3,4.3776834279345783E-2]
[null,1537,1.0087765935872355,0.97635541885179178,0.97713489588842639,1.0057246135060287,1.0081858254631926,0.98908311147116379,0.98956250942534374,null,6.7338115141907373,0,1.0532330031770206E-2,0.18981725883874873,0.12251106898876594,8.1667299043491084E-2,0,1.0532330031770206E-2,0.26402961509266754,5.9137128223829416,0,1.9107663223820879E-2,0.10105297037866803,-1.457444144337939E-3,4.3370260385969348E-2]
[null,1538,1.0253173065483467,0.99404370911673523,0.99124727502357035,1.0042191771132172,1.0019370281157709,1.0465282938097602,0.98519479520248587,null,6.7413046548803717,0,1.0747139711379772E-2,0.19778560169356144,0.11941557431845119,8.2538110523578387E-2,0,1.0747139711379772E-2,0.26369112622756846,5.9128507290220584,0,1.9020481192982507E-2,0.10455492452845115,-2.8067010381832491E-3,4.4254808411903906E-2]
[null,1539,0.97342992161631781,0.98550978164692471,1.0132994883122273,1.0104108521434003,0.99046883758640847,0.99854729650162688,0.994315455532363,null,6.7662229102311766,0,1.0634089162374526E-2,0.20220321982184708,0.12578794085788825,8.4077784268905748E-2,0,1.0634089162374526E-2,0.27581535515529398,5.9119431069157162,0,1.9303897506465089E-2,0.10572700915691126,-2.424689825200459E-3,4.3789286373347891E-2]
[null,1540,0.98541429492170129,0.99789066151458927,0.99791426871506905,0.99671488672724029,0.98516875843255824,0.98863107441505849,1.0148291423180704,null,6.7544430010332723,0,1.0485017192444988E-2,0.19487771843526513,0.12393276473890463,8.3126933734713318E-2,0,1.0485017192444988E-2,0.27696046809556535,5.9120724685332293,0,1.923578641812821E-2,0.10267645021689846,-1.615023674433507E-3,4.3175434534999557E-2]
[null,1541,1.0346079450028678,0.99036884585446017,1.025001690949811,0.98648619899171641,0.98874000980428867,1.0219432067056695,0.98662995850294843,null,6.7286815468506243,0,1.0114004470023941E-2,0.19567233786298996,0.11790257629657264,8.4559164366537806E-2,0,1.0114004470023941E-2,0.25958338932457847,5.9099805373230403,0,1.8972735136914817E-2,0.10172389585083008,-1.3607594927111789E-3,4.1647670181872494E-2]
[null,1542,0.98524541881353545,0.95441372162604776,1.0154269468818888,1.0324254397045047,1.0052929382330844,1.0052246806637954,1.0292948110532785,null,6.7777185394399417,0,1.0703298523367695E-2,0.20416098781960443,0.12584204301897814,8.4324041955535972E-2,0,1.0703298523367695E-2,0.28313006185609652,5.9130112743220122,0,1.9236734685856172E-2,0.10663860646874855,-2.6994888900021209E-3,4.4074278203110724E-2]
[null,1543,0.95632378668935525,0.9739211184986919,1.0190488790379988,1.0060783042212118,1.0231324659376191,0.9912971817135634,0.99543091467729727,null,6.7792911987423672,0,1.074613394521731E-2,0.206079478218121,0.12853047142464061,8.4495836003636485E-2,0,1.074613394521731E-2,0.28048399753690872,5.9113807344209661,0,1.9404074567079894E-2,0.10744859289998528,-2.7826531748394541E-3,4.4250666845866579E-2]
[null,1544,0.98169859526076231,1.0263982941755372,1.0323551053830493,1.013834040366655,1.0233324173778771,0.96020805059743519,0.98518840524342099,null,6.7361682889650796,0,9.7997722089362554E-3,0.19166527013424756,0.12235279202618742,8.5139099514283903E-2,0,9.7997722089362554E-3,0.26702748245653773,5.911032956028893,0,1.9256726077669428E-2,9.9281749093438884E-2,5.8495971851262729E-5,4.035371766197085E-2]
[null,1545,0.98385397318436663,0.96438313237071982,1.0076632030585839,0.98684996191645558,1.0038887589500733,1.018875787685078,0.96385982859290609,null,6.760660660250319,0,1.0889366863588408E-2,0.20533681939274331,0.12564815829544235,8.3586723645197411E-2,0,1.0889366863588408E-2,0.26665755308304873,5.9109900426079669,0,1.9244560278080157E-2,0.10766515768515965,-3.3088292465248735E-3,4.4840474509209687E-2]
[null,1546,1.0291636076612123,0.99318487184206661,1.0370502049951684,0.97584658735955276,0.98921493919958137,0.9878011266553981,1.0189033771826721,null,6.7276681171709711,0,9.7127594397859954E-3,0.19128598667983618,0.11816854564632984,8.5386925323609197E-2,0,9.7127594397859954E-3,0.26628574640985581,5.9087083455360094,0,1.9000609877751793E-2,9.8857753010985705E-2,-2.1209879710070045E-5,3.9995414566305641E-2]
[null,1547,1.0207361032571183,0.99111275282104383,1.031439952809432,0.97832180301349236,1.0115472428324976,0.98995849635222899,0.98114652050541895,null,6.7241507887995686,0,9.8715638522493161E-3,0.19280841444326641,0.11934878725741212,8.4939755858310914E-2,0,9.8715638522493161E-3,0.25874174421977297,5.9091677781684062,0,1.9044344676509513E-2,9.9918707555757616E-2,-4.6808625056698886E-4,4.064934287069788E-2]
[null,1548,1.0089477878569679,1.0150579114991074,1.0204262160134008,0.99159769137134202,1.0124116541622661,1.0276791294795946,0.97582857052278626,null,6.7407577178465719,0,1.0361467488354191E-2,0.19910797203585717,0.11980156864255864,8.4335844501743709E-2,0,1.0361467488354191E-2,0.2635252955619326,5.9105195029437247,0,1.9106746261320362E-2,0.10374327395497904,-2.0491649001300989E-3,4.2666678844581196E-2]
[null,1549,1.0354382023120825,0.97625472762137488,0.98633905628403185,0.99302213989616139,0.95741122426012859,1.0221248784633865,0.96938973431206665,null,6.723195412071151,0,1.0519636070631831E-2,0.19219492945929542,0.11919475305482376,8.210853038236246E-2,0,1.0519636070631831E-2,0.25494896253924432,5.9125182715991969,0,1.8968510019763244E-2,0.10184864042420247,-1.9051743211846402E-3,4.3317988913442372E-2]
[null,1550,0.99484399361782416,0.99986050683263261,1.0265576682823834,1.0249930230108957,0.98224263042239046,1.0075800797846453,1.0026498324997997,null,6.7555887959147096,0,1.0314073357050048E-2,0.20000263393391296,0.12211855149659438,8.4868100847896921E-2,0,1.0314073357050048E-2,0.27287405087843741,5.9119710403127943,0,1.9183347947523195E-2,0.10389560569830975,-1.7960534484743006E-3,4.2471518247711629E-2]
[null,1551,0.96518499488404264,1.0357881163576217,1.0254980589241787,0.97731100634209089,1.034908970221905,1.0193364612069662,1.0284354546074377,null,6.7801901482766693,0,1.060360006702846E-2,0.20529501242522732,0.12412672810765348,8.4993798690700575E-2,0,1.060360006702846E-2,0.28928343668493373,5.9094563046091011,0,1.9351738213394764E-2,0.10670038542681493,-2.6809935867274032E-3,4.3663737705569458E-2]
[null,1552,0.98994196776073873,1.0003760660992689,0.98739366899184688,1.0019895419261808,1.0008643769953391,0.99243716673725757,0.99065742366319809,null,6.7448451228227908,0,1.0562639193820052E-2,0.19328264187889424,0.12344165950990083,8.2375960602506987E-2,0,1.0562639193820052E-2,0.26944424226021502,5.912944500925934,0,1.9210483390788423E-2,0.10237112470518334,-1.7205585710987244E-3,4.3495068120460875E-2]
[null,1553,1.0296429505595557,0.99733137456638277,0.98884040922951477,0.98397458859631037,0.99054748641549406,0.97769302918464795,1.0077024498054099,null,6.7159376469338765,0,1.0004926569681978E-2,0.1834703819824392,0.11880058257907854,8.235373248015837E-2,0,1.0004926569681978E-2,0.26218200130809194,5.9118904018477858,0,1.8998143831218114E-2,9.710397921063986E-2,-6.0083108945339526E-5,4.1198506803406781E-2]
[null,1554,1.0015302819791341,0.9965713681799061,1.0081279808651487,0.98104347968552097,0.98852959727543033,0.97917227211450419,0.98310039949030503,null,6.7307115556942492,0,1.0132548384911996E-2,0.19119729790930914,0.12181141692945031,8.3562526216564501E-2,0,1.0132548384911996E-2,0.26313704655174064,5.9106499668041792,0,1.9146763872723929E-2,0.10022825692105504,-7.4575023346883573E-4,4.1724030722687711E-2]
[null,1555,1.0360021120400948,1.0062895381562542,1.0184681610960427,0.97431060259606361,1.0191845731388267,1.0260935684837671,0.9861259028062207,null,6.7249314357209302,0,1.0130161301592888E-2,0.1941000924118467,0.11711430459590312,8.4142751377341424E-2,0,1.0130161301592888E-2,0.25929612777641459,5.9096976639386245,0,1.8965644187268312E-2,0.10123158224621666,-1.3309319511542305E-3,4.17142011384646E-2]
[null,1556,0.98817855151109113,1.0093359702176006,1.0079022069040298,1.0397118636415137,0.99134180550753848,1.0195260015857788,1.0220939726084817,null,6.7679471463881233,0,1.0636655364918207E-2,0.2006425207944369,0.1228346394843009,8.3833896356584323E-2,0,1.0636655364918207E-2,0.2810694801001824,5.9138329523739603,0,1.9220310724864915E-2,0.10519132841719621,-2.4778354020610731E-3,4.3799853538655738E-2]
[null,1557,0.97938504319287245,1.0088381822430237,1.0087881956454952,0.95835173585164701,0.99162974826130124,0.9961567922550425,0.98763330219468326,null,6.7510832305463877,0,1.048025220060762E-2,0.19795173544778871,0.12394502062580212,8.3705728580632785E-2,0,1.048025220060762E-2,0.27182509458277426,5.9093864123040438,0,1.9269844260580028E-2,0.10373512470652106,-1.8915431085103108E-3,4.315581314675021E-2]
[null,1558,1.0043229884335552,0.96311777143679067,0.96592212239514241,0.99569443965238824,1.0003524056102799,1.0395076882788412,0.96469079178862382,null,6.7511075290468412,0,1.1293378510713914E-2,0.2001730401070409,0.12393751913770389,8.0952266546542154E-2,0,1.1293378510713914E-2,0.26329160440370397,5.9137827941418033,0,1.9131627777853998E-2,0.10716814495462715,-3.8335905831209283E-3,4.6504122560680067E-2]
[null,1559,0.99310393551178944,0.98544303849765758,0.99007863418862008,0.96772699976074017,0.98510991403425663,0.97954484141395071,1.0085536525279215,null,6.7435771260023145,0,1.0434936668916065E-2,0.19170753047200964,0.12374043717482706,8.2556790403714261E-2,0,1.0434936668916065E-2,0.27235225542307162,5.9109433569603995,0,1.9192949470086186E-2,0.1014009479441197,-1.2863536990199514E-3,4.2969211853108341E-2]
[null,1560,1.0121427536816792,1.0290165379840714,0.99723851316901635,1.0448077275678151,1.0372008086998654,1.0055622079800588,1.0053306721526467,null,6.7362559616773412,0,1.0253369106137229E-2,0.19038151234537556,0.11919896276092694,8.3003305443683895E-2,0,1.0253369106137229E-2,0.26840688993673761,5.9147095327220542,0,1.9089690080348123E-2,0.10034120832879147,-1.0966888879883074E-3,4.2221548947406526E-2]
[null,1561,0.99510792306130214,0.98654193440096538,0.99064198427924599,0.96355451343365228,1.0157335901533431,1.0262111024469271,0.97822880069493845,null,6.7519977403948603,0,1.0899480425253216E-2,0.20040929898299178,0.1234255866796327,8.2530398700876612E-2,0,1.0899480425253216E-2,0.2679710846313349,5.9106864892312068,0,1.9181894535606658E-2,0.10597385313018211,-3.0629858529755381E-3,4.4882120355998506E-2]
[null,1562,1.012833850172641,1.0110079518542736,0.9770320984227916,1.0123996101458179,0.98097541158482515,1.0183969687045042,0.98616507374301099,null,6.7352563725876236,0,1.0641805454403614E-2,0.19176100673669103,0.12033174559562763,8.1670441229528698E-2,0,1.0641805454403614E-2,0.2644156938909823,5.9140793346283784,0,1.9086014848417106E-2,0.10209302403550556,-2.0019490679808027E-3,4.3821060690474894E-2]
[null,1563,1.0054714521947896,1.0139942895803487,0.99270695367969231,0.969308156198883,0.99200337920343873,0.97788617521959753,1.0368825428482307,null,6.7368304576478435,0,1.0140739983676988E-2,0.1870299423359871,0.12078155341337608,8.2770807770275637E-2,0,1.0140739983676988E-2,0.27613171181867235,5.9108824390910089,0,1.912542765651427E-2,9.8797304289231211E-2,-4.4649099556660747E-4,4.1757762268351706E-2]
[null,1564,1.0199422316983349,0.99983424936830334,1.0012201392903048,0.98764642755907595,1.0339984156161688,1.0219738730353951,0.97833266620881798,null,6.732536231411224,0,1.0432823600242511E-2,0.19485967174001972,0.11958340143589014,8.3108836805043343E-2,0,1.0432823600242511E-2,0.26096402688365472,5.9113966950550418,0,1.9048501745515312E-2,0.10249849105524536,-1.8839039216112493E-3,4.2960510612422842E-2]
[null,1565,0.98533106279097848,0.98866586653063715,0.99768145897602034,1.0215927257587758,1.0013675263395367,0.98752804335629585,0.9829641584221297,null,6.7483419637669284,0,1.0518100938225102E-2,0.19542519757200791,0.12440897213761135,8.3014222849967789E-2,0,1.0518100938225102E-2,0.26827227165209377,5.9134300378069433,0,1.9236253739907189E-2,0.10297682032601105,-1.7334798290504331E-3,4.3311667511434844E-2]
[null,1566,1.0095332228503007,1.0303903772544565,1.0185205664209278,0.99279714242728134,1.0216149217041146,1.0027584772588238,1.0447280841692754,null,6.7464885222011253,0,1.0056485806655595E-2,0.19270336478735353,0.1190515055942646,8.4434548219602459E-2,0,1.0056485806655595E-2,0.27940118566931804,5.9106934362675627,0,1.9103612864410327E-2,0.10050053245817156,-8.1048222362436952E-4,4.1410818564062077E-2]
[null,1567,1.0036567937786669,0.98099458421681751,1.0168493292089327,0.99296803449687865,0.99332140210091302,0.98433820425451934,0.98398090119350889,null,6.7359194906009456,0,1.015549872894189E-2,0.19412007171675391,0.12215664881660478,8.4115143461896899E-2,0,1.015549872894189E-2,0.26345699873249473,5.9107982135898718,0,1.9135230813448801E-2,0.10132284476756978,-1.0041974520952675E-3,4.1818536154393848E-2]
[null,1568,0.9613692165195874,0.9831047095674561,0.99997813521562073,1.0149387716739442,1.0324333603870741,0.98843478970645937,1.0289062649211662,null,6.7805738628331369,0,1.0794598877259292E-2,0.20124613207725542,0.12775280863321697,8.3417714229501297E-2,0,1.0794598877259292E-2,0.28796603659567616,5.9129414752032821,0,1.9374156809300918E-2,0.10592314420877989,-2.4978417334612386E-3,4.4450236809579144E-2]
[null,1569,1.0016478949477621,1.0265146517573152,0.9987495325000072,1.0430089004643233,0.99813298380699311,0.98428384772209254,0.98294527470100412,null,6.7296573080988029,0,1.0138738309528876E-2,0.1886750299572445,0.12053727311431454,8.3027707231740577E-2,0,1.0138738309528876E-2,0.26325881471564627,5.9145275094412399,0,1.9146124723765826E-2,9.9367144527685317E-2,-6.3181534333434108E-4,4.174951973049449E-2]
[null,1570,0.9777453080698788,1.0157278516941037,1.037923373375176,0.95884233970739996,0.98962188639611248,0.99448261958454165,0.96281580904102615,null,6.7460049008230802,0,1.0186433807791603E-2,0.20087363128440069,0.12325428651840972,8.5417969738608324E-2,0,1.0186433807791603E-2,0.26527015246123808,5.9077390899745188,0,1.9279179394065031E-2,0.10376838111554749,-1.5437109665652365E-3,4.1945921302858201E-2]
[null,1571,1.0149356955865139,0.99823862912581762,0.96468622419671834,0.98688207785545801,1.0127220185371513,0.99643721358682535,0.98905451910432352,null,6.7259853535614136,0,1.0560406844299127E-2,0.18683796387937854,0.12091948785724385,8.0860983155453189E-2,0,1.0560406844299127E-2,0.26273381121736367,5.9133733288339512,0,1.9074868051781855E-2,0.10009113793052719,-1.3921030667649785E-3,4.3485875702477111E-2]
[null,1572,1.0011885573204773,1.0273109959360658,1.0128619279590474,0.96895577697361901,0.98856967563646259,1.0054700908305279,1.0034223188216083,null,6.740905750136835,0,1.0231290271233902E-2,0.19441820191131917,0.12029313645863768,8.3951284811387472E-2,0,1.0231290271233902E-2,0.27086265195357645,5.9097281300090589,0,1.9148621772990145E-2,0.10167839321998949,-1.3053022352844019E-3,4.2130632235160732E-2]
[null,1573,1.0344209380319307,0.97203861510622436,1.0358611852857165,1.0078526368889638,0.99685157179265615,0.97867336582865261,1.016697926945811,null,6.7256234131924488,0,9.6729030886901698E-3,0.19016667170027213,0.11860658188346454,8.5301563087784221E-2,0,9.6729030886901698E-3,0.2637119775489053,5.9105062373570671,0,1.8973687737238967E-2,9.8336477999996147E-2,1.8892267106349235E-4,3.9831293206659048E-2]
[null,1574,1.0145675213050647,0.9969277668524531,1.0213153898784069,0.98453879560624369,1.0140789163768258,0.98707164578560358,1.0271112978130668,null,6.737978784774274,0,9.9658370065771086E-3,0.19175750526949709,0.11998335230996089,8.4502745075579117E-2,0,9.9658370065771086E-3,0.27215876172056686,5.9100871613188817,0,1.9076817267956153E-2,9.98696476435805E-2,-4.9474877197341666E-4,4.1037542940223791E-2]
[null,1575,0.97257136147571055,0.99123455414441364,1.0031069710180645,1.0232078016140589,0.96616024388142285,0.97509262958592358,0.97898641357228133,null,6.7516053470929958,0,1.0460517540173712E-2,0.19592374153477721,0.12580548456349122,8.3369538998471326E-2,0,1.0460517540173712E-2,0.2694913998291929,5.9132121874044872,0,1.9308841416900469E-2,0.10296176265256347,-1.5421586346137776E-3,4.3074549327721992E-2]
[null,1576,0.98954530953040254,0.98850217001132512,1.0134891055658564,1.0333831806515028,1.0109554285975773,1.0285647555437702,0.97480284968018638,null,6.7616068370063998,0,1.0759597423364209E-2,0.20464713566267648,0.12358580223881585,8.4009732800643735E-2,0,1.0759597423364209E-2,0.26877012582125503,5.9131735299470858,0,1.9212690872377775E-2,0.1069948504285872,-3.0931378175107489E-3,4.4306107052465731E-2]
[null,1577,1.01391017360338,1.0213486232406734,0.98495244074457355,1.0413510052722363,1.0068229701398679,1.0332899801870286,0.9836125020391363,null,6.7399249967273409,0,1.0665194741787027E-2,0.19445400983069772,0.1195719064308584,8.2187815097284025E-2,0,1.0665194741787027E-2,0.26471226971199319,5.9152075254134822,0,1.9080300967996875E-2,0.10311718423929024,-2.3233885770427565E-3,4.3917373612781828E-2]
[null,1578,1.0372503923278629,1.0064562811341977,1.0053485325544063,0.98670937079878673,1.0029113648629979,1.0200078449422758,1.0169129992122898,null,6.7294762623897908,0,1.0173325601092272E-2,0.19117830454787396,0.11720336911959826,8.3436991638927191E-2,0,1.0173325601092272E-2,0.26648460394638496,5.9111133367909172,0,1.8959311414502421E-2,0.10035635317482364,-1.1479522840837765E-3,4.1891944040844162E-2]
[null,1579,1.0406791325499833,1.0191497046489981,0.96907069297294635,1.0141153123595106,1.0171300063760313,1.0087182771829222,1.0374854541631557,null,6.7243347892250265,0,1.0294607719224949E-2,0.18332520535220287,0.11687731311544217,8.1243360158658504E-2,0,1.0294607719224949E-2,0.26973443934748986,5.9146076001230536,0,1.894199491243545E-2,9.7992790468183169E-2,-7.7927646834470771E-4,4.2391362215902249E-2]
[null,1580,1.0199786374267827,0.95699564696898753,0.97941478442749286,1.0351020263821371,0.98486262947914294,1.0060258704675171,1.0196648999410425,null,6.7465102061595532,0,1.0665277445272823E-2,0.19286465231935401,0.12209797149623262,8.1920132365051787E-2,0,1.0665277445272823E-2,0.27091385857864142,5.9151756045861017,0,1.9048310967153217E-2,0.10255808450870831,-1.9861228327093488E-3,4.3917714171015657E-2]
[null,1581,1.0069068209925054,0.99994389917431048,1.0364757572158119,1.0230971676710563,1.0035927133312497,1.0243048690666507,0.99994166578681187,null,6.7536194637127327,0,1.0269623059667405E-2,0.20208144133300754,0.12046420593715311,8.5445650165169168E-2,0,1.0269623059667405E-2,0.2704590733046624,5.911293855729217,0,1.911769852824111E-2,0.10446626417046015,-1.9972052901273706E-3,4.2288479834947906E-2]
[null,1582,1.0039700387622832,1.0077435474242067,1.0256629780970954,1.0426280809399384,1.0201635712688444,1.0061465027334584,1.0266257951555395,null,6.754430979295047,0,1.017948656083043E-2,0.19713186959934911,0.12064582612513268,8.4876466603280118E-2,0,1.017948656083043E-2,0.2766380759984659,5.9129752866333778,0,1.9133536069138018E-2,0.10244935524951802,-1.3367507596517443E-3,4.1917313776435934E-2]
[null,1583,1.0012564427426858,0.99409675151859267,1.0027048330059178,1.0022734229655574,1.0142031005908883,1.0176049808747099,0.96102557685963985,null,6.7411599524756642,0,1.0594459200863153E-2,0.19831428892213793,0.12206796882882616,8.3210550910845976E-2,0,1.0594459200863153E-2,0.26079833726088053,5.9121035584954349,0,1.9148252590271683E-2,0.1042388334322619,-2.3479352107068836E-3,4.3626097245714257E-2]
[null,1584,1.0093580731470828,1.0252319032764232,1.0466661510196369,1.0048868982495218,0.99968457517886911,0.99586859267660255,1.0138892745571382,null,6.7396152929327728,0,9.7666228202063117E-3,0.19509795068510255,0.11878615788598594,8.606317133307205E-2,0,9.7666228202063117E-3,0.27065126510033433,5.9097143373193965,0,1.9104549929093179E-2,0.10035555426358488,-3.7490796335170375E-4,4.0217214379552182E-2]
[null,1585,0.97577831308266927,0.99073952087075801,1.0117299923200775,0.97103095612180834,0.95898268245543417,1.0012047048789174,1.0153109072269135,null,6.7681103861884564,0,1.0627212605789573E-2,0.20160358994893324,0.12525026668662428,8.4023821370689061E-2,0,1.0627212605789573E-2,0.28116383776475362,5.9099046114049081,0,1.9290419033825997E-2,0.10549525649324623,-2.3823864518357583E-3,4.3760969937312502E-2]
[null,1586,0.96551178003024885,0.97554326354006438,0.97996319895763284,0.97629285485795447,1.006534077007603,0.99380271792008879,0.99093257418368419,null,6.7663730685877699,0,1.1033510725622373E-2,0.19968598447251376,0.12798857403786501,8.1992974441525993E-2,0,1.1033510725622373E-2,0.27671788822057536,5.9119661733548483,0,1.9349826511325417E-2,0.10615625157498564,-2.9186373022842154E-3,4.543403327641455E-2]
[null,1587,1.0192411973007298,0.99436510945996726,1.0325567820595083,1.0379442771173482,0.98424394134238447,1.0057226104915558,1.0110140045789127,null,6.7421651736607684,0,1.0019566686982926E-2,0.19602245872726479,0.11934641523690676,8.5186223773519879E-2,0,1.0019566686982926E-2,0.26845721262576339,5.9123235723219194,0,1.9052178061436779E-2,0.1015287175526037,-1.0103968392534341E-3,4.1258792200608352E-2]
[null,1588,0.97400656769375282,0.9865364470600686,0.99968213828351904,0.99558020195793195,0.97004734408784132,0.9819637619806334,1.0122598819181678,null,6.761769983101428,0,1.057172837721825E-2,0.19700469792836756,0.12592535540536576,8.3263629255920818E-2,0,1.057172837721825E-2,0.27895710809639018,5.9119119166453205,0,1.9300581855502884E-2,0.10370596838958658,-1.8317702349105532E-3,4.3532495759880316E-2]
[null,1589,0.99258095592826179,1.0302687462072195,1.0121670428250078,0.98231760564394743,1.0099253592592055,0.99492457864294226,1.0124503464482897,null,6.7455041083031189,0,1.0205425435721519E-2,0.19372735789965742,0.12120989624898597,8.3969687575869534E-2,0,1.0205425435721519E-2,0.27463950922267322,5.9104896148486095,0,1.9195841815352832E-2,0.10135188262502702,-1.103807379352361E-3,4.2024125446289827E-2]
[null,1590,1.0059057226872832,1.0006895965605864,1.0071637623663441,0.97638317804103003,0.99534251871439394,1.0193077851558099,1.0024122026679776,null,6.7476437894455836,0,1.0492299902132157E-2,0.19770321572399829,0.12109969529494526,8.3603255694518014E-2,0,1.0492299902132157E-2,0.27086883902881809,5.9104527213670215,0,1.9123086883301228E-2,0.10368823449007089,-2.1006824743110795E-3,4.3205423437217325E-2]
[null,1591,1.0017752633266008,1.0084225243549985,1.0051511961162023,0.9611702199274037,1.0054694515348217,1.0117883960899781,1.0020276834207269,null,6.745008070580548,0,1.0441776451310759E-2,0.1961657286053253,0.12126279113354571,8.3470657338260201E-2,0,1.0441776451310759E-2,0.27108923459283302,5.9097443903640752,0,1.914543272985025E-2,0.10298450182465342,-1.8520428675769291E-3,4.2997376859573812E-2]
[null,1592,0.99733445670580789,1.0096058110405277,0.96499743322259246,1.0040043963426519,0.99508004766305436,1.0109707641960193,1.0135507906490058,null,6.7495384545889987,0,1.0847845189941998E-2,0.19201214936445601,0.1224917155392275,8.1057143318275751E-2,0,1.0847845189941998E-2,0.27526720436647811,5.9142823077516056,0,1.9169664033261327E-2,0.10284687854522383,-2.258103977243929E-3,4.4669495647716169E-2]
[null,1593,0.98451412746597866,1.0008299608501259,1.0334129363701339,1.0294042000381669,0.99841855526055345,0.98281223318349364,1.0117301387945361,null,6.7563128844579641,0,1.0101008996579749E-2,0.19786599187918419,0.12321974914512417,8.5336737982968064E-2,0,1.0101008996579749E-2,0.27583727293371113,5.9118125920026632,0,1.9240844764191557E-2,0.10244058159733982,-1.0350429825532704E-3,4.1594157135337359E-2]
[null,1594,1.0016017694011323,0.98945686012414691,0.97540137616811884,0.9795656666031054,1.0196093645717363,0.95556675415204617,1.0167160952540581,null,6.728812538031077,0,1.0205339615089234E-2,0.18345155213049558,0.12276471863531244,8.1617938503956683E-2,0,1.0205339615089234E-2,0.26985790760860978,5.9123937006313447,0,1.9146375367816874E-2,9.7748998386035943E-2,-1.9242528469878628E-4,4.2023772052201584E-2]
[null,1595,0.976893408487017,0.98918833232273895,0.98868996586777125,1.0163771005865425,1.0102093693902288,1.0445314335130531,0.99794686801241972,null,6.7806812230357876,0,1.1307192521858191E-2,0.20730509242665812,0.12562966661173475,8.2610849184011903E-2,0,1.1307192521858191E-2,0.2802073279207159,5.9136501933155339,0,1.9284041691555075E-2,0.10972703154969381,-4.2939858638824128E-3,4.6561006199769883E-2]
[null,1596,0.99378618184935286,1.0395191943293158,0.97845171255218943,0.97954642411454407,0.97375439066892933,1.0337338545349615,1.007107749265963,null,6.7535196043959189,0,1.0865421832903073E-2,0.19620337095598361,0.12125535347903711,8.1894293967188059E-2,0,1.0865421832903073E-2,0.27636578691992686,5.912225222718126,0,1.918918087396107E-2,0.10438383379967256,-2.7393114528830344E-3,4.4741873134904055E-2]
[null,1597,1.0375513616007428,0.99720288335249674,1.014622306175389,1.0380031815100998,0.9837347392595599,1.0262124302208064,1.0302012369940237,null,6.7406002596088328,0,1.018982178847946E-2,0.19413533026468202,0.11743458661893208,8.4104443455187083E-2,0,1.018982178847946E-2,0.27058473108485337,5.913358551485719,0,1.8957786817759576E-2,0.10144222563069265,-1.3772681532878701E-3,4.195987240429272E-2]
[null,1598,1.0128575882128652,1.0147562865346975,1.014854560564969,1.003499382670916,1.0168272792710833,0.96988973699997738,1.0079880729583361,null,6.7244549192710918,0,9.7899279250746596E-3,0.18658071545394153,0.11945664366570447,8.4030045892441646E-2,0,9.7899279250746596E-3,0.26576482343899793,5.911481062178007,0,1.9085888699272895E-2,9.748350842425571E-2,2.5905086521878532E-4,4.031318065324601E-2]
[null,1599,0.9888556102100603,1.0051494761810178,0.9875658350201405,0.98778390288742868,0.95901980095604189,1.0106237124036157,1.0357067034312457,null,6.7637542131855213,0,1.0744473644139673E-2,0.19666017769805202,0.12333895568875944,8.2566438392157715E-2,0,1.0744473644139673E-2,0.2837502563089408,5.9121670828562465,0,1.9216533402428529E-2,0.10415106727081905,-2.3401284534344674E-3,4.4243830021551446E-2]
[null,1600,1.0044344396965812,1.0002109193629125,0.98838445974907119,1.0257876679834828,1.0140026848920642,1.0112650880906702,0.99806828522222668,null,6.745429889582315,0,1.059931740138588E-2,0.194238963505384,0.12165024281277692,8.2451806284391374E-2,0,1.059931740138588E-2,0.26930969815998662,5.9141758377591866,0,1.9131025473452787E-2,0.10282677480783052,-2.0005616714294299E-3,4.3646102450739382E-2]
[null,1601,1.0056683569813418,1.0378446244415902,1.0044622411881068,1.005714299832853,0.97016287298372983,1.0136316338431752,1.0216146147330645,null,6.745263618983393,0,1.029904305432033E-2,0.19328693656709395,0.11942445185952376,8.3515247288253061E-2,0,1.029904305432033E-2,0.27520241288634761,5.9121903816522812,0,1.912436606415353E-2,0.10150783046589958,-1.3976339365266769E-3,4.24096261363648E-2]
[null,1602,0.97303431416859443,0.97934960879867039,1.0246870313438563,1.0264371001118631,0.98387174829917234,0.99754514492559965,0.97775909459515165,null,6.7646064535582768,0,1.0550639333584562E-2,0.20402481374372791,0.12593195895457382,8.473392056513826E-2,0,1.0550639333584562E-2,0.2713226741676647,5.9121568602914856,0,1.9306174478267654E-2,0.10608249437220973,-2.3980978466985178E-3,4.3445654831906627E-2]
[null,1603,0.95577699300734309,1.0250388904522949,0.99925427067896977,0.99433027712362421,1.0031764070217613,1.0186622215828207,1.0399843434171272,null,6.7911759818679176,0,1.0998365726131625E-2,0.204825226235376,0.12638517769749336,8.345781640123999E-2,0,1.0998365726131625E-2,0.29540685916900394,5.9118683981861189,0,1.9407335846414228E-2,0.10784572055002621,-3.3098646418441863E-3,4.5289312424088353E-2]
[null,1604,0.97326159188260297,1.016486797886514,1.0042972638177068,1.0262608511022562,0.98148266758176528,0.9662174260515326,0.98257867427976964,null,6.7439809237101453,0,1.0236311036797738E-2,0.19206268285835235,0.1244347667310242,8.3441994130883795E-2,0,1.0236311036797738E-2,0.2692255431340389,5.9133100094514903,0,1.9304866124610992E-2,0.10087314314959543,-8.2338872394239039E-4,4.2151306854089646E-2]
[null,1605,0.97608389363203119,0.97097598673744456,1.0213708051350334,0.97577644438171596,1.0090573155233806,1.0187407196746983,1.0078704329783441,null,6.7781948373957412,0,1.0812123198455821E-2,0.20805836174498493,0.12603557314382863,8.4622745867038107E-2,0,1.0812123198455821E-2,0.28098215587302056,5.9096106014032408,0,1.9288669938657285E-2,0.10835637627812407,-3.2820456982080117E-3,4.452239884505356E-2]
[null,1606,0.99669335598648678,0.98883570972093771,1.0243497075992658,0.99131460699926643,0.97820880538844912,0.9604434593383997,0.98419378403428526,null,6.7303890547787963,0,9.8791308832435476E-3,0.19094412991357557,0.12247595883398761,8.4572582826883097E-2,0,9.8791308832435476E-3,0.26305556921759199,5.9102788971298494,0,1.9173180041777163E-2,9.9297673981963694E-2,-8.9439724286773497E-5,4.0680502557450822E-2]
[null,1607,1.0429703998342013,1.0218995875676118,0.98001564577321976,1.0277387899887744,0.99148268938026496,0.99398581847359313,1.0246230837213934,null,6.7150764920754717,0,1.0014363968946477E-2,0.18125543095860094,0.1163023938927914,8.1865432020709672E-2,0,1.0014363968946477E-2,0.26444604666455312,5.9147444440952697,0,1.8930486564972128E-2,9.6355745207014801E-2,-6.0855662221245301E-5,4.1237368333783546E-2]
[null,1608,1.0461722230090202,1.0126947133753572,1.0168070738486428,0.98482602229666361,1.0070543016242786,0.97050822991393582,1.0135879772501637,null,6.7036362787832777,0,9.4762743915672316E-3,0.18112552664124196,0.11571168634060675,8.4040486739356421E-2,0,9.4762743915672316E-3,0.2588072119891931,5.9103607280312254,0,1.8914489208705268E-2,9.4542186960566918E-2,1.1123516418667372E-3,3.9021611230510199E-2]
[null,1609,1.0113409787029912,1.0086976676664754,1.0068581759104072,0.99442577108748598,1.0115009059364393,1.0169648729212009,0.97462108073492915,null,6.734718460501929,0,1.0379217016693023E-2,0.19548395560218251,0.12007111635796182,8.3472863470607936E-2,0,1.0379217016693023E-2,0.2616493543244669,5.9114449720459552,0,1.9093960191351959E-2,0.10253982850780592,-1.7773582413868852E-3,4.2739768242982243E-2]
[null,1610,1.0223278176301329,0.99179537062474266,1.0016456720158433,1.0325302859507413,0.99122709337627635,1.0062745289963584,0.99101273014401514,null,6.7322893364165726,0,1.0280266374567906E-2,0.19213134745875132,0.11968239110675119,8.3186484551924386E-2,0,1.0280266374567906E-2,0.26237672622998037,5.9137983321426457,0,1.9036029192652033E-2,0.10104201686511007,-1.2962982425081431E-3,4.2332307111268723E-2]
[null,1611,0.99652490349126888,1.0069465779776774,1.0202065319229081,1.0275715302443955,1.0104502049466348,1.0360783379186038,1.0128783218917674,null,6.7667844100464141,0,1.061480927656905E-2,0.20390996189529143,0.12168908995579458,8.4544173483599758E-2,0,1.061480927656905E-2,0.27783098447353904,5.9124755958703172,0,1.9174104641523172E-2,0.10625680056835318,-2.8061960772946867E-3,4.3709895235292694E-2]
[null,1612,1.0226878188891337,0.99743883779269205,1.0382168831849108,0.99832160890537713,1.0077859928073645,1.0347654040062184,1.0202964613808763,null,6.7514379012593198,0,1.0209789006775083E-2,0.201421508046561,0.11869189876190056,8.55647551603953E-2,0,1.0209789006775083E-2,0.27272186998704967,5.9098542719485856,0,1.9034152052068067E-2,0.10403647402319922,-1.9291225756379953E-3,4.2042093855201711E-2]
[null,1613,1.012622471190868,1.0180129791093857,1.0084586060763359,1.0170638579223206,1.0112507220299793,0.96770350235950386,0.98429921095338113,null,6.717016909855305,0,9.8114727329180664E-3,0.1852293738829624,0.11944951114235765,8.3557258220612177E-2,0,9.8114727329180664E-3,0.25934383782461184,5.912577616857539,0,1.9087138423435037E-2,9.7083900425919439E-2,2.863747407566529E-4,4.0401898337112337E-2]
[null,1614,0.97199703426434281,0.97204136221235693,0.97771136180152396,1.025842351934106,0.96364891291766996,1.0010671581214157,1.0048279985559423,null,6.7716104510554063,0,1.1078764693400876E-2,0.19983616903944654,0.12736108789804335,8.1923653167887689E-2,0,1.1078764693400876E-2,0.27947742195487052,5.914768751574349,0,1.9312153483167949E-2,0.10635599966960026,-3.045166792778259E-3,4.5620381060820427E-2]
[null,1615,0.97463360663745835,1.0049994395776396,0.99495587394441809,1.0168117176525286,1.0028700970205349,1.0190651146011034,1.0257654061929353,null,6.7773748912066649,0,1.0922344402363914E-2,0.20211799170605965,0.12500500368664788,8.3078598022248706E-2,0,1.0922344402363914E-2,0.28597813341550948,5.9133243074225943,0,1.929698090387174E-2,0.1066479829565927,-3.0503770509677499E-3,4.4976270144104144E-2]
[null,1616,0.99755016312450262,0.99962775346988797,1.0053208482179978,0.97136769526248434,0.9872032938529367,0.97804552925734067,0.97484711849317462,null,6.7294387233126374,0,1.0172884087639899E-2,0.19116217021953485,0.12220063377194283,8.3364378919678406E-2,0,1.0172884087639899E-2,0.26183295034103909,5.9102858649647914,0,1.9168482043970318E-2,0.10034926037330505,-8.1514328865901872E-4,4.1890125967033745E-2]
[null,1617,1.0121411161715224,1.00142392869045,1.0019021172220799,0.99865696383815306,1.000850430537138,0.9905033590314789,0.99896830020791039,null,6.7316234912823232,0,1.0176495456369707E-2,0.19026419968001373,0.12041591278306721,8.3221559714808768E-2,0,1.0176495456369707E-2,0.2655801365290571,5.9119533374908553,0,1.908969879454174E-2,0.10004734893121442,-8.5369958190122672E-4,4.1904996940663436E-2]
[null,1618,1.009896812102197,0.99910655303254248,0.98058135027885407,1.0216422613836977,0.9932381149246412,1.035072963851313,1.0155314272603619,null,6.7549802730331159,0,1.0868992682540039E-2,0.19688900250477137,0.12118948490439974,8.2035169240237238E-2,0,1.0868992682540039E-2,0.27479515427123669,5.9143836866222621,0,1.9101668671028367E-2,0.10463694333249528,-2.8074137714362572E-3,4.4756577258121544E-2]
[null,1619,1.0056513025352858,0.9925610679058795,1.0399820852752311,0.97338617842166841,0.96714331429655331,0.9827052043221528,1.0021706617633015,null,6.7375789050337831,0,9.8658237258618109E-3,0.19514385382578875,0.12090595589882788,8.5585247019301341E-2,0,9.8658237258618109E-3,0.26756704169667705,5.9084045573098312,0,1.9124457995041023E-2,0.10070707011453055,-4.8498487815318471E-4,4.0625706051938548E-2]
[null,1620,1.0261863305575498,0.9850679329685641,0.99586326921047941,0.97810207962625739,0.96453581600136618,0.99047793041464494,0.97457681882795821,null,6.7169265479286668,0,1.0161474178488278E-2,0.1882911212809717,0.11966359648266049,8.2698960884118974E-2,0,1.0161474178488278E-2,0.25569063891009575,5.911181420936634,0,1.9015978489969519E-2,9.930735940348781E-2,-7.6567045130552386E-4,4.1843141992035503E-2]
[null,1621,1.00236929639543,1.0156247089732202,0.99010969260539405,1.0125077787560219,0.97448931582503495,1.0087555100395322,1.0157843483779829,null,6.7472789933640014,0,1.0509813146126316E-2,0.19309202964087763,0.1211255703786575,8.2615566461353054E-2,0,1.0509813146126316E-2,0.27426072829272363,5.9133620826245528,0,1.9142207663868746E-2,0.10213167716866683,-1.7284087254415563E-3,4.3277539858744038E-2]
[null,1622,0.9805403294537105,0.99376946807331301,1.0425241899170243,0.98844788257778093,1.0132142465897194,0.99512976911990558,0.97466878465668438,null,6.7538408313541751,0,1.021825349747482E-2,0.20287512660393073,0.1238922942232959,8.5761756665967928E-2,0,1.021825349747482E-2,0.26804905356627534,5.909069431021539,0,1.9263285878393446E-2,0.10456702476769246,-1.7140904942054569E-3,4.2076949121280051E-2]
[null,1623,1.0199149789396111,1.022212988928856,1.0352068797992831,1.0198369804681244,1.010688953789928,1.0123548697396216,1.0163331331906535,null,6.739749771039877,0,9.9373623848633911E-3,0.1951770824901477,0.11790808605228187,8.5358130082053799E-2,0,9.9373623848633911E-3,0.27003730188368646,5.9111915964200445,0,1.9048644568126105E-2,0.10095972455879292,-8.5108453156164691E-4,4.0920289516300425E-2]
[null,1624,0.99334292131086943,1.0172988002921859,1.0085426730521658,1.0172856034936242,1.0019717445471201,0.99490670312170015,0.98464956570047413,null,6.7412731552236798,0,1.0285398880474094E-2,0.1942007267862435,0.121800482956765,8.3667281607593597E-2,0,1.0285398880474094E-2,0.2670007923021287,5.9125848336522555,0,1.9191628769921476E-2,0.10178180284167031,-1.3078355499427331E-3,4.2353441857038432E-2]
[null,1625,1.0006483194252165,1.0076718566177381,0.99635437248360692,1.0183231819634579,1.0226620538560207,1.0112039999549236,1.0021757495347265,null,6.7481126791034773,0,1.0531456583134154E-2,0.1952889327575951,0.12159982174462064,8.296972473166675E-2,0,1.0531456583134154E-2,0.27137210292235703,5.9133277186938633,0,1.9151561545591965E-2,0.10297294464332953,-1.9367916155041429E-3,4.3366663679954141E-2]
[null,1626,0.99457881075990273,1.0043737059972937,0.99493486667245934,1.0263935201072536,1.0218030026496989,1.0063083024299404,1.0195657613824942,null,6.756288999855335,0,1.0572336207915785E-2,0.1956349988889865,0.12252907877295389,8.2967215804104794E-2,0,1.0572336207915785E-2,0.27732574613723715,5.913843350332046,0,1.9184809038649213E-2,0.10322829737012904,-1.9594951872764269E-3,4.3534998698502934E-2]
[null,1627,1.0246902109629721,0.99630514631706246,1.0268208454096259,0.97941613218981605,1.0295649166558807,0.9558372609819743,0.99419142485255274,null,6.7103805286030145,0,9.5117303950446076E-3,0.1845159973494831,0.11872577209062395,8.4645091749835838E-2,0,9.5117303950446076E-3,0.2579866572417524,5.9094938030703492,0,1.9023735128250816E-2,9.5838352876729108E-2,9.8350635409341657E-4,3.9167612741896667E-2]
[null,1628,0.98940479136403092,0.99639301881950315,1.0127402784879156,1.0279964622246387,0.98450922943150943,1.0043179739464498,1.0009281340536229,null,6.7573386796615935,0,1.0478578472797014E-2,0.19908140227032295,0.12322516531646276,8.4024795756743778E-2,0,1.0478578472797014E-2,0.27360369143042385,5.9129251238918075,0,1.9213473308372489E-2,0.10412344885375506,-2.0073421998357275E-3,4.3148921033538568E-2]
[null,1629,1.0356393785371056,1.0029223059308767,1.0077379327821181,1.0005891473759629,1.0357176591271138,1.0379808666067112,0.99069558719719975,null,6.7320564796915709,0,1.0362651111888891E-2,0.19542635482424847,0.11750764513390437,8.3530491304920115E-2,0,1.0362651111888891E-2,0.26167682241294715,5.911728223389173,0,1.8967487268661615E-2,0.10246496926761556,-1.9170667055234628E-3,4.267155279561996E-2]
[null,1630,1.0272325954299462,0.98927055841677336,1.0259100504767598,0.98563679710433294,1.0208950152344189,0.98538273052970538,1.0308833139959743,null,6.731516617479488,0,9.8190451749833717E-3,0.19022118755895528,0.11878496966822737,8.4753485866296038E-2,0,9.8190451749833717E-3,0.26971263755323771,5.9098823395710909,0,1.9010567550589396E-2,9.8845874011912221E-2,-1.2752460651649993E-4,4.0433080305692794E-2]
[null,1631,0.99394134824793567,1.0051362646067985,0.96978751466941515,1.0097391679967143,0.99786862547751254,1.0143638601662477,0.99136645953471603,null,6.7487792532544306,0,1.0896651098241696E-2,0.19425297220657803,0.12303952292834114,8.1298669446329283E-2,0,1.0896651098241696E-2,0.27053320240340251,5.9143319225288762,0,1.9188324487072181E-2,0.10379658505337515,-2.5324154905155445E-3,4.4870469690966502E-2]
[null,1632,1.0237585558465814,0.99706587038350503,0.96599654219004405,0.98952885258619594,0.99584184234771789,1.0078517003610763,1.015505663415164,null,6.7319790014182388,0,1.0582585672128841E-2,0.18759510262525239,0.11991016813144122,8.1019429734487974E-2,0,1.0582585672128841E-2,0.26851773695934184,5.9134453691917468,0,1.9028576752513123E-2,0.10043043610207708,-1.5450222464229737E-3,4.3577204167795681E-2]
[null,1633,1.0462136163523013,1.0210664838532262,1.0286548329336025,0.99410942909913125,1.0016836483363023,1.0380410042159065,1.0048967187898059,null,6.7269401185325464,0,9.9953809645085458E-3,0.19442468824483364,0.1151139775789248,8.4830602864363322E-2,0,9.9953809645085458E-3,0.26259238956625308,5.9101816719306859,0,1.8914283035134174E-2,0.10089406475709356,-1.1707591450990623E-3,4.1159199700356981E-2]
[null,1634,1.0259945591357618,0.99397806416846446,1.0203389812331936,1.0219004921433266,0.98956271174788135,0.99487173257957395,0.98171359065223629,null,6.7235465396723217,0,9.9538399536957152E-3,0.19125024126237211,0.11880580107309541,8.4275809045664229E-2,0,9.9538399536957152E-3,0.25796341449491433,5.9121616214004966,0,1.901697146572779E-2,9.9653361164496024E-2,-5.6882144629574435E-4,4.0988141211854026E-2]
[null,1635,1.0213758643947397,1.0457751858772812,0.9852683923014387,0.96916778545314064,1.0376922106469539,1.0137678681717568,0.98063515803913992,null,6.7181856614747533,0,1.0279887422798378E-2,0.18751671202126116,0.11757539028293812,8.2093055548374289E-2,0,1.0279887422798378E-2,0.26001205781571451,5.9112881334967859,0,1.9040999301338846E-2,9.9422701519679232E-2,-1.0941351666698704E-3,4.2330746655332707E-2]
[null,1636,0.97258679458290231,0.9997027578386195,0.9953380352144886,1.0010572804046045,1.0292261504981479,1.0112290520491358,1.0037662005991062,null,6.7697121322310592,0,1.0882143348625641E-2,0.20148815539864912,0.12552579070973088,8.3007804950090844E-2,0,1.0882143348625641E-2,0.2797304974849939,5.9124514528070478,0,1.9308752470256201E-2,0.10629543228182001,-2.9064832318649041E-3,4.4810729360330738E-2]
[null,1637,0.99764918124277835,0.99883334610653707,0.98495545938216356,0.9827430361331787,0.98929014080346489,1.0040065789602481,1.0048652441447152,null,6.7468536931124534,0,1.0632822821590258E-2,0.19386465416465551,0.12260917754914739,8.2247853099300036E-2,0,1.0632822821590258E-2,0.27230698149212945,5.912039270095927,0,1.9167939633436184E-2,0.10280449924506145,-1.9707539746012075E-3,4.3784071807398524E-2]
[null,1638,1.0372231778376149,1.0185578709546068,0.99993360055741232,1.0029792824196921,1.0250282056359179,1.0044983880992882,0.99771873843522063,null,6.7166839296722189,0,1.0015041257684298E-2,0.18670034580729875,0.11674466574242573,8.3025226370540856E-2,0,1.0015041257684298E-2,0.25993673553952673,5.9122976548682944,0,1.8959449316457783E-2,9.8269342386378369E-2,-4.8964764695634739E-4,4.124015728825299E-2]
[null,1639,1.0165420195876202,0.99797230560304118,1.0022444282777354,0.96805546246240948,0.99118020513057281,0.97132143153191464,1.0114408088987463,null,6.7234397091051425,0,9.9479444998360495E-3,0.18608544190119791,0.12005397300655295,8.3225476428600079E-2,0,9.9479444998360495E-3,0.26596484580212426,5.9102803322476225,0,1.9066380248077532E-2,9.7833397486257814E-2,-3.4002797503419468E-5,4.0963864782211597E-2]
[null,1640,1.0007868201656671,1.017654102019945,0.9636967564890847,1.0125929917763485,1.0192497922551707,1.0194659530117407,1.0194089172881597,null,6.7508510761165814,0,1.0876574638785701E-2,0.19214907780853094,0.12170583975669573,8.0999396491580569E-2,0,1.0876574638785701E-2,0.27662871436417158,5.9148172251338176,0,1.9150807573816465E-2,0.10298770159857876,-2.3754850150167189E-3,4.4787798404403271E-2]
[null,1641,0.99981676066937231,0.9631237200297903,1.0220958346606155,0.99232993287572702,1.0216316139708841,0.98325883473141462,0.98485379385436522,null,6.7423864824968893,0,1.021688601670822E-2,0.19681512521093314,0.12343019207083258,8.4457528418700564E-2,0,1.021688601670822E-2,0.26479403520305955,5.9104632838206772,0,1.9156092785937523E-2,0.10246434607942639,-1.2654391715630872E-3,4.2071318078885707E-2]
[null,1642,1.0125216598303084,0.96322217027691681,0.99201421185835137,0.96184944691025287,1.0322130863718935,0.99231467239307292,1.0008578413676295,null,6.7370395357689636,0,1.0452456888193852E-2,0.19258121208383017,0.12244347683259074,8.2593931511931284E-2,0,1.0452456888193852E-2,0.26652585865704509,5.9105179182580345,0,1.9087674446692945E-2,0.10176483953080225,-1.5167325495717189E-3,4.3041356997611489E-2]
[null,1643,1.0428866965351147,0.99993089147999581,1.0126446080163245,1.032950798191709,1.0207700263710666,0.98653314523237157,1.0316709024164008,null,6.7211776178306497,0,9.7511690750751619E-3,0.18523519685908635,0.11674196545211241,8.3913788202608336E-2,0,9.7511690750751619E-3,0.26585046872277196,5.9131982620402415,0,1.8930906091575737E-2,9.6886193340653987E-2,2.6725851383440366E-4,4.0153578607766194E-2]
[null,1644,0.98100539579895041,0.97645515872582278,1.0348632021945152,0.97389315401676602,0.99164774592941163,0.9896768844622974,0.95666851568666789,null,6.7481904596123927,0,1.0303252953140154E-2,0.20226070052911485,0.12485767520088453,8.5203887397271222E-2,0,1.0303252953140154E-2,0.26262969495124744,5.9087300157922966,0,1.9260650129112229E-2,0.10464149012453015,-1.8206162624342611E-3,4.2426961750370792E-2]
[null,1645,1.0109049314215153,1.0052443768115438,0.99041186377788759,0.98862050065088658,0.98899343759342118,0.97516307575122207,0.99457311754719102,null,6.7230242882319891,0,1.0115782371416413E-2,0.18593595866460186,0.1205918297402622,8.2470302116085178E-2,0,1.0115782371416413E-2,0.26326047170303851,5.9120541325048661,0,1.9096285345254507E-2,9.8331818247993308E-2,-3.7150135346733222E-4,4.1654991263352044E-2]
[null,1646,1.0182970124118436,1.0266340975336217,1.0226626951851971,0.9890354663469858,1.0186738776206905,0.99264917055536672,0.98194068005922652,null,6.7203395525452043,0,9.8490764916972246E-3,0.18988888612659172,0.11812329109315521,8.4416384140064582E-2,0,9.8490764916972246E-3,0.25948038232917248,5.910252752732772,0,1.9057137490098474E-2,9.8830888075493464E-2,-2.6691336468587804E-4,4.0556743922545345E-2]
[null,1647,0.98928768049152016,0.95272589825572984,1.0084847076618038,0.95842927645235709,1.0038372650918206,0.97241970660577504,0.99693412789074543,null,6.7478643624018462,0,1.0382384639893166E-2,0.19601511196823643,0.12555145144237151,8.3660727701213286E-2,0,1.0382384639893166E-2,0.26993464031888931,5.9094077924256379,0,1.9214125577235813E-2,0.10273568054486219,-1.4079795281121967E-3,4.2752811951504502E-2]
[null,1648,0.9555691718428474,1.0291154312899289,0.99104961971430139,1.0044012766603785,0.99763181825683656,1.0350855700779102,1.0121302261749237,null,6.7890119499137853,0,1.1239374882642837E-2,0.20678388026681715,0.12637081635246014,8.2869509297858593E-2,0,1.1239374882642837E-2,0.28911989822513912,5.9128715829776075,0,1.9408576347396591E-2,0.10932243247703446,-4.0164912631049932E-3,4.6281745232570864E-2]
[null,1649,1.0089759932938422,0.98095759845327901,1.0023777580484465,1.0382024966897281,0.97201790349761774,0.99387652359217293,1.0041399903156905,null,6.7426758563904672,0,1.0329915847426336E-2,0.19326873212439158,0.12178658031042744,8.3316637199199586E-2,0,1.0329915847426336E-2,0.26831507969988483,5.9140636172386074,0,1.9106595215279455E-2,0.10160325116760958,-1.3213913681559592E-3,4.2536754803223012E-2]
[null,1650,0.98626875552513182,0.96491368451143811,0.99328720188015529,1.0037507603282194,0.9808633658268241,0.97458035131767429,1.0044782580467391,null,6.7516929196496003,0,1.0519286272995228E-2,0.19417856709159792,0.12559008900608007,8.2789534422047284E-2,0,1.0519286272995228E-2,0.27286446330629482,5.9127116398058153,0,1.923099345650869E-2,0.10254387793111269,-1.5327938788969324E-3,4.3316548509036497E-2]
[null,1651,1.0279318758629377,0.99411953968047539,0.96488648938309041,1.0397648765819991,0.96607822821641687,1.0001256074490297,0.96987033537509781,null,6.7171782404461355,0,1.0482214297754922E-2,0.18550973177183328,0.11958473311918043,8.0805684942516789E-2,0,1.0482214297754922E-2,0.25474838809363803,5.9162219961975717,0,1.900695724227227E-2,9.9369562540489967E-2,-1.2327061749274175E-3,4.3163892713562531E-2]
[null,1652,1.0213704894237994,0.98852354506712625,1.0029059385202124,1.0204176237022913,1.0113546962267495,1.0003038610783217,1.0061065897716726,null,6.7347537220424005,0,1.0232066418953743E-2,0.19158783468349963,0.11992975622825788,8.330593230250416E-2,0,1.0232066418953743E-2,0.26610182855169345,5.9130727410491071,0,1.9041027390143982E-2,0.10069319901896287,-1.1124254550932162E-3,4.2133828273321891E-2]
[null,1653,0.98011812991933212,1.007328935587225,1.0177713036729807,1.0368752946285289,0.99860597322464484,1.0271203552897188,1.0027611173495097,null,6.7727431112462027,0,1.072027332238035E-2,0.20519533502360696,0.12375417117119165,8.4414288933842188E-2,0,1.072027332238035E-2,0.27879010398504761,5.9131177230804681,0,1.9265680847454648E-2,0.10705500090783872,-2.9933701072925897E-3,4.414417740404325E-2]
[null,1654,1.00158515269356,1.0088240532871096,1.0143581230946577,1.0002237419933473,1.0007509443491305,1.0347013253816468,0.98882582266633279,null,6.7534476429001922,0,1.0592816098373781E-2,0.20173424621401845,0.12109404135845446,8.4051100864768816E-2,0,1.0592816098373781E-2,0.2697046311543852,5.9113323797025652,0,1.9146465667880613E-2,0.10542666393421705,-2.6612172382218082E-3,4.3619331242124353E-2]
[null,1655,1.0018950863114962,0.9810785145138704,1.0041026462904619,1.0051483662043728,1.0057048968330979,0.97181978186979967,0.96517751457248224,null,6.7265841518121725,0,1.0156196658901192E-2,0.19050458879760612,0.12260870178069161,8.3257676897274133E-2,0,1.0156196658901192E-2,0.25770882264057204,5.9121800952213661,0,1.9144781890766693E-2,0.10006447191540264,-7.0639743724249275E-4,4.1821410105739337E-2]
[null,1656,0.99883942632104883,1.0135128015975317,1.0422330555745061,1.0105023972787892,0.97759683400084652,0.9694232165386707,0.97673734381586008,null,6.7284635278060074,0,9.6924205029585153E-3,0.1923524177323214,0.12067479782305929,8.5663504194587473E-2,0,9.6924205029585153E-3,0.26115259174997107,5.910277557550434,0,1.9161428015536931E-2,9.9157441648732469E-2,1.121266467166777E-4,3.9911662444645869E-2]
[null,1657,1.0108208346325509,1.0272433792530249,0.97919574843847101,1.0050056555876421,1.0056057079540053,1.0218265905823178,1.0349143041912257,null,6.7480825145723662,0,1.0606185938051054E-2,0.19173375317036648,0.11976623286752078,8.1981817393003489E-2,0,1.0606185938051054E-2,0.27820316454071758,5.9135606416798243,0,1.909673400897632E-2,0.10196790110469715,-1.9021160549194506E-3,4.3674385862172614E-2]
[null,1658,0.99099484706909657,1.0154479484252183,0.96993769408880059,1.0066113062898772,1.0140281027252616,1.0426333791600093,0.99525498114676014,null,6.7610163291757965,0,1.11831873605431E-2,0.19940547100918604,0.12289977333297673,8.1363930323865283E-2,0,1.11831873605431E-2,0.2749547077976548,5.9141546161114036,0,1.9204632479688892E-2,0.10654171160133981,-3.5588884978874835E-3,4.6050375017570255E-2]
[null,1659,1.0120516650287181,1.0057385383496913,1.0038236682551014,0.99566400614917372,0.98669444825117869,0.98386716730524393,0.98017142680141778,null,6.7232168621443904,0,1.007368333982761E-2,0.1888787904406144,0.12018409020794811,8.3263106487510299E-2,0,1.007368333982761E-2,0.25996504584681046,5.9116833068798993,0,1.9090174861656831E-2,9.922422911873742E-2,-5.5351664340498976E-4,4.1481634944617637E-2]
[null,1660,1.0243086758566029,0.9508308272176822,0.99491689529956728,0.97073988623709595,0.99816205318631923,0.95597769977134583,1.0309688086049675,null,6.7257247400987943,0,9.9839482033094746E-3,0.18474229684297983,0.12160895570502882,8.2799542833462872E-2,0,9.9839482033094746E-3,0.26800904619050364,5.9108364414514591,0,1.9025716824591993E-2,9.7481552006138478E-2,1.0906661993046843E-4,4.1112121624694832E-2]
[null,1661,0.99188859513578342,1.0243163541001041,1.0226580133353436,0.98549317796112335,0.96912040799200017,0.98207668032259687,0.98123730112035112,null,6.7345017329527881,0,1.0013329492921566E-2,0.19305432536630746,0.12137802310622625,8.4493951940756318E-2,0,1.0013329492921566E-2,0.26524231308813023,5.9100616553978176,0,1.9199675617287772E-2,0.10047862603664016,-6.3994614602456187E-4,4.1233108545642834E-2]
[null,1662,1.0069881948860757,0.96970150871526184,1.0319813888826637,1.027282703231047,0.97874772662325615,1.0401927679674703,0.97321093680631587,null,6.7583783522903556,0,1.060794901980291E-2,0.20735713864320035,0.12202934071886126,8.5096327516114623E-2,0,1.060794901980291E-2,0.26500602088230801,5.9117810589598196,0,1.9117261008679286E-2,0.10742974346491499,-3.120184822556952E-3,4.3681645919009894E-2]
[null,1663,1.0179228093250514,1.0189702174478701,1.0032657103721816,1.0001103406312317,0.95528950728077178,1.0354315063893555,1.0363083261695645,null,6.7522006852300063,0,1.0486791466793823E-2,0.19646203330912576,0.11887802051245512,8.3474332583952954E-2,0,1.0486791466793823E-2,0.2780564080091415,5.9119550508282233,0,1.9059105576184818E-2,0.10323651710415614,-2.1035233741980297E-3,4.3182740680958988E-2]
[null,1664,1.0227591475733087,1.0050347838294216,0.99814553585383625,0.9848147353747897,1.0000609878559161,1.0341223597500362,1.0406084281646013,null,6.7507927060489585,0,1.0532650555248498E-2,0.19583013982785427,0.11906303758320529,8.3142738760853763E-2,0,1.0532650555248498E-2,0.27791124759410152,5.9114163623807494,0,1.9033780282533427E-2,0.10316639906309297,-2.1425796880344275E-3,4.3371580244601894E-2]
[null,1665,1.0289946271429189,0.9741325834010568,0.97959320791129634,0.97678610762939488,1.0344958976219583,0.96117600869899644,1.0087964187616432,null,6.7133498139232453,0,1.0022370040684989E-2,0.18128667627602918,0.12016871644221042,8.1762189404996549E-2,0,1.0022370040684989E-2,0.26129208021122596,5.9120132064015829,0,1.9001479769379603E-2,9.6392743631715391E-2,1.6238587392507963E-4,4.1270335912175105E-2]
[null,1666,1.0023900766924854,0.9962093989872135,1.0047641097013789,1.02333107358701,0.99357466918938742,0.99480812246792538,1.0329533394329313,null,6.7520322073657537,0,1.0317415225661764E-2,0.19371831998770683,0.12178779722542377,8.3581436309388135E-2,0,1.0317415225661764E-2,0.27776248570514633,5.9131253241361961,0,1.9142094914718234E-2,0.10171915663378997,-1.289687014445732E-3,4.2485279467824238E-2]
[null,1667,1.0094719435288229,0.99225394988663673,1.0344980888574604,1.0219565675173947,0.99542062569098644,1.0130885162512251,1.0086830156848505,null,6.7509975343084792,0,1.0182563444207022E-2,0.1997836566841748,0.12056716848360863,8.5332017474310504E-2,0,1.0182563444207022E-2,0.27115206507621281,5.9113472846184472,0,1.9103940676616114E-2,0.10337844812742038,-1.5970306668275772E-3,4.192998383451594E-2]
[null,1668,1.0347869205271842,0.99203487633169041,0.98899246143113395,0.99556299724028074,0.96754791034651455,0.98339500309054972,1.0214893956597102,null,6.7199851172149501,0,1.0034787631014013E-2,0.18405946533037135,0.11845931983509822,8.2408964567604825E-2,0,1.0034787631014013E-2,0.2650291655188608,5.9125083306535808,0,1.8971823770658675E-2,9.7408369498878697E-2,-1.8179129899997446E-4,4.1321469338901337E-2]
[null,1669,0.99997444514210776,1.0212917181671377,1.0091707646781733,0.96323253045488955,0.98078497732395564,0.99526387378681114,0.96586198641468346,null,6.7279147574376825,0,1.019813233360938E-2,0.19273216678644364,0.12079157899131102,8.3574183311967545E-2,0,1.019813233360938E-2,0.26016750635921543,5.9096284685436631,0,1.9155232969671501E-2,0.10098073126959406,-1.1092045441000989E-3,4.1994093749915841E-2]
[null,1670,0.9881731364879448,0.99264156646790014,0.97118812660955545,0.98815266916218669,1.0078057532054416,0.98069412736779649,0.9862149357412302,null,6.7394716485408264,0,1.0640397201956859E-2,0.1900796372261282,0.12435225633578208,8.1333492694744797E-2,0,1.0640397201956859E-2,0.26765626756086774,5.9130883867763133,0,1.9220340956239305E-2,0.10149513592813915,-1.5691306949506445E-3,4.3815261757558732E-2]
[null,1671,0.96098977340822822,0.97396006648481581,0.97990373167897316,0.97178470327335797,1.0038526341494352,1.01860275746786,1.0296753801367016,null,6.7913486624284465,0,1.1370567281385354E-2,0.20576792419274656,0.12867556439243974,8.2180659967517306E-2,0,1.1370567281385354E-2,0.29144095443566631,5.911725737156349,0,1.9376395859012973E-2,0.10939276495616528,-4.0333107106635064E-3,4.6821972179216076E-2]
[null,1672,1.038078761774369,1.0130620209601027,0.994262461532883,1.0311794481390979,1.0092392233336365,0.96437087874686112,0.99349531473548036,null,6.7018499548383099,0,9.677120870598124E-3,0.17889119044333451,0.11700286339193472,8.2628796758449724E-2,0,9.677120870598124E-3,0.25506432490034936,5.9141396202197951,0,1.8955117339434589E-2,9.4424895849916604E-2,8.944846532737235E-4,3.9848661281818819E-2]
[null,1673,1.00985914735009,0.96265338679467816,0.99402568529327773,1.0382025429639272,0.98692041260743468,1.014346533422869,1.0470035109152553,null,6.7648196572747787,0,1.0696614203157619E-2,0.19766815701601523,0.12275754041562598,8.297701560553862E-2,0,1.0696614203157619E-2,0.28174814373090712,5.9145324389493279,0,1.910187000791538E-2,0.10434832086482605,-2.360582677627628E-3,4.4046753362250279E-2]
[null,1674,1.0084152576549927,1.0014280609644708,0.9528535732132114,1.0004494261285579,1.0095165206709737,1.0316948204135934,1.0008818638212407,null,6.7465195861526173,0,1.1103410627782417E-2,0.1930209442178345,0.1217614473677831,8.0237140237711488E-2,0,1.1103410627782417E-2,0.27083928383039885,5.9147445151766691,0,1.9109599658212503E-2,0.1040232576429025,-2.938470610685862E-3,4.5721868631790827E-2]
[null,1675,0.99533899155282346,1.0131966577215161,0.96896432738985272,1.0105501254901623,1.0113404590141948,1.0167397220023191,1.0375572094692311,null,6.7599543421157691,0,1.0877393175032109E-2,0.19367279126363671,0.12249001801257636,8.1409370335272693E-2,0,1.0877393175032109E-2,0.28288510966053626,5.9144206270631834,0,1.9180622715845801E-2,0.10352942225225803,-2.4247881785107433E-3,4.4791168990971957E-2]
[null,1676,0.99331000023608884,0.98779337959614277,0.96879759647230446,0.99178313364157022,1.0084961687025884,0.9881996534404931,1.009048445870697,null,6.7459982399186798,0,1.0711054396997405E-2,0.19066390668654204,0.12399634129950611,8.1259179048017952E-2,0,1.0711054396997405E-2,0.27320244573704683,5.9134149862994425,0,1.9191810662942906E-2,0.10192954553522152,-1.7661908602631077E-3,4.4106215510223826E-2]
[null,1677,0.9950745011290546,0.98547569370681365,0.99486213254853229,0.97426322128747844,1.0337201205131061,1.0021179909400368,1.0044090196910893,null,6.7508577643304131,0,1.0609721853138134E-2,0.19630563683939795,0.12340347266395263,8.2865573548910082E-2,0,1.0609721853138134E-2,0.27286508995150804,5.9110299281436189,0,1.9182078541534316E-2,0.10358591408670659,-2.0688755763561529E-3,4.3688946131131799E-2]
[null,1678,1.0193290077683537,1.0147664375640941,1.0067007820916629,1.038164270661984,1.0099715266393718,1.0033210946026101,1.0105605626298926,null,6.7349266948539714,0,1.0135058390295203E-2,0.19084094772419291,0.11884756369276682,8.3577725883036816E-2,0,1.0135058390295203E-2,0.26784257020659868,5.9138173712258677,0,1.9051717294849845E-2,0.10011217266550319,-8.9774031693937184E-4,4.173436647809145E-2]
[null,1679,0.9924076639569569,1.0201125069292443,0.99127330471887498,1.0232848405227171,1.021375413927806,0.98270969557885346,0.98807839248573937,null,6.7363392838418017,0,1.0311250895885041E-2,0.18977101953942033,0.12210413777032511,8.2599715146967567E-2,0,1.0311250895885041E-2,0.26699300567794643,5.9138797809713326,0,1.9196800881220808E-2,0.10031689387019241,-9.8196587062245782E-4,4.2459895855013488E-2]
[null,1680,0.96928772165394528,1.0023708367213848,1.0103204881684216,0.99275117171861582,1.0458336033601991,0.97983235965986915,0.9891844033028474,null,6.7556543124704449,0,1.0430634041625923E-2,0.19746197061741141,0.12552904580393828,8.3850330254397934E-2,0,1.0430634041625923E-2,0.27358558201115718,5.9111582768742599,0,1.9327830647407552E-2,0.1034000576974632,-1.6102758353598434E-3,4.2951494399766657E-2]
[null,1681,1.0114936704311825,1.0098343844511837,0.98435315455225403,1.030582589546692,1.0049986673286717,1.0104722562860431,1.0059860187257743,null,6.7403973420512067,0,1.0510950590760864E-2,0.19147147758042954,0.12041333929825469,8.2204707003079788E-2,0,1.0510950590760864E-2,0.26937243648284787,5.9146586145171369,0,1.9093146460509351E-2,0.10156598893481432,-1.6645918791547535E-3,4.3282223653291534E-2]
[null,1682,0.99561817619403004,1.0082267908098126,1.029618924128527,0.9740601658521304,0.96666648225797591,0.96180761236339674,1.0138190189471079,null,6.7356559784268999,0,9.7765660746927299E-3,0.19043964322535778,0.12155936639074472,8.4997352442851878E-2,0,9.7765660746927299E-3,0.27123890099810416,5.9090429403375202,0,1.9179086848419614E-2,9.8779332321811991E-2,1.6119693039398495E-4,4.0258158931693926E-2]
[null,1683,0.99867459599177466,1.0000131601141491,0.97972299081042247,1.0079486448244559,1.0062158490256574,1.0079108909221031,1.006083129026504,null,6.7486886488839302,0,1.0706553423121146E-2,0.19369962045971201,0.12252280104525072,8.1945154366907247E-2,0,1.0706553423121146E-2,0.27270663675616497,5.9136907120898075,0,1.9162328846879365E-2,0.10298619173790677,-2.112477719645396E-3,4.4087681300944884E-2]
[null,1684,0.97864901761372824,0.99300252902385666,0.97860282473233717,0.99352775089203405,1.0293335623011746,0.99993969753293077,1.0166009130360836,null,6.7635472699268506,0,1.0882564140868321E-2,0.19655698813887357,0.12540355285910515,8.1969109557751677E-2,0,1.0882564140868321E-2,0.28048752700565821,5.9129727594598789,0,1.9274030639325767E-2,0.10456404797022878,-2.4932078118558233E-3,4.481246210788787E-2]
[null,1685,0.98177814242567274,1.0039739798027807,1.0110143844423691,1.0257584404555637,0.9890454992241281,0.98875337914817685,1.0021211352187596,null,6.7552314987104003,0,1.0378282164605273E-2,0.19667281426893321,0.12383954797863603,8.392854990448069E-2,0,1.0378282164605273E-2,0.27448076286684131,5.9129023656856132,0,1.9256276132888925E-2,0.10295148944290011,-1.5362262583781077E-3,4.2735918688482345E-2]
[null,1686,1.0153106534830458,1.0369862734261888,0.95549965358221356,0.96535603892159561,0.99759059282068163,0.98291003910225516,0.98811645493850608,null,6.7113070879942054,0,1.0327014904691354E-2,0.18023167667062867,0.11921135415187387,8.0247697946962085E-2,0,1.0327014904691354E-2,0.26080240935535137,5.9127047490700138,0,1.907288437424709E-2,9.700086873695371E-2,-4.8936154921288861E-4,4.2524809237388918E-2]
[null,1687,1.0185265716291303,1.030902784200127,0.97529976782325023,0.95962460435048269,0.99434020071596307,1.0391205817302431,1.0116639858857022,null,6.7394740308426462,0,1.0724163517382423E-2,0.19274887934161891,0.11876121070861097,8.1617211564117359E-2,0,1.0724163517382423E-2,0.27145123243455505,5.9113211777209553,0,1.9055930860586389E-2,0.10270815420233595,-2.3499625247663282E-3,4.4160196534632885E-2]
[null,1688,0.99840516666631374,1.0354021258967978,0.97645738049928676,0.9975898266134442,0.98073596604028079,0.98326234890804876,0.99431482811560967,null,6.728569033043617,0,1.0322510038486049E-2,0.18584885448928509,0.1209226291119293,8.1658677605833063E-2,0,1.0322510038486049E-2,0.26696291311483017,5.9133102324289677,0,1.9163801973516355E-2,9.8973925947841324E-2,-7.7826062877753852E-4,4.2506259000191747E-2]
[null,1689,1.0152186188238832,1.0083264534171044,0.9891970623690447,1.0079475159454128,1.0033776265868359,1.0084315594461373,1.0038377518055681,null,6.7358998327247059,0,1.0413829376594689E-2,0.19106985524737069,0.11995472075389761,8.2466666189530996E-2,0,1.0413829376594689E-2,0.26764472455614424,5.9131663646144359,0,1.9073371138786037E-2,0.1011081038364616,-1.4662693922130744E-3,4.2882295780286891E-2]
[null,1690,1.0063221176065236,1.0151655703735651,1.0046219812207215,1.0038598748771179,1.0219104915852393,0.99681717533854608,0.9938663874764696,null,6.734717257605916,0,1.0216337493644524E-2,0.19178012730003821,0.12040333727188386,8.3402922778082436E-2,0,1.0216337493644524E-2,0.26621365187523055,5.9120811525772963,0,1.91208443589597E-2,0.1007085297237445,-1.0623676378652041E-3,4.2069059358542861E-2]
[null,1691,0.97947679449143166,0.98672004226210397,1.0040718443798318,0.95167992483989783,1.0131124950586861,0.97173241667444166,0.98788824361916083,null,6.7446877137515111,0,1.0362501351759212E-2,0.19436547669603055,0.1251282511091481,8.3380458455275655E-2,0,1.0362501351759212E-2,0.26974778385915166,5.9092924414077483,0,1.9269322837030242E-2,0.10209400167523058,-1.2609583981708936E-3,4.2670936110062244E-2]
[null,1692,1.0177528769502104,0.97145461323523974,0.98072935799202243,1.0077718173170285,0.99689012952850287,1.0059842694025949,1.0055543910516629,null,6.7399593522738286,0,1.0607474149410096E-2,0.19219385996686872,0.12160895947137772,8.1938716046537088E-2,0,1.0607474149410096E-2,0.26758090492121989,5.9136257005104556,0,1.9059999797428607E-2,0.10213413577961455,-1.862614706936831E-3,4.3679690487256083E-2]
[null,1693,1.0137983568880178,1.0239028951688298,0.98392885788649909,0.97377007688090211,1.0255464194178288,1.0030282758317945,0.98140302893649012,null,6.7234845823960407,0,1.0352162608064043E-2,0.18846029476535495,0.11948427667979636,8.2031840941062667E-2,0,1.0352162608064043E-2,0.26138566613906472,5.9116110116810567,0,1.9080894004884448E-2,9.9989912528946331E-2,-1.1876773478783585E-3,4.2628363003753326E-2]
[null,1694,1.0105270986355186,1.0213790250609549,0.98527680174616239,1.0134821666797182,1.0019605247753816,0.99430314778228257,1.0400774496993686,null,6.7410354675744859,0,1.0294103087526034E-2,0.18777836370443438,0.11996486349594143,8.235238243369733E-2,0,1.0294103087526034E-2,0.27709745143442099,5.9136830956252133,0,1.9098301702138425E-2,9.9561012793938225E-2,-8.8928784768833142E-4,4.2389284232387206E-2]
[null,1695,1.0313853500642693,1.0169211796238695,1.0146365252866787,1.0001849902862869,0.99947655640818478,1.0381678563416539,0.97589134820215695,null,6.7289736000007006,0,1.028344898667707E-2,0.19592322771767609,0.11721473262835945,8.3917249466171961E-2,0,1.028344898667707E-2,0.25870977208372026,5.911314416760507,0,1.898919912314442E-2,0.10237574341430572,-1.816153734638368E-3,4.2345412541450432E-2]
[null,1696,0.99563867237373216,1.0164210004690926,1.0353410821621669,1.0064070608561009,0.9638300379042597,0.98729289392074271,1.006918123095466,null,6.744704881267821,0,9.9506555067744428E-3,0.19547692841674563,0.12105528598004801,8.5381713689208022E-2,0,9.9506555067744428E-3,0.27174348063441189,5.9104584078018734,0,1.9178974127535216E-2,0.10110818394333736,-6.7312155158168554E-4,4.0975028226242653E-2]
[null,1697,1.0076061274970776,0.98836944793205417,0.98436923251963471,1.0037085702436723,0.98081735891181965,1.0070697532050659,1.0194628738644012,null,6.7480955592650602,0,1.0613048018281527E-2,0.19333593358490614,0.12192092512952922,8.2247189748443486E-2,0,1.0613048018281527E-2,0.27393559256996269,5.9132050201677879,0,1.9113940902467E-2,0.1025541649392059,-1.9198504643990271E-3,4.3702642687156963E-2]
[null,1698,0.98913037706525864,1.0067496463321186,1.025053832841414,1.0070469879460464,0.99500690074122233,1.0249211104677618,1.0103903675682386,null,6.7664277341673218,0,1.0535072705860207E-2,0.2038343232573486,0.12251583410137595,8.4834428285769981E-2,0,1.0535072705860207E-2,0.27815991653499433,5.9110882562825706,0,1.9215001948406901E-2,0.10596433929648715,-2.5659197693309729E-3,4.3381554229694176E-2]
[null,1699,0.9947803495260531,1.0146239239545412,0.97442163898758982,1.0413243042652982,0.99939551744139954,0.96639085066146269,0.98210358842452905,null,6.7271323969343939,0,1.0289303312160897E-2,0.18469211840134128,0.12238902524032719,8.1514432338642015E-2,0,1.0289303312160897E-2,0.26325534990205895,5.9157863273291076,0,1.918369853948473E-2,9.8458401594649109E-2,-5.1647602298327845E-4,4.236951961176174E-2]
[null,1700,1.006366636615537,1.0403710474339867,1.0265910475872828,0.97549729990238854,0.98334665904636454,0.98827175991855476,0.98142289168337471,null,6.7237865447752858,0,9.831744636549445E-3,0.19065909322255767,0.1188170009235336,8.4683029347388569E-2,0,9.831744636549445E-3,0.26191430545396605,5.9092953561777337,0,1.9120604708491973E-2,9.9040281402173053E-2,-2.2850088856737289E-4,4.0485374428002006E-2]
[null,1701,0.98866717922342184,0.97537478283180978,0.97978993399653502,0.98740080487739612,1.0195966939414443,1.0141406608702677,0.98285645604789629,null,6.7557148384984558,0,1.0998081780005461E-2,0.19899362430385242,0.12500289639131781,8.1899213222260417E-2,0,1.0998081780005461E-2,0.26996211741408227,5.9125762084557838,0,1.9217584142667336E-2,0.105797360441302,-3.0223090572967549E-3,4.5288143184481343E-2]
[null,1702,0.99088283449810699,0.97453717356518865,0.98733664369270357,0.96649924264265963,1.0028946676078869,0.98628424331148778,1.0111240034766789,null,6.7504263399194366,0,1.0605976657699329E-2,0.19405925089019016,0.12462320487251287,8.2412941262692205E-2,0,1.0605976657699329E-2,0.27441943601458718,5.9110292892888578,0,1.9205254348971579E-2,0.10278537752344268,-1.7819383647528313E-3,4.367352408293472E-2]
[null,1703,0.99245996877146747,1.0039980417798211,1.0355505073319473,0.96721195076141653,0.9984011885349674,1.0134043510394757,0.9812935271530997,null,6.7505530430072955,0,1.0298740337162106E-2,0.20237754095298813,0.12203784812374857,8.5317313881963217E-2,0,1.0298740337162106E-2,0.26821892189556451,5.9083292083112271,0,1.9196511370534113E-2,0.10466671584430404,-1.999396974023732E-3,4.240837960098888E-2]
[null,1704,1.0176530935219747,1.0262169313287681,0.96665663681989467,1.0100444192188045,1.039901802593451,0.99390506978541882,1.0041970230361088,null,6.7235735258611422,0,1.0364065502067537E-2,0.18390164707828055,0.11923522442860696,8.1036797413049186E-2,0,1.0364065502067537E-2,0.2655541081226741,5.914518829209273,0,1.9060525018771753E-2,9.8420399831689404E-2,-8.3138224383031225E-4,4.2677377002623557E-2]
[null,1705,0.99395031544107659,1.0310867480728658,1.0144196101052763,1.0075508177376136,0.9889240389631585,1.02043775059858,0.97874700751331045,null,6.7466841705580922,0,1.0428586474730555E-2,0.19862465807349816,0.12096226788743047,8.4030505909956948E-2,0,1.0428586474730555E-2,0.26746568459584924,5.9117247598273659,0,1.9188275003945751E-2,0.10379843670946212,-2.053480333162952E-3,4.2943062883744838E-2]
[null,1706,1.0121642165861198,1.0021466025851209,0.9925290319189084,1.0043368755830955,1.0089498965431138,0.9740596115531952,1.0210032134425897,null,6.7304617259229778,0,1.0086457433158929E-2,0.18597973109795396,0.12055157628653733,8.2700721414401754E-2,0,1.0086457433158929E-2,0.26984674542819836,5.9127856307104869,0,1.908957586570597E-2,9.825124480736E-2,-2.7773607491881627E-4,4.1534236387252156E-2]
[null,1707,1.0074342262854645,1.010217094629746,0.96445773618557984,1.0172364998227614,0.99334441858037359,0.98809397726440074,1.0370264000858664,null,6.7403521188114963,0,1.0498292379572923E-2,0.18567598814466499,0.12124417521034896,8.1049424352456864E-2,0,1.0498292379572923E-2,0.27660233526140826,5.9150270743540974,0,1.9114864106041803E-2,9.9480107344166263E-2,-1.0719493543861246E-3,4.3230099392697174E-2]
[null,1708,0.98800363710955574,1.0231395089784803,0.991621980412005,0.98132957251406461,1.0087999992729597,1.0204724552430682,0.97181892284300031,null,6.7470213926579561,0,1.073831403936297E-2,0.19773298247459792,0.12249661767463192,8.2594483085790774E-2,0,1.073831403936297E-2,0.26721220758417225,5.9115926681024806,0,1.9221287416892816E-2,0.10450759058757839,-2.5549101336445096E-3,4.4218465865449766E-2]
[null,1709,1.0264915566629864,1.0310702494523873,0.98988764206306534,1.0239985987196352,1.0354343057400779,1.0001597500550821,1.0464961955530063,null,6.7332506865839639,0,1.0111830737296061E-2,0.18571892921139602,0.11757119353833836,8.2617423828038689E-2,0,1.0111830737296061E-2,0.27494738076684544,5.9139955347763378,0,1.9014398820918391E-2,9.8242719628912567E-2,-4.9561312423669873E-4,4.1638719137409089E-2]
[null,1710,1.021660325245481,0.99847460632272544,0.97293653777564337,1.0022807060777952,1.0199164336388282,1.03759672921293,1.0383899010844611,null,6.7522393805127647,0,1.0844961818456263E-2,0.19423748255455822,0.1199631310813758,8.1585602595351026E-2,0,1.0844961818456263E-2,0.2779810565407701,5.9137567258322941,0,1.903951317262282E-2,0.10362421132804066,-2.6059650294091782E-3,4.4657622437158921E-2]
[null,1711,1.0387261814123232,1.0073217905216001,0.97637742152045248,1.0197813726068825,0.9637027747176613,0.9913092781943148,1.016069248070844,null,6.716435114535642,0,1.0122119953145055E-2,0.1822193607668415,0.11751543489328134,8.1617024651744793E-2,0,1.0122119953145055E-2,0.26318964452163363,5.9145143610946036,0,1.8951844079268004E-2,9.7044927683866383E-2,-2.9857145246436797E-4,4.1681088296863095E-2]
[null,1712,0.95641826036444411,0.99104810161556045,0.97887728763461568,0.99523375676009107,0.98440399326887762,1.0024022889927833,1.0225561465234356,null,6.7838030247916379,0,1.1169694196697654E-2,0.2018252058907552,0.12841422406570882,8.2100846378158385E-2,0,1.1169694196697654E-2,0.28895954371619642,5.9130498905133662,0,1.9403511469016622E-2,0.10735186379125326,-3.2968736033686108E-3,4.5994812570548313E-2]
[null,1713,0.99508104021858423,1.0035654403171388,0.96834071704672242,1.0133668488432919,0.97173803969256078,1.0147765128725166,1.0152925440985867,null,6.755129583908734,0,1.0909626950011669E-2,0.19406692343047641,0.12300230712432644,8.1292797170624723E-2,0,1.0909626950011669E-2,0.27679883793631482,5.9146068832462078,0,1.9182042539314784E-2,0.10377265729451619,-2.5167667719862533E-3,4.4923901938939727E-2]
[null,1714,0.98122332650078348,1.005417585921939,1.0277104398355774,1.0049953329404178,0.96516515061975061,0.98950365010433494,1.0229587819209551,null,6.7618496983563894,0,1.0234948339772544E-2,0.19880685665816472,0.12351727768469295,8.5029130304385109E-2,0,1.0234948339772544E-2,0.28043595944763722,5.9108242525167443,0,1.9259415873251064E-2,0.10321597684668787,-1.3848664854682054E-3,4.2145695510290931E-2]
[null,1715,1.0096807022219234,1.0431128774704979,1.0014416450812951,1.0051044517950531,0.9729873186306438,1.0291263616955921,1.0092473755224975,null,6.7437925749991736,0,1.0419863536788459E-2,0.19468147865865906,0.11876440637003312,8.328624429052317E-2,0,1.0419863536788459E-2,0.27217115530675756,5.9123276895500112,0,1.9102824090299078E-2,0.1023935008636977,-1.841867508730893E-3,4.290714337792436E-2]
[null,1716,1.0005166185915395,0.9995809572887111,1.0178488220284243,1.0098341774015385,0.97361500593831707,0.96002184460148599,0.99200948675802869,null,6.7281251735029439,0,9.84750904330043E-3,0.18851148856488853,0.12160461796976843,8.4196770572500204E-2,0,9.84750904330043E-3,0.26398917798772331,5.9116523255872817,0,1.9152278693586211E-2,9.8346905824482952E-2,1.2131885366627167E-4,4.0550289449042771E-2]
[null,1717,1.0387168255632089,0.99913873829301914,1.0156695499071646,0.96185825660457769,0.98669794349125739,0.99434003239167867,0.98585747781420086,null,6.71133755878662,0,9.8450502257620108E-3,0.18785768539417452,0.11719282242441846,8.3912793995511381E-2,0,9.8450502257620108E-3,0.25577554667557717,5.9091847296520106,0,1.8951891352033037E-2,9.8111219800356947E-2,-1.8929498353951308E-4,4.0540164476072747E-2]
[null,1718,1.036079607900338,1.0065645261445397,1.0085414896275209,0.99006992110540648,1.0196356893730285,1.0067637532072804,1.0138547424615121,null,6.7248179584176322,0,1.002409587241888E-2,0.18926667945587841,0.11727297213253514,8.3614264147136963E-2,0,1.002409587241888E-2,0.26476936760793524,5.9111142909149574,0,1.896525059117625E-2,9.9195896195538882E-2,-6.5820520759166785E-4,4.1277442580068664E-2]
[null,1719,0.97867318910050882,0.96483843164891381,1.0224569787186639,1.0158587480550803,1.0241220989976758,1.0217462498599135,0.98836057455771387,null,6.7755271682095346,0,1.0834472673648843E-2,0.20882364792732558,0.12600004117246472,8.4640277768089411E-2,0,1.0834472673648843E-2,0.27518119411514408,5.9117136557555803,0,1.9273893056333639E-2,0.10869680834412963,-3.4167799353684684E-3,4.4614430005840144E-2]
[null,1720,0.99833279760090754,0.9800171565654201,0.99954135817376433,1.0265570994833566,0.98484042679409001,1.0024096286868704,1.0013629808237441,null,6.7521635558410571,0,1.0560143651998631E-2,0.196747776191599,0.12318587300085432,8.317214302335374E-2,0,1.0560143651998631E-2,0.27124446905373834,5.9135939117719882,0,1.9164197792706918E-2,0.10357796394123722,-2.0075708578563391E-3,4.3484791923430147E-2]
[null,1721,0.95344341512464315,1.0013866553195461,0.98917137077762074,1.03948669961676,0.99853638254743493,1.0127132405666281,1.0252029713850661,null,6.7925234378896704,0,1.1168872757445426E-2,0.20491536162862739,0.12808062634530379,8.2810109667664791E-2,0,1.1168872757445426E-2,0.29156093473917799,5.9148725480700683,0,1.9421296213723065E-2,0.10843609611904499,-3.5649649238624942E-3,4.5991430029918394E-2]
[null,1722,0.98190761636576651,0.99380718475161978,1.0136771737005366,0.99969671900945856,0.97575630758655119,1.043227868851559,1.0338239464258507,null,6.7870438614231237,0,1.0970873463201445E-2,0.20872368588416326,0.12427711946489471,8.42665418468065E-2,0,1.0970873463201445E-2,0.28865583290764857,5.911342700888258,0,1.9255543941836019E-2,0.10911604139170585,-3.7697090809694282E-3,4.5176104178782282E-2]
[null,1723,1.0078665854520139,0.99728225150243599,0.96190034831085802,0.97635734395442819,1.0234478641503866,1.0096960595781943,0.99489558100876474,null,6.7369779169719308,0,1.0806568556056174E-2,0.19040351935648983,0.12186522155236201,8.0740771005648582E-2,0,1.0806568556056174E-2,0.26737872638920951,5.9129549902013396,0,1.9112542700784479E-2,0.10214460404187567,-2.1219840921202762E-3,4.4499525816341284E-2]
[null,1724,1.0058293053698915,1.0161550717394396,0.99153412275691299,1.0250267000061954,0.99026996802588707,0.95938837668842636,0.98664621815415432,null,6.7183311730432571,0,9.9464952060608434E-3,0.18312875007563351,0.12065744761111982,8.2535637523183131E-2,0,9.9464952060608434E-3,0.26094097737921279,5.913959390174794,0,1.9123498635820517E-2,9.6793069928202288E-2,2.345048668792766E-4,4.0957896848409961E-2]
[null,1725,0.99190724443609779,1.044017060686615,1.0033369688213334,1.0138862207239339,1.0000668193278786,1.0088792715057313,1.0015864189240127,null,6.7469223242960021,0,1.0376845800997903E-2,0.19442280392453523,0.12081535584579438,8.3423353941245268E-2,0,1.0376845800997903E-2,0.27304751514206665,5.9126954793370512,0,1.9199572280579173E-2,0.10216133588821844,-1.5730960623027165E-3,4.2730003998810384E-2]
[null,1726,0.972655748093742,0.99984433305233344,0.97883704946539829,0.97179283491593493,0.9677922454065474,0.98835475621309177,1.004480738168062,null,6.7574003872271922,0,1.0788771813992577E-2,0.19493068050562337,0.12582571812817217,8.1931331478487787E-2,0,1.0788771813992577E-2,0.2776522309951438,5.9117848681540019,0,1.930835510041903E-2,0.1036867203204736,-2.1457594553534699E-3,4.4426242000225408E-2]
[null,1727,0.99266694922070731,0.97070003802109339,1.0059111345213563,0.98195749692216516,0.95520143239983835,1.0037568061501185,0.95733377881234505,null,6.7445820361895032,0,1.0619062506094961E-2,0.19972096934790981,0.12424142594299172,8.3398211602900313E-2,0,1.0619062506094961E-2,0.26103211031010853,5.9108247697384924,0,1.9195366018990325E-2,0.10481148264201411,-2.3697086913410641E-3,4.3727409277433738E-2]
[null,1728,1.0137752082377516,0.98465427931809735,1.0051058929105072,1.0134346743699127,0.9680459040012489,0.98279626550426558,0.99331626132999784,null,6.7302044720655108,0,1.0125849084568659E-2,0.19021775773076541,0.12097698056945394,8.3397503018330127E-2,0,1.0125849084568659E-2,0.26310302192038137,5.912571231025419,0,1.9081016793602499E-2,9.9864135216449254E-2,-7.0361840519827222E-4,4.169644419630486E-2]
[null,1729,0.99197870243471664,1.0249349083697556,0.95896126661986625,1.0035881873346677,0.9947069865458289,0.97744214758180492,0.98908615059809379,null,6.7300379554369503,0,1.053206582664319E-2,0.18475838677912346,0.12252375677530587,8.0569908444159066E-2,0,1.053206582664319E-2,0.26679529311195871,5.91458615770732,0,1.9199176364190714E-2,9.9263337618626546E-2,-1.0272338000219055E-3,4.3369172436283049E-2]
[null,1730,0.9960056303606416,1.0009518267732451,0.9938978725888018,0.98115302386606551,1.0284167973840468,1.0360324133300498,1.0342276183926948,null,6.7692928678029025,0,1.0894783645560126E-2,0.20129209485404073,0.12254014254605193,8.2957067056895151E-2,0,1.0894783645560126E-2,0.28385329702588702,5.9114561757137585,0,1.9176956788764809E-2,0.1062681467673178,-3.1137928030292713E-3,4.4862779853217974E-2]
[null,1731,1.0243624294485225,0.99438812842960123,0.95384685285345427,0.99848348774791207,0.99850556994880735,1.0139208922889771,0.99464348246425738,null,6.7282026187997301,0,1.0765457411626199E-2,0.18742253734314782,0.12018681314958726,8.020076396977692E-2,0,1.0765457411626199E-2,0.26341011250127672,5.914584980062747,0,1.9025437538674105E-2,0.10095537969769504,-1.9136429042614766E-3,4.4330237441089576E-2]
[null,1732,1.03125867375753,1.0141763152608716,0.99379740672538175,0.97475002292653667,1.0071588735805934,1.0134596062657673,0.96773833700257406,null,6.7147353153278759,0,1.0236303318392943E-2,0.18909784803018759,0.11773324629076232,8.2550971730078623E-2,0,1.0236303318392943E-2,0.25440160749858443,5.9111157164307473,0,1.8989848404394164E-2,9.9835431043948569E-2,-1.140629171906244E-3,4.2151275071072525E-2]
[null,1733,1.0050383951019424,1.0208237822543575,1.01349535181587,0.99937126656468422,1.0054674012798677,1.028131983756519,0.97162435611600728,null,6.7412287905123884,0,1.0444315959348959E-2,0.19865233057876905,0.12012459162848066,8.3911200324340809E-2,0,1.0444315959348959E-2,0.26338154457821833,5.9113354711320181,0,1.9127763903744092E-2,0.1038602898439103,-2.1722355787558594E-3,4.3007834101659544E-2]
[null,1734,0.99955984947234922,1.0233469351919375,0.98096376233098881,1.0144080014231405,0.99877409823393293,1.0355710097891251,0.99148783532739371,null,6.7509000445062437,0,1.0870869047035426E-2,0.19703474722323547,0.12126724132361648,8.2002439802329324E-2,0,1.0870869047035426E-2,0.27084597329947296,5.9139715219025497,0,1.9157494243197792E-2,0.10469435737162228,-2.8380344529143667E-3,4.4764303793133113E-2]
[null,1735,1.0112964414008556,1.0239768071142099,1.0144313223192358,1.0087191467255967,0.97469004883735189,1.0017160085694812,1.0254902612952854,null,6.7412878683116606,0,1.0091392680456284E-2,0.19220573832011922,0.11921677368714916,8.411567980268321E-2,0,1.0091392680456284E-2,0.27373181912446148,5.9117872174230151,0,1.9094197587606661E-2,0.10044341922735051,-8.615357179068392E-4,4.1554558857181387E-2]
[null,1736,1.0257767700141702,1.0464795371150635,1.018134988334163,0.99926069984008958,1.0359255577784934,0.95741762843166944,1.0314647774658747,null,6.7117341280160341,0,9.3904758004883637E-3,0.17983859728210372,0.116449355426792,8.4247525048494323E-2,0,9.3904758004883637E-3,0.26712756779335955,5.9110647011879589,0,1.9018099609127474E-2,9.3809001741082337E-2,1.5109720230837935E-3,3.8668307904027338E-2]
[null,1737,0.97865597158068229,1.0107634802348044,1.0072258546791135,1.019272462092367,0.99059897032221567,1.0208751635465056,1.000879226981471,null,6.7681572415578346,0,1.0754217203286081E-2,0.20265707512147149,0.12397269784268358,8.3736740191701853E-2,0,1.0754217203286081E-2,0.27802673504963743,5.9127667954256715,0,1.9273991056969045E-2,0.10628308788764472,-2.8438332817765817E-3,4.4283952263827468E-2]
[null,1738,0.99043874408340737,0.99335691292291517,1.0179471695647391,0.9797807810757011,1.0013201895764059,1.0160234273085216,1.0165757295913014,null,6.764086020797726,0,1.0555293816311661E-2,0.20209006065703231,0.12314738139650386,8.4382282604966524E-2,0,1.0555293816311661E-2,0.27876834713971815,5.9100229949518415,0,1.9207721226078233E-2,0.10542576828434984,-2.4233566260705953E-3,4.346482116330979E-2]
[null,1739,1.0105890618001441,1.0114487350861989,0.98141755269945563,0.99791451493672656,1.0064250770463088,1.0036668908682762,0.97809605788206599,null,6.7284262740098457,0,1.046912526758154E-2,0.18988092075533089,0.12049787968081968,8.1894710989628583E-2,0,1.046912526758154E-2,0.26150042353328173,5.9130548750231311,0,1.9097970923790529E-2,0.10087026277618819,-1.4807640893938151E-3,4.3109994417069045E-2]
[null,1740,1.0170277467571662,1.0218116701131039,1.0131178048326122,1.0230656210185312,1.0216793049528146,0.9996552353834226,0.96721692488097044,null,6.7218261649872524,0,1.003448034553707E-2,0.19075058362587,0.11866950889086057,8.3811914137570026E-2,0,1.003448034553707E-2,0.2565559893730297,5.9126372075652416,0,1.9063818948953877E-2,9.9747663385665847E-2,-7.3072493194500986E-4,4.132020399200205E-2]
[null,1741,1.0097957200024421,1.004872008568449,0.9953086199810447,1.0084453515222249,0.98421724354150797,0.9685629357202532,1.0249144414618154,null,6.7309557515760243,0,1.0017041249965181E-2,0.18546228591197947,0.12065180425537883,8.2891604602034236E-2,0,1.0017041249965181E-2,0.27097137448926495,5.9128523991999886,0,1.9102209092668708E-2,9.7842388590320489E-2,-6.6707466095786556E-5,4.1248392900480317E-2]
[null,1742,0.99933386299422478,0.99141056728020893,0.9927883902451704,1.0404211749358299,0.96350984894765024,1.0402111805517658,0.96430874199475969,null,6.754060543839949,0,1.0957727234258929E-2,0.20212237964403729,0.1226216439487646,8.2669387309571393E-2,0,1.0957727234258929E-2,0.26426853832339964,5.9147214753451021,0,1.915872760100714E-2,0.10676545145809879,-3.3890301379708252E-3,4.5121970347938502E-2]
[null,1743,1.0355426637104854,0.99723155916913275,1.0031765511255715,0.9972781359793873,0.97321941576687587,0.99943529120539687,1.0006833424342176,null,6.7205148614786028,0,1.004307714394787E-2,0.18812453950423627,0.11786926366862463,8.3234835981869759E-2,0,1.004307714394787E-2,0.26087994078779975,5.9118070252089252,0,1.8967978903382792E-2,9.8859717409133407E-2,-5.8404406305319183E-4,4.1355604077684655E-2]
[null,1744,1.0414057439941145,0.98468241451545424,0.99851849368243084,0.98868679382674596,1.0232815193792493,0.98016770651852447,1.01583710418197,null,6.7146898983016525,0,9.8874516693942746E-3,0.18393578171266811,0.11788525150204919,8.2950156175544451E-2,0,9.8874516693942746E-3,0.26167472371305406,5.9116047031479795,0,1.8938339878111735E-2,9.6882305275366468E-2,1.0387082310671886E-4,4.0714766073774805E-2]
[null,1745,1.0368369293643471,1.0069445842524611,1.0202180579507723,0.99737707847040546,0.99344446757927851,1.032461709791676,1.0250890721339585,null,6.7385524399626844,0,1.0166401116628657E-2,0.19529939313130704,0.11695772379479369,8.4412118732804242E-2,0,1.0166401116628657E-2,0.26991206884205848,5.9108436670305764,0,1.8961407305002433E-2,0.10176928416304512,-1.4666532832390881E-3,4.1863430246335293E-2]
[null,1746,0.99466798528896205,1.0055683656619192,0.9682863335564329,1.0324072776801092,0.96627771021643238,1.0027578787772982,1.0101513614870483,null,6.7498984340131836,0,1.0776199703359956E-2,0.19167796023122094,0.1229562930368736,8.1270755455097557E-2,0,1.0776199703359956E-2,0.27434262669836218,5.9156393581711253,0,1.9184317622388276E-2,0.10249802060620204,-2.0453700944765684E-3,4.4374472286392526E-2]
[null,1747,1.031276302529744,1.0256197964914708,0.98484450307214721,0.98938931092762183,1.0394779084708012,0.99355597375105664,1.0253615216757339,null,6.7204828882132039,0,1.0065344354244448E-2,0.1834878137007783,0.11736423500335724,8.2180638810597534E-2,0,1.0065344354244448E-2,0.26757278943673818,5.9124046795749985,0,1.8989758038311853E-2,9.73071590033249E-2,-2.7148184117908218E-4,4.1447296486270269E-2]
[null,1748,0.98123575267724028,1.0162180106901955,0.99083907985558872,0.99756246812657101,0.98560608181155607,0.99216239020238417,1.0048407589736483,null,6.7520613786654025,0,1.0550212980849826E-2,0.19404399096101757,0.12369165681724031,8.2668986907432795E-2,0,1.0550212980849826E-2,0.27555391047186301,5.9125136685537312,0,1.9259345513818308E-2,0.10259787903518805,-1.71195878212259E-3,4.3443899187232939E-2]
[null,1749,0.99502825386521554,0.96581963396891757,0.99562878282166711,1.0134575316918328,1.0105002544954242,0.99993716252760678,0.99751293139278219,null,6.7542581242328756,0,1.0671821943371483E-2,0.19767911059564122,0.12439316874953078,8.2916748693414657E-2,0,1.0671821943371483E-2,0.27101374450031829,5.9131053750451548,0,1.9182333178279276E-2,0.10427087886218653,-2.2478986409589638E-3,4.3944663249308714E-2]
[null,1750,1.0146508364589943,1.0098844420423327,0.98091776208590675,1.0303539726701545,0.97087905485930415,0.9705805162878417,1.0115433179584894,null,6.7238744041111644,0,1.0094559241911633E-2,0.18295162852204908,0.12009894777445854,8.194956207374357E-2,0,1.0094559241911633E-2,0.26627861370994049,5.914836082823407,0,1.9076376050720944E-2,9.7213534432247353E-2,-9.7939469030322636E-5,4.1567598193627583E-2]
[null,1751,0.99928314892432868,1.0242525895816856,0.98644421890215417,1.0083740530578242,0.97610494012328586,1.0325242205395755,1.0021396384968277,null,6.7528676955192743,0,1.0786113127172757E-2,0.19709423030724774,0.1211569200510255,8.2375178087957093E-2,0,1.0786113127172757E-2,0.27354642792937089,5.9133422789835208,0,1.9159004457898351E-2,0.10443941070824808,-2.6610490071230937E-3,4.441529400113E-2]
[null,1752,1.0089667599755365,0.95824408158226271,0.96320231560038527,1.012194554003518,1.0062331554108104,0.97686795755918987,1.0108945998601233,null,6.7372825697033383,0,1.0612105246622032E-2,0.18733922616176057,0.12366818304466015,8.0863952136927167E-2,0,1.0612105246622032E-2,0.26866817760804579,5.9148224578158484,0,1.9106644660709295E-2,0.10043475685235465,-1.3195890982400026E-3,4.3698760521270245E-2]
[null,1753,0.99617046620321126,0.9900963206614174,1.0277656207451926,1.0229315731645989,1.0034446523752143,0.9936009468786563,1.0251026415995981,null,6.7571003474706082,0,1.0189436221187438E-2,0.19793896252022147,0.1224125044094231,8.500255071662785E-2,0,1.0189436221187438E-2,0.2773588218779689,5.9117899645656662,0,1.9176051093206328E-2,0.10276260154982997,-1.2993939691464198E-3,4.1958284706812579E-2]
[null,1754,1.0097740903392134,1.0089684795001652,1.0264699232622645,1.0286430669749307,0.96599286072076285,1.0297406609220885,0.97898559162845611,null,6.7456026270831639,0,1.0345610905144291E-2,0.20058816042338082,0.11987899124599885,8.4748758822506362E-2,0,1.0345610905144291E-2,0.26442246704328565,5.9121732772397406,0,1.9102324735322623E-2,0.10420426175916721,-2.1169984435258789E-3,4.2601384257289432E-2]
[null,1755,0.95988274113618022,0.99738402973572826,1.0368740370385483,1.0220065499730964,0.97392495020996583,0.97929102847239236,0.9727135312268913,null,6.7628360243485197,0,1.0307023830074312E-2,0.20293678051495684,0.12648738906276596,8.5490265343619656E-2,0,1.0307023830074312E-2,0.27170691988852258,5.9112117573913272,0,1.9382938444010379E-2,0.10488799251234651,-1.7105083594247061E-3,4.2442489550394563E-2]
[null,1756,0.99182650275812967,0.99239460535376345,1.0347076479626416,0.96561240258110048,1.0210328006640979,1.0184190189391173,0.99996915516303142,null,6.760354269553277,0,1.041570337505285E-2,0.20442119459558133,0.12270116800567619,8.5345016096806808E-2,0,1.041570337505285E-2,0.27409918866424432,5.9082917825879875,0,1.9200019702275979E-2,0.10576729754183582,-2.3614102135098027E-3,4.2890012572378323E-2]
[null,1757,0.98124968899290244,0.991187033382956,1.0080772957418795,0.97242530734247079,0.98693275407627856,0.98808651912133494,1.0423470971785302,null,6.7658537225178197,0,1.0460834383094466E-2,0.19737711612851308,0.12459971974192556,8.3858925139845136E-2,0,1.0460834383094466E-2,0.28571102734811027,5.9101871475399879,0,1.9259266605803085E-2,0.10347039865739975,-1.6857326742400552E-3,4.3075854030473718E-2]
[null,1758,0.9739465137718063,0.9853301424084886,0.97516238726310966,0.95700733117413062,1.0468024474552353,0.98914973464508971,0.98829724220149151,null,6.753907774361303,0,1.0885707893830518E-2,0.19561247934864318,0.12646643617415707,8.1630785391006447E-2,0,1.0885707893830518E-2,0.27303148684587863,5.9111872030012531,0,1.9300926975737865E-2,0.10424123617155572,-2.3881870699505301E-3,4.4825407523019029E-2]
[null,1759,1.0219817294402183,1.0038827419379694,1.0229198596390159,1.0375915888598453,0.99492150167288862,1.0035524165696859,0.97300180818663884,null,6.7265070050642963,0,1.0014738795246536E-2,0.19315628485751873,0.1187524437758659,8.4438905652257104E-2,0,1.0014738795246536E-2,0.25736744066242251,5.9128611327077749,0,1.9037835033658343E-2,0.10051874134417073,-8.6469077114785162E-4,4.1238911801770604E-2]
[null,1760,0.9986181011569043,1.0111518756037663,0.98574541576672892,1.0081905411631564,0.99069949457358042,0.99066584221979148,0.98306935666363926,null,6.7340496556817051,0,1.0419305053418482E-2,0.1901943539463819,0.1218764618687023,8.2215538120204198E-2,0,1.0419305053418482E-2,0.264790262620759,5.9133710947397731,0,1.9162637671095776E-2,0.10081837719228254,-1.283914120311335E-3,4.290484364281312E-2]
[null,1761,0.99486289286417062,0.98544159324732183,1.0116825584521714,1.0025285748586052,0.99745469606478243,1.0053761229378237,1.0044952472480124,null,6.755436380464138,0,1.0491288532050867E-2,0.19901106826849502,0.12311223538765205,8.3935952699553909E-2,0,1.0491288532050867E-2,0.27328826062802936,5.9116092081057969,0,1.9183243847143813E-2,0.10414108162348297,-2.0459288912530317E-3,4.3201258795239728E-2]
[null,1762,1.0049636517254816,0.9991562666577023,1.0267166630142064,1.02455571847141,0.9970388775844321,0.98220507622424047,0.98918936230874344,null,6.7347241264448439,0,9.9546963717186288E-3,0.19307925437138526,0.1209199296836749,8.4757640002486576E-2,0,9.9546963717186288E-3,0.26415161278448523,5.9119382451680593,0,1.9128167331473909E-2,0.10029127566245068,-5.3366634801099342E-4,4.0991667788835645E-2]
[null,1763,0.9778768973662435,1.0386471104309718,1.0051195640034296,1.0044070260143267,0.98302572330245142,1.010718912480959,0.96754111935638698,null,6.7489317739146442,0,1.0551753267659983E-2,0.19822253584141,0.1227681176468368,8.3457221282668761E-2,0,1.0551753267659983E-2,0.26776994735378506,5.9120826198484835,0,1.9278429091071511E-2,0.10406593074376926,-2.1632697075385323E-3,4.345024181415634E-2]
[null,1764,0.99753779914111773,1.0015309362903888,1.0015963029785939,0.96942382285305906,0.96151983760275517,0.99423255859251358,1.0058035435259114,null,6.7435580707904634,0,1.0366643090219223E-2,0.19373150267205844,0.12217924934426806,8.3264103409330548E-2,0,1.0366643090219223E-2,0.27166450129747571,5.9103907558384448,0,1.9168549780095395E-2,0.10188603605924598,-1.4146186622972664E-3,4.2687991051838611E-2]
[null,1765,0.99304910570787941,0.9796488208871923,0.97653852856565337,1.0032561096012911,0.98722720279755405,1.0321408884415864,1.0194367518498151,null,6.7696626346987561,0,1.1154591561592245E-2,0.2008540295779849,0.12429504283666702,8.1845960169129525E-2,0,1.1154591561592245E-2,0.28047512465087249,5.9136121140274112,0,1.9193252564063092E-2,0.106960589208699,-3.5061009434266951E-3,4.5932622607353091E-2]
[null,1766,1.0113153335104803,1.0396509773035205,1.0151016112080169,1.0356405652376779,1.0252528788144561,0.98134537062614169,0.96995608149231327,null,6.7170758064101239,0,9.8161926371053507E-3,0.18714968833519285,0.11848002369031736,8.3949612510589106E-2,0,9.8161926371053507E-3,0.25695827306748542,5.9132035539514298,0,1.9094096884834308E-2,9.7768858585410748E-2,5.0365322422129356E-5,4.0421334062443914E-2]
[null,1767,1.0022171069820134,0.98470113307559259,1.0358231463575518,0.95515249570532257,0.99541130578173442,0.98333201345805632,0.96848949505066761,null,6.7311901101006137,0,9.9760746355502875E-3,0.19611591977154683,0.12178631944351145,8.5205645245408704E-2,0,9.9760746355502875E-3,0.25958509193841278,5.9076620024344573,0,1.914303355141498E-2,0.1014147626129718,-8.0236457121083695E-4,4.1079699674105331E-2]
[null,1768,1.0357564038114047,0.95981009268909612,1.0054428533336233,0.99446941148393564,0.99290078186270314,1.0205750405856917,0.99734785703443396,null,6.7349161554247816,0,1.0402262025706556E-2,0.19550781052716126,0.11961994918689996,8.3392318641264021E-2,0,1.0402262025706556E-2,0.26230298876468366,5.9115273462033517,0,1.8966892511710857E-2,0.10262426949947588,-1.8600833980063622E-3,4.2834663488241248E-2]
[null,1769,0.97614562019240558,0.99898096424085558,1.0415792856633226,0.96666470722842579,1.0088067826362155,1.0184541901273487,1.0119803577086688,null,6.7748534244654754,0,1.0490020249115672E-2,0.20798039321854478,0.12420847357770923,8.5877480171085943E-2,0,1.0490020249115672E-2,0.28178886261990976,5.9079482525866291,0,1.9288316758446312E-2,0.10724786981676118,-2.6822605154715826E-3,4.3196036231858546E-2]
[null,1770,0.99497660836998791,1.0304690901684543,0.98649578383252245,0.98391780515562699,0.99355873188556254,1.003750232648589,1.0067650061481423,null,6.7434508899480505,0,1.0503211468106051E-2,0.1919394560541047,0.12138620847714818,8.2356925812932483E-2,0,1.0503211468106051E-2,0.27322443575630134,5.9120174551368336,0,1.9182617565583052E-2,0.10170529829406721,-1.6118624726362027E-3,4.3250355323711472E-2]
[null,1771,0.96514083136815687,1.0047962421360395,1.0069140215011028,0.98602097646755138,1.0002383606700145,1.0106880413962531,0.99528021976269154,null,6.7719858713050254,0,1.0826352406718174E-2,0.20392224236634787,0.1260128774216141,8.3713008785725782E-2,0,1.0826352406718174E-2,0.27941906508126324,5.9109876445332876,0,1.9351996670473111E-2,0.10696311825153884,-2.9650739972037522E-3,4.458099219197327E-2]
[null,1772,0.98278491646171418,1.0406887063163921,1.0016295000642792,0.97964264530515988,1.0048677775009081,1.0352686358532928,1.0108507925287025,null,6.765205484330453,0,1.0777866798557573E-2,0.20142634340034021,0.12212470196920241,8.3395515527435016E-2,0,1.0777866798557573E-2,0.28067378351801631,5.9109411264540226,0,1.925058778425064E-2,0.10593111228083106,-2.9190236913346022E-3,4.4381337087684443E-2]
[null,1773,0.98056806943975805,1.0023716574303432,0.99550869575402889,0.98211515092333035,0.98877517771583556,1.0363500072026242,0.96621986573709551,null,6.7616529486732784,0,1.1047432182832119E-2,0.20460029841034724,0.12436812262226984,8.2865952613238342E-2,0,1.1047432182832119E-2,0.26937920678087224,5.91141814863514,0,1.9263128592754301E-2,0.10792808378333407,-3.6613521239546656E-3,4.5491359359277284E-2]
[null,1774,1.0047199030180216,1.0122665786059781,0.99877144564531173,0.98355171063797597,1.0115120106617459,1.0034673212436038,1.0344692859048759,null,6.7484575685782682,0,1.0366369076989637E-2,0.1929173471751639,0.12084204976616947,8.3185766163923758E-2,0,1.0366369076989637E-2,0.27819103680043272,5.9113129898018952,0,1.9129483383332219E-2,0.10160028700600947,-1.4082542327935072E-3,4.2686862714131704E-2]
[null,1775,0.98954955256457189,0.99412572986764758,1.0287395883975794,0.98944287645721196,0.96752991598483207,0.97935118226053997,1.0361025153954881,null,6.7566373372173247,0,1.0084314238409955E-2,0.19617914886695795,0.12301277431478475,8.5085160143447525E-2,0,1.0084314238409955E-2,0.28075980709125514,5.9099246966830759,0,1.9212667249688429E-2,0.1018002832075941,-8.6261143223129318E-4,4.1525411092750313E-2]
[null,1776,0.96953737495202352,1.0173449013282301,0.99094628491250392,0.98347179840180032,1.0146408128942963,1.0285841104970839,1.0319323150992041,null,6.7822871769288628,0,1.1063191363020962E-2,0.20351124826990055,0.12512657987914649,8.2858837771467783E-2,0,1.1063191363020962E-2,0.29001413137922444,5.9117460913263375,0,1.9326382388921686E-2,0.10759780056858695,-3.4501475129838448E-3,4.5556252858265422E-2]
[null,1777,0.98809864757810673,1.0346384850902399,0.99858396980780451,1.0234895395034969,1.0066178567985988,1.0153454247870093,0.97727171811788249,null,6.7472573908922682,0,1.0567938500006273E-2,0.19661391807046719,0.12180855311902404,8.3069328845994675E-2,0,1.0567938500006273E-2,0.26811521748456729,5.9134819054174583,0,1.9220756851825241E-2,0.10355673968495448,-2.125918302122309E-3,4.3516889720094397E-2]
[null,1778,0.99275067235751779,0.97534341988786932,0.98214477045649307,0.98394011789153857,1.0290796548744716,1.0104910554780313,1.0105128876626903,null,6.7589975040617132,0,1.0891196935347626E-2,0.19774935122305626,0.12444584162975371,8.2123764078938483E-2,0,1.0891196935347626E-2,0.2760674375494177,5.912259318967056,0,1.9194902862472295E-2,0.10501198506456463,-2.7031077325159933E-3,4.4848010418973516E-2]
[null,1779,1.0006368103340624,0.97845493403294836,0.98226611704941347,1.0016762739899552,1.0038374445107803,1.0058543534601918,1.0174307304452954,null,6.7536828074924147,0,1.0739968349544243E-2,0.19503862885469278,0.12330559735339353,8.2133035077612049E-2,0,1.0739968349544243E-2,0.27528258431430364,5.913211400872302,0,1.9151624208295071E-2,0.10356620729659471,-2.2315485051032421E-3,4.4225278020320002E-2]
[null,1780,0.96084158289403243,1.0455466303810208,0.97311243651321511,1.011089116728493,0.98729367465414231,0.96193143933926128,1.0199521831026994,null,6.7530207109150249,0,1.048020092227327E-2,0.1877534914680917,0.12522424880311298,8.1664815537524527E-2,0,1.048020092227327E-2,0.28236649001697484,5.914223339235857,0,1.9377270794214335E-2,0.10015620491072544,-9.0075184317680462E-4,4.3155601991696574E-2]
[null,1781,1.0026419641237865,1.0176169655214118,0.98731850741156879,1.0048050162843414,1.0162179212555302,1.0125019438986005,0.99828941055741693,null,6.7426966673487518,0,1.056282633842737E-2,0.19326452490910589,0.12104926657888614,8.2376946386231636E-2,0,1.056282633842737E-2,0.26978865646486716,5.9131008585182974,0,1.9140728602655782E-2,0.10236536994290883,-1.8855228028432903E-3,4.349583874864333E-2]
[null,1782,0.99405058227069443,0.98530284907775656,1.0088573541623411,0.98602553985641572,1.0049949424370417,0.9745423887640996,1.0290221720140562,null,6.7492052887601828,0,1.0203636715121346E-2,0.19274673719688548,0.12327361775926005,8.3800982161807674E-2,0,1.0203636715121346E-2,0.27715831959441506,5.9108778514439928,0,1.9187721768287827E-2,0.101004027639823,-8.6072861752639856E-4,4.2016759813238727E-2]
[null,1783,1.032754634027284,0.9706230025643281,1.0168324857204671,0.97723789306716635,1.0334740573577519,1.0376099169193174,1.0082564990428917,null,6.7444686304529533,0,1.0451159369962226E-2,0.19976657961258654,0.11922099348720615,8.4154293694508386E-2,0,1.0451159369962226E-2,0.26742089689677673,5.9099493028477639,0,1.8982191004396541E-2,0.10427096030294664,-2.3326014417165098E-3,4.3036014048483291E-2]
[null,1784,0.96879924330629008,0.97713440364556203,0.9993515636353657,0.96878274755455618,0.98019607602777359,1.0448604089199223,1.034335631246128,null,6.7984977457479525,0,1.1359124158411076E-2,0.21157421301391346,0.1270945307936113,8.3413035079630105E-2,0,1.1359124158411076E-2,0.29306519845756918,5.9104822632953216,0,1.9330666507862505E-2,0.11139385061237456,-4.6308634479438338E-3,4.6774851435607931E-2]
[null,1785,1.0272531674907417,1.0258953312357197,0.99616347192273791,0.97259584712941771,0.9929950758848981,0.99650992859267262,1.0216365047072293,null,6.7233327008251447,0,1.0034038689000236E-2,0.18601248825415601,0.11760778000242311,8.2877099319108569E-2,0,1.0034038689000236E-2,0.26793559831760944,5.910867032209449,0,1.9010461269117745E-2,9.8090927222534069E-2,-3.8707109825232713E-4,4.1318385328995295E-2]
[null,1786,1.0192240941139752,0.97551470205976853,1.0107682135685061,0.98061818124228128,0.98519673019140885,1.0091841387417972,0.97901282979018278,null,6.7334198651422579,0,1.0332282937232732E-2,0.1957297719221662,0.12067436832426363,8.3687985071412771E-2,0,1.0332282937232732E-2,0.26044067285931627,5.9104772687692888,0,1.9052267815977304E-2,0.10247031035449725,-1.6592820323889205E-3,4.2546502057719489E-2]
[null,1787,1.0045412412738923,1.0084361344628523,1.0095679475622488,0.9687954681118518,1.007913100813457,0.98658414972244135,0.99693085645213975,null,6.7325362175787751,0,1.0114440521630368E-2,0.19126292604815628,0.1208458385212404,8.3689625154727762E-2,0,1.0114440521630368E-2,0.26662555646269659,5.9099065441487131,0,1.9130448422262632E-2,0.10019124279879862,-7.6542974259436749E-4,4.1649465764773463E-2]
[null,1788,0.99595010591286093,0.9971942881646243,0.99641325460776919,0.985530546330743,0.96632460938869813,0.97118042821916239,0.99812518968764896,null,6.7346525762520493,0,1.0207402509061979E-2,0.18929638743213503,0.1226842036187959,8.2903335866822567E-2,0,1.0207402509061979E-2,0.2678737048137772,5.9115521176067807,0,1.9177261937035686E-2,9.9810241681013212E-2,-6.7694338671441272E-4,4.2032266682399906E-2]
[null,1789,0.97366476410980618,1.0170541397266162,0.99580636195095462,1.0101902495132062,1.0176414009770274,0.98156158479883315,1.0208094681308086,null,6.7588325675494652,0,1.0469450791814631E-2,0.19398153801315401,0.12451780224476397,8.3061345297911718E-2,0,1.0469450791814631E-2,0.28107048720276989,5.9129188510013577,0,1.930254671415774E-2,0.10231146084748534,-1.4427986400525018E-3,4.3111334867919772E-2]
[null,1790,1.0280697685903963,0.99677130701214345,1.0292118871635283,0.97864569692143621,1.0401479427212206,0.97767861978335957,0.99040815145618022,null,6.7156941116254973,0,9.6748624127131252E-3,0.1883451750491234,0.11826912941562903,8.4793944988450567E-2,0,9.6748624127131252E-3,0.25814683033042918,5.9093141654720425,0,1.9006245896948763E-2,9.7712465083530792E-2,2.6679403510406993E-4,3.9839361354238913E-2]
[null,1791,1.0014493567117282,0.97452464783397608,1.0144678631774218,0.99797566190263587,0.99966733961393284,1.0271415206414398,0.98358949627035985,null,6.7558001697000005,0,1.0672849919102752E-2,0.20329145824700756,0.12279574520426875,8.4033189245512563E-2,0,1.0672849919102752E-2,0.26800089440805519,5.9112046604320376,0,1.9147203735395038E-2,0.10623470959349986,-2.8565874361807216E-3,4.3948896270397206E-2]
[null,1792,0.98101725325703804,1.0121032085382429,0.99770131646020366,1.0027601993446955,1.0062653557885566,0.98249091218297058,1.0226123963512046,null,6.7549609694178452,0,1.0405339571406165E-2,0.19333579189790837,0.12379006710562576,8.3153637618930507E-2,0,1.0405339571406165E-2,0.27959603744709066,5.9124111266139172,0,1.9260582960001642E-2,0.10187482896949736,-1.3084394687751628E-3,4.2847336273649533E-2]
[null,1793,1.0284928846324162,0.97641526689105707,1.006876359470513,1.0245878784152338,0.98964921978882003,0.99292438075895906,1.0135171579391733,null,6.7318949655754103,0,1.0104540314602839E-2,0.19031577159405147,0.11961461110660024,8.3548539518113807E-2,0,1.0104540314602839E-2,0.26564714265547601,5.9130738072464197,0,1.9004064364623992E-2,9.9827992455417763E-2,-7.4566183969724262E-4,4.1608698474405258E-2]
[null,1794,0.97770133161799211,1.0361148264047519,1.0333785799120729,1.0301740138204212,0.96836044367167362,0.97999629229795537,0.9961643848824866,null,6.7492620839538677,0,9.9932495454069983E-3,0.19574518171567257,0.12237124058451411,8.5295470397620171E-2,0,9.9932495454069983E-3,0.2729073978244565,5.9118561676137196,0,1.9279430186412413E-2,0.10134428650864824,-6.8751377305542355E-4,4.1150422895875262E-2]
[null,1795,0.99521225527111279,1.0153926975541896,1.0080208848054686,1.0179235035641228,1.0053837746561605,1.0144442649437739,1.0158071114534102,null,6.7566481109782552,0,1.0480867844006567E-2,0.1977385952726104,0.12167274057882371,8.3767576849916925E-2,0,1.0480867844006567E-2,0.27681689481740152,5.9126488743158729,0,1.9181320209513901E-2,0.1036627903559118,-1.999029678485963E-3,4.3158348256686629E-2]
[null,1796,1.0171636786149763,0.97849950291472831,1.0181381666525937,1.0381590869798911,0.9750534287779421,0.97616806547726531,1.0039393385847062,null,6.7318028895507274,0,9.9371098301035184E-3,0.19030817332838829,0.12063323025235263,8.4241029809213136E-2,0,9.9371098301035184E-3,0.26449116640825115,5.9131660900687049,0,1.9063102601621154E-2,9.9270079178056317E-2,-2.892316366175925E-4,4.0919249540752343E-2]
[null,1797,0.95894852706626865,0.98518575048530665,1.0074317260578762,0.98011548537069237,1.0159577695451347,0.99030407776638929,0.99305581613495464,null,6.771347431703691,0,1.0762160631014057E-2,0.20286859531322274,0.1278202259654731,8.3733139277370514E-2,0,1.0762160631014057E-2,0.27880900878395537,5.9106392392430953,0,1.9388471422289454E-2,0.10638317428257371,-2.6110844696226442E-3,4.4316661885333862E-2]
[null,1798,0.9921998128269347,0.97179863703209834,1.006226549756966,1.0428357474273637,1.023602978942608,1.0008148725797883,1.0119367597096716,null,6.7620436627236113,0,1.0584868428986679E-2,0.19917086012198859,0.12423765009244458,8.366014319926493E-2,0,1.0584868428986679E-2,0.27575195953425663,5.9140966423911783,0,1.9197951652940966E-2,0.10450645981309753,-2.1646082357845648E-3,4.3586604154220693E-2]
[null,1799,1.0057368285771131,1.0003118332012937,0.98009916880956527,1.0082691414073468,1.0250150178161248,1.0379175778034555,1.0224363764720374,null,6.7599803083062815,0,1.0942892075994746E-2,0.19808591264595934,0.12164098089589701,8.2039034532379138E-2,0,1.0942892075994746E-2,0.27806560092852678,5.9136873167165849,0,1.9123997003835696E-2,0.10529845886876808,-3.0218750924388502E-3,4.5060881806766317E-2]
[null,1800,0.98715109582025629,0.99555420699167108,1.0278124124207377,0.9959672280940447,0.98600121473847024,0.98100480961536995,1.0013163593637509,null,6.749442720621639,0,1.0127882425345255E-2,0.19675683556896376,0.12325871883682599,8.491478924684516E-2,0,1.0127882425345255E-2,0.27213608389897814,5.9103306766618928,0,1.9226052816087729E-2,0.10214653792614276,-1.0317914658011305E-3,4.1704817131701703E-2]
[null,1801,1.0189933107972937,0.95323688767060988,1.0111642463695669,0.98253499602981242,1.0312364585699034,0.98904536139385091,1.0449179501041994,null,6.7479514961509768,0,1.022570488706688E-2,0.1938244030084354,0.12181477679829741,8.3928429260525614E-2,0,1.022570488706688E-2,0.27631875750750101,5.9105583497295049,0,1.9053479221186085E-2,0.10145292666590797,-1.1072586577055602E-3,4.2107632617322262E-2]
[null,1802,1.0350850660812376,1.0072496163148219,1.0152377755219397,0.98247004903964286,0.98152540807882882,0.99094913323966738,0.96714440773201704,null,6.7070880134954312,0,9.8155764318740794E-3,0.18717565194445915,0.11723214164598671,8.3842543344379433E-2,0,9.8155764318740794E-3,0.25142920710818273,5.9103229980464977,0,1.8970306275182501E-2,9.7775850883127E-2,-7.9482391370388675E-5,4.0418796638981999E-2]
[null,1803,1.017110063504318,0.97621546344206755,1.0171848367787903,0.97411222508338691,1.0140617818547719,1.0133802882297454,0.99373789287892278,null,6.7406127997907967,0,1.0335423995838122E-2,0.19765739991325157,0.12077029700821136,8.4146137814339259E-2,0,1.0335423995838122E-2,0.26530096250823343,5.9097603031581318,0,1.9063385125039682E-2,0.10315211734331466,-1.7972394576994094E-3,4.2559436377968878E-2]
[null,1804,0.99675181219840692,1.0038890259080755,1.0145781707000978,0.99442188717806779,0.98639683509943277,0.99418030239532318,1.0017697698782217,null,6.7450802814437765,0,1.0246859655915758E-2,0.19520925869489511,0.12191599627581784,8.4075453195660316E-2,0,1.0246859655915758E-2,0.27078288410397228,5.9110063615943522,0,1.917285926116442E-2,0.10200561183735968,-1.282887709479209E-3,4.219474419003346E-2]
[null,1805,0.99069400544522257,0.96326671103796246,0.9894691622852626,1.0222352581074154,1.0274108359097753,0.98521402786463042,1.0080044337907672,null,6.7547797782616907,0,1.0629682897202536E-2,0.19510896856253862,0.12518756899651159,8.2575365136784637E-2,0,1.0629682897202536E-2,0.27364623657465398,5.9139235095184617,0,1.9206303004898246E-2,0.10323146244940319,-1.870778139219457E-3,4.3771142157655596E-2]
[null,1806,0.98608366318146368,0.97672523375010223,1.0047099278474965,1.0339419137544525,0.9979888731977451,1.000557662336393,1.0143279063744055,null,6.7654880561072925,0,1.0638817765699226E-2,0.19973690055703311,0.12478480112411017,8.359063055655569E-2,0,1.0638817765699226E-2,0.27803414935845289,5.9137017799939828,0,1.9232030997960638E-2,0.1048822575353605,-2.2832519363456022E-3,4.3808757920178992E-2]
[null,1807,0.99545070067713992,0.97051143167642029,0.99955770044647074,0.99767231441230919,1.0478942203711781,1.0369148527567398,1.0129190129973074,null,6.7717139725958475,0,1.1000992673355059E-2,0.20496626943713833,0.1240248211542803,8.3251388891597417E-2,0,1.1000992673355059E-2,0.2786285393098058,5.9120319710470959,0,1.9180008071466879E-2,0.10790371784430881,-3.5728728850263638E-3,4.5300129725175269E-2]
[null,1808,0.9958412855050538,1.008958135891812,0.99017678731605008,1.005311765635766,1.0090087097824432,1.0272322789665957,0.99304354515571835,null,6.7538419022049769,0,1.0802254421328546E-2,0.1984846632616292,0.12223992110208667,8.2580658125611647E-2,0,1.0802254421328546E-2,0.27167445811133928,5.9129693956007197,0,1.9177860085071181E-2,0.10498047689911155,-2.7472919580162737E-3,4.4481760977420258E-2]
[null,1809,0.99807733841945423,0.97041199939645928,0.98457360303953934,0.99860050668018996,0.9929253359668071,1.0284136288418051,1.0105345777678252,null,6.764350985041566,0,1.1025823984903716E-2,0.20091628953186277,0.12398713362719034,8.2289505144977931E-2,0,1.1025823984903716E-2,0.27639415118273131,5.9129175900349669,0,1.9165595473584412E-2,0.10656424481052615,-3.2859054105999178E-3,4.5402380646323959E-2]
[null,1810,1.0031165954505521,0.99919114275729248,1.0314331540553903,1.0062698163109793,1.0161462884937196,1.0011903025472393,0.98637583642683757,null,6.7421779503355213,0,1.0123715762016273E-2,0.19773138268432117,0.12105154233392025,8.5056104678370575E-2,0,1.0123715762016273E-2,0.2656536923837759,5.9106778083220863,0,1.9138155926345605E-2,0.10247026882504889,-1.2886643721080021E-3,4.1687659553751387E-2]
[null,1811,1.0367106560048107,1.0136370300149211,0.98177696419299787,0.96340657182400813,1.0187703326077968,1.0236815638373382,0.99744341137827996,null,6.7213323885762488,0,1.0395964922249E-2,0.18865455641984327,0.11735383894675151,8.1893795820796714E-2,0,1.0395964922249E-2,0.26173850773676349,5.9111696049956004,0,1.8962047732184066E-2,0.10020076033716473,-1.4494565498995445E-3,4.2808733137045689E-2]
[null,1812,0.99411504003968898,0.99313578274986802,0.98813498300575442,0.96464817849876183,1.0295844452745169,1.00895420721518,0.99087340867204088,null,6.7478897984369972,0,1.071974525353195E-2,0.1963732222254827,0.12326723009772471,8.2402385165749464E-2,0,1.071974525353195E-2,0.27000021058889762,5.9108849364701292,0,1.9187366172848497E-2,0.10396955758304344,-2.3371127773966836E-3,4.4142002910518285E-2]
[null,1813,1.0038058707597812,0.96119709458641311,0.97989570802925263,0.95944159663002171,1.0004940336942718,0.95486912547103464,0.96777600038637124,null,6.7184465444455519,0,1.0262424839272243E-2,0.1857121694587115,0.1238389121660203,8.170710522082672E-2,0,1.0262424839272243E-2,0.25649477550493449,5.9110589113534227,0,1.9134424132741395E-2,9.8730885314223027E-2,-4.8947754992056708E-4,4.2258838844596108E-2]
[null,1814,0.99426538485486193,0.95626301816104231,0.98555011802947956,0.98894278407111136,1.0100407652609809,0.97908908116630045,1.0072541784511242,null,6.7487264715257806,0,1.0594817647273432E-2,0.19334215956212561,0.12517727332408549,8.228462088281191E-2,0,1.0594817647273432E-2,0.27193508687047052,5.9123414764470699,0,1.9186536941842816E-2,0.10249696786472652,-1.6652236315841131E-3,4.3627573264230689E-2]
[null,1815,1.0059095474041593,1.0268138138199889,1.0035958136537473,1.0219655452547227,0.98064636011293815,0.9546703126778161,1.0182050967078411,null,6.7239044318966208,0,9.7494504320460255E-3,0.18273783376824509,0.11992323149636459,8.3386641302762146E-2,0,9.7494504320460255E-3,0.26875891437243382,5.9131174831299571,0,1.9123066276569182E-2,9.6009030326976261E-2,7.0172968162785941E-4,4.0146501541679272E-2]
[null,1816,1.0290249311845105,1.0093116696205791,0.97051802677444099,0.9731289184207117,1.0304090596881443,0.98273177766407815,1.0137442752692554,null,6.7155335269168948,0,1.0172366330157893E-2,0.18153805214346416,0.11863464935068214,8.123349636799708E-2,0,1.0172366330157893E-2,0.26424153496050007,5.9123126407229663,0,1.9001323746751047E-2,9.6966912879237019E-2,-2.8307718858555035E-4,4.1887993933880256E-2]
[null,1817,0.98140621638818137,0.98182687171489491,0.98585723009451365,0.96665896174481214,0.96479399890569295,1.0099209748205986,0.96531362203746052,null,6.752542925372425,0,1.0944161636171177E-2,0.19980823462338845,0.12548033580818932,8.2218679171101691E-2,0,1.0944161636171177E-2,0.26664884956969731,5.9111199169056894,0,1.9258380494935997E-2,0.10590859527245042,-2.9661761026258567E-3,4.5066109629599595E-2]
[null,1818,1.0204917991565632,1.0167655937615729,1.0231815196829921,1.0187160295108251,0.97088939144424613,1.0064671960649199,0.97608944695001043,null,6.7260698800485512,0,1.0001433450842021E-2,0.19297432547989865,0.11831595487266178,8.4459480479585874E-2,0,1.0001433450842021E-2,0.2587020115714852,5.9118263743080357,0,1.9045623273867003E-2,0.10041112257744263,-8.491352762024486E-4,4.1184122761775806E-2]
[null,1819,0.99546911184215015,0.96280481841156829,1.017207109894019,1.0347507660447828,1.0038745395299704,0.96506847305632615,0.99474159142387419,null,6.7427839579697437,0,1.0116302041264853E-2,0.19347322917077639,0.12407999539051358,8.4214848486388341E-2,0,1.0116302041264853E-2,0.26687391432508861,5.913035209068938,0,1.9179906783054063E-2,0.10096740134938005,-6.9767777569062128E-4,4.1657131171290128E-2]
[null,1820,0.97399329053877604,0.98249095176882861,1.0354738423649661,1.0044044787688482,0.99931966757412005,1.0180676840270966,1.021385747966459,null,6.7838706646822482,0,1.0641265673038958E-2,0.20908471996652606,0.12543494122151452,8.5574926860927103E-2,0,1.0641265673038958E-2,0.28517885978804425,5.9103425235455243,0,1.9300658153513599E-2,0.10813962911570726,-3.0044319363993059E-3,4.3818837966892746E-2]
[null,1821,0.9999756508189348,1.0182268348186514,1.0372026246038135,0.99654151382409861,0.97723729432700146,0.99879392132485334,1.0223885119665543,null,6.7497268606970096,0,9.9989621218708642E-3,0.19696689731819711,0.12040948456910822,8.5545002826196218E-2,0,9.9989621218708642E-3,0.27580892763806314,5.9098172253745114,0,1.9155226396444534E-2,0.1017860927049155,-9.3594239937783131E-4,4.1173946268952752E-2]
[null,1822,0.99662657827831325,0.97797620100894456,1.0084850368373464,1.0143783075778805,0.98172930235885147,1.0321911613253318,0.98178037877070479,null,6.7604573882901828,0,1.0817356367724762E-2,0.20422729715258026,0.12332971268636085,8.3691336371307962E-2,0,1.0817356367724762E-2,0.26922465935291312,5.9124310038086243,0,1.9173546532953313E-2,0.10703984366286765,-3.2039593820649202E-3,4.4543948104633642E-2]
[null,1823,0.98340769518557281,0.9943415315514853,0.9671840420573653,0.98235386915296952,0.99856648570982853,0.97754395350982282,1.0137936539619423,null,6.7482819386439203,0,1.0686994151799236E-2,0.18978033424829294,0.12494466942442886,8.1190945138396892E-2,0,1.0686994151799236E-2,0.27614394356489963,5.9129929110258193,0,1.9247074868587816E-2,0.10153959131899695,-1.5646706485724299E-3,4.4007139703061776E-2]
[null,1824,1.0121348310622678,0.98965778327726306,1.0398034779756411,1.0122240752351106,1.0128582083570856,1.0186366237302298,1.0098479241888665,null,6.7520882164473415,0,1.0175401820700947E-2,0.2012141493225123,0.12027568439944882,8.5654355942990409E-2,0,1.0175401820700947E-2,0.27131267358768063,5.9105125686431839,0,1.9089732241716117E-2,0.1038488044582196,-1.72024569205744E-3,4.1900493543639374E-2]
[null,1825,0.9756679015251607,1.0106913559055908,0.97522295448497776,0.9999005169841253,0.99516367094629765,0.99554978110746672,1.0130811568437539,null,6.7596134346265648,0,1.0817830894207632E-2,0.19441022828995824,0.12496536870637392,8.1753252636658946E-2,0,1.0817830894207632E-2,0.27975420665804895,5.913502860632736,0,1.9291051281730039E-2,0.10359741261567834,-2.2068483148490552E-3,4.4545902120227555E-2]
[null,1826,0.98483152935394092,0.99871684856939469,0.9734579196403258,1.0078520583723527,1.0000672631919099,1.0018861781732165,1.006620609017729,null,6.7561580851106902,0,1.085725540710614E-2,0.19460822508525347,0.1244274059281532,8.1600152139892509E-2,0,1.085725540710614E-2,0.2761096192406336,5.9140294235928605,0,1.9239060119970123E-2,0.10379482382076057,-2.3588700638707849E-3,4.4708245247041888E-2]
[null,1827,0.95844080136144105,0.98375189279932462,1.0258159784229692,0.99891606937047572,1.0200809963763884,1.0300411694173848,1.0303909584085924,null,6.8022060679148275,0,1.1028064908775283E-2,0.21361342037974437,0.12759779524519843,8.5088258443048487E-2,0,1.1028064908775283E-2,0.29355019810013644,5.9106051141917364,0,1.9391483003661249E-2,0.11100646377313329,-4.0582735937962147E-3,4.5411608371957485E-2]
[null,1828,1.0033189568820846,0.98885993766124014,0.97977657764003223,1.0236673661945406,1.008001757275937,0.98913395909135637,0.99492870844540438,null,6.7379170006189542,0,1.0508339696754252E-2,0.19012871562496592,0.12250300669517272,8.1881273290054998E-2,0,1.0508339696754252E-2,0.26678798387205543,5.9145375154445397,0,1.9137059793098484E-2,0.10108490090075932,-1.4149274581914974E-3,4.3271472456494084E-2]
[null,1829,1.0016714643869522,1.034777849634795,1.0417272541004541,1.0112522340380379,0.97030715384750521,0.99637638826216257,1.0087340289550628,null,6.7419827986003877,0,9.8502292583720064E-3,0.1953382609396736,0.11934780359059424,8.5772876735375259E-2,0,9.8502292583720064E-3,0.27129583122597117,5.91034764795429,0,1.9145996657453063E-2,0.10072150824535152,-5.4861755885309428E-4,4.0561490810527255E-2]
[null,1830,1.0270456191387267,1.0285634134801205,1.0010120560523885,1.0041360404568305,0.96354491672156251,0.9935607405392215,0.97734424427080713,null,6.7122101775338496,0,9.9530104704733963E-3,0.18584064054277058,0.11742198124732137,8.3042094750759771E-2,0,9.9530104704733963E-3,0.25609515790403659,5.9122995286005064,0,1.9011533721718651E-2,9.7764471985410606E-2,-2.4995676626324466E-4,4.0984725547587017E-2]
[null,1831,0.97839514884444923,1.0030473263414998,0.99258626913958292,1.0175410176644188,0.99163202584897991,0.97423179165478346,1.0278952821561349,null,6.7570858588450795,0,1.0431897590881456E-2,0.19236546961053316,0.12466648508794213,8.286555459923671E-2,0,1.0431897590881456E-2,0.28105359008584002,5.9134961086855489,0,1.9275476059338333E-2,0.10162186950454299,-1.2153922585981312E-3,4.2956697470697552E-2]
[null,1832,0.99908561967483622,0.97355852907601603,1.0159914102592784,1.0244278973450793,0.99738901079920017,1.0001329672066293,1.0073383379328773,null,6.7550159642306147,0,1.0407342957645964E-2,0.19868164148176026,0.12310601751276871,8.4208578381873678E-2,0,1.0407342957645964E-2,0.27253874656433352,5.9125469468552696,0,1.9160083072220686E-2,0.10374769927810497,-1.8293347773128642E-3,4.2855585861595588E-2]
[null,1833,1.0077286277483641,0.96202817069129598,0.96009901080544513,1.0093559151728044,0.97768757466054002,0.98689718407950078,0.98438562259728712,null,6.7337605610290145,0,1.0745062895281012E-2,0.18881382201381991,0.12368257926390573,8.0592491038460251E-2,0,1.0745062895281012E-2,0.26283874511217969,5.9148367033901126,0,1.9113283201281871E-2,0.10138390320927376,-1.7472226528905067E-3,4.4246256452868678E-2]
[null,1834,1.0109813194134469,0.960047237685143,1.044910374431812,1.0017953833825124,0.97429884232218755,1.0122155912821942,1.0145017184589102,null,6.7574464057299615,0,1.0209636624024467E-2,0.20341956913778642,0.12178681883702698,8.5979701779964751E-2,0,1.0209636624024467E-2,0.27261409330214414,5.9096504630081803,0,1.9095877873331855E-2,0.10472566282375909,-1.8672474023892674E-3,4.20414663701578E-2]
[null,1835,1.010340468644817,0.98988975944765478,0.99929885850118216,1.0118469675979038,1.0033175985731655,0.97389564708116705,1.0081158783381308,null,6.7314668792158878,0,1.0096503657271497E-2,0.18804205226726972,0.1212392959028301,8.3089131441381761E-2,0,1.0096503657271497E-2,0.26702898663441982,5.9128125539215395,0,1.9099298235316489E-2,9.9006757122420991E-2,-4.2680125928025404E-4,4.1575604949986474E-2]
[null,1836,1.0365089566021977,0.98661503438448284,0.97432944891745277,1.0123215637291827,1.0174769291378394,0.97008178076514029,1.0100919420929491,null,6.711379525777514,0,1.0033157315446198E-2,0.18006967757808379,0.11878609845762234,8.1448154384363106E-2,0,1.0033157315446198E-2,0.26043379067061073,5.914223354335892,0,1.8963071025249776E-2,9.5998644029053989E-2,1.4197930705936844E-4,4.1314755989578414E-2]
[null,1837,1.0003613013879027,0.96640201847316176,1.0177528756990932,0.98605635550324089,1.0114071188261795,0.9868275515413365,0.97954035147828444,null,6.7405912894866811,0,1.0272443013785099E-2,0.19661811343331317,0.1232786955652314,8.4166988080928568E-2,0,1.0272443013785099E-2,0.26351482710734864,5.9103731560354076,0,1.9153124681998174E-2,0.10258100437324075,-1.3947116948551605E-3,4.2300091904071434E-2]
[null,1838,0.9872567984305729,0.96366996999435173,1.0291857549929884,0.99365874479602123,1.0213898798005216,0.96881408123342327,0.97356198572685682,null,6.7429962157875263,0,1.0129278949208589E-2,0.19718390164455377,0.12483389438565246,8.488287458217636E-2,0,1.0129278949208589E-2,0.26372991419931802,5.910126647219883,0,1.9225461529553959E-2,0.10229926086797865,-9.9630640998900886E-4,4.1710567768398932E-2]
[null,1839,1.0249477368459268,0.97772589861648285,1.0074241796104582,0.97912605548077392,1.0055622349726834,1.0111734845925937,1.0068483174828136,null,6.7369656139044771,0,1.0314968226605615E-2,0.19443676828994647,0.11995381507689648,8.3561256523302749E-2,0,1.0314968226605615E-2,0.26650565279906341,5.9105862011581225,0,1.9022398370786935E-2,0.10196195159812464,-1.5376330730292966E-3,4.2475203161260626E-2]
[null,1840,1.0080038800586779,1.0306654179530936,0.97924577943769098,0.98693264536908809,0.98733849127204376,1.0224149056609129,0.995926199829963,null,6.7379921542596266,0,1.0626353874357066E-2,0.19211260065815206,0.11994035632269971,8.1844202659731288E-2,0,1.0626353874357066E-2,0.26849157385066041,5.9125808520204766,0,1.9111805960754499E-2,0.10216681965715491,-2.0134907041283508E-3,4.375743383412193E-2]
[null,1841,0.96990669431270271,0.97158229797564333,0.9930900589249162,1.0014643678561086,1.0084133208013835,1.0090835278258687,0.96374137732184273,null,6.7650056282060547,0,1.104467830504934E-2,0.20381736514046236,0.12736125495678424,8.273095272990473E-2,0,1.104467830504934E-2,0.26941900888356024,5.9125990687074976,0,1.9324241305426055E-2,0.10764460477948518,-3.3708876778019304E-3,4.548001938073977E-2]
[null,1842,0.98706656187014141,1.0104433150542118,1.0133171076772187,1.0065700338175501,1.0431867768434975,1.0345159833849618,1.0009608250725543,null,6.7673199458552142,0,1.0749106918211841E-2,0.20439556930629491,0.12281620182147884,8.40909569849735E-2,0,1.0749106918211841E-2,0.2769925911543295,5.9117345791680513,0,1.9226525779049902E-2,0.10687240379289244,-3.0717911713446324E-3,4.4262909019488594E-2]
[null,1843,1.0011994754833611,0.97893623535819918,0.98259536133263969,1.0299866876306083,1.0227196242428194,1.0398028632473135,0.96062705855048447,null,6.7525256482772908,0,1.1090689563099365E-2,0.20150614490113999,0.12320589911220875,8.2009489555211715E-2,0,1.1090689563099365E-2,0.26286107916590601,5.9147236133872285,0,1.9148562393136979E-2,0.10698286068952959,-3.5814864787601739E-3,4.5669485551691119E-2]
[null,1844,1.0333725329270536,1.0285420414791526,0.97298210494654913,1.0003604737949781,0.98544203575116829,0.97748369947374347,1.0123283133318048,null,6.7086141195439666,0,9.9729865664770039E-3,0.17863214947866857,0.11720345214198645,8.1378202632866076E-2,0,9.9729865664770039E-3,0.26212460279465605,5.9136504148299567,0,1.8979034623568879E-2,9.5296704912603503E-2,2.8257457434590591E-4,4.1066983555317349E-2]
[null,1845,0.96929946962651159,1.000964285572989,0.9833726863165414,1.0112177938411731,0.96221118801493866,1.015143012911863,1.0240759771481835,null,6.7787919474512792,0,1.1070369929018494E-2,0.20136901246498007,0.12611802658046056,8.2362331738533856E-2,0,1.1070369929018494E-2,0.28671222033743043,5.9136660573961999,0,1.9327762479764522E-2,0.10686850275147013,-3.2177792128711617E-3,4.5585812915306161E-2]
[null,1846,1.0148998647777157,1.0207856379886691,0.98760759595133651,1.0094635964960568,0.9984930969776673,0.96627628020754119,0.99398683837518742,null,6.7148233271895208,0,9.9430779929717862E-3,0.1820031992317476,0.11943335342072481,8.2282365595073209E-2,0,9.9430779929717862E-3,0.26112151715056409,5.9133366244220689,0,1.9075057687845023E-2,9.63867343737283E-2,2.4064993461343794E-4,4.0943825373150493E-2]
[null,1847,1.0054539093285217,1.0364996906094566,1.0006640838531466,1.0185024102146694,1.0202028751489485,1.0065755683674107,1.0107788238126498,null,6.7403033035476199,0,1.0269232078051206E-2,0.19164625204852095,0.11958176411248581,8.3241490571195301E-2,0,1.0269232078051206E-2,0.27168895114947206,5.9130954908991296,0,1.9125522257286677E-2,0.1008360262141324,-1.1990635468537758E-3,4.2286869842244522E-2]
[null,1848,0.9809314252677146,0.96980911813859338,1.0240926025230623,1.0052219721087434,0.98861485761082812,0.98420048107057867,0.98085165039729538,null,6.7548478567564016,0,1.0374523973619303E-2,0.20044287628954011,0.12541986662147125,8.464674057340113E-2,0,1.0374523973619303E-2,0.26881772498720224,5.9110449929116831,0,1.926106918768997E-2,0.1042505362874126,-1.756393228932782E-3,4.2720443126935188E-2]
[null,1849,1.0182021782350963,1.0292891881117476,0.96182766240023121,0.97668324139623752,1.0083828411720104,0.99761763790311531,0.98645405820968157,null,6.7170371069855506,0,1.0427601785544818E-2,0.18370657391610454,0.11911482120446203,8.0653049684785247E-2,0,1.0427601785544818E-2,0.26102208130923688,5.9129765409729895,0,1.9057636124718433E-2,9.8555548460982911E-2,-9.8815279667754247E-4,4.293900810894611E-2]
[null,1850,0.9741768800569095,0.99669418839005353,0.99262044877723776,0.9991561194529559,1.0159223081968267,1.0212258255060718,0.97897104460094697,null,6.7657743514647342,0,1.1012052310346352E-2,0.20307388204065133,0.12552427407593164,8.2752158527540601E-2,0,1.1012052310346352E-2,0.2733506736582122,5.9125005158438189,0,1.9299603329181264E-2,0.10727702960938855,-3.3494569617551033E-3,4.5345671341763434E-2]
[null,1851,1.0370550289069662,1.0209899081201701,0.9742154878512167,0.98291215175102575,0.96965575992186537,1.000617425042458,1.0353585685222282,null,6.7215109441602561,0,1.0193936477768929E-2,0.18292431005248411,0.11711023653429296,8.1537392194160563E-2,0,1.0193936477768929E-2,0.26935776042863074,5.9126395814429058,0,1.8960301525496191E-2,9.7526081934032838E-2,-5.2153591415162077E-4,4.1976815962399362E-2]
[null,1852,0.97489704984269843,0.96038368081645598,0.99288609084135038,1.01523995954486,0.9767528920257621,1.0278774591552879,1.0154193096966133,null,6.7867570139414477,0,1.1250586533537247E-2,0.20755441473198366,0.12730222934648261,8.2927785062331463E-2,0,1.1250586533537247E-2,0.28442648828172279,5.9133550061952667,0,1.9295469387330736E-2,0.10962943582714083,-4.0617277061712623E-3,4.6327912815354554E-2]
[null,1853,1.0218132225803118,0.98139845273493154,0.98548547085560811,1.0261257847573149,1.0312324954803544,0.99926816220940562,0.99059695340030962,null,6.7300014464722366,0,1.0405824679733481E-2,0.18987506906532697,0.12054615237349563,8.2171401949578809E-2,0,1.0405824679733481E-2,0.26183492427194532,5.9143549887043498,0,1.9038714722284106E-2,0.10066220140328566,-1.3313398814264385E-3,4.2849333863395379E-2]
[null,1854,0.99212672479778574,1.0209640034646221,0.99677463354420204,1.0439029841462064,0.99787839817245128,1.0046140558707473,1.0048795423627082,null,6.7513056375556291,0,1.048980658673271E-2,0.19463777686565426,0.1219952045556728,8.3045826383330593E-2,0,1.048980658673271E-2,0.27368473515697017,5.9146866458312513,0,1.9198356420784459E-2,0.10260815157114588,-1.7462156373760597E-3,4.3195156408195989E-2]
[null,1855,1.0247371187410499,1.0038198638640297,0.97523553015062969,1.0107570104138079,0.98469713594636854,0.99281708933933277,0.99075522622207213,null,6.7196175126566766,0,1.030148648833016E-2,0.18513431576500092,0.11930633551826336,8.1502518677090005E-2,0,1.030148648833016E-2,0.26030332047006299,5.9140891161468936,0,1.9023491590748502E-2,9.8653837633040045E-2,-8.15110907125863E-4,4.2419687762702253E-2]
[null,1856,0.97887059989348291,1.0456011538939698,0.98811660329414286,1.0075859129355051,1.0314904859603797,0.99965079405120427,1.0432124807683627,null,6.7624066433121266,0,1.0551406863120141E-2,0.19328419169841593,0.12263579000298276,8.2661921851254497E-2,0,1.0551406863120141E-2,0.28723070919855437,5.9132068645379761,0,1.9272769657526743E-2,0.10233501287518866,-1.6694318916924611E-3,4.3448815381918977E-2]
[null,1857,1.0215270244576857,1.0123286130781544,0.99251619151290349,1.0156808886685367,0.99924009721919171,1.0361103560109379,1.0170325548562862,null,6.7458101168250506,0,1.0584862459948143E-2,0.19516588642750834,0.11896487743037512,8.2736615768623734E-2,0,1.0584862459948143E-2,0.27203811350325485,5.9133994807133421,0,1.904020948219939E-2,0.10310485893948872,-2.2265050145274571E-3,4.358657957478243E-2]
[null,1858,1.0248827196672488,0.98447747655422013,1.0025934266438683,0.964812024817015,1.0032362702807451,1.0014229410372413,1.032519076753506,null,6.7375651806494092,0,1.0229160635356407E-2,0.19144478836820658,0.11972076037693091,8.3329238604764141E-2,0,1.0229160635356407E-2,0.27230109533984342,5.9100854045689815,0,1.9022735796573965E-2,0.10063361787264831,-1.0943230522177246E-3,4.2121862773678263E-2]
[null,1859,1.0387245356474479,1.0213284137950789,1.0255422391606153,1.0145702019536635,0.99364609400448878,1.0307462859350238,1.0231499421861254,null,6.7348435210632589,0,1.0022896640830352E-2,0.19406476153910399,0.1159884356530838,8.4736209021368386E-2,0,1.0022896640830352E-2,0.26861035947049222,5.911466535240697,0,1.8951852394844478E-2,0.10086136525867065,-1.1085018728480337E-3,4.1272504357842361E-2]
[null,1860,1.0313252323861151,0.99747556620653788,1.0157455775554278,1.0193014471002106,0.99667684047534566,1.0127928230060395,0.99494389427494179,null,6.7292189193704495,0,1.0106160171895862E-2,0.19286173408070054,0.11811004288528368,8.4040054209679693E-2,0,1.0106160171895862E-2,0.2616790440490166,5.9122840049831149,0,1.8989507237290773E-2,0.10072087322565905,-1.0817100587162535E-3,4.1615368758414088E-2]
[null,1861,1.0209746132798674,1.002081455807974,1.0200257749028911,1.000846201384838,1.0149702275079076,0.99571722301782684,1.0211730258451712,null,6.7351691509179945,0,9.979259790442398E-3,0.19164983560675436,0.11900862351680735,8.4400318697161469E-2,0,9.979259790442398E-3,0.26965051622621355,5.9110421076746782,0,1.9043096993516105E-2,9.9876981876572068E-2,-5.9514524872101866E-4,4.1092815575014596E-2]
[null,1862,0.99265634103067446,1.0011085812577163,0.97900564621887887,1.0145764065225018,0.99435650983970791,0.9883464304730718,1.027804875158183,null,6.7513149261587859,0,1.0564032222577071E-2,0.19091785796485272,0.12322506025893612,8.1980168893652491E-2,0,1.0564032222577071E-2,0.27836217203046953,5.9140885055855161,0,1.9195424709090209E-2,0.10154366011080278,-1.4987277594733937E-3,4.3500804364932408E-2]
[null,1863,1.0426721797578968,1.0081884134750012,1.0105529992172961,0.99834533192015118,0.99937705832398438,0.97402985331267544,1.0264232646300753,null,6.7115897871468517,0,9.6132790306100967E-3,0.18205130161784808,0.11642016888803391,8.3724807536024015E-2,0,9.6132790306100967E-3,0.26331702073980678,5.9114473500112581,0,1.8931981571706422E-2,9.5319370765912056E-2,7.9201406808833788E-4,3.9585771948172033E-2]
[null,1864,1.0300913010083255,1.0013085670508348,0.97975126849601368,0.99649219609454853,0.9759075404589943,0.98975539400871282,1.0166092438513663,null,6.7218173435784703,0,1.0187138387254985E-2,0.18431025859400105,0.1187239809688795,8.1840890122715754E-2,0,1.0187138387254985E-2,0.26545453107627764,5.9130698184448303,0,1.8995839306982714E-2,9.7992669281299419E-2,-5.1946685219691482E-4,4.1948822635677924E-2]
[null,1865,1.0383195432316894,1.0408716863956917,0.9835668861039828,0.96089550916274824,0.98824207813541665,1.0300946728367384,0.99832078372342758,null,6.7180182705458886,0,1.031095358841074E-2,0.18760933319363268,0.11590437778106868,8.2004960349059394E-2,0,1.031095358841074E-2,0.26187609181501881,5.9109350601807948,0,1.8953899506413886E-2,9.9556439106364261E-2,-1.2805629822160926E-3,4.2458671595753075E-2]
[null,1866,1.0245940282774426,1.0171906707564453,1.0053692887947707,0.98520952266671669,1.0174144916806895,1.0044797018897591,0.96060613766769276,null,6.7148885042255273,0,1.0096060210074172E-2,0.18973215629139156,0.11814830901381371,8.3261667471958747E-2,0,1.0096060210074172E-2,0.25337192208602027,5.9110311154388242,0,1.9024234562742715E-2,9.9596193632319058E-2,-8.5087318490745603E-4,4.1573778913358554E-2]
[null,1867,0.97021355121420916,0.99511209200431427,0.99847781367228772,0.99353084819424564,0.97714834303402787,0.99790034105867842,1.0122738079550306,null,6.7692575031495359,0,1.0756687820967097E-2,0.20009407878195443,0.12600404508496515,8.3222036546501274E-2,0,1.0756687820967097E-2,0.28153403831397344,5.9118687775778129,0,1.9322463580166406E-2,0.10539530338414058,-2.477365947665277E-3,4.4294125827684348E-2]
[null,1868,1.0238610138657274,0.96424855264004194,1.0236138046665579,0.95327685574864385,0.99481986057042104,1.0173230277513634,0.99664438103310871,null,6.7400914748541449,0,1.0303724239997633E-2,0.19893406623946835,0.12044681184907097,8.4521459584923339E-2,0,1.0303724239997633E-2,0.26483746069851871,5.90826632611744,0,1.9028043867574559E-2,0.10349016988644856,-1.8617658150653243E-3,4.2428902425763956E-2]
[null,1869,0.99337629591541243,0.98775728016438757,1.0378703749560458,1.0175100643733004,1.0074666237066141,0.97152643617550549,0.99596706072031727,null,6.7432398506271785,0,9.9130124589573917E-3,0.19546653368517916,0.12267849935064239,8.5497162929040985E-2,0,9.9130124589573917E-3,0.26817714793035419,5.9109108446595791,0,1.9191444383398152E-2,0.10097777051802061,-4.7957368457911866E-4,4.0820020855544766E-2]
[null,1870,0.99674172284781171,0.99348306953181409,1.0113862983737787,1.0262193772286829,0.99736569501276517,0.97838813870280539,1.0084686073351097,null,6.7440621945691941,0,1.0157625365476812E-2,0.19259727586331829,0.12248696880834202,8.3906278417638619E-2,0,1.0157625365476812E-2,0.27118374264663886,5.9129061314602076,0,1.917291462416025E-2,0.10079954963050643,-8.1796014673765226E-4,4.1827293265117457E-2]
[null,1871,1.0003076305945204,0.99467979231268877,1.0159713500086576,1.0034752480266071,0.99065989117540654,0.99703113117197251,0.99321555575058151,null,6.7437150002612416,0,1.0267689411709134E-2,0.19600976357295249,0.12190492845279483,8.412868787569236E-2,0,1.0267689411709134E-2,0.26787578456298428,5.9114160408125249,0,1.91534170794555E-2,0.10235350952835805,-1.4076490403590574E-3,4.2280517416832239E-2]
[null,1872,1.0207592362591191,1.0181242750589883,1.0111945578971597,1.0266541818198678,0.99819610112407287,0.99364031235253825,0.98283488201024061,null,6.7219005159207885,0,9.9697880512925989E-3,0.18898207452798452,0.11844206120248627,8.3731508265766821E-2,0,9.9697880512925989E-3,0.25923365066214882,5.9129405250769347,0,1.9044223638647956E-2,9.8916838881160249E-2,-4.4417897344416532E-4,4.105381263910244E-2]
[null,1873,1.0141387039981165,0.97420918047643523,1.0086004604844847,0.97482380318923145,1.0291847955736106,1.0000969122305339,1.0080862574356053,null,6.740989802456637,0,1.0316037509951621E-2,0.19479588641433773,0.12138513699947402,8.3660951197702796E-2,0,1.0316037509951621E-2,0.26866953048542946,5.910287120246787,0,1.9079089329196434E-2,0.10209080996268331,-1.4583284587347913E-3,4.2479606279754119E-2]
[null,1874,1.0248149405162337,1.0283224243462197,0.99854478518362899,0.97212883020617613,1.0194627210150367,1.0157125386843451,1.0221953428111858,null,6.7322553373072171,0,1.0220089587377376E-2,0.1901312350392706,0.11773320946446646,8.3058889836010216E-2,0,1.0220089587377376E-2,0.27048651546051389,5.910708370507221,0,1.9023087602010765E-2,0.10014425427214318,-1.1147346871081634E-3,4.2084509812686959E-2]
[null,1875,0.9797348486670252,0.97701415257194246,1.0247027926583314,0.99344012181792518,0.98249965635538383,0.95437540081594385,1.0125508699246422,null,6.7502577857908097,0,1.0035142698486084E-2,0.19406083137592758,0.12518988818700352,8.475798647293234E-2,0,1.0035142698486084E-2,0.27483298338157591,5.9103734031092765,0,1.9267856836171857E-2,0.10090094998606428,-4.4904500169660783E-4,4.1322931443551661E-2]
[null,1876,0.97146802198433324,0.98095176635052928,0.99152098562580826,0.98953261521487834,1.0209545447535606,0.97972317298537381,0.99644534254794859,null,6.7583414812754361,0,1.0676740438001115E-2,0.19656974783501455,0.1266997398246664,8.2700890218303735E-2,0,1.0676740438001115E-2,0.27514037334844854,5.9120416690007271,0,1.9315207689303313E-2,0.10389801659776569,-1.9890799735332743E-3,4.396491673473412E-2]
[null,1877,0.99568188145033254,1.0073157946912119,1.0029788509969857,1.0118848659841468,0.95653807757527098,0.99336122967173135,1.033147127462031,null,6.7534308506899254,0,1.033880446754111E-2,0.19360733275270828,0.12209934220116447,8.3485089077327726E-2,0,1.033880446754111E-2,0.27942983121863624,5.9126075188325879,0,1.9178736509902445E-2,0.10175091051083908,-1.3012669719863845E-3,4.2573356558740248E-2]
[null,1878,0.96563662592724508,0.98152779179696381,1.0114503338782583,0.9907902384914461,0.96073736069059668,1.033783570244289,0.98937841534642668,null,6.7848629946659491,0,1.1135464235626167E-2,0.21115795238868326,0.12704501898827059,8.4007712593490338E-2,0,1.1135464235626167E-2,0.28013147205256539,5.9109881517490335,0,1.9349096500991054E-2,0.11051014438877296,-4.180413679423527E-3,4.5853859683561891E-2]
[null,1879,1.0035418824631797,0.97854686944913061,1.0109081192846652,1.0079119023717356,0.96160986258927039,0.96332618361008771,1.0427544361149457,null,6.7443116479543228,0,1.0002359911498006E-2,0.18951911527423002,0.1224054315914522,8.3943556159965918E-2,0,1.0002359911498006E-2,0.27716305073082265,5.9119440960663345,0,1.913585278154243E-2,9.9211985140311348E-2,-1.993775521872338E-4,4.1187937761853317E-2]
[null,1880,1.0062260795289157,0.98686877811736129,0.98575570823494552,1.036536139025749,1.0032894970983448,0.95897552129999586,1.0107006581388811,null,6.7298490902687096,0,1.0114419487425216E-2,0.18463178054240892,0.12213659840764193,8.227040433108794E-2,0,1.0114419487425216E-2,0.26739298138766626,5.9149027428322221,0,1.9121361414161812E-2,9.786926058651424E-2,-1.2541838265290933E-4,4.1649379149660597E-2]
[null,1881,0.98962916134030487,0.99256934824102883,0.982078581275591,0.99198565975290243,0.99910192588767543,1.0049291930263959,1.0487698057550505,null,6.7667011257204042,0,1.0784816157167762E-2,0.19579859001282401,0.12396844001972826,8.22656465545029E-2,0,1.0784816157167762E-2,0.28666362766568337,5.9126978981008556,0,1.9212224072951721E-2,0.10397950403751158,-2.2947580531522257E-3,4.4409953309501482E-2]
[null,1882,0.9942880720318239,1.0415806225335653,1.0299962035692356,1.0276152675904779,0.98466049556123381,1.001331258299603,1.0108090912635259,null,6.7483846527926339,0,1.0047646563310383E-2,0.19582925684331332,0.12014051826319772,8.5101736922873567E-2,0,1.0047646563310383E-2,0.27425970511629977,5.9119140183262209,0,1.9186411831864054E-2,0.10155607645505084,-9.7749109947757856E-4,4.1374420133293156E-2]
[null,1883,1.0202888057741233,0.99733508073173827,0.97141359180042919,0.97975660092132522,1.0070782560948923,1.0168247413518139,1.0149415610144361,null,6.7375878985117401,0,1.0661477439380935E-2,0.19051997661977524,0.1202068921555858,8.1371753745304531E-2,0,1.0661477439380935E-2,0.27012991179228096,5.9126221283547036,0,1.9046686131951821E-2,0.10171873517812137,-1.9302518891139854E-3,4.3902066423128723E-2]
[null,1884,0.9629459902075177,0.98260047746251433,0.97785172360547823,0.98510934018535246,0.98223689533682113,0.97110271568110273,1.0087845221772902,null,6.7628777549800132,0,1.0796715861511669E-2,0.19478920579022627,0.12800108372735483,8.1912521089273674E-2,0,1.0796715861511669E-2,0.28011359392113183,5.9125589390604958,0,1.936487135270298E-2,0.10366263291742162,-1.9840470525152279E-3,4.4458954173921261E-2]
[null,1885,1.0255961433978413,1.0132303036640236,1.0133774910016708,0.97988965707739828,0.97316831663758741,0.99505627956005593,0.970449471852454,null,6.71439326834646,0,9.9384306266038017E-3,0.18899735112301791,0.11807098162042773,8.3773850777667525E-2,0,9.9384306266038017E-3,0.25493140812673626,5.9102895665511239,0,1.9019035614946278E-2,9.8818183155638395E-2,-4.3179696875420877E-4,4.0924688345647497E-2]
[null,1886,0.96790525751113921,1.0218699455205049,1.0096509521396577,1.0017218278595894,1.009393145352441,1.0266037228742924,1.0104347988060418,null,6.7784574257140964,0,1.0860597677603107E-2,0.20539791166915236,0.12475620539576347,8.3959271831992185E-2,0,1.0860597677603107E-2,0.28424282575303539,5.911680994655276,0,1.9335863954264017E-2,0.1075913010226552,-3.2289566900928182E-3,4.4722008122046422E-2]
[null,1887,1.0193077064216605,0.99151519941479782,1.0433651591539062,0.99743481177701965,1.0072415172661888,0.99933944642738171,1.0345366329563703,null,6.7452340491980154,0,9.8735236172738487E-3,0.19627440243157246,0.11927277933875978,8.5901394377209395E-2,0,9.8735236172738487E-3,0.27412161984705186,5.9095055445956532,0,1.905182906180268E-2,0.10112333390468413,-6.7426719296116797E-4,4.0657412834243747E-2]
[null,1888,1.0231335538720288,1.001575253499972,1.0170087081450514,0.99303764116030391,0.9897422829188538,1.004399905083063,0.99892427297417674,null,6.7304891094155295,0,1.0073780785291012E-2,0.1926034662522193,0.11883721600747787,8.413125289734863E-2,0,1.0073780785291012E-2,0.26401733982150599,5.9107928692400939,0,1.9031829703789971E-2,0.10052333571068352,-9.3023642527761735E-4,4.1482036207691288E-2]
[null,1889,0.98269724847476403,0.97320818833240463,0.95689097765509334,1.0069160362514968,0.98920421326132757,1.0058846370518109,1.0120420887283423,null,6.7643622520971052,0,1.120646436552835E-2,0.1959850863131887,0.12630877616352254,8.0599699267206712E-2,0,1.120646436552835E-2,0.27884190419667176,5.9148775833964304,0,1.9251082651659517E-2,0.10540519467785968,-3.0533001503850513E-3,4.614622558094706E-2]
[null,1890,1.0064759814864244,1.0179838346038219,1.0049690521350365,1.0075819563445312,0.98780665324574501,1.0228628404543543,1.003660588904963,null,6.7471948106465822,0,1.0466069314719131E-2,0.19656907944230467,0.12024507567605321,8.3494193255188698E-2,0,1.0466069314719131E-2,0.27120029347024632,5.9122626894486201,0,1.9120016183633862E-2,0.10320557201913395,-1.9995193957166777E-3,4.3097410547121004E-2]
[null,1891,1.0180066706755746,1.0058328536326233,0.98971939752183369,1.0084326434259883,1.0039917913184908,0.97459278907722735,0.98389829725259148,null,6.7160504053907681,0,1.0042889863130447E-2,0.18440672264292096,0.11973519270899452,8.2378525091537549E-2,0,1.0042889863130447E-2,0.25856007800038583,5.9131635347445597,0,1.9058664389473061E-2,9.7556765819463528E-2,-1.6391089517561671E-4,4.1354832888613233E-2]
[null,1892,1.0278441099439282,0.98837153131652677,0.96937487733066297,0.99544497196823689,1.0129845285531194,1.0153132615527556,1.0008610857288345,null,6.7304106734563174,0,1.0627178713987778E-2,0.18933308923999836,0.11979178275043854,8.1179892409623519E-2,0,1.0627178713987778E-2,0.26437711132709263,5.9135815397670335,0,1.9007410098516735E-2,0.10118870250272388,-1.8096850160132236E-3,4.3760830376905216E-2]
[null,1893,1.0268467902321801,0.96698282198324137,1.0082875981214274,1.0336269277545285,0.99751828113334196,0.99696602288204328,0.99194352196751623,null,6.7312771704006886,0,1.0191737124118963E-2,0.19235962096562639,0.12024626365934464,8.3578474470286976E-2,0,1.0191737124118963E-2,0.26088353415213617,5.9134823046040808,0,1.9012561525428105E-2,0.10082959622205034,-1.0829446138012834E-3,4.1967759415539152E-2]
[null,1894,0.95402048010048157,0.97430529539982369,1.033837363416175,0.97785589939919293,0.98568445835833129,1.0149736300079455,1.0159479841369017,null,6.7967962570758749,0,1.0885550874640351E-2,0.21336796147516152,0.12852326778136972,8.5513326652605443E-2,0,1.0885550874640351E-2,0.28938297415725628,5.9090036233555363,0,1.9417837631255045E-2,0.11044340630472152,-3.6809012279770204E-3,4.4824760945942302E-2]
[null,1895,1.0186935526023688,0.99432912366913184,0.969023528411738,1.0020813865642195,1.0030548068174887,1.0039303402728528,1.0018236753928396,null,6.7317205577908581,0,1.0578395483774103E-2,0.18836567317710903,0.12058401125805583,8.1183046526995387E-2,0,1.0578395483774103E-2,0.26588606003248072,5.9139595036433814,0,1.9055053502045893E-2,0.10068945936980359,-1.5621994369895034E-3,4.3559949717976582E-2]
[null,1896,1.0185003183721635,1.0160770640288495,0.97535663933765304,0.99663284581611644,1.0197855677876824,0.99093304349883726,1.0014785125912271,null,6.7229733777010363,0,1.0290196906615357E-2,0.18496466818658633,0.11945339712617019,8.1554922665274129E-2,0,1.0290196906615357E-2,0.26444584067005916,5.9133188696099461,0,1.9056068827737908E-2,9.8557448056944955E-2,-7.5103671635902219E-4,4.2373199274671328E-2]
[null,1897,0.96917375095947589,0.98366767279947254,0.98024752529011316,1.0009120744311937,0.97010924181867608,1.0268759375943193,0.99607379279309904,null,6.7783488294786549,0,1.1314513190462675E-2,0.20485800574747132,0.12707720608871889,8.2074462129797007E-2,0,1.1314513190462675E-2,0.28024168736899979,5.913281422114375,0,1.9328492048459003E-2,0.10889027790641402,-3.9938753356312581E-3,4.6591151410052704E-2]
[null,1898,1.0053318906073136,0.9672345323585253,0.99147386959632833,1.0466114384531915,1.0056896665871553,0.96967106808698922,1.0390611174674573,null,6.7472074591624969,0,1.0273508686450631E-2,0.18913262696918259,0.12312443393691408,8.2753136563023161E-2,0,1.0273508686450631E-2,0.27639370091495663,5.9151294040957278,0,1.9126180340607708E-2,9.9969432979817641E-2,-7.259367921577483E-4,4.2304480154425443E-2]
[null,1899,1.011799717077225,1.0012726751417116,0.97630421721421956,1.0208339375837672,0.9782342362518075,0.97922047858805028,1.0382128010253502,null,6.7370263291792751,0,1.029194026494786E-2,0.18525635451193828,0.12093516291343775,8.1770082125106933E-2,0,1.029194026494786E-2,0.27497255272011784,5.9145752843537966,0,1.9091516204002297E-2,9.8665967349995082E-2,-6.2096911310327314E-4,4.2380378113978358E-2]
[null,1900,1.0002157669506384,0.96942705732965784,1.0151200297163063,0.99233155085541103,1.0199788315801122,0.99510277241749734,0.98724907421012764,null,6.7456361508928593,0,1.0370081224872015E-2,0.19771518747978289,0.12319292708618604,8.404745090553814E-2,0,1.0370081224872015E-2,0.26637121676047432,5.9108625269432187,0,1.9153917623652986E-2,0.10328744143666531,-1.6966660210395684E-3,4.2702148678373651E-2]
[null,1901,0.98454577079416539,1.0411910325904181,1.0209818849043797,0.99798970824104005,1.0386608531748922,1.0215425828367959,1.0062871131712852,null,6.7598534832396506,0,1.0435617884096263E-2,0.20069775670941412,0.12151835559750529,8.4568761034968104E-2,0,1.0435617884096263E-2,0.277636250793033,5.91083297122014,0,1.924066679274395E-2,0.1045430047414616,-2.156300625588684E-3,4.2972016975968634E-2]
[null,1902,0.97519561313920577,0.98212678990080593,1.0365009574761843,0.95417507895642673,0.96320782128415061,0.97351432152143302,1.0021184717971214,null,6.7564890109093918,0,1.0155493421182179E-2,0.19984308563244249,0.12527865471792282,8.5462481159280665E-2,0,1.0155493421182179E-2,0.27511013507804477,5.9075697981542383,0,1.9293757354994938E-2,0.10330786946212536,-1.1952849476452958E-3,4.1818514297984097E-2]
[null,1903,0.97029784107819061,1.001413624310326,0.9794210745945634,1.0134974435196935,1.0243127041636999,1.0207878879031085,0.97276728873274576,null,6.7653685919684072,0,1.1156705440882568E-2,0.20175323231339359,0.12604122695543973,8.1930836990365172E-2,0,1.1156705440882568E-2,0.27258850620281322,5.9140073070016896,0,1.9321975457480069E-2,0.10728435520253345,-3.5001753413236767E-3,4.5941327186014159E-2]
[null,1904,0.9656753283888313,1.0045999338446903,0.9864203526050831,0.99295988556009429,0.99620371593102353,1.0102164915931642,0.99000140888799926,null,6.768391708713712,0,1.1011526542275222E-2,0.20120607954895481,0.12634928985654303,8.2420300272490934E-2,0,1.1011526542275222E-2,0.27770358978156795,5.9125103999073678,0,1.9348870234749259E-2,0.10661953323383069,-3.1098604442231915E-3,4.5343506322429748E-2]
[null,1905,0.99662190744795731,0.96357738512691538,0.96581809124576379,0.99004463073174054,1.011030748881782,0.9824651215678456,0.95260463828433484,null,6.7302292129277426,0,1.0754908975921728E-2,0.19059931550795534,0.12487332637523869,8.0857302426614014E-2,0,1.0754908975921728E-2,0.25677509626232581,5.9134829442518262,0,1.9173572169365202E-2,0.10204793433929786,-1.8670792652905879E-3,4.4286800860410133E-2]
[null,1906,0.99569507882576536,1.040025163653745,1.010412906450469,0.99891246835119785,0.98948331319065708,1.00872830965743,1.0236464077909282,null,6.7507875244462294,0,1.0288926869809195E-2,0.19480596683123083,0.12040879058216025,8.3918611950889357E-2,0,1.0288926869809195E-2,0.27803444245669445,5.9114859487455229,0,1.9178663938310882E-2,0.10200459133166428,-1.4174608794031362E-3,4.2367969489161675E-2]
[null,1907,1.0229352428967968,1.0029607543214545,1.0070379770062103,0.99207478257890425,1.0216555575215149,0.9886397859988586,1.0076210730662054,null,6.7256479195002203,0,9.9985877372542002E-3,0.18836526113639324,0.11897803589550955,8.3524916381979272E-2,0,9.9985877372542002E-3,0.26487520044050633,5.9113077593921757,0,1.9032862684762973E-2,9.8796966462790764E-2,-4.0548751364118259E-4,4.1172404619739304E-2]
[null,1908,0.99852552749879386,1.0152520440295842,0.99654303099040364,1.0302192408530744,1.0238491320648759,0.99659201084479521,1.0305025897203348,null,6.7508847924555635,0,1.0366313890810908E-2,0.19228037485409799,0.12149006911401254,8.3080690843231664E-2,0,1.0366313890810908E-2,0.27814523686958736,5.9139600806861425,0,1.9163143792681921E-2,0.10137706420419683,-1.2985033756572376E-3,4.2686635467270473E-2]
[null,1909,1.0042909347986573,1.0043592501977345,1.0354036674004119,0.97854846394825579,1.016492785027223,1.0101870023927202,1.0076800305031579,null,6.7486077712689259,0,1.014484924093426E-2,0.19931022280845026,0.12058562118855611,8.5366118961193865E-2,0,1.014484924093426E-2,0.27187866717863224,5.9089500560686661,0,1.913180102671206E-2,0.10308775293643602,-1.4771523580439094E-3,4.1774683458316628E-2]
[null,1910,0.95695667428933551,1.0403060280254586,1.0356266115971438,1.02852418856334,0.99327436191830698,1.0183547020623303,0.98893939746304294,null,6.7777058412015414,0,1.0570350347629971E-2,0.20773822898548128,0.12477821409402269,8.5538532706505313E-2,0,1.0570350347629971E-2,0.28044575795100901,5.9116364005573061,0,1.9400304445168944E-2,0.10743518349377118,-2.7936023110448852E-3,4.3526821279315904E-2]
[null,1911,0.97669624544381095,0.9841214654997078,0.99930653637165634,1.0133098465690082,0.982038311372876,1.0486902018950313,0.98365612865915653,null,6.7803329880373049,0,1.1274538410390196E-2,0.20998471645240546,0.12570900127006768,8.3223053375961267E-2,0,1.1274538410390196E-2,0.2767296704261018,5.9128911814283596,0,1.9285168226988614E-2,0.11055945345383157,-4.4757989773746556E-3,4.6426542380959848E-2]
[null,1912,1.0071677336762721,1.0259476857817582,0.97720941541237549,1.0048296038096718,0.9630525400806651,1.0363894338138213,1.0040587028132799,null,6.7479057548743162,0,1.082090840272199E-2,0.19503968459216903,0.12029752776876011,8.1779654221377757E-2,0,1.082090840272199E-2,0.27225043350927031,5.9136603429513412,0,1.9116295940153141E-2,0.10382935327097843,-2.6261121322522433E-3,4.4558574752513576E-2]
[null,1913,0.99222129435587259,0.99516702389035905,1.0000416410469288,0.99821340222289778,1.012699665073711,1.0206612470335654,1.0127541783880101,null,6.7625772031805962,0,1.0743067335689145E-2,0.20030426223838868,0.1231769384537215,8.3268553070462423E-2,0,1.0743067335689145E-2,0.27761687499640841,5.9120340220571777,0,1.9197832697709683E-2,0.10542407890033927,-2.6833983272840736E-3,4.4238039093665756E-2]
[null,1914,1.0008791468985028,1.0002405250270834,1.0179303059339349,0.99260166760734281,0.98772320943036518,1.0345798676332811,1.0149036022308935,null,6.7627495785181972,0,1.06046975586945E-2,0.20303087156040367,0.1215269634825118,8.4367266385400125E-2,0,1.06046975586945E-2,0.27710519123105937,5.9107166378771341,0,1.9150305080499343E-2,0.10591744842560412,-2.7333625053171072E-3,4.3668256980903972E-2]
[null,1915,0.96211488429322567,0.99898352482075747,1.0052813735342805,0.9555835243291918,1.0395461233853391,1.008412561889356,0.97757390189568905,null,6.7676364892972023,0,1.0878424177392369E-2,0.20440826749843555,0.12673480567703621,8.3532337710978122E-2,0,1.0878424177392369E-2,0.275151629313866,5.9094351463514583,0,1.9369761855947423E-2,0.10730480669396382,-3.0956802796676566E-3,4.4795414475179929E-2]
[null,1916,1.0277879585212202,1.0111757869977214,1.0397831169811338,0.99299223095648803,1.0087890464203613,0.97018978881251461,0.98143028495847184,null,6.7096953798642689,0,9.4565009798274514E-3,0.18699257355713531,0.1174295571765142,8.5413911401584219E-2,0,9.4565009798274514E-3,0.25509975639113286,5.9094750689835065,0,1.9007699870256828E-2,9.6509855154765456E-2,8.2676948886804401E-4,3.8940187840501857E-2]
[null,1917,1.007507207400173,1.0180104280806652,0.96772360947803471,1.028736957260191,1.0326319484551911,1.0045118979012693,1.0090318799698876,null,6.7385840544052753,0,1.060671456094781E-2,0.18850571148873191,0.12080398510496777,8.1183043061000992E-2,0,1.060671456094781E-2,0.27058893268765172,5.9154715333744585,0,1.9114472119036136E-2,0.1008302355777476,-1.5904216454930549E-3,4.3676562637170083E-2]
[null,1918,1.0083153016956201,0.98623690239317285,1.0079579463230608,0.99945742049414332,1.0274344447858126,1.0143151378851016,1.0229862366868137,null,6.7537550610709385,0,1.0473804617401805E-2,0.19758692263053901,0.12150047876970663,8.3730864580921188E-2,0,1.0473804617401805E-2,0.27545066120901041,5.9116546091560078,0,1.9110135576981113E-2,0.1035865044941596,-1.9943784931226293E-3,4.312926314673568E-2]
[null,1919,1.0016420882604113,0.9596086855676641,0.98226604055109523,0.99756113467374063,1.0481433841551115,0.97815478701564096,1.0215187997933428,null,6.7464723109681994,0,1.0521111201519381E-2,0.1910641449884514,0.12414389693598783,8.2108063291687003E-2,0,1.0521111201519381E-2,0.27362130462569811,5.9129889493226617,0,1.9146156275761689E-2,0.10145574607582945,-1.3800137877548906E-3,4.332406323987379E-2]
[null,1920,1.0035727431414465,1.0196332785941482,0.96522382818037589,1.0018146997266792,0.97424229186748779,0.97930309517432723,1.0012450896818461,null,6.7273974040115192,0,1.0396592380493294E-2,0.18408664682651937,0.12124589694244239,8.0963851612070953E-2,0,1.0396592380493294E-2,0.26718310741568269,5.9141516244759211,0,1.9135685731285431E-2,9.8590521000173986E-2,-7.7124689098798029E-4,4.2811316898412277E-2]
[null,1921,1.0112616370232077,1.0001792506033866,0.99920132886681845,1.0123363734742252,1.0140043272314834,1.0335921635119711,0.97334989494173896,null,6.7428156651754811,0,1.0659211260970077E-2,0.19849350075832745,0.12063066444939634,8.3028222557963799E-2,0,1.0659211260970077E-2,0.26291066849335698,5.9128444810961307,0,1.9094383119211879E-2,0.10451465393871968,-2.5936439414261641E-3,4.3892734703797516E-2]
[null,1922,1.0131964846350454,0.97346038996250361,1.0238658956471354,1.004707280806405,1.0025114083848403,0.99035043710741155,0.98701161237873003,null,6.7352245096055361,0,1.0092643231230384E-2,0.19493138324250275,0.12124779593880629,8.454274405457822E-2,0,1.0092643231230384E-2,0.26242562699547373,5.911030229495867,0,1.9084088374056684E-2,0.10139530758997677,-9.9237448840593773E-4,4.1559708402679391E-2]
[null,1923,1.0012007073753129,0.99377819292230163,0.99636236833942171,0.97335607125980628,0.99514675272628772,1.0034825407095331,0.99789981233778435,null,6.7436796630643716,0,1.0507497835077902E-2,0.19484696499936585,0.12220939617690471,8.291250612658338E-2,0,1.0507497835077902E-2,0.26948230307158422,5.9108969872666712,0,1.9148555693413203E-2,0.10273949304116417,-1.824549131270515E-3,4.3268005819956677E-2]
[null,1924,1.0324225419920376,1.0161131456518189,1.0197985003052801,0.98816210471720756,0.99983870056280488,0.96700804562321718,1.0178667667222634,null,6.7121915681366433,0,9.5290703395137181E-3,0.18294251366682612,0.11704035490605251,8.4285910036013337E-2,0,9.5290703395137181E-3,0.26301491439633151,5.9103698620665179,0,1.8983888973838393E-2,9.5349896052875818E-2,9.6521249136379548E-4,3.9239015546825413E-2]
[null,1925,0.99131306510508244,1.0162887466875785,1.0163281438587723,0.96141504954383561,1.0077528225099548,1.0149127613618762,0.99396777778308543,null,6.751072080010017,0,1.0446789862918375E-2,0.19953410033797817,0.12195130019444449,8.4176337005820681E-2,0,1.0446789862918375E-2,0.27198028318888551,5.9091232104354079,0,1.9202866569527161E-2,0.10417552832487588,-2.0895672431455285E-3,4.3018021196219967E-2]
[null,1926,1.024673611890466,0.98540249833355142,0.99197411096252075,1.006380724222979,0.98466309813770569,0.97922027137361656,0.9879943615404998,null,6.7183145701855702,0,1.009355813832709E-2,0.18595763041735877,0.11989531266973175,8.2516443666742198E-2,0,1.009355813832709E-2,0.25855420133353091,5.9129270487936063,0,1.9023821313258259E-2,9.8266732938463525E-2,-3.9009677437933825E-4,4.1563475827256245E-2]
[null,1927,1.0388048965997785,0.99769075241952665,0.96863572870908721,1.0304566996352558,1.001048760868583,0.98329763182128282,1.0172749591165864,null,6.7153079856520916,0,1.0149145729612149E-2,0.18061813913244962,0.11809685633796639,8.1137437681062394E-2,0,1.0149145729612149E-2,0.26281913056067818,5.9155148633890535,0,1.8951446384837801E-2,9.6566907982051628E-2,-1.8917144995768835E-4,4.1792375633945715E-2]
[null,1928,1.0245357486467257,0.97905431365649764,0.9710113130262189,0.96353038589113571,0.99633891462942081,1.0454127511309794,0.98145338254866588,null,6.7392558486403304,0,1.1006519352970664E-2,0.19656842137580438,0.12060503712887166,8.1240597303267464E-2,0,1.1006519352970664E-2,0.26293319444079999,5.9117667682911659,0,1.9024537228922576E-2,0.10496922101033308,-3.1748157469577857E-3,4.5322887608120047E-2]
[null,1929,1.0146548156605326,1.0327222802064351,1.0090549629539576,0.97425681593983127,0.99997618002291944,1.0048183522787262,1.0006005152752759,null,6.7294476735277184,0,1.0099880155787692E-2,0.19084260007066328,0.11851723547987278,8.3658067189258112E-2,0,1.0099880155787692E-2,0.26640108306797983,5.9102307279736408,0,1.9076354979629184E-2,9.9996434777697887E-2,-8.6433878090140406E-4,4.1589508769881843E-2]
[null,1930,0.98248176956208588,1.0034443675939095,1.0067286886648923,1.0137909739371007,1.0004608728410729,0.99582332074556301,0.98053607006240551,null,6.7505955521694263,0,1.0486589726140236E-2,0.1974683661321705,0.12385895654964924,8.3580544917154873E-2,0,1.0486589726140236E-2,0.26903810658197513,5.9124987334220087,0,1.9252299360253945E-2,0.10358738084856425,-1.8707455912094558E-3,4.3181909948856026E-2]
[null,1931,0.97725930089829049,0.96240497324407293,1.0380228063077581,1.0173776657347429,1.0091862012786113,1.000012170107949,0.97654225832785846,null,6.7663340869153306,0,1.0486814843452291E-2,0.20682744111681578,0.12600244742208905,8.5536417609210186E-2,0,1.0486814843452291E-2,0.27025955773117627,5.9108948075703163,0,1.92819522874123E-2,0.10683883739068947,-2.4902111542614625E-3,4.3182836941877689E-2]
[null,1932,0.95900153312538106,0.97983413194327451,1.0044499044880806,0.98979456701276547,1.0057870560372066,1.0170177407645316,0.98305512205813395,null,6.7808947152863812,0,1.1106604321891816E-2,0.208439006569624,0.12815084934339693,8.3552703884830021E-2,0,1.1106604321891816E-2,0.27864111774279982,5.9113307935421728,0,1.9388157200020947E-2,0.10946586000180986,-3.8087926939478203E-3,4.5735019695676976E-2]
[null,1933,0.98617703127326528,1.0376138755090096,0.97706688031204048,0.97934280150370023,0.99132018810409639,1.0058660053959803,1.0416730158826495,null,6.7579508912168755,0,1.0675320699123423E-2,0.19237486727359368,0.12230628344986505,8.1926536861740271E-2,0,1.0675320699123423E-2,0.28534319035499539,5.9122902948828937,0,1.9231507571254847E-2,0.10241805582572457,-1.8989155059310769E-3,4.395907050273988E-2]
[null,1934,1.0091952422932735,1.0145383499942018,1.0097413503274617,1.0077458961706109,1.0159383846218593,0.99562693526904378,0.98292162155021112,null,6.7300636373949638,0,1.0132330672681952E-2,0.1916504189299284,0.1199954027541494,8.3671878897132138E-2,0,1.0132330672681952E-2,0.2624381434879185,5.9120013723427949,0,1.9105421378714852E-2,0.10038561589999261,-9.07750518150221E-4,4.1723134222475707E-2]
[null,1935,1.0011451101214854,0.98901329370829849,1.0252714593658065,0.973865535321223,0.97979347028201536,0.9981266889284317,1.0291477625212055,null,6.7537287848789553,0,1.0212053542796631E-2,0.19764809011353277,0.12190505840769343,8.4813786306696184E-2,0,1.0212053542796631E-2,0.27751725398543164,5.9092832236710215,0,1.9148858079081205E-2,0.10273740264809998,-1.3763071440657179E-3,4.2051418811466061E-2]
[null,1936,0.98484806490449228,1.0340523898919871,1.0051366631883163,1.0040662589400331,0.99632956459751487,0.99287283203047449,1.0332511224731709,null,6.7559404598331643,0,1.0311454539175334E-2,0.19371325068291687,0.12211516293226643,8.3652064432613943E-2,0,1.0311454539175334E-2,0.28223553346133623,5.9120632394885488,0,1.9238967177647701E-2,0.10169771470580379,-1.2362074698045976E-3,4.2460734421835761E-2]
[null,1937,0.99899695289321133,1.0249704348041877,0.98970595236089765,1.0229856310731325,0.98822580039762287,0.99664404921038752,0.98681920744558971,null,6.7357686062318356,0,1.0381572923926696E-2,0.19062179343470814,0.12109743833924987,8.2490172257724842E-2,0,1.0381572923926696E-2,0.26613416923317845,5.9139508936781597,0,1.9160567378516114E-2,0.10084540353862993,-1.2813010779689524E-3,4.2749469449634654E-2]
[null,1938,0.9916251509896854,0.98479199863306388,0.97973920604348064,1.0348040857521819,0.99576910789950457,0.98157760938868432,1.0201500417451126,null,6.7515435051539718,0,1.0570035681120771E-2,0.19123438490450959,0.12415288132449891,8.2010322523320661E-2,0,1.0570035681120771E-2,0.27608139034175194,5.9151416260151555,0,1.9201135789783115E-2,0.10167464998033059,-1.4784112640158222E-3,4.3525525538639594E-2]
[null,1939,0.97231164053843733,1.0224436280437896,0.95600245128970629,0.99548600629535411,0.99062653942576595,1.0039825054725586,1.0395483678370363,null,6.768767598087515,0,1.1076819213567681E-2,0.19346212337920643,0.12517913464893657,8.066508360761851E-2,0,1.1076819213567681E-2,0.28874428717257916,5.9143072038534443,0,1.9310338707300874E-2,0.10409503733709254,-2.607980539819059E-3,4.5612369921149837E-2]
[null,1940,1.0298757153618645,0.99953818971258346,1.0025802811878155,0.99885298003629774,1.0168645723658349,1.0031589309293272,0.96978615821069936,null,6.7170829976818709,0,1.0131215140969645E-2,0.18960798864259951,0.11841923517026028,8.3114097436731094E-2,0,1.0131215140969645E-2,0.25452398709084662,5.9119257343570704,0,1.8996947168166668E-2,9.9668747713604497E-2,-8.9228055884721629E-4,4.1718540661441671E-2]
[null,1941,0.97980506465231154,0.99906688775084318,0.98271961656831142,0.97219197557989345,0.9955043237823018,1.0004969469029195,1.0124048770934473,null,6.759747162333821,0,1.0808594171874039E-2,0.1964169688075092,0.12487289164766129,8.2190909434366605E-2,0,1.0808594171874039E-2,0.27899819803144249,5.9115925094003066,0,1.9267458074140788E-2,0.1042744543833533,-2.3740943866929387E-3,4.4507866941733081E-2]
[null,1942,1.0281471203942831,1.0047981986577206,0.99324387119017099,1.0135716099594205,1.0059134341073925,0.97136160176516739,0.99140702802430536,null,6.710836215169393,0,9.8847870215568786E-3,0.1824544420977105,0.11853922859105523,8.258857588274543E-2,0,9.8847870215568786E-3,0.25768517781718475,5.9132448608046424,0,1.9005846946796495E-2,9.6354556803950664E-2,2.5973269703891968E-4,4.070379352827002E-2]
[null,1943,0.97038614373851062,1.0177062855973371,1.0141332746767526,1.0327100071506861,0.98663622295687514,0.98955662251725285,0.9891750120174988,null,6.7583947689457027,0,1.0419239023535802E-2,0.19836255046370491,0.12455420330651107,8.4122377875297763E-2,0,1.0419239023535802E-2,0.27406917917141838,5.913100445842379,0,1.932146418763658E-2,0.10367611935798302,-1.7161430027440028E-3,4.2904571743509139E-2]
[null,1944,0.98765742891255925,0.9646602823836361,1.0353550013357027,0.98486611954882819,0.99091218778923584,0.97466483576874108,0.9869735546407965,null,6.7486704728274276,0,1.0126915728951245E-2,0.19894358661878098,0.12461144583383969,8.5313160400135979E-2,0,1.0126915728951245E-2,0.26781495961076818,5.9092941173948779,0,1.9223221604111676E-2,0.10290057173445506,-1.131426817558514E-3,4.1700836448016712E-2]
[null,1945,1.0212805546529988,0.99106508192516352,0.98959668967656989,1.0151216494528077,0.99492567912486574,1.0134654925489366,0.98732278703843657,null,6.7329033953749571,0,1.0477267882149541E-2,0.19234773954581358,0.12006183346766219,8.2425364619731198E-2,0,1.0477267882149541E-2,0.26231305504772773,5.9135319125391774,0,1.9041497419848175E-2,0.10176403298369409,-1.7255645032285636E-3,4.3143524254528713E-2]
[null,1946,0.98835527563216286,0.98094122979495701,1.0020214505829868,0.98056504321161742,1.0097316569619836,0.99157983612242617,1.0049457037232812,null,6.7535336462603093,0,1.0524418337986481E-2,0.19680390255929026,0.12433514012331198,8.3329378147229599E-2,0,1.0524418337986481E-2,0.27391049586529381,5.910968913468432,0,1.9219324278757617E-2,0.10348001780032309,-1.851207421533128E-3,4.3337681439196973E-2]
[null,1947,1.0284913637032367,1.005260936118342,1.0406354342601705,1.0224440060799438,0.97163307901296414,1.0224127271417274,0.96807682385375782,null,6.7285438186766102,0,9.9762906050842332E-3,0.19751938749038433,0.11760915851770978,8.5502468734200351E-2,0,9.9762906050842332E-3,0.25613004162807551,5.9110159285468624,0,1.9004072203126342E-2,0.10190047219620965,-1.2182996381627728E-3,4.1080588998204964E-2]
[null,1948,0.98849637473751817,1.0023199265733995,1.0171202465653171,1.0152418591138161,0.97545518861008473,0.98504520722160427,0.98980193576983777,null,6.7457192745435819,0,1.0221593523666873E-2,0.19546179491780735,0.12296261267674335,8.4223755514563528E-2,0,1.0221593523666873E-2,0.26894041146180703,5.9119861472330637,0,1.9218536939084797E-2,0.10200953907494439,-1.1742260290721585E-3,4.2090702754636423E-2]
[null,1949,0.99683725481691854,0.98491208199770997,0.96881207905068722,0.98358235257868598,0.99914713001836275,0.97669451874291613,0.99840412117227351,null,6.7360785079428736,0,1.0561972067433815E-2,0.18801418513411469,0.12370177467836484,8.1189905707005586E-2,0,1.0561972067433815E-2,0.26829980932921904,5.9129707859000664,0,1.9172390459336906E-2,0.10051226354440411,-1.2749278223906776E-3,4.3492321012746415E-2]
[null,1950,1.0178876906233649,0.97419499468857595,1.0014363256943291,0.95620122422297282,0.99905788645243154,0.98176470177031672,1.0437248582551839,null,6.7390494204502192,0,1.0153081977894626E-2,0.189695520509154,0.12107236635507554,8.329241827452219E-2,0,1.0153081977894626E-2,0.27533877170120996,5.9096851872317844,0,1.9059290353981611E-2,9.977137969065443E-2,-6.7409806991099478E-4,4.1808584403746879E-2]
[null,1951,1.0165141407400715,0.99049862262387078,0.98478376286705516,0.97461416577262749,1.0064951642465991,1.0024879456406706,1.0012817036686905,null,6.7331356121965458,0,1.0458747073998879E-2,0.19064223672335909,0.12074090158045073,8.2149711157741653E-2,0,1.0458747073998879E-2,0.2662435759048889,5.9116093598237613,0,1.9066527330948418E-2,0.10110435760282882,-1.4883167905778232E-3,4.3067258863145261E-2]
[null,1952,0.99643101279084378,0.96411879656371546,0.996160693394886,0.98633528056261977,1.0017775220633536,0.98043715015579569,1.0014980539098965,null,6.7453680742508588,0,1.0452024092706892E-2,0.19376036546843772,0.12429552841277282,8.2914694494058361E-2,0,1.0452024092706892E-2,0.26985710933701329,5.9116097487745041,0,1.9174620123194066E-2,0.10217679659096768,-1.4603637729237032E-3,4.3039574822830919E-2]
[null,1953,1.0130012493481519,1.0224183386006247,1.0001560551313065,0.99963665114041311,1.0001708161831371,0.98667377451684779,0.99887574013854397,null,6.7255652130843009,0,1.0054298293878633E-2,0.18749395582631886,0.11935133100994157,8.3103231029632726E-2,0,1.0054298293878633E-2,0.26478395475927546,5.9121045076103291,0,1.9085125378699205E-2,9.8676155392940806E-2,-4.3485869864339752E-4,4.140181077580931E-2]
[null,1954,1.0296310805540856,1.0243714855821566,1.0063148869338658,0.96615613795860256,1.0417863972893824,0.97484862431479558,0.99441724277901977,null,6.7070325199478953,0,9.7129602272087116E-3,0.18278845199021657,0.11722286152497312,8.3371937222516943E-2,0,9.7129602272087116E-3,0.2582728423672066,5.9099480859997007,0,1.8998204870394636E-2,9.5906289251701249E-2,5.2760534800712084E-4,3.9996241373173542E-2]
[null,1955,0.99616393848913876,0.97892706758719283,1.0036142895427116,1.0260283803537795,0.9818487123146723,1.0184546324127688,1.0311805901801805,null,6.7690225325399309,0,1.0719450421764644E-2,0.20092442813456868,0.12343171346408968,8.3563005586723568E-2,0,1.0719450421764644E-2,0.28152906680986861,5.9133359947174347,0,1.917608695423028E-2,0.10556315773462664,-2.6417097073889147E-3,4.4140788845778614E-2]
[null,1956,1.0176155275361309,0.9918920159276774,0.98787104162616313,1.0062379983019332,0.97202670942628544,1.0110715416788956,0.99420271098984014,null,6.7355545397920595,0,1.0502217060055111E-2,0.19231307889693591,0.12048576117481065,8.2345847979580042E-2,0,1.0502217060055111E-2,0.26485932161115583,5.9131476432995544,0,1.9060722778268924E-2,0.10183333301931967,-1.7374294959212977E-3,4.3246260528355729E-2]
[null,1957,1.0049330965731664,1.0279316697384393,1.0333427537358557,1.0330185672494892,0.97094712518132442,0.99746643830833126,0.99379110995613729,null,6.737730028510545,0,9.9297088638425676E-3,0.1944902657597182,0.1194340938236364,8.5206037675302895E-2,0,9.9297088638425676E-3,0.26655501609102439,5.9120118940488267,0,1.9128332270334544E-2,0.10069633898351686,-6.8072382082444416E-4,4.0888773679012655E-2]
[null,1958,1.0060690673234838,1.0105236629440744,0.98767149626578044,0.98708061737868136,0.98365825009747099,0.9736054033626752,0.9527214874057599,null,6.7131239017377888,0,1.0149673492432589E-2,0.18580243388242992,0.12096842400479911,8.2165892943734706E-2,0,1.0149673492432589E-2,0.253208154019335,5.9121232039146596,0,1.9122206957922591E-2,9.839562550376299E-2,-4.5658835616003242E-4,4.1794548867301988E-2]
[null,1959,1.0147808709008235,1.0040939998148379,1.026488579598305,1.0149407712261944,1.0238186389996711,1.0063323190842022,1.0167516346612011,null,6.7434059840769409,0,1.0081268394821036E-2,0.19546828921962217,0.11951847888539811,8.4830895395893877E-2,0,1.0081268394821036E-2,0.27111424311050858,5.9114320019725719,0,1.9075687564030459E-2,0.10154359081045371,-1.0900717325315211E-3,4.1512868850991085E-2]
[null,1960,1.0063177894106774,0.99413907811798641,0.97422883851034947,1.0362202644564029,1.0295662865700166,0.99175119631253217,0.96082250074448849,null,6.7267545668287658,0,1.0531597837604094E-2,0.18898719343101328,0.12198048648090966,8.1416489151611024E-2,0,1.0531597837604094E-2,0.25705196999557023,5.9155209434947134,0,1.912086765922022E-2,0.10075783260239132,-1.4484613273845544E-3,4.3367245340718993E-2]
[null,1961,1.0344187320854314,1.033321032770109,0.97451707891550132,0.97816470192901672,1.0223776699304152,1.0000875954547956,1.0012528966982874,null,6.7116045839382465,0,1.0159499434275767E-2,0.18238798516785723,0.11684091823797724,8.1443094640651123E-2,0,1.0159499434275767E-2,0.26099327955099633,5.9123664005053591,0,1.8973698976230347E-2,9.7225423418378212E-2,-4.612269060702147E-4,4.1835010346859748E-2]
[null,1962,1.0012599986159054,0.99243609383931886,0.98735071690597542,1.0116408237275618,1.0000965609791328,1.0038306687169833,1.0301887164442336,null,6.7542034625057257,0,1.0599649921016677E-2,0.19394753698160641,0.12243674151677258,8.2495795309579234E-2,0,1.0599649921016677E-2,0.2782177297264426,5.9134685704891607,0,1.9148233253671428E-2,0.10272548546276949,-1.8841019416738442E-3,4.36474717073927E-2]
[null,1963,1.0025391624752185,0.97468043984238983,1.0010957822859405,0.99662761467931493,0.97065974403370237,1.009086719132497,1.0410403559468704,null,6.7622974444179471,0,1.0596292544389549E-2,0.19787641696806807,0.12290788411297418,8.3384685506947206E-2,0,1.0596292544389549E-2,0.28153334556166826,5.9118890495812053,0,1.9141286146334442E-2,0.10409176016711651,-2.160630254404191E-3,4.3633646628032964E-2]
[null,1964,0.97284844880431054,0.98306166125964123,1.0028574811008759,0.99310977297135172,0.99696147182003114,0.96976017967660799,1.0133081010012095,null,6.758745642718031,0,1.0439590326053178E-2,0.19545953621165604,0.12619170531638488,8.3452007669384876E-2,0,1.0439590326053178E-2,0.27841261418821989,5.9115997500558111,0,1.9307244890741652E-2,0.10273052621757002,-1.3961166166200916E-3,4.2988374784878887E-2]
[null,1965,1.0381147300826541,0.99917073125397038,0.97703027246368579,1.0101566995768574,0.98204154226533591,1.0114982702507955,1.0138958364254431,null,6.7249730239201773,0,1.0364474061499932E-2,0.18676310173579388,0.11795575661259786,8.1670981811388293E-2,0,1.0364474061499932E-2,0.26471752373090679,5.913958177797519,0,1.8954935381753388E-2,9.9432244400482317E-2,-1.1587569279110259E-3,4.2679059377645288E-2]
[null,1966,0.98484527973267699,1.0384896274432016,1.0238153072207385,0.98297420242980738,0.98836129030549846,1.0057299470684278,1.0066406631179199,null,6.7533680283388131,0,1.0256896219698615E-2,0.19808897885711785,0.12155403500570067,8.4713349531358145E-2,0,1.0256896219698615E-2,0.27618107365907074,5.9098590670941018,0,1.9238982832204959E-2,0.10304032293333332,-1.543854547325769E-3,4.2236072973249481E-2]
[null,1967,0.98209189138482711,0.99248121534729361,0.98903189343688025,1.0278603273793836,0.99475167810522935,1.0114786280611339,0.97463162754385335,null,6.7568142949210799,0,1.0872691474335337E-2,0.19944007373698366,0.12479215531541042,8.2492036250514184E-2,0,1.0872691474335337E-2,0.2690711542708516,5.9142518769709733,0,1.9254502176861657E-2,0.10554605385570877,-2.8053658805959809E-3,4.4771808224374168E-2]
[null,1968,0.96991734088747139,0.98164277582848869,0.99198642606831089,1.020678386994043,1.0213978021801062,1.0104900126065115,1.0018541437032025,null,6.7753042721192438,0,1.1021827534169909E-2,0.20306321315122808,0.12685754127282564,8.2818257095793699E-2,0,1.1021827534169909E-2,0.28008939085759543,5.9136991443940534,0,1.9324179607400151E-2,0.10730528265252,-3.2386608857150221E-3,4.5385923973543858E-2]
[null,1969,1.0181328780404819,1.0011484223577167,1.0008036516564116,0.99715113310856351,0.99447644322717454,0.98611007533588713,1.0341089126663152,null,6.735113633502456,0,1.0082593880162614E-2,0.18820208436834454,0.11974065684766204,8.3249838161679066E-2,0,1.0082593880162614E-2,0.27288482987923185,5.9119337736788502,0,1.9058000561339463E-2,9.9016991662637902E-2,-4.9086862098686934E-4,4.1518326963700128E-2]
[null,1970,0.9970200598046558,1.0083704420941237,0.99851654294457326,0.99029553611220311,1.0098155244549247,0.9767505840641203,0.97825370213160001,null,6.7290408954725409,0,1.0187367577697904E-2,0.18951455498905412,0.12196805596450984,8.2967766197491771E-2,0,1.0187367577697904E-2,0.26267982653152694,5.9116917553976416,0,1.91713877249114E-2,9.982084289527636E-2,-7.2306062900162355E-4,4.1949766401127506E-2]
[null,1971,0.99765542635434912,1.0073321980899874,1.017123855729934,0.99623872899708366,1.0054624308814506,0.97285705009309509,1.0027344992971616,null,6.7358964148739728,0,9.9810653742287685E-3,0.19086332937369158,0.12159082611002764,8.4206864386005914E-2,0,9.9810653742287685E-3,0.26875523396514994,5.9109592387228851,0,1.9167905427000489E-2,9.9609468994725947E-2,-3.5670275317885866E-4,4.1100250647664933E-2]
[null,1972,0.99088463801430315,1.0126880560792293,1.0254985393412641,0.98000638698783815,1.0077782538711038,0.99978910840992008,0.99744112535336604,null,6.7488588161234544,0,1.0228764060336766E-2,0.19803799873064112,0.12200309292195069,8.4753335671350585E-2,0,1.0228764060336766E-2,0.27167365259728249,5.9096018838974711,0,1.920524433513069E-2,0.10292858825312629,-1.4652100318371948E-3,4.2120229748335104E-2]
[null,1973,1.0275073386891094,1.0318764505027931,0.97206685658374925,0.98809376721018505,1.017324578601468,0.99723118362499907,1.0059917744958391,null,6.7169518438062266,0,1.0226530861710265E-2,0.18292482673990682,0.11773622662957337,8.1334110044370703E-2,0,1.0226530861710265E-2,0.26374077294246928,5.9130372234470645,0,1.9009148495150011E-2,9.7631631670855534E-2,-5.7312999705458963E-4,4.211103383388571E-2]
[null,1974,1.0352504816514321,1.0276533783556043,0.98371953889057751,1.0197578843174193,1.0132867251924504,1.0274718428784431,1.0178721833471527,null,6.7299247004688594,0,1.0370358866387897E-2,0.18873295038257751,0.11684108135115154,8.2133576452143781E-2,0,1.0370358866387897E-2,0.26768584631064568,5.9141085283056283,0,1.896946472320794E-2,0.10014505236652865,-1.3950913797404711E-3,4.2703291956717716E-2]
[null,1975,0.97029035223256543,1.0082469212468417,0.9989885422555369,0.99652968560701938,1.0179203727019035,1.0177983942509232,0.97757740769382551,null,6.7650710242131069,0,1.0904003363596593E-2,0.20298796156655299,0.12532511165528148,8.3149971252243118E-2,0,1.0904003363596593E-2,0.27361622659856738,5.9120021815486599,0,1.9322018821959868E-2,0.10689246441044951,-3.1256566516540928E-3,4.4900745011043519E-2]
[null,1976,0.98274713173911965,1.0193105802106037,0.99937326721803599,1.042487874828403,1.037596913003624,1.015261768947886,1.0211119325030518,null,6.7674369825704783,0,1.0685312213356985E-2,0.19903024088074209,0.12319030217455758,8.3315933938128389E-2,0,1.0685312213356985E-2,0.28181533882475412,5.9144643075870222,0,1.9250801060262796E-2,0.10478831787054428,-2.4184735454647103E-3,4.4000213779930464E-2]
[null,1977,1.014705701641986,0.99788822509032649,1.0087752226545981,0.99488889595458596,1.0011459572945054,0.99577910776103107,0.98304097888559672,null,6.728674972785158,0,1.0159097608999492E-2,0.1918820596273437,0.12015425875931152,8.3585765222996711E-2,0,1.0159097608999492E-2,0.26121196420751425,5.9113614393703875,0,1.9076085537330648E-2,0.10055500207851274,-9.8495772012978226E-4,4.1833355701894281E-2]
[null,1978,0.99433839360227083,0.965228717268792,0.97358837194025394,0.97441088329517278,1.0036335934564105,0.97919708354347301,0.99321407022858776,null,6.7411923818458082,0,1.0663477872698101E-2,0.19117192237158509,0.12492808722034281,8.1477674517883056E-2,0,1.0663477872698101E-2,0.26801950706277633,5.9122142755591689,0,1.9186134350520325E-2,0.10195538498770013,-1.6709080756364249E-3,4.3910303851464931E-2]
[null,1979,1.0074084316531602,0.99892271994711368,0.98696368729640771,0.95811181488810393,1.0203780881591038,0.99833934671266145,1.026716135511341,null,6.7424612077166763,0,1.0451656079275404E-2,0.1911298881256511,0.12137994050357148,8.2390106579084965E-2,0,1.0451656079275404E-2,0.27499090568791767,5.9105965984686506,0,1.911500266451838E-2,0.101252663207784,-1.4319569295291456E-3,4.3038059409023992E-2]
[null,1980,1.0111143997952532,0.97397220974025467,0.99556419146079245,1.0155585186903442,1.0205530668128744,0.99577638352183229,0.98142170794944361,null,6.7352667145512992,0,1.0421299773492401E-2,0.19302009499829154,0.12200446632512724,8.2791742399268689E-2,0,1.0421299773492401E-2,0.26192634055557729,5.9132225409332593,0,1.9095168137628838E-2,0.10181663441789295,-1.5233307607804823E-3,4.2913057545030595E-2]
[null,1981,0.97870717171221211,1.0197446800022112,0.98566492204926237,1.0013744531448967,1.0016191974951492,1.0273115967872646,0.99907978973353728,null,6.7654626029037654,0,1.0985446928356473E-2,0.20050479030523691,0.12393723362046344,8.2382111003386674E-2,0,1.0985446928356473E-2,0.2779941367390939,5.9130071113539726,0,1.9273699640362598E-2,0.10628801541586323,-3.1606102889268884E-3,4.5236115114310561E-2]
[null,1982,0.97868248611316111,1.0450847398310934,1.0027362542101854,1.0087282029993763,0.99126220990260827,1.0020832959880754,0.98534121426400945,null,6.7487626266670206,0,1.0447139294868289E-2,0.19556575630749781,0.12240917584202954,8.3363948187529929E-2,0,1.0447139294868289E-2,0.27160517382403176,5.912450606384569,0,1.9273840139974494E-2,0.10279253527537743,-1.7178693887869934E-3,4.3019460094793155E-2]
[null,1983,1.0200264325092412,1.0028532802782208,1.0051386707792347,0.98753489878490774,0.98214840613226762,1.0143167132039796,1.0002737362103449,null,6.7352329062568614,0,1.0305091481683499E-2,0.19359428845666715,0.11935739526685751,8.3420093649669028E-2,0,1.0305091481683499E-2,0.2660622008849019,5.9111697996303754,0,1.9048060525389144E-2,0.10163515948511377,-1.4886241257816163E-3,4.2434532483666396E-2]
[null,1984,0.97614202111931891,0.97997816691088147,1.0081355219977894,1.0174710167832426,0.99303772937443169,0.95557758560824302,0.97984835392795033,null,6.7435948991824333,0,1.0218765462905418E-2,0.19282633402662738,0.12582164863306428,8.3643412179041129E-2,0,1.0218765462905418E-2,0.26699551007429739,5.9126179282774487,0,1.9288337349998665E-2,0.10108184277546073,-7.5917143730366702E-4,4.207905730379681E-2]
[null,1985,1.0352341310594053,1.0298064290710718,1.003982575167923,0.99618274525085371,1.0181032710304951,1.0293840979003397,1.0193222634830235,null,6.7311693471116918,0,1.019851523501797E-2,0.191264362818404,0.11638372308002058,8.3383173710162808E-2,0,1.019851523501797E-2,0.26825994022761873,5.91170237489104,0,1.8969547894892969E-2,0.10046953201506474,-1.2589779952790266E-3,4.1995670469762499E-2]
[null,1986,0.96066160031326508,1.0194559925414655,1.0097061702918038,0.96713645881973109,1.0314770048872892,1.0197930797104684,1.0107362722678934,null,6.7799438030626709,0,1.0880378457544118E-2,0.20578883168668022,0.12581479820861619,8.3959481144177131E-2,0,1.0880378457544118E-2,0.28582787466383119,5.9098090625076534,0,1.9378333796735283E-2,0.10779312789471714,-3.2311686927366415E-3,4.4803461852995927E-2]
[null,1987,0.9906473711682533,0.99060306432856127,0.96715095743843016,0.96322190798576524,1.0446396888602185,1.0021835341218954,0.97178365964793934,null,6.7409066169211238,0,1.0894177486665563E-2,0.19345000416949898,0.12421921198649147,8.1030418971459142E-2,0,1.0894177486665563E-2,0.26508805035054911,5.9119602264706916,0,1.9206562048376088E-2,0.10350472590099585,-2.4128667757203526E-3,4.4860283798782423E-2]
[null,1988,0.98600088435231081,1.0063416494994768,0.95969101140487789,0.99592619419599182,1.0157242421933677,1.0137572923489921,1.0057704062860697,null,6.7564179178084371,0,1.1069026192426789E-2,0.19438866981106973,0.12415901887334919,8.0737701039636497E-2,0,1.1069026192426789E-2,0.27658559991522452,5.9141324726584523,0,1.9232495143575907E-2,0.10439882864081568,-2.797147920882777E-3,4.5580279647197706E-2]
[null,1989,1.0359538071952901,1.0011175729059394,0.99904980228035978,0.99289476940560628,1.0108665667463477,1.0305931932146422,1.0211508377900174,null,6.7363261351533934,0,1.0372162913433019E-2,0.19310479263428684,0.11771398640671088,8.308402704731134E-2,0,1.0372162913433019E-2,0.26895858608172279,5.9118022986975669,0,1.8965889554012665E-2,0.10168494122247483,-1.6991071920361832E-3,4.2710720701341118E-2]
[null,1990,0.96875661032861582,0.99635936164912975,1.0169589284934621,0.99141321349218403,0.99530078572042402,0.99793515045639991,1.0171026887245791,null,6.7730889912040606,0,1.0594879003547676E-2,0.20255157110646216,0.12577099817884632,8.439305425738243E-2,0,1.0594879003547676E-2,0.28332610526197599,5.9107079483257818,0,1.9330914149255241E-2,0.10571803237584083,-2.337458369932897E-3,4.3627825918447022E-2]
[null,1991,1.0054115732551165,1.0068846037017074,1.0201017466380602,1.0225161439220221,0.99256748755524138,1.0141155173306229,0.99128097816201011,null,6.7454099072169793,0,1.0299178677101674E-2,0.1978160486087534,0.1206184356442932,8.4392367443434674E-2,0,1.0299178677101674E-2,0.26746851142529288,5.9122084838550384,0,1.9125750570249216E-2,0.10308660319375616,-1.7164781306838075E-3,4.241018460683843E-2]
[null,1992,0.96999588208999699,0.97046213225464695,0.97232897073925639,1.0347798828155692,0.99442233419382753,1.0013460771576015,1.0332278802898975,null,6.781621444252993,0,1.1164687315805111E-2,0.19978361885288887,0.12781082387965645,8.1705913075587527E-2,0,1.1164687315805111E-2,0.28800658651687694,5.9155470558252601,0,1.9323724494681293E-2,0.10661555953599093,-3.1460330541783067E-3,4.5974195126224401E-2]
[null,1993,1.0031815632836176,0.96649738029993415,0.98976864265357989,0.99423152838351714,1.0027071031545172,0.99599750694409106,1.0217354734492077,null,6.7517343656160396,0,1.0594264230933152E-2,0.19454521717334658,0.12345813106861188,8.2590155515311042E-2,0,1.0594264230933152E-2,0.27493675620707025,5.9123932040524947,0,1.9137803966219041E-2,0.10291781019090251,-1.8700069521640581E-3,4.3625294394245853E-2]
[null,1994,0.97153541962153456,0.96199271843965051,1.017759133696168,1.0179311505367208,1.0433164740697969,1.0101504680620388,0.98519175686583349,null,6.7755327523489033,0,1.0848413936516234E-2,0.20764431872891151,0.12716871152540513,8.4351773689560469E-2,0,1.0848413936516234E-2,0.27521441316253453,5.9120949142906642,0,1.9314818390055461E-2,0.10833334057617024,-3.2613756592748825E-3,4.4671837644875763E-2]
[null,1995,0.97962978218267549,0.98412109136223203,0.98529644953591899,0.98880411471949414,1.0126965162363637,0.97573854039451058,1.0380547933626261,null,6.7610276259245428,0,1.0587498731324325E-2,0.1931359249031083,0.12560129470512374,8.2426966411623337E-2,0,1.0587498731324325E-2,0.28379663178400144,5.9123480280022411,0,1.9268453623654865E-2,0.10240061288329437,-1.5477216595768852E-3,4.3597435271070753E-2]
[null,1996,0.99835243467567858,0.98817134018884922,1.0072569913432976,0.98111499658170875,1.0352459724913601,1.0230681376402146,1.0006649058769892,null,6.7568094899844233,0,1.0667190990893444E-2,0.20102638373958204,0.12263009213111796,8.3640900682103655E-2,0,1.0667190990893444E-2,0.27293780419509023,5.9107031374175616,0,1.916409038297948E-2,0.10542624967543768,-2.6447620507302249E-3,4.3925593811282977E-2]
[null,1997,0.95986012152744549,1.0281477859957981,0.96148726455947964,1.0139857992732939,1.0181402697475701,1.006701864643484,0.99782806303304195,null,6.7679224103858067,0,1.1170742291541982E-2,0.19669922883466806,0.12641737686804619,8.0921697340290172E-2,0,1.1170742291541982E-2,0.28096948078082373,5.9150120963722594,0,1.938307228372366E-2,0.10554401649529545,-3.0236870278648551E-3,4.5999128438563346E-2]
[null,1998,0.98128315830973389,0.99186375975349861,0.99528333433499228,1.0090625186281776,1.0039399455666789,0.99330504402445008,0.99950551208446181,null,6.7567114763978608,0,1.0630823344048157E-2,0.19681888770984701,0.12480677942619868,8.2938775500663225E-2,0,1.0630823344048157E-2,0.27443235067985078,5.9128871696681244,0,1.9259077110254961E-2,0.10383497804931527,-2.0423800611738111E-3,4.3775838314773906E-2]
[null,1999,1.0049807694842439,0.9608449706935116,0.98663847112759528,0.9650030685804506,0.96776202116932775,0.99943915075472756,1.0078539813130427,null,6.7472739223119369,0,1.0667663851528744E-2,0.1949859724297463,0.12358555198803045,8.2323437771156777E-2,0,1.0667663851528744E-2,0.27110522847256524,5.9109871252048043,0,1.9128074932991766E-2,0.10331223143635211,-2.081240890923943E-3,4.3927540967213068E-2]
[null,2000,1.0021794995675832,1.0176367978659493,1.0066252249843362,0.97876463962153892,0.98005155205463634,0.99906152298088458,1.0038729465516316,null,6.7395798224623764,0,1.0253000978842375E-2,0.19304018226204717,0.12074621632213835,8.3562804423660278E-2,0,1.0253000978842375E-2,0.27019626498817362,5.9106118687697577,0,1.9143237674531705E-2,0.10126964632743228,-1.2104313700930516E-3,4.2220033064730524E-2]

{"sheet":"Cash Flow Analysis","index":10,"n_rows":282,"n_cols":33,"rows_kept":282,"cut":false,"hidden":false,"merged":[[14,3,14,4],[52,22,52,23]]}
[]
["TABLE OF CONTENTS"]
["DCF Calculations"]
["Yearly Cash Flow Calculations"]
["Specific Item Cost Calculation"]
["Feedstock, Utility, and Byproduct Cost Information"]
[]
[]
[]
[]
[]
[]
[]
[]
["DCF CALCULATION INPUTS:",null,null,"DCF CALCULATION OUTPUTS:"]
["Process",null,null,{"$f":"\"Hydrogen Cost (Year \"&TEXT(ref_year,\"0\")&\" Real $/kg)\"","v":"Hydrogen Cost (Year 2016 Real $/kg)"},{"$f":"H2_price_nominal/INFLATION_FACTOR","v":6.750047990935756}]
["Actual Hydrogen Produced (kg/yr)",{"$f":"output_kgyear","v":470850},null,"Hydrogen Cost (Start-up Year Nominal $/kg)",{"$f":"+SUM(X57:AB57)/AC57*(1+inflation_rate)^construct","v":6.6241884111243934}]
["Actual Hydrogen Energy Produced (MMBtu(LHV)/yr)",{"$f":"B17*H2_LHV_MJ_p_kg/1000/mmBTU_to_GJ","v":53650.852977513299},null,"After Tax Real IRR",{"$f":"((E20+1)/(1+B30))-1","v":8.0000000000002736E-2}]
["Actual Hydrogen Energy Produced (MJ(LHV)/yr)",{"$f":"B17*H2_LHV_MJ_p_kg","v":56601649.891276531},null,"Pre Tax Real IRR",{"$f":"((E21+1)/(1+B30))-1","v":7.8384109070473995E-2}]
["Design Capacity (kg/day)",{"$f":"design_cap","v":1500},null,"After Tax Nominal IRR",{"$f":"IRR(AA65:AA113)","v":0.10052000000000261}]
["Design Capacity (kg/yr)",{"$f":"B20*365","v":547500},null,"Pre Tax Nominal IRR",{"$f":"IRR(AC65:AC113)","v":9.8873407142813008E-2}]
["Capacity Factor",{"$f":"cap_factor","v":0.86},null,"After Tax Real Capital Recovery Factor",{"$f":"(real_irr*(1+real_irr)^anal_period)/(((1+real_irr)^anal_period)-1)","v":0.10185220882315059}]
[null,null,null,"After Tax Nominal Capital Recovery Factor",{"$f":"(nominal_irr*(1+nominal_irr)^anal_period)/(((1+nominal_irr)^anal_period)-1)","v":0.11787679477462062}]
["Financial",null,null,"Total Real Fixed Charge Rate",{"$f":"(E22*(1-total_tax_rate*INDEX(Depreciation!B12:H37,MATCH(\"NPV - Real IRR\",Depreciation!B12:B37,0),MATCH(depr_length,recovery_period,0))))/(1-total_tax_rate)","v":0.11010937660003045}]
["Start-up Year",{"$f":"startup_year","v":2015},null,"Total Nominal Fixed Charge Rate",{"$f":"(E23*(1-total_tax_rate*INDEX(Depreciation!B12:H37,MATCH(\"NPV - Nominal IRR\",Depreciation!B12:B37,0),MATCH(depr_length,recovery_period,0))))/(1-total_tax_rate)","v":0.12930300426323382}]
["After-Tax Real IRR",{"$f":"real_irr","v":0.08},null,"NPV",{"$f":"NPV(nominal_irr,AA65:AA113)","v":8.7071894903132806E-9}]
["After-Tax Nominal IRR",{"$f":"((1+B26)*(1+B30))-1","v":0.10051999999999994}]
["Analysis Period (yrs)",{"$f":"anal_period","v":20}]
["Plant Life (yrs)",{"$f":"plant_life","v":20}]
["Inflation Rate",{"$f":"inflation_rate","v":1.9E-2}]
["Debt Financing",{"$f":"100%-equity","v":0.6}]
["Equity Financing",{"$f":"equity","v":0.4}]
["Total Tax Rate",{"$f":"total_tax_rate","v":0.25739999999999996}]
[]
["Cost of Debt Financing"]
["Debt Financing Period (yrs)",{"$f":"debt_period","v":0}]
["Interest Rate on Debt",{"$f":"debt_interest","v":3.6999999999999998E-2}]
[]
["Construction/Start Up Information"]
["Construction Period (yrs)",{"$f":"construct","v":1}]
["Start-up Period (yrs)",{"$f":"start_time","v":0.57999999999999996}]
["% Revenue During Start-up",{"$f":"percnt_revs","v":0.5}]
["% Variable Costs During Start-up",{"$f":"percnt_var","v":0.5}]
["% Fixed Costs During Start-up",{"$f":"percnt_fixed","v":0.75}]
[]
["Depreciation Parameters"]
["Depreciation Type",{"$f":"depr_type","v":"MACRS"}]
["Depreciation Period (yrs)",{"$f":"depr_length","v":7}]
[]
["Plant Costs (Inflated to Start-up Year $)"]
["Total Depreciable Capital Costs",{"$f":"(total_cap-non_dep_cap)*INFLATION_FACTOR","v":2151893.8178031025}]
["Total Non-Depreciable Capital Costs",{"$f":"non_dep_cap*INFLATION_FACTOR","v":0}]
["Total Capital Investment",{"$f":"SUM(B51:B52)","v":2151893.8178031025},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Closed form formulas for calculating price of hydrogen."]
["Decommissioning",{"$f":"decom_percent*depr_cap_infl","v":215189.38178031027},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Capital Costs","Depr","Principal","Op costs","Tax incentives","H2 sales (kg)"]
["Salvage Value",{"$f":"salvage_perct*B53","v":215189.38178031027},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Discounted values",{"$f":"-SUM(H116:K116)","v":1735318.2870998234},{"$f":"-U116","v":1943148.466692155},{"$f":"-Z116","v":186568.84132367116},{"$f":"-SUM(L116:S116)","v":27315398.116797481},{"$f":"+AF116","v":0},{"$f":"+AE116","v":4496442.7623530524}]
["Fixed Operating Costs ($/year)",{"$f":"fixed*INFLATION_FACTOR","v":123265.25065055313},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Tax coefficient",1,{"$f":"-total_tax_rate","v":-0.25739999999999996},1,{"$f":"1-total_tax_rate","v":0.74260000000000004},-1,{"$f":"1-total_tax_rate","v":0.74260000000000004}]
["Other Raw Material ($/year)",{"$f":"total_other_raw*INFLATION_FACTOR","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LCOE cost contribution factors",{"$f":"+X55*X56","v":1735318.2870998234},-500166.41532656061,186568.84132367116,{"$f":"+AA55*AA56","v":20284414.641533811},{"$f":"+AB55*AB56","v":0},{"$f":"+AC55*AC56","v":3339058.3953233771}]
["Other Variable O&M Costs (not including tax credits and incentives)",{"$f":"(var_misc+royalties+operator_profit+CO2_OandMcost+waste_treat+solidwaste_treat)*INFLATION_FACTOR","v":2519.0363342095493}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Target after-tax nominal IRR",{"$f":"+(1+real_irr)*(1+inflation_rate)-1","v":0.10051999999999994}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+D16","v":"Hydrogen Cost (Year 2016 Real $/kg)"},{"$f":"+SUM(X57:AB57)/AC57*(1+inflation_rate)^construct/INFLATION_FACTOR","v":6.750047990935756}]
[]
[]
["CASH FLOW ANALYSIS"]
["Actual Year\n(beginning of year)","Analysis Year","Operation Year","Plant Life","Inflation Price Increase Factor","Revenue from Hydrogen Sales","Portion of Initial Depreciable Capital Investment Financed with Debt (value ONLY used in debt financing calculations)","Initial Equity Depreciable Capital","Yearly Replacement Costs","Cash from Working Capital Reserve","Other Non-Depreciable Capital Costs","Salvage Value","Decommissioning Costs","Fixed Operating Cost","Feedstock Cost","Other Raw Material Cost","Revenue from Byproduct Sales","Other Variable Operating Costs","Debt Interest","Pre-Depreciation Income","Depreciation Charge","Taxable Income","Tax Rate","Total Taxes","After-Tax Income","Principal Payment","After-Tax Post-Depreciation Cash Flow","Cumulative Cash Flow","Pre-Tax Cash Flow",null,"H2 sales (kg/year)","Tax Credit"]
[{"$f":"startup_year-construct","v":2014},1,{"$f":"IF(construct=0,1,-construct)","v":-1},{"$f":"IF(C65=\"\",\"\",IF(C65<=plant_life,C65,IF(D64=plant_life,1,D64+1)))","v":-1},{"$f":"IF(C65=\"\",\"\",(1+inflation_rate)^(A65-$B$25))","v":0.9813542688910698},{"$f":"IF(C65=\"\",\"\",IF(C65<0,0,IF(AND(C65=1,start_time<1),E65*(H2_price_nominal*output_kgyear*start_time*percnt_revs+H2_price_nominal*output_kgyear*(1-start_time)),IF(C65<=start_time,H2_price_nominal*E65*output_kgyear*percnt_revs,H2_price_nominal*output_kgyear*E65))))","v":0},{"$f":"-$B$31*depr_cap_infl*E65","v":-1267062.1105808259},{"$f":"IF(C65<0,-E65*equity*depr_cap_infl*percent_cap1,IF(C65=1,-E65*equity*depr_cap_infl,0))","v":-844708.07372055063},{"$f":"IF(OR(C65<0,C65=\"\"),\"\",-E65*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C65,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":""},{"$f":"IF(AND(C65>=1,C65<anal_period),WorkingCap*SUM(N65:R65)-WorkingCap*SUM(N64:R64),0)","v":0},{"$f":"IF(C65=-construct,-E65*non_dep_infl,\"\")","v":0},{"$f":"IF(C65=anal_period,salvage*E65,\"\")","v":""},{"$f":"IF(D65=plant_life,-E65*decom,\"\")","v":""},{"$f":"IF(C65=\"\",\"\",IF(C65<0,0,IF(AND(C65=1,start_time<1),-(inflated_fixed*percnt_fixed*start_time+(inflated_fixed*(1-start_time))),IF(C65<=start_time,-inflated_fixed*percnt_fixed*E65,-inflated_fixed*E65))))","v":0},{"$f":"IF(C65=\"\",\"\",IF(C65<0,0,IF(AND(C65=1,start_time<1),-(SUM(B139:E139)*output_kgyear*E65*percnt_var*start_time+SUM(B139:E139)*output_kgyear*E65*(1-start_time)),IF(C65<=start_time,-SUM(B139:E139)*output_kgyear*E65*percnt_var,-SUM(B139:E139)*output_kgyear*E65))))","v":0},{"$f":"IF(C65=\"\",\"\",IF(C65<0,0,IF(AND(C65=1,start_time<1),-(inflated_otherraw*E65*percnt_var*start_time+inflated_otherraw*E65*(1-start_time)),IF(C65<=start_time,-inflated_otherraw*E65*percnt_var,-(inflated_otherraw*E65)))))","v":0},{"$f":"IF(C65=\"\",\"\",IF(C65<0,0,IF(AND(C65=1,start_time<1),SUM(K139:N139,T139:V139)*output_kgyear*E65*percnt_revs*start_time+SUM(K139:N139,T139:V139)*output_kgyear*E65*(1-start_time),IF(C65<=start_time,SUM(K139:N139,T139:V139)*output_kgyear*E65*percnt_revs,SUM(K139:N139,T139:V139)*output_kgyear*E65))))","v":0},{"$f":"IF(C65=\"\",\"\",IF(C65<0,0,IF(AND(C65=1,start_time<1),-((SUM(F139:J139,P139:R139)*output_kgyear+inflated_othervar)*E65*percnt_var*start_time+(SUM(F139:J139,P139:R139)*output_kgyear+inflated_othervar)*E65*(1-start_time)),IF(C65<=start_time,-(SUM(F139:J139,P139:R139)*output_kgyear+inflated_othervar)*E65*percnt_var,-E65*(SUM(F139:J139,P139:R139)*output_kgyear+inflated_othervar)))))","v":0},{"$f":"IF(B65=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E14))","v":-46881.298091490557},{"$f":"IF(C65=\"\",\"\",F65+SUM(L65:S65))","v":-46881.298091490557},{"$f":"IF(C65=\"\",\"\",IF(C65<-1,0,IF(C65=anal_period,-LOOKUP(C65,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C65,depr_yr,depr_cost))))","v":0},{"$f":"IF(C65=\"\",\"\",SUM(T65:U65))","v":-46881.298091490557},{"$f":"IF(C65=\"\",\"\",$B$33)","v":0.25739999999999996},{"$f":"IF(C65=\"\",\"\",tax_credit-(V65*W65 +Upstream_CO2_taxpYear + Proc_CO2_taxpYear))","v":12067.246128749668},{"$f":"IF(C65=\"\",\"\",SUM(T65,X65))","v":-34814.051962740887},{"$f":"IF(C65=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F14))","v":0},{"$f":"IF(C65=\"\",\"\",SUM(H65,I65,J65,K65,T65,X65,Z65))","v":-879522.12568329147},{"$f":"AA65","v":-879522.12568329147},{"$f":"IF(C65=\"\",\"\",SUM(H65,I65,J65,K65,T65,Z65))","v":-891589.37181204115},null,{"$f":"IF(C65=\"\",\"\",IF(C65<0,0,IF(AND(C65=1,start_time<1),(output_kgyear*start_time*percnt_revs+output_kgyear*(1-start_time)),IF(C65<=start_time,output_kgyear*percnt_revs,output_kgyear))))","v":0},{"$f":"IF(C65=\"\",\"\",tax_credit)","v":0}]
[{"$f":"IF(B66<>\"\",A65+1,\"\")","v":2015},{"$f":"IF(MAX($B$65:B65)<(construct+anal_period),B65+1,\"\")","v":2},{"$f":"IF(B66=\"\",\"\",IF(C65=-1,1,C65+1))","v":1},1,1,2214489.3704983238,null,{"$f":"IF(C66<0,-E66*equity*depr_cap_infl*percent_cap2,0)","v":0},{"$f":"IF(OR(C66<0,C66=\"\"),\"\",-E66*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C66,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":0},{"$f":"IF(AND(C66>=1,C66<anal_period),WorkingCap*SUM(N66:R66)-WorkingCap*SUM(N65:R65),IF(C66<0,0,IF(B66=\"\",\"\",-SUM(J$65:J65))))","v":-263868.71350209083},"","","",-105391.78930622293,-1647448.7526047856,0,0,-6284.2147695969143,{"$f":"IF(B66=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E15))","v":-46881.298091490557},408483.31572622783,{"$f":"IF(C66=\"\",\"\",IF(C66<-1,0,IF(C66=anal_period,-LOOKUP(C66,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C66,depr_yr,depr_cost))))","v":-301771.95933666668},106711.35638956114,0.25739999999999996,-27467.503134673036,381015.81259155477,{"$f":"IF(C66=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F15))","v":0},117147.09908946395,{"$f":"IF(C66=\"\",\"\",AB65+AA66)","v":-762375.02659382753},144614.60222413699,null,334303.5,0]
[2016,{"$f":"IF(MAX($B$65:B66)<(construct+anal_period),B66+1,\"\")","v":3},2,2,1.0189999999999999,3178260.0965321008,null,{"$f":"IF(C67<0,-E67*equity*depr_cap_infl*percent_cap3,0)","v":0},{"$f":"IF(OR(C67<0,C67=\"\"),\"\",-E67*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C67,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":0},{"$f":"IF(AND(C67>=1,C67<anal_period),WorkingCap*SUM(N67:R67)-WorkingCap*SUM(N66:R66),IF(C67<0,0,IF(B67=\"\",\"\",-SUM(J$65:J66))))","v":-105491.26425879501},"","","",-125607.29041291363,-2327773.3854809464,0,0,-9019.1758453792318,{"$f":"IF(B67=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E16))","v":-46881.298091490557},668978.94670137111,{"$f":"IF(C67=\"\",\"\",IF(C67<-1,0,IF(C67=anal_period,-LOOKUP(C67,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C67,depr_yr,depr_cost))))","v":-517172.51813540707},151806.42856596404,0.25739999999999996,-39074.974712879142,629903.97198849195,{"$f":"IF(C67=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F16))","v":0},524412.70772969699,-237962.31886413053,563487.68244257616,null,470850,0]
[2017,{"$f":"IF(MAX($B$65:B67)<(construct+anal_period),B67+1,\"\")","v":4},3,3,1.0383609999999999,3238647.0383662106,null,{"$f":"IF(C68<0,-E68*equity*depr_cap_infl*percent_cap4,0)","v":0},{"$f":"IF(OR(C68<0,C68=\"\"),\"\",-E68*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C68,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":0},{"$f":"IF(AND(C68>=1,C68<anal_period),WorkingCap*SUM(N68:R68)-WorkingCap*SUM(N67:R67),IF(C68<0,0,IF(B68=\"\",\"\",-SUM(J$65:J67))))","v":-7037.6466893266188},"","","",-127993.82893075899,-2372133.1272175494,0,0,-9190.5401864414362,{"$f":"IF(B68=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E17))","v":-46881.298091490557},682448.24393997015,{"$f":"IF(C68=\"\",\"\",IF(C68<-1,0,IF(C68=anal_period,-LOOKUP(C68,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C68,depr_yr,depr_cost))))","v":-369348.60523431073},313099.63870565942,0.25739999999999996,-80591.84700283673,{"$f":"IF(C68=\"\",\"\",SUM(T68,X68))","v":601856.3969371334},{"$f":"IF(C68=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F17))","v":0},594818.75024780678,356856.43138367624,675410.59725064354,null,470850,0]
[2018,{"$f":"IF(MAX($B$65:B68)<(construct+anal_period),B68+1,\"\")","v":5},4,4,1.0580898589999999,3300181.332095169,null,{"$f":"IF(C69=\"\",\"\",0)","v":0},{"$f":"IF(OR(C69<0,C69=\"\"),\"\",-E69*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C69,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":0},{"$f":"IF(AND(C69>=1,C69<anal_period),WorkingCap*SUM(N69:R69)-WorkingCap*SUM(N68:R68),IF(C69<0,0,IF(B69=\"\",\"\",-SUM(J$65:J68))))","v":-118631.80529851955},"","","",-130425.7116804434,-3160405.3261944526,0,0,-9365.1604499838231,{"$f":"IF(B69=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E18))","v":-46881.298091490557},-46896.164321201853,{"$f":"IF(C69=\"\",\"\",IF(C69<-1,0,IF(C69=anal_period,-LOOKUP(C69,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C69,depr_yr,depr_cost))))","v":-263760.0960192419},-310656.26034044375,0.25739999999999996,79962.921411630217,33066.757090428364,{"$f":"IF(C69=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F18))","v":0},-85565.04820809119,271291.38317558507,-165527.96961972141,null,470850,0]
[2019,{"$f":"IF(MAX($B$65:B69)<(construct+anal_period),B69+1,\"\")","v":6},5,5,1.0781935663209998,3362884.777404977,null,0,{"$f":"IF(OR(C70<0,C70=\"\"),\"\",-E70*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C70,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":0},{"$f":"IF(AND(C70>=1,C70<anal_period),WorkingCap*SUM(N70:R70)-WorkingCap*SUM(N69:R69),IF(C70<0,0,IF(B70=\"\",\"\",-SUM(J$65:J69))))","v":-8154.9468591763289},"","","",-132903.80020237181,-3212115.6120184837,0,0,-9543.0984985335162,{"$f":"IF(B70=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E19))","v":-46881.298091490557},-38559.031405902933,{"$f":"IF(C70=\"\",\"\",IF(C70<-1,0,IF(C70=anal_period,-LOOKUP(C70,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C70,depr_yr,depr_cost))))","v":-188581.07745811291},-227140.10886401584,0.25739999999999996,58465.86402159767,19906.832615694737,{"$f":"IF(C70=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F19))","v":0},11751.885756518408,283043.26893210347,-46713.978265079262,null,470850,0]
[2020,{"$f":"IF(MAX($B$65:B70)<(construct+anal_period),B70+1,\"\")","v":7},6,6,1.0986792440810986,3426779.5881756707,null,0,{"$f":"IF(OR(C71<0,C71=\"\"),\"\",-E71*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C71,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":-252446.70767227848},{"$f":"IF(AND(C71>=1,C71<anal_period),WorkingCap*SUM(N71:R71)-WorkingCap*SUM(N70:R70),IF(C71<0,0,IF(B71=\"\",\"\",-SUM(J$65:J70))))","v":-13677.387227493338},"","","",-135428.97240621687,-3300591.7024597889,0,0,-9724.4173700056508,{"$f":"IF(B71=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E20))","v":-46881.298091490557},-65846.802151831333,{"$f":"IF(C71=\"\",\"\",IF(C71<-1,0,IF(C71=anal_period,-LOOKUP(C71,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C71,depr_yr,depr_cost))))","v":-224444.53496605135},-290291.33711788268,0.25739999999999996,74720.990174142993,8874.1880223116605,{"$f":"IF(C71=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F20))","v":0},-257249.90687746019,25793.362054643279,-331970.89705160318,null,470850,0]
[2021,{"$f":"IF(MAX($B$65:B71)<(construct+anal_period),B71+1,\"\")","v":8},7,7,1.1195541497186396,3491888.4003510089,null,0,{"$f":"IF(OR(C72<0,C72=\"\"),\"\",-E72*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C72,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":0},{"$f":"IF(AND(C72>=1,C72<anal_period),WorkingCap*SUM(N72:R72)-WorkingCap*SUM(N71:R71),IF(C72<0,0,IF(B72=\"\",\"\",-SUM(J$65:J71))))","v":-14193.397297140735},"","","",-138002.12288193501,-3392456.4367016456,0,0,-9909.1813000357597,{"$f":"IF(B72=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E21))","v":-46881.298091490557},-95360.638624098152,{"$f":"IF(C72=\"\",\"\",IF(C72<-1,0,IF(C72=anal_period,-LOOKUP(C72,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C72,depr_yr,depr_cost))))","v":-250405.2761670539},-345765.91479115206,0.25739999999999996,89000.146467242521,-6360.492156855631,{"$f":"IF(C72=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F21))","v":0},-20553.889453996366,5239.4726006469136,-109554.03592123889,null,470850,0]
[2022,{"$f":"IF(MAX($B$65:B72)<(construct+anal_period),B72+1,\"\")","v":9},8,8,1.1408256785632938,3558234.2799576782,null,0,{"$f":"IF(OR(C73<0,C73=\"\"),\"\",-E73*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C73,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":0},{"$f":"IF(AND(C73>=1,C73<anal_period),WorkingCap*SUM(N73:R73)-WorkingCap*SUM(N72:R72),IF(C73<0,0,IF(B73=\"\",\"\",-SUM(J$65:J72))))","v":-8191.3966213716194},"","","",-140624.16321669176,-3444255.4327313323,0,0,-10097.455744736439,{"$f":"IF(B73=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E22))","v":-46881.298091490557},-83624.069826573133,{"$f":"IF(C73=\"\",\"\",IF(C73<-1,0,IF(C73=anal_period,-LOOKUP(C73,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C73,depr_yr,depr_cost))))","v":-138337.8793917229},-221961.94921829604,0.25739999999999996,57133.005728789394,-26491.064097783739,{"$f":"IF(C73=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F22))","v":0},-34682.460719155359,-29442.988118508445,-91815.466447944753,null,470850,0]
[2023,{"$f":"IF(MAX($B$65:B73)<(construct+anal_period),B73+1,\"\")","v":10},9,9,1.1625013664559962,3625840.7312768735,null,0,{"$f":"IF(OR(C74<0,C74=\"\"),\"\",-E74*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C74,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":0},{"$f":"IF(AND(C74>=1,C74<anal_period),WorkingCap*SUM(N74:R74)-WorkingCap*SUM(N73:R73),IF(C74<0,0,IF(B74=\"\",\"\",-SUM(J$65:J73))))","v":-390.29561833909247},"","","",-143296.02231780891,-3443993.6927599921,0,0,-10289.307403886431,{"$f":"IF(B74=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E23))","v":-46881.298091490557},-18619.589296304621,{"$f":"IF(C74=\"\",\"\",IF(C74<-1,0,IF(C74=anal_period,-LOOKUP(C74,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C74,depr_yr,depr_cost))))","v":-31530.593788267583},-50150.1830845722,0.25739999999999996,12908.657125968883,-5710.9321703357382,{"$f":"IF(C74=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F23))","v":0},-6101.2277886748307,-35544.215907183272,-19009.884914643713,null,470850,0]
[2024,{"$f":"IF(MAX($B$65:B74)<(construct+anal_period),B74+1,\"\")","v":11},10,10,1.1845888924186601,3694731.7051711339,null,0,{"$f":"IF(OR(C75<0,C75=\"\"),\"\",-E75*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C75,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":0},{"$f":"IF(AND(C75>=1,C75<anal_period),WorkingCap*SUM(N75:R75)-WorkingCap*SUM(N74:R74),IF(C75<0,0,IF(B75=\"\",\"\",-SUM(J$65:J74))))","v":-3393.4977751247352},"","","",-146018.64674184725,-3463698.8899961119,0,0,-10484.804244560271,{"$f":"IF(B75=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E24))","v":-46881.298091490557},27648.066097124014,{"$f":"IF(C75=\"\",\"\",IF(C75<-1,0,IF(C75=anal_period,-LOOKUP(C75,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C75,depr_yr,depr_cost))))","v":-22543.490995134471},5104.5751019895433,0.25739999999999996,-1313.9176312521083,26334.148465871906,{"$f":"IF(C75=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F24))","v":0},22940.65069074717,-12603.565216436102,24254.568321999279,null,470850,0]
[2025,{"$f":"IF(MAX($B$65:B75)<(construct+anal_period),B75+1,\"\")","v":12},11,11,1.2070960813746145,3764931.6075693853,null,0,{"$f":"IF(OR(C76<0,C76=\"\"),\"\",-E76*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C76,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":-924526.52652047004},{"$f":"IF(AND(C76>=1,C76<anal_period),WorkingCap*SUM(N76:R76)-WorkingCap*SUM(N75:R75),IF(C76<0,0,IF(B76=\"\",\"\",-SUM(J$65:J75))))","v":-6666.8808514275588},"","","",-148793.00102994236,-3505171.1967702205,0,0,-10684.015525206916,{"$f":"IF(B76=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E25))","v":-46881.298091490557},53402.096152524929,{"$f":"IF(C76=\"\",\"\",IF(C76<-1,0,IF(C76=anal_period,-LOOKUP(C76,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C76,depr_yr,depr_cost))))","v":-154633.08696414242},-101230.99081161749,0.25739999999999996,26056.857034910339,79458.953187435269,{"$f":"IF(C76=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F25))","v":0},-851734.45418446232,-864338.01940089837,-877791.31121937267,null,470850,0]
[2026,{"$f":"IF(MAX($B$65:B76)<(construct+anal_period),B76+1,\"\")","v":13},12,12,1.2300309069207322,3836465.3081132038,null,0,{"$f":"IF(OR(C77<0,C77=\"\"),\"\",-E77*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C77,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":0},{"$f":"IF(AND(C77>=1,C77<anal_period),WorkingCap*SUM(N77:R77)-WorkingCap*SUM(N76:R76),IF(C77<0,0,IF(B77=\"\",\"\",-SUM(J$65:J76))))","v":6791.4248841910157},"","","",-151620.06804951126,-3456864.9675610652,0,0,-10887.011820185848,{"$f":"IF(B77=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E26))","v":-46881.298091490557},170211.96259095054,{"$f":"IF(C77=\"\",\"\",IF(C77<-1,0,IF(C77=anal_period,-LOOKUP(C77,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C77,depr_yr,depr_cost))))","v":-248960.03733999757},-78748.074749047024,0.25739999999999996,20269.7544404047,190481.71703135525,{"$f":"IF(C77=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F26))","v":0},197273.14191554626,-667064.8774853521,177003.38747514156,null,470850,0]
[2027,{"$f":"IF(MAX($B$65:B77)<(construct+anal_period),B77+1,\"\")","v":14},13,13,1.253401494152226,3909358.1489673541,null,0,{"$f":"IF(OR(C78<0,C78=\"\"),\"\",-E78*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C78,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":0},{"$f":"IF(AND(C78>=1,C78<anal_period),WorkingCap*SUM(N78:R78)-WorkingCap*SUM(N77:R77),IF(C78<0,0,IF(B78=\"\",\"\",-SUM(J$65:J77))))","v":-6889.6356554062804},"","","",-154500.84934245195,-3499708.2374129165,0,0,-11093.865044769378,{"$f":"IF(B78=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E27))","v":-46881.298091490557},197173.89907572558,{"$f":"IF(C78=\"\",\"\",IF(C78<-1,0,IF(C78=anal_period,-LOOKUP(C78,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C78,depr_yr,depr_cost))))","v":-172958.81265061384},24215.086425111745,0.25739999999999996,-6232.963245823762,190940.93582990181,{"$f":"IF(C78=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F27))","v":0},184051.30017449553,-483013.57731085655,190284.2634203193,null,470850,0]
[2028,{"$f":"IF(MAX($B$65:B78)<(construct+anal_period),B78+1,\"\")","v":15},14,14,1.277216122541118,3983635.9537977329,null,0,{"$f":"IF(OR(C79<0,C79=\"\"),\"\",-E79*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C79,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":0},{"$f":"IF(AND(C79>=1,C79<anal_period),WorkingCap*SUM(N79:R79)-WorkingCap*SUM(N78:R78),IF(C79<0,0,IF(B79=\"\",\"\",-SUM(J$65:J78))))","v":-2653.6609622200485},"","","",-157436.36547995851,-3514253.0109210266,0,0,-11304.648480619993,{"$f":"IF(B79=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E28))","v":-46881.298091490557},253760.63082463713,{"$f":"IF(C79=\"\",\"\",IF(C79<-1,0,IF(C79=anal_period,-LOOKUP(C79,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C79,depr_yr,depr_cost))))","v":-115473.36316240671},138287.26766223041,0.25739999999999996,-35595.142696258103,218165.48812837905,{"$f":"IF(C79=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F28))","v":0},215511.827166159,-267501.75014469755,251106.96986241709,null,470850,0]
[2029,{"$f":"IF(MAX($B$65:B79)<(construct+anal_period),B79+1,\"\")","v":16},15,15,1.3014832288693996,4059325.0369198909,null,0,{"$f":"IF(OR(C80<0,C80=\"\"),\"\",-E80*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C80,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":0},{"$f":"IF(AND(C80>=1,C80<anal_period),WorkingCap*SUM(N80:R80)-WorkingCap*SUM(N79:R79),IF(C80<0,0,IF(B80=\"\",\"\",-SUM(J$65:J79))))","v":-6865.8362950539449},"","","",-160427.65642407775,-3556819.1736228019,0,0,-11519.436801751775,{"$f":"IF(B80=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E29))","v":-46881.298091490557},283677.47197976895,{"$f":"IF(C80=\"\",\"\",IF(C80<-1,0,IF(C80=anal_period,-LOOKUP(C80,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C80,depr_yr,depr_cost))))","v":-82560.218818277979},201117.25316149095,0.25739999999999996,-51767.580963767767,231909.89101600117,{"$f":"IF(C80=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F29))","v":0},225044.05472094723,-42457.695423750323,276811.635684715,null,470850,0]
[2030,{"$f":"IF(MAX($B$65:B80)<(construct+anal_period),B80+1,\"\")","v":17},16,16,1.3262114102179181,4136452.2126213685,null,0,{"$f":"IF(OR(C81<0,C81=\"\"),\"\",-E81*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C81,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":-304727.4315871303},{"$f":"IF(AND(C81>=1,C81<anal_period),WorkingCap*SUM(N81:R81)-WorkingCap*SUM(N80:R80),IF(C81<0,0,IF(B81=\"\",\"\",-SUM(J$65:J80))))","v":-1572.5767720466247},"","","",-163475.78189613522,-3564036.0239984882,0,0,-11738.306100985059,{"$f":"IF(B81=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E30))","v":-46881.298091490557},350320.80253426917,{"$f":"IF(C81=\"\",\"\",IF(C81<-1,0,IF(C81=anal_period,-LOOKUP(C81,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C81,depr_yr,depr_cost))))","v":-126013.31613942684},224307.48639484233,0.25739999999999996,-57736.746998032409,292584.05553623673,{"$f":"IF(C81=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F30))","v":0},-13715.952822940162,-56173.648246690485,44020.794175092247,null,470850,0]
[2031,{"$f":"IF(MAX($B$65:B81)<(construct+anal_period),B81+1,\"\")","v":18},17,17,1.3514094270120585,4215044.8046611743,null,0,{"$f":"IF(OR(C82<0,C82=\"\"),\"\",-E82*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C82,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":0},{"$f":"IF(AND(C82>=1,C82<anal_period),WorkingCap*SUM(N82:R82)-WorkingCap*SUM(N81:R81),IF(C82<0,0,IF(B82=\"\",\"\",-SUM(J$65:J81))))","v":16501.504209771054},"","","",-166581.82175216178,-3450696.928261403,0,0,-11961.333916903774,{"$f":"IF(B82=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E31))","v":-46881.298091490557},538923.4226392149,{"$f":"IF(C82=\"\",\"\",IF(C82<-1,0,IF(C82=anal_period,-LOOKUP(C82,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C82,depr_yr,depr_cost))))","v":-157187.9668139662},381735.45582524873,0.25739999999999996,-98258.706329419016,440664.71630979585,{"$f":"IF(C82=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F31))","v":0},457166.22051956691,400992.57227287639,555424.92684898595,null,470850,0]
[2032,{"$f":"IF(MAX($B$65:B82)<(construct+anal_period),B82+1,\"\")","v":19},18,18,1.3770862061252875,4295130.6559497369,null,0,{"$f":"IF(OR(C83<0,C83=\"\"),\"\",-E83*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C83,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":0},{"$f":"IF(AND(C83>=1,C83<anal_period),WorkingCap*SUM(N83:R83)-WorkingCap*SUM(N82:R82),IF(C83<0,0,IF(B83=\"\",\"\",-SUM(J$65:J82))))","v":-14158.858865144779},"","","",-169746.87636545286,-3541697.0007379893,0,0,-12188.599261324945,{"$f":"IF(B83=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E32))","v":-46881.298091490557},524616.88149347901,{"$f":"IF(C83=\"\",\"\",IF(C83<-1,0,IF(C83=anal_period,-LOOKUP(C83,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C83,depr_yr,depr_cost))))","v":-94530.710867402056},430086.17062607699,0.25739999999999996,-110704.1803191522,413912.70117432682,{"$f":"IF(C83=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F32))","v":0},399753.84230918204,800746.41458205844,510458.02262833423,null,470850,0]
[2033,{"$f":"IF(MAX($B$65:B83)<(construct+anal_period),B83+1,\"\")","v":20},19,19,1.4032508440416678,4376738.1384127811,null,0,{"$f":"IF(OR(C84<0,C84=\"\"),\"\",-E84*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C84,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":0},{"$f":"IF(AND(C84>=1,C84<anal_period),WorkingCap*SUM(N84:R84)-WorkingCap*SUM(N83:R83),IF(C84<0,0,IF(B84=\"\",\"\",-SUM(J$65:J83))))","v":-11112.244032450486},"","","",-172972.06701639644,-3612321.8535840837,0,0,-12420.182647290118,{"$f":"IF(B84=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E33))","v":-46881.298091490557},532142.73707351973,{"$f":"IF(C84=\"\",\"\",IF(C84<-1,0,IF(C84=anal_period,-LOOKUP(C84,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C84,depr_yr,depr_cost))))","v":-38060.456205232571},494082.28086828714,0.25739999999999996,-127176.77909549708,404965.95797802263,{"$f":"IF(C84=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F33))","v":0},393853.71394557215,1194600.1285276306,521030.49304106925,null,470850,0]
[2034,{"$f":"IF(MAX($B$65:B84)<(construct+anal_period),B84+1,\"\")","v":21},20,20,1.4299126100784596,4459896.1630426245,null,0,{"$f":"IF(OR(C85<0,C85=\"\"),\"\",-E85*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C85,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":0},{"$f":"IF(AND(C85>=1,C85<anal_period),WorkingCap*SUM(N85:R85)-WorkingCap*SUM(N84:R84),IF(C85<0,0,IF(B85=\"\",\"\",-SUM(J$65:J84))))","v":569657.11548716552},"",307702.0105626536,-307702.0105626536,-176258.53628970796,-3685364.5341464262,0,0,-12656.166117588631,{"$f":"IF(B85=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E34))","v":-46881.298091490557},538735.6283974112,{"$f":"IF(C85=\"\",\"\",IF(C85<-1,0,IF(C85=anal_period,-LOOKUP(C85,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C85,depr_yr,depr_cost))))","v":-95196.849627819509},443538.77876959171,0.25739999999999996,-114166.88165529289,424568.74674211832,{"$f":"IF(C85=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F34))","v":-1267062.1105808259},-272836.24835154216,921763.88017608842,-158669.36669624923,null,470850,0]
["",{"$f":"IF(MAX($B$65:B85)<(construct+anal_period),B85+1,\"\")","v":""},"","","","",null,"",{"$f":"IF(OR(C86<0,C86=\"\"),\"\",-E86*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C86,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":""},{"$f":"IF(AND(C86>=1,C86<anal_period),WorkingCap*SUM(N86:R86)-WorkingCap*SUM(N85:R85),IF(C86<0,0,IF(B86=\"\",\"\",-SUM(J$65:J85))))","v":""},"","","","","","","","",{"$f":"IF(B86=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E35))","v":""},"",{"$f":"IF(C86=\"\",\"\",IF(C86<-1,0,IF(C86=anal_period,-LOOKUP(C86,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C86,depr_yr,depr_cost))))","v":""},"","","","",{"$f":"IF(C86=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F35))","v":""},"","","",null,"",""]
["",{"$f":"IF(MAX($B$65:B86)<(construct+anal_period),B86+1,\"\")","v":""},"","","","",null,"",{"$f":"IF(OR(C87<0,C87=\"\"),\"\",-E87*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C87,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":""},{"$f":"IF(AND(C87>=1,C87<anal_period),WorkingCap*SUM(N87:R87)-WorkingCap*SUM(N86:R86),IF(C87<0,0,IF(B87=\"\",\"\",-SUM(J$65:J86))))","v":""},"","","","","","","","",{"$f":"IF(B87=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E36))","v":""},"",{"$f":"IF(C87=\"\",\"\",IF(C87<-1,0,IF(C87=anal_period,-LOOKUP(C87,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C87,depr_yr,depr_cost))))","v":""},"","","","",{"$f":"IF(C87=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F36))","v":""},"","","",null,"",""]
["",{"$f":"IF(MAX($B$65:B87)<(construct+anal_period),B87+1,\"\")","v":""},"","","","",null,"",{"$f":"IF(OR(C88<0,C88=\"\"),\"\",-E88*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C88,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":""},{"$f":"IF(AND(C88>=1,C88<anal_period),WorkingCap*SUM(N88:R88)-WorkingCap*SUM(N87:R87),IF(C88<0,0,IF(B88=\"\",\"\",-SUM(J$65:J87))))","v":""},"","","","","","","","",{"$f":"IF(B88=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E37))","v":""},"",{"$f":"IF(C88=\"\",\"\",IF(C88<-1,0,IF(C88=anal_period,-LOOKUP(C88,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C88,depr_yr,depr_cost))))","v":""},"","","","",{"$f":"IF(C88=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F37))","v":""},"","","",null,"",""]
["",{"$f":"IF(MAX($B$65:B88)<(construct+anal_period),B88+1,\"\")","v":""},"","","","",null,"",{"$f":"IF(OR(C89<0,C89=\"\"),\"\",-E89*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C89,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":""},{"$f":"IF(AND(C89>=1,C89<anal_period),WorkingCap*SUM(N89:R89)-WorkingCap*SUM(N88:R88),IF(C89<0,0,IF(B89=\"\",\"\",-SUM(J$65:J88))))","v":""},"","","","","","","","",{"$f":"IF(B89=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E38))","v":""},"",{"$f":"IF(C89=\"\",\"\",IF(C89<-1,0,IF(C89=anal_period,-LOOKUP(C89,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C89,depr_yr,depr_cost))))","v":""},"","","","",{"$f":"IF(C89=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F38))","v":""},"","","",null,"",""]
["",{"$f":"IF(MAX($B$65:B89)<(construct+anal_period),B89+1,\"\")","v":""},"","","","",null,"",{"$f":"IF(OR(C90<0,C90=\"\"),\"\",-E90*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C90,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":""},{"$f":"IF(AND(C90>=1,C90<anal_period),WorkingCap*SUM(N90:R90)-WorkingCap*SUM(N89:R89),IF(C90<0,0,IF(B90=\"\",\"\",-SUM(J$65:J89))))","v":""},"","","","","","","","",{"$f":"IF(B90=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E39))","v":""},"",{"$f":"IF(C90=\"\",\"\",IF(C90<-1,0,IF(C90=anal_period,-LOOKUP(C90,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C90,depr_yr,depr_cost))))","v":""},"","","","",{"$f":"IF(C90=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F39))","v":""},"","","",null,"",""]
["",{"$f":"IF(MAX($B$65:B90)<(construct+anal_period),B90+1,\"\")","v":""},"","","","",null,"",{"$f":"IF(OR(C91<0,C91=\"\"),\"\",-E91*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C91,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":""},{"$f":"IF(AND(C91>=1,C91<anal_period),WorkingCap*SUM(N91:R91)-WorkingCap*SUM(N90:R90),IF(C91<0,0,IF(B91=\"\",\"\",-SUM(J$65:J90))))","v":""},"","","","","","","","",{"$f":"IF(B91=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E40))","v":""},"",{"$f":"IF(C91=\"\",\"\",IF(C91<-1,0,IF(C91=anal_period,-LOOKUP(C91,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C91,depr_yr,depr_cost))))","v":""},"","","","",{"$f":"IF(C91=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F40))","v":""},"","","",null,"",""]
["",{"$f":"IF(MAX($B$65:B91)<(construct+anal_period),B91+1,\"\")","v":""},"","","","",null,"",{"$f":"IF(OR(C92<0,C92=\"\"),\"\",-E92*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C92,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":""},{"$f":"IF(AND(C92>=1,C92<anal_period),WorkingCap*SUM(N92:R92)-WorkingCap*SUM(N91:R91),IF(C92<0,0,IF(B92=\"\",\"\",-SUM(J$65:J91))))","v":""},"","","","","","","","",{"$f":"IF(B92=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E41))","v":""},"",{"$f":"IF(C92=\"\",\"\",IF(C92<-1,0,IF(C92=anal_period,-LOOKUP(C92,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C92,depr_yr,depr_cost))))","v":""},"","","","",{"$f":"IF(C92=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F41))","v":""},"","","",null,"",""]
["",{"$f":"IF(MAX($B$65:B92)<(construct+anal_period),B92+1,\"\")","v":""},"","","","",null,"",{"$f":"IF(OR(C93<0,C93=\"\"),\"\",-E93*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C93,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":""},{"$f":"IF(AND(C93>=1,C93<anal_period),WorkingCap*SUM(N93:R93)-WorkingCap*SUM(N92:R92),IF(C93<0,0,IF(B93=\"\",\"\",-SUM(J$65:J92))))","v":""},"","","","","","","","",{"$f":"IF(B93=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E42))","v":""},"",{"$f":"IF(C93=\"\",\"\",IF(C93<-1,0,IF(C93=anal_period,-LOOKUP(C93,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C93,depr_yr,depr_cost))))","v":""},"","","","",{"$f":"IF(C93=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F42))","v":""},"","","",null,"",""]
["",{"$f":"IF(MAX($B$65:B93)<(construct+anal_period),B93+1,\"\")","v":""},"","","","",null,"",{"$f":"IF(OR(C94<0,C94=\"\"),\"\",-E94*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C94,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":""},{"$f":"IF(AND(C94>=1,C94<anal_period),WorkingCap*SUM(N94:R94)-WorkingCap*SUM(N93:R93),IF(C94<0,0,IF(B94=\"\",\"\",-SUM(J$65:J93))))","v":""},"","","","","","","","",{"$f":"IF(B94=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E43))","v":""},"",{"$f":"IF(C94=\"\",\"\",IF(C94<-1,0,IF(C94=anal_period,-LOOKUP(C94,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C94,depr_yr,depr_cost))))","v":""},"","","","",{"$f":"IF(C94=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F43))","v":""},"","","",null,"",""]
["",{"$f":"IF(MAX($B$65:B94)<(construct+anal_period),B94+1,\"\")","v":""},"","","","",null,"",{"$f":"IF(OR(C95<0,C95=\"\"),\"\",-E95*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C95,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":""},{"$f":"IF(AND(C95>=1,C95<anal_period),WorkingCap*SUM(N95:R95)-WorkingCap*SUM(N94:R94),IF(C95<0,0,IF(B95=\"\",\"\",-SUM(J$65:J94))))","v":""},"","","","","","","","",{"$f":"IF(B95=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E44))","v":""},"",{"$f":"IF(C95=\"\",\"\",IF(C95<-1,0,IF(C95=anal_period,-LOOKUP(C95,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C95,depr_yr,depr_cost))))","v":""},"","","","",{"$f":"IF(C95=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F44))","v":""},"","","",null,"",""]
["",{"$f":"IF(MAX($B$65:B95)<(construct+anal_period),B95+1,\"\")","v":""},"","","","",null,"",{"$f":"IF(OR(C96<0,C96=\"\"),\"\",-E96*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C96,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":""},{"$f":"IF(AND(C96>=1,C96<anal_period),WorkingCap*SUM(N96:R96)-WorkingCap*SUM(N95:R95),IF(C96<0,0,IF(B96=\"\",\"\",-SUM(J$65:J95))))","v":""},"","","","","","","","",{"$f":"IF(B96=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E45))","v":""},"",{"$f":"IF(C96=\"\",\"\",IF(C96<-1,0,IF(C96=anal_period,-LOOKUP(C96,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C96,depr_yr,depr_cost))))","v":""},"","","","",{"$f":"IF(C96=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F45))","v":""},"","","",null,"",""]
["",{"$f":"IF(MAX($B$65:B96)<(construct+anal_period),B96+1,\"\")","v":""},"",{"$f":"IF(C97=\"\",\"\",IF(C97<=plant_life,C97,IF(D96=plant_life,1,D96+1)))","v":""},{"$f":"IF(C97=\"\",\"\",(1+inflation_rate)^(A97-$B$25))","v":""},{"$f":"IF(C97=\"\",\"\",IF(C97<0,0,IF(AND(C97=1,start_time<1),E97*(H2_price_nominal*output_kgyear*start_time*percnt_revs+H2_price_nominal*output_kgyear*(1-start_time)),IF(C97<=start_time,H2_price_nominal*E97*output_kgyear*percnt_revs,H2_price_nominal*output_kgyear*E97))))","v":""},null,"",{"$f":"IF(OR(C97<0,C97=\"\"),\"\",-E97*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C97,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":""},{"$f":"IF(AND(C97>=1,C97<anal_period),WorkingCap*SUM(N97:R97)-WorkingCap*SUM(N96:R96),IF(C97<0,0,IF(B97=\"\",\"\",-SUM(J$65:J96))))","v":""},{"$f":"IF(C97=-construct,-E97*non_dep_infl,\"\")","v":""},{"$f":"IF(C97=anal_period,salvage*E97,\"\")","v":""},{"$f":"IF(D97=plant_life,-E97*decom,\"\")","v":""},{"$f":"IF(C97=\"\",\"\",IF(C97<0,0,IF(AND(C97=1,start_time<1),-(inflated_fixed*percnt_fixed*start_time+(inflated_fixed*(1-start_time))),IF(C97<=start_time,-inflated_fixed*percnt_fixed*E97,-inflated_fixed*E97))))","v":""},{"$f":"IF(C97=\"\",\"\",IF(C97<0,0,IF(AND(C97=1,start_time<1),-(SUM(B171:E171)*output_kgyear*E97*percnt_var*start_time+SUM(B171:E171)*output_kgyear*E97*(1-start_time)),IF(C97<=start_time,-SUM(B171:E171)*output_kgyear*E97*percnt_var,-SUM(B171:E171)*output_kgyear*E97))))","v":""},{"$f":"IF(C97=\"\",\"\",IF(C97<0,0,IF(AND(C97=1,start_time<1),-(inflated_otherraw*E97*percnt_var*start_time+inflated_otherraw*E97*(1-start_time)),IF(C97<=start_time,-inflated_otherraw*E97*percnt_var,-(inflated_otherraw*E97)))))","v":""},"",{"$f":"IF(C97=\"\",\"\",IF(C97<0,0,IF(AND(C97=1,start_time<1),-((SUM(F171:J171,P171:R171)*output_kgyear+inflated_othervar)*E97*percnt_var*start_time+(SUM(F171:J171,P171:R171)*output_kgyear+inflated_othervar)*E97*(1-start_time)),IF(C97<=start_time,-(SUM(F171:J171,P171:R171)*output_kgyear+inflated_othervar)*E97*percnt_var,-E97*(SUM(F171:J171,P171:R171)*output_kgyear+inflated_othervar)))))","v":""},{"$f":"IF(B97=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E46))","v":""},{"$f":"IF(C97=\"\",\"\",F97+SUM(L97:S97))","v":""},{"$f":"IF(C97=\"\",\"\",IF(C97<-1,0,IF(C97=anal_period,-LOOKUP(C97,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C97,depr_yr,depr_cost))))","v":""},{"$f":"IF(C97=\"\",\"\",SUM(T97:U97))","v":""},{"$f":"IF(C97=\"\",\"\",$B$33)","v":""},{"$f":"IF(C97=\"\",\"\",tax_credit-(V97*W97 +Upstream_CO2_taxpYear + Proc_CO2_taxpYear))","v":""},{"$f":"IF(C97=\"\",\"\",SUM(T97,X97))","v":""},{"$f":"IF(C97=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F46))","v":""},{"$f":"IF(C97=\"\",\"\",SUM(H97,I97,J97,K97,T97,X97,Z97))","v":""},"",{"$f":"IF(C97=\"\",\"\",SUM(H97,I97,J97,K97,T97,Z97))","v":""},null,{"$f":"IF(C97=\"\",\"\",IF(C97<0,0,IF(AND(C97=1,start_time<1),(output_kgyear*start_time*percnt_revs+output_kgyear*(1-start_time)),IF(C97<=start_time,output_kgyear*percnt_revs,output_kgyear))))","v":""},{"$f":"IF(C97=\"\",\"\",tax_credit)","v":""}]
["",{"$f":"IF(MAX($B$65:B97)<(construct+anal_period),B97+1,\"\")","v":""},"","","","",null,"",{"$f":"IF(OR(C98<0,C98=\"\"),\"\",-E98*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C98,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":""},{"$f":"IF(AND(C98>=1,C98<anal_period),WorkingCap*SUM(N98:R98)-WorkingCap*SUM(N97:R97),IF(C98<0,0,IF(B98=\"\",\"\",-SUM(J$65:J97))))","v":""},"","","","","","","","",{"$f":"IF(B98=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E47))","v":""},"",{"$f":"IF(C98=\"\",\"\",IF(C98<-1,0,IF(C98=anal_period,-LOOKUP(C98,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C98,depr_yr,depr_cost))))","v":""},"","","","",{"$f":"IF(C98=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F47))","v":""},"","","",null,"",""]
["",{"$f":"IF(MAX($B$65:B98)<(construct+anal_period),B98+1,\"\")","v":""},"","","","",null,"",{"$f":"IF(OR(C99<0,C99=\"\"),\"\",-E99*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C99,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":""},{"$f":"IF(AND(C99>=1,C99<anal_period),WorkingCap*SUM(N99:R99)-WorkingCap*SUM(N98:R98),IF(C99<0,0,IF(B99=\"\",\"\",-SUM(J$65:J98))))","v":""},"","","","","","","","",{"$f":"IF(B99=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E48))","v":""},"",{"$f":"IF(C99=\"\",\"\",IF(C99<-1,0,IF(C99=anal_period,-LOOKUP(C99,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C99,depr_yr,depr_cost))))","v":""},"","","","",{"$f":"IF(C99=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F48))","v":""},"","","",null,"",""]
["",{"$f":"IF(MAX($B$65:B99)<(construct+anal_period),B99+1,\"\")","v":""},"","","","",null,"",{"$f":"IF(OR(C100<0,C100=\"\"),\"\",-E100*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C100,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":""},{"$f":"IF(AND(C100>=1,C100<anal_period),WorkingCap*SUM(N100:R100)-WorkingCap*SUM(N99:R99),IF(C100<0,0,IF(B100=\"\",\"\",-SUM(J$65:J99))))","v":""},"","","","","","","","",{"$f":"IF(B100=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E49))","v":""},"",{"$f":"IF(C100=\"\",\"\",IF(C100<-1,0,IF(C100=anal_period,-LOOKUP(C100,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C100,depr_yr,depr_cost))))","v":""},"","","","",{"$f":"IF(C100=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F49))","v":""},"","","",null,"",""]
["",{"$f":"IF(MAX($B$65:B100)<(construct+anal_period),B100+1,\"\")","v":""},"","","","",null,"",{"$f":"IF(OR(C101<0,C101=\"\"),\"\",-E101*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C101,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":""},{"$f":"IF(AND(C101>=1,C101<anal_period),WorkingCap*SUM(N101:R101)-WorkingCap*SUM(N100:R100),IF(C101<0,0,IF(B101=\"\",\"\",-SUM(J$65:J100))))","v":""},"","","","","","","","",{"$f":"IF(B101=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E50))","v":""},"",{"$f":"IF(C101=\"\",\"\",IF(C101<-1,0,IF(C101=anal_period,-LOOKUP(C101,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C101,depr_yr,depr_cost))))","v":""},"","","","",{"$f":"IF(C101=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F50))","v":""},"","","",null,"",""]
["",{"$f":"IF(MAX($B$65:B101)<(construct+anal_period),B101+1,\"\")","v":""},"","","","",null,"",{"$f":"IF(OR(C102<0,C102=\"\"),\"\",-E102*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C102,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":""},{"$f":"IF(AND(C102>=1,C102<anal_period),WorkingCap*SUM(N102:R102)-WorkingCap*SUM(N101:R101),IF(C102<0,0,IF(B102=\"\",\"\",-SUM(J$65:J101))))","v":""},"","","","","","","","",{"$f":"IF(B102=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E51))","v":""},"",{"$f":"IF(C102=\"\",\"\",IF(C102<-1,0,IF(C102=anal_period,-LOOKUP(C102,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C102,depr_yr,depr_cost))))","v":""},"","","","",{"$f":"IF(C102=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F51))","v":""},"","","",null,"",""]
["",{"$f":"IF(MAX($B$65:B102)<(construct+anal_period),B102+1,\"\")","v":""},"","","","",null,"",{"$f":"IF(OR(C103<0,C103=\"\"),\"\",-E103*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C103,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":""},{"$f":"IF(AND(C103>=1,C103<anal_period),WorkingCap*SUM(N103:R103)-WorkingCap*SUM(N102:R102),IF(C103<0,0,IF(B103=\"\",\"\",-SUM(J$65:J102))))","v":""},"","","","","","","","",{"$f":"IF(B103=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E52))","v":""},"",{"$f":"IF(C103=\"\",\"\",IF(C103<-1,0,IF(C103=anal_period,-LOOKUP(C103,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C103,depr_yr,depr_cost))))","v":""},"","","","",{"$f":"IF(C103=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F52))","v":""},"","","",null,"",""]
["",{"$f":"IF(MAX($B$65:B103)<(construct+anal_period),B103+1,\"\")","v":""},"","","","",null,"",{"$f":"IF(OR(C104<0,C104=\"\"),\"\",-E104*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C104,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":""},{"$f":"IF(AND(C104>=1,C104<anal_period),WorkingCap*SUM(N104:R104)-WorkingCap*SUM(N103:R103),IF(C104<0,0,IF(B104=\"\",\"\",-SUM(J$65:J103))))","v":""},"","","","","","","","",{"$f":"IF(B104=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E53))","v":""},"",{"$f":"IF(C104=\"\",\"\",IF(C104<-1,0,IF(C104=anal_period,-LOOKUP(C104,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C104,depr_yr,depr_cost))))","v":""},"","","","",{"$f":"IF(C104=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F53))","v":""},"","","",null,"",""]
["",{"$f":"IF(MAX($B$65:B104)<(construct+anal_period),B104+1,\"\")","v":""},"","","","",null,"",{"$f":"IF(OR(C105<0,C105=\"\"),\"\",-E105*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C105,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":""},{"$f":"IF(AND(C105>=1,C105<anal_period),WorkingCap*SUM(N105:R105)-WorkingCap*SUM(N104:R104),IF(C105<0,0,IF(B105=\"\",\"\",-SUM(J$65:J104))))","v":""},"","","","","","","","",{"$f":"IF(B105=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E54))","v":""},"",{"$f":"IF(C105=\"\",\"\",IF(C105<-1,0,IF(C105=anal_period,-LOOKUP(C105,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C105,depr_yr,depr_cost))))","v":""},"","","","",{"$f":"IF(C105=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F54))","v":""},"","","",null,"",""]
["",{"$f":"IF(MAX($B$65:B105)<(construct+anal_period),B105+1,\"\")","v":""},"","","","",null,"",{"$f":"IF(OR(C106<0,C106=\"\"),\"\",-E106*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C106,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":""},{"$f":"IF(AND(C106>=1,C106<anal_period),WorkingCap*SUM(N106:R106)-WorkingCap*SUM(N105:R105),IF(C106<0,0,IF(B106=\"\",\"\",-SUM(J$65:J105))))","v":""},"","","","","","","","",{"$f":"IF(B106=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E55))","v":""},{"$f":"IF(C106=\"\",\"\",F106+SUM(L106:S106))","v":""},{"$f":"IF(C106=\"\",\"\",IF(C106<-1,0,IF(C106=anal_period,-LOOKUP(C106,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C106,depr_yr,depr_cost))))","v":""},"","","","",{"$f":"IF(C106=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F55))","v":""},"","",{"$f":"IF(C106=\"\",\"\",SUM(H106,I106,J106,K106,T106,Z106))","v":""},null,"",""]
["",{"$f":"IF(MAX($B$65:B106)<(construct+anal_period),B106+1,\"\")","v":""},"","","","",null,"",{"$f":"IF(OR(C107<0,C107=\"\"),\"\",-E107*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C107,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":""},{"$f":"IF(AND(C107>=1,C107<anal_period),WorkingCap*SUM(N107:R107)-WorkingCap*SUM(N106:R106),IF(C107<0,0,IF(B107=\"\",\"\",-SUM(J$65:J106))))","v":""},"","","","","","","","",{"$f":"IF(B107=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E56))","v":""},"",{"$f":"IF(C107=\"\",\"\",IF(C107<-1,0,IF(C107=anal_period,-LOOKUP(C107,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C107,depr_yr,depr_cost))))","v":""},"","","","",{"$f":"IF(C107=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F56))","v":""},"","","",null,"",""]
["",{"$f":"IF(MAX($B$65:B107)<(construct+anal_period),B107+1,\"\")","v":""},"","","","",null,"",{"$f":"IF(OR(C108<0,C108=\"\"),\"\",-E108*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C108,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":""},{"$f":"IF(AND(C108>=1,C108<anal_period),WorkingCap*SUM(N108:R108)-WorkingCap*SUM(N107:R107),IF(C108<0,0,IF(B108=\"\",\"\",-SUM(J$65:J107))))","v":""},"","","","","","","","",{"$f":"IF(B108=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E57))","v":""},"",{"$f":"IF(C108=\"\",\"\",IF(C108<-1,0,IF(C108=anal_period,-LOOKUP(C108,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C108,depr_yr,depr_cost))))","v":""},"","","","",{"$f":"IF(C108=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F57))","v":""},"","","",null,"",""]
["",{"$f":"IF(MAX($B$65:B108)<(construct+anal_period),B108+1,\"\")","v":""},"","","","",null,"",{"$f":"IF(OR(C109<0,C109=\"\"),\"\",-E109*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C109,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":""},{"$f":"IF(AND(C109>=1,C109<anal_period),WorkingCap*SUM(N109:R109)-WorkingCap*SUM(N108:R108),IF(C109<0,0,IF(B109=\"\",\"\",-SUM(J$65:J108))))","v":""},"","","","","","","","",{"$f":"IF(B109=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E58))","v":""},"",{"$f":"IF(C109=\"\",\"\",IF(C109<-1,0,IF(C109=anal_period,-LOOKUP(C109,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C109,depr_yr,depr_cost))))","v":""},"","","","",{"$f":"IF(C109=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F58))","v":""},"","","",null,"",""]
["",{"$f":"IF(MAX($B$65:B109)<(construct+anal_period),B109+1,\"\")","v":""},"","","","",null,"",{"$f":"IF(OR(C110<0,C110=\"\"),\"\",-E110*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C110,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":""},{"$f":"IF(AND(C110>=1,C110<anal_period),WorkingCap*SUM(N110:R110)-WorkingCap*SUM(N109:R109),IF(C110<0,0,IF(B110=\"\",\"\",-SUM(J$65:J109))))","v":""},"","","","",{"$f":"IF(C110=\"\",\"\",IF(C110<0,0,IF(AND(C110=1,start_time<1),-(SUM(B185:E185)*output_kgyear*E110*percnt_var*start_time+SUM(B185:E185)*output_kgyear*E110*(1-start_time)),IF(C110<=start_time,-SUM(B185:E185)*output_kgyear*E110*percnt_var,-SUM(B185:E185)*output_kgyear*E110))))","v":""},"",{"$f":"IF(C110=\"\",\"\",IF(C110<0,0,IF(AND(C110=1,start_time<1),SUM(K185:N185,T185:V185)*output_kgyear*E110*percnt_revs*start_time+SUM(K185:N185,T185:V185)*output_kgyear*E110*(1-start_time),IF(C110<=start_time,SUM(K185:N185,T185:V185)*output_kgyear*E110*percnt_revs,SUM(K185:N185,T185:V185)*output_kgyear*E110))))","v":""},{"$f":"IF(C110=\"\",\"\",IF(C110<0,0,IF(AND(C110=1,start_time<1),-((SUM(F185:J185,P185:R185)*output_kgyear+inflated_othervar)*E110*percnt_var*start_time+(SUM(F185:J185,P185:R185)*output_kgyear+inflated_othervar)*E110*(1-start_time)),IF(C110<=start_time,-(SUM(F185:J185,P185:R185)*output_kgyear+inflated_othervar)*E110*percnt_var,-E110*(SUM(F185:J185,P185:R185)*output_kgyear+inflated_othervar)))))","v":""},{"$f":"IF(B110=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E59))","v":""},"",{"$f":"IF(C110=\"\",\"\",IF(C110<-1,0,IF(C110=anal_period,-LOOKUP(C110,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C110,depr_yr,depr_cost))))","v":""},"","","","",{"$f":"IF(C110=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F59))","v":""},"","","",null,"",""]
["",{"$f":"IF(MAX($B$65:B110)<(construct+anal_period),B110+1,\"\")","v":""},"","","","",null,"",{"$f":"IF(OR(C111<0,C111=\"\"),\"\",-E111*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C111,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":""},{"$f":"IF(AND(C111>=1,C111<anal_period),WorkingCap*SUM(N111:R111)-WorkingCap*SUM(N110:R110),IF(C111<0,0,IF(B111=\"\",\"\",-SUM(J$65:J110))))","v":""},"","","","",{"$f":"IF(C111=\"\",\"\",IF(C111<0,0,IF(AND(C111=1,start_time<1),-(SUM(B278:E278)*output_kgyear*E111*percnt_var*start_time+SUM(B278:E278)*output_kgyear*E111*(1-start_time)),IF(C111<=start_time,-SUM(B278:E278)*output_kgyear*E111*percnt_var,-SUM(B278:E278)*output_kgyear*E111))))","v":""},"",{"$f":"IF(C111=\"\",\"\",IF(C111<0,0,IF(AND(C111=1,start_time<1),SUM(K278:N278,T278:V278)*output_kgyear*E111*percnt_revs*start_time+SUM(K278:N278,T278:V278)*output_kgyear*E111*(1-start_time),IF(C111<=start_time,SUM(K278:N278,T278:V278)*output_kgyear*E111*percnt_revs,SUM(K278:N278,T278:V278)*output_kgyear*E111))))","v":""},{"$f":"IF(C111=\"\",\"\",IF(C111<0,0,IF(AND(C111=1,start_time<1),-((SUM(F278:J278,P278:R278)*output_kgyear+inflated_othervar)*E111*percnt_var*start_time+(SUM(F278:J278,P278:R278)*output_kgyear+inflated_othervar)*E111*(1-start_time)),IF(C111<=start_time,-(SUM(F278:J278,P278:R278)*output_kgyear+inflated_othervar)*E111*percnt_var,-E111*(SUM(F278:J278,P278:R278)*output_kgyear+inflated_othervar)))))","v":""},{"$f":"IF(B111=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E60))","v":""},"",{"$f":"IF(C111=\"\",\"\",IF(C111<-1,0,IF(C111=anal_period,-LOOKUP(C111,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C111,depr_yr,depr_cost))))","v":""},"","","","",{"$f":"IF(C111=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F60))","v":""},"","","",null,"",""]
["",{"$f":"IF(MAX($B$65:B111)<(construct+anal_period),B111+1,\"\")","v":""},"","","","",null,"",{"$f":"IF(OR(C112<0,C112=\"\"),\"\",-E112*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C112,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":""},{"$f":"IF(AND(C112>=1,C112<anal_period),WorkingCap*SUM(N112:R112)-WorkingCap*SUM(N111:R111),IF(C112<0,0,IF(B112=\"\",\"\",-SUM(J$65:J111))))","v":""},"","","","",{"$f":"IF(C112=\"\",\"\",IF(C112<0,0,IF(AND(C112=1,start_time<1),-(SUM(B279:E279)*output_kgyear*E112*percnt_var*start_time+SUM(B279:E279)*output_kgyear*E112*(1-start_time)),IF(C112<=start_time,-SUM(B279:E279)*output_kgyear*E112*percnt_var,-SUM(B279:E279)*output_kgyear*E112))))","v":""},"",{"$f":"IF(C112=\"\",\"\",IF(C112<0,0,IF(AND(C112=1,start_time<1),SUM(K279:N279,T279:V279)*output_kgyear*E112*percnt_revs*start_time+SUM(K279:N279,T279:V279)*output_kgyear*E112*(1-start_time),IF(C112<=start_time,SUM(K279:N279,T279:V279)*output_kgyear*E112*percnt_revs,SUM(K279:N279,T279:V279)*output_kgyear*E112))))","v":""},{"$f":"IF(C112=\"\",\"\",IF(C112<0,0,IF(AND(C112=1,start_time<1),-((SUM(F279:J279,P279:R279)*output_kgyear+inflated_othervar)*E112*percnt_var*start_time+(SUM(F279:J279,P279:R279)*output_kgyear+inflated_othervar)*E112*(1-start_time)),IF(C112<=start_time,-(SUM(F279:J279,P279:R279)*output_kgyear+inflated_othervar)*E112*percnt_var,-E112*(SUM(F279:J279,P279:R279)*output_kgyear+inflated_othervar)))))","v":""},{"$f":"IF(B112=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E61))","v":""},"",{"$f":"IF(C112=\"\",\"\",IF(C112<-1,0,IF(C112=anal_period,-LOOKUP(C112,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C112,depr_yr,depr_cost))))","v":""},"","","","",{"$f":"IF(C112=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F61))","v":""},"","","",null,"",""]
["",{"$f":"IF(MAX($B$65:B112)<(construct+anal_period),B112+1,\"\")","v":""},"","","","",null,"",{"$f":"IF(OR(C113<0,C113=\"\"),\"\",-E113*INDEX('Replacement Costs'!$A$16:$H$57,MATCH(C113,'Replacement Costs'!$C$16:$C$57,0),MATCH(\"Total Yearly Replacement Costs\",'Replacement Costs'!$A$16:$H$16,0)))","v":""},{"$f":"IF(AND(C113>=1,C113<anal_period),WorkingCap*SUM(N113:R113)-WorkingCap*SUM(N112:R112),IF(C113<0,0,IF(B113=\"\",\"\",-SUM(J$65:J112))))","v":""},"","","","",{"$f":"IF(C113=\"\",\"\",IF(C113<0,0,IF(AND(C113=1,start_time<1),-(SUM(B280:E280)*output_kgyear*E113*percnt_var*start_time+SUM(B280:E280)*output_kgyear*E113*(1-start_time)),IF(C113<=start_time,-SUM(B280:E280)*output_kgyear*E113*percnt_var,-SUM(B280:E280)*output_kgyear*E113))))","v":""},"",{"$f":"IF(C113=\"\",\"\",IF(C113<0,0,IF(AND(C113=1,start_time<1),SUM(K280:N280,T280:V280)*output_kgyear*E113*percnt_revs*start_time+SUM(K280:N280,T280:V280)*output_kgyear*E113*(1-start_time),IF(C113<=start_time,SUM(K280:N280,T280:V280)*output_kgyear*E113*percnt_revs,SUM(K280:N280,T280:V280)*output_kgyear*E113))))","v":""},{"$f":"IF(C113=\"\",\"\",IF(C113<0,0,IF(AND(C113=1,start_time<1),-((SUM(F280:J280,P280:R280)*output_kgyear+inflated_othervar)*E113*percnt_var*start_time+(SUM(F280:J280,P280:R280)*output_kgyear+inflated_othervar)*E113*(1-start_time)),IF(C113<=start_time,-(SUM(F280:J280,P280:R280)*output_kgyear+inflated_othervar)*E113*percnt_var,-E113*(SUM(F280:J280,P280:R280)*output_kgyear+inflated_othervar)))))","v":""},{"$f":"IF(B113=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!E62))","v":""},"",{"$f":"IF(C113=\"\",\"\",IF(C113<-1,0,IF(C113=anal_period,-LOOKUP(C113,depr_yr,depr_cost)-Depreciation!$C$141-Depreciation!$B$166,-LOOKUP(C113,depr_yr,depr_cost))))","v":""},"","","","",{"$f":"IF(C113=\"\",\"\",IF($B$31=0,\"\",-'Debt Financing Calculations'!F62))","v":""},"","","",null,"",""]
[null,null,null,null,"Cumulative Total",{"$f":"SUM(F65:F113)","v":74128915.349884406},-1267062.1105808259,-844708.07372055063,-1481700.6657798789,0,0,307702.0105626536,-307702.0105626536,-2947505.3717430066,-65151805.2851815,0,0,-210360.9215297859,-984507.25992130151,4834736.5115087908,-3593470.8500812557,1241265.6614275365,5.4053999999999984,-319501.7812514478,4515234.7302573435,-1267062.1105808259,921763.88017608842,-77672.894690314191,1241265.6614275363]
[null,null,null,null,"PV of Cash Flow",{"$f":"NPV(nominal_irr,F65:F113)","v":26560094.901041213},-1151330.3807116873,-767553.58714112476,-481840.1411845478,-327422.94660965214,0,41169.311551920473,-41169.311551920473,-1064432.9361534091,-23276655.461224169,0,0,-75371.479711126114,-403986.92696527275,1739648.0969872379,-1765663.9285902621,-26015.831603023722,2.2180749943810913,6696.4750546183022,1746344.5720418568,-169527.89710652345,8.7071894903132806E-9,-1226903.7016897448,-6696.475054609562]
[null,null,null,null,"Discounted Values ",{"$f":"+F65+NPV($X$59,F66:F113)","v":29229915.640493877},-1267062.1105808259,{"$f":"+H65+NPV($X$59,H66:H113)","v":-844708.07372055063},-530274.71217641851,-360335.50120285433,0,45307.650749119508,-45307.650749119508,-1171429.7348955497,-25616424.868186422,0,0,-82947.820851688535,-444595.69286382193,1914517.5236963958,-1943148.466692155,-28630.942995759568,2.441035892816279,7369.6047271085008,1921887.1284235036,-186568.84132367116,9.6624717116355896E-9,-1350232.0617835973,-7369.6047270986019,null,{"$f":"+AE65+NPV(real_irr,AE66:AE113)","v":4496442.7623530524},{"$f":"+AF65+NPV($X$59,AF66:AF113)","v":0}]
["Specific Item Cost Calculation",null,null,null,"Expenses $/kg H2",null,null,{"$f":"-H116/$AE$116*(1+inflation_rate)^construct/INFLATION_FACTOR","v":0.19506796071780513},{"$f":"-I116/$AE$116*(1+inflation_rate)^construct/INFLATION_FACTOR","v":0.12245604125561525},{"$f":"-J116/$AE$116*(1+inflation_rate)^construct/INFLATION_FACTOR","v":8.3212074775459749E-2},{"$f":"-K116/$AE$116*(1+inflation_rate)^construct/INFLATION_FACTOR","v":0},null,{"$f":"-M116/$AE$116*(1+inflation_rate)^construct/INFLATION_FACTOR","v":1.0462870323492518E-2},{"$f":"-N116/$AE$116*(1+inflation_rate)^construct/INFLATION_FACTOR","v":0.27051761030742788},{"$f":"-O116/$AE$116*(1+inflation_rate)^construct/INFLATION_FACTOR","v":5.9155865977564952},{"$f":"-P116/$AE$116*(1+inflation_rate)^construct/INFLATION_FACTOR","v":0},null,{"$f":"-R116/$AE$116*(1+inflation_rate)^construct/INFLATION_FACTOR","v":1.9155093650587738E-2},{"$f":"-S116/$AE$116*(1+inflation_rate)^construct/INFLATION_FACTOR","v":0.10267023347944998},null,null,null,null,{"$f":"-X116/$AE$116*(1+inflation_rate)^construct/INFLATION_FACTOR","v":-1.701858677734073E-3},null,{"$f":"-Z116/$AE$116*(1+inflation_rate)^construct/INFLATION_FACTOR","v":4.3084237670649013E-2},null,null,null,null,null,null,{"$f":"+SUM(F117:AC117)","v":6.7605108612592479}]
["Cost Component","After Tax Present Value","% of Total","$/kg of H2","Revenues $/kg H2",{"$f":"F116/$AE$116*(1+inflation_rate)^construct/INFLATION_FACTOR","v":6.7500479909357587},null,null,null,null,null,{"$f":"L116/$AE$116*(1+inflation_rate)^construct/INFLATION_FACTOR","v":1.0462870323492518E-2},null,null,null,null,{"$f":"Q116/$AE$116*(1+inflation_rate)^construct/INFLATION_FACTOR","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+SUM(F118:AC118)","v":6.7605108612592515}]
["Capital-Related Costs",{"$f":"(SUM(H115:K115)+L115*(1-total_tax_rate)+S115*(1-total_tax_rate)+U115*(-total_tax_rate)+Z115)/(1-total_tax_rate)","v":-2102465.7124005789},{"$f":"B119/SUM($B$118:$B$125)","v":7.9158817776594559E-2},{"$f":"H2_price_real*C119","v":0.53432581889775166}]
["Decommissioning Costs",{"$f":"M115","v":-41169.311551920473},1.550043842287121E-3,1.046287032349252E-2]
["Fixed O&M",{"$f":"N115","v":-1064432.9361534091},4.0076398074604828E-2,0.27051761030742794]
["Feedstock Costs",{"$f":"O115","v":-23276655.461224169},0.87637696883047222,5.915586597756497]
["Other Raw Material Costs",{"$f":"P115","v":0},0,0]
["Byproduct Credits",{"$f":"Q115","v":0},0,0]
["Other Variable Costs (including utilities)",{"$f":"R115","v":-75371.479711126114},2.8377714760413533E-3,1.9155093650587731E-2]
[]
[]
["INFLATION FACTOR (1 + inflation rate)^(startup year - reference year) = ",{"$f":"(1+inflation_rate)^(startup_year-ref_year)","v":0.9813542688910698}]
["Feedstock, Utility and Byproduct Cost Information (Start-Up Year $)"]
[null,"Energy Feedstocks",null,null,null,"Energy Utilities",null,null,null,"Carbon Sequestration Electricity Usage","Energy Byproducts",null,null,null,"Other Material Inputs",null,null,null,"Other Material Byproducts"]
["Feedstock Name",{"$f":"Input_Sheet_Template!$B$75","v":"Ethanol"},{"$f":"Input_Sheet_Template!$B$77","v":"Commercial Electricity"},null,null,null,null,null,null,{"$f":"IF(CO2_CashFlow_eUse>0,'HyARC Physical Property Data'!A77,\"\")","v":""},null,null,null,null,"Type",{"$f":"Input_Sheet_Template!$B$138","v":"Process Water"},null,null,"Type"]
["LHV (GJ or mmBtu/usage unit)",{"$f":"Input_Sheet_Template!$C$75","v":8.1000000000000003E-2},{"$f":"Input_Sheet_Template!$C$77","v":3.5999999999999995E-3},null,null,null,null,null,null,{"$f":"IF(J131=\"\",0,VLOOKUP(J131,MASTER_PROPERTY_TABLE,9,FALSE))","v":0},null,null,null,null,"Usage (/kg H2)",{"$f":"Input_Sheet_Template!$D$138","v":5.77},null,null,"Usage (/kg H2)"]
["Usage (/kg H2)",{"$f":"feedstockEthanol_Usage","v":2.1909999999999998},{"$f":"feedstockCommercial_Electricity_Usage","v":0.49},null,null,null,null,null,null,{"$f":" CO2_eUse_kWhpkg","v":0},null,null,null,null,"Cost (/usage unit)",{"$f":"Input_Sheet_Template!$C$138","v":2.374951094500801E-3},null,null,"Price (/usage unit)"]
["Price ($/ usage unit)",{"$f":"feedstockEthanol_Price","v":2.2678388613174403},{"$f":"feedstockCommercial_Electricity_Price","v":0.10775596291985907},null,null,null,null,null,null,{"$f":"IF(J131=\"\",0,CO2_eCost)","v":0},null,null,null,null,"Lookup Price?",{"$f":"Input_Sheet_Template!$F$138","v":"Yes"},null,null,"Lookup Price?"]
["Lookup Price?",{"$f":"Input_Sheet_Template!$G$75","v":"yes"},{"$f":"Input_Sheet_Template!$G$77","v":"yes"},null,null,null,null,null,null,{"$f":"IF(J131=\"\",\"\",\"yes\")","v":""}]
["CO2 Emissions (kg CO2/kg H2)",{"$f":"IF(B131=\"\",0,VLOOKUP(B131,MASTER_PROPERTY_TABLE,11,FALSE)*B132*B133)","v":12.580919189999999},{"$f":"IF(C131=\"\",0,VLOOKUP(C131,MASTER_PROPERTY_TABLE,11,FALSE)*C132*C133)","v":0},{"$f":"IF(D131=\"\",0,VLOOKUP(D131,MASTER_PROPERTY_TABLE,11,FALSE)*D132*D133)","v":0},{"$f":"IF(E131=\"\",0,VLOOKUP(E131,MASTER_PROPERTY_TABLE,11,FALSE)*E132*E133)","v":0},{"$f":"IF(F131=\"\",,VLOOKUP(F131,MASTER_PROPERTY_TABLE,11,FALSE)*F132*F133)","v":0},{"$f":"IF(G131=\"\",,VLOOKUP(G131,MASTER_PROPERTY_TABLE,11,FALSE)*G132*G133)","v":0},{"$f":"IF(H131=\"\",,VLOOKUP(H131,MASTER_PROPERTY_TABLE,11,FALSE)*H132*H133)","v":0},{"$f":"IF(I131=\"\",,VLOOKUP(I131,MASTER_PROPERTY_TABLE,11,FALSE)*I132*I133)","v":0},{"$f":"IF($J$131=\"\",0,VLOOKUP($J$131,MASTER_PROPERTY_TABLE,12,FALSE)*$J$132*$J$133)","v":0}]
["Unit System Conversion Factor",{"$f":"IF(B131=\"\",0,IF(VLOOKUP(B131,MASTER_PROPERTY_TABLE,12,FALSE)=\"English\",mmBTU_to_GJ,1))","v":1},{"$f":"IF(C131=\"\",0,IF(VLOOKUP(C131,MASTER_PROPERTY_TABLE,12,FALSE)=\"English\",mmBTU_to_GJ,1))","v":1},{"$f":"IF(D131=\"\",0,IF(VLOOKUP(D131,MASTER_PROPERTY_TABLE,12,FALSE)=\"English\",mmBTU_to_GJ,1))","v":0},{"$f":"IF(E131=\"\",,IF(VLOOKUP(E131,MASTER_PROPERTY_TABLE,12,FALSE)=\"English\",mmBTU_to_GJ,1))","v":0},{"$f":"IF(F131=\"\",,IF(VLOOKUP(F131,MASTER_PROPERTY_TABLE,12,FALSE)=\"English\",mmBTU_to_GJ,1))","v":0},{"$f":"IF(G131=\"\",,IF(VLOOKUP(G131,MASTER_PROPERTY_TABLE,12,FALSE)=\"English\",mmBTU_to_GJ,1))","v":0},{"$f":"IF(H131=\"\",,IF(VLOOKUP(H131,MASTER_PROPERTY_TABLE,12,FALSE)=\"English\",mmBTU_to_GJ,1))","v":0},{"$f":"IF(I131=\"\",,IF(VLOOKUP(I131,MASTER_PROPERTY_TABLE,12,FALSE)=\"English\",mmBTU_to_GJ,1))","v":0},{"$f":"IF($J$131=\"\",0,IF(VLOOKUP($J$131,MASTER_PROPERTY_TABLE,12,FALSE)=\"English\",mmBTU_to_GJ,1))","v":0},{"$f":"IF(K131=\"\",,IF(VLOOKUP(K131,MASTER_PROPERTY_TABLE,12,FALSE)=\"English\",mmBTU_to_GJ,1))","v":0},{"$f":"IF(L131=\"\",,IF(VLOOKUP(L131,MASTER_PROPERTY_TABLE,12,FALSE)=\"English\",mmBTU_to_GJ,1))","v":0},{"$f":"IF(M131=\"\",,IF(VLOOKUP(M131,MASTER_PROPERTY_TABLE,12,FALSE)=\"English\",mmBTU_to_GJ,1))","v":0},{"$f":"IF(N131=\"\",,IF(VLOOKUP(N131,MASTER_PROPERTY_TABLE,12,FALSE)=\"English\",mmBTU_to_GJ,1))","v":0}]
["Actual Year",{"$f":"IF(B$131=\"\",\"\",B$131&\" ($/kg of H2)\")","v":"Ethanol ($/kg of H2)"},"Commercial Electricity ($/kg of H2)","","","","","","",null,"","","","",null,{"$f":"IF(P$131=\"\",\"\",P$131&\" ($/kg of H2)\")","v":"Process Water ($/kg of H2)"},{"$f":"IF(Q$131=\"\",\"\",Q$131&\" ($/kg of H2)\")","v":""},{"$f":"IF(R$131=\"\",\"\",R$131&\" ($/kg of H2)\")","v":""},null,{"$f":"IF(T$131=\"\",\"\",T$131&\" ($/kg of H2)\")","v":""},{"$f":"IF(U$131=\"\",\"\",U$131&\" ($/kg of H2)\")","v":""},{"$f":"IF(V$131=\"\",\"\",V$131&\" ($/kg of H2)\")","v":""}]
[{"$f":"IF(A65=\"\",\"\",A65)","v":2014},{"$f":"IF($A139=\"\",\"\",IF($B$131=\"\",\"\",IF($B$135=\"no\",INFLATION_FACTOR*$B$133*$B$134,INFLATION_FACTOR*$B$133*$B$132*INDEX(FEEDPRICETABLE,MATCH($B$131,List_Energy_Feedstocks,0),MATCH($A139,Feedstock_Year,0)))))","v":0},{"$f":"IF($A139=\"\",\"\",IF($C$131=\"\",\"\",IF($C$135=\"no\",INFLATION_FACTOR*$C$133*$C$134,INFLATION_FACTOR*$C$133*$C$132*INDEX(FEEDPRICETABLE,MATCH($C$131,List_Energy_Feedstocks,0),MATCH($A139,Feedstock_Year,0)))))","v":5.2871468005088615E-2},{"$f":"IF($A139=\"\",\"\",IF($D$131=\"\",\"\",IF($D$135=\"no\",INFLATION_FACTOR*$D$133*$D$134,INFLATION_FACTOR*$D$133*$D$132*INDEX(FEEDPRICETABLE,MATCH($D$131,List_Energy_Feedstocks,0),MATCH($A139,Feedstock_Year,0)))))","v":""},{"$f":"IF($A139=\"\",\"\",IF($E$131=\"\",\"\",IF($E$135=\"no\",INFLATION_FACTOR*$E$133*$E$134,INFLATION_FACTOR*$E$133*$E$132*INDEX(FEEDPRICETABLE,MATCH($E$131,List_Energy_Feedstocks,0),MATCH($A139,Feedstock_Year,0)))))","v":""},{"$f":"IF($A139=\"\",\"\",IF($F$131=\"\",\"\",IF($F$135=\"no\",INFLATION_FACTOR*$F$133*$F$134,INFLATION_FACTOR*$F$133*$F$132*INDEX(FEEDPRICETABLE,MATCH($F$131,List_Energy_Feedstocks,0),MATCH($A139,Feedstock_Year,0)))))","v":""},{"$f":"IF($A139=\"\",\"\",IF($G$131=\"\",\"\",IF($G$135=\"no\",INFLATION_FACTOR*$G$133*$G$134,INFLATION_FACTOR*$G$133*$G$132*INDEX(FEEDPRICETABLE,MATCH($G$131,List_Energy_Feedstocks,0),MATCH($A139,Feedstock_Year,0)))))","v":""},{"$f":"IF($A139=\"\",\"\",IF($H$131=\"\",\"\",IF($H$135=\"no\",INFLATION_FACTOR*$H$133*$H$134,INFLATION_FACTOR*$H$133*$H$132*INDEX(FEEDPRICETABLE,MATCH(H$131,List_Energy_Feedstocks,0),MATCH($A139,Feedstock_Year,0)))))","v":""},{"$f":"IF($A139=\"\",\"\",IF($I$131=\"\",\"\",IF($I$135=\"no\",INFLATION_FACTOR*$I$133*$I$134,INFLATION_FACTOR*$I$133*$I$132*INDEX(FEEDPRICETABLE,MATCH($I$131,List_Energy_Feedstocks,0),MATCH($A139,Feedstock_Year,0)))))","v":""},{"$f":"IF($A139=\"\",\"\",IF($J$131=\"\",\"\",IF($J$135=\"no\",INFLATION_FACTOR*$J$133*$J$134,INFLATION_FACTOR*$J$133*$J$132*INDEX(FEEDPRICETABLE,MATCH($J$131,List_Energy_Feedstocks,0),MATCH($A139,Feedstock_Year,0)))))","v":""},{"$f":"IF($A139=\"\",\"\",IF($K$131=\"\",\"\",IF($K$135=\"no\",INFLATION_FACTOR*$K$133*$K$134,INFLATION_FACTOR*$K$133*$K$132*INDEX(FEEDPRICETABLE,MATCH($K$131,List_Energy_Feedstocks,0),MATCH($A139,Feedstock_Year,0)))))","v":""},{"$f":"IF($A139=\"\",\"\",IF($L$131=\"\",\"\",IF($L$135=\"no\",INFLATION_FACTOR*$L$133*$L$134,INFLATION_FACTOR*$L$133*$L$132*INDEX(FEEDPRICETABLE,MATCH($L$131,List_Energy_Feedstocks,0),MATCH($A139,Feedstock_Year,0)))))","v":""},{"$f":"IF($A139=\"\",\"\",IF(M$131=\"\",\"\",IF($M$135=\"no\",INFLATION_FACTOR*$M$133*$M$134,INFLATION_FACTOR*$M$133*$M$132*INDEX(FEEDPRICETABLE,MATCH($M$131,List_Energy_Feedstocks,0),MATCH($A139,Feedstock_Year,0)))))","v":""},{"$f":"IF($A139=\"\",\"\",IF($N$131=\"\",\"\",IF($N$135=\"no\",INFLATION_FACTOR*$N$133*$N$134,INFLATION_FACTOR*$N$133*$N$132*INDEX(FEEDPRICETABLE,MATCH($N$131,List_Energy_Feedstocks,0),MATCH($A139,Feedstock_Year,0)))))","v":""},null,{"$f":"IF(OR($A139=\"\",$P$131=\"\"),\"\",IF($P$134=\"No\",INFLATION_FACTOR*$P$132*$P$133,INFLATION_FACTOR*$P$132*INDEX(Tbl_Other_Inputs_and_Byproducts,MATCH($P$131,Other_Inputs_List,0),MATCH($A139,Other_Inputs_years,0))))","v":1.3447956639126223E-2},{"$f":"IF(OR($A139=\"\",$Q$131=\"\"),\"\",IF($Q$134=\"No\",INFLATION_FACTOR*$Q$132*$Q$133,INFLATION_FACTOR*$Q$132*INDEX(Tbl_Other_Inputs_and_Byproducts,MATCH($Q$131,Other_Inputs_List,0),MATCH($A139,Other_Inputs_years,0))))","v":""},{"$f":"IF(OR($A139=\"\",$R$131=\"\"),\"\",IF($R$134=\"No\",INFLATION_FACTOR*$R$132*$R$133,INFLATION_FACTOR*$R$132*INDEX(Tbl_Other_Inputs_and_Byproducts,MATCH($R$131,Other_Inputs_List,0),MATCH($A139,Other_Inputs_years,0))))","v":""},null,{"$f":"IF(OR($A139=\"\",$T$131=\"\"),\"\",IF($T$134=\"No\",INFLATION_FACTOR*$T$132*$T$133,INFLATION_FACTOR*$T$132*INDEX(Tbl_Other_Inputs_and_Byproducts,MATCH($T$131,Other_Inputs_List,0),MATCH($A139,Other_Inputs_years,0))))","v":""},{"$f":"IF(OR($A139=\"\",$U$131=\"\"),\"\",IF($U$134=\"No\",INFLATION_FACTOR*$U$132*$U$133,INFLATION_FACTOR*$U$132*INDEX(Tbl_Other_Inputs_and_Byproducts,MATCH($U$131,Other_Inputs_List,0),MATCH($A139,Other_Inputs_years,0))))","v":""},{"$f":"IF(OR($A139=\"\",$V$131=\"\"),\"\",IF($V$134=\"No\",INFLATION_FACTOR*$V$132*$V$133,INFLATION_FACTOR*$V$132*INDEX(Tbl_Other_Inputs_and_Byproducts,MATCH($V$131,Other_Inputs_List,0),MATCH($A139,Other_Inputs_years,0))))","v":""}]
[2015,{"$f":"IF($A140=\"\",\"\",IF($B$131=\"\",\"\",IF($B$135=\"no\",INFLATION_FACTOR*$B$133*$B$134,INFLATION_FACTOR*$B$133*$B$132*INDEX(FEEDPRICETABLE,MATCH($B$131,List_Energy_Feedstocks,0),MATCH($A140,Feedstock_Year,0)))))","v":4.8761873848346529},5.1815919362837047E-2,"","",{"$f":"IF($A140=\"\",\"\",IF($F$131=\"\",\"\",IF($F$135=\"no\",INFLATION_FACTOR*$F$133*$F$134,INFLATION_FACTOR*$F$133*$F$132*INDEX(FEEDPRICETABLE,MATCH($F$131,List_Energy_Feedstocks,0),MATCH($A140,Feedstock_Year,0)))))","v":""},"","","","","","","","",null,{"$f":"IF(OR($A140=\"\",$P$131=\"\"),\"\",IF($P$134=\"No\",INFLATION_FACTOR*$P$132*$P$133,INFLATION_FACTOR*$P$132*INDEX(Tbl_Other_Inputs_and_Byproducts,MATCH($P$131,Other_Inputs_List,0),MATCH($A140,Other_Inputs_years,0))))","v":1.3447956639126223E-2},{"$f":"IF(OR($A140=\"\",$Q$131=\"\"),\"\",IF($Q$134=\"No\",INFLATION_FACTOR*$Q$132*$Q$133,INFLATION_FACTOR*$Q$132*INDEX(Tbl_Other_Inputs_and_Byproducts,MATCH($Q$131,Other_Inputs_List,0),MATCH($A140,Other_Inputs_years,0))))","v":""},"",null,"","",""]
[2016,4.8014342367457328,5.0154058577075562E-2,"","","","","","","","","","","",null,1.3447956639126223E-2,"","",null,"","",""]
[2017,4.8014342367457328,5.0424142636563668E-2,"","","","","","","","","","","",null,1.3447956639126223E-2,"","",null,"","",""]
[2018,6.2934325876329709,5.019469509640901E-2,"","","","","","","","","","","",null,1.3447956639126223E-2,"","",null,"","",""]
[2019,6.2763187796006932,5.08855169270701E-2,"","","","","","","","","","","",null,1.3447956639126223E-2,"","",null,"","",""]
[2020,6.3285231392977872,5.1735859772286695E-2,"","","","","","","","","","","",null,1.3447956639126223E-2,"","",null,"","",""]
[2021,6.3834763489897011,5.2087459688850521E-2,"","","","","","","","","","","",null,1.3447956639126223E-2,"","",null,"","",""]
[2022,6.3581938498241115,5.3805790267741502E-2,"","","","","","","","","","","",null,1.3447956639126223E-2,"","",null,"","",""]
[2023,6.2376077913573305,5.4357244716442099E-2,"","","","","","","","","","","",null,1.3447956639126223E-2,"","",null,"","",""]
[2024,6.1557262328963178,5.4249450757263167E-2,"","","","","","","","","","","",null,1.3447956639126223E-2,"","",null,"","",""]
[2025,6.1120106507206051,5.5143720416111111E-2,"","","","","","","","","","","",null,1.3447956639126223E-2,"","",null,"","",""]
[2026,5.9130315428735702,5.5724334708374262E-2,"","","","","","","","","","","",null,1.3447956639126223E-2,"","",null,"","",""]
[2027,5.8741886271324235,5.5870954313412977E-2,"","","","","","","","","","","",null,1.3447956639126223E-2,"","",null,"","",""]
[2028,5.7876787925196238,5.5996266821416882E-2,"","","","","","","","","","","",null,1.3447956639126223E-2,"","",null,"","",""]
[2029,5.748091892200808,5.6084944117454516E-2,"","","","","","","","","","","",null,1.3447956639126223E-2,"","",null,"","",""]
[2030,5.6512960382525455,5.6214870483217674E-2,"","","","","","","","","","","",null,1.3447956639126223E-2,"","",null,"","",""]
[2031,5.3668408883163359,5.613031645337814E-2,"","","","","","","","","","","",null,1.3447956639126223E-2,"","",null,"","",""]
[2032,5.4062223277779466,5.5978966495594036E-2,"","","","","","","","","","","",null,1.3447956639126223E-2,"","",null,"","",""]
[2033,5.4114799629765393,5.5765232652367047E-2,"","","","","","","","","","","",null,1.3447956639126223E-2,"","",null,"","",""]
[2034,5.4181844751590322,5.5608668313374202E-2,"","","","","","","","","","","",null,1.3447956639126223E-2,"","",null,"","",""]
["","","","","","","","","","","","","","",null,"","","",null,"","",""]
["","","","","","","","","","","","","","",null,"","","",null,"","",""]
["","","","","","","","","","","","","","",null,"","","",null,"","",""]
["","","","","","","","","","","","","","",null,"","","",null,"","",""]
["","","","","","","","","","","","","","",null,"","","",null,"","",""]
["","","","","","","","","","","","","","",null,"","","",null,"","",""]
["","","","","","","","","","","","","","",null,"","","",null,"","",""]
["","","","","","","","","","","","","","",null,"","","",null,"","",""]
["","","","","","","","","","","","","","",null,"","","",null,"","",""]
["","","","","","","","","","","","","","",null,"","","",null,"","",""]
["","","","","","","","","","","","","","",null,"","","",null,"","",""]
["","","","","","","","","","","","","","",null,"","","",null,"","",""]
["","","","","","","","","","","","","","",null,"","","",null,"","",""]
["","","","","","","","","","","","","","",null,"","","",null,"","",""]
["","","","","","","","","","","","","","",null,"","","",null,"","",""]
["","","","","","","","","","","","","","",null,"","","",null,"","",""]
["","","","","","","","","","","","","","",null,"","","",null,"","",""]
["","","","","","","","","","","","","","",null,"","","",null,"","",""]
["","","","","","","","","","","","","","",null,"","","",null,"","",""]
["","","","","","","","","","","","","","",null,"","","",null,"","",""]
["","","","","","","","","","","","","","",null,"","","",null,"","",""]
["","","","","","","","","","","","","","",null,"","","",null,"","",""]
["","","","","","","","","","","","","","",null,"","","",null,"","",""]
[]
["Tables to calculate equivalent price in startup year"]
["Actual Year",{"$f":"IF(B$131=\"\",\"\",B$131&\" ($/year)\")","v":"Ethanol ($/year)"},{"$f":"IF(C$131=\"\",\"\",C$131&\" ($/year)\")","v":"Commercial Electricity ($/year)"},"","","","","","","","","","",""]
[{"$f":"+A139","v":2014},{"$f":"IF($C65=\"\",\"\",IF($C65<0,0,IF(AND($C65=1,start_time<1),-(SUM(B139)*output_kgyear*$E65*percnt_var*start_time+SUM(B139)*output_kgyear*$E65*(1-start_time)),IF($C65<=start_time,-SUM(B139)*output_kgyear*$E65*percnt_var,-SUM(B139)*output_kgyear*$E65))))","v":0},{"$f":"IF($C65=\"\",\"\",IF($C65<0,0,IF(AND($C65=1,start_time<1),-(SUM(C139)*output_kgyear*$E65*percnt_var*start_time+SUM(C139)*output_kgyear*$E65*(1-start_time)),IF($C65<=start_time,-SUM(C139)*output_kgyear*$E65*percnt_var,-SUM(C139)*output_kgyear*$E65))))","v":0},0,0,0,0,0,0,0,0,0,0,0]
[{"$f":"+A140","v":2015},{"$f":"IF($C66=\"\",\"\",IF($C66<0,0,IF(AND($C66=1,start_time<1),-(SUM(B140)*output_kgyear*$E66*percnt_var*start_time+SUM(B140)*output_kgyear*$E66*(1-start_time)),IF($C66<=start_time,-SUM(B140)*output_kgyear*$E66*percnt_var,-SUM(B140)*output_kgyear*$E66))))","v":-1630126.5094060716},-17322.243198714194,0,0,0,0,0,0,0,0,0,0,0]
[2016,{"$f":"IF($C67=\"\",\"\",IF($C67<0,0,IF(AND($C67=1,start_time<1),-(SUM(B141)*output_kgyear*$E67*percnt_var*start_time+SUM(B141)*output_kgyear*$E67*(1-start_time)),IF($C67<=start_time,-SUM(B141)*output_kgyear*$E67*percnt_var,-SUM(B141)*output_kgyear*$E67))))","v":-2303709.6612687907},-24063.724212155332,0,0,0,0,0,0,0,0,0,0,0]
[2017,{"$f":"IF($C68=\"\",\"\",IF($C68<0,0,IF(AND($C68=1,start_time<1),-(SUM(B142)*output_kgyear*$E68*percnt_var*start_time+SUM(B142)*output_kgyear*$E68*(1-start_time)),IF($C68<=start_time,-SUM(B142)*output_kgyear*$E68*percnt_var,-SUM(B142)*output_kgyear*$E68))))","v":-2347480.1448328979},-24652.982384651503,0,0,{"$f":"IF($C68=\"\",\"\",IF($C68<0,0,IF(AND($C68=1,start_time<1),-(SUM(F142)*output_kgyear*$E68*percnt_var*start_time+SUM(F142)*output_kgyear*$E68*(1-start_time)),IF($C68<=start_time,-SUM(F142)*output_kgyear*$E68*percnt_var,-SUM(F142)*output_kgyear*$E68))))","v":0},0,0,0,0,0,0,0,0]
[2018,{"$f":"IF($C69=\"\",\"\",IF($C69<0,0,IF(AND($C69=1,start_time<1),-(SUM(B143)*output_kgyear*$E69*percnt_var*start_time+SUM(B143)*output_kgyear*$E69*(1-start_time)),IF($C69<=start_time,-SUM(B143)*output_kgyear*$E69*percnt_var,-SUM(B143)*output_kgyear*$E69))))","v":-3135398.248278433},-25007.077916019018,0,0,0,0,0,0,0,0,0,0,0]
[2019,{"$f":"IF($C70=\"\",\"\",IF($C70<0,0,IF(AND($C70=1,start_time<1),-(SUM(B144)*output_kgyear*$E70*percnt_var*start_time+SUM(B144)*output_kgyear*$E70*(1-start_time)),IF($C70<=start_time,-SUM(B144)*output_kgyear*$E70*percnt_var,-SUM(B144)*output_kgyear*$E70))))","v":-3186282.6918713078},-25832.920147176334,0,0,0,0,0,0,0,0,0,0,0]
[2020,{"$f":"IF($C71=\"\",\"\",IF($C71<0,0,IF(AND($C71=1,start_time<1),-(SUM(B145)*output_kgyear*$E71*percnt_var*start_time+SUM(B145)*output_kgyear*$E71*(1-start_time)),IF($C71<=start_time,-SUM(B145)*output_kgyear*$E71*percnt_var,-SUM(B145)*output_kgyear*$E71))))","v":-3273828.0633177222},-26763.639142066309,0,0,0,0,0,0,0,0,0,0,0]
[2021,{"$f":"IF($C72=\"\",\"\",IF($C72<0,0,IF(AND($C72=1,start_time<1),-(SUM(B146)*output_kgyear*$E72*percnt_var*start_time+SUM(B146)*output_kgyear*$E72*(1-start_time)),IF($C72<=start_time,-SUM(B146)*output_kgyear*$E72*percnt_var,-SUM(B146)*output_kgyear*$E72))))","v":-3364998.9453075598},-27457.491394085344,0,0,0,0,0,0,0,0,0,0,0]
[2022,{"$f":"IF($C73=\"\",\"\",IF($C73<0,0,IF(AND($C73=1,start_time<1),-(SUM(B147)*output_kgyear*$E73*percnt_var*start_time+SUM(B147)*output_kgyear*$E73*(1-start_time)),IF($C73<=start_time,-SUM(B147)*output_kgyear*$E73*percnt_var,-SUM(B147)*output_kgyear*$E73))))","v":-3415353.2343775881},-28902.198353744225,0,0,0,0,0,0,0,0,0,0,0]
[2023,{"$f":"IF($C74=\"\",\"\",IF($C74<0,0,IF(AND($C74=1,start_time<1),-(SUM(B148)*output_kgyear*$E74*percnt_var*start_time+SUM(B148)*output_kgyear*$E74*(1-start_time)),IF($C74<=start_time,-SUM(B148)*output_kgyear*$E74*percnt_var,-SUM(B148)*output_kgyear*$E74))))","v":-3414240.5064523877},-29753.186307604752,0,0,0,0,0,0,0,0,0,0,0]
[2024,{"$f":"IF($C75=\"\",\"\",IF($C75<0,0,IF(AND($C75=1,start_time<1),-(SUM(B149)*output_kgyear*$E75*percnt_var*start_time+SUM(B149)*output_kgyear*$E75*(1-start_time)),IF($C75<=start_time,-SUM(B149)*output_kgyear*$E75*percnt_var,-SUM(B149)*output_kgyear*$E75))))","v":-3433440.5167040159},-30258.373292096334,0,0,0,0,0,0,0,0,0,0,0]
[2025,{"$f":"IF($C76=\"\",\"\",IF($C76<0,0,IF(AND($C76=1,start_time<1),-(SUM(B150)*output_kgyear*$E76*percnt_var*start_time+SUM(B150)*output_kgyear*$E76*(1-start_time)),IF($C76<=start_time,-SUM(B150)*output_kgyear*$E76*percnt_var,-SUM(B150)*output_kgyear*$E76))))","v":-3473829.6462181667},-31341.550552054072,0,0,0,0,0,0,0,0,0,0,0]
[2026,{"$f":"IF($C77=\"\",\"\",IF($C77<0,0,IF(AND($C77=1,start_time<1),-(SUM(B151)*output_kgyear*$E77*percnt_var*start_time+SUM(B151)*output_kgyear*$E77*(1-start_time)),IF($C77<=start_time,-SUM(B151)*output_kgyear*$E77*percnt_var,-SUM(B151)*output_kgyear*$E77))))","v":-3424591.6589445188},-32273.308616546197,0,0,0,0,0,0,0,0,0,0,0]
[2027,{"$f":"IF($C78=\"\",\"\",IF($C78<0,0,IF(AND($C78=1,start_time<1),-(SUM(B152)*output_kgyear*$E78*percnt_var*start_time+SUM(B152)*output_kgyear*$E78*(1-start_time)),IF($C78<=start_time,-SUM(B152)*output_kgyear*$E78*percnt_var,-SUM(B152)*output_kgyear*$E78))))","v":-3466735.2063063555},-32973.031106560731,0,0,0,0,0,0,0,0,0,0,0]
[2028,{"$f":"IF($C79=\"\",\"\",IF($C79<0,0,IF(AND($C79=1,start_time<1),-(SUM(B153)*output_kgyear*$E79*percnt_var*start_time+SUM(B153)*output_kgyear*$E79*(1-start_time)),IF($C79<=start_time,-SUM(B153)*output_kgyear*$E79*percnt_var,-SUM(B153)*output_kgyear*$E79))))","v":-3480578.1321368371},-33674.87878418959,0,0,0,0,0,0,0,0,0,0,0]
[2029,{"$f":"IF($C80=\"\",\"\",IF($C80<0,0,IF(AND($C80=1,start_time<1),-(SUM(B154)*output_kgyear*$E80*percnt_var*start_time+SUM(B154)*output_kgyear*$E80*(1-start_time)),IF($C80<=start_time,-SUM(B154)*output_kgyear*$E80*percnt_var,-SUM(B154)*output_kgyear*$E80))))","v":-3522450.1303951214},-34369.043227680741,0,0,0,0,0,0,0,0,0,0,0]
[2030,{"$f":"IF($C81=\"\",\"\",IF($C81<0,0,IF(AND($C81=1,start_time<1),-(SUM(B155)*output_kgyear*$E81*percnt_var*start_time+SUM(B155)*output_kgyear*$E81*(1-start_time)),IF($C81<=start_time,-SUM(B155)*output_kgyear*$E81*percnt_var,-SUM(B155)*output_kgyear*$E81))))","v":-3528932.8368666084},-35103.187131879844,0,0,0,0,0,0,0,0,0,0,0]
[2031,{"$f":"IF($C82=\"\",\"\",IF($C82<0,0,IF(AND($C82=1,start_time<1),-(SUM(B156)*output_kgyear*$E82*percnt_var*start_time+SUM(B156)*output_kgyear*$E82*(1-start_time)),IF($C82<=start_time,-SUM(B156)*output_kgyear*$E82*percnt_var,-SUM(B156)*output_kgyear*$E82))))","v":-3414980.5832441822},-35716.345017221502,0,0,0,0,0,0,0,0,0,0,0]
[2032,{"$f":"IF($C83=\"\",\"\",IF($C83<0,0,IF(AND($C83=1,start_time<1),-(SUM(B157)*output_kgyear*$E83*percnt_var*start_time+SUM(B157)*output_kgyear*$E83*(1-start_time)),IF($C83<=start_time,-SUM(B157)*output_kgyear*$E83*percnt_var,-SUM(B157)*output_kgyear*$E83))))","v":-3505400.1806354946},-36296.820102494217,0,0,0,0,0,0,0,0,0,0,0]
[2033,{"$f":"IF($C84=\"\",\"\",IF($C84<0,0,IF(AND($C84=1,start_time<1),-(SUM(B158)*output_kgyear*$E84*percnt_var*start_time+SUM(B158)*output_kgyear*$E84*(1-start_time)),IF($C84<=start_time,-SUM(B158)*output_kgyear*$E84*percnt_var,-SUM(B158)*output_kgyear*$E84))))","v":-3575476.6122655864},-36845.241318498069,0,0,0,0,0,0,0,0,0,0,0]
[2034,{"$f":"IF($C85=\"\",\"\",IF($C85<0,0,IF(AND($C85=1,start_time<1),-(SUM(B159)*output_kgyear*$E85*percnt_var*start_time+SUM(B159)*output_kgyear*$E85*(1-start_time)),IF($C85<=start_time,-SUM(B159)*output_kgyear*$E85*percnt_var,-SUM(B159)*output_kgyear*$E85))))","v":-3647924.6439968301},-37439.890149596511,0,0,0,0,0,0,0,0,0,0,0]
["",{"$f":"IF($C86=\"\",\"\",IF($C86<0,0,IF(AND($C86=1,start_time<1),-(SUM(B160)*output_kgyear*$E86*percnt_var*start_time+SUM(B160)*output_kgyear*$E86*(1-start_time)),IF($C86<=start_time,-SUM(B160)*output_kgyear*$E86*percnt_var,-SUM(B160)*output_kgyear*$E86))))","v":""},"","","","","","","","","","","",""]
["",{"$f":"IF($C87=\"\",\"\",IF($C87<0,0,IF(AND($C87=1,start_time<1),-(SUM(B161)*output_kgyear*$E87*percnt_var*start_time+SUM(B161)*output_kgyear*$E87*(1-start_time)),IF($C87<=start_time,-SUM(B161)*output_kgyear*$E87*percnt_var,-SUM(B161)*output_kgyear*$E87))))","v":""},"","","","","","","","","","","",""]
["",{"$f":"IF($C88=\"\",\"\",IF($C88<0,0,IF(AND($C88=1,start_time<1),-(SUM(B162)*output_kgyear*$E88*percnt_var*start_time+SUM(B162)*output_kgyear*$E88*(1-start_time)),IF($C88<=start_time,-SUM(B162)*output_kgyear*$E88*percnt_var,-SUM(B162)*output_kgyear*$E88))))","v":""},"","","","","","","","","","","",""]
["",{"$f":"IF($C89=\"\",\"\",IF($C89<0,0,IF(AND($C89=1,start_time<1),-(SUM(B163)*output_kgyear*$E89*percnt_var*start_time+SUM(B163)*output_kgyear*$E89*(1-start_time)),IF($C89<=start_time,-SUM(B163)*output_kgyear*$E89*percnt_var,-SUM(B163)*output_kgyear*$E89))))","v":""},"","","","","","","","","","","",""]
["",{"$f":"IF($C90=\"\",\"\",IF($C90<0,0,IF(AND($C90=1,start_time<1),-(SUM(B164)*output_kgyear*$E90*percnt_var*start_time+SUM(B164)*output_kgyear*$E90*(1-start_time)),IF($C90<=start_time,-SUM(B164)*output_kgyear*$E90*percnt_var,-SUM(B164)*output_kgyear*$E90))))","v":""},"","","","","","","","","","","",""]
["",{"$f":"IF($C91=\"\",\"\",IF($C91<0,0,IF(AND($C91=1,start_time<1),-(SUM(B165)*output_kgyear*$E91*percnt_var*start_time+SUM(B165)*output_kgyear*$E91*(1-start_time)),IF($C91<=start_time,-SUM(B165)*output_kgyear*$E91*percnt_var,-SUM(B165)*output_kgyear*$E91))))","v":""},"","","","","","","","","","","",""]
["",{"$f":"IF($C92=\"\",\"\",IF($C92<0,0,IF(AND($C92=1,start_time<1),-(SUM(B166)*output_kgyear*$E92*percnt_var*start_time+SUM(B166)*output_kgyear*$E92*(1-start_time)),IF($C92<=start_time,-SUM(B166)*output_kgyear*$E92*percnt_var,-SUM(B166)*output_kgyear*$E92))))","v":""},"","","","","","","","","","","",""]
["",{"$f":"IF($C93=\"\",\"\",IF($C93<0,0,IF(AND($C93=1,start_time<1),-(SUM(B167)*output_kgyear*$E93*percnt_var*start_time+SUM(B167)*output_kgyear*$E93*(1-start_time)),IF($C93<=start_time,-SUM(B167)*output_kgyear*$E93*percnt_var,-SUM(B167)*output_kgyear*$E93))))","v":""},"","","","","","","","","","","",""]
["",{"$f":"IF($C94=\"\",\"\",IF($C94<0,0,IF(AND($C94=1,start_time<1),-(SUM(B168)*output_kgyear*$E94*percnt_var*start_time+SUM(B168)*output_kgyear*$E94*(1-start_time)),IF($C94<=start_time,-SUM(B168)*output_kgyear*$E94*percnt_var,-SUM(B168)*output_kgyear*$E94))))","v":""},"","","","","","","","","","","",""]
["",{"$f":"IF($C95=\"\",\"\",IF($C95<0,0,IF(AND($C95=1,start_time<1),-(SUM(B169)*output_kgyear*$E95*percnt_var*start_time+SUM(B169)*output_kgyear*$E95*(1-start_time)),IF($C95<=start_time,-SUM(B169)*output_kgyear*$E95*percnt_var,-SUM(B169)*output_kgyear*$E95))))","v":""},"","","","","","","","","","","",""]
["",{"$f":"IF($C96=\"\",\"\",IF($C96<0,0,IF(AND($C96=1,start_time<1),-(SUM(B170)*output_kgyear*$E96*percnt_var*start_time+SUM(B170)*output_kgyear*$E96*(1-start_time)),IF($C96<=start_time,-SUM(B170)*output_kgyear*$E96*percnt_var,-SUM(B170)*output_kgyear*$E96))))","v":""},"","","","","","","","","","","",""]
["",{"$f":"IF($C97=\"\",\"\",IF($C97<0,0,IF(AND($C97=1,start_time<1),-(SUM(B171)*output_kgyear*$E97*percnt_var*start_time+SUM(B171)*output_kgyear*$E97*(1-start_time)),IF($C97<=start_time,-SUM(B171)*output_kgyear*$E97*percnt_var,-SUM(B171)*output_kgyear*$E97))))","v":""},"","","","","","","","","","","",""]
["",{"$f":"IF($C98=\"\",\"\",IF($C98<0,0,IF(AND($C98=1,start_time<1),-(SUM(B172)*output_kgyear*$E98*percnt_var*start_time+SUM(B172)*output_kgyear*$E98*(1-start_time)),IF($C98<=start_time,-SUM(B172)*output_kgyear*$E98*percnt_var,-SUM(B172)*output_kgyear*$E98))))","v":""},"","","","","","","","","","","",""]
["",{"$f":"IF($C99=\"\",\"\",IF($C99<0,0,IF(AND($C99=1,start_time<1),-(SUM(B173)*output_kgyear*$E99*percnt_var*start_time+SUM(B173)*output_kgyear*$E99*(1-start_time)),IF($C99<=start_time,-SUM(B173)*output_kgyear*$E99*percnt_var,-SUM(B173)*output_kgyear*$E99))))","v":""},"","","","","","","","","","","",""]
["",{"$f":"IF($C100=\"\",\"\",IF($C100<0,0,IF(AND($C100=1,start_time<1),-(SUM(B174)*output_kgyear*$E100*percnt_var*start_time+SUM(B174)*output_kgyear*$E100*(1-start_time)),IF($C100<=start_time,-SUM(B174)*output_kgyear*$E100*percnt_var,-SUM(B174)*output_kgyear*$E100))))","v":""},"","","","","","","","","","","",""]
["",{"$f":"IF($C101=\"\",\"\",IF($C101<0,0,IF(AND($C101=1,start_time<1),-(SUM(B175)*output_kgyear*$E101*percnt_var*start_time+SUM(B175)*output_kgyear*$E101*(1-start_time)),IF($C101<=start_time,-SUM(B175)*output_kgyear*$E101*percnt_var,-SUM(B175)*output_kgyear*$E101))))","v":""},"","","","","","","","","","","",""]
["",{"$f":"IF($C102=\"\",\"\",IF($C102<0,0,IF(AND($C102=1,start_time<1),-(SUM(B176)*output_kgyear*$E102*percnt_var*start_time+SUM(B176)*output_kgyear*$E102*(1-start_time)),IF($C102<=start_time,-SUM(B176)*output_kgyear*$E102*percnt_var,-SUM(B176)*output_kgyear*$E102))))","v":""},"","","","","","","","","","","",""]
["",{"$f":"IF($C103=\"\",\"\",IF($C103<0,0,IF(AND($C103=1,start_time<1),-(SUM(B177)*output_kgyear*$E103*percnt_var*start_time+SUM(B177)*output_kgyear*$E103*(1-start_time)),IF($C103<=start_time,-SUM(B177)*output_kgyear*$E103*percnt_var,-SUM(B177)*output_kgyear*$E103))))","v":""},"","","","","","","","","","","",""]
["",{"$f":"IF($C104=\"\",\"\",IF($C104<0,0,IF(AND($C104=1,start_time<1),-(SUM(B178)*output_kgyear*$E104*percnt_var*start_time+SUM(B178)*output_kgyear*$E104*(1-start_time)),IF($C104<=start_time,-SUM(B178)*output_kgyear*$E104*percnt_var,-SUM(B178)*output_kgyear*$E104))))","v":""},"","","","","","","","","","","",""]
["",{"$f":"IF($C105=\"\",\"\",IF($C105<0,0,IF(AND($C105=1,start_time<1),-(SUM(B179)*output_kgyear*$E105*percnt_var*start_time+SUM(B179)*output_kgyear*$E105*(1-start_time)),IF($C105<=start_time,-SUM(B179)*output_kgyear*$E105*percnt_var,-SUM(B179)*output_kgyear*$E105))))","v":""},"","","","","","","","","","","",""]
["",{"$f":"IF($C106=\"\",\"\",IF($C106<0,0,IF(AND($C106=1,start_time<1),-(SUM(B180)*output_kgyear*$E106*percnt_var*start_time+SUM(B180)*output_kgyear*$E106*(1-start_time)),IF($C106<=start_time,-SUM(B180)*output_kgyear*$E106*percnt_var,-SUM(B180)*output_kgyear*$E106))))","v":""},"","","","","","","","","","","",""]
["",{"$f":"IF($C107=\"\",\"\",IF($C107<0,0,IF(AND($C107=1,start_time<1),-(SUM(B181)*output_kgyear*$E107*percnt_var*start_time+SUM(B181)*output_kgyear*$E107*(1-start_time)),IF($C107<=start_time,-SUM(B181)*output_kgyear*$E107*percnt_var,-SUM(B181)*output_kgyear*$E107))))","v":""},"","","","","","","","","","","",""]
["",{"$f":"IF($C108=\"\",\"\",IF($C108<0,0,IF(AND($C108=1,start_time<1),-(SUM(B182)*output_kgyear*$E108*percnt_var*start_time+SUM(B182)*output_kgyear*$E108*(1-start_time)),IF($C108<=start_time,-SUM(B182)*output_kgyear*$E108*percnt_var,-SUM(B182)*output_kgyear*$E108))))","v":""},"","","","","","","","","","","",""]
[]
["Discounted value",{"$f":"+B186+NPV($X$59,B187:B228)","v":-25382381.493191231},{"$f":"+C186+NPV($X$59,C187:C228)","v":-234043.37499518201},0,0,0,0,0,0,0,0,0,0,0]
["Cost per kg H2",{"$f":"-B231/$AE$116*(1+inflation_rate)^construct/INFLATION_FACTOR","v":5.8615390927069262},{"$f":"-C231/$AE$116*(1+inflation_rate)^construct/INFLATION_FACTOR","v":5.4047505049568456E-2},0,0,{"$f":"-F231/$AE$116*(1+inflation_rate)^construct/INFLATION_FACTOR","v":0},0,0,0,0,0,0,0,0]
["Levelized and escalated cost in startup year",{"$f":"IF(B132>0,B232/B133*(1+inflation_rate)^construct,\"\")","v":2.7261106049604553},{"$f":"IF(C132>0,C232/C133*(1+inflation_rate)^construct,\"\")","v":0.1123967502969597},"","","","","","","","","","",""]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Lookup Electricity Prices in Startup Year"]
["Feed","LHV","Price Table Start Year Column (relative)","Raw Price ($/GJ)","Price in Usage Units"]
[{"$f":"'HyARC Physical Property Data'!A76","v":"Commercial Electricity"},{"$f":"VLOOKUP(A281,MASTER_PROPERTY_TABLE,9,FALSE)","v":3.5999999999999995E-3},{"$f":"MATCH(startup_year,Feedstock_Year,0)","v":19},{"$f":"VLOOKUP(A281,FEEDPRICETABLE,C281,FALSE)","v":29.932211922183079},{"$f":"B281*D281","v":0.10775596291985907}]
[{"$f":"'HyARC Physical Property Data'!A77","v":"Industrial Electricity"},{"$f":"VLOOKUP(A282,MASTER_PROPERTY_TABLE,9,FALSE)","v":3.5999999999999995E-3},{"$f":"MATCH(startup_year,Feedstock_Year,0)+2","v":21},{"$f":"VLOOKUP(A282,FEEDPRICETABLE,C282,FALSE)","v":19.537493744407882},{"$f":"B282*D282","v":7.033497747986836E-2}]

{"sheet":"Energy Feed & Utility Prices","index":11,"n_rows":142,"n_cols":104,"rows_kept":142,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Further extrapolated to allow 2040 comission year using GCAM"]
["AEO_2009_Reference_Case",{"$f":"\"Prices are in $(\" & ref_year&\")/GJ LHV\"","v":"Prices are in $(2016)/GJ LHV"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Except as noted,values are extrapolated based on PNNL mini-CAM model (see AEO Data tab)"]
["Year","Source Data Year","Reference year Conversion","Display Units","Use Category","LHV (MJ/kg)","HHV (MJ/kg)",2004,2005,2006,2007,2008,2009,2010,2011,2012,2013,2014,2015,2016,2017,2018,2019,2020,2021,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,2033,2034,2035,2036,2037,2038,2039,2040,2041,2042,2043,2044,2045,2046,2047,2048,2049,2050,2051,2052,2053,2054,2055,2056,2057,2058,2059,2060,2061,2062,2063,2064,2065,2066,2067,2068,2069,2070,{"$f":"+BV5+1","v":2071},{"$f":"+BW5+1","v":2072},{"$f":"+BX5+1","v":2073},{"$f":"+BY5+1","v":2074},{"$f":"+BZ5+1","v":2075},{"$f":"+CA5+1","v":2076},{"$f":"+CB5+1","v":2077},{"$f":"+CC5+1","v":2078},{"$f":"+CD5+1","v":2079},{"$f":"+CE5+1","v":2080},{"$f":"+CF5+1","v":2081},{"$f":"+CG5+1","v":2082},{"$f":"+CH5+1","v":2083},{"$f":"+CI5+1","v":2084},{"$f":"+CJ5+1","v":2085},{"$f":"+CK5+1","v":2086},{"$f":"+CL5+1","v":2087},{"$f":"+CM5+1","v":2088},{"$f":"+CN5+1","v":2089},{"$f":"+CO5+1","v":2090},{"$f":"+CP5+1","v":2091},{"$f":"+CQ5+1","v":2092},{"$f":"+CR5+1","v":2093},{"$f":"+CS5+1","v":2094},{"$f":"+CT5+1","v":2095},{"$f":"+CU5+1","v":2096},{"$f":"+CV5+1","v":2097},{"$f":"+CW5+1","v":2098},{"$f":"+CX5+1","v":2099},{"$f":"+CY5+1","v":2100}]
["Feedstock Type"]
[{"$f":"'HyARC Physical Property Data'!A73","v":"Residential Natural Gas"},2007,{"$f":"VLOOKUP(ref_year,DeflatorTable,2,FALSE)/VLOOKUP(B7,DeflatorTable,2,FALSE)","v":1.1413971588333081},{"$f":"'HyARC Physical Property Data'!H73","v":"mmBtu"},"Feed Utility",{"$f":"'HyARC Physical Property Data'!$E$6","v":47.141269049911173},{"$f":"'HyARC Physical Property Data'!$I$6","v":52.224661236371581},{"$f":"((13.7000589370728/(mmBTU_to_GJ))*($C$7))*($G$7/$F$7)","v":16.420301417436011},{"$f":"((13.7000589370728/(mmBTU_to_GJ))*($C$7))*($G$7/$F$7)","v":16.420301417436011},{"$f":"((13.7000589370728/(mmBTU_to_GJ))*($C$7))*($G$7/$F$7)","v":16.420301417436011},{"$f":"((12.6911582946777/(mmBTU_to_GJ))*($C$7))*($G$7/$F$7)","v":15.211076499173579},{"$f":"((12.9778490066528/(mmBTU_to_GJ))*($C$7))*($G$7/$F$7)","v":15.55469165629321},{"$f":"((10.7176141738892/(mmBTU_to_GJ))*($C$7))*($G$7/$F$7)","v":12.845671395968969},{"$f":"((11.192774772644/(mmBTU_to_GJ))*($C$7))*($G$7/$F$7)","v":13.415178453499211},{"$f":"((11.4872808456421/(mmBTU_to_GJ))*($C$7))*($G$7/$F$7)","v":13.768160766210887},{"$f":"((11.3991556167603/(mmBTU_to_GJ))*($C$7))*($G$7/$F$7)","v":13.662537657042796},{"$f":"((11.3077983856201/(mmBTU_to_GJ))*($C$7))*($G$7/$F$7)","v":13.553040808972668},{"$f":"((11.2896461486816/(mmBTU_to_GJ))*($C$7))*($G$7/$F$7)","v":13.531284318486023},{"$f":"((11.3454151153564/(mmBTU_to_GJ))*($C$7))*($G$7/$F$7)","v":13.598126603380225},{"$f":"((11.5382986068726/(mmBTU_to_GJ))*($C$7))*($G$7/$F$7)","v":13.829308460603693},{"$f":"((11.7583208084106/(mmBTU_to_GJ))*($C$7))*($G$7/$F$7)","v":14.093017608453076},{"$f":"((11.9751005172729/(mmBTU_to_GJ))*($C$7))*($G$7/$F$7)","v":14.352840444037428},{"$f":"((12.23952293396/(mmBTU_to_GJ))*($C$7))*($G$7/$F$7)","v":14.669765780159871},{"$f":"((12.557071685791/(mmBTU_to_GJ))*($C$7))*($G$7/$F$7)","v":15.050366056680263},{"$f":"((12.7957820892334/(mmBTU_to_GJ))*($C$7))*($G$7/$F$7)","v":15.336474079573154},{"$f":"((12.8716516494751/(mmBTU_to_GJ))*($C$7))*($G$7/$F$7)","v":15.427408071412112},{"$f":"((12.6602811813354/(mmBTU_to_GJ))*($C$7))*($G$7/$F$7)","v":15.174068519112346},{"$f":"((12.6240320205688/(mmBTU_to_GJ))*($C$7))*($G$7/$F$7)","v":15.130621834054226},{"$f":"((12.5992183685303/(mmBTU_to_GJ))*($C$7))*($G$7/$F$7)","v":15.100881257928895},{"$f":"((12.7868556976318/(mmBTU_to_GJ))*($C$7))*($G$7/$F$7)","v":15.325775290513809},{"$f":"((13.07555103302/(mmBTU_to_GJ))*($C$7))*($G$7/$F$7)","v":15.671793103039724},{"$f":"((13.407883644104/(mmBTU_to_GJ))*($C$7))*($G$7/$F$7)","v":16.070112677423158},{"$f":"((13.6725673675537/(mmBTU_to_GJ))*($C$7))*($G$7/$F$7)","v":16.387351204592733},{"$f":"((13.9620389938354/(mmBTU_to_GJ))*($C$7))*($G$7/$F$7)","v":16.734299445996175},{"$f":"($BB7-$AH7)/20+AH7","v":16.876364426263383},{"$f":"($BB7-$AH7)/20+AI7","v":17.01842940653059},17.160494386797797,17.302559367065005,17.444624347332212,17.586689327599419,17.728754307866627,17.870819288133834,18.012884268401042,18.154949248668249,18.297014228935456,18.439079209202664,18.581144189469871,18.723209169737078,18.865274150004286,19.007339130271493,19.149404110538701,{"$f":"($BB7-$AH7)/20+AY7","v":19.291469090805908},19.433534071073115,{"$f":"1.16978897829057*AH7","v":19.575599051340316},{"$f":"($BQ7-$BB7)/15+BB7","v":19.769431803386947},{"$f":"($BQ7-$BB7)/15+BC7","v":19.963264555433579},20.15709730748021,20.350930059526842,20.544762811573474,20.738595563620105,20.932428315666737,21.126261067713369,21.32009381976,21.513926571806632,21.707759323853264,21.901592075899895,22.095424827946527,22.289257579993158,{"$f":"1.14852629914794*BB7","v":22.483090332039815},{"$f":"($BV7-$BQ7)/5+BQ7","v":22.705712345401611},{"$f":"($BV7-$BQ7)/5+BR7","v":22.928334358763408},{"$f":"($BV7-$BQ7)/5+BS7","v":23.150956372125204},{"$f":"($BV7-$BQ7)/5+BT7","v":23.373578385487001},{"$f":"1.04950876638265*BQ7","v":23.59620039884879},{"$f":"+BV7*BW$133/BV$133","v":23.674546722408877},{"$f":"+BW7*BX$133/BW$133","v":23.753153178800169},23.832020631740154,23.911149947814113,23.990541996484659,24.041736091563465,24.093039431167519,24.144452248416805,24.195974776928761,24.247607250819346,24.264371987566129,24.281148315411173,24.297936242368532,24.314735776457805,24.331546925704139,24.337245159046461,24.34294472686469,24.348645629471353,24.354347867179047,24.360051440300435,24.368695752977374,24.377343133141338,24.38599358188084,24.394647100284782,24.403303689442453,24.416626216805682,24.429956017353625,24.443293095056941,24.456637453888455,24.469989097823163]
[{"$f":"'HyARC Physical Property Data'!A71","v":"Commercial Natural Gas"},2007,{"$f":"VLOOKUP(ref_year,DeflatorTable,2,FALSE)/VLOOKUP(B8,DeflatorTable,2,FALSE)","v":1.1413971588333081},{"$f":"'HyARC Physical Property Data'!H71","v":"mmBtu"},"Feed Utility",{"$f":"'HyARC Physical Property Data'!$E$6","v":47.141269049911173},{"$f":"'HyARC Physical Property Data'!$I$6","v":52.224661236371581},{"$f":"((11.8960943222046/(mmBTU_to_GJ))*($C$8))*($G$8/$F$8)","v":14.25814701659854},{"$f":"((11.8960943222046/(mmBTU_to_GJ))*($C$8))*($G$8/$F$8)","v":14.25814701659854},{"$f":"((11.8960943222046/(mmBTU_to_GJ))*($C$8))*($G$8/$F$8)","v":14.25814701659854},{"$f":"((10.9898433685303/(mmBTU_to_GJ))*($C$8))*($G$8/$F$8)","v":13.1719536003861},{"$f":"((11.3387994766235/(mmBTU_to_GJ))*($C$8))*($G$8/$F$8)","v":13.590197383326352},{"$f":"((8.90759468078613/(mmBTU_to_GJ))*($C$8))*($G$8/$F$8)","v":10.676259878492866},{"$f":"((9.46560573577881/(mmBTU_to_GJ))*($C$8))*($G$8/$F$8)","v":11.345067929562392},{"$f":"((9.74632167816162/(mmBTU_to_GJ))*($C$8))*($G$8/$F$8)","v":11.681521984817001},{"$f":"((9.72109222412109/(mmBTU_to_GJ))*($C$8))*($G$8/$F$8)","v":11.651283046295227},{"$f":"((9.67193412780762/(mmBTU_to_GJ))*($C$8))*($G$8/$F$8)","v":11.59236426628982},{"$f":"((9.71388721466064/(mmBTU_to_GJ))*($C$8))*($G$8/$F$8)","v":11.642647431835503},{"$f":"((9.83065605163574/(mmBTU_to_GJ))*($C$8))*($G$8/$F$8)","v":11.782601537733989},{"$f":"((10.0382099151611/(mmBTU_to_GJ))*($C$8))*($G$8/$F$8)","v":12.031366671890995},{"$f":"((10.2545003890991/(mmBTU_to_GJ))*($C$8))*($G$8/$F$8)","v":12.290603131536537},{"$f":"((10.476261138916/(mmBTU_to_GJ))*($C$8))*($G$8/$F$8)","v":12.556396028579952},{"$f":"((10.746561050415/(mmBTU_to_GJ))*($C$8))*($G$8/$F$8)","v":12.880365877199319},{"$f":"((11.0803880691528/(mmBTU_to_GJ))*($C$8))*($G$8/$F$8)","v":13.280476584323763},{"$f":"((11.3143692016602/(mmBTU_to_GJ))*($C$8))*($G$8/$F$8)","v":13.560916306474725},{"$f":"((11.4017143249512/(mmBTU_to_GJ))*($C$8))*($G$8/$F$8)","v":13.665604414633171},{"$f":"((11.2125005722046/(mmBTU_to_GJ))*($C$8))*($G$8/$F$8)","v":13.438820948467498},{"$f":"((11.1975994110107/(mmBTU_to_GJ))*($C$8))*($G$8/$F$8)","v":13.420961057543121},{"$f":"((11.159740447998/(mmBTU_to_GJ))*($C$8))*($G$8/$F$8)","v":13.37558493274866},{"$f":"((11.3503875732422/(mmBTU_to_GJ))*($C$8))*($G$8/$F$8)","v":13.604086377542172},{"$f":"((11.6409521102905/(mmBTU_to_GJ))*($C$8))*($G$8/$F$8)","v":13.952344534785565},{"$f":"((11.9785671234131/(mmBTU_to_GJ))*($C$8))*($G$8/$F$8)","v":14.356995369062137},{"$f":"((12.2332496643066/(mmBTU_to_GJ))*($C$8))*($G$8/$F$8)","v":14.662246908959766},{"$f":"((12.5188312530518/(mmBTU_to_GJ))*($C$8))*($G$8/$F$8)","v":15.004532718678215},{"$f":"($BB8-$AH8)/20+AH8","v":15.131912932679805},15.259293146681395,15.386673360682986,15.514053574684576,15.641433788686166,15.768814002687757,15.896194216689347,16.023574430690935,16.150954644692526,16.278334858694116,16.405715072695706,16.533095286697296,16.660475500698887,16.787855714700477,16.915235928702067,17.042616142703658,17.169996356705248,17.297376570706838,17.424756784708428,{"$f":"1.16978897829057*AH8","v":17.552136998710015},{"$f":"($BQ8-$BB8)/15+BB8","v":17.725933928747082},17.899730858784149,18.073527788821217,18.247324718858284,18.421121648895351,18.594918578932418,18.768715508969485,18.942512439006553,19.11630936904362,19.290106299080687,19.463903229117754,19.637700159154821,19.811497089191889,19.985294019228956,{"$f":"1.14852629914794*BB8","v":20.159090949266044},{"$f":"($BV8-$BQ8)/5+BQ8","v":20.358701294124806},20.558311638983568,20.75792198384233,20.957532328701092,{"$f":"1.04950876638265*BQ8","v":21.15714267355985},{"$f":"+BV8*BW$134/BV$134","v":21.227390608290499},{"$f":"+BW8*BX$134/BW$134","v":21.297871786820185},21.368586983586905,21.439536975600014,21.510722542448768,21.556624880762481,21.602625171372235,21.648723623301212,21.694920446018617,21.741215849440653,21.75624767326148,21.771289890048781,21.78634250698822,21.801405531270447,21.816478970091065,21.821588196736581,21.826698619917845,21.831810239915068,21.836923057008537,21.8420370714786,21.849787851414753,21.857541381762392,21.865297663497515,21.873056697596471,21.880818485035956,21.89276390876655,21.904715853877878,21.916674323930163,21.928639322485584,21.940610853108243]
[{"$f":"'HyARC Physical Property Data'!A72","v":"Industrial Natural Gas"},2007,{"$f":"VLOOKUP(ref_year,DeflatorTable,2,FALSE)/VLOOKUP(B9,DeflatorTable,2,FALSE)","v":1.1413971588333081},{"$f":"'HyARC Physical Property Data'!H72","v":"mmBtu"},"Feed Utility",{"$f":"'HyARC Physical Property Data'!$E$6","v":47.141269049911173},{"$f":"'HyARC Physical Property Data'!$I$6","v":52.224661236371581},{"$f":"((7.95407009124756/(mmBTU_to_GJ))*($C$9))*($G$9/$F$9)","v":9.5334063155208515},{"$f":"((7.95407009124756/(mmBTU_to_GJ))*($C$9))*($G$9/$F$9)","v":9.5334063155208515},{"$f":"((7.95407009124756/(mmBTU_to_GJ))*($C$9))*($G$9/$F$9)","v":9.5334063155208515},{"$f":"((7.51525163650513/(mmBTU_to_GJ))*($C$9))*($G$9/$F$9)","v":9.0074573887680014},{"$f":"((8.80127239227294/(mmBTU_to_GJ))*($C$9))*($G$9/$F$9)","v":10.54882655628621},{"$f":"((4.84856796264648/(mmBTU_to_GJ))*($C$9))*($G$9/$F$9)","v":5.8112850284270117},{"$f":"((5.49891996383666/(mmBTU_to_GJ))*($C$9))*($G$9/$F$9)","v":6.5907689661258342},{"$f":"((5.82616424560547/(mmBTU_to_GJ))*($C$9))*($G$9/$F$9)","v":6.9829898878355561},{"$f":"((5.87778615951538/(mmBTU_to_GJ))*($C$9))*($G$9/$F$9)","v":7.0448616936459612},{"$f":"((5.95383930206299/(mmBTU_to_GJ))*($C$9))*($G$9/$F$9)","v":7.1360157193411098},{"$f":"((6.10985708236694/(mmBTU_to_GJ))*($C$9))*($G$9/$F$9)","v":7.3230119206594617},{"$f":"((6.32948446273804/(mmBTU_to_GJ))*($C$9))*($G$9/$F$9)","v":7.5862478528390263},{"$f":"((6.51258134841919/(mmBTU_to_GJ))*($C$9))*($G$9/$F$9)","v":7.8056999052198099},{"$f":"((6.70273017883301/(mmBTU_to_GJ))*($C$9))*($G$9/$F$9)","v":8.0336041152607454},{"$f":"((6.89887094497681/(mmBTU_to_GJ))*($C$9))*($G$9/$F$9)","v":8.2686900017610387},{"$f":"((7.15282821655273/(mmBTU_to_GJ))*($C$9))*($G$9/$F$9)","v":8.5730722650476565},{"$f":"((7.46860218048096/(mmBTU_to_GJ))*($C$9))*($G$9/$F$9)","v":8.9515453571194765},{"$f":"((7.67867755889893/(mmBTU_to_GJ))*($C$9))*($G$9/$F$9)","v":9.2033326705791669},{"$f":"((7.75380706787109/(mmBTU_to_GJ))*($C$9))*($G$9/$F$9)","v":9.2933796687952501},{"$f":"((7.55847835540771/(mmBTU_to_GJ))*($C$9))*($G$9/$F$9)","v":9.0592670749107693},{"$f":"((7.54617786407471/(mmBTU_to_GJ))*($C$9))*($G$9/$F$9)","v":9.0445242350297033},{"$f":"((7.45927095413208/(mmBTU_to_GJ))*($C$9))*($G$9/$F$9)","v":8.9403613505435402},{"$f":"((7.60022306442261/(mmBTU_to_GJ))*($C$9))*($G$9/$F$9)","v":9.109300487741784},{"$f":"((7.85960483551025/(mmBTU_to_GJ))*($C$9))*($G$9/$F$9)","v":9.4201843228413633},{"$f":"((8.19417572021484/(mmBTU_to_GJ))*($C$9))*($G$9/$F$9)","v":9.8211865957207394},{"$f":"((8.42161273956299/(mmBTU_to_GJ))*($C$9))*($G$9/$F$9)","v":10.09378282529417},{"$f":"((8.69355010986328/(mmBTU_to_GJ))*($C$9))*($G$9/$F$9)","v":10.419715261607452},{"$f":"($BB9-$AH9)/20+AH9","v":10.508172902024802},10.596630542442151,10.6850881828595,10.77354582327685,10.862003463694199,10.950461104111548,11.038918744528898,11.127376384946247,11.215834025363597,11.304291665780946,11.392749306198295,11.481206946615645,11.569664587032994,11.658122227450344,11.746579867867693,11.835037508285042,11.923495148702392,12.011952789119741,12.10041042953709,{"$f":"1.16978897829057*AH9","v":12.18886806995444},12.309559234303295,12.43025039865215,12.550941563001006,12.671632727349861,12.792323891698716,12.913015056047572,13.033706220396427,13.154397384745282,13.275088549094137,13.395779713442993,13.516470877791848,13.637162042140703,13.757853206489559,13.878544370838414,{"$f":"1.14852629914794*BB9","v":13.999235535187266},14.137852511516721,14.276469487846176,14.415086464175632,14.553703440505087,{"$f":"1.04950876638265*BQ9","v":14.692320416834542},{"$f":"+BV9*BW$135/BV$135","v":14.741103240754025},{"$f":"+BW9*BX$135/BW$135","v":14.79004803799304},14.839155346350635,14.888425705411509,14.937859656551939,14.969735977130417,15.001680319489591,15.033692828783058,15.065773650474167,15.09792293033667,15.10836159757225,15.118807482076999,15.129260588840916,15.139720922857455,15.150188489123522,15.153736529429171,15.157285400654516,15.160835102994151,15.164385636642713,15.167937001794892,15.173319436656698,15.178703781508307,15.184090037027495,15.189478203892271,15.194868282780888,15.203163637010553,15.211463519933757,15.219767934022853,15.228076881751546,15.236390365594895]
[{"$f":"'HyARC Physical Property Data'!A74","v":"Electric Utility Natural Gas"},2007,1.1413971588333081,{"$f":"'HyARC Physical Property Data'!H74","v":"mmBtu"},"Feed Utility",{"$f":"'HyARC Physical Property Data'!$E$6","v":47.141269049911173},{"$f":"'HyARC Physical Property Data'!$I$6","v":52.224661236371581},{"$f":"((7.05463790893555/(mmBTU_to_GJ))*($C$10))*($G$10/$F$10)","v":8.4553855853953603},{"$f":"((7.05463790893555/(mmBTU_to_GJ))*($C$10))*($G$10/$F$10)","v":8.4553855853953603},{"$f":"((7.05463790893555/(mmBTU_to_GJ))*($C$10))*($G$10/$F$10)","v":8.4553855853953603},{"$f":"((7.01915979385375/(mmBTU_to_GJ))*($C$10))*($G$10/$F$10)","v":8.4128630425332123},{"$f":"((8.87161254882813/(mmBTU_to_GJ))*($C$10))*($G$10/$F$10)","v":10.63313324268012},{"$f":"((4.55562210083008/(mmBTU_to_GJ))*($C$10))*($G$10/$F$10)","v":5.4601727177347454},{"$f":"((5.12931346893311/(mmBTU_to_GJ))*($C$10))*($G$10/$F$10)","v":6.1477745177052308},{"$f":"((5.45354604721069/(mmBTU_to_GJ))*($C$10))*($G$10/$F$10)","v":6.5363857411404362},{"$f":"((5.51876354217529/(mmBTU_to_GJ))*($C$10))*($G$10/$F$10)","v":6.6145526256719327},{"$f":"((5.53977298736572/(mmBTU_to_GJ))*($C$10))*($G$10/$F$10)","v":6.6397336430839395},{"$f":"((5.68350362777709/(mmBTU_to_GJ))*($C$10))*($G$10/$F$10)","v":6.8120030069834847},{"$f":"((5.8920464515686/(mmBTU_to_GJ))*($C$10))*($G$10/$F$10)","v":7.0619534663813974},{"$f":"((6.08193254470825/(mmBTU_to_GJ))*($C$10))*($G$10/$F$10)","v":7.2895427708255562},{"$f":"((6.26939964294434/(mmBTU_to_GJ))*($C$10))*($G$10/$F$10)","v":7.5142327720166309},{"$f":"((6.47751331329346/(mmBTU_to_GJ))*($C$10))*($G$10/$F$10)","v":7.7636688665559168},{"$f":"((6.73541975021362/(mmBTU_to_GJ))*($C$10))*($G$10/$F$10)","v":8.0727844295748614},{"$f":"((7.02784395217896/(mmBTU_to_GJ))*($C$10))*($G$10/$F$10)","v":8.4232715012056651},{"$f":"((7.25390911102295/(mmBTU_to_GJ))*($C$10))*($G$10/$F$10)","v":8.6942234777810281},{"$f":"((7.3283839225769/(mmBTU_to_GJ))*($C$10))*($G$10/$F$10)","v":8.7834857838294642},{"$f":"((7.15062761306763/(mmBTU_to_GJ))*($C$10))*($G$10/$F$10)","v":8.5704347163559618},{"$f":"((7.19241189956665/(mmBTU_to_GJ))*($C$10))*($G$10/$F$10)","v":8.6205155650572607},{"$f":"((7.13988399505615/(mmBTU_to_GJ))*($C$10))*($G$10/$F$10)","v":8.5575578778786525},{"$f":"((7.28062534332275/(mmBTU_to_GJ))*($C$10))*($G$10/$F$10)","v":8.7262444047796599},{"$f":"((7.5354790687561/(mmBTU_to_GJ))*($C$10))*($G$10/$F$10)","v":9.0317011191042926},{"$f":"((7.86007928848267/(mmBTU_to_GJ))*($C$10))*($G$10/$F$10)","v":9.4207529817684019},{"$f":"((8.07421207427979/(mmBTU_to_GJ))*($C$10))*($G$10/$F$10)","v":9.6774033292080919},{"$f":"((8.33951759338379/(mmBTU_to_GJ))*($C$10))*($G$10/$F$10)","v":9.9953871139061636},{"$f":"($BB10-$AH10)/20+AH10","v":10.080242442190606},10.165097770475048,10.249953098759491,10.334808427043933,10.419663755328376,10.504519083612818,10.589374411897261,10.674229740181703,10.759085068466145,10.843940396750588,10.92879572503503,11.013651053319473,11.098506381603915,11.183361709888358,11.2682170381728,11.353072366457242,11.437927694741685,11.522783023026127,11.60763835131057,{"$f":"1.16978897829057*AH10","v":11.692493679595019},11.808269867197748,11.924046054800476,12.039822242403204,12.155598430005933,12.271374617608661,12.387150805211389,12.502926992814118,12.618703180416846,12.734479368019574,12.850255555622303,12.966031743225031,13.081807930827759,13.197584118430488,13.313360306033216,{"$f":"1.14852629914794*BB10","v":13.429136493635946},13.562108489912774,13.695080486189601,13.828052482466429,13.961024478743257,{"$f":"1.04950876638265*BQ10","v":14.093996475020086},{"$f":"+BV10*BW$136/BV$136","v":14.140792687521339},{"$f":"+BW10*BX$136/BW$136","v":14.187744277208072},14.234851759978229,14.282115653442684,14.329536476930937,14.360114679496878,14.390758133752827,14.42146697894121,14.452241354601584,14.483081400571274,14.493094967866853,14.503115458518533,14.513142877313106,14.523177229040675,14.53321851849465,14.536622069883558,14.540026418354136,14.543431564093051,14.546837507287016,14.550244248122791,14.555407490947415,14.560572565980214,14.565739473871359,14.570908215271251,14.576078790830522,14.584036328507008,14.591998210452399,14.59996443903837,14.607935016637887,14.615909945625214]
[{"$f":"'HyARC Physical Property Data'!A75","v":"Bio Methane"},2007,1.1413971588333081,{"$f":"'HyARC Physical Property Data'!H75","v":"mmBtu"},"Feed Utility",{"$f":"'HyARC Physical Property Data'!$E$6","v":47.141269049911173},{"$f":"'HyARC Physical Property Data'!$I$6","v":52.224661236371581},{"$f":"13.11*($C$11/mmBTU_to_GJ)","v":14.183617774696369},14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,{"$f":"13.11*($C$11/mmBTU_to_GJ)","v":14.183617774696369},14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,{"$f":"+BV11*BW$136/BV$136","v":14.230711556264829},{"$f":"+BW11*BX$136/BW$136","v":14.277961703035571},14.325368734187041,14.372933170621517,14.420655534970821,14.451428179067991,14.482266489779443,14.51317060723302,14.54414067185559,14.575176824373679,14.585254066221541,14.595338275449933,14.605429456876088,14.615527615320566,14.625632755607262,14.629057949594106,14.632483945731124,14.635910744206171,14.639338345207147,14.642766748922,14.647962823919764,14.6531607427764,14.658360506146211,14.663562114683737,14.668765569043746,14.676773707333766,14.68478621751715,14.692803101980653,14.700824363112332,14.708850003301547]
[{"$f":"'HyARC Physical Property Data'!A85","v":"Woody Biomass"},2005,{"$f":"VLOOKUP(ref_year,DeflatorTable,2,FALSE)/VLOOKUP(B12,DeflatorTable,2,FALSE)","v":1.208440716126562},{"$f":"+'HyARC Physical Property Data'!$H$85","v":"kg"},"Feed",{"$f":"'HyARC Physical Property Data'!$E$45","v":19.551069237418005},{"$f":"'HyARC Physical Property Data'!$I$45","v":20.588656379262464},{"$f":"1.27*($C$12)","v":1.5347197094807337},1.5347197094807337,1.5347197094807337,1.5347197094807337,1.5347197094807337,1.5347197094807337,1.5347197094807337,1.5347197094807337,{"$f":"1.28*($C$12)","v":1.5468041166419995},{"$f":"1.32*($C$12)","v":1.595141745287062},{"$f":"1.32*($C$12)","v":1.595141745287062},{"$f":"1.34*($C$12)","v":1.6193105596095931},{"$f":"1.34*($C$12)","v":1.6193105596095931},{"$f":"1.36*($C$12)","v":1.6434793739321245},{"$f":"1.36*($C$12)","v":1.6434793739321245},{"$f":"1.38*($C$12)","v":1.6676481882546554},{"$f":"1.4*($C$12)","v":1.6918170025771868},{"$f":"1.46*($C$12)","v":1.7643234455447805},{"$f":"1.48*($C$12)","v":1.7884922598673119},{"$f":"1.48*($C$12)","v":1.7884922598673119},{"$f":"1.51*($C$12)","v":1.8247454813511086},{"$f":"1.52*($C$12)","v":1.8368298885123742},{"$f":"1.62*($C$12)","v":1.9576739601250306},{"$f":"1.72*($C$12)","v":2.0785180317376866},{"$f":"1.82*($C$12)","v":2.1993621033503428},{"$f":"1.91*($C$12)","v":2.3081217678017332},{"$f":"2.01*($C$12)","v":2.4289658394143894},{"$f":"2.11*($C$12)","v":2.5498099110270456},{"$f":"2.2*($C$12)","v":2.6585695754784364},{"$f":"2.3*($C$12)","v":2.7794136470910926},{"$f":"2.4*($C$12)","v":2.9002577187037488},{"$f":"2.5*($C$12)","v":3.021101790316405},{"$f":"2.57*($C$12)","v":3.1056926404452643},{"$f":"2.64*($C$12)","v":3.190283490574124},{"$f":"2.71*($C$12)","v":3.2748743407029832},{"$f":"2.78*($C$12)","v":3.359465190831842},{"$f":"2.85*($C$12)","v":3.4440560409607017},{"$f":"2.92*($C$12)","v":3.528646891089561},{"$f":"2.99*($C$12)","v":3.6132377412184207},{"$f":"3.07*($C$12)","v":3.7099129985085453},{"$f":"3.14*($C$12)","v":3.794503848637405},{"$f":"3.21*($C$12)","v":3.8790946987662642},{"$f":"3.28*($C$12)","v":3.963685548895123},{"$f":"3.35*($C$12)","v":4.0482763990239832},{"$f":"3.42*($C$12)","v":4.1328672491528424},{"$f":"3.49*($C$12)","v":4.2174580992817017},{"$f":"3.56*($C$12)","v":4.3020489494105609},{"$f":"3.64*($C$12)","v":4.3987242067006855},{"$f":"3.71*($C$12)","v":4.4833150568295448},{"$f":"3.78*($C$12)","v":4.567905906958404},{"$f":"3.85*($C$12)","v":4.6524967570872642},{"$f":"3.92*($C$12)","v":4.7370876072161234},{"$f":"3.99*($C$12)","v":4.8216784573449827},{"$f":"4.06*($C$12)","v":4.906269307473841},{"$f":"4.14*($C$12)","v":5.0029445647639665},{"$f":"4.21*($C$12)","v":5.0875354148928258},{"$f":"4.28*($C$12)","v":5.1721262650216859},{"$f":"4.35*($C$12)","v":5.2567171151505443},{"$f":"4.42*($C$12)","v":5.3413079652794044},{"$f":"4.49*($C$12)","v":5.4258988154082637},{"$f":"4.56*($C$12)","v":5.5104896655371221},{"$f":"4.63*($C$12)","v":5.5950805156659822},{"$f":"4.71*($C$12)","v":5.6917557729561068},{"$f":"4.78*($C$12)","v":5.7763466230849669},{"$f":"4.85*($C$12)","v":5.8609374732138253},{"$f":"4.92*($C$12)","v":5.9455283233426854},{"$f":"4.99*($C$12)","v":6.0301191734715447},{"$f":"+BV12*BW$138/BV$138","v":6.0446132076616896},{"$f":"+BW12*BX$138/BW$138","v":6.0591420798079438},6.0737058736470511,6.0883046731170198,6.1029385623576156,6.1157485681116217,6.1285854619369617,6.1414493002714252,6.1543401396712598,6.167258036811428,6.183149548139812,6.1990820079952069,6.215055521891923,6.2310701956161552,6.2471261352266838,6.2604975997429575,6.2738976847896071,6.2873264516265444,6.3007839616448056,6.3142702763668277,6.326614172551615,6.3389822000716718,6.3513744061018391,6.3637908379091801,6.376231542853164,6.3909193633613004,6.4056410176582252,6.4203965836809767,6.4351861395461265,6.450009763550189]
[{"$f":"'HyARC Physical Property Data'!A86","v":"Woody Biomass B2A"},2007,{"$f":"VLOOKUP(ref_year,DeflatorTable,2,FALSE)/VLOOKUP(B13,DeflatorTable,2,FALSE)","v":1.1413971588333081},{"$f":"+'HyARC Physical Property Data'!$H$86","v":"kg"},"Feed",{"$f":"'HyARC Physical Property Data'!$E$45","v":19.551069237418005},{"$f":"'HyARC Physical Property Data'!$I$45","v":20.588656379262464},{"$f":"3.80872262322035*($C$13)","v":4.3472651809278515},{"$f":"3.80872262322035*($C$13)","v":4.3472651809278515},{"$f":"3.80872262322035*($C$13)","v":4.3472651809278515},{"$f":"3.80872262322035*($C$13)","v":4.3472651809278515},{"$f":"3.58036841709093*($C$13)","v":4.0866223388440961},{"$f":"3.28153451771169*($C$13)","v":3.7455341751295528},{"$f":"3.05599949931226*($C$13)","v":3.4881091459110256},{"$f":"2.9206784882726*($C$13)","v":3.3336541283799068},{"$f":"2.85865635821276*($C$13)","v":3.2628622453448157},3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,3.2628622453448157,{"$f":"+BV13*BW$138/BV$138","v":3.2707048825433991},{"$f":"+BW13*BX$138/BW$138","v":3.2785663703564443},3.2864467540934128,3.2943460791726715,3.3022643911217555,3.3091958103748405,3.3161417786061929,3.323102326353971,3.3300774842204302,3.3370672828720607,3.3456660867834271,3.3542870477034605,3.3629302227253368,3.3715956690893476,3.3802834441832799,3.3875186654915184,3.3947693732014868,3.4020356004605672,3.4093173804870895,3.416614746570485,3.4232939566595637,3.4299862240731356,3.4366915743372313,3.4434100330277828,3.4501416257707223,3.4580891196135033,3.466054920721676,3.474039071266517,3.4820416135164467,3.490062589837251]
[{"$f":"'HyARC Physical Property Data'!$A$87","v":"Woody Biomass MYPP"},2007,{"$f":"VLOOKUP(ref_year,DeflatorTable,2,FALSE)/VLOOKUP(B14,DeflatorTable,2,FALSE)","v":1.1413971588333081},{"$f":"+'HyARC Physical Property Data'!$H$87","v":"kg"},"Feed",18.608000000000001,null,{"$f":"4.44432502149613*$C$14","v":5.0727399524674635},{"$f":"4.44432502149613*$C$14","v":5.0727399524674635},5.0727399524674635,5.0727399524674635,5.0727399524674635,5.0727399524674635,5.0727399524674635,{"$f":"N14-($N$14-$U$14)/7","v":4.9524277749801975},4.8321155974929315,4.7118034200056655,4.5914912425183996,4.4711790650311336,4.3508668875438676,{"$f":"3.70647033533964*$C$14","v":4.2305547100566034},{"$f":"3.70647033533964*$C$14","v":4.2305547100566034},4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,{"$f":"+BV14*BW$138/BV$138","v":4.2407232992414734},{"$f":"+BW14*BX$138/BW$138","v":4.2509163297143298},4.2611338602224134,4.2713759496541703,4.2816426570395922,4.2906297812770164,4.2996357693964899,4.3086606609931088,4.3177044957450779,4.3267673134138871,4.3379163315619822,4.3490940779953462,4.3603006267397229,4.3715360520116029,4.3828004282187161,4.3921814554525627,4.4015825620108968,4.4110037908718764,4.4204451851056508,4.4299067878745575,4.4385669033121991,4.4472439485867392,4.4559379567946618,4.4646489610971525,4.4733769947202253,4.4836815387008029,4.494009819475032,4.5043618917212536,4.5147378102437621,4.525137629973095]
[{"$f":"'HyARC Physical Property Data'!A79","v":"Electric Utility Steam Coal"},2007,{"$f":"VLOOKUP(ref_year,DeflatorTable,2,FALSE)/VLOOKUP(B15,DeflatorTable,2,FALSE)","v":1.1413971588333081},{"$f":"+'HyARC Physical Property Data'!$H$79","v":"kg"},"Feed",{"$f":"'HyARC Physical Property Data'!E42","v":22.7322030001394},{"$f":"'HyARC Physical Property Data'!I42","v":23.967615189707661},{"$f":"1.73552525043488*($C$15/mmBTU_to_GJ*$G$15/$F$15)","v":1.9796962563875427},{"$f":"1.73552525043488*($C$15/mmBTU_to_GJ*$G$15/$F$15)","v":1.9796962563875427},{"$f":"1.73552525043488*($C$15/mmBTU_to_GJ*$G$15/$F$15)","v":1.9796962563875427},{"$f":"1.78000020980835*($C$15/mmBTU_to_GJ*$G$15/$F$15)","v":2.0304283967309829},{"$f":"1.9310736656189*($C$15/mmBTU_to_GJ*$G$15/$F$15)","v":2.2027563734243398},{"$f":"1.98230564594269*($C$15/mmBTU_to_GJ*$G$15/$F$15)","v":2.2611961798339055},{"$f":"1.86225914955139*($C$15/mmBTU_to_GJ*$G$15/$F$15)","v":2.1242603447380195},{"$f":"1.87335216999054*($C$15/mmBTU_to_GJ*$G$15/$F$15)","v":2.1369140419572981},{"$f":"1.85759365558624*($C$15/mmBTU_to_GJ*$G$15/$F$15)","v":2.1189384625385577},{"$f":"1.88174879550934*($C$15/mmBTU_to_GJ*$G$15/$F$15)","v":2.1464919885194074},{"$f":"1.90431761741638*($C$15/mmBTU_to_GJ*$G$15/$F$15)","v":2.1722360174404782},{"$f":"1.90719401836395*($C$15/mmBTU_to_GJ*$G$15/$F$15)","v":2.1755170991685295},{"$f":"1.91704928874969*($C$15/mmBTU_to_GJ*$G$15/$F$15)","v":2.1867589073090032},{"$f":"1.92595064640045*($C$15/mmBTU_to_GJ*$G$15/$F$15)","v":2.1969125967546401},{"$f":"1.94080138206482*($C$15/mmBTU_to_GJ*$G$15/$F$15)","v":2.2138526820642528},{"$f":"1.94636797904968*($C$15/mmBTU_to_GJ*$G$15/$F$15)","v":2.2202024434457042},{"$f":"1.95628917217255*($C$15/mmBTU_to_GJ*$G$15/$F$15)","v":2.2315194489916172},{"$f":"1.96225011348724*($C$15/mmBTU_to_GJ*$G$15/$F$15)","v":2.2383190349972262},{"$f":"1.97535526752472*($C$15/mmBTU_to_GJ*$G$15/$F$15)","v":2.2532679528426334},{"$f":"1.98115420341492*($C$15/mmBTU_to_GJ*$G$15/$F$15)","v":2.259882740884458},{"$f":"1.98549652099609*($C$15/mmBTU_to_GJ*$G$15/$F$15)","v":2.264835979022211},{"$f":"1.98988306522369*($C$15/mmBTU_to_GJ*$G$15/$F$15)","v":2.2698396660522224},{"$f":"1.99634909629822*($C$15/mmBTU_to_GJ*$G$15/$F$15)","v":2.277215402883896},{"$f":"2.00744533538818*($C$15/mmBTU_to_GJ*$G$15/$F$15)","v":2.2898727715858902},{"$f":"2.02021908760071*($C$15/mmBTU_to_GJ*$G$15/$F$15)","v":2.3044436626915257},{"$f":"2.03361201286316*($C$15/mmBTU_to_GJ*$G$15/$F$15)","v":2.3197208382886583},{"$f":"2.04451942443848*($C$15/mmBTU_to_GJ*$G$15/$F$15)","v":2.3321628133374963},{"$f":"(($BB$15-$AH$15)/20+AH15)","v":2.3372909448097223},{"$f":"(($BB$15-$AH$15)/20+AI15)","v":2.3424190762819483},2.3475472077541744,2.3526753392264004,2.3578034706986264,2.3629316021708524,2.3680597336430784,2.3731878651153044,2.3783159965875305,2.3834441280597565,2.3885722595319825,2.3937003910042085,2.3988285224764345,2.4039566539486605,2.4090847854208866,2.4142129168931126,2.4193410483653386,2.4244691798375646,2.4295973113097906,{"$f":"(1.04397747398165*AH15)","v":2.434725442782018},{"$f":"(($BQ$15-$BB$15)/15+BB15)","v":2.4393430815285027},{"$f":"(($BQ$15-$BB$15)/15+BC15)","v":2.4439607202749873},2.448578359021472,2.4531959977679567,2.4578136365144414,2.4624312752609261,2.4670489140074108,2.4716665527538955,2.4762841915003801,2.4809018302468648,2.4855194689933495,2.4901371077398342,2.4947547464863189,2.4993723852328036,{"$f":"(1.02844862093285*BB15)","v":2.5039900239792892},{"$f":"(($BV$15-$BQ$15)/5+BQ15)","v":2.5087390281800759},{"$f":"(($BV$15-$BQ$15)/5+BR15)","v":2.5134880323808626},{"$f":"(($BV$15-$BQ$15)/5+BS15)","v":2.5182370365816493},{"$f":"(($BV$15-$BQ$15)/5+BT15)","v":2.522986040782436},{"$f":"(1.00948287364428*BQ15)","v":2.5277350449832223},{"$f":"+BV15*BW$139/BV$139","v":2.536281204043199},{"$f":"+BW15*BX$139/BW$139","v":2.5448562572844797},2.5534603023969979,2.5620934374009732,2.5707557606480269,2.5781162379988212,2.585497789551864,2.5929004756459051,2.6003243567924534,2.6077694936762716,2.6134538634410465,2.6191506238943774,2.6248598020452683,2.6305814249615964,2.6363155197702408,2.640202757935151,2.6440957278193635,2.6479944378742784,2.6518988965637571,2.6558091123641421,2.6571185824873536,2.6584286982563667,2.659739459989523,2.6610508680053204,2.6623629226224148,2.6604772171816178,2.6585928473532499,2.6567098121913197,2.6548281107505058,2.6529477420861576]
[{"$f":"'HyARC Physical Property Data'!A76","v":"Commercial Electricity"},2007,1.1413971588333081,{"$f":"'HyARC Physical Property Data'!$H$76","v":"kWh"},"Feed Utility Byprod",null,null,{"$f":"(28.3762531280518/(mmBTU_to_GJ))*($C$16)","v":30.700070804448433},{"$f":"(28.3762531280518/(mmBTU_to_GJ))*($C$16)","v":30.700070804448433},{"$f":"(28.3762531280518/(mmBTU_to_GJ))*($C$16)","v":30.700070804448433},{"$f":"(28.0297355651855/(mmBTU_to_GJ))*($C$16)","v":30.325175864409157},{"$f":"(29.057315826416/(mmBTU_to_GJ))*($C$16)","v":31.436907798666674},{"$f":"(27.6067714691162/(mmBTU_to_GJ))*($C$16)","v":29.867573952047074},{"$f":"(24.8355846405029/(mmBTU_to_GJ))*($C$16)","v":26.869446205340434},{"$f":"(25.5812511444092/(mmBTU_to_GJ))*($C$16)","v":27.676177607232201},{"$f":"(25.4402256011963/(mmBTU_to_GJ))*($C$16)","v":27.523603053349618},{"$f":"(25.4701290130615/(mmBTU_to_GJ))*($C$16)","v":27.555955346565124},{"$f":"(25.6722831726074/(mmBTU_to_GJ))*($C$16)","v":27.774664525097851},{"$f":"(25.7632827758789/(mmBTU_to_GJ))*($C$16)","v":27.87311636266093},{"$f":"(26.1006698608398/(mmBTU_to_GJ))*($C$16)","v":28.238133102188346},{"$f":"(26.4680442810059/(mmBTU_to_GJ))*($C$16)","v":28.635592931008837},{"$f":"(26.885612487793/(mmBTU_to_GJ))*($C$16)","v":29.087357068303547},{"$f":"(27.1694507598877/(mmBTU_to_GJ))*($C$16)","v":29.394439719807853},{"$f":"(27.6201095581055/(mmBTU_to_GJ))*($C$16)","v":29.882004337712146},{"$f":"(28.0024471282958/(mmBTU_to_GJ))*($C$16)","v":30.29565269442346},{"$f":"(28.2454071044922/(mmBTU_to_GJ))*($C$16)","v":30.558509402045058},{"$f":"(28.1863746643066/(mmBTU_to_GJ))*($C$16)","v":30.494642615782649},{"$f":"(28.2032489776611/(mmBTU_to_GJ))*($C$16)","v":30.512898817981785},{"$f":"(28.1397113800049/(mmBTU_to_GJ))*($C$16)","v":30.444157933200852},{"$f":"(28.178466796875/(mmBTU_to_GJ))*($C$16)","v":30.486087149034912},{"$f":"(28.4951820373535/(mmBTU_to_GJ))*($C$16)","v":30.828739163860856},{"$f":"(28.9155654907227/(mmBTU_to_GJ))*($C$16)","v":31.283549096842975},{"$f":"(29.2894115447998/(mmBTU_to_GJ))*($C$16)","v":31.688010541359226},{"$f":"(29.6516952514648/(mmBTU_to_GJ))*($C$16)","v":32.079962762666369},{"$f":"($BB16-$AH16)/20+AH16","v":32.070504288889573},32.061045815112777,32.051587341335981,32.042128867559185,32.032670393782389,32.023211920005593,32.013753446228797,32.004294972452001,31.994836498675209,31.985378024898417,31.975919551121624,31.966461077344832,31.957002603568039,31.947544129791247,31.938085656014454,31.928627182237662,31.91916870846087,31.909710234684077,31.900251760907285,{"$f":"0.994103189054944*AH16","v":31.890793287130489},{"$f":"($BQ16-$BB16)/15+BB16","v":31.911051832953525},31.931310378776562,31.951568924599599,31.971827470422635,31.992086016245672,32.012344562068712,32.032603107891752,32.052861653714793,32.073120199537833,32.093378745360873,32.113637291183913,32.133895837006953,32.154154382829994,32.174412928653034,{"$f":"1.00952871208344*BB16","v":32.194671474476053},{"$f":"($BV16-$BQ16)/5+BQ16","v":32.215123058149487},32.235574641822922,32.256026225496356,32.276477809169791,{"$f":"1.00317623736115*BQ16","v":32.296929392843232},{"$f":"+BV16*BW$140/BV$140","v":32.282708933053591},{"$f":"+BW16*BX$140/BW$140","v":32.268494734586014},32.254286794683622,32.240085110590741,32.225889679552914,32.20007724517788,32.174285486159683,32.148514385937681,32.122763927964499,32.097034095706015,32.061589809857011,32.026184664615073,31.990818616757792,31.9554916231105,31.920203640546202,31.881731115497008,31.843304960301854,31.804925119072454,31.766591535987885,31.728304155294506,31.683957370716094,31.639672569825585,31.59544966598812,31.551288572689923,31.50718920353814,31.46414036817173,31.421150351197987,31.378219072252289,31.335346451079825,31.292532407535425]
[{"$f":"'HyARC Physical Property Data'!A77","v":"Industrial Electricity"},2007,1.1413971588333081,{"$f":"'HyARC Physical Property Data'!$H$77","v":"kWh"},"Feed Utility Byprod",null,null,{"$f":"(18.4008941650391/(mmBTU_to_GJ))*($C$17)","v":19.907799355419932},{"$f":"(18.4008941650391/(mmBTU_to_GJ))*($C$17)","v":19.907799355419932},{"$f":"(18.4008941650391/(mmBTU_to_GJ))*($C$17)","v":19.907799355419932},{"$f":"(18.6226921081543/(mmBTU_to_GJ))*($C$17)","v":20.147761006705959},{"$f":"(20.3344097137451/(mmBTU_to_GJ))*($C$17)","v":21.999656373290122},{"$f":"(19.1594867706299/(mmBTU_to_GJ))*($C$17)","v":20.728515416778507},{"$f":"(16.8281726837158/(mmBTU_to_GJ))*($C$17)","v":18.206282928482938},{"$f":"(17.2643089294434/(mmBTU_to_GJ))*($C$17)","v":18.678135697902565},{"$f":"(17.1560707092285/(mmBTU_to_GJ))*($C$17)","v":18.561033520622512},{"$f":"(17.0836048126221/(mmBTU_to_GJ))*($C$17)","v":18.482633171334495},{"$f":"(17.1988334655762/(mmBTU_to_GJ))*($C$17)","v":18.607298249152503},{"$f":"(17.3181438446045/(mmBTU_to_GJ))*($C$17)","v":18.736379318007696},{"$f":"(17.6150741577148/(mmBTU_to_GJ))*($C$17)","v":19.057626157586448},{"$f":"(17.9101543426514/(mmBTU_to_GJ))*($C$17)","v":19.376871356368099},{"$f":"(18.2101707458496/(mmBTU_to_GJ))*($C$17)","v":19.701457015338534},{"$f":"(18.456880569458/(mmBTU_to_GJ))*($C$17)","v":19.968370656782042},{"$f":"(18.8030014038086/(mmBTU_to_GJ))*($C$17)","v":20.342836379000801},{"$f":"(19.0852069854736/(mmBTU_to_GJ))*($C$17)","v":20.648152634090209},{"$f":"(19.30615234375/(mmBTU_to_GJ))*($C$17)","v":20.887191879771816},{"$f":"(19.3043308258057/(mmBTU_to_GJ))*($C$17)","v":20.885221192182819},{"$f":"(19.3253479003906/(mmBTU_to_GJ))*($C$17)","v":20.90795941892992},{"$f":"(19.3248138427734/(mmBTU_to_GJ))*($C$17)","v":20.907381625710087},{"$f":"(19.3542194366455/(mmBTU_to_GJ))*($C$17)","v":20.939195333102905},{"$f":"(19.6148834228516/(mmBTU_to_GJ))*($C$17)","v":21.221205885961488},{"$f":"(19.97239112854/(mmBTU_to_GJ))*($C$17)","v":21.607990985045614},{"$f":"(20.29469871521/(mmBTU_to_GJ))*($C$17)","v":21.956693320302069},{"$f":"(20.5609893798828/(mmBTU_to_GJ))*($C$17)","v":22.244791337440805},22.238232670989351,22.231674004537897,22.225115338086443,22.218556671634989,22.211998005183535,22.205439338732081,22.198880672280627,22.192322005829173,22.185763339377718,22.179204672926264,22.17264600647481,22.166087340023356,22.159528673571902,22.152970007120448,22.146411340668994,22.13985267421754,22.133294007766086,22.126735341314632,22.120176674863178,{"$f":"0.994103189054944*AH17","v":22.113618008411699},22.127665628353387,22.141713248295076,22.155760868236765,22.169808488178454,22.183856108120143,22.197903728061831,22.21195134800352,22.225998967945209,22.240046587886898,22.254094207828587,22.268141827770275,22.282189447711964,22.296237067653653,22.310284687595342,{"$f":"1.00952871208344*BB17","v":22.324332307537027},22.338513783204611,22.352695258872195,22.36687673453978,22.381058210207364,{"$f":"1.00317623736115*BQ17","v":22.395239685874952},{"$f":"+BV17*BW$141/BV$141","v":22.402006623717899},{"$f":"+BW17*BX$141/BW$141","v":22.40877560625643},22.415546634108377,22.422319707891749,22.429094828224738,22.426558269957198,22.424021998554906,22.421486013985415,22.418950316216293,22.416414905215102,22.406246620986774,22.39608294918218,22.385923887709083,22.375769434476197,22.365619587393184,22.353167809865965,22.340722964709347,22.328285048063812,22.315854056072002,22.303429984878701,22.286408389138984,22.269399783989581,22.252404159516296,22.2354215058125,22.218451812979119,22.202497084041635,22.186553811949913,22.17062198847697,22.154701605401723,22.138792654509]
[{"$f":"'HyARC Physical Property Data'!A78","v":"Residential Electricity"},2007,1.1413971588333081,{"$f":"'HyARC Physical Property Data'!$H$78","v":"kWh"},"Feed Utility Byprod",null,null,{"$f":"(31.2067794799805/(mmBTU_to_GJ))*($C$18)","v":33.762397568518793},{"$f":"(31.2067794799805/(mmBTU_to_GJ))*($C$18)","v":33.762397568518793},{"$f":"(31.2067794799805/(mmBTU_to_GJ))*($C$18)","v":33.762397568518793},{"$f":"(31.181957244873/(mmBTU_to_GJ))*($C$18)","v":33.735542565080316},{"$f":"(31.772819519043/(mmBTU_to_GJ))*($C$18)","v":34.374792348018154},{"$f":"(30.736837387085/(mmBTU_to_GJ))*($C$18)","v":33.253970488284573},{"$f":"(28.6163578033447/(mmBTU_to_GJ))*($C$18)","v":30.959838381891004},{"$f":"(29.8736190795898/(mmBTU_to_GJ))*($C$18)","v":32.320060608068538},{"$f":"(30.101655960083/(mmBTU_to_GJ))*($C$18)","v":32.56677212229048},{"$f":"(30.4253902435303/(mmBTU_to_GJ))*($C$18)","v":32.917017990862689},{"$f":"(30.7938537597656/(mmBTU_to_GJ))*($C$18)","v":33.315656105142033},{"$f":"(30.8830280303955/(mmBTU_to_GJ))*($C$18)","v":33.412133128021651},{"$f":"(31.1491451263428/(mmBTU_to_GJ))*($C$18)","v":33.700043362364035},{"$f":"(31.4898681640625/(mmBTU_to_GJ))*($C$18)","v":34.068669245968131},{"$f":"(31.8156299591064/(mmBTU_to_GJ))*($C$18)","v":34.42110866522836},{"$f":"(32.0206985473633/(mmBTU_to_GJ))*($C$18)","v":34.642970943903613},{"$f":"(32.4303588867188/(mmBTU_to_GJ))*($C$18)","v":35.086179614450586},{"$f":"(32.7907905578613/(mmBTU_to_GJ))*($C$18)","v":35.476128131413226},{"$f":"(32.9940071105957/(mmBTU_to_GJ))*($C$18)","v":35.695986705743984},{"$f":"(32.9234657287598/(mmBTU_to_GJ))*($C$18)","v":35.61966847559453},{"$f":"(32.9201545715332/(mmBTU_to_GJ))*($C$18)","v":35.616086157631599},{"$f":"(32.902271270752/(mmBTU_to_GJ))*($C$18)","v":35.596738338956506},{"$f":"(32.9582405090332/(mmBTU_to_GJ))*($C$18)","v":35.657291068393683},{"$f":"(33.321102142334/(mmBTU_to_GJ))*($C$18)","v":36.049868544506616},{"$f":"(33.7343635559082/(mmBTU_to_GJ))*($C$18)","v":36.496973192192904},{"$f":"(34.1495399475098/(mmBTU_to_GJ))*($C$18)","v":36.94614964128175},{"$f":"(34.4904899597167/(mmBTU_to_GJ))*($C$18)","v":37.315021087004148},37.304019105766102,37.293017124528063,37.282015143290025,37.271013162051986,37.260011180813947,37.249009199575909,37.23800721833787,37.227005237099831,37.216003255861793,37.205001274623754,37.193999293385716,37.182997312147677,37.171995330909638,37.1609933496716,37.149991368433561,37.138989387195522,37.127987405957484,37.116985424719445,37.105983443481406,{"$f":"0.994103189054944*AH18","v":37.094981462243304},37.118545955449591,37.142110448655878,37.165674941862164,37.189239435068451,37.212803928274738,37.236368421481025,37.259932914687312,37.283497407893599,37.307061901099885,37.330626394306172,37.354190887512459,37.377755380718746,37.401319873925033,37.42488436713132,{"$f":"1.00952871208344*BB18","v":37.448448860337564},37.472237892815023,37.496026925292483,37.519815957769943,37.543604990247402,{"$f":"1.00317623736115*BQ18","v":37.567394022724876},{"$f":"+BV18*BW$142/BV$142","v":37.550852957486022},{"$f":"+BW18*BX$142/BW$142","v":37.534319175340556},37.517792673081715,37.501273447504133,37.484761495403866,37.454736786829947,37.424736127578718,37.394759498387039,37.364806880007208,37.334878253206945,37.293649892574038,37.252467059817484,37.211329704661502,37.170237776885841,37.129191226325716,37.084440454820722,37.039743620163904,36.995100657346704,36.950511501438903,36.905976087588542,36.854392449105958,36.802880909292512,36.751441367375584,36.70007372272341,36.648777874844889,36.598703995041703,36.548698532074873,36.498761392465255,36.448892482861424,36.399091710039507]
[]
[]
[]
["AEO_2013_Reference_Case",{"$f":"\"Prices are in $(\" & ref_year&\")/GJ LHV\"","v":"Prices are in $(2016)/GJ LHV"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Except as noted,values are extrapolated based on PNNL mini-CAM model (see AEO Data tab)"]
["Year","Source Data Year","Reference year Conversion","Display Units","Use Category","LHV (MJ/kg)","HHV (MJ/kg)",2004,2005,2006,2007,2008,2009,2010,2011,2012,2013,2014,2015,2016,2017,2018,2019,2020,2021,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,2033,2034,2035,2036,2037,2038,2039,2040,2041,2042,2043,2044,2045,2046,2047,2048,2049,2050,2051,2052,2053,2054,2055,2056,2057,2058,2059,2060,2061,2062,2063,2064,2065,2066,2067,2068,2069,2070,{"$f":"+BV23+1","v":2071},{"$f":"+BW23+1","v":2072},{"$f":"+BX23+1","v":2073},{"$f":"+BY23+1","v":2074},{"$f":"+BZ23+1","v":2075},{"$f":"+CA23+1","v":2076},{"$f":"+CB23+1","v":2077},{"$f":"+CC23+1","v":2078},{"$f":"+CD23+1","v":2079},{"$f":"+CE23+1","v":2080},{"$f":"+CF23+1","v":2081},{"$f":"+CG23+1","v":2082},{"$f":"+CH23+1","v":2083},{"$f":"+CI23+1","v":2084},{"$f":"+CJ23+1","v":2085},{"$f":"+CK23+1","v":2086},{"$f":"+CL23+1","v":2087},{"$f":"+CM23+1","v":2088},{"$f":"+CN23+1","v":2089},{"$f":"+CO23+1","v":2090},{"$f":"+CP23+1","v":2091},{"$f":"+CQ23+1","v":2092},{"$f":"+CR23+1","v":2093},{"$f":"+CS23+1","v":2094},{"$f":"+CT23+1","v":2095},{"$f":"+CU23+1","v":2096},{"$f":"+CV23+1","v":2097},{"$f":"+CW23+1","v":2098},{"$f":"+CX23+1","v":2099},{"$f":"+CY23+1","v":2100}]
["Feedstock Type"]
[{"$f":"'HyARC Physical Property Data'!A73","v":"Residential Natural Gas"},2011,{"$f":"VLOOKUP(ref_year,DeflatorTable,2,FALSE)/VLOOKUP(B25,DeflatorTable,2,FALSE)","v":1.0771767810026385},{"$f":"'HyARC Physical Property Data'!H73","v":"mmBtu"},"Feed Utility",{"$f":"'HyARC Physical Property Data'!$E$6","v":47.141269049911173},{"$f":"'HyARC Physical Property Data'!$I$6","v":52.224661236371581},14.386141835345208,14.386141835345208,14.386141835345208,13.326716630976858,13.627764477872551,11.254339733155913,{"$f":"((N42/(mmBTU_to_GJ))*($C25))*($G25/$F25)","v":12.848820030872972},12.218751960936617,11.836476203703018,11.8517734777777,11.597927407987708,11.487750612568879,12.060887123888937,12.431586993598115,12.891966623565866,13.149168727974281,13.320350247045116,13.528204956004251,13.803266322492309,14.062393594046176,14.234621399609106,14.336189236658935,14.525745808772006,14.629217321677178,14.801367079923402,14.969684601807232,15.121948129980476,15.323390516643737,15.521017633752583,15.763176966206016,16.117258413059144,16.51303296272155,16.993618929872834,17.437235353556446,17.919522525987844,18.161000923881019,18.508607836809013,{"$f":"($BB25-$AR25)/10+AR25","v":18.515839395504365},{"$f":"($BB25-$AR25)/10+AS25","v":18.523070954199717},18.530302512895069,18.537534071590422,18.544765630285774,18.551997188981126,18.559228747676478,18.56646030637183,18.573691865067183,{"$f":"'AEO Data'!$B$30*AM25","v":18.580923423762542},{"$f":"($BQ25-$BB25)/15+BB25","v":18.732326935626944},{"$f":"($BQ25-$BB25)/15+BC25","v":18.883730447491345},19.035133959355747,19.186537471220149,19.33794098308455,19.489344494948952,19.640748006813354,19.792151518677755,19.943555030542157,20.094958542406559,20.246362054270961,20.397765566135362,20.549169077999764,20.700572589864166,{"$f":"'AEO Data'!$C$30*BB25","v":20.851976101728582},{"$f":"($BV25-$BQ25)/5+BQ25","v":20.971163273815758},{"$f":"($BV25-$BQ25)/5+BR25","v":21.090350445902935},{"$f":"($BV25-$BQ25)/5+BS25","v":21.209537617990112},{"$f":"($BV25-$BQ25)/5+BT25","v":21.328724790077288},{"$f":"'AEO Data'!$D$30*BQ25","v":21.447911962164458},{"$f":"+BV25*BW$133/BV$133","v":21.519125336431191},{"$f":"+BW25*BX$133/BW$133","v":21.590575160040096},21.66226221807252,21.734187298216501,21.806351190775437,21.852884379410604,21.899516866531133,21.946248864032874,21.993080584263836,22.040012240025163,22.055250650944551,22.070499597664231,22.085759087468627,22.101029127647202,22.116309725494457,22.121489169854147,22.126669827193954,22.131851697797941,22.137034781950248,22.142219079935074,22.15007638128591,22.157936470848,22.165799349610761,22.173665018563963,22.181533478697713,22.193643072156416,22.205759276621244,22.217882095701352,22.230011533007868,22.242147592153891]
[{"$f":"'HyARC Physical Property Data'!A71","v":"Commercial Natural Gas"},2011,{"$f":"VLOOKUP(ref_year,DeflatorTable,2,FALSE)/VLOOKUP(B26,DeflatorTable,2,FALSE)","v":1.0771767810026385},{"$f":"'HyARC Physical Property Data'!H71","v":"mmBtu"},"Feed Utility",{"$f":"'HyARC Physical Property Data'!$E$6","v":47.141269049911173},{"$f":"'HyARC Physical Property Data'!$I$6","v":52.224661236371581},12.491836786393147,12.491836786393147,12.491836786393147,11.540201846875071,11.906633267965836,9.3536765847618941,{"$f":"((N43/(mmBTU_to_GJ))*($C26))*($G26/$F26)","v":10.629111361129928},9.9955549154729031,9.1313053061952658,9.5723721841997591,9.3150739345461275,9.1670102569081706,9.6835669880973843,9.9819022906517407,10.374954233193641,10.576898837373108,10.709472950445942,10.871133827998989,11.106678367581321,11.324324055865388,11.461664710860044,11.530251335438004,11.690741503240439,11.750101577638928,11.876771241534755,11.995898593723251,12.099846308372394,12.252762493092598,12.390975242017417,12.576341012559455,12.876005381738906,13.213362080405979,13.642549930583472,14.027368446772995,14.457440833206514,14.646759870007866,14.945407361829057,{"$f":"($BB26-$AR26)/10+AR26","v":14.937670833817531},14.929934305806006,14.92219777779448,14.914461249782955,14.906724721771429,14.898988193759903,14.891251665748378,14.883515137736852,14.875778609725327,{"$f":"'AEO Data'!$B$30*AM26","v":14.868042081713805},{"$f":"($BQ26-$BB26)/15+BB26","v":14.989191807934644},15.110341534155483,15.231491260376322,15.35264098659716,15.473790712817999,15.594940439038838,15.716090165259677,15.837239891480516,15.958389617701355,16.079539343922193,16.200689070143032,16.32183879636387,16.442988522584709,16.564138248805548,{"$f":"'AEO Data'!$C$30*BB26","v":16.68528797502638},{"$f":"($BV26-$BQ26)/5+BQ26","v":16.780658901959232},16.876029828892083,16.971400755824934,17.066771682757786,{"$f":"'AEO Data'!$D$30*BQ26","v":17.162142609690644},{"$f":"+BV26*BW$134/BV$134","v":17.219125969517879},{"$f":"+BW26*BX$134/BW$134","v":17.276298530855151},17.333660921907107,17.391213772964214,17.448957716409694,17.486192540053562,17.523506820139147,17.56090072622079,17.598374428214658,17.635928096399496,17.648121534241135,17.660323402596077,17.672533707293155,17.684752454165238,17.696979649049226,17.701124125345881,17.705269572242276,17.709415989965713,17.713563378743547,17.717711738803196,17.723998976765952,17.730288445793402,17.736580146677259,17.742874080209511,17.749170247182427,17.758860074809945,17.768555192417683,17.778255602893598,17.78796130912724,17.797672314009723]
[{"$f":"'HyARC Physical Property Data'!A72","v":"Industrial Natural Gas"},2011,{"$f":"VLOOKUP(ref_year,DeflatorTable,2,FALSE)/VLOOKUP(B27,DeflatorTable,2,FALSE)","v":1.0771767810026385},{"$f":"'HyARC Physical Property Data'!H72","v":"mmBtu"},"Feed Utility",{"$f":"'HyARC Physical Property Data'!$E$6","v":47.141269049911173},{"$f":"'HyARC Physical Property Data'!$I$6","v":52.224661236371581},8.3524006010892204,8.3524006010892204,8.3524006010892204,7.891606632326889,9.2420298006250725,5.091378564817072,{"$f":"((N44/(mmBTU_to_GJ))*($C27))*($G27/$F27)","v":6.2030197526312536},5.530967881908893,4.2526580284486375,4.9022628122135865,4.9487111457393711,5.0024201419600187,5.5040732290196832,5.7324521200318364,6.0189830487143103,6.1643784130172916,6.2544314430514243,6.3802934868874104,6.5919159583386113,6.7988318372561878,6.9111566305652739,6.9577474852780874,7.0760185792238648,7.1203087347746017,7.2355314588866548,7.3367328128841169,7.4218281416265226,7.552074408644514,7.6589686922794975,7.8228205503030184,8.1087248382107671,8.4216617757126304,8.8376765961745321,9.2227722368943912,9.6133017806499446,9.7721812328148197,10.045586638844041,{"$f":"($BB27-$AR27)/10+AR27","v":9.9886567534439159},9.9317268680437891,9.8747969826436623,9.8178670972435356,9.7609372118434088,9.704007326443282,9.6470774410431552,9.5901475556430285,9.5332176702429017,{"$f":"'AEO Data'!$B$30*AM27","v":9.476287784842782},9.5535037131011205,9.6307196413594589,9.7079355696177974,9.7851514978761358,9.8623674261344743,9.9395833543928127,10.016799282651151,10.09401521090949,10.171231139167828,10.248447067426167,10.325662995684505,10.402878923942843,10.480094852201182,10.55731078045952,{"$f":"'AEO Data'!$C$30*BB27","v":10.634526708717866},10.695312274494174,10.756097840270483,10.816883406046792,10.8776689718231,{"$f":"'AEO Data'!$D$30*BQ27","v":10.938454537599405},{"$f":"+BV27*BW$135/BV$135","v":10.974773423011646},{"$f":"+BW27*BX$135/BW$135","v":11.011212897802675},11.047773362364691,11.084455218419302,11.121258869021963,11.144990837396005,11.168773448087572,11.192606809163733,11.216491028922169,11.240426215891658,11.24819781927016,11.255974795916359,11.263757149545318,11.27154488387467,11.279338002624618,11.281979523941867,11.284621663880072,11.28726442258411,11.28990780019889,11.292551796869356,11.296559027678859,11.300567680478631,11.304577755773273,11.308589254067567,11.312602175866472,11.318778079504572,11.324957354761789,11.331140003478794,11.337326027497264,11.343515428659883]
[{"$f":"'HyARC Physical Property Data'!A74","v":"Electric Utility Natural Gas"},2011,1.0771767810026385,{"$f":"'HyARC Physical Property Data'!H74","v":"mmBtu"},"Feed Utility",{"$f":"'HyARC Physical Property Data'!$E$6","v":47.141269049911173},{"$f":"'HyARC Physical Property Data'!$I$6","v":52.224661236371581},7.4079259090132386,7.4079259090132386,7.4079259090132386,7.3706710915002853,9.3158925097981644,4.7837623175056114,{"$f":"((N45/(mmBTU_to_GJ))*($C28))*($G28/$F28)","v":5.9476183921097752},5.4007770397969708,3.7573064138727101,4.2027122702379316,4.2509986746282031,4.3458453934769246,4.8441571504850804,5.0319853704252662,5.3192198560786403,5.4545256252362373,5.5388246451241194,5.6639944431945244,5.884484899616556,6.0953551759139817,6.2414495727057346,6.309346213759178,6.4573499420089364,6.5161274893334484,6.6361077064030667,6.7471554646315317,6.8465029120770557,6.9944896735188342,7.1183428472899974,7.2910592969227492,7.5766389532378176,7.8957257930721285,8.3082759913445337,8.6812923959032329,9.0738262852414806,9.2242743649608752,9.4762823638863765,{"$f":"($BB28-$AR28)/10+AR28","v":9.4171031281586099},9.3579238924308434,9.2987446567030769,9.2395654209753104,9.1803861852475439,9.1212069495197774,9.0620277137920109,9.0028484780642444,8.9436692423364779,{"$f":"'AEO Data'!$B$30*AM28","v":8.8844900066087185},8.9568837707638682,9.029277534919018,9.1016712990741677,9.1740650632293175,9.2464588273844672,9.318852591539617,9.3912463556947667,9.4636401198499165,9.5360338840050662,9.608427648160216,9.6808214123153657,9.7532151764705155,9.8256089406256653,9.898002704780815,{"$f":"'AEO Data'!$C$30*BB28","v":9.9703964689359541},10.027385952998422,10.08437543706089,10.141364921123358,10.198354405185826,{"$f":"'AEO Data'!$D$30*BQ28","v":10.255343889248296},{"$f":"+BV28*BW$136/BV$136","v":10.289394646445894},{"$f":"+BW28*BX$136/BW$136","v":10.323558462169682},10.357835711807217,10.392226771992446,10.426732020609851,10.448981918528062,10.471279296131797,10.493624254739295,10.516016895885006,10.538457321320044,10.545743585110182,10.553034886605404,10.560331229288767,10.567632616645735,10.574939052164185,10.577415609469975,10.579892746763608,10.582370464180912,10.584848761857746,10.587327639930004,10.591084617650559,10.594842928557549,10.598602573124062,10.602363551823357,10.60612586512886,10.611916081234606,10.617709458400572,10.62350599835248,10.629305702816991,10.635108573521714]
[{"$f":"'HyARC Physical Property Data'!A75","v":"Bio Methane"},2007,1.1413971588333081,{"$f":"'HyARC Physical Property Data'!H75","v":"mmBtu"},"Feed Utility",{"$f":"'HyARC Physical Property Data'!$E$6","v":47.141269049911173},{"$f":"'HyARC Physical Property Data'!$I$6","v":52.224661236371581},12.42654028436019,12.42654028436019,12.42654028436019,12.42654028436019,12.42654028436019,12.42654028436019,{"$f":"13.11*($C$29/mmBTU_to_GJ)","v":14.183617774696369},14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,{"$f":"13.11*($C$29/mmBTU_to_GJ)","v":14.183617774696369},14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,{"$f":"+BV29*BW$136/BV$136","v":14.230711556264829},{"$f":"+BW29*BX$136/BW$136","v":14.277961703035571},14.325368734187041,14.372933170621517,14.420655534970821,14.451428179067991,14.482266489779443,14.51317060723302,14.54414067185559,14.575176824373679,14.585254066221541,14.595338275449933,14.605429456876088,14.615527615320566,14.625632755607262,14.629057949594106,14.632483945731124,14.635910744206171,14.639338345207147,14.642766748922,14.647962823919764,14.6531607427764,14.658360506146211,14.663562114683737,14.668765569043746,14.676773707333766,14.68478621751715,14.692803101980653,14.700824363112332,14.708850003301547]
[{"$f":"'HyARC Physical Property Data'!A85","v":"Woody Biomass"},2005,{"$f":"VLOOKUP(ref_year,DeflatorTable,2,FALSE)/VLOOKUP(B30,DeflatorTable,2,FALSE)","v":1.208440716126562},{"$f":"+'HyARC Physical Property Data'!$H$85","v":"kg"},"Feed",{"$f":"'HyARC Physical Property Data'!$E$45","v":19.551069237418005},{"$f":"'HyARC Physical Property Data'!$I$45","v":20.588656379262464},1.3438238843289665,1.3438238843289665,1.3438238843289665,1.3438238843289665,1.3438238843289665,1.3438238843289665,{"$f":"1.27*($C$30)","v":1.5347197094807337},{"$f":"1.27*($C$30)","v":1.5347197094807337},{"$f":"1.28*($C$30)","v":1.5468041166419995},{"$f":"1.32*($C$30)","v":1.595141745287062},{"$f":"1.32*($C$30)","v":1.595141745287062},{"$f":"1.34*($C$30)","v":1.6193105596095931},{"$f":"1.34*($C$30)","v":1.6193105596095931},{"$f":"1.36*($C$30)","v":1.6434793739321245},{"$f":"1.36*($C$30)","v":1.6434793739321245},{"$f":"1.38*($C$30)","v":1.6676481882546554},{"$f":"1.4*($C$30)","v":1.6918170025771868},{"$f":"1.46*($C$30)","v":1.7643234455447805},{"$f":"1.48*($C$30)","v":1.7884922598673119},{"$f":"1.48*($C$30)","v":1.7884922598673119},{"$f":"1.51*($C$30)","v":1.8247454813511086},{"$f":"1.52*($C$30)","v":1.8368298885123742},{"$f":"1.62*($C$30)","v":1.9576739601250306},{"$f":"1.72*($C$30)","v":2.0785180317376866},{"$f":"1.82*($C$30)","v":2.1993621033503428},{"$f":"1.91*($C$30)","v":2.3081217678017332},{"$f":"2.01*($C$30)","v":2.4289658394143894},{"$f":"2.11*($C$30)","v":2.5498099110270456},{"$f":"2.2*($C$30)","v":2.6585695754784364},{"$f":"2.3*($C$30)","v":2.7794136470910926},{"$f":"2.4*($C$30)","v":2.9002577187037488},{"$f":"2.5*($C$30)","v":3.021101790316405},{"$f":"2.57*($C$30)","v":3.1056926404452643},{"$f":"2.64*($C$30)","v":3.190283490574124},{"$f":"2.71*($C$30)","v":3.2748743407029832},{"$f":"2.78*($C$30)","v":3.359465190831842},{"$f":"2.85*($C$30)","v":3.4440560409607017},{"$f":"2.92*($C$30)","v":3.528646891089561},{"$f":"2.99*($C$30)","v":3.6132377412184207},{"$f":"3.07*($C$30)","v":3.7099129985085453},{"$f":"3.14*($C$30)","v":3.794503848637405},{"$f":"3.21*($C$30)","v":3.8790946987662642},{"$f":"3.28*($C$30)","v":3.963685548895123},{"$f":"3.35*($C$30)","v":4.0482763990239832},{"$f":"3.42*($C$30)","v":4.1328672491528424},{"$f":"3.49*($C$30)","v":4.2174580992817017},{"$f":"3.56*($C$30)","v":4.3020489494105609},{"$f":"3.64*($C$30)","v":4.3987242067006855},{"$f":"3.71*($C$30)","v":4.4833150568295448},{"$f":"3.78*($C$30)","v":4.567905906958404},{"$f":"3.85*($C$30)","v":4.6524967570872642},{"$f":"3.92*($C$30)","v":4.7370876072161234},{"$f":"3.99*($C$30)","v":4.8216784573449827},{"$f":"4.06*($C$30)","v":4.906269307473841},{"$f":"4.14*($C$30)","v":5.0029445647639665},{"$f":"4.21*($C$30)","v":5.0875354148928258},{"$f":"4.28*($C$30)","v":5.1721262650216859},{"$f":"4.35*($C$30)","v":5.2567171151505443},{"$f":"4.42*($C$30)","v":5.3413079652794044},{"$f":"4.49*($C$30)","v":5.4258988154082637},{"$f":"4.56*($C$30)","v":5.5104896655371221},{"$f":"4.63*($C$30)","v":5.5950805156659822},{"$f":"4.71*($C$30)","v":5.6917557729561068},{"$f":"4.78*($C$30)","v":5.7763466230849669},{"$f":"4.85*($C$30)","v":5.8609374732138253},{"$f":"4.92*($C$30)","v":5.9455283233426854},{"$f":"4.99*($C$30)","v":6.0301191734715447},{"$f":"+BV30*BW$138/BV$138","v":6.0446132076616896},{"$f":"+BW30*BX$138/BW$138","v":6.0591420798079438},6.0737058736470511,6.0883046731170198,6.1029385623576156,6.1157485681116217,6.1285854619369617,6.1414493002714252,6.1543401396712598,6.167258036811428,6.183149548139812,6.1990820079952069,6.215055521891923,6.2310701956161552,6.2471261352266838,6.2604975997429575,6.2738976847896071,6.2873264516265444,6.3007839616448056,6.3142702763668277,6.326614172551615,6.3389822000716718,6.3513744061018391,6.3637908379091801,6.376231542853164,6.3909193633613004,6.4056410176582252,6.4203965836809767,6.4351861395461265,6.450009763550189]
[{"$f":"'HyARC Physical Property Data'!$A$87","v":"Woody Biomass MYPP"},2007,{"$f":"VLOOKUP(ref_year,DeflatorTable,2,FALSE)/VLOOKUP(B31,DeflatorTable,2,FALSE)","v":1.1413971588333081},{"$f":"+'HyARC Physical Property Data'!$H$87","v":"kg"},"Feed",18.608000000000001,null,4.4443250214961303,4.4443250214961303,4.4443250214961303,4.4443250214961303,4.4443250214961303,4.4443250214961303,{"$f":"4.44432502149613*$C$31","v":5.0727399524674635},{"$f":"N31-($N$31-$U$31)/7","v":4.9524277749801975},4.8321155974929315,4.7118034200056655,4.5914912425183996,4.4711790650311336,4.3508668875438676,{"$f":"3.70647033533964*$C$31","v":4.2305547100566034},{"$f":"3.70647033533964*$C$31","v":4.2305547100566034},4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,4.2305547100566034,{"$f":"+BV31*BW$138/BV$138","v":4.2407232992414734},{"$f":"+BW31*BX$138/BW$138","v":4.2509163297143298},4.2611338602224134,4.2713759496541703,4.2816426570395922,4.2906297812770164,4.2996357693964899,4.3086606609931088,4.3177044957450779,4.3267673134138871,4.3379163315619822,4.3490940779953462,4.3603006267397229,4.3715360520116029,4.3828004282187161,4.3921814554525627,4.4015825620108968,4.4110037908718764,4.4204451851056508,4.4299067878745575,4.4385669033121991,4.4472439485867392,4.4559379567946618,4.4646489610971525,4.4733769947202253,4.4836815387008029,4.494009819475032,4.5043618917212536,4.5147378102437621,4.525137629973095]
[{"$f":"'HyARC Physical Property Data'!A79","v":"Electric Utility Steam Coal"},2011,{"$f":"VLOOKUP(ref_year,DeflatorTable,2,FALSE)/VLOOKUP(B32,DeflatorTable,2,FALSE)","v":1.0771767810026385},{"$f":"+'HyARC Physical Property Data'!$H$79","v":"kg"},"Feed",{"$f":"'HyARC Physical Property Data'!E42","v":22.7322030001394},{"$f":"'HyARC Physical Property Data'!I42","v":23.967615189707661},1.7344499599167666,1.7344499599167666,1.7344499599167666,1.7788973636542149,1.9298772179141501,1.9810774561110811,{"$f":"N50*($C32/mmBTU_to_GJ*$G32/$F32)","v":2.4738067312648084},2.562092342657099,2.5893000409210973,2.5157066296517416,2.5782561311129801,2.5794316793643168,2.6463884102586808,2.6614358584795466,2.6700253268837741,2.6738598533226581,2.7085589804154591,2.7412837892912716,2.7897299412646319,2.829150638531758,2.8628658360442274,2.8975789577590683,2.9373430615208616,2.9731875946021442,3.0056045217930829,3.0446516703026871,3.0864493002977911,3.1186476960830318,3.1475444375762862,3.18024986928312,3.2161686815121526,3.2620441290677542,3.3016661335903748,3.3385419626650465,3.3748515478018035,3.4125282998609028,3.4464921710419247,{"$f":"($BB32-$AR32)/10+AR32","v":3.4437798221078069},3.441067473173689,3.4383551242395711,3.4356427753054533,3.4329304263713354,3.4302180774372175,3.4275057285030996,3.4247933795689818,3.4220810306348639,{"$f":"('AEO Data'!$B$28*AM32)","v":3.4193686817007474},{"$f":"(($BQ$32-$BB$32)/15+BB32)","v":3.4313687390140855},{"$f":"(($BQ$32-$BB$32)/15+BC32)","v":3.4433687963274235},3.4553688536407616,3.4673689109540997,3.4793689682674378,3.4913690255807759,3.503369082894114,3.5153691402074521,3.5273691975207901,3.5393692548341282,3.5513693121474663,3.5633693694608044,3.5753694267741425,3.5873694840874806,{"$f":"('AEO Data'!$C$28*BB32)","v":3.5993695414008169},{"$f":"(($BV$32-$BQ$32)/5+BQ32)","v":3.6109087635521795},{"$f":"(($BV$32-$BQ$32)/5+BR32)","v":3.6224479857035421},{"$f":"(($BV$32-$BQ$32)/5+BS32)","v":3.6339872078549047},{"$f":"(($BV$32-$BQ$32)/5+BT32)","v":3.6455264300062673},{"$f":"('AEO Data'!$D$28*BQ32)","v":3.657065652157629},{"$f":"+BV32*BW$139/BV$139","v":3.6694300274580169},{"$f":"+BW32*BX$139/BW$139","v":3.6818362061579366},3.6942843295928096,3.7067745395759086,3.7193069783999695,3.7299559382094629,3.7406353876627754,3.7513454140565434,3.7620861049373482,3.7728575481024307,3.7810815561772397,3.7893234907992221,3.7975833910443488,3.8058612960737661,3.8141572451339845,3.8197812068711383,3.8254134611205277,3.8310540201094327,3.8367028960831631,3.8423601013050841,3.8442546108659763,3.8461500545315284,3.8480464327623092,3.8499437460191142,3.8518419947629661,3.8491138019441373,3.8463875414569224,3.8436632119326841,3.8409408120037543,3.8382203403034345]
[{"$f":"'HyARC Physical Property Data'!A76","v":"Commercial Electricity"},2011,1.0771767810026385,{"$f":"'HyARC Physical Property Data'!$H$76","v":"kWh"},"Feed Utility Byprod",null,null,26.896922396257633,26.896922396257633,26.896922396257633,26.568469730033652,27.542479456318485,26.167555894896875,{"$f":"(N51/(mmBTU_to_GJ))*($C33)","v":31.133552693543749},30.610864657554803,29.061789491552979,28.354246688716874,28.429556150508322,28.316980456176768,28.823692582125577,29.117226828521051,29.247133327289326,29.177516055596545,29.167046509897588,29.278527670097162,29.26715860520952,29.230231351523717,29.234638076629693,29.084632786454755,28.975210003876501,28.966039196438619,29.081694289036999,29.178046986332202,29.254591883104705,29.386069732646401,29.520327821405793,29.693042652777955,29.886409668746637,30.281916310070152,30.734461248733886,31.144263200115045,31.594533304780605,32.138219651364906,32.414492522727556,{"$f":"($BB33-$AR33)/10+AR33","v":32.12574672681761},31.837000930907664,31.548255134997717,31.259509339087771,30.970763543177824,30.682017747267878,30.393271951357931,30.104526155447985,29.815780359538039,{"$f":"'AEO Data'!$B$33*AM33","v":29.527034563628085},{"$f":"($BQ33-$BB33)/15+BB33","v":29.544237717052788},29.56144087047749,29.578644023902193,29.595847177326895,29.613050330751598,29.630253484176301,29.647456637601003,29.664659791025706,29.681862944450408,29.699066097875111,29.716269251299813,29.733472404724516,29.750675558149219,29.767878711573921,{"$f":"'AEO Data'!$C$33*BB33","v":29.78508186499861},{"$f":"($BV33-$BQ33)/5+BQ33","v":29.765026073611775},29.744970282224941,29.724914490838106,29.704858699451272,{"$f":"'AEO Data'!$D$33*BQ33","v":29.684802908064434},{"$f":"+BV33*BW$140/BV$140","v":29.671732577415259},{"$f":"+BW33*BX$140/BW$140","v":29.658668001681953},29.645609178330599,29.632556104828407,29.619508778643699,29.595784014667533,29.572078253856809,29.54839148099029,29.524723680858934,29.501074838265872,29.468497232300709,29.435955601309892,29.403449905566777,29.3709801053886,29.33854616113641,29.303185235347783,29.267866929089987,29.232591190994896,29.1973579697563,29.16216721412983,29.121407129980525,29.080704016372799,29.040057793678688,28.999468382381522,28.95893570307577,28.919368591982021,28.879855542138877,28.840396479681488,28.800991330845925,28.761640021969036]
[{"$f":"'HyARC Physical Property Data'!A77","v":"Industrial Electricity"},2011,1.0771767810026385,{"$f":"'HyARC Physical Property Data'!$H$77","v":"kWh"},"Feed Utility Byprod",null,null,17.44160584363896,17.44160584363896,17.44160584363896,17.651840860809763,19.274322003549859,18.160650967421709,{"$f":"(N52/(mmBTU_to_GJ))*($C34)","v":20.686330589978613},20.395642949142793,18.823552956770747,18.524341835586291,18.425452923007665,18.26043454526129,18.754222591879351,19.028024593279895,19.177936970576098,19.120789424026807,19.113803600770296,19.250773520364145,19.360178945591421,19.49113403256262,19.561495628305966,19.585178202178344,19.679504173492226,19.769484680938866,19.876209926971701,20.022596719978992,20.141018778526679,20.284500767797521,20.450430916980327,20.629529169428153,20.858104040315624,21.232143722567496,21.710953396316075,22.126345435731348,22.531327148645097,22.961372876364592,23.222533621153197,{"$f":"($BB34-$AR34)/10+AR34","v":22.97056615223179},22.718598683310383,22.466631214388975,22.214663745467568,21.962696276546161,21.710728807624754,21.458761338703347,21.20679386978194,20.954826400860533,{"$f":"'AEO Data'!$B$33*AM34","v":20.702858931939144},{"$f":"($BQ34-$BB34)/15+BB34","v":20.714920910522487},20.72698288910583,20.739044867689174,20.751106846272517,20.76316882485586,20.775230803439204,20.787292782022547,20.79935476060589,20.811416739189234,20.823478717772577,20.83554069635592,20.847602674939264,20.859664653522607,20.87172663210595,{"$f":"'AEO Data'!$C$33*BB34","v":20.883788610689287},20.869726507061667,20.855664403434048,20.841602299806429,20.827540196178809,{"$f":"'AEO Data'!$D$33*BQ34","v":20.813478092551186},{"$f":"+BV34*BW$141/BV$141","v":20.819767085860629},{"$f":"+BW34*BX$141/BW$141","v":20.826057979450106},20.832350773893804,20.838645469766085,20.844942067641483,20.842584664877659,20.840227528717975,20.837870659132275,20.83551405609041,20.833157719562244,20.823707614808125,20.814261796705171,20.804820263308923,20.795383012675799,20.785950042863099,20.77437772649537,20.762811852869294,20.751252418397954,20.739699419496432,20.728152852581804,20.712333481367292,20.696526183225924,20.680730948943744,20.664947769313819,20.649176635136243,20.634348778597502,20.619531569714763,20.604725000842109,20.58992906433911,20.575143752570824]
[{"$f":"'HyARC Physical Property Data'!A78","v":"Residential Electricity"},2011,1.0771767810026385,{"$f":"'HyARC Physical Property Data'!$H$78","v":"kWh"},"Feed Utility Byprod",null,null,29.579885763014694,29.579885763014694,29.579885763014694,29.556357578078675,30.116416605727963,29.134443020933652,{"$f":"(N53/(mmBTU_to_GJ))*($C35)","v":35.248515023946787},35.057638277332465,33.966003843989547,33.233617566807133,33.701326704097838,33.757355212019654,34.284141624879645,34.53730982005527,34.545858825920035,34.349778958096259,34.322062331653513,34.366342976028214,34.399461822706293,34.411956052345289,34.551308013105078,34.673225025322317,34.843428145906536,34.985992237617076,35.137048158036244,35.236409803173729,35.28809897335217,35.415531539096392,35.539081163325783,35.65784015868649,35.819984363315783,36.165866338206058,36.58927134764722,36.936418367117263,37.270112418562192,37.681875750603361,37.878431414047952,{"$f":"($BB35-$AR35)/10+AR35","v":37.617018946505915},37.355606478963878,37.094194011421841,36.832781543879804,36.571369076337767,36.30995660879573,36.048544141253693,35.787131673711656,35.525719206169619,{"$f":"'AEO Data'!$B$33*AM35","v":35.264306738627596},{"$f":"($BQ35-$BB35)/15+BB35","v":35.284852563435471},35.305398388243347,35.325944213051223,35.346490037859098,35.367035862666974,35.387581687474849,35.408127512282725,35.428673337090601,35.449219161898476,35.469764986706352,35.490310811514227,35.510856636322103,35.531402461129979,35.551948285937854,{"$f":"'AEO Data'!$C$33*BB35","v":35.572494110745708},35.548541364057677,35.524588617369645,35.500635870681613,35.476683123993581,{"$f":"'AEO Data'!$D$33*BQ35","v":35.452730377305556},{"$f":"+BV35*BW$142/BV$142","v":35.437120406443277},{"$f":"+BW35*BX$142/BW$142","v":35.42151730871003},35.405921081079541,35.390331720526888,35.37474922402847,35.346414602332743,35.318102676226502,35.289813427530937,35.261546838081799,35.23330288972938,35.194395268068625,35.155530611526075,35.11670887265597,35.077930004064953,35.039193958412007,34.996962201921704,34.954781346181527,34.912651329842227,34.870572091628503,34.828543570338908,34.779863568050295,34.731251606006261,34.682707589106663,34.634231422384289,34.585823011004663,34.538567783278886,34.491377121214782,34.444250936595139,34.397189141323274,34.350191647422875]
[]
[]
[]
["AEO 2013 Reference Case Values:"]
["2011 $/MMBtu"]
[]
["Residential Natural Gas",null,null,null,null,null,null,null,null,null,null,null,null,11.359373,10.802343,10.464380999999999,10.477905,10.253485,10.156079999999999,10.662777999999999,10.990506,11.397518,11.624905,11.776242999999999,11.960003,12.203179,12.432268000000001,12.584531,12.674325,12.841908,12.933384999999999,13.085578999999999,13.234385,13.368997999999999,13.547089,13.721807,13.935895,14.248931000000001,14.598827,15.023702999999999,15.415895000000001,15.842275000000001,16.055761,16.363073]
["Commercial Natural Gas",null,null,null,null,null,null,null,null,null,null,null,null,9.3969749999999994,8.8368610000000007,8.0727960000000003,8.4627339999999993,8.2352620000000005,8.1043620000000001,8.5610389999999992,8.8247909999999994,9.1722800000000007,9.3508150000000008,9.4680210000000002,9.6109419999999997,9.8191819999999996,10.011597999999999,10.133018,10.193654,10.33554,10.388019,10.500005,10.605323,10.697221000000001,10.832411,10.954602,11.11848,11.383407,11.681657,12.061093,12.401303,12.781521,12.948893999999999,13.212922000000001]
["Industrial Natural Gas",null,null,null,null,null,null,null,null,null,null,null,null,5.4839599999999997,4.8898130000000002,3.7596859999999999,4.3339879999999997,4.3750520000000002,4.4225349999999999,4.8660360000000003,5.0679410000000003,5.3212570000000001,5.4497980000000004,5.5294119999999998,5.6406840000000003,5.8277749999999999,6.0107049999999997,6.1100089999999998,6.1511990000000001,6.2557600000000004,6.2949159999999997,6.396782,6.4862520000000004,6.561483,6.6766310000000004,6.771134,6.9159920000000001,7.1687539999999998,7.4454149999999997,7.813205,8.1536600000000004,8.4989190000000008,8.6393810000000002,8.8810929999999999]
[{"$f":"'HyARC Physical Property Data'!$A$74","v":"Electric Utility Natural Gas"},null,null,null,null,null,null,null,null,null,null,null,null,5.258165,4.7747140000000003,3.3217560000000002,3.7155300000000002,3.758219,3.8420709999999998,4.2826180000000003,4.4486730000000003,4.7026110000000001,4.8222319999999996,4.8967590000000003,5.0074189999999996,5.20235,5.388776,5.5179349999999996,5.5779610000000002,5.7088080000000003,5.7607720000000002,5.8668440000000004,5.9650189999999998,6.0528500000000003,6.1836820000000001,6.2931780000000002,6.4458729999999997,6.6983480000000002,6.9804459999999997,7.345173,7.6749489999999998,8.0219799999999992,8.1549879999999995,8.3777830000000009]
[{"$f":"'HyARC Physical Property Data'!$A$85","v":"Woody Biomass"}]
["Pyrolysis Oil",null,null,null,null,null,null,null,null,null,null,null,null,13.6,13.6,13.6,13.6,13.6,13.6,13.6,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11,14.11]
["Methanol",null,null,null,null,null,null,null,null,null,null,null,null,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6,23.6]
["Ethanol (E85)",null,null,null,null,null,null,null,null,null,null,null,null,25.561684,25.303816000000001,33.642014000000003,31.120284999999999,24.805427999999999,24.941547,24.510408000000002,24.773121,25.840997999999999,26.808551999999999,29.644617,29.383793000000001,28.224442,28.253482999999999,27.145426,27.272445999999999,27.519344,26.363682000000001,26.241467,26.599018000000001,26.941008,27.294556,27.667862,28.194492,28.632065000000001,29.186733,29.790071000000001,30.397635000000001,30.990224999999999,31.671036000000001,30.576360999999999]
["Electric Utility Steam Coal",null,null,null,null,null,null,null,null,null,null,null,null,2.2979889999999998,2.38,2.4052739999999999,2.3369110000000002,2.3950149999999999,2.3961070000000002,2.4583050000000002,2.472283,2.4802620000000002,2.4838239999999998,2.516057,2.5464560000000001,2.591459,2.6280779999999999,2.6593969999999998,2.691643,2.7285810000000001,2.7618779999999998,2.7919909999999999,2.8282630000000002,2.8670900000000001,2.8969999999999998,2.9238430000000002,2.954224,2.98759,3.030205,3.0670109999999999,3.1012659999999999,3.134995,3.169994,3.2015440000000002]
["Commercial Electricity",null,null,null,null,null,null,null,null,null,null,null,null,30.492578999999999,29.980651999999999,28.463469,27.770492999999998,27.844252000000001,27.733993999999999,28.230274000000001,28.517765000000001,28.644997,28.576813000000001,28.566559000000002,28.675744999999999,28.66461,28.628443000000001,28.632759,28.485842000000002,28.378672000000002,28.369689999999999,28.482963999999999,28.577332999999999,28.652301999999999,28.781072999999999,28.912566999999999,29.081726,29.271111999999999,29.658476,30.101704000000002,30.503069,30.944068999999999,31.476562000000001,31.747146999999998]
["Industrial Electricity",null,null,null,null,null,null,null,null,null,null,null,null,20.260442999999999,19.975739999999998,18.436015999999999,18.142965,18.046112000000001,17.884491000000001,18.368113000000001,18.636278000000001,18.783104000000002,18.727132999999998,18.720291,18.854441000000001,18.961594000000002,19.089853000000002,19.158766,19.181961000000001,19.274345,19.362473000000001,19.467001,19.610374,19.726358000000001,19.866886000000001,20.029399999999999,20.204810999999999,20.42868,20.795019,21.263971000000002,21.670811,22.067454999999999,22.488647,22.744430999999999]
["Residential Electricity",null,null,null,null,null,null,null,null,null,null,null,null,34.522823000000002,34.335875999999999,33.266716000000002,32.549408,33.007488000000002,33.062362999999998,33.578304000000003,33.826259999999998,33.834632999999997,33.642589999999998,33.615443999999997,33.658813000000002,33.691249999999997,33.703487000000003,33.839970000000001,33.959377000000003,34.126075999999998,34.265704999999997,34.413651000000002,34.510967000000001,34.561591999999997,34.686400999999996,34.807406999999998,34.923721,35.082526999999999,35.421287999999997,35.835976000000002,36.175975999999999,36.502800000000001,36.906086000000002,37.098595000000003]
[]
[]
["AEO_2013_High_Price_Case",{"$f":"\"Prices are in $(\" & ref_year&\")/GJ LHV\"","v":"Prices are in $(2016)/GJ LHV"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Except as noted,values are extrapolated based on PNNL mini-CAM model (see AEO Data tab)"]
["Year","Source Data Year","Reference year Conversion","Display Units","Use Category","LHV (MJ/kg)","HHV (MJ/kg)",2004,2005,2006,2007,2008,2009,2010,2011,2012,2013,2014,2015,2016,2017,2018,2019,2020,2021,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,2033,2034,2035,2036,2037,2038,2039,2040,2041,2042,2043,2044,2045,2046,2047,2048,2049,2050,2051,2052,2053,2054,2055,2056,2057,2058,2059,2060,2061,2062,2063,2064,2065,2066,2067,2068,2069,2070,{"$f":"+BV57+1","v":2071},{"$f":"+BW57+1","v":2072},{"$f":"+BX57+1","v":2073},{"$f":"+BY57+1","v":2074},{"$f":"+BZ57+1","v":2075},{"$f":"+CA57+1","v":2076},{"$f":"+CB57+1","v":2077},{"$f":"+CC57+1","v":2078},{"$f":"+CD57+1","v":2079},{"$f":"+CE57+1","v":2080},{"$f":"+CF57+1","v":2081},{"$f":"+CG57+1","v":2082},{"$f":"+CH57+1","v":2083},{"$f":"+CI57+1","v":2084},{"$f":"+CJ57+1","v":2085},{"$f":"+CK57+1","v":2086},{"$f":"+CL57+1","v":2087},{"$f":"+CM57+1","v":2088},{"$f":"+CN57+1","v":2089},{"$f":"+CO57+1","v":2090},{"$f":"+CP57+1","v":2091},{"$f":"+CQ57+1","v":2092},{"$f":"+CR57+1","v":2093},{"$f":"+CS57+1","v":2094},{"$f":"+CT57+1","v":2095},{"$f":"+CU57+1","v":2096},{"$f":"+CV57+1","v":2097},{"$f":"+CW57+1","v":2098},{"$f":"+CX57+1","v":2099},{"$f":"+CY57+1","v":2100}]
["Feedstock Type"]
[{"$f":"'HyARC Physical Property Data'!A73","v":"Residential Natural Gas"},2011,{"$f":"VLOOKUP(ref_year,DeflatorTable,2,FALSE)/VLOOKUP(B59,DeflatorTable,2,FALSE)","v":1.0771767810026385},{"$f":"'HyARC Physical Property Data'!H73","v":"mmBtu"},"Feed Utility",{"$f":"'HyARC Physical Property Data'!$E$6","v":47.141269049911173},{"$f":"'HyARC Physical Property Data'!$I$6","v":52.224661236371581},13.568796522291001,13.568796522291001,13.568796522291001,12.569562315288914,12.891154499364562,11.574514296329017,{"$f":"N74*(1/mmBTU_to_GJ*$C59*$G59/$F59)","v":12.848820030872973},12.218751960936617,11.847089507654712,11.878954304161503,11.689024462272872,11.571127769223187,12.158272077211455,12.546766735129951,13.025386814796633,13.318825496567992,13.569389054574135,13.810438757785679,14.116363879109715,14.398431406172943,14.538561404399491,14.725122769343848,14.945168695396804,15.119136164337942,15.386893885550919,15.591935497746983,15.825560525786523,16.097797484306195,16.489221744402556,16.917726397778729,17.360396073577061,17.767820033598468,18.289975811421051,18.631226958079775,19.172403658768356,19.659398554853915,19.991300990315715,{"$f":"($BB59-$AR59)/10+AR59","v":19.99145536068955},{"$f":"($BB59-$AR59)/10+AS59","v":19.991609731063384},19.991764101437219,19.991918471811054,19.992072842184889,19.992227212558724,19.992381582932559,19.992535953306394,19.992690323680229,{"$f":"'AEO Data'!$B$30*AM59","v":19.992844694054046},{"$f":"($BQ59-$BB59)/15+BB59","v":20.155753007586423},{"$f":"($BQ59-$BB59)/15+BC59","v":20.3186613211188},20.481569634651176,20.644477948183553,20.80738626171593,20.970294575248307,21.133202888780684,21.29611120231306,21.459019515845437,21.621927829377814,21.784836142910191,21.947744456442567,22.110652769974944,22.273561083507321,{"$f":"'AEO Data'!$C$30*BB59","v":22.43646939703968},{"$f":"($BV59-$BQ59)/5+BQ59","v":22.564713325864819},{"$f":"($BV59-$BQ59)/5+BR59","v":22.692957254689958},22.821201183515097,22.949445112340236,{"$f":"'AEO Data'!$D$30*BQ59","v":23.077689041165382},{"$f":"+BV59*BW$133/BV$133","v":23.154313754554682},{"$f":"+BW59*BX$133/BW$133","v":23.231192884523196},23.308327275808772,23.385717775954042,23.463365235315731,23.513434373015976,23.563610354663151,23.613893408254576,23.664283762274096,23.714781645693119,23.731177988110947,23.747585666920095,23.764004689958508,23.780435065069565,23.796876800102055,23.802449818424297,23.808024141898198,23.813599770829413,23.819176705523667,23.82475494628676,23.833209305741288,23.841666665276783,23.850127025957839,23.858590388849432,23.867056755016911,23.880086528392884,23.893123415130006,23.906167419111679,23.919218544223433,23.932276794352919]
[{"$f":"'HyARC Physical Property Data'!A71","v":"Commercial Natural Gas"},2011,{"$f":"VLOOKUP(ref_year,DeflatorTable,2,FALSE)/VLOOKUP(B60,DeflatorTable,2,FALSE)","v":1.0771767810026385},{"$f":"'HyARC Physical Property Data'!H71","v":"mmBtu"},"Feed Utility",{"$f":"'HyARC Physical Property Data'!$E$6","v":47.141269049911173},{"$f":"'HyARC Physical Property Data'!$I$6","v":52.224661236371581},11.78211597551449,11.78211597551449,11.78211597551449,10.884547954455588,11.412186165255939,10.075756967258858,{"$f":"N75*(1/mmBTU_to_GJ*$C60*$G60/$F60)","v":10.629111361129928},9.9955492598702431,9.1410917610380729,9.5969684001679578,9.4058916020598868,9.2495164507528447,9.7764218036892636,10.090174279094695,10.498071047498478,10.736649252347618,10.944404422699936,11.141369834297564,11.405591672727528,11.642166663114509,11.748018053618996,11.902757604636774,12.090527006309296,12.220015422570853,12.435619438294673,12.592485495912598,12.770738780549461,12.989189826652307,13.318649041764999,13.691788738461685,14.075018030303756,14.417815418729715,14.885419515535311,15.176266800167872,15.67029726596243,16.106982183025981,16.379635393901427,{"$f":"($BB60-$AR60)/10+AR60","v":16.364004498297199},16.348373602692966,16.332742707088734,16.317111811484502,16.301480915880269,16.285850020276037,16.270219124671804,16.254588229067572,16.23895733346334,{"$f":"'AEO Data'!$B$30*AM60","v":16.223326437859122},{"$f":"($BQ60-$BB60)/15+BB60","v":16.355519469432206},16.487712501005291,16.619905532578375,16.75209856415146,16.884291595724545,17.016484627297629,17.148677658870714,17.280870690443798,17.413063722016883,17.545256753589968,17.677449785163052,17.809642816736137,17.941835848309221,18.074028879882306,{"$f":"'AEO Data'!$C$30*BB60","v":18.206221911455369},{"$f":"($BV60-$BQ60)/5+BQ60","v":18.310286298131796},18.414350684808223,18.51841507148465,18.622479458161077,{"$f":"'AEO Data'!$D$30*BQ60","v":18.726543844837511},{"$f":"+BV60*BW$134/BV$134","v":18.788721476762582},{"$f":"+BW60*BX$134/BW$134","v":18.851105556708379},18.913696770143034,18.976495804810636,19.039503350738787,19.080132284630061,19.120847917750758,19.161650435110815,19.20254002211496,19.243516864563571,19.25682178537409,19.270135905174534,19.283459230325061,19.296791767190232,19.310133522139004,19.314655784821952,19.319179106578872,19.323703487657788,19.328228928306782,19.332755428773996,19.339615774830435,19.34647855532247,19.353343771113977,19.360211423069138,19.36708151205244,19.37765460808377,19.388233476299188,19.398818119849906,19.409408541888862,19.420004745570715]
[{"$f":"'HyARC Physical Property Data'!A72","v":"Industrial Natural Gas"},2011,1.0771767810026385,{"$f":"'HyARC Physical Property Data'!H72","v":"mmBtu"},"Feed Utility",{"$f":"'HyARC Physical Property Data'!$E$6","v":47.141269049911173},{"$f":"'HyARC Physical Property Data'!$I$6","v":52.224661236371581},7.8800725307970341,7.8800725307970341,7.8800725307970341,7.4431315976064605,8.8750360136942668,6.5580125743803235,{"$f":"N76*(1/mmBTU_to_GJ*$C61*$G61/$F61)","v":6.2030163592696592},5.5300347074699987,4.260790785073671,4.9204025921851677,4.9951990684837728,5.0372880634792523,5.5611676689925886,5.805087024993802,6.0936211681384362,6.2815263042747977,6.446729851334049,6.6107547707989633,6.8493465490944869,7.0700971632388772,7.1542932511583484,7.2893513049194398,7.4302708252773213,7.5360419062240371,7.7520157983618185,7.8975966664320465,8.0540057513550476,8.2613853896907425,8.5847569141002449,8.9483974605692502,9.3215688286408334,9.648490940400265,10.068364012996796,10.306145908991411,10.735979628992679,11.099317035159109,11.325040055162141,{"$f":"($BB61-$AR61)/10+AR61","v":11.278211053887526},11.231382052612911,11.184553051338296,11.137724050063682,11.090895048789067,11.044066047514452,10.997237046239837,10.950408044965222,10.903579043690607,{"$f":"'AEO Data'!$B$30*AM61","v":10.856750042415998},{"$f":"($BQ61-$BB61)/15+BB61","v":10.945214433897943},11.033678825379889,11.122143216861835,11.21060760834378,11.299071999825726,11.387536391307671,11.476000782789617,11.564465174271563,11.652929565753508,11.741393957235454,11.8298583487174,11.918322740199345,12.006787131681291,12.095251523163236,{"$f":"'AEO Data'!$C$30*BB61","v":12.183715914645184},{"$f":"($BV61-$BQ61)/5+BQ61","v":12.253356443595324},12.322996972545464,12.392637501495605,12.462278030445745,{"$f":"'AEO Data'!$D$30*BQ61","v":12.531918559395887},{"$f":"+BV61*BW$135/BV$135","v":12.573528213903272},{"$f":"+BW61*BX$135/BW$135","v":12.61527602469854},12.657162450501191,12.699187951553807,12.741352989627112,12.768542122597896,12.795789275227369,12.823094571325321,12.85045813496574,12.87788009048738,12.886783825496796,12.895693716526967,12.904609767834151,12.913531983677547,12.922460368319303,12.925486694379064,12.928513729177656,12.931541472881056,12.934569925655282,12.937599087666396,12.942190073530147,12.946782688533204,12.951376933253679,12.955972808269884,12.960570314160341,12.967645895190305,12.974725339001436,12.981808647702545,12.988895823403597,12.995986868215709]
[{"$f":"'HyARC Physical Property Data'!A74","v":"Electric Utility Natural Gas"},2011,1.0771767810026385,{"$f":"'HyARC Physical Property Data'!H74","v":"mmBtu"},"Feed Utility",{"$f":"'HyARC Physical Property Data'!$E$6","v":47.141269049911173},{"$f":"'HyARC Physical Property Data'!$I$6","v":52.224661236371581},6.9870463159656619,6.9870463159656619,6.9870463159656619,6.9519071777354364,9.0904707383294223,6.2626950486669273,{"$f":"N77*(1/mmBTU_to_GJ*$C62*$G62/$F62)","v":5.9476195232303075},5.4007770397969699,3.7643838350413934,4.2147881130374945,4.337012473242587,4.4297507834196734,4.9169062986207761,5.1166395621601932,5.3977920127130385,5.5768800643025109,5.731085726429189,5.8852472748551197,6.1240381303642737,6.3478846214047309,6.46780941356828,6.6168153146093855,6.7826918783851724,6.9152648603374747,7.1044436381928611,7.2503909893154548,7.4075070245709522,7.6133030941618562,7.9366802741740186,8.2829207934993665,8.6352320367199251,8.9389684398145519,9.3489317654302884,9.5889623290425074,10.016230667677213,10.374123990723158,10.560031568000021,{"$f":"($BB62-$AR62)/10+AR62","v":10.509865972613389},10.459700377226756,10.409534781840124,10.359369186453492,10.30920359106686,10.259037995680227,10.208872400293595,10.158706804906963,10.108541209520331,{"$f":"'AEO Data'!$B$30*AM62","v":10.058375614133693},{"$f":"($BQ62-$BB62)/15+BB62","v":10.140334586618534},10.222293559103376,10.304252531588217,10.386211504073058,10.4681704765579,10.550129449042741,10.632088421527582,10.714047394012423,10.796006366497265,10.877965338982106,10.959924311466947,11.041883283951789,11.12384225643663,11.205801228921471,{"$f":"'AEO Data'!$C$30*BB62","v":11.287760201406321},{"$f":"($BV62-$BQ62)/5+BQ62","v":11.35227956451322},11.416798927620118,11.481318290727016,11.545837653833914,{"$f":"'AEO Data'!$D$30*BQ62","v":11.610357016940812},{"$f":"+BV62*BW$136/BV$136","v":11.648906816150932},{"$f":"+BW62*BX$136/BW$136","v":11.687584612029626},11.726390829563474,11.765325895150129,11.804390236603014,11.829579958294525,11.854823433044533,11.880120775558206,11.905472100785488,11.930877523921614,11.939126503657128,11.947381186717189,11.955641577045064,11.963907678586745,11.97217949529095,11.974983273965139,11.977787709259525,11.980592801327882,11.98339855032402,11.986204956401787,11.990458334261309,11.99471322145788,11.9989696185271,12.003227526004752,12.007486944426816,12.014042207411556,12.020601049119556,12.027163471504549,12.033729476521339,12.040299066125799]
[{"$f":"'HyARC Physical Property Data'!A75","v":"Bio Methane"},2007,1.1413971588333081,{"$f":"'HyARC Physical Property Data'!H75","v":"mmBtu"},"Feed Utility",{"$f":"'HyARC Physical Property Data'!$E$6","v":47.141269049911173},{"$f":"'HyARC Physical Property Data'!$I$6","v":52.224661236371581},12.42654028436019,12.42654028436019,12.42654028436019,12.42654028436019,12.42654028436019,12.42654028436019,{"$f":"13.11*($C$63/mmBTU_to_GJ)","v":14.183617774696369},14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,{"$f":"13.11*($C$63/mmBTU_to_GJ)","v":14.183617774696369},14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,{"$f":"+BV63*BW$136/BV$136","v":14.230711556264829},14.277961703035571,14.325368734187041,14.372933170621517,14.420655534970821,14.451428179067991,14.482266489779443,14.51317060723302,14.54414067185559,14.575176824373679,14.585254066221541,14.595338275449933,14.605429456876088,14.615527615320566,14.625632755607262,14.629057949594106,14.632483945731124,14.635910744206171,14.639338345207147,14.642766748922,14.647962823919764,14.6531607427764,14.658360506146211,14.663562114683737,14.668765569043746,14.676773707333766,14.68478621751715,14.692803101980653,14.700824363112332,14.708850003301547]
[{"$f":"'HyARC Physical Property Data'!A85","v":"Woody Biomass"},2005,{"$f":"VLOOKUP(ref_year,DeflatorTable,2,FALSE)/VLOOKUP(B64,DeflatorTable,2,FALSE)","v":1.208440716126562},{"$f":"+'HyARC Physical Property Data'!$H$85","v":"kg"},"Feed",{"$f":"'HyARC Physical Property Data'!$E$45","v":19.551069237418005},{"$f":"'HyARC Physical Property Data'!$I$45","v":20.588656379262464},1.3438238843289665,1.3438238843289665,1.3438238843289665,1.3438238843289665,1.3438238843289665,1.3438238843289665,{"$f":"1.27*($C$64)","v":1.5347197094807337},{"$f":"1.27*($C$64)","v":1.5347197094807337},{"$f":"1.28*($C$64)","v":1.5468041166419995},{"$f":"1.32*($C$64)","v":1.595141745287062},{"$f":"1.32*($C$64)","v":1.595141745287062},{"$f":"1.34*($C$64)","v":1.6193105596095931},{"$f":"1.34*($C$64)","v":1.6193105596095931},{"$f":"1.36*($C$64)","v":1.6434793739321245},{"$f":"1.36*($C$64)","v":1.6434793739321245},{"$f":"1.38*($C$64)","v":1.6676481882546554},{"$f":"1.4*($C$64)","v":1.6918170025771868},{"$f":"1.46*($C$64)","v":1.7643234455447805},{"$f":"1.48*($C$64)","v":1.7884922598673119},{"$f":"1.48*($C$64)","v":1.7884922598673119},{"$f":"1.51*($C$64)","v":1.8247454813511086},{"$f":"1.52*($C$64)","v":1.8368298885123742},{"$f":"1.62*($C$64)","v":1.9576739601250306},{"$f":"1.72*($C$64)","v":2.0785180317376866},{"$f":"1.82*($C$64)","v":2.1993621033503428},{"$f":"1.91*($C$64)","v":2.3081217678017332},{"$f":"2.01*($C$64)","v":2.4289658394143894},{"$f":"2.11*($C$64)","v":2.5498099110270456},{"$f":"2.2*($C$64)","v":2.6585695754784364},{"$f":"2.3*($C$64)","v":2.7794136470910926},{"$f":"2.4*($C$64)","v":2.9002577187037488},{"$f":"2.5*($C$64)","v":3.021101790316405},{"$f":"2.57*($C$64)","v":3.1056926404452643},{"$f":"2.64*($C$64)","v":3.190283490574124},{"$f":"2.71*($C$64)","v":3.2748743407029832},{"$f":"2.78*($C$64)","v":3.359465190831842},{"$f":"2.85*($C$64)","v":3.4440560409607017},{"$f":"2.92*($C$64)","v":3.528646891089561},{"$f":"2.99*($C$64)","v":3.6132377412184207},{"$f":"3.07*($C$64)","v":3.7099129985085453},{"$f":"3.14*($C$64)","v":3.794503848637405},{"$f":"3.21*($C$64)","v":3.8790946987662642},{"$f":"3.28*($C$64)","v":3.963685548895123},{"$f":"3.35*($C$64)","v":4.0482763990239832},{"$f":"3.42*($C$64)","v":4.1328672491528424},{"$f":"3.49*($C$64)","v":4.2174580992817017},{"$f":"3.56*($C$64)","v":4.3020489494105609},{"$f":"3.64*($C$64)","v":4.3987242067006855},{"$f":"3.71*($C$64)","v":4.4833150568295448},{"$f":"3.78*($C$64)","v":4.567905906958404},{"$f":"3.85*($C$64)","v":4.6524967570872642},{"$f":"3.92*($C$64)","v":4.7370876072161234},{"$f":"3.99*($C$64)","v":4.8216784573449827},{"$f":"4.06*($C$64)","v":4.906269307473841},{"$f":"4.14*($C$64)","v":5.0029445647639665},{"$f":"4.21*($C$64)","v":5.0875354148928258},{"$f":"4.28*($C$64)","v":5.1721262650216859},{"$f":"4.35*($C$64)","v":5.2567171151505443},{"$f":"4.42*($C$64)","v":5.3413079652794044},{"$f":"4.49*($C$64)","v":5.4258988154082637},{"$f":"4.56*($C$64)","v":5.5104896655371221},{"$f":"4.63*($C$64)","v":5.5950805156659822},{"$f":"4.71*($C$64)","v":5.6917557729561068},{"$f":"4.78*($C$64)","v":5.7763466230849669},{"$f":"4.85*($C$64)","v":5.8609374732138253},{"$f":"4.92*($C$64)","v":5.9455283233426854},{"$f":"4.99*($C$64)","v":6.0301191734715447},{"$f":"+BV64*BW$138/BV$138","v":6.0446132076616896},{"$f":"+BW64*BX$138/BW$138","v":6.0591420798079438},6.0737058736470511,6.0883046731170198,6.1029385623576156,6.1157485681116217,6.1285854619369617,6.1414493002714252,6.1543401396712598,6.167258036811428,6.183149548139812,6.1990820079952069,6.215055521891923,6.2310701956161552,6.2471261352266838,6.2604975997429575,6.2738976847896071,6.2873264516265444,6.3007839616448056,6.3142702763668277,6.326614172551615,6.3389822000716718,6.3513744061018391,6.3637908379091801,6.376231542853164,6.3909193633613004,6.4056410176582252,6.4203965836809767,6.4351861395461265,6.450009763550189]
[{"$f":"'HyARC Physical Property Data'!A79","v":"Electric Utility Steam Coal"},2011,{"$f":"VLOOKUP(ref_year,DeflatorTable,2,FALSE)/VLOOKUP(B65,DeflatorTable,2,FALSE)","v":1.0771767810026385},{"$f":"+'HyARC Physical Property Data'!$H$79","v":"kg"},"Feed",{"$f":"'HyARC Physical Property Data'!$E$42","v":22.7322030001394},{"$f":"'HyARC Physical Property Data'!$I$42","v":23.967615189707661},1.6359074751967535,1.6359074751967535,1.6359074751967535,1.6778298347292193,1.8315470257945772,1.8060149340317679,{"$f":"N79*($C65/mmBTU_to_GJ*$G65/$F65)","v":2.4738067312648084},2.562092342657099,2.5992975836043981,2.5097040133060879,2.6554020233616504,2.6808248690608902,2.7666904873496958,2.7733379328185648,2.7935332489312734,2.8081877712256396,2.8455997019753716,2.875157420232656,2.9218811571857422,2.9595180783974975,3.001801214126441,3.0485410987203423,3.0887358062372043,3.1212689964420113,3.1614959992405027,3.2059762906296831,3.2488525830312334,3.2862978855719831,3.3267574143982119,3.3693139835116237,3.4131279155898357,3.462467570354963,3.500480193343015,3.5291401027709814,3.5647628749184039,3.6129969545423934,3.658942375208194,{"$f":"($BB65-$AR65)/10+AR65","v":3.6559939686764786},{"$f":"($BB65-$AR65)/10+AS65","v":3.6530455621447633},3.6500971556130479,3.6471487490813326,3.6442003425496172,3.6412519360179019,3.6383035294861865,3.6353551229544712,3.6324067164227558,{"$f":"('AEO Data'!$B$28*AM65)","v":3.6294583098910396},{"$f":"($BQ65-$BB65)/15+BB65","v":3.6421956634171884},{"$f":"($BQ65-$BB65)/15+BC65","v":3.6549330169433372},3.667670370469486,3.6804077239956348,3.6931450775217836,3.7058824310479324,3.7186197845740812,3.73135713810023,3.7440944916263788,3.7568318451525275,3.7695691986786763,3.7823065522048251,3.7950439057309739,3.8077812592571227,{"$f":"('AEO Data'!$C$28*BB65)","v":3.8205186127832693},{"$f":"($BV65-$BQ65)/5+BQ65","v":3.8327668169477032},3.845015021112137,3.8572632252765708,3.8695114294410047,{"$f":"('AEO Data'!$D$28*BQ65)","v":3.8817596336054376},{"$f":"+BV65*BW$139/BV$139","v":3.8948836892010701},{"$f":"+BW65*BX$139/BW$139","v":3.9080521166413131},3.9212650659453869,3.934522687639721,3.9478251327596676,3.9591283759223899,3.9704639820448935,3.9818320437874131,3.9932326540754852,4.0046659061007048,4.0133952059294913,4.0221435337314686,4.0309109309834765,4.0396974392527643,4.0485031001971885,4.0544726040914778,4.0604509099987238,4.0664380308974657,4.0724339797853757,4.0784387696792948,4.0804496799112764,4.0824615816402954,4.0844744753552202,4.0864883615451566,4.0885032406994535,4.0856074248284502,4.0827136600135576,4.0798219448020498,4.0769322777422268,4.0740446573834195]
[{"$f":"'HyARC Physical Property Data'!A76","v":"Commercial Electricity"},2011,1.0771767810026385,{"$f":"'HyARC Physical Property Data'!$H$76","v":"kWh"},"Feed Utility Byprod",null,null,26.764062885406638,26.764062885406638,26.764062885406638,26.478521097803213,27.879470162766175,27.895326399478549,{"$f":"N80*($C66)","v":32.845898091688653},{"$f":"O80*($C66)","v":32.294462213720315},30.700817944591027,29.936886325857518,30.351947314643798,30.31116863324538,30.903469366754614,31.264578879287598,31.3554312005277,31.211201538258571,31.282410463720318,31.412854417546175,31.504922871372031,31.44926299274406,31.362652593667544,31.455675426121374,31.429995531662264,31.467324015831135,31.469078736807386,31.609617991424798,31.830758075857517,32.094287220976256,32.269189492084429,32.612192740105542,33.178551825197886,33.706074378627967,34.261722017810023,34.758917736147751,35.188647718337727,35.787504149736144,36.169038011213715,{"$f":"($BB66-$AR66)/10+AR66","v":35.838717572225882},35.508397133238049,35.178076694250215,34.847756255262382,34.517435816274549,34.187115377286716,33.856794938298883,33.52647449931105,33.196154060323217,{"$f":"'AEO Data'!$B$33*AM66","v":32.865833621335355},{"$f":"($BQ66-$BB66)/15+BB66","v":32.884982038593449},32.904130455851544,32.923278873109638,32.942427290367732,32.961575707625826,32.98072412488392,32.999872542142015,33.019020959400109,33.038169376658203,33.057317793916297,33.076466211174392,33.095614628432486,33.11476304569058,33.133911462948674,{"$f":"'AEO Data'!$C$33*BB66","v":33.153059880206783},33.130736260086941,33.108412639967099,33.086089019847257,33.063765399727416,{"$f":"'AEO Data'!$D$33*BQ66","v":33.04144177960756},{"$f":"+BV66*BW$140/BV$140","v":33.026893508206783},{"$f":"+BW66*BX$140/BW$140","v":33.012351642464765},32.997816179561063,32.983287116676486,32.968764450993078,32.94235698552729,32.915970672028941,32.889605493555642,32.863261433178565,32.83693847398245,32.800677122537721,32.764455813973655,32.728274504071479,32.692133148661256,32.656031703621828,32.61667230567209,32.57736034649939,32.538095768927107,32.498878515847522,32.459708530221761,32.414339458662745,32.369033799646459,32.323791464540925,32.27861236483804,32.233496412153421,32.189455210275135,32.145474182677603,32.101553247143634,32.057692321568368,32.013891323959122]
[{"$f":"'HyARC Physical Property Data'!A77","v":"Industrial Electricity"},2011,1.0771767810026385,{"$f":"'HyARC Physical Property Data'!$H$77","v":"kWh"},"Feed Utility Byprod",null,null,17.365230901091444,17.365230901091444,17.365230901091444,17.575551809904887,19.530121721487372,19.467200489895287,{"$f":"N81*($C67)","v":21.824080926781001},21.517382844986805,19.878853696569919,19.559017289577834,19.681393189313983,19.595758712401054,20.147114879287596,20.469555899736147,20.570052184696571,20.520463274406332,20.569618082453825,20.73793341754617,20.92149511279683,21.047268428100264,21.075329960422163,21.244222662269127,21.339939513852244,21.483012288258571,21.593541397757257,21.800339950527704,21.997833850263849,22.197943135224271,22.447729658970974,22.811336067282323,23.297994842348285,23.815261595646437,24.308689349604222,24.764817703166226,25.184108765171505,25.713819064643797,26.032369322559369,{"$f":"($BB67-$AR67)/10+AR67","v":25.751290753982193},25.470212185405018,25.189133616827842,24.908055048250667,24.626976479673491,24.345897911096316,24.06481934251914,23.783740773941965,23.502662205364789,{"$f":"'AEO Data'!$B$33*AM67","v":23.22158363678761},{"$f":"($BQ67-$BB67)/15+BB67","v":23.235113084359032},23.248642531930454,23.262171979501876,23.275701427073297,23.289230874644719,23.302760322216141,23.316289769787563,23.329819217358985,23.343348664930406,23.356878112501828,23.37040756007325,23.383937007644672,23.397466455216094,23.410995902787516,{"$f":"'AEO Data'!$C$33*BB67","v":23.424525350358955},23.408752441092101,23.392979531825247,23.377206622558393,23.36143371329154,{"$f":"'AEO Data'!$D$33*BQ67","v":23.345660804024686},{"$f":"+BV67*BW$141/BV$141","v":23.3527149207825},{"$f":"+BW67*BX$141/BW$141","v":23.359771169009782},23.366829549350573,23.373890062449121,23.380952708949849,23.378308502870599,23.375664595830738,23.373020987796441,23.370377678733899,23.367734668609302,23.357134857315337,23.346539854189601,23.335949657051067,23.325364263719699,23.314783672016446,23.301803459317899,23.288830473189584,23.275864709608204,23.262906164552696,23.249954834004228,23.232210866712229,23.214480441312137,23.196763547469015,23.179060174855813,23.161370313153348,23.144738488925565,23.128118607755269,23.111510661066333,23.094914640288788,23.078330536858825]
[{"$f":"'HyARC Physical Property Data'!A78","v":"Residential Electricity"},2011,1.0771767810026385,{"$f":"'HyARC Physical Property Data'!$H$78","v":"kWh"},"Feed Utility Byprod",null,null,29.433773538887177,29.433773538887177,29.433773538887177,29.415861064534436,30.500905105766051,30.574559070308627,37.187183350263851,36.985808382585752,35.861648381926123,35.074328023746702,35.926786339050132,36.073591531002634,36.674317941292877,36.975630139182059,36.950708577176783,36.706312246042216,36.737241222955141,36.822931713060683,36.936536162269128,36.968069435356199,37.072613750659634,37.406478230870711,37.597953943931394,37.769102253957783,37.892630732849597,38.064576153693928,38.24699927308707,38.482771726912929,38.653685212401051,38.945181098284962,39.434103021767804,39.943878010554087,40.396384895778361,40.762839359498678,41.106692500000001,41.598897658311344,41.849125824538255,{"$f":"($BB68-$AR68)/10+AR68","v":41.559027079314276},41.268928334090297,40.978829588866319,40.68873084364234,40.398632098418361,40.108533353194382,39.818434607970403,39.528335862746424,39.238237117522445,{"$f":"'AEO Data'!$B$33*AM68","v":38.948138372298473},{"$f":"($BQ68-$BB68)/15+BB68","v":38.9708304851343},38.993522597970127,39.016214710805954,39.038906823641781,39.061598936477608,39.084291049313435,39.106983162149263,39.12967527498509,39.152367387820917,39.175059500656744,39.197751613492571,39.220443726328398,39.243135839164225,39.265827952000052,{"$f":"'AEO Data'!$C$33*BB68","v":39.288520064835851},39.262065131259057,39.235610197682263,39.209155264105469,39.182700330528675,{"$f":"'AEO Data'!$D$33*BQ68","v":39.156245396951888},{"$f":"+BV68*BW$142/BV$142","v":39.139004754462078},{"$f":"+BW68*BX$142/BW$142","v":39.121771703092165},39.104546239499747,39.087328360343896,39.070118062285161,39.038823507859021,39.007554019882264,38.976309578277061,38.94509016298165,38.913895753950342,38.870923707359104,38.827999114171142,38.785121921984356,38.742292078454511,38.699509531295178,38.652866099235652,38.606278885194918,38.559747821414987,38.513272840219521,38.466853874013751,38.413088590063794,38.359398454078047,38.305783361021881,38.252243206007478,38.198777884293627,38.146586211792602,38.094465849705919,38.042416700600896,37.990438667177955,37.93853165227047]
[]
[]
["AEO 2013 High Oil Price Case Values (except for BioMethane and Woody Biomass):"]
["2011 $/MMBtu"]
[]
["Residential Natural Gas",null,null,null,null,null,null,null,null,null,null,null,null,11.359373,10.802343,10.473763999999999,10.501935,10.334021999999999,10.229792,10.748874000000001,11.092333999999999,11.515472000000001,11.774895000000001,11.996413,12.209519999999999,12.479982,12.729352,12.853237999999999,13.018173000000001,13.212711000000001,13.366512,13.603230999999999,13.784504,13.991047,14.231726,14.577776,14.956607999999999,15.347963,15.708157999999999,16.169785000000001,16.471478000000001,16.949921,17.380462999999999,17.673891000000001]
["Commercial Natural Gas",null,null,null,null,null,null,null,null,null,null,null,null,9.3969749999999994,8.8368559999999992,8.081448,8.4844790000000003,8.3155520000000003,8.1773039999999995,8.6431299999999993,8.9205120000000004,9.2811249999999994,9.4920469999999995,9.6757190000000008,9.8498520000000003,10.083444999999999,10.292596,10.386177,10.522978999999999,10.688981999999999,10.803459999999999,10.994071,11.132752999999999,11.290343,11.483471,11.774739,12.104623999999999,12.443429,12.746489,13.159888,13.417020000000001,13.853782000000001,14.239846,14.480893]
["Industrial Natural Gas",null,null,null,null,null,null,null,null,null,null,null,null,5.4839570000000002,4.8889880000000003,3.7668759999999999,4.3500249999999996,4.4161510000000002,4.4533610000000001,4.916512,5.1321560000000002,5.3872429999999998,5.5533659999999996,5.6994189999999998,5.84443,6.055364,6.2505249999999997,6.3249610000000001,6.4443630000000001,6.5689469999999996,6.6624569999999999,6.8533949999999999,6.9821,7.1203779999999997,7.3037179999999999,7.5896039999999996,7.9110909999999999,8.2410040000000002,8.5300290000000007,8.90123,9.1114479999999993,9.4914550000000002,9.8126739999999995,10.012231]
[{"$f":"'HyARC Physical Property Data'!$A$74","v":"Electric Utility Natural Gas"},null,null,null,null,null,null,null,null,null,null,null,null,5.2581660000000001,4.7747140000000003,3.3280129999999999,3.7262059999999999,3.8342619999999998,3.9162499999999998,4.3469340000000001,4.5235139999999996,4.7720750000000001,4.9304030000000001,5.0667330000000002,5.2030240000000001,5.4141339999999998,5.6120320000000001,5.7180549999999997,5.8497880000000002,5.9964360000000001,6.1136410000000003,6.2808900000000003,6.4099190000000004,6.5488220000000004,6.7307620000000004,7.0166529999999998,7.3227570000000002,7.6342280000000002,7.902755,8.2651950000000003,8.4774010000000004,8.8551400000000005,9.1715459999999993,9.3359030000000001]
["Woody Biomass"]
["Electric Utility Steam Coal",null,null,null,null,null,null,null,null,null,null,null,null,2.2979889999999998,2.38,2.414561,2.3313350000000002,2.4666779999999999,2.490294,2.5700569999999998,2.5762320000000001,2.594992,2.6086049999999998,2.6433580000000001,2.6708150000000002,2.7142179999999998,2.74918,2.7884579999999999,2.8318759999999998,2.8692139999999999,2.899435,2.9368029999999998,2.9781219999999999,3.0179510000000001,3.0527350000000002,3.090319,3.1298509999999999,3.1705510000000001,3.2163840000000001,3.2516949999999998,3.2783180000000001,3.3114089999999998,3.3562150000000002,3.398895]
["Commercial Electricity",null,null,null,null,null,null,null,null,null,null,null,null,30.492578999999999,29.980651999999999,28.501187999999999,27.791989999999998,28.177313000000002,28.139455999999999,28.689319999999999,29.024557000000001,29.108899999999998,28.975003999999998,29.041111000000001,29.162209000000001,29.247681,29.196009,29.115604000000001,29.201962000000002,29.178121999999998,29.212776000000002,29.214404999999999,29.344874999999998,29.550170999999999,29.794819,29.957190000000001,30.275618000000001,30.801399,31.291125999999998,31.806963,32.268535999999997,32.667476999999998,33.223427000000001,33.577624999999998]
["Industrial Electricity",null,null,null,null,null,null,null,null,null,null,null,null,20.260445000000001,19.975721,18.454588000000001,18.157667,18.271274999999999,18.191776000000001,18.703628999999999,19.002967999999999,19.096264000000001,19.050228000000001,19.095860999999999,19.252116999999998,19.422526999999999,19.539289,19.565339999999999,19.722131999999998,19.810991000000001,19.943812999999999,20.046423000000001,20.238405,20.421748999999998,20.607520999999998,20.839410999999998,21.176966,21.628757,22.108962999999999,22.567038,22.990486000000001,23.379736000000001,23.871493999999998,24.167221000000001]
["Residential Electricity",null,null,null,null,null,null,null,null,null,null,null,null,34.522823000000002,34.335875999999999,33.292259000000001,32.561348000000002,33.352730000000001,33.489016999999997,34.046703000000001,34.326427000000002,34.303291000000002,34.076405000000001,34.105117999999997,34.184669,34.290134000000002,34.319408000000003,34.416462000000003,34.726405999999997,34.904162999999997,35.063048999999999,35.177726999999997,35.337353,35.506706000000001,35.725586,35.884253999999999,36.154865000000001,36.608756999999997,37.082008000000002,37.502094,37.842292999999998,38.16151,38.618450000000003,38.850749999999998]
[]
[]
[]
["AEO_2014_Reference_Case",{"$f":"\"Prices are in $(\" & ref_year&\")/GJ LHV\"","v":"Prices are in $(2016)/GJ LHV"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Except as noted,values are extrapolated based on PNNL mini-CAM model (see AEO Data tab)"]
["Year","Source Data Year","Reference year Conversion","Display Units","Use Category","LHV (MJ/kg)","HHV (MJ/kg)",2004,2005,2006,2007,2008,2009,2010,2011,2012,2013,2014,2015,2016,2017,2018,2019,2020,2021,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,2033,2034,2035,2036,2037,2038,2039,2040,2041,2042,2043,2044,2045,2046,2047,2048,2049,2050,2051,2052,2053,2054,2055,2056,2057,2058,2059,2060,2061,2062,2063,2064,2065,2066,2067,2068,2069,2070,{"$f":"+BV87+1","v":2071},{"$f":"+BW87+1","v":2072},{"$f":"+BX87+1","v":2073},{"$f":"+BY87+1","v":2074},{"$f":"+BZ87+1","v":2075},{"$f":"+CA87+1","v":2076},{"$f":"+CB87+1","v":2077},{"$f":"+CC87+1","v":2078},{"$f":"+CD87+1","v":2079},{"$f":"+CE87+1","v":2080},{"$f":"+CF87+1","v":2081},{"$f":"+CG87+1","v":2082},{"$f":"+CH87+1","v":2083},{"$f":"+CI87+1","v":2084},{"$f":"+CJ87+1","v":2085},{"$f":"+CK87+1","v":2086},{"$f":"+CL87+1","v":2087},{"$f":"+CM87+1","v":2088},{"$f":"+CN87+1","v":2089},{"$f":"+CO87+1","v":2090},{"$f":"+CP87+1","v":2091},{"$f":"+CQ87+1","v":2092},{"$f":"+CR87+1","v":2093},{"$f":"+CS87+1","v":2094},{"$f":"+CT87+1","v":2095},{"$f":"+CU87+1","v":2096},{"$f":"+CV87+1","v":2097},{"$f":"+CW87+1","v":2098},{"$f":"+CX87+1","v":2099},{"$f":"+CY87+1","v":2100}]
["Feedstock Type"]
[{"$f":"'HyARC Physical Property Data'!A73","v":"Residential Natural Gas"},2012,{"$f":"VLOOKUP(ref_year,DeflatorTable,2,FALSE)/VLOOKUP(B89,DeflatorTable,2,FALSE)","v":1.0573833607504113},{"$f":"'HyARC Physical Property Data'!H73","v":"mmBtu"},"Feed Utility",{"$f":"'HyARC Physical Property Data'!$E$6","v":47.141269049911173},{"$f":"'HyARC Physical Property Data'!$I$6","v":52.224661236371581},12.595706345448797,12.595706345448797,12.595706345448797,12.595706345448797,13.121338604068761,11.086947084595193,10.600250548835966,{"$f":"O106*($C89/mmBTU_to_GJ*$G89/$F89)","v":12.191092687749757},11.61240672324179,11.532824509346533,12.433025993412414,12.210932169261609,11.863496968910505,12.225430935188502,12.719978977683732,12.909977432874298,12.870974664401787,13.107127561470831,13.208746611585347,13.387263083436196,13.662847338627605,13.851960856121453,13.96794321118545,14.119468528118476,14.321017807473346,14.638900308030435,14.992739925739963,15.156051458043953,15.225075488052026,15.481925045932627,15.921613613246663,16.217219445034317,16.649245584437377,16.824194547104348,16.965891170823646,17.341637715454421,17.740732402979265,{"$f":"($BB89-$AR89)/10+AR89","v":17.791465746273797},{"$f":"($BB89-$AR89)/10+AS89","v":17.842199089568329},17.89293243286286,17.943665776157392,17.994399119451923,18.045132462746455,18.095865806040987,18.146599149335518,18.19733249263005,{"$f":"'AEO Data'!$B$30*AM89","v":18.248065835924574},{"$f":"($BQ89-$BB89)/15+BB89","v":18.396757114031804},18.545448392139033,18.694139670246262,18.842830948353491,18.99152222646072,19.140213504567949,19.288904782675178,19.437596060782408,19.586287338889637,19.734978616996866,19.883669895104095,20.032361173211324,20.181052451318553,20.329743729425783,{"$f":"'AEO Data'!$C$30*BB89","v":20.478435007533015},{"$f":"($BV89-$BQ89)/5+BQ89","v":20.595487067510991},20.712539127488967,20.829591187466942,20.946643247444918,{"$f":"'AEO Data'!$D$30*BQ89","v":21.063695307422901},{"$f":"+BV89*BW$133/BV$133","v":21.133632969420677},{"$f":"+BW89*BX$133/BW$133","v":21.203802845020782},21.274205705240661,21.344842323657751,21.415713476418006,21.461413072202582,21.507210187645192,21.553105030845796,21.599097810348415,21.645188735142085,21.66015416604937,21.675129944019229,21.690116076205594,21.705112569767344,21.720119431868312,21.725206091961226,21.730293943305,21.73538298617861,21.740473220861105,21.745564647631596,21.753281193740353,21.761000478112514,21.768722501719765,21.776447265534141,21.784174770528026,21.796067433429702,21.807966588908322,21.819872240508388,21.831784391776338,21.84370304626054]
[{"$f":"'HyARC Physical Property Data'!A71","v":"Commercial Natural Gas"},2012,1.0573833607504113,{"$f":"'HyARC Physical Property Data'!H71","v":"mmBtu"},"Feed Utility",{"$f":"'HyARC Physical Property Data'!$E$6","v":47.141269049911173},{"$f":"'HyARC Physical Property Data'!$I$6","v":52.224661236371581},10.902002401006685,10.902002401006685,10.902002401006685,10.902002401006685,11.622313273930342,8.8092072972420112,8.4393179300649965,{"$f":"O107*($C90/mmBTU_to_GJ*$G90/$F90)","v":9.9495366192776444},9.0080039923979545,9.2291706860885867,10.088576209235033,9.9025871769087672,9.6855387189987159,10.001081741855701,10.447347938925514,10.599788172624031,10.53794690542658,10.753568581730253,10.835192703309655,10.990940627596027,11.244415874735946,11.421938595973796,11.526345699484116,11.655064717432735,11.833099303511471,12.114892556946344,12.427240033139398,12.540484299922209,12.538704431505849,12.7448604944287,13.044138206972995,13.272322223428063,13.616748413543148,13.732951725447354,13.833902353361841,14.16332901606795,14.520292008609179,{"$f":"($BB90-$AR90)/10+AR90","v":14.561701375004496},14.603110741399814,14.644520107795131,14.685929474190448,14.727338840585766,14.768748206981083,14.810157573376401,14.851566939771718,14.892976306167036,{"$f":"'AEO Data'!$B$30*AM90","v":14.934385672562355},15.056075988312308,15.177766304062262,15.299456619812215,15.421146935562168,15.542837251312122,15.664527567062075,15.786217882812029,15.907908198561982,16.029598514311935,16.151288830061887,16.272979145811838,16.39466946156179,16.516359777311742,16.638050093061693,{"$f":"'AEO Data'!$C$30*BB90","v":16.759740408811648},16.855536896132378,16.951333383453107,17.047129870773837,17.142926358094567,{"$f":"'AEO Data'!$D$30*BQ90","v":17.238722845415303},{"$f":"+BV90*BW$134/BV$134","v":17.295960474142827},{"$f":"+BW90*BX$134/BW$134","v":17.353388148627904},17.411006499878322,17.468816160997019,17.526817767189005,17.564218738594064,17.601699520988237,17.63926028468245,17.676901200351057,17.71462243903262,17.726870285951581,17.739126601002145,17.751391390039156,17.763664658921517,17.775946413512166,17.78010938312746,17.784273327673461,17.78843824737849,17.792604142470921,17.796771013179182,17.803086305807149,17.809403839455182,17.815723614918522,17.82204563299269,17.828369894473493,17.838102959667598,17.84784133844666,17.85758503371153,17.867334048364647,17.877088385310028]
[{"$f":"'HyARC Physical Property Data'!A72","v":"Industrial Natural Gas"},2012,1.0573833607504113,{"$f":"'HyARC Physical Property Data'!H72","v":"mmBtu"},"Feed Utility",{"$f":"'HyARC Physical Property Data'!$E$6","v":47.141269049911173},{"$f":"'HyARC Physical Property Data'!$I$6","v":52.224661236371581},7.3783194821098821,7.3783194821098821,7.3783194821098821,7.3783194821098821,8.8676108815331158,4.0882509003775072,4.7404242582948717,{"$f":"O108*($C91/mmBTU_to_GJ*$G91/$F91)","v":5.655737860285754},4.1875429462406233,5.101776855163612,5.3291370023953855,5.4842809039627953,5.7166186869466191,6.0244693028238556,6.490891427131448,6.6038403445700586,6.4314251683822734,6.5896202729491558,6.6115305308780448,6.7200414358025036,6.9144745724995795,7.0183809145278193,7.0574158827408624,7.1387235585943367,7.2521565824768235,7.4789127069896324,7.7602540537211651,7.8876606546590935,8.02124849544348,8.2390597541033976,8.4081761223903708,8.613534964151059,8.930664656981202,8.9872951178917102,9.0273060713436681,9.2571600329629291,9.5415659067244984,{"$f":"($BB91-$AR91)/10+AR91","v":9.5566281987255213},9.5716904907265441,9.5867527827275669,9.6018150747285897,9.6168773667296126,9.6319396587306354,9.6470019507316582,9.6620642427326811,9.6771265347337039,{"$f":"'AEO Data'!$B$30*AM91","v":9.6921888267347267},9.7711639881168519,9.8501391494989772,9.9291143108811024,10.008089472263228,10.087064633645353,10.166039795027478,10.245014956409603,10.323990117791729,10.402965279173854,10.481940440555979,10.560915601938104,10.63989076332023,10.718865924702355,10.79784108608448,{"$f":"'AEO Data'!$C$30*BB91","v":10.876816247466609},10.938986708602901,11.001157169739193,11.063327630875484,11.125498092011776,{"$f":"'AEO Data'!$D$30*BQ91","v":11.187668553148065},{"$f":"+BV91*BW$135/BV$135","v":11.224814902370914},{"$f":"+BW91*BX$135/BW$135","v":11.262084588395711},11.299478020736903,11.336995610268644,11.37463776922932,11.398910429994142,11.42323488687525,11.447611250401838,11.472039631338966,11.496520140688052,11.504468806784013,11.512422968568401,11.520382629840926,11.528347794403915,11.536318466062333,11.539020169933924,11.541722506520692,11.544425475970817,11.54712907843251,11.549833314054016,11.553931842777482,11.558031825888838,11.562133263904183,11.566236157339798,11.570340506712146,11.576657117772855,11.582977177269267,11.589300687083989,11.595627649100658,11.60195806520394]
[{"$f":"'HyARC Physical Property Data'!A74","v":"Electric Utility Natural Gas"},2012,1.0573833607504113,{"$f":"'HyARC Physical Property Data'!H74","v":"mmBtu"},"Feed Utility",{"$f":"'HyARC Physical Property Data'!$E$6","v":47.141269049911173},{"$f":"'HyARC Physical Property Data'!$I$6","v":52.224661236371581},7.0668336992239764,7.0668336992239764,7.0668336992239764,7.0668336992239764,8.8481430201027482,4.0298473160863999,4.7209563968645023,{"$f":"O109*($C92/mmBTU_to_GJ*$G92/$F92)","v":5.4205498450968195},3.8171937443247086,4.7973527358134387,4.9625507287783099,4.9171202258938838,4.9685332185021656,5.2081048397471088,5.6206345914253779,5.7508958659119411,5.6343006054419362,5.8207548685021111,5.8784978859648298,6.0180882025189186,6.2425492627668415,6.3929997745675973,6.4554939192627536,6.5567554412237641,6.6927371661663972,6.9326085780990629,7.2098860955081534,7.3471713547744324,7.468747582004128,7.6952494396003139,7.8732995703813753,8.0908132590253317,8.4061308836985837,8.4723502052726456,8.5254853288315022,8.7688220990470462,9.0589717403181744,{"$f":"($BB92-$AR92)/10+AR92","v":9.0634753505716894},9.0679789608252044,9.0724825710787194,9.0769861813322343,9.0814897915857493,9.0859934018392643,9.0904970120927793,9.0950006223462943,9.0995042325998092,{"$f":"'AEO Data'!$B$30*AM92","v":9.1040078428533171},9.178190310969315,9.252372779085313,9.3265552472013109,9.4007377153173088,9.4749201834333068,9.5491026515493047,9.6232851196653026,9.6974675877813006,9.7716500558972985,9.8458325240132964,9.9200149921292944,9.9941974602452923,10.06837992836129,10.142562396477288,{"$f":"'AEO Data'!$C$30*BB92","v":10.216744864593281},10.275142443911728,10.333540023230174,10.391937602548621,10.450335181867068,{"$f":"'AEO Data'!$D$30*BQ92","v":10.508732761185513},{"$f":"+BV92*BW$136/BV$136","v":10.543624843944501},{"$f":"+BW92*BX$136/BW$136","v":10.578632778677932},10.613756950048424,10.648997743995791,10.684355547741282,10.707155195779537,10.730003496630621,10.752900554116147,10.775846472279273,10.79884135538518,10.806307648063903,10.813779102919245,10.821255723520322,10.828737513438721,10.836224476248493,10.838762224292379,10.841300566654439,10.843839503473856,10.846379034889845,10.848919161041659,10.85276896610733,10.856620137299787,10.860472675103804,10.864326580004334,10.868181852486501,10.874115133158696,10.880051652994538,10.885991413762385,10.891934417231562,10.897880665172362]
[{"$f":"'HyARC Physical Property Data'!A75","v":"Bio Methane"},2007,1.1413971588333081,{"$f":"'HyARC Physical Property Data'!H75","v":"mmBtu"},"Feed Utility",{"$f":"'HyARC Physical Property Data'!$E$6","v":47.141269049911173},{"$f":"'HyARC Physical Property Data'!$I$6","v":52.224661236371581},12.42654028436019,12.42654028436019,12.42654028436019,12.42654028436019,12.42654028436019,12.42654028436019,12.42654028436019,{"$f":"13.11*($C$93/mmBTU_to_GJ)","v":14.183617774696369},14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,{"$f":"13.11*($C$93/mmBTU_to_GJ)","v":14.183617774696369},14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,14.183617774696369,{"$f":"+BV93*BW$136/BV$136","v":14.230711556264829},{"$f":"+BW93*BX$136/BW$136","v":14.277961703035571},14.325368734187041,14.372933170621517,14.420655534970821,14.451428179067991,14.482266489779443,14.51317060723302,14.54414067185559,14.575176824373679,14.585254066221541,14.595338275449933,14.605429456876088,14.615527615320566,14.625632755607262,14.629057949594106,14.632483945731124,14.635910744206171,14.639338345207147,14.642766748922,14.647962823919764,14.6531607427764,14.658360506146211,14.663562114683737,14.668765569043746,14.676773707333766,14.68478621751715,14.692803101980653,14.700824363112332,14.708850003301547]
[{"$f":"'HyARC Physical Property Data'!A85","v":"Woody Biomass"},2005,1.208440716126562,{"$f":"+'HyARC Physical Property Data'!$H$85","v":"kg"},"Feed Utility",{"$f":"'HyARC Physical Property Data'!$E$45","v":19.551069237418005},{"$f":"'HyARC Physical Property Data'!$I$45","v":20.588656379262464},1.3438238843289665,1.3438238843289665,1.3438238843289665,1.3438238843289665,1.3438238843289665,1.3438238843289665,1.3438238843289665,{"$f":"1.27*($C$94)","v":1.5347197094807337},{"$f":"1.28*($C$94)","v":1.5468041166419995},{"$f":"1.32*($C$94)","v":1.595141745287062},{"$f":"1.32*($C$94)","v":1.595141745287062},{"$f":"1.34*($C$94)","v":1.6193105596095931},{"$f":"1.34*($C$94)","v":1.6193105596095931},{"$f":"1.36*($C$94)","v":1.6434793739321245},{"$f":"1.36*($C$94)","v":1.6434793739321245},{"$f":"1.38*($C$94)","v":1.6676481882546554},{"$f":"1.4*($C$94)","v":1.6918170025771868},{"$f":"1.46*($C$94)","v":1.7643234455447805},{"$f":"1.48*($C$94)","v":1.7884922598673119},{"$f":"1.48*($C$94)","v":1.7884922598673119},{"$f":"1.51*($C$94)","v":1.8247454813511086},{"$f":"1.52*($C$94)","v":1.8368298885123742},{"$f":"1.62*($C$94)","v":1.9576739601250306},{"$f":"1.72*($C$94)","v":2.0785180317376866},{"$f":"1.82*($C$94)","v":2.1993621033503428},{"$f":"1.91*($C$94)","v":2.3081217678017332},{"$f":"2.01*($C$94)","v":2.4289658394143894},{"$f":"2.11*($C$94)","v":2.5498099110270456},{"$f":"2.2*($C$94)","v":2.6585695754784364},{"$f":"2.3*($C$94)","v":2.7794136470910926},{"$f":"2.4*($C$94)","v":2.9002577187037488},{"$f":"2.5*($C$94)","v":3.021101790316405},{"$f":"2.57*($C$94)","v":3.1056926404452643},{"$f":"2.64*($C$94)","v":3.190283490574124},{"$f":"2.71*($C$94)","v":3.2748743407029832},{"$f":"2.78*($C$94)","v":3.359465190831842},{"$f":"2.85*($C$94)","v":3.4440560409607017},{"$f":"2.92*($C$94)","v":3.528646891089561},{"$f":"2.99*($C$94)","v":3.6132377412184207},{"$f":"3.07*($C$94)","v":3.7099129985085453},{"$f":"3.14*($C$94)","v":3.794503848637405},{"$f":"3.21*($C$94)","v":3.8790946987662642},{"$f":"3.28*($C$94)","v":3.963685548895123},{"$f":"3.35*($C$94)","v":4.0482763990239832},{"$f":"3.42*($C$94)","v":4.1328672491528424},{"$f":"3.49*($C$94)","v":4.2174580992817017},{"$f":"3.56*($C$94)","v":4.3020489494105609},{"$f":"3.64*($C$94)","v":4.3987242067006855},{"$f":"3.71*($C$94)","v":4.4833150568295448},{"$f":"3.78*($C$94)","v":4.567905906958404},{"$f":"3.85*($C$94)","v":4.6524967570872642},{"$f":"3.92*($C$94)","v":4.7370876072161234},{"$f":"3.99*($C$94)","v":4.8216784573449827},{"$f":"4.06*($C$94)","v":4.906269307473841},{"$f":"4.14*($C$94)","v":5.0029445647639665},{"$f":"4.21*($C$94)","v":5.0875354148928258},{"$f":"4.28*($C$94)","v":5.1721262650216859},{"$f":"4.35*($C$94)","v":5.2567171151505443},{"$f":"4.42*($C$94)","v":5.3413079652794044},{"$f":"4.49*($C$94)","v":5.4258988154082637},{"$f":"4.56*($C$94)","v":5.5104896655371221},{"$f":"4.63*($C$94)","v":5.5950805156659822},{"$f":"4.71*($C$94)","v":5.6917557729561068},{"$f":"4.78*($C$94)","v":5.7763466230849669},{"$f":"4.85*($C$94)","v":5.8609374732138253},{"$f":"4.92*($C$94)","v":5.9455283233426854},{"$f":"4.99*($C$94)","v":6.0301191734715447},{"$f":"+BV94*BW$138/BV$138","v":6.0446132076616896},{"$f":"+BW94*BX$138/BW$138","v":6.0591420798079438},6.0737058736470511,6.0883046731170198,6.1029385623576156,6.1157485681116217,6.1285854619369617,6.1414493002714252,6.1543401396712598,6.167258036811428,6.183149548139812,6.1990820079952069,6.215055521891923,6.2310701956161552,6.2471261352266838,6.2604975997429575,6.2738976847896071,6.2873264516265444,6.3007839616448056,6.3142702763668277,6.326614172551615,6.3389822000716718,6.3513744061018391,6.3637908379091801,6.376231542853164,6.3909193633613004,6.4056410176582252,6.4203965836809767,6.4351861395461265,6.450009763550189]
[{"$f":"'HyARC Physical Property Data'!A80","v":"Metallurgical Coal"},2012,1.0573833607504113,{"$f":"+'HyARC Physical Property Data'!H80","v":"kg"},"Feed",{"$f":"'HyARC Physical Property Data'!$E$44","v":28.610197070281195},{"$f":"'HyARC Physical Property Data'!$I$44","v":29.865267156269461},3.3844321322674711,3.3844321322674711,3.3844321322674711,3.3844321322674711,4.1181843560652975,4.3291381204071717,4.4025133427869543,{"$f":"O111*($C95/mmBTU_to_GJ*$G95/$F95)","v":7.4646268248681658},7.5851395215871422,7.7775593409707655,7.8596002100362519,8.1180797941829823,8.3154796499973287,8.4204203168350222,8.5695650843522451,8.6847148258729252,8.8178648881479358,8.9203207679009697,9.032455285683552,9.1423770351781108,9.254374497336233,9.3655611342351488,9.4622292909766781,9.5719166858156743,9.6949560186649464,9.8138135856290027,9.952872733147867,10.036208830175799,10.120782612728425,10.210359448686875,10.292143992347839,10.394155225990989,10.475670889533738,10.567574532429569,10.574325829716853,10.604382860519015,10.668415039021042,{"$f":"($BB95-$AR95)/10+AR95","v":10.691118846164347},{"$f":"($BB95-$AR95)/10+AS95","v":10.713822653307652},10.736526460450957,10.759230267594262,10.781934074737567,10.804637881880872,10.827341689024177,10.850045496167482,10.872749303310787,{"$f":"('AEO Data'!$B$28*AM95)","v":10.895453110454083},{"$f":"($BQ95-$BB95)/15+BB95","v":10.933690011458628},10.971926912463173,11.010163813467718,11.048400714472264,11.086637615476809,11.124874516481354,11.163111417485899,11.201348318490444,11.239585219494989,11.277822120499534,11.316059021504079,11.354295922508625,11.39253282351317,11.430769724517715,{"$f":"('AEO Data'!$C$28*BB95)","v":11.469006625522269},{"$f":"($BV95-$BQ95)/5+BQ95","v":11.505775124501078},11.542543623479887,11.579312122458695,11.616080621437504,{"$f":"('AEO Data'!$D$28*BQ95)","v":11.65284912041631},{"$f":"+BV95*BW$139/BV$139","v":11.692246881776873},11.731777845205377,11.771442461052049,11.811241181189736,11.851174459019044,11.88510623212686,11.919135157228366,11.953261512484969,11.987485576854503,12.021807630093496,12.048012553487283,12.074274597909055,12.100593887870218,12.126970548153587,12.153404703813971,12.171324857241729,12.189271433874072,12.207244472671922,12.225244012653652,12.243270092895166,12.249306745274442,12.255346374078453,12.261388980774752,12.267434566831614,12.273483133718042,12.264790038675994,12.256103100802259,12.247422315735818,12.238747679118744,12.2300791865962]
[{"$f":"'HyARC Physical Property Data'!A81","v":"Other Industrial Coal"},2012,1.0573833607504113,{"$f":"+'HyARC Physical Property Data'!H81","v":"kg"},"Feed",{"$f":"'HyARC Physical Property Data'!$E$42","v":22.7322030001394},{"$f":"'HyARC Physical Property Data'!$I$42","v":23.967615189707661},1.7045706620386931,1.7045706620386931,1.7045706620386931,1.7045706620386931,1.9454339077615519,2.0288096466656182,1.8805861108361666,{"$f":"O112*($C96/mmBTU_to_GJ*$G96/$F96)","v":3.4949975895838294},3.4233926279260714,3.5031491911574184,3.4679009642856751,3.5676645631136981,3.6321947292652106,3.657322669869095,3.7204040616159686,3.7630990523312531,3.7970908293363905,3.8194247804976293,3.8460511617330089,3.8731023477172322,3.9067337803956139,3.938949197244515,3.9691747948345282,3.9994574557490128,4.0328902235199751,4.0631242749358352,4.1048449622221792,4.1376658843474177,4.1685794120157826,4.201707842056229,4.2273873947966729,4.2580071520168321,4.2903546598946027,4.3224348155299417,4.3507255437290757,4.3846898458002084,4.4275856148793746,{"$f":"($BB96-$AR96)/10+AR96","v":4.4311636364046505},4.4347416579299264,4.4383196794552022,4.4418977009804781,4.445475722505754,4.4490537440310298,4.4526317655563057,4.4562097870815816,4.4597878086068574,{"$f":"('AEO Data'!$B$28*AM96)","v":4.4633658301321333},{"$f":"($BQ96-$BB96)/15+BB96","v":4.4790297291608097},4.494693628189486,4.5103575272181624,4.5260214262468388,4.5416853252755152,4.5573492243041915,4.5730131233328679,4.5886770223615443,4.6043409213902207,4.620004820418897,4.6356687194475734,4.6513326184762498,4.6669965175049262,4.6826604165336025,{"$f":"('AEO Data'!$C$28*BB96)","v":4.6983243155622842},4.7133866778434639,4.7284490401246435,4.7435114024058231,4.7585737646870028,{"$f":"('AEO Data'!$D$28*BQ96)","v":4.7736361269681806},{"$f":"+BV96*BW$139/BV$139","v":4.789775577072529},4.8059695939353695,4.8222183620444703,4.838522066511346,4.8548808930733625,4.8687811792854072,4.882721264199219,4.8967012617647283,4.9107212862581244,4.9247814522827849,4.9355164036860302,4.9462747549462529,4.9570565570700476,4.9678618611751908,4.9786907184908857,4.9860317808284806,4.9933836675372394,5.0007463945776598,5.0081199779337728,5.0155044336131782,5.0179773723413712,5.0204515303738297,5.0229269083117432,5.0254035067565965,5.0278813263101725,5.024320165248267,5.0207615264949217,5.0172054082636297,5.013651808769148,5.010100726227499]
[{"$f":"'HyARC Physical Property Data'!A79","v":"Electric Utility Steam Coal"},2012,1.0573833607504113,{"$f":"+'HyARC Physical Property Data'!$H$79","v":"kg"},"Feed",{"$f":"'HyARC Physical Property Data'!$E$42","v":22.7322030001394},{"$f":"'HyARC Physical Property Data'!$I$42","v":23.967615189707661},1.6675147780813302,1.6675147780813302,1.6675147780813302,1.6675147780813302,1.899114052814848,1.9917537627082553,1.8435302268788039,{"$f":"O113*($C97/mmBTU_to_GJ*$G97/$F97)","v":2.5597920484602081},2.5255804719830319,2.508514311053105,2.4620013612393787,2.5403070366096241,2.5596198017585623,2.6274226552413431,2.6949877448721598,2.7359771762226828,2.7594809255355894,2.7929327144147083,2.8274782170128665,2.8557773990378479,2.8944082129768782,2.9312151139892806,2.966511950359648,2.9977467234102231,3.0275126442197702,3.0554092127887573,3.0915672826673535,3.1167332654875524,3.1431165992298116,3.1708409210971538,3.1960671374265175,3.2230993023025833,3.2506534909247415,3.2748293193925355,3.2978596544579739,3.3327063246019542,3.3706196200721661,{"$f":"($BB97-$AR97)/10+AR97","v":3.3714122172383907},3.3722048144046153,3.3729974115708399,3.3737900087370645,3.3745826059032891,3.3753752030695137,3.3761678002357383,3.3769603974019629,3.3777529945681875,{"$f":"('AEO Data'!$B$28*AM97)","v":3.3785455917344129},{"$f":"($BQ97-$BB97)/15+BB97","v":3.3904023830051258},3.4022591742758386,3.4141159655465514,3.4259727568172642,3.437829548087977,3.4496863393586898,3.4615431306294027,3.4733999219001155,3.4852567131708283,3.4971135044415411,3.5089702957122539,3.5208270869829668,3.5326838782536796,3.5445406695243924,{"$f":"('AEO Data'!$C$28*BB97)","v":3.5563974607951057},3.5677989187133954,3.5792003766316851,3.5906018345499748,3.6020032924682646,{"$f":"('AEO Data'!$D$28*BQ97)","v":3.6134047503865552},{"$f":"+BV97*BW$139/BV$139","v":3.6256215101320701},3.6378795741955314,3.6501790822249895,3.6625201743406386,3.6749029911364137,3.6854248153589553,3.6959767652161704,3.7065589269624799,3.7171713870992669,3.7278142323755787,3.7359400558283795,3.7440835918072533,3.7522448789216503,3.760423955865182,3.768620861415803,3.7741776799118107,3.7797426919175763,3.7853159095144004,3.7908973448013987,3.796487009895527,3.7983589013238204,3.8002317157047045,3.8021054534932484,3.8039801151447463,3.805855701114718,3.803160079589381,3.8004663673259764,3.7977745629722066,3.7950846651767312,3.7923966725891693]
[{"$f":"'HyARC Physical Property Data'!A76","v":"Commercial Electricity"},2012,1.0573833607504113,{"$f":"'HyARC Physical Property Data'!$H$76","v":"kWh"},"Feed Utility Byprod",null,null,26.706046857142852,26.706046857142852,26.706046857142852,26.706046857142852,28.244819428571425,26.82655314285714,25.371207999999996,{"$f":"O114*($C98)","v":32.283135281491724},{"$f":"P114*($C98)","v":31.249217372283084},31.153358168947534,31.319492127821917,31.713042813009693,31.867220938224076,32.111549454009307,32.486400314462216,32.794032257288862,32.56691477046656,32.389706835655034,32.033284052413286,31.890145009485142,32.24751415083476,32.302516061110914,32.38566340168353,32.600838800829514,32.680488317244759,32.795928145654685,33.053412625214378,33.31428601844528,33.35913704845823,33.34702472206083,33.547734059448395,33.819217237321062,34.102738724755874,34.318819244058659,34.39246810990165,34.626804352927799,34.901427959381891,{"$f":"($BB98-$AR98)/10+AR98","v":34.70890076364649},34.516373567911089,34.323846372175687,34.131319176440286,33.938791980704885,33.746264784969483,33.553737589234082,33.361210393498681,33.168683197763279,{"$f":"'AEO Data'!$B$33*AM98","v":32.976156002027878},{"$f":"($BQ98-$BB98)/15+BB98","v":32.995368695731926},33.014581389435975,33.033794083140023,33.053006776844072,33.07221947054812,33.091432164252168,33.110644857956217,33.129857551660265,33.149070245364314,33.168282939068362,33.187495632772411,33.206708326476459,33.225921020180508,33.245133713884556,{"$f":"'AEO Data'!$C$33*BB98","v":33.264346407588576},33.241947852661184,33.219549297733792,33.1971507428064,33.174752187879008,{"$f":"'AEO Data'!$D$33*BQ98","v":33.152353632951616},{"$f":"+BV98*BW$140/BV$140","v":33.137756526643614},{"$f":"+BW98*BX$140/BW$140","v":33.123165847496566},33.108581592680558,33.094003759366935,33.079432344728289,33.052936236007881,33.026461350256774,33.000007670475696,32.973575179679017,32.947163860894676,32.91078078916545,32.874437894730825,32.838135133223581,32.801872460325534,32.765649831767405,32.726158314166163,32.686714394582069,32.647318015646562,32.60796912006024,32.568667650592751,32.523146286411503,32.477688547633022,32.432294345327811,32.386963590690684,32.341696195040562,32.297507157866328,32.25337849696286,32.209310129836972,32.16530197410821,32.121353947508659]
[{"$f":"'HyARC Physical Property Data'!A77","v":"Industrial Electricity"},2012,1.0573833607504113,{"$f":"'HyARC Physical Property Data'!$H$77","v":"kWh"},"Feed Utility Byprod",null,null,17.630996571428568,17.630996571428568,17.630996571428568,17.630996571428568,18.734092571428569,18.576507428571425,17.751502857142853,{"$f":"O115*($C99)","v":21.515674690350355},20.614325162612442,21.234320838805083,21.012944943631656,21.260067066255996,21.264334665499984,21.45053776056141,21.773568377270657,22.056475524972875,21.961455884025764,21.942053956739354,21.839343966609501,21.848738817769767,22.148172867400511,22.288834461114416,22.455557382520738,22.693200063315949,22.825154105054075,22.985164756886352,23.25006678072171,23.513378499982501,23.624497859980398,23.72471031061216,23.954574879405691,24.226613183542757,24.521924495449934,24.752620167565013,24.871397097861468,25.127647611039166,25.43300195010675,{"$f":"($BB99-$AR99)/10+AR99","v":25.251969841122818},25.070937732138887,24.889905623154956,24.708873514171025,24.527841405187093,24.346809296203162,24.165777187219231,23.984745078235299,23.803712969251368,{"$f":"'AEO Data'!$B$33*AM99","v":23.622680860267447},{"$f":"($BQ99-$BB99)/15+BB99","v":23.636443996632064},23.65020713299668,23.663970269361297,23.677733405725913,23.69149654209053,23.705259678455146,23.719022814819763,23.732785951184379,23.746549087548996,23.760312223913612,23.774075360278228,23.787838496642845,23.801601633007461,23.815364769372078,{"$f":"'AEO Data'!$C$33*BB99","v":23.829127905736687},23.813082557250695,23.797037208764703,23.780991860278711,23.764946511792719,{"$f":"'AEO Data'!$D$33*BQ99","v":23.748901163306734},{"$f":"+BV99*BW$141/BV$141","v":23.75607712303141},{"$f":"+BW99*BX$141/BW$141","v":23.763255251041588},23.770435547992431,23.777618014539303,23.78480265133777,23.782112772933441,23.779423198733689,23.776733928704111,23.774044962810308,23.771356301017885,23.76057340337865,23.749795396957229,23.739022279534925,23.728254048894051,23.717490702817912,23.704286288042756,23.691089224659521,23.677899508575415,23.664717135699917,23.651542101944788,23.633491650128491,23.615454974107841,23.597432063369389,23.579422907407711,23.561427495725386,23.544508396580287,23.52760144678038,23.510706637601409,23.493823960325379,23.476953406240558]
[{"$f":"'HyARC Physical Property Data'!A78","v":"Residential Electricity"},2012,1.0573833607504113,{"$f":"'HyARC Physical Property Data'!$H$78","v":"kWh"},"Feed Utility Byprod",null,null,29.496230857142855,29.496230857142855,29.496230857142855,29.496230857142855,30.858878857142852,29.96898628571428,28.680495999999998,{"$f":"O116*($C100)","v":36.958599009222638},36.829914396835953,35.967931251618772,36.384210392145889,36.946828217650761,37.180918090353856,37.557365599681496,37.974121620104306,38.254262652934798,38.221123201025513,38.131149393475901,37.858692365527979,37.743955697052961,38.1089157935494,38.215330854975328,38.326908061968432,38.563554687637811,38.678694219173288,38.832728540250606,39.103972749483745,39.394125087973819,39.478120450001747,39.513366209565646,39.723129920671305,39.988020313289695,40.267543834237514,40.49663228364426,40.571116482342241,40.796195334045009,41.063070435231531,{"$f":"($BB100-$AR100)/10+AR100","v":40.855881419218811},40.648692403206091,40.441503387193372,40.234314371180652,40.027125355167932,39.819936339155213,39.612747323142493,39.405558307129773,39.198369291117054,{"$f":"'AEO Data'!$B$33*AM100","v":38.991180275104313},{"$f":"($BQ100-$BB100)/15+BB100","v":39.013897465177614},39.036614655250915,39.059331845324216,39.082049035397517,39.104766225470819,39.12748341554412,39.150200605617421,39.172917795690722,39.195634985764023,39.218352175837325,39.241069365910626,39.263786555983927,39.286503746057228,39.309220936130529,{"$f":"'AEO Data'!$C$33*BB100","v":39.331938126203802},39.305453957065893,39.278969787927984,39.252485618790075,39.226001449652166,{"$f":"'AEO Data'!$D$33*BQ100","v":39.199517280514264},{"$f":"+BV100*BW$142/BV$142","v":39.182257585250959},{"$f":"+BW100*BX$142/BW$142","v":39.165005489496558},39.147760989904967,39.130524083131569,39.113294765833224,39.08196562754182,39.050661583400931,39.01938261331054,38.988128697186724,38.956899814961638,38.913880279614062,38.870908250110908,38.827983673992158,38.785106498855733,38.74227667235742,38.695581694263772,38.64894299631591,38.60236051068096,38.555834169607792,38.509363905426945,38.455539205026732,38.401789735637358,38.348115392108113,38.294516069435261,38.24099166276185,38.188742312821311,38.136564352100841,38.084457683060059,38.032422208291884,37.980457830522298]
[]
[]
["AEO 2014 Reference Case Values:"]
["2012 $/MMBtu"]
[]
["Residential Natural Gas",null,null,null,null,null,null,null,null,null,null,null,null,null,10.979644,10.458463,10.386789,11.197535999999999,10.997512,10.684602,11.01057,11.455973999999999,11.627091999999999,11.591965,11.804651,11.896172,12.056948999999999,12.305148000000001,12.475469,12.579926,12.716393999999999,12.897914999999999,13.184208999999999,13.502886999999999,13.64997,13.712135,13.943460999999999,14.339456999999999,14.605688000000001,14.994783,15.152347000000001,15.279963,15.618371,15.977807]
["Commercial Natural Gas",null,null,null,null,null,null,null,null,null,null,null,null,null,8.9608349999999994,8.1128640000000001,8.3120530000000006,9.0860579999999995,8.9185510000000008,8.7230709999999991,9.0072580000000002,9.4091780000000007,9.5464699999999993,9.490774,9.6849690000000006,9.7584820000000008,9.8987529999999992,10.127039999999999,10.286922000000001,10.380953999999999,10.496881999999999,10.657225,10.911016,11.192325,11.294316,11.292712999999999,11.478382999999999,11.747921,11.953430000000001,12.263629999999999,12.368285999999999,12.459205000000001,12.755896,13.077387]
["Industrial Natural Gas",null,null,null,null,null,null,null,null,null,null,null,null,null,5.093718,3.77142,4.594805,4.7995720000000004,4.9392990000000001,5.148549,5.425808,5.8458810000000003,5.9476060000000004,5.7923239999999998,5.9347989999999999,5.9545320000000004,6.0522600000000004,6.2273719999999999,6.3209530000000003,6.356109,6.4293370000000003,6.531498,6.7357209999999998,6.9891050000000003,7.1038509999999997,7.224164,7.420331,7.5726420000000001,7.7575940000000001,8.0432100000000002,8.0942129999999999,8.1302479999999999,8.3372609999999998,8.5934050000000006]
[{"$f":"'HyARC Physical Property Data'!$A$74","v":"Electric Utility Natural Gas"},null,null,null,null,null,null,null,null,null,null,null,null,null,4.881901,3.4378730000000002,4.3206319999999998,4.4694140000000004,4.4284980000000003,4.4748020000000004,4.6905669999999997,5.0621029999999996,5.1794200000000004,5.0744109999999996,5.242337,5.2943420000000003,5.4200609999999996,5.622217,5.7577170000000004,5.8140010000000002,5.9051999999999998,6.0276690000000004,6.2437040000000001,6.4934279999999998,6.6170710000000001,6.726566,6.9305599999999998,7.0909170000000001,7.286816,7.5708000000000002,7.630439,7.6782940000000002,7.8974500000000001,8.1587669999999992]
["Woody Biomass"]
["Metallurgical Coal",null,null,null,null,null,null,null,null,null,null,null,null,null,7.1348120000000002,7.25,7.4339180000000002,7.5123340000000001,7.7593930000000002,7.9480709999999997,8.0483750000000001,8.1909299999999998,8.3009920000000008,8.4282590000000006,8.5261879999999994,8.6333680000000008,8.7384330000000006,8.8454820000000005,8.9517559999999996,9.0441529999999997,9.1489940000000001,9.2665970000000009,9.3802029999999998,9.5131180000000004,9.5927720000000001,9.6736090000000008,9.7592280000000002,9.8373989999999996,9.9349030000000003,10.012817,10.10066,10.107113,10.135842,10.197044999999999]
["Other Industrial Coal",null,null,null,null,null,null,null,null,null,null,null,null,null,3.3073760000000001,3.2396150000000001,3.3150900000000001,3.2817340000000002,3.3761420000000002,3.437208,3.4609869999999998,3.5206819999999999,3.5610849999999998,3.5932520000000001,3.6143869999999998,3.6395840000000002,3.6651829999999999,3.697009,3.7274949999999998,3.7560980000000002,3.7847550000000001,3.8163930000000001,3.8450039999999999,3.8844850000000002,3.9155440000000001,3.944798,3.9761479999999998,4.0004489999999997,4.0294249999999998,4.0600360000000002,4.0903939999999999,4.1171660000000001,4.1493070000000003,4.1898999999999997]
["Electric Utility Steam Coal",null,null,null,null,null,null,null,null,null,null,null,null,null,2.4223750000000002,2.39,2.37385,2.329834,2.4039359999999999,2.422212,2.4863749999999998,2.5503130000000001,2.589102,2.6113439999999999,2.6429999999999998,2.675691,2.7024710000000001,2.7390279999999998,2.7738589999999999,2.807261,2.8368190000000002,2.8649870000000002,2.8913859999999998,2.9256030000000002,2.9494180000000001,2.9743849999999998,3.0006210000000002,3.0244930000000001,3.050074,3.076149,3.099027,3.1208209999999998,3.153797,3.1896749999999998]
["Commercial Electricity",null,null,null,null,null,null,null,null,null,null,null,null,null,30.531154999999998,29.553346999999999,29.462689999999998,29.619807999999999,29.992000999999998,30.137812,30.368880999999998,30.723389000000001,31.014326000000001,30.799534000000001,30.631943,30.294862999999999,30.159492,30.497467,30.549484,30.628119000000002,30.831617000000001,30.906943999999999,31.016119,31.259630000000001,31.506346000000001,31.548763000000001,31.537307999999999,31.727125000000001,31.983875000000001,32.252009999999999,32.456364000000001,32.526015999999998,32.747635000000002,33.007354999999997]
["Industrial Electricity",null,null,null,null,null,null,null,null,null,null,null,null,null,20.348036,19.495602000000002,20.081951,19.872589000000001,20.106300000000001,20.110336,20.286434,20.591933999999998,20.859487999999999,20.769625000000001,20.751276000000001,20.654140000000002,20.663025000000001,20.946209,21.079236999999999,21.236912,21.461658,21.586451,21.737777999999999,21.988303999999999,22.237325999999999,22.342414999999999,22.437189,22.654578999999998,22.911854000000002,23.191139,23.409314999999999,23.521646,23.76399,24.052772999999998]
["Residential Electricity",null,null,null,null,null,null,null,null,null,null,null,null,null,34.952885000000002,34.831184,34.015979999999999,34.409668000000003,34.941752999999999,35.163139000000001,35.519157,35.913296000000003,36.178234000000003,36.146892999999999,36.061802,35.804130999999998,35.695621000000003,36.040774999999996,36.141415000000002,36.246937000000003,36.470740999999997,36.579631999999997,36.725307000000001,36.981831,37.256236999999999,37.335673999999997,37.369007000000003,37.567386999999997,37.817901999999997,38.082256000000001,38.298912000000001,38.369354000000001,38.582217999999997,38.834609999999998]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["AEO_2017_Reference_Case","Prices are in $(2012)/GJ LHV",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Values are extrapolated based on PNNL GCAM model for years 2050-2100"]
["Year","Source Data Year","Reference year Conversion","Display Units","Use Category","LHV (MJ/kg)","HHV (MJ/kg)",2004,{"$f":"+H131+1","v":2005},{"$f":"+I131+1","v":2006},2007,2008,2009,2010,2011,2012,2013,2014,2015,2016,2017,2018,2019,2020,2021,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,2033,2034,2035,2036,2037,2038,2039,2040,2041,2042,2043,2044,2045,2046,2047,2048,2049,2050,2051,2052,2053,2054,2055,2056,2057,2058,2059,2060,2061,2062,2063,2064,2065,2066,2067,2068,2069,{"$f":"+BU131+1","v":2070},2071,2072,2073,2074,2075,2076,2077,2078,2079,2080,2081,2082,2083,2084,2085,2086,2087,2088,2089,2090,2091,2092,2093,2094,2095,2096,2097,2098,2099,2100]
["Feedstock Type"]
["Residential Natural Gas",2016,{"$f":"VLOOKUP(ref_year,DeflatorTable,2,FALSE)/VLOOKUP(B133,DeflatorTable,2,FALSE)","v":1},"mmBtu","Feed Utility",47.141269049911173,52.224661236371581,13.604875014867702,15.571757228276402,16.331995797204218,15.155672177020728,15.783516201764996,13.69149010361817,12.691188457250465,12.04142243701838,11.415954621928984,10.886628367710442,11.368469484946878,9.7183315387998359,9.390001099467705,10.023002570479671,10.033707215541167,10.158951752324048,10.289627280447673,10.38663350570965,10.458822090960101,10.541361785535555,10.671303703310535,10.821196220864106,10.961130973142659,11.387951919139837,11.524366479125279,11.653679994237272,11.727599293307653,11.827238554162054,11.877874728924342,11.891573527850655,11.9827791131466,12.163475682807357,12.259449735369497,12.356256919064013,12.41256198723101,12.490714236969412,12.496378391289182,12.55376491863939,12.651412816002184,12.770777096192051,12.886454368298935,13.010888521557151,13.118997475015544,13.217679440712152,13.363983523149482,13.453606254075613,13.593337225701765,13.668907227280409,13.744897348292845,13.821309924326409,13.898147303952761,13.975411848800078,14.050424531225174,14.12583984239463,14.201659943408417,14.277887006966159,14.354523217429389,14.422221698840277,14.490239458315362,14.558578001626712,14.627238841647882,14.696223498387408,14.75529333521281,14.814600596681556,14.874146237095607,14.933931214592636,14.993956491161448,15.043740835540882,15.093690478582264,15.143805969125756,15.19408785783383,15.244536697197322,15.277067444573643,15.309667610230484,15.342337342301477,15.375076789236356,15.407886099801638,15.41853907481957,15.42919941527855,15.439867126271025,15.450542212892964,15.461224680243861,15.464845562477739,15.468467292690251,15.472089871079984,15.475713297845573,15.479337573185701,15.484830510437597,15.490325396891745,15.49582223323983,15.501321020173785,15.506821758385787,15.515287417782641,15.523757698847955,15.532232604104841,15.540712136077792,15.549196297292674]
["Commercial Natural Gas",2016,1,"mmBtu","Feed Utility",47.141269049911173,52.224661236371581,11.934322920018829,13.90423046997279,14.274140536522257,13.139550648884942,13.897221248926272,11.345666428533674,10.551848524158197,9.7270239269114924,8.6825570363966911,8.5236392646415098,9.2232797097563566,7.6085885488542795,6.813801352724405,7.4731047451509687,7.9843107853990691,8.5650780622071245,9.1477570858798014,9.2514909161219876,9.3094669856386769,9.3761326413005577,9.4891655040111615,9.6143446414218783,9.7258827967425425,10.087086372666475,10.198695614261233,10.304737378868989,10.357640731866367,10.427655972763532,10.453569289213085,10.441948105124277,10.506270757192036,10.658282593530579,10.722901912315555,10.786351624937444,10.817805879498341,10.86596540847121,10.838793391061706,10.868085675073171,10.937640276914211,11.027299024885883,11.114692490256441,11.212257927541287,11.293368314098968,11.35816487466068,11.46581792814789,11.521194135666732,11.628119265707223,11.692763949840026,11.757768015837698,11.823133461626696,11.888862296240635,11.954956539882032,12.019124477688386,12.083636835336717,12.148495461492134,12.213702214742405,12.279258963651227,12.337170130194249,12.395354416085945,12.453813109405683,12.512547504307637,12.571558901049444,12.622088884688262,12.672821967979766,12.723758967260437,12.774900702147928,12.826247995554251,12.868834910334423,12.911563226193937,12.954433412625956,12.997445940682496,13.040601282979605,13.06842899033459,13.096316080020177,13.124262678753999,13.152268913524093,13.180334911589481,13.189447763127433,13.198566915268799,13.207692372369801,13.216824138789674,13.225962218890665,13.22905962240266,13.232157751299196,13.23525660575015,13.23835618592544,13.241456491995026,13.246155303510076,13.250855782427021,13.255557929337549,13.260261744833558,13.264967229507157,13.272208990341527,13.279454704679821,13.286704374680379,13.293958002502723,13.30121559030755]
["Industrial Natural Gas",2016,1,"mmBtu","Feed Utility",47.141269049911173,52.224661236371581,8.2641705904266125,10.495609596381577,9.3614571685358463,8.8987432965993278,10.965509816201024,6.0111731674040234,6.1171751211856922,5.6004077154944953,4.1590520124961925,4.894763142071362,5.8241384234641265,3.5390282601113117,3.3168400539876552,3.8686572087168831,4.230424735748624,4.6374903322667231,5.0398775041324821,5.0452222441273262,4.9894479534735598,5.0008757828968315,5.0866427943161305,5.1985543895300337,5.3142743134013735,5.4069765017212355,5.498883471588238,5.5761078084954727,5.5953977798334869,5.6194116710392619,5.6053299540498323,5.5496627667157004,5.5482476759527453,5.6344516310034729,5.6381945602887429,5.6485162872871211,5.6430123140383071,5.6644386648670784,5.6215300420072483,5.6260767200982693,5.6802473044084865,5.7631623345111542,5.819991545472468,5.8947240715184783,5.9518546882819487,6.0145186606208574,6.1247620979360331,6.1606322318436177,6.238633778680942,6.2733164733478626,6.3081919809530058,6.3432613734093088,6.3785257285888406,6.4139861303559274,6.4484130445592944,6.4830247443854354,6.5178222216666768,6.5528064735589808,6.5879785025705191,6.6190485794679574,6.6502651883672899,6.6816290203394662,6.7131407697146503,6.7448011340975915,6.7719111125525773,6.7991300565526132,6.8264584040725946,6.8538965948478108,6.8814450703810159,6.904293491437457,6.9272177759701634,6.9502181758681845,6.9732949438569127,6.996448333500866,7.0113782521851409,7.0263400302445289,7.0413337356646508,7.0563594365762032,7.0714172012552687,7.0763063619291211,7.0811989029567863,7.0860948266754322,7.090994135423843,7.0958968315424205,7.0975586278944007,7.0992208134244059,7.1008833882235782,7.1025463523830812,7.1042097059940996,7.1067306780935082,7.1092525447752264,7.1117753063567024,7.1142989631554965,7.1168235154892816,7.1207088122192239,7.1245962300542702,7.1284857701523974,7.1323774336722154,7.1362712217729669]
["Electric Utility Natural Gas",2016,1,"mmBtu","Feed Utility",47.141269049911173,52.224661236371581,8.4160389626855991,10.630483084185546,10.241695834954719,9.4549147526367854,10.431438353650302,7.3081429877632402,6.8860004096407268,6.1462564207083838,5.0701845410069568,5.147940545971605,5.9174075441245835,4.3672641892083037,3.755553639162041,3.3468214009493336,3.6078009129373227,3.9595869792693468,4.2992239274502966,4.3362295461094007,4.2972619462853157,4.3209431537283329,4.4388231525151278,4.5598555906037213,4.6705511366221319,4.7905826799714895,4.8909868291351355,4.9795195705251665,5.0140428564929254,5.034241784322349,5.0303794300966009,4.9817061843162831,5.005816752854825,5.1117353012541518,5.1218001698488047,5.1563490468752367,5.1654177598155924,5.1952502995101684,5.1548078964528896,5.1691436283950809,5.2239208155775625,5.3036701369405987,5.3698761013633396,5.4477553798092231,5.5105548899774046,5.5735610242489493,5.6745566112130543,5.7069198222653581,5.8107835034348891,5.8430876323795795,5.8755713510037442,5.9082356577077126,5.9410815564422617,5.974110056739474,6.006175946840397,6.0384139498247791,6.0708249895043265,6.1034099946492821,6.1361698990150408,6.1651091662794615,6.1941849162690321,6.2233977926605295,6.2527484421664239,6.2822375145491964,6.3074882699506478,6.3328405179567433,6.3582946665057261,6.3838511251755019,6.4095103051902287,6.4307917640583545,6.4521438836275307,6.473566898512062,6.4950610441052419,6.5166265565819383,6.5305325700258869,6.5444682579046409,6.5584336835413142,6.5724289103941489,6.5864540020568016,6.5910078603528843,6.5955648671755291,6.6001250247016205,6.6046883351095476,6.6092548005792047,6.6108026296665843,6.6123508212418631,6.6138993753899316,6.6154482921957012,6.6169975717441041,6.6193456536491393,6.6216945687853457,6.6240443174483996,6.6263948999340831,6.6287463165382841,6.6323651566473876,6.6359859723945851,6.6396087648584388,6.6432335351180996,6.6468602842533091]
["Ethanol",2016,1,"gallons","Feed Utility",null,null,null,null,null,null,null,null,null,null,null,null,null,27.998010633548642,27.568794266352821,27.568794266352821,36.135525279048387,36.037261504206917,36.337007617833024,36.652537032081327,36.507370404014004,35.814991403627182,35.344845249766706,35.093839856000677,33.951344964462741,33.728317364797284,33.231596652847486,33.004297255059264,32.448516450458627,30.815236659478707,31.041356345576048,31.071544546844798,31.110040402020914,31.143817410433492,31.179755153943066,30.752314563292465,30.012734677252613,30.324526268143508,30.035968788554065,31.293355180765982,31.295727022165543,31.296025054592718,31.301613162602152,31.660506295003675,31.055935098471778,30.462962330563911,29.883984668715232,29.295445133161515,28.669316257730994,28.70046965895181,28.731656912895144,28.762878056346903,28.794133126132998,28.825422159119345,28.856745192211925,28.888102262356831,28.91949340654028,28.950918661788695,28.982378065168749,29.013871653787358,29.045399464791785,29.076961535369652,29.108557902748995,29.1401886041983,29.171853677026547,29.203553158583262,29.235287086258548,29.267055497483163,29.298858429728512,29.330695920506734,29.362568007370712,29.394474727914172,29.426416119771645,29.458392220618595,29.490403068171396,29.522448700187429,29.554529154465094,29.586644468843872,29.618794681204349,29.650979829468291,29.683199951598645,29.715455085599643,29.747745269516795,29.780070541436949,29.812430939488344,29.844826501840682,29.87725726670508,29.909723272334233,29.942224557022374,29.974761159105356,30.007333116960684,30.039940469007583,30.072583253706998,30.105261509561693,30.137975275116265,30.170724588957185,30.203509489712854,30.236330016053664,30.269186206692016]
["Woody Biomass",2016,1,"kg","Feed Utility",19.551069237418005,20.588656379262464,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.0967849132778742,5.1179587571540939,5.1392205646528959,5.1605707012062227,5.1820095337641501,5.2035374308011946,5.2223240063357927,5.2411784079262249,5.2601008804480855,5.2790916696610548,5.2981510222120916,5.3113630812048802,5.3246080872582748,5.3378861225327325,5.3511972693935945,5.3645416104115968,5.3779717491778074,5.3914355103185612,5.4049329780075288,5.4184642366291094,5.4320293707789578,5.4450858323773135,5.458173676572823,5.471292978796904,5.4844438146622805,5.4976262599634209,5.509165721372697,5.5207294039936956,5.5323173586664938,5.5439296363378796,5.5555662880615797,5.5698816197819898,5.5842338386011479,5.598623039568059,5.6130493179766479,5.6275127693663878,5.6395580019552014,5.6516290163830023,5.6637258678337163,5.6758486116093856,5.6879973031304223,5.6991168854631553,5.7102582056949531,5.7214213063216786,5.732606229922272,5.7438130191589121,5.7570440466225028,5.7703055521130002,5.7835976058373566,5.796920278164249,5.8102736396244499]
["Electric Utility Steam Coal",2016,1,"kg","Feed",22.7322030001394,23.967615189707661,{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},{"$error":"#N/A"},2.2148742453355847,2.3408877437334223,2.3629142410275352,2.4181318326423913,2.3501923436687169,2.2749877363600257,2.2671813119268305,2.0920368648072634,1.9706687398025258,2.067600203211962,2.1142782942327232,2.1573963846468813,2.1900363582596567,2.1929897559939948,2.2028650611910647,2.2090827406317772,2.2092997907220093,2.2079918032786887,2.2065492258230841,2.1995552842692714,2.1903510334996437,2.1795345460335755,2.1771697426487315,2.177831318906295,2.1809505846135182,2.1861806387528246,2.1973402359685172,2.2020565733003745,2.2177912831167257,2.2206593773221517,2.2289385587115755,2.2351116907538557,2.2481536525075447,2.2492673374683427,2.2496910116619402,2.2544263053335558,2.2540196918457411,2.2546357728878843,2.2490256441364247,2.2531477002168603,2.2540841434009193,2.2596705767276806,2.2620458060993922,2.2703711301923084,2.2787270951418623,2.2871138137198912,2.2955313991132824,2.3039799649255008,2.3125787529279784,2.3212096328567045,2.3298727244834101,2.338568148026833,2.3472960241543843,2.3559838582312191,2.3647038478010849,2.3734561118781943,2.3822407699172565,2.3910579418151077,2.3997099382358895,2.4083932417365861,2.4171079656012542,2.4258542235238663,2.434632129609795,2.4428635118796533,2.4511227240845761,2.4594098603163279,2.467725014984794,2.476068282819055,2.4831576550549128,2.4902673252765117,2.4973973516001715,2.5045477923086086,2.5117187058514112,2.5171937058097216,2.5226806400759916,2.5281795346644143,2.5336904156458884,2.539213309148141,2.5429573704375228,2.5467069523323964,2.5504620629728754,2.554222710511076,2.5579889031111347,2.5592501421168059,2.5605120029875006,2.5617744860298348,2.5630375915505756,2.564301319856642,2.5624850697467836,2.5606701060553489,2.5588564278711901,2.5570440342838041,2.555232924383334]
["Commercial Electricity",2016,1,"kWh","Feed Utility Byprod",null,null,28.373013628420669,29.17093293229123,30.878569780545078,30.682595180991225,31.992353762541459,31.4429334181984,31.156600892671783,30.676058322376605,29.679126186318804,29.700131988890092,30.54196479432273,29.932211922183079,28.972214109999999,29.128232055928784,28.995688380521983,29.39475155821113,29.885964346916182,30.089071101439163,31.081689502737298,31.400245105473072,31.337976372818122,31.854564117923594,32.189964324168578,32.274661250208517,32.347049824843424,32.398275541772193,32.473329377777105,32.424485524938959,32.33705604252286,32.213589610409308,32.123147965605618,32.189031672252469,32.20134665837643,32.137342472816606,32.106067355666433,32.055398007309563,31.985796962436115,31.883579639374592,31.88043762605966,31.921825950470875,31.967798865652629,32.011030694105337,32.04019407500644,32.084258086774547,32.12290532445671,32.1438833578502,32.210559439498944,32.212518425109167,32.214477529861206,32.216436753762309,32.218396096819724,32.220355559040698,32.225068562587758,32.229782255525173,32.234496637953782,32.239211709974448,32.243927471688032,32.234738373564198,32.225551894213289,32.216368032888994,32.207186788845206,32.198008161336034,32.188328675270981,32.178652099089362,32.168978431916393,32.15930767287756,32.14963982109861,32.135484213462775,32.121334838594358,32.107191693749044,32.093054776183735,32.078924083156537,32.05322936592912,32.027555229768936,32.001901658190874,31.976268634723027,31.950656142906677,31.915373500092528,31.880129819385399,31.844925057760001,31.809759172238564,31.774632119890772,31.736335048107414,31.698084134709202,31.659879324062725,31.621720560601634,31.583607788826551,31.539463246970023,31.495380406125889,31.451359180054389,31.407399482636293,31.363501227872742,31.320648715953933,31.277854754187555,31.235119262575491,31.192442161228929,31.1498233703682]
["Industrial Electricity",2016,1,"kWh","Feed Utility Byprod",null,null,18.232352698801531,19.279059481202857,20.106975671052609,20.31728323383771,21.702415417864383,21.137326303769196,20.699724047437488,20.430734156114106,19.619402543384187,19.94482547791937,20.190684361237558,19.439058682545589,18.777772519999996,19.537493744407882,19.094688812726531,19.340880484069093,19.700726786066333,19.809231927025674,20.448628319255093,20.513438149254636,20.459361398826221,20.950622526197662,21.163384692376518,21.285322295688569,21.423623959296947,21.53228264660833,21.607771530610695,21.635145433038627,21.585785019942069,21.508628925857963,21.446118499871098,21.521952389257063,21.600204159779199,21.583872325260458,21.588666383585327,21.605374501448264,21.554715579078266,21.491324631109631,21.516251270074765,21.58191413536343,21.663232093841465,21.742367229796333,21.822824570449338,21.895024529503647,21.976239175929997,22.046603213478718,22.114819497732821,22.13487665280584,22.15495199882406,22.175045552285859,22.195157329704575,22.215287347608523,22.237407284551185,22.259549246489641,22.281713255354351,22.303899333097611,22.326107501693581,22.336823207612067,22.347544056673097,22.358270051345187,22.369001194098043,22.379737487402554,22.390100389733625,22.400468090590362,22.410840592194713,22.421217896769658,22.431600006539206,22.438377931004013,22.44515790348412,22.451939924598356,22.458723994965737,22.465510115205461,22.462969438648798,22.46042904942313,22.45788894749596,22.455349132834797,22.452809605407158,22.442624812220661,22.432444638946507,22.422269083489063,22.412098143753649,22.401931817646531,22.389459823741635,22.376994773462549,22.364536662943497,22.352085488320853,22.339641245733144,22.322592014179389,22.305555794307125,22.288532576186064,22.271522349893491,22.254525105514261,22.238544472899552,22.222575315731635,22.206617625770171,22.190671394780733,22.174736614534808]
["Residential Electricity",2016,1,"kWh","Feed Utility Byprod",null,null,31.081820315099751,31.795307521355493,33.946842042036877,33.862138723062856,35.110516897292094,35.620882248372396,35.284315436843215,35.109707376782602,34.944303180720262,35.113313940081568,35.603854676435802,35.586699324775935,34.861101349999998,34.664653819323334,34.410290069910978,34.908531869398402,35.616671532127199,35.947520321196222,36.987705865849776,37.546039262370911,37.510823122184988,38.008797637281816,38.419808048103611,38.480927078752217,38.529894147798792,38.610432052895767,38.669048846696292,38.631731396248163,38.567872226687491,38.465126969563705,38.413723063041203,38.515467425425761,38.527084818246614,38.521472793861179,38.546973809920992,38.560691565187064,38.568356561168315,38.569368829711408,38.651143635977618,38.781520601750053,38.929117506558889,39.08758776785308,39.228047610742941,39.393119417357944,39.595269824540118,39.769550621009692,39.980674011616443,39.983105560972888,39.985537258211586,39.987969103341534,39.990401096371727,39.99283323731116,39.998683153044055,40.00453392446812,40.010385551708517,40.016238034890421,40.022091374139045,40.01068560090993,39.999283078177193,39.987883805014484,39.976487780495717,39.965095003695069,39.953080546830584,39.941069701797218,39.929062467509169,39.917058842880955,39.905058826827435,39.887488478960996,39.869925867384971,39.852370988693046,39.8348238394804,39.817284416343718,39.785391393336162,39.75352391614198,39.721681964299371,39.689865517362925,39.658074554903607,39.614280722534119,39.57053525105394,39.526838087058842,39.48318917720357,39.439588468201791,39.392053039782866,39.344574904480901,39.297153993242112,39.249790237095944,39.202483567154964,39.147690090479308,39.092973198877175,39.038332785305279,38.983768742869955,38.929280964826951,38.876091192919297,38.822974095147039,38.769929572214203,38.716957524960492,38.66405785436109]

{"sheet":"Non-Energy Material Prices","index":12,"n_rows":8,"n_cols":104,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
["Other Inputs and Byproducts","Units","Source Data Year","Reference Year Conversion - Chemical price indexes are used to update costs to reference year dollars",2001,2002,2003,2004,2005,2006,2007,2008,2009,2010,2011,2012,2013,2014,2015,2016,2017,2018,2019,2020,2021,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,2033,2034,2035,2036,2037,2038,2039,2040,2041,2042,2043,2044,2045,2046,2047,2048,2049,2050,2051,2052,2053,2054,2055,2056,2057,2058,2059,2060,2061,2062,2063,2064,2065,2066,2067,2068,2069,2070,{"$f":"+BV1+1","v":2071},{"$f":"+BW1+1","v":2072},2073,2074,2075,2076,2077,2078,2079,2080,2081,2082,2083,2084,2085,2086,2087,2088,2089,2090,2091,2092,2093,2094,2095,2096,2097,2098,2099,2100]
["Cooling Water","gal",2005,{"$f":"VLOOKUP(ref_year,Chemical_price_indexes,2,FALSE)/VLOOKUP(C2,Chemical_price_indexes,2,FALSE)","v":1.4260544580886279},{"$f":"0.000079485*($D$2)","v":1.1334993860117458E-4},1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,{"$f":"0.000079485*($D$2)","v":1.1334993860117458E-4},1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,{"$f":"0.000079485*($D$2)","v":1.1334993860117458E-4},1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,{"$f":"+BV2","v":1.1334993860117458E-4},{"$f":"+BW2","v":1.1334993860117458E-4},1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4,1.1334993860117458E-4]
["Demineralized Water","gal",2005,1.4260544580886279,{"$f":"0.0049962*($D$3)","v":7.1248532835024025E-3},7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,{"$f":"0.0049962*($D$3)","v":7.1248532835024025E-3},7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,{"$f":"0.0049962*($D$3)","v":7.1248532835024025E-3},7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,{"$f":"+BV3","v":7.1248532835024025E-3},7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3,7.1248532835024025E-3]
["Process Water","gal",2005,1.4260544580886279,{"$f":"0.0016654*($D$4)","v":2.374951094500801E-3},2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,{"$f":"0.0016654*($D$4)","v":2.374951094500801E-3},2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,{"$f":"0.0016654*($D$4)","v":2.374951094500801E-3},2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3,2.374951094500801E-3]
["Oxygen","kg",2005,1.4260544580886279,{"$f":"0.02*($D$5)","v":2.8521089161772557E-2},2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,{"$f":"0.02*($D$5)","v":2.8521089161772557E-2},2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,{"$f":"0.02*($D$5)","v":2.8521089161772557E-2},2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2,2.8521089161772557E-2]
["Sulfuric Acid","kg",2005,1.4260544580886279,{"$f":"0*($D$6)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"0*($D$6)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"0*($D$6)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
["Steam","kg",2007,1.3138219380226268,{"$f":"0.0135*($D$7)","v":1.7736596163305463E-2},1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,{"$f":"0.0135*($D$7)","v":1.7736596163305463E-2},1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,{"$f":"0.0135*($D$7)","v":1.7736596163305463E-2},1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2,1.7736596163305463E-2]
["Compressed Inert Gas","kg",2002,1.6980292434837889,{"$f":"0.0256*($D$8)","v":4.3469548633185001E-2},4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,{"$f":"0.0256*($D$8)","v":4.3469548633185001E-2},4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,{"$f":"0.0256*($D$8)","v":4.3469548633185001E-2},4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2,4.3469548633185001E-2]

{"sheet":"AEO Data","index":13,"n_rows":929,"n_cols":72,"rows_kept":929,"cut":false,"hidden":false,"merged":[[26,9,26,10],[27,9,28,9],[27,10,28,10],[35,0,36,3],[55,0,55,10],[37,0,37,1],[37,4,37,8],[44,9,47,10],[52,0,52,10],[53,0,54,10],[0,0,0,71],[1,0,2,71],[4,0,4,71],[8,0,8,71],[748,4,748,8],[735,0,735,2],[731,0,731,12],[618,2,618,24],[619,2,619,24],[13,0,13,71],[18,0,18,71],[20,0,20,19],[22,0,22,19],[24,0,24,10],[25,0,25,10],[26,4,36,8]]}
["Hydrogen Analysis Resource Center:  Feedstock and Utility Assumptions"]
["Feedstock and Utility Price Projections for 2001 - 2070 With EIA Units, Year 2005"]
[]
[null,"Units",2001,2002,2003,2004,2005,2006,2007,2008,2009,2010,2011,2012,2013,2014,2015,2016,2017,2018,2019,2020,2021,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,2033,2034,2035,2036,2037,2038,2039,2040,2041,2042,2043,2044,2045,2046,2047,2048,2049,2050,2051,2052,2053,2054,2056,2056,2057,2058,2059,2060,2061,2062,2063,2064,2065,2066,2067,2068,2069,2070]
["Natural Gas Prices (HHV Basis)"]
["Commercial Natural Gas Prices","$(2005)/MMBtu",8.9541000728991982,6.8979457774252282,8.4197996967243682,8.8059982398770913,8.8656468751295598,8.2234977371287847,7.8073426530046319,7.4325694992857168,7.297531685739191,7.1966502441550162,7.2405429268783017,7.2944294079294778,7.4037989917791105,7.5440859727139706,7.6385998163583153,7.6698249061152577,7.596507558282819,7.644327174942454,7.7875295315148705,8.0180296178133954,8.1425457338117244,8.1602542175436898,8.1927349319997838,8.2544961582939571,8.3511330316651513,8.4290329061652454,8.5069327806653394,8.5848326551654335,8.6627325296655275,8.7406324041656216,8.8185322786657157,8.8964321531658097,8.9743320276659038,9.0522319021659978,9.1301317766660848,9.2578200706648097,9.3855083646635347,9.5131966586622596,9.6408849526609846,9.7685732466597095,9.8962615406584344,10.023949834657159,10.151638128655884,10.279326422654609,10.407014716653334,10.534703010652059,10.662391304650784,10.790079598649509,10.917767892648234,11.045456186646948,11.066404719719236,11.087353252791523,11.10830178586381,11.129250318936098,11.150198852008385,11.171147385080673,11.19209591815296,11.213044451225247,11.233992984297535,11.254941517369822,11.27589005044211,11.296838583514397,11.317787116586684,11.338735649658972,11.359684182731248,11.381228672680008,11.402773162628767,11.424317652577527,11.445862142526286,11.467406632475045]
["Industrial Natural Gas Prices","$(2005)/MMBtu",5.2088497969877503,4.0515519538015683,5.7953765594734321,6.3059286733843276,6.3351569917966728,5.6603640970194089,5.2154936812958672,4.824472465605103,4.7214620293311338,4.5987567766657387,4.6224680014376371,4.6768878495918127,4.7861952984108127,4.922351045428587,5.0173813554475863,5.0686005039035118,5.0229759936062797,5.0914502886106439,5.2365480121576597,5.4816269649649545,5.5841408180740668,5.5850370537559959,5.6052826350589937,5.6612136071582997,5.7676752715740598,5.8539244792759346,5.9401736869778095,6.0264228946796843,6.1126721023815591,6.1989213100834339,6.2851705177853088,6.3714197254871836,6.4576689331890584,6.5439181408909333,6.6301673485928063,6.7228927087931387,6.8156180689934711,6.9083434291938035,7.0010687893941359,7.0937941495944683,7.1865195097948007,7.2792448699951331,7.3719702301954655,7.4646955903957979,7.5574209505961303,7.6501463107964627,7.7428716709967951,7.8355970311971275,7.9283223913974599,8.021047751597786,8.0362602680624171,8.0514727845270482,8.0666853009916792,8.0818978174563103,8.0971103339209414,8.1123228503855724,8.1275353668502035,8.1427478833148346,8.1579603997794656,8.1731729162440967,8.1883854327087278,8.2035979491733588,8.2188104656379899,8.234022982102621,8.2492354985672645,8.2648807901462327,8.2805260817252009,8.2961713733041691,8.3118166648831373,8.3274619564621091]
["Electric Utility Natural Gas Prices","$(2005)/MMBtu",5.6269638934579786,3.8422456293735823,5.691139826234779,6.2376343214286925,6.1731978092553481,5.4998161252939477,5.0667498741509744,4.6999946247856554,4.5877827360944901,4.4974766767249967,4.5471429464952013,4.6470168064225401,4.7885290901615907,4.9298490038457894,5.0143193411377212,5.0431599369588911,4.9958503246307417,5.071809156885692,5.2209958625289659,5.4542850660827948,5.5514960671370845,5.5489887943807661,5.5622220646660265,5.6263508841676488,5.730461856104295,5.8123040182474703,5.8941461803906456,5.9759883425338209,6.0578305046769962,6.1396726668201715,6.2215148289633468,6.3033569911065221,6.3851991532496974,6.4670413153928727,6.5488834775360516,6.6404720525202734,6.7320606275044952,6.823649202488717,6.9152377774729388,7.0068263524571606,7.0984149274413824,7.1900035024256042,7.2815920774098259,7.3731806523940477,7.4647692273782695,7.5563578023624913,7.6479463773467131,7.7395349523309349,7.8311235273151567,7.9227121022993829,7.9377381178566102,7.9527641334138375,7.9677901489710647,7.982816164528292,7.9978421800855193,8.0128681956427457,8.0278942111999729,8.0429202267572002,8.0579462423144275,8.0729722578716547,8.087998273428882,8.1030242889861093,8.1180503045433365,8.1330763201005638,8.1481023356577857,8.1635558206357306,8.1790093056136755,8.1944627905916203,8.2099162755695652,8.2253697605475136]
["Electricity Prices"]
["Commercial Electricity","$(2005)/MMBtu",24.866788774356646,24.345010037692106,24.223933219909672,24.020635352944481,23.91295186528621,22.837542614846832,21.69091966017233,21.090846376599046,21.058556043876806,20.987678365887316,20.983490961902529,21.313707333690761,21.638938984780914,22.13258341123478,22.313049388381657,22.486876361774936,22.494946956634521,22.662665807975912,22.922821701697636,23.270139622238439,23.509686568997985,23.493712398241108,23.423848763951703,23.513217827059155,23.645542576627872,23.786749293232678,23.927956009837484,24.06916272644229,24.210369443047096,24.351576159651902,24.492782876256708,24.633989592861514,24.77519630946632,24.916403026071126,25.057609742675933,25.047759076850095,25.037908411024258,25.028057745198421,25.018207079372583,25.008356413546746,24.998505747720909,24.988655081895072,24.978804416069234,24.968953750243397,24.95910308441756,24.949252418591723,24.939401752765885,24.929551086940048,24.919700421114211,24.90984975528837,24.925673674379027,24.941497593469684,24.957321512560341,24.973145431650998,24.988969350741655,25.004793269832312,25.020617188922969,25.036441108013626,25.052265027104283,25.068088946194941,25.083912865285598,25.099736784376255,25.115560703466912,25.131384622557569,25.147208541648205,25.163183242307905,25.179157942967606,25.195132643627307,25.211107344287008,25.227082044946716]
["Industrial Electricity","$(2005)/MMBtu",16.038863482553147,15.36037109932807,15.664056310113844,16.390134465019642,16.26049394877451,15.718549229064077,15.083546116666987,14.764544869368896,14.679648534306921,14.510741661179726,14.370329416023063,14.522587083420669,14.791267903345901,15.142176731577413,15.304996360023072,15.443286072533045,15.485992224711291,15.663456831338236,15.910829809476709,16.241389166634008,16.419768400912066,16.405212897174714,16.372526888577397,16.449089176249931,16.568027554817903,16.704753726753587,16.841479898689272,16.978206070624957,17.114932242560641,17.251658414496326,17.388384586432011,17.525110758367695,17.66183693030338,17.798563102239065,17.935289274174743,17.928238540168429,17.921187806162116,17.914137072155803,17.90708633814949,17.900035604143177,17.892984870136864,17.885934136130551,17.878883402124238,17.871832668117925,17.864781934111612,17.857731200105299,17.850680466098986,17.843629732092673,17.83657899808636,17.829528264080036,17.840854426840831,17.852180589601627,17.863506752362422,17.874832915123218,17.886159077884013,17.897485240644809,17.908811403405604,17.9201375661664,17.931463728927195,17.94278989168799,17.954116054448786,17.965442217209581,17.976768379970377,17.988094542731172,17.999420705491971,18.010854791996724,18.022288878501477,18.033722965006231,18.045157051510984,18.056591138015737]
["Coal Prices (HHV Basis)"]
["Electric Utility Steam Coal","$(2005)/MMBtu",1.3268491834774256,1.32388562245189,1.3334961719108085,1.3380821099821107,1.3443425871291239,1.3528785733681756,1.3415886383011697,1.3403624656065469,1.330997225248586,1.3164209684110997,1.3072140481112184,1.3019573002491378,1.2978333982656636,1.295833644439585,1.2953486183904279,1.2970626753456174,1.2955796364343368,1.3002382724914889,1.3044509032987155,1.3304805103337984,1.3397570218680066,1.3519914094007222,1.3569265463442153,1.3726611244228613,1.3854931266802686,1.3951349014789893,1.4047766762777101,1.4144184510764308,1.4240602258751516,1.4337020006738723,1.4433437754725931,1.4529855502713138,1.4626273250700346,1.4722690998687553,1.481910874667477,1.4862555877963981,1.4906003009253193,1.4949450140542404,1.4992897271831616,1.5036344403120827,1.5079791534410039,1.512323866569925,1.5166685796988462,1.5210132928277673,1.5253580059566885,1.5297027190856096,1.5340474322145308,1.5383921453434519,1.5427368584723731,1.5470815716012942,1.5500157274134729,1.5529498832256516,1.5558840390378303,1.5588181948500091,1.5617523506621878,1.5646865064743665,1.5676206622865452,1.5705548180987239,1.5734889739109026,1.5764231297230813,1.57935728553526,1.5822914413474387,1.5852255971596174,1.5881597529717961,1.5910939087839742,1.5941115372826113,1.5971291657812485,1.6001467942798857,1.6031644227785229,1.6061820512771605]
["Transportation Fuels (HHV Basis)"]
["Distillate (Diesel) Fuel Oil for Transportation","$(2005)/MMBtu",10.789461735918687,9.9590971559848445,11.383831536994775,12.531178240506115,12.036300060884058,12.613383383121093,13.01890940036416,12.908589399085846,12.946875513724528,13.039098811599491,13.088955960183741,13.133508268392355,13.038477461293056,12.989168095138872,12.752903866318045,12.539506322932722,12.335074118848111,12.292193988584152,12.304560350921868,12.340337204483362,12.418707870087554,12.438495640484758,12.492141534697302,12.624332072599859,13.025979869770596,13.053872203635709,13.081764537500822,13.109656871365935,13.137549205231048,13.165441539096161,13.193333872961274,13.221226206826387,13.2491185406915,13.277010874556613,13.304903208421727,13.445726499778688,13.586549791135649,13.72737308249261,13.868196373849571,14.009019665206532,14.149842956563493,14.290666247920454,14.431489539277415,14.572312830634376,14.713136121991337,14.853959413348298,14.994782704705258,15.135605996062219,15.27642928741918,15.417252578776129,15.505038084680947,15.592823590585766,15.680609096490585,15.768394602395404,15.856180108300222,15.943965614205041,16.03175112010986,16.119536626014678,16.207322131919497,16.295107637824316,16.382893143729135,16.470678649633953,16.558464155538772,16.646249661443591,16.734035167348416,16.829318405103567,16.924601642858718,17.019884880613869,17.11516811836902,17.210451356124164]
["Motor Gasoline","$(2005)/MMBtu",12.730520250245322,11.801320287416596,13.477350603859424,15.275134761378448,14.956036086352325,15.333911517881027,14.969645149302909,14.856007634468792,14.855665643260203,14.676357863084307,14.660823111264261,14.621396694543213,14.496914877081778,14.525867813038341,14.406443289990676,14.511791494657368,14.408484301477108,14.421367627269808,14.483474821414545,14.423047758498246,14.678410804496627,14.842794247393387,14.985196801851416,15.125157698145465,15.225733932459173,15.312322281050708,15.398910629642243,15.485498978233778,15.572087326825313,15.658675675416848,15.745264024008383,15.831852372599919,15.918440721191454,16.005029069782989,16.091617418374518,16.26193617174043,16.432254925106342,16.602573678472254,16.772892431838166,16.943211185204078,17.113529938569989,17.283848691935901,17.454167445301813,17.624486198667725,17.794804952033637,17.965123705399549,18.135442458765461,18.305761212131372,18.476079965497284,18.646398718863171,18.752570913712709,18.858743108562248,18.964915303411786,19.071087498261324,19.177259693110862,19.283431887960401,19.389604082809939,19.495776277659477,19.601948472509015,19.708120667358553,19.814292862208092,19.92046505705763,20.026637251907168,20.132809446756706,20.238981641606255,20.354221969500514,20.469462297394774,20.584702625289033,20.699942953183292,20.815183281077545]
["Ethanol","$(2005)/MMBtu",15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999,15.730049999999999]
["Methanol","$(2005)/MMBtu",8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985]
["Biomass (HHV Basis)"]
["Biomass Prices (Dry Biomass Delivered)*","$(2005)/MMBtu",1.2696286520685174,1.2696286520685174,1.2696286520685174,1.2696286520685174,1.2696286520685174,1.2696286520685174,1.2696286520685174,1.2696286520685174,1.2696286520685174,1.2696286520685174,1.2716814065585227,1.2809188017635484,1.3178683825836508,1.3209475143186591,1.3435278137087219,1.3466069454437304,1.3630289813637759,1.3578970951387617,1.383556526263833,1.4030576939188868,1.460534819639046,1.4800359872941,1.4861942507641173,1.5118536818891883,1.5262229633192279,1.6236006669873051,1.7209783706553823,1.8183560743234595,1.9157337779915367,2.0131114816596138,2.1104891853276913,2.2078668889957687,2.3052445926638461,2.4026222963319235,2.5,2.5714285714285716,2.6428571428571432,2.7142857142857149,2.7857142857142865,2.8571428571428581,2.9285714285714297,3,3.071428571428573,3.1428571428571446,3.2142857142857162,3.2857142857142878,3.3571428571428594,3.428571428571431,3.5,3.5714285714285743,3.6428571428571459,3.7142857142857175,3.7857142857142891,3.8571428571428608,3.9285714285714324,4,4.0714285714285747,4.1428571428571459,4.2142857142857171,4.2857142857142883,4.3571428571428594,4.4285714285714306,4.5,4.571428571428573,4.6428571428571441,4.7142857142857153,4.7857142857142865,4.8571428571428577,4.9285714285714288,5]
["* Biomass prices shown for years 2001 through 2009 are the same as the EIA value for 2010.  For the post-2025 biomass prices:  The value for 2035 was chosen based on a review of the literature, which indicated a price of $2.50/MMBtu delivered dry English ton (in 2000$) was a reasonable mid-range projection.  Values for the 2026 through 2034 were interpolated from the 2025 and 2035 values.  The value of $5.00/MMBtu delivered dry English ton in 2065 was based on judgment.  An EIA paper by Zia Haq entitled, “Biomass for Electricity Generation” (available from EIA’s website) indicates that about 7 quads of biomass per year  would be available if the price rose to  $5/MMBtu."]
[]
["Table 1 reflects values for base case feedstock and fuel values, based on the H2A analysis done for DOE's Hydrogen, Fuel Cells and Infrastructure Program.  Values from 2001 through 2025 were derived from EIA AEO 2004, and 2002 dollars are converted to 2005 dollars by multiplying the prices in 2002$/MMBtu by the GDP Implicit Price Deflator for 2005, divided by that for 2002 (from AEO 2004 Table A2; see table 2 below). For the period between 2025 and 2035, the 2025 values were extrapolated based on the ratio of the 2025 and 2015 values. For the period between 2035 and 2070, ratios in Table 2, derived from projections of a long-term model (MiniCAM) developed by Pacific Northwest National Laboratory were used to extrapolate the 2035 values (except for ethanol, methanol and biomass; see footnote)."]
[]
["Hydrogen Analysis Resource Center:  Price Ratios from PNNL GCAM Model"]
[]
[null,"Ratio 2050 to 2035 Price","Ratio 2065 to 2050 Price","Ratio 2070 to 2065 Price",null,null,null,null,null,"GDP Implicit Deflator Price Index [1]"]
["Coal Delivered to Utilities",{"$f":"G40/F40","v":1.0482288241385485},{"$f":"H40/G40","v":1.0526415477404851},{"$f":"I40/H40","v":1.0160295046377366},null,null,null,null,null,"Year","Value"]
["Wellhead Gas",{"$f":"G41/F41","v":1.1441282284851997},{"$f":"H41/G41","v":1.1360328119345371},{"$f":"I41/H41","v":1.0363018547359477}]
["Gas Delivered to Utilities",1.1252277801242987,1.1222249629995065,1.0285793469898747,null,null,null,null,null,1991,84.5]
["Crude Oil Price",1.0687839040840581,1.0213566498986533,1.0031375164207406,null,null,null,null,null,1992,86.4]
["Delivered Diesel",1.03736526166104,1.0084486821562659,1.0010687685088917,null,null,null,null,null,1993,88.4]
["Average Electricity",0.975071533164794,1.0087393571750138,0.99663324890666094,null,null,null,null,null,1994,90.3]
["Dry Biomass at Farmgate",1.0938371922267365,1.0852680569229392,1.0142672175626977,null,null,null,null,null,1995,92.1]
["Ethanol",1.0046194107582356,1.003094645903579,0.99710816742279029,null,null,null,null,null,1996,93.9]
[null,null,null,null,null,null,null,null,null,1997,95.4]
[null,null,null,null,null,null,null,null,null,1998,96.5]
["In Units Consistent with EIA AEO",null,"From AEO","From AEO","From GCAM",null,null,null,null,1999,97.9]
[null,"Units",2000,2005,2020,2035,2050,2065,2070,2000,100]
["Coal Delivered to Utilities","$/English ton",25.276500000000002,25.071000000000002,49.911552427759986,51.73380738099187,54.228868079187265,57.083559627090274,57.998580810871225,2001,102.4]
["Wellhead Gas","$/mcf",3.83,2.88,3.4820792312666162,3.718467288972283,4.254403392012021,4.8331418485312492,5.0085938618348607,2002,104.1]
["Gas Delivered to Utilities","$/mcf",4.333333333333333,3.2058823529411766,5.3135477999345282,5.6703709369749671,6.3804589018936815,7.1603102550975084,7.3649472464330987,2003,106]
["Crude Oil Price","$/bbl",28.35,23.27,38.166254666132858,44.018296607182357,47.046046898954408,48.050792851691,48.201553003292787,2004,108.3]
["Delivered Diesel","$/gallon",1.5176666666666667,1.2925714285714285,1.9428327208531595,2.1262391061548653,2.2056865867102777,2.2243217316177319,2.2266990166381286,2005,110.5]
["Average Electricity","c/kWh",6.9,6.4,7.2674708046079139,7.0885496188632935,6.9118429447797478,6.9722480090117775,6.9487741854044058,"[2]"]
["Dry Biomass at Farmgate","$/mmBtu",null,null,3.9267286033597717,3.4025762910602637,3.7218644965506216,4.0392206503019663,4.0968490901035652]
["Ethanol","$/mmBtu",null,null,24.686324737923844,23.090083577893328,23.196746158381607,23.268531873857007,23.201243175360347]
["Biomass delivery (assuming $10/English ton average delivery price)","$/English ton",null,null,10,10,10,10]
[null,"$/mmBtu HHV",null,null,{"$f":"E48*$B$61","v":0.65713983050847458},{"$f":"F48*$B$61","v":0.65713983050847458},{"$f":"G48*$B$61","v":0.65713983050847458},{"$f":"H48*$B$61","v":0.65713983050847458}]
["Biomass delivered $/mmBtu HHV","$/mmBtu",null,null,{"$f":"E49+E46","v":4.5838684338682461},{"$f":"F49+F46","v":4.0597161215687381},{"$f":"G49+G46","v":4.3790043270590964},{"$f":"H49+H46","v":4.6963604808104407}]
[]
["Note:"]
["[2] values in italics are projections"]
["Source:"]
[]
["[1] Available from Short Term Energy Outlook, Table A.2 at http://www.eia.doe.gov/emeu/steo/pub/a2tab.html"]
[]
["Biomass conversion $/dry English ton to $/mmBtu HHV"]
["Biomass LHV (kJ/kg)",19022]
["Biomass HHV (kJ/kg)",17700]
["Conversion factor",{"$f":"2.205/2000/B60*mmBTU_to_GJ*1000000","v":6.5713983050847455E-2}]
[]
[]
[null,"Report","Annual Energy Outlook 2010"]
[null,"Scenario","aeo2010r",null,null,"Reference case"]
[null,"Datekey","d111809a"]
[null,"Release Date",null," December 2009"]
[]
[]
[]
[]
["aeo2010r.d111809a"]
[]
["Table 3.  Energy Prices by Sector and Source"]
["(2008 dollars per million Btu, unless otherwise noted)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2008-"]
[" Sector and Source",2007,2008,2009,2010,2011,2012,2013,2014,2015,2016,2017,2018,2019,2020,2021,2022,2023,2024,2025,2026,2027,2028,2029,2030,2031,2032,2033,2034,2035,2035]
[]
[" Residential"]
["   Liquefied Petroleum Gases",26.25,29.35,24.9,24.01,24.09,25.25,26.47,27.44,28.03,28.67,29.21,29.8,30.06,30.29,30.53,30.73,31.01,31.28,31.55,31.7,31.98,32.229999999999997,32.590000000000003,32.81,33.17,33.51,33.9,34.26,34.65,6.0000000000000001E-3]
["   Distillate Fuel Oil",20.3,24.47,17.98,17.57,17.72,18.84,19.86,20.58,21.08,22,22.66,23.32,23.74,24.1,24.24,24.44,24.76,24.94,25.23,25.5,25.72,26.04,26.44,26.61,27.05,27.45,27.82,28.24,28.66,6.0000000000000001E-3]
["   Natural Gas",12.94,13.48,11.39,10.89,11.78,11.87,11.48,11.41,11.56,11.65,11.69,11.76,11.83,11.95,12.07,12.26,12.29,12.2,12.29,12.46,12.66,12.9,13.16,13.44,13.78,13.93,14.03,14.25,14.4,2E-3]
["   Electricity",31.82,33.29,32.33,30.94,29.9,31.08,31.47,31.49,31.43,31.64,31.8,31.78,31.68,31.84,32.01,32.08,32.200000000000003,32.28,32.26,32.4,32.57,32.729999999999997,33.130000000000003,33.46,33.81,34.11,34.26,34.49,34.71,2E-3]
[]
[" Commercial"]
["   Liquefied Petroleum Gases",20.65,26.15,19.82,20.78,20.86,22.02,23.23,24.19,24.77,25.41,25.95,26.53,26.79,27.02,27.25,27.46,27.73,28,28.26,28.41,28.68,28.93,29.28,29.5,29.86,30.19,30.58,30.94,31.32,7.0000000000000001E-3]
["   Distillate Fuel Oil",17.48,21.5,15.8,14.82,15.24,16.38,17.399999999999999,18.11,18.72,19.559999999999999,20.2,20.84,21.26,21.6,21.78,22.04,22.29,22.43,22.72,22.97,23.21,23.53,23.93,24.11,24.54,24.94,25.28,25.69,26.13,7.0000000000000001E-3]
["   Residual Fuel",8.39,15.52,9.27,9.4499999999999993,9.6300000000000008,10.85,11.98,12.76,13.13,13.68,14.17,14.69,15.26,15.46,15.68,15.89,16.12,16.34,16.54,16.63,16.82,17.059999999999999,17.28,17.54,17.89,18.12,18.25,18.68,18.84,7.0000000000000001E-3]
["   Natural Gas",11.2,11.94,9.0500000000000007,8.67,9.7200000000000006,10.07,9.92,9.85,9.99,10.08,10.11,10.16,10.23,10.35,10.46,10.65,10.69,10.62,10.7,10.86,11.04,11.28,11.52,11.78,12.11,12.26,12.32,12.52,12.66,2E-3]
["   Electricity",28.81,30.47,28.94,27.37,25.72,26.72,26.81,26.55,26.55,26.81,26.97,26.98,26.93,27.12,27.31,27.42,27.62,27.77,27.72,27.87,28.05,28.25,28.67,28.99,29.37,29.73,29.9,30.15,30.37,0]
[]
[" Industrial 1/"]
["   Liquefied Petroleum Gases",22.01,24.2,18.64,18.36,18.46,19.61,20.9,21.9,22.49,23.25,23.76,24.31,24.62,24.86,25.09,25.3,25.59,25.86,26.12,26.27,26.55,26.8,27.15,27.38,27.74,28.08,28.48,28.86,29.25,7.0000000000000001E-3]
["   Distillate Fuel Oil",18.07,22.31,16.399999999999999,14.38,15.38,16.55,17.59,18.32,19,19.8,20.440000000000001,21.08,21.49,21.83,22.03,22.36,22.56,22.67,22.97,23.22,23.48,23.81,24.22,24.4,24.84,25.25,25.6,26.02,26.48,6.0000000000000001E-3]
["   Residual Fuel Oil",8.84,16.309999999999999,9.75,13.12,13.24,14.32,15.31,16.079999999999998,16.47,16.96,17.37,17.82,18.09,18.2,18.43,18.61,18.82,19.03,19.23,19.3,19.489999999999998,19.73,19.98,20.27,20.61,20.87,21.12,21.44,21.72,1.0999999999999999E-2]
["   Natural Gas 2/",7.58,9.11,4.2,4.87,5.97,6.39,6.33,6.28,6.45,6.52,6.51,6.55,6.6,6.7,6.78,6.96,7.01,6.96,7.02,7.15,7.29,7.51,7.73,7.98,8.2899999999999991,8.4,8.42,8.61,8.73,-2E-3]
["   Metallurgical Coal",3.69,4.49,4.72,4.8,4.8600000000000003,5.0199999999999996,5.05,5.08,5.08,5.09,5.16,5.22,5.29,5.32,5.35,5.36,5.35,5.32,5.24,5.16,5.14,5.14,5.1100000000000003,5.1100000000000003,5.09,5.08,5.08,5.0599999999999996,5.0599999999999996,4.0000000000000001E-3]
["   Other Industrial Coal",2.48,2.84,2.79,2.69,2.69,2.69,2.66,2.68,2.69,2.68,2.69,2.68,2.67,2.66,2.65,2.65,2.63,2.63,2.63,2.64,2.63,2.64,2.65,2.66,2.67,2.67,2.69,2.7,2.71,-2E-3]
["   Coal to Liquids","- -","- -","- -","- -",1.26,1.04,1.04,1.41,1.42,1.46,1.48,1.48,1.47,1.46,1.49,1.5,1.52,1.49,1.49,1.47,1.46,1.45,1.44,1.44,1.44,1.44,1.46,1.48,1.51,"- -"]
["   Electricity",19.02,20.21,20.04,19.149999999999999,17.11,17.73,17.62,17.350000000000001,17.37,17.62,17.75,17.77,17.75,17.920000000000002,18.07,18.190000000000001,18.38,18.53,18.5,18.61,18.78,18.97,19.3,19.579999999999998,19.88,20.16,20.3,20.52,20.71,1E-3]
[]
[" Transportation"]
["   Liquefied Petroleum Gases 3/",23.83,29.93,25.2,23.89,23.98,25.13,26.33,27.29,27.88,28.53,29.07,29.65,29.91,30.13,30.36,30.56,30.83,31.1,31.36,31.5,31.77,32.01,32.36,32.58,32.93,33.26,33.64,34,34.380000000000003,5.0000000000000001E-3]
["   E85 4/",27.43,26.93,23.29,20.64,20.97,22.13,24.21,25.23,25.55,25.08,25.9,26.54,26.68,26.95,27.32,27.82,28.31,28.55,28.86,29.22,29.49,30.03,30.44,30.64,30.86,31.29,31.49,31.77,32.229999999999997,7.0000000000000001E-3]
["   Motor Gasoline 5/",23.66,26.76,19.14,20.55,20.88,22.03,24.02,24.94,25.37,25.94,26.47,26.89,27.2,27.59,27.82,28.18,28.42,28.54,28.87,29.19,29.47,29.9,30.27,30.42,30.77,31.16,31.44,31.81,32.33,7.0000000000000001E-3]
["   Jet Fuel 6/",15.77,22.71,12.73,14.79,15.16,16.54,17.690000000000001,18.46,19.04,19.760000000000002,20.41,20.97,21.35,21.69,21.85,22.09,22.41,22.61,22.92,23.19,23.48,23.9,24.26,24.51,24.9,25.3,25.64,26.05,26.48,6.0000000000000001E-3]
["   Diesel Fuel (distillate fuel oil) 7/",21.55,27.65,17.77,19.12,19.309999999999999,20.51,21.54,22.25,22.93,23.68,24.26,24.91,25.29,25.6,25.79,26.12,26.26,26.34,26.63,26.83,27.09,27.4,27.8,27.96,28.38,28.78,29.09,29.49,29.96,3.0000000000000001E-3]
["   Residual Fuel Oil",9.19,14.49,8.86,10.210000000000001,10.32,11.5,12.44,13.18,13.58,13.9,14.43,14.81,14.97,14.99,15.23,15.34,15.55,15.75,15.93,15.98,16.27,16.5,16.8,17.100000000000001,17.420000000000002,17.690000000000001,17.93,18.239999999999998,18.600000000000001,8.9999999999999993E-3]
["   Natural Gas 8/",13.84,15.96,11.36,12,13.09,13.49,13.36,13.25,13.37,13.41,13.38,13.37,13.38,13.44,13.46,13.58,13.54,13.41,13.43,13.54,13.65,13.83,14,14.19,14.46,14.54,14.55,14.7,14.78,-3.0000000000000001E-3]
["   Electricity",32.03,33.729999999999997,32.299999999999997,30.29,27.63,29.66,29.72,29.07,28.79,29.01,29.04,28.87,28.59,28.55,28.54,28.43,28.48,28.64,28.63,28.88,29.32,29.79,30.51,31.01,31.61,32.15,32.47,32.89,33.26,-1E-3]
[]
[" Electric Power 9/"]
["   Distillate Fuel Oil",15.75,19.37,14.24,13.91,14.06,15.2,16.21,16.89,17.36,18.22,18.88,19.510000000000002,19.920000000000002,20.25,20.399999999999999,20.58,20.89,21.07,21.35,21.6,21.83,22.14,22.54,22.71,23.14,23.54,23.87,24.28,24.7,8.9999999999999993E-3]
["   Residual Fuel Oil",9.0399999999999991,14.56,8.7799999999999994,12,12.17,13.34,14.37,15.11,15.53,15.93,16.45,16.89,17.14,17.22,17.47,17.63,17.850000000000001,18.079999999999998,18.3,18.38,18.68,18.940000000000001,19.23,19.55,19.899999999999999,20.190000000000001,20.43,20.77,21.12,1.4E-2]
["   Natural Gas",7.26,9.09,4.1399999999999997,4.8499999999999996,5.82,6.17,5.94,5.9,6.08,6.16,6.17,6.22,6.29,6.42,6.52,6.69,6.74,6.7,6.75,6.91,7.05,7.27,7.51,7.73,8.02,8.14,8.17,8.35,8.4600000000000009,-3.0000000000000001E-3]
["   Steam Coal",1.8,2.0499999999999998,2.15,1.99,1.98,1.99,1.99,1.99,2.0099999999999998,1.99,2,1.99,1.99,1.98,1.98,1.99,1.99,1.99,1.99,2,2,2.0099999999999998,2.02,2.0299999999999998,2.04,2.0499999999999998,2.06,2.0699999999999998,2.09,1E-3]
[]
[" Average Price to All Users 10/"]
["   Liquefied Petroleum Gases",18.940000000000001,20.190000000000001,18.36,16.850000000000001,16.87,17.87,18.97,19.82,20.3,20.84,21.26,21.71,21.93,22.15,22.36,22.56,22.83,23.09,23.34,23.49,23.75,24,24.34,24.55,24.91,25.25,25.63,25.99,26.37,0.01]
["   E85 4/",27.43,26.93,23.29,20.64,20.97,22.13,24.21,25.23,25.55,25.08,25.9,26.54,26.68,26.95,27.32,27.82,28.31,28.55,28.86,29.22,29.49,30.03,30.44,30.64,30.86,31.29,31.49,31.77,32.229999999999997,7.0000000000000001E-3]
["   Motor Gasoline 5/",23.55,26.54,19.149999999999999,20.55,20.88,22.03,24.01,24.94,25.36,25.93,26.46,26.89,27.2,27.59,27.82,28.17,28.41,28.54,28.87,29.18,29.47,29.9,30.27,30.41,30.76,31.16,31.43,31.81,32.32,7.0000000000000001E-3]
["   Jet Fuel",15.77,22.71,12.73,14.79,15.16,16.54,17.690000000000001,18.46,19.04,19.760000000000002,20.41,20.97,21.35,21.69,21.85,22.09,22.41,22.61,22.92,23.19,23.48,23.9,24.26,24.51,24.9,25.3,25.64,26.05,26.48,6.0000000000000001E-3]
["   Distillate Fuel Oil",20.71,26.27,17.46,17.73,18.149999999999999,19.45,20.62,21.35,22.03,22.8,23.45,24.07,24.47,24.79,24.99,25.32,25.5,25.59,25.89,26.12,26.38,26.71,27.11,27.29,27.73,28.13,28.46,28.87,29.34,4.0000000000000001E-3]
["   Residual Fuel Oil",9.07,14.77,8.9600000000000009,10.9,11.01,12.17,13.13,13.86,14.26,14.63,15.14,15.55,15.76,15.81,16.05,16.190000000000001,16.399999999999999,16.600000000000001,16.8,16.850000000000001,17.13,17.37,17.66,17.96,18.3,18.559999999999999,18.79,19.12,19.46,0.01]
["   Natural Gas",9.19,10.53,6.57,6.87,7.87,8.1999999999999993,8.0500000000000007,8.02,8.14,8.2200000000000006,8.2200000000000006,8.27,8.33,8.44,8.5500000000000007,8.73,8.77,8.68,8.75,8.89,9.0399999999999991,9.26,9.49,9.74,10.050000000000001,10.17,10.210000000000001,10.4,10.54,0]
["   Metallurgical Coal",3.69,4.49,4.72,4.8,4.8600000000000003,5.0199999999999996,5.05,5.08,5.08,5.09,5.16,5.22,5.29,5.32,5.35,5.36,5.35,5.32,5.24,5.16,5.14,5.14,5.1100000000000003,5.1100000000000003,5.09,5.08,5.08,5.0599999999999996,5.0599999999999996,4.0000000000000001E-3]
["   Other Coal",1.84,2.1,2.19,2.0299999999999998,2.02,2.0299999999999998,2.0299999999999998,2.0299999999999998,2.0499999999999998,2.0299999999999998,2.04,2.0299999999999998,2.02,2.02,2.02,2.0299999999999998,2.02,2.02,2.02,2.0299999999999998,2.0299999999999998,2.04,2.0499999999999998,2.06,2.0699999999999998,2.08,2.09,2.1,2.12,0]
["   Coal to Liquids","- -","- -","- -","- -",1.26,1.04,1.04,1.41,1.42,1.46,1.48,1.48,1.47,1.46,1.49,1.5,1.52,1.49,1.49,1.47,1.46,1.45,1.44,1.44,1.44,1.44,1.46,1.48,1.51,"- -"]
["   Electricity",27.25,28.81,28.07,26.77,25.2,26.1,26.17,25.97,25.95,26.2,26.36,26.37,26.31,26.51,26.7,26.84,27.04,27.19,27.17,27.33,27.53,27.74,28.16,28.49,28.86,29.21,29.38,29.64,29.87,1E-3]
[]
["Non-Renewable Energy Expenditures by Sector"]
["(billion 2008 dollars)"]
[" Residential",241.67,254.66,231.65,223.76,222.61,230.62,228.9,229.4,230.89,234.53,236.76,239.14,241.36,245.14,247.96,251.14,253.92,256.67,258.7,262.54000000000002,266.58999999999997,271.26,275.8,280.39999999999998,285.83,290.58999999999997,292.89999999999998,297.16000000000003,301.11,6.0000000000000001E-3]
[" Commercial",176.61,191.19,168.7,163.43,163.69,172.64,173.85,174.18,176.9,180.82,184.11,186.86,189.36,193.15,196.83,200.4,204.1,207.27,210.07,214.23,218.63,223.34,229.36,234.79,240.94,246.37,250.61,256.01,261.07,1.2E-2]
[" Industrial",219.69,244.81,175.42,163.24,173.51,191.66,201.52,207.49,213.14,218.86,223.15,228.05,231.33,234.86,236.42,237.67,239.07,240.3,241.75,242.96,245.17,247.67,250.95,253.51,257.7,259.55,261.58,265.05,267.18,3.0000000000000001E-3]
[" Transportation",613.37,705.86,465.68,508.22,528.5,567.33000000000004,615.79,640.91999999999996,655.77,671.91,690.32,704.34,717.08,729.77,737.71,743.52,757.24,767.89,782.71,795.25,808.06,822.03,834.45,846.64,856.24,869.12,883.55,894.05,908.01,8.9999999999999993E-3]
["   Total Non-Renewable Expenditures",1251.3499999999999,1396.52,1041.45,1058.6500000000001,1088.31,1162.25,1220.05,1251.99,1276.69,1306.1199999999999,1334.33,1358.39,1379.14,1402.91,1418.92,1432.73,1454.32,1472.13,1493.23,1514.98,1538.45,1564.3,1590.55,1615.34,1640.71,1665.62,1688.65,1712.28,1737.37,8.0000000000000002E-3]
[" Transportation Renewable Expenditures",0.05,0.17,0.04,0.09,0.11,0.13,0.15,0.17,0.21,2.34,3.15,4,5.31,7.12,9.59,17.39,15.56,14.53,15.06,16.98,18.95,20.57,23.66,25.05,31.91,36.74,40.74,48.35,56.42,0.24099999999999999]
["   Total Expenditures",1251.3900000000001,1396.69,1041.49,1058.74,1088.42,1162.3699999999999,1220.2,1252.1600000000001,1276.9000000000001,1308.46,1337.48,1362.4,1384.44,1410.03,1428.51,1450.12,1469.88,1486.66,1508.29,1531.96,1557.41,1584.86,1614.21,1640.39,1672.62,1702.37,1729.39,1760.62,1793.79,8.9999999999999993E-3]
[]
[]
["Prices in Nominal Dollars"]
[" Residential"]
["   Liquefied Petroleum Gases",25.67,29.35,25.28,24.73,25.15,26.73,28.51,30.06,31.23,32.520000000000003,33.75,35.06,36.020000000000003,37.020000000000003,38.1,39.200000000000003,40.409999999999997,41.61,42.82,43.92,45.24,46.58,48.12,49.52,51.18,52.85,54.62,56.39,58.23,2.5999999999999999E-2]
["   Distillate Fuel Oil",19.86,24.47,18.260000000000002,18.100000000000001,18.489999999999998,19.940000000000001,21.4,22.55,23.49,24.96,26.17,27.44,28.46,29.45,30.25,31.17,32.25,33.17,34.24,35.33,36.380000000000003,37.630000000000003,39.049999999999997,40.159999999999997,41.73,43.3,44.82,46.47,48.16,2.5000000000000001E-2]
["   Natural Gas",12.66,13.48,11.57,11.22,12.29,12.56,12.36,12.51,12.88,13.22,13.5,13.83,14.18,14.61,15.06,15.64,16.010000000000002,16.22,16.68,17.260000000000002,17.91,18.649999999999999,19.440000000000001,20.29,21.26,21.98,22.61,23.44,24.2,2.1999999999999999E-2]
["   Electricity",31.12,33.29,32.83,31.88,31.21,32.9,33.9,34.5,35.020000000000003,35.89,36.74,37.39,37.97,38.92,39.950000000000003,40.92,41.95,42.94,43.78,44.88,46.07,47.3,48.93,50.5,52.16,53.81,55.2,56.77,58.33,2.1000000000000001E-2]
[]
[" Commercial"]
["   Liquefied Petroleum Gases",20.2,26.15,20.12,21.4,21.77,23.3,25.02,26.51,27.61,28.83,29.98,31.22,32.11,33.020000000000003,34.01,35.020000000000003,36.130000000000003,37.24,38.35,39.36,40.57,41.81,43.24,44.53,46.07,47.62,49.27,50.92,52.64,2.5999999999999999E-2]
["   Distillate Fuel Oil",17.100000000000001,21.5,16.04,15.27,15.91,17.34,18.739999999999998,19.850000000000001,20.86,22.18,23.33,24.52,25.47,26.39,27.18,28.11,29.04,29.83,30.83,31.82,32.83,34.01,35.340000000000003,36.380000000000003,37.86,39.340000000000003,40.74,42.29,43.92,2.7E-2]
["   Residual Fuel",8.2100000000000009,15.52,9.41,9.74,10.050000000000001,11.48,12.9,13.98,14.63,15.52,16.37,17.29,18.29,18.899999999999999,19.57,20.27,21.01,21.73,22.45,23.04,23.8,24.66,25.52,26.47,27.6,28.58,29.4,30.75,31.66,2.7E-2]
["   Natural Gas",10.96,11.94,9.18,8.93,10.15,10.65,10.68,10.8,11.14,11.44,11.67,11.96,12.27,12.65,13.05,13.58,13.92,14.13,14.53,15.05,15.62,16.3,17.010000000000002,17.78,18.690000000000001,19.329999999999998,19.86,20.61,21.27,2.1999999999999999E-2]
["   Electricity",28.18,30.47,29.38,28.19,26.85,28.28,28.88,29.09,29.58,30.41,31.16,31.75,32.270000000000003,33.15,34.090000000000003,34.97,35.99,36.94,37.619999999999997,38.61,39.68,40.82,42.33,43.75,45.32,46.89,48.18,49.63,51.04,1.9E-2]
[]
[" Industrial 1/"]
["   Liquefied Petroleum Gases",21.53,24.2,18.920000000000002,18.920000000000002,19.260000000000002,20.76,22.51,24,25.06,26.38,27.45,28.6,29.51,30.38,31.31,32.270000000000003,33.340000000000003,34.39,35.450000000000003,36.4,37.549999999999997,38.729999999999997,40.1,41.33,42.81,44.29,45.9,47.5,49.15,2.7E-2]
["   Distillate Fuel Oil",17.68,22.31,16.649999999999999,14.82,16.05,17.52,18.95,20.07,21.18,22.46,23.62,24.81,25.76,26.68,27.5,28.52,29.39,30.15,31.18,32.159999999999997,33.21,34.409999999999997,35.770000000000003,36.83,38.33,39.83,41.25,42.82,44.51,2.5999999999999999E-2]
["   Residual Fuel Oil",8.65,16.309999999999999,9.89,13.52,13.82,15.16,16.489999999999998,17.62,18.350000000000001,19.239999999999998,20.059999999999999,20.97,21.68,22.24,23,23.74,24.52,25.31,26.1,26.74,27.57,28.51,29.51,30.6,31.8,32.92,34.03,35.29,36.5,0.03]
["   Natural Gas 2/",7.41,9.11,4.26,5.0199999999999996,6.23,6.76,6.82,6.89,7.18,7.39,7.52,7.71,7.91,8.19,8.4700000000000006,8.8800000000000008,9.14,9.26,9.52,9.9,10.31,10.85,11.41,12.04,12.79,13.25,13.56,14.17,14.67,1.7999999999999999E-2]
["   Metallurgical Coal",3.61,4.49,4.79,4.9400000000000004,5.07,5.31,5.44,5.56,5.66,5.77,5.97,6.14,6.34,6.5,6.68,6.84,6.98,7.07,7.11,7.15,7.27,7.43,7.55,7.72,7.86,8.02,8.18,8.33,8.5,2.4E-2]
["   Other Industrial Coal",2.4300000000000002,2.84,2.83,2.77,2.81,2.85,2.86,2.93,3,3.04,3.11,3.16,3.2,3.26,3.31,3.38,3.43,3.5,3.56,3.65,3.72,3.82,3.91,4.01,4.12,4.21,4.33,4.4400000000000004,4.55,1.7999999999999999E-2]
["   Coal to Liquids","- -","- -","- -","- -",1.32,1.1000000000000001,1.1200000000000001,1.55,1.58,1.65,1.72,1.74,1.76,1.79,1.86,1.91,1.98,1.99,2.02,2.04,2.0699999999999998,2.1,2.13,2.1800000000000002,2.2200000000000002,2.2799999999999998,2.35,2.44,2.5299999999999998,"- -"]
["   Electricity",18.600000000000001,20.21,20.350000000000001,19.73,17.86,18.77,18.98,19.010000000000002,19.36,19.989999999999998,20.51,20.91,21.27,21.9,22.56,23.2,23.95,24.64,25.11,25.79,26.57,27.41,28.5,29.55,30.67,31.8,32.71,33.76,34.799999999999997,0.02]
[]
[" Transportation"]
["   Liquefied Petroleum Gases 3/",23.31,29.93,25.58,24.61,25.02,26.61,28.36,29.9,31.07,32.36,33.58,34.89,35.840000000000003,36.82,37.89,38.979999999999997,40.17,41.36,42.56,43.64,44.94,46.27,47.79,49.17,50.81,52.46,54.21,55.95,57.77,2.5000000000000001E-2]
["   E85 4/",26.83,26.93,23.64,21.26,21.89,23.43,26.07,27.64,28.47,28.45,29.92,31.23,31.97,32.94,34.090000000000003,35.479999999999997,36.880000000000003,37.979999999999997,39.17,40.479999999999997,41.72,43.4,44.96,46.25,47.62,49.36,50.75,52.29,54.17,2.5999999999999999E-2]
["   Motor Gasoline 5/",23.15,26.76,19.43,21.17,21.79,23.32,25.87,27.33,28.27,29.42,30.58,31.65,32.6,33.72,34.72,35.94,37.020000000000003,37.96,39.18,40.44,41.69,43.21,44.7,45.91,47.47,49.16,50.66,52.36,54.33,2.7E-2]
["   Jet Fuel 6/",15.42,22.71,12.92,15.23,15.82,17.510000000000002,19.05,20.23,21.21,22.42,23.58,24.67,25.58,26.51,27.27,28.18,29.2,30.07,31.1,32.130000000000003,33.21,34.54,35.83,36.99,38.42,39.92,41.32,42.87,44.51,2.5000000000000001E-2]
["   Diesel Fuel (distillate fuel oil) 7/",21.08,27.65,18.04,19.7,20.149999999999999,21.71,23.2,24.38,25.56,26.86,28.03,29.31,30.31,31.28,32.19,33.32,34.22,35.03,36.130000000000003,37.17,38.32,39.61,41.05,42.2,43.79,45.41,46.88,48.53,50.35,2.1999999999999999E-2]
["   Residual Fuel Oil",8.99,14.49,9,10.51,10.77,12.17,13.4,14.45,15.13,15.77,16.670000000000002,17.43,17.940000000000001,18.32,19,19.57,20.260000000000002,20.94,21.63,22.13,23.02,23.85,24.8,25.81,26.88,27.91,28.9,30.02,31.26,2.9000000000000001E-2]
["   Natural Gas 8/",13.54,15.96,11.54,12.36,13.66,14.28,14.39,14.52,14.9,15.21,15.46,15.74,16.04,16.43,16.8,17.32,17.64,17.829999999999998,18.23,18.760000000000002,19.309999999999999,19.98,20.67,21.42,22.31,22.94,23.44,24.19,24.84,1.7000000000000001E-2]
["   Electricity",31.32,33.729999999999997,32.79,31.2,28.83,31.39,32.01,31.85,32.08,32.909999999999997,33.549999999999997,33.97,34.26,34.89,35.61,36.26,37.11,38.1,38.86,40,41.47,43.05,45.05,46.8,48.78,50.72,52.33,54.13,55.89,1.9E-2]
[]
[" Electric Power 9/"]
["   Distillate Fuel Oil",15.41,19.37,14.46,14.33,14.68,16.09,17.46,18.510000000000002,19.350000000000001,20.67,21.81,22.96,23.88,24.75,25.46,26.24,27.22,28.03,28.98,29.93,30.88,32,33.28,34.28,35.71,37.130000000000003,38.46,39.950000000000003,41.52,2.9000000000000001E-2]
["   Residual Fuel Oil",8.84,14.56,8.92,12.37,12.7,14.13,15.48,16.55,17.3,18.07,19.010000000000002,19.88,20.54,21.05,21.8,22.48,23.26,24.05,24.83,25.46,26.42,27.37,28.4,29.5,30.7,31.85,32.92,34.19,35.49,3.4000000000000002E-2]
["   Natural Gas",7.1,9.09,4.2,4.99,6.07,6.53,6.4,6.47,6.77,6.99,7.13,7.32,7.53,7.85,8.1300000000000008,8.5399999999999991,8.7799999999999994,8.91,9.17,9.57,9.9700000000000006,10.51,11.09,11.66,12.38,12.84,13.16,13.75,14.22,1.7000000000000001E-2]
["   Steam Coal",1.76,2.0499999999999998,2.1800000000000002,2.0499999999999998,2.0699999999999998,2.1,2.15,2.19,2.2400000000000002,2.2599999999999998,2.31,2.34,2.38,2.42,2.4700000000000002,2.54,2.59,2.65,2.69,2.77,2.82,2.9,2.98,3.06,3.15,3.23,3.32,3.41,3.51,0.02]
[]
[" Average Price to All Users 10/"]
["   Liquefied Petroleum Gases",18.53,20.190000000000001,18.64,17.36,17.61,18.920000000000002,20.43,21.72,22.62,23.64,24.56,25.55,26.28,27.06,27.91,28.78,29.75,30.7,31.68,32.54,33.6,34.69,35.950000000000003,37.049999999999997,38.44,39.83,41.29,42.77,44.32,0.03]
["   E85 4/",26.83,26.93,23.64,21.26,21.89,23.43,26.07,27.64,28.47,28.45,29.92,31.23,31.97,32.94,34.090000000000003,35.479999999999997,36.880000000000003,37.979999999999997,39.17,40.479999999999997,41.72,43.4,44.96,46.25,47.62,49.36,50.75,52.29,54.17,2.5999999999999999E-2]
["   Motor Gasoline 5/",23.03,26.54,19.440000000000001,21.17,21.79,23.32,25.87,27.33,28.27,29.42,30.58,31.64,32.6,33.71,34.71,35.93,37.020000000000003,37.950000000000003,39.17,40.43,41.68,43.21,44.69,45.9,47.46,49.15,50.65,52.35,54.32,2.7E-2]
["   Jet Fuel",15.42,22.71,12.92,15.23,15.82,17.510000000000002,19.05,20.23,21.21,22.42,23.58,24.67,25.58,26.51,27.27,28.18,29.2,30.07,31.1,32.130000000000003,33.21,34.54,35.83,36.99,38.42,39.92,41.32,42.87,44.51,2.5000000000000001E-2]
["   Distillate Fuel Oil",20.260000000000002,26.27,17.73,18.260000000000002,18.940000000000001,20.58,22.21,23.39,24.55,25.86,27.09,28.33,29.33,30.3,31.19,32.29,33.22,34.04,35.14,36.19,37.31,38.6,40.04,41.2,42.78,44.38,45.87,47.52,49.31,2.4E-2]
["   Residual Fuel Oil",8.8699999999999992,14.77,9.1,11.22,11.49,12.89,14.14,15.19,15.89,16.600000000000001,17.5,18.3,18.89,19.329999999999998,20.03,20.64,21.36,22.08,22.8,23.35,24.24,25.11,26.08,27.11,28.23,29.29,30.29,31.46,32.700000000000003,0.03]
["   Natural Gas",8.99,10.53,6.67,7.08,8.2100000000000009,8.68,8.67,8.7799999999999994,9.07,9.33,9.5,9.73,9.98,10.32,10.67,11.14,11.42,11.55,11.88,12.31,12.79,13.39,14.02,14.7,15.51,16.05,16.46,17.12,17.71,1.9E-2]
["   Metallurgical Coal",3.61,4.49,4.79,4.9400000000000004,5.07,5.31,5.44,5.56,5.66,5.77,5.97,6.14,6.34,6.5,6.68,6.84,6.98,7.07,7.11,7.15,7.27,7.43,7.55,7.72,7.86,8.02,8.18,8.33,8.5,2.4E-2]
["   Other Coal",1.8,2.1,2.2200000000000002,2.09,2.11,2.14,2.19,2.23,2.2799999999999998,2.2999999999999998,2.35,2.39,2.4300000000000002,2.4700000000000002,2.52,2.58,2.64,2.69,2.74,2.81,2.87,2.95,3.03,3.11,3.2,3.28,3.37,3.46,3.56,0.02]
["   Coal to Liquids","- -","- -","- -","- -",1.32,1.1000000000000001,1.1200000000000001,1.55,1.58,1.65,1.72,1.74,1.76,1.79,1.86,1.91,1.98,1.99,2.02,2.04,2.0699999999999998,2.1,2.13,2.1800000000000002,2.2200000000000002,2.2799999999999998,2.35,2.44,2.5299999999999998,"- -"]
["   Electricity",26.66,28.81,28.5,27.58,26.29,27.63,28.19,28.46,28.92,29.72,30.45,31.03,31.53,32.4,33.33,34.229999999999997,35.22,36.159999999999997,36.869999999999997,37.86,38.94,40.090000000000003,41.58,43,44.53,46.07,47.34,48.78,50.19,2.1000000000000001E-2]
[]
["Non-Renewable Energy Expenditures by Sector"]
["(billion nominal dollars)"]
[" Residential",236.38,254.66,235.17,230.51,232.31,244.12,246.57,251.37,257.29000000000002,266.02999999999997,273.52999999999997,281.39999999999998,289.27,299.58999999999997,309.45,320.3,330.83,341.36,351.09,363.72,377.1,392.03,407.27,423.22,441.01,458.4,471.99,489.06,506.03,2.5999999999999999E-2]
[" Commercial",172.75,191.19,171.27,168.36,170.83,182.74,187.26,190.86,197.13,205.11,212.7,219.88,226.94,236.05,245.65,255.58,265.91000000000003,275.66000000000003,285.08999999999997,296.79000000000002,309.27,322.77,338.69,354.37,371.75,388.64,403.84,421.34,438.74,3.1E-2]
[" Industrial",214.89,244.81,178.09,168.16,181.07,202.87,217.07,227.35,237.51,248.26,257.8,268.36,277.25,287.02999999999997,295.06,303.12,311.48,319.60000000000002,328.09,336.58,346.81,357.93,370.58,382.62,397.61,409.44,421.52,436.23,449,2.3E-2]
[" Transportation",599.94000000000005,705.86,472.76,523.54,551.54,600.52,663.3,702.29,730.78,762.17,797.53,828.81,859.4,891.87,920.68,948.26,986.59,1021.27,1062.24,1101.69,1143.03,1188,1232.23,1277.8499999999999,1321.12,1371.03,1423.78,1471.43,1525.95,2.9000000000000001E-2]
["   Total Non-Renewable Expenditures",1223.96,1396.52,1057.29,1090.58,1135.76,1230.25,1314.19,1371.86,1422.72,1481.57,1541.56,1598.45,1652.86,1714.54,1770.84,1827.25,1894.81,1957.89,2026.51,2098.7800000000002,2176.1999999999998,2260.73,2348.7600000000002,2438.06,2531.5,2627.51,2721.14,2818.06,2919.72,2.8000000000000001E-2]
[" Transportation Renewable Expenditures",0.04,0.17,0.04,0.09,0.11,0.13,0.16,0.18,0.24,2.65,3.64,4.71,6.36,8.6999999999999993,11.96,22.18,20.28,19.329999999999998,20.440000000000001,23.52,26.81,29.72,34.94,37.81,49.23,57.96,65.66,79.569999999999993,94.81,0.26500000000000001]
["   Total Expenditures",1224,1396.69,1057.33,1090.67,1135.8699999999999,1230.3800000000001,1314.36,1372.05,1422.95,1484.22,1545.2,1603.16,1659.22,1723.24,1782.8,1849.44,1915.09,1977.22,2046.94,2122.3000000000002,2203.0100000000002,2290.46,2383.6999999999998,2475.87,2580.73,2685.47,2786.79,2897.63,3014.53,2.9000000000000001E-2]
[]
[]
[]
["   1/ Includes energy for combined heat and power plants, except those whose primary business is to sell electricity, or electricity and heat, to the public."]
["   2/ Excludes use for lease and plant fuel."]
["   3/ Includes Federal and State taxes while excluding county and local taxes."]
["   4/ E85 refers to a blend of 85 percent ethanol (renewable) and 15 percent motor gasoline (nonrenewable).  To address cold starting issues,"]
["the percentage of ethanol varies seasonally.  The annual average ethanol content of 74 percent is used for this forecast."]
["   5/ Sales weighted-average price for all grades.  Includes Federal, State, and local taxes."]
["   6/ Kerosene-type jet fuel.  Includes Federal and State taxes while excluding county and local taxes."]
["   7/ Diesel fuel for on-road use.  Includes Federal and State taxes while excluding county and local taxes."]
["   8/ Compressed natural gas used as a vehicle fuel.  Includes estimated motor vehicle fuel taxes and estimated dispensing costs or charges."]
["   9/ Includes electricity-only and combined heat and power plants whose primary business is to sell electricity, or electricity and heat, to the public."]
["   10/ Weighted averages of end-use fuel prices are derived from the prices shown in each sector and the corresponding sectoral consumption."]
["   Btu = British thermal unit."]
["   - - = Not applicable."]
["   Note:  Data for 2007 and 2008 are model results and may differ slightly from official EIA data reports."]
["   Sources:  2007 and 2008 prices for motor gasoline, distillate fuel oil, and jet fuel are based on prices in the Energy Information Administration (EIA), Petroleum Marketing Annual"]
["2008, DOE/EIA-0487(2008) (Washington, DC, August 2009).  2007 residential and commercial natural gas delivered prices:  EIA,"]
["Natural Gas Annual 2007, DOE/EIA-0131(2007) (Washington, DC, January, 2009).  2008 residential and commercial natural gas"]
["delivered prices:  EIA, Natural Gas Monthly, DOE/EIA-0130(2009/07) (Washington, DC, July 2009).  2007 and 2008"]
["industrial natural gas delivered prices are estimated based on:  EIA, Manufacturing Energy Consumption Survey and"]
["industrial and wellhead prices from the Natural Gas Annual 2007, DOE/EIA-0131(2007) (Washington, DC, January, 2009) and the"]
["Natural Gas Monthly, DOE/EIA-0130(2009/07) (Washington, DC, July 2009).  2007 transportation sector natural gas delivered prices are based on:  EIA, Natural Gas Annual"]
["2007, DOE/EIA-0131(2007) (Washington, DC, January, 2009) and estimated State taxes, Federal taxes, and dispensing costs or charges."]
["2008 transportation sector natural gas delivered prices are model results. 2007 and 2008 electric power sector natural gas prices:  EIA, Electric Power Monthly,"]
["April 2008 and April 2009, Table 4.13.B.  2007 and 2008 coal prices based on:  EIA, Quarterly Coal Report,"]
["October-December 2008, DOE/EIA-0121(2008/4Q) (Washington, DC, March 2009) and EIA, AEO2010 National Energy Modeling System run aeo2010r.d111809a."]
["2007 and 2008 electricity prices:  EIA, Annual Energy Review 2008, DOE/EIA-0384(2008) (Washington, DC, June 2009)."]
["2007 and 2008 E85 prices derived from monthly prices in the Clean Cities Alternative Price Report."]
["Projections:  EIA, AEO2010 National Energy Modeling System run aeo2010r.d111809a."]
["Scenario:","stimulus","d041409a",null,"with American Recovery and Reinvestment Act"]
[]
[" Table   3.  Energy Prices by Sector and Source"]
["                      (2007 dollars per million Btu, unless otherwise noted)"]
[]
[]
[]
[null,"2006","2007","2008","2009","2010","2011","2012","2013","2014","2015","2016","2017","2018","2019","2020","2021","2022","2023","2024","2025","2026","2027","2028","2029","2030","2027","2028","2029","2030",2031,2032,2033,2034,2035,2036,2037,2038,2039,2040,2041,2042,2043,2044,2045,2046,2047,2048,2049,2050,2051,2052,2053,2054,2055,2056,2057,2058,2059,2060,2061,2062,2063,2064,2065,2066,2067,2068,2069,2070]
[]
[]
[" Residential"]
["   Liquefied Petroleum Gases",23.882804870605501,24.973464965820298,28.470840454101602,21.505495071411101,20.697200775146499,23.0020751953125,24.980747222900401,26.7403888702393,28.254840850830099,29.8807067871094,30.930690765380898,31.804765701293899,32.682899475097699,33.084945678710902,33.339298248291001,33.569530487060497,33.692008972167997,34.029460906982401,34.165733337402301,33.722698211669901,33.999015808105497,34.276668548583999,34.616855621337898,34.804977416992202,35.163482666015597,23.653226852416999,23.781959533691399,23.869001388549801,23.909082412719702]
["   Distillate Fuel Oil",18.4642543792725,19.664405822753899,23.940315246581999,15.6857194900513,13.3512983322144,15.708171844482401,17.491518020629901,18.8044624328613,20.071212768554702,21.571735382080099,22.444984436035199,23.2645053863525,23.975505828857401,24.350082397460898,24.6401481628418,24.7862453460693,24.899822235107401,25.1952934265137,25.492937088012699,25.134300231933601,25.433099746704102,25.7546691894531,26.098386764526399,26.3820476531982,26.7700805664063,13.801754951477101,13.897899627685501,14.058331489563001,14.125551223754901]
["   Natural Gas",13.7000589370728,12.691158294677701,12.9778490066528,10.717614173889199,11.192774772644,11.487280845642101,11.3991556167603,11.307798385620099,11.2896461486816,11.345415115356399,11.538298606872599,11.7583208084106,11.975100517272899,12.23952293396,12.557071685791,12.7957820892334,12.871651649475099,12.660281181335399,12.6240320205688,12.5992183685303,12.7868556976318,13.07555103302,13.407883644104,13.6725673675537,13.962038993835399,11.116808891296399,11.2574377059937,11.3709173202515,11.426144599914601]
["   Electricity",31.206779479980501,31.181957244873001,31.772819519043001,30.736837387085,28.616357803344702,29.873619079589801,30.101655960083001,30.425390243530298,30.7938537597656,30.883028030395501,31.149145126342798,31.4898681640625,31.815629959106399,32.020698547363303,32.4303588867188,32.7907905578613,32.994007110595703,32.923465728759801,32.920154571533203,32.902271270752003,32.958240509033203,33.321102142333999,33.734363555908203,34.149539947509801,34.490489959716797,26.5695495605469,26.6057014465332,26.7373046875,26.757972717285199]
[]
[" Commercial",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12.0537929534912,12.2529897689819,12.3258762359619,12.452996253967299]
["   Liquefied Petroleum Gases",21.1974983215332,23.041419982910199,23.540430068969702,20.975297927856399,17.540355682373001,19.827720642089801,21.7962131500244,23.5440998077393,25.047388076782202,26.6623840332031,27.701774597168001,28.565574645996101,29.4346523284912,29.8274021148682,30.0731811523438,30.2960014343262,30.4115695953369,30.7421360015869,30.871879577636701,30.422807693481399,30.6932373046875,30.965314865112301,31.299940109252901,31.482862472534201,31.836189270019499,7.3951959609985396,7.4624595642089799,7.2386937141418501,7.3113985061645499]
["   Distillate Fuel Oil",15.019946098327599,16.054100036621101,20.9568576812744,13.740292549133301,10.759732246398899,13.277551651001,15.102119445800801,16.819028854370099,18.163129806518601,19.404659271240199,20.2805690765381,21.141357421875,21.870569229126001,22.288406372070298,22.606428146362301,22.643785476684599,22.862098693847699,23.111530303955099,23.2818489074707,23.1139316558838,23.4434604644775,23.529294967651399,23.9437866210938,24.471529006958001,24.6476936340332,9.0512752532959002,9.1702537536621094,9.2454566955566406,9.3029346466064506,{"$f":"AD253+($AI$253-$AD$253)/5","v":9.3577216364198588},{"$f":"AE253+($AI$253-$AD$253)/5","v":9.4125086262332669},{"$f":"AF253+($AI$253-$AD$253)/5","v":9.467295616046675},{"$f":"AG253+($AI$253-$AD$253)/5","v":9.5220826058600831},{"$f":"T423*$E$742","v":9.5768695956734877},{"$f":"AI253+($AX$253-$AI$253)/15","v":9.6852727225982509},{"$f":"AJ253+($AX$253-$AI$253)/15","v":9.7936758495230141},9.9020789764477772,10.01048210337254,10.118885230297304,10.227288357222067,10.33569148414683,10.444094611071593,10.552497737996356,10.660900864921119,10.769303991845883,10.877707118770646,10.986110245695409,11.094513372620172,{"$f":"AI253*$B$742","v":11.202916499544939},{"$f":"AX253+($BM$253-$AX$253)/15","v":11.313845014700993},{"$f":"AY253+($BM$253-$AX$253)/15","v":11.424773529857047},11.535702045013101,11.646630560169156,11.75755907532521,11.868487590481264,11.979416105637318,12.090344620793372,12.201273135949426,12.312201651105481,12.423130166261535,12.534058681417589,12.644987196573643,12.755915711729697,{"$f":"AX253*$C$742","v":12.866844226885757},{"$f":"BM253+($BR$253-$BM$253)/5","v":12.994248543867917},{"$f":"BN253+($BR$253-$BM$253)/5","v":13.121652860850077},{"$f":"BO253+($BR$253-$BM$253)/5","v":13.249057177832237},{"$f":"BP253+($BR$253-$BM$253)/5","v":13.376461494814397},{"$f":"BM253*$D$742","v":13.503865811796555}]
["   Residual Fuel",8.8815975189209002,10.3074436187744,13.411918640136699,6.6991925239562997,5.8016228675842303,8.5975322723388707,10.1285858154297,11.654000282287599,12.9474182128906,14.400235176086399,15.2041673660278,15.658245086669901,16.352220535278299,16.605510711669901,16.856744766235401,17.043632507324201,17.1953125,17.403110504150401,17.4520969390869,17.016120910644499,17.163618087768601,17.311967849731399,17.516565322876001,17.704761505126999,17.873653411865199,24.1571254730225,24.207300186157202,24.2876873016357,24.267208099365199,{"$f":"AD254+($AI$254-$AD$254)/5","v":24.075703794494256},{"$f":"AE254+($AI$254-$AD$254)/5","v":23.884199489623313},{"$f":"AF254+($AI$254-$AD$254)/5","v":23.69269518475237},{"$f":"AG254+($AI$254-$AD$254)/5","v":23.501190879881428},{"$f":"T424*$E$745","v":23.309686575010492},{"$f":"AI254+($AX$254-$AI$254)/15","v":23.300523054015734},{"$f":"AJ254+($AX$254-$AI$254)/15","v":23.291359533020977},23.282196012026219,23.273032491031461,23.263868970036704,23.254705449041946,23.245541928047189,23.236378407052431,23.227214886057673,23.218051365062916,23.208887844068158,23.199724323073401,23.190560802078643,23.181397281083886,{"$f":"AI254*$B$745","v":23.172233760089139},{"$f":"AX254+($BM$254-$AX$254)/15","v":23.186953863011141},{"$f":"AY254+($BM$254-$AX$254)/15","v":23.201673965933143},23.216394068855145,23.231114171777147,23.245834274699149,23.260554377621151,23.275274480543153,23.289994583465155,23.304714686387157,23.31943478930916,23.334154892231162,23.348874995153164,23.363595098075166,23.378315200997168,{"$f":"AX254*$C$745","v":23.393035303919145},{"$f":"BM254+($BR$254-$BM$254)/5","v":23.407895670463727},{"$f":"BN254+($BR$254-$BM$254)/5","v":23.422756037008309},{"$f":"BO254+($BR$254-$BM$254)/5","v":23.437616403552891},{"$f":"BP254+($BR$254-$BM$254)/5","v":23.452476770097473},{"$f":"BM254*$D$745","v":23.467337136642058}]
["   Natural Gas",11.896094322204601,10.9898433685303,11.3387994766235,8.9075946807861293,9.4656057357788104,9.7463216781616193,9.7210922241210902,9.6719341278076207,9.7138872146606392,9.8306560516357404,10.038209915161101,10.2545003890991,10.476261138916,10.746561050415,11.0803880691528,11.314369201660201,11.4017143249512,11.212500572204601,11.1975994110107,11.159740447998001,11.3503875732422,11.640952110290501,11.9785671234131,12.2332496643066,12.5188312530518]
["   Electricity",28.3762531280518,28.029735565185501,29.057315826416001,27.6067714691162,24.835584640502901,25.581251144409201,25.4402256011963,25.470129013061499,25.672283172607401,25.763282775878899,26.100669860839801,26.468044281005898,26.885612487793001,27.169450759887699,27.620109558105501,28.002447128295898,28.245407104492202,28.186374664306602,28.203248977661101,28.139711380004901,28.178466796875,28.495182037353501,28.915565490722699,29.289411544799801,29.651695251464801,16.318952560424801,16.4172878265381,16.5084934234619,16.549221038818398]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12.788073539733899,13.069622039794901,13.0597486495972,13.2463188171387]
[" Industrial 1/",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9.5039434432983398,9.4975557327270508,9.6068582534790004,9.5831336975097692]
["   Liquefied Petroleum Gases",21.041078567504901,23.3795166015625,26.646581649780298,22.2440700531006,16.6379299163818,18.920274734497099,20.8892612457275,22.636520385742202,24.1346244812012,25.742292404174801,26.783767700195298,27.652248382568398,28.520401000976602,28.932659149169901,29.169765472412099,29.4143581390381,29.524629592895501,29.853767395019499,29.959171295166001,29.528638839721701,29.7813510894775,30.054143905639599,30.3852443695068,30.4649448394775,30.849096298217798,6.3330101966857901,6.4338274002075204,6.5134425163268999,6.5598897933959996,{"$f":"AD259+($AI$259-$AD$259)/5","v":6.5507078532683796},{"$f":"AE259+($AI$259-$AD$259)/5","v":6.5415259131407595},{"$f":"AF259+($AI$259-$AD$259)/5","v":6.5323439730131394},{"$f":"AG259+($AI$259-$AD$259)/5","v":6.5231620328855193},{"$f":"T429*$E$742","v":6.5139800927579001},{"$f":"AI259+($AX$259-$AI$259)/15","v":6.5877135610615332},{"$f":"AJ259+($AX$259-$AI$259)/15","v":6.6614470293651662},6.7351804976687992,6.8089139659724323,6.8826474342760653,6.9563809025796983,7.0301143708833314,7.1038478391869644,7.1775813074905974,7.2513147757942304,7.3250482440978635,7.3987817124014965,7.4725151807051295,7.5462486490087626,{"$f":"AI259*$B$742","v":7.6199821173123929},{"$f":"AX259+($BM$259-$AX$259)/15","v":7.6954333002095865},{"$f":"AY259+($BM$259-$AX$259)/15","v":7.77088448310678},7.8463356660039736,7.9217868489011671,7.9972380317983607,8.0726892146955542,8.1481403975927478,8.2235915804899413,8.2990427633871349,8.3744939462843284,8.449945129181522,8.5253963120787155,8.6008474949759091,8.6762986778731026,{"$f":"AX259*$C$742","v":8.7517498607702962},{"$f":"BM259+($BR$259-$BM$259)/5","v":8.8384075286295438},{"$f":"BN259+($BR$259-$BM$259)/5","v":8.9250651964887915},{"$f":"BO259+($BR$259-$BM$259)/5","v":9.0117228643480392},{"$f":"BP259+($BR$259-$BM$259)/5","v":9.0983805322072868},{"$f":"BM259*$D$742","v":9.1850382000665363}]
["   Distillate Fuel Oil",15.7354278564453,16.8219394683838,21.937858581543001,14.291754722595201,10.6247463226318,13.4027051925659,15.2648477554321,17.266075134277301,18.658037185668899,19.740333557128899,20.622322082519499,21.514814376831101,22.261856079101602,22.720048904418899,23.0620517730713,23.029100418090799,23.327865600585898,23.5460414886475,23.635374069213899,23.588466644287099,23.9423828125,23.870851516723601,24.336980819702099,25.037542343139599,25.073137283325199,2.7168338298797599,2.7307398319244398,2.7413196563720699,2.7546591758728001]
["   Residual Fuel Oil",9.2125787734985405,10.5954837799072,13.7473258972168,6.9127345085143999,9.8444128036499006,12.2499532699585,13.9352369308472,15.428977966308601,16.646518707275401,18.037969589233398,18.8180332183838,19.4296264648438,20.112428665161101,20.448431015014599,20.727931976318398,20.973798751831101,21.101537704467798,21.306892395019499,21.394767761230501,21.017236709594702,21.180326461791999,21.338615417480501,21.660650253295898,21.793584823608398,22.078443527221701,2.2517027854919398,2.2682161331176802,2.2745745182037398,2.2862651348114]
["   Natural Gas 2/",7.9540700912475604,7.5152516365051296,8.8012723922729492,4.8485679626464799,5.4989199638366699,5.8261642456054696,5.87778615951538,5.9538393020629901,6.1098570823669398,6.3294844627380398,6.5125813484191903,6.7027301788330096,6.8988709449768102,7.1528282165527299,7.4686021804809597,7.6786775588989302,7.7538070678710902,7.5584783554077104,7.5461778640747097,7.4592709541320801,7.6002230644226101,7.8596048355102504,8.1941757202148402,8.4216127395629901,8.6935501098632795,1.2833950519561801,1.3286876678466799,1.33012855052948,1.33445107936859]
["   Metallurgical Coal",3.6353600025177002,3.6099998950958301,4.0558156967163104,4.0487108230590803,3.9977276325225799,4.1121706962585396,4.1809573173522896,4.2343683242797896,4.27162742614746,4.2985162734985396,4.3192996978759801,4.3337044715881303,4.3530845642089799,4.3696141242981001,4.3899216651916504,4.4470157623290998,4.5093812942504901,4.5352845191955602,4.5618190765380904,4.5643453598022496,4.5493078231811497,4.5490665435790998,4.5331215858459499,4.4955492019653303,4.4319190979003897,17.3004150390625,17.331628799438501,17.425392150878899,17.430723190307599,{"$f":"AD263+($AI$263-$AD$263)/5","v":17.267158349957999},{"$f":"AE263+($AI$263-$AD$263)/5","v":17.103593509608398},{"$f":"AF263+($AI$263-$AD$263)/5","v":16.940028669258798},{"$f":"AG263+($AI$263-$AD$263)/5","v":16.776463828909197},{"$f":"T433*$E$745","v":16.612898988559596},{"$f":"AI263+($AX$263-$AI$263)/15","v":16.606368113587273},{"$f":"AJ263+($AX$263-$AI$263)/15","v":16.599837238614949},16.593306363642625,16.586775488670302,16.580244613697978,16.573713738725655,16.567182863753331,16.560651988781007,16.554121113808684,16.54759023883636,16.541059363864036,16.534528488891713,16.527997613919389,16.521466738947066,{"$f":"AI263*$B$745","v":16.514935863974742},{"$f":"AX263+($BM$263-$AX$263)/15","v":16.525426935236357},{"$f":"AY263+($BM$263-$AX$263)/15","v":16.535918006497972},16.546409077759588,16.556900149021203,16.567391220282818,16.577882291544434,16.588373362806049,16.598864434067664,16.60935550532928,16.619846576590895,16.63033764785251,16.640828719114126,16.651319790375741,16.661810861637356,{"$f":"AX263*$C$745","v":16.672301932898996},{"$f":"BM263+($BR$263-$BM$263)/5","v":16.682892970558111},{"$f":"BN263+($BR$263-$BM$263)/5","v":16.693484008217226},{"$f":"BO263+($BR$263-$BM$263)/5","v":16.704075045876341},{"$f":"BP263+($BR$263-$BM$263)/5","v":16.714666083535455},{"$f":"BM263*$D$745","v":16.725257121194577}]
["   Other Industrial Coal",2.4029970169067401,2.4299483299255402,2.5420303344726598,2.4490520954132098,2.3906834125518799,2.4765830039978001,2.4936084747314502,2.5247271060943599,2.54471778869629,2.53918480873108,2.54552221298218,2.5526983737945601,2.5639333724975599,2.5611753463745099,2.56861472129822,2.5710935592651398,2.57420825958252,2.5741758346557599,2.5788726806640598,2.5789062976837198,2.59378290176392,2.6088099479675302,2.6259028911590598,2.64452123641968,2.6644773483276398]
["   Coal to Liquids",0,0,0,0,0,1.5133428573608401,1.3742095232009901,1.19064140319824,1.3664953708648699,1.33487153053284,1.31654036045074,1.30223417282104,1.30838906764984,1.32146644592285,1.3489345312118499,1.3524934053421001,1.3570195436477701,1.3626403808593801,1.37119424343109,1.3635557889938399,1.3662919998168901,1.37254309654236,1.37609398365021,1.3784751892089799,1.3805129528045701,24.056577682495099,24.1739406585693,24.2586994171143,24.288969039916999]
["   Electricity",18.400894165039102,18.6226921081543,20.334409713745099,19.159486770629901,16.828172683715799,17.264308929443398,17.156070709228501,17.083604812622099,17.1988334655762,17.318143844604499,17.615074157714801,17.910154342651399,18.210170745849599,18.456880569458001,18.803001403808601,19.085206985473601,19.30615234375,19.3043308258057,19.3253479003906,19.324813842773398,19.354219436645501,19.614883422851602,19.97239112854,20.29469871521,20.560989379882798,21.3195495605469,21.43874168396,21.398374557495099,21.4992275238037,{"$f":"AD266+($AI$266-$AD$266)/5","v":21.318281718011935},{"$f":"AE266+($AI$266-$AD$266)/5","v":21.13733591222017},{"$f":"AF266+($AI$266-$AD$266)/5","v":20.956390106428405},{"$f":"AG266+($AI$266-$AD$266)/5","v":20.775444300636639},{"$f":"T436*$E$747","v":20.594498494844878},{"$f":"AI266+($AX$266-$AI$266)/15","v":20.60819416894353},{"$f":"AJ266+($AX$266-$AI$266)/15","v":20.621889843042183},20.635585517140836,20.649281191239488,20.662976865338141,20.676672539436794,20.690368213535447,20.704063887634099,20.717759561732752,20.731455235831405,20.745150909930057,20.75884658402871,20.772542258127363,20.786237932226015,{"$f":"AI266*$B$747","v":20.799933606324664},{"$f":"AX266+($BM$266-$AX$266)/15","v":20.807002050879195},{"$f":"AY266+($BM$266-$AX$266)/15","v":20.814070495433725},20.821138939988256,20.828207384542786,20.835275829097316,20.842344273651847,20.849412718206377,20.856481162760907,20.863549607315438,20.870618051869968,20.877686496424499,20.884754940979029,20.891823385533559,20.89889183008809,{"$f":"AX266*$C$747","v":20.905960274642634},{"$f":"BM266+($BR$266-$BM$266)/5","v":20.913064750255749},{"$f":"BN266+($BR$266-$BM$266)/5","v":20.920169225868865},{"$f":"BO266+($BR$266-$BM$266)/5","v":20.92727370148198},{"$f":"BP266+($BR$266-$BM$266)/5","v":20.934378177095095},{"$f":"BM266*$D$747","v":20.94148265270821}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17.292875289916999,17.531343460083001,17.526832580566399,17.756109237670898,{"$f":"AD267+($AI$267-$AD$267)/5","v":18.740759573600641},{"$f":"AE267+($AI$267-$AD$267)/5","v":19.725409909530384},{"$f":"AF267+($AI$267-$AD$267)/5","v":20.710060245460127},{"$f":"AG267+($AI$267-$AD$267)/5","v":21.69471058138987},{"$f":"T437*$E$744","v":22.67936091731961},{"$f":"AI267+($AX$267-$AI$267)/15","v":22.91940642537169},{"$f":"AJ267+($AX$267-$AI$267)/15","v":23.159451933423771},23.399497441475852,23.639542949527932,23.879588457580013,24.119633965632094,24.359679473684174,24.599724981736255,24.839770489788336,25.079815997840416,25.319861505892497,25.559907013944578,25.799952521996659,26.039998030048739,{"$f":"AI267*$B$744","v":26.28004353810082},{"$f":"AX267+($BM$267-$AX$267)/15","v":26.429681543018035},{"$f":"AY267+($BM$267-$AX$267)/15","v":26.579319547935249},26.728957552852464,26.878595557769678,27.028233562686893,27.177871567604107,27.327509572521322,27.477147577438537,27.626785582355751,27.776423587272966,27.92606159219018,28.075699597107395,28.225337602024609,28.374975606941824,{"$f":"AX267*$C$744","v":28.524613611859053},{"$f":"BM267+($BR$267-$BM$267)/5","v":28.687032150691561},{"$f":"BN267+($BR$267-$BM$267)/5","v":28.849450689524069},{"$f":"BO267+($BR$267-$BM$267)/5","v":29.011869228356577},{"$f":"BP267+($BR$267-$BM$267)/5","v":29.174287767189085},{"$f":"BM267*$D$744","v":29.336706306021593}]
[" Transportation",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,11.227470397949199,11.517865180969199,11.5089683532715,11.7493782043457]
["   Liquefied Petroleum Gases 3/",22.296371459960898,25.0072345733643,28.759458541870099,21.685003280639599,20.534326553344702,22.796831130981399,24.8035278320313,26.570152282714801,28.076972961425799,29.693559646606399,30.7330017089844,31.595745086669901,32.463813781738303,32.853603363037102,33.095050811767599,33.3141899108887,33.425758361816399,33.752655029296903,33.878787994384801,33.426109313964801,33.692680358886697,33.960933685302699,34.291332244872997,34.467491149902301,34.819602966308601,16.025825500488299,16.333782196044901,16.2625331878662,16.470952987670898,{"$f":"AD269+($AI$269-$AD$269)/5","v":17.380928094850553},{"$f":"AE269+($AI$269-$AD$269)/5","v":18.290903202030208},{"$f":"AF269+($AI$269-$AD$269)/5","v":19.200878309209862},{"$f":"AG269+($AI$269-$AD$269)/5","v":20.110853416389517},{"$f":"T439*$E$744","v":21.020828523569172},{"$f":"AI269+($AX$269-$AI$269)/15","v":21.243319601735415},{"$f":"AJ269+($AX$269-$AI$269)/15","v":21.465810679901658},21.688301758067901,21.910792836234144,22.133283914400387,22.35577499256663,22.578266070732873,22.800757148899116,23.023248227065359,23.245739305231602,23.468230383397845,23.690721461564088,23.913212539730331,24.135703617896574,{"$f":"AI269*$B$744","v":24.358194696062842},{"$f":"AX269+($BM$269-$AX$269)/15","v":24.496889734844629},{"$f":"AY269+($BM$269-$AX$269)/15","v":24.635584773626416},24.774279812408203,24.91297485118999,25.051669889971777,25.190364928753564,25.32905996753535,25.467755006317137,25.606450045098924,25.745145083880711,25.883840122662498,26.022535161444285,26.161230200226072,26.299925239007859,{"$f":"AX269*$C$744","v":26.438620277789649},{"$f":"BM269+($BR$269-$BM$269)/5","v":26.589161215265516},{"$f":"BN269+($BR$269-$BM$269)/5","v":26.739702152741383},{"$f":"BO269+($BR$269-$BM$269)/5","v":26.89024309021725},{"$f":"BP269+($BR$269-$BM$269)/5","v":27.040784027693118},{"$f":"BM269*$D$744","v":27.191324965168981}]
["   E85 4/",25.5142211914063,26.818180084228501,34.073703765869098,20.3962516784668,18.869060516357401,22.499189376831101,24.345371246337901,25.8835773468018,27.376197814941399,25.5507621765137,26.3307495117188,27.042121887206999,27.074653625488299,28.861484527587901,29.593324661254901,29.691083908081101,29.8394565582275,30.056737899780298,30.123649597168001,30.045396804809599,30.335887908935501,30.1821899414063,30.567377090454102,31.227724075317401,30.935503005981399,8.1832656860351598,8.1197490692138707,8.3803300857543892,8.2735004425048793]
["   Motor Gasoline 5/",21.784559249877901,22.982162475585898,26.1744689941406,15.6736001968384,17.7131462097168,20.6617527008057,22.301433563232401,23.517950057983398,24.816135406494102,26.137458801269499,27.061580657958999,27.993299484252901,28.802474975585898,29.411088943481399,29.938217163085898,30.057752609252901,30.3159790039063,30.494945526123001,30.528341293335,30.4458103179932,30.726751327514599,30.704950332641602,31.110511779785199,31.9617519378662,31.583656311035199,13.240598678588899,13.359972000122101,13.395259857177701,13.453570365905801]
["   Jet Fuel 6/",15.2446508407593,16.0964660644531,22.1856594085693,10.540905952453601,10.4131317138672,12.992267608642599,14.8510446548462,16.4927158355713,17.888269424438501,19.120731353759801,20.025011062622099,20.925888061523398,21.650459289550799,22.054113388061499,22.358533859252901,22.535087585449201,22.624557495117202,22.875423431396499,23.088819503784201,22.878332138061499,23.229129791259801,23.440977096557599,23.911849975585898,24.3618278503418,24.669164657592798,24.345100402831999,24.401657104492202,24.482112884521499,24.4609375]
["   Diesel Fuel (distillate fuel oil) 7/",20.2724208831787,20.921422958373999,27.066003799438501,15.379162788391101,14.6322994232178,17.082887649536101,18.906814575195298,21.012025833129901,22.391767501831101,23.401908874511701,24.249780654907202,25.151100158691399,25.830009460449201,26.267305374145501,26.5901203155518,26.487575531005898,26.7318305969238,26.979133605956999,27.001283645629901,26.997362136840799,27.317785263061499,27.182266235351602,27.638069152831999,28.388862609863299,28.337171554565401]
["   Residual Fuel Oil",8.20648097991943,9.4357099533081108,14.2847747802734,6.3925981521606401,6.5852246284484899,8.6673641204834002,10.3328533172607,11.815202713012701,13.023598670959499,14.4141092300415,15.219378471374499,15.915946006774901,16.592523574829102,16.9536838531494,17.162534713745099,17.429744720458999,17.456914901733398,17.5628662109375,17.630765914916999,17.410764694213899,17.6028347015381,17.926630020141602,18.257143020629901,18.451654434204102,18.835027694702099,10.4858131408691,10.572740554809601,10.740042686462401,10.786236763000501]
["   Natural Gas 8/",15.5415086746216,15.4958410263062,16.8896675109863,12.7877197265625,13.502610206604,13.8291311264038,13.8390712738037,13.843875885009799,13.934069633483899,14.0993509292603,14.229956626892101,14.3684740066528,14.5119123458862,14.701403617858899,14.9462375640869,15.0934410095215,15.092455863952599,14.8220539093018,14.7596139907837,14.661186218261699,14.786495208740201,15.012266159057599,15.2852840423584,15.4684591293335,15.6974124908447,6.7344188690185502,6.7479009628295898,6.8497943878173801,6.84698486328125]
["   Electricity",30.349004745483398,30.777971267700199,33.734138488769503,31.501590728759801,27.327030181884801,28.561843872070298,28.965305328369102,28.9159030914307,28.7644939422607,28.526710510253899,28.644361495971701,28.6527919769287,28.819505691528299,28.888120651245099,29.142557144165,29.470201492309599,29.764074325561499,29.801677703857401,29.921939849853501,30.035243988037099,30.304817199706999,30.8045558929443,31.450147628784201,31.910936355590799,32.484222412109403,6.1479806900024396,6.2516684532165501,6.3134694099426296,6.3304243087768599,{"$f":"AD276+($AI$276-$AD$276)/5","v":6.3370805697154289},{"$f":"AE276+($AI$276-$AD$276)/5","v":6.3437368306539978},{"$f":"AF276+($AI$276-$AD$276)/5","v":6.3503930915925668},{"$f":"AG276+($AI$276-$AD$276)/5","v":6.3570493525311358},{"$f":"T446*$E$742","v":6.363705613469703},{"$f":"AI276+($AX$276-$AI$276)/15","v":6.4357380850865695},{"$f":"AJ276+($AX$276-$AI$276)/15","v":6.5077705567034361},6.5798030283203026,6.6518354999371692,6.7238679715540357,6.7959004431709022,6.8679329147877688,6.9399653864046353,7.0119978580215019,7.0840303296383684,7.156062801255235,7.2280952728721015,7.3001277444889681,7.3721602161058346,{"$f":"AI276*$B$742","v":7.4441926877227056},{"$f":"AX276+($BM$276-$AX$276)/15","v":7.51790324705948},{"$f":"AY276+($BM$276-$AX$276)/15","v":7.5916138063962544},7.6653243657330288,7.7390349250698032,7.8127454844065776,7.886456043743352,7.9601666030801264,8.0338771624169016,8.107587721753676,8.1812982810904504,8.2550088404272248,8.3287193997639992,8.4024299591007736,8.476140518437548,{"$f":"AX276*$C$742","v":8.5498510777743242},{"$f":"BM276+($BR$276-$BM$276)/5","v":8.6345095936975138},{"$f":"BN276+($BR$276-$BM$276)/5","v":8.7191681096207034},{"$f":"BO276+($BR$276-$BM$276)/5","v":8.8038266255438931},{"$f":"BP276+($BR$276-$BM$276)/5","v":8.8884851414670827},{"$f":"BM276*$D$742","v":8.9731436573902759}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.65011918544769,1.6656291484832799,1.67491066455841,1.68971908092499,{"$f":"AD277+($AI$277-$AD$277)/5","v":1.6902380098146863},{"$f":"AE277+($AI$277-$AD$277)/5","v":1.6907569387043826},{"$f":"AF277+($AI$277-$AD$277)/5","v":1.6912758675940789},{"$f":"AG277+($AI$277-$AD$277)/5","v":1.6917947964837752},{"$f":"T447*$E$740","v":1.692313725373471},{"$f":"AI277+($AX$277-$AI$277)/15","v":1.6972753042285647},{"$f":"AJ277+($AX$277-$AI$277)/15","v":1.7022368830836583},1.7071984619387519,1.7121600407938455,1.7171216196489392,1.7220831985040328,1.7270447773591264,1.7320063562142201,1.7369679350693137,1.7419295139244073,1.7468910927795009,1.7518526716345946,1.7568142504896882,1.7617758293447818,{"$f":"AI277*$B$740","v":1.7667374081998766},{"$f":"AX277+($BM$277-$AX$277)/15","v":1.7700881577207939},{"$f":"AY277+($BM$277-$AX$277)/15","v":1.7734389072417112},1.7767896567626285,1.7801404062835458,1.783491155804463,1.7868419053253803,1.7901926548462976,1.7935434043672149,1.7968941538881322,1.8002449034090495,1.8035956529299668,1.8069464024508841,1.8102971519718014,1.8136479014927187,{"$f":"AX277*$C$740","v":1.8169986510136373},{"$f":"BM277+($BR$277-$BM$277)/5","v":1.8204447247375162},{"$f":"BN277+($BR$277-$BM$277)/5","v":1.823890798461395},{"$f":"BO277+($BR$277-$BM$277)/5","v":1.8273368721852739},{"$f":"BP277+($BR$277-$BM$277)/5","v":1.8307829459091527},{"$f":"BM277*$D$740","v":1.8342290196330318}]
[" Electric Power 9/"]
["   Distillate Fuel Oil",13.773189544677701,14.7725219726563,19.176651000976602,12.4995737075806,9.7914295196533203,12.0805196762085,13.8671321868896,15.216549873352101,16.469785690307599,17.9636936187744,18.832237243652301,19.641151428222699,20.348432540893601,20.710233688354499,20.980741500854499,21.161005020141602,21.2950553894043,21.596014022827099,21.884708404541001,21.582948684692401,21.8727416992188,22.200710296630898,22.548530578613299,22.812198638916001,23.2114353179932,18.0768718719482,18.184886932373001,18.263076782226602,18.304286956787099]
["   Residual Fuel Oil",8.3781757354736293,8.5664386749267596,14.309384346008301,6.51324510574341,6.6763448715209996,9.3123388290405291,10.994701385498001,12.5300750732422,13.7526693344116,15.155575752258301,15.963142395019499,16.617677688598601,17.274333953857401,17.322587966918899,17.542411804199201,17.799869537353501,17.916141510009801,18.075910568237301,18.1613368988037,17.935956954956101,18.128087997436499,18.400978088378899,18.7218933105469,18.9085083007813,19.247135162353501,21.3195495605469,21.43874168396,21.398374557495099,21.4992275238037]
["   Natural Gas",7.0546379089355504,7.0191597938537598,8.8716125488281303,4.5556221008300799,5.1293134689331099,5.4535460472106898,5.5187635421752903,5.53977298736572,5.6835036277770996,5.8920464515686,6.0819325447082502,6.2693996429443404,6.4775133132934597,6.7354197502136204,7.0278439521789604,7.2539091110229501,7.3283839225768999,7.1506276130676296,7.1924118995666504,7.1398839950561497,7.2806253433227504,7.5354790687561,7.8600792884826696,8.0742120742797905,8.3395175933837908,17.291141510009801,17.529483795166001,17.525184631347699,17.7543029785156]
["   Steam Coal",1.7355252504348799,1.7800002098083501,1.9310736656189,1.98230564594269,1.86225914955139,1.87335216999054,1.85759365558624,1.8817487955093399,1.9043176174163801,1.90719401836395,1.9170492887496899,1.9259506464004501,1.94080138206482,1.94636797904968,1.9562891721725499,1.9622501134872401,1.9753552675247199,1.9811542034149201,1.98549652099609,1.9898830652236901,1.99634909629822,2.00744533538818,2.0202190876007098,2.0336120128631601,2.0445194244384801,11.227470397949199,11.517865180969199,11.5089683532715,11.7493782043457]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15.2353620529175,15.5302953720093,15.500846862793001,15.7047281265259]
[" Average Price to All Users 10/",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.7013258934020996,7.6767330169677699,7.8322434425354004,7.7872447967529297]
["   Liquefied Petroleum Gases",15.657142639160201,18.5313529968262,19.701341629028299,16.4090671539307,16.297544479370099,18.4262371063232,20.2184352874756,21.813219070434599,23.252103805541999,24.811630249023398,25.812454223632798,26.627546310424801,27.460300445556602,27.8579425811768,28.113265991210898,28.325565338134801,28.4571437835693,28.7732944488525,28.920036315918001,28.525373458862301,28.814060211181602,29.1242790222168,29.486963272094702,29.629682540893601,30.0484523773193,7.8213167190551802,7.9383788108825701,8.0273618698120099,8.0851049423217791]
["   E85 4/",25.5142211914063,26.818180084228501,34.073703765869098,20.3962516784668,18.869060516357401,22.499189376831101,24.345371246337901,25.8835773468018,27.376197814941399,25.5507621765137,26.3307495117188,27.042121887206999,27.074653625488299,28.861484527587901,29.593324661254901,29.691083908081101,29.8394565582275,30.056737899780298,30.123649597168001,30.045396804809599,30.335887908935501,30.1821899414063,30.567377090454102,31.227724075317401,30.935503005981399,2.7168338298797599,2.7307398319244398,2.7413196563720699,2.7546591758728001]
["   Motor Gasoline 5/",21.649000167846701,22.8191947937012,26.0107421875,15.8019914627075,17.711067199706999,20.6589241027832,22.298402786254901,23.5152263641357,24.813198089599599,26.134485244751001,27.0586547851563,27.9900207519531,28.799554824829102,29.408401489257798,29.935087203979499,30.054672241210898,30.314332962036101,30.492042541503899,30.525100708007798,30.442491531372099,30.723676681518601,30.701581954956101,31.107343673706101,31.957983016967798,31.580909729003899,1.67883205413818,1.6938681602478001,1.7024568319320701,1.71655297279358]
["   Jet Fuel",15.2446508407593,16.0964660644531,22.1856594085693,10.540905952453601,10.4131317138672,12.992267608642599,14.8510446548462,16.4927158355713,17.888269424438501,19.120731353759801,20.025011062622099,20.925888061523398,21.650459289550799,22.054113388061499,22.358533859252901,22.535087585449201,22.624557495117202,22.875423431396499,23.088819503784201,22.878332138061499,23.229129791259801,23.440977096557599,23.911849975585898,24.3618278503418,24.669164657592798,1.2833950519561801,1.3286876678466799,1.33012855052948,1.33445107936859]
["   Distillate Fuel Oil",19.171348571777301,19.9431552886963,25.721439361572301,15.1513471603394,13.5963325500488,16.098552703857401,18.014595031738299,20.0945529937744,21.487236022949201,22.551927566528299,23.4185886383057,24.295482635498001,25.028078079223601,25.4735622406006,25.7968635559082,25.744600296020501,26.0401725769043,26.245742797851602,26.316581726074201,26.282798767089801,26.623888015747099,26.532428741455099,26.9911499023438,27.692060470581101,27.7130451202393,23.429731369018601,23.480413436889599,23.589033126831101,23.596023559570298]
["   Residual Fuel Oil",8.4246683120727504,9.3672227859497106,14.1781015396118,6.5043296813964799,6.9149212837219203,9.2013835906982404,10.8588418960571,12.3554439544678,13.5696716308594,14.9571332931519,15.7562828063965,16.419845581054702,17.090215682983398,17.3671054840088,17.589653015136701,17.8480415344238,17.911899566650401,18.041828155517599,18.112939834594702,17.862413406372099,18.047613143920898,18.333000183105501,18.6528930664063,18.8375339508057,19.187860488891602]
["   Natural Gas",9.5015735626220703,9.0060253143310494,10.1816816329956,6.76324558258057,7.4289712905883798,7.7374553680419904,7.7907910346984899,7.79954290390015,7.91036033630371,8.0721502304077095,8.2674913406372106,8.4630060195922905,8.6615943908691406,8.9140930175781303,9.2212562561035192,9.4307956695556605,9.4883728027343803,9.2674760818481392,9.2395153045654297,9.1623344421386701,9.3142642974853498,9.5711297988891602,9.9057645797729492,10.151716232299799,10.4206848144531]
["   Metallurgical Coal",3.6353600025177002,3.6099998950958301,4.0558156967163104,4.0487108230590803,3.9977276325225799,4.1121706962585396,4.1809573173522896,4.2343683242797896,4.27162742614746,4.2985162734985396,4.3192996978759801,4.3337044715881303,4.3530845642089799,4.3696141242981001,4.3899216651916504,4.4470157623290998,4.5093812942504901,4.5352845191955602,4.5618190765380904,4.5643453598022496,4.5493078231811497,4.5490665435790998,4.5331215858459499,4.4955492019653303,4.4319190979003897,253.732666015625,257.28918457031301,259.96432495117199,262.21316528320301]
["   Other Coal",1.7776364088058501,1.81885313987732,1.9676311016082799,2.0067975521087602,1.88941025733948,1.9042230844497701,1.89033174514771,1.9154095649719201,1.93832087516785,1.94072294235229,1.9500694274902299,1.9586881399154701,1.9732190370559699,1.9783339500427199,1.98810267448425,1.9938982725143399,2.0064799785614,2.0119984149932901,2.0163278579711901,2.0205180644989,2.0271856784820601,2.0382561683654798,2.0508835315704301,2.0641281604766801,2.0750961303710902,208.50216674804699,213.246017456055,217.97378540039099,222.08200073242199]
["   Coal to Liquids",0,0,0,0,0,1.5133428573608401,1.3742095232009901,1.19064140319824,1.3664953708648699,1.33487153053284,1.31654036045074,1.30223417282104,1.30838906764984,1.32146644592285,1.3489345312118499,1.3524934053421001,1.3570195436477701,1.3626403808593801,1.37119424343109,1.3635557889938399,1.3662919998168901,1.37254309654236,1.37609398365021,1.3784751892089799,1.3805129528045701,212.89649963378901,216.30204772949199,219.267822265625,222.079177856445]
["   Electricity",26.672916412353501,26.680915832519499,27.799331665039102,26.6892414093018,24.2756156921387,25.0947151184082,25.0493679046631,25.093559265136701,25.339256286621101,25.454051971435501,25.7708930969238,26.1124782562256,26.474697113037099,26.7419338226318,27.1641750335693,27.529588699340799,27.7828693389893,27.754991531372099,27.792310714721701,27.7856330871582,27.867961883544901,28.2280673980713,28.6754856109619,29.0858860015869,29.4564533233643,588.97521972656295,607.12139892578102,615.45501708984398,632.78991699218795]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1264.10656738281,1293.95861816406,1312.66088867188,1339.16430664063]
["Non-Renewable Energy Expenditures by Sector",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.38684526085853599,0.443235874176025,0.46923574805259699,0.51463860273361195]
["(billion 2007 dollars)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1264.49340820313,1294.40185546875,1313.13012695313,1339.67895507813]
[" Residential",231.10064697265599,238.40081787109401,250.00378417968801,223.81915283203099,215.29118347168,224.09677124023401,227.34310913085901,227.85260009765599,231.24415588378901,234.18721008300801,238.75100708007801,243.18489074707,248.169021606445,252.72660827636699,258.44952392578102,262.50808715820301,265.94851684570301,267.30322265625,270.58847045898398,272.04168701171898,276.25186157226602,282.20260620117199,288.93267822265602,293.60751342773398,298.90402221679699]
[" Commercial",170.28274536132801,172.89260864257801,183.352294921875,163.89425659179699,157.14476013183599,164.69047546386699,166.42567443847699,169.00093078613301,173.04789733886699,176.93461608886699,182.04042053222699,187.24485778808599,192.69107055664099,197.508544921875,203.26272583007801,208.31881713867199,212.33370971679699,214.22947692871099,217.23475646972699,219.65505981445301,223.61666870117199,229.31947326660199,235.82908630371099,241.79779052734401,247.76422119140599]
[" Industrial",216.08058166503901,226.88609313964801,248.66896057128901,181.39601135253901,151.70443725585901,172.23597717285199,186.63681030273401,200.19924926757801,207.03741455078099,213.45352172851599,218.62767028808599,224.29528808593801,229.96401977539099,233.76069641113301,239.065841674805,241.45851135253901,242.383544921875,242.41815185546901,242.89247131347699,240.916915893555,241.41357421875,242.50785827636699,244.85752868652301,245.86729431152301,245.87216186523401]
[" Transportation",564.62982177734398,596.84759521484398,693.65460205078102,393.76574707031301,430.90808105468801,516.84307861328102,568.141357421875,610.89111328125,646.41064453125,676.39013671875,696.72686767578102,719.33160400390602,737.13671875,750.27301025390602,759.33123779296898,760.33734130859398,761.04602050781295,771.55059814453102,780.57421875,783.147216796875,796.70227050781295,794.56842041015602,811.39251708984398,832.07995605468795,835.36431884765602]
["   Total Non-Renewable Expenditures",1182.09375,1235.02709960938,1375.6796875,962.87518310546898,955.04846191406295,1077.86633300781,1148.54699707031,1207.94384765625,1257.74011230469,1300.96545410156,1336.14599609375,1374.056640625,1407.96081542969,1434.26879882813,1460.109375,1472.62280273438,1481.71179199219,1495.50146484375,1511.28991699219,1515.76086425781,1537.984375,1548.59838867188,1581.01184082031,1613.3525390625,1627.90478515625]
[" Transportation Renewable Expenditures",3.2131362706422799E-2,4.0145620703697198E-2,3.7687420845031697E-2,2.54867300391197E-2,5.4010055959224701E-2,6.77362531423569E-2,8.3178348839283003E-2,9.4869345426559407E-2,0.113030456006527,1.97330021858215,4.8567194938659703,6.7303171157836896,10.514961242675801,15.7356252670288,22.100711822509801,25.9892463684082,35.539012908935497,35.597633361816399,34.1677055358887,35.613494873046903,37.140151977539098,45.276290893554702,47.974498748779297,53.190200805664098,54.179977416992202]
["   Total Expenditures",1182.12585449219,1235.06726074219,1375.71740722656,962.90069580078102,955.10247802734398,1077.93408203125,1148.63012695313,1208.03869628906,1257.85314941406,1302.93872070313,1341.00268554688,1380.78698730469,1418.47583007813,1450.00439453125,1482.21008300781,1498.61206054688,1517.25085449219,1531.09912109375,1545.45764160156,1551.37438964844,1575.12451171875,1593.87463378906,1628.986328125,1666.54272460938,1682.08471679688]
[]
[]
["Prices in Nominal Dollars"]
[" Residential"]
["   Liquefied Petroleum Gases",23.2563285827637,24.973464965820298,29.096658706665,22.194786071777301,21.477947235107401,24.1509113311768,26.557428359985401,28.936630249023398,31.2247924804688,33.758499145507798,35.743316650390597,37.599853515625,39.552177429199197,40.9905815124512,42.334590911865199,43.7123832702637,44.985881805419901,46.523696899414098,47.765018463134801,48.143123626708999,49.548942565917997,50.986961364746101,52.580905914306598,53.965934753417997,55.648300170898402]
["   Distillate Fuel Oil",17.979913711547901,19.664405822753899,24.466548919677699,16.188474655151399,13.8549404144287,16.4927158355713,18.5955104827881,20.348911285400401,22.1809597015381,24.3712253570557,25.9372863769531,27.5034885406494,29.0146675109863,30.168525695800799,31.2883205413818,32.275276184082003,33.246475219726598,34.4459838867188,35.640113830566399,35.882171630859403,37.065284729003899,38.310382843017599,39.641868591308601,40.905982971191399,42.365245819091797]
["   Natural Gas",13.3406887054443,12.691158294677701,13.2631158828735,11.061133384704601,11.614992141723601,12.061012268066399,12.1186227798462,12.236530303955099,12.476335525512701,12.8177757263184,13.333586692810099,13.900782585144,14.492022514343301,15.1641521453857,15.945101737976101,16.661958694458001,17.186347961425799,17.308622360229499,17.6488857269287,17.9868679046631,18.635103225708001,19.4500408172607,20.3657627105713,21.1996364593506,22.095756530761701]
["   Electricity",30.388185501098601,31.181957244873001,32.471218109130902,31.722009658813501,29.6958332061768,31.365653991699201,32.001548767089801,32.924289703369098,34.030689239502003,34.890899658203097,35.995761871337898,37.227577209472699,38.5026245117188,39.672031402587898,41.180412292480497,42.698352813720703,44.053905487060497,45.011627197265597,46.023651123046903,46.971866607666001,48.032154083252003,49.565544128417997,51.240451812744098,52.949665069580099,54.583251953125]
[]
[" Commercial"]
["   Liquefied Petroleum Gases",20.6414604187012,23.041419982910199,24.0578727722168,21.6475944519043,18.202018737793001,20.8180141448975,23.171899795532202,25.4778232574463,27.6801948547363,30.122516632080099,32.012001037597699,33.770454406738303,35.6212158203125,36.9546508789063,38.187240600585902,39.449775695800803,40.605808258056598,42.0293998718262,43.160079956054702,43.432140350341797,44.7312202453613,46.061283111572301,47.542713165283203,48.814918518066399,50.382663726806598]
["   Distillate Fuel Oil",14.625953674316399,16.054100036621101,21.4175109863281,14.1806936264038,11.1656141281128,13.940697669982899,16.055301666259801,18.2004089355469,20.072311401367202,21.922914505004901,23.436100006103501,24.993484497070298,26.4673175811768,27.614213943481399,28.7058811187744,29.4854850769043,30.5256862640381,31.597146987915,32.548923492431598,32.997859954833999,34.165657043457003,35.000114440917997,36.3691596984863,37.943679809570298,39.006439208984403]
["   Residual Fuel",8.64862155914307,10.3074436187744,13.7067270278931,6.9139137268066397,6.0204734802246103,9.0269355773925799,10.767860412597701,12.611166954040501,14.3083610534668,16.269037246704102,17.569841384887699,18.511304855346701,19.7891235351563,20.573390960693398,21.404872894287099,22.193275451660199,22.9593410491943,23.7928276062012,24.398706436157202,24.292516708373999,25.0136394500732,25.751762390136701,26.606601715087901,27.4516487121582,28.286119461059599]
["   Natural Gas",11.5840444564819,10.9898433685303,11.588038444519,9.1930990219116193,9.8226709365844709,10.233100891113301,10.334647178649901,10.4663095474243,10.734943389892599,11.106437683105501,11.600093841552701,12.1229543685913,12.6781578063965,13.3144483566284,14.069993019104,14.7329454421997,15.223674774169901,15.329276084899901,15.6546773910522,15.9318437576294,16.5416469573975,17.316057205200199,18.194717407226602,18.967941284179702,19.811794281005898]
["   Electricity",27.631908416748001,28.029735565185501,29.6960258483887,28.491619110107401,25.7724418640137,26.858903884887699,27.045906066894499,27.5620422363281,28.370775222778299,29.106733322143601,30.1617736816406,31.290737152099599,32.536418914794901,33.661582946777301,35.072307586669901,36.4632377624512,37.713531494140597,38.535266876220703,39.429233551025398,40.172752380371101,41.0662841796875,42.386928558349602,43.920989990234403,45.4139213562012,46.925571441650398]
[]
[" Industrial 1/"]
["   Liquefied Petroleum Gases",20.489143371581999,23.3795166015625,27.232301712036101,22.957033157348601,17.265552520751999,19.8652458190918,22.207704544067401,24.495702743530298,26.6714878082275,29.0830192565918,30.951156616210898,32.690711975097699,34.514808654785199,35.846107482910199,37.040077209472699,38.301750183105497,39.421558380127003,40.814861297607401,41.884078979492202,42.155609130859403,43.402267456054702,44.705905914306598,46.153343200683601,47.236614227294901,48.820529937744098]
["   Distillate Fuel Oil",15.3226671218872,16.8219394683838,22.4200763702393,14.749831199646,11.025536537170399,14.0721025466919,16.2283020019531,18.6841716766357,20.619239807128899,22.302150726318398,23.831027984619102,25.434989929199201,26.940843582153299,28.1489963531494,29.2844352722168,29.987220764160199,31.1475830078125,32.191192626953097,33.043167114257798,33.6753120422363,34.892765045166001,35.508182525634801,36.966400146484403,38.821296691894503,39.679729461669901]
["   Residual Fuel Oil",8.9709205627441406,10.5954837799072,14.049506187439,7.1343002319335902,10.215766906738301,12.8617763519287,14.814771652221699,16.696189880371101,18.396284103393601,20.378862380981399,21.7460041046143,22.969861984252901,24.3396511077881,25.3345756530762,26.3205471038818,27.310920715331999,28.174968719482401,29.129919052123999,29.910713195800799,30.004579544067401,30.867444992065401,31.741449356079102,32.901214599609403,33.791465759277301,34.9404487609863]
["   Natural Gas 2/",7.7454247474670401,7.5152516365051296,8.9947338104247994,5.0039734840393102,5.7063522338867196,6.1171517372131303,6.2487673759460396,6.4428400993347203,6.7520828247070304,7.1508984565734899,7.5258989334106401,7.9240221977233896,8.3488731384277308,8.8619937896728498,9.4837093353271502,9.9987487792968803,10.352954864501999,10.3336448669434,10.549848556518601,10.6489877700806,11.076291084289601,11.6912574768066,12.4464559555054,13.0579080581665,13.758059501647899]
["   Metallurgical Coal",3.53999996185303,3.6099998950958301,4.1449666023254403,4.1784791946411097,4.1485314369201696,4.3175525665283203,4.44484186172485,4.5821456909179696,4.7206311225891104,4.8563599586486799,4.9913563728332502,5.1233406066894496,5.2680139541626003,5.4137320518493697,5.5743689537048304,5.7906579971313503,6.0209679603576696,6.20045709609985,6.3775997161865199,6.5161404609680202,6.6299972534179696,6.7667918205261204,6.88553714752197,6.9704546928405797,7.0137753486633301]
["   Other Industrial Coal",2.3399634361267099,2.4299483299255402,2.5979068279266402,2.52754878997803,2.4808654785156299,2.6002757549285902,2.6509947776794398,2.73208808898926,2.8122007846832302,2.8687095642089799,2.94158983230591,3.0178208351135298,3.1028199195861799,3.17316722869873,3.2616541385650599,3.3479356765747101,3.4371068477630602,3.5193088054657,3.6053638458252002,3.6816923618316699,3.7800858020782502,3.88063645362854,3.98858737945557,4.1003923416137704,4.2166938781738299]
["   Coal to Liquids",0,0,0,0,0,1.5889266729354901,1.46094393730164,1.28843116760254,1.5101318359375,1.50810551643372,1.5213859081268299,1.53951179981232,1.58338570594788,1.63723039627075,1.71289122104645,1.76114201545715,1.8119050264358501,1.8629466295242301,1.9169825315475499,1.9466364383697501,1.9911848306655899,2.0416746139526398,2.09020328521729,2.1373581886291499,2.1847438812255899]
["   Electricity",17.918214797973601,18.6226921081543,20.7813816070557,19.773582458496101,17.462970733642599,18.126573562622099,18.238889694213899,18.4867153167725,19.006654739379901,19.565620422363299,20.355871200561499,21.173530578613299,22.037576675415,22.867145538330099,23.876249313354499,24.851699829101602,25.777753829956101,26.392097473144499,27.017583847045898,27.588447570800799,28.206142425537099,29.1773777008057,30.336851119995099,31.4674072265625,32.538986206054702]
[]
[" Transportation"]
["   Liquefied Petroleum Gases 3/",21.711509704589801,25.0072345733643,29.391622543335,22.380046844482401,21.3089294433594,23.935417175293001,26.369024276733398,28.752412796020501,31.0282287597656,33.547065734863303,35.514869689941399,37.352748870849602,39.287044525146499,40.7039604187012,42.024444580078097,43.379894256591797,44.630382537841797,46.145259857177699,47.363857269287102,47.7197074890137,49.102500915527301,50.517303466796903,52.086456298828097,53.442653656005902,55.104091644287102]
["   E85 4/",24.84494972229,26.818180084228501,34.822681427002003,21.049989700317401,19.580844879150401,23.622909545898398,25.881950378418001,28.009447097778299,30.2537937164307,28.866632461547901,30.4276523590088,31.969417572021499,32.765193939208999,35.757926940917997,37.577915191650398,38.662086486816399,39.8419189453125,41.092353820800803,42.114028930664098,42.893341064453097,44.2104301452637,44.896373748779297,46.4299926757813,48.419319152832003,48.957271575927699]
["   Motor Gasoline 5/",21.213121414184599,22.982162475585898,26.749811172485401,16.175968170166001,18.381326675415,21.693702697753899,23.709007263183601,25.449525833129901,27.424634933471701,29.529468536376999,31.27219581604,33.093906402587898,34.856166839599602,36.438858032226598,38.015861511230497,39.139541625976598,40.478176116943402,41.691452026367202,42.679801940917997,43.464977264404297,44.780059814453097,45.673988342285199,47.254981994628899,49.557445526122997,49.9830131530762]
["   Jet Fuel 6/",14.844763755798301,16.0964660644531,22.673322677612301,10.878761291503899,10.805939674377401,13.641165733337401,15.7883806228638,17.847295761108398,19.768560409545898,21.6021404266357,23.1407794952393,24.738756179809599,26.200944900512699,27.323936462402301,28.3911018371582,29.343944549560501,30.208518981933601,31.274351119995099,32.279064178466797,32.661514282226598,33.853298187255902,34.868740081787102,36.320652008056598,37.773586273193402,39.040420532226598]
["   Diesel Fuel (distillate fuel oil) 7/",19.740650177001999,20.921422958373999,27.660943984985401,15.872093200683601,15.1842641830444,17.936090469360401,20.100133895873999,22.737785339355501,24.745433807373001,26.438911437988299,28.0228977203369,29.7338352203369,31.2589511871338,32.543869018554702,33.764415740966797,34.490653991699197,35.692588806152301,36.884777069091797,37.7488403320313,38.541912078857401,39.811958312988303,40.433952331542997,41.980552673339801,44.0175971984863,44.845256805419901]
["   Residual Fuel Oil",7.9912142753601101,9.4357099533081108,14.5987691879272,6.5974926948547399,6.8336348533630398,9.1002550125122106,10.9850196838379,12.7856092453003,14.3925485610962,16.284711837768601,17.587419509887699,18.815961837768601,20.079933166503899,21.0047607421875,21.793167114257798,22.696048736572301,23.3086338043213,24.011238098144499,24.648492813110401,24.8559169769287,25.6537380218506,26.666080474853501,27.731492996215799,28.609724044799801,29.807550430297901]
["   Natural Gas 8/",15.1338348388672,15.4958410263062,17.260919570922901,13.197589874267599,14.011960029602101,14.5198259353638,14.7125358581543,14.9809007644653,15.3987216949463,15.929105758666999,16.444049835205099,16.986526489257798,17.562019348144499,18.214298248291001,18.978889465331999,19.653842926025401,20.151586532592798,20.264110565185501,20.6345119476318,20.930568695068398,21.5493049621582,22.330928802490199,23.217420578002901,23.984209060668899,24.842088699340799]
["   Electricity",29.552911758422901,30.777971267700199,34.475650787353501,32.511272430419901,28.3578701019287,29.9883632659912,30.793474197387699,31.290824890136701,31.788017272949201,32.228786468505902,33.101249694824197,33.873565673828097,34.876777648925803,35.790927886962898,37.005527496337898,38.374465942382798,39.741268157958999,40.743644714355497,41.832027435302699,42.8788452148438,44.165149688720703,45.822151184082003,47.770866394042997,49.4786567687988,51.408214569091797]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2027,2028,2029,2030,2031,2032,2033,2034,2035,2036,2037,2038,2039,2040,2041,2042,2043,2044,2045,2046,2047,2048,2049,2050,2051,2052,2053,2054,2055,2056,2057,2058,2059,2060,2061,2062,2063,2064,2065,2066,2067,2068,2069,2070]
[" Electric Power 9/"]
["   Distillate Fuel Oil",13.411901473999,14.7725219726563,19.598173141479499,12.9002075195313,10.160784721374499,12.683879852294901,14.742367744445801,16.466316223144499,18.200975418090799,20.294946670532202,21.762416839599599,23.219928741455099,24.625257492065401,25.658937454223601,26.641567230224599,27.554689407348601,28.433355331420898,29.525194168090799,30.595668792724599,30.812200546264599,31.8765468597412,33.023826599121101,34.249851226806598,35.370849609375,36.733474731445298]
["   Residual Fuel Oil",8.1584053039550799,8.5664386749267596,14.623919486999499,6.72200632095337,6.9281921386718803,9.7774429321289098,11.688641548156699,13.5591955184937,15.198254585266101,17.122402191162099,18.4469089508057,19.645553588867202,20.905046463012699,21.461814880371101,22.275539398193398,23.178005218505898,23.921798706054702,24.712652206420898,25.390251159668001,25.605690002441399,26.419223785400401,27.371679306030298,28.437421798706101,29.318086624145501,30.4597358703613]
["   Natural Gas",6.8695855140686,7.0191597938537598,9.0666198730468803,4.70163822174072,5.3228030204772896,5.7259230613708496,5.8670849800109899,5.9947657585143999,6.2809138298034703,6.6566915512084996,7.0282440185546902,7.4117355346679696,7.8389544486999503,8.3448457717895508,8.9240303039550799,9.4456386566162092,9.7849264144897496,9.7760477066040004,10.055270195007299,10.193024635314901,10.610521316528301,11.20911693573,11.9389839172363,12.519255638122599,13.197782516479499]
["   Steam Coal",1.6900001764297501,1.7800002098083501,1.97352075576782,2.0458421707153298,1.9325078725814799,1.9669165611267101,1.97483730316162,2.0363006591796902,2.1044862270355198,2.15470170974731,2.2153303623199498,2.2768745422363299,2.3487181663513201,2.4114518165588401,2.4841165542602499,2.5551335811614999,2.63751268386841,2.7085535526275599,2.7758009433746298,2.84079241752625,2.9094073772430402,2.9860992431640598,3.0685904026031499,3.1531631946563698,3.23557353019714]
[]
[" Average Price to All Users 10/"]
["   Liquefied Petroleum Gases",15.246436119079601,18.5313529968262,20.134397506713899,16.9350070953369,16.912326812744102,19.346534729003899,21.4945392608643,23.604782104492202,25.696203231811499,28.031579971313501,29.828712463378899,31.479301452636701,33.231895446777301,34.5145874023438,35.698520660400398,36.883983612060497,37.996242523193402,39.337680816650398,40.431327819824197,40.7233276367188,41.9925727844238,43.322719573974602,44.788909912109403,45.941520690917997,47.553462982177699]
["   E85 4/",24.84494972229,26.818180084228501,34.822681427002003,21.049989700317401,19.580844879150401,23.622909545898398,25.881950378418001,28.009447097778299,30.2537937164307,28.866632461547901,30.4276523590088,31.969417572021499,32.765193939208999,35.757926940917997,37.577915191650398,38.662086486816399,39.8419189453125,41.092353820800803,42.114028930664098,42.893341064453097,44.2104301452637,44.896373748779297,46.4299926757813,48.419319152832003,48.957271575927699]
["   Motor Gasoline 5/",21.081119537353501,22.8191947937012,26.582485198974599,16.308473587036101,18.3791694641113,21.690732955932599,23.705785751342798,25.446578979492202,27.421388626098601,29.526109695434599,31.268815994262699,33.090030670166001,34.852634429931598,36.4355278015137,38.011890411377003,39.135532379150398,40.475978851318402,41.687484741210902,42.675270080566399,43.460239410400398,44.775581359863303,45.668975830078097,47.250167846679702,49.551605224609403,49.978668212890597]
["   Jet Fuel",14.844763755798301,16.0964660644531,22.673322677612301,10.878761291503899,10.805939674377401,13.641165733337401,15.7883806228638,17.847295761108398,19.768560409545898,21.6021404266357,23.1407794952393,24.738756179809599,26.200944900512699,27.323936462402301,28.3911018371582,29.343944549560501,30.208518981933601,31.274351119995099,32.279064178466797,32.661514282226598,33.853298187255902,34.868740081787102,36.320652008056598,37.773586273193402,39.040420532226598]
["   Distillate Fuel Oil",18.668458938598601,19.9431552886963,26.286823272705099,15.636975288391101,14.1092176437378,16.902593612670898,19.1516017913818,21.744958877563501,23.745824813842798,25.478622436523398,27.0623779296875,28.722316741943398,30.288469314575199,31.560461044311499,32.757129669189503,33.523193359375,34.769081115722699,35.882114410400398,36.791599273681598,37.5217895507813,38.800697326660199,39.467311859130902,40.997920989990199,42.937191009521499,43.857540130615199]
["   Residual Fuel Oil",8.2036781311035192,9.3672227859497106,14.4897508621216,6.7128052711486799,7.1757683753967303,9.6609458923339808,11.544206619262701,13.370221138000501,14.996021270751999,16.898206710815401,18.207862854003899,19.411674499511701,20.6822299957275,21.516969680786101,22.335527420043899,23.2407321929932,23.916133880615199,24.6660556793213,25.322589874267599,25.500698089599599,26.3019409179688,27.270561218261701,28.332614898681602,29.2080383300781,30.365930557251001]
["   Natural Gas",9.2523355484008807,9.0060253143310494,10.405486106872599,6.98002004623413,7.7092094421386701,8.12390232086182,8.2825136184692401,8.4401350021362305,8.7418422698974592,9.1197204589843803,9.5538625717163104,10.0050344467163,10.4820852279663,11.0441122055054,11.7092485427856,12.280260086059601,12.668963432311999,12.670117378234901,12.917200088501,13.0803108215332,13.574273109436,14.23717212677,15.0462560653687,15.740474700927701,16.4913539886475]
["   Metallurgical Coal",3.53999996185303,3.6099998950958301,4.1449666023254403,4.1784791946411097,4.1485314369201696,4.3175525665283203,4.44484186172485,4.5821456909179696,4.7206311225891104,4.8563599586486799,4.9913563728332502,5.1233406066894496,5.2680139541626003,5.4137320518493697,5.5743689537048304,5.7906579971313503,6.0209679603576696,6.20045709609985,6.3775997161865199,6.5161404609680202,6.6299972534179696,6.7667918205261204,6.88553714752197,6.9704546928405797,7.0137753486633301]
["   Other Coal",1.73100674152374,1.81885313987732,2.01088166236877,2.0711190700531001,1.96068322658539,1.99932932853699,2.0096416473388699,2.07272601127625,2.1420636177063002,2.1925818920135498,2.2534883022308301,2.3155770301818799,2.38794946670532,2.4510562419891402,2.52451372146606,2.5963439941406299,2.6790707111358598,2.7507226467132599,2.8189043998718302,2.8845274448394802,2.9543473720550502,3.0319309234619101,3.1151678562164302,3.20047926902771,3.2839629650115998,{"$f":"Z527+($AI$357-$Y$527)/10","v":8.0623037763536161},{"$f":"AA357+($AI$357-$Y$527)/10","v":8.1146083992868938},8.1669130222201716,8.2192176451534493,8.2715222680867271,8.3238268910200048,8.3761315139532826,8.4284361368865603,{"$f":"T527*$E$742","v":8.4807407598198452},{"$f":"AI357+($AX$357-$AI$357)/15","v":8.5767365137369804},{"$f":"AJ357+($AX$357-$AI$357)/15","v":8.6727322676541156},8.7687280215712509,8.8647237754883861,8.9607195294055213,9.0567152833226565,9.1527110372397917,9.248706791156927,9.3447025450740622,9.4406982989911974,9.5366940529083326,9.6326898068254678,9.728685560742603,9.8246813146597383,{"$f":"AI357*$B$742","v":9.9206770685768717},{"$f":"AX357+($BM$357-$AX$357)/15","v":10.018909165246043},{"$f":"AY357+($BM$357-$AX$357)/15","v":10.117141261915215},10.215373358584387,10.313605455253558,10.41183755192273,10.510069648591902,10.608301745261073,10.706533841930245,10.804765938599417,10.902998035268588,11.00123013193776,11.099462228606932,11.197694325276103,11.295926421945275,{"$f":"AX357*$C$742","v":11.394158518614441},{"$f":"BM357+($BR$357-$BM$357)/5","v":11.506980665059427},{"$f":"BN357+($BR$357-$BM$357)/5","v":11.619802811504412},{"$f":"BO357+($BR$357-$BM$357)/5","v":11.732624957949398},{"$f":"BP357+($BR$357-$BM$357)/5","v":11.845447104394383},{"$f":"BM357*$D$742","v":11.95826925083937}]
["   Coal to Liquids",0,0,0,0,0,1.5889266729354901,1.46094393730164,1.28843116760254,1.5101318359375,1.50810551643372,1.5213859081268299,1.53951179981232,1.58338570594788,1.63723039627075,1.71289122104645,1.76114201545715,1.8119050264358501,1.8629466295242301,1.9169825315475499,1.9466364383697501,1.9911848306655899,2.0416746139526398,2.09020328521729,2.1373581886291499,2.1847438812255899,{"$f":"Z528+($AI$358-$Y$528)/10","v":22.224617194901626},{"$f":"AA358+($AI$358-$Y$528)/10","v":22.135413455621489},22.046209716341352,21.957005977061215,21.867802237781078,21.778598498500941,21.689394759220804,21.600191019940667,{"$f":"T528*$E$745","v":21.510987280660522},{"$f":"AI358+($AX$358-$AI$358)/15","v":21.502530865644818},{"$f":"AJ358+($AX$358-$AI$358)/15","v":21.494074450629114},21.48561803561341,21.477161620597705,21.468705205582001,21.460248790566297,21.451792375550593,21.443335960534888,21.434879545519184,21.42642313050348,21.417966715487776,21.409510300472071,21.401053885456367,21.392597470440663,{"$f":"AI358*$B$745","v":21.384141055424955},{"$f":"AX358+($BM$358-$AX$358)/15","v":21.397725276976207},{"$f":"AY358+($BM$358-$AX$358)/15","v":21.411309498527459},21.42489372007871,21.438477941629962,21.452062163181214,21.465646384732466,21.479230606283718,21.49281482783497,21.506399049386221,21.519983270937473,21.533567492488725,21.547151714039977,21.560735935591229,21.574320157142481,{"$f":"AX358*$C$745","v":21.587904378693722},{"$f":"BM358+($BR$358-$BM$358)/5","v":21.601618040381013},{"$f":"BN358+($BR$358-$BM$358)/5","v":21.615331702068303},{"$f":"BO358+($BR$358-$BM$358)/5","v":21.629045363755594},{"$f":"BP358+($BR$358-$BM$358)/5","v":21.642759025442885},{"$f":"BM358*$D$745","v":21.656472687130176}]
["   Electricity",25.973251342773398,26.680915832519499,28.4103908538818,27.544679641723601,25.191349029541001,26.348068237304702,26.6303806304932,27.154542922973601,28.002742767333999,28.757371902465799,29.780685424804702,30.870384216308601,32.039138793945298,33.131908416747997,34.493354797363303,35.847507476806598,37.095943450927699,37.945499420166001,38.854724884033203,39.667263031005902,40.613765716552699,41.989593505859403,43.556324005127003,45.098350524902301,46.616588592529297]
[]
["Non-Renewable Energy Expenditures by Sector"]
["(billion nominal dollars)"]
[" Residential",225.03859096661196,238.40081787109398,255.49913625772319,230.9929746666815,223.41247611699868,235.2892736225177,241.6920712265439,246.56659612211084,255.55094332875294,264.57905396662414,275.89920726734971,287.49516661999758,300.32909110683801,313.11554742582229,328.18192619930682,341.8235015289352,355.09694320426638,365.44612056098629,378.29315112389759,388.37155634393389,402.59953615177363,419.77981120164446,438.87123825530841,455.24534715742953,473.03338245571979]
[" Commercial",165.81601818957134,172.89260864257801,187.38257557629601,169.14737359110225,163.07263216137929,172.91593328178766,176.9297785804325,182.88131988639063,191.23749630338142,199.89645601118545,210.36479941888081,221.36240217535854,233.19080564556924,244.70314616363081,258.1051490216438,271.26123343313407,283.50995205362011,292.88584879534454,303.70259464185926,313.58347456242666,325.89089746765683,341.11550736031069,358.21009848865214,374.9131546581271,392.1016075075479]
[" Industrial",210.41252056252281,226.88609313964801,254.13497179068762,187.2100922767749,157.4270874391178,180.83829470805441,198.41655822177904,216.64201952030527,228.79975664936245,241.15463361452254,252.64480203410886,265.1637238738445,278.29776899368039,289.61773721654419,303.56832242347855,314.41390898844122,323.63277263436424,331.42426143912343,339.57307272400601,343.93727888891527,351.82746805051073,360.73339056833169,371.92375563686846,381.22301587849751,389.10731115707301]
[" Transportation",549.81888270324475,596.84759521484398,708.90187629235277,406.38667462869051,447.16295305198071,542.65678113398656,604.00010341071868,661.06483901631009,714.35686387994281,764.16924059162022,805.13331786340132,850.39970498506295,892.06783074940802,929.55049698437085,964.20679928883487,990.06920191633094,1016.1557534719609,1054.8326731961108,1091.2729592511287,1118.0349113947391,1161.085260138974,1181.9301954596156,1232.4560893451367,1290.1595195386233,1322.0136898683704,{"$f":"Z536+($AI$366-$Y$536)/10","v":5.5334229650972304},{"$f":"AA366+($AI$366-$Y$536)/10","v":5.5639341150042458},5.5944452649112613,5.6249564148182767,5.6554675647252921,5.6859787146323075,5.716489864539323,5.7470010144463384,{"$f":"T536*$E$742","v":5.7775121643533494},{"$f":"AI366+($AX$366-$AI$366)/15","v":5.8429093568498098},{"$f":"AJ366+($AX$366-$AI$366)/15","v":5.9083065493462703},5.9737037418427308,6.0391009343391913,6.1044981268356517,6.1698953193321122,6.2352925118285727,6.3006897043250332,6.3660868968214936,6.4314840893179541,6.4968812818144146,6.5622784743108751,6.6276756668073356,6.693072859303796,{"$f":"AI366*$B$742","v":6.7584700518002592},{"$f":"AX366+($BM$366-$AX$366)/15","v":6.8253907547799981},{"$f":"AY366+($BM$366-$AX$366)/15","v":6.8923114577597371},6.959232160739476,7.026152863719215,7.0930735666989539,7.1599942696786929,7.2269149726584319,7.2938356756381708,7.3607563786179098,7.4276770815976487,7.4945977845773877,7.5615184875571266,7.6284391905368656,7.6953598935166045,{"$f":"AX366*$C$742","v":7.7622805964963462},{"$f":"BM366+($BR$366-$BM$366)/5","v":7.8391407838260445},{"$f":"BN366+($BR$366-$BM$366)/5","v":7.9160009711557429},{"$f":"BO366+($BR$366-$BM$366)/5","v":7.9928611584854412},{"$f":"BP366+($BR$366-$BM$366)/5","v":8.0697213458151396},{"$f":"BM366*$D$742","v":8.1465815331448379}]
["   Total Non-Renewable Expenditures",1151.0859678463546,1235.02709960938,1405.9186066996403,993.73713091111074,991.07514876947641,1131.7003147881212,1221.038560105055,1307.1547250090439,1389.9450601614428,1469.7993497059265,1544.0421618496678,1624.4209976542634,1703.8854780296228,1776.9868521708881,1854.0622550605767,1917.5679054742993,1978.3954213642144,2044.5889248527621,2112.8417777408945,2163.9271994062915,2241.4031618089139,2303.558949985179,2401.4612280803153,2501.5410135735665,2576.2560875804752]
[" Transportation Renewable Expenditures",3.1288517293273019E-2,4.0145620703697205E-2,3.8515830891447944E-2,2.6303627333810531E-2,5.6047443014104255E-2,7.1119337023784479E-2,8.8428224145552056E-2,0.10266115711707489,0.12491143634290662,2.2293869286864165,5.6123954184121017,7.9566359351664051,12.724991751969894,19.495647700796784,28.06371652814466,33.841758141316177,47.452021910622882,48.667640008057987,47.767774332439714,50.842459413568172,54.12672288853372,67.349033728123644,72.870357898145016,82.472655922369356,85.74303480046683]
["   Total Expenditures",1151.1172301979784,1235.06726074219,1405.957155546361,993.76346133595302,991.13120249830877,1131.7714475332546,1221.1269368042056,1307.2573637523753,1390.0699789505047,1472.0286986549243,1549.6545225531884,1632.3776685401217,1716.6105344121597,1796.4824632434897,1882.1259667447755,1951.4096785174786,2025.8475094892897,2093.2565961526161,2160.609578738799,2214.7697023873047,2295.5298624598372,2370.9079156203875,2474.3315685955818,2584.0136458368329,2661.9990499371279,{"$f":"Z539+($AI$369-$Y$539)/10","v":15.611683809514826},{"$f":"AA369+($AI$369-$Y$539)/10","v":15.541748469704389},15.471813129893953,15.401877790083516,15.331942450273079,15.262007110462642,15.192071770652205,15.122136430841769,{"$f":"T539*$E$745","v":15.052201091031337},{"$f":"AI369+($AX$369-$AI$369)/15","v":15.046283758755285},{"$f":"AJ369+($AX$369-$AI$369)/15","v":15.040366426479233},15.034449094203181,15.028531761927129,15.022614429651076,15.016697097375024,15.010779765098972,15.00486243282292,14.998945100546868,14.993027768270816,14.987110435994763,14.981193103718711,14.975275771442659,14.969358439166607,{"$f":"AI369*$B$745","v":14.963441106890555},{"$f":"AX369+($BM$369-$AX$369)/15","v":14.972946595029557},{"$f":"AY369+($BM$369-$AX$369)/15","v":14.982452083168559},14.991957571307561,15.001463059446563,15.010968547585565,15.020474035724567,15.029979523863569,15.03948501200257,15.048990500141572,15.058495988280574,15.068001476419576,15.077506964558578,15.08701245269758,15.096517940836582,{"$f":"AX369*$C$745","v":15.106023428975591},{"$f":"BM369+($BR$369-$BM$369)/5","v":15.115619492174282},{"$f":"BN369+($BR$369-$BM$369)/5","v":15.125215555372973},{"$f":"BO369+($BR$369-$BM$369)/5","v":15.134811618571664},{"$f":"BP369+($BR$369-$BM$369)/5","v":15.144407681770355},{"$f":"BM369*$D$745","v":15.154003744969049}]
[]
[]
[]
["   1/ Includes energy for combined heat and power plants, except those whose primary business is to sell electricity, or electricity and heat, to the public."]
["   2/ Excludes use for lease and plant fuel.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Z544+($AI$374-$Y$544)/10","v":11.584123362673006},{"$f":"AA374+($AI$374-$Y$544)/10","v":11.952852829654059},12.321582296635112,12.690311763616165,13.059041230597218,13.427770697578271,13.796500164559324,14.165229631540377,{"$f":"T544*$E$744","v":14.533959098521429},{"$f":"AI374+($AX$374-$AI$374)/15","v":14.687791105011014},{"$f":"AJ374+($AX$374-$AI$374)/15","v":14.841623111500599},14.995455117990184,15.14928712447977,15.303119130969355,15.45695113745894,15.610783143948526,15.764615150438111,15.918447156927696,16.072279163417281,16.226111169906865,16.379943176396448,16.533775182886032,16.687607189375615,{"$f":"AI374*$B$744","v":16.841439195865195},{"$f":"AX374+($BM$374-$AX$374)/15","v":16.937333989857837},{"$f":"AY374+($BM$374-$AX$374)/15","v":17.033228783850479},17.129123577843121,17.225018371835763,17.320913165828404,17.416807959821046,17.512702753813688,17.60859754780633,17.704492341798971,17.800387135791613,17.896281929784255,17.992176723776897,18.088071517769539,18.18396631176218,{"$f":"AX374*$C$744","v":18.27986110575484},{"$f":"BM374+($BR$374-$BM$374)/5","v":18.383946243287554},{"$f":"BN374+($BR$374-$BM$374)/5","v":18.488031380820267},{"$f":"BO374+($BR$374-$BM$374)/5","v":18.592116518352981},{"$f":"BP374+($BR$374-$BM$374)/5","v":18.696201655885694},{"$f":"BM374*$D$744","v":18.800286793418415}]
["   3/ Includes Federal and State taxes while excluding county and local taxes."]
["   4/ E85 refers to a blend of 85 percent ethanol (renewable) and 15 percent motor gasoline (nonrenewable).  To address cold starting issues, the percentage of ethanol varies",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Z546+($AI$376-$Y$546)/10","v":13.665763245709009},{"$f":"AA376+($AI$376-$Y$546)/10","v":14.091688195895063},14.517613146081118,14.943538096267172,15.369463046453227,15.795387996639281,16.221312946825336,16.64723789701139,{"$f":"T546*$E$744","v":17.073162847197445},{"$f":"AI376+($AX$376-$AI$376)/15","v":17.253870586919582},{"$f":"AJ376+($AX$376-$AI$376)/15","v":17.43457832664172},17.615286066363858,17.795993806085995,17.976701545808133,18.157409285530271,18.338117025252409,18.518824764974546,18.699532504696684,18.880240244418822,19.060947984140959,19.241655723863097,19.422363463585235,19.603071203307373,{"$f":"AI376*$B$744","v":19.783778943029514},{"$f":"AX376+($BM$376-$AX$376)/15","v":19.896427356509733},{"$f":"AY376+($BM$376-$AX$376)/15","v":20.009075769989952},20.121724183470171,20.23437259695039,20.347021010430609,20.459669423910828,20.572317837391047,20.684966250871266,20.797614664351485,20.910263077831704,21.022911491311923,21.135559904792142,21.248208318272361,21.36085673175258,{"$f":"AX376*$C$744","v":21.47350514523281},{"$f":"BM376+($BR$376-$BM$376)/5","v":21.595774823509927},{"$f":"BN376+($BR$376-$BM$376)/5","v":21.718044501787045},{"$f":"BO376+($BR$376-$BM$376)/5","v":21.840314180064162},{"$f":"BP376+($BR$376-$BM$376)/5","v":21.962583858341279},{"$f":"BM376*$D$744","v":22.084853536618393}]
["seasonally.  The annual average ethanol content of 74 percent is used for this forecast."]
["   5/ Sales weighted-average price for all grades.  Includes Federal, State, and local taxes."]
["   6/ Kerosene-type jet fuel.  Includes Federal and State taxes while excluding county and local taxes."]
["   7/ Diesel fuel for on-road use.  Includes Federal and State taxes while excluding county and local taxes.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Z550+($AI$380-$Y$550)/10","v":17.944433063730909},{"$f":"AA380+($AI$380-$Y$550)/10","v":17.852387205459664},17.760341347188419,17.668295488917174,17.576249630645929,17.484203772374684,17.392157914103439,17.300112055832194,{"$f":"T550*$E$747","v":17.208066197560942},{"$f":"AI380+($AX$380-$AI$380)/15","v":17.219509839491277},{"$f":"AJ380+($AX$380-$AI$380)/15","v":17.230953481421611},17.242397123351946,17.253840765282281,17.265284407212615,17.27672804914295,17.288171691073284,17.299615333003619,17.311058974933953,17.322502616864288,17.333946258794622,17.345389900724957,17.356833542655291,17.368277184585626,{"$f":"AI380*$B$747","v":17.379720826515971},{"$f":"AX380+($BM$380-$AX$380)/15","v":17.385626979648983},{"$f":"AY380+($BM$380-$AX$380)/15","v":17.391533132781994},17.397439285915006,17.403345439048017,17.409251592181029,17.41515774531404,17.421063898447052,17.426970051580064,17.432876204713075,17.438782357846087,17.444688510979098,17.45059466411211,17.456500817245121,17.462406970378133,{"$f":"AX380*$C$747","v":17.468313123511169},{"$f":"BM380+($BR$380-$BM$380)/5","v":17.474249382977746},{"$f":"BN380+($BR$380-$BM$380)/5","v":17.480185642444322},{"$f":"BO380+($BR$380-$BM$380)/5","v":17.486121901910899},{"$f":"BP380+($BR$380-$BM$380)/5","v":17.492058161377475},{"$f":"BM380*$D$747","v":17.497994420844059}]
["   8/ Compressed natural gas used as a vehicle fuel.  Includes estimated motor vehicle fuel taxes and estimated dispensing costs or charges."]
["   9/ Includes electricity-only and combined heat and power plants whose primary business is to sell electricity, or electricity and heat, to the public."]
["   10/ Weighted averages of end-use fuel prices are derived from the prices shown in each sector and the corresponding sectoral consumption."]
["   Btu = British thermal unit."]
["   - - = Not applicable."]
["   Note:  Data for 2006 and 2007 are model results and may differ slightly from official EIA data reports."]
["   Sources:  2006 and 2007 prices for motor gasoline, distillate fuel oil, and jet fuel are based on prices in the Energy Information Administration (EIA), Petroleum Marketing Annual"]
["2007, DOE/EIA-0487(2007) (Washington, DC, August 2008).  2006 residential and commercial natural gas delivered prices:  EIA, Natural Gas Annual 2006, DOE/EIA-0131(2006)"]
["(Washington, DC, October, 2007).  2007 residential and commercial natural gas delivered prices:  EIA, Natural Gas Monthly, DOE/EIA-0130(2008/04) (Washington, DC, April 2008)."]
["2006 and 2007 industrial natural gas delivered prices are estimated based on:  EIA, Manufacturing Energy Consumption Survey 1994 and industrial and wellhead prices from the"]
["Natural Gas Annual 2006, DOE/EIA-0131(2006) (Washington, DC, October, 2007) and the Natural Gas Monthly, DOE/EIA-0130(2008/04) (Washington, DC, April 2008).  2006"]
["transportation sector natural gas delivered prices are based on:  EIA, Natural Gas Annual 2006, DOE/EIA-0131(2006) (Washington, DC, October, 2007) and estimated State taxes,",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Z562+($AI$392-$Y$562)/10","v":5.5024940130181221},{"$f":"AA392+($AI$392-$Y$562)/10","v":5.5327298577229831},5.5629657024278441,5.593201547132705,5.623437391837566,5.6536732365424269,5.6839090812472879,5.7141449259521488,{"$f":"T562*$E$742","v":5.7443807706570116},{"$f":"AI392+($AX$392-$AI$392)/15","v":5.809402940121136},{"$f":"AJ392+($AX$392-$AI$392)/15","v":5.8744251095852604},5.9394472790493849,6.0044694485135093,6.0694916179776337,6.1345137874417581,6.1995359569058825,6.264558126370007,6.3295802958341314,6.3946024652982558,6.4596246347623802,6.5246468042265047,6.5896689736906291,6.6546911431547535,{"$f":"AI392*$B$742","v":6.7197133126188779},{"$f":"AX392+($BM$392-$AX$392)/15","v":6.7862502559294402},{"$f":"AY392+($BM$392-$AX$392)/15","v":6.8527871992400025},6.9193241425505647,6.985861085861127,7.0523980291716892,7.1189349724822515,7.1854719157928137,7.252008859103376,7.3185458024139383,7.3850827457245005,7.4516196890350628,7.518156632345625,7.5846935756561873,7.6512305189667495,{"$f":"AX392*$C$742","v":7.7177674622773127},{"$f":"BM392+($BR$392-$BM$392)/5","v":7.7941868915344088},{"$f":"BN392+($BR$392-$BM$392)/5","v":7.8706063207915049},{"$f":"BO392+($BR$392-$BM$392)/5","v":7.947025750048601},{"$f":"BP392+($BR$392-$BM$392)/5","v":8.023445179305698},{"$f":"BM392*$D$742","v":8.099864608562795}]
["Federal taxes, and dispensing costs or charges.  2007 transportation sector natural gas delivered prices are model results.  2006 and 2007 electric power sector natural gas prices:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Z563+($AI$393-$Y$563)/10","v":1.3116492415795387},{"$f":"AA393+($AI$393-$Y$563)/10","v":1.314474997718583},1.3173007538576273,1.3201265099966717,1.322952266135716,1.3257780222747604,1.3286037784138047,1.3314295345528491,{"$f":"T563*$E$740","v":1.3342552906918941},{"$f":"AI393+($AX$393-$AI$393)/15","v":1.3381671025139799},{"$f":"AJ393+($AX$393-$AI$393)/15","v":1.3420789143360656},1.3459907261581514,1.3499025379802372,1.353814349802323,1.3577261616244087,1.3616379734464945,1.3655497852685803,1.3694615970906661,1.3733734089127518,1.3772852207348376,1.3811970325569234,1.3851088443790092,1.3890206562010949,{"$f":"AI393*$B$740","v":1.3929324680231794},{"$f":"AX393+($BM$393-$AX$393)/15","v":1.3955742685410359},{"$f":"AY393+($BM$393-$AX$393)/15","v":1.3982160690588925},1.4008578695767491,1.4034996700946056,1.4061414706124622,1.4087832711303188,1.4114250716481753,1.4140668721660319,1.4167086726838884,1.419350473201745,1.4219922737196016,1.4246340742374581,1.4272758747553147,1.4299176752731713,{"$f":"AX393*$C$740","v":1.4325594757910274},{"$f":"BM393+($BR$393-$BM$393)/5","v":1.4352764318903966},{"$f":"BN393+($BR$393-$BM$393)/5","v":1.4379933879897657},{"$f":"BO393+($BR$393-$BM$393)/5","v":1.4407103440891349},{"$f":"BP393+($BR$393-$BM$393)/5","v":1.4434273001885041},{"$f":"BM393*$D$740","v":1.4461442562878735}]
["EIA, Electric Power Monthly, April 2007 and April 2008, Table 4.13.B.  2006 and 2007 coal prices based on:  EIA, Quarterly Coal Report, October-December 2007,"]
["DOE/EIA-0121(2007/4Q) (Washington, DC, March 2008) and EIA, AEO2009 National Energy Modeling System run nostimls.d041409a.  2006 and 2007 electricity prices:  EIA, Annual"]
["Energy Review 2007, DOE/EIA-0384(2007) (Washington, DC, June 2008).  2006 and 2007 E85 prices derived from monthly prices in the Clean Cities Alternative Fuel Price Report."]
["Projections:  EIA, AEO2009 National Energy Modeling System run stimulus.d041409a."]
[]
[]
[]
[]
[]
["AEO 2007 Report #: DOE/EIA-0383(2007)"]
["Release date full report: February 2007"]
["Next release date full report: February 2008"]
[]
[" Table   3.  Energy Prices by Sector and Source"]
["                     (2005 dollars per million Btu, unless otherwise noted)"]
[]
[]
[]
[null,null,null,"2004","2005","2006","2007","2008","2009","2010","2011","2012","2013","2014","2015","2016","2017","2018","2019","2020","2021","2022","2023","2024","2025","2026"]
[]
[]
[" Residential"]
["   Liquefied Petroleum Gases",null,null,18.210411071777301,19.293371200561499,21.158409118652301,24.5404376983643,24.494813919067401,23.9600429534912,23.672391891479499,23.2634162902832,23.106723785400401,22.905719757080099,22.942964553833001,22.881586074829102,22.979688644409201,23.190465927123999,23.129106521606399,23.088548660278299,23.183416366577099,23.1546516418457,23.285535812377901,23.420475006103501,23.540468215942401,23.532218933105501,23.562456130981399]
["   Distillate Fuel Oil",null,null,12.893347740173301,14.727064132690399,16.906724929809599,17.4485054016113,16.910488128662099,15.8367977142334,14.87486743927,14.031831741333001,13.359474182128899,12.596385955810501,12.5241403579712,12.595507621765099,12.630928039550801,12.738121032714799,12.8303670883179,13.052293777465801,13.1472158432007,13.2630777359009,13.422198295593301,13.360619544982899,13.513841629028301,13.560380935668899,13.627392768859901]
["   Natural Gas",null,null,10.721179008483899,12.4281768798828,13.040691375732401,11.8341617584229,11.7410221099854,11.2507781982422,10.9759874343872,10.5919141769409,10.441241264343301,10.249824523925801,10.2927255630493,10.2421607971191,10.3305416107178,10.557685852050801,10.4870929718018,10.439262390136699,10.539955139160201,10.5361185073853,10.6743927001953,10.830116271972701,10.948052406311,10.9735927581787,11.0174913406372]
["   Electricity",null,null,27.0989685058594,27.587884902954102,27.636594772338899,27.492031097412099,27.368114471435501,27.154861450195298,26.912786483764599,26.5094184875488,26.281187057495099,26.172458648681602,26.036540985107401,25.993564605712901,26.085290908813501,26.304872512817401,26.445003509521499,26.355556488037099,26.368726730346701,26.419284820556602,26.420993804931602,26.4647102355957,26.5621242523193,26.608213424682599,26.564920425415]
[" Commercial"]
["   Distillate Fuel Oil",null,null,10.4802904129028,12.6793832778931,14.632154464721699,15.3235988616943,14.4384679794312,13.4501142501831,12.7189273834229,11.9810342788696,11.338329315185501,10.8460388183594,10.667523384094199,10.728004455566399,10.8701782226563,10.9251909255981,11.0219278335571,11.292310714721699,11.349814414978001,11.461010932922401,11.6882877349854,11.5126600265503,11.6838274002075,11.8503408432007,11.857501029968301]
["   Residual Fuel Oil",null,null,6.2490105628967303,8.4144115447997994,10.1003465652466,7.8816242218017596,7.7979149818420401,7.67907810211182,7.5374598503112802,7.0601482391357404,6.9191079139709499,5.9906802177429199,6.31249952316284,6.4941840171814,6.4476203918456996,6.5857205390930202,6.7015118598937997,6.98899221420288,7.0690569877624503,7.2425847053527797,7.4012169837951696,7.2363023757934597,7.3775544166564897,7.1704416275024396,7.2997760772705096]
["   Natural Gas",null,null,9.4024562835693395,11.2028198242188,11.3786783218384,10.2688541412354,10.157588958740201,9.6297473907470703,9.3356885910034197,8.9214458465576207,8.7509040832519496,8.5351839065551793,8.5524559020996094,8.47686672210693,8.5459880828857404,8.7391986846923793,8.6564092636108398,8.5963792800903303,8.6742591857910192,8.6351099014282209,8.7470979690551793,8.8685941696166992,8.9716949462890607,8.9597854614257795,8.9777603149414098]
["   Electricity",null,null,24.591539382934599,25.251781463623001,25.738388061523398,25.3376979827881,25.268539428710898,24.918291091918899,24.500482559204102,23.8594665527344,23.593626022338899,23.443479537963899,23.311824798583999,23.328050613403299,23.4844055175781,23.749778747558601,23.944339752197301,23.889307022094702,23.952335357666001,24.000473022460898,24.006351470947301,24.077814102172901,24.1955890655518,24.23095703125,24.1812038421631]
[" Industrial 1/"]
["   Liquefied Petroleum Gases",null,null,11.1755380630493,16.959981918335,18.9578742980957,17.513134002685501,17.389408111572301,16.750247955322301,16.423851013183601,15.943309783935501,15.769355773925801,15.620997428894,15.627494812011699,15.565483093261699,15.6823263168335,15.8655786514282,15.8662757873535,15.8647546768188,15.9073581695557,15.883088111877401,15.994482994079601,16.1067924499512,16.2546577453613,16.219263076782202,16.2301216125488]
["   Distillate Fuel Oil",null,null,10.9898891448975,13.0814533233643,15.1407413482666,15.435567855835,14.2919836044312,13.4232997894287,12.948052406311,12.4780015945435,11.882830619811999,11.641848564147899,11.349123954772899,11.401933670043899,11.6324548721313,11.632493019104,11.737724304199199,12.060711860656699,12.0405569076538,12.1396341323853,12.421196937561,12.169375419616699,12.3622283935547,12.619636535644499,12.5786838531494]
["   Residual Fuel Oil",null,null,5.7738895416259801,7.7708010673522896,9.3422021865844709,9.8767166137695295,10.084191322326699,9.7906637191772496,9.5023155212402308,8.7792091369628906,8.4676847457885707,8.0373468399047905,7.9767365455627397,8.2131023406982404,8.4110374450683594,8.5568304061889595,8.6100654602050799,8.8084278106689506,8.9135255813598597,9.0664196014404297,9.2084608078002894,9.1494617462158203,9.2910699844360405,9.2583961486816406,9.38494873046875]
["   Natural Gas 2/",null,null,6.4688553810119602,8.1627740859985405,7.4494204521179199,7.3632249832153303,7.2901554107665998,6.7422003746032697,6.4267692565918004,6.0213589668273899,5.8671450614929199,5.6813068389892596,5.6900143623352104,5.6504640579223597,5.7415480613708496,5.91982173919678,5.8755149841308603,5.8359832763671902,5.9000439643859899,5.8858833312988299,6.0041050910949698,6.1238050460815403,6.2412667274475098,6.2102909088134801,6.2538614273071298]
["   Metallurgical Coal",null,null,2.3078472614288299,3.0599997043609601,3.2548489570617698,3.2975256443023699,3.2872827053070099,3.1889374256134002,3.0940959453582799,2.9914577007293701,2.8927016258239702,2.78926348686218,2.7408642768859899,2.7166485786438002,2.7061200141906698,2.7063503265380899,2.7045123577117902,2.68979120254517,2.7072892189025901,2.71812868118286,2.7191135883331299,2.7064330577850302,2.68589544296265,2.69574999809265,2.7049932479858398]
["   Other Industrial Coal",null,null,1.80300605297089,2.1500017642974898,2.2005796432495099,2.2392640113830602,2.2450914382934601,2.2358458042144802,2.2614977359771702,2.2480733394622798,2.2308864593505899,2.2124359607696502,2.2059276103973402,2.1967613697052002,2.18912577629089,2.1856777667999299,2.1763286590576199,2.1755278110504199,2.18182468414307,2.19542455673218,2.2050869464874299,2.2089655399322501,2.2187693119049099,2.2309319972991899,2.2423520088195801]
["   Coal to Liquids",null,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A",0.88956671953201305,0.881245017051697,0.88442194461822499,0.89085346460342396,0.88840740919113204,0.89322775602340698,0.90440875291824296,0.91453087329864502,0.95469778776168801,0.96978461742401101,1.01334369182587,1.02781510353088,1.0294380187988299,1.1219843626022299,1.2297383546829199,1.26935982704163]
["   Electricity",null,null,15.8847751617432,16.691057205200199,18.258220672607401,18.768579483032202,18.8538303375244,18.518165588378899,18.014034271240199,17.2542610168457,16.790317535400401,16.590124130248999,16.466903686523398,16.461626052856399,16.6055717468262,16.851476669311499,17.021175384521499,17.000881195068398,17.070917129516602,17.1260585784912,17.140884399414102,17.206485748291001,17.3262729644775,17.353824615478501,17.310489654541001]
[" Transportation"]
["   Liquefied Petroleum Gases 3/",null,null,19.6766357421875,23.9161167144775,26.805564880371101,22.710954666137699,22.759067535400401,22.268846511840799,24.343835830688501,23.932544708251999,23.763250350952099,23.536403656005898,23.5618801116943,23.4868278503418,23.560710906982401,23.7542419433594,23.654756546020501,23.5774955749512,23.664421081543001,23.6253147125244,23.741106033325199,23.8700561523438,23.973831176757798,23.953416824340799,23.9759330749512]
["   E85 4/",null,null,20.914932250976602,23.101913452148398,24.811454772949201,27.774848937988299,25.9952602386475,24.2666110992432,21.291254043579102,20.525190353393601,20.3361301422119,20.197395324706999,20.009881973266602,20.093305587768601,20.196292877197301,20.4327602386475,20.4076957702637,20.624263763427699,20.610368728637699,20.617734909057599,21.067132949829102,20.970218658447301,20.962213516235401,21.257926940918001,21.098123550415]
["   Motor Gasoline 5/",null,null,15.721848487854,18.644901275634801,21.1534824371338,20.964454650878899,19.721015930175799,18.6920680999756,17.902309417724599,17.232242584228501,16.863773345947301,16.565891265869102,16.0857257843018,16.063297271728501,16.111997604370099,16.240406036376999,16.3247375488281,16.6728916168213,16.6320400238037,16.751285552978501,17.051519393920898,16.920253753662099,17.1026096343994,17.3232307434082,17.144313812255898]
["   Jet Fuel 6/",null,null,9.2184209823608398,13.1439361572266,14.9574270248413,12.9907026290894,11.722384452819799,11.2624855041504,10.9056959152222,10.3720808029175,10.059165954589799,10.0335283279419,9.8430700302124006,9.8874025344848597,10.0322532653809,10.087176322936999,10.2108345031738,10.523097038269,10.506872177124,10.5880041122437,10.8930578231812,10.788450241088899,10.9106340408325,11.0979099273682,11.0487413406372]
["   Distillate Fuel Oil 7/",null,null,13.583283424377401,17.522464752197301,19.7921543121338,19.706336975097699,18.211244583129901,17.3085613250732,16.8088684082031,16.001249313354499,15.3922462463379,15.213009834289601,14.822114944458001,14.859941482543899,15.1213598251343,15.075839042663601,15.158118247985801,15.4795846939087,15.4157457351685,15.4886207580566,15.773143768310501,15.4716739654541,15.639728546142599,15.912574768066399,15.834021568298301]
["   Residual Fuel Oil",null,null,4.8536195755004901,5.5067763328552202,7.1623473167419398,8.8221101760864293,9.0483112335205096,8.6029233932495099,8.0481967926025408,7.6902847290039098,7.3429737091064498,7.1018238067626998,6.97245073318481,7.0413579940795898,7.0324416160583496,7.12284135818481,7.14320993423462,7.1685328483581499,7.3589744567871103,7.4886426925659197,7.6476154327392596,7.6766633987426802,7.8515577316284197,7.8973522186279297,8.0370302200317401]
["   Natural Gas 8/",null,null,11.913727760314901,14.761161804199199,11.981869697570801,12.283256530761699,12.1389265060425,12.3170175552368,13.965456008911101,13.507596015930201,13.291357994079601,13.0437335968018,12.940827369689901,12.861621856689499,12.894752502441399,13.0291633605957,12.9489841461182,12.946153640747101,12.9756631851196,12.953050613403301,13.079764366149901,13.110743522644,13.198463439941399,13.2244005203247,13.175202369689901]
["   Electricity",null,null,26.1035976409912,25.216188430786101,26.121034622192401,25.629154205322301,25.7473449707031,25.392839431762699,24.861566543579102,24.317947387695298,24.125808715820298,23.980707168579102,23.787378311157202,23.809650421142599,23.876377105712901,24.074831008911101,24.262081146240199,24.183790206909201,24.2170009613037,24.245899200439499,24.2234077453613,24.307447433471701,24.4279899597168,24.465734481811499,24.386825561523398]
[" Electric Power 9/"]
["   Distillate Fuel Oil",null,null,9.5153579711914098,11.3847246170044,13.235827445983899,14.263434410095201,13.7692108154297,12.704180717468301,11.7051839828491,10.7794647216797,10.0299482345581,9.2896862030029297,9.1972703933715803,9.2599020004272496,9.2775526046752894,9.4403448104858398,9.5352287292480504,9.7515039443969709,9.8428487777709996,9.9595317840576207,10.1106100082397,10.0771369934082,10.217479705810501,10.254093170166,10.318883895874]
["   Residual Fuel Oil",null,null,4.9909768104553196,6.9611043930053702,7.8457942008972203,7.1943798065185502,7.2948379516601598,6.9926204681396502,6.5808119773864702,6.2065305709838903,5.9029440879821804,5.45705270767212,5.4534096717834499,5.5995068550109899,5.6287369728088397,5.7370648384094203,5.8140759468078604,6.0071105957031303,6.0822205543518102,6.22955322265625,6.4186983108520499,6.3188004493713397,6.5342454910278303,6.5804891586303702,6.6370191574096697]
["   Natural Gas",null,null,6.1140975952148402,8.1813249588012695,6.9707522392272896,7.1151452064514196,7.0668158531189,6.5265731811523402,6.2202811241149902,5.8298497200012198,5.6925516128540004,5.4995698928832999,5.54103326797485,5.5007095336914098,5.59739446640015,5.7880721092224103,5.7225790023803702,5.6709170341491699,5.7639327049255398,5.72597312927246,5.8378243446350098,5.9462161064147896,6.05735063552856,6.0477237701415998,6.0664491653442401]
["   Steam Coal",null,null,1.4011929035186801,1.5299999713897701,1.6714243888855,1.69177293777466,1.70398998260498,1.7000321149826001,1.7052028179168699,1.66678094863892,1.63700723648071,1.6199716329574601,1.61296951770782,1.59987056255341,1.59190189838409,1.5892090797424301,1.57604885101318,1.5779995918273899,1.5809644460678101,1.5890377759933501,1.59825491905212,1.6020262241363501,1.6148724555969201,1.62832856178284,1.63934326171875]
[" Average Price to All Users 10/"]
["   Liquefied Petroleum Gases",null,null,12.6906900405884,17.482444763183601,19.464084625244102,18.995626449585,18.880571365356399,18.286575317382798,18.020065307617202,17.571559906005898,17.417589187622099,17.2678737640381,17.291303634643601,17.241743087768601,17.364793777465799,17.562221527099599,17.562810897827099,17.558799743652301,17.620630264282202,17.599321365356399,17.721448898315401,17.8418064117432,17.9907836914063,17.9618225097656,17.988685607910199]
["   E85 4/",null,null,20.914932250976602,23.101913452148398,24.811454772949201,27.774848937988299,25.9952602386475,24.2666110992432,21.291254043579102,20.525190353393601,20.3361301422119,20.197395324706999,20.009881973266602,20.093305587768601,20.196292877197301,20.4327602386475,20.4076957702637,20.624263763427699,20.610368728637699,20.617734909057599,21.067132949829102,20.970218658447301,20.962213516235401,21.257926940918001,21.098123550415]
["   Motor Gasoline 5/",null,null,15.706001281738301,18.602125167846701,21.1080112457275,20.962741851806602,19.720066070556602,18.690637588501001,17.900485992431602,17.230388641357401,16.861814498901399,16.564214706420898,16.0839519500732,16.0615749359131,16.110080718994102,16.238643646240199,16.322971343994102,16.671089172363299,16.630247116088899,16.7495441436768,17.049686431884801,16.918500900268601,17.100944519043001,17.321361541748001,17.142530441284201]
["   Jet Fuel",null,null,9.2184209823608398,13.1439361572266,14.9574270248413,12.9907026290894,11.722384452819799,11.2624855041504,10.9056959152222,10.3720808029175,10.059165954589799,10.0335283279419,9.8430700302124006,9.8874025344848597,10.0322532653809,10.087176322936999,10.2108345031738,10.523097038269,10.506872177124,10.5880041122437,10.8930578231812,10.788450241088899,10.9106340408325,11.0979099273682,11.0487413406372]
["   Distillate Fuel Oil",null,null,12.9106340408325,16.217037200927699,18.421550750732401,18.437913894653299,17.199058532714801,16.296318054199201,15.704516410827599,14.921827316284199,14.360170364379901,14.182985305786101,13.862556457519499,13.915904045105,14.153459548950201,14.1445617675781,14.2399711608887,14.558382987976101,14.527869224548301,14.6189737319946,14.9021968841553,14.6463842391968,14.8252000808716,15.0819444656372,15.031323432922401]
["   Residual Fuel Oil",null,null,5.0985417366027797,6.5886197090148899,7.9185199737548801,8.2529850006103498,8.4050197601318395,8.0572872161865199,7.6087560653686497,7.1943945884704599,6.8676166534423801,6.4547815322876003,6.4073238372802699,6.54701900482178,6.5695567131042498,6.6816062927246103,6.7372307777404803,6.86507225036621,6.9956922531127903,7.1396765708923304,7.3088741302490199,7.2670574188232404,7.4510564804077104,7.4737396240234402,7.5808291435241699]
["   Natural Gas",null,null,7.8259296417236301,9.6487970352172905,9.1377601623535192,8.7611961364746094,8.6626396179199201,8.1270828247070295,7.8336372375488299,7.4448304176330602,7.2887372970581099,7.0927038192748997,7.1150150299072301,7.0641679763793901,7.1520218849182102,7.3469972610473597,7.2896466255187997,7.2448530197143599,7.3207983970642099,7.3070926666259801,7.4372458457946804,7.5700182914733896,7.6924967765808097,7.6794857978820801,7.7304539680481001]
["   Metallurgical Coal",null,null,2.3078472614288299,3.0599997043609601,3.2548489570617698,3.2975256443023699,3.2872827053070099,3.1889374256134002,3.0940959453582799,2.9914577007293701,2.8927016258239702,2.78926348686218,2.7408642768859899,2.7166485786438002,2.7061200141906698,2.7063503265380899,2.7045123577117902,2.68979120254517,2.7072892189025901,2.71812868118286,2.7191135883331299,2.7064330577850302,2.68589544296265,2.69574999809265,2.7049932479858398,2027,2028,2029,2030,2031,2032,2033,2034,2035,2036,2037,2038,2039,2040,2041,2042,2043,2044,2045,2046,2047,2048,2049,2050,2051,2052,2053,2054,2055,2056,2057,2058,2059,2060,2061,2062,2063,2064,2065,2066,2067,2068,2069,2070]
["   Other Coal",null,null,1.43066883087158,1.5706532001495399,1.7059867382049601,1.7268872261047401,1.7392324209213299,1.7345312833786,1.7401528358459499,1.7026997804641699,1.67319643497467,1.6556009054184,1.6479283571243299,1.63474309444427,1.6263667345046999,1.6231272220611599,1.60980331897736,1.6111264228820801,1.61373710632324,1.6214674711227399,1.6300570964813199,1.6331868171691899,1.6452817916870099,1.6581670045852701,1.6686607599258401]
["   Coal to Liquids",null,null,"N/A","N/A","N/A","N/A","N/A","N/A","N/A",0.88956671953201305,0.881245017051697,0.88442194461822499,0.89085346460342396,0.88840740919113204,0.89322775602340698,0.90440875291824296,0.91453087329864502,0.95469778776168801,0.96978461742401101,1.01334369182587,1.02781510353088,1.0294380187988299,1.1219843626022299,1.2297383546829199,1.26935982704163]
["   Electricity",null,null,23.009492874145501,23.734071731567401,24.3845615386963,24.318822860717798,24.297929763793899,24.022377014160199,23.662025451660199,23.093143463134801,22.802413940429702,22.663448333740199,22.5459308624268,22.5456428527832,22.688844680786101,22.9480895996094,23.136041641235401,23.0899753570557,23.154170989990199,23.213594436645501,23.230543136596701,23.3047065734863,23.429094314575199,23.4709377288818,23.433801651001001]
["Non-Renewable Energy Expenditures by Sector"]
["(billion 2005 dollars)"]
[" Residential",null,null,195.98880004882801,215.13366699218801,218.80557250976599,221.29866027832,223.50036621093801,221.10458374023401,220.438400268555,218.08479309082,218.45701599121099,217.84970092773401,219.40165710449199,221.00289916992199,224.59239196777301,228.53056335449199,230.97148132324199,232.57162475585901,236.03457641601599,237.58020019531301,240.43632507324199,243.39186096191401,247.24427795410199,248.98767089843801,251.02548217773401]
[" Commercial",null,null,141.77845764160199,154.38449096679699,157.84999084472699,156.06527709960901,159.312088012695,158.53677368164099,157.966796875,156.350173950195,157.31393432617199,158.58882141113301,160.74195861816401,163.37489318847699,167.20817565918,172.04411315918,175.58262634277301,178.093505859375,181.73991394043,185.01341247558599,188.79048156738301,192.86947631835901,197.36026000976599,201.10684204101599,204.49230957031301]
[" Industrial",null,null,184.22943115234401,196.07313537597699,205.39855957031301,217.87611389160199,214.14784240722699,207.11370849609401,200.48422241210901,191.81477355957,187.29217529296901,184.91578674316401,184.25204467773401,184.11447143554699,186.80691528320301,189.66255187988301,190.49990844726599,192.03105163574199,194.88296508789099,196.87213134765599,200.07191467285199,202.13279724121099,205.48814392089801,206.97822570800801,209.30905151367199]
[" Transportation",null,null,385.00112915039102,474.66281127929699,545.7236328125,538.79211425781295,508.11019897460898,488.44781494140602,476.37777709960898,463.41403198242199,458.16046142578102,458.57275390625,452.78533935546898,459.41848754882801,469.74392700195301,478.67190551757801,487.87078857421898,505.29348754882801,511.07485961914102,521.646240234375,538.77532958984398,540.642822265625,554.21173095703102,570.280029296875,574.30035400390602]
["   Total Non-Renewable Expenditures",null,null,906.997802734375,1040.25415039063,1127.77770996094,1134.0322265625,1105.07055664063,1075.20288085938,1055.26721191406,1029.66381835938,1021.22357177734,1019.92706298828,1017.18103027344,1027.91076660156,1048.35144042969,1068.9091796875,1084.9248046875,1107.98962402344,1123.73229980469,1141.11193847656,1168.07409667969,1179.03698730469,1204.30444335938,1227.35278320313,1239.12719726563]
[" Transportation Renewable Expenditures",null,null,2.27928571403027E-2,3.3822253346443197E-2,4.68330308794975E-2,4.2311083525419201E-2,4.6379543840885197E-2,5.0339180976152399E-2,6.3796535134315505E-2,7.1353547275066403E-2,7.5695373117923695E-2,8.06071981787682E-2,8.2480475306510898E-2,8.9031867682933793E-2,9.6231654286384596E-2,0.10344713926315301,0.112680315971375,0.13150542974471999,0.15408998727798501,0.18660007417201999,0.21707823872566201,0.243339464068413,0.28575915098190302,0.31987324357032798,0.34808513522148099]
["   Total Expenditures",null,null,907.02056884765602,1040.28796386719,1127.82458496094,1134.07458496094,1105.11694335938,1075.25317382813,1055.3310546875,1029.73522949219,1021.29925537109,1020.00769042969,1017.26348876953,1027.99975585938,1048.44763183594,1069.01257324219,1085.03747558594,1108.12109375,1123.88635253906,1141.29858398438,1168.29113769531,1179.2802734375,1204.59020996094,1227.67260742188,1239.47534179688]
["Woody Biomass","See High A Case"]
["Methanol","See High A Case"]
["Prices for Woody Biomass, Methanol and Steam are taken from the AEO High A case below",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Z641+($AI$471-$Y$641)/10","v":8.1072037368774854},{"$f":"AA471+($AI$471-$Y$641)/10","v":8.1552847846985532},8.203365832519621,8.2514468803406888,8.2995279281617567,8.3476089759828245,8.3956900238038923,8.4437710716249601,{"$f":"T641*$E$742","v":8.4918521194460261},{"$f":"AI471+($AX$471-$AI$471)/15","v":8.5879736457897184},{"$f":"AJ471+($AX$471-$AI$471)/15","v":8.6840951721334108},8.7802166984771031,8.8763382248207954,8.9724597511644877,9.06858127750818,9.1647028038518723,9.2608243301955646,9.3569458565392569,9.4530673828829492,9.5491889092266415,9.6453104355703339,9.7414319619140262,9.8375534882577185,{"$f":"AI471*$B$742","v":9.9336750146014001},{"$f":"AX471+($BM$471-$AX$471)/15","v":10.032035813725209},{"$f":"AY471+($BM$471-$AX$471)/15","v":10.130396612849017},10.228757411972826,10.327118211096634,10.425479010220442,10.523839809344251,10.622200608468059,10.720561407591868,10.818922206715676,10.917283005839485,11.015643804963293,11.114004604087102,11.21236540321091,11.310726202334719,{"$f":"AX471*$C$742","v":11.409087001458516},{"$f":"BM471+($BR$471-$BM$471)/5","v":11.522056966057418},{"$f":"BN471+($BR$471-$BM$471)/5","v":11.63502693065632},{"$f":"BO471+($BR$471-$BM$471)/5","v":11.747996895255222},{"$f":"BP471+($BR$471-$BM$471)/5","v":11.860966859854123},{"$f":"BM471*$D$742","v":11.973936824453022}]
["   1/ Includes energy for combined heat and power plants, except those whose primary business is to sell electricity, or electricity and heat, to the public.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Z642+($AI$472-$Y$642)/10","v":22.490795032640289},{"$f":"AA472+($AI$472-$Y$642)/10","v":22.394891584604984},22.29898813656968,22.203084688534375,22.10718124049907,22.011277792463765,21.915374344428461,21.819470896393156,{"$f":"T642*$E$745","v":21.723567448357841},{"$f":"AI472+($AX$472-$AI$472)/15","v":21.715027463671497},{"$f":"AJ472+($AX$472-$AI$472)/15","v":21.706487478985153},21.697947494298809,21.689407509612465,21.680867524926121,21.672327540239777,21.663787555553434,21.65524757086709,21.646707586180746,21.638167601494402,21.629627616808058,21.621087632121714,21.61254764743537,21.604007662749027,{"$f":"AI472*$B$745","v":21.595467678062693},{"$f":"AX472+($BM$472-$AX$472)/15","v":21.609186144316791},{"$f":"AY472+($BM$472-$AX$472)/15","v":21.622904610570888},21.636623076824986,21.650341543079083,21.664060009333181,21.677778475587278,21.691496941841375,21.705215408095473,21.71893387434957,21.732652340603668,21.746370806857765,21.760089273111863,21.77380773936596,21.787526205620058,{"$f":"AX472*$C$745","v":21.801244671874137},{"$f":"BM472+($BR$472-$BM$472)/5","v":21.815093857443394},{"$f":"BN472+($BR$472-$BM$472)/5","v":21.82894304301265},{"$f":"BO472+($BR$472-$BM$472)/5","v":21.842792228581906},{"$f":"BP472+($BR$472-$BM$472)/5","v":21.856641414151163},{"$f":"BM472*$D$745","v":21.870490599720426}]
["   2/ Excludes use for lease and plant fuel."]
["   3/ Includes Federal and State taxes while excluding county and local taxes."]
["   4/ E85 refers to a blend of 85 percent ethanol (renewable) and 15 percent motor gasoline (nonrenewable).  To address cold starting issues, the percentage of ethanol actually"]
["varies seasonally.  The annual average ethanol content of 74 percent is used for this forecast."]
["   5/ Sales weighted-average price for all grades.  Includes Federal, State, and local taxes."]
["   6/ Kerosene-type jet fuel.  Includes Federal and State taxes while excluding county and local taxes."]
["   7/ Diesel fuel for on-road use.  Includes Federal and State taxes while excluding county and local taxes."]
["   8/ Compressed natural gas used as a vehicle fuel.  Includes estimated motor vehicle fuel taxes and estimated dispensing costs or charges.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Z650+($AI$480-$Y$650)/10","v":5.5873463921161282},{"$f":"AA480+($AI$480-$Y$650)/10","v":5.6146233040707969},5.6419002160254657,5.6691771279801344,5.6964540399348031,5.7237309518894719,5.7510078638441406,5.7782847757988094,{"$f":"T650*$E$742","v":5.8055616877534817},{"$f":"AI480+($AX$480-$AI$480)/15","v":5.8712763802445851},{"$f":"AJ480+($AX$480-$AI$480)/15","v":5.9369910727356885},6.0027057652267919,6.0684204577178953,6.1341351502089987,6.1998498427001021,6.2655645351912055,6.3312792276823089,6.3969939201734123,6.4627086126645157,6.5284233051556191,6.5941379976467225,6.6598526901378259,6.7255673826289293,{"$f":"AI480*$B$742","v":6.791282075120038},{"$f":"AX480+($BM$480-$AX$480)/15","v":6.858527674659193},{"$f":"AY480+($BM$480-$AX$480)/15","v":6.925773274198348},6.993018873737503,7.060264473276658,7.1275100728158129,7.1947556723549679,7.2620012718941229,7.3292468714332779,7.3964924709724329,7.4637380705115879,7.5309836700507429,7.5982292695898979,7.6654748691290528,7.7327204686682078,{"$f":"AX480*$C$742","v":7.7999660682073682},{"$f":"BM480+($BR$480-$BM$480)/5","v":7.8771994077800587},{"$f":"BN480+($BR$480-$BM$480)/5","v":7.9544327473527492},{"$f":"BO480+($BR$480-$BM$480)/5","v":8.0316660869254388},{"$f":"BP480+($BR$480-$BM$480)/5","v":8.1088994264981284},{"$f":"BM480*$D$742","v":8.1861327660708199}]
["   9/ Includes electricity-only and combined heat and power plants whose primary business is to sell electricity, or electricity and heat, to the public."]
["   10/ Weighted averages of end-use fuel prices are derived from the prices shown in each sector and the corresponding sectoral consumption."]
["   Btu = British thermal unit.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Z653+($AI$483-$Y$653)/10","v":15.747041087587585},{"$f":"AA483+($AI$483-$Y$653)/10","v":15.673905881106727},15.600770674625869,15.527635468145011,15.454500261664153,15.381365055183295,15.308229848702437,15.235094642221579,{"$f":"T653*$E$745","v":15.161959435740725},{"$f":"AI483+($AX$483-$AI$483)/15","v":15.155998955184113},{"$f":"AJ483+($AX$483-$AI$483)/15","v":15.150038474627502},15.144077994070891,15.138117513514279,15.132157032957668,15.126196552401057,15.120236071844445,15.114275591287834,15.108315110731223,15.102354630174611,15.096394149618,15.090433669061388,15.084473188504777,15.078512707948166,{"$f":"AI483*$B$745","v":15.072552227391549},{"$f":"AX483+($BM$483-$AX$483)/15","v":15.082127028094042},{"$f":"AY483+($BM$483-$AX$483)/15","v":15.091701828796536},15.101276629499029,15.110851430201523,15.120426230904016,15.130001031606509,15.139575832309003,15.149150633011496,15.15872543371399,15.168300234416483,15.177875035118976,15.18744983582147,15.197024636523963,15.206599437226457,{"$f":"AX483*$C$745","v":15.216174237928941},{"$f":"BM483+($BR$483-$BM$483)/5","v":15.225840274150585},{"$f":"BN483+($BR$483-$BM$483)/5","v":15.235506310372228},{"$f":"BO483+($BR$483-$BM$483)/5","v":15.245172346593872},{"$f":"BP483+($BR$483-$BM$483)/5","v":15.254838382815516},{"$f":"BM483*$D$745","v":15.264504419037157}]
["   N/A = Not applicable."]
["   Note:  Data for 2004 and 2005 are model results and may differ slightly from official EIA data reports."]
["   Sources:  2004 and 2005 prices for motor gasoline, distillate fuel oil, and jet fuel are based on prices in the Energy Information Administration (EIA), Petroleum Marketing Annual 2005,"]
["DOE/EIA-0487(2005) (Washington, DC, August 2006).  2004 residential and commercial natural gas delivered prices:  EIA, Natural Gas Annual 2004, DOE/EIA-0131(2004)"]
["(Washington, DC, December 2005).  2005 residential and commercial natural gas delivered prices:  EIA, Natural Gas Monthly, DOE/EIA-0130(2006/04) (Washington, DC, April 2006).",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Z658+($AI$488-$Y$658)/10","v":13.224797394153365},{"$f":"AA488+($AI$488-$Y$658)/10","v":13.589441040570847},13.954084686988329,14.318728333405812,14.683371979823294,15.048015626240776,15.412659272658258,15.777302919075741,{"$f":"T658*$E$744","v":16.141946565493228},{"$f":"AI488+($AX$488-$AI$488)/15","v":16.312798018423909},{"$f":"AJ488+($AX$488-$AI$488)/15","v":16.483649471354589},16.654500924285269,16.82535237721595,16.99620383014663,17.16705528307731,17.337906736007991,17.508758188938671,17.679609641869352,17.850461094800032,18.021312547730712,18.192164000661393,18.363015453592073,18.533866906522753,{"$f":"AI488*$B$744","v":18.704718359453445},{"$f":"AX488+($BM$488-$AX$488)/15","v":18.811222625087144},{"$f":"AY488+($BM$488-$AX$488)/15","v":18.917726890720843},19.024231156354542,19.130735421988241,19.23723968762194,19.34374395325564,19.450248218889339,19.556752484523038,19.663256750156737,19.769761015790436,19.876265281424136,19.982769547057835,20.089273812691534,20.195778078325233,{"$f":"AX488*$C$744","v":20.302282343958908},{"$f":"BM488+($BR$488-$BM$488)/5","v":20.417883104696291},{"$f":"BN488+($BR$488-$BM$488)/5","v":20.533483865433674},{"$f":"BO488+($BR$488-$BM$488)/5","v":20.649084626171057},{"$f":"BP488+($BR$488-$BM$488)/5","v":20.76468538690844},{"$f":"BM488*$D$744","v":20.880286147645826}]
["2004 and 2005 industrial natural gas delivered prices are estimated based on:  EIA, Manufacturing Energy Consumption Survey 1994 and industrial and wellhead prices from the"]
["Natural Gas Annual 2004, DOE/EIA-0131(2004) (Washington, DC, December 2005) and the Natural Gas Monthly, DOE/EIA-0130(2006/04) (Washington, DC, April 2006).  2004",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Z660+($AI$490-$Y$660)/10","v":15.4577980437679},{"$f":"AA490+($AI$490-$Y$660)/10","v":15.88385635596555},16.309914668163202,16.735972980360852,17.162031292558503,17.588089604756153,18.014147916953803,18.440206229151453,{"$f":"T660*$E$744","v":18.866264541349103},{"$f":"AI490+($AX$490-$AI$490)/15","v":19.065951034869943},{"$f":"AJ490+($AX$490-$AI$490)/15","v":19.265637528390783},19.465324021911623,19.665010515432463,19.864697008953303,20.064383502474143,20.264069995994983,20.463756489515823,20.663442983036663,20.863129476557503,21.062815970078343,21.262502463599183,21.462188957120024,21.661875450640864,{"$f":"AI490*$B$744","v":21.861561944161682},{"$f":"AX490+($BM$490-$AX$490)/15","v":21.986041209538687},{"$f":"AY490+($BM$490-$AX$490)/15","v":22.110520474915692},22.234999740292697,22.359479005669701,22.483958271046706,22.608437536423711,22.732916801800716,22.857396067177721,22.981875332554726,23.10635459793173,23.230833863308735,23.35531312868574,23.479792394062745,23.60427165943975,{"$f":"AX490*$C$744","v":23.728750924816747},{"$f":"BM490+($BR$490-$BM$490)/5","v":23.863861924249427},{"$f":"BN490+($BR$490-$BM$490)/5","v":23.998972923682107},{"$f":"BO490+($BR$490-$BM$490)/5","v":24.134083923114787},{"$f":"BP490+($BR$490-$BM$490)/5","v":24.269194922547467},{"$f":"BM490*$D$744","v":24.404305921980139}]
["transportation sector natural gas delivered prices are based on:  EIA, Natural Gas Annual 2004, DOE/EIA-0131(2004) (Washington, DC, December 2005) and estimated state taxes,"]
["federal taxes, and dispensing costs or charges.  2005 transportation sector natural gas delivered prices are model results.  2004 and 2005 electric power sector natural gas prices:"]
["EIA, Electric Power Monthly, May 2005 through April 2006, Table 4.11.A.  2004 and 2005 coal prices based on:  EIA, Quarterly Coal Report, October-December 2005, DOE/EIA-0121"]
["(2005/4Q) (Washington, DC, March 2006) and EIA, AEO2007 National Energy Modeling System run aeo2007.d112106a.  2004 and 2005 electricity prices:  EIA, Annual Energy Review",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Z664+($AI$494-$Y$664)/10","v":19.493346965415647},{"$f":"AA494+($AI$494-$Y$664)/10","v":19.39274662152437},19.292146277633094,19.191545933741818,19.090945589850541,18.990345245959265,18.889744902067989,18.789144558176712,{"$f":"T664*$E$747","v":18.68854421428545},{"$f":"AI494+($AX$494-$AI$494)/15","v":18.700972398006513},{"$f":"AJ494+($AX$494-$AI$494)/15","v":18.713400581727576},18.72582876544864,18.738256949169703,18.750685132890766,18.763113316611829,18.775541500332892,18.787969684053955,18.800397867775018,18.812826051496081,18.825254235217145,18.837682418938208,18.850110602659271,18.862538786380334,{"$f":"AI494*$B$747","v":18.874966970101411},{"$f":"AX494+($BM$494-$AX$494)/15","v":18.881381252955478},{"$f":"AY494+($BM$494-$AX$494)/15","v":18.887795535809545},18.894209818663612,18.900624101517678,18.907038384371745,18.913452667225812,18.919866950079879,18.926281232933945,18.932695515788012,18.939109798642079,18.945524081496146,18.951938364350212,18.958352647204279,18.964766930058346,{"$f":"AX494*$C$747","v":18.971181212912409},{"$f":"BM494+($BR$494-$BM$494)/5","v":18.97762819226703},{"$f":"BN494+($BR$494-$BM$494)/5","v":18.984075171621651},{"$f":"BO494+($BR$494-$BM$494)/5","v":18.990522150976272},{"$f":"BP494+($BR$494-$BM$494)/5","v":18.996969130330893},{"$f":"BM494*$D$747","v":19.003416109685507}]
["2005, DOE/EIA-0384(2005) (Washington, DC, July 2006).  2004 and 2005 ethanol prices derived from weekly spot prices in the Oxy Fuel News.  Projections:  EIA, AEO2007 National"]
["Energy Modeling System run aeo2007.d112106a."]
[]
[]
[]
["Raw EIA Price Data"]
["AEO 2005 Reference Case"]
[" Report #: DOE/EIA-0383(2005)"]
["Release date full report: January 2005"]
["Energy Prices"]
["Name of file: aeotab_3.xls"]
["http://www.eia.doe.gov/oiaf/aeo/index.html",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Z676+($AI$506-$Y$676)/10","v":5.5529965108452508},{"$f":"AA506+($AI$506-$Y$676)/10","v":5.5809474506703411},5.6088983904954315,5.6368493303205218,5.6648002701456122,5.6927512099707025,5.7207021497957928,5.7486530896208832,{"$f":"T676*$E$742","v":5.77660402944597},{"$f":"AI506+($AX$506-$AI$506)/15","v":5.8419909425225587},{"$f":"AJ506+($AX$506-$AI$506)/15","v":5.9073778555991474},5.9727647686757361,6.0381516817523249,6.1035385948289136,6.1689255079055023,6.234312420982091,6.2996993340586798,6.3650862471352685,6.4304731602118572,6.4958600732884459,6.5612469863650347,6.6266338994416234,6.6920208125182121,{"$f":"AI506*$B$742","v":6.7574077255948062},{"$f":"AX506+($BM$506-$AX$506)/15","v":6.8243179096825601},{"$f":"AY506+($BM$506-$AX$506)/15","v":6.8912280937703141},6.958138277858068,7.025048461945822,7.091958646033576,7.1588688301213299,7.2257790142090839,7.2926891982968378,7.3595993823845918,7.4265095664723457,7.4934197505600997,7.5603299346478536,7.6272401187356076,7.6941503028233615,{"$f":"AX506*$C$742","v":7.7610604869111093},{"$f":"BM506+($BR$506-$BM$506)/5","v":7.8379085930167243},{"$f":"BN506+($BR$506-$BM$506)/5","v":7.9147566991223393},{"$f":"BO506+($BR$506-$BM$506)/5","v":7.9916048052279542},{"$f":"BP506+($BR$506-$BM$506)/5","v":8.0684529113335692},{"$f":"BM506*$D$742","v":8.1453010174391842}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Z677+($AI$507-$Y$677)/10","v":1.3364941226202385},{"$f":"AA507+($AI$507-$Y$677)/10","v":1.3402060190972878},1.343917915574337,1.3476298120513863,1.3513417085284356,1.3550536050054849,1.3587655014825342,1.3624773979595834,{"$f":"T677*$E$740","v":1.3661892944366323},{"$f":"AI507+($AX$507-$AI$507)/15","v":1.3701947313799723},{"$f":"AJ507+($AX$507-$AI$507)/15","v":1.3742001683233123},1.3782056052666523,1.3822110422099922,1.3862164791533322,1.3902219160966722,1.3942273530400122,1.3982327899833522,1.4022382269266922,1.4062436638700322,1.4102491008133722,1.4142545377567122,1.4182599747000522,1.4222654116433922,{"$f":"AI507*$B$740","v":1.4262708485867317},{"$f":"AX507+($BM$507-$AX$507)/15","v":1.428975877834666},{"$f":"AY507+($BM$507-$AX$507)/15","v":1.4316809070826002},1.4343859363305345,1.4370909655784687,1.439795994826403,1.4425010240743372,1.4452060533222715,1.4479110825702057,1.45061611181814,1.4533211410660742,1.4560261703140085,1.4587311995619427,1.461436228809877,1.4641412580578113,{"$f":"AX507*$C$740","v":1.4668462873057471},{"$f":"BM507+($BR$507-$BM$507)/5","v":1.4696282709053681},{"$f":"BN507+($BR$507-$BM$507)/5","v":1.4724102545049891},{"$f":"BO507+($BR$507-$BM$507)/5","v":1.4751922381046101},{"$f":"BP507+($BR$507-$BM$507)/5","v":1.4779742217042311},{"$f":"BM507*$D$740","v":1.4807562053038525}]
[" Table   3.  Energy Prices by Sector and Source"]
["                      (2003 Dollars per Million Btu, Unless Otherwise Noted)"]
[]
["","2002","2003","2004","2005","2006","2007","2008","2009","2010","2011","2012","2013","2014","2015","2016","2017","2018","2019","2020","2021","2022","2023","2024","2025",2026]
["","","","","","","","","","","","","","","","","","","","","","","","",""]
["","","","","","","","","","","","","","","","","","","","","","","","",""]
[" Residential",15.0220499038696,15.811363220214799,16.4251308441162,16.464759826660199,15.680528640747101,15.0112085342407,14.5817928314209,14.458288192749,14.326377868652299,14.293612480163601,14.4205980300903,14.6031141281128,14.8352861404419,14.979790687561,15.0010738372803,15.073490142822299,15.2468109130859,15.482013702392599,15.6422672271729,15.809124946594199,15.869408607482899,15.910493850708001,16.000511169433601,16.127393722534201]
["   Primary Energy 1/",8.3285751342773402,9.67810153961182,10.6516561508179,10.5737972259521,9.7301187515258807,9.2126417160034197,8.7946681976318395,8.5506849288940394,8.3542766571044904,8.2684001922607404,8.3419942855834996,8.4596767425537092,8.6078786849975604,8.7398357391357404,8.7483062744140607,8.7686567306518608,8.8867673873901403,9.0631914138793892,9.2055320739746094,9.3421277999877894,9.4150266647338903,9.4582109451293892,9.5390539169311506,9.6245632171630895]
["     Petroleum Products 2/",10.0436496734619,11.266843795776399,13.0600261688232,12.5262813568115,11.260459899902299,10.814398765564,10.6458578109741,10.453662872314499,10.443992614746101,10.420529365539601,10.4911556243896,10.5971431732178,10.650529861450201,10.7566242218018,10.8697347640991,10.955939292907701,11.0780487060547,11.222780227661101,11.364427566528301,11.5109758377075,11.6184797286987,11.7467203140259,11.8437652587891,11.9311771392822]
["       Distillate Fuel",8.3698368072509801,9.5702075958252006,10.537187576293899,10.120927810668899,9.0704116821289098,8.6811342239379901,8.4951152801513707,8.3145399093627894,8.2864685058593803,8.2537784576415998,8.2966070175170898,8.3739995956420898,8.4385089874267596,8.4884243011474592,8.5346355438232404,8.5863618850708008,8.7058753967285192,8.7835302352905291,8.8462095260620099,8.9105930328369105,8.9716310501098597,9.0270709991455096,9.0740833282470703,9.1169166564941406]
["       Liquefied Petroleum Gas",12.976583480835,14.582922935485801,17.5701904296875,17.073207855224599,15.3619232177734,14.740796089172401,14.555371284484901,14.281338691711399,14.253823280334499,14.190848350524901,14.252662658691399,14.348473548889199,14.316626548767101,14.447472572326699,14.6025552749634,14.6705665588379,14.712552070617701,14.8757133483887,15.056845664978001,15.2477731704712,15.3445425033569,15.4947566986084,15.580441474914601,15.645468711853001]
["     Natural Gas",7.8179483413696298,9.2187824249267596,9.9373922348022496,10.0359506607056,9.3121318817138707,8.7750911712646502,8.2899227142334002,8.0357856750488299,7.7935147285461399,7.6957306861877397,7.7737927436828604,7.89709520339966,8.0722961425781303,8.21258449554443,8.1957035064697301,8.2030982971191406,8.3247480392456108,8.5131444931030291,8.6595201492309606,8.7975921630859393,8.8660669326782209,8.8930187225341797,8.9751634597778303,9.0651559829711896]
["   Electricity",25.222642898559599,25.415189743041999,25.1893119812012,25.147850036621101,24.3894958496094,23.460399627685501,22.990982055664102,23.018142700195298,22.960025787353501,22.974227905273398,23.1215305328369,23.312740325927699,23.5714206695557,23.632020950317401,23.589054107666001,23.650138854980501,23.8146667480469,24.0346794128418,24.122148513793899,24.230636596679702,24.181154251098601,24.130558013916001,24.148235321044901,24.238166809081999]
["","","","","","","","","","","","","","","","","","","","","","","","",""]
[" Commercial",15.064169883728001,15.629265785217299,15.835299491882299,15.918291091918899,15.0829524993896,14.3196773529053,13.910519599914601,13.8424997329712,13.762632369995099,13.8186712265015,14.058515548706101,14.316973686218301,14.661353111267101,14.869439125061,14.9301090240479,15.044508934021,15.2485342025757,15.517853736877401,15.7009220123291,15.889198303222701,15.933961868286101,15.975202560424799,16.0630493164063,16.195989608764599]
["   Primary Energy 1/",6.5697088241577104,7.9157042503356898,8.3734645843505895,8.3683490753173793,7.7444124221801802,7.3380589485168501,7.0368156433105504,6.9020848274231001,6.8100509643554696,6.84179735183716,6.8974781036376998,6.9808845520019496,7.1057710647582999,7.20139837265015,7.18692874908447,7.1932849884033203,7.2944316864013699,7.4377117156982404,7.5399260520935103,7.6392593383789098,7.6873850822448704,7.6958703994751003,7.7559337615966797,7.8220491409301802]
["     Petroleum Products 2/",6.9482707977294904,8.0266513824462908,8.9197750091552699,8.6532449722290004,7.9109911918640101,7.48618364334106,7.32971286773682,7.1282916069030797,7.1344366073608398,7.2035880088806197,7.21549415588379,7.2433881759643599,7.2548027038574201,7.2826437950134304,7.3254833221435502,7.3667011260986301,7.4382300376892099,7.5099358558654803,7.5474686622619602,7.6315479278564498,7.69354152679443,7.7161302566528303,7.7569241523742702,7.8363184928893999]
["       Distillate Fuel",6.1493649482727104,7.03082323074341,7.7272844314575204,7.4210705757141104,6.8826036453247097,6.5409913063049299,6.4167842864990199,6.2535924911498997,6.2965154647827104,6.4007697105407697,6.4218788146972701,6.4483299255371103,6.4679012298584002,6.4912290573120099,6.52826023101807,6.5738272666931197,6.6604804992675799,6.7330570220947301,6.75683689117432,6.8434348106384304,6.9099073410034197,6.9186587333679199,6.9633812904357901,7.0585165023803702]
["       Residual Fuel",4.2683343887329102,4.9646224975585902,5.0606441497802699,5.3499689102172896,5.0606269836425799,4.6454811096191397,4.44089698791504,4.3064308166503897,4.2577414512634304,4.3118896484375,4.3638815879821804,4.4166550636291504,4.4711151123046902,4.5238728523254403,4.5756058692932102,4.6275658607482901,4.6890521049499503,4.7516570091247603,4.8052668571472203,4.8599562644958496,4.9139251708984402,4.9674754142761204,5.0218071937561,5.0773591995239302]
["     Natural Gas",6.6170339584350604,8.0769119262695295,8.4474086761474592,8.5042705535888707,7.8856530189514196,7.4673976898193404,7.1177520751953098,6.9923906326293901,6.8716683387756303,6.8934268951415998,6.9598770141601598,7.0576272010803196,7.21203565597534,7.32529544830322,7.2944836616516104,7.2903637886047399,7.3995337486267099,7.56237888336182,7.6814393997192401,7.78521823883057,7.8287162780761701,7.8313083648681596,7.8953433036804199,7.9576945304870597,{"$f":"Y527+($AI$357-$Y$527)/10","v":8.0099991534203383}]
["   Electricity",23.353584289550799,23.2374382019043,23.0415229797363,22.938554763793899,21.8424968719482,20.6924953460693,20.1292018890381,20.063879013061499,19.9343872070313,19.938108444213899,20.262083053588899,20.589830398559599,21.038742065429702,21.2544975280762,21.300868988037099,21.4323215484619,21.647081375122099,21.937980651855501,22.104045867919901,22.281753540039102,22.24875831604,22.2471523284912,22.287950515747099,22.4030246734619,{"$f":"Y528+($AI$358-$Y$528)/10","v":22.313820934181763}]
["","","","","","","","","","","","","","","","","","","","","","","","",""]
[" Industrial 3/",6.3922061920165998,7.7839651107788104,8.7301359176635707,8.5276689529418892,7.7321057319641104,7.2916359901428196,7.0938224792480504,6.9649901390075701,6.8520793914794904,6.8315567970275897,6.8953166007995597,6.99013376235962,7.1103782653808603,7.2379879951477104,7.276611328125,7.3343372344970703,7.4634890556335396,7.6215224266052202,7.7529444694518999,7.8803434371948198,7.9471721649169904,7.99715328216553,8.05676174163818,8.1260271072387695]
["   Primary Energy",4.9298634529113796,6.4939708709716797,7.4592456817626998,7.2321572303771999,6.3973078727722203,5.9808039665222203,5.7940292358398402,5.64864206314087,5.54791307449341,5.5448842048645002,5.5862631797790501,5.6484580039978001,5.7157526016235396,5.8273496627807599,5.8644676208496103,5.9049983024597203,6.0105843544006303,6.1420850753784197,6.2661328315734899,6.3902029991149902,6.4639844894409197,6.5222811698913601,6.5781168937683097,6.6401424407959002,null,{"$f":"Z701+($AI$531-$Y$701)/10","v":1.6707610713595051},{"$f":"AA531+($AI$531-$Y$701)/10","v":1.7872284374395671},1.903695803519629,2.0201631695996909,2.1366305356797528,2.2530979017598147,2.3695652678398766,2.4860326339199386,2.6025,{"$f":"AI531+($BM$531-$AI$531)/30","v":2.6824166666666667},{"$f":"AJ531+($BM$531-$AI$531)/30","v":2.7623333333333333},2.8422499999999999,2.9221666666666666,3.0020833333333332,3.0819999999999999,3.1619166666666665,3.2418333333333331,3.3217499999999998,3.4016666666666664,3.481583333333333,3.5614999999999997,3.6414166666666663,3.7213333333333329,3.8012499999999996,3.8811666666666662,3.9610833333333328,4.0409999999999995,4.1209166666666661,4.2008333333333328,4.2807499999999994,4.360666666666666,4.4405833333333327,4.5204999999999993,4.6004166666666659,4.6803333333333326,4.7602499999999992,4.8401666666666658,4.9200833333333325,5,5.0799166666666666,5.1598333333333333,5.2397499999999999,5.3196666666666665,5.3995833333333332]
["     Petroleum Products 2/",6.5291514396667498,8.2850980758666992,9.8001232147216797,9.3072748184204102,8.1255960464477504,7.6394152641296396,7.5353851318359402,7.29905128479004,7.2437157630920401,7.2615475654602104,7.28952884674072,7.3323044776916504,7.3129158020019496,7.4180650711059597,7.5101509094238299,7.5518846511840803,7.6326026916503897,7.7444272041320801,7.8752341270446804,8.0334920883178693,8.1469945907592791,8.2539978027343803,8.3047761917114293,8.3638219833374006,null,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.2799999999999994,8.2799999999999994,{"$f":"AI532+($AX$532-$AI$532)/15","v":8.2855063337213686},{"$f":"AJ532+($AX$532-$AI$532)/15","v":8.2910126674427378},8.296519001164107,8.3020253348854762,8.3075316686068454,8.3130380023282147,8.3185443360495839,8.3240506697709531,8.3295570034923223,8.3350633372136915,8.3405696709350607,8.34607600465643,8.3515823383777992,8.3570886720991684,{"$f":"AI532*$B$747","v":8.3625950058205305},{"$f":"AX532+($BM$532-$AX$532)/15","v":8.3654368677345836},{"$f":"AY532+($BM$532-$AX$532)/15","v":8.3682787296486367},8.3711205915626898,8.373962453476743,8.3768043153907961,8.3796461773048492,8.3824880392189023,8.3853299011329554,8.3881717630470085,8.3910136249610616,8.3938554868751147,8.3966973487891678,8.399539210703221,8.4023810726172741,{"$f":"AX532*$C$747","v":8.4052229345313236},{"$f":"BM532+($BR$532-$BM$532)/5","v":8.4080792827007791},{"$f":"BN532+($BR$532-$BM$532)/5","v":8.4109356308702345},{"$f":"BO532+($BR$532-$BM$532)/5","v":8.41379197903969},{"$f":"BP532+($BR$532-$BM$532)/5","v":8.4166483272091455},{"$f":"BM532*$D$747","v":8.4195046753785974}]
["       Distillate Fuel",6.3323707580566397,7.2384452819824201,7.96527099609375,7.6527137756347701,7.15256595611572,6.8207654953002903,6.8779778480529803,6.7174663543701199,6.78255271911621,7.1339807510376003,7.1601362228393599,7.1876134872436497,7.1760501861572301,7.19400835037231,7.2192950248718297,7.2771706581115696,7.32332468032837,7.37906789779663,7.3721222877502397,7.4461221694946298,7.5145907402038601,7.4954967498779297,7.5633401870727504,7.7325506210327104,null,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78]
["       Liquefied Petroleum Gas",8.4833917617797905,12.566796302795399,15.1470994949341,13.2375335693359,11.1595468521118,10.509430885314901,10.3245944976807,10.044970512390099,10.0157480239868,9.9449577331543004,10.002993583679199,10.097089767456101,10.020875930786101,10.2241611480713,10.3367824554443,10.319104194641101,10.409514427185099,10.552604675293001,10.737306594848601,10.9299325942993,11.0452260971069,11.198148727416999,11.303442955017101,11.352322578430201,null,{"$f":"AA533*GJ_p_MMBtu","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$f":"AH533*GJ_p_MMBtu","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$f":"BN533*GJ_p_MMBtu","v":{"$error":"#NAME?"}},{"$f":"BO533*GJ_p_MMBtu","v":{"$error":"#NAME?"}},{"$f":"BP533*GJ_p_MMBtu","v":{"$error":"#NAME?"}},{"$f":"BQ533*GJ_p_MMBtu","v":{"$error":"#NAME?"}},{"$f":"BR533*GJ_p_MMBtu","v":{"$error":"#NAME?"}}]
["       Residual Fuel",3.9384419918060298,4.5867881774902299,4.6800308227539098,4.9388971328735396,4.6724338531494096,4.2573971748352104,4.0660681724548304,3.9201312065124498,3.8699574470520002,3.9242179393768302,3.9701111316680899,4.0123748779296902,4.03127193450928,4.0987625122070304,4.1393604278564498,4.1877317428588903,4.2278647422790501,4.2813539505004901,4.3376803398132298,4.4096555709838903,4.4638853073120099,4.5156707763671902,4.5648870468139604,4.6165790557861301]
["     Natural Gas 4/",3.88655662536621,5.55936574935913,6.0491561889648402,6.0767245292663601,5.4288315773010298,4.9784579277038601,4.6095819473266602,4.5152282714843803,4.3734540939331099,4.3719940185546902,4.4435229301452601,4.5411396026611301,4.7005810737609899,4.81768798828125,4.7900476455688503,4.8231658935546902,4.9558763504028303,5.1147346496581996,5.2329874038696298,5.3250308036804199,5.3559622764587402,5.3499736785888699,5.4079699516296396,5.4724006652831996,{"$f":"Y536+($AI$366-$Y$536)/10","v":5.502911815190215}]
["     Metallurgical Coal",1.88388228416443,1.8499996662139899,1.9631321430206301,1.9065624475479099,1.8876701593398999,1.8568421602249101,1.8503668308258101,1.8461718559265099,1.81827020645142,1.79229772090912,1.7775920629501301,1.7720992565155,1.7673192024230999,1.76388168334961,1.7582092285156301,1.7531107664108301,1.7537478208541899,1.7550060749053999,1.75110328197479,1.741095662117,1.72283828258514,1.7066173553466799,1.6973831653595,1.68216860294342]
["     Steam Coal",1.5976041555404701,1.5543407201767001,1.5665656328201301,1.6037170886993399,1.59409379959106,1.5766631364822401,1.5775339603424099,1.5708864927291899,1.5649564266204801,1.56413578987122,1.5547889471054099,1.54732978343964,1.54787278175354,1.5495419502258301,1.5494637489318801,1.5568271875381501,1.55967605113983,1.5613601207733201,1.5625598430633501,1.5681461095809901,1.5708984136581401,1.6035954952239999,1.60524129867554,1.6024739742279099]
["   Electricity",14.734835624694799,15.0261535644531,15.7151737213135,15.5977983474731,15.0554456710815,14.415571212768601,14.123340606689499,14.033378601074199,13.8423414230347,13.6992740631104,13.8484916687012,14.089280128479,14.438159942626999,14.622407913208001,14.680962562561,14.817166328430201,15.035754203796399,15.3131446838379,15.467190742492701,15.608844757080099,15.623446464538601,15.6070909500122,15.6627254486084,15.7515544891357,{"$f":"Y539+($AI$369-$Y$539)/10","v":15.681619149325263}]
["","","","","","","","","","","","","","","","","","","","","","","","",""]
[" Transportation",10.068477630615201,11.4567165374756,12.984972000122101,12.646059036254901,12.0215864181519,11.451254844665501,11.2903280258179,11.054517745971699,10.953487396240201,10.9616088867188,10.9120273590088,10.9370317459106,10.932166099548301,10.949841499328601,10.9948740005493,11.046938896179199,11.074780464172401,11.117128372192401,11.155697822570801,11.209436416626,11.2737817764282,11.3331050872803,11.350456237793001,11.462995529174799]
["   Primary Energy",10.0396184921265,11.4297380447388,12.961000442504901,12.6219329833984,11.9984340667725,11.4290685653687,11.2685947418213,11.0320892333984,10.930870056152299,10.938961982727101,10.8886499404907,10.913072586059601,10.9073333740234,10.9247722625732,10.969937324523899,11.021965980529799,11.049379348754901,11.0911350250244,11.129392623901399,11.182910919189499,11.247509956359901,11.307147026061999,11.324338912963899,11.436959266662599]
["     Petroleum Products 2/",10.0409812927246,11.431476593017599,12.9638833999634,12.6248769760132,12.0015964508057,11.432228088378899,11.2722625732422,11.0358724594116,10.934929847717299,10.9432172775269,10.892875671386699,10.9173030853271,10.911340713501,10.928663253784199,10.9740562438965,11.026309967041,11.0536193847656,11.0952548980713,11.1333513259888,11.1867895126343,11.251508712768601,11.3113117218018,11.328408241271999,11.4412240982056]
["       Distillate Fuel 5/",9.5535230636596697,10.9202365875244,12.0208587646484,11.5461339950562,11.286841392517101,11.003821372985801,10.8476676940918,10.675346374511699,10.7599039077759,10.8244476318359,10.807107925415,10.788902282714799,10.7359352111816,10.7108716964722,10.6978845596313,10.720422744751,10.715018272399901,10.7237329483032,10.658562660217299,10.6896152496338,10.7133436203003,10.6396188735962,10.6814889907837,10.8466644287109,{"$f":"Y544+($AI$374-$Y$544)/10","v":11.215393895691953}]
["       Jet Fuel 6/",6.0538434982299796,6.4578518867492702,8.1168746948242205,7.6875572204589799,7.0150871276855504,6.5790328979492196,6.5712537765502903,6.42602443695068,6.2476048469543501,6.2184038162231401,6.2436552047729501,6.2858424186706499,6.2737250328064,6.2926135063171396,6.3336305618286097,6.3623290061950701,6.4419050216674796,6.5377755165100098,6.5789065361022896,6.7034192085266104,6.8036813735961896,6.8691210746765101,6.8930430412292498,6.9258189201354998]
["       Motor Gasoline 7/",11.3207235336304,12.9284992218018,14.6530704498291,14.346965789794901,13.634911537170399,12.9354457855225,12.7248182296753,12.444727897644,12.3216390609741,12.333900451660201,12.228641510009799,12.2244319915771,12.232741355896,12.2594261169434,12.3207359313965,12.3872022628784,12.4125566482544,12.451280593872101,12.520702362060501,12.5581102371216,12.622034072876,12.7203483581543,12.7153625488281,12.8139133453369,{"$f":"Y546+($AI$376-$Y$546)/10","v":13.239838295522954}]
["       Residual Fuel",3.83150410652161,4.4939312934875497,4.5839381217956499,4.8374905586242702,4.5451078414917001,4.1204147338867196,3.9213058948516801,3.7859048843383798,3.7380118370056201,3.79148626327515,3.8454215526580802,3.8996179103851301,3.9557838439941402,4.0096635818481401,4.0587000846862802,4.1115031242370597,4.1679596900939897,4.2270021438598597,4.2823433876037598,4.3368558883667001,4.3924484252929696,4.4465680122375497,4.5027370452880904,4.5619544982910201]
["       Liquefied Petroleum Gas8/",15.146578788757299,16.654964447021499,20.603065490722699,20.419296264648398,16.382719039916999,15.8189392089844,15.6014108657837,15.311073303222701,15.2448682785034,15.179443359375,15.2014074325562,15.2481698989868,15.181710243225099,15.278540611267101,15.3825387954712,15.370577812194799,15.3893880844116,15.510032653808601,15.6597127914429,15.774450302124,15.847083091735801,16.037206649780298,16.107362747192401,16.244932174682599]
["     Natural Gas 9/",7.2317700386047399,9.0444478988647496,9.7142534255981392,9.7951860427856392,9.2951183319091797,8.9833269119262695,8.7195968627929705,8.6326360702514595,8.5613536834716797,8.6190090179443395,8.7080965042114293,8.8271207809448207,8.9910020828247106,9.1132879257202095,9.1042909622192401,9.1039905548095703,9.2009325027465803,9.3432521820068395,9.4465293884277308,9.5402717590331996,9.5791873931884801,9.5845136642456108,9.6436891555786097,9.694091796875]
["     Ethanol (E85) 10/",14.6543264389038,16.232709884643601,19.6646022796631,19.5902194976807,19.473403930664102,18.312351226806602,18.154972076416001,17.744245529174801,17.108533859252901,16.985416412353501,16.891477584838899,17.106473922729499,17.298709869384801,17.370653152465799,17.404756546020501,17.4316711425781,17.495216369628899,17.111986160278299,17.221326828002901,17.6731853485107,17.676996231079102,17.866504669189499,17.993064880371101,18.128524780273398,{"$f":"Y550+($AI$380-$Y$550)/10","v":18.036478922002154}]
["   Electricity",20.034517288208001,20.636144638061499,21.1998176574707,20.923387527465799,19.967187881469702,19.089002609252901,18.799640655517599,18.828804016113299,18.807792663574201,18.831340789794901,19.0241508483887,19.232509613037099,19.521226882934599,19.590469360351602,19.544775009155298,19.5792236328125,19.706111907958999,19.899772644043001,19.988050460815401,20.054973602294901,19.979206085205099,19.890190124511701,19.9172687530518,19.9590148925781]
["","","","","","","","","","","","","","","","","","","","","","","","",""]
[" Average End-Use Energy",10.2607097625732,11.4965677261353,12.498481750488301,12.3126974105835,11.5857706069946,11.0374755859375,10.8027191162109,10.6485815048218,10.5555610656738,10.564617156982401,10.6249675750732,10.7333173751831,10.851320266723601,10.9544372558594,11.0046529769897,11.070010185241699,11.175311088561999,11.313448905944799,11.4217777252197,11.534593582153301,11.6029949188232,11.660957336425801,11.7183265686035,11.827390670776399]
["   Primary Energy",7.8488264083862296,9.3171482086181605,10.5270042419434,10.2914838790894,9.5772314071655291,9.0944671630859393,8.8957033157348597,8.7092790603637695,8.6138839721679705,8.6225843429565394,8.6363019943237305,8.7009534835815394,8.7555856704711896,8.8331260681152308,8.8750228881835902,8.9212465286254901,8.9933633804321307,9.0904560089111293,9.1763067245483398,9.2688179016113299,9.3425512313842791,9.4030828475952095,9.4481410980224592,9.5455484390258807]
["   Electricity",21.599882125854499,21.735733032226602,21.728578567504901,21.659519195556602,20.859115600585898,19.947565078735401,19.5044040679932,19.468164443969702,19.363897323608398,19.340778350830099,19.565423965454102,19.829431533813501,20.184032440185501,20.348131179809599,20.384618759155298,20.4941310882568,20.6934413909912,20.961088180541999,21.1064147949219,21.2582683563232,21.2429523468018,21.2300205230713,21.277418136596701,21.3841457366943]
["","","","","","","","","","","","","","","","","","","","","","","","",""]
[" Electric Power 11/","","","","","","","","","","","","","","","","","","","","","","","",""]
["   Fossil Fuel Average",1.8996955156326301,2.2409727573394802,2.4238619804382302,2.3792355060577401,2.2243471145629901,2.11745405197144,2.0720956325531001,2.06648945808411,2.0576293468475302,2.0898380279540998,2.13185787200928,2.1827101707458501,2.2442750930786102,2.2846662998199498,2.2886507511138898,2.31255102157593,2.3658699989318799,2.41897773742676,2.4451649188995401,2.4616906642913801,2.4596512317657502,2.4499151706695601,2.46315670013428,2.4591720104217498]
["     Petroleum Products",4.3748912811279297,5.2786889076232901,5.9517397880554199,5.8145914077758798,5.36482858657837,4.9555935859680202,4.76583051681519,4.6106519699096697,4.5544371604919398,4.5760931968689,4.6005949974060103,4.65545606613159,4.7050404548645002,4.76641750335693,4.8219771385192898,4.8744759559631303,4.9555630683898899,5.0235657691955602,5.0990805625915501,5.1768889427185103,5.2447147369384801,5.3197603225707999,5.3696103096008301,5.4173326492309597]
["       Distillate Fuel",5.6938004493713397,6.4773354530334499,7.1750502586364702,6.8899459838867196,6.2672758102417001,5.8609590530395499,5.6430783271789604,5.4534807205200204,5.3617582321167001,5.3288640975952104,5.3712139129638699,5.41644287109375,5.4747476577758798,5.5268063545227104,5.5894103050231898,5.6297807693481401,5.7926478385925302,5.9167857170104998,6.0082931518554696,6.11431789398193,6.21482229232788,6.2930455207824698,6.3174986839294398,6.3298768997192401]
["       Residual Fuel",3.9850425720214799,4.7911210060119602,5.5054435729980504,5.3836607933044398,4.9928164482116699,4.5735058784484899,4.37508344650269,4.2357888221740696,4.1871180534362802,4.2367839813232404,4.2823972702026403,4.3351020812988299,4.38077735900879,4.4392328262329102,4.4927945137023899,4.5466628074645996,4.5988087654113796,4.6550941467285201,4.7130184173584002,4.7694864273071298,4.8261427879333496,4.8835220336914098,4.9410810470581099,5.0030183792114302]
["     Natural Gas",3.6857740879058798,5.4593739509582502,5.9836626052856401,5.9217834472656303,5.2677536010742196,4.83196926116943,4.4959845542907697,4.3869647979736301,4.2738447189331099,4.3073697090148899,4.4138617515564,4.5377993583679199,4.6997785568237296,4.8059244155883798,4.7723231315612802,4.7962751388549796,4.93237209320068,5.0951194763183603,5.2029786109924299,5.2939982414245597,5.3285460472106898,5.3187093734741202,5.3844461441040004,5.4420223236084002,{"$f":"Y562+($AI$392-$Y$562)/10","v":5.4722581683132612}]
["     Steam Coal",1.2699717283248899,1.27919089794159,1.2833664417266799,1.28942894935608,1.29215919971466,1.28011155128479,1.2771430015564,1.2664887905120801,1.2516112327575699,1.2440552711486801,1.2386393547058101,1.23525643348694,1.23468470573425,1.2341449260711701,1.23174548149109,1.2347780466079701,1.23870933055878,1.2427853345871001,1.24646520614624,1.2552444934845,1.26424860954285,1.2944931983947801,1.3030458688736,1.30599772930145,{"$f":"Y563+($AI$393-$Y$563)/10","v":1.3088234854404943}]
["","","","","","","","","","","","","","","","","","","","","","","","",""]
[" Average Price to All Users 12/","","","","","","","","","","","","","","","","","","","","","","","",""]
["   Petroleum Products 2/",9.0916013717651403,10.5092258453369,12.005053520202599,11.630154609680201,10.867414474487299,10.341483116149901,10.206826210021999,9.9809312820434606,9.9117403030395508,9.9329805374145508,9.9184780120849592,9.9575662612915004,9.9538516998290998,10.000968933105501,10.066521644592299,10.122728347778301,10.166119575500501,10.2242088317871,10.2887620925903,10.370365142822299,10.451409339904799,10.528607368469199,10.560112953186,10.6600894927979]
["     Distillate Fuel",8.7129955291747994,9.89868068695068,10.9323616027832,10.516496658325201,10.0722150802612,9.7644062042236293,9.6708259582519496,9.5059432983398402,9.5328626632690394,9.6073579788208008,9.6717586517334002,9.7472448348999006,9.7227439880371094,9.7185726165771502,9.7264575958252006,9.7659683227539098,9.7933034896850604,9.8243274688720703,9.7878532409668004,9.8349857330322301,9.8761272430419904,9.8313732147216797,9.8799133300781303,10.0311069488525]
["     Jet Fuel",6.0538434982299796,6.4578518867492702,8.1168746948242205,7.6875572204589799,7.0150871276855504,6.5790328979492196,6.5712537765502903,6.42602443695068,6.2476048469543501,6.2184038162231401,6.2436552047729501,6.2858424186706499,6.2737250328064,6.2926135063171396,6.3336305618286097,6.3623290061950701,6.4419050216674796,6.5377755165100098,6.5789065361022896,6.7034192085266104,6.8036813735961896,6.8691210746765101,6.8930430412292498,6.9258189201354998]
["     Liquefied Petroleum Gas",9.5166797637939506,13.0396432876587,15.6858806610107,14.0742273330688,12.086350440979,11.4653730392456,11.285403251647899,11.0092105865479,10.989564895629901,10.925596237182599,10.987684249877899,11.0838632583618,11.0187425613403,11.2084665298462,11.3385829925537,11.336560249328601,11.412732124328601,11.5561437606812,11.7385349273682,11.9240121841431,12.033415794372599,12.184607505798301,12.2847499847412,12.335958480835]
["     Motor Gasoline 7/",11.3185987472534,12.9258327484131,14.650143623352101,14.3442440032959,13.623025894165,12.923449516296399,12.7128458023071,12.432819366455099,12.310016632080099,12.3222455978394,12.2171115875244,12.2130832672119,12.22132396698,12.248191833496101,12.309587478637701,12.376181602478001,12.4016332626343,12.440443038940399,12.509931564331101,12.547391891479499,12.611403465271,12.7098541259766,12.7049369812012,12.8036108016968]
["     Residual Fuel",3.9308724403381299,4.6628575325012198,5.07232666015625,5.1433629989623997,4.8060836791992196,4.3862032890319798,4.1832194328308097,4.0440359115600604,3.9943466186523402,4.04720115661621,4.0966601371765101,4.1477751731872603,4.19142723083496,4.2503523826599103,4.3018612861633301,4.3527650833129901,4.4055538177490199,4.4662823677062997,4.5225110054016104,4.5828208923339799,4.6386957168579102,4.6918659210205096,4.7469024658203098,4.8068332672119096]
["   Natural Gas",5.1461992263793901,6.8558807373046902,7.3508329391479501,7.3838677406311,6.7167663574218803,6.2544136047363299,5.8490047454834002,5.6922402381896999,5.5182204246520996,5.4887638092040998,5.5592789649963397,5.6574964523315403,5.8102455139160201,5.9230461120605504,5.8875889778137198,5.8938632011413601,6.0147280693054199,6.1772904396057102,6.2973737716674796,6.40012407302856,6.4435343742370597,6.4505195617675799,6.5169725418090803,6.5874438285827601]
["   Coal",1.2938040494918801,1.29924309253693,1.30395972728729,1.3117660284042401,1.3130011558532699,1.3001606464386,1.2972036600112899,1.28666663169861,1.2722240686416599,1.2649568319320701,1.25909507274628,1.25531446933746,1.25464415550232,1.25405156612396,1.2516055107116699,1.25465047359467,1.2582825422287001,1.2619441747665401,1.26514172554016,1.27338314056396,1.2817230224609399,1.31160092353821,1.3194112777710001,1.3217089176178001]
["   Ethanol (E85) 10/",14.6543264389038,16.232709884643601,19.6646022796631,19.5902194976807,19.473403930664102,18.312351226806602,18.154972076416001,17.744245529174801,17.108533859252901,16.985416412353501,16.891477584838899,17.106473922729499,17.298709869384801,17.370653152465799,17.404756546020501,17.4316711425781,17.495216369628899,17.111986160278299,17.221326828002901,17.6731853485107,17.676996231079102,17.866504669189499,17.993064880371101,18.128524780273398]
["   Electricity",21.599882125854499,21.735733032226602,21.728578567504901,21.659519195556602,20.859115600585898,19.947565078735401,19.5044040679932,19.468164443969702,19.363897323608398,19.340778350830099,19.565423965454102,19.829431533813501,20.184032440185501,20.348131179809599,20.384618759155298,20.4941310882568,20.6934413909912,20.961088180541999,21.1064147949219,21.2582683563232,21.2429523468018,21.2300205230713,21.277418136596701,21.3841457366943]
["","","","","","","","","","","","","","","","","","","","","","","","",""]
["Non-Renewable Energy Expenditures by Sector","","","","","","","","","","","","","","","","","","","","","","","",""]
["(billion 2003 dollars)","","","","","","","","","","","","","","","","","","","","","","","",""]
[" Residential",163.90481567382801,177.16523742675801,181.72630310058599,185.23806762695301,178.77069091796901,174.57431030273401,173.49729919433599,174.68045043945301,175.87545776367199,177.93170166015599,181.97520446777301,185.45910644531301,189.89924621582,193.20950317382801,195.50482177734401,197.60719299316401,201.40017700195301,205.80612182617199,209.76078796386699,212.75457763671901,215.110427856445,217.42091369628901,220.97119140625,223.85739135742199]
[" Commercial",122.690147399902,128.153732299805,130.48348999023401,132.28971862793,128.48481750488301,125.5166015625,125.36106109619099,127.820442199707,129.92327880859401,133.10743713378901,137.92835998535199,142.925369262695,148.816970825195,153.52194213867199,157.03869628906301,161.345138549805,166.52362060546901,172.33033752441401,177.27947998046901,182.50421142578099,186.391357421875,190.50810241699199,195.38455200195301,200.92575073242199]
[" Industrial",124.39901733398401,147.11244201660199,168.10716247558599,167.31402587890599,151.68084716796901,143.54243469238301,141.56742858886699,140.77819824218801,139.57333374023401,140.39901733398401,142.75350952148401,145.42568969726599,149.20526123046901,152.35485839843801,153.50325012207,156.35830688476599,160.767654418945,165.76315307617199,169.931716918945,173.961990356445,176.65931701660199,179.21453857421901,182.00726318359401,184.95687866210901]
[" Transportation",263.72879028320301,302.59255981445301,352.23770141601602,351.05020141601602,340.83407592773398,332.5693359375,335.96701049804699,336.85531616210898,341.13198852539102,348.16427612304699,352.90618896484398,359.69818115234398,365.95080566406301,372.46246337890602,379.283447265625,387.02755737304699,393.88119506835898,401.07183837890602,407.83190917968801,415.10699462890602,423.06927490234398,431.36416625976602,438.52017211914102,449.30920410156301]
["   Total Non-Renewable Expenditures",674.72277832031295,755.02398681640602,832.5546875,835.89202880859398,799.77044677734398,776.20269775390602,776.392822265625,780.13439941406295,786.50402832031295,799.60241699218795,815.563232421875,833.50836181640602,853.872314453125,871.54876708984398,885.33020019531295,902.33819580078102,922.57263183593795,944.971435546875,964.80389404296898,984.32775878906295,1001.23034667969,1018.50769042969,1036.88317871094,1059.04919433594]
["   Transportation Renewable Expenditures",1.1704622767865699E-2,1.72001253813505E-2,2.0739471539855E-2,2.2893460467457799E-2,2.3359816521406201E-2,2.56899110972881E-2,2.8361881151795401E-2,3.0972529202699699E-2,3.4895084798336001E-2,3.86636592447758E-2,4.1480015963315998E-2,4.3943785130977603E-2,4.6801801770925501E-2,4.9450792372226701E-2,5.3890265524387401E-2,5.8303136378526701E-2,6.2215700745582601E-2,6.0202639549970599E-2,6.6687978804111495E-2,6.8060472607612596E-2,7.0131160318851499E-2,7.4032962322235094E-2,7.6179362833499895E-2,7.9960107803344699E-2]
["   Total Expenditures",674.73449707031295,755.04119873046898,832.575439453125,835.91491699218795,799.79382324218795,776.22839355468795,776.42120361328102,780.16534423828102,786.53894042968795,799.64105224609398,815.604736328125,833.55230712890602,853.91912841796898,871.59820556640602,885.38409423828102,902.396484375,922.63482666015602,945.03161621093795,964.87060546875,984.39581298828102,1001.30047607422,1018.58172607422,1036.95935058594,1059.12915039063]
["Woody Biomass","See High A Case"]
["Methanol","See High A Case"]
["","","","","","","","","","","","","","","","","","","","","","","","",""]
["   1/ Weighted average price includes fuels below as well as coal."]
["   2/ This quantity is the weighted average for all petroleum products, not just those listed below."]
["   3/ Includes energy for combined heat and power plants, except those whose primary business is to sell electricity, or electricity and heat, to the public."]
["   4/ Excludes use for lease and plant fuel."]
["   5/ Diesel fuel containing 500 parts per million (ppm) or 15 ppm sulfur.  Price includes Federal and State taxes while excluding county and local taxes."]
["   6/ Kerosene-type jet fuel.  Price includes Federal and State taxes while excluding county and local taxes."]
["   7/ Sales weighted-average price for all grades. Includes Federal, State, and local taxes."]
["   8/ Includes Federal and State taxes while excluding county and local taxes."]
["   9/ Compressed natural gas used as a vehicle fuel.  Price includes estimated motor vehicle fuel taxes."]
["   10/ E85 refers to a blend of 85 percent ethanol (renewable) and 15 percent motor gasoline (nonrenewable).  To address cold starting issues, the percentage of ethanol actually"]
["varies seasonally.  The annual average ethanol content of 74 percent is used for this forecast."]
["   11/ Includes electricity-only and combined heat and power plants whose primary business is to sell electricity, or electricity and heat, to the public."]
["   12/ Weighted averages of end-use fuel prices are derived from the prices shown in each sector and the corresponding sectoral consumption."]
["   Btu = British thermal unit."]
["   Note:  Data for 2002 and 2003 are model results and may differ slightly from official EIA data reports."]
["   Sources:  2002 and 2003 prices for motor gasoline, distillate, and jet fuel are based on prices in the Energy Information Administration (EIA), Petroleum Marketing Annual"]
["2003, DOE/EIA-0487(2003) (Washington, DC, August 2004).  2002 residential and commercial natural gas delivered prices:  EIA, Natural Gas Annual 2002, DOE/EIA-0131(2002)"]
["(Washington, DC, January 2004).  2003 residential and commercial natural gas delivered prices:  EIA, Natural Gas Monthly, DOE/EIA-0130(2004/07) (Washington, DC, July 2004)."]
["2002 and 2003 electric power sector natural gas prices:  EIA, Electric Power Monthly, DOE/EIA-0226, May 2003 through April 2004, Table 4.11.A.  2002 and 2003 industrial natural"]
["gas delivered prices are estimated based on:  EIA, Manufacturing Energy Consumption Survey 1994 and industrial and wellhead prices from the Natural Gas Annual 2002,"]
["DOE/EIA-0131(2002) (Washington, DC, January 2004) and the Natural Gas Monthly, DOE/EIA-0130(2004/07) (Washington, DC, July 2004).  2002 transportation sector natural"]
["gas delivered prices are based on:  EIA, Natural Gas Annual 2002, DOE/EIA-0131(2002) (Washington, DC, January 2004) and estimated state and federal taxes.  2003"]
["transportation sector natural gas delivered prices are model results.  2002 and 2003 coal prices based on:  EIA, Quarterly Coal Report, October-December 2003,"]
["DOE/EIA-0121(2003/4Q) (Washington, DC, March 2004) and EIA, AEO2005 National Energy Modeling System run aeo2005.d102004a.  2002 and 2003 electricity prices:"]
["Annual Energy Review 2003, DOE/EIA-0384(2003) (Washington, DC, September 2004).  2002 and 2003 ethanol prices derived from weekly spot prices in the Oxy Fuel"]
["News.  Projections:  EIA, AEO2005 National Energy Modeling System run aeo2005.d102004a."]
[]
[]
[]
["Energy Prices in High A Case File",null,"Projections Vary in Cases With Different Oil Price Assumptions  "]
["AEO 2005 Appendix C, Table 3",null,"The historical record shows substantial variability in world oil prices, and there is similar uncertainty about future prices. Four AEO2005 cases with different price paths allow an assessment of alternative views on the future of oil prices (Figure 40). In the reference case, with both OPEC and non-OPEC producers scheduled to add new production capacity over the next 5 years, prices in 2010 are projected to be more than $10 per barrel lower than current prices (all prices in 2003 dollars per barrel). After 2010, oil prices are projected to rise by about 1.3 percent per year, to more than $30 per barrel in 2025. (In nominal dollars, the reference case price is about $52 in 2025.) In the low price case, prices are projected to decline from their high in 2004 to $21 per barrel in 2009 and to remain at that level out to 2025. The high A price case projects that prices will remain at about $34 through 2015 and then increase on average by 1.4 percent per year, to more than $39 per barrel in 2025. In the high B case, world oil prices are projected to fall from current levels to $37 per barrel in 2010 and then rise to $48 per barrel in 2025.  "]
["Name of file: aeo_hw-3.xls",null,"Projected prices in all four cases are higher than in AEO2004 [130], reflecting recent improved production discipline by OPEC members and limited ability of other producers to expand production despite increasing demand and high utilization rates that have led to higher prices. The price projections in the high A and B cases are sufficiently robust to encourage greater market penetration of alternative energy supplies. "]
["http://www.eia.doe.gov/oiaf/aeo/index.html"]
[]
[" Table   3.  Energy Prices by Sector and Source"]
["                      (2003 Dollars per Million Btu, Unless Otherwise Noted)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Extrapolated values (DMS 8/14/07 based on PNNL Mini-CAM Model"]
["","2002","2003","2004","2005","2006","2007","2008","2009","2010","2011","2012","2013","2014","2015","2016","2017","2018","2019","2020","2021","2022","2023","2024","2025",2026]
["","","","","","","","","","","","","","","","","","","","","","","","",""]
[" Residential",15.0220499038696,15.811363220214799,16.426000595092798,16.4650573730469,15.8399600982666,15.268068313598601,14.8466091156006,14.7514638900757,14.6550188064575,14.6146650314331,14.723385810852101,14.890528678894,15.1057291030884,15.213768959045399,15.3079509735107,15.3113193511963,15.4291744232178,15.6326360702515,15.9024982452393,16.1096382141113,16.157627105712901,16.2051906585693,16.309419631958001,16.471462249755898]
["   Primary Energy 1/",8.3285751342773402,9.67810153961182,10.65163230896,10.5740642547607,9.9307842254638707,9.5159215927124006,9.1046285629272496,8.8910932540893608,8.7197055816650408,8.6297874450683594,8.6824674606323207,8.7884712219238299,8.9080095291137695,9.0072793960571307,9.0682640075683594,9.0415534973144496,9.1060371398925799,9.2553215026855504,9.4607038497924805,9.6327857971191406,9.6968526840209996,9.7728433609008807,9.8535881042480504,9.9786624908447301]
["     Petroleum Products 2/",10.0436496734619,11.266843795776399,13.0600233078003,12.5262851715088,12.207064628601101,12.234001159668001,12.201937675476101,12.2015285491943,12.262092590331999,12.1512393951416,12.1732091903687,12.1968584060669,12.177050590515099,12.2115392684937,12.3804988861084,12.519121170043899,12.6585578918457,12.798875808715801,12.8676557540894,13.13560962677,13.328717231750501,13.556846618652299,13.722979545593301,13.940701484680201]
["       Distillate Fuel",8.3698368072509801,9.5702075958252006,10.537187576293899,10.120927810668899,9.8627185821533203,9.8399791717529297,9.8302927017211896,9.8297405242919904,9.8252134323120099,9.7093524932861293,9.7021694183349592,9.7383060455322301,9.80072116851807,9.7244081497192401,9.8378829956054705,9.8340024948120099,9.9226865768432599,10.0213985443115,10.078977584838899,10.280327796936,10.3802833557129,10.4678192138672,10.5482635498047,10.6469841003418]
["       Liquefied Petroleum Gas",12.976583480835,14.582922935485801,17.570188522338899,17.073205947876001,16.564285278320298,16.581449508666999,16.4250888824463,16.346086502075199,16.4532871246338,16.288703918456999,16.298521041870099,16.236286163330099,15.99489402771,16.1197624206543,16.286623001098601,16.56103515625,16.690963745117202,16.804660797119102,16.7820129394531,17.028240203857401,17.2251377105713,17.515983581543001,17.670423507690401,17.9113578796387]
["     Natural Gas",7.8179483413696298,9.2187824249267596,9.9373655319213903,10.036292076110801,9.3139858245849592,8.7959203720092791,8.3035001754760707,8.0470056533813494,7.8287873268127397,7.7531881332397496,7.8190288543701199,7.9488449096679696,8.1063919067382795,8.2242641448974592,8.2648267745971697,8.2073183059692401,8.2647809982299805,8.4262142181396502,8.6721630096435494,8.83197021484375,8.8790025711059606,8.93493747711182,9.0109558105468803,9.1305398941040004]
["   Electricity",25.222642898559599,25.415189743041999,25.1915378570557,25.148117065429702,24.4542636871338,23.578901290893601,23.091381072998001,23.1348171234131,23.120912551879901,23.118898391723601,23.2529602050781,23.4250183105469,23.684103012085,23.7079162597656,23.7613220214844,23.722099304199201,23.8309440612793,24.013486862182599,24.267650604248001,24.4126377105713,24.3365364074707,24.2477512359619,24.2885627746582,24.396659851074201]
["","","","","","","","","","","","","","","","","","","","","","","","",""]
[" Commercial",15.064169883728001,15.629265785217299,15.835695266723601,15.918652534484901,15.2065124511719,14.526217460632299,14.119109153747599,14.0872592926025,14.0534925460815,14.108097076416,14.338217735290501,14.584888458251999,14.9309749603271,15.096228599548301,15.2413949966431,15.255002975463899,15.399823188781699,15.6329202651978,15.9477081298828,16.179660797119102,16.227045059204102,16.249193191528299,16.367641448974599,16.5326118469238]
["   Primary Energy 1/",6.5697088241577104,7.9157042503356898,8.3734045028686506,8.3685989379882795,7.9054894447326696,7.6067800521850604,7.3189792633056596,7.2159371376037598,7.1498117446899396,7.1872353553771999,7.2290387153625497,7.30631303787231,7.4108529090881303,7.4683656692504901,7.4930505752563503,7.43192434310913,7.4779849052429199,7.60019826889038,7.7867598533630398,7.91162109375,7.9430484771728498,7.9890594482421902,8.0587644577026403,8.1779403686523402]
["     Petroleum Products 2/",6.9482707977294904,8.0266513824462908,8.9197740554809606,8.6532411575317401,8.7558631896972692,8.8328323364257795,8.8167963027954102,8.8182945251464808,8.8873138427734393,8.9125509262084996,8.9192247390747106,8.8803482055664098,8.8586578369140607,8.7692289352416992,8.7682600021362305,8.7373514175415004,8.7862501144409197,8.8491783142089808,8.8908815383911097,9.0514831542968803,9.1475715637206996,9.2663307189941406,9.3906812667846697,9.6513500213622994]
["       Distillate Fuel",6.1493649482727104,7.03082323074341,7.7272830009460396,7.4210705757141104,7.6805524826049796,7.8215904235839799,7.8266153335571298,7.8668313026428196,7.9658513069152797,8.0328092575073207,8.0569534301757795,8.0234899520874006,8.0314903259277308,7.91062688827515,7.8695487976074201,7.7933855056762704,7.8344025611877397,7.89571285247803,7.9562859535217303,8.1191616058349592,8.2043952941894496,8.3111848831176793,8.4434480667114293,8.7515277862548793]
["       Residual Fuel",4.2683343887329102,4.9646224975585902,5.0606441497802699,5.3499693870544398,5.6657009124755904,5.6566004753112802,5.6533966064453098,5.65053033828735,5.6487455368042001,5.6555466651916504,5.6602473258972203,5.6679368019104004,5.6729874610900897,5.6782984733581499,5.7556295394897496,5.8296666145324698,5.9058866500854501,5.9829258918762198,6.0580596923828098,6.1354246139526403,6.2122497558593803,6.2891340255737296,6.3645572662353498,6.4413762092590297]
["     Natural Gas",6.6170339584350604,8.0769119262695295,8.4473829269409197,8.5046024322509801,7.8886041641235396,7.4893965721130398,7.1298856735229501,7.0003471374511701,6.9035739898681596,6.94567918777466,6.9973711967468297,7.1022868156433097,7.2368607521057102,7.3275256156921396,7.3574790954589799,7.2871475219726598,7.3330197334289604,7.4703903198242196,7.6915035247802699,7.8109488487243697,7.8279361724853498,7.8590941429138201,7.9183402061462402,8.0110416412353498,{"$f":"Y641+($AI$471-$Y$641)/10","v":8.0591226890564176}]
["   Electricity",23.353584289550799,23.2374382019043,23.0424194335938,22.939121246337901,21.907506942748999,20.807579040527301,20.2319431304932,20.2009677886963,20.132976531982401,20.128959655761701,20.445728302001999,20.757715225219702,21.231256484985401,21.404373168945298,21.571121215820298,21.578863143920898,21.739751815795898,21.989313125610401,22.322486877441399,22.5522785186768,22.5369548797607,22.469936370849599,22.555665969848601,22.682601928710898,{"$f":"Y642+($AI$472-$Y$642)/10","v":22.586698480675594}]
["","","","","","","","","","","","","","","","","","","","","","","","",""]
[" Industrial 3/",6.3922061920165998,7.7839651107788104,8.7313165664672905,8.5384979248046893,8.1135501861572301,7.8849329948425302,7.7104330062866202,7.6478543281555202,7.5814275741577104,7.5381202697753897,7.5780467987060502,7.6416735649108896,7.7132387161254901,7.8013410568237296,7.8755207061767596,7.9062352180481001,7.9948873519897496,8.1163215637206996,8.2487821578979492,8.4059162139892596,8.4608268737793004,8.5343141555786097,8.6114902496337908,8.7719221115112305]
["   Primary Energy",4.9298634529113796,6.4939708709716797,7.4592781066894496,7.2447438240051296,6.84521436691284,6.6732459068298304,6.51676225662231,6.4484291076660201,6.3966798782348597,6.3644347190856898,6.3782010078430202,6.3993859291076696,6.4120607376098597,6.4825568199157697,6.5450062751770002,6.5706739425659197,6.6389350891113299,6.7355680465698198,6.8303794860839799,6.9826822280883798,7.0502834320068404,7.1402068138122603,7.2155933380126998,7.3827753067016602]
["     Petroleum Products 2/",6.5291514396667498,8.2850980758666992,9.8001213073730504,9.3321943283081108,9.0226831436157209,9.0089912414550799,8.9738616943359393,8.8902368545532209,8.9552536010742205,8.9079008102416992,8.89520359039307,8.8468990325927699,8.7482786178588903,8.7885036468505895,8.8624305725097692,8.9473028182983398,9.0262336730956996,9.1055555343627894,9.0882310867309606,9.3312444686889595,9.4788913726806605,9.6528720855712908,9.7811794281005895,10.0579071044922]
["       Distillate Fuel",6.3323707580566397,7.2384452819824201,7.96527099609375,7.6527161598205602,7.9603652954101598,8.0741472244262695,8.2605934143066406,8.3100318908691406,8.4493141174316406,8.8189620971679705,8.8862495422363299,8.8418188095092791,8.8337812423706108,8.6748180389404297,8.5509977340698207,8.4207677841186506,8.4376201629638707,8.4841489791870099,8.5509052276611293,8.6700105667114293,8.74859523773193,8.8432664871215803,9.0058250427246094,9.3929624557495099]
["       Liquefied Petroleum Gas",8.4833917617797905,12.566796302795399,15.1471004486084,13.237501144409199,12.375891685485801,12.379506111145,12.2225999832153,12.080751419067401,12.212836265564,12.0270395278931,11.9549217224121,11.879666328430201,11.6303720474243,11.7905416488647,11.941043853759799,12.1426992416382,12.289721488952599,12.378883361816399,12.2595558166504,12.590350151061999,12.7815389633179,12.973883628845201,13.0949363708496,13.367587089538601]
["       Residual Fuel",3.9384419918060298,4.5867881774902299,4.6800308227539098,4.9388952255248997,5.2859730720520002,5.2723593711853001,5.2104086875915501,5.1732821464538601,5.1717634201049796,5.17871141433716,5.1878075599670401,5.1966009140014604,5.2060360908508301,5.2088470458984402,5.2896075248718297,5.3583388328552202,5.44156694412231,5.5192761421203604,5.5953726768493697,5.6724872589111301,5.7441039085388201,5.8200716972351101,5.9009070396423304,5.9898118972778303]
["     Natural Gas 4/",3.88655662536621,5.55936574935913,6.0491261482238796,6.0771641731262198,5.4298515319824201,5.0030980110168501,4.6280007362365696,4.5291852951049796,4.41147708892822,4.4342226982116699,4.4864263534545898,4.5912823677062997,4.7218933105468803,4.8130536079406703,4.8621869087219203,4.81842041015625,4.8841061592102104,5.0232949256896999,5.2583932876586896,5.3567323684692401,5.3575921058654803,5.37701320648193,5.4306664466857901,5.5327925682067898,{"$f":"Y650+($AI$480-$Y$650)/10","v":5.5600694801614594}]
["     Metallurgical Coal",1.88388228416443,1.8499996662139899,1.9633457660675,1.8999761343002299,1.88347840309143,1.8588999509811399,1.8578026294708301,1.85227739810944,1.8239538669586199,1.79700314998627,1.78184306621552,1.7756989002227801,1.77074086666107,1.7668309211730999,1.7627635002136199,1.7565006017684901,1.75614774227142,1.7571268081664999,1.75483202934265,1.7449706792831401,1.72660219669342,1.70969367027283,1.70006084442139,1.6866580247878999]
["     Steam Coal",1.5976041555404701,1.5543407201767001,1.5670678615570099,1.6038056612014799,1.6009258031845099,1.58739173412323,1.58863317966461,1.5846539735794101,1.5799860954284699,1.5764416456222501,1.5679914951324501,1.5610833168029801,1.5600349903106701,1.56054711341858,1.56748187541962,1.5675091743469201,1.5641727447509799,1.5615659952163701,1.58828938007355,1.58737933635712,1.59387278556824,1.5848928689956701,1.5860744714736901,1.5880702733993499]
["   Electricity",14.734835624694799,15.0261535644531,15.722662925720201,15.5983018875122,15.078427314758301,14.4692840576172,14.1632738113403,14.081834793090801,13.919806480407701,13.785112380981399,13.931169509887701,14.1889085769653,14.5255270004272,14.681715965271,14.814373970031699,14.8553409576416,15.0255784988403,15.2628774642944,15.5799751281738,15.7510900497437,15.7371273040771,15.705772399902299,15.779216766357401,15.8933115005493,{"$f":"Y653+($AI$483-$Y$653)/10","v":15.820176294068443}]
["","","","","","","","","","","","","","","","","","","","","","","","",""]
[" Transportation",10.068477630615201,11.4567165374756,12.984992980956999,12.648449897766101,12.9899549484253,12.831539154052701,12.772025108337401,12.778377532959,12.6527404785156,12.633409500122101,12.627567291259799,12.5634212493896,12.5677394866943,12.4416351318359,12.463407516479499,12.3592376708984,12.3700494766235,12.4214639663696,12.406385421752899,12.599157333374,12.7199811935425,12.8404388427734,12.9761352539063,13.180356025695801]
["   Primary Energy",10.0396184921265,11.4297380447388,12.961000442504901,12.6243276596069,12.9694175720215,12.812975883483899,12.7542219161987,12.7604532241821,12.634376525878899,12.614933013916,12.6084880828857,12.543541908264199,12.546923637390099,12.4202537536621,12.441800117492701,12.3374538421631,12.3479681015015,12.3989114761353,12.3829250335693,12.575768470764199,12.6970834732056,12.8181715011597,12.9540061950684,13.1585645675659]
["     Petroleum Products 2/",10.0409812927246,11.431476593017599,12.9638833999634,12.6272735595703,12.9738121032715,12.8180704116821,12.7602338790894,12.7672443389893,12.6416578292847,12.622591972351101,12.616462707519499,12.551496505737299,12.554883956909199,12.4279336929321,12.4496717453003,12.3454332351685,12.356036186218301,12.4068956375122,12.3903903961182,12.5835561752319,12.7052898406982,12.826750755310099,12.9629173278809,13.167941093444799]
["       Distillate Fuel 5/",9.5535230636596697,10.9202365875244,12.0208587646484,11.5461339950562,12.0997161865234,12.488727569580099,12.3829002380371,12.4196271896362,12.508094787597701,12.555921554565399,12.5986595153809,12.507498741149901,12.460197448730501,12.2335548400879,12.028847694396999,11.832740783691399,11.7916069030762,11.803469657897899,11.8377895355225,11.9129686355591,11.9319505691528,11.983411788940399,12.11021900177,12.4955101013184,{"$f":"Y658+($AI$488-$Y$658)/10","v":12.860153747735882}]
["       Jet Fuel 6/",6.0538434982299796,6.4578518867492702,8.1168746948242205,7.6875567436218297,7.8739576339721697,7.8265089988708496,7.9840884208679199,8.0166091918945295,7.8608303070068404,7.81276655197144,7.8045797348022496,7.7928524017334002,7.7725591659545898,7.7157216072082502,7.7164225578308097,7.6991229057312003,7.7546834945678702,7.8412432670593297,7.8916783332824698,8.0530261993408203,8.1459932327270508,8.2922735214233398,8.4199304580688494,8.7479171752929705]
["       Motor Gasoline 7/",11.3207235336304,12.9284992218018,14.6530704498291,14.346966743469199,14.7094535827637,14.3600215911865,14.2510118484497,14.250683784484901,14.0786781311035,14.0637760162354,14.0259552001953,13.906542778015099,13.9343166351318,13.819755554199199,13.920813560485801,13.821713447570801,13.8340721130371,13.8936500549316,13.8356838226318,14.0806474685669,14.2383365631104,14.3749399185181,14.5092010498047,14.605681419372599,{"$f":"Y660+($AI$490-$Y$660)/10","v":15.03173973157025}]
["       Residual Fuel",3.83150410652161,4.4939312934875497,4.5839381217956499,4.8374896049499503,5.1729192733764604,5.1682701110839799,5.1688323020935103,5.1695828437805202,5.16760349273682,5.1733479499816903,5.1798586845397896,5.1877336502075204,5.1953010559081996,5.2001247406005904,5.2810626029968297,5.3552770614623997,5.4362750053405797,5.5152239799499503,5.5921721458435103,5.6705627441406303,5.7475032806396502,5.8269476890564,5.9046044349670401,5.9824995994567898]
["       Liquefied Petroleum Gas8/",15.146578788757299,16.654964447021499,20.603065490722699,20.419296264648398,17.4092102050781,17.409763336181602,17.1964435577393,17.156021118164102,17.248268127441399,17.105394363403299,17.085474014282202,16.997465133666999,16.7497043609619,16.830522537231399,16.954969406127901,17.1650085449219,17.2562961578369,17.321376800537099,17.262313842773398,17.454835891723601,17.584600448608398,17.847267150878899,17.9585571289063,18.1527404785156]
["     Natural Gas 9/",7.2317700386047399,9.0444478988647496,9.7142210006713903,9.7955017089843803,9.2987012863159197,9.0087041854858398,8.73461818695068,8.6602125167846697,8.6087532043456996,8.6854057312011701,8.7734069824218803,8.9131555557250994,9.0697097778320295,9.1761322021484393,9.2086582183837908,9.1414461135864293,9.1881532669067401,9.3183298110961896,9.5262966156005895,9.6340904235839808,9.6386470794677699,9.6553201675415004,9.7052288055419904,9.7829256057739293]
["     Ethanol (E85) 10/",14.6543264389038,16.232709884643601,19.6646022796631,19.716905593872099,20.910398483276399,20.088336944580099,20.034643173217798,19.876234054565401,19.0899848937988,19.0770473480225,18.9334907531738,18.8203315734863,18.8769016265869,18.733657836914102,18.836368560791001,18.717578887939499,18.677961349487301,18.768825531005898,18.702945709228501,19.039726257324201,19.213029861450199,19.429216384887699,19.537574768066399,19.6945476531982,{"$f":"Y664+($AI$494-$Y$664)/10","v":19.593947309306923}]
["   Electricity",20.034517288208001,20.636144638061499,21.2071418762207,20.9249382019043,20.016746520996101,19.1842136383057,18.876358032226602,18.930015563964801,18.9569396972656,18.971715927123999,19.161241531372099,19.352525711059599,19.6624240875244,19.699916839599599,19.754545211791999,19.6803493499756,19.749149322509801,19.913064956665,20.148523330688501,20.261070251464801,20.168498992919901,20.043989181518601,20.096965789794901,20.154518127441399]
["","","","","","","","","","","","","","","","","","","","","","","","",""]
[" Average End-Use Energy",10.2607097625732,11.4965677261353,12.4990587234497,12.3170623779297,12.135007858276399,11.845267295837401,11.6573295593262,11.6295518875122,11.5503234863281,11.540096282959,11.6076335906982,11.667243003845201,11.774538040161101,11.796236991882299,11.871965408325201,11.843188285827599,11.9137773513794,12.034348487854,12.153738975524901,12.3460960388184,12.4321403503418,12.5191946029663,12.636996269226101,12.8200740814209]
["   Primary Energy",7.8488264083862296,9.3171482086181605,10.527009010314901,10.2968044281006,10.2268390655518,10.0435380935669,9.9028997421264595,9.8629217147827095,9.7728738784790004,9.75823974609375,9.7822933197021502,9.7888011932372994,9.8279809951782209,9.8149814605712908,9.8643417358398402,9.8190460205078107,9.8615427017211896,9.9469861984252894,10.0096731185913,10.190193176269499,10.288735389709499,10.396104812622101,10.5091648101807,10.694952964782701]
["   Electricity",21.599882125854499,21.735733032226602,21.731866836547901,21.659553527831999,20.918876647949201,20.055833816528299,19.596654891967798,19.579929351806602,19.517631530761701,19.486770629882798,19.702039718627901,19.955158233642599,20.317079544067401,20.442613601684599,20.578334808349599,20.580734252929702,20.7274265289307,20.953577041626001,21.262916564941399,21.454774856567401,21.4308891296387,21.3733520507813,21.452013015747099,21.5757865905762]
["","","","","","","","","","","","","","","","","","","","","","","","",""]
[" Electric Power 11/","","","","","","","","","","","","","","","","","","","","","","","",""]
["   Fossil Fuel Average",1.8996955156326301,2.2409727573394802,2.4239859580993701,2.3793189525604199,2.2557969093322798,2.16659760475159,2.1260316371917698,2.1242508888244598,2.1216156482696502,2.1531240940093999,2.1922359466552699,2.2451419830322301,2.2968165874481201,2.3293662071228001,2.3501963615417498,2.3520054817199698,2.3871843814849898,2.4302341938018799,2.5017471313476598,2.5190291404724099,2.50686860084534,2.48747658729553,2.5030989646911599,2.5170097351074201]
["     Petroleum Products",4.3748912811279297,5.2786889076232901,5.9517350196838397,5.8146204948425302,6.06520652770996,6.0658583641052202,6.0610094070434597,6.0499844551086399,6.0430412292480504,6.00789546966553,5.9784431457519496,5.9840416908264196,6.0042037963867196,6.0128812789917001,6.0971722602844203,6.1627969741821298,6.2556800842285201,6.3419466018676802,6.4189195632934597,6.5561437606811497,6.6497230529785201,6.7551417350768999,6.8526744842529297,6.9808459281921396]
["       Distillate Fuel",5.6938004493713397,6.4773354530334499,7.1750593185424796,6.8899416923522896,7.0708780288696298,7.0249619483947798,6.9838500022888201,6.9665460586547896,6.9450497627258301,6.8211231231689498,6.8083920478820801,6.7952175140380904,6.8354115486145002,6.8402228355407697,6.9283905029296902,6.9566001892089799,7.0452814102172896,7.1418867111206099,7.2127375602722203,7.4472899436950701,7.5714774131774902,7.7267389297485396,7.8528199195861799,8.0614786148071307]
["       Residual Fuel",3.9850425720214799,4.7911210060119602,5.5054440498352104,5.3836627006530797,5.6116971969604501,5.6101722717285201,5.61515140533447,5.6134881973266602,5.6123900413513201,5.6186213493347203,5.6204733848571804,5.6265015602111799,5.6295571327209499,5.6379580497741699,5.71999168395996,5.7965455055236799,5.8776378631591797,5.9570369720459002,6.0351238250732404,6.1149992942810103,6.1950988769531303,6.27585792541504,6.3545475006103498,6.4353322982788104]
["     Natural Gas",3.6857740879058798,5.4593739509582502,5.9836130142211896,5.9218006134033203,5.2758417129516602,4.86041164398193,4.5085921287536603,4.4009499549865696,4.3143215179443404,4.3619651794433603,4.4577717781066903,4.5935211181640598,4.72908592224121,4.8101162910461399,4.8377823829650897,4.7923994064331099,4.8652648925781303,5.0083761215209996,5.2321648597717303,5.32541704177856,5.3230118751525897,5.3357062339782697,5.3972234725952104,5.4970946311950701,{"$f":"Y676+($AI$506-$Y$676)/10","v":5.5250455710201605}]
["     Steam Coal",1.2699717283248899,1.27919089794159,1.2835900783538801,1.28959560394287,1.29778397083282,1.28695380687714,1.28577756881714,1.27679371833801,1.26281106472015,1.25397908687592,1.2489364147186299,1.2449804544448899,1.2430621385574301,1.24259686470032,1.24424111843109,1.2428184747695901,1.24728739261627,1.2513284683227499,1.2762980461120601,1.2851967811584499,1.2969329357147199,1.3016670942306501,1.31676089763641,1.3290703296661399,{"$f":"Y677+($AI$507-$Y$677)/10","v":1.3327822261431892}]
["","","","","","","","","","","","","","","","","","","","","","","","",""]
[" Average Price to All Users 12/","","","","","","","","","","","","","","","","","","","","","","","",""]
["   Petroleum Products 2/",9.0916013717651403,10.5092258453369,12.005053520202599,11.6376342773438,11.8251142501831,11.7351989746094,11.6926622390747,11.6848964691162,11.6311902999878,11.6124935150146,11.616386413574199,11.566198348999,11.5507049560547,11.475526809692401,11.520403861999499,11.477831840515099,11.5152139663696,11.577165603637701,11.5678558349609,11.7752237319946,11.90793800354,12.0465354919434,12.1843271255493,12.407506942749]
["     Distillate Fuel",8.7129955291747994,9.89868068695068,10.9323635101318,10.516573905944799,10.8896884918213,11.1545400619507,11.1602163314819,11.210696220397899,11.2655477523804,11.312797546386699,11.4240579605103,11.453408241271999,11.43030834198,11.241268157959,11.0996809005737,10.9476537704468,10.947796821594199,10.974308013916,11.019621849060099,11.1190385818481,11.172901153564499,11.2430562973022,11.376879692077599,11.7449541091919]
["     Jet Fuel",6.0538434982299796,6.4578518867492702,8.1168746948242205,7.6875567436218297,7.8739576339721697,7.8265089988708496,7.9840884208679199,8.0166091918945295,7.8608303070068404,7.81276655197144,7.8045797348022496,7.7928524017334002,7.7725591659545898,7.7157216072082502,7.7164225578308097,7.6991229057312003,7.7546834945678702,7.8412432670593297,7.8916783332824698,8.0530261993408203,8.1459932327270508,8.2922735214233398,8.4199304580688494,8.7479171752929705]
["     Liquefied Petroleum Gas",9.5166797637939506,13.0396432876587,15.6858806610107,14.0740518569946,13.2904262542725,13.309534072876,13.149743080139199,13.0244760513306,13.1580867767334,12.982262611389199,12.9337568283081,12.8646802902222,12.621651649475099,12.775475502014199,12.937217712402299,13.1492967605591,13.286898612976101,13.3753395080566,13.277045249939,13.584378242492701,13.775920867919901,13.987989425659199,14.116153717041,14.3756980895996]
["     Motor Gasoline 7/",11.3185987472534,12.9258327484131,14.650143623352101,14.344244956970201,14.6975507736206,14.347893714904799,14.238919258117701,14.238542556762701,14.0666351318359,14.0516872406006,14.0139780044556,13.894681930541999,13.9225015640259,13.8080444335938,13.9091501235962,13.810170173645,13.822598457336399,13.882239341735801,13.824323654174799,14.0693578720093,14.2271223068237,14.3637847900391,14.4981489181519,14.5947113037109]
["     Residual Fuel",3.9308724403381299,4.6628575325012198,5.07232666015625,5.1433587074279803,5.4173622131347701,5.4097323417663601,5.3977632522582999,5.3867764472961399,5.3854241371154803,5.3919448852539098,5.3981180191040004,5.4056487083435103,5.4104261398315403,5.4168543815612802,5.4972262382507298,5.5698432922363299,5.6456804275512704,5.7250947952270499,5.8020553588867196,5.88106393814087,5.9598326683044398,6.0394186973571804,6.11779880523682,6.2010583877563503]
["   Natural Gas",5.1461992263793901,6.8558807373046902,7.3508062362670898,7.3840570449829102,6.7167382240295401,6.27575588226318,5.86295366287231,5.7038016319274902,5.5520119667053196,5.5432248115539604,5.5985813140869096,5.70459079742432,5.8318381309509304,5.9191007614135698,5.9519534111022896,5.8878293037414604,5.94315385818481,6.08443307876587,6.3156557083129901,6.4281539916992196,6.4433326721191397,6.4763746261596697,6.5396862030029297,6.6462817192077601]
["   Coal",1.2938040494918801,1.29924309253693,1.3041912317276001,1.3119194507598899,1.3187216520309399,1.3072546720504801,1.3059933185577399,1.2971544265747099,1.2836289405822801,1.2749706506729099,1.26953566074371,1.2652333974838299,1.2631930112838701,1.2626041173934901,1.26433837413788,1.26277422904968,1.2691743373870801,1.27585673332214,1.3034254312515301,1.3139834403991699,1.32844221591949,1.3343856334686299,1.3519768714904801,1.3668735027313199]
["   Ethanol (E85) 10/",14.6543264389038,16.232709884643601,19.6646022796631,19.716905593872099,20.910398483276399,20.088336944580099,20.034643173217798,19.876234054565401,19.0899848937988,19.0770473480225,18.9334907531738,18.8203315734863,18.8769016265869,18.733657836914102,18.836368560791001,18.717578887939499,18.677961349487301,18.768825531005898,18.702945709228501,19.039726257324201,19.213029861450199,19.429216384887699,19.537574768066399,19.6945476531982]
["   Electricity",21.599882125854499,21.735733032226602,21.731866836547901,21.659553527831999,20.918876647949201,20.055833816528299,19.596654891967798,19.579929351806602,19.517631530761701,19.486770629882798,19.702039718627901,19.955158233642599,20.317079544067401,20.442613601684599,20.578334808349599,20.580734252929702,20.7274265289307,20.953577041626001,21.262916564941399,21.454774856567401,21.4308891296387,21.3733520507813,21.452013015747099,21.5757865905762]
["","","","","","","","","","","","","","","","","","","","","","","","",""]
["Non-Renewable Energy Expenditures by Sector","","","","","","","","","","","","","","","","","","","","","","","",""]
["(billion 2003 dollars)","","","","","","","","","","","","","","","","","","","","","","","",""]
[" Residential",163.90481567382801,177.16523742675801,181.73590087890599,185.241622924805,180.05682373046901,176.427001953125,175.07618713378901,176.51165771484401,178.08059692382801,180.014236450195,183.85498046875,187.18310546875,191.43936157226599,194.37899780273401,197.52023315429699,198.76248168945301,201.94073486328099,206.017013549805,211.20541381835901,214.41099548339801,216.40347290039099,218.64796447753901,222.25126647949199,225.36584472656301]
[" Commercial",122.690147399902,128.153732299805,130.48612976074199,132.29133605957,129.27566528320301,126.887260437012,126.692184448242,129.41491699218801,131.90731811523401,135.04089355468801,139.741943359375,144.63902282714801,150.53921508789099,154.864669799805,159.25378417968801,162.59527587890599,167.29981994628901,172.854415893555,179.18412780761699,184.76553344726599,188.65592956543,192.56275939941401,197.80290222168,203.64804077148401]
[" Industrial",124.39901733398401,147.11244201660199,168.13270568847699,167.53501892089801,157.82022094726599,152.842697143555,151.28466796875,151.59564208984401,151.94683837890599,152.62234497070301,154.60144042968801,156.88139343261699,159.98997497558599,162.62356567382801,164.507247924805,166.59835815429699,170.382568359375,174.95167541503901,179.57080078125,184.12712097168,186.42012023925801,189.56260681152301,192.98284912109401,198.25885009765599]
[" Transportation",263.72879028320301,302.59255981445301,352.23825073242199,351.13717651367199,366.34793090820301,368.76159667968801,374.76626586914102,382.39471435546898,385.90115356445301,392.12625122070301,398.68222045898398,403.06192016601602,409.94515991210898,412.30630493164102,418.64147949218801,421.60382080078102,428.44393920898398,436.35858154296898,441.71078491210898,454.05059814453102,464.07431030273398,474.87463378906301,486.72909545898398,501.322265625]
["   Total Non-Renewable Expenditures",674.72277832031295,755.02398681640602,832.593017578125,836.20513916015602,833.50061035156295,824.91857910156295,827.8193359375,839.91693115234398,847.8359375,859.8037109375,876.880615234375,891.76544189453102,911.91369628906295,924.17352294921898,939.92272949218795,949.55993652343795,968.06707763671898,990.18170166015602,1011.67114257813,1037.35424804688,1055.55383300781,1075.64794921875,1099.76611328125,1128.59497070313]
["   Transportation Renewable Expenditures",1.1704622767865699E-2,1.72001253813505E-2,2.0739471539855E-2,2.2715086117386801E-2,2.5078095495700801E-2,2.8324941173195801E-2,3.1410280615091303E-2,3.5102743655443198E-2,3.9645586162805599E-2,4.3348435312509502E-2,4.6531450003385502E-2,4.9735426902771003E-2,5.3442426025867497E-2,5.6060969829559298E-2,6.0336232185363797E-2,6.3296250998973805E-2,6.6096656024455996E-2,6.9950148463249207E-2,7.2811737656593295E-2,7.6670221984386402E-2,8.0276548862457303E-2,8.4626309573650402E-2,8.8446177542209597E-2,9.2330038547515897E-2]
["   Total Expenditures",674.73449707031295,755.04119873046898,832.61376953125,836.22784423828102,833.52569580078102,824.94689941406295,827.85076904296898,839.95202636718795,847.87561035156295,859.84704589843795,876.92712402343795,891.815185546875,911.96716308593795,924.22961425781295,939.98309326171898,949.62322998046898,968.13317871093795,990.25164794921898,1011.74395751953,1037.43090820313,1055.63415527344,1075.73254394531,1099.85461425781,1128.68725585938]
["Biomass and Methanol data added from h2a_central_biomass_gasification_current_final.xls"]
["Woody Biomass",1.1960935989170374,1.1960935989170374,1.1960935989170374,1.1960935989170374,1.1960935989170374,1.1960935989170374,1.1960935989170374,1.1960935989170374,1.1960935989170374,1.198027460839296,1.2067298394894606,1.2415393540901181,1.244440146973506,1.2657126281183524,1.2686134210017406,1.2840843163798106,1.2792496615741635,1.3034229356023981,1.3217946238638563,1.3759427576871011,1.3943144459485595,1.4001160317153356,1.4242893057435699,1.4378263391993813,{"$f":"Y701+($AI$531-$Y$701)/10","v":1.5542937052794432}]
["Methanol",8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985,8.7353999999999985]
["Steam $(2005)/GJ",4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78,4.78]
["Steam $(2005)/mmBTU",{"$f":"B703*GJ_p_MMBtu","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"},{"$error":"#NAME?"}]
["Values for steam were copied from the H2A model version 1.  Biomass values were taken from the note at the bottom of this section."]
["   1/ Weighted average price includes fuels below as well as coal.",null,null,null,"","","","","","","","","","","","","","","","","","","","",""]
["   2/ This quantity is the weighted average for all petroleum products, not just those listed below."]
["   3/ Includes energy for combined heat and power plants, except those whose primary business is to sell electricity, or electricity and heat, to the public."]
["   4/ Excludes use for lease and plant fuel."]
["   5/ Diesel fuel containing 500 parts per million (ppm) or 15 ppm sulfur.  Price includes Federal and State taxes while excluding county and local taxes."]
["   6/ Kerosene-type jet fuel.  Price includes Federal and State taxes while excluding county and local taxes."]
["   7/ Sales weighted-average price for all grades. Includes Federal, State, and local taxes."]
["   8/ Includes Federal and State taxes while excluding county and local taxes."]
["   9/ Compressed natural gas used as a vehicle fuel.  Price includes estimated motor vehicle fuel taxes."]
["   10/ E85 refers to a blend of 85 percent ethanol (renewable) and 15 percent motor gasoline (nonrenewable).  To address cold starting issues, the percentage of ethanol actually"]
["varies seasonally.  The annual average ethanol content of 74 percent is used for this forecast."]
["   11/ Includes electricity-only and combined heat and power plants whose primary business is to sell electricity, or electricity and heat, to the public."]
["   12/ Weighted averages of end-use fuel prices are derived from the prices shown in each sector and the corresponding sectoral consumption."]
["   Btu = British thermal unit."]
["   Note:  Data for 2002 and 2003 are model results and may differ slightly from official EIA data reports."]
["   Sources:  2002 and 2003 prices for motor gasoline, distillate, and jet fuel are based on prices in the Energy Information Administration (EIA), Petroleum Marketing Annual"]
["2003, DOE/EIA-0487(2003) (Washington, DC, August 2004).  2002 residential and commercial natural gas delivered prices:  EIA, Natural Gas Annual 2002, DOE/EIA-0131(2002)"]
["(Washington, DC, January 2004).  2003 residential and commercial natural gas delivered prices:  EIA, Natural Gas Monthly, DOE/EIA-0130(2004/07) (Washington, DC, July 2004)."]
["2002 and 2003 electric power sector natural gas prices:  EIA, Electric Power Monthly, DOE/EIA-0226, May 2003 through April 2004, Table 4.11.A.  2002 and 2003 industrial natural"]
["gas delivered prices are estimated based on:  EIA, Manufacturing Energy Consumption Survey 1994 and industrial and wellhead prices from the Natural Gas Annual 2002,"]
["DOE/EIA-0131(2002) (Washington, DC, January 2004) and the Natural Gas Monthly, DOE/EIA-0130(2004/07) (Washington, DC, July 2004).  2002 transportation sector natural"]
["gas delivered prices are based on:  EIA, Natural Gas Annual 2002, DOE/EIA-0131(2002) (Washington, DC, January 2004) and estimated state and federal taxes.  2003"]
["transportation sector natural gas delivered prices are model results.  2002 and 2003 coal prices based on:  EIA, Quarterly Coal Report, October-December 2003,"]
["DOE/EIA-0121(2003/4Q) (Washington, DC, March 2004) and EIA, AEO2005 National Energy Modeling System run aeo2005.d102004a.  2002 and 2003 electricity prices:"]
["Annual Energy Review 2003, DOE/EIA-0384(2003) (Washington, DC, September 2004).  2002 and 2003 ethanol prices derived from weekly spot prices in the Oxy Fuel"]
["News.  Projections:  EIA, AEO2005 National Energy Modeling System run hw2005.d102004a."]
["* Biomass prices shown for years 2001 through 2009 are the same as the EIA value for 2010.  For the post-2025 biomass prices:  The value for 2035 was chosen based on a review of the literature, which indicated a price of $2.50/MMBtu delivered dry English ton (in 2000$) was a reasonable mid-range projection.  Values for the 2026 through 2034 were interpolated from the 2025 and 2035 values.  The value of $5.00/MMBtu delivered dry English ton in 2065 was based on judgment.  An EIA paper by Zia Haq entitled, “Biomass for Electricity Generation” (available from EIA’s website) indicates that about 7 quads of biomass per year  would be available if the price rose to  $5/MMBtu."]
["Note:  when steam is an important input or output, the price should be externally provided and should be based on the specific characteristics of the steam needed or produced. "]
[]
[]
["Table E.  Price Ratios from PNNL Mini-CAM Model"]
[null," Ratio 2050 to 2035 Price"," Ratio 2065 to 2050 Price","Extrapolated Ratio 2070 to 2065 Price","Ratio 2035 to 2020 Price"]
[]
[]
["Coal Delivered to Utilities",1.0439774739816527,1.0284486209328481,1.0094828736442827,{"$f":"F752/E752","v":1.0704312355553662}]
["Wellhead Gas",1.2097805877102306,1.1729343042703535,1.0576447680901178,1.1340871534488071]
["Gas Delivered to Utilities",1.1697889782905726,1.1485262991479412,1.049508766382647,1.1040561955262993]
["Crude Oil Price",1.1587647303602575,1.0854096786599328,1.0284698928866443,1.363594657351775]
["Delivered Diesel",1.1587647303602575,1.0854096786599328,1.0284698928866443,1.3635946573517748]
["Average Electricity",0.99410318905494366,1.0095287120834378,1.0031762373611459,0.97316968165904427]
["Dry Biomass at Farmgate",1.0099752422488564,1.0050974522479115,1.0016991507493038,0.99922998787640482]
["Ethanol",1.0099752422488564,1.0050974522479115,1.0016991507493038,0.99922998787640471]
[]
[null,null,null,null,"From MiniCAM"]
["In Units Consistent with EIA AEO",null,"From AEO","From AEO"]
[null,"Units",2000,2005,2020,2035,2050,2065,2080]
["Coal Delivered to Utilities","$/English ton",25.276500000000002,25.071000000000002,24.427484559,26.147942478000001,27.297862937999998,28.074449492999999,29.9967939]
["Wellhead Gas","$/mcf",3.83,2.88,3.1020351176470586,3.5179781764705877,4.2559817058823528,4.9919869411764699,5.7211905294117642]
["Gas Delivered to Utilities","$/mcf",4.333333333333333,3.2058823529411766,4.0727964705882354,4.4965961764705868,5.2600686470588229,6.0413271764705883,6.8262844117647052]
["Crude Oil Price","$/bbl",28.35,23.27,17.294973600000002,23.583333599999996,27.327535199999996,29.661571199999997]
["Delivered Diesel","$/gallon",1.5176666666666667,1.2925714285714285,0.93587519480519499,1.2761544155844153,1.4787627272727271,1.6050633766233764]
["Average Electricity","c/kWh",6.9,6.4,6.9130361604720001,6.7275571995839982,6.6878860666559987,6.7516130074319989,6.8294477356799987]
["Dry Biomass at Farmgate","$/mmBtu",null,null,3.8637053999999993,3.8607302999999993,3.8992420199999995,3.9191182199999997,4.4580291000000001]
["Ethanol","$/mmBtu",null,null,19.318526999999996,19.303651499999994,19.496210099999995,19.595591099999996,22.290145499999998]
[]
["Biomass delivered (assuming $10/English ton average delivery price)","$/English ton",null,null,76.455732879999985,76.404561159999986,77.066962743999994,77.40883338399999,86.678100520000001]
[null,17.2,"MMBtu/English ton"]
[]
["AEO 2009 High price case"]
["Report #:DOE/EIA-0383(2009)"]
["Release date: March 2009"]
["Next release date, early release: November 2009"]
[]
[" Table   3.  Energy Prices by Sector and Source"]
["                      (2007 dollars per million Btu, unless otherwise noted)"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2007-"]
[null,"2006","2007","2008","2009","2010","2011","2012","2013","2014","2015","2016","2017","2018","2019","2020","2021","2022","2023","2024","2025","2026","2027","2028","2029","2030","2030"]
[]
[]
[" Residential"]
["   Liquefied Petroleum Gases",23.883546829223601,24.976987838745099,28.3833827972412,22.3542995452881,27.926952362060501,30.764682769775401,33.661342620849602,36.453559875488303,39.494522094726598,41.980697631835902,43.916378021240199,45.360519409179702,46.395816802978501,47.017768859863303,47.646530151367202,48.008190155029297,48.261722564697301,48.628421783447301,48.848987579345703,49.201820373535199,49.638439178466797,49.873706817627003,50.123619079589801,50.456356048583999,50.7625923156738,3.13153266906738E-2]
["   Distillate Fuel Oil",18.464220046997099,19.6639919281006,23.795093536376999,18.337640762329102,20.694063186645501,23.041601181030298,25.2962837219238,27.2604274749756,30.121095657348601,32.154388427734403,33.5627632141113,34.602504730224602,35.554206848144503,36.023918151855497,36.510219573974602,36.482681274414098,36.622692108154297,37.053558349609403,37.097206115722699,37.402278900146499,37.843147277832003,38.237148284912102,38.632442474365199,38.983299255371101,39.194442749023402,3.0443191528320299E-2]
["   Natural Gas",13.7000589370728,12.691158294677701,13.015861511230501,11.686484336853001,12.3283596038818,12.249480247497599,12.273024559021,12.2969045639038,12.4211750030518,12.5907487869263,12.705096244811999,12.9095964431763,13.0879106521606,13.1304607391357,12.9131679534912,12.562335968017599,12.61110496521,12.871636390686,13.125649452209499,13.3413944244385,13.6169128417969,13.8638000488281,14.1467199325562,14.4200448989868,14.611619949340801,6.1453580856323199E-3]
["   Electricity",31.206779479980501,31.187788009643601,32.338191986083999,32.416282653808601,31.140913009643601,31.8760585784912,31.922065734863299,32.300529479980497,32.352581024169901,32.639389038085902,32.894443511962898,33.117340087890597,33.414459228515597,33.629150390625,33.777111053466797,33.604824066162102,33.664745330810497,34.025123596191399,34.538562774658203,35.105255126953097,35.529582977294901,35.8877983093262,36.209835052490199,36.388431549072301,36.494224548339801,6.8550109863281302E-3]
[]
[" Commercial"]
["   Liquefied Petroleum Gases",21.1974983215332,23.041419982910199,23.604557037353501,18.681890487670898,24.74609375,27.568971633911101,30.4514064788818,33.230876922607401,36.258987426757798,38.733001708984403,40.657176971435497,42.090251922607401,43.1152153015137,43.7275390625,44.347579956054702,44.701267242431598,44.947372436523402,45.307144165039098,45.5213012695313,45.867866516113303,46.298439025878899,46.528209686279297,46.772487640380902,47.099220275878899,47.399448394775398,3.1858563423156697E-2]
["   Distillate Fuel Oil",15.0199489593506,16.054103851318398,20.836805343627901,16.0582466125488,18.1372261047363,20.7669353485107,23.078548431396499,25.270603179931602,28.107904434204102,30.082014083862301,31.343215942382798,32.504638671875,33.3633842468262,33.805187225341797,34.229515075683601,34.103286743164098,34.2811889648438,34.681198120117202,34.715034484863303,35.0353393554688,35.459774017333999,35.835098266601598,36.246971130371101,36.616977691650398,36.9903373718262,3.6957502365112298E-2]
["   Residual Fuel",8.8815975189209002,10.2142028808594,13.357634544372599,6.7629709243774396,12.823133468627899,15.3392543792725,17.4722385406494,19.700599670410199,21.254331588745099,22.305961608886701,23.786525726318398,25.024957656860401,25.9401969909668,26.507759094238299,27.019905090331999,27.1827697753906,27.4323539733887,27.776666641235401,28.037864685058601,28.392919540405298,28.7309265136719,28.9971923828125,29.337739944458001,29.677482604980501,29.9862384796143,4.79378700256348E-2]
["   Natural Gas",11.896094322204601,10.9898433685303,11.522585868835399,10.173228263855,10.782675743103001,10.7339086532593,10.799374580383301,10.8246822357178,10.967120170593301,11.158206939697299,11.2802991867065,11.486307144165,11.6717615127563,11.7226161956787,11.525540351867701,11.1890621185303,11.2596950531006,11.5338354110718,11.800594329834,12.0026235580444,12.273542404174799,12.5177307128906,12.805614471435501,13.061990737915,13.243557929992701,8.1434249877929705E-3]
["   Electricity",28.3762531280518,28.073511123657202,29.5588493347168,29.575660705566399,27.526445388793899,27.8994140625,27.624683380126999,27.748167037963899,27.707677841186499,28.011663436889599,28.3554382324219,28.5976047515869,28.930782318115199,29.165691375732401,29.300102233886701,29.014184951782202,29.003173828125,29.329126358032202,29.795009613037099,30.299129486083999,30.6775302886963,31.039953231811499,31.389379501342798,31.541213989257798,31.7004203796387,5.2967071533203099E-3]
[]
[" Industrial 1/"]
["   Liquefied Petroleum Gases",21.0410861968994,23.3795356750488,25.519689559936499,18.770734786987301,23.917289733886701,26.7415580749512,29.674488067626999,32.454425811767599,35.485988616943402,37.9550170898438,39.876785278320298,41.308006286621101,42.332942962646499,42.9459419250488,43.565265655517599,43.919185638427699,44.164951324462898,44.525180816650398,44.739585876464801,45.087501525878899,45.519046783447301,45.747432708740199,45.991909027099602,46.318729400634801,46.6203422546387,3.0462384223937999E-2]
["   Distillate Fuel Oil",15.735449790954601,16.821935653686499,21.808429718017599,16.708997726440401,17.9886360168457,21.028125762939499,23.343002319335898,25.786291122436499,28.5029201507568,30.4483127593994,31.613187789916999,32.863849639892599,33.663894653320298,34.092327117919901,34.4815673828125,34.296230316162102,34.5044975280762,34.907333374023402,34.931465148925803,35.251617431640597,35.650547027587898,36.0166206359863,36.444431304931598,36.830661773681598,37.303695678710902,3.5232901573181201E-2]
["   Residual Fuel Oil",9.2125148773193395,10.494535446166999,13.694963455200201,6.9981408119201696,17.262666702270501,19.511152267456101,21.9067897796631,24.078254699706999,26.237388610839801,27.981674194335898,29.130001068115199,30.3923149108887,31.137657165527301,31.575212478637699,32.042640686035199,31.994066238403299,32.249111175537102,32.508918762207003,32.660282135009801,32.957084655761697,33.298637390136697,33.551937103271499,33.991706848144503,34.317066192627003,34.482418060302699,5.3082466125488302E-2]
["   Natural Gas 2/",7.9563031196594203,7.5151352882385298,8.9608917236328107,6.6214537620544398,7.1234536170959499,7.0705270767211896,7.1530704498290998,7.2213044166564897,7.3800201416015598,7.5896773338317898,7.6845889091491699,7.8647842407226598,8.0319690704345703,8.0643510818481392,7.8568081855773899,7.5151796340942401,7.5926008224487296,7.8076257705688503,8.0573301315307599,8.2859725952148402,8.5280551910400408,8.7343835830688494,8.9821290969848597,9.2285404205322301,9.4173421859741193,9.8584890365600603E-3]
["   Metallurgical Coal",3.6353600025177002,3.6099998950958301,4.0379996299743697,4.5020823478698704,4.3855228424072301,4.3762397766113299,4.3997368812561,4.4189567565918004,4.4347076416015598,4.4522905349731401,4.4603638648986799,4.4635276794433603,4.4729104042053196,4.4708456993103001,4.4873232841491699,4.5196957588195801,4.5735583305358896,4.6242790222168004,4.6478152275085396,4.6480631828308097,4.6606159210205096,4.6456594467163104,4.6185407638549796,4.56589651107788,4.4889969825744602,9.5199346542358398E-3]
["   Other Industrial Coal",2.4029979705810498,2.4299483299255402,2.5571811199188201,2.56162786483765,2.56748747825623,2.60902070999146,2.6235916614532502,2.6379292011261,2.6488504409789999,2.67559719085693,2.6456270217895499,2.6335513591766402,2.63612961769104,2.6347033977508501,2.63350534439087,2.6284878253936799,2.6334505081176802,2.6471104621887198,2.6563882827758798,2.6693737506866499,2.6800231933593799,2.6932156085968,2.7120738029479998,2.7318363189697301,2.7488965988159202,5.3765773773193403E-3]
["   Coal to Liquids","- -","- -",0,0,0,1.41293036937714,1.2184369564056401,1.17754483222961,1.3116322755813601,1.2733211517334,1.2851463556289699,1.28024590015411,1.30277991294861,1.29882299900055,1.29265284538269,1.32939457893372,1.3688597679138199,1.4024136066436801,1.4137438535690301,1.42857146263123,1.43632352352142,1.44281482696533,1.44536685943604,1.4501197338104199,1.4655066728591899,"- -"]
["   Electricity",18.411262512206999,18.634252548217798,20.706560134887699,20.639848709106399,18.9005832672119,18.9754123687744,18.748577117919901,18.7451286315918,18.622827529907202,18.823989868164102,19.081008911132798,19.220748901367202,19.446659088134801,19.608354568481399,19.6959743499756,19.505567550659201,19.549434661865199,19.802045822143601,20.232648849487301,20.693027496337901,21.023696899414102,21.339708328247099,21.629344940185501,21.733781814575199,21.762773513793899,6.7706108093261701E-3]
[]
[" Transportation"]
["   Liquefied Petroleum Gases 3/",22.2963676452637,25.0072422027588,28.459692001342798,22.469375610351602,27.7350177764893,30.574182510376001,33.472511291503899,36.259494781494098,39.291736602783203,41.768077850341797,43.697544097900398,45.127403259277301,46.152801513671903,46.761356353759801,47.381011962890597,47.734935760497997,47.977794647216797,48.333538055419901,48.545326232910199,48.889308929443402,49.317207336425803,49.543441772460902,49.784286499023402,50.108409881591797,50.406246185302699,3.0945181846618701E-2]
["   E85 4/",25.5142211914063,26.671012878418001,33.849239349365199,33.586345672607401,27.6864833831787,30.227962493896499,32.657257080078097,32.785953521728501,32.346141815185497,33.964523315429702,35.691123962402301,37.409137725830099,37.7480278015137,37.745933532714801,36.169681549072301,35.874843597412102,36.162742614746101,36.566848754882798,36.620006561279297,36.971061706542997,37.408500671386697,37.711296081542997,38.137138366699197,38.524795532226598,38.908096313476598,1.65539979934692E-2]
["   Motor Gasoline 5/",21.784559249877901,22.982162475585898,26.493778228759801,18.863723754882798,25.437911987304702,27.775495529174801,29.9758186340332,32.350837707519503,35.054023742675803,37.158294677734403,38.482601165771499,39.982501983642599,40.787757873535199,41.354404449462898,41.681800842285199,41.651054382324197,41.988578796386697,42.463710784912102,42.524349212646499,42.938045501708999,43.455722808837898,43.8155326843262,44.317115783691399,44.772129058837898,45.225753784179702,2.9869914054870599E-2]
["   Jet Fuel 6/",15.2446508407593,16.0964660644531,22.0368041992188,14.6258354187012,18.117679595947301,20.790958404541001,23.098089218139599,25.277437210083001,28.108070373535199,30.063097000122099,31.2007732391357,32.563095092773402,33.216217041015597,33.609565734863303,33.985622406005902,33.9229927062988,34.1160697937012,34.517745971679702,34.4479789733887,34.882648468017599,35.356975555419901,35.6980171203613,36.117191314697301,36.502471923828097,36.943180084228501,3.6781191825866699E-2]
["   Diesel Fuel (distillate fuel oil) 7/",20.2724208831787,20.921422958373999,27.137769699096701,19.170770645141602,22.028490066528299,24.713983535766602,27.011182785034201,29.495634078979499,32.183456420898402,34.083713531494098,35.161376953125,36.449062347412102,37.198707580566399,37.612049102783203,37.951786041259801,37.7472534179688,37.957847595214801,38.353157043457003,38.333263397216797,38.682945251464801,39.052806854247997,39.384151458740199,39.812137603759801,40.192409515380902,40.681694030761697,2.93352603912354E-2]
["   Residual Fuel Oil",8.20648097991943,9.3524312973022496,13.736819267272899,7.9047741889953604,13.998456954956101,16.239332199096701,18.616979598998999,20.834623336791999,23.251203536987301,25.300340652465799,26.520757675170898,27.721658706665,28.4222621917725,28.894708633422901,29.233545303344702,29.354173660278299,29.542749404907202,29.811567306518601,29.883472442626999,30.208297729492202,30.753358840942401,31.1088161468506,31.5337104797363,31.915937423706101,32.455944061279297,5.55877685546875E-2]
["   Natural Gas 8/",16.0437107086182,15.4583129882813,17.019536972045898,14.5970249176025,15.1249084472656,15.054651260376,15.074832916259799,15.052045822143601,15.142041206359901,15.2916584014893,15.3377676010132,15.4715919494629,15.583300590515099,15.570981025695801,15.303962707519499,14.909815788269,14.9584617614746,15.1840562820435,15.399169921875,15.568284988403301,15.7804002761841,15.981484413146999,16.220918655395501,16.434350967407202,16.567071914672901,3.0162334442138698E-3]
["   Electricity",30.389289855956999,30.640342712402301,34.162754058837898,33.815212249755902,30.533897399902301,30.904481887817401,30.761266708373999,30.656822204589801,30.208518981933601,30.091423034668001,30.193696975708001,30.0047798156738,29.991252899169901,30.379962921142599,30.558404922485401,30.327966690063501,30.564914703369102,31.263238906860401,32.143627166747997,32.985675811767599,33.582263946533203,34.167488098144503,34.703441619872997,34.847152709960902,34.984054565429702,5.7690143585205104E-3]
[]
[" Electric Power 9/"]
["   Distillate Fuel Oil",13.773189544677701,14.7723951339722,19.0520629882813,14.607873916626,17.083803176879901,19.3275451660156,21.593971252441399,23.5840148925781,26.404422760009801,28.420751571655298,29.800575256347699,30.8314094543457,31.78662109375,32.266555786132798,32.755008697509801,32.748939514160199,32.898239135742202,33.249435424804702,33.280975341796903,33.615665435791001,34.1393432617188,34.519859313964801,34.915023803710902,35.267223358154297,35.541374206542997,3.8909077644348103E-2]
["   Residual Fuel Oil",8.3781757354736293,8.3772602081298793,13.767860412597701,8.0074138641357404,15.1507024765015,17.445198059081999,19.8086948394775,22.028682708740199,24.317232131958001,26.1839485168457,27.423599243164102,28.603431701660199,29.3214435577393,29.774486541748001,30.1320896148682,30.226545333862301,30.416906356811499,30.663860321044901,30.799253463745099,31.115032196044901,31.5948371887207,31.898286819458001,32.294849395752003,32.6415824890137,33.036785125732401,6.1471939086914097E-2]
["   Natural Gas",7.0546379089355504,7.0191588401794398,9.1784105300903303,6.3232793807983398,6.7862815856933603,6.7554225921630904,6.8966388702392596,6.9007439613342303,7.0371451377868697,7.2394108772277797,7.3461008071899396,7.5131673812866202,7.6775636672973597,7.7008471488952601,7.47206687927246,7.1458010673522896,7.2566452026367196,7.4941387176513699,7.74432277679443,7.9791569709777797,8.1962327957153303,8.3967161178588903,8.6154594421386701,8.8489608764648402,9.0075101852416992,1.09031200408936E-2]
["   Steam Coal",1.7355251312255899,1.78000032901764,1.9430780410766599,1.9159911870956401,1.9215773344039899,1.94381320476532,1.96493256092072,1.9859246015548699,2.01386618614197,2.0425341129303001,2.0265669822692902,2.0264971256256099,2.0284991264343302,2.03088283538818,2.0331871509552002,2.0308041572570801,2.03707003593445,2.0511178970336901,2.0604875087738002,2.07539582252502,2.08802461624146,2.09706377983093,2.11007905006409,2.1255011558532702,2.14128541946411,8.0668926239013707E-3]
[]
[" Average Price to All Users 10/"]
["   Liquefied Petroleum Gases",15.6574239730835,18.532711029052699,19.588813781738299,17.695808410644499,22.89772605896,25.525800704956101,28.135374069213899,30.695905685424801,33.5143013000488,35.840816497802699,37.6836967468262,39.047306060791001,40.043754577636697,40.646400451660199,41.227584838867202,41.557403564453097,41.8039360046387,42.135208129882798,42.369644165039098,42.704635620117202,43.125633239746101,43.351551055908203,43.615390777587898,43.933467864990199,44.235824584960902,3.8550496101379401E-2]
["   E85 4/",25.5142211914063,26.671012878418001,33.849239349365199,33.586345672607401,27.6864833831787,30.227962493896499,32.657257080078097,32.785953521728501,32.346141815185497,33.964523315429702,35.691123962402301,37.409137725830099,37.7480278015137,37.745933532714801,36.169681549072301,35.874843597412102,36.162742614746101,36.566848754882798,36.620006561279297,36.971061706542997,37.408500671386697,37.711296081542997,38.137138366699197,38.524795532226598,38.908096313476598,1.65539979934692E-2]
["   Motor Gasoline 5/",21.648998260498001,22.819190979003899,26.322273254394499,18.9177551269531,25.436496734619102,27.772588729858398,29.973018646240199,32.347999572753899,35.050952911377003,37.155685424804702,38.4801635742188,39.979705810546903,40.785068511962898,41.3517036437988,41.679214477539098,41.648273468017599,41.985744476318402,42.461280822753899,42.522396087646499,42.935802459716797,43.453563690185497,43.8141899108887,44.316211700439503,44.771690368652301,45.225814819335902,3.0188679695129401E-2]
["   Jet Fuel",15.2446508407593,16.0964660644531,22.0368041992188,14.6258354187012,18.117679595947301,20.790958404541001,23.098089218139599,25.277437210083001,28.108070373535199,30.063097000122099,31.2007732391357,32.563095092773402,33.216217041015597,33.609565734863303,33.985622406005902,33.9229927062988,34.1160697937012,34.517745971679702,34.4479789733887,34.882648468017599,35.356975555419901,35.6980171203613,36.117191314697301,36.502471923828097,36.943180084228501,3.6781191825866699E-2]
["   Distillate Fuel Oil",19.1713962554932,19.9431247711182,25.703296661376999,18.5521545410156,20.9619140625,23.6791477203369,26.0628471374512,28.599927902221701,31.3183403015137,33.263851165771499,34.408931732177699,35.652828216552699,36.441574096679702,36.859718322753899,37.242115020752003,37.054904937744098,37.2623291015625,37.674507141113303,37.684783935546903,38.020187377929702,38.413318634033203,38.774890899658203,39.204498291015597,39.593456268310497,40.074676513671903,3.0806779861450199E-2]
["   Residual Fuel Oil",8.4246597290039098,9.2489309310913104,13.7205715179443,7.74660301208496,14.567358970642101,16.791095733642599,19.158735275268601,21.380689620971701,23.7013645172119,25.618089675903299,26.856208801269499,28.053350448608398,28.769941329956101,29.23703956604,29.5975856781006,29.6960258483887,29.894676208496101,30.160924911498999,30.265388488769499,30.587467193603501,31.0885925292969,31.417993545532202,31.8338527679443,32.200790405273402,32.660762786865199,5.6387543678283698E-2]
["   Natural Gas",9.5026035308837908,9.0057582855224592,10.3350286483765,8.2461471557617205,8.7815446853637695,8.7498798370361293,8.8216104507446307,8.8623371124267596,9.0222139358520508,9.1982822418212908,9.3107128143310494,9.4842357635497994,9.6566028594970703,9.6935338973999006,9.4843921661377006,9.1274719238281303,9.1924381256103498,9.4196281433105504,9.6638069152831996,9.8748388290405291,10.1317024230957,10.353573799133301,10.619698524475099,10.875740051269499,11.0649738311768,8.99326801300049E-3]
["   Metallurgical Coal",3.6353600025177002,3.6099998950958301,4.0379996299743697,4.5020823478698704,4.3855228424072301,4.3762397766113299,4.3997368812561,4.4189567565918004,4.4347076416015598,4.4522905349731401,4.4603638648986799,4.4635276794433603,4.4729104042053196,4.4708456993103001,4.4873232841491699,4.5196957588195801,4.5735583305358896,4.6242790222168004,4.6478152275085396,4.6480631828308097,4.6606159210205096,4.6456594467163104,4.6185407638549796,4.56589651107788,4.4889969825744602,9.5199346542358398E-3]
["   Other Coal",1.77764248847961,1.81885325908661,1.9807318449020399,1.95691537857056,1.96047616004944,1.9828474521637001,2.0030708312988299,2.0230474472045898,2.04939866065979,2.0778627395629901,2.0609514713287398,2.0600180625915501,2.0618624687194802,2.0638909339904798,2.06605005264282,2.0636281967163099,2.0698127746582,2.0836849212646502,2.0928261280059801,2.1075301170349099,2.11965775489807,2.12851786613464,2.1413710117340101,2.1563785076141402,2.1716537475585902,7.7377557754516602E-3]
["   Coal to Liquids","- -","- -",0,0,0,1.41293036937714,1.2184369564056401,1.17754483222961,1.3116322755813601,1.2733211517334,1.2851463556289699,1.28024590015411,1.30277991294861,1.29882299900055,1.29265284538269,1.32939457893372,1.3688597679138199,1.4024136066436801,1.4137438535690301,1.42857146263123,1.43632352352142,1.44281482696533,1.44536685943604,1.4501197338104199,1.4655066728591899,"- -"]
["   Electricity",26.6758422851563,26.701194763183601,28.207727432251001,28.274074554443398,26.651882171630898,27.076250076293899,26.8856010437012,27.034772872924801,27.029661178588899,27.3082084655762,27.613113403320298,27.833410263061499,28.1487426757813,28.391799926757798,28.5583095550537,28.353569030761701,28.399204254150401,28.738731384277301,29.230339050293001,29.757205963134801,30.155431747436499,30.516889572143601,30.855388641357401,31.007261276245099,31.1231689453125,6.6850185394287101E-3]
[]
["Non-Renewable Energy Expenditures by Sector"]
["(billion 2007 dollars)"]
[" Residential",231.08920288085901,238.37773132324199,252.94381713867199,239.17680358886699,239.69950866699199,245.75201416015599,249.44010925293,251.653884887695,255.77357482910199,260.52627563476602,265.15460205078102,269.22512817382801,274.38430786132801,278.28405761718801,280.47280883789102,279.25845336914102,282.19268798828102,287.70663452148398,294.26138305664102,299.7646484375,305.77548217773398,311.16711425781301,317.20748901367199,320.85021972656301,324.46701049804699,1.34958028793335E-2]
[" Commercial",170.28286743164099,173.08578491210901,185.76397705078099,178.33143615722699,175.53163146972699,180.70600891113301,182.55152893066401,186.30380249023401,190.25302124023401,195.77976989746099,200.96725463867199,206.10406494140599,211.46237182617199,215.83396911621099,218.91777038574199,219.36863708496099,222.59973144531301,228.27235412597699,234.30972290039099,240.46255493164099,246.24565124511699,251.95404052734401,257.89071655273398,262.67080688476602,267.35046386718801,1.9083023071289101E-2]
[" Industrial",216.12767028808599,226.84164428710901,256.28231811523398,205.24591064453099,215.22320556640599,231.62438964843801,251.65115356445301,268.80010986328102,283.12625122070301,295.85977172851602,303.21740722656301,310.33920288085898,314.45690917968801,315.63778686523398,314.44158935546898,311.38638305664102,313.677490234375,317.87069702148398,322.22720336914102,327.49166870117199,332.22317504882801,336.22024536132801,341.05575561523398,345.55453491210898,349.17462158203102,1.8929958343505901E-2]
[" Transportation",564.63043212890602,596.754638671875,694.30163574218795,484.89761352539102,634.28308105468795,713.26568603515602,779.22229003906295,844.09631347656295,905.84466552734398,934.9755859375,954.39727783203102,974.517578125,987.50305175781295,994.324462890625,995.15118408203102,988.80041503906295,994.07275390625,1004.81390380859,1007.67785644531,1021.18786621094,1038.30029296875,1054.15161132813,1073.83544921875,1093.56530761719,1116.07727050781,2.7594208717346198E-2]
["   Total Non-Renewable Expenditures",1182.13012695313,1235.05981445313,1389.29174804688,1107.65173339844,1264.73742675781,1371.34814453125,1462.86511230469,1550.85412597656,1634.99755859375,1687.14135742188,1723.73657226563,1760.18603515625,1787.806640625,1804.08032226563,1808.9833984375,1798.81384277344,1812.54272460938,1838.66357421875,1858.47619628906,1888.90673828125,1922.54455566406,1953.49304199219,1989.98937988281,2022.64086914063,2057.0693359375,2.2428870201110802E-2]
[" Transportation Renewable Expenditures",3.2134380191564602E-2,4.0766973048448597E-2,3.9758257567882503E-2,2.0912932232022299E-2,6.9471828639507294E-2,8.6778029799461406E-2,0.106363005936146,0.55913984775543202,7.9643964767456099,27.973939895629901,38.499557495117202,49.285560607910199,55.498867034912102,59.983543395996101,63.057430267333999,67.662658691406307,73.058197021484403,78.445304870605497,82.808517456054702,87.534194946289105,92.150848388671903,96.100090026855497,99.981544494628906,103.37892150878901,106.394973754883,0.407824020385742]
["   Total Expenditures",1182.16223144531,1235.1005859375,1389.33154296875,1107.67260742188,1264.80688476563,1371.43493652344,1462.97143554688,1551.41320800781,1642.9619140625,1715.11535644531,1762.23608398438,1809.47155761719,1843.30554199219,1864.06384277344,1872.04077148438,1866.4765625,1885.60095214844,1917.10888671875,1941.28466796875,1976.44091796875,2014.69543457031,2049.59301757813,2089.97094726563,2126.01977539063,2163.46435546875,2.4671554565429701E-2]
[]
[]
["Prices in Nominal Dollars"]
[" Residential"]
["   Liquefied Petroleum Gases",23.257051467895501,24.976987838745099,29.065778732299801,23.2960910797119,29.4280681610107,32.889183044433601,36.6288871765137,40.505104064941399,44.8352661132813,48.719963073730497,52.086635589599602,54.978519439697301,57.4362182617188,59.445770263671903,61.391433715820298,62.804817199707003,63.970870971679702,65.233825683593807,66.208908081054702,67.332000732421903,68.596176147460895,69.652244567871094,70.7481689453125,71.979537963867202,73.22802734375,4.7877073287963902E-2]
["   Distillate Fuel Oil",17.9798793792725,19.6639919281006,24.3671779632568,19.1102085113525,21.806400299072301,24.6327724456787,27.526374816894499,30.2902221679688,34.194293975830099,37.316211700439503,39.8068237304688,41.9394340515137,44.014728546142599,45.545963287353501,47.042560577392599,47.727027893066399,48.543346405029297,49.706432342529297,50.280788421630902,51.184494018554702,52.296066284179702,53.400947570800803,54.528671264648402,55.612415313720703,56.540290832519503,4.6990871429443401E-2]
["   Natural Gas",13.3406887054443,12.691158294677701,13.3287906646729,12.1788377761841,12.9910278320313,13.095386505126999,13.3549995422363,13.6636142730713,14.100858688354499,14.6119728088379,15.068768501281699,15.646878242492701,16.202325820922901,16.6011772155762,16.638313293456999,16.434179306030298,16.716007232666001,17.266981124877901,17.790235519409201,18.257511138916001,18.8174343109131,19.361801147460898,19.9677219390869,20.5712070465088,21.078121185302699,2.2302865982055699E-2]
["   Electricity",30.388185501098601,31.187788009643601,33.115669250488303,33.781986236572301,32.814785003662102,34.077308654785199,34.736278533935497,35.890495300292997,36.7275390625,37.879070281982401,39.014167785644503,40.139362335205099,41.365802764892599,42.518196105957003,43.5210151672363,43.962184906005902,44.622589111328097,45.6438598632813,46.812854766845703,48.041049957275398,49.098915100097699,50.119911193847699,51.109226226806598,51.910655975341797,52.645065307617202,2.3023962974548302E-2]
[]
[" Commercial"]
["   Liquefied Petroleum Gases",20.6414604187012,23.041419982910199,24.172060012817401,19.4689617156982,26.076234817504901,29.4727878570557,33.1359672546387,36.924243927002003,41.162197113037102,44.950904846191399,48.2210884094238,51.014842987060497,53.374961853027301,55.285846710205099,57.140815734863303,58.478668212890597,59.577701568603501,60.778411865234403,61.698631286621101,62.76953125,63.9805717468262,64.980018615722699,66.018135070800795,67.190345764160199,68.376495361328097,4.8429012298583998E-2]
["   Distillate Fuel Oil",14.6259565353394,16.054103851318398,21.337766647338899,16.734783172607401,19.112129211425799,22.201026916503899,25.113124847412099,28.0792446136475,31.9088649749756,34.911155700683601,37.174346923828097,39.3967475891113,41.302574157714801,42.740764617919901,44.103927612304702,44.6142768859863,45.439685821533203,46.523967742919901,47.052040100097699,47.945369720458999,49.002445220947301,50.046310424804702,51.161643981933601,52.236690521240199,53.3607368469238,5.3609848022460903E-2]
["   Residual Fuel",8.64862155914307,10.2142028808594,13.678780555725099,7.0478959083557102,13.512396812439,16.3985290527344,19.012569427490199,21.890174865722699,24.128501892089801,25.886793136596701,28.2118015289307,30.3311157226563,32.112957000732401,33.514438629150398,34.8145141601563,35.560783386230497,36.361560821533203,37.261711120605497,38.001945495605497,38.855312347412102,39.703739166259801,40.496681213378899,41.409446716308601,42.337013244628899,43.256912231445298,6.4766526222229004E-2]
["   Natural Gas",11.5840444564819,10.9898433685303,11.799612998962401,10.6018285751343,11.362260818481399,11.475154876709,11.7514343261719,12.0277652740479,12.4501762390137,12.9494619369507,13.3789005279541,13.921801567077599,14.449187278747599,14.8212032318115,14.8503885269165,14.6376485824585,14.924715995788601,15.472354888916,15.9942817687988,16.425422668456999,16.961009979248001,17.481918334960898,18.074787139892599,18.633848190307599,19.104610443115199,2.43330001831055E-2]
["   Electricity",27.631908416748001,28.073511123657202,30.269506454467798,30.8216876983643,29.006034851074201,29.8260498046875,30.060043334960898,30.832170486450199,31.454517364501999,32.508445739746101,33.630722045898402,34.661285400390597,35.815185546875,36.874931335449197,37.752494812011697,37.956661224365199,38.443679809570298,39.3442993164063,40.383541107177699,41.463935852050803,42.393783569335902,43.349544525146499,44.305282592773402,44.995758056640597,45.729721069335902,2.1440625190734901E-2]
[]
[" Industrial 1/"]
["   Liquefied Petroleum Gases",20.489151000976602,23.3795356750488,26.133235931396499,19.561550140380898,25.202880859375,28.5882358551025,32.290554046630902,36.061496734619098,40.28466796875,44.048030853271499,47.2955131530762,50.066734313964801,52.406539916992202,54.297653198242202,56.132820129394503,57.455539703369098,58.540603637695298,59.729427337646499,60.639110565185497,61.701614379882798,62.903518676757798,63.889602661132798,64.916366577148395,66.076919555664105,67.252586364746094,4.7010421752929701E-2]
["   Distillate Fuel Oil",15.3226890563965,16.821935653686499,22.332750320434599,17.412950515747099,18.955553054809599,22.4802551269531,25.400894165039102,28.652246475219702,32.3572998046875,35.336254119872997,37.494544982910199,39.832122802734403,41.674594879150398,43.103801727294901,44.428688049316399,44.866687774658203,45.735679626464801,46.827323913574197,47.345386505127003,48.241344451904297,49.266075134277301,50.299819946289098,51.440353393554702,52.541526794433601,53.812774658203097,5.1857590675353997E-2]
["   Residual Fuel Oil",8.9708585739135707,10.494535446166999,14.024219512939499,7.2929735183715803,18.1905612945557,20.858524322509801,23.838066101074201,26.7543754577637,29.785404205322301,32.473640441894503,34.549385070800803,36.836536407470703,38.547210693359403,39.921348571777301,41.286190032958999,41.854972839355497,42.746166229247997,43.609909057617202,44.267074584960902,45.101306915283203,46.015933990478501,46.857711791992202,47.978397369384801,48.9557075500488,49.742916107177699,6.9993734359741197E-2]
["   Natural Gas 2/",7.7475991249084499,7.5151352882385298,9.17633056640625,6.9004168510437003,7.5063500404357901,7.5587930679321298,7.7836766242981001,8.0238990783691406,8.3780012130737305,8.8080673217773402,9.1142396926879901,9.5323905944824201,9.9432659149169904,10.195965766906699,10.1233129501343,9.8314371109008807,10.063985824585,10.473736763000501,10.920739173889199,11.339237213134799,11.7850589752197,12.198199272155801,12.6780385971069,13.1651611328125,13.585069656372101,2.6075601577758799E-2]
["   Metallurgical Coal",3.53999996185303,3.6099998950958301,4.1350817680358896,4.6917557716369602,4.6212515830993697,4.6784477233886701,4.7876124382018999,4.9100909233093297,5.03440189361572,5.1670279502868697,5.2901754379272496,5.4099502563476598,5.5372896194457999,5.6526045799255398,5.7818107604980504,5.9127135276794398,6.0622472763061497,6.2033557891845703,6.2995529174804696,6.3608093261718803,6.4405817985534703,6.4879999160766602,6.5189485549926802,6.51357221603394,6.4756422042846697,2.57315635681152E-2]
["   Other Industrial Coal",2.3399641513824498,2.4299483299255402,2.6186611652374299,2.6695497035980198,2.70549392700195,2.7891905307769802,2.8548843860626198,2.9311156272888201,3.00704789161682,3.1051175594329798,3.1378228664398198,3.19195532798767,3.2634260654449498,3.3311228752136199,3.39320969581604,3.4386153221130402,3.4906363487243701,3.5510332584381099,3.60041379928589,3.6530005931854199,3.7035679817199698,3.7612707614898699,3.82802057266235,3.89715647697449,3.9654450416564901,2.1521687507629401E-2]
["   Coal to Liquids","- -","- -",0,0,0,1.5105023384094201,1.3258528709411599,1.3084201812744101,1.4890010356903101,1.4777305126190201,1.52423667907715,1.55170238018036,1.6127909421920801,1.64213514328003,1.6655528545379601,1.7391279935836801,1.8144223690032999,1.881303191185,1.91615927219391,1.9549800157546999,1.98487901687622,2.0149953365325901,2.0400972366332999,2.06869769096375,2.1140794754028298,"- -"]
["   Electricity",17.9283123016357,18.634252548217798,21.204389572143601,21.5094089508057,19.916519165039102,20.2857875823975,20.401430130004901,20.8285102844238,21.1411457061768,21.845851898193398,22.630865097045898,23.2962131500244,24.0742092132568,24.791343688964801,25.377799987793001,25.517387390136701,25.912757873535199,26.5639553070068,27.422914505004901,28.318119049072301,29.052991867065401,29.802448272705099,30.529249191284201,31.004766464233398,31.394081115722699,2.29382514953613E-2]
[]
[" Transportation"]
["   Liquefied Petroleum Gases 3/",21.711505889892599,25.0072422027588,29.143922805786101,23.416013717651399,29.225816726684599,32.6855278015137,36.423408508300803,40.289470672607401,44.605060577392599,48.473209381103501,51.827091217041001,54.695976257324197,57.1353759765625,59.121578216552699,61.049320220947301,62.447345733642599,63.594524383544901,64.838249206542997,65.797332763671903,66.904335021972699,68.152259826660199,69.191001892089801,70.269203186035199,71.483169555664105,72.713973999023395,4.7500967979431201E-2]
["   E85 4/",24.84494972229,26.671012878418001,34.663047790527301,35.0013427734375,29.174674987793001,32.315399169921903,35.536281585693402,36.4298706054688,36.720230102539098,39.4169311523438,42.331146240234403,45.341171264648402,46.730594635009801,47.723148345947301,46.603786468505902,46.931846618652301,47.933681488037102,49.053524017333999,49.634002685546903,50.5943794250488,51.695419311523402,52.666557312011697,53.829563140869098,54.958328247070298,56.1272163391113,3.2878637313842801E-2]
["   Motor Gasoline 5/",21.213121414184599,22.982162475585898,27.130744934081999,19.658454895019499,26.805238723754901,29.6935729980469,32.618450164794901,35.946395874023402,39.7942924499512,43.123409271240199,45.641952514648402,48.460178375244098,50.493659973144503,52.285430908203097,53.706020355224602,54.488346099853501,55.6558227539063,56.964015960693402,57.636627197265597,58.7601127624512,60.052177429199197,61.191566467285199,62.552440643310497,63.8705863952637,65.240806579589801,4.6408414840698201E-2]
["   Jet Fuel 6/",14.844763755798301,16.0964660644531,22.566616058349599,15.2420244216919,19.09153175354,22.226709365844702,25.1343898773193,28.086837768554702,31.909053802490199,34.889202117919901,37.005405426025398,39.467597961425803,41.120388031005902,42.493434906005902,43.789676666259801,44.378414154052699,45.220821380615199,46.304702758789098,46.690078735351598,47.736415863037102,48.860385894775398,49.854866027832003,50.978462219238303,52.073341369628899,53.292709350585902,5.3430676460266099E-2]
["   Diesel Fuel (distillate fuel oil) 7/",19.740650177001999,20.921422958373999,27.790218353271499,19.978439331054702,23.2125549316406,26.4206447601318,29.3924560546875,32.773857116699197,36.535545349121101,39.555255889892599,41.702842712402301,44.177524566650398,46.0505561828613,47.553874969482401,48.899986267089801,49.381351470947301,50.3130912780762,51.4498100280762,51.9561157226563,52.937068939208999,53.967716217041001,55.002819061279297,56.193782806396499,57.337295532226598,58.685737609863303,4.5865178108215297E-2]
["   Residual Fuel Oil",7.9912142753601101,9.3524312973022496,14.067081451416,8.2378034591674805,14.7508955001831,17.360763549804702,20.2582302093506,23.1502380371094,26.3954048156738,29.3618679046631,31.454713821411101,33.599609375,35.185657501220703,36.532318115234403,37.666736602783203,38.401439666747997,39.158885955810497,39.991481781005902,40.503440856933601,41.339633941650398,42.498569488525398,43.445716857910199,44.508998870849602,45.530326843261697,46.819606781005902,7.2539210319519001E-2]
["   Natural Gas 8/",15.6228637695313,15.4583129882813,17.4287223815918,15.2119998931885,15.9378957748413,16.094272613525401,16.403812408447301,16.724969863891602,17.189661026001001,17.746465682983398,18.191225051879901,18.7521057128906,19.291521072387699,19.686790466308601,19.718795776367202,19.5051784515381,19.827426910400401,20.369035720825199,20.871717453002901,21.304979324340799,21.807193756103501,22.319299697876001,22.895399093627901,23.444755554199201,23.898975372314499,1.91235542297363E-2]
["   Electricity",29.592140197753899,30.640342712402301,34.984100341796903,35.239852905273402,32.175140380859403,33.0386352539063,33.47314453125,34.064102172851598,34.293540954589801,34.922073364257798,35.810970306396499,36.366832733154297,37.128005981445298,38.410163879394503,39.373786926269503,39.675365447997997,40.513767242431598,41.9388618469238,43.566810607910199,45.140434265136697,46.407882690429702,47.717372894287102,48.982990264892599,49.711910247802699,50.466556549072301,2.1920561790466302E-2]
[]
[" Electric Power 9/"]
["   Distillate Fuel Oil",13.411901473999,14.7723951339722,19.510114669799801,15.2233066558838,18.0020847320557,20.662237167358398,23.4976692199707,26.205204010009801,29.975025177001999,32.983203887939503,35.344711303710902,37.368736267089801,39.350601196289098,40.795433044433601,42.204059600830099,42.842506408691399,43.6065864562988,44.603294372558601,45.108348846435497,46.002567291259801,47.177719116210902,48.209484100341797,49.2816352844238,50.311172485351598,51.270523071289098,5.5592775344848598E-2]
["   Residual Fuel Oil",8.1584053039550799,8.3772602081298793,14.098869323730501,8.3447675704956108,15.9650764465332,18.64990234375,21.555006027221701,24.477008819580099,27.6055908203125,30.387323379516602,32.525520324707003,34.668350219726598,36.2988090515137,37.644645690917997,38.824489593505902,39.542682647705099,40.317581176757798,41.134811401367202,41.744674682617202,42.580486297607401,43.661422729492202,44.548267364502003,45.583328247070298,46.565509796142599,47.657505035400398,7.8517913818359403E-2]
["   Natural Gas",6.8695855140686,7.0191588401794398,9.3990793228149396,6.5896801948547399,7.1510548591613796,7.2219285964965803,7.50463819503784,7.6677107810974103,7.9887604713439897,8.4015712738037092,8.7127790451049805,9.1062192916870099,9.5045261383056605,9.7363777160644496,9.6275825500488299,9.3482122421264595,9.6186761856079102,10.053201675415,10.4964952468872,10.919364929199199,11.3265085220337,11.7266225814819,12.160493850708001,12.623664855956999,12.993863105773899,2.71370410919189E-2]
["   Steam Coal",1.6900000572204601,1.78000032901764,1.9897937774658201,1.9967122077941899,2.0248651504516602,2.07804608345032,2.1381585597991899,2.2066454887390101,2.2861962318420401,2.3704271316528298,2.4035921096801802,2.4561846256256099,2.5112030506134002,2.5676970481872599,2.6197137832641602,2.6567192077636701,2.70013451576233,2.7515239715576199,2.79274225234985,2.8401501178741499,2.8854753971099898,2.9287014007568399,2.97832083702087,3.03217673301697,3.0889301300048801,2.4255156517028802E-2]
[]
[" Average Price to All Users 10/"]
["   Liquefied Petroleum Gases",15.2467098236084,18.532711029052699,20.059770584106399,18.4413356781006,24.128513336181602,27.2885227203369,30.6157550811768,34.107528686523402,38.046356201171903,41.594432830810497,44.694419860839801,47.326686859130902,49.5726127624512,51.390285491943402,53.120773315429702,54.365833282470703,55.411079406738303,56.523338317871101,57.4269409179688,58.440696716308601,59.596019744872997,60.543582916259801,61.561973571777301,62.674179077148402,63.812778472900398,5.5228352546691901E-2]
["   E85 4/",24.84494972229,26.671012878418001,34.663047790527301,35.0013427734375,29.174674987793001,32.315399169921903,35.536281585693402,36.4298706054688,36.720230102539098,39.4169311523438,42.331146240234403,45.341171264648402,46.730594635009801,47.723148345947301,46.603786468505902,46.931846618652301,47.933681488037102,49.053524017333999,49.634002685546903,50.5943794250488,51.695419311523402,52.666557312011697,53.829563140869098,54.958328247070298,56.1272163391113,3.2878637313842801E-2]
["   Motor Gasoline 5/",21.081117630004901,22.819190979003899,26.955116271972699,19.714763641357401,26.803747177123999,29.690465927123999,32.615406036377003,35.943241119384801,39.790805816650398,43.1203804016113,45.639060974121101,48.456787109375,50.490329742431598,52.282016754150398,53.702690124511697,54.484706878662102,55.652065277099602,56.960758209228501,57.633979797363303,58.757045745849602,60.0491943359375,61.189689636230497,62.551162719726598,63.869960784912102,65.240898132324205,4.6732306480407701E-2]
["   Jet Fuel",14.844763755798301,16.0964660644531,22.566616058349599,15.2420244216919,19.09153175354,22.226709365844702,25.1343898773193,28.086837768554702,31.909053802490199,34.889202117919901,37.005405426025398,39.467597961425803,41.120388031005902,42.493434906005902,43.789676666259801,44.378414154052699,45.220821380615199,46.304702758789098,46.690078735351598,47.736415863037102,48.860385894775398,49.854866027832003,50.978462219238303,52.073341369628899,53.292709350585902,5.3430676460266099E-2]
["   Distillate Fuel Oil",18.668506622314499,19.9431247711182,26.3212585449219,19.3337593078613,22.088649749755898,25.314346313476602,28.360517501831101,31.778598785400401,35.553440093994098,38.6037788391113,40.810413360595703,43.2124633789063,45.113254547119098,46.602684020996101,47.985591888427699,48.475616455078097,49.391181945800803,50.539421081542997,51.077178955078097,52.030094146728501,53.083995819091797,54.151943206787102,55.336112976074197,56.4828491210938,57.8100776672363,4.7360301017761203E-2]
["   Residual Fuel Oil",8.2036705017089808,9.2489309310913104,14.050442695617701,8.0729684829711896,15.3503770828247,17.950630187988299,20.8477458953857,23.756994247436499,26.906440734863299,29.730625152587901,31.8525714874268,34.001632690429702,35.6160697937012,36.965137481689503,38.135795593261697,38.8486518859863,39.6253662109375,40.460136413574197,41.021083831787102,41.8585205078125,42.961837768554702,43.8775024414063,44.932643890380902,45.936691284179702,47.115070343017599,7.3351860046386705E-2]
["   Natural Gas",9.2533378601074201,9.0057582855224592,10.5835046768188,8.5935592651367205,9.2535657882690394,9.3541154861450195,9.5993127822875994,9.8473205566406303,10.2422647476196,10.6749057769775,11.042889595031699,11.495222091674799,11.954499244689901,12.2557830810547,12.220417022705099,11.9406547546387,12.184568405151399,12.6361980438232,13.0981245040894,13.513578414916999,14.0011653900146,14.459515571594199,14.989423751831101,15.515007019043001,15.961875915527299,2.51965522766113E-2]
["   Metallurgical Coal",3.53999996185303,3.6099998950958301,4.1350817680358896,4.6917557716369602,4.6212515830993697,4.6784477233886701,4.7876124382018999,4.9100909233093297,5.03440189361572,5.1670279502868697,5.2901754379272496,5.4099502563476598,5.5372896194457999,5.6526045799255398,5.7818107604980504,5.9127135276794398,6.0622472763061497,6.2033557891845703,6.2995529174804696,6.3608093261718803,6.4405817985534703,6.4879999160766602,6.5189485549926802,6.51357221603394,6.4756422042846697,2.57315635681152E-2]
["   Other Coal",1.73101270198822,1.81885325908661,2.02835273742676,2.0393605232238801,2.0658547878265399,2.1197760105133101,2.17965912818909,2.2478942871093799,2.3265335559845002,2.41142725944519,2.4443736076354998,2.4968132972717298,2.5525057315826398,2.6094300746917698,2.6620569229125999,2.6996600627899201,2.7435350418090798,2.7952117919921902,2.8365733623504599,2.8841254711151101,2.9291899204254199,2.9726293087005602,3.0224885940551802,3.0762255191803001,3.1327383518218999,2.3920774459838898E-2]
["   Coal to Liquids","- -","- -",0,0,0,1.5105023384094201,1.3258528709411599,1.3084201812744101,1.4890010356903101,1.4777305126190201,1.52423667907715,1.55170238018036,1.6127909421920801,1.64213514328003,1.6655528545379601,1.7391279935836801,1.8144223690032999,1.881303191185,1.91615927219391,1.9549800157546999,1.98487901687622,2.0149953365325901,2.0400972366332999,2.06869769096375,2.1140794754028298,"- -"]
["   Electricity",25.976100921630898,26.701194763183601,28.885900497436499,29.465267181396499,28.0844612121582,28.946041107177699,29.255804061889599,30.039487838745099,30.684814453125,31.692062377929702,32.750293731689503,33.735057830810497,34.847049713134801,35.896480560302699,36.796710968017599,37.092437744140597,37.643119812011697,38.552295684814503,39.618198394775398,40.722320556640597,41.672286987304702,42.619045257568402,43.551567077636697,44.234035491943402,44.897003173828097,2.2851228713989299E-2]
[]
["Non-Renewable Energy Expenditures by Sector"]
["(billion nominal dollars)"]
[" Residential",225.02744706750701,238.37773132324199,259.02512631031902,249.25337512780601,252.583736500312,262.72278901234898,271.43045070142699,279.62336448741098,290.36118712182201,302.34922046937697,314.484301838607,326.31017799182001,339.67713347638499,351.841652659175,361.38263928723802,365.32884829527302,374.04615460167003,385.95134111753299,398.835809936602,410.22373705988099,422.55616886606703,434.56743167122602,447.73002080536401,457.71538257287102,468.062769957282,2.9771340183983201E-2]
[" Commercial",165.816137057829,173.08578491210901,190.230139498157,185.844578933267,184.96673437998101,193.184934067249,198.64505320450101,207.01010076743199,215.98045512613399,227.20879369248601,238.355458583971,249.80526361731199,261.78221655566898,272.88440826998601,282.07041522732101,286.98036020566298,295.05574420107399,306.22172255954098,317.57856616547701,329.069649877649,340.29091622717101,351.87208183072499,364.00595788799001,374.718362251543,385.668787945372,3.54482424126734E-2]
[" Industrial",210.45837399270499,226.84164428710901,262.44389197505598,213.892966172706,226.79179338269401,247.619560147584,273.83641803280398,298.67526634090802,321.41269661935701,343.35489244766001,359.62835975479601,376.14186022230598,389.28546003433701,399.06892807031301,405.15061668110599,407.35894410523099,415.77923171469001,426.41568562175598,436.74010603899097,448.16777725737001,459.10467071246399,469.55594536729899,481.39122134917898,492.95782400236197,503.70495393538602,3.5292797975979E-2]
[" Transportation",549.81947704453,596.754638671875,710.99412877519103,505.32645703543398,668.37680019736001,762.52132045534597,847.91759438910901,937.91141444555603,1028.33974387788,1085.06959183805,1131.9545626373499,1181.14904998321,1222.4904861899099,1257.1498536367301,1282.2289721541099,1293.5591115037901,1317.64254291509,1347.93302348928,1365.7857849230099,1397.4813404476599,1434.8442550222801,1472.1991410293999,1515.6904697150001,1560.0477492924799,1610.00718661163,4.4096217008691797E-2]
["   Total Non-Renewable Expenditures",1151.1213905869799,1235.05981445313,1422.6932865587301,1154.31734546592,1332.71906446034,1466.04865262005,1591.82954953581,1723.220162996,1856.09413471179,1957.9824453226099,2044.42271900984,2133.4064257913801,2213.2352962563,2280.9449005124402,2330.8327023315501,2353.2272042248301,2402.5237543345802,2466.5217523188298,2518.9403084269702,2584.9425046425499,2656.7959475688699,2728.1946425186502,2808.81762668277,2885.4393181192499,2967.4436544262699,3.8847823819442302E-2]
[" Transportation Renewable Expenditures",3.1291455626044802E-2,4.0766973048448597E-2,4.0714130927948497E-2,2.1793998683964599E-2,7.3206049344282806E-2,9.2770617127286306E-2,0.115739841221496,0.62128413204559196,9.0414016273646407,32.464667528422702,45.662064193132402,59.735806102059101,68.705445338854702,75.838728317784501,81.248020694409604,88.517002347113603,96.838574567007299,105.232438138034,112.23695677008899,119.789323919834,127.344773281206,134.21074205079,141.121318213276,147.47729532082599,153.48101506159901,0.43043202909376699]
["   Total Expenditures",1151.1526529385901,1235.1005859375,1422.73403823545,1154.33909891658,1332.7922559459801,1466.1414381637601,1591.9452461077601,1723.8413828856601,1865.13548978575,1990.4471814707699,2090.0847289103099,2193.14218565799,2281.9407840971799,2356.78359989211,2412.0806492987499,2441.7442864187801,2499.3623693526101,2571.7542006915,2631.1772031527198,2704.7318076809502,2784.14076302281,2862.4052247444101,2949.93897720213,3032.91659167235,3120.92473552298,4.1126546811574502E-2]
[]
[]
[]
["   1/ Includes energy for combined heat and power plants, except those whose primary business is to sell electricity, or electricity and heat, to the public."]
["   2/ Excludes use for lease and plant fuel."]
["   3/ Includes Federal and State taxes while excluding county and local taxes."]
["   4/ E85 refers to a blend of 85 percent ethanol (renewable) and 15 percent motor gasoline (nonrenewable).  To address cold starting issues, the percentage of ethanol varies"]
["seasonally.  The annual average ethanol content of 74 percent is used for this forecast."]
["   5/ Sales weighted-average price for all grades.  Includes Federal, State, and local taxes."]
["   6/ Kerosene-type jet fuel.  Includes Federal and State taxes while excluding county and local taxes."]
["   7/ Diesel fuel for on-road use.  Includes Federal and State taxes while excluding county and local taxes."]
["   8/ Compressed natural gas used as a vehicle fuel.  Includes estimated motor vehicle fuel taxes and estimated dispensing costs or charges."]
["   9/ Includes electricity-only and combined heat and power plants whose primary business is to sell electricity, or electricity and heat, to the public."]
["   10/ Weighted averages of end-use fuel prices are derived from the prices shown in each sector and the corresponding sectoral consumption."]
["   Btu = British thermal unit."]
["   - - = Not applicable."]
["   Note:  Data for 2006 and 2007 are model results and may differ slightly from official EIA data reports."]
["   Sources:  2006 and 2007 prices for motor gasoline, distillate fuel oil, and jet fuel are based on prices in the Energy Information Administration (EIA), Petroleum Marketing Annual"]
["2007, DOE/EIA-0487(2007) (Washington, DC, August 2008).  2006 residential and commercial natural gas delivered prices:  EIA, Natural Gas Annual 2006, DOE/EIA-0131(2006)"]
["(Washington, DC, October, 2007).  2007 residential and commercial natural gas delivered prices:  EIA, Natural Gas Monthly, DOE/EIA-0130(2008/04) (Washington, DC, April 2008)."]
["2006 and 2007 industrial natural gas delivered prices are estimated based on:  EIA, Manufacturing Energy Consumption Survey 1994 and industrial and wellhead prices from the"]
["Natural Gas Annual 2006, DOE/EIA-0131(2006) (Washington, DC, October, 2007) and the Natural Gas Monthly, DOE/EIA-0130(2008/04) (Washington, DC, April 2008).  2006"]
["transportation sector natural gas delivered prices are based on:  EIA, Natural Gas Annual 2006, DOE/EIA-0131(2006) (Washington, DC, October, 2007) and estimated State taxes,"]
["Federal taxes, and dispensing costs or charges.  2007 transportation sector natural gas delivered prices are model results.  2006 and 2007 electric power sector natural gas prices:"]
["EIA, Electric Power Monthly, April 2007 and April 2008, Table 4.13.B.  2006 and 2007 coal prices based on:  EIA, Quarterly Coal Report, October-December 2007,"]
["DOE/EIA-0121(2007/4Q) (Washington, DC, March 2008) and EIA, AEO2009 National Energy Modeling System run aeo2009.d120908a.  2006 and 2007 electricity prices:  EIA, Annual"]
["Energy Review 2007, DOE/EIA-0384(2007) (Washington, DC, June 2008).  2006 and 2007 E85 prices derived from monthly prices in the Clean Cities Alternative Fuel Price Report."]
["Projections:  EIA, AEO2009 National Energy Modeling System run hp2009.d121108a."]

{"sheet":"HyARC Physical Property Data","index":14,"n_rows":526,"n_cols":21,"rows_kept":526,"cut":false,"hidden":false,"merged":[[51,0,51,10],[50,0,50,10],[91,3,91,4],[58,0,58,10],[1,0,1,10],[2,0,2,10],[3,2,3,4],[3,6,3,8],[55,0,55,10],[56,0,56,10],[92,10,92,11],[91,0,91,1],[57,0,57,10],[52,0,52,10],[134,2,134,4],[134,5,134,7],[53,0,53,10],[91,6,91,7],[92,3,92,4],[54,0,54,10],[60,0,60,10],[61,0,61,10],[91,10,91,11]]}
["HyARC Energy Constants and Assumptions"]
["Hydrogen Analysis Resource Center:  Lower and Higher Heating Values of Hydrogen and Fuels"]
[]
["Fuels",null,"Lower Heating Value (LHV) [1]",null,null,null,"Higher Heating Value (HHV) [1]",null,null,null,"Density",null,null,null,"HHV/LHV Ratios for Price Tables (HHV values from EIA, LHV values from GREET)"]
["Gaseous Fuels @ 32 F and 1 atm",null,"Btu/ft3 [2]","Btu/lb [3]","MJ/kg [4]",null,"Btu/ft3 [2]","Btu/lb [3]","MJ/kg [4]",null,"grams/ft3",null,null,null,null,null,null,2005,2007,2005,2007]
["Natural gas",null,983,{"$f":"C6/$K6*453.59","v":20267.225909090906},{"$f":"D6*1.05506/1000*2.2046","v":47.141269049911173},null,1089,{"$f":"G6/$K6*453.59","v":22452.704999999998},{"$f":"H6*1.05506/1000*2.2046","v":52.224661236371581},null,22,null,null,null,"Feedstock","Units","LHV","HHV","HHV","HHV/LHV","HHV/LHV"]
["Hydrogen",null,290,{"$f":"C7/K7*453.59","v":51682.028917177428},{"$f":"D7*1.05506/1000*2.2046","v":120.21163829516094},null,343,{"$f":"G7/$K7*453.59","v":61127.365236523648},{"$f":"H7*1.05506/1000*2.2046","v":142.1813515008283},null,2.5451999999999999,null,null,null,"Commercial Natural Gas_metric","Btu/scf",930,1027,1030,{"$f":"R7/Q7","v":1.1043010752688172},{"$f":"S7/Q7","v":1.10752688172043}]
["Still gas (in refineries)",null,1458,20162.628658536585,46.897977385211739,null,1584,21905.078048780488,50.950889011094226,null,32.799999999999997,null,null,null,"Industrial Natural Gas_metric","Btu/scf",930,1027,1030,{"$f":"R8/Q8","v":1.1043010752688172},{"$f":"S8/Q8","v":1.10752688172043}]
["Liquid Fuels",null,"Btu/gal [2]","Btu/lb [3]","MJ/kg [4]",null,"Btu/gal [2]","Btu/lb [3]","MJ/kg [4]",null,"grams/gal",null,null,null,"Electric Utility Natural Gas_metric","Btu/scf",930,1027,1030,{"$f":"R9/Q9","v":1.1043010752688172},{"$f":"S9/Q9","v":1.10752688172043}]
["Crude oil",null,129670,18351.642839313572,42.685651034654214,null,138350,19580.086271450855,45.542992370204438,null,3205,null,null,null,"Commercial Electricity_metric",null,null,null,null,1,1]
["Conventional gasoline",null,116090,18679.412238382403,43.448037830811678,null,124340,20006.874991131608,46.535696648144757,null,2819,null,null,null,"Industrial Electricity_metric",null,null,null,null,1,1]
["Reformulated or low-sulfur gasoline",null,113601.50975397152,18210.67343395916,42.357758273433376,null,121848.38036482914,19532.672304147527,45.432708180380153,null,2829.5773353012783,null,null,null,"Electric Utility Steam Coal_metric","Btu/short ton",19546300,20754000,20231000,{"$f":"R12/Q12","v":1.0617866296946226},{"$f":"S12/Q12","v":1.0350296475547802}]
["CA reformulated gasoline",null,113927.15396104372,18271.813278014368,42.499968650482714,null,122174.43408423416,19594.524828536756,45.576576241392928,null,2828.193183616288,null,null,null,"Retail Diesel_metric","Btu/gallon",128450,{"$f":"5825000/42","v":138690.47619047618},{"$f":"5799000/42","v":138071.42857142858},{"$f":"R13/Q13","v":1.0797234425105191},{"$f":"S13/Q13","v":1.0749040760718458}]
["U.S. conventional diesel",null,128450,18397.106251973477,42.791398263097854,null,137380,19676.095421534574,45.766308239660439,null,3167,null,null,null,"E85 Ethanol_metric","Btu/gallon",86668,94706,94854,{"$f":"R14/Q14","v":1.0927447270041999},{"$f":"S14/Q14","v":1.0944523930401071}]
["Low-sulfur diesel",null,129487.84757606639,18320.147467881456,42.612393264440954,null,138490,19593.786369307545,45.574858596098856,null,3206,null,null,null,"Methanol_metric","Btu/gallon",null,null,null,{"$f":"$I$19/$E$19","v":1.1388646288209607},{"$f":"$I$19/$E$19","v":1.1388646288209607}]
["Petroleum naphtha",null,116920,19320.124881602911,44.938326005089621,null,125080,20668.501712204008,48.074630659567319,null,2745,null,null,null,"Retail Gasoline_metric","Btu/gallon",116090,{"$f":"5194000/42","v":123666.66666666667},{"$f":"5218000/42","v":124238.09523809524},{"$f":"R16/Q16","v":1.0652654549631033},{"$f":"S16/Q16","v":1.0701877443198831}]
["NG-based FT naphtha",null,111520,19081.236061863448,44.382674127774621,null,119740,20487.69015465862,47.654065638986118,null,2651,null,null,null,"Woody Biomass_metric","Btu/short ton",16811000,17200000,17200000,{"$f":"R17/Q17","v":1.0231396109690083},{"$f":"S17/Q17","v":1.0231396109690083}]
["Residual oil",null,140352.52220119376,16967.617416108602,39.466428278669781,null,150110,18147.226785714287,42.210182303804245,null,3752,null,null,null,"Steam_metric","GJ/kg",2.8300000000000001E-3,null,null,1,1]
["Methanol",null,57250,8638.7317032601459,20.093562745097504,null,65200,9838.345974717231,22.883847877386152,null,3006]
["Ethanol",null,76330,11587.19032797858,26.95163409308779,null,84530,12831.982161981257,29.847001570663057,null,2988]
["Butanol",null,99837,14774.898802610114,34.366197069261162,null,108458,16050.722420880913,37.33374402013208,null,3065]
["Acetone",null,83127,12721.179463562754,29.589276125600549,null,89511,13698.142540485829,31.861677857719279,null,2964]
["E-Diesel Additives",null,116090,18679.412238382403,43.448037830811678,null,124340,20006.874991131608,46.535696648144757,null,2819]
["Liquefied petroleum gas (LPG)",null,84950,20037.686167446696,46.607362990589891,null,91410,21561.446645865835,50.151607427543532,null,1923]
["Liquefied natural gas (LNG)",null,74720,20908.23244910549,48.632240823804793,null,84820,23734.425539790249,55.205924339870478,null,1621]
["Dimethyl ether (DME)",null,68930,12416.981215250198,28.881715479040551,null,75610,13620.3097299444,31.680639886410216,null,2518]
["Dimethoxy methane (DMM)",null,72200,10061.197542242702,23.402197342183918,null,79196.89540113158,11036.227276497471,25.670102147722705,null,3255]
["Methyl ester (biodiesel, BD)",null,119550,16134.09238321928,37.527661324991804,null,127960,17269.079559654863,40.167624785829787,null,3361]
["Fischer-Tropsch diesel (FTD)",null,123670,18593.130692741131,43.247348226059557,null,130030,19549.323069274113,45.471437614898726,null,3017]
["Renewable Diesel I (SuperCetane)",null,117059,18729.027093474426,43.563441253226593,null,125294,20046.598045855379,46.628091888549989,null,2835]
["Renewable Diesel II (UOP-HDO)",null,122887,18907.840681818183,43.979359026862895,null,130817,20127.979318181817,46.817383529723436,null,2948]
["Renewable Gasoline",null,115983,18589.656879858656,43.23926818844334,null,124230,19911.479045936394,46.313807084230582,null,2830]
["Liquid Hydrogen",null,30500,51621.249999999993,120.070267428715,null,36020,60963.849999999991,141.80101746827262,null,268]
["Methyl tertiary butyl ether (MTBE)",null,93540,15093.848665955175,35.108069755183983,null,101130,16318.59007470651,37.95680023884708,null,2811]
["Ethyl tertiary butyl ether (ETBE)",null,96720,15612.535516014234,36.314527731276172,null,104530,16873.225160142349,39.246873281123854,null,2810]
["Tertiary amyl methyl ether (TAME)",null,100480,15645.974322004806,36.392305901657274,null,108570,16905.687023686918,39.322379097760042,null,2913]
["Butane",null,94970,19465.631405332126,45.27677203684572,null,103220,21156.601807501127,49.209944294442614,null,2213]
["Isobutane",null,90060,19287.212181303115,44.861771548798892,null,98560,21107.568649669498,49.095893891290459,null,2118]
["Isobutylene",null,95720,19271.031868619615,44.824136379735997,null,103010,20738.706569019083,48.237926122822877,null,2253]
["Propane",null,84250,19903.623697916668,46.295535660398848,null,91420,21597.498854166668,50.235464333218552,null,1920]
["Solid Fuels",null,"Btu/ton [2]","Btu/lb [5]","MJ/kg [4]",null,"Btu/ton [2]","Btu/lb [5]","MJ/kg [4]"]
["Coal (wet basis) [6]",null,19546300,{"$f":"C42/2000","v":9773.15},{"$f":"D42*1.05506/1000*2.2046","v":22.7322030001394},null,20608570,{"$f":"G42/2000","v":10304.285},{"$f":"H42*1.05506/1000*2.2046","v":23.967615189707661}]
["Bituminous coal (wet basis) [7]",null,22460600,11230.3,26.121512445062798,null,23445900,{"$f":"G43/2000","v":11722.95},27.267409091284208]
["Coking coal (wet basis)",null,24600497.144575384,12300.248572287692,28.610197070281195,null,25679670,12839.834999999999,29.865267156269461]
["Farmed trees (dry basis)",null,16811000,8405.5,19.551069237418005,null,17703170,8851.5849999999991,20.588656379262464]
["Herbaceous biomass (dry basis)",null,14797554.763920812,7398.7773819604063,17.209447250841734,null,15582870,7791.4350000000004,18.122763088911064]
["Corn stover (dry basis)",null,14075990,7037.9949999999999,16.370272742561625,null,14974460,7487.23,17.415186738025483]
["Forest residue (dry basis)",null,13243490,6621.7449999999999,15.40208137142662,null,14164160,7082.08,16.472813803454081]
["Sugar cane bagasse",null,12947318,6473.6589999999997,15.057635515844886,null,14062678,7031.3389999999999,16.354790984564566]
["Petroleum coke",null,25370000,12685,29.505123226060004,null,26920000,13460,31.307761814960006]
["Notes:"]
["[1] The lower heating value (also known as net calorific value) of a fuel is defined as the amount of heat released by combusting a specified quantity (initially at 25°C) and returning the temperature of the combustion products to 150°C, which assumes the latent heat of vaporization of water in the reaction products is not recovered."]
["The higher heating value (also known as gross calorific value or gross energy) of a fuel is defined as the amount of heat released by a specified quantity (initially at 25°C) once it is combusted and the products have returned to a temperature of 25°C, which takes into account the latent heat of vaporization of water in the combustion products."]
["[2] Btu =  British thermal unit. "]
["[3] The heating values for gaseous fuels in units of Btu/lb are calculated based on the heating values in units of Btu/ft3 and the corresponding fuel density values. The heating values for liquid fuels in units of Btu/lb are calculated based on heating values in units of Btu/gal and the corresponding fuel density values."]
["[4] The heating values in units of MJ/kg, are converted from the heating values in units of Btu/lb."]
["[5] For solid fuels, the heating values in units of Btu/lb are converted from the heating values in units of Btu/ton."]
["[6] Coal characteristics assumed by GREET for electric power production."]
["[7] Coal characteristics assumed by GREET for hydrogen and Fischer-Tropsch diesel production."]
[]
["Source:"]
["GREET Transportation Fuel Cycle Analysis Model, GREET 1.8b, developed by Argonne National Laboratory, Argonne, IL, released May 8, 2008. http://www.transportation.anl.gov/software/GREET/index.html"]
[]
[]
[]
[]
[]
[]
["TABLE A - Energy Feedstock and Utility Properties Table"]
["Feedstock Type","Source","Source Year (for original price data)","H2a Reference Year","Units for Feedstock Price Table","HHV/LHV Source","HHV/LHV","H2A Usage Input Unit/ kg H2","H2A LHV (GJ/ H2A usage input unit)","List","CO2 Emissions Factor (kg CO2 produced/GJ feed)","Unit System","CH4 Emissions Factor (kg CH4 produced/GJ or mmBtu feed)","N2O Emissions Factor (kg N2O produced/GJ or mmBtu feed)"]
["Commercial Natural Gas","Energy Information Administration Annual Energy Outlook.  See AEO Data sheet for original data","see Energy Feed Tab",2007,"$(2007)/GJ LHV",null,null,"mmBtu",{"$f":"mmBTU_to_GJ","v":1.0549999999999999},"Feed Utility",56.31533863997597,"Metric"]
["Industrial Natural Gas","Energy Information Administration Annual Energy Outlook.  See AEO Data sheet for original data","see Energy Feed Tab",2007,"$(2007)/GJ LHV",null,null,"mmBtu",{"$f":"mmBTU_to_GJ","v":1.0549999999999999},"Feed Utility",56.31533863997597,"Metric"]
["Residential Natural Gas","Energy Information Administration Annual Energy Outlook.  See AEO Data sheet for original data","see Energy Feed Tab",2007,"$(2007)/GJ LHV",null,null,"mmBtu",{"$f":"mmBTU_to_GJ","v":1.0549999999999999},"Feed Utility",56.31533863997597,"Metric"]
["Electric Utility Natural Gas","Energy Information Administration Annual Energy Outlook.  See AEO Data sheet for original data","see Energy Feed Tab",2007,"$(2007)/GJ LHV",null,null,"mmBtu",{"$f":"mmBTU_to_GJ","v":1.0549999999999999},"Feed Utility",56.31533863997597,"Metric"]
["Bio Methane",null,"see Energy Feed Tab",2007,"$(2007)/GJ LHV",null,null,"mmBtu",{"$f":"mmBTU_to_GJ","v":1.0549999999999999},"Feed Utility",56.31533863997597,"Metric"]
["Commercial Electricity","Energy Information Administration Annual Energy Outlook.  See AEO Data sheet for original data","see Energy Feed Tab",2007,"$(2007)/GJ",null,null,"kWh",{"$f":"1/MJ_to_kWh/1000","v":3.5999999999999995E-3},"Feed Utility Byprod",0,"Metric"]
["Industrial Electricity","Energy Information Administration Annual Energy Outlook.  See AEO Data sheet for original data","see Energy Feed Tab",2007,"$(2007)/GJ",null,null,"kWh",{"$f":"1/MJ_to_kWh/1000","v":3.5999999999999995E-3},"Feed Utility Byprod",0,"Metric"]
["Residential Electricity","Energy Information Administration Annual Energy Outlook.  See AEO Data sheet for original data","see Energy Feed Tab",2007,"$(2007)/GJ",null,null,"kWh",{"$f":"1/MJ_to_kWh/1000","v":3.5999999999999995E-3},"Feed Utility Byprod",0,"Metric"]
["Electric Utility Steam Coal","Energy Information Administration Annual Energy Outlook.  See AEO Data sheet for original data","see Energy Feed Tab",2007,"$(2007)/GJ LHV",null,null,"kg",{"$f":"$C$42/2000/lb_to_kg/1000000*mmBTU_to_GJ","v":2.2735034516249999E-2},"Feed",102.75287348239476,"Metric"]
["Metallurgical Coal","Energy Information Administration Annual Energy Outlook.  See AEO Data sheet for original data","see Energy Feed Tab",2007,"$(2007)/GJ LHV",null,null,"kg",{"$f":"$C$42/2000/lb_to_kg/1000000*mmBTU_to_GJ","v":2.2735034516249999E-2},"Feed",102.75287348239476,"Metric"]
["Other Industrial Coal","Energy Information Administration Annual Energy Outlook.  See AEO Data sheet for original data","see Energy Feed Tab",2007,"$(2007)/GJ LHV",null,null,"kg",{"$f":"$C$42/2000/lb_to_kg/1000000*mmBTU_to_GJ","v":2.2735034516249999E-2},"Feed",102.75287348239476,"Metric"]
["Retail Diesel","Energy Information Administration Annual Energy Outlook.  See AEO Data sheet for original data","see Energy Feed Tab",2007,"$(2007)/GJ LHV",null,null,"L",{"$f":"$C$14/gal_to_liters*mmBTU_to_GJ/1000000","v":3.5803104359313075E-2},"Feed Utility",74.122324937568308,"Metric"]
["E85 Ethanol","Energy Information Administration Annual Energy Outlook.  See AEO Data sheet for original data","see Energy Feed Tab",2007,"$(2007)/GJ LHV",null,null,"L",{"$f":"$Q$14/gal_to_liters*mmBTU_to_GJ/1000000","v":2.4157130779392338E-2},"Feed",71.019041167591709,"Metric"]
["Retail Gasoline","Energy Information Administration Annual Energy Outlook.  See AEO Data sheet for original data","see Energy Feed Tab",2007,"$(2007)/GJ LHV",null,null,"L",{"$f":"$C$11/gal_to_liters*mmBTU_to_GJ/1000000","v":3.2357978863936591E-2},"Feed",72.833307273582633,"Metric"]
["Woody Biomass","* Biomass prices shown for years 2001 through 2009 are the same as the EIA value for 2010.  For the post-2025 biomass prices:  The value for 2035 was chosen based on a review of the literature, which indicated a price of $2.50/MMBtu delivered dry English ton (in 2000$) was a reasonable mid-range projection.  Values for the 2026 through 2034 were interpolated from the 2025 and 2035 values.  The value of $5.00/MMBtu delivered dry English ton in 2065 was based on judgment.  An EIA paper by Zia Haq entitled, “Biomass for Electricity Generation” (available from EIA’s website) indicates that about 7 quads of biomass per year  would be available if the price rose to  $5/MMBtu.","see Energy Feed Tab",2007,"$(2007)/GJ",null,null,"kg",{"$f":"$E$45/1000","v":1.9551069237418006E-2},"Feed",97.876597052612851,"Metric"]
["Woody Biomass B2A",null,null,null,"$(2007)/GJ",null,null,"kg",{"$f":"$E$45/1000","v":1.9551069237418006E-2},"Feed",97.876597052612851,"Metric"]
["Woody Biomass MYPP","Biomass Multi-Year Program Plan April 2011, Table B-4. LHV from Table B-7 (8,000 Btu/lb). Prices starting in 2010 $82.70, 2011 $71.60, 2012, $61.57, 2013; $68.97",null,null,"$(2007)/GJ",null,null,"kg",{"$f":"18.608/1000","v":1.8608E-2},"Feed",97.876597052612851,"Metric"]
["Ethanol","Biomass Program MYPP April 2011, HyARC data (see AEO data tab for additional information)",2007,{"$f":"ref_year","v":2016},"$(2007)/GJ LHV","HyARC","N/A","gallons",8.1000000000000003E-2,"Feed",70.89,"Metric"]
["Steam","Note:  when steam is an important input or output, the price should be externally provided and should be based on the specific characteristics of the steam needed or produced. ","see Energy Feed Tab",2007,"$(2007)/GJ",null,null,"kg",2.8300000000000001E-3,"Feed Utility Byprod",0,"Metric"]
[]
[]
["TABLE B - GDP Implicit Deflator Price Index",null,null,"TABLE B2 - Plant Cost Index",null,null,"TABLE B3 - Labor Index",null,null,null,"TABLE B4 - SRI Chemical Price Index"]
["GDP Implicit Price Deflator (Index, 2005=100), Available from Federal Reserve Bank of St. Louis (FRED): http://research.stlouisfed.org/fred2/series/GDPDEF/",null,null,"From Chemical Engineering Magazine                                              Averaged Annual Index",null,null,"From the Bureau of Labor Statistics, Average Hourly Earnings of Chemical Manufacturing Workers (Production and Nonsupervisory Employees)  From series CEU3232500008",null,null,null,"SRI Inorganic Price Index  (Index, 1982=100),                                                     Current Index at http://www.sriconsulting.com/CEH/ "]
["Year","Value",null,"Year","Value",null,"Year","Value",null,null,"Year","Value"]
[1992,70.800676680058203,null,1992,358.2,null,1992,13.7,null,null,1992,80.280791320995533]
[1993,72.480274460589698,null,1993,359.2,null,1993,13.97,null,null,1993,81.174218251435875]
[1994,74.02700932145197,null,1994,368.1,null,1994,14.33,null,null,1994,82.961072112316543]
[1995,75.581637029027263,null,1995,381.1,null,1995,14.86,null,null,1995,91.512444160816855]
[1996,76.96367448847775,null,1996,381.7,null,1996,15.37,null,null,1996,93.044033184428855]
[1997,78.291514400498826,null,1997,386.5,null,1997,15.78,null,null,1997,93.873643905552015]
[1998,79.172882283453163,null,1998,389.5,null,1998,16.23,null,null,1998,94.894703254626677]
[1999,80.287352239332165,null,1999,390.6,null,1999,16.399999999999999,null,null,1999,95.532865347798349]
[2000,82.107442691355487,null,2000,394.1,null,2000,17.09,null,null,2000,100]
[2001,83.960946194463943,null,2001,394.3,null,2001,17.57,null,null,2001,101.08487555839186]
[2002,85.268264705031157,null,2002,395.6,null,2002,17.97,null,null,2002,100.38289725590302]
[2003,86.946283916220068,null,2003,402,null,2003,18.5,null,null,2003,105.04148053605616]
[2004,89.280198689261255,null,2004,444.2,null,2004,19.170000000000002,null,null,2004,110.27440970006384]
[2005,92.081633082603915,null,2005,468.2,null,2005,19.670000000000002,null,null,2005,119.52776005105299]
[2006,94.92568884819687,null,2006,499.6,null,2006,19.600000000000001,null,null,2006,125.5902999361838]
[2007,97.490337840148811,null,2007,525.4,null,2007,19.55,null,null,2007,129.73835354179963]
[2008,99.368309168067654,null,2008,575.4,null,2008,19.5,null,null,2008,145.6285896617741]
[2009,100,null,2009,521.9,null,2009,20.3,null,null,2009,143.39502233567327]
[2010,101.19839722592747,null,2010,550.79999999999995,null,2010,21.07,null,null,2010,149.13848117421827]
[2011,103.30263015961967,null,2011,585.70000000000005,null,2011,21.45,null,null,2011,160.8806636885769]
[2012,105.23637760431055,null,2012,584.6,null,2012,21.447500000000002,null,null,2012,166.11359285258459]
[2013,107.07698945778775,null,2013,567.29999999999995,null,2013,21.4025,null,null,2013,168.41097638800255]
[2014,109.07756300464888,null,2014,576.1,null,2014,21.488333333333333,null,null,2014,171.79323548181239]
[2015,110.1730901284166,null,2015,556.79999999999995,null,2015,21.754999999999999,null,null,2015,168.98532227185709]
[2016,111.27519462444519,null,{"$f":"+D118+1","v":2016},541.70000000000005,null,2016,22.714999999999993,null,null,2016,170.4530950861519]
[2017,113.38521564572694,null,{"$f":"+D119+1","v":2017},567.5,null,2017,24.275833333333328,null,null,{"$f":"+K119+1","v":2017},177.13905876096783]
[2018,116.09509301719851,null,2018,603.1,null,2018,25.462500000000002,null,null,{"$f":"+K120+1","v":2018},185.15820260568998]
[2019,118.17196408228557,null,2019,607.5,null,2019,25.46083333333333,null,null,{"$f":"+K121+1","v":2019},186.37596383940442]
[2020,119.58504673880728,null,2020,596.20000000000005,null,2020,26.035833333333333,null,null,{"$f":"+K122+1","v":2020},184.41371975538419]
[2021,124.54122828480547,null,2021,708.01666666666677,null,2021,26.685000000000002,null,null,{"$f":"+K123+1","v":2021},205.95490561021009]
["3/1/2022 source: https://fred.stlouisfed.org/series/GDPDEF#0",null,null,"3/2/2022 source: https://www.chemengonline.com/pci",null,null,"3/1/2022 source: http://data.bls.gov/timeseries/CEU3232500008?data_tool=Xgtable",null,null,null,"Base date: December 1984 for the Producer price index - chemical mfg (adjusted to 1982 base)"]
[null,null,null,null,null,null,null,null,null,null,"5/15/17:  Same information as BLS data for Chemical Mfg:  https://data.bls.gov/pdq/SurveyOutputServlet"]
[null,null,null,null,null,null,null,null,null,null,"3/1/2022 source: https://alfred.stlouisfed.org/series?seid=PCU325325"]
[]
[]
[]
[]
[]
[]
["Table C1 2010 Upstream Energy and Emissions for H2 Feedstocks: for each MJ (LHV, or as noted) of feedstock available at H2 production site.  Source: GREET1_2013, 01/20/2014 for year 2010 technologies"]
[null,null,"Energy: J/MJ",null,null,"Greenhouse Gas Emissions: grams/MJ",null,null,"Total Greenhouse Gas Emissions: grams/MJ"]
["Feedstock/Fuel","Description","Total Energy ","Fossil Fuels","Petroleum","CO2","CH4","N2O","GHGs"]
["Commercial Natural Gas","North American sources -- at plant gate",{"$f":"+AVERAGEIFS(D$167:D$526,$B$167:$B$526,$A137,$C$167:$C$526,\">=\"&startup_year,$C$167:$C$526,\"<=\"&(startup_year+anal_period))","v":1092600},1092000,3991.8,5.7817600000000002,0.18464100000000003,8.6175999999999993E-4,11.6076]
["Industrial Natural Gas","North American sources -- at plant gate",1092600,1092000,3991.8,5.7817600000000002,0.18464100000000003,8.6175999999999993E-4,11.6076]
["Electric Utility Natural Gas","North American sources -- at plant gate",1092600,1092000,3991.8,5.7817600000000002,0.18464100000000003,8.6175999999999993E-4,11.6076]
["Residential Natural Gas","North American sources -- at plant gate",1092600,1092000,3991.8,5.7817600000000002,0.18464100000000003,8.6175999999999993E-4,11.6076]
["Bio Methane","From waste and intermediate fuels",-1186800,0,0,-85.798000000000002,0.54692000000000007,-1.8314E-3,-70.083999999999989]
["Commercial Electricity","U.S. Average - at Wall Outlet",1837000,1430400,25410,150.98000000000002,0.21918739999999998,2.2404E-3,156.858]
["Industrial Electricity","U.S. Average - at Wall Outlet",1837000,1430400,25410,150.98000000000002,0.21918739999999998,2.2404E-3,156.858]
["Residential Electricity","U.S. Average - at Wall Outlet",1837000,1430400,25410,150.98000000000002,0.21918739999999998,2.2404E-3,156.858]
["Electric Utility Steam Coal","at Plant Gate",1022000,1021000,15538,1.7482800000000001,0.14098174399999999,3.36786E-5,6.0087799999999998]
["Metallurgical Coal","at Plant Gate",1022000,1021000,15538,1.7482800000000001,0.14098174399999999,3.36786E-5,6.0087799999999998]
["Other Industrial Coal","at Plant Gate",{"$f":"+AVERAGEIFS(D$167:D$526,$B$167:$B$526,$A147,$C$167:$C$526,\">=\"&startup_year,$C$167:$C$526,\"<=\"&(startup_year+anal_period))","v":1022000},1021000,15538,1.7482800000000001,0.14098174399999999,3.36786E-5,6.0087799999999998]
["Retail Diesel","at Forecourt",1209800,1203200,1052200,18.333400000000001,0.1638558,2.9598999999999999E-4,23.360400000000002]
["E85 Ethanol","84 wt% ethanol from corn and 16 wt% gasoline",1598600,703960,287120,39.183399999999999,0.11269999999999999,2.5806000000000003E-2,46.212000000000003]
["Ethanol","Ethanol for gasoline blending from GREET 2021",1813320.0000000002,547200,48780.72,32.962800000000001,9.4511600000000001E-2,7.9808599999999993E-2,53.151400000000002]
["Retail Gasoline","at Forecourt",1251000,1243400,1078600,24.240199999999998,0.1695246,3.8440400000000003E-4,29.561399999999999]
["Woody Biomass","Biomass for Gasification Hydrogen Production ",1190200,52136,29376,3.8460799999999997,8.4834799999999981E-3,-3.8248612000000002E-3,3.0997200000000005]
["Woody Biomass B2A","Biomass for Gasification Hydrogen Production ",1190200,52136,29376,3.8460799999999997,8.4834799999999981E-3,-3.8248612000000002E-3,3.0997200000000005]
["Woody Biomass MYPP","Biomass for Gasification Hydrogen Production ",1190200,52136,29376,3.8460799999999997,8.4834799999999981E-3,-3.8248612000000002E-3,3.0997200000000005]
["Steam","GREET.NET, natural gas feedstock",1384200,1383400,5061.2,78.630040000000008,0.27492,2.33154E-3,87.653500000000008]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"GREET.NET 2017 upstream emmissions tables"]
[null,null,null,"Energy: J/MJ",null,null,"Greenhouse Gas Emissions: grams/MJ",null,null,"Total Greenhouse Gas Emissions: grams/MJ"]
[null,"Feedstock","Year","Total Energy ","Fossil Fuels","Petroleum","CO2","CH4","N2O","GHGs"]
[null,"Commercial Natural Gas",2005,1094000,1094000,4252,5.9984999999999999,0.18232600000000002,8.8801999999999994E-5,11.536999999999999]
[null,"Industrial Natural Gas",2005,1094000,1094000,4252,5.9984999999999999,0.18232600000000002,8.8801999999999994E-5,11.536999999999999]
[null,"Electric Utility Natural Gas",2005,1094000,1094000,4252,5.9984999999999999,0.18232600000000002,8.8801999999999994E-5,11.536999999999999]
[null,"Residential Natural Gas",2005,1094000,1094000,4252,5.9984999999999999,0.18232600000000002,8.8801999999999994E-5,11.536999999999999]
[null,"Bio Methane",2005,-1208000,0,0,-85.789999999999992,0.54689999999999994,-1.4884E-3,-70]
[null,"Commercial Electricity",2005,2475000,2129000,124000,251.83,0.31369799999999998,3.6604999999999997E-3,255.85999999999999]
[null,"Industrial Electricity",2005,2475000,2129000,124000,251.83,0.31369799999999998,3.6604999999999997E-3,255.85999999999999]
[null,"Residential Electricity",2005,2475000,2129000,124000,251.83,0.31369799999999998,3.6604999999999997E-3,255.85999999999999]
[null,"Electric Utility Steam Coal",2005,1023000,1022000,15840,1.9352,0.14136591000000001,3.6392E-5,6.2023000000000001]
[null,"Metallurgical Coal",2005,1023000,1022000,15840,1.9352,0.14136591000000001,3.6392E-5,6.2023000000000001]
[null,"Other Industrial Coal",2005,1023000,1022000,15840,1.9352,0.14136591000000001,3.6392E-5,6.2023000000000001]
[null,"Retail Diesel",2005,1205000,1200000,1056000,18.433,0.18217,2.0549999999999998E-4,23.908999999999999]
[null,"E85 Ethanol",2005,1760000,783400,307400,47.923999999999999,0.13161500000000001,3.3619999999999997E-2,56.43]
[null,"Retail Gasoline",2005,1248000,1242000,1084000,24.465,0.18840200000000001,2.7361999999999997E-4,30.237000000000002]
[null,"Woody Biomass",2005,1195000,56800,32280,4.3339999999999996,9.434399999999999E-3,-3.8369229999999999E-3,3.6147]
[null,"Woody Biomass B2A",2005,1195000,56800,32280,4.3339999999999996,9.434399999999999E-3,-3.8369229999999999E-3,3.6147]
[null,"Woody Biomass MYPP",2005,1195000,56800,32280,4.3339999999999996,9.434399999999999E-3,-3.8369229999999999E-3,3.6147]
[null,"Steam",2005,1387000,1386000,5427,78.934799999999996,0.27050000000000002,1.418723E-3,87.571399999999997]
[null,"Commercial Natural Gas",2010,1094000,1093000,4104,5.9177,0.18431800000000001,8.6370000000000001E-4,11.7387]
[null,"Industrial Natural Gas",2010,1094000,1093000,4104,5.9177,0.18431800000000001,8.6370000000000001E-4,11.7387]
[null,"Electric Utility Natural Gas",2010,1094000,1093000,4104,5.9177,0.18431800000000001,8.6370000000000001E-4,11.7387]
[null,"Residential Natural Gas",2010,1094000,1093000,4104,5.9177,0.18431800000000001,8.6370000000000001E-4,11.7387]
[null,"Bio Methane",2010,-1208000,0,0,-85.789999999999992,0.54600000000000004,-1.8614999999999999E-3,-70.12]
[null,"Commercial Electricity",2010,2254000,1938000,52730,220.67,0.288267,3.4012000000000001E-3,228.91000000000003]
[null,"Industrial Electricity",2010,2254000,1938000,52730,220.67,0.288267,3.4012000000000001E-3,228.91000000000003]
[null,"Residential Electricity",2010,2254000,1938000,52730,220.67,0.288267,3.4012000000000001E-3,228.91000000000003]
[null,"Electric Utility Steam Coal",2010,1023000,1022000,15710,1.8761000000000001,0.14136795000000002,3.5802E-5,6.1511000000000005]
[null,"Metallurgical Coal",2010,1023000,1022000,15710,1.8761000000000001,0.14136795000000002,3.5802E-5,6.1511000000000005]
[null,"Other Industrial Coal",2010,1023000,1022000,15710,1.8761000000000001,0.14136795000000002,3.5802E-5,6.1511000000000005]
[null,"Retail Diesel",2010,1206000,1201000,1056000,18.166999999999998,0.18199899999999999,2.9639E-4,23.741999999999997]
[null,"E85 Ethanol",2010,1687000,740000,297100,42.921999999999997,0.12687100000000001,2.955E-2,50.54]
[null,"Retail Gasoline",2010,1248000,1242000,1083000,24.158999999999999,0.18823500000000001,3.8572999999999998E-4,30.041]
[null,"Woody Biomass",2010,1194000,56320,32080,4.2514000000000003,9.6048000000000001E-3,-3.820487E-3,3.5488999999999997]
[null,"Woody Biomass B2A",2010,1194000,56320,32080,4.2514000000000003,9.6048000000000001E-3,-3.820487E-3,3.5488999999999997]
[null,"Woody Biomass MYPP",2010,1194000,56320,32080,4.2514000000000003,9.6048000000000001E-3,-3.820487E-3,3.5488999999999997]
[null,"Steam",2010,1386000,1385000,5215,78.8352,0.27453,2.3346E-3,87.848799999999997]
[null,"Commercial Natural Gas",2015,1093000,1092000,4020,5.8287000000000004,0.18472100000000002,8.6249999999999999E-4,11.659600000000001]
[null,"Industrial Natural Gas",2015,1093000,1092000,4020,5.8287000000000004,0.18472100000000002,8.6249999999999999E-4,11.659600000000001]
[null,"Electric Utility Natural Gas",2015,1093000,1092000,4020,5.8287000000000004,0.18472100000000002,8.6249999999999999E-4,11.659600000000001]
[null,"Residential Natural Gas",2015,1093000,1092000,4020,5.8287000000000004,0.18472100000000002,8.6249999999999999E-4,11.659600000000001]
[null,"Bio Methane",2015,-1194000,0,0,-85.789999999999992,0.54659999999999997,-1.8422E-3,-70.099999999999994]
[null,"Commercial Electricity",2015,2038000,1688000,38920,180.61,0.25748300000000002,2.7356999999999998E-3,187.32]
[null,"Industrial Electricity",2015,2038000,1688000,38920,180.61,0.25748300000000002,2.7356999999999998E-3,187.32]
[null,"Residential Electricity",2015,2038000,1688000,38920,180.61,0.25748300000000002,2.7356999999999998E-3,187.32]
[null,"Electric Utility Steam Coal",2015,1022000,1021000,15590,1.8048999999999999,0.14106285999999998,3.4603000000000001E-5,6.0683999999999996]
[null,"Metallurgical Coal",2015,1022000,1021000,15590,1.8048999999999999,0.14106285999999998,3.4603000000000001E-5,6.0683999999999996]
[null,"Other Industrial Coal",2015,1022000,1021000,15590,1.8048999999999999,0.14106285999999998,3.4603000000000001E-5,6.0683999999999996]
[null,"Retail Diesel",2015,1210000,1204000,1053000,18.527999999999999,0.16494200000000001,2.9771000000000002E-4,23.579000000000001]
[null,"E85 Ethanol",2015,1642000,724000,290600,41.042999999999999,0.1162,2.7609999999999999E-2,48.36]
[null,"Retail Gasoline",2015,1252000,1245000,1081000,24.462,0.17067199999999999,3.8633E-4,29.811999999999998]
[null,"Woody Biomass",2015,1191000,53390,29910,3.9701,8.6864999999999998E-3,-3.8232459999999998E-3,3.2326999999999999]
[null,"Woody Biomass B2A",2015,1191000,53390,29910,3.9701,8.6864999999999998E-3,-3.8232459999999998E-3,3.2326999999999999]
[null,"Woody Biomass MYPP",2015,1191000,53390,29910,3.9701,8.6864999999999998E-3,-3.8232459999999998E-3,3.2326999999999999]
[null,"Steam",2015,1385000,1384000,5105,78.707400000000007,0.27494000000000002,2.3330999999999998E-3,87.730800000000002]
[null,"Commercial Natural Gas",2020,1093000,1092000,3993,5.7995000000000001,0.18462100000000001,8.6209999999999998E-4,11.6227]
[null,"Industrial Natural Gas",2020,1093000,1092000,3993,5.7995000000000001,0.18462100000000001,8.6209999999999998E-4,11.6227]
[null,"Electric Utility Natural Gas",2020,1093000,1092000,3993,5.7995000000000001,0.18462100000000001,8.6209999999999998E-4,11.6227]
[null,"Residential Natural Gas",2020,1093000,1092000,3993,5.7995000000000001,0.18462100000000001,8.6209999999999998E-4,11.6227]
[null,"Bio Methane",2020,-1185000,0,0,-85.800000000000011,0.54700000000000004,-1.8286999999999999E-3,-70.08]
[null,"Commercial Electricity",2020,1866000,1484000,26490,161.61000000000001,0.22423899999999999,2.4153E-3,168.06]
[null,"Industrial Electricity",2020,1866000,1484000,26490,161.61000000000001,0.22423899999999999,2.4153E-3,168.06]
[null,"Residential Electricity",2020,1866000,1484000,26490,161.61000000000001,0.22423899999999999,2.4153E-3,168.06]
[null,"Electric Utility Steam Coal",2020,1022000,1021000,15530,1.7706,0.14096106,3.4058000000000005E-5,6.0322999999999993]
[null,"Metallurgical Coal",2020,1022000,1021000,15530,1.7706,0.14096106,3.4058000000000005E-5,6.0322999999999993]
[null,"Other Industrial Coal",2020,1022000,1021000,15530,1.7706,0.14096106,3.4058000000000005E-5,6.0322999999999993]
[null,"Retail Diesel",2020,1211000,1205000,1052000,18.605999999999998,0.162991,3.0018999999999998E-4,23.607999999999997]
[null,"E85 Ethanol",2020,1591000,703100,286400,39.366999999999997,0.11210000000000001,2.5360000000000001E-2,46.16]
[null,"Retail Gasoline",2020,1252000,1245000,1078000,24.533999999999999,0.16861900000000002,3.8906999999999999E-4,29.833999999999996]
[null,"Woody Biomass",2020,1190000,52190,29260,3.8701999999999996,8.4535000000000009E-3,-3.824488E-3,3.1251000000000002]
[null,"Woody Biomass B2A",2020,1190000,52190,29260,3.8701999999999996,8.4535000000000009E-3,-3.824488E-3,3.1251000000000002]
[null,"Woody Biomass MYPP",2020,1190000,52190,29260,3.8701999999999996,8.4535000000000009E-3,-3.824488E-3,3.1251000000000002]
[null,"Steam",2020,1384000,1384000,5066,78.656899999999993,0.27494000000000002,2.3319E-3,87.680599999999998]
[null,"Commercial Natural Gas",2025,1093000,1092000,3984,5.7702,0.18462100000000001,8.6159999999999991E-4,11.5953]
[null,"Industrial Natural Gas",2025,1093000,1092000,3984,5.7702,0.18462100000000001,8.6159999999999991E-4,11.5953]
[null,"Electric Utility Natural Gas",2025,1093000,1092000,3984,5.7702,0.18462100000000001,8.6159999999999991E-4,11.5953]
[null,"Residential Natural Gas",2025,1093000,1092000,3984,5.7702,0.18462100000000001,8.6159999999999991E-4,11.5953]
[null,"Bio Methane",2025,-1185000,0,0,-85.800000000000011,0.54700000000000004,-1.8286999999999999E-3,-70.08]
[null,"Commercial Electricity",2025,1787000,1356000,23200,145.11000000000001,0.20658799999999999,2.1538999999999998E-3,150.89999999999998]
[null,"Industrial Electricity",2025,1787000,1356000,23200,145.11000000000001,0.20658799999999999,2.1538999999999998E-3,150.89999999999998]
[null,"Residential Electricity",2025,1787000,1356000,23200,145.11000000000001,0.20658799999999999,2.1538999999999998E-3,150.89999999999998]
[null,"Electric Utility Steam Coal",2025,1022000,1021000,15530,1.7374000000000001,0.14096106999999999,3.3522000000000002E-5,5.9969999999999999]
[null,"Metallurgical Coal",2025,1022000,1021000,15530,1.7374000000000001,0.14096106999999999,3.3522000000000002E-5,5.9969999999999999]
[null,"Other Industrial Coal",2025,1022000,1021000,15530,1.7374000000000001,0.14096106999999999,3.3522000000000002E-5,5.9969999999999999]
[null,"Retail Diesel",2025,1210000,1203000,1052000,18.323,0.16309799999999999,2.9605000000000001E-4,23.334]
[null,"E85 Ethanol",2025,1588000,698600,286300,38.775999999999996,0.1116,2.5360000000000001E-2,45.71]
[null,"Retail Gasoline",2025,1251000,1243000,1078000,24.223999999999997,0.16872600000000001,3.8451000000000002E-4,29.523000000000003]
[null,"Woody Biomass",2025,1190000,51790,29250,3.8201000000000001,8.410599999999999E-3,-3.8247120000000001E-3,3.0718000000000001]
[null,"Woody Biomass B2A",2025,1190000,51790,29250,3.8201000000000001,8.410599999999999E-3,-3.8247120000000001E-3,3.0718000000000001]
[null,"Woody Biomass MYPP",2025,1190000,51790,29250,3.8201000000000001,8.410599999999999E-3,-3.8247120000000001E-3,3.0718000000000001]
[null,"Steam",2025,1384000,1383000,5053,78.616100000000003,0.27494000000000002,2.3316999999999999E-3,87.639700000000005]
[null,"Commercial Natural Gas",2030,1092000,1092000,3981,5.7552000000000003,0.18462100000000001,8.6129999999999996E-4,11.5802]
[null,"Industrial Natural Gas",2030,1092000,1092000,3981,5.7552000000000003,0.18462100000000001,8.6129999999999996E-4,11.5802]
[null,"Electric Utility Natural Gas",2030,1092000,1092000,3981,5.7552000000000003,0.18462100000000001,8.6129999999999996E-4,11.5802]
[null,"Residential Natural Gas",2030,1092000,1092000,3981,5.7552000000000003,0.18462100000000001,8.6129999999999996E-4,11.5802]
[null,"Bio Methane",2030,-1185000,0,0,-85.800000000000011,0.54700000000000004,-1.8286999999999999E-3,-70.08]
[null,"Commercial Electricity",2030,1749000,1310000,19790,134.88,0.20275799999999999,1.9713E-3,140.09]
[null,"Industrial Electricity",2030,1749000,1310000,19790,134.88,0.20275799999999999,1.9713E-3,140.09]
[null,"Residential Electricity",2030,1749000,1310000,19790,134.88,0.20275799999999999,1.9713E-3,140.09]
[null,"Electric Utility Steam Coal",2030,1022000,1021000,15520,1.716,0.14096175,3.3149000000000004E-5,5.9754000000000005]
[null,"Metallurgical Coal",2030,1022000,1021000,15520,1.716,0.14096175,3.3149000000000004E-5,5.9754000000000005]
[null,"Other Industrial Coal",2030,1022000,1021000,15520,1.716,0.14096175,3.3149000000000004E-5,5.9754000000000005]
[null,"Retail Diesel",2030,1209000,1202000,1052000,18.120999999999999,0.16412299999999999,2.9339999999999998E-4,23.162000000000003]
[null,"E85 Ethanol",2030,1586000,697000,286200,38.404000000000003,0.1118,2.5350000000000001E-2,45.44]
[null,"Retail Gasoline",2030,1250000,1242000,1078000,24.006999999999998,0.16975200000000001,3.8147000000000002E-4,29.335999999999999]
[null,"Woody Biomass",2030,1190000,51650,29230,3.7881999999999998,8.4297E-3,-3.825901E-3,3.0377000000000001]
[null,"Woody Biomass B2A",2030,1190000,51650,29230,3.7881999999999998,8.4297E-3,-3.825901E-3,3.0377000000000001]
[null,"Woody Biomass MYPP",2030,1190000,51650,29230,3.7881999999999998,8.4297E-3,-3.825901E-3,3.0377000000000001]
[null,"Steam",2030,1384000,1383000,5048,78.598700000000008,0.27484000000000003,2.3306000000000004E-3,87.622100000000003]
[null,"Commercial Natural Gas",2035,1092000,1092000,3981,5.7552000000000003,0.18462100000000001,8.6129999999999996E-4,11.5802]
[null,"Industrial Natural Gas",2035,1092000,1092000,3981,5.7552000000000003,0.18462100000000001,8.6129999999999996E-4,11.5802]
[null,"Electric Utility Natural Gas",2035,1092000,1092000,3981,5.7552000000000003,0.18462100000000001,8.6129999999999996E-4,11.5802]
[null,"Residential Natural Gas",2035,1092000,1092000,3981,5.7552000000000003,0.18462100000000001,8.6129999999999996E-4,11.5802]
[null,"Bio Methane",2035,-1185000,0,0,-85.800000000000011,0.54700000000000004,-1.8286999999999999E-3,-70.08]
[null,"Commercial Electricity",2035,1745000,1314000,18650,132.69,0.204869,1.9257999999999999E-3,137.91999999999999]
[null,"Industrial Electricity",2035,1745000,1314000,18650,132.69,0.204869,1.9257999999999999E-3,137.91999999999999]
[null,"Residential Electricity",2035,1745000,1314000,18650,132.69,0.204869,1.9257999999999999E-3,137.91999999999999]
[null,"Electric Utility Steam Coal",2035,1022000,1021000,15520,1.7124999999999999,0.14096197999999999,3.3061000000000001E-5,5.9708000000000006]
[null,"Metallurgical Coal",2035,1022000,1021000,15520,1.7124999999999999,0.14096197999999999,3.3061000000000001E-5,5.9708000000000006]
[null,"Other Industrial Coal",2035,1022000,1021000,15520,1.7124999999999999,0.14096197999999999,3.3061000000000001E-5,5.9708000000000006]
[null,"Retail Diesel",2035,1209000,1202000,1052000,18.088999999999999,0.16412499999999999,2.9260000000000001E-4,23.119]
[null,"E85 Ethanol",2035,1586000,697100,286100,38.326999999999998,0.1118,2.5350000000000001E-2,45.39]
[null,"Retail Gasoline",2035,1250000,1242000,1078000,23.973999999999997,0.169854,3.8064000000000001E-4,29.302]
[null,"Woody Biomass",2035,1190000,51660,29230,3.7818000000000001,8.4370999999999995E-3,-3.8259590000000003E-3,3.0312999999999999]
[null,"Woody Biomass B2A",2035,1190000,51660,29230,3.7818000000000001,8.4370999999999995E-3,-3.8259590000000003E-3,3.0312999999999999]
[null,"Woody Biomass MYPP",2035,1190000,51660,29230,3.7818000000000001,8.4370999999999995E-3,-3.8259590000000003E-3,3.0312999999999999]
[null,"Steam",2035,1384000,1383000,5034,78.571100000000001,0.27494000000000002,2.3304000000000003E-3,87.594300000000004]
[null,"Commercial Natural Gas",2040,1092000,1092000,3975,5.7453000000000003,0.18462200000000001,8.6110000000000006E-4,11.577199999999999]
[null,"Industrial Natural Gas",2040,1092000,1092000,3975,5.7453000000000003,0.18462200000000001,8.6110000000000006E-4,11.577199999999999]
[null,"Electric Utility Natural Gas",2040,1092000,1092000,3975,5.7453000000000003,0.18462200000000001,8.6110000000000006E-4,11.577199999999999]
[null,"Residential Natural Gas",2040,1092000,1092000,3975,5.7453000000000003,0.18462200000000001,8.6110000000000006E-4,11.577199999999999]
[null,"Bio Methane",2040,-1185000,0,0,-85.800000000000011,0.54700000000000004,-1.8286999999999999E-3,-70.08]
[null,"Commercial Electricity",2040,1732000,1300000,17320,129.32,0.20383000000000001,1.8644999999999998E-3,134.37]
[null,"Industrial Electricity",2040,1732000,1300000,17320,129.32,0.20383000000000001,1.8644999999999998E-3,134.37]
[null,"Residential Electricity",2040,1732000,1300000,17320,129.32,0.20383000000000001,1.8644999999999998E-3,134.37]
[null,"Electric Utility Steam Coal",2040,1022000,1021000,15510,1.7054,0.14096210000000001,3.2928999999999996E-5,5.9637000000000002]
[null,"Metallurgical Coal",2040,1022000,1021000,15510,1.7054,0.14096210000000001,3.2928999999999996E-5,5.9637000000000002]
[null,"Other Industrial Coal",2040,1022000,1021000,15510,1.7054,0.14096210000000001,3.2928999999999996E-5,5.9637000000000002]
[null,"Retail Diesel",2040,1209000,1202000,1052000,18.032,0.16412599999999999,2.9167E-4,23.062000000000001]
[null,"E85 Ethanol",2040,1586000,696600,286100,38.200000000000003,0.1118,2.5350000000000001E-2,45.3]
[null,"Retail Gasoline",2040,1250000,1242000,1078000,23.914999999999999,0.16985499999999998,3.7957999999999997E-4,29.232999999999997]
[null,"Woody Biomass",2040,1190000,51610,29220,3.7715999999999998,8.4332999999999995E-3,-3.8260220000000001E-3,3.02]
[null,"Woody Biomass B2A",2040,1190000,51610,29220,3.7715999999999998,8.4332999999999995E-3,-3.8260220000000001E-3,3.02]
[null,"Woody Biomass MYPP",2040,1190000,51610,29220,3.7715999999999998,8.4332999999999995E-3,-3.8260220000000001E-3,3.02]
[null,"Steam",2040,1384000,1383000,5034,78.571100000000001,0.27494000000000002,2.3304000000000003E-3,87.594300000000004]
[null,"Commercial Natural Gas",2045,1092000,1092000,3972,5.7410000000000005,0.18462200000000001,8.6110000000000006E-4,11.565900000000001]
[null,"Industrial Natural Gas",2045,1092000,1092000,3972,5.7410000000000005,0.18462200000000001,8.6110000000000006E-4,11.565900000000001]
[null,"Electric Utility Natural Gas",2045,1092000,1092000,3972,5.7410000000000005,0.18462200000000001,8.6110000000000006E-4,11.565900000000001]
[null,"Residential Natural Gas",2045,1092000,1092000,3972,5.7410000000000005,0.18462200000000001,8.6110000000000006E-4,11.565900000000001]
[null,"Bio Methane",2045,-1185000,0,0,-85.800000000000011,0.54700000000000004,-1.8286999999999999E-3,-70.08]
[null,"Commercial Electricity",2045,1724000,1293000,15580,126.71000000000001,0.203795,1.8165E-3,131.63]
[null,"Industrial Electricity",2045,1724000,1293000,15580,126.71000000000001,0.203795,1.8165E-3,131.63]
[null,"Residential Electricity",2045,1724000,1293000,15580,126.71000000000001,0.203795,1.8165E-3,131.63]
[null,"Electric Utility Steam Coal",2045,1022000,1021000,15510,1.6997,0.14096223999999999,3.2833999999999998E-5,5.9580000000000002]
[null,"Metallurgical Coal",2045,1022000,1021000,15510,1.6997,0.14096223999999999,3.2833999999999998E-5,5.9580000000000002]
[null,"Other Industrial Coal",2045,1022000,1021000,15510,1.6997,0.14096223999999999,3.2833999999999998E-5,5.9580000000000002]
[null,"Retail Diesel",2045,1209000,1202000,1052000,17.989000000000001,0.164127,2.9079000000000003E-4,23.018999999999998]
[null,"E85 Ethanol",2045,1586000,696300,286000,38.110999999999997,0.1118,2.5350000000000001E-2,45.23]
[null,"Retail Gasoline",2045,1249000,1242000,1078000,23.861000000000001,0.16985599999999998,3.7867E-4,29.189]
[null,"Woody Biomass",2045,1190000,51590,29220,3.7631000000000001,8.4335E-3,-3.8260760000000003E-3,3.0114000000000001]
[null,"Woody Biomass B2A",2045,1190000,51590,29220,3.7631000000000001,8.4335E-3,-3.8260760000000003E-3,3.0114000000000001]
[null,"Woody Biomass MYPP",2045,1190000,51590,29220,3.7631000000000001,8.4335E-3,-3.8260760000000003E-3,3.0114000000000001]
[null,"Steam",2045,1384000,1383000,5034,78.571100000000001,0.27494000000000002,2.3304000000000003E-3,87.594300000000004]
[null,"Commercial Natural Gas",2050,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Industrial Natural Gas",2050,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Electric Utility Natural Gas",2050,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Residential Natural Gas",2050,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Bio Methane",2050,-1185000,0,0,-85.800000000000011,0.54700000000000004,-1.8286999999999999E-3,-70.08]
[null,"Commercial Electricity",2050,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Industrial Electricity",2050,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Residential Electricity",2050,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Electric Utility Steam Coal",2050,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Metallurgical Coal",2050,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Other Industrial Coal",2050,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Retail Diesel",2050,1209000,1202000,1052000,17.969000000000001,0.164128,2.9025999999999998E-4,22.988]
[null,"E85 Ethanol",2050,1585000,696300,286000,38.049999999999997,0.1118,2.5350000000000001E-2,45.19]
[null,"Retail Gasoline",2050,1249000,1242000,1078000,23.84,0.16985799999999998,3.7813000000000001E-4,29.157000000000004]
[null,"Woody Biomass",2050,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Woody Biomass B2A",2050,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Woody Biomass MYPP",2050,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Steam",2050,1384000,1383000,5034,78.571100000000001,0.27494000000000002,2.3304000000000003E-3,87.594300000000004]
[null,"Commercial Natural Gas",2055,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Industrial Natural Gas",2055,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Electric Utility Natural Gas",2055,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Residential Natural Gas",2055,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Bio Methane",2055,-1185000,0,0,-85.800000000000011,0.54700000000000004,-1.8286999999999999E-3,-70.08]
[null,"Commercial Electricity",2055,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Industrial Electricity",2055,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Residential Electricity",2055,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Electric Utility Steam Coal",2055,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Metallurgical Coal",2055,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Other Industrial Coal",2055,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Retail Diesel",2055,1209000,1202000,1052000,17.969000000000001,0.164128,2.9025999999999998E-4,22.988]
[null,"E85 Ethanol",2055,1585000,696300,286000,38.049999999999997,0.1118,2.5350000000000001E-2,45.19]
[null,"Retail Gasoline",2055,1249000,1242000,1078000,23.84,0.16985799999999998,3.7813000000000001E-4,29.157000000000004]
[null,"Woody Biomass",2055,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Woody Biomass B2A",2055,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Woody Biomass MYPP",2055,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Steam",2055,1384000,1383000,5034,78.571100000000001,0.27494000000000002,2.3304000000000003E-3,87.594300000000004]
[null,"Commercial Natural Gas",2060,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Industrial Natural Gas",2060,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Electric Utility Natural Gas",2060,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Residential Natural Gas",2060,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Bio Methane",2060,-1185000,0,0,-85.800000000000011,0.54700000000000004,-1.8286999999999999E-3,-70.08]
[null,"Commercial Electricity",2060,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Industrial Electricity",2060,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Residential Electricity",2060,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Electric Utility Steam Coal",2060,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Metallurgical Coal",2060,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Other Industrial Coal",2060,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Retail Diesel",2060,1209000,1202000,1052000,17.969000000000001,0.164128,2.9025999999999998E-4,22.988]
[null,"E85 Ethanol",2060,1585000,696300,286000,38.049999999999997,0.1118,2.5350000000000001E-2,45.19]
[null,"Retail Gasoline",2060,1249000,1242000,1078000,23.84,0.16985799999999998,3.7813000000000001E-4,29.157000000000004]
[null,"Woody Biomass",2060,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Woody Biomass B2A",2060,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Woody Biomass MYPP",2060,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Steam",2060,1384000,1383000,5034,78.571100000000001,0.27494000000000002,2.3304000000000003E-3,87.594300000000004]
[null,"Commercial Natural Gas",2065,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Industrial Natural Gas",2065,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Electric Utility Natural Gas",2065,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Residential Natural Gas",2065,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Bio Methane",2065,-1185000,0,0,-85.800000000000011,0.54700000000000004,-1.8286999999999999E-3,-70.08]
[null,"Commercial Electricity",2065,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Industrial Electricity",2065,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Residential Electricity",2065,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Electric Utility Steam Coal",2065,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Metallurgical Coal",2065,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Other Industrial Coal",2065,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Retail Diesel",2065,1209000,1202000,1052000,17.969000000000001,0.164128,2.9025999999999998E-4,22.988]
[null,"E85 Ethanol",2065,1585000,696300,286000,38.049999999999997,0.1118,2.5350000000000001E-2,45.19]
[null,"Retail Gasoline",2065,1249000,1242000,1078000,23.84,0.16985799999999998,3.7813000000000001E-4,29.157000000000004]
[null,"Woody Biomass",2065,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Woody Biomass B2A",2065,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Woody Biomass MYPP",2065,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Steam",2065,1384000,1383000,5034,78.571100000000001,0.27494000000000002,2.3304000000000003E-3,87.594300000000004]
[null,"Commercial Natural Gas",2070,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Industrial Natural Gas",2070,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Electric Utility Natural Gas",2070,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Residential Natural Gas",2070,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Bio Methane",2070,-1185000,0,0,-85.800000000000011,0.54700000000000004,-1.8286999999999999E-3,-70.08]
[null,"Commercial Electricity",2070,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Industrial Electricity",2070,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Residential Electricity",2070,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Electric Utility Steam Coal",2070,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Metallurgical Coal",2070,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Other Industrial Coal",2070,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Retail Diesel",2070,1209000,1202000,1052000,17.969000000000001,0.164128,2.9025999999999998E-4,22.988]
[null,"E85 Ethanol",2070,1585000,696300,286000,38.049999999999997,0.1118,2.5350000000000001E-2,45.19]
[null,"Retail Gasoline",2070,1249000,1242000,1078000,23.84,0.16985799999999998,3.7813000000000001E-4,29.157000000000004]
[null,"Woody Biomass",2070,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Woody Biomass B2A",2070,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Woody Biomass MYPP",2070,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Steam",2070,1384000,1383000,5034,78.571100000000001,0.27494000000000002,2.3304000000000003E-3,87.594300000000004]
[null,"Commercial Natural Gas",2075,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Industrial Natural Gas",2075,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Electric Utility Natural Gas",2075,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Residential Natural Gas",2075,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Bio Methane",2075,-1185000,0,0,-85.800000000000011,0.54700000000000004,-1.8286999999999999E-3,-70.08]
[null,"Commercial Electricity",2075,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Industrial Electricity",2075,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Residential Electricity",2075,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Electric Utility Steam Coal",2075,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Metallurgical Coal",2075,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Other Industrial Coal",2075,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Retail Diesel",2075,1209000,1202000,1052000,17.969000000000001,0.164128,2.9025999999999998E-4,22.988]
[null,"E85 Ethanol",2075,1585000,696300,286000,38.049999999999997,0.1118,2.5350000000000001E-2,45.19]
[null,"Retail Gasoline",2075,1249000,1242000,1078000,23.84,0.16985799999999998,3.7813000000000001E-4,29.157000000000004]
[null,"Woody Biomass",2075,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Woody Biomass B2A",2075,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Woody Biomass MYPP",2075,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Steam",2075,1384000,1383000,5034,78.571100000000001,0.27494000000000002,2.3304000000000003E-3,87.594300000000004]
[null,"Commercial Natural Gas",2080,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Industrial Natural Gas",2080,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Electric Utility Natural Gas",2080,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Residential Natural Gas",2080,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Bio Methane",2080,-1185000,0,0,-85.800000000000011,0.54700000000000004,-1.8286999999999999E-3,-70.08]
[null,"Commercial Electricity",2080,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Industrial Electricity",2080,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Residential Electricity",2080,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Electric Utility Steam Coal",2080,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Metallurgical Coal",2080,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Other Industrial Coal",2080,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Retail Diesel",2080,1209000,1202000,1052000,17.969000000000001,0.164128,2.9025999999999998E-4,22.988]
[null,"E85 Ethanol",2080,1585000,696300,286000,38.049999999999997,0.1118,2.5350000000000001E-2,45.19]
[null,"Retail Gasoline",2080,1249000,1242000,1078000,23.84,0.16985799999999998,3.7813000000000001E-4,29.157000000000004]
[null,"Woody Biomass",2080,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Woody Biomass B2A",2080,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Woody Biomass MYPP",2080,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Steam",2080,1384000,1383000,5034,78.571100000000001,0.27494000000000002,2.3304000000000003E-3,87.594300000000004]
[null,"Commercial Natural Gas",2085,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Industrial Natural Gas",2085,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Electric Utility Natural Gas",2085,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Residential Natural Gas",2085,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Bio Methane",2085,-1185000,0,0,-85.800000000000011,0.54700000000000004,-1.8286999999999999E-3,-70.08]
[null,"Commercial Electricity",2085,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Industrial Electricity",2085,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Residential Electricity",2085,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Electric Utility Steam Coal",2085,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Metallurgical Coal",2085,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Other Industrial Coal",2085,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Retail Diesel",2085,1209000,1202000,1052000,17.969000000000001,0.164128,2.9025999999999998E-4,22.988]
[null,"E85 Ethanol",2085,1585000,696300,286000,38.049999999999997,0.1118,2.5350000000000001E-2,45.19]
[null,"Retail Gasoline",2085,1249000,1242000,1078000,23.84,0.16985799999999998,3.7813000000000001E-4,29.157000000000004]
[null,"Woody Biomass",2085,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Woody Biomass B2A",2085,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Woody Biomass MYPP",2085,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Steam",2085,1384000,1383000,5034,78.571100000000001,0.27494000000000002,2.3304000000000003E-3,87.594300000000004]
[null,"Commercial Natural Gas",2090,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Industrial Natural Gas",2090,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Electric Utility Natural Gas",2090,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Residential Natural Gas",2090,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Bio Methane",2090,-1185000,0,0,-85.800000000000011,0.54700000000000004,-1.8286999999999999E-3,-70.08]
[null,"Commercial Electricity",2090,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Industrial Electricity",2090,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Residential Electricity",2090,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Electric Utility Steam Coal",2090,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Metallurgical Coal",2090,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Other Industrial Coal",2090,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Retail Diesel",2090,1209000,1202000,1052000,17.969000000000001,0.164128,2.9025999999999998E-4,22.988]
[null,"E85 Ethanol",2090,1585000,696300,286000,38.049999999999997,0.1118,2.5350000000000001E-2,45.19]
[null,"Retail Gasoline",2090,1249000,1242000,1078000,23.84,0.16985799999999998,3.7813000000000001E-4,29.157000000000004]
[null,"Woody Biomass",2090,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Woody Biomass B2A",2090,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Woody Biomass MYPP",2090,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Steam",2090,1384000,1383000,5034,78.571100000000001,0.27494000000000002,2.3304000000000003E-3,87.594300000000004]
[null,"Commercial Natural Gas",2095,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Industrial Natural Gas",2095,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Electric Utility Natural Gas",2095,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Residential Natural Gas",2095,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Bio Methane",2095,-1185000,0,0,-85.800000000000011,0.54700000000000004,-1.8286999999999999E-3,-70.08]
[null,"Commercial Electricity",2095,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Industrial Electricity",2095,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Residential Electricity",2095,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Electric Utility Steam Coal",2095,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Metallurgical Coal",2095,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Other Industrial Coal",2095,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Retail Diesel",2095,1209000,1202000,1052000,17.969000000000001,0.164128,2.9025999999999998E-4,22.988]
[null,"E85 Ethanol",2095,1585000,696300,286000,38.049999999999997,0.1118,2.5350000000000001E-2,45.19]
[null,"Retail Gasoline",2095,1249000,1242000,1078000,23.84,0.16985799999999998,3.7813000000000001E-4,29.157000000000004]
[null,"Woody Biomass",2095,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Woody Biomass B2A",2095,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Woody Biomass MYPP",2095,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Steam",2095,1384000,1383000,5034,78.571100000000001,0.27494000000000002,2.3304000000000003E-3,87.594300000000004]
[null,"Commercial Natural Gas",2100,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Industrial Natural Gas",2100,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Electric Utility Natural Gas",2100,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Residential Natural Gas",2100,1092000,1092000,3971,5.7390999999999996,0.18462200000000001,8.61E-4,11.5648]
[null,"Bio Methane",2100,-1185000,0,0,-85.800000000000011,0.54700000000000004,-1.8286999999999999E-3,-70.08]
[null,"Commercial Electricity",2100,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Industrial Electricity",2100,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Residential Electricity",2100,1721000,1293000,15050,125.08,0.20477100000000001,1.7827000000000001E-3,129.82]
[null,"Electric Utility Steam Coal",2100,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Metallurgical Coal",2100,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Other Industrial Coal",2100,1022000,1021000,15510,1.6964999999999999,0.14096238999999999,3.2765999999999998E-5,5.9536999999999995]
[null,"Retail Diesel",2100,1209000,1202000,1052000,17.969000000000001,0.164128,2.9025999999999998E-4,22.988]
[null,"E85 Ethanol",2100,1585000,696300,286000,38.049999999999997,0.1118,2.5350000000000001E-2,45.19]
[null,"Retail Gasoline",2100,1249000,1242000,1078000,23.84,0.16985799999999998,3.7813000000000001E-4,29.157000000000004]
[null,"Woody Biomass",2100,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Woody Biomass B2A",2100,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Woody Biomass MYPP",2100,1190000,51590,29220,3.7582,8.4366999999999984E-3,-3.8261190000000002E-3,3.0054000000000003]
[null,"Steam",2100,1384000,1383000,5034,78.571100000000001,0.27494000000000002,2.3304000000000003E-3,87.594300000000004]

{"sheet":"Debt Financing Calculations","index":15,"n_rows":57,"n_cols":7,"rows_kept":57,"cut":false,"hidden":false,"merged":[[11,1,11,6]]}
["Debt Financing Calculations"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["ANNUAL LOAN CALCULATION (if debt financing is assumed)"]
[]
["Analysis Year","Loan Year","Principal Owed","Annual Payment","Interest","Principal Payment","New Principal"]
[{"$f":"'Cash Flow Analysis'!B65","v":1},{"$f":"IF(B13=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A14=1,1,IF(A13=debt_period,\"\",B13+1))))","v":1},{"$f":"IF(OR(A14=\"\",B14=\"\",B14=\"N/A\"),\"\",IF(B14=1,-'Cash Flow Analysis'!G65,IF(B14=\"N/A\",0,G13)))","v":1267062.1105808259},{"$f":"IF(debt_period=0,\nE14+F14,\nIF(OR(A14=\"\",B14=\"\",B14=\"N/A\"),\"\",IF(B14=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G65),IF(G13=0,\"\",D13))))","v":46881.298091490557},{"$f":"IF(OR(A14=\"\",B14=\"\",B14=\"N/A\"),\"\",C14*debt_interest)","v":46881.298091490557},{"$f":"IF(debt_period=0,\nIF(B14=(anal_period+construct),0,0),\nIF(OR(A14=\"\",B14=\"\",B14=\"N/A\"),\"\",D14-E14))","v":0},{"$f":"IF(OR(A14=\"\",B14=\"\",B14=\"N/A\"),\"\",C14-F14)","v":1267062.1105808259}]
[{"$f":"'Cash Flow Analysis'!B66","v":2},{"$f":"IF(B14=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A15=1,1,IF(A14=debt_period,\"\",B14+1))))","v":2},{"$f":"IF(OR(A15=\"\",B15=\"\",B15=\"N/A\"),\"\",IF(B15=1,-'Cash Flow Analysis'!G66,IF(B15=\"N/A\",0,G14)))","v":1267062.1105808259},{"$f":"IF(debt_period=0,\nE15+F15,\nIF(OR(A15=\"\",B15=\"\",B15=\"N/A\"),\"\",IF(B15=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G66),IF(G14=0,\"\",D14))))","v":46881.298091490557},46881.298091490557,{"$f":"IF(debt_period=0,\nIF(B15=(anal_period+construct),C14,0),\nIF(OR(A15=\"\",B15=\"\",B15=\"N/A\"),\"\",D15-E15))","v":0},1267062.1105808259]
[{"$f":"'Cash Flow Analysis'!B67","v":3},{"$f":"IF(B15=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A16=1,1,IF(A15=debt_period,\"\",B15+1))))","v":3},{"$f":"IF(OR(A16=\"\",B16=\"\",B16=\"N/A\"),\"\",IF(B16=1,-'Cash Flow Analysis'!G67,IF(B16=\"N/A\",0,G15)))","v":1267062.1105808259},{"$f":"IF(debt_period=0,\nE16+F16,\nIF(OR(A16=\"\",B16=\"\",B16=\"N/A\"),\"\",IF(B16=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G67),IF(G15=0,\"\",D15))))","v":46881.298091490557},46881.298091490557,{"$f":"IF(debt_period=0,\nIF(B16=(anal_period+construct),C16,0),\nIF(OR(A16=\"\",B16=\"\",B16=\"N/A\"),\"\",D16-E16))","v":0},1267062.1105808259]
[{"$f":"'Cash Flow Analysis'!B68","v":4},{"$f":"IF(B16=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A17=1,1,IF(A16=debt_period,\"\",B16+1))))","v":4},{"$f":"IF(OR(A17=\"\",B17=\"\",B17=\"N/A\"),\"\",IF(B17=1,-'Cash Flow Analysis'!G68,IF(B17=\"N/A\",0,G16)))","v":1267062.1105808259},{"$f":"IF(debt_period=0,\nE17+F17,\nIF(OR(A17=\"\",B17=\"\",B17=\"N/A\"),\"\",IF(B17=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G68),IF(G16=0,\"\",D16))))","v":46881.298091490557},46881.298091490557,0,1267062.1105808259]
[{"$f":"'Cash Flow Analysis'!B69","v":5},{"$f":"IF(B17=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A18=1,1,IF(A17=debt_period,\"\",B17+1))))","v":5},{"$f":"IF(OR(A18=\"\",B18=\"\",B18=\"N/A\"),\"\",IF(B18=1,-'Cash Flow Analysis'!G69,IF(B18=\"N/A\",0,G17)))","v":1267062.1105808259},{"$f":"IF(debt_period=0,\nE18+F18,\nIF(OR(A18=\"\",B18=\"\",B18=\"N/A\"),\"\",IF(B18=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G69),IF(G17=0,\"\",D17))))","v":46881.298091490557},46881.298091490557,0,1267062.1105808259]
[{"$f":"'Cash Flow Analysis'!B70","v":6},{"$f":"IF(B18=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A19=1,1,IF(A18=debt_period,\"\",B18+1))))","v":6},{"$f":"IF(OR(A19=\"\",B19=\"\",B19=\"N/A\"),\"\",IF(B19=1,-'Cash Flow Analysis'!G70,IF(B19=\"N/A\",0,G18)))","v":1267062.1105808259},{"$f":"IF(debt_period=0,\nE19+F19,\nIF(OR(A19=\"\",B19=\"\",B19=\"N/A\"),\"\",IF(B19=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G70),IF(G18=0,\"\",D18))))","v":46881.298091490557},46881.298091490557,0,1267062.1105808259]
[{"$f":"'Cash Flow Analysis'!B71","v":7},{"$f":"IF(B19=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A20=1,1,IF(A19=debt_period,\"\",B19+1))))","v":7},{"$f":"IF(OR(A20=\"\",B20=\"\",B20=\"N/A\"),\"\",IF(B20=1,-'Cash Flow Analysis'!G71,IF(B20=\"N/A\",0,G19)))","v":1267062.1105808259},{"$f":"IF(debt_period=0,\nE20+F20,\nIF(OR(A20=\"\",B20=\"\",B20=\"N/A\"),\"\",IF(B20=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G71),IF(G19=0,\"\",D19))))","v":46881.298091490557},46881.298091490557,0,1267062.1105808259]
[{"$f":"'Cash Flow Analysis'!B72","v":8},{"$f":"IF(B20=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A21=1,1,IF(A20=debt_period,\"\",B20+1))))","v":8},{"$f":"IF(OR(A21=\"\",B21=\"\",B21=\"N/A\"),\"\",IF(B21=1,-'Cash Flow Analysis'!G72,IF(B21=\"N/A\",0,G20)))","v":1267062.1105808259},{"$f":"IF(debt_period=0,\nE21+F21,\nIF(OR(A21=\"\",B21=\"\",B21=\"N/A\"),\"\",IF(B21=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G72),IF(G20=0,\"\",D20))))","v":46881.298091490557},46881.298091490557,0,1267062.1105808259]
[{"$f":"'Cash Flow Analysis'!B73","v":9},{"$f":"IF(B21=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A22=1,1,IF(A21=debt_period,\"\",B21+1))))","v":9},{"$f":"IF(OR(A22=\"\",B22=\"\",B22=\"N/A\"),\"\",IF(B22=1,-'Cash Flow Analysis'!G73,IF(B22=\"N/A\",0,G21)))","v":1267062.1105808259},{"$f":"IF(debt_period=0,\nE22+F22,\nIF(OR(A22=\"\",B22=\"\",B22=\"N/A\"),\"\",IF(B22=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G73),IF(G21=0,\"\",D21))))","v":46881.298091490557},46881.298091490557,0,1267062.1105808259]
[{"$f":"'Cash Flow Analysis'!B74","v":10},{"$f":"IF(B22=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A23=1,1,IF(A22=debt_period,\"\",B22+1))))","v":10},{"$f":"IF(OR(A23=\"\",B23=\"\",B23=\"N/A\"),\"\",IF(B23=1,-'Cash Flow Analysis'!G74,IF(B23=\"N/A\",0,G22)))","v":1267062.1105808259},{"$f":"IF(debt_period=0,\nE23+F23,\nIF(OR(A23=\"\",B23=\"\",B23=\"N/A\"),\"\",IF(B23=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G74),IF(G22=0,\"\",D22))))","v":46881.298091490557},46881.298091490557,0,1267062.1105808259]
[{"$f":"'Cash Flow Analysis'!B75","v":11},{"$f":"IF(B23=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A24=1,1,IF(A23=debt_period,\"\",B23+1))))","v":11},{"$f":"IF(OR(A24=\"\",B24=\"\",B24=\"N/A\"),\"\",IF(B24=1,-'Cash Flow Analysis'!G75,IF(B24=\"N/A\",0,G23)))","v":1267062.1105808259},{"$f":"IF(debt_period=0,\nE24+F24,\nIF(OR(A24=\"\",B24=\"\",B24=\"N/A\"),\"\",IF(B24=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G75),IF(G23=0,\"\",D23))))","v":46881.298091490557},46881.298091490557,0,1267062.1105808259]
[{"$f":"'Cash Flow Analysis'!B76","v":12},{"$f":"IF(B24=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A25=1,1,IF(A24=debt_period,\"\",B24+1))))","v":12},{"$f":"IF(OR(A25=\"\",B25=\"\",B25=\"N/A\"),\"\",IF(B25=1,-'Cash Flow Analysis'!G76,IF(B25=\"N/A\",0,G24)))","v":1267062.1105808259},{"$f":"IF(debt_period=0,\nE25+F25,\nIF(OR(A25=\"\",B25=\"\",B25=\"N/A\"),\"\",IF(B25=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G76),IF(G24=0,\"\",D24))))","v":46881.298091490557},46881.298091490557,0,1267062.1105808259]
[{"$f":"'Cash Flow Analysis'!B77","v":13},{"$f":"IF(B25=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A26=1,1,IF(A25=debt_period,\"\",B25+1))))","v":13},{"$f":"IF(OR(A26=\"\",B26=\"\",B26=\"N/A\"),\"\",IF(B26=1,-'Cash Flow Analysis'!G77,IF(B26=\"N/A\",0,G25)))","v":1267062.1105808259},{"$f":"IF(debt_period=0,\nE26+F26,\nIF(OR(A26=\"\",B26=\"\",B26=\"N/A\"),\"\",IF(B26=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G77),IF(G25=0,\"\",D25))))","v":46881.298091490557},46881.298091490557,0,1267062.1105808259]
[{"$f":"'Cash Flow Analysis'!B78","v":14},{"$f":"IF(B26=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A27=1,1,IF(A26=debt_period,\"\",B26+1))))","v":14},{"$f":"IF(OR(A27=\"\",B27=\"\",B27=\"N/A\"),\"\",IF(B27=1,-'Cash Flow Analysis'!G78,IF(B27=\"N/A\",0,G26)))","v":1267062.1105808259},{"$f":"IF(debt_period=0,\nE27+F27,\nIF(OR(A27=\"\",B27=\"\",B27=\"N/A\"),\"\",IF(B27=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G78),IF(G26=0,\"\",D26))))","v":46881.298091490557},46881.298091490557,0,1267062.1105808259]
[{"$f":"'Cash Flow Analysis'!B79","v":15},{"$f":"IF(B27=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A28=1,1,IF(A27=debt_period,\"\",B27+1))))","v":15},{"$f":"IF(OR(A28=\"\",B28=\"\",B28=\"N/A\"),\"\",IF(B28=1,-'Cash Flow Analysis'!G79,IF(B28=\"N/A\",0,G27)))","v":1267062.1105808259},{"$f":"IF(debt_period=0,\nE28+F28,\nIF(OR(A28=\"\",B28=\"\",B28=\"N/A\"),\"\",IF(B28=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G79),IF(G27=0,\"\",D27))))","v":46881.298091490557},46881.298091490557,0,1267062.1105808259]
[{"$f":"'Cash Flow Analysis'!B80","v":16},{"$f":"IF(B28=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A29=1,1,IF(A28=debt_period,\"\",B28+1))))","v":16},{"$f":"IF(OR(A29=\"\",B29=\"\",B29=\"N/A\"),\"\",IF(B29=1,-'Cash Flow Analysis'!G80,IF(B29=\"N/A\",0,G28)))","v":1267062.1105808259},{"$f":"IF(debt_period=0,\nE29+F29,\nIF(OR(A29=\"\",B29=\"\",B29=\"N/A\"),\"\",IF(B29=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G80),IF(G28=0,\"\",D28))))","v":46881.298091490557},46881.298091490557,0,1267062.1105808259]
[{"$f":"'Cash Flow Analysis'!B81","v":17},{"$f":"IF(B29=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A30=1,1,IF(A29=debt_period,\"\",B29+1))))","v":17},{"$f":"IF(OR(A30=\"\",B30=\"\",B30=\"N/A\"),\"\",IF(B30=1,-'Cash Flow Analysis'!G81,IF(B30=\"N/A\",0,G29)))","v":1267062.1105808259},{"$f":"IF(debt_period=0,\nE30+F30,\nIF(OR(A30=\"\",B30=\"\",B30=\"N/A\"),\"\",IF(B30=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G81),IF(G29=0,\"\",D29))))","v":46881.298091490557},46881.298091490557,0,1267062.1105808259]
[{"$f":"'Cash Flow Analysis'!B82","v":18},{"$f":"IF(B30=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A31=1,1,IF(A30=debt_period,\"\",B30+1))))","v":18},{"$f":"IF(OR(A31=\"\",B31=\"\",B31=\"N/A\"),\"\",IF(B31=1,-'Cash Flow Analysis'!G82,IF(B31=\"N/A\",0,G30)))","v":1267062.1105808259},{"$f":"IF(debt_period=0,\nE31+F31,\nIF(OR(A31=\"\",B31=\"\",B31=\"N/A\"),\"\",IF(B31=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G82),IF(G30=0,\"\",D30))))","v":46881.298091490557},46881.298091490557,0,1267062.1105808259]
[{"$f":"'Cash Flow Analysis'!B83","v":19},{"$f":"IF(B31=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A32=1,1,IF(A31=debt_period,\"\",B31+1))))","v":19},{"$f":"IF(OR(A32=\"\",B32=\"\",B32=\"N/A\"),\"\",IF(B32=1,-'Cash Flow Analysis'!G83,IF(B32=\"N/A\",0,G31)))","v":1267062.1105808259},{"$f":"IF(debt_period=0,\nE32+F32,\nIF(OR(A32=\"\",B32=\"\",B32=\"N/A\"),\"\",IF(B32=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G83),IF(G31=0,\"\",D31))))","v":46881.298091490557},46881.298091490557,0,1267062.1105808259]
[{"$f":"'Cash Flow Analysis'!B84","v":20},{"$f":"IF(B32=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A33=1,1,IF(A32=debt_period,\"\",B32+1))))","v":20},{"$f":"IF(OR(A33=\"\",B33=\"\",B33=\"N/A\"),\"\",IF(B33=1,-'Cash Flow Analysis'!G84,IF(B33=\"N/A\",0,G32)))","v":1267062.1105808259},{"$f":"IF(debt_period=0,\nE33+F33,\nIF(OR(A33=\"\",B33=\"\",B33=\"N/A\"),\"\",IF(B33=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G84),IF(G32=0,\"\",D32))))","v":46881.298091490557},46881.298091490557,0,1267062.1105808259]
[{"$f":"'Cash Flow Analysis'!B85","v":21},{"$f":"IF(B33=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A34=1,1,IF(A33=debt_period,\"\",B33+1))))","v":21},{"$f":"IF(OR(A34=\"\",B34=\"\",B34=\"N/A\"),\"\",IF(B34=1,-'Cash Flow Analysis'!G85,IF(B34=\"N/A\",0,G33)))","v":1267062.1105808259},{"$f":"IF(debt_period=0,\nE34+F34,\nIF(OR(A34=\"\",B34=\"\",B34=\"N/A\"),\"\",IF(B34=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G85),IF(G33=0,\"\",D33))))","v":1313943.4086723165},46881.298091490557,1267062.1105808259,0]
[{"$f":"'Cash Flow Analysis'!B86","v":""},{"$f":"IF(B34=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A35=1,1,IF(A34=debt_period,\"\",B34+1))))","v":22},{"$f":"IF(OR(A35=\"\",B35=\"\",B35=\"N/A\"),\"\",IF(B35=1,-'Cash Flow Analysis'!G86,IF(B35=\"N/A\",0,G34)))","v":""},{"$f":"IF(debt_period=0,\nE35+F35,\nIF(OR(A35=\"\",B35=\"\",B35=\"N/A\"),\"\",IF(B35=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G86),IF(G34=0,\"\",D34))))","v":{"$error":"#VALUE!"}},"",0,""]
[{"$f":"'Cash Flow Analysis'!B87","v":""},{"$f":"IF(B35=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A36=1,1,IF(A35=debt_period,\"\",B35+1))))","v":23},{"$f":"IF(OR(A36=\"\",B36=\"\",B36=\"N/A\"),\"\",IF(B36=1,-'Cash Flow Analysis'!G87,IF(B36=\"N/A\",0,G35)))","v":""},{"$f":"IF(debt_period=0,\nE36+F36,\nIF(OR(A36=\"\",B36=\"\",B36=\"N/A\"),\"\",IF(B36=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G87),IF(G35=0,\"\",D35))))","v":{"$error":"#VALUE!"}},"",0,""]
[{"$f":"'Cash Flow Analysis'!B88","v":""},{"$f":"IF(B36=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A37=1,1,IF(A36=debt_period,\"\",B36+1))))","v":24},{"$f":"IF(OR(A37=\"\",B37=\"\",B37=\"N/A\"),\"\",IF(B37=1,-'Cash Flow Analysis'!G88,IF(B37=\"N/A\",0,G36)))","v":""},{"$f":"IF(debt_period=0,\nE37+F37,\nIF(OR(A37=\"\",B37=\"\",B37=\"N/A\"),\"\",IF(B37=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G88),IF(G36=0,\"\",D36))))","v":{"$error":"#VALUE!"}},"",0,""]
[{"$f":"'Cash Flow Analysis'!B89","v":""},{"$f":"IF(B37=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A38=1,1,IF(A37=debt_period,\"\",B37+1))))","v":25},{"$f":"IF(OR(A38=\"\",B38=\"\",B38=\"N/A\"),\"\",IF(B38=1,-'Cash Flow Analysis'!G89,IF(B38=\"N/A\",0,G37)))","v":""},{"$f":"IF(debt_period=0,\nE38+F38,\nIF(OR(A38=\"\",B38=\"\",B38=\"N/A\"),\"\",IF(B38=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G89),IF(G37=0,\"\",D37))))","v":{"$error":"#VALUE!"}},"",0,""]
[{"$f":"'Cash Flow Analysis'!B90","v":""},{"$f":"IF(B38=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A39=1,1,IF(A38=debt_period,\"\",B38+1))))","v":26},{"$f":"IF(OR(A39=\"\",B39=\"\",B39=\"N/A\"),\"\",IF(B39=1,-'Cash Flow Analysis'!G90,IF(B39=\"N/A\",0,G38)))","v":""},{"$f":"IF(debt_period=0,\nE39+F39,\nIF(OR(A39=\"\",B39=\"\",B39=\"N/A\"),\"\",IF(B39=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G90),IF(G38=0,\"\",D38))))","v":{"$error":"#VALUE!"}},"",0,""]
[{"$f":"'Cash Flow Analysis'!B91","v":""},{"$f":"IF(B39=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A40=1,1,IF(A39=debt_period,\"\",B39+1))))","v":27},{"$f":"IF(OR(A40=\"\",B40=\"\",B40=\"N/A\"),\"\",IF(B40=1,-'Cash Flow Analysis'!G91,IF(B40=\"N/A\",0,G39)))","v":""},{"$f":"IF(debt_period=0,\nE40+F40,\nIF(OR(A40=\"\",B40=\"\",B40=\"N/A\"),\"\",IF(B40=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G91),IF(G39=0,\"\",D39))))","v":{"$error":"#VALUE!"}},"",0,""]
[{"$f":"'Cash Flow Analysis'!B92","v":""},{"$f":"IF(B40=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A41=1,1,IF(A40=debt_period,\"\",B40+1))))","v":28},{"$f":"IF(OR(A41=\"\",B41=\"\",B41=\"N/A\"),\"\",IF(B41=1,-'Cash Flow Analysis'!G92,IF(B41=\"N/A\",0,G40)))","v":""},{"$f":"IF(debt_period=0,\nE41+F41,\nIF(OR(A41=\"\",B41=\"\",B41=\"N/A\"),\"\",IF(B41=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G92),IF(G40=0,\"\",D40))))","v":{"$error":"#VALUE!"}},"",0,""]
[{"$f":"'Cash Flow Analysis'!B93","v":""},{"$f":"IF(B41=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A42=1,1,IF(A41=debt_period,\"\",B41+1))))","v":29},{"$f":"IF(OR(A42=\"\",B42=\"\",B42=\"N/A\"),\"\",IF(B42=1,-'Cash Flow Analysis'!G93,IF(B42=\"N/A\",0,G41)))","v":""},{"$f":"IF(debt_period=0,\nE42+F42,\nIF(OR(A42=\"\",B42=\"\",B42=\"N/A\"),\"\",IF(B42=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G93),IF(G41=0,\"\",D41))))","v":{"$error":"#VALUE!"}},"",0,""]
[{"$f":"'Cash Flow Analysis'!B94","v":""},{"$f":"IF(B42=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A43=1,1,IF(A42=debt_period,\"\",B42+1))))","v":30},{"$f":"IF(OR(A43=\"\",B43=\"\",B43=\"N/A\"),\"\",IF(B43=1,-'Cash Flow Analysis'!G94,IF(B43=\"N/A\",0,G42)))","v":""},{"$f":"IF(debt_period=0,\nE43+F43,\nIF(OR(A43=\"\",B43=\"\",B43=\"N/A\"),\"\",IF(B43=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G94),IF(G42=0,\"\",D42))))","v":{"$error":"#VALUE!"}},"",0,""]
[{"$f":"'Cash Flow Analysis'!B95","v":""},{"$f":"IF(B43=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A44=1,1,IF(A43=debt_period,\"\",B43+1))))","v":31},{"$f":"IF(OR(A44=\"\",B44=\"\",B44=\"N/A\"),\"\",IF(B44=1,-'Cash Flow Analysis'!G95,IF(B44=\"N/A\",0,G43)))","v":""},{"$f":"IF(debt_period=0,\nE44+F44,\nIF(OR(A44=\"\",B44=\"\",B44=\"N/A\"),\"\",IF(B44=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G95),IF(G43=0,\"\",D43))))","v":{"$error":"#VALUE!"}},"",0,""]
[{"$f":"'Cash Flow Analysis'!B96","v":""},{"$f":"IF(B44=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A45=1,1,IF(A44=debt_period,\"\",B44+1))))","v":32},{"$f":"IF(OR(A45=\"\",B45=\"\",B45=\"N/A\"),\"\",IF(B45=1,-'Cash Flow Analysis'!G96,IF(B45=\"N/A\",0,G44)))","v":""},{"$f":"IF(debt_period=0,\nE45+F45,\nIF(OR(A45=\"\",B45=\"\",B45=\"N/A\"),\"\",IF(B45=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G96),IF(G44=0,\"\",D44))))","v":{"$error":"#VALUE!"}},"",0,""]
[{"$f":"'Cash Flow Analysis'!B97","v":""},{"$f":"IF(B45=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A46=1,1,IF(A45=debt_period,\"\",B45+1))))","v":33},{"$f":"IF(OR(A46=\"\",B46=\"\",B46=\"N/A\"),\"\",IF(B46=1,-'Cash Flow Analysis'!G97,IF(B46=\"N/A\",0,G45)))","v":""},{"$f":"IF(debt_period=0,\nE46+F46,\nIF(OR(A46=\"\",B46=\"\",B46=\"N/A\"),\"\",IF(B46=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G97),IF(G45=0,\"\",D45))))","v":{"$error":"#VALUE!"}},"",0,""]
[{"$f":"'Cash Flow Analysis'!B98","v":""},{"$f":"IF(B46=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A47=1,1,IF(A46=debt_period,\"\",B46+1))))","v":34},{"$f":"IF(OR(A47=\"\",B47=\"\",B47=\"N/A\"),\"\",IF(B47=1,-'Cash Flow Analysis'!G98,IF(B47=\"N/A\",0,G46)))","v":""},{"$f":"IF(debt_period=0,\nE47+F47,\nIF(OR(A47=\"\",B47=\"\",B47=\"N/A\"),\"\",IF(B47=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G98),IF(G46=0,\"\",D46))))","v":{"$error":"#VALUE!"}},"",0,""]
[{"$f":"'Cash Flow Analysis'!B99","v":""},{"$f":"IF(B47=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A48=1,1,IF(A47=debt_period,\"\",B47+1))))","v":35},{"$f":"IF(OR(A48=\"\",B48=\"\",B48=\"N/A\"),\"\",IF(B48=1,-'Cash Flow Analysis'!G99,IF(B48=\"N/A\",0,G47)))","v":""},{"$f":"IF(debt_period=0,\nE48+F48,\nIF(OR(A48=\"\",B48=\"\",B48=\"N/A\"),\"\",IF(B48=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G99),IF(G47=0,\"\",D47))))","v":{"$error":"#VALUE!"}},"",0,""]
[{"$f":"'Cash Flow Analysis'!B100","v":""},{"$f":"IF(B48=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A49=1,1,IF(A48=debt_period,\"\",B48+1))))","v":36},{"$f":"IF(OR(A49=\"\",B49=\"\",B49=\"N/A\"),\"\",IF(B49=1,-'Cash Flow Analysis'!G100,IF(B49=\"N/A\",0,G48)))","v":""},{"$f":"IF(debt_period=0,\nE49+F49,\nIF(OR(A49=\"\",B49=\"\",B49=\"N/A\"),\"\",IF(B49=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G100),IF(G48=0,\"\",D48))))","v":{"$error":"#VALUE!"}},"",0,""]
[{"$f":"'Cash Flow Analysis'!B101","v":""},{"$f":"IF(B49=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A50=1,1,IF(A49=debt_period,\"\",B49+1))))","v":37},{"$f":"IF(OR(A50=\"\",B50=\"\",B50=\"N/A\"),\"\",IF(B50=1,-'Cash Flow Analysis'!G101,IF(B50=\"N/A\",0,G49)))","v":""},{"$f":"IF(debt_period=0,\nE50+F50,\nIF(OR(A50=\"\",B50=\"\",B50=\"N/A\"),\"\",IF(B50=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G101),IF(G49=0,\"\",D49))))","v":{"$error":"#VALUE!"}},"",0,""]
[{"$f":"'Cash Flow Analysis'!B102","v":""},{"$f":"IF(B50=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A51=1,1,IF(A50=debt_period,\"\",B50+1))))","v":38},{"$f":"IF(OR(A51=\"\",B51=\"\",B51=\"N/A\"),\"\",IF(B51=1,-'Cash Flow Analysis'!G102,IF(B51=\"N/A\",0,G50)))","v":""},{"$f":"IF(debt_period=0,\nE51+F51,\nIF(OR(A51=\"\",B51=\"\",B51=\"N/A\"),\"\",IF(B51=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G102),IF(G50=0,\"\",D50))))","v":{"$error":"#VALUE!"}},"",0,""]
[{"$f":"'Cash Flow Analysis'!B103","v":""},{"$f":"IF(B51=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A52=1,1,IF(A51=debt_period,\"\",B51+1))))","v":39},{"$f":"IF(OR(A52=\"\",B52=\"\",B52=\"N/A\"),\"\",IF(B52=1,-'Cash Flow Analysis'!G103,IF(B52=\"N/A\",0,G51)))","v":""},{"$f":"IF(debt_period=0,\nE52+F52,\nIF(OR(A52=\"\",B52=\"\",B52=\"N/A\"),\"\",IF(B52=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G103),IF(G51=0,\"\",D51))))","v":{"$error":"#VALUE!"}},"",0,""]
[{"$f":"'Cash Flow Analysis'!B104","v":""},{"$f":"IF(B52=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A53=1,1,IF(A52=debt_period,\"\",B52+1))))","v":40},{"$f":"IF(OR(A53=\"\",B53=\"\",B53=\"N/A\"),\"\",IF(B53=1,-'Cash Flow Analysis'!G104,IF(B53=\"N/A\",0,G52)))","v":""},{"$f":"IF(debt_period=0,\nE53+F53,\nIF(OR(A53=\"\",B53=\"\",B53=\"N/A\"),\"\",IF(B53=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G104),IF(G52=0,\"\",D52))))","v":{"$error":"#VALUE!"}},"",0,""]
[{"$f":"'Cash Flow Analysis'!B105","v":""},{"$f":"IF(B53=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A54=1,1,IF(A53=debt_period,\"\",B53+1))))","v":41},{"$f":"IF(OR(A54=\"\",B54=\"\",B54=\"N/A\"),\"\",IF(B54=1,-'Cash Flow Analysis'!G105,IF(B54=\"N/A\",0,G53)))","v":""},{"$f":"IF(debt_period=0,\nE54+F54,\nIF(OR(A54=\"\",B54=\"\",B54=\"N/A\"),\"\",IF(B54=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G105),IF(G53=0,\"\",D53))))","v":{"$error":"#VALUE!"}},"",0,""]
[{"$f":"'Cash Flow Analysis'!B106","v":""},{"$f":"IF(B54=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A55=1,1,IF(A54=debt_period,\"\",B54+1))))","v":42},{"$f":"IF(OR(A55=\"\",B55=\"\",B55=\"N/A\"),\"\",IF(B55=1,-'Cash Flow Analysis'!G106,IF(B55=\"N/A\",0,G54)))","v":""},{"$f":"IF(debt_period=0,\nE55+F55,\nIF(OR(A55=\"\",B55=\"\",B55=\"N/A\"),\"\",IF(B55=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G106),IF(G54=0,\"\",D54))))","v":{"$error":"#VALUE!"}},"",0,""]
[{"$f":"'Cash Flow Analysis'!B107","v":""},{"$f":"IF(B55=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A56=1,1,IF(A55=debt_period,\"\",B55+1))))","v":43},{"$f":"IF(OR(A56=\"\",B56=\"\",B56=\"N/A\"),\"\",IF(B56=1,-'Cash Flow Analysis'!G107,IF(B56=\"N/A\",0,G55)))","v":""},{"$f":"IF(debt_period=0,\nE56+F56,\nIF(OR(A56=\"\",B56=\"\",B56=\"N/A\"),\"\",IF(B56=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G107),IF(G55=0,\"\",D55))))","v":{"$error":"#VALUE!"}},"",0,""]
[{"$f":"'Cash Flow Analysis'!B108","v":""},{"$f":"IF(B56=\"\",\"\",IF('Cash Flow Analysis'!$B$31=0,\"N/A\",IF(A57=1,1,IF(A56=debt_period,\"\",B56+1))))","v":44},{"$f":"IF(OR(A57=\"\",B57=\"\",B57=\"N/A\"),\"\",IF(B57=1,-'Cash Flow Analysis'!G108,IF(B57=\"N/A\",0,G56)))","v":""},{"$f":"IF(F57=0,E57,\nIF(OR(A57=\"\",B57=\"\",B57=\"N/A\"),\"\",IF(B57=1,((debt_interest*(1+debt_interest)^debt_period)/((1+debt_interest)^debt_period-1))*(-'Cash Flow Analysis'!G108),IF(G56=0,\"\",D56))))","v":""},"",0,""]

{"sheet":"Depreciation","index":16,"n_rows":166,"n_cols":24,"rows_kept":166,"cut":false,"hidden":false,"merged":[[12,2,12,7],[143,0,143,1]]}
["Depreciation"]
[]
["DO NOT ENTER ANYTHING ON THIS PAGE.  THE VALUES CALCULATED"]
["ON THIS PAGE ARE USED IN THE CASH FLOW ANALYSIS TAB."]
[]
[null,"= Calculated Cells (do not change formulas)"]
[null,"= Input Required"]
[null,"= Optional Input; To Provide Additional Information Only"]
[null,"= H2A Guidelines/Information Cells"]
[]
[]
[null,"MACRS Depreciation Table (Half-Year Convention)"]
[null,null,"Recovery Period"]
[null,"Recovery Period",3,5,7,10,15,20]
[null,1,0.33329999999999999,0.2,0.1429,0.1,0.05,3.7499999999999999E-2]
[null,2,0.44450000000000001,0.32,0.24490000000000001,0.18,9.5000000000000001E-2,7.2190000000000004E-2]
[null,3,0.14810000000000001,0.192,0.1749,0.14399999999999999,8.5500000000000007E-2,6.6769999999999996E-2]
[null,4,7.4099999999999999E-2,0.1152,0.1249,0.1152,7.6999999999999999E-2,6.1769999999999999E-2]
[null,5,null,0.1152,8.9300000000000004E-2,9.2200000000000004E-2,6.93E-2,5.713E-2]
[null,6,null,5.7599999999999998E-2,8.9200000000000002E-2,7.3700000000000002E-2,6.2300000000000001E-2,5.2850000000000001E-2]
[null,7,null,null,8.9300000000000004E-2,6.5500000000000003E-2,5.8999999999999997E-2,4.888E-2]
[null,8,null,null,4.4600000000000001E-2,6.5500000000000003E-2,5.8999999999999997E-2,4.5220000000000003E-2]
[null,9,null,null,null,6.5600000000000006E-2,5.91E-2,4.462E-2]
[null,10,null,null,null,6.5500000000000003E-2,5.8999999999999997E-2,4.4609999999999997E-2]
[null,11,null,null,null,3.2800000000000003E-2,5.91E-2,4.462E-2]
[null,12,null,null,null,null,5.8999999999999997E-2,4.4609999999999997E-2]
[null,13,null,null,null,null,5.91E-2,4.462E-2]
[null,14,null,null,null,null,5.8999999999999997E-2,4.4609999999999997E-2]
[null,15,null,null,null,null,5.91E-2,4.462E-2]
[null,16,null,null,null,null,2.9499999999999998E-2,4.4609999999999997E-2]
[null,17,null,null,null,null,null,4.462E-2]
[null,18,null,null,null,null,null,4.4609999999999997E-2]
[null,19,null,null,null,null,null,4.462E-2]
[null,20,null,null,null,null,null,4.4609999999999997E-2]
[null,21,null,null,null,null,null,2.231E-2]
[null,"NPV - Real IRR",{"$f":"NPV(real_irr,C15:C35)","v":0.861730483722558},0.81132579180653486,0.76611247423420981,0.70592323058796147,0.57966874115937961,0.50624177952518146]
[null,"NPV - Nominal IRR",{"$f":"NPV(nominal_irr,C15:C35)","v":0.83149291060393982},0.77231075823151107,0.72034649543580254,0.65286934217044934,0.51586770297474116,0.44094384285873256]
[]
[]
[]
["Inputs from Cash-Input Sheet"]
["Depreciation Type",{"$f":"depr_type","v":"MACRS"}]
["Depreciation Period (yrs)",{"$f":"depr_length","v":7}]
["Total Initial Depreciable Capital",{"$f":"-('Cash Flow Analysis'!G65+SUM('Cash Flow Analysis'!H65:H113))","v":2111770.1843013763}]
[]
[]
["DEPRECIATION CALCULATION TABLE"]
["Operation Year","Annual Depreciable Capital",1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,"Total"]
[{"$f":"IF('Cash Flow Analysis'!C65=\"\",\"\",'Cash Flow Analysis'!C65)","v":-1},{"$f":"IF(A49=\"\",\"\",IF(A49<1,0,IF(A49=1,$B$44-'Cash Flow Analysis'!I65,-'Cash Flow Analysis'!I65)))","v":0},{"$f":"IF(B49=\"\",\"\",IF(AND($B$42=\"Straight Line\",$C$48<=depr_length),B49/depr_length,IF(AND($B$42=\"MACRS\",$C$48<=depr_length+1),B49*INDEX(MACRS_Table,MATCH($C$48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":0},{"$f":"IF($B$49=\"\",\"\",IF(AND($B$42=\"Straight Line\",D48<=depr_length),$B$49/depr_length,IF(AND($B$42=\"MACRS\",D48<=depr_length+1),$B$49*INDEX(MACRS_Table,MATCH(D48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":0},0,0,0,0,0,0,"","","","","","","","","","","","","",{"$f":"SUM(C49:W49)","v":0}]
[{"$f":"IF('Cash Flow Analysis'!C66=\"\",\"\",'Cash Flow Analysis'!C66)","v":1},{"$f":"IF(A50=\"\",\"\",IF(A50<1,0,IF(A50=1,$B$44-'Cash Flow Analysis'!I66,-'Cash Flow Analysis'!I66)))","v":2111770.1843013763},{"$f":"IF($B$50=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$50/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$50*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":301771.95933666668},517172.51813540707,369348.60523431073,263760.0960192419,188581.07745811291,188369.90043968277,188581.07745811291,94184.950219841383,"","","","","","","","","","","","","",2111770.1843013763]
[{"$f":"IF('Cash Flow Analysis'!C67=\"\",\"\",'Cash Flow Analysis'!C67)","v":2},{"$f":"IF(A51=\"\",\"\",IF(A51<1,0,IF(A51=1,$B$44-'Cash Flow Analysis'!I67,-'Cash Flow Analysis'!I67)))","v":0},{"$f":"IF($B$51=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$51/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$51*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":0},0,0,0,0,0,0,0,"","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C68=\"\",\"\",'Cash Flow Analysis'!C68)","v":3},{"$f":"IF(A52=\"\",\"\",IF(A52<1,0,IF(A52=1,$B$44-'Cash Flow Analysis'!I68,-'Cash Flow Analysis'!I68)))","v":0},{"$f":"IF($B$52=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$52/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$52*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":0},0,0,0,0,0,0,0,"","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C69=\"\",\"\",'Cash Flow Analysis'!C69)","v":4},{"$f":"IF(A53=\"\",\"\",IF(A53<1,0,IF(A53=1,$B$44-'Cash Flow Analysis'!I69,-'Cash Flow Analysis'!I69)))","v":0},{"$f":"IF($B$53=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$53/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$53*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":0},0,0,0,0,0,0,0,"","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C70=\"\",\"\",'Cash Flow Analysis'!C70)","v":5},{"$f":"IF(A54=\"\",\"\",IF(A54<1,0,IF(A54=1,$B$44-'Cash Flow Analysis'!I70,-'Cash Flow Analysis'!I70)))","v":0},{"$f":"IF($B$54=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$54/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$54*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":0},0,0,0,0,0,0,0,"","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C71=\"\",\"\",'Cash Flow Analysis'!C71)","v":6},{"$f":"IF(A55=\"\",\"\",IF(A55<1,0,IF(A55=1,$B$44-'Cash Flow Analysis'!I71,-'Cash Flow Analysis'!I71)))","v":252446.70767227848},{"$f":"IF($B$55=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$55/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$55*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":36074.634526368594},61824.198708941003,44152.929171881508,31530.593788267583,22543.490995134471,22518.246324367243,22543.490995134471,11259.123162183621,"","","","","","","","","","","","","",252446.70767227845]
[{"$f":"IF('Cash Flow Analysis'!C72=\"\",\"\",'Cash Flow Analysis'!C72)","v":7},{"$f":"IF(A56=\"\",\"\",IF(A56<1,0,IF(A56=1,$B$44-'Cash Flow Analysis'!I72,-'Cash Flow Analysis'!I72)))","v":0},{"$f":"IF($B$56=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$56/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$56*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":0},0,0,0,0,0,0,0,"","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C73=\"\",\"\",'Cash Flow Analysis'!C73)","v":8},{"$f":"IF(A57=\"\",\"\",IF(A57<1,0,IF(A57=1,$B$44-'Cash Flow Analysis'!I73,-'Cash Flow Analysis'!I73)))","v":0},{"$f":"IF($B$57=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$57/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$57*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":0},0,0,0,0,0,0,0,"","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C74=\"\",\"\",'Cash Flow Analysis'!C74)","v":9},{"$f":"IF(A58=\"\",\"\",IF(A58<1,0,IF(A58=1,$B$44-'Cash Flow Analysis'!I74,-'Cash Flow Analysis'!I74)))","v":0},{"$f":"IF($B$58=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$58/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$58*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":0},0,0,0,0,0,0,0,"","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C75=\"\",\"\",'Cash Flow Analysis'!C75)","v":10},{"$f":"IF(A59=\"\",\"\",IF(A59<1,0,IF(A59=1,$B$44-'Cash Flow Analysis'!I75,-'Cash Flow Analysis'!I75)))","v":0},{"$f":"IF($B$59=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$59/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$59*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":0},0,0,0,0,0,0,0,"","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C76=\"\",\"\",'Cash Flow Analysis'!C76)","v":11},{"$f":"IF(A60=\"\",\"\",IF(A60<1,0,IF(A60=1,$B$44-'Cash Flow Analysis'!I76,-'Cash Flow Analysis'!I76)))","v":924526.52652047004},{"$f":"IF($B$60=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$60/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$60*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":132114.84063977518},226416.54634486311,161699.68948843022,115473.36316240671,82560.218818277979,82467.76616562593,82560.218818277979,41233.883082812965,"","","","","","","","","","","","","",924526.52652046992]
[{"$f":"IF('Cash Flow Analysis'!C77=\"\",\"\",'Cash Flow Analysis'!C77)","v":12},{"$f":"IF(A61=\"\",\"\",IF(A61<1,0,IF(A61=1,$B$44-'Cash Flow Analysis'!I77,-'Cash Flow Analysis'!I77)))","v":0},{"$f":"IF($B$61=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$61/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$61*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":0},0,0,0,0,0,0,0,"","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C78=\"\",\"\",'Cash Flow Analysis'!C78)","v":13},{"$f":"IF(A62=\"\",\"\",IF(A62<1,0,IF(A62=1,$B$44-'Cash Flow Analysis'!I78,-'Cash Flow Analysis'!I78)))","v":0},{"$f":"IF($B$62=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$62/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$62*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":0},0,0,0,0,0,0,0,"","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C79=\"\",\"\",'Cash Flow Analysis'!C79)","v":14},{"$f":"IF(A63=\"\",\"\",IF(A63<1,0,IF(A63=1,$B$44-'Cash Flow Analysis'!I79,-'Cash Flow Analysis'!I79)))","v":0},{"$f":"IF($B$63=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$63/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$63*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":0},0,0,0,0,0,0,0,"","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C80=\"\",\"\",'Cash Flow Analysis'!C80)","v":15},{"$f":"IF(A64=\"\",\"\",IF(A64<1,0,IF(A64=1,$B$44-'Cash Flow Analysis'!I80,-'Cash Flow Analysis'!I80)))","v":0},{"$f":"IF($B$64=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$64/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$64*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":0},0,0,0,0,0,0,0,"","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C81=\"\",\"\",'Cash Flow Analysis'!C81)","v":16},{"$f":"IF(A65=\"\",\"\",IF(A65<1,0,IF(A65=1,$B$44-'Cash Flow Analysis'!I81,-'Cash Flow Analysis'!I81)))","v":304727.4315871303},{"$f":"IF($B$65=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$65/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$65*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":43545.549973800917},74627.747995688216,53296.827784589092,38060.456205232571,27212.159640730737,27181.686897572024,27212.159640730737,13590.843448786012,"","","","","","","","","","","","","",304727.43158713024]
[{"$f":"IF('Cash Flow Analysis'!C82=\"\",\"\",'Cash Flow Analysis'!C82)","v":17},{"$f":"IF(A66=\"\",\"\",IF(A66<1,0,IF(A66=1,$B$44-'Cash Flow Analysis'!I82,-'Cash Flow Analysis'!I82)))","v":0},{"$f":"IF($B$66=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$66/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$66*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":0},0,0,0,0,0,0,0,"","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C83=\"\",\"\",'Cash Flow Analysis'!C83)","v":18},{"$f":"IF(A67=\"\",\"\",IF(A67<1,0,IF(A67=1,$B$44-'Cash Flow Analysis'!I83,-'Cash Flow Analysis'!I83)))","v":0},{"$f":"IF($B$67=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$67/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$67*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":0},0,0,0,0,0,0,0,"","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C84=\"\",\"\",'Cash Flow Analysis'!C84)","v":19},{"$f":"IF(A68=\"\",\"\",IF(A68<1,0,IF(A68=1,$B$44-'Cash Flow Analysis'!I84,-'Cash Flow Analysis'!I84)))","v":0},{"$f":"IF($B$68=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$68/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$68*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":0},0,0,0,0,0,0,0,"","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C85=\"\",\"\",'Cash Flow Analysis'!C85)","v":20},{"$f":"IF(A69=\"\",\"\",IF(A69<1,0,IF(A69=1,$B$44-'Cash Flow Analysis'!I85,-'Cash Flow Analysis'!I85)))","v":0},{"$f":"IF($B$69=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$69/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$69*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":0},0,0,0,0,0,0,0,"","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C86=\"\",\"\",'Cash Flow Analysis'!C86)","v":""},{"$f":"IF(A70=\"\",\"\",IF(A70<1,0,IF(A70=1,$B$44-'Cash Flow Analysis'!I86,-'Cash Flow Analysis'!I86)))","v":""},{"$f":"IF($B$70=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$70/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$70*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":""},"","","","","","","","","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C87=\"\",\"\",'Cash Flow Analysis'!C87)","v":""},{"$f":"IF(A71=\"\",\"\",IF(A71<1,0,IF(A71=1,$B$44-'Cash Flow Analysis'!I87,-'Cash Flow Analysis'!I87)))","v":""},{"$f":"IF($B$71=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$71/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$71*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":""},"","","","","","","","","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C88=\"\",\"\",'Cash Flow Analysis'!C88)","v":""},{"$f":"IF(A72=\"\",\"\",IF(A72<1,0,IF(A72=1,$B$44-'Cash Flow Analysis'!I88,-'Cash Flow Analysis'!I88)))","v":""},{"$f":"IF($B$72=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$72/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$72*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":""},"","","","","","","","","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C89=\"\",\"\",'Cash Flow Analysis'!C89)","v":""},{"$f":"IF(A73=\"\",\"\",IF(A73<1,0,IF(A73=1,$B$44-'Cash Flow Analysis'!I89,-'Cash Flow Analysis'!I89)))","v":""},{"$f":"IF($B$73=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$73/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$73*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":""},"","","","","","","","","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C90=\"\",\"\",'Cash Flow Analysis'!C90)","v":""},{"$f":"IF(A74=\"\",\"\",IF(A74<1,0,IF(A74=1,$B$44-'Cash Flow Analysis'!I90,-'Cash Flow Analysis'!I90)))","v":""},{"$f":"IF($B$74=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$74/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$74*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":""},"","","","","","","","","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C91=\"\",\"\",'Cash Flow Analysis'!C91)","v":""},{"$f":"IF(A75=\"\",\"\",IF(A75<1,0,IF(A75=1,$B$44-'Cash Flow Analysis'!I91,-'Cash Flow Analysis'!I91)))","v":""},{"$f":"IF($B$75=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$75/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$75*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":""},"","","","","","","","","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C92=\"\",\"\",'Cash Flow Analysis'!C92)","v":""},{"$f":"IF(A76=\"\",\"\",IF(A76<1,0,IF(A76=1,$B$44-'Cash Flow Analysis'!I92,-'Cash Flow Analysis'!I92)))","v":""},{"$f":"IF($B$76=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$76/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$76*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":""},"","","","","","","","","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C93=\"\",\"\",'Cash Flow Analysis'!C93)","v":""},{"$f":"IF(A77=\"\",\"\",IF(A77<1,0,IF(A77=1,$B$44-'Cash Flow Analysis'!I93,-'Cash Flow Analysis'!I93)))","v":""},{"$f":"IF($B$77=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$77/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$77*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":""},"","","","","","","","","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C94=\"\",\"\",'Cash Flow Analysis'!C94)","v":""},{"$f":"IF(A78=\"\",\"\",IF(A78<1,0,IF(A78=1,$B$44-'Cash Flow Analysis'!I94,-'Cash Flow Analysis'!I94)))","v":""},{"$f":"IF($B$78=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$78/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$78*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":""},"","","","","","","","","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C95=\"\",\"\",'Cash Flow Analysis'!C95)","v":""},{"$f":"IF(A79=\"\",\"\",IF(A79<1,0,IF(A79=1,$B$44-'Cash Flow Analysis'!I95,-'Cash Flow Analysis'!I95)))","v":""},{"$f":"IF($B$79=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$79/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$79*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":""},"","","","","","","","","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C96=\"\",\"\",'Cash Flow Analysis'!C96)","v":""},{"$f":"IF(A80=\"\",\"\",IF(A80<1,0,IF(A80=1,$B$44-'Cash Flow Analysis'!I96,-'Cash Flow Analysis'!I96)))","v":""},{"$f":"IF($B$80=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$80/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$80*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":""},"","","","","","","","","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C97=\"\",\"\",'Cash Flow Analysis'!C97)","v":""},{"$f":"IF(A81=\"\",\"\",IF(A81<1,0,IF(A81=1,$B$44-'Cash Flow Analysis'!I97,-'Cash Flow Analysis'!I97)))","v":""},{"$f":"IF($B$81=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$81/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$81*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":""},"","","","","","","","","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C98=\"\",\"\",'Cash Flow Analysis'!C98)","v":""},{"$f":"IF(A82=\"\",\"\",IF(A82<1,0,IF(A82=1,$B$44-'Cash Flow Analysis'!I98,-'Cash Flow Analysis'!I98)))","v":""},{"$f":"IF($B$82=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$82/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$82*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":""},"","","","","","","","","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C99=\"\",\"\",'Cash Flow Analysis'!C99)","v":""},{"$f":"IF(A83=\"\",\"\",IF(A83<1,0,IF(A83=1,$B$44-'Cash Flow Analysis'!I99,-'Cash Flow Analysis'!I99)))","v":""},{"$f":"IF($B$83=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$83/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$83*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":""},"","","","","","","","","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C100=\"\",\"\",'Cash Flow Analysis'!C100)","v":""},{"$f":"IF(A84=\"\",\"\",IF(A84<1,0,IF(A84=1,$B$44-'Cash Flow Analysis'!I100,-'Cash Flow Analysis'!I100)))","v":""},{"$f":"IF($B$84=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$84/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$84*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":""},"","","","","","","","","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C101=\"\",\"\",'Cash Flow Analysis'!C101)","v":""},{"$f":"IF(A85=\"\",\"\",IF(A85<1,0,IF(A85=1,$B$44-'Cash Flow Analysis'!I101,-'Cash Flow Analysis'!I101)))","v":""},{"$f":"IF($B$85=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$85/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$85*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":""},"","","","","","","","","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C102=\"\",\"\",'Cash Flow Analysis'!C102)","v":""},{"$f":"IF(A86=\"\",\"\",IF(A86<1,0,IF(A86=1,$B$44-'Cash Flow Analysis'!I102,-'Cash Flow Analysis'!I102)))","v":""},{"$f":"IF($B$86=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$86/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$86*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":""},"","","","","","","","","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C103=\"\",\"\",'Cash Flow Analysis'!C103)","v":""},{"$f":"IF(A87=\"\",\"\",IF(A87<1,0,IF(A87=1,$B$44-'Cash Flow Analysis'!I103,-'Cash Flow Analysis'!I103)))","v":""},{"$f":"IF($B$87=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$87/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$87*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":""},"","","","","","","","","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C104=\"\",\"\",'Cash Flow Analysis'!C104)","v":""},{"$f":"IF(A88=\"\",\"\",IF(A88<1,0,IF(A88=1,$B$44-'Cash Flow Analysis'!I104,-'Cash Flow Analysis'!I104)))","v":""},{"$f":"IF($B$88=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$88/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$88*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":""},"","","","","","","","","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C105=\"\",\"\",'Cash Flow Analysis'!C105)","v":""},{"$f":"IF(A89=\"\",\"\",IF(A89<1,0,IF(A89=1,$B$44-'Cash Flow Analysis'!I105,-'Cash Flow Analysis'!I105)))","v":""},{"$f":"IF($B$89=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$89/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$89*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":""},"","","","","","","","","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C106=\"\",\"\",'Cash Flow Analysis'!C106)","v":""},{"$f":"IF(A90=\"\",\"\",IF(A90<1,0,IF(A90=1,$B$44-'Cash Flow Analysis'!I106,-'Cash Flow Analysis'!I106)))","v":""},{"$f":"IF($B$90=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$90/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$90*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":""},"","","","","","","","","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C107=\"\",\"\",'Cash Flow Analysis'!C107)","v":""},{"$f":"IF(A91=\"\",\"\",IF(A91<1,0,IF(A91=1,$B$44-'Cash Flow Analysis'!I107,-'Cash Flow Analysis'!I107)))","v":""},{"$f":"IF($B$91=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$91/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$91*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":""},"","","","","","","","","","","","","","","","","","","","",0]
[{"$f":"IF('Cash Flow Analysis'!C108=\"\",\"\",'Cash Flow Analysis'!C108)","v":""},{"$f":"IF(A92=\"\",\"\",IF(A92<1,0,IF(A92=1,$B$44-'Cash Flow Analysis'!I108,-'Cash Flow Analysis'!I108)))","v":""},{"$f":"IF($B$92=\"\",\"\",IF(AND($B$42=\"Straight Line\",C48<=depr_length),$B$92/depr_length,IF(AND($B$42=\"MACRS\",C48<=depr_length+1),$B$92*INDEX(MACRS_Table,MATCH(C48,recovery_year,0),MATCH($B$43,recovery_period,0)),\"\")))","v":""},"","","","","","","","","","","","","","","","","","","","",0]
[]
[]
["DEPRECIATION CHARGES TO CASH FLOW TAB"]
["Operation Year","Depreciation Charge","Post Analysis Depreciation"]
[{"$f":"IF('Cash Flow Analysis'!C65=\"\",\"\",'Cash Flow Analysis'!C65)","v":-1},{"$f":"C49","v":0},{"$f":"IF(A97=\"\",B97,0)","v":0}]
[{"$f":"IF('Cash Flow Analysis'!C66=\"\",\"\",'Cash Flow Analysis'!C66)","v":1},{"$f":"SUM(D49,C50)","v":301771.95933666668},0]
[{"$f":"IF('Cash Flow Analysis'!C67=\"\",\"\",'Cash Flow Analysis'!C67)","v":2},{"$f":"SUM(E49,D50,C51)","v":517172.51813540707},0]
[{"$f":"IF('Cash Flow Analysis'!C68=\"\",\"\",'Cash Flow Analysis'!C68)","v":3},{"$f":"SUM(F49,E50,D51,C52)","v":369348.60523431073},0]
[{"$f":"IF('Cash Flow Analysis'!C69=\"\",\"\",'Cash Flow Analysis'!C69)","v":4},{"$f":"SUM(G49,F50,E51,D52,C53)","v":263760.0960192419},0]
[{"$f":"IF('Cash Flow Analysis'!C70=\"\",\"\",'Cash Flow Analysis'!C70)","v":5},{"$f":"SUM(H49,G50,F51,E52,D53,C54)","v":188581.07745811291},0]
[{"$f":"IF('Cash Flow Analysis'!C71=\"\",\"\",'Cash Flow Analysis'!C71)","v":6},{"$f":"SUM(I49,H50,G51,F52,E53,D54,C55)","v":224444.53496605135},0]
[{"$f":"IF('Cash Flow Analysis'!C72=\"\",\"\",'Cash Flow Analysis'!C72)","v":7},{"$f":"SUM(J49,I50,H51,G52,F53,E54,D55,C56)","v":250405.2761670539},0]
[{"$f":"IF('Cash Flow Analysis'!C73=\"\",\"\",'Cash Flow Analysis'!C73)","v":8},{"$f":"SUM(K49,J50,I51,H52,G53,F54,E55,D56,C57)","v":138337.8793917229},0]
[{"$f":"IF('Cash Flow Analysis'!C74=\"\",\"\",'Cash Flow Analysis'!C74)","v":9},{"$f":"SUM(L49,K50,J51,I52,H53,G54,F55,E56,D57,C58)","v":31530.593788267583},0]
[{"$f":"IF('Cash Flow Analysis'!C75=\"\",\"\",'Cash Flow Analysis'!C75)","v":10},{"$f":"SUM(M49,L50,K51,J52,I53,H54,G55,F56,E57,D58,C59)","v":22543.490995134471},0]
[{"$f":"IF('Cash Flow Analysis'!C76=\"\",\"\",'Cash Flow Analysis'!C76)","v":11},{"$f":"SUM(N49,M50,L51,K52,J53,I54,H55,G56,F57,E58,D59,C60)","v":154633.08696414242},0]
[{"$f":"IF('Cash Flow Analysis'!C77=\"\",\"\",'Cash Flow Analysis'!C77)","v":12},{"$f":"SUM(O49,N50,M51,L52,K53,J54,I55,H56,G57,F58,E59,D60,C61)","v":248960.03733999757},0]
[{"$f":"IF('Cash Flow Analysis'!C78=\"\",\"\",'Cash Flow Analysis'!C78)","v":13},{"$f":"SUM(P49,O50,N51,M52,L53,K54,J55,I56,H57,G58,F59,E60,D61,C62)","v":172958.81265061384},0]
[{"$f":"IF('Cash Flow Analysis'!C79=\"\",\"\",'Cash Flow Analysis'!C79)","v":14},{"$f":"SUM(Q49,P50,O51,N52,M53,L54,K55,J56,I57,H58,G59,F60,E61,D62,C63)","v":115473.36316240671},0]
[{"$f":"IF('Cash Flow Analysis'!C80=\"\",\"\",'Cash Flow Analysis'!C80)","v":15},{"$f":"SUM(R49,Q50,P51,O52,N53,M54,L55,K56,J57,I58,H59,G60,F61,E62,D63,C64)","v":82560.218818277979},0]
[{"$f":"IF('Cash Flow Analysis'!C81=\"\",\"\",'Cash Flow Analysis'!C81)","v":16},{"$f":"SUM(S49,R50,Q51,P52,O53,N54,M55,L56,K57,J58,I59,H60,G61,F62,E63,D64,C65)","v":126013.31613942684},0]
[{"$f":"IF('Cash Flow Analysis'!C82=\"\",\"\",'Cash Flow Analysis'!C82)","v":17},{"$f":"SUM(T49,S50,R51,Q52,P53,O54,N55,M56,L57,K58,J59,I60,H61,G62,F63,E64,D65,C66)","v":157187.9668139662},0]
[{"$f":"IF('Cash Flow Analysis'!C83=\"\",\"\",'Cash Flow Analysis'!C83)","v":18},{"$f":"SUM(U49,T50,S51,R52,Q53,P54,O55,N56,M57,L58,K59,J60,I61,H62,G63,F64,E65,D66,C67)","v":94530.710867402056},0]
[{"$f":"IF('Cash Flow Analysis'!C84=\"\",\"\",'Cash Flow Analysis'!C84)","v":19},{"$f":"SUM(V49,U50,T51,S52,R53,Q54,P55,O56,N57,M58,L59,K60,J61,I62,H63,G64,F65,E66,D67,C68)","v":38060.456205232571},0]
[{"$f":"IF('Cash Flow Analysis'!C85=\"\",\"\",'Cash Flow Analysis'!C85)","v":20},{"$f":"SUM(W49,V50,U51,T52,S53,R54,Q55,P56,O57,N58,M59,L60,K61,J62,I63,H64,G65,F66,E67,D68,C69)","v":27212.159640730737},0]
[{"$f":"IF('Cash Flow Analysis'!C86=\"\",\"\",'Cash Flow Analysis'!C86)","v":""},27181.686897572024,27181.686897572024]
[{"$f":"IF('Cash Flow Analysis'!C87=\"\",\"\",'Cash Flow Analysis'!C87)","v":""},27212.159640730737,27212.159640730737]
[{"$f":"IF('Cash Flow Analysis'!C88=\"\",\"\",'Cash Flow Analysis'!C88)","v":""},13590.843448786012,13590.843448786012]
[{"$f":"IF('Cash Flow Analysis'!C89=\"\",\"\",'Cash Flow Analysis'!C89)","v":""},0,0]
[{"$f":"IF('Cash Flow Analysis'!C90=\"\",\"\",'Cash Flow Analysis'!C90)","v":""},0,0]
[{"$f":"IF('Cash Flow Analysis'!C91=\"\",\"\",'Cash Flow Analysis'!C91)","v":""},0,0]
[{"$f":"IF('Cash Flow Analysis'!C92=\"\",\"\",'Cash Flow Analysis'!C92)","v":""},0,0]
[{"$f":"IF('Cash Flow Analysis'!C93=\"\",\"\",'Cash Flow Analysis'!C93)","v":""},0,0]
[{"$f":"IF('Cash Flow Analysis'!C94=\"\",\"\",'Cash Flow Analysis'!C94)","v":""},0,0]
[{"$f":"IF('Cash Flow Analysis'!C95=\"\",\"\",'Cash Flow Analysis'!C95)","v":""},0,0]
[{"$f":"IF('Cash Flow Analysis'!C96=\"\",\"\",'Cash Flow Analysis'!C96)","v":""},0,0]
[{"$f":"IF('Cash Flow Analysis'!C97=\"\",\"\",'Cash Flow Analysis'!C97)","v":""},0,0]
[{"$f":"IF('Cash Flow Analysis'!C98=\"\",\"\",'Cash Flow Analysis'!C98)","v":""},0,0]
[{"$f":"IF('Cash Flow Analysis'!C99=\"\",\"\",'Cash Flow Analysis'!C99)","v":""},0,0]
[{"$f":"IF('Cash Flow Analysis'!C100=\"\",\"\",'Cash Flow Analysis'!C100)","v":""},0,0]
[{"$f":"IF('Cash Flow Analysis'!C101=\"\",\"\",'Cash Flow Analysis'!C101)","v":""},0,0]
[{"$f":"IF('Cash Flow Analysis'!C102=\"\",\"\",'Cash Flow Analysis'!C102)","v":""},0,0]
[{"$f":"IF('Cash Flow Analysis'!C103=\"\",\"\",'Cash Flow Analysis'!C103)","v":""},0,0]
[{"$f":"IF('Cash Flow Analysis'!C104=\"\",\"\",'Cash Flow Analysis'!C104)","v":""},0,0]
[{"$f":"IF('Cash Flow Analysis'!C105=\"\",\"\",'Cash Flow Analysis'!C105)","v":""},0,0]
[{"$f":"IF('Cash Flow Analysis'!C106=\"\",\"\",'Cash Flow Analysis'!C106)","v":""},0,0]
[{"$f":"IF('Cash Flow Analysis'!C107=\"\",\"\",'Cash Flow Analysis'!C107)","v":""},0,0]
[{"$f":"IF('Cash Flow Analysis'!C108=\"\",\"\",'Cash Flow Analysis'!C108)","v":""},0,0]
["Totals",{"$f":"SUM(B97:B140)","v":3593470.8500812561},{"$f":"SUM(C97:C140)","v":67984.689987088772}]
[]
[{"$f":"IF('Cash Flow Analysis'!C109=\"\",\"\",'Cash Flow Analysis'!C109)","v":""}]
["Remaining Book Value Calculation for Greater than 40-year Plant Life "]
["Year after 40","Depreciation Charge"]
[1,{"$f":"SUM(D92,E91,F90,G89,H88,I87,J86,K85,L84,M83,N82,O81,P80,Q79,R78,S77,T76,U75,V74,W73)","v":0}]
[2,{"$f":"SUM(E92,F91,G90,H89,I88,J87,K86,L85,M84,N83,O82,P81,Q80,R79,S78,T77,U76,V75,W74)","v":0}]
[3,{"$f":"SUM(F92,G91,H90,I89,J88,K87,L86,M85,N84,O83,P82,Q81,R80,S79,T78,U77,V76,W75)","v":0}]
[4,{"$f":"SUM(G92,H91,I90,J89,K88,L87,M86,N85,O84,P83,Q82,R81,S80,T79,U78,V77,W76)","v":0}]
[5,{"$f":"SUM(H92,I91,J90,K89,L88,M87,N86,O85,P84,Q83,R82,S81,T80,U79,V78,W77)","v":0}]
[6,{"$f":"SUM(I92,J91,K90,L89,M88,N87,O86,P85,Q84,R83,S82,T81,U80,V79,W78)","v":0}]
[7,{"$f":"SUM(J92,K91,L90,M89,N88,O87,P86,Q85,R84,S83,T82,U81,V80,W79)","v":0}]
[8,{"$f":"SUM(K92,L91,M90,N89,O88,P87,Q86,R85,S84,T83,U82,V81,W80)","v":0}]
[9,{"$f":"SUM(L92,M91,N90,O89,P88,Q87,R86,S85,T84,U83,V82,W81)","v":0}]
[10,{"$f":"SUM(M92,N91,O90,P89,Q88,R87,S86,T85,U84,V83,W82)","v":0}]
[11,{"$f":"SUM(N92,O91,P90,Q89,R88,S87,T86,U85,V84,W83)","v":0}]
[12,{"$f":"SUM(O92,P91,Q90,R89,S88,T87,U86,V85,W84)","v":0}]
[13,{"$f":"SUM(P92,Q91,R90,S89,T88,U87,V86,W85)","v":0}]
[14,{"$f":"SUM(Q92,R91,S90,T89,U88,V87,W86)","v":0}]
[15,{"$f":"SUM(R92,S91,T90,U89,V88,W87)","v":0}]
[16,{"$f":"SUM(S92,T91,U90,V89,W88)","v":0}]
[17,{"$f":"SUM(T92,U91,V90,W89)","v":0}]
[18,{"$f":"SUM(U92,V91,W90)","v":0}]
[19,{"$f":"SUM(V92,W91)","v":0}]
[20,{"$f":"SUM(W92)","v":0}]
["Totals",{"$f":"SUM(B146:B165)","v":0}]

{"sheet":"Constants and Conversions","index":17,"n_rows":31,"n_cols":5,"rows_kept":31,"cut":false,"hidden":false,"merged":[]}
["To Convert From","To","Multiply by:"]
["General"]
["miles","km",1.6093,"km/mile"]
["gallons","liters",3.7850000000000001,"L/gal"]
["MPG","kWh/km",1.8263969224024776E-2,"(kWh/km)/MPG"]
["scf","Nm3",2.6852999999999998E-2,"Nm3/scf","60 degrees F, 1 atm"]
["lb","kg",{"$f":"1/2.205","v":0.45351473922902491},"kg/lb"]
["ncf","Nm3",2.8316999999999998E-2,"Nm3/ncf","0 degrees C (32 F), 1 atm"]
["MPa","psi",145.03800000000001,"psi/MPa"]
[]
["Energy"]
["MJ","kWh",0.27777777777777779]
["gallon of gasoline eq (GGE) -conventional gasoline","kWh",34.022625288888882]
["kg H2 (LHV)","GGE",0.97933196399532141]
["kg H2 (LHV)","kWh",{"$f":"kgH2_to_GJ*MJ_to_kWh*1000","v":33.392121748655818}]
["kg H2 (LHV)","GJ",{"$f":"H2_LHV_MJ_p_kg/1000","v":0.12021163829516093}]
["btu ","kWh",2.9308323563892143E-4]
["mmBTU","GJ",1.0549999999999999]
[]
[]
["Greenhouse Gas Emissions Factors",null,"IPCC Fourth Assessment Report: Climate Change 2007 (http://www.ipcc.ch/publications_and_data/ar4/wg1/en/ch2s2-10-2.html) Table 2.14 100-year potential"]
["CO2",1]
["CH4",25]
["N2O",298]
[]
[]
["Energy Feedstock Conversions"]
["Usage unit","Conversion from $/GJ"]
["mmBtu",{"$f":"mmBTU_to_GJ","v":1.0549999999999999}]
["kWh",{"$f":"1/MJ_to_kWh/1000","v":3.5999999999999995E-3}]
["GJ",1]

{"sheet":"Lists","index":18,"n_rows":80,"n_cols":29,"rows_kept":80,"cut":false,"hidden":false,"merged":[]}
["Cancelled"]
[null,null,null,null,null,null,null,null,null,"Price_Tables"]
["Use_Default",null,"Yes_No",null,"Temp_var_location",null,"Sensitivity_Variables",null,null,"AEO_2009_Reference_Case",null,null,"Import_Variable_List",null,"Input_Value_Defaults",null,"Default used?","Export_Variable_List",null,"CO2_Location",null,"CO2_Terrain",null,null,"CO2_Value_Defaults",null,"Default used?","Scaling_Method_Defaults"]
["Use H2A Value",null,"Yes",null,100000,null,"Operating Capacity Factor (fraction)","cap_factor",null,"AEO_2013_Reference_Case",null,null,"title",null,{"$f":"M7","v":"ref_year"},2016,true,"title",null,1,"USA, Canada, Europe, Japan, Australia","cultivated land",1.1000000000000001,null,"CO2_Capture_Efficiency",0.9,false,"Engin","Skip"]
["Enter Value",null,"No",null,null,null,"Plant Design Capacity (kg of H2/day)","design_cap",null,"AEO_2013_High_Price_Case",null,null,"cap_factor",null,{"$f":"M18","v":"depr_type"},"MACRS",true,"H2_Price_real",null,1.2,"UK","grassland",1,null,"CO2_MaintFactor",0.04,false,"Site_prep","Skip"]
[null,null,null,null,null,null,"Assumed start-up year","startup_year",null,"AEO_2014_Reference_Case",null,null,"design_cap",null,{"$f":"M19","v":"equity"},0.4,true,"H2_Price_nominal",null,null,null,"wooded",1.05,null,"CO2_Pin_psia",14.7,false,"Process_cont","Skip"]
["Add_As_List",null,"Feed_Type_List",null,null,null,"Length of Construction Period (years)","construct",null,"AEO_2017_Reference_Case",null,null,"ref_year",null,{"$f":"M25","v":"decom_percent"},0.1,true,"result_cap_contr",null,null,null,"jungle",1.1000000000000001,null,"CO2_credit",0,true,"Project_cont","Skip"]
["Feedstock",null,"Feed",null,null,null,"Start-up Time (years)","start_time",null,null,null,null,"startup_year",null,"salvage_perct",0.1,true,"result_decom_contr",null,null,null,"stony desert",1.1000000000000001,null,"n_CO2_pumps",1,false,"Fees","Skip"]
["Utility",null,"Utility",null,null,null,"Plant life (years)","plant_life",null,null,null,null,"construct",null,"inflation_rate",1.9E-2,true,"result_fixed_o_m_contr",null,null,null,"<20% Mountainous",1.3,null,"CO2_PipeLength",100,true,"Other_indirect","Skip"]
["Byproduct",null,"Feed Utility",null,null,null,"Decommissioning costs (fraction of depreciable capital investment)","decom_percent",null,null,null,null,"percent_cap1",null,"real_irr",0.08,true,"result_feed_contr",null,null,null,">50% Mountainous",1.5,null,"CO2_Pump_Eff",0.75,false,"Permitting","Skip"]
[null,null,"Feed Utility Byprod",null,null,null,"Salvage value (fraction of total capital investment)","salvage_perct",null,"Price_Table_in_Use","Energy_Feed_List",null,"percent_cap2",null,"state_tax_rate",0.06,true,"result_byprod_contr",null,null,null,null,null,null,"CO2_ControlSystem","Yes",false,"acre_cost","Use Baseline Value"]
[null,null,"Byproduct",null,null,null,"Inflation rate (fraction)","inflation_rate",null,{"$f":"TMP_PriceTable","v":"AEO_2017_Reference_Case"},{"$f":"J12&\"_Feeds\"","v":"AEO_2017_Reference_Case_Feeds"},null,"percent_cap3",null,"fed_tax_rate",0.21,true,"result_other_var_contr",null,null,null,null,null,null,"CO2_SurgeTank","Yes",false,"acres","Use Scale Factor"]
[null,null,null,null,null,null,"After-tax Real IRR (fraction)","real_irr",null,null,"Energy_Feed_Years",null,"percent_cap4",null,"WorkingCap",0.15,true,"result_other_mat_contr",null,null,null,null,null,null,"CO2_PipeElevation",0,true,"FTEs",0.25]
["Delete_As_List",null,"ColorList",null,null,null,"State Taxes (fraction)","state_tax_rate",null,null,{"$f":"J12&\"_Years\"","v":"AEO_2017_Reference_Case_Years"},null,"start_time",null,"overhead_rate",0.2,true,"cap_factor",null,null,null,null,null,null,"CO2_Pipeline_Temp",53,false,"FTE_cost","Use Baseline Value"]
["Energy Feedstock",null,"Input",null,null,null,"Federal Taxes (fraction)","fed_tax_rate",null,null,null,null,"plant_life",null,"tax_ins_rate",0.02,true,"design_cap",null,null,null,null,null,null,null,null,null,"licensing","Use Scale Factor"]
["Energy Utility",null,"Calculated",null,null,null,"WORKING CAPITAL (fraction of yearly change in operating costs)","WorkingCap",null,null,null,null,"anal_period",null,"royalties",0,null,"ref_year",null,null,null,null,null,null,null,null,null,"rent","Use Scale Factor"]
["Energy Byproduct",null,"Error",null,null,null,"Total Direct Capital Cost","direct_cap",null,null,null,null,"depr_length",null,"operator_profit",0,null,"startup_year",null,null,null,null,null,null,null,null,null,"material","Use Scale Factor"]
["Other Feed",null,"Information",null,null,null,"Total Capital Investment","total_cap",null,null,null,null,"depr_type",null,"tax_credit",0,null,"construct",null,null,null,null,null,null,null,null,null,"prod_maint","Use Scale Factor"]
["Other Byproduct",null,"UserInfo",null,null,null,"Total Fixed Operating Cost","fixed",null,null,null,null,"equity",null,"Proc_CO2_tax",0,null,"percent_cap1",null,null,null,null,null,null,null,null,null,"other_fees","Use Scale Ratio"]
["All",null,null,null,null,null,"Cost of land ($/acre)","acre_cost",null,null,null,null,"debt_interest",null,"Upstream_CO2_tax",0,null,"percent_cap2",null,null,null,null,null,null,null,null,null,"other_fixed","Use Scale Factor"]
[null,null,null,null,null,null,"Labor Requirement (FTE)","FTEs",null,null,null,null,"debt_period",null,null,null,null,"percent_cap3",null,null,null,null,null,null,null,null,null,"var_misc","Use Scale Ratio"]
[null,null,null,null,null,null,"G&A rate (fraction of labor cost)","overhead_rate",null,null,null,null,"percnt_fixed",null,null,null,null,"percent_cap4",null,null,null,null,null,null,null,null,null,"total_other_raw","Use Scale Ratio"]
["Scaling_validation",null,null,null,null,null,"Property tax and insurance rate (fraction of total capital investment)","tax_ins_rate",null,null,null,null,"percnt_revs",null,null,null,null,"start_time",null,null,null,null,null,null,null,null,null,"waste_treat","Use Scale Ratio"]
["Use Scale Ratio",null,null,null,null,null,"Rent ($/year)","rent",null,null,null,null,"percnt_var",null,null,null,null,"plant_life",null,null,null,null,null,null,null,null,null,"solidwaste_treat","Use Scale Ratio"]
["Use Scale Factor",null,null,null,null,null,"Material costs for maintenance and repairs ($/year)","material",null,null,null,null,"decom_percent",null,null,null,null,"anal_period",null,null,null,null,null,null,null,null,null,"royalties","Use Scale Ratio"]
["Use Baseline Value",null,null,null,null,null,"Production Maintenance and Repairs ($/year)","prod_maint",null,null,null,null,"salvage_perct",null,null,null,null,"depr_length",null,null,null,null,null,null,null,null,null,"operator_profit","Use Scale Ratio"]
["Skip",null,null,null,null,null,"Waste treatment costs ($/year)","waste_treat",null,null,null,null,"inflation_rate",null,null,null,null,"depr_type",null,null,null,null,null,null,null,null,null,"tax_credit","Use Scale Ratio"]
[0.1,null,null,null,null,null,"Solid waste disposal costs ($/year)","solidwaste_treat",null,null,null,null,"real_irr",null,null,null,null,"equity",null,null,null,null,null,null,null,null,null,"CO2_OandMCost","Skip"]
[0.2,null,null,null,null,null,"CO2 sequestration capital costs ($/year)","CO2_seq",null,null,null,null,"state_tax_rate",null,null,null,null,"debt_interest"]
[0.25,null,null,null,null,null,"feedstock Industrial Natural Gas Usage","feedstockIndustrial_Natural_Gas_Usage",null,null,null,null,"fed_tax_rate",null,null,null,null,"debt_period"]
[0.3,null,null,null,null,null,"feedstock Ethanol Usage","feedstockEthanol_Usage",null,null,null,null,"WorkingCap",null,null,null,null,"percnt_fixed"]
[0.4,null,null,null,null,null,"feedstock Commercial Electricity Usage","feedstockCommercial_Electricity_Usage",null,null,null,null,"acre_cost",null,null,null,null,"percnt_revs"]
[0.5,null,null,null,null,null,null,null,null,null,null,null,"acres",null,null,null,null,"percnt_var"]
[0.6,null,null,null,null,null,null,null,null,null,null,null,"FTEs",null,null,null,null,"decom_percent"]
[0.7,null,null,null,null,null,null,null,null,null,null,null,"FTE_cost",null,null,null,null,"salvage_perct"]
[0.8,null,null,null,null,null,null,null,null,null,null,null,"overhead_rate",null,null,null,null,"inflation_rate"]
[0.9,null,null,null,null,null,null,null,null,null,null,null,"tax_ins_rate",null,null,null,null,"real_irr"]
[null,null,null,null,null,null,null,null,null,null,null,null,"rent",null,null,null,null,"state_tax_rate"]
[null,null,null,null,null,null,null,null,null,null,null,null,"material",null,null,null,null,"fed_tax_rate"]
[null,null,null,null,null,null,null,null,null,null,null,null,"prod_maint",null,null,null,null,"WorkingCap"]
[null,null,null,null,null,null,null,null,null,null,null,null,"other_fees",null,null,null,null,"direct_cap"]
[null,null,null,null,null,null,null,null,null,null,null,null,"other_fixed",null,null,null,null,"Engin"]
[null,null,null,null,null,null,null,null,null,null,null,null,"total_other_raw",null,null,null,null,"Site_prep"]
[null,null,null,null,null,null,null,null,null,null,null,null,"var_misc",null,null,null,null,"Process_cont"]
[null,null,null,null,null,null,null,null,null,null,null,null,"waste_treat",null,null,null,null,"Project_cont"]
[null,null,null,null,null,null,null,null,null,null,null,null,"solidwaste_treat",null,null,null,null,"Fees"]
[null,null,null,null,null,null,null,null,null,null,null,null,"replace_factor",null,null,null,null,"Other_indirect"]
[null,null,null,null,null,null,null,null,null,null,null,null,"royalties",null,null,null,null,"Permitting"]
[null,null,null,null,null,null,null,null,null,null,null,null,"operator_profit",null,null,null,null,"acre_cost"]
[null,null,null,null,null,null,null,null,null,null,null,null,"tax_credit",null,null,null,null,"acres"]
[null,null,null,null,null,null,null,null,null,null,null,null,"CO2_seq",null,null,null,null,"FTEs"]
[null,null,null,null,null,null,null,null,null,null,null,null,"CO2_OandMCost",null,null,null,null,"FTE_cost"]
[null,null,null,null,null,null,null,null,null,null,null,null,"CO2_capture_efficiency",null,null,null,null,"overhead_rate"]
[null,null,null,null,null,null,null,null,null,null,null,null,"CO2_MaintFactor",null,null,null,null,"tax_ins_rate"]
[null,null,null,null,null,null,null,null,null,null,null,null,"CO2_PipeFactor",null,null,null,null,"rent"]
[null,null,null,null,null,null,null,null,null,null,null,null,"CO2_SiteCap",null,null,null,null,"material"]
[null,null,null,null,null,null,null,null,null,null,null,null,"CO2_Nwells",null,null,null,null,"prod_maint"]
[null,null,null,null,null,null,null,null,null,null,null,null,"CO2_WellDepth",null,null,null,null,"other_fees"]
[null,null,null,null,null,null,null,null,null,null,null,null,"CO2_location_factor",null,null,null,null,"other_fixed"]
[null,null,null,null,null,null,null,null,null,null,null,null,"CO2_TerrainType",null,null,null,null,"total_other_raw"]
[null,null,null,null,null,null,null,null,null,null,null,null,"CO2_PipeLength",null,null,null,null,"total_utilities"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"total_byproducts"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"var_misc"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"waste_treat"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"solidwaste_treat"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"replace_factor"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"royalties"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"operator_profit"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"tax_credit"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CO2_seq"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CO2_OandMCost"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CO2_capture_efficiency"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CO2_MaintFactor"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CO2_PipeFactor"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CO2_SiteCap"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CO2_Nwells"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CO2_WellDepth"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CO2_location_factor"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CO2_TerrainType"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CO2_PipeLength"]